**3GPP TSG-SA5 Meeting #162 *S5-253790***

Goteborg, Sweden, 25 - 29 August 2025

|  |
| --- |
| *CR-Form-v12.3* |
| **CHANGE REQUEST** |
|  |
|  | **290** | **CR** | **0250** | **rev** | **1** | **Current version:** | **19.3.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | Rel-19 CR 32.290 Correction of handling of unused units |
|  |  |
| ***Source to WG:*** | Ericsson |
| ***Source to TSG:*** | SA5 |
|  |  |
| ***Work item code:*** | TEI19 |  | ***Date:*** | 2025-08-15 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-19 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19) Rel-20 (Release 20)* |
|  |  |
| ***Reason for change:*** | The statement of returning unused quota is unclear. |
|  |  |
| ***Summary of change:*** | Adding a note that returning unused quota is implicit i.e. they should be considered returned not sent in the message. |
|  |  |
| ***Consequences if not approved:*** | Unclear descriptions in the specification may lead to interoperability issues. |
|  |  |
| ***Clauses affected:*** | 5.4.8.1 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** | Revision of S5-253575. |

\* \* \* First Change \* \* \* \*

5.4.8.1 General

The quota can be consumed in the network e.g., seconds, bytes. Quota management applies for charging per rating group, including requested quota, granted quota and used units.

The following applies for quota management:

- NF consumer shall request units via charging data request.

- CHF as NF producer may either grant or deny the request for units via charging data response.

- NF consumer shall report the used units via charging data request with the quota management indicating online.

The following applies when the quota management indicates online:

- NF consumer shall, if quota management is still applicable for the rating group, include requested units.

- NF consumer shall return all unused granted units to the CHF.

NOTE: The returning unused units.is implicit i.e. they should be considered returned not sent in the message.

\* \* \* End of Changes \* \* \* \*