**3GPP TSG-SA WG6 Meeting #68S6-253429**

**Gothenburg, Sweden 25th – 29th August 2025 (revision of S6-253320)**

|  |
| --- |
| *CR-Form-v12.3* |
| **CHANGE REQUEST** |
|  |
|  | **282** | **CR** |  **0387** | **rev** | **1** | **Current version:** |  |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | Clarification on the one-to-one communication |
|  |  |
| ***Source to WG:*** | Huawei, Hisilicon, China BroadNet |
| ***Source to TSG:*** | S6 |
|  |  |
| ***Work item code:*** | **enhMC** |  | ***Date:*** | 07 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-19 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19) Rel-20 (Release 20)* |
|  |  |
| ***Reason for change:*** | In clause 7.7, the one-to-one communication release procedures apply to the SDS one-to-one communication, FD one-to-one communication. However, there is no clue in clause 7.7 reflecting this idea. It is the same issue for the group communication.Thus, new text should be added to capture this linkage. |
|  |  |
| ***Summary of change:*** | Add new text in clause 7.7.1 to clarify the one-to-one/group communication is the ones established in clause 7.4(SDS) or 7.5(FD). |
|  |  |
| ***Consequences if not approved:*** | Ambiguous description cause incorrect implementation. |
|  |  |
| ***Clauses affected:*** | 7.7.1 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

/\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\* First changes \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

## 7.7 Communication release

### 7.7.1 General

The subclauses below describe the MCData communication release procedures, which may be initiated either by the sender or the MCData server or the authorized MCData user. The one-to-one communication in this clause refers to the SDS one-to-one communication established in clause 7.4 or the FD one-to-one communication established in clause 7.5. The group communication in this clause refers to the SDS group communication established in clause 7.4 or the FD group communication established in clause 7.5.