3GPP TSG-RAN WG2 #109-e R2-200xxxx

Electronic Meeting, 24th February – 6th March 2020

**Title:** [DRAFT] LS on Sidelink UE capability for (NG)EN-DC and NE-DC

**Response to:**

**Release:** Rel-16

**Work Item:** 5G\_V2X\_NRSL-Core

**Source:** OPPO [To be RAN WG2]

**To:** RAN4

**Cc:**

**Contact Person:**

#### Name: Qianxi Lu

E-mail Address: [qianxi.lu@oppo.com](mailto:qianxi.lu@oppo.com)

**Send any reply LS to: 3GPP Liaisons Coordinator,** [**mailto:3GPPLiaison@etsi.org**](mailto:3GPPLiaison@etsi.org)

**Attachments:** none

**1. Overall Description:**

In order to support PC5 operation controlled by MN in (NG)EN-DC and NE-DC scenario, RAN2 is discussing PC5 capability signalling design in such scenario.

RAN2 kindly ask RAN4 to feedback for the following questions:

**Question 1**: Does PC5 capability (e.g., band combination(s)) need to introduced for (NG)EN-DC and NE-DC scenario?

**Question 2**: If the answer to Question 1 is yes, for a same Uu band combination, do we need to introduce different PC5 capability (e.g., band combination(s)) for (NG)EN-DC and NE-DC scenarios respectively?

**2. Actions:**

**To RAN4 group.**

**ACTION:** RAN2 kindly ask RAN4 to feedback for Question 1 and 2 above.

**3. Date of Next TSG-RAN WG2 Meetings:**

TSG-RAN WG2 Meeting #109bis 2020-04-20 to 2020-04-24 Sapporo, Japan

TSG-RAN WG2 Meeting #110 2020-05-25 to 2020-05-29 Athens, Greece