**3GPP TSG-RAN WG3 Meeting#108-e R3-204114**

**1st – 12th June 2020**

Title: M4 measurement for EN-DC

Release: Release 16

Work Item: NR\_SON\_MDT-Core

Source: RAN3

To: RAN2

Cc:

**Contact Person:**

Name: DAPENG LI

E-mail Address: li.dapeng@zte.com.cn

**Send any reply LS to: 3GPP Liaisons Coordinator, <mailto:3GPPLiaison@etsi.org>**

Attachments: None

**1. Overall Description:**

RAN3 thanks RAN2 further progress on NR MDT in EN-DC scenario. And RAN3 achieves same agreement that M5-M7 measurements in EN-DC for SN-terminated SCG/split bearers and MN terminated SCG/split bearers are not supported in Rel-16.

In addition, RAN3 believes that M4 measurement is also not supported for MN terminated SCG/split bearer in Rel-16.

Take M4 on MN terminated SCG/split bearer for example, in case of management based MDT, there is no agreement that eNB O&M provide NR MDT configuration for NR PDCP in the MN.

**2. Actions:**

RAN3 kindly asks RAN2 to take above into account and feedback if needed.

**3. Date of Next RAN3 Meetings:**

RAN3#109-e 24-28 Aug 2020 e-meeting