3GPP TSG-RAN WG3 Meeting #114-e R3-215981

Online, 1 – 11 November 2021

**Agenda item: 21.3**

**Source: ZTE**

**Title: (TP for eIIOT BLCR for TS 38.463) Survival time remaining issues**

**Document for: Discussion and Decision**

# 1 Introduction

This E1AP TP captures the agreements from CB # NRIIOR2\_NewQoS.

# 2. TP for 38.463 on top of R3-213174

*Start of Text Proposal for TS 38.463 BL CR*

###### 9.3.1.XX Survival Time

This IE indicates the Survival Time of the TSC QoS flow as defined in TS 23.501 [20].

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| Survival Time | M |  | INTEGER (0.1920000, …) | Survival Time expressed in units of 1 us. |

*Next Change*

9.4.5 Information Element Definitions

-- S

//SKIP the unrelated part//

SDAP-Header-DL ::= ENUMERATED {

present,

absent,

...

}

SDAP-Header-UL ::= ENUMERATED {

present,

absent,

...

}

SubscriberProfileIDforRFP ::= INTEGER (1..256, ...)

SurvivalTime ::= INTEGER (0..1920000, ...)

*End of Text Proposal for TS 38.463 BL CR*