3GPP TSG-RAN WG3 Meeting #120 R3-233338

Korea, 22 – 26 May, 2023

**Agenda item: 10.2.4**

**Source: Nokia - moderator**

**Title: Summary of discussions on CB # SONMDT4\_SNPN**

**Document for: Approval**

# 1 Introduction

This paper provides summary of discussions at RAN3#120 on:

**CB: # SONMDT4\_SNPN**

**- Finalize the stage3 CRs**

**- Other open issues, if any**

(moderator - Nok)

Please provide your comments by Thursday the 25th at 18.00 Korean time.

A draft NGAP TP is uploaded based on the following agreements from online discussion:

* + **Set the range of maxnoofCAGforMDT to 256**
  + **Add separate SNPN Cell Based MDT and SNPN TAI Based MDT area scope**
  + **No need to introduce user consent of SNPN over interfaces.**

# 2 For the Chairman’s Notes

[To be completed]

# 3 Discussion

## 3.1 Open issue: Introduce SNPN wide IE?

Is it needed to introduce SNPN wide IE (choice alternative)?

|  |  |  |
| --- | --- | --- |
| Company | Answer  (yes/no) | Comment |
| Nokia | No | No need to add SNPN-wide choice alternative, but see proposals for multi-SNPN area scope in section 3.2. |
|  |  |  |
|  |  |  |

## 3.2 Other open issues

Do you see other open issues?

|  |  |
| --- | --- |
| Company | Comment |
| Nokia | We would like to remind about the following two proposals from our paper 2588:  **Proposal 3: Introduce support of multi-SNPN area scope for MDT in Rel-18.**  **Proposal 4: Incorporate the multi-SNPN area scope directly in the Area Scope configuration**  If companies can agree we will update the NGAP TP accordingly based on 2588 (with some IE name correction). |
|  |  |
|  |  |

# 4 Conclusion, Recommendations [if needed]

If needed

# 5 References

|  |  |
| --- | --- |
|  |  |
|  |  |