**3GPP TSG-RAN WG3 Meeting #125-bis R3-245718**

**Hefei, China, 14th Oct – 18th Oct, 2024**

Agenda Item: 11.4

Source: Lenovo (Moderator)

Title: SoD of CB # AIRAN4\_SplitArchitecture

Document for: Approval

# 1 Introduction

**CB: # AIRAN4\_SplitArchitecture**

**- Check the open issues above and capture agreements if any**

(moderator - Lenovo)

Summary of offline disc [R3-245718](Inbox\R3-245718.zip)

# 2 Summary for chairman notes

**Introducing Data Collection Reporting Initiation and Data Collection Reporting procedures over F1 interface to transfer measured EC from DU to CU**

# 3 Discussion

**How to transfer measured EC from DU to CU? Reusing Resource Status procedure or Introducing Data Collection Report Initiation procedure?**

CATT, HW, ZTE, Nok, QC, TI, Jio: Prefer to introduce Data Collection Report Initiation procedure

E///, NEC: Reusing the existing Resource Status procedure

**Introducing Data Collection Reporting Initiation and Data Collection Reporting procedures over F1 interface to transfer measured EC from DU to CU**