3GPP TSG-RAN WG3 Meeting #127bis R3-25xxxx

Wuhan, China, 07th – 11th May 2025

**Title:** (TP for 38.420) Inter-CU LTM

**Source:** ZTE Corporation

Agenda item: 13.2

**Document for:** Discussion and Decision

# Introduction

This TP is to include a new XnAP procedure

# TP to 38.420

===============================Start of the change====================================

### 6.2.xx L1/L2 Triggered Mobility procedures

The following procedures are used to support the L1/L2 Triggered Mobility:

- Handover Preparation

- LTM Configuration Update

- Cell Switch Notification

- TA Information Transfer

- LTM Cancel

- CSI-RS Coordination

===============================End of the change====================================