**3GPP T****SG-RAN WG3 Meeting #127bis R3-252428**

**Wuhan, China, 7th – 11th April 2025**

**Agenda item:** 19.2

**Source:** CATT

**Title:** (TP to BL CR for 38.470) introduction of Evolution of NR duplex operation: Sub-band full duplex (SBFD)

**Document for:** Agreement

# Introduction

This paper reflects the agreements achieved in RAN3#127bis.

# TP to TS38.470

<<<< Start of change >>>

5.2 F1-C functions

<<<Unchanged part omitted>>>

5.2.x CLI mitigation function

The CLI mitigation function enables the transfer of CLI measurements and CLI mitigation request between gNB-DU and gNB-CU.

<<<Next change>>>

## 6.1 Control plane procedures

<<<Unchanged part omitted>>>

6.1. x CLI mitigation function

The following procedures are used to report the result of CLI measurements and to request the CLI mitigation:

- CLI MEASUREMENT UPDATE

<<<< End of change >>>