**3GPP TSG-RAN WG4 Meeting #104-e R4-2212439**

**Electronic Meeting, 15-26 August 2022**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.2* | | | | | | | | |
| **DRAFT CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **38.101-1** | **CR** |  | **rev** |  | **Current version:** | **17.6.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network |  | Core Network |  |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | draft CR to add CA\_n25A-n66(2A)-n77(2A) and CA\_n25(2A)-n66A-n77(2A) configurations for BCS 4 and 5 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Ericsson, T-Mobile US | | | | | | | | | |
| ***Source to TSG:*** | R4 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | NR\_CADC\_R18\_3BDL\_xBUL | | | | |  | ***Date:*** | | | 2022-08-15 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | B |  | | | | | ***Release:*** | | | Rel-18 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18)*  *Rel-19 (Release 19)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | Adding CA\_n25A-n66(2A)-n77(2A) and CA\_n25(2A)-n66A-n77(2A) configurations for BCS 4 and 5 | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | CA\_n25A-n66(2A)-n77(2A) and CA\_n25(2A)-n66A-n77(2A) configurations for BCS 4 and 5 are added | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | CA\_n25A-n66(2A)-n77(2A) and CA\_n25(2A)-n66A-n77(2A) configurations for BCS 4 and 5 don’t exist in the specification | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 5.5A.3.2 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

---Start of changes---

#### 5.5A.3.2 Configurations for inter-band CA (three bands)

Table 5.5A.3.2-1: NR CA configurations and bandwidth combinations sets defined for inter-band CA (three bands)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **NR CA configuration** | **Uplink CA configuration**  **or single uplink carrier6** | **NR Band** | **Channel bandwidth (MHz) (NOTE 3)** | **Bandwidth combination set** |
| CA\_n1A-n3A-n5A | CA\_n1A-n3A  CA\_n1A-n5A  CA\_n3A-n5A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n5 | 5, 10, 15, 20 |  |
| CA\_n1A-n3A-n7A | - | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  | CA\_n1A-n3A  CA\_n1A-n7A  CA\_n3A-n7A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 1 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n1 | 5, 10, 15, 20 | 2 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
| CA\_n1A-n3A-n7B | - | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  | CA\_n1A-n3A  CA\_n1A-n7A  CA\_n3A-n7A  CA\_n7B | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 1 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n7 | CA\_n7B\_BCS0 |  |
| CA\_n1A-n3(2A)-n7A | - | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n3 | CA\_n3(2A)\_BCS1 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
| CA\_n1(2A)-n3A-n7A | - | n1 | CA\_n1(2A)\_BCS0 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
| CA\_n1(2A)-n3B-n7A | - | n1 | CA\_n1(2A)\_BCS0 | 0 |
|  |  | n3 | CA\_n3B\_BCS0 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
| CA\_n1(2A)-n3(2A)-n7A | - | n1 | CA\_n1(2A)\_BCS0 | 0 |
|  |  | n3 | CA\_n3(2A)\_BCS1 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
| CA\_n1A-n3A-n8A | - | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n8 | 5, 10, 15, 20 |  |
| CA\_n1A-n3A-n18A | CA\_n1A-n3A  CA\_n1A-n18A  CA\_n3A-n18A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n18 | 5, 10, 15 |  |
| CA\_n1A-n3A-n20A | CA\_n1A-n3A CA\_n1A-n20A CA\_n3A-n20A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n20 | 5, 10, 15, 20 |  |
| CA\_n1A-n3A-n28A | - | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n28 | 5, 10, 15, 202 |  |
|  | CA\_n1A-n3A  CA\_n1A-n28A  CA\_n3A-n28A | n1 | 5, 10, 15, 20 | 1 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 2 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n28 | 5, 10, 15, 201, 301 |  |
| CA\_n1A-n3A-n41A | CA\_n1A-n3A  CA\_n1A-n41A  CA\_n3A-n41A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
| CA\_n1A-n3A-n67A | CA\_n1A-n3A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n67 | 5, 10, 15, 20 |  |
| CA\_n1A-n3A-n77A | CA\_n1A-n3A  CA\_n1A-n77A  CA\_n3A-n77A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n77 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 1 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
| CA\_n1A-n3A-n77(2A) | CA\_n1A-n3A  CA\_n1A-n77A  CA\_n3A-n77A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n1A-n3A-n78A | CA\_n1A-n3A  CA\_n1A-n78A7  CA\_n3A-n78A7 | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n78 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 1 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n1 | 5, 10, 15, 20 | 2 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n3A-n78(2A) | CA\_n1A-n3A  CA\_n1A-n78A  CA\_n3A-n78A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n1A-n3A-n79A | CA\_n1A-n3A  CA\_n1A-n79A  CA\_n3A-n79A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n1A-n5A-n7A | CA\_n1A-n5A  CA\_n1A-n7A  CA\_n5A-n7A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
| CA\_n1A-n5A-n7B | CA\_n1A-n5A  CA\_n1A-n7A  CA\_n5A-n7A  CA\_n7B | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n7 | CA\_n7B\_BCS0 |  |
| CA\_n1A-n5A-n28A | - | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | 28 | 5, 10, 15, 20, 30 |  |
| CA\_n1A-n5A-n78A | CA\_n1A-n5A  CA\_n1A-n78A  CA\_n5A-n78A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 704, 80, 90, 100 |  |
| CA\_n1A-n7A-n8A | CA\_n1A-n7A  CA\_n1A-n8A  CA\_n7A-n8A | n1 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n8 | 5, 10, 15, 20 |  |
| CA\_n1A-n7A-n40A | CA\_n1A-n7A  CA\_n1A-n40A  CA\_n7A-n40A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80 |  |
| CA\_n1A-n7A-n79A | - | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n1A-n7A-n79C | - | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n79 | CA\_n79C\_BCS0 |  |
| CA\_n1(2A)-n7A-n79A | - | n1 | CA\_n1(2A)\_BCS0 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n1(2A)-n7A-n79C | - | n1 | CA\_n1(2A)\_BCS0 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n79 | CA\_n79C\_BCS0 |  |
| CA\_n1A-n8A-n28A | - | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n28 | 10, 15, 20 |  |
| CA\_n1A-n8A-n40A | CA\_n1A-n8A  CA\_n1A-n40A  CA\_n8A-n40A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80 |  |
| CA\_n1A-n8A-n77A | - | n1 | 5, 10, 15, 20 | 0 |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n77 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
| CA\_n1A-n8A-n77(2A) | - | n1 | 5, 10, 15, 20 | 0 |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n1A-n7A-n28A | CA\_n1A-n7A  CA\_n1A-n28A  CA\_n7A-n28A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n28 | 5, 10, 15, 20 |  |
| CA\_n1A-n7B-n28A | CA\_n1A-n28A  CA\_n1A-n7A  CA\_n7A-n28A  CA\_n7B | n1 | 5, 10, 15, 20 | 0 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n28 | 5, 10, 15, 20 |  |
| CA\_n1A-n7A-n78A | CA\_n1A-n7A  CA\_n1A-n78A  CA\_n7A-n78A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n78 | 10, 15, 20, 40, 50, 60, 80, 901,100 |  |
|  |  | n1 | 5, 10, 15, 20 | 1 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 901, 100 |  |
| CA\_n1A-n7B-n78A | CA\_n1A-n78A  CA\_n1A-n7A  CA\_n7A-n78A  CA\_n7B | n1 | 5, 10, 15, 20 | 0 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 704, 80, 90, 100 |  |
| CA\_n1A-n7A-n78(2A) | CA\_n1A-n7A  CA\_n1A-n78A  CA\_n7A-n78A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
|  |  | n1 | 5, 10, 15, 20 | 1 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n1A-n8A-n78A | CA\_n1A-n8A  CA\_n1A-n78A  CA\_n8A-n78A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  | - | n1 | 5, 10, 15, 20 | 1 |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 80, 90, 100 |  |
| CA\_n1A-n8A-n78(2A) | - | n1 | 5, 10, 15, 20 | 0 |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78(2A)\_BCS1 |  |
| CA\_n1A-n8A-n79A | - | n1 | 5, 10, 15, 20 | 0 |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n1A-n18A-n28A | CA\_n1A-n18A  CA\_n1A-n28A  CA\_n18A-n28A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n18 | 5, 10, 15 |  |
|  |  | n28 | 5, 10 |  |
| CA\_n1A-n18A-n41A | CA\_n1A-n18A  CA\_n1A-n41A  CA\_n18A-n41A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n18 | 5, 10, 15 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
| CA\_n1A-n18A-n77A | CA\_n1A-n18A  CA\_n1A-n77A  CA\_n18A-n77A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n18 | 5, 10, 15 |  |
|  |  | n77 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
| CA\_n1A-n18A-n77(2A) | CA\_n1A-n18A  CA\_n1A-n77A  CA\_n18A-n77A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n18 | 5, 10, 15 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n1A-n20A-n67A | CA\_n1A-n20A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n20 | 5, 10, 15, 20 |  |
|  |  | n67 | 5, 10, 15, 20 |  |
| CA\_n1A-n20A-n78A | - | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n20 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n28A-n38A | - | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n28 | 5, 10, 15, 20, 30 |  |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n1A-n28A-n40A | - | n1 | 5, 10, 15, 20 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80 |  |
| CA\_n1A-n28A-n40B | - | n1 | 5, 10, 15, 20 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n40 | CA\_n40B\_BCS0 |  |
| CA\_n1A-n28A-n41A | CA\_n1A-n28A  CA\_n1A-n41A  CA\_n28A-n41A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
| CA\_n1A-n28A-n77A | CA\_n1A-n28A  CA\_n1A-n77A  CA\_n28A-n77A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n77 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
| CA\_n1A-n28A-n77(2A) | CA\_n1A-n28A CA\_n1A-n77A  CA\_n28A-n77A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n77 | CA\_n77(2A)\_BCS0 |  |
|  |  | n1 | 5, 10, 15, 20 | 1 |
|  |  | n28 | 5, 10 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n1A-n28A-n78A | CA\_n1A-n28A  CA\_n1A-n78A  CA\_n28A-n78A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n28 | 5, 10, 15, 202 |  |
|  |  | n78 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n1 | 5, 10, 15, 20 | 1 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 2 |
|  |  | n28 | 5, 10, 15, 20, 30 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n28A-n78(2A) | CA\_n1A-n28A  CA\_n1A-n78A  CA\_n28A-n78A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n1A-n28A-n79A | CA\_n1A-n28A  CA\_n1A-n79A  CA\_n28A-n79A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n1A-n38A-n78A | - | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n40A-n78A | CA\_n1A-n40A  CA\_n1A-n78A  CA\_n40A-n78A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n78 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  | CA\_n1A-n40A  CA\_n1A-n78A  CA\_n40A-n78A | n1 | 5, 10, 15, 20 | 1 |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80 |  |
|  |  | n78 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  | CA\_n1A-n40A  CA\_n1A-n78A  CA\_n40A-n78A | n1 | 5, 10, 15, 20 | 2 |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n40B-n78A | - | n1 | 5, 10, 15, 20 | 0 |
|  |  | n40 | CA\_n40B\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
| CA\_n1A-n41A-n77A | CA\_n1A-n41A  CA\_n1A-n77A  CA\_n41A-n77A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n77 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
| CA\_n1A-n41A-n77(2A) | CA\_n1A-n41A  CA\_n1A-n77A  CA\_n41A-n77A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n1A-n77A-n79A4 | CA\_n1A-n77A  CA\_n1A-n79A  CA\_n77A-n79A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n77 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n1A-n77(2A)-n79A4 | CA\_n1A-n77A  CA\_n1A-n79A  CA\_n77A-n79A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n77 | CA\_n77(2A)\_BCS0 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n1A-n78A-n79A5 | CA\_n1A-n78A  CA\_n1A-n79A  CA\_n78A-n79A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n78 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
|  |  | n1 | 5, 10, 15, 20 | 1 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n1A-n78(2A)-n79A | - | n1 | 5, 10, 15, 20 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS1 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n2A-n5A-n30A | CA\_n2A-n5A  CA\_n2A-n30A  CA\_n5A-n30A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n30 | 5, 10 |  |
| CA\_n2A-n5A-n48A | CA\_n2A-n5A  CA\_n2A-n48A  CA\_n5A-n48A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2A-n5A-n48B | CA\_n2A-n5A  CA\_n2A-n48A  CA\_n5A-n48A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n48 | CA\_n48B\_BCS0 |  |
|  |  | n2 | 5, 10, 15, 20 | 1 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n48 | CA\_n48B\_BCS1 |  |
|  |  | n2 | 5, 10, 15, 20 | 2 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n48 | CA\_n48B\_BCS2 |  |
| CA\_n2A-n5A-n48(2A) | CA\_n2A-n5A  CA\_n2A-n48A  CA\_n5A-n48A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n2 | 5, 10, 15, 20 | 1 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n48 | CA\_n48(2A)\_BCS1 |  |
| CA\_n2A-n5A-n48(A-B) | CA\_n2A-n5A  CA\_n2A-n48A  CA\_n5A-n48A | n2 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n5 | 5, 10, 15, 20, 251 |  |
|  |  | n48 | CA\_n48(A-B)\_BCS0 |  |
|  |  | n2 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n5 | 5, 10, 15, 20, 251 |  |
|  |  | n48 | CA\_n48(A-B)\_BCS1 |  |
| CA\_n2(2A)-n5A-n30A | CA\_n2A-n5A  CA\_n2A-n30A  CA\_n5A-n30A | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n30 | 5, 10 |  |
| CA\_n2A-n5A-n66A | CA\_n2A-n5A  CA\_n2A-n66A  CA\_n5A-n66A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n2(2A)-n5A-n66A | CA\_n2A-n5A  CA\_n2A-n66A  CA\_n5A-n66A | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n2(2A)-n5A-n66(2A) | CA\_n2A-n5A  CA\_n2A-n66A  CA\_n5A-n66A | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
| CA\_n2A-n5A-n66(2A) | CA\_n2A-n5A  CA\_n2A-n66A  CA\_n5A-n66A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n66 | CA\_n66(2A)\_BCS0 |  |
| CA\_n2A-n5A-n66(3A) | CA\_n2A-n5A  CA\_n2A-n66A  CA\_n5A-n66A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n66 | CA\_n66(3A)\_BCS0 |  |
| CA\_n2A-n5A-n77A | n777, 9  CA\_n2A-n5A  CA\_n2A-n77A7  CA\_n5A-n77A7 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2A-n5A-n77C | CA\_n2A-n5A  CA\_n2A-n77A  CA\_n5A-n77A | n2 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n5 | 5, 10, 15, 20, 251 |  |
|  |  | n77 | CA\_n77C\_BCS0 |  |
|  |  | n2 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n5 | 5, 10, 15, 20, 251 |  |
|  |  | n77 | CA\_n77C\_BCS1 |  |
| CA\_n2A-n5A-n77(2A) | n777  CA\_n2A-n5A  CA\_n2A-n77A7  CA\_n5A-n77A7 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n2(2A)-n5A-n77A | n777  CA\_n2A-n5A  CA\_n2A-n77A7  CA\_n5A-n77A7 | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2A-n12A-n30A | CA\_n2A-n12A  CA\_n2A-n30A  CA\_n12A-n30A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n12 | 5, 10, 15 |  |
|  |  | n30 | 5, 10 |  |
| CA\_n2(2A)-n12A-n30A | CA\_n2A-n12A  CA\_n2A-n30A  CA\_n12A-n30A | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n12 | 5, 10, 15 |  |
|  |  | n30 | 5, 10 |  |
| CA\_n2A-n12A-n66A | CA\_n2A-n12A  CA\_n2A-n66A  CA\_n12A-n66A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n12 | 5, 10, 15 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n2(2A)-n12A-n66A | CA\_n2A-n12A  CA\_n2A-n66A  CA\_n12A-n66A | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n12 | 5, 10, 15 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n2A-n12A-n66(2A) | CA\_n2A-n12A  CA\_n2A-n66A  CA\_n12A-n66A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n12 | 5, 10, 15 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
| CA\_n2(2A)-n12A-n66(2A) | CA\_n2A-n12A  CA\_n2A-n66A  CA\_n12A-n66A | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n12 | 5, 10, 15 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
| CA\_n2A-n12A-n66(3A) | CA\_n2A-n12A  CA\_n2A-n66A  CA\_n12A-n66A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n12 | 5, 10, 15 |  |
|  |  | n66 | CA\_n66(3A)\_BCS0 |  |
| CA\_n2A-n12A-n77A | n777  CA\_n2A-n12A  CA\_n2A-n77A7  CA\_n12A-n77A7 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n12 | 5, 10, 15 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2(2A)-n12A-n77A | n777  CA\_n2A-n12A  CA\_n2A-n77A7  CA\_n12A-n77A7 | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n12 | 5, 10, 15 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2A-n12A-n77(2A) | n777  CA\_n2A-n12A  CA\_n2A-n77A7  CA\_n12A-n77A7 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n12 | 5, 10, 15 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n2A-n14A-n30A | CA\_n2A-n14A  CA\_n2A-n30A  CA\_n14A-n30A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n14 | 5, 10 |  |
|  |  | n30 | 5, 10 |  |
| CA\_n2(2A)-n14A-n30A | CA\_n2A-n14A  CA\_n2A-n30A  CA\_n14A-n30A | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n14 | 5, 10 |  |
|  |  | n30 | 5, 10 |  |
| CA\_n2A-n14A-n66A | CA\_n2A-n14A  CA\_n2A-n66A  CA\_n14A-n66A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n14 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n2(2A)-n14A-n66A | CA\_n2A-n14A  CA\_n2A-n66A  CA\_n14A-n66A | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n14 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n2(2A)-n14A-n66(2A) | CA\_n2A-n14A  CA\_n2A-n66A  CA\_n14A-n66A | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n14 | 5, 10 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
| CA\_n2A-n14A-n66(2A) | CA\_n2A-n14A  CA\_n2A-n66A  CA\_n14A-n66A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n14 | 5, 10 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
| CA\_n2A-n14A-n66(3A) | CA\_n2A-n14A  CA\_n2A-n66A  CA\_n14A-n66A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n14 | 5, 10 |  |
|  |  | n66 | CA\_n66(3A)\_BCS0 |  |
| CA\_n2A-n14A-n77A | n777  CA\_n2A-n14A  CA\_n2A-n77A7  CA\_n14A-n77A7 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n14 | 5, 10 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2A-n14A-n77(2A) | n777  CA\_n2A-n14A CA\_n2A-n77A7 CA\_n14A-n77A7 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n14 | 5, 10 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n2(2A)-n14A-n77A | n777  CA\_n2A-n14A CA\_n2A-n77A7 CA\_n14A-n77A7 | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n14 | 5, 10 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2A-n29A-n30A | CA\_n2A-n30A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n29 | 5, 10 |  |
|  |  | n30 | 5, 10 |  |
| CA\_n2(2A)-n29A-n30A | CA\_n2A-n30A | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n29 | 5, 10 |  |
|  |  | n30 | 5, 10 |  |
| CA\_n2A-n29A-n66A | CA\_n2A-n66A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n29 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n2(2A)-n29A-n66A | CA\_n2A-n66A | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n29 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n2A-n29A-n66(2A) | CA\_n2A-n66A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n29 | 5, 10 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
| CA\_n2(2A)-n29A-n66(2A) | CA\_n2A-n66A | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n29 | 5, 10 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
| CA\_n2A-n29A-n77A | n777  CA\_n2A-n77A7 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n29 | 5, 10 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2(2A)-n29A-n77A | n777  CA\_n2A-n77A7 | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n29 | 5, 10 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2A-n29A-n77(2A) | n777  CA\_n2A-n77A7 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n29 | 5, 10 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n2A-n30A-n66A | CA\_n2A-n30A  CA\_n30A-n66A  CA\_n2A-n66A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 40 |  |
| CA\_n2(2A)-n30A-n66A | CA\_n2A-n30A  CA\_n30A-n66A  CA\_n2A-n66A | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 40 |  |
| CA\_n2(2A)-n30A-n66(2A) | CA\_n2A-n30A  CA\_n30A-n66A  CA\_n2A-n66A | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
| CA\_n2A-n30A-n66(2A) | CA\_n2A-n30A  CA\_n30A-n66A  CA\_n2A-n66A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | CA\_n66(2A)\_BCS0 |  |
| CA\_n2A-n30A-n66(3A) | CA\_n2A-n30A  CA\_n30A-n66A  CA\_n2A-n66A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | CA\_n66(3A)\_BCS0 |  |
| CA\_n2A-n30A-n77A | n777  CA\_n2A-n30A  CA\_n2A-n77A7  CA\_n30A-n77A7 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2A-n30A-n77(2A) | n777  CA\_n2A-n30A CA\_n2A-n77A7 CA\_n30A-n77A7 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n2(2A)-n30A-n77A | n777  CA\_n2A-n30A CA\_n2A-n77A7 CA\_n30A-n77A7 | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2A-n48A-n66A | CA\_n2A-n48A  CA\_n2A-n66A  CA\_n48A-n66A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n2A-n48(A-B)-n66A | CA\_n2A-n48A  CA\_n2A-n66A  CA\_n48A-n66A | n2 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n48 | CA\_n48(A-B)\_BCS0 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n2 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n48 | CA\_n48(A-B)\_BCS1 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n2A-n48B-n66A | CA\_n2A-n48A  CA\_n2A-n66A  CA\_n48A-n66A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n48 | CA\_n48B\_BCS0 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n2 | 5, 10, 15, 20 | 1 |
|  |  | n48 | CA\_n48B\_BCS1 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n2 | 5, 10, 15, 20 | 2 |
|  |  | n48 | CA\_n48B\_BCS2 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n2A-n48(2A)-n66A | CA\_n2A-n48A  CA\_n2A-n66A  CA\_n48A-n66A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n2 | 5, 10, 15, 20 | 1 |
|  |  | n48 | CA\_n48(2A)\_BCS1 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n2A-n48A-n77A | n777, 9  CA\_n2A-n48A  CA\_n2A-n77A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2A-n48A-n77C | CA\_n2A-n48A  CA\_n2A-n77A  CA\_n77C | n2 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n77 | CA\_n77C\_BCS0 |  |
|  |  | n2 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n77 | CA\_n77C\_BCS1 |  |
| CA\_n2A-n48B-n77A | CA\_n2A-n48A  CA\_n2A-n77A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n48 | CA\_n48B\_BCS0 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n2 | 5, 10, 15, 20 | 1 |
|  |  | n48 | CA\_n48B\_BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n2 | 5, 10, 15, 20 | 2 |
|  |  | n48 | CA\_n48B\_BCS2 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2A-n48(2A)-n77A | CA\_n2A-n48A  CA\_n2A-n77A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n2 | 5, 10, 15, 20 | 1 |
|  |  | n48 | CA\_n48(2A)\_BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2A-n66A-n71A | - | n2 | 5, 10, 15, 20 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
| CA\_n2A-n66A-n77A | n777, 9  CA\_n2A-n66A  CA\_n66A-n77A7  CA\_n2A-n77A7 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2(2A)-n66A-n77A | n777  CA\_n2A-n66A  CA\_n66A-n77A7  CA\_n2A-n77A7 | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2A-n66(2A)-n77A | n777  CA\_n2A-n66A  CA\_n66A-n77A7  CA\_n2A-n77A7 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2A-n66A-n77C | CA\_n2A-n66A  CA\_n66A-n77A  CA\_n2A-n77A | n2 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77C\_BCS0 |  |
|  |  | n2 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77C\_BCS1 |  |
| CA\_n2A-n66A-n77(2A) | n777  CA\_n2A-n66A  CA\_n66A-n77A7  CA\_n2A-n77A7 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n2A-n66A-n78A | - | n2 | 5, 10, 15, 20 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2A-n66A-n78(2A) | - | n2 | 5, 10, 15, 20 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n2A-n71A-n78A | - | n2 | 5, 10, 15, 20 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2A-n71A-n78(2A) | - | n2 | 5, 10, 15, 20 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n3A-n5A-n7A | - | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40 |  |
|  | CA\_n3A-n5A  CA\_n3A-n7A  CA\_n5A-n7A | n3 | 5, 10, 15, 20, 25, 30, 40, 50 | 1 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
| CA\_n3A-n5A-n7B | - | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  | CA\_n3A-n5A  CA\_n3A-n7A  CA\_n5A-n7A  CA\_n7B | n3 | 5, 10, 15, 20, 25, 30, 40, 50 | 1 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n7 | CA\_n7B\_BCS0 |  |
| CA\_n3A-n5A-n28A | - | n3 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n28 | 5, 10, 15, 20, 30 |  |
| CA\_n3A-n5A-n78A | CA\_n3A-n5A  CA\_n3A-n78A  CA\_n5A-n78A | n3 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3A-n7A-n8A | - | n3 | 5, 10, 15, 20, 25, 30, 35, 40, 50 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 35, 40, 50 |  |
|  |  | n8 | 5, 10, 15, 20, 35 |  |
| CA\_n3A-n7A-n28A | - | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n28 | 5, 10, 15, 20 |  |
|  | CA\_n3A-n7A  CA\_n3A-n28A  CA\_n7A-n28A | n3 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40, 50 | 2 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n28 | 5, 10, 15, 20 |  |
| CA\_n3A-n7B-n28A | - | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n28 | 5, 10, 15, 20 |  |
|  | CA\_n3A-n7A  CA\_n3A-n28A  CA\_n7A-n28A  CA\_n7B | n3 | 5, 10, 15, 20, 25, 30, 40, 50 | 1 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n28 | 5, 10, 15, 20 |  |
| CA\_n3A-n7A-n78A | - | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 80, 90, 100 |  |
|  | CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n78A | n3 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 704, 80, 90, 100 |  |
| CA\_n3A-n7B-n78A | - | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 80, 90, 100 |  |
|  | CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n78A  CA\_n7B | n3 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 704, 80, 90, 100 |  |
| CA\_n3A-n7A-n78(2A) | CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n78A | n3 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n3A-n8A-n28A | - | n3 | 5, 10, 15, 20, 25, 30, 35, 40, 50 | 0 |
|  |  | n8 | 5, 10, 15, 20, 35 |  |
|  |  | n28 | 5, 10, 15, 20, 30 |  |
| CA\_n3A-n8A-n41A | - | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
| CA\_n3A-n8A-n77A | - | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n77 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
| CA\_n3A-n8A-n77(2A) | - | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n3A-n8A-n78A | CA\_n3A-n8A  CA\_n3A-n78A  CA\_n8A-n78A | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
| CA\_n3A-n18A-n28A | CA\_n3A-n18A  CA\_n3A-n28A  CA\_n18A-n28A | n3 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n18 | 5, 10, 15 |
|  |  | n28 | 5, 10 |
| CA\_n3A-n18A-n41A | CA\_n3A-n41A  CA\_n3A-n18A  CA\_n18A-n41A | n3 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n18 | 5, 10, 15 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |
| CA\_n3A-n28A-n41B | - | n3 | 5, 10, 15, 20 | 0 |
|  |  | n28 | 5, 10 |  |
|  |  | n41 | CA\_n41B\_BCS0 |  |
| CA\_n3A-n18A-n77A | CA\_n3A-n18A  CA\_n3A-n77A  CA\_n18A-n77A | n3 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n18 | 5, 10, 15 |
|  |  | n77 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |
| CA\_n3A-n18A-n77(2A) | CA\_n3A-n18A  CA\_n3A-n77A  CA\_n18A-n77A | n3 | 5, 10, 15, 20 | 0 |
|  |  | n18 | 5, 10, 15 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n3A-n20A-n67A | CA\_n3A-n20A | n3 | 5, 10, 15, 20, 25, 30, 40 | 0 |
| n20 | 5, 10, 15, 20 |
| n67 | 5, 10, 15, 20 |
| CA\_n3A-n20A-n78A | - | n3 | 5, 10, 15, 20, 25, 30, 40 | 0 |
| n20 | 5, 10, 15, 20 |
| n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |
| CA\_n3A-n28A-n41A | CA\_n3A-n28A  CA\_n3A-n41A  CA\_n28A-n41A | n3 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n28 | 5, 10, 15, 20, 30 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
| CA\_n3A-n28A-n41B | CA\_n3An28A  CA\_n3A-n41A  CA\_n28A-n41A | n3 | 5, 10, 15, 20 | 0 |
|  |  | n28 | 5, 10 |  |
|  |  | n41 | CA\_n41B\_BCS0 |  |
| CA\_n3A-n28A-n77A | CA\_n3A-n28A  CA\_n3A-n77A  CA\_n28A-n77A | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n77 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n28 | 5, 10, 15, 20, 30 |  |
|  |  | n77 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
| CA\_n3A-n28A-n77(2A) | CA\_n3A-n28A  CA\_n3A-n77A  CA\_n28A-n77A | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  | CA\_n77(2A) | n28 | 5, 10, 15, 20 |  |
|  |  | n77 | CA\_n77(2A)\_BCS0 |  |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n28 | 5, 10, 15, 20, 30 |  |
|  |  | n77 | CA\_n77(2A)\_BCS0 |  |
| CA\_n3A-n28A-n77(3A) | CA\_n3A-n28A  CA\_n3A-n77A  CA\_n28A-n77A | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n77 | CA\_n77(3A)\_BCS0 |  |
| CA\_n3A-n28A-n78A | CA\_n3A-n28A  CA\_n3A-n78A  CA\_n28A-n78A | n3 | 5, 10, 15, 20 | 0 |
|  |  | n28 | 5, 10, 15, 202 |  |
|  |  | n78 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n28 | 5, 10, 15, 202 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40 | 2 |
|  |  | n28 | 5, 10 |  |
|  |  | n78 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
| CA\_n3A-n28A-n78(2A) | CA\_n3A-n28A  CA\_n3A-n78A  CA\_n28A-n78A | n3 | 5, 10, 15, 20 | 0 |
|  |  | n28 | 5, 10, 15, 202 |  |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n28 | 5, 10 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40 | 2 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n3A-n28A-n79A | CA\_n3A-n28A  CA\_n3A-n79A  CA\_n28A-n79A | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n79 | 40, 50, 80, 100 |  |
| CA\_n3A-n38A-n40A | - | n3 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3A-n77A-n79A4 | CA\_n3A-n77A  CA\_n3A-n79A  CA\_n77A-n79A | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n77 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n3A-n77(2A)-n79A4 | CA\_n3A-n77A  CA\_n3A-n79A  CA\_n77A-n79A | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n77 | CA\_n77(2A)\_BCS0 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n3A-n40A-n41A | CA\_n3A-n40A  CA\_n3A-n41A  CA\_n40A-n41A | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80 |  |
|  |  | n41 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
| CA\_n3A-n41A-n77A | CA\_n3A-n41A | n3 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  | CA\_n3A-n77A | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  | CA\_n41A-n77A | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3A-n41B-n77A | CA\_n3A-n41A  CA\_n3A-n77A  CA\_n41A-n77A | n3 | 5, 10, 15, 20 | 0 |
|  |  | n41 | CA\_n41B\_BCS0 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3A-n41A-n77(2A) | CA\_n3A-n41A | n3 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  | CA\_n3A-n77A | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  | CA\_n41A-n77A | n77 | CA\_n77(2A)\_BCS0 |  |
| CA\_n3A-n41A-n77(3A) | CA\_n3A-n41A  CA\_n3A-n77A  CA\_n41A-n77A | n3 | 5, 10, 15, 20 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n77 | CA\_n77(3A)\_BCS1 |  |
| CA\_n3A-n41A-n78A | - | n3 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | CA\_n3A-n41A | n3 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  | CA\_n3A-n78A | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  | CA\_n41A-n78A | n78 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
| CA\_n3A-n41A-n78(2A) | CA\_n3A-n41A | n3 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  | CA\_n3A-n78A | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  | CA\_n41A-n78A | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n3A-n41A-n79A | - | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n41 | 10, 15, 20, 40, 50, 60, 80, 100 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
|  |  | n3 | 5, 10, 15, 20, 25, 30 | 1 |
|  |  | n41 | 10, 15, 20, 40, 50, 60, 80 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n5A-n7A-n28A | - | n5 | 5, 10, 15, 20 | 0 |
|  |  | n7 | 5, 10, 15, 25, 30, 40, 50 |  |
|  |  | n28 | 5, 10, 15, 20, 30 |  |
| CA\_n5A-n7A-n78A | CA\_n5A-n78A7  CA\_n7A-n78A7 | n5 | 5, 10, 15, 20 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | CA\_n5A-n7A  CA\_n5A-n78A  CA\_n7A-n78A | n5 | 5, 10, 15, 20 | 1 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 704, 80, 90, 100 |  |
| CA\_n5A-n7B-n78A | CA\_n5A-n78A7  CA\_n7A-n78A7 | n5 | 5, 10, 15, 20 | 0 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | CA\_n5A-n7A  CA\_n5A-n78A  CA\_n7A-n78A  CA\_n7B | n5 | 5, 10, 15, 20 | 1 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 704, 80, 90, 100 |  |
| CA\_n5A-n12A-n77A | n777  CA\_n5A-n12A  CA\_n5A-n77A7  CA\_n12A-n77A7 | n5 | 5, 10, 15, 20 | 0 |
|  |  | n12 | 5, 10, 15 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n5A-n12A-n77(2A) | n777  CA\_n5A-n12A CA\_n5A-n77A7 CA\_n12A-n77A7 | n5 | 5, 10, 15, 20 | 0 |
|  |  | n12 | 5, 10, 15 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n5A-n14A-n77A | n777  CA\_n5A-n14A  CA\_n5A-n77A7  CA\_n14A-n77A7 | n5 | 5, 10, 15, 20 | 0 |
|  |  | n14 | 5, 10 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n5A-n14A-n77(2A) | n777  CA\_n5A-n14A CA\_n5A-n77A7 CA\_n14A-n77A7 | n5 | 5, 10, 15, 20 | 0 |
|  |  | n14 | 5, 10 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n5A-n25A-n66A | CA\_n5A-n25A  CA\_n5A-n66A  CA\_n25A-n66A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n5A-n25(2A)-n66A | CA\_n5A-n25A  CA\_n5A-n66A  CA\_n25A-n66A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n5A-n25A-n66(2A) | CA\_n5A-n25A  CA\_n5A-n66A  CA\_n25A-n66A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
| CA\_n5A-n25(2A)-n66(2A) | CA\_n5A-n25A  CA\_n5A-n66A  CA\_n25A-n66A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
| CA\_n5A-n25A-n77A | CA\_n5A-n25A | n5 | 5, 10, 15, 20 | 0 |
|  | CA\_n5A-n77A | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  | CA\_n25A-n77A | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n5A-n25(2A)-n77A | CA\_n5A-n25A  CA\_n5A-n77A  CA\_n25A-n77A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n5A-n25A-n77(2A) | CA\_n5A-n25A  CA\_n5A-n77A  CA\_n25A-n77A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n5A-n25(2A)-n77(2A) | CA\_n5A-n25A  CA\_n5A-n77A  CA\_n25A-n77A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n5A-n25A-n78A | CA\_n5A-n25A  CA\_n5A-n78A  CA\_n25A-n78A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n5A-n25(2A)-n78A | CA\_n5A-n25A  CA\_n5A-n78A  CA\_n25A-n78A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n5A-n25A-n78(2A) | CA\_n5A-n25A  CA\_n5A-n78A  CA\_n25A-n78A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n5A-n25(2A)-n78(2A) | CA\_n5A-n25A  CA\_n5A-n78A  CA\_n25A-n78A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n5A-n29A-n77A | n777  CA\_n5A-n77A7 | n5 | 5, 10, 15, 20 | 0 |
|  |  | n29 | 5, 10 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n5A-n29A-n77(2A) | n777  CA\_n5A-n77A7 | n5 | 5, 10, 15, 20 | 0 |
|  |  | n29 | 5, 10 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n5A-n30A-n66A | CA\_n5A-n30A  CA\_n30A-n66A  CA\_n5A-n66A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 40 |  |
| CA\_n5A-n30A-n66(2A) | CA\_n5A-n30A  CA\_n30A-n66A  CA\_n5A-n66A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | CA\_n66(2A)\_BCS0 |  |
| CA\_n5A-n30A-n66(3A) | CA\_n5A-n30A  CA\_n30A-n66A  CA\_n5A-n66A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | CA\_n66(3A)\_BCS0 |  |
| CA\_n5A-n30A-n77A | n777  CA\_n5A-n30A  CA\_n5A-n77A7  CA\_n30A-n77A7 | n5 | 5, 10, 15, 20 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n5A-n30A-n77(2A) | n777  CA\_n5A-n30A CA\_n5A-n77A7 CA\_n30A-n77A7 | n5 | 5, 10, 15, 20 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n5A-n40A-n78A | CA\_n5A-n40A  CA\_n5A-n78A  CA\_n40A-n78A | n5 | 5, 10, 15, 20, 251 | 0 |
|  |  | n40 | 58, 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90,100 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90,100 |  |
| CA\_n5A-n48A-n66A | CA\_n5A-n48A  CA\_n5A-n66A  CA\_n48A-n66A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n5A-n48(A-B)-n66A | CA\_n5A-n48A  CA\_n5A-n66A  CA\_n48A-n66A | n5 | 5, 10, 15, 20, 251 | 0 |
|  |  | n48 | CA\_n48(A-B)\_BCS0 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n5 | 5, 10, 15, 20, 251 | 1 |
|  |  | n48 | CA\_n48(A-B)\_BCS1 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n5A-n48B-n66A | CA\_n5A-n48A  CA\_n5A-n66A  CA\_n48A-n66A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n48 | CA\_n48B\_BCS0 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n5 | 5, 10, 15, 20 | 1 |
|  |  | n48 | CA\_n48B\_BCS1 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n5 | 5, 10, 15, 20 | 2 |
|  |  | n48 | CA\_n48B\_BCS2 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n5A-n48(2A)-n66A | CA\_n5A-n48A  CA\_n5A-n66A  CA\_n48A-n66A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n5 | 5, 10, 15, 20 | 1 |
|  |  | n48 | CA\_n48(2A)\_BCS1 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n5A-n48A-n77A | n777, 9  CA\_n5A-n48A  CA\_n5A-n77A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n5A-n48A-n77C | CA\_n5A-n48A  CA\_n5A-n77A  CA\_n77C | n5 | 5, 10, 15, 20, 251 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n77 | CA\_n77C\_BCS0 |  |
|  |  | n5 | 5, 10, 15, 20, 251 | 1 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n77 | CA\_n77C\_BCS1 |  |
| CA\_n5A-n48B-n77A | CA\_n5A-n48A  CA\_n5A-n77A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n48 | CA\_n48B\_BCS0 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n5 | 5, 10, 15, 20 | 1 |
|  |  | n48 | CA\_n48B\_BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n5 | 5, 10, 15, 20 | 2 |
|  |  | n48 | CA\_n48B\_BCS2 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n5A-n48B-n77C | CA\_n5A-n48A  CA\_n5A-n77A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n48 | CA\_n48B\_BCS0 |  |
|  |  | n77 | CA\_n77C\_BCS0 |  |
|  |  | n5 | 5, 10, 15, 20 | 1 |
|  |  | n48 | CA\_n48B\_BCS0 |  |
|  |  | n77 | CA\_n77C BCS1 |  |
|  |  | n5 | 5, 10, 15, 20 | 2 |
|  |  | n48 | CA\_n48B\_BCS1 |  |
|  |  | n77 | CA\_n77C BCS0 |  |
|  |  | n5 | 5, 10, 15, 20 | 3 |
|  |  | n48 | CA\_n48B\_BCS1 |  |
|  |  | n77 | CA\_n77C BCS1 |  |
| CA\_n5A-n48(2A)-n77A | CA\_n5A-n48A  CA\_n5A-n77A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n5 | 5, 10, 15, 20 | 1 |
|  |  | n48 | CA\_n48(2A)\_BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n5A-n48(2A)-n77C | CA\_n5A-n48A  CA\_n5A-n77A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n77 | CA\_n77C\_BCS0 |  |
|  |  | n5 | 5, 10, 15, 20 | 1 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n77 | CA\_n77C\_BCS1 |  |
|  |  | n5 | 5, 10, 15, 20 | 2 |
|  |  | n48 | CA\_n48(2A)\_BCS1 |  |
|  |  | n77 | CA\_n77C\_BCS0 |  |
|  |  | n5 | 5, 10, 15, 20 | 3 |
|  |  | n48 | CA\_n48(2A)\_BCS1 |  |
|  |  | n77 | CA\_n77C\_BCS1 |  |
| CA\_n5A-n66A-n77A | n777, 9  CA\_n5A-n66A  CA\_n66A-n77A7  CA\_n5A-n77A7 | n5 | 5, 10, 15, 20 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n5A-n66(2A)-n77A | n777  CA\_n5A-n66A  CA\_n66A-n77A7  CA\_n5A-n77A7 | n5 | 5, 10, 15, 20 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n5A-n66(2A)-n77(2A) | CA\_n5A-n66A  CA\_n66A-n77A  CA\_n5A-n77A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n5A-n66A-n77C | CA\_n5A-n66A  CA\_n66A-n77A  CA\_n5A-n77A | n5 | 5, 10, 15, 20, 251 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77C\_BCS0 |  |
|  |  | n5 | 5, 10, 15, 20, 251 | 1 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77C\_BCS1 |  |
| CA\_n5A-n66A-n77(2A) | n777  CA\_n5A-n66A  CA\_n66A-n77A7  CA\_n5A-n77A7 | n5 | 5, 10, 15, 20 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n5A-n66A-n78A | CA\_n5A-n66A  CA\_n5A-n78A  CA\_n66A-n78A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n5 | 5, 10, 15, 20 | 1 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n5A-n66(2A)-n78A | CA\_n5A-n66A CA\_n5A-n78A CA\_n66A-n78A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n5A-n66A-n78(2A) | CA\_n5A-n66A CA\_n5A-n78A CA\_n66A-n78A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n5A-n66(2A)-n78(2A) | CA\_n5A-n66A CA\_n5A-n78A CA\_n66A-n78A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n7A-n8A-n28A | - | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n28 | 5, 10, 15, 20, 30 |  |
| CA\_n7A-n8A-n40A | CA\_n7A-n8A  CA\_n7A-n40A  CA\_n8A-n40A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80 |  |
| CA\_n7A-n8A-n78A | CA\_n7A-n8A  CA\_n7A-n78A  CA\_n8A-n78A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7A-n25A-n66A | CA\_n7A-n25A  CA\_n7A-n66A  CA\_n25A-n66A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n7A-n25(2A)-n66A | CA\_n7A-n25A  CA\_n7A-n66A  CA\_n25A-n66A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n7A-n25(2A)-n66(2A) | CA\_n7A-n25A  CA\_n7A-n66A  CA\_n25A-n66A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
| CA\_n7A-n25A-n66(2A) | CA\_n7A-n25A  CA\_n7A-n66A  CA\_n25A-n66A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
| CA\_n7(2A)-n25A-n66A | CA\_n7A-n25A  CA\_n7A-n66A  CA\_n25A-n66A | n7 | CA\_n7(2A)\_BCS0 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n7(2A)-n25(2A)-n66A | CA\_n7A-n25A  CA\_n7A-n66A  CA\_n25A-n66A | n7 | CA\_n7(2A)\_BCS0 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n7(2A)-n25A-n66(2A) | CA\_n7A-n25A  CA\_n7A-n66A  CA\_n25A-n66A | n7 | CA\_n7(2A)\_BCS0 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
| CA\_n7(2A)-n25(2A)-n66(2A) | CA\_n7A-n25A  CA\_n7A-n66A  CA\_n25A-n66A | n7 | CA\_n7(2A)\_BCS0 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
| CA\_n7A-n25A-n77A | CA\_n7A-n25A  CA\_n7A\_n77A  CA\_n25A-n77A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7A-n25(2A)-n77A | CA\_n7A-n25A  CA\_n7A\_n77A  CA\_n25A-n77A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7A-n25A-n77(2A) | CA\_n7A-n25A  CA\_n7A\_n77A  CA\_n25A-n77A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n7A-n25(2A)-n77(2A) | CA\_n7A-n25A  CA\_n7A\_n77A  CA\_n25A-n77A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n7(2A)-n25A-n77A | CA\_n7A-n25A  CA\_n7A\_n77A  CA\_n25A-n77A | n7 | CA\_n7(2A)\_BCS0 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7(2A)-n25(2A)-n77A | CA\_n7A-n25A  CA\_n7A\_n77A  CA\_n25A-n77A | n7 | CA\_n7(2A)\_BCS0 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7(2A)-n25A-n77(2A) | CA\_n7A-n25A  CA\_n7A\_n77A  CA\_n25A-n77A | n7 | CA\_n7(2A)\_BCS0 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n7(2A)-n25(2A)-n77(2A) | CA\_n7A-n25A  CA\_n7A\_n77A  CA\_n25A-n77A | n7 | CA\_n7(2A)\_BCS0 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n7A-n25A-n78A | CA\_n7A-n25A  CA\_n7A-n78A  CA\_n25A-n78A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 704, 80, 904, 100 |  |
| CA\_n7(2A)-n25A-n78A | - | n7 | CA\_n7(2A)\_BCS0 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 704, 80, 904, 100 |  |
| CA\_n7A-n25(2A)-n78A | - | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 704, 80, 904, 100 |  |
| CA\_n7(2A)-n25(2A)-n78A | - | n7 | CA\_n7(2A)\_BCS0 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 704, 80, 904, 100 |  |
| CA\_n7A-n25A-n78(2A) | CA\_n7A-n25A  CA\_n7A-n78A  CA\_n25A-n78A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 1 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n7(2A)-n25A-n78(2A) | - | n7 | CA\_n7(2A)\_BCS0 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
| CA\_n7A-n25(2A)-n78(2A) | - | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
| CA\_n7(2A)-n25(2A)-n78(2A) | - | n7 | CA\_n7(2A)\_BCS0 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
| CA\_n7A-n28A-n78(2A) | CA\_n7A-n28A  CA\_n7A-n78A  CA\_n28A-n78A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n7A-n28A-n78A | CA\_n7A-n78A7  CA\_n28A-n78A7 | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 80, 90, 100 |  |
|  | CA\_n7A-n28A  CA\_n7A-n78A  CA\_n28A-n78A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 1 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 704, 80, 90, 100 |  |
| CA\_n7B-n28A-n78A | CA\_n7A-n78A7  CA\_n28A-n78A7 | n7 | CA\_n7B\_BCS0 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 80, 90, 100 |  |
|  | CA\_n7A-n28A  CA\_n7A-n78A  CA\_n28A-n78A  CA\_n7B | n7 | CA\_n7B\_BCS0 | 1 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 704, 80, 90, 100 |  |
| CA\_n7A-n40A-n78A | CA\_n7A-n40A  CA\_n7A-n78A  CA\_n40A-n78A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n40 | 5, 10, 15, 20, 30, 40, 50, 60, 80 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7A-n46A-n78A | CA\_n7A-n46A CA\_n7A-n78A CA\_n46A-n78A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n46 | 20, 40, 60, 80 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7A-n46C-n78A | CA\_n7A-n46A CA\_n7A-n78A CA\_n46A-n78A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n46 | CA\_n46C\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7A-n46D-n78A | CA\_n7A-n46A CA\_n7A-n78A CA\_n46A-n78A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n46 | CA\_n46D\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7A-n66A-n77A | CA\_n7A-n66A  CA\_n7A-n77A  CA\_n66A-n77A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7A-n66(2A)-n77A | CA\_n7A-n66A  CA\_n7A-n77A  CA\_n66A-n77A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7A-n66A-n77(2A) | CA\_n7A-n66A CA\_n7A-n77A CA\_n66A-n77A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n7A-n66(2A)-n77(2A) | CA\_n7A-n66A CA\_n7A-n77A CA\_n66A-n77A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n7(2A)-n66A-n77A | CA\_n7A-n66A CA\_n7A-n77A CA\_n66A-n77A | n7 | CA\_n7(2A)\_BCS0 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7(2A)-n66(2A)-n77A | CA\_n7A-n66A CA\_n7A-n77A CA\_n66A-n77A | n7 | CA\_n7(2A)\_BCS0 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7(2A)-n66A-n77(2A) | CA\_n7A-n66A CA\_n7A-n77A CA\_n66A-n77A | n7 | CA\_n7(2A)\_BCS0 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n7(2A)-n66(2A)-n77(2A) | CA\_n7A-n66A CA\_n7A-n77A CA\_n66A-n77A | n7 | CA\_n7(2A)\_BCS0 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n7A-n66A-n78A | CA\_n7A-n66A  CA\_n7A-n78A  CA\_n66A-n78A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 1 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7A-n66A-n78(2A) | CA\_n7A-n66A  CA\_n7A-n78A  CA\_n66A-n78A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | CA\_n78(2A)\_BCS1 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 1 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n7(2A)-n66A-n78A | CA\_n7A-n66A  CA\_n7A-n78A  CA\_n66A-n78A | n7 | CA\_n7(2A)\_BCS0 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7A-n66(2A)-n78A | CA\_n7A-n66A  CA\_n7A-n78A  CA\_n66A-n78A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7(2A)-n66(2A)-n78A | CA\_n7A-n66A  CA\_n7A-n78A  CA\_n66A-n78A | n7 | CA\_n7(2A)\_BCS0 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7A-n66(2A)-n78(2A) | - | n7 | CA\_n7(2A)\_BCS0 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7(2A)-n66A-n78(2A) | CA\_n7A-n66A  CA\_n7A-n78A  CA\_n66A-n78A | n7 | CA\_n7(2A)\_BCS0 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n7(2A)-n66(2A)-n78(2A) | CA\_n7A-n66A  CA\_n7A-n78A  CA\_n66A-n78A | n7 | CA\_n7(2A)\_BCS0 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n8A-n28A-n78A | - | n8 | 5, 10, 15, 20 | 0 |
|  | n28 | 5, 10, 15, 20 |
|  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |
| CA\_n8A-n38A-n40A | - | n8 | 5, 10, 15, 20 | 0 |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n8A-n39A-n41A | - | n8 | 5, 10, 15, 20 | 0 |
|  |  | n39 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n41 | 10, 15, 20, 40, 50, 60, 80, 100 |  |
|  |  | n8 | 5, 10, 15, 20 | 1 |
|  |  | n39 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n41 | 10, 15, 20, 40, 50, 60 |  |
| CA\_n8A-n39A-n79A | - | n8 | 5, 10, 15, 20 | 0 |
|  |  | n39 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n8A-n40A-n41A | CA\_n8A-n40A  CA\_n8A-n41A  CA\_n40A-n41A | n8 | 5, 10, 15, 20 | 0 |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80 |  |
|  |  | n41 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
| CA\_n8A-n40A-n78A | CA\_n8A-n40A  CA\_n8A-n78A  CA\_n40A-n78A | n8 | 5, 10, 15, 20 | 0 |
|  |  | n40 | 5, 10, 15, 20, 30, 40, 50, 60, 80 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n8A-n41A-n79A | - | n8 | 5, 10, 15, 20 | 0 |
|  |  | n41 | 10, 15, 20, 40, 50, 60, 80, 100 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
|  |  | n8 | 5, 10, 15, 20 | 1 |
|  |  | n41 | 10, 15, 20, 40, 50, 60 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n8A-n78A-n79A | - | n8 | 5, 10, 15, 20 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n8A-n78(2A)-n79A | - | n8 | 5, 10, 15, 20 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS1 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n12A-n30A-n66A | CA\_n12A-n30A  CA\_n12A-n66A  CA\_n30A-n66A | n12 | 5, 10, 15 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n12A-n30A-n66(2A) | CA\_n12A-n30A  CA\_n12A-n66A  CA\_n30A-n66A | n12 | 5, 10, 15 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
| CA\_n12A-n30A-n66(3A) | CA\_n12A-n30A  CA\_n12A-n66A  CA\_n30A-n66A | n12 | 5, 10, 15 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | CA\_n66(3A)\_BCS0 |  |
| CA\_n12A-n30A-n77A | n777  CA\_n12A-n30A,  CA\_n12A-n77A7  CA\_n30A-n77A7 | n12 | 5, 10 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n12A-n30A-n77(2A) | n777  CA\_n12A-n30A CA\_n12A-n77A7 CA\_n30A-n77A7 | n12 | 5, 10 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n12A-n66A-n77A | n777  CA\_n12A-n66A  CA\_n12A-n77A7 CA\_n66A-n77A7 | n12 | 5, 10, 15 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n12A-n66(2A)-n77A | n777  CA\_n12A-n66A CA\_n12A-n77A7 CA\_n66A-n77A7 | n12 | 5, 10, 15 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n12A-n66A-n77(2A) | n777  CA\_n12A-n66A CA\_n12A-n77A7 CA\_n66A-n77A7 | n12 | 5, 10, 15 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n13A-n25A-n66A | CA\_n13A-n25A  CA\_n13A-n66A  CA\_n25A-n66A | n13 | 5, 10 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n13A-n25A-n77A | - | n13 | 5, 10 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n13A-n66A-n77A | n777, 9 | n13 | 5, 10 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n14A-n30A-n66A | CA\_n14A-n30A  CA\_n14A-n66A  CA\_n30A-n66A | n14 | 5, 10 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n14A-n30A-n66(2A) | CA\_n14A-n30A  CA\_n14A-n66A  CA\_n30A-n66A | n14 | 5, 10 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
| CA\_n14A-n30A-n66(3A) | CA\_n14A-n30A  CA\_n14A-n66A  CA\_n30A-n66A | n14 | 5, 10 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | CA\_n66(3A)\_BCS0 |  |
| CA\_n14A-n30A-n77A | n777  CA\_n14A-n30A  CA\_n14A-n77A7  CA\_n30A-n77A7 | n14 | 5, 10 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n14A-n30A-n77(2A) | n777  CA\_n14A-n30A  CA\_n14A-n77A7 CA\_n30A-n77A7 | n14 | 5, 10 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n14A-n66A-n77A | n777  CA\_n14A-n66A  CA\_n14A-n77A7  CA\_n66A-n77A7 | n14 | 5, 10 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n14A-n66(2A)-n77A | n777  CA\_n14A-n66A CA\_n14A-n77A7 CA\_n66A-n77A7 | n14 | 5, 10 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n14A-n66A-n77(2A) | n777  CA\_n14A-n66A CA\_n14A-n77A7 CA\_n66A-n77A7 | n14 | 5, 10 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n18A-n28A-n41A | CA\_n18A-n28A  CA\_n18A-n41A  CA\_n28A-n41A | n18 | 5, 10, 15 | 0 |
|  |  | n28 | 5, 10 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
| CA\_n18A-n28A-n77A | CA\_n18A-n28A  CA\_n18A-n41A  CA\_n28A-n41A | n18 | 5, 10, 15 | 0 |
|  |  | n28 | 5, 10 |  |
|  |  | n77 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
| CA\_n18A-n28A-n77(2A) | CA\_n18A-n28A  CA\_n18A-n77A  CA\_n28A-n77A | n18 | 5, 10, 15 | 0 |
|  |  | n28 | 5, 10 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n18A-n41A-n77A | CA\_n18A-n28A  CA\_n18A-n41A  CA\_n28A-n41A | n18 | 5, 10, 15 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n77 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
| CA\_n18A-n41A-n77(2A) | CA\_n18A-n41A  CA\_n18A-n77A  CA\_n41A-n77A | n18 | 5, 10, 15 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n20A-n28A-n78A | - | n20 | 5, 10, 15, 20 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
| CA\_n24A-n41A-n48A | CA\_n24A-n41A  CA\_n24A\_n48A  CA\_n41A\_n48A | n24 | 5, 10 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n48 | 5, 10, 15, 20, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n24A-n41(2A)-n48A | CA\_n24A-n41A  CA\_n24A\_n48A  CA\_n41A\_n48A | n24 | 5, 10 | 0 |
|  |  | n41 | CA\_n41(2A) BCS1 |  |
|  |  | n48 | 5, 10, 15, 20, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n24A-n41A-n48(2A) | CA\_n24A-n41A  CA\_n24A\_n48A  CA\_n41A\_n48A | n24 | 5, 10 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n48 | CA\_n48(2A) BCS0 |  |
| CA\_n24A-n41(2A)-n48(2A) | CA\_n24A-n41A  CA\_n24A\_n48A  CA\_n41A\_n48A | n24 | 5, 10 | 0 |
|  |  | n41 | CA\_n41(2A) BCS1 |  |
|  |  | n48 | CA\_n48(2A) BCS0 |  |
| CA\_n24A-n41A-n77A | CA\_n24A-n41A  CA\_n24A\_n77A  CA\_n41A\_n77A | n24 | 5, 10 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n24A-n41(2A)-n77A | CA\_n24A-n41A  CA\_n24A\_n77A  CA\_n41A\_n77A | n24 | 5, 10 | 0 |
|  |  | n41 | CA\_n41(2A)\_BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n24 | 5, 10 | 1 |
|  |  | n41 | CA\_n41(2A) BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n24A-n41A-n77(2A) | CA\_n24A-n41A  CA\_n24A\_n77A  CA\_n41A\_n77A | n24 | 5, 10 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n77 | CA\_n77(2A)\_BCS0 |  |
|  |  | n24 | 5, 10 | 1 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n77 | CA\_n77(2A) BCS0 |  |
| CA\_n24A-n41(2A)-n77(2A) | CA\_n24A-n41A  CA\_n24A\_n77A  CA\_n41A\_n77A | n24 | 5, 10 | 0 |
|  |  | n41 | CA\_n41(2A)\_BCS1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS0 |  |
|  |  | n24 | 5, 10 | 1 |
|  |  | n41 | CA\_n41(2A) BCS1 |  |
|  |  | n77 | CA\_n77(2A) BCS0 |  |
| CA\_n24A-n48A-n77A |  | n24 | 5, 10 | 0 |
|  |  | n48 | 5, 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n24A-n48(2A)-n77A |  | n24 | 5, 10 | 0 |
|  |  | n48 | CA\_n48(2A) BCS0 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n24A-n48A-n77(2A) |  | n24 | 5, 10 | 0 |
|  |  | n48 | 5, 10, 15, 20, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n77 | CA\_n77(2A) BCS0 |  |
| CA\_n24A-n48(2A)-n77(2A) |  | n24 | 5, 10 | 0 |
|  |  | n48 | CA\_n48(2A) BCS0 |  |
|  |  | n77 | CA\_n77(2A) BCS0 |  |
| CA\_n25A-n29A-n66A | CA\_n25A-n66A | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n29 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n25A-n38A-n66A | CA\_n25A-n38A  CA\_n25A-n66A  CA\_n38A-n66A | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n25(2A)-n38A-n66A | CA\_n25A-n38A  CA\_n25A-n66A  CA\_n38A-n66A | n25 | CA\_n25(2A)\_BCS0 | 0 |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n25(2A)-n38A-n66(2A) | CA\_n25A-n38A  CA\_n25A-n66A  CA\_n38A-n66A | n25 | CA\_n25(2A)\_BCS0 | 0 |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
| CA\_n25A-n38A-n66(2A) | CA\_n25A-n38A  CA\_n25A-n66A  CA\_n38A-n66A | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n38 | 5, 10, 15, 20 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
| CA\_n25A-n38A-n78A | CA\_n25A-n38A  CA\_n25A-n78A  CA\_n38A-n78A | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n25A-n38A-n78(2A) | CA\_n25A-n38A  CA\_n25A-n78A  CA\_n38A-n78A | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n25(2A)-n38A-n78A | CA\_n25A-n38A  CA\_n25A-n78A  CA\_n38A-n78A | n25 | CA\_n25(2A)\_BCS0 | 0 |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n25(2A)-n38A-n78(2A) | CA\_n25A-n38A  CA\_n25A-n78A  CA\_n38A-n78A | n25 | CA\_n25(2A)\_BCS0 | 0 |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n25A-n41A-n66A | - | n25 | 5, 10, 15, 20 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n66 | 5, 10, 15, 20, 40 |  |
|  | CA\_n25A-n41A  CA\_n25A-n66A  CA\_n41A-n66A | n25 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  | CA\_n25A-n41A  CA\_n25A-n66A  CA\_n41A-n66A | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n41A-n66(2A) | - | n25 | 5, 10, 15, 20 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  | CA\_n25A-n41A  CA\_n25A-n66A  CA\_n41A-n66A | n25 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  | CA\_n25A-n41A  CA\_n25A-n66A  CA\_n41A-n66A | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | CA\_n66(2A) BCS 4 and 5 |  |
| CA\_n25A-n41C-n66A | - | n25 | 5, 10, 15, 20 | 0 |
|  |  | n41 | CA\_n41C\_BCS0 |  |
|  |  | n66 | 5, 10, 15, 20, 40 |  |
|  | CA\_n25A-n41A  CA\_n25A-n66A  CA\_n41A-n66A | n25 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n41 | CA\_n41C\_BCS1 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  | CA\_n25A-n41A  CA\_n25A-n66A  CA\_n41A-n66A | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41C BCS 4 and 5 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n41(2A)-n66A | - | n25 | 5, 10, 15, 20 | 0 |
|  |  | n41 | CA\_n41(2A)\_BCS1 |  |
|  |  | n66 | 5, 10, 15, 20, 40 |  |
|  | CA\_n25A-n41A  CA\_n25A-n66A  CA\_n41A-n66A | n25 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n41 | CA\_n41(2A)\_BCS1 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  | CA\_n25A-n41A  CA\_n25A-n66A  CA\_n41A-n66A | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41(2A) BCS 4 and 5 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25(2A)-n41A-n66A | - | n25 | CA\_n25(2A)\_BCS1 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n66 | 5, 10, 15, 20, 40 |  |
|  | CA\_n25A-n41A  CA\_n25A-n66A  CA\_n41A-n66A | n25 | CA\_n25(2A)\_BCS1 | 1 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n66 | 5, 10, 15, 20, 30, 40 |  |
|  | CA\_n25A-n41A  CA\_n25A-n66A  CA\_n41A-n66A | n25 | CA\_n25(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n41A-n71A | - | n25 | 5, 10, 15, 20 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  | CA\_n25A-n41A | n25 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  | CA\_n41A-n71A | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | CA\_n25A-n71A | n71 | 5, 10, 15, 20 |  |
|  | CA\_n25A-n41A  CA\_n41A-n71A  CA\_n25A-n71A | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n41A-n71B | - | n25 | 5, 10, 15, 20 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n71 | CA\_n71B\_BCS2 |  |
|  | CA\_n25A-n41A  CA\_n41A-n71A  CA\_n25A-n71A | n25 | 5, 10, 15, 20, 30, 40 | 1 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n71 | CA\_n71B\_BCS2 |  |
|  | CA\_n25A-n41A  CA\_n41A-n71A  CA\_n25A-n71A | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | CA\_n71B BCS 4 and 5 |  |
| CA\_n25A-n41A-n71(2A) | - | n25 | 5, 10, 15, 20 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n71 | CA\_n71(2A)\_BCS0 |  |
|  | CA\_n25A-n41A  CA\_n41A-n71A  CA\_n25A-n71A | n25 | 5, 10, 15, 20, 30, 40 | 1 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n71 | CA\_n71(2A)\_BCS0 |  |
|  | CA\_n25A-n41A  CA\_n41A-n71A  CA\_n25A-n71A | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | CA\_n71(2A) BCS 4 and 5 |  |
| CA\_n25A-n41(2A)-n71A | - | n25 | 5, 10, 15, 20 | 0 |
|  |  | n41 | CA\_n41(2A)\_BCS1 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  | CA\_n25A-n41A  CA\_n41A-n71A  CA\_n25A-n71A | n25 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n41 | CA\_n41(2A)\_BCS1 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  | CA\_n25A-n41A  CA\_n41A-n71A  CA\_n25A-n71A | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41(2A) BCS 4 and 5 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n41C-n71A | - | n25 | 5, 10, 15, 20 | 0 |
|  |  | n41 | CA\_n41C\_BCS0 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  | CA\_n25A-n41A  CA\_n41A-n71A  CA\_n25A-n71A | n25 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n41 | CA\_n41C\_BCS1 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  | CA\_n25A-n41A  CA\_n41A-n71A  CA\_n25A-n71A  CA\_n41C | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41C BCS 4 and 5 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25(2A)-n41A-n71A | - | n25 | CA\_n25(2A)\_BCS1 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  | CA\_n25A-n41A  CA\_n41A-n71A  CA\_n25A-n71A | n25 | CA\_n25(2A)\_BCS1 | 1 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  | CA\_n25A-n41A  CA\_n41A-n71A  CA\_n25A-n71A | n25 | CA\_n25(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n41A-n77A | CA\_n25A-n41A  CA\_n25A-n77A  CA\_n41A-n77A | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | CA\_n25A-n41A  CA\_n25A-n77A  CA\_n41A-n77A | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n41(2A)-n77A | CA\_n25A-n41A  CA\_n25A-n77A  CA\_n41A-n77A | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n41 | CA\_n41(2A)\_BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n41 | CA\_n41(2A)\_BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 80, 90, 100 |  |
|  | CA\_n25A-n41A  CA\_n25A-n77A  CA\_n41A-n77A | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41(2A) BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n41A-n77(2A) | CA\_n25A-n41A  CA\_n25A-n77A  CA\_n41A-n77A | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
|  | CA\_n25A-n41A  CA\_n25A-n77A  CA\_n41A-n77A | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(2A) BCS 4 and 5 |  |
| CA\_n25A-n41(2A)-n77(2A) | CA\_n25A-n41A  CA\_n25A-n77A  CA\_n41A-n77A | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41(2A) BCS 4 and 5 |  |
|  |  | n77 | CA\_n77(2A) BCS 4 and 5 |  |
| CA\_n25(2A)-n41A-n77A | CA\_n25A-n41A  CA\_n25A-n77A  CA\_n41A-n77A | n25 | CA\_n25(2A)\_BCS1 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | CA\_n25A-n41A  CA\_n25A-n77A  CA\_n41A-n77A | n25 | CA\_n25(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n41C-n77A | CA\_n41C  CA\_n25A-n41A  CA\_n25A-n77A  CA\_n41A-n77A | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n41 | CA\_n41C\_BCS0 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n41 | CA\_n41C\_BCS2 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | CA\_n41C  CA\_n25A-n41A  CA\_n25A-n77A  CA\_n41A-n77A | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41C BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n41C-n77(2A) | CA\_n41C  CA\_n25A-n41A  CA\_n25A-n77A  CA\_n41A-n77A | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41C BCS 4 and 5 |  |
|  |  | n77 | CA\_n77(2A) BCS 4 and 5 |  |
| CA\_n25A-n41A-n78A | CA\_n25A-n41A  CA\_n25A-n78A  CA\_n41A-n78A | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n25A-n41A-n78(2A) | CA\_n25A-n41A  CA\_n25A-n78A  CA\_n41A-n78A | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n25A-n48A-n66A | CA\_n25A-n48A  CA\_n25A-n66A  CA\_n48A-n66A | n25 | 5, 10, 15, 20 | 0 |
|  |  | n48 | 5, 10, 15, 20, 40, 50 |  |
|  |  | n66 | 5, 10, 15, 20, 40 |  |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n48 | 5, 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n25A-n48(2A)-n66A | CA\_n25A-n48A  CA\_n25A-n66A  CA\_n48A-n66A | n25 | 5, 10, 15, 20 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n66 | 5, 10, 15, 20, 40 |  |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n25A-n48C-n66A | CA\_n25A-n48A  CA\_n25A-n66A  CA\_n48A-n66A | n25 | 5, 10, 15, 20 | 0 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
|  |  | n66 | 5, 10, 15, 20, 40 |  |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n25A-n66A-n71A | - | n25 | 5, 10, 15, 20 | 0 |
|  |  | n66 | 5, 10, 15, 20, 40 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  | CA\_n25A-n66A  CA\_n25A-n71A  CA\_n66A-n71A | n25 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  | CA\_n25A-n66A  CA\_n25A-n71A  CA\_n66A-n71A | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n66A-n71B | CA\_n25A-n66A  CA\_n25A-n71A  CA\_n66A-n71A | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n71 | CA\_n71B\_BCS2 |  |
|  | CA\_n25A-n66A  CA\_n25A-n71A  CA\_n66A-n71A | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | CA\_n71B BCS 4 and 5 |  |
| CA\_n25A-n66A-n71(2A) | CA\_n25A-n66A  CA\_n25A-n71A  CA\_n66A-n71A | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n71 | CA\_n71(2A)\_BCS0 |  |
|  | CA\_n25A-n66A  CA\_n25A-n71A  CA\_n66A-n71A | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | CA\_n71(2A) BCS 4 and 5 |  |
| CA\_n25A-n66(2A)-n71A | CA\_n25A-n66A  CA\_n25A-n71A  CA\_n66A-n71A | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  | CA\_n25A-n66A  CA\_n25A-n71A  CA\_n66A-n71A | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | CA\_n66(2A) BCS 4 and 5 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25(2A)-n66A-n71A | CA\_n25A-n66A  CA\_n25A-n71A  CA\_n66A-n71A | n25 | CA\_n25(2A)\_BCS1 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  | CA\_n25A-n66A  CA\_n25A-n71A  CA\_n66A-n71A | n25 | CA\_n25(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n66A-n77A | CA\_n25A-n66A  CA\_n25A-n77A  CA\_n66A-n77A | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | CA\_n25A-n66A  CA\_n25A-n77A  CA\_n66A-n77A | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n66(2A)-n77A | CA\_n25A-n66A  CA\_n25A-n77A  CA\_n66A-n77A | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | CA\_n25A-n66A  CA\_n25A-n77A  CA\_n66A-n77A | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | CA\_n66(2A) BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n66A-n77(2A) | CA\_n25A-n66A  CA\_n25A-n77A  CA\_n66A-n77A | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
|  | CA\_n25A-n66A  CA\_n25A-n77A  CA\_n66A-n77A | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(2A) BCS 4 and 5 |  |
| CA\_n25A-n66(2A)-n77(2A) | CA\_n25A-n66A  CA\_n25A-n77A  CA\_n66A-n77A | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | CA\_n66(2A) BCS 4 and 5 |  |
|  |  | n77 | CA\_n77(2A) BCS 4 and 5 |  |
| CA\_n25(2A)-n66A-n77A | CA\_n25A-n66A  CA\_n25A-n77A  CA\_n66A-n77A | n25 | CA\_n25(2A)\_BCS0 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | CA\_n25A-n66A  CA\_n25A-n77A  CA\_n66A-n77A | n25 | CA\_n25(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25(2A)-n66(2A)-n77A | CA\_n25A-n66A  CA\_n25A-n77A  CA\_n66A-n77A | n25 | CA\_n25(2A)\_BCS0 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n25(2A)-n66A-n77(2A) | CA\_n25A-n66A  CA\_n25A-n77A  CA\_n66A-n77A | n25 | CA\_n25(2A)\_BCS0 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
|  |  | n25 | CA\_n25(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(2A) BCS 4 and 5 |  |
| CA\_n25(2A)-n66(2A)-n77(2A) | CA\_n25A-n66A  CA\_n25A-n77A  CA\_n66A-n77A | n25 | CA\_n25(2A)\_BCS0 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n25A-n66A-n78A | CA\_n25A-n66A  CA\_n25A-n78A  CA\_n66A-n78A | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n25(2A)-n66A-n78A | CA\_n25A-n66A CA\_n25A-n78A CA\_n66A-n78A | n25 | CA\_n25(2A)\_BCS0 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n25A-n66(2A)-n78A | CA\_n25A-n66A CA\_n25A-n78A CA\_n66A-n78A | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n25A-n66A-n78(2A) | CA\_n25A-n66A CA\_n25A-n78A CA\_n66A-n78A | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n25(2A)-n66(2A)-n78A | CA\_n25A-n66A CA\_n25A-n78A CA\_n66A-n78A | n25 | CA\_n25(2A)\_BCS0 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n25(2A)-n66A-n78(2A) | CA\_n25A-n66A CA\_n25A-n78A CA\_n66A-n78A | n25 | CA\_n25(2A)\_BCS0 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n25A-n66(2A)-n78(2A) | CA\_n25A-n66A CA\_n25A-n78A CA\_n66A-n78A | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n25(2A)-n66(2A)-n78(2A) | CA\_n25A-n66A CA\_n25A-n78A CA\_n66A-n78A | n25 | CA\_n25(2A)\_BCS0 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n25A-n71A-n77A | CA\_n25A-n71A  CA\_n25A-n77A  CA\_n71A-n77A | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | CA\_n25A-n71A  CA\_n25A-n77A  CA\_n71A-n77A | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n71B-n77A | CA\_n25A-n71A  CA\_n25A-n77A  CA\_n71A-n77A | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n71 | CA\_n71B\_BCS2 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | CA\_n25A-n71A  CA\_n25A-n77A  CA\_n71A-n77A | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n71 | CA\_n71B BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n71(2A)-n77A | CA\_n25A-n71A  CA\_n25A-n77A  CA\_n71A-n77A | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n71 | CA\_n71(2A)\_BCS0 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | CA\_n25A-n71A  CA\_n25A-n77A  CA\_n71A-n77A | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n71 | CA\_n71(2A) BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25(2A)-n71A-n77A | CA\_n25A-n71A  CA\_n25A-n77A  CA\_n71A-n77A | n25 | CA\_n25(2A)\_BCS1 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | CA\_n25A-n71A  CA\_n25A-n77A  CA\_n71A-n77A | n25 | CA\_n25(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n71A-n78A | CA\_n25A-n71A  CA\_n25A-n78A  CA\_n71A-n78A | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n25A-n71A-n78(2A) | CA\_n25A-n71A  CA\_n25A-n78A  CA\_n71A-n78A | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n26A-n66A-n70A | CA\_n26A-n66A  CA\_n26A-n70A | n26 | 5, 10, 15, 20 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n70 | 5, 10, 15, 201, 251 |  |
| CA\_n26A-n66(2A)-n70A | CA\_n26A-n66A  CA\_n26A-n70A | n26 | 5, 10, 15, 20 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS0 |  |
|  |  | n70 | 5, 10, 15, 201, 251 |  |
| CA\_n28A-n38A-n78A | - | n28 | 5, 10, 15, 20, 30 | 0 |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n28A-n39A-n40A | - | n28 | 5, 10, 15, 20, 30 | 0 |
|  |  | n39 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80, 100 |  |
| CA\_n28A-n39A-n41A | CA\_n28A-n39A  CA\_n28A-n41A  CA\_n39A-n41A | n28 | 5, 10, 15, 20, 30 | 0 |
|  |  | n39 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n28A-n39A-n41C | CA\_n28A-n39A  CA\_n28A-n41A  CA\_n39A-n41A | n28 | 5, 10, 15, 20, 30 | 0 |
|  |  | n39 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n41 | CA\_n41C\_BCS1 |  |
| CA\_n28A-n39A-n79A | - | n28 | 5, 10, 15, 20, 30 | 0 |
|  |  | n39 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n28A-n40A-n41A | CA\_n28A-n40A  CA\_n28A-n41A  CA\_n40A-n41A | n28 | 5, 10, 15, 20, 30 | 0 |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n28A-n40A-n78A | CA\_n28A-n40A  CA\_n28A-n78A  CA\_n40A-n78A | n28 | 5, 10, 15, 20 | 0 |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n78 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  | CA\_n28A-n40A  CA\_n28A-n78A  CA\_n40A-n78A | n28 | 5, 10, 15, 20 | 1 |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80, 100 |  |
|  |  | n78 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
| CA\_n28A-n40B-n78A | - | n28 | 5, 10, 15, 20 | 0 |
|  |  | n40 | CA\_n40\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
| CA\_n28A-n40A-n79A | CA\_n28A-n40A  CA\_n28A-n79A  CA\_n40A-n79A | n28 | 5, 10, 15, 20, 30 | 0 |
|  |  | n40 | 10, 15, 20, 25, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n28A-n41A-n77A | CA\_n28A-n41A | n28 | 5, 10, 15, 20, 30 | 0 |
|  | CA\_n28A-n77A | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  | CA\_n41A-n77A | n77 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n28A-n41B-n77A | CA\_n28A-n41A  CA\_n28A-n77A  CA\_n41A-n77A | n28 | 5, 10 | 0 |
|  |  | n41 | CA\_n41B\_BCS0 |  |
|  |  | n77 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n28A-n41A-n77(2A) | CA\_n28A-n41A | n28 | 5, 10, 15, 20, 30 | 0 |
|  | CA\_n28A-n77A | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  | CA\_n41A-n77A | n77 | CA\_n77(2A)\_BCS0 |  |
| CA\_n28A-n41A-n77(3A) | CA\_n28A-n41A  CA\_n28A-n77A  CA\_n41A-n77A | n28 | 5, 10 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n77 | CA\_n77(3A)\_BCS1 |  |
| CA\_n28A-n41A-n78A | CA\_n28A-n41A  CA\_n41A-n78A  CA\_n28A-n78A | n28 | 5, 10, 15, 20 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 90, 100 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 80, 90, 100 |  |
| CA\_n28A-n41A-n78(2A) | CA\_n78(2A) | n28 | 5, 10, 15, 20, 30 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n28A-n41A-n79A | CA\_n28A-n41A  CA\_n28A-n79A  CA\_n41A-n79A | n28 | 5, 10, 15, 20, 30 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n28A-n41C-n79A | CA\_n28A-n41A  CA\_n28A-n79A  CA\_n41A-n79A | n28 | 5, 10, 15, 20, 30 | 0 |
|  |  | n41 | CA\_n41C\_BCS1 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n28A-n46A-n78A | CA\_n28A-n46A  CA\_n28A-n78A  CA\_n46A-n78A | n28 | 5, 10, 15, 20 | 0 |
|  |  | n46 | 20, 40, 60, 80 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n28A-n46C-n78A | CA\_n28A-n46A  CA\_n28A-n78A  CA\_n46A-n78A | n28 | 5, 10, 15, 20 | 0 |
|  |  | n46 | CA\_n46C\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n28A-n46D-n78A | CA\_n28A-n46A  CA\_n28A-n78A  CA\_n46A-n78A | n28 | 5, 10, 15, 20 | 0 |
|  |  | n46 | CA\_n46D\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n28A-n77A-n79A4 | CA\_n28A-n77A  CA\_n28A-n79A  CA\_n77A-n79A | n28 | 5, 10, 15, 20 | 0 |
|  |  | n77 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n28A-n77(2A)-n79A4 | CA\_n28A-n77A  CA\_n28A-n79A  CA\_n77A-n79A | n28 | 5, 10, 15, 20 | 0 |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n28A-n78A-n79A | CA\_n28A-n78A  CA\_n28A-n79A  CA\_n78A-n79A | n28 | 5, 10, 15, 20 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n29A-n30A-n66A | CA\_n30A-n66A | n29 | 5, 10 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n29A-n30A-n66(2A) | CA\_n30A-n66A | n29 | 5, 10 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
| CA\_n29A-n30A-n77A | n777  CA\_n30A-n77A7 | n29 | 5, 10 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n29A-n30A-n77(2A) | n777  CA\_n30A-n77A7 | n29 | 5, 10 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n29A-n66A-n70A | - | n29 | 5, 10 | 0 |
|  |  | n66 | 5, 10, 15, 20, 40 |  |
|  |  | n70 | 5, 10, 15, 201,251 |  |
| CA\_n29A-n66B-n70A | - | n29 | 5, 10 | 0 |
|  |  | n66 | CA\_n66B\_BCS0. |  |
|  |  | n70 | 5, 10, 15, 201,251 |  |
| CA\_n29A-n66(2A)-n70A | - | n29 | 5, 10 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS0 |  |
|  |  | n70 | 5, 10, 15, 201,251 |  |
| CA\_n29A-n66A-n77A | n777  CA\_n66A-n77A7 | n29 | 5, 10 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n29A-n66(2A)-n77A | n777  CA\_n66A-n77A7 | n29 | 5, 10 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n29A-n66A-n77(2A) | n777  CA\_n66A-n77A7 | n29 | 5, 10 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n30A-n66A-n77A | n777  CA\_n30A-n66A  CA\_n30A-n77A7  CA\_n66A-n77A7 | n30 | 5, 10 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n30A-n66(2A)-n77A | n777  CA\_n30A-n66A CA\_n30A-n77A7 CA\_n66A-n77A7 | n30 | 5, 10 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n30A-n66A-n77(2A) | n777  CA\_n30A-n66A CA\_n30A-n77A7 CA\_n66A-n77A7 | n30 | 5, 10 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n38A-n66A-n78A | CA\_n38A-n66A  CA\_n38A-n78A  CA\_n66A-n78A | n38 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n38A-n66A-n78(2A) | CA\_n38A-n66A  CA\_n38A-n78A  CA\_n66A-n78A | n38 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n38A-n66(2A)-n78A | CA\_n38A-n66A  CA\_n38A-n78A  CA\_n66A-n78A | n38 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n38A-n66(2A)-n78(2A) | CA\_n38A-n66A  CA\_n38A-n78A  CA\_n66A-n78A | n38 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n39A-n40A-n41A | CA\_n39A-n40A  CA\_n39A-n41A  CA\_n40A-n41A | n39 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80 |  |
|  |  | n41 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
| CA\_n39A-n40A-n79A | CA\_n39A-n40A  CA\_n40A-n79A  CA\_n39A-n79A | n39 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n39A-n41A-n79A | - | n39 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n41 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
|  |  | n39 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n41 | 10, 15, 20, 40, 50, 60 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n40A-n41A-n79A | CA\_n40A-n41A  CA\_n40A-n79A  CA\_n41A-n79A | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80 | 0 |
|  |  | n41 | 10, 15, 20, 40, 50, 60, 80, 100 |  |
|  |  | n79 | , 40, 50, 60, 80, 100 |  |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n41 | 10, 15, 20, 40, 50, 60 |  |
|  |  | n79 | , 40, 50, 60, 80, 100 |  |
| CA\_n41A-n66A-n70A | CA\_n41A-n66A  CA\_n41A-n70A | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n66 | 10, 15, 20, 25, 30, 40 |  |
|  |  | n70 | 5, 10, 15, 201, 251 |  |
| CA\_n41A-n66A-n71A | - | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 | 0 |
|  |  | n66 | 5, 10, 15, 20, 40 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  | CA\_n41A-n71A  CA\_n66A-n71A  CA\_n41A-n66A | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 1 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  | CA\_n41A-n71A  CA\_n66A-n71A  CA\_n41A-n66A | n41 | n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41A-n66A-n71B | CA\_n41A-n66A  CA\_n41A-n71A  CA\_n66A-n71A | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n71 | CA\_n71B\_BCS2 |  |
|  | CA\_n41A-n66A  CA\_n41A-n71A  CA\_n66A-n71A | n41 | n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | CA\_n71B BCS 4 and 5 |  |
| CA\_n41A-n66A-n71(2A) | CA\_n41A-n66A  CA\_n41A-n71A  CA\_n66A-n71A | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n71(2A)\_BCS0 |  |
|  | CA\_n41A-n66A  CA\_n41A-n71A  CA\_n66A-n71A | n41 | n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | CA\_n71(2A) BCS 4 and 5 |  |
| CA\_n41A-n66(2A)-n71A | CA\_n41A-n66A  CA\_n66A-n71A  CA\_n41A-n71A | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  | CA\_n41A-n66A  CA\_n66A-n71A  CA\_n41A-n71A | n41 | n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | CA\_n66(2A) BCS 4 and 5 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41(2A)-n66A-n71A | - | n41 | CA\_n41(2A)\_BCS1 | 0 |
|  |  | n66 | 5, 10, 15, 20, 40 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  | CA\_n41A-n71A  CA\_n66A-n71A  CA\_n41A-n66A | n41 | CA\_n41(2A)\_BCS1 | 1 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  | CA\_n41A-n71A  CA\_n66A-n71A  CA\_n41A-n66A | n41 | CA\_n41(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41C-n66A-n71A | - | n41 | CA\_n41C\_BCS0 | 0 |
|  |  | n66 | 5, 10, 15, 20, 40 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  | CA\_n41A-n71A  CA\_n66A-n71A  CA\_n41A-n66A | n41 | CA\_n41C\_BCS1 | 1 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  | CA\_n41A-n71A  CA\_n66A-n71A  CA\_n41A-n66A  CA\_n41C | n41 | CA\_n41C BCS 4 and 5 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41A-n66A-n77A | CA\_n41A-n66A  CA\_n41A-n77A  CA\_n66A-n77A | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 1 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | CA\_n41A-n66A  CA\_n41A-n77A  CA\_n66A-n77A | n41 | n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41A-n66A-n77(2A) | CA\_n41A-n77A  CA\_n66A-n77A  CA\_n41A-n66A | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
|  | CA\_n41A-n77A  CA\_n66A-n77A  CA\_n41A-n66A | n41 | n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(2A) BCS 4 and 5 |  |
| CA\_n41A-n66(2A)-n77A | CA\_n41A-n66A  CA\_n41A-n77A  CA\_n66A-n77A | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | CA\_n41A-n66A  CA\_n41A-n77A  CA\_n66A-n77A | n41 | n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | CA\_n66(2A) BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41A-n66(2A)-n77(2A) | CA\_n41A-n66A  CA\_n41A-n77A  CA\_n66A-n77A | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
|  | CA\_n41A-n66A  CA\_n41A-n77A  CA\_n66A-n77A | n41 | n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | CA\_n66(2A) BCS 4 and 5 |  |
|  |  | n77 | CA\_n77(2A) BCS 4 and 5 |  |
| CA\_n41(2A)-n66A-n77A | CA\_n41A-n66A  CA\_n41A-n77A  CA\_n66A-n77A | n41 | CA\_n41(2A)\_BCS1 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | CA\_n41A-n66A  CA\_n41A-n77A  CA\_n66A-n77A | n41 | CA\_n41(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41(2A)-n66A-n77(2A) | CA\_n41A-n66A  CA\_n41A-n77A  CA\_n66A-n77A | n41 | CA\_n41(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(2A) BCS 4 and 5 |  |
| CA\_n41C-n66A-n77A | CA\_41C  CA\_n41A-n66A  CA\_n41A-n77A  CA\_n66A-n77A | n41 | CA\_n41C\_BCS0 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | CA\_41C  CA\_n41A-n66A  CA\_n41A-n77A  CA\_n66A-n77A | n41 | CA\_n41C BCS 4 and 5 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41C-n66A-n77(2A) | CA\_41C  CA\_n41A-n66A  CA\_n41A-n77A  CA\_n66A-n77A | n41 | CA\_n41C BCS 4 and 5 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(2A) BCS 4 and 5 |  |
| CA\_n41A-n66A-n78A | CA\_n41A-n66A  CA\_n41A-n78A  CA\_n66A-n78A | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n41A-n66A-n78(2A) | CA\_n41A-n66A  CA\_n41A-n78A  CA\_n66A-n78A | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n41A-n66(2A)-n78A | CA\_n41A-n66A  CA\_n41A-n78A  CA\_n66A-n78A | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n41A-n66(2A)-n78(2A) | CA\_n41A-n66A  CA\_n41A-n78A  CA\_n66A-n78A | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n41A-n70A-n78A | CA\_n41A-n70A  CA\_n41A-n78A  CA\_n70A-n78A | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n70 | 5, 10, 15, 20, 25 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n41A-n71A-n77A | CA\_n41A-n71A  CA\_n41A-n77A  CA\_n71A-n77A | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 1 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41A-n71B-n77A | CA\_n41A-n71A  CA\_n41A-n77A  CA\_n71A-n77A | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n71 | CA\_n71B\_BCS2 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | CA\_n41A-n71A  CA\_n41A-n77A  CA\_n71A-n77A | n41 | n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n71 | CA\_n71B BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41A-n71(2A)-n77A | CA\_n41A-n71A  CA\_n41A-n77A  CA\_n71A-n77A | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n71 | CA\_n71(2A)\_BCS0 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | CA\_n41A-n71A  CA\_n41A-n77A  CA\_n71A-n77A | n41 | n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n71 | CA\_n71(2A) BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41A-n71A-n77(2A) | CA\_n41A-n71A  CA\_n41A-n77A  CA\_n71A-n77A | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
|  | CA\_n41A-n71A  CA\_n41A-n77A  CA\_n71A-n77A | n41 | n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(2A) BCS 4 and 5 |  |
| CA\_n41(2A)-n71A-n77A | CA\_n41A-n71A  CA\_n41A-n77A  CA\_n71A-n77A | n41 | CA\_n41(2A)\_BCS1 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | CA\_n41A-n71A  CA\_n41A-n77A  CA\_n71A-n77A | n41 | CA\_n41(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41(2A)-n71A-n77(2A) |  | n41 | CA\_n41(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(2A) BCS 4 and 5 |  |
| CA\_n41C-n71A-n77A | CA\_41C  CA\_n41A-n71A  CA\_n41A-n77A  CA\_n71A-n77A | n41 | CA\_n41C\_BCS0 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | CA\_41C  CA\_n41A-n71A  CA\_n41A-n77A  CA\_n71A-n77A | n41 | CA\_n41C BCS 4 and 5 | 4 and 5 |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41C-n71A-n77(2A) | CA\_41C  CA\_n41A-n71A  CA\_n41A-n77A  CA\_n71A-n77A | n41 | CA\_n41C BCS 4 and 5 | 4 and 5 |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(2A) BCS 4 and 5 |  |
| CA\_n41A-n71A-n78A | CA\_n41A-n71A  CA\_n41A-n78A  CA\_n71A-n78A | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n41A-n71A-n78(2A) | CA\_n41A-n71A  CA\_n41A-n78A  CA\_n71A-n78A | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n46A-n48A-n96A | CA\_n46A-n48A  CA\_n48A-n96A | n46 | 10, 20, 40, 60, 80 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46B-n48A-n96A | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46C-n48A-n96A | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46D-n48A-n96A | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46M-n48A-n96A | - | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46N-n48A-n96A | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46N\_BCS0 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46A-n48B-n96A | CA\_n48B  CA\_n46A-n48A  CA\_n48A-n96A  CA\_n46A-n48B  CA\_n48B-n96A | n46 | 10, 20, 40, 60, 80 | 0 |
|  |  | n48 | CA\_n48B\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46B-n48B-n96A | CA\_n48B  CA\_n46A-n48A  CA\_n48A-n96A  CA\_n46A-n48B  CA\_n48B-n96A | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n48 | CA\_n48B\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46C-n48B-n96A | CA\_n48B  CA\_n46A-n48A  CA\_n48A-n96A  CA\_n46A-n48B  CA\_n48B-n96A | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n48 | CA\_n48B\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46D-n48B-n96A | CA\_n48B  CA\_n46A-n48A  CA\_n48A-n96A  CA\_n46A-n48B  CA\_n48B-n96A | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n48 | CA\_n48B\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46M-n48B-n96A |  | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n48 | CA\_n48B\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46N-n48B-n96A | CA\_n48B  CA\_n46A-n48A  CA\_n48A-n96A  CA\_n46A-n48B  CA\_n48B-n96A | n46 | CA\_n46N\_BCS0 | 0 |
|  |  | n48 | CA\_n48B\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46A-n48C-n96A | CA\_n48B  CA\_n46A-n48A  CA\_n48A-n96A  CA\_n46A-n48B  CA\_n48B-n96A | n46 | 10, 20, 40, 60, 80 | 0 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46B-n48C-n96A | CA\_n48B  CA\_n46A-n48A  CA\_n48A-n96A  CA\_n46A-n48B  CA\_n48B-n96A | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46C-n48C-n96A | CA\_n48B  CA\_n46A-n48A  CA\_n48A-n96A  CA\_n46A-n48B  CA\_n48B-n96A | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46D-n48C-n96A | CA\_n48B  CA\_n46A-n48A  CA\_n48A-n96A  CA\_n46A-n48B  CA\_n48B-n96A | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46M-n48C-n96A | - | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46N-n48C-n96A | CA\_n48B  CA\_n46A-n48A  CA\_n48A-n96A  CA\_n46A-n48B  CA\_n48B-n96A | n46 | CA\_n46N\_BCS0 | 0 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46A-n48A-n96B | CA\_n46A-n48A  CA\_n48A-n96A | n46 | 10, 20, 40, 60, 80 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n96 | CA\_n96B\_BCS0 |  |
| CA\_n46B-n48A-n96B | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n96 | CA\_n96B\_BCS0 |  |
| CA\_n46C-n48A-n96B | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n96 | CA\_n96B\_BCS0 |  |
| CA\_n46D-n48A-n96B | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n96 | CA\_n96B\_BCS0 |  |
| CA\_n46M-n48A-n96B | - | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n96 | CA\_n96B\_BCS0 |  |
| CA\_n46N-n48A-n96B | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46N\_BCS0 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n96 | CA\_n96B\_BCS0 |  |
| CA\_n46A-n48A-n96C | - | n46 | 10, 20, 40, 60, 80 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46B-n48A-n96C | - | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46C-n48A-n96C | - | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46D-n48A-n96C | - | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46M-n48A-n96C | - | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46N-n48A-n96C | - | n46 | CA\_n46N\_BCS0 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46A-n48B-n96C | CA\_n48B  CA\_n46A-n48A  CA\_n48A-n96A  CA\_n46A-n48B  CA\_n48B-n96A | n46 | 10, 20, 40, 60, 80 | 0 |
|  |  | n48 | CA\_n48B\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46B-n48B-n96C | CA\_n48B  CA\_n46A-n48A  CA\_n48A-n96A  CA\_n46A-n48B  CA\_n48B-n96A | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n48 | CA\_n48B\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46C-n48B-n96C | CA\_n48B  CA\_n46A-n48A  CA\_n48A-n96A  CA\_n46A-n48B  CA\_n48B-n96A | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n48 | CA\_n48B\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46D-n48B-n96C | CA\_n48B  CA\_n46A-n48A  CA\_n48A-n96A  CA\_n46A-n48B  CA\_n48B-n96A | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n48 | CA\_n48B\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46M-n48B-n96C | - | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n48 | CA\_n48B\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46N-n48B-n96C | CA\_n48B  CA\_n46A-n48A  CA\_n48A-n96A  CA\_n46A-n48B  CA\_n48B-n96A | n46 | CA\_n46N\_BCS0 | 0 |
|  |  | n48 | CA\_n48B\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46A-n48C-n96C | - | n46 | 10, 20, 40, 60, 80 | 0 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46B-n48C-n96C | - | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46C-n48C-n96C | - | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46D-n48C-n96C | - | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46M-n48C-n96C | - | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46N-n48C-n96C | - | n46 | CA\_n46N\_BCS0 | 0 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46A-n48A-n96D | - | n46 | 10, 20, 40, 60, 80 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46B-n48A-n96D | - | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46C-n48A-n96D | - | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46D-n48A-n96D | - | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46M-n48A-n96D | - | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46N-n48A-n96D | - | n46 | CA\_n46N\_BCS0 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46A-n48C-n96D | CA\_n48B  CA\_n46A-n48A  CA\_n48A-n96A  CA\_n46A-n48B  CA\_n48B-n96A | n46 | 10, 20, 40, 60, 80 | 0 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46B-n48C-n96D | CA\_n48B  CA\_n46A-n48A  CA\_n48A-n96A  CA\_n46A-n48B  CA\_n48B-n96A | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46C-n48C-n96D | CA\_n48B  CA\_n46A-n48A  CA\_n48A-n96A  CA\_n46A-n48B  CA\_n48B-n96A | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46D-n48C-n96D | CA\_n48B  CA\_n46A-n48A  CA\_n48A-n96A  CA\_n46A-n48B  CA\_n48B-n96A | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46M-n48C-n96D | - | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46N-n48C-n96D | CA\_n48B  CA\_n46A-n48A  CA\_n48A-n96A  CA\_n46A-n48B  CA\_n48B-n96A | n46 | CA\_n46N\_BCS0 | 0 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46A-n48A-n96E | - | n46 | 10, 20, 40, 60, 80 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46B-n48A-n96E | - | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46C-n48A-n96E | - | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46D-n48A-n96E | - | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46M-n48A-n96E | - | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46N-n48A-n96E | - | n46 | CA\_n46N\_BCS0 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46A-n48C-n96E | CA\_n48B  CA\_n46A-n48A  CA\_n48A-n96A  CA\_n46A-n48B  CA\_n48B-n96A | n46 | 10, 20, 40, 60, 80 | 0 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46B-n48C-n96E | CA\_n48B  CA\_n46A-n48A  CA\_n48A-n96A  CA\_n46A-n48B  CA\_n48B-n96A | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46C-n48C-n96E | CA\_n48B  CA\_n46A-n48A  CA\_n48A-n96A  CA\_n46A-n48B  CA\_n48B-n96A | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46D-n48C-n96E | CA\_n48B  CA\_n46A-n48A  CA\_n48A-n96A  CA\_n46A-n48B  CA\_n48B-n96A | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46M-n48C-n96E | - | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46N-n48C-n96E | CA\_n48B  CA\_n46A-n48A  CA\_n48A-n96A  CA\_n46A-n48B  CA\_n48B-n96A | n46 | CA\_n46N\_BCS0 | 0 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46A-n48(2A)-n96A | CA\_n46A-n48A  CA\_n48A-n96A | n46 | 10, 20, 40, 60, 80 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46B-n48(2A)-n96A | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46C-n48(2A)-n96A | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46D-n48(2A)-n96A | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46M-n48(2A)-n96A | - | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46N-n48(2A)-n96A | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46N\_BCS0 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46A-n48(2A)-n96B | CA\_n46A-n48A  CA\_n48A-n96A | n46 | 20, 40, 60, 80 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | CA\_n96B\_BCS0 |  |
| CA\_n46B-n48(2A)-n96B | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | CA\_n96B\_BCS0 |  |
| CA\_n46C-n48(2A)-n96B | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | CA\_n96B\_BCS0 |  |
| CA\_n46D-n48(2A)-n96B | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | CA\_n96B\_BCS0 |  |
| CA\_n46M-n48(2A)-n96B | - | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | CA\_n96B\_BCS0 |  |
| CA\_n46N-n48(2A)-n96B | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46N\_BCS0 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | CA\_n96B\_BCS0 |  |
| CA\_n46A-n48(2A)-n96C | CA\_n46A-n48A  CA\_n48A-n96A | n46 | 10, 20, 40, 60, 80 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46B-n48(2A)-n96C | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46C-n48(2A)-n96C | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46D-n48(2A)-n96C | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46M-n48(2A)-n96C | - | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46N-n48(2A)-n96C | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46N\_BCS0 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46A-n48(2A)-n96D | CA\_n46A-n48A  CA\_n48A-n96A | n46 | 10, 20, 40, 60, 80 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46B-n48(2A)-n96D | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46C-n48(2A)-n96D | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46D-n48(2A)-n96D | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46M-n48(2A)-n96D | - | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46N-n48(2A)-n96D | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46N\_BCS0 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46A-n48(2A)-n96E | CA\_n46A-n48A  CA\_n48A-n96A | n46 | 10, 20, 40, 60, 80 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46B-n48(2A)-n96E | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46C-n48(2A)-n96E | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46D-n48(2A)-n96E | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46M-n48(2A)-n96E | - | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46N-n48(2A)-n96E | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46N\_BCS0 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46A-n48(3A)-n96A | CA\_n46A-n48A  CA\_n48A-n96A | n46 | 10, 20, 40, 60, 80 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46B-n48(3A)-n96A | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46C-n48(3A)-n96A | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46D-n48(3A)-n96A | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46M-n48(3A)-n96A | - | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46N-n48(3A)-n96A | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46N\_BCS0 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46A-n48(3A)-n96B | CA\_n46A-n48A  CA\_n48A-n96A | n46 | 10, 20, 40, 60, 80 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | CA\_n96B\_BCS0 |  |
| CA\_n46B-n48(3A)-n96B | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | CA\_n96B\_BCS0 |  |
| CA\_n46C-n48(3A)-n96B | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | CA\_n96B\_BCS0 |  |
| CA\_n46D-n48(3A)-n96B | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | CA\_n96B\_BCS0 |  |
| CA\_n46M-n48(3A)-n96B | - | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | CA\_n96B\_BCS0 |  |
| CA\_n46N-n48(3A)-n96B | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46N\_BCS0 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | CA\_n96B\_BCS0 |  |
| CA\_n46A-n48(3A)-n96C | CA\_n46A-n48A  CA\_n48A-n96A | n46 | 10, 20, 40, 60, 80 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46B-n48(3A)-n96C | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46C-n48(3A)-n96C | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46D-n48(3A)-n96C | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46M-n48(3A)-n96C | - | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46N-n48(3A)-n96C | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46N\_BCS0 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46A-n48(3A)-n96D | CA\_n46A-n48A  CA\_n48A-n96A | n46 | 10, 20, 40, 60, 80 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46B-n48(3A)-n96D | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46C-n48(3A)-n96D | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46D-n48(3A)-n96D | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46M-n48(3A)-n96D | - | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46N-n48(3A)-n96D | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46N\_BCS0 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46A-n48(3A)-n96E | CA\_n46A-n48A  CA\_n48A-n96A | n46 | 10, 20, 40, 60, 80 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46B-n48(3A)-n96E | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46C-n48(3A)-n96E | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46D-n48(3A)-n96E | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46M-n48(3A)-n96E | - | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46N-n48(3A)-n96E | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46N\_BCS0 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46A-n48(4A)-n96A | CA\_n46A-n48A  CA\_n48A-n96A | n46 | 10, 20, 40, 60, 80 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46B-n48(4A)-n96A | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46C-n48(4A)-n96A | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46D-n48(4A)-n96A | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46M-n48(4A)-n96A | - | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46N-n48(4A)-n96A | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46N\_BCS0 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | 20, 40, 60, 80 |  |
| CA\_n46A-n48(4A)-n96B | CA\_n46A-n48A  CA\_n48A-n96A | n46 | 10, 20, 40, 60, 80 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | CA\_n96B\_BCS0 |  |
| CA\_n46B-n48(4A)-n96B | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | CA\_n96B\_BCS0 |  |
| CA\_n46C-n48(4A)-n96B | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | CA\_n96B\_BCS0 |  |
| CA\_n46D-n48(4A)-n96B | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | CA\_n96B\_BCS0 |  |
| CA\_n46M-n48(4A)-n96B | - | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | CA\_n96B\_BCS0 |  |
| CA\_n46N-n48(4A)-n96B | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46N\_BCS0 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | CA\_n96B\_BCS0 |  |
| CA\_n46A-n48(4A)-n96C | CA\_n46A-n48A  CA\_n48A-n96A | n46 | 10, 20, 40, 60, 80 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46B-n48(4A)-n96C | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46C-n48(4A)-n96C | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46D-n48(4A)-n96C | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46M-n48(4A)-n96C | - | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46N-n48(4A)-n96C | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46N\_BCS0 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | CA\_n96C\_BCS0 |  |
| CA\_n46A-n48(4A)-n96D | CA\_n46A-n48A  CA\_n48A-n96A | n46 | 10, 20, 40, 60, 80 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46B-n48(4A)-n96D | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46C-n48(4A)-n96D | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46D-n48(4A)-n96D | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46M-n48(4A)-n96D |  | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46N-n48(4A)-n96D | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46N\_BCS0 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | CA\_n96D\_BCS0 |  |
| CA\_n46A-n48(4A)-n96E | CA\_n46A-n48A  CA\_n48A-n96A | n46 | 10, 20, 40, 60, 80 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46B-n48(4A)-n96E | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46B\_BCS0 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46C-n48(4A)-n96E | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46C\_BCS0 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46D-n48(4A)-n96E | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46D\_BCS0 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46M-n48(4A)-n96E | - | n46 | CA\_n46M\_BCS0 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n46N-n48(4A)-n96E | CA\_n46A-n48A  CA\_n48A-n96A | n46 | CA\_n46N\_BCS0 | 0 |
|  |  | n48 | CA\_n48(4A)\_BCS0 |  |
|  |  | n96 | CA\_n96E\_BCS0 |  |
| CA\_n48A-n66A-n70A | CA\_n48A-n66A  CA\_n48A-n70A | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n70 | 5, 10, 15, 201, 251 |  |
| CA\_n48A-n66(2A)-n70A | CA\_n48A-n66A  CA\_n48A-n70A | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS0 |  |
|  |  | n70 | 5, 10, 15, 201, 251 |  |
| CA\_n48(2A)-n66A-n70A | CA\_n48A-n66A  CA\_n48A-n70A | n48 | CA\_n48(2A)\_BCS1 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n70 | 5, 10, 15, 201, 251 |  |
| CA\_n48B-n66A-n70A | CA\_n48A-n66A  CA\_n48A-n70A | n48 | CA\_n48B\_BCS2 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n70 | 5, 10, 15, 201, 251 |  |
| CA\_n48A-n66A-n71A | CA\_n48A-n71A  CA\_n66A-n71A  CA\_n48A-n66A | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
| CA\_n48A-n66(2A)-n71A | CA\_n48A-n71A  CA\_n66A-n71A  CA\_n48A-n66A | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS0 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
| CA\_n48(2A)-n66A-n71A | CA\_n48A-n71A  CA\_n66A-n71A  CA\_n48A-n66A | n48 | CA\_n48(2A)\_BCS1 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
| CA\_n48B-n66A-n71A | CA\_n48A-n71A  CA\_n66A-n71A  CA\_n48A-n66A | n48 | CA\_n48B\_BCS2 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
| CA\_n48A-n66A-n71(2A) | CA\_n48A-n71A  CA\_n66A-n71A  CA\_n48A-n66A | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n71 | CA\_n71(2A)\_BCS0 |  |
| CA\_n48A-n66A-n77A | n777, 9  CA\_n48A-n66A  CA\_n66A-n77A | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n48A-n66A-n77C | CA\_n48A-n66A  CA\_n66A-n77A  CA\_n77C | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77C\_BCS0 |  |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 1 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77C\_BCS1 |  |
| CA\_n48B-n66A-n77A | CA\_n48A-n66A  CA\_n66A-n77A | n48 | CA\_n48B\_BCS0 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n48 | CA\_n48B\_BCS1 | 1 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n48 | CA\_n48B\_BCS2 | 2 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n48(2A)-n66A-n77A | CA\_n48A-n66A  CA\_n66A-n77A | n48 | CA\_n48(2A)\_BCS0 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n48 | CA\_n48(2A)\_BCS1 | 1 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n48(2A)-n66A-n77C | CA\_n48A-n66A  CA\_n66A-n77A | n48 | CA\_n48(2A)\_BCS0 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77C\_BCS0 |  |
|  |  | n48 | CA\_n48(2A)\_BCS0 | 1 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77C\_BCS1 |  |
|  |  | n48 | CA\_n48(2A)\_BCS1 | 2 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77C\_BCS0 |  |
|  |  | n48 | CA\_n48(2A)\_BCS1 | 3 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77C\_BCS1 |  |
| CA\_n48A-n70A-n71A | CA\_n48A-n71A  CA\_n70A-n71A  CA\_n48A-n70A | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n70 | 5, 10, 15, 201, 251 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
| CA\_n48(2A)-n70A-n71A | CA\_n48A-n71A  CA\_n70A-n71A  CA\_n48A-n70A | n48 | CA\_n48(2A)\_BCS1 | 0 |
|  |  | n70 | 5, 10, 15, 201, 251 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
| CA\_n48B-n70A-n71A | CA\_n48A-n71A  CA\_n70A-n71A  CA\_n48A-n70A | n48 | CA\_n48B\_BCS2 | 0 |
|  |  | n70 | 5, 10, 15, 201, 251 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
| CA\_n48A-n70A-n71(2A) | CA\_n48A-n71A  CA\_n70A-n71A  CA\_n48A-n70A | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n70 | 5, 10, 15, 201, 251 |  |
|  |  | n71 | CA\_n71(2A)\_BCS0 |  |
| CA\_n66A-n70A-n71A | CA\_n66A-n71A  CA\_n70A-n71A | n66 | 5, 10, 15, 20, 40 | 0 |
|  |  | n70 | 5, 10, 15, 201, 251 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
| CA\_n66A-n70A-n78A | CA\_n66A-n78A CA\_n70A-n78A | n66 | 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n70 | 5, 10, 15, 201, 251 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n66A-n70A-n71(2A) | CA\_n66A-n71A  CA\_n70A-n71A | n66 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n70 | 5, 10, 15, 201, 251 |  |
|  |  | n71 | CA\_n71(2A)\_BCS0 |  |
| CA\_n66B-n70A-n71A | CA\_n66A-n71A  CA\_n70A-n71A | n66 | CA\_n66B\_BCS0 | 0 |
|  |  | n70 | 5, 10, 15, 201,251 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
| CA\_n66(2A)-n70A-n71A | CA\_n66A-n71A  CA\_n70A-n71A | n66 | CA\_n66(2A)\_BCS0 | 0 |
|  |  | n70 | 5, 10, 15, 201, 251 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
| CA\_n66A-n71A-n77A | CA\_n66A-n71A  CA\_n66A-n77A  CA\_n71A-n77A | n66 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | CA\_n66A-n71A  CA\_n66A-n77A  CA\_n71A-n77A | n66 | n66 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n66A-n71B-n77A | CA\_n66A-n71A  CA\_n66A-n77A  CA\_n71A-n77A | n66 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n71 | CA\_n71B\_BCS2 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | CA\_n66A-n71A  CA\_n66A-n77A  CA\_n71A-n77A | n66 | n66 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n71 | CA\_n71B BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n66A-n71(2A)-n77A | CA\_n66A-n71A  CA\_n66A-n77A  CA\_n71A-n77A | n66 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n71 | CA\_n71(2A)\_BCS0 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n71 | CA\_n71(2A) BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n66(2A)-n71A-n77A | CA\_n66A-n71A  CA\_n66A-n77A  CA\_n71A-n77A | n66 | CA\_n66(2A)\_BCS1 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | CA\_n66A-n71A  CA\_n66A-n77A  CA\_n71A-n77A | n66 | CA\_n66(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n66A-n71A-n77(2A) | CA\_n66A-n71A  CA\_n66A-n77A  CA\_n71A-n77A | n66 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
|  | CA\_n66A-n71A  CA\_n66A-n77A  CA\_n71A-n77A | n66 | n66 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(2A) BCS 4 and 5 |  |
| CA\_n66(2A)-n71A-n77(2A) | CA\_n66A-n71A  CA\_n66A-n77A  CA\_n71A-n77A | n66 | CA\_n66(2A)\_BCS1 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
|  | CA\_n66A-n71A  CA\_n66A-n77A  CA\_n71A-n77A | n66 | CA\_n66(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_n77(2A) BCS 4 and 5 |  |
| CA\_n66A-n71A-n78A | CA\_n66A-n78A  CA\_n66A-n71A  CA\_n71A-n78A | n66 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n66A-n71A-n78(2A) | CA\_n66A-n78A  CA\_n66A-n71A  CA\_n71A-n78A | n66 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n66(2A)-n71A-n78A | CA\_n66A-n78A  CA\_n66A-n71A  CA\_n71A-n78A | n66 | CA\_n66(2A)\_BCS1 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n66(2A)-n71A-n78(2A) | CA\_n66A-n78A  CA\_n66A-n71A  CA\_n71A-n78A | n66 | CA\_n66(2A)\_BCS1 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| NOTE 1: This UE channel bandwidth is applicable only to downlink  NOTE 2: For the 20 MHz bandwidth, the minimum requirements are specified for NR UL carrier frequencies confined to either 713-723 MHz or 728-738 MHz.  NOTE 3: The SCS of each channel bandwidth for NR band refers to Table 5.3.5-1.  NOTE 4: The minimum requirements only apply for non-simultaneous Tx/Rx between all carriers for TDD combinations.  NOTE 5: Simultaneous Rx/Tx capability for TDD combinations does not apply for UEs supporting band n78 with an n77 implementation.  NOTE 6: Only single uplink carriers with power class other than PC3 are listed.  NOTE 7: Power Class 2 is allowed for this uplink combination or single uplink carrier in this downlink/uplink combination  NOTE 8: For this bandwidth, the minimum requirements are restricted to operation when carrier is configured as an SCell part of DC or CA configuration.  NOTE 9: Power Class 1.5 is allowed for single uplink carrier in this downlink/uplink combination | | | | |

---End of changes---