{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["TDoc_List","CR_Packs_List","Parameters"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":6,"comments":1,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"TDoc_List","index":0,"n_rows":2022,"n_cols":31,"rows_kept":2022,"cut":false,"hidden":false,"merged":[]}
["TDoc","Title","Source","Contact","Contact ID","Type","For","Abstract","Secretary Remarks","Agenda item sort order","Agenda item","Agenda item description","TDoc sort order within agenda item","TDoc Status","Reservation date","Uploaded","Is revision of","Revised to","Release","Spec","Version","Related WIs","CR","CR revision","CR category","TSG CR Pack","Reply to","To","Cc","Original LS","Reply in"]
["R4-1609010","Agenda for RAN4#81","Chairman","Xutao Zhou","40317","agenda","Approval","---","","1","2","Approval of the agenda",901000000,"approved","2016-10-31T14:50:37.500","2016-11-14T00:39:26.227","","","","","","","","","","","","","","",""]
["R4-1609011","RAN4#80bis Meeting Report","MCC","Juha Korhonen","21609","report","Approval","---","","2","3","Letters / reports from other groups / meetings",90110000,"approved","2016-10-31T14:50:37.517","2016-11-14T00:30:23.080","","","","","","","","","","","","","","",""]
["R4-1609012","Invitation to consider integration of satellite-based solutions into IMT-2020 networks","ITU-R WP 5D, AT&T","Marc Grant","16986","LS in","","---","","2","3","Letters / reports from other groups / meetings",90120000,"noted","2016-10-31T14:50:37.517","2016-10-31T15:08:13.777","","","","","","","","","","","","ITU-R WP 4B","3GPP, ETSI TC/SES, ITU-T SG 13","3GPP_ETSI_ITU-T SG 13",""]
["R4-1609013","Suitability of technical conditions of ECC DEC (11) 06 for 5G","ECC PT1, Ofcom","Juha Korhonen","21609","LS in","","---","","2","3","Letters / reports from other groups / meetings",90130000,"noted","2016-10-31T14:50:37.517","2016-10-31T15:08:13.793","","","","","","","","","","","","ETSI ERM, RAN","","ECC PT1(16)133 Annex 23 - LS to 3GPP on suitability of C-Band framework","R4-1610592, R4-1610994"]
["R4-1609014","Characteristics of terrestrial IMT systems for frequency sharing / interference analysis in the frequency range between 24.25 GHz and 86 GHz","ITU-R WP 5D","Sergio Buonomo","56608","LS in","","---","","2","3","Letters / reports from other groups / meetings",901400000,"noted","2016-10-31T14:50:37.533","2016-10-31T15:08:13.807","","","","","","","","","","","","3GPP, 3GPP2, ARIB, ATIS, CCSA, ETSI, IEEE, ITRI, TIA, TSDSI, TTA, TTC and WiMAX Forum","","LS_EOs_5D_374Att4.13","R4-1700112"]
["R4-1609015","FINALIZATION OF THE REVISION OF RECOMMENDATIONS ITU-R M.2070 AND ITU-R M.2071 AND STUDIES ON PROTECTION RNSS OPERATION FROM UNWANTED EMISSIONS OF IMT STATIONS","ITU-R WP 5D","Sergio Buonomo","56608","LS in","","---","","2","3","Letters / reports from other groups / meetings",901500000,"noted","2016-10-31T14:50:37.533","2016-10-31T15:08:13.840","","","","","","","","","","","","3GPP","","LS_EOs_5D_374Att5.6",""]
["R4-1609016","LS on wider bandwidth operation for NR","RAN1, NTT DOCOMO","Kazuaki Takeda","59634","LS in","","---","","2","3","Letters / reports from other groups / meetings",901600000,"noted","2016-10-31T14:50:37.533","2016-10-31T15:08:13.840","","","Rel-14","","","FS_NR_newRAT","","","","","","RAN4","RAN2","R1-1610655",""]
["R4-1609017","LS on V2X UE transmission chain","RAN1, Huawei","Yi Shi","60150","LS in","","---","","2","3","Letters / reports from other groups / meetings",901700000,"noted","2016-10-31T14:50:37.533","2016-10-31T15:08:13.840","","","Rel-14","","","LTE_V2X-Core","","","","","","RAN2, RAN4","","R1-1611000",""]
["R4-1609018","Reply LS on CSI measurement ambiguity in LAA","RAN1, LGE","Seonwook Kim","60310","LS in","","---","","2","3","Letters / reports from other groups / meetings",901800000,"noted","2016-10-31T14:50:37.547","2016-10-31T15:08:13.840","","","Rel-13","","","LTE_LAA-Perf","","","","","","RAN4","","R1-1611026",""]
["R4-1609019","Response LS to IEEE 802.11 regarding LAA","RAN1, Qualcomm","Srinivas Yerramalli","60673","LS in","","---","","2","3","Letters / reports from other groups / meetings",901900000,"noted","2016-10-31T14:50:37.547","2016-10-31T15:08:13.840","","","Rel-13","","","LTE_LAA","","","","","","IEEE 802 LAN/MAN Standards Committee","Wi-Fi Alliance, The City of New York Office of the Mayor, RAN, RAN2, RAN4","R1-1611031",""]
["R4-1609020","LS on configuration of NPRS power for NB-IoT downlink positioning","RAN1, Huawei","Yiling Wu","61661","LS in","","---","","2","3","Letters / reports from other groups / meetings",902000000,"noted","2016-10-31T14:50:37.547","2016-10-31T15:08:13.857","","","Rel-14","","","NB_IOTenh","","","","","","RAN4","","R1-1611032",""]
["R4-1609021","LS for SRS Carrier-Based Switching Agreements","RAN1, Huawei","Xiao Weimin","56706","LS in","","---","","2","3","Letters / reports from other groups / meetings",902100000,"noted","2016-10-31T14:50:37.563","2016-10-31T15:08:13.857","","","Rel-14","","","LTE_SRS_switch","","","","","","RAN2, RAN4","","R1-1611049",""]
["R4-1609022","LS on L1 parameters for SRS Carrier-Based Switching","RAN1, Huawei","Xiao Weimin","56706","LS in","","---","","2","3","Letters / reports from other groups / meetings",902200000,"noted","2016-10-31T14:50:37.563","2016-10-31T15:08:13.857","","","Rel-14","","","LTE_SRS_switch","","","","","","RAN2","RAN4","R1-1611050",""]
["R4-1609023","LS on Multipath RSTD reporting and CRS usage together with PRS","RAN1, Ericsson & Intel","Johan Bergman","51222","LS in","","---","","2","3","Letters / reports from other groups / meetings",902300000,"noted","2016-10-31T14:50:37.580","2016-10-31T15:08:13.857","","","Rel-14","","","UTRA_LTE_iPos_enh2-Core","","","","","","RAN2","RAN3, RAN4","R1-1611052",""]
["R4-1609024","LS on FeMTC VoLTE enhancements","RAN1, Huawei","Matthew Webb","45858","LS in","","---","","2","3","Letters / reports from other groups / meetings",902400000,"noted","2016-10-31T14:50:37.580","2016-10-31T15:08:13.857","","","Rel-14","","","LTE_feMTC","","","","","","RAN2, RAN4","","R1-1611053",""]
["R4-1609025","LS on implication of sTTI operation on UL ON/OFF time mask","RAN1, Ericsson","Daniel Larsson","39861","LS in","","---","","2","3","Letters / reports from other groups / meetings",902500000,"noted","2016-10-31T14:50:37.580","2016-10-31T15:08:13.730","","","Rel-15","","","LTE_sTTIandPT","","","","","","RAN4","","R1-1611054",""]
["R4-1609026","LS on Shortened TTI and processing time for LTE","RAN1, Ericsson","Daniel Larsson","39861","LS in","","---","","2","3","Letters / reports from other groups / meetings",902600000,"noted","2016-10-31T14:50:37.580","2016-10-31T15:08:13.730","","","Rel-15","","","LTE_sTTIandPT","","","","","","RAN2, RAN4","","R1-1611055",""]
["R4-1609027","Reply LS on A New PRACH Cyclic Shift Restriction Set","RAN1, Huawei","Chao Luo","53355","LS in","","---","","2","3","Letters / reports from other groups / meetings",902700000,"noted","2016-10-31T14:50:37.593","2016-10-31T15:08:13.747","","","Rel-14","","","LTE_high_speed","","","","","","RAN4, RAN2","","R1-1611056",""]
["R4-1609028","LS on RAN1 agreements potentially related to RAN2/4 in LTE-based V2X services","RAN1, LGE","Hanbyul Seo","57341","LS in","","---","","2","3","Letters / reports from other groups / meetings",902800000,"noted","2016-10-31T14:50:37.593","2016-10-31T15:08:13.747","","","Rel-14","","","LTE_V2X-Core","","","","","","RAN2, RAN4","","R1-1611066",""]
["R4-1609029","LS on Multi-carrier enhancements for UMTS","RAN2, Ericsson","Cecilia Eklof","59618","LS in","","---","","2","3","Letters / reports from other groups / meetings",902900000,"noted","2016-10-31T14:50:37.610","2016-10-31T15:08:13.747","","","Rel-14","","","UTRA_MCe-Core","","","","","","RAN4","RAN1","R2-167169",""]
["R4-1609030","LS on periodic WLAN measurement reporting","RAN2, MediaTek","Pavan Nuggehalli","60166","LS in","","---","","2","3","Letters / reports from other groups / meetings",903000000,"noted","2016-10-31T14:50:37.610","2016-10-31T15:08:13.747","","","Rel-13","","","LTE_WLAN_radio-Core","","","","","","RAN4","","R2-167301",""]
["R4-1609031","Reply LS on performance enhancements indicator for high speed scenarios","RAN2, Ericsson","Mattias Bergstrom","46046","LS in","","---","","2","3","Letters / reports from other groups / meetings",903100000,"noted","2016-10-31T14:50:37.627","2016-10-31T15:08:13.747","","","Rel-14","","","LTE_high_speed-Core","","","","","","RAN4","","R2-167308",""]
["R4-1609032","LS on RAN2 agreements for mobility enhancement","RAN2, Ericsson","Candy Yiu","46260","LS in","","---","","2","3","Letters / reports from other groups / meetings",903200000,"noted","2016-10-31T14:50:37.627","2016-10-31T15:08:13.760","","","Rel-14","","","LTE_eMob-Core","","","","","","RAN3","RAN1, RAN4","R2-167312",""]
["R4-1609033","LS on RAN2 agreements for NR DL-based mobility and Cell definition","RAN2, Ericsson","Icaro Leonardo Da Silva","58721","LS in","","---","","2","3","Letters / reports from other groups / meetings",903300000,"noted","2016-10-31T14:50:37.627","2016-10-31T15:08:13.760","","","Rel-14","","","FS_NR_newRAT","","","","","","RAN1","RAN3, RAN4","R2-167313",""]
["R4-1609034","Response LS on Measurement gap enhancement","RAN2, Ericsson","Hakan Palm","18830","LS in","","---","","2","3","Letters / reports from other groups / meetings",903400000,"noted","2016-10-31T14:50:37.640","2016-10-31T15:08:13.760","","","Rel-14","","","LTE_meas_gap_enh-Core","","","","","","RAN4","RAN1","R2-167317",""]
["R4-1609035","LS on RF requirements for category NB1 Ues","RAN5, Rohde&Schwarz","Niels Petrovic","49274","LS in","","---","","2","3","Letters / reports from other groups / meetings",903500000,"noted","2016-10-31T14:50:37.640","2016-10-31T15:08:13.777","","","Rel-13","","","NB_IOT-UEConTest","","","","","","RAN4","","R5-167202",""]
["R4-1609036","LS on NB-IoT RRC Re-establishment test configurations","RAN5, CMCC","Jinqiang Xing","62081","LS in","","---","","2","3","Letters / reports from other groups / meetings",903600000,"noted","2016-10-31T14:50:37.657","2016-10-31T15:08:13.777","","","Rel-13","","","","","","","","","RAN4","","R5-167203",""]
["R4-1609037","LS on RRM NPDSCH Reference Channel for UE category NB1","RAN5, CMCC","Jinqiang Xing","62081","LS in","","---","","2","3","Letters / reports from other groups / meetings",903700000,"noted","2016-10-31T14:50:37.657","2016-10-31T15:08:13.777","","","Rel-13","","","","","","","","","RAN4","","R5-167204",""]
["R4-1609038","Requirements for mobile backhaul/fronthaul in a G.fast Deployment Environment","ITU-T SG15, Nokia","Frank Van der Putten","19393","LS in","","---","","2","3","Letters / reports from other groups / meetings",903800000,"noted","2016-10-31T14:50:37.657","2016-10-31T15:08:13.777","","","","","","","","","","","","RAN1, RAN4, The NGMN, BBF WWC","","SG15-LS405",""]
["R4-1609039","Implications of Wi-Fi Field Measurements for Multi-Node Testing","Hewlett-Packard Enterprise","Stuart Strickland","67266","discussion","Discussion","---","","140","7.1.2","Multi-node testing [FS_LTE_LAA_multinode_test]",903900000,"noted","2016-10-31T17:43:48.660","2016-11-07T16:09:55.857","","","Rel-13","","0.0.3","FS_LTE_LAA_multinode_test","","","","","","","","",""]
["R4-1609040","Revision of WID: LTE Advanced inter-band CA Rel-14 for 2DL1UL","Qualcomm Incorporated","Ville Vintola","44963","WID revised","Endorsement","Revised WID with added new CA combinations.","","152","8.2.1","Rapporteur Input (WID/CRs) [LTE_CA_R14_2DL1UL-Core]",964200000,"revised","2016-10-31T20:27:38.823","2016-11-07T03:27:31.063","","R4-1610908","Rel-14","","","LTE_CA_R14_2DL1UL","","","","","","","","",""]
["R4-1609041","TR 36 714-02-01_Rel14_2DL 1UL CA","Qualcomm Incorporated","Ville Vintola","44963","draft TR","Approval","TR Prepared based on approved input from previous meeting","","152","8.2.1","Rapporteur Input (WID/CRs) [LTE_CA_R14_2DL1UL-Core]",904000000,"approved","2016-10-31T20:36:35.713","2016-11-07T03:27:31.047","","","Rel-14","36.714-02-01","0.4.0","LTE_CA_R14_2DL1UL","","","","","","","","",""]
["R4-1609042","Technical Report of B11/B21 Globalization(TR36.745 v0.2.0)","SoftBank Corp.","Kenichi Kihara","41094","draft TR","Approval","36.745(v0.2.0) reflecting agreed TPs in the last meeting.","","387","9.2.1","General  [FS_LTE_B11_B21_global]",904200000,"approved","2016-11-01T00:58:19.250","2016-11-02T04:06:12.833","","","Rel-14","36.745","0.2.0","FS_LTE_B11_B21_global","","","","","","","","",""]
["R4-1609043","TP for TR36.745: Evaluation results and conclusion (section 6 and 7)","SoftBank Corp.","Kenichi Kihara","41094","pCR","Approval","TP to capture agreements in the last meeting on prerequisites and evaluation results based on simulations and measurements.","","388","9.2.2","UE RF (36.101) [FS_LTE_B11_B21_global]",83900,"revised","2016-11-01T01:00:58.137","2016-11-02T04:06:29.867","","R4-1610837","","36.745","0.2.0","","","","","","","","","",""]
["R4-1609044","Description on limitation of operation on Power class 1 UE","SoftBank Corp.","Kenichi Kihara","41094","other","Approval","This paper proposes a descrition to capture B3/B28 HP-UE restrictions in 36.101.","","234","8.16.2","UE RF (36.101)  [LTE_HPUE_B3_B20_B28]",904400000,"noted","2016-11-01T01:04:08.033","2016-11-02T04:06:45.513","","","Rel-14","","","","","","","","","","","",""]
["R4-1609045","TP for TR36.714-02-01: MSD study of LTE-A Inter-band Carrier Aggregation (2DL/1UL) of Band 11 and Band 28","SoftBank Corp.","Kenichi Kihara","41094","pCR","Approval","This paper is to propose MSD values for B11+B28 and some corrections.","","153","8.2.2","UE RF (36.101) [LTE_CA_R14_2DL1UL-Core]",904500000,"approved","2016-11-01T01:06:51.180","2016-11-02T04:06:58.650","","","","36.714-02-01","0.4.0","LTE_CA_R14_2DL1UL-Core","","","","","","","","",""]
["R4-1609046","TP for TR36.714-02-01: the support of CA_8A-41A BCS1","SoftBank Corp.","Kenichi Kihara","41094","pCR","Approval","This paper is to complete 8A-41A BCS1.","","153","8.2.2","UE RF (36.101) [LTE_CA_R14_2DL1UL-Core]",904600000,"withdrawn","2016-11-01T01:08:47.023","2016-11-02T04:07:11.440","","R4-1609129","","36.714-02-01","0.4.0","LTE_CA_R14_2DL1UL-Core","","","","","","","","",""]
["R4-1609047","TP for TR36.714-02-01: the support of CA_28A-41A BCS1","SoftBank Corp.","Kenichi Kihara","41094","pCR","Approval","This paper is to complete 28A-41A BCS1.","","153","8.2.2","UE RF (36.101) [LTE_CA_R14_2DL1UL-Core]",904700000,"withdrawn","2016-11-01T01:10:50.280","2016-11-02T04:07:26.340","","R4-1609130","","36.714-02-01","0.4.0","LTE_CA_R14_2DL1UL-Core","","","","","","","","",""]
["R4-1609048","TP for TR36.714-03-01: the support of CA_8A-28A-41A BCS0","SoftBank Corp.","Kenichi Kihara","41094","pCR","Approval","This paper is to complete 3DL/1UL of 8A-28A-41A.","","159","8.3.2","UE RF (36.101) [LTE_CA_R14_3DL1UL-Core]",75800000,"withdrawn","2016-11-01T01:13:03.300","2016-11-02T04:10:02.590","","R4-1609131","","36.714-03-01","0.4.0","","","","","","","","","",""]
["R4-1609049","WF on inter-cell interference model and reference receiver for BS IC","China Telecom","Shan Yang","48340","other","Approval","---","","395","9.4.1","General  [FS_LTE _IC_BS]",904900000,"noted","2016-11-01T01:36:41.653","2016-11-19T17:47:25.053","","","Rel-14","","","","","","","","","","","",""]
["R4-1609050","Reference receiver for BS IC","China Telecom","Shan Yang","48340","discussion","Discussion","---","","397","9.4.3","Reference receiver [FS_LTE _IC_BS]",905000000,"noted","2016-11-01T01:36:41.670","2016-11-04T15:31:51.107","","","Rel-14","","","","","","","","","","","",""]
["R4-1609051","Inter-cell interference model for BS IC receiver","China Telecom","Shan Yang","48340","discussion","Discussion","---","","398","9.4.4","Interference model [FS_LTE _IC_BS]",905100000,"noted","2016-11-01T01:36:41.700","2016-11-04T15:31:51.107","","","Rel-14","","","","","","","","","","","",""]
["R4-1609052","Intra-cell interference model for BS IC receiver","China Telecom","Shan Yang","48340","discussion","Discussion","---","","398","9.4.4","Interference model [FS_LTE _IC_BS]",905200000,"noted","2016-11-01T01:36:41.730","2016-11-04T15:31:51.107","","","Rel-14","","","","","","","","","","","",""]
["R4-1609053","Link level simulation assumptions for BS IC receiver","China Telecom","Shan Yang","48340","discussion","Discussion","---","","399","9.4.5","Link level evaluation [FS_LTE _IC_BS]",905300000,"noted","2016-11-01T01:36:41.747","2016-11-04T15:31:51.107","","","Rel-14","","","","","","","","","","","",""]
["R4-1609054","Updated NR coexistence results for downlink in Urban Macro scenario","China Telecom","Shan Yang","48340","discussion","Discussion","---","","410","11.3.1","Co-existence [FS_NR_newRAT]",9000,"noted","2016-11-01T01:36:41.777","2016-11-04T15:31:51.120","","","","","","","","","","","","","","",""]
["R4-1609055","NR coexistence results for uplink in Urban Macro scenario","China Telecom","Shan Yang","48340","discussion","Discussion","---","","410","11.3.1","Co-existence [FS_NR_newRAT]",912300000,"noted","2016-11-01T01:36:41.810","2016-11-04T15:31:51.120","","","","","","","","","","","","","","",""]
["R4-1609056","TR 38.803 v0.3.0","DOCOMO Communications Lab.","Kunihiko Teshima","57760","draft TR","Approval","This is a draft TR 38.803 version 0.3.0","","407","11.1","General   [FS_NR_newRAT]",0,"reserved","2016-11-01T10:24:37.763",null,"","","Rel-15","38.803","0.3.0","FS_NR_newRAT","","","","","","","","",""]
["R4-1609057","Analysis of MBS Performance Requirements","NextNav, AT&T, Broadcom","Bill Shvodian","61097","discussion","Discussion","Discussion of performance requirements for MBS measurement accuracy","","63","5.9.2","RRM [WI code or TEI13]",905700000,"noted","2016-11-01T18:38:46.097","2016-11-04T14:01:04.987","","","Rel-13","37.171","13.0.0","UTRA_LTE_iPos_enh-Perf","","","","","","","","",""]
["R4-1609058","Removal of square brackets from MBS measurement accuracy requirements","NextNav, AT&T, Broadcom","Bill Shvodian","61097","CR","Agreement","Category F CR. Removes the square brackets from the MBS Measurement accuracy requirements","","63","5.9.2","RRM [WI code or TEI13]",905800000,"revised","2016-11-01T18:46:13.597","2016-11-04T14:01:05.003","","R4-1611010","Rel-13","37.171","13.0.0","UTRA_LTE_iPos_enh-Perf","0001","","F","","","","","",""]
["R4-1609059","Addition of 1.4 and 3 MHz channel bandwidths for BAND 65 in TS36.101 (Rel-13)","HUGHES Network Systems Ltd","Pasquale Amodio","61328","CR","Endorsement","Update the relevant clauses within E-UTRA technical specification 36.101 Release 13 to include support for the 1.4 and 3 MHz Channel Bandwidths in BAND 65.","","70","5.10.2","New spectrum [WI code]",168000,"revised","2016-11-01T19:58:37.527","2016-11-04T20:52:29.407","","R4-1610819","Rel-13","36.101","13.5.0","","3968","","B","","","","","",""]
["R4-1609060","Addition of 1.4 and 3 MHz channel bandwidths for BAND 65 in TS36.101 (Rel-14)","HUGHES Network Systems Ltd","Pasquale Amodio","61328","CR","Endorsement","Mirror CR - •\tUpdate the related clauses within E-UTRA technical specifications 36.101 Release 14, to include support for the 1.4 and 3 MHz Channel Bandwidth in BAND 65.","","70","5.10.2","New spectrum [WI code]",905900000,"revised","2016-11-01T20:03:03.320","2016-11-04T20:52:29.407","","R4-1610820","Rel-14","36.101","14.1.0","","3969","","B","","","","","",""]
["R4-1609061","Simulations on 4RX+ CA tests","Intel Corporation","Yang Tang","56725","other","Discussion","---","","359","8.30.3.2","Extend existing 2Rx CA requirement to 4Rx [LTE_4Rx_AP_DL_CA-Perf]",906100000,"revised","2016-11-01T22:26:03.743","2016-11-07T18:58:23.500","","R4-1610640","","","","LTE_4Rx_AP_DL_CA-Perf","","","","","","","","",""]
["R4-1609062","Discussion on 2RX/4RX+CA+IRC tests","Intel Corporation","Yang Tang","56725","other","Discussion","---","","360","8.30.3.3","Extend MMSE-IRC requirement from 2Rx to 4Rx [LTE_4Rx_AP_DL_CA-Perf]",971200000,"noted","2016-11-01T22:26:03.757","2016-11-07T18:58:23.500","","","","","","LTE_4Rx_AP_DL_CA-Perf","","","","","","","","",""]
["R4-1609063","Discussion on 2RX/4RX+CA WI test scope","Intel Corporation","Yang Tang","56725","other","Discussion","---","","358","8.30.3.1","Applicability [LTE_4Rx_AP_DL_CA-Perf]",999600000,"withdrawn","2016-11-01T22:26:03.773",null,"","","","","","LTE_4Rx_AP_DL_CA-Perf","","","","","","","","",""]
["R4-1609064","Simulation results on TM2 IRC test","Intel Corporation","Yang Tang","56725","other","Discussion","---","","33","5.2.3.2","UE demodulation and CSI [LTE_4Rx_AP_DL-Perf]",906400000,"noted","2016-11-01T22:26:03.803","2016-11-07T18:58:23.517","","","","","","LTE_4Rx_AP_DL-Perf","","","","","","","","",""]
["R4-1609065","Discussion and simulation on TM9 MU test 8.3.1.1","Intel Corporation","Yang Tang","56725","other","Discussion","---","","33","5.2.3.2","UE demodulation and CSI [LTE_4Rx_AP_DL-Perf]",971400000,"noted","2016-11-01T22:26:03.820","2016-11-07T18:58:23.533","","","","","","LTE_4Rx_AP_DL-Perf","","","","","","","","",""]
["R4-1609066","CR on 4-RX TM9 MU test","Intel Corporation","Yang Tang","56725","CR","Agreement","---","","33","5.2.3.2","UE demodulation and CSI [LTE_4Rx_AP_DL-Perf]",989100000,"revised","2016-11-01T22:26:03.837","2016-11-07T18:58:23.547","","R4-1610686","Rel-13","36.101","13.5.0","LTE_4Rx_AP_DL-Perf","3970","","F","","","","","",""]
["R4-1609067","CR on 4-RX TM9 MU test","Intel Corporation","Yang Tang","56725","CR","Agreement","---","","33","5.2.3.2","UE demodulation and CSI [LTE_4Rx_AP_DL-Perf]",989300000,"revised","2016-11-01T22:26:03.960","2016-11-07T18:58:23.563","","R4-1610687","Rel-14","36.101","14.1.0","LTE_4Rx_AP_DL-Perf","3971","","A","","","","","",""]
["R4-1609068","CR on 4-RX TM9 MU test applicalbility rule","Intel Corporation","Yang Tang","56725","CR","Agreement","---","","33","5.2.3.2","UE demodulation and CSI [LTE_4Rx_AP_DL-Perf]",989500000,"noted","2016-11-01T22:26:04.070","2016-11-07T18:58:23.580","","","Rel-13","36.101","13.5.0","LTE_4Rx_AP_DL-Perf","3972","","F","","","","","",""]
["R4-1609069","CR on 4-RX TM9 MU test applicalbility rule","Intel Corporation","Yang Tang","56725","CR","Agreement","---","","33","5.2.3.2","UE demodulation and CSI [LTE_4Rx_AP_DL-Perf]",989600000,"withdrawn","2016-11-01T22:26:04.163","2016-11-07T18:58:23.593","","","Rel-14","36.101","14.1.0","LTE_4Rx_AP_DL-Perf","3973","","A","","","","","",""]
["R4-1609070","Discussion on 1RX UE capability signalling and requirement","Intel Corporation","Yang Tang","56725","other","Discussion","---","","336","8.27.5","UE demodulation (36.101) [LTE_UE_cat_1RX-Perf]",907000000,"noted","2016-11-01T22:26:04.287","2016-11-07T18:58:23.610","","","","","","LTE_UE_cat_1RX-Perf","","","","","","","","",""]
["R4-1609071","LS to RAN2 on 1RX UE capability signalling","Intel Corporation","Yang Tang","56725","LS out","Approval","---","","336","8.27.5","UE demodulation (36.101) [LTE_UE_cat_1RX-Perf]",907100000,"withdrawn","2016-11-01T22:26:04.303",null,"","","Rel-14","","","LTE_UE_cat_1RX-Perf","","","","","","RAN2","","",""]
["R4-1609072","Discussion on new 1RX UE performance test","Intel Corporation","Yang Tang","56725","other","Discussion","---","","336","8.27.5","UE demodulation (36.101) [LTE_UE_cat_1RX-Perf]",945200000,"noted","2016-11-01T22:26:04.320","2016-11-07T18:58:23.610","","","","","","LTE_UE_cat_1RX-Perf","","","","","","","","",""]
["R4-1609073","Discussion on Rel-14 eLAA UE performance test","Intel Corporation","Yang Tang","56725","other","Discussion","---","","257","8.18.6","UE/BS demodulation and CSI (36.101/36.104) [LTE_eLAA-Perf]",970800000,"noted","2016-11-01T22:26:04.333","2016-11-07T18:58:23.610","","","","","","LTE_eLAA-Perf","","","","","","","","",""]
["R4-1609074","Considerations on NR RRM with the multiple numerologiesConsideration on NR RRM","Intel Corporation","Yang Tang","56725","other","Discussion","[For Discussion]","","425","11.6.1.1","RRM general [FS_NR_newRAT]",4800000,"noted","2016-11-01T22:26:04.367","2016-11-07T18:58:23.627","","","","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1609075","Considerations on the RRM requirements for the initial access in NR","Intel Corporation","Yang Tang","56725","other","Discussion","[For Discussion]","","425","11.6.1.1","RRM general [FS_NR_newRAT]",9074000,"noted","2016-11-01T22:26:04.380","2016-11-07T18:58:23.640","","","","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1609076","Discussion on the network assistant signaling for ehanced RRM requirements in HST","Intel Corporation","Yang Tang","56725","other","Discussion","[For Discussion]","","341","8.28.2.1","Enhancement in connected mode (DRX) [LTE_high_speed]",952300000,"noted","2016-11-01T22:26:04.397","2016-11-07T18:58:23.640","","","","","","LTE_high_speed","","","","","","","","",""]
["R4-1609077","NR coexistence study methodology, assumption and discussion","Intel Corporation","Yang Tang","56725","other","Discussion","---","","410","11.3.1","Co-existence [FS_NR_newRAT]",1650000,"noted","2016-11-01T22:26:04.413","2016-11-07T18:58:23.673","","","","","","","","","","","","","","",""]
["R4-1609078","Simulation results -  Indoor","Intel Corporation","Yang Tang","56725","other","Discussion","---","","410","11.3.1","Co-existence [FS_NR_newRAT]",1660000,"noted","2016-11-01T22:26:04.443","2016-11-07T18:58:23.673","","","","","","","","","","","","","","",""]
["R4-1609079","Simulation results -  Dense Urban","Intel Corporation","Yang Tang","56725","other","Discussion","---","","410","11.3.1","Co-existence [FS_NR_newRAT]",3530000,"noted","2016-11-01T22:26:04.460","2016-11-07T18:58:23.673","","","","","","","","","","","","","","",""]
["R4-1609080","Simulation results -  Urban Macro","Intel Corporation","Yang Tang","56725","other","Discussion","---","","410","11.3.1","Co-existence [FS_NR_newRAT]",9077000,"noted","2016-11-01T22:26:04.477","2016-11-07T18:58:23.687","","","","","","","","","","","","","","",""]
["R4-1609081","Issues of 2UL 7A-7A and 66A-66A","Intel Corporation","Yang Tang","56725","other","Approval","---","","145","8.1","LTE Advanced Intra-band CA including contiguous and non-contiguous [LTE_CA_R14_intra]",908100000,"noted","2016-11-01T22:26:04.507","2016-11-07T18:58:23.687","","","","","","","","","","","","","","",""]
["R4-1609082","V2V RRM performance requirements","Intel Corporation","Yang Tang","56725","discussion","Discussion","---","","266","8.19.3.1","UE transmission timing accuracy test [LTE_SL_V2V-Perf]",9082000,"noted","2016-11-01T22:26:04.523","2016-11-07T18:58:23.687","","","Rel-14","","","LTE_SL_V2V-Perf","","","","","","","","",""]
["R4-1609083","V2V UE demodulation performance requirements","Intel Corporation","Yang Tang","56725","discussion","Discussion","---","","269","8.19.4.1","Single-link PSSCH and PSCCH  [LTE_SL_V2V-Perf]",947700000,"noted","2016-11-01T22:26:04.537","2016-11-07T18:58:23.703","","","Rel-14","","","LTE_SL_V2V-Perf","","","","","","","","",""]
["R4-1609084","V2V UE demodulation reference receiver assumptions","Intel Corporation","Yang Tang","56725","discussion","Discussion","---","","269","8.19.4.1","Single-link PSSCH and PSCCH  [LTE_SL_V2V-Perf]",948000000,"noted","2016-11-01T22:26:04.553","2016-11-07T18:58:23.720","","","Rel-14","","","LTE_SL_V2V-Perf","","","","","","","","",""]
["R4-1609085","V2X RRM UE transmit timing requirements","Intel Corporation","Yang Tang","56725","discussion","Discussion","---","","281","8.20.4.1","UE Transmit timing [LTE_V2X-Core]",2110000,"noted","2016-11-01T22:26:04.583","2016-11-07T18:58:23.720","","","Rel-14","","","LTE_V2X-Core","","","","","","","","",""]
["R4-1609086","V2X PSSCH-RSRP measurements accuracy analysis","Intel Corporation","Yang Tang","56725","discussion","Discussion","---","","285","8.20.4.5","Autonomous resource selection/reselection [LTE_V2X-Core]",63800000,"revised","2016-11-01T22:26:04.600","2016-11-07T18:58:23.737","","R4-1610638","Rel-14","","","LTE_V2X-Core","","","","","","","","",""]
["R4-1609087","V2X S-RSRP measurements accuracy analysis","Intel Corporation","Yang Tang","56725","discussion","Discussion","---","","283","8.20.4.3","Initiation/cease of SLSS requirement [LTE_V2X-Core]",9087000,"revised","2016-11-01T22:26:04.617","2016-11-07T18:58:23.750","","R4-1610682","Rel-14","","","LTE_V2X-Core","","","","","","","","",""]
["R4-1609088","Enhanced CRS-IM scenarios and simulation assumptions","Intel Corporation","Yang Tang","56725","discussion","Discussion","---","","367","8.31.2.1","Performance evaluation: scenarios and receiver [LTE_eCRSIM_eSUMIMO]",71700000,"noted","2016-11-01T22:26:04.647","2016-11-07T18:58:23.767","","","Rel-14","","","LTE_eCRSIM_eSUMIMO","","","","","","","","",""]
["R4-1609089","Enhanced CRS-IM reference receivers","Intel Corporation","Yang Tang","56725","discussion","Discussion","---","","367","8.31.2.1","Performance evaluation: scenarios and receiver [LTE_eCRSIM_eSUMIMO]",908800000,"noted","2016-11-01T22:26:04.663","2016-11-07T18:58:23.783","","","Rel-14","","","LTE_eCRSIM_eSUMIMO","","","","","","","","",""]
["R4-1609090","Enhanced CRS-IM performance analysis for PDSCH","Intel Corporation","Yang Tang","56725","discussion","Discussion","---","","367","8.31.2.1","Performance evaluation: scenarios and receiver [LTE_eCRSIM_eSUMIMO]",908900000,"noted","2016-11-01T22:26:04.677","2016-11-07T18:58:23.813","","","Rel-14","","","LTE_eCRSIM_eSUMIMO","","","","","","","","",""]
["R4-1609091","Enhanced CRS-IM performance analysis for DL Control Channels","Intel Corporation","Yang Tang","56725","discussion","Discussion","---","","367","8.31.2.1","Performance evaluation: scenarios and receiver [LTE_eCRSIM_eSUMIMO]",974600000,"noted","2016-11-01T22:26:04.693","2016-11-07T18:58:23.827","","","Rel-14","","","LTE_eCRSIM_eSUMIMO","","","","","","","","",""]
["R4-1609092","Enhanced SU-MIMO IM scenarios and simulation assumptions","Intel Corporation","Yang Tang","56725","discussion","Discussion","---","","370","8.31.3.1","Performance evaluation: scenarios and receiver [LTE_eCRSIM_eSUMIMO]",936200000,"noted","2016-11-01T22:26:04.723","2016-11-07T18:58:23.860","","","Rel-14","","","LTE_eCRSIM_eSUMIMO","","","","","","","","",""]
["R4-1609093","Enhanced SU-MIMO IM performance analysis","Intel Corporation","Yang Tang","56725","discussion","Discussion","---","","370","8.31.3.1","Performance evaluation: scenarios and receiver [LTE_eCRSIM_eSUMIMO]",948200000,"noted","2016-11-01T22:26:04.740","2016-11-07T18:58:23.890","","","Rel-14","","","LTE_eCRSIM_eSUMIMO","","","","","","","","",""]
["R4-1609094","On interruption requirments for SRS carrier based switching","Intel Corporation","Yang Tang","56725","discussion","Discussion","---","","291","8.21.3","RRM core and performance (36.133) [LTE_SRS_switch-Core/Perf]",9094000,"noted","2016-11-01T22:26:04.757","2016-11-07T18:58:23.907","","","Rel-14","","","","","","","","","","","",""]
["R4-1609095","On SRS switching and measurement gap","Intel Corporation","Yang Tang","56725","discussion","Discussion","---","","291","8.21.3","RRM core and performance (36.133) [LTE_SRS_switch-Core/Perf]",90950000,"noted","2016-11-01T22:26:04.787","2016-11-07T18:58:23.907","","","Rel-14","","","","","","","","","","","",""]
["R4-1609096","WF on RRM for SRS carrier based switching","Intel Corporation","Yang Tang","56725","discussion","Approval","---","","291","8.21.3","RRM core and performance (36.133) [LTE_SRS_switch-Core/Perf]",909600000,"noted","2016-11-01T22:26:04.803","2016-11-07T18:58:23.923","","","Rel-14","","","","","","","","","","","",""]
["R4-1609097","On RACH requirement for SRS carrier based switching","Intel Corporation","Yang Tang","56725","discussion","Approval","---","","291","8.21.3","RRM core and performance (36.133) [LTE_SRS_switch-Core/Perf]",90970000,"noted","2016-11-01T22:26:04.817","2016-11-07T18:58:23.923","","","Rel-14","","","","","","","","","","","",""]
["R4-1609098","Draft LS on UE behavior during SRS switching","Intel Corporation","Yang Tang","56725","LS out","Approval","---","","291","8.21.3","RRM core and performance (36.133) [LTE_SRS_switch-Core/Perf]",909800000,"withdrawn","2016-11-01T22:26:04.850",null,"","","Rel-14","","","","","","","","","","","",""]
["R4-1609099","On interruption during HO for further mobility enhancement","Intel Corporation","Yang Tang","56725","discussion","Discussion","---","","327","8.26.3","RRM core (36.133) [LTE_eMob-Core]",909900000,"noted","2016-11-01T22:26:04.867","2016-11-07T18:58:23.923","","","Rel-14","","","","","","","","","","","",""]
["R4-1609100","LS on interruption during HO for make-before-break","Intel Corporation","Yang Tang","56725","LS out","Approval","---","","327","8.26.3","RRM core (36.133) [LTE_eMob-Core]",974800000,"noted","2016-11-01T22:26:04.880","2016-11-07T18:58:23.923","","","Rel-14","","","","","","","","","","","",""]
["R4-1609101","On OTDOA measurement for further indoor positioning enhancements","Intel Corporation","Yang Tang","56725","discussion","Discussion","---","","297","8.22.3.1","OTDOA/E-CID enhancement [UTRA_LTE_iPos_enh2]",73000,"noted","2016-11-01T22:26:04.913","2016-11-07T18:58:23.937","","","Rel-14","","","","","","","","","","","",""]
["R4-1609102","On UE requirement in IDLE mode for Cat1 1Rx","Intel Corporation","Yang Tang","56725","discussion","Discussion","---","","334","8.27.3","RRM core (36.133) [LTE_UE_cat_1RX-Core]",43000,"noted","2016-11-01T22:26:04.927","2016-11-07T18:58:23.937","","","Rel-14","","","","","","","","","","","",""]
["R4-1609103","On cell identification, measurement and accuracy requirement for Cat1 1Rx","Intel Corporation","Yang Tang","56725","discussion","Discussion","---","","334","8.27.3","RRM core (36.133) [LTE_UE_cat_1RX-Core]",44000,"noted","2016-11-01T22:26:04.943","2016-11-07T18:58:23.953","","","Rel-14","","","","","","","","","","","",""]
["R4-1609104","Further discussion on ECID positioning for NB-IoT","Intel Corporation","Yang Tang","56725","discussion","Discussion","---","","307","8.24.3.1.1","E-CID  [NB_IOTenh-Core]",840000,"noted","2016-11-01T22:26:04.973","2016-11-07T18:58:23.953","","","Rel-14","","","","","","","","","","","",""]
["R4-1609105","LS on ECID measurement quantity for NB-IoT","Intel Corporation","Yang Tang","56725","LS out","Approval","---","","307","8.24.3.1.1","E-CID  [NB_IOTenh-Core]",8600000,"revised","2016-11-01T22:26:04.990","2016-11-07T18:58:23.953","","R4-1610697","Rel-14","","","","","","","","","","","",""]
["R4-1609106","Wayforward on ECID positioning for NB-IoT","Intel Corporation","Yang Tang","56725","discussion","Approval","---","","306","8.24.3.1","Positioning [NB_IOTenh-Core]",9106000,"noted","2016-11-01T22:26:05.020","2016-11-07T18:58:23.970","","","Rel-14","","","","","","","","","","","",""]
["R4-1609107","Reference receiver performance for bidirectional HST SFN","Intel Corporation","Yang Tang","56725","other","Discussion","---","","345","8.28.3.1","Enhancement for bi-directional RRH arrangement [LTE_high_speed]",947000000,"noted","2016-11-01T22:26:05.037","2016-11-07T21:57:54.637","","","Rel-14","36.101","","LTE_high_speed","","","","","","","","",""]
["R4-1609108","Discussion on HST CSI","Intel Corporation","Yang Tang","56725","other","Discussion","---","","347","8.28.3.3","CQI reporting [LTE_high_speed]",71400000,"noted","2016-11-01T22:26:05.067","2016-11-07T21:57:54.637","","","Rel-14","36.101","","LTE_high_speed","","","","","","","","",""]
["R4-1609109","NPBCH Demodulation Performance","Intel Corporation","Yang Tang","56725","other","Discussion","---","","129","6.3.4.1.1","NPBCH  [NB_IOT-Perf]",5360000,"noted","2016-11-01T22:26:05.083","2016-11-07T21:57:54.637","","","Rel-13","36.101","","NB_IOT-Perf","","","","","","","","",""]
["R4-1609110","NPDCCH Demodulation Performance","Intel Corporation","Yang Tang","56725","other","Discussion","---","","130","6.3.4.1.2","NPDCCH [NB_IOT-Perf]",53700000,"noted","2016-11-01T22:26:05.100","2016-11-07T21:57:54.637","","","Rel-13","36.101","","NB_IOT-Perf","","","","","","","","",""]
["R4-1609111","NPDSCH Demodulation Performance","Intel Corporation","Yang Tang","56725","other","Discussion","---","","131","6.3.4.1.3","NPDSCH [NB-IOT-Perf]",53800000,"noted","2016-11-01T22:26:05.130","2016-11-07T21:57:54.637","","","Rel-13","36.101","","NB_IOT-Perf","","","","","","","","",""]
["R4-1609112","Discussion on SI acquisition delay for NB-IoT","Intel Corporation","Yang Tang","56725","other","Discussion","---","","56","5.6.4","RRM core (36.133)  [NB_IOT-Core]",911200000,"noted","2016-11-01T22:26:05.147","2016-11-07T21:57:54.650","","","Rel-13","36.101","","NB_IOT-Perf","","","","","","","","",""]
["R4-1609113","MIB acquisition delay simulation results for eMTC RRM","Intel Corporation","Yang Tang","56725","discussion","","---","","48","5.5.3.1","Evaluation of MIB and SIB reading delay, and update of requirement for handover and RRC Re-establishment [LTE_MTCe2_L1-Core]",550000,"noted","2016-11-01T22:26:05.177","2016-11-07T18:58:23.970","","","Rel-13","","","","","","","","","","","",""]
["R4-1609114","Simulations results for MPBCH demod","Intel Corporation","Yang Tang","56725","discussion","","---","","97","6.1.2.1","PBCH [LTE_MTCe2_L1-Perf]",916800000,"noted","2016-11-01T22:26:05.193","2016-11-07T18:58:23.970","","","Rel-13","","","","","","","","","","","",""]
["R4-1609115","CR on eMTC PBCH requirements correction","Intel Corporation","Yang Tang","56725","CR","","---","","97","6.1.2.1","PBCH [LTE_MTCe2_L1-Perf]",946500000,"revised","2016-11-01T22:26:05.223","2016-11-07T18:58:23.970","","R4-1610887","Rel-13","36.101","13.5.0","","3974","","F","","","","","",""]
["R4-1609116","MPDCCH simulation results for discussion","Intel Corporation","Yang Tang","56725","discussion","","---","","98","6.1.2.2","MPDCCH [LTE_MTCe2_L1-Perf]",966400000,"noted","2016-11-01T22:26:05.333","2016-11-07T18:58:23.983","","","Rel-13","","","","","","","","","","","",""]
["R4-1609117","MPDSCH simulation results for discussion","Intel Corporation","Yang Tang","56725","discussion","","---","","99","6.1.2.3","MPDSCH [LTE_MTCe2_L1-Perf]",968400000,"noted","2016-11-01T22:26:05.347","2016-11-07T18:58:23.983","","","Rel-13","","","","","","","","","","","",""]
["R4-1609118","On per-CC based measurement gap enhancement","Intel Corporation","Yang Tang","56725","other","Discussion","---","","351","8.29.2","RRM core (36.133) [LTE_meas_gap_enh-Core]",9120000,"noted","2016-11-01T22:26:05.380","2016-11-07T18:58:24","","","","","","","","","","","","","","",""]
["R4-1609119","WF on measurement gap enhancement","Intel Corporation","Yang Tang","56725","other","Approval","---","","350","8.29.1","General [LTE_meas_gap_enh-Core]",911800000,"revised","2016-11-01T22:26:05.397","2016-11-19T17:47:25.163","","R4-1610691","","","","","","","","","","","","",""]
["R4-1609120","Core requirements for measurement gap enhancement","Intel Corporation","Yang Tang","56725","other","Discussion","---","","351","8.29.2","RRM core (36.133) [LTE_meas_gap_enh-Core]",954800001,"noted","2016-11-01T22:26:05.427","2016-11-07T18:58:24","","","","","","","","","","","","","","",""]
["R4-1609121","Draft LS on measurement gap enhancement","Intel Corporation","Yang Tang","56725","LS out","Approval","---","","351","8.29.2","RRM core (36.133) [LTE_meas_gap_enh-Core]",954500000,"revised","2016-11-01T22:26:05.443","2016-11-07T18:58:24","","R4-1610690","","","","","","","","","","","","",""]
["R4-1609122","NR RF parameters and template for WP5D","Intel Corporation","Yang Tang","56725","other","Approval","---","","411","11.3.2","RF parameters not related co-existence [FS_NR_newRAT]",912200000,"noted","2016-11-01T22:26:05.473","2016-11-07T18:58:24.017","","","","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1609123","NF values in ITU-R WP5D related coexistence simulations","Intel Corporation","Yang Tang","56725","other","Approval","---","","410","11.3.1","Co-existence [FS_NR_newRAT]",949700000,"noted","2016-11-01T22:26:05.490","2016-11-07T18:58:24.017","","","","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1609124","3GPP MIMO OTA data template for performance requirement phase","ROHDE & SCHWARZ","Thorsten Hertel","60675","discussion","Approval","This updated spreadsheet presents a data template to be used during the upcoming performance requirement phase. The substitution approach with the maximum downlink RS-EPRE and the updated reference coordinate system/device orientation have been taken into","","222","8.14.1","General [LTE_MIMO_OTA-Core]",32100000,"revised","2016-11-02T00:58:19.850","2016-11-07T16:10:00.287","","R4-1610783","Rel-14","37.977","","","","","","","","","","",""]
["R4-1609125","Proposal for maximum downlink RS-EPRE","ROHDE & SCHWARZ","Thorsten Hertel","60675","discussion","Approval","The substitution value of the maximum downlink RS EPRE has not been defined and was considered an open action item of the performance requirement framework. This contribution proposes a value suitable for the UMi channel model","","222","8.14.1","General [LTE_MIMO_OTA-Core]",53000000,"noted","2016-11-02T01:04:22.847","2016-11-07T16:05:17.083","","","Rel-14","37.977","","","","","","","","","","",""]
["R4-1609126","Status of alignment and harmonization devices","ROHDE & SCHWARZ","Thorsten Hertel","60675","discussion","Discussion","This contribution provides the status of the alignment work and harmonization devices.","","222","8.14.1","General [LTE_MIMO_OTA-Core]",78400000,"noted","2016-11-02T02:19:14.727","2016-11-07T16:07:38.420","","","Rel-14","37.977","","","","","","","","","","",""]
["R4-1609127","TP for TR 36.714-03-01: operating bands, channel bandwidths, co-existence studies for CA_1C-3A_BCS0","China Unicom","Hu Rongyi","70322","pCR","","---","","159","8.3.2","UE RF (36.101) [LTE_CA_R14_3DL1UL-Core]",76000000,"approved","2016-11-02T04:59:33.280","2016-11-02T05:22:25.037","","","","36.714-03-01","0.4.0","LTE_CA_R14_3DL1UL","","","B","","","","","",""]
["R4-1609128","TP for TR 36.714-03-01: ?TIB and ?RIB values and REFSENS requirements for CA_1C-3A _BCS0","China Unicom","Hu Rongyi","70322","pCR","","---","","159","8.3.2","UE RF (36.101) [LTE_CA_R14_3DL1UL-Core]",76100000,"approved","2016-11-02T05:08:29.453","2016-11-02T05:22:25.053","","","","36.714-03-01","0.4.0","LTE_CA_R14_3DL1UL","","","B","","","","","",""]
["R4-1609129","TP for TR36.714-02-01: the support of CA_8A-41A BCS1","SoftBank Corp., APT, MTI, Sharp","Kenichi Kihara","41094","pCR","Approval","This paper is to complete 8A-41A BCS1. (Revision: add supporting IMs)","","153","8.2.2","UE RF (36.101) [LTE_CA_R14_2DL1UL-Core]",912900000,"approved","2016-11-02T05:52:50.643","2016-11-02T08:10:39.257","R4-1609046","","","36.714-02-01","0.4.0","LTE_CA_R14_2DL1UL-Core","","","","","","","","",""]
["R4-1609130","TP for TR36.714-02-01: the support of CA_28A-41A BCS1","SoftBank Corp., APT, MTI, Sharp","Kenichi Kihara","41094","pCR","Approval","This paper is to complete 28A-41A BCS1. (Revision: Add supporting IMs)","","153","8.2.2","UE RF (36.101) [LTE_CA_R14_2DL1UL-Core]",913000000,"approved","2016-11-02T05:55:15.580","2016-11-02T08:10:57.617","R4-1609047","","","36.714-02-01","0.4.0","LTE_CA_R14_2DL1UL-Core","","","","","","","","",""]
["R4-1609131","TP for TR36.714-03-01: the support of CA_8A-28A-41A BCS0","SoftBank Corp., APT, MTI, Sharp","Kenichi Kihara","41094","pCR","Approval","This paper is to complete 3DL/1UL of 8A-28A-41A.","","159","8.3.2","UE RF (36.101) [LTE_CA_R14_3DL1UL-Core]",76200000,"approved","2016-11-02T05:57:08.307","2016-11-02T08:11:15.167","R4-1609048","","","36.714-03-01","0.4.0","","","","","","","","","",""]
["R4-1609132","Correction of frequency error for category M1","Intel Corporation","Yang Tang","56725","CR","Agreement","---","","45","5.5.1","UE RF (36.101)  [LTE_MTCe2_L1-Core]",4970000,"noted","2016-11-02T06:49:06.013","2016-11-07T22:52:33.787","","","Rel-13","36.101","13.5.0","LTE_MTCe2_L1-Core","3975","","F","","","","","",""]
["R4-1609133","Correction of frequency error for category M1","Intel Corporation","Yang Tang","56725","CR","Agreement","---","","45","5.5.1","UE RF (36.101)  [LTE_MTCe2_L1-Core]",5080000,"withdrawn","2016-11-02T06:49:06.137",null,"","","Rel-14","36.101","14.1.0","LTE_MTCe2_L1-Core","3976","","A","","","","","",""]
["R4-1609134","Correction of power control for category M1","Intel Corporation","Yang Tang","56725","CR","Agreement","---","","45","5.5.1","UE RF (36.101)  [LTE_MTCe2_L1-Core]",913200000,"revised","2016-11-02T06:49:06.247","2016-11-07T22:52:33.803","","R4-1610848","Rel-13","36.101","13.5.0","LTE_MTCe2_L1-Core","3977","","F","","","","","",""]
["R4-1609135","Correction of power control for category M1","Intel Corporation, Ericsson, Qualcomm, Sony, Sierra Wireless, Verizon Wireless","Yang Tang","56725","CR","Agreement","---","","45","5.5.1","UE RF (36.101)  [LTE_MTCe2_L1-Core]",913300000,"agreed","2016-11-02T06:49:06.340","2016-11-19T17:47:25.193","","","Rel-14","36.101","14.1.0","LTE_MTCe2_L1-Core","3978","","A","RP-162430","","","","",""]
["R4-1609136","Summary of eMTC MIB acquisition delay simulation results","Intel Corporation","Yang Tang","56725","discussion","Discussion","---","","48","5.5.3.1","Evaluation of MIB and SIB reading delay, and update of requirement for handover and RRC Re-establishment [LTE_MTCe2_L1-Core]",2220000,"revised","2016-11-02T06:49:06.467","2016-11-07T22:52:33.803","","R4-1610652","Rel-13","","","LTE_MTCe2_L1-Core","","","","","","","","",""]
["R4-1609137","CR on cell re-selection test case for Cat-M1 in normal coverage","Intel Corporation","Yang Tang","56725","CR","Agreement","---","","85","6.1.1.2.5","Others  [LTE_MTCe2_L1-Perf]",913700000,"revised","2016-11-02T06:49:06.483","2016-11-07T22:52:33.817","","R4-1610869","Rel-13","36.133","13.5.0","LTE_MTCe2_L1-Perf","4162","","F","","","","","",""]
["R4-1609138","CR on cell re-selection test case for Cat-M1 in normal coverage","Intel Corporation","Yang Tang","56725","CR","Agreement","---","","85","6.1.1.2.5","Others  [LTE_MTCe2_L1-Perf]",913800000,"revised","2016-11-02T06:49:06.577",null,"","R4-1610870","Rel-14","36.133","14.1.0","LTE_MTCe2_L1-Perf","4163","","A","","","","","",""]
["R4-1609139","CR on cell re-selection test case for Cat-M1 in extended coverage","Intel Corporation","Yang Tang","56725","CR","Agreement","---","","87","6.1.1.3.1","Intra-frequency Cell Re-Selection [LTE_MTCe2_L1-Perf]",41000000,"noted","2016-11-02T06:49:06.683","2016-11-07T22:52:33.847","","","Rel-13","36.133","13.5.0","LTE_MTCe2_L1-Perf","4164","","F","","","","","",""]
["R4-1609140","CR on cell re-selection test case for Cat-M1 in extended coverage","Intel Corporation","Yang Tang","56725","CR","Agreement","---","","87","6.1.1.3.1","Intra-frequency Cell Re-Selection [LTE_MTCe2_L1-Perf]",41100000,"withdrawn","2016-11-02T06:49:06.763",null,"","","Rel-14","36.133","14.1.0","LTE_MTCe2_L1-Perf","4165","","A","","","","","",""]
["R4-1609141","CR on RRC re-establishment test case for Cat-M1 in CE Mode A","Intel Corporation","Yang Tang","56725","CR","Agreement","---","","84","6.1.1.2.4","RRC Re-establishment [LTE_MTCe2_L1-Perf]",914100000,"revised","2016-11-02T06:49:06.857","2016-11-07T22:52:33.880","","R4-1610867","Rel-13","36.133","13.5.0","LTE_MTCe2_L1-Perf","4166","","F","","","","","",""]
["R4-1609142","CR on RRC re-establishment test case for Cat-M1 in CE Mode A","Intel Corporation","Yang Tang","56725","CR","Agreement","---","","84","6.1.1.2.4","RRC Re-establishment [LTE_MTCe2_L1-Perf]",914200000,"revised","2016-11-02T06:49:06.950","2016-11-19T17:47:25.210","","R4-1610868","Rel-14","36.133","14.1.0","LTE_MTCe2_L1-Perf","4167","","A","","","","","",""]
["R4-1609143","CR on RRC re-establishment test case for Cat-M1 in CE Mode B","Intel Corporation","Yang Tang","56725","CR","Agreement","---","","89","6.1.1.3.3","RRC Re-establishment [LTE_MTCe2_L1-Perf]",6200000,"revised","2016-11-02T06:49:07.060","2016-11-07T22:52:33.897","","R4-1610890","Rel-13","36.133","13.5.0","LTE_MTCe2_L1-Perf","4168","","F","","","","","",""]
["R4-1609144","CR on RRC re-establishment test case for Cat-M1 in CE Mode B","Intel Corporation","Yang Tang","56725","CR","Agreement","---","","89","6.1.1.3.3","RRC Re-establishment [LTE_MTCe2_L1-Perf]",6300000,"agreed","2016-11-02T06:49:07.167","2016-11-19T17:47:25.223","","","Rel-14","36.133","14.1.0","LTE_MTCe2_L1-Perf","4169","","A","RP-162382","","","","",""]
["R4-1609145","Correction of transmit timing for NB-IoT","Intel Corporation, Nokia, Alcatel-Lucent Shanghai Bell","Yang Tang","56725","CR","Agreement","---","","56","5.6.4","RRM core (36.133)  [NB_IOT-Core]",3800000,"agreed","2016-11-02T06:49:07.277","2016-11-07T22:52:33.910","","","Rel-14","36.133","14.1.0","NB_IOT-Core","4170","","A","RP-162433","","","","",""]
["R4-1609146","Summary of NB-IoT SI acquisition delay simulation results","Intel Corporation","Yang Tang","56725","discussion","Discussion","---","","56","5.6.4","RRM core (36.133)  [NB_IOT-Core]",914600000,"revised","2016-11-02T06:49:07.417","2016-11-07T22:52:33.927","","R4-1610547","Rel-13","36.133","","NB_IOT-Perf","","","","","","","","",""]
["R4-1609147","CR on cell re-selection test case for Cat-NB1 in normal coverage","Intel Corporation","Yang Tang","56725","CR","Agreement","---","","120","6.3.3.3","Cell Re-selection test [NB_IOT-Perf]",2280000,"noted","2016-11-02T06:49:07.433","2016-11-07T22:52:33.943","","","Rel-13","36.133","13.5.0","NB_IOT-Perf","4171","","F","","","","","",""]
["R4-1609148","CR on cell re-selection test case for Cat-NB1 in normal coverage","Intel Corporation","Yang Tang","56725","CR","Agreement","---","","120","6.3.3.3","Cell Re-selection test [NB_IOT-Perf]",2290000,"withdrawn","2016-11-02T06:49:07.527",null,"","","Rel-14","36.133","14.1.0","NB_IOT-Perf","4172","","A","","","","","",""]
["R4-1609149","On repetition level feedback for FeMTC","Intel Corporation","Yang Tang","56725","discussion","Discussion","---","","320","8.25.3.2.2","RLM  [LTE_feMTC-Core]",2510000,"noted","2016-11-02T06:49:07.637","2016-11-07T22:52:33.943","","","Rel-14","","","LTE_feMTC-Core","","","","","","","","",""]
["R4-1609150","On PBCH demodulation performance and possible solutions","Intel Corporation","Yang Tang","56725","discussion","Discussion","---","","323","8.25.4","Other specifications [LTE_feMTC-Core]",915000000,"noted","2016-11-02T06:49:07.667","2016-11-07T22:52:33.957","","","Rel-14","","","LTE_feMTC-Core","","","","","","","","",""]
["R4-1609151","LS to RAN1, RAN2 on PBCH demodulation performance","Intel Corporation","Yang Tang","56725","LS out","Approval","---","","323","8.25.4","Other specifications [LTE_feMTC-Core]",915100000,"revised","2016-11-02T06:49:07.683","2016-11-07T22:52:33.973","","R4-1610670","Rel-14","","","LTE_feMTC-Core","","","","","","RAN1, RAN2","","",""]
["R4-1609152","On repetition level feedback for eNB-IoT","Intel Corporation","Yang Tang","56725","discussion","Discussion","---","","309","8.24.3.2","Mobility enhancement [NB_IOTenh-Core]",46000,"noted","2016-11-02T06:49:07.697","2016-11-07T22:52:33.990","","","Rel-14","","","NB_IOTenh-Core","","","","","","","","",""]
["R4-1609153","On NPBCH demodulation performance and possible solutions","Intel Corporation","Yang Tang","56725","discussion","Discussion","---","","310","8.24.4","Other specifications [NB_IOTenh-Core]",915300000,"noted","2016-11-02T06:49:07.713","2016-11-07T22:52:34.003","","","Rel-14","","","NB_IOTenh-Core","","","","","","","","",""]
["R4-1609154","LS to RAN1, RAN2 on NPBCH demodulation performance","Intel Corporation","Yang Tang","56725","LS out","Approval","---","","310","8.24.4","Other specifications [NB_IOTenh-Core]",915400000,"revised","2016-11-02T06:49:07.747","2016-11-07T22:52:34.020","","R4-1610699","Rel-14","","","NB_IOTenh-Core","","","","","","","","",""]
["R4-1609155","Lab alignment test plan","Intel Corporation","Yang Tang","56725","other","Approval","---","","223","8.14.2","Performance requirements [LTE_MIMO_OTA-Core]",7860000,"revised","2016-11-02T06:49:07.760","2016-11-07T22:52:34.037","","R4-1610786","Rel-14","","","LTE_MIMO_OTA-Core","","","","","","","","",""]
["R4-1609156","MIMO OTA evening adhoc minutes","Intel Corporation","Yang Tang","56725","report","Approval","---","","222","8.14.1","General [LTE_MIMO_OTA-Core]",7830000,"approved","2016-11-02T06:49:07.777","2016-11-19T17:47:25.223","","","Rel-14","","","LTE_MIMO_OTA-Core","","","","","","","","",""]
["R4-1609157","MIMO OTA Way Forward","Intel Corporation","Yang Tang","56725","other","Approval","---","","222","8.14.1","General [LTE_MIMO_OTA-Core]",32000000,"approved","2016-11-02T06:49:07.807","2016-11-19T17:47:25.240","","","Rel-14","","","LTE_MIMO_OTA-Core","","","","","","","","",""]
["R4-1609158","Max output power test considerations","Intel Corporation, CATR","Yang Tang","56725","discussion","Discussion","---","","419","11.5.2.3","Testability [FS_NR_newRAT]",9158000,"noted","2016-11-02T06:49:07.823","2016-11-07T22:52:34.050","","","Rel-14","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1609159","REFSENS test considerations","Intel Corporation, CATR","Yang Tang","56725","discussion","Discussion","---","","419","11.5.2.3","Testability [FS_NR_newRAT]",9858000,"noted","2016-11-02T06:49:07.840","2016-11-07T22:52:34.050","","","Rel-14","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1609160","On test interface for NR UE","Intel Corporation, CATR","Yang Tang","56725","discussion","Discussion","---","","419","11.5.2.3","Testability [FS_NR_newRAT]",916200000,"noted","2016-11-02T06:49:07.853","2016-11-07T22:52:34.083","","","Rel-14","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1609161","Skeleton TR on NR UE testability","Intel Corporation, CATR","Yang Tang","56725","discussion","Discussion","---","","419","11.5.2.3","Testability [FS_NR_newRAT]",980900000,"withdrawn","2016-11-02T06:49:07.887",null,"","","Rel-14","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1609162","Way Forward on NR UE testability","Intel Corporation, CATR","Yang Tang","56725","other","Approval","---","","419","11.5.2.3","Testability [FS_NR_newRAT]",981800000,"revised","2016-11-02T06:49:07.900","2016-11-19T17:47:25.240","","R4-1610926","Rel-14","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1609163","On test interface for NR RRM","Intel Corporation, CATR","Yang Tang","56725","discussion","Discussion","---","","426","11.6.1.2","Testability [FS_NR_newRAT]",916300000,"available","2016-11-02T06:49:07.917","2016-11-07T22:52:34.083","","","Rel-14","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1609164","On RRM testability","Intel Corporation, CATR","Yang Tang","56725","discussion","Discussion","---","","426","11.6.1.2","Testability [FS_NR_newRAT]",916400000,"noted","2016-11-02T06:49:07.947","2016-11-07T22:52:34.097","","","Rel-14","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1609165","Way Forward on RRM testability","Intel Corporation, CATR","Yang Tang","56725","other","Approval","---","","426","11.6.1.2","Testability [FS_NR_newRAT]",0,"withdrawn","2016-11-02T06:49:07.963",null,"","","Rel-14","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1609166","Motivation for the new WID on UE requirements for transmit antenna selection","Intel Corporation","Yang Tang","56725","discussion","Discussion","---","","430","13","Revision of the Work Plan",3510000,"available","2016-11-02T06:49:07.997","2016-11-07T22:52:34.113","","","Rel-14","","","","","","","","","","","",""]
["R4-1609167","New WID: UE requirements for transmit antenna selection","Intel Corporation","Yang Tang","56725","WID new","Discussion","---","","430","13","Revision of the Work Plan",3520000,"available","2016-11-02T06:49:08.010","2016-11-07T22:52:34.113","","","Rel-14","","","","","","","","","","","",""]
["R4-1609168","CR on eMTC PBCH requirements correction","Intel Corporation","Yang Tang","56725","CR","Agreement","---","","97","6.1.2.1","PBCH [LTE_MTCe2_L1-Perf]",968200000,"withdrawn","2016-11-02T06:49:08.027",null,"","","Rel-14","36.101","14.1.0","","3979","","A","","","","","",""]
["R4-1609169","Discussion on multiple unlicensed carrier extension in Rel-14 LAA demodulation","Ericsson","Shaohua Li","45543","discussion","Discussion","Discussion on multiple unlicensed carrier extension in Rel-14 LAA demodulation","","107","6.2.4.1","General [LTE_LAA-Perf]",917500000,"noted","2016-11-02T08:43:06.497","2016-11-05T14:29:05.277","","","","","","LTE_LAA-Perf","","","","","","","","",""]
["R4-1609170","Clean up and clarification for LAA CSI requirements","Ericsson","Shaohua Li","45543","CR","Approval","clean up and make some clarification for LAA CSI requirements","","110","6.2.5","UE CSI reporting (36.101) [LTE_LAA-Perf]",917100000,"revised","2016-11-02T08:43:06.527","2016-11-05T14:29:05.277","","R4-1610644","Rel-13","36.101","13.5.0","LTE_LAA-Perf","3980","","F","","","","","",""]
["R4-1609171","Clean up and clarification for LAA CSI requirements","Ericsson","Shaohua Li","45543","CR","Approval","clean up and make some clarification for LAA CSI requirements","","110","6.2.5","UE CSI reporting (36.101) [LTE_LAA-Perf]",971000000,"revised","2016-11-02T08:43:06.637","2016-11-19T17:47:25.257","","R4-1611016","Rel-14","36.101","14.1.0","LTE_LAA-Perf","3981","","A","","","","","",""]
["R4-1609172","Add PDCCH performance requirements for LAA demodulation","Ericsson","Shaohua Li","45543","CR","Approval","Add PDCCH performance requirements for LAA demodulation","","109","6.2.4.3","PDCCH [LTE_LAA-Perf]",917200000,"revised","2016-11-02T08:43:06.730","2016-11-05T14:29:05.200","","R4-1610643","Rel-13","36.101","13.5.0","LTE_LAA-Perf","3982","","F","","","","","",""]
["R4-1609173","Add PDCCH performance requirements for LAA demodulation","Ericsson","Shaohua Li","45543","CR","Approval","Add PDCCH performance requirements for LAA demodulation","","109","6.2.4.3","PDCCH [LTE_LAA-Perf]",942900000,"agreed","2016-11-02T08:43:06.840","2016-11-19T17:47:25.270","","","Rel-14","36.101","14.1.0","LTE_LAA-Perf","3983","","A","RP-162386","","","","",""]
["R4-1609174","Discussion on the trigger transmission in LAA CSI requirements","Ericsson","Shaohua Li","45543","discussion","Discussion","Discussion on how to transmit the trigger in the CSI test","","110","6.2.5","UE CSI reporting (36.101) [LTE_LAA-Perf]",64400000,"noted","2016-11-02T08:43:06.933","2016-11-05T14:29:05.200","","","","","","LTE_LAA-Perf","","","","","","","","",""]
["R4-1609175","Simulation assumption for 10MHz LAA performance","Ericsson","Shaohua Li","45543","discussion","Approval","Provide simulation assumption for 10MHz LAA performance","","107","6.2.4.1","General [LTE_LAA-Perf]",942600000,"noted","2016-11-02T08:43:06.963","2016-11-05T14:29:05.230","","","","","","LTE_LAA-Perf","","","","","","","","",""]
["R4-1609176","Introduce performance requirements for LAA under 10MHz","Ericsson","Shaohua Li","45543","CR","Approval","Introduce performance requirements for LAA under 10MHz","","107","6.2.4.1","General [LTE_LAA-Perf]",942700000,"noted","2016-11-02T08:43:06.980","2016-11-05T14:29:05.230","","","Rel-14","36.101","14.1.0","LTE_LAA-Perf","3984","","B","","","","","",""]
["R4-1609177","Introduce CSI requirements for LAA under 10MHz","Ericsson","Shaohua Li","45543","CR","Approval","Introduce CSI requirements for LAA operation under 10MHz","","107","6.2.4.1","General [LTE_LAA-Perf]",971100000,"noted","2016-11-02T08:43:07.073","2016-11-05T14:29:05.247","","","Rel-14","36.101","14.1.0","LTE_LAA-Perf","3985","","B","","","","","",""]
["R4-1609178","LBT model for LAA with two or more LAA Scells in Rel-14","Ericsson","Shaohua Li","45543","discussion","Discussion","Provide LBT model for LAA with two or more LAA Scells","","107","6.2.4.1","General [LTE_LAA-Perf]",917700000,"noted","2016-11-02T08:43:07.167","2016-11-05T14:29:05.247","","","","","","LTE_LAA-Perf","","","","","","","","",""]
["R4-1609179","Overview on Rel-14 eLAA demodulation","Ericsson","Shaohua Li","45543","discussion","Discussion","Provide our view on eLAA demodulation","","257","8.18.6","UE/BS demodulation and CSI (36.101/36.104) [LTE_eLAA-Perf]",907300000,"noted","2016-11-02T08:43:07.183","2016-11-05T14:29:05.263","","","","","","LTE_eLAA-Perf","","","","","","","","",""]
["R4-1609180","Discussion on the open issues for V2V demodulation","Ericsson","Shaohua Li","45543","discussion","Discussion","Discussion on the open issues for V2V demodulation","","269","8.19.4.1","Single-link PSSCH and PSCCH  [LTE_SL_V2V-Perf]",952500000,"noted","2016-11-02T08:43:07.213","2016-11-05T14:29:05.293","","","","","","LTE_SL_V2V-Perf","","","","","","","","",""]
["R4-1609181","Simulation results summary for PDSCH for LAA requirements","Ericsson","Shaohua Li","45543","discussion","Discussion","summary simulation results for LAA PDSCH","","108","6.2.4.2","PDSCH [LTE_LAA-Perf]",13300000,"withdrawn","2016-11-02T08:43:07.230",null,"","","","","","LTE_LAA-Perf","","","","","","","","",""]
["R4-1609182","Revised WID: Basket WI for LTE Advanced inter-band CA Rel-14 for 4DL/1UL","Ericsson","Per Lindell","56972","WID revised","Endorsement","Revised WID: Basket WI for LTE Advanced inter-band CA Rel-14 for 4DL/1UL, including new updates compared to approved version at RAN 73","","164","8.4.1","Rapporteur Input (WID/CRs) [LTE_CA_R14_4DL1UL-Core]",918800000,"agreed","2016-11-02T13:53:15.737","2016-11-22T12:17:26.813","","","Rel-14","36.714-04-01","0.2.0","LTE_CA_R14_4DL1UL-Core","","","","","","","","",""]
["R4-1609183","Revised WID: Basket WI for LTE Advanced Intra-band CA","Ericsson","Per Lindell","56972","WID revised","Endorsement","Revised WID: Basket WI for LTE Advanced Intra-band CA, including new updates compared to approved version at RAN 73","","146","8.1.1","Rapporteur Input (WID/CRs) [LTE_CA_R14_intra-Core]",919100000,"endorsed","2016-11-02T13:53:15.750","2016-11-22T12:17:26.877","","","Rel-14","36.714-00-00","0.2.0","LTE_CA_R14_intra-Core","","","","","","","","",""]
["R4-1609184","TR 4DL/1UL TR 36.714-04-01 version 0.4.0","Ericsson","Per Lindell","56972","draft TR","Approval","TR 4DL/1UL TR 36.714-04-01 version 0.4.0 including the approved TP's from RAN4 #80bis","","164","8.4.1","Rapporteur Input (WID/CRs) [LTE_CA_R14_4DL1UL-Core]",918200000,"approved","2016-11-02T13:53:15.767","2016-11-04T12:40:07.537","","","Rel-14","36.714-04-01","0.2.0","LTE_CA_R14_4DL1UL","","","","","","","","",""]
["R4-1609185","TR Intra-band TR 36.714-00-00 version 0.4.0","Ericsson","Per Lindell","56972","draft TR","Approval","TR Intra-band TR 36.714-00-00 version 0.4.0 including the approved TP's from RAN4 #80bis","","146","8.1.1","Rapporteur Input (WID/CRs) [LTE_CA_R14_intra-Core]",918300000,"approved","2016-11-02T13:53:16.390","2016-11-04T12:40:07.537","","","Rel-14","36.714-00-00","0.2.0","LTE_CA_R14_intra","","","","","","","","",""]
["R4-1609186","Introduction of additional band combinations for 4DL inter-band CA","Ericsson","Per Lindell","56972","CR","Endorsement","Introduction of Rel-14 4DL/1UL combinations in 36.101 (big CR)","","164","8.4.1","Rapporteur Input (WID/CRs) [LTE_CA_R14_4DL1UL-Core]",918400000,"agreed","2016-11-02T13:53:17.017","2016-11-22T12:17:26.877","","","Rel-14","36.101","14.1.0","LTE_CA_R14_4DL1UL-Core","3986","","B","RP-162401","","","","",""]
["R4-1609187","Introduction of additional band combinations for 4DL inter-band CA","Ericsson","Per Lindell","56972","CR","Endorsement","Introduction of Rel-14 4DL/1UL combinations in 36.104 (big CR)","","164","8.4.1","Rapporteur Input (WID/CRs) [LTE_CA_R14_4DL1UL-Core]",918600000,"agreed","2016-11-02T13:53:17.107","2016-11-22T12:17:26.877","","","Rel-14","36.104","14.1.0","LTE_CA_R14_4DL1UL-Core","0883","","B","RP-162401","","","","",""]
["R4-1609188","Introduction of Rel-14 4DL/1UL combinations in 36.141","Ericsson","Per Lindell","56972","CR","Endorsement","Introduction of Rel-14 4DL/1UL combinations in 36.141 (big CR)","","164","8.4.1","Rapporteur Input (WID/CRs) [LTE_CA_R14_4DL1UL-Core]",0,"agreed","2016-11-02T13:53:17.187","2016-11-22T12:17:26.877","","","Rel-14","36.141","14.1.0","LTE_CA_R14_4DL1UL","0918","","B","RP-162457","","","","",""]
["R4-1609189","Introduction of additional band combinations for Intra-band CA","Ericsson","Per Lindell","56972","CR","Endorsement","Introduction of Intra-band combinations in 36.101 (big CR)","","146","8.1.1","Rapporteur Input (WID/CRs) [LTE_CA_R14_intra-Core]",918500000,"agreed","2016-11-02T13:53:17.263","2016-11-22T12:17:26.893","","","Rel-14","36.101","14.1.0","LTE_CA_R14_intra-Core","3987","","B","RP-162398","","","","",""]
["R4-1609190","Introduction of additional band combinations for Intra-band CA","Ericsson","Per Lindell","56972","CR","Endorsement","Introduction of Intra-band combinations in 36.104 (big CR)","","146","8.1.1","Rapporteur Input (WID/CRs) [LTE_CA_R14_intra-Core]",918900000,"agreed","2016-11-02T13:53:17.343","2016-11-22T12:17:26.893","","","Rel-14","36.104","14.1.0","LTE_CA_R14_intra-Core","0884","","B","RP-162398","","","","",""]
["R4-1609191","Introduction of additional band combinations for Intra-band CA","Ericsson","Per Lindell","56972","CR","Endorsement","Introduction of Intra-band combinations in 36.141 (big CR)","","146","8.1.1","Rapporteur Input (WID/CRs) [LTE_CA_R14_intra-Core]",919000000,"agreed","2016-11-02T13:53:17.420","2016-11-22T12:17:26.893","","","Rel-14","36.141","14.1.0","LTE_CA_R14_intra-Core","0919","","B","RP-162398","","","","",""]
["R4-1609192","Requirements to complete the Intra-band CA combination 12A-12A","Ericsson, US Cellular","Per Lindell","56972","pCR","Approval","Requirements to complete the Intra-band CA combination 12A-12A","","147","8.1.2","UE RF (36.101) [LTE_CA_R14_intra-Core]",925300000,"approved","2016-11-02T13:53:17.513","2016-11-04T12:40:07.597","","","","36.714-00-00","0.2.0","LTE_CA_R14_intra-Core","","","","","","","","",""]
["R4-1609193","Requirements to complete the 3DL CA combination 2A-12A-12A","Ericsson, US Cellular","Per Lindell","56972","pCR","Approval","Channel bandwidth and insertion loss values to complete 3DL CA combination 2A-12A-12A","","159","8.3.2","UE RF (36.101) [LTE_CA_R14_3DL1UL-Core]",76300000,"revised","2016-11-02T13:53:17.530","2016-11-04T12:40:07.613","","R4-1610758","","36.714-03-01","0.4.0","LTE_CA_R14_3DL1UL-Core","","","","","","","","",""]
["R4-1609194","Requirements to complete the 3DL CA combination 4A-12A-12A","Ericsson, US Cellular","Per Lindell","56972","pCR","Approval","Channel bandwidth, insertion loss values and MSD to complete 3DL CA combination 4A-12A-12A","","159","8.3.2","UE RF (36.101) [LTE_CA_R14_3DL1UL-Core]",912700000,"revised","2016-11-02T13:53:17.547","2016-11-04T12:40:07.613","","R4-1610760","","36.714-03-01","0.4.0","LTE_CA_R14_3DL1UL-Core","","","","","","","","",""]
["R4-1609195","Requirements to complete the 3DL CA combination 5A-12A-12A","Ericsson, US Cellular","Per Lindell","56972","pCR","Approval","Channel bandwidth and insertion loss values to complete 3DL CA combination 5A-12A-12A","","159","8.3.2","UE RF (36.101) [LTE_CA_R14_3DL1UL-Core]",913100000,"revised","2016-11-02T13:53:17.560","2016-11-04T12:40:07.630","","R4-1610761","","36.714-03-01","0.4.0","LTE_CA_R14_3DL1UL-Core","","","","","","","","",""]
["R4-1609196","Requirements to complete the 3DL CA combination 5A-12A-66A","Ericsson, US Cellular","Per Lindell","56972","pCR","Approval","Channel bandwidth, insertion loss values and MSD to complete 3DL CA combination 5A-12A-66A","","159","8.3.2","UE RF (36.101) [LTE_CA_R14_3DL1UL-Core]",919400000,"revised","2016-11-02T13:53:17.577","2016-11-04T12:40:07.647","","R4-1610762","","36.714-03-01","0.4.0","LTE_CA_R14_3DL1UL-Core","","","","","","","","",""]
["R4-1609197","Requirements to complete the 3DL CA combination 12B-66A","Ericsson, US Cellular","Per Lindell","56972","pCR","Approval","Channel bandwidth, insertion loss values and MSD to complete 3DL CA combination 12B-66A","","159","8.3.2","UE RF (36.101) [LTE_CA_R14_3DL1UL-Core]",919600000,"revised","2016-11-02T13:53:17.607","2016-11-04T12:40:07.647","","R4-1610763","","36.714-03-01","0.4.0","LTE_CA_R14_3DL1UL-Core","","","","","","","","",""]
["R4-1609198","Requirements to complete the 4DL CA combination 2A-4A-12A-12A","Ericsson, US Cellular","Per Lindell","56972","pCR","Approval","Channel bandwidth, insertion loss values and MSD to complete 4DL CA combination 2A-4A-12A-12A","","165","8.4.2","UE RF (36.101) [LTE_CA_R14_4DL1UL-Core]",30400000,"noted","2016-11-02T13:53:17.623","2016-11-04T12:40:07.660","","","","36.714-04-01","0.2.0","LTE_CA_R14_4DL1UL-Core","","","","","","","","",""]
["R4-1609199","Requirements to complete the 4DL CA combination 4A-4A-12A-12A","Ericsson, US Cellular","Per Lindell","56972","pCR","Approval","Channel bandwidth, insertion loss values and MSD to complete 4DL CA combination 4A-4A-12A-12A","","165","8.4.2","UE RF (36.101) [LTE_CA_R14_4DL1UL-Core]",30500000,"noted","2016-11-02T13:53:17.640","2016-11-04T12:40:07.660","","","","36.714-04-01","0.2.0","LTE_CA_R14_4DL1UL-Core","","","","","","","","",""]
["R4-1609200","Requirements to complete the 4DL CA combination 4A-5A-12A-12A","Ericsson, US Cellular","Per Lindell","56972","pCR","Approval","Channel bandwidth, insertion loss values and MSD to complete 4DL CA combination 4A-5A-12A-12A","","165","8.4.2","UE RF (36.101) [LTE_CA_R14_4DL1UL-Core]",30600000,"noted","2016-11-02T13:53:17.653","2016-11-04T12:40:07.677","","","","36.714-04-01","0.2.0","LTE_CA_R14_4DL1UL-Core","","","","","","","","",""]
["R4-1609201","Requirements to complete the 3DL CA combination 40A-42C","Ericsson","Per Lindell","56972","pCR","Approval","Channel bandwidth and insertion loss values to complete 3DL CA combination 40A-42C","","159","8.3.2","UE RF (36.101) [LTE_CA_R14_3DL1UL-Core]",920100000,"approved","2016-11-02T13:53:17.670","2016-11-04T12:40:07.693","","","","36.714-03-01","0.4.0","LTE_CA_R14_3DL1UL-Core","","","","","","","","",""]
["R4-1609202","Requirements to complete the 3DL CA combination 40C-42A","Ericsson","Per Lindell","56972","pCR","Approval","Channel bandwidth and insertion loss values to complete 3DL CA combination 40C-42A","","159","8.3.2","UE RF (36.101) [LTE_CA_R14_3DL1UL-Core]",920200000,"approved","2016-11-02T13:53:17.700","2016-11-04T12:40:07.693","","","","36.714-03-01","0.4.0","LTE_CA_R14_3DL1UL-Core","","","","","","","","",""]
["R4-1609203","Requirements to complete the 4DL CA combination 40C-42C","Ericsson","Per Lindell","56972","pCR","Approval","Channel bandwidth and insertion loss values to complete 4DL CA combination 40C-42C","","165","8.4.2","UE RF (36.101) [LTE_CA_R14_4DL1UL-Core]",30700000,"approved","2016-11-02T13:53:17.717","2016-11-04T12:40:07.707","","","","36.714-04-01","0.2.0","LTE_CA_R14_4DL1UL-Core","","","","","","","","",""]
["R4-1609204","Requirements for eLAA dual uplink 2A-46A","Ericsson","Per Lindell","56972","pCR","Approval","Requirements for eLAA dual uplink 2A-46A","","247","8.18.2.4","Other requirements [LTE_eLAA-Core]",50200000,"revised","2016-11-02T13:53:17.733","2016-11-04T12:40:07.723","","R4-1610736","","36.714-02-02","0.4.0","LTE_eLAA-Core","","","","","","","","",""]
["R4-1609205","Requirements for eLAA dual uplink 3A-46A","Ericsson","Per Lindell","56972","pCR","Approval","Requirements for eLAA dual uplink 3A-46A","","247","8.18.2.4","Other requirements [LTE_eLAA-Core]",73700000,"revised","2016-11-02T13:53:17.763","2016-11-04T12:40:07.723","","R4-1610775","","36.714-02-02","0.4.0","LTE_eLAA-Core","","","","","","","","",""]
["R4-1609206","Requirements for eLAA dual uplink 7A-46A","Ericsson","Per Lindell","56972","pCR","Approval","Requirements for eLAA dual uplink 7A-46A","","247","8.18.2.4","Other requirements [LTE_eLAA-Core]",920400000,"revised","2016-11-02T13:53:17.780","2016-11-04T12:40:07.740","","R4-1610737","","36.714-02-02","0.4.0","LTE_eLAA-Core","","","","","","","","",""]
["R4-1609207","Requirements for eLAA dual uplink 46A-66A","Ericsson","Per Lindell","56972","pCR","Approval","Requirements for eLAA dual uplink 46A-66A","","247","8.18.2.4","Other requirements [LTE_eLAA-Core]",920600000,"approved","2016-11-02T13:53:17.797","2016-11-04T12:40:07.740","","","","36.714-02-02","0.4.0","LTE_eLAA-Core","","","","","","","","",""]
["R4-1609208","Public Safety LTE and Ultra High Definition TV(UHDTV) in Korea","Korea Testing Laboratory","Song Raphael","38072","discussion","Approval","---","","234","8.16.2","UE RF (36.101)  [LTE_HPUE_B3_B20_B28]",920800000,"noted","2016-11-02T14:29:54.960","2016-11-03T14:51:47.050","","","Rel-14","36.101","14.1.0","","","","","","","","","",""]
["R4-1609209","PCC and SCC assignment in 20MHz+10MHz test cases A.8.20.2B and A.9.2.27","ANRITSU LTD","Ian Rose","9381","CR","","This CR updates test cases A.8.20.2B and A.9.2.27 to also allow the PCell to be 10MHz Channel BW, and the SCell to be 20MHz Channel BW.","","14","4.2.3","RRM (Radio Resource Management)  [WI code or TEI12]",118000,"agreed","2016-11-02T14:35:23.047","2016-11-04T10:04:54.227","","R4-1610725","Rel-12","36.133","12.13.0","LTE_CA_B39_B41-Perf","4173","","F","RP-162415","","","","",""]
["R4-1609210","PCC and SCC assignment in 20MHz+10MHz test case A.8.20.2B and A.9.2.27","ANRITSU LTD","Ian Rose","9381","CR","","This CR updates test cases A.8.20.2B and A.9.2.27 to also allow the PCell to be 10MHz Channel BW, and the SCell to be 20MHz Channel BW.","","14","4.2.3","RRM (Radio Resource Management)  [WI code or TEI12]",119000,"agreed","2016-11-02T14:38:08.343","2016-11-19T17:47:25.303","","","Rel-13","36.133","13.5.0","LTE_CA_B39_B41-Perf","4174","","A","RP-162415","","","","",""]
["R4-1609211","PCC and SCC assignment in 20MHz+10MHz test case A.8.20.2B and A.9.2.27","ANRITSU LTD","Ian Rose","9381","CR","","This CR updates test cases A.8.20.2B and A.9.2.27 to also allow the PCell to be 10MHz Channel BW, and the SCell to be 20MHz Channel BW.","","14","4.2.3","RRM (Radio Resource Management)  [WI code or TEI12]",366000,"agreed","2016-11-02T14:41:12.157","2016-11-19T17:47:25.317","","","Rel-14","36.133","14.1.0","LTE_CA_B39_B41-Perf","4175","","A","RP-162415","","","","",""]
["R4-1609212","Alignment of CQI Index to Modulation coding scheme Mapping in Table A.4-15","ANRITSU LTD","Ian Rose","9381","CR","","Split Table A.4-15 into two separate tables, one for MCS.11A/ MCS.12A and one for MCS.11B/ MCS.12B.\nThis allows the Imcs values to correspond to the correct modulation scheme and coding rate.","","15","4.2.4","UE demodulation performance  [WI code or TEI12]",1270000,"withdrawn","2016-11-02T14:49:15.587",null,"","","Rel-12","36.101","12.13.0","LTE_SC_enh_L1-Perf","3988","","F","","","","","",""]
["R4-1609213","Alignment of CQI Index to Modulation coding scheme Mapping in Table A.4-15","ANRITSU LTD","Ian Rose","9381","CR","","Split Table A.4-15 into two separate tables, one for MCS.11A/ MCS.12A and one for MCS.11B/ MCS.12B.\nThis allows the Imcs values to correspond to the correct modulation scheme and coding rate.","","15","4.2.4","UE demodulation performance  [WI code or TEI12]",3720000,"withdrawn","2016-11-02T14:52:32.800",null,"","","Rel-13","36.101","13.5.0","LTE_SC_enh_L1-Perf","3989","","A","","","","","",""]
["R4-1609214","Alignment of CQI Index to Modulation coding scheme Mapping in Table A.4-15","ANRITSU LTD","Ian Rose","9381","CR","","Split Table A.4-15 into two separate tables, one for MCS.11A/ MCS.12A and one for MCS.11B/ MCS.12B.\nThis allows the Imcs values to correspond to the correct modulation scheme and coding rate.","","15","4.2.4","UE demodulation performance  [WI code or TEI12]",3730000,"withdrawn","2016-11-02T14:55:25.070",null,"","","Rel-14","36.101","14.1.0","LTE_SC_enh_L1-Perf","3990","","A","","","","","",""]
["R4-1609215","Remove redundant requirement for Intra-frequency relative CSI-RSRP","ANRITSU LTD","Ian Rose","9381","CR","","Remove redundant row specifying Normal condition +/-3dB accuracy.\nThe CR R4-167442 was endorsed at RAN4#80bis.","","14","4.2.3","RRM (Radio Resource Management)  [WI code or TEI12]",1210000,"withdrawn","2016-11-02T15:02:21.670",null,"","","Rel-12","36.101","12.13.0","LTE_SC_enh_L1-Core","3991","","F","","","","","",""]
["R4-1609216","Remove redundant requirement for Intra-frequency relative CSI-RSRP","Anritsu, Ericsson, ZTE, LGE","Ian Rose","9381","CR","","Remove redundant row specifying Normal condition +/-3dB accuracy.\nThe CR R4-167442 was endorsed at RAN4#80bis.","","14","4.2.3","RRM (Radio Resource Management)  [WI code or TEI12]",900000,"agreed","2016-11-02T15:05:46.217","2016-11-04T11:34:42.450","","","Rel-12","36.133","12.13.0","LTE_SC_enh_L1-Core","4176","","F","RP-162418","","","","",""]
["R4-1609217","Remove redundant requirement for Intra-frequency relative CSI-RSRP","Anritsu, Ericsson, ZTE, LGE","Ian Rose","9381","CR","","Remove redundant row specifying Normal condition +/-3dB accuracy.\nThe CR R4-167442 was endorsed at RAN4#80bis.","","14","4.2.3","RRM (Radio Resource Management)  [WI code or TEI12]",910000,"agreed","2016-11-02T15:10:35.427","2016-11-19T17:47:25.317","","","Rel-13","36.133","13.5.0","LTE_SC_enh_L1-Core","4177","","A","RP-162418","","","","",""]
["R4-1609218","Remove redundant requirement for Intra-frequency relative CSI-RSRP","Anritsu, Ericsson, ZTE, LGE","Ian Rose","9381","CR","","Remove redundant row specifying Normal condition +/-3dB accuracy.\nThe CR R4-167442 was endorsed at RAN4#80bis.","","14","4.2.3","RRM (Radio Resource Management)  [WI code or TEI12]",1200000,"agreed","2016-11-02T15:12:54.030","2016-11-19T17:47:25.333","","","Rel-14","36.133","14.1.0","LTE_SC_enh_L1-Core","4178","","A","RP-162418","","","","",""]
["R4-1609219","Scenarios and assumptions for NR in-band emission, EVM and in-band selectivity requirements with different numerologies","Nokia, Alcatel-Lucent Shanghai Bell","Tuomo Säynäjäkangas","69937","discussion","Approval","Propose scenarios and assumptions for developing the first phase NR requirements for DL and UL in-band emission, EVM and in-band Rx selectivity requirements when different numerologies are used in frequency domain","","415","11.5.1","Common issues for UE and BS [FS_NR_newRAT]",48400000,"noted","2016-11-02T15:25:04.313","2016-11-04T19:52:09.333","","","","","","","","","","","","","","",""]
["R4-1609220","Correction to cell mapping for periodic CQI reporting on multiple cells","ANRITSU LTD","Ian Rose","9381","CR","","Randomly choosing the allocation of PCell and SCell leads to the test condition not being repeatable.","","15","4.2.4","UE demodulation performance  [WI code or TEI12]",37100000,"withdrawn","2016-11-02T15:25:13.300",null,"","","Rel-10","36.101","10.23.0","LTE_CA_B39_B41-Perf, LTE_CA_B1_B3-Perf","3992","","F","","","","","",""]
["R4-1609221","NR UL in-band emissions and EVM requirements at UE TX","Nokia, Alcatel-Lucent Shanghai Bell","Tuomo Säynäjäkangas","69937","discussion","Approval","Discuss 5G NR UL in-band emission and EVM requirements at UE Tx following the RAN4 agreements.","","415","11.5.1","Common issues for UE and BS [FS_NR_newRAT]",48700000,"noted","2016-11-02T15:27:49.673","2016-11-04T19:52:09.347","","","","","","","","","","","","","","",""]
["R4-1609222","Correction to cell mapping for periodic CQI reporting on multiple cells","ANRITSU LTD","Ian Rose","9381","CR","","Randomly choosing the allocation of PCell and SCell leads to the test condition not being repeatable.","","15","4.2.4","UE demodulation performance  [WI code or TEI12]",37400000,"withdrawn","2016-11-02T15:28:13.573",null,"","","Rel-11","36.101","11.18.0","LTE_CA_B39_B41-Perf, LTE_CA_B1_B3-Perf","3993","","A","","","","","",""]
["R4-1609223","NR UL selectivity requirements at BS RX","Nokia, Alcatel-Lucent Shanghai Bell","Tuomo Säynäjäkangas","69937","discussion","Approval","Discuss 5G NR UL  in-band selectivity requirements at BS Rx following the RAN4 agreements.","","415","11.5.1","Common issues for UE and BS [FS_NR_newRAT]",62600000,"noted","2016-11-02T15:29:41.057","2016-11-04T19:52:09.347","","","","","","","","","","","","","","",""]
["R4-1609224","Correction to cell mapping for periodic CQI reporting on multiple cells","ANRITSU LTD","Ian Rose","9381","CR","","Randomly choosing the allocation of PCell and SCell leads to the test condition not being repeatable.","","15","4.2.4","UE demodulation performance  [WI code or TEI12]",13600000,"revised","2016-11-02T15:31:03.097","2016-11-04T13:34:29.607","","R4-1610727","Rel-12","36.101","12.13.0","LTE_CA_B39_B41-Perf, LTE_CA_B1_B3-Perf","3994","","F","","","","","",""]
["R4-1609225","NR DL in-band EVM and emission requirements at BS TX","Nokia, Alcatel-Lucent Shanghai Bell","Tuomo Säynäjäkangas","69937","discussion","Approval","Discuss 5G NR DL in-band EVM and emission requirements at BS Tx following the RAN4 agreements.","","415","11.5.1","Common issues for UE and BS [FS_NR_newRAT]",92210000,"noted","2016-11-02T15:32:34.593","2016-11-04T19:52:09.363","","","","","","","","","","","","","","",""]
["R4-1609226","Correction to cell mapping for periodic CQI reporting on multiple cells","ANRITSU LTD","Ian Rose","9381","CR","","Randomly choosing the allocation of PCell and SCell leads to the test condition not being repeatable.","","15","4.2.4","UE demodulation performance  [WI code or TEI12]",36900000,"agreed","2016-11-02T15:34:08.927","2016-11-22T12:17:26.907","","","Rel-13","36.101","13.5.0","LTE_CA_B39_B41-Perf, LTE_CA_B1_B3-Perf","3995","","A","RP-162415","","","","",""]
["R4-1609227","NR DL selectivity requirements at UE RX","Nokia, Alcatel-Lucent Shanghai Bell","Tuomo Säynäjäkangas","69937","discussion","Approval","Discuss 5G NR DL in-band selectivity requirements at UE Rx following the RAN4 agreements.","","415","11.5.1","Common issues for UE and BS [FS_NR_newRAT]",59300000,"noted","2016-11-02T15:34:39.050","2016-11-04T19:52:09.363","","","","","","","","","","","","","","",""]
["R4-1609228","Boundary between unwanted and spurious emissions for NR BS","Nokia, Alcatel-Lucent Shanghai Bell","Tuomo Säynäjäkangas","69937","discussion","Approval","Discuss further on how to specify boundary between unwanted and spurious emissions for NR BS.","","421","11.5.3.1","Transmitter characteristics [FS_NR_newRAT]",35700000,"noted","2016-11-02T15:36:32.460","2016-11-04T19:52:09.380","","","","","","","","","","","","","","",""]
["R4-1609229","Correction to cell mapping for periodic CQI reporting on multiple cells","ANRITSU LTD","Ian Rose","9381","CR","","Randomly choosing the allocation of PCell and SCell leads to the test condition not being repeatable.","","15","4.2.4","UE demodulation performance  [WI code or TEI12]",37000000,"agreed","2016-11-02T15:37:05.207","2016-11-22T12:17:26.907","","","Rel-14","36.101","14.1.0","LTE_CA_B39_B41-Perf, LTE_CA_B1_B3-Perf","3996","","A","RP-162415","","","","",""]
["R4-1609230","Spurious emissions for NR BS","Nokia, Alcatel-Lucent Shanghai Bell","Tuomo Säynäjäkangas","69937","discussion","Approval","Discuss further on how to specify spurious emissions for NR BS.","","421","11.5.3.1","Transmitter characteristics [FS_NR_newRAT]",40200000,"noted","2016-11-02T15:38:03.940","2016-11-04T19:52:09.380","","","","","","","","","","","","","","",""]
["R4-1609231","Response to WP5D on general RF parameters","Nokia, Alcatel-Lucent Shanghai Bell","Tuomo Säynäjäkangas","69937","discussion","Approval","Contribution propose content to be added for general RF parameters.","","412","11.3.3","others  [FS_NR_newRAT]",923100000,"noted","2016-11-02T15:39:48.070","2016-11-04T19:52:09.380","","","","","","","","","","","","","","",""]
["R4-1609232","Correct InformationBitPayload for Sub-Frame 1, 6 and Max T-put of TDD PDSCH RMC","ANRITSU LTD","Ian Rose","9381","CR","","Corrects the Information Bit Payload for Sub-Frames 1, 6 of PDSCH Reference channel R.4 TDD.","","14","4.2.3","RRM (Radio Resource Management)  [WI code or TEI12]",923400000,"withdrawn","2016-11-02T15:44:04.720","2016-11-04T16:05:55.153","","","Rel-12","36.133","12.13.0","TEI12","4179","","F","","","","","",""]
["R4-1609233","Correct InformationBitPayload for Sub-Frame 1, 6 and Max T-put of TDD PDSCH RMC","ANRITSU LTD","Ian Rose","9381","CR","","Corrects the Information Bit Payload for Sub-Frames 1, 6 of PDSCH Reference channel R.4 TDD.","","14","4.2.3","RRM (Radio Resource Management)  [WI code or TEI12]",923200000,"agreed","2016-11-02T15:46:53.170","2016-11-19T17:47:25.350","","","Rel-13","36.133","13.5.0","TEI12","4180","","A","RP-162420","","","","",""]
["R4-1609234","Correct InformationBitPayload for Sub-Frame 1, 6 and Max T-put of TDD PDSCH RMC","ANRITSU LTD","Ian Rose","9381","CR","","Corrects the Information Bit Payload for Sub-Frames 1, 6 of PDSCH Reference channel R.4 TDD.","","14","4.2.3","RRM (Radio Resource Management)  [WI code or TEI12]",923300000,"agreed","2016-11-02T15:49:09.013","2016-11-19T17:47:25.380","","","Rel-14","36.133","14.1.0","TEI12","4181","","A","RP-162420","","","","",""]
["R4-1609235","eLAA MPR and A-MPR requirements based on 5GHz WiFi PA measurements","Skyworks Solutions Inc.","Dominique Brunel","65099","discussion","Approval","This contribution proposes MPR and A-MPR values for eLAA based on RAN4#80bis way forwards R4-168820 [1] based on a set of LTE, eLAA and WiFi measurement taken from a standard 5GHz WiFi PA.","","244","8.18.2.1","MPR [LTE_eLAA-Core]",923500000,"noted","2016-11-02T16:37:12.737","2016-11-04T18:32:36.410","","","Rel-14","","","","","","","","","","","",""]
["R4-1609236","Correction of DUT testing conditions","Intel Corporation","Yang Tang","56725","CR","Approval","---","","223","8.14.2","Performance requirements [LTE_MIMO_OTA-Core]",52800000,"agreed","2016-11-02T16:50:26.747","2016-11-19T17:47:25.380","","","Rel-14","37.977","14.1.0","LTE_MIMO_OTA-Core","0040","","F","RP-162389","","","","",""]
["R4-1609237","Discussion on UE to UE and in-device co-existence between mmW NR and sub-6GHz NR and LTE","Skyworks Solutions Inc.","Dominique Brunel","65099","discussion","Approval","This contribution discusses the aspects of UE to UE and in device coexistence between mmW NR radio and sub-6GHz LTE or NR radios.","","416","11.5.2","UE RF  [FS_NR_newRAT]",959000000,"noted","2016-11-02T17:38:00.913","2016-11-04T18:32:36.427","","","Rel-15","","","","","","","","","","","",""]
["R4-1609238","Considerations on the wider measurement bandwidth for NR RRM","Intel","Yang Tang","56725","discussion","Discussion","---","","425","11.6.1.1","RRM general [FS_NR_newRAT]",35000000,"noted","2016-11-02T17:45:59.803","2016-11-07T18:58:24.030","","","","","","","","","","","","","","",""]
["R4-1609239","Draft LS on the network assistant signaling for HST","Intel","Yang Tang","56725","LS out","Approval","---","","343","8.28.2.3","Others [LTE_high_speed]",9552000,"noted","2016-11-02T17:47:03.590","2016-11-07T18:58:24.030","","","","","","","","","","","","","","",""]
["R4-1609240","UE cat M1 out of band blocking, Removal of Range 4","Sony","Olof Zander","57059","CR","Approval","---","","45","5.5.1","UE RF (36.101)  [LTE_MTCe2_L1-Core]",913400000,"agreed","2016-11-02T18:02:13.197","2016-11-04T17:47:39.040","","","Rel-13","36.101","13.5.0","LTE_MIMO_OTA-Core","3997","","F","RP-162430","","","","",""]
["R4-1609241","Network Assistance in NR waveform selection","AT&T","Marc Grant","16986","discussion","Discussion","---","","415","11.5.1","Common issues for UE and BS [FS_NR_newRAT]",48500000,"noted","2016-11-02T20:31:55.660","2016-11-04T16:16:56.093","","","","","","","","","","","","","","",""]
["R4-1609242","Additional margin in NB-IoT BS Demodulation Requirements","Nokia, Alcatel-Lucent Shanghai Bell","Ren Da","45542","other","Approval","---","","132","6.3.4.2","BS Demodulation  [NB_IOT-Perf]",53900000,"noted","2016-11-02T21:32:12.257","2016-11-04T15:45:03.477","","","","","","","","","","","","","","",""]
["R4-1609243","Parameter Settings in NPRACH Test Requirements","Nokia, Alcatel-Lucent Shanghai Bell","Ren Da","45542","other","Approval","---","","133","6.3.4.2.1","NPRACH  [NB_IOT-Perf]",924400000,"noted","2016-11-02T21:32:12.270","2016-11-04T15:45:03.477","","","","","","","","","","","","","","",""]
["R4-1609244","CR: NPRACH performance requirements (Rel-13, TS36.141)","Nokia, Alcatel-Lucent Shanghai Bell","Ren Da","45542","CR","Approval","---","","133","6.3.4.2.1","NPRACH  [NB_IOT-Perf]",944200000,"revised","2016-11-02T21:32:12.303","2016-11-04T15:45:03.477","","R4-1610561","Rel-13","36.104","13.5.0","NB_IOT-Perf","0885","","B","","","","","",""]
["R4-1609245","CR: NPRACH performance requirements (Rel-14, TS36.141)","Nokia, Alcatel-Lucent Shanghai Bell","Ren Da","45542","CR","Approval","---","","133","6.3.4.2.1","NPRACH  [NB_IOT-Perf]",967100000,"agreed","2016-11-02T21:32:12.397","2016-11-19T17:47:25.397","","","Rel-14","36.104","14.1.0","NB_IOT-Perf","0886","","B","RP-162379","","","","",""]
["R4-1609246","Updated NB-IoT NPRACH Simulation Results","Nokia, Alcatel-Lucent Shanghai Bell, Ericsson","Ren Da","45542","discussion","Discussion","---","","133","6.3.4.2.1","NPRACH  [NB_IOT-Perf]",56000000,"noted","2016-11-02T21:32:12.490","2016-11-04T15:45:03.477","","","","","","","","","","","","","","",""]
["R4-1609247","CR: Correction of Fixed Reference Channels for NPUSCH format 1 (Rel-13, 36.104)","Nokia, Alcatel-Lucent Shanghai Bell, Ericsson","Ren Da","45542","CR","Approval","Based on R4-168746 endorsed in RAN4#80bis","","134","6.3.4.2.2","NPUSCH format 1 [NB_IOT-Perf]",924900000,"agreed","2016-11-02T21:32:12.507","2016-11-04T15:45:03.477","","","Rel-13","36.104","13.5.0","NB_IOT-Perf","0887","","F","RP-162379","","","","",""]
["R4-1609248","CR: Correction of Fixed Reference Channels for NPUSCH format 1 (Rel-14, 36.104)","Nokia, Alcatel-Lucent Shanghai Bell, Ericsson","Ren Da","45542","CR","Approval","---","","134","6.3.4.2.2","NPUSCH format 1 [NB_IOT-Perf]",925000000,"agreed","2016-11-02T21:32:12.613","2016-11-19T17:47:25.413","","","Rel-14","36.104","14.1.0","NB_IOT-Perf","0888","","A","RP-162379","","","","",""]
["R4-1609249","CR: Correction of Fixed Reference Channels for NPUSCH format 1 (Rel-13, 36.141)","Nokia, Alcatel-Lucent Shanghai Bell, Ericsson","Ren Da","45542","CR","Approval","Based on R4-168747 endorsed in RAN4#80bis","","134","6.3.4.2.2","NPUSCH format 1 [NB_IOT-Perf]",925100000,"agreed","2016-11-02T21:32:12.693","2016-11-04T15:45:03.493","","","Rel-13","36.141","13.5.0","NB_IOT-Perf","0920","","F","RP-162379","","","","",""]
["R4-1609250","CR: Correction of Fixed Reference Channels for NPUSCH format 1 (Rel-14, 36.141)","Nokia, Alcatel-Lucent Shanghai Bell, Ericsson","Ren Da","45542","CR","Approval","---","","134","6.3.4.2.2","NPUSCH format 1 [NB_IOT-Perf]",934200000,"agreed","2016-11-02T21:32:12.787","2016-11-19T17:47:25.413","","","Rel-14","36.141","14.1.0","NB_IOT-Perf","0921","","A","RP-162379","","","","",""]
["R4-1609251","Updated Simulation Results for NB-IoT NPUSCH Format 1","Nokia, Alcatel-Lucent Shanghai Bell","Ren Da","45542","discussion","Discussion","---","","134","6.3.4.2.2","NPUSCH format 1 [NB_IOT-Perf]",56300000,"revised","2016-11-02T21:32:12.897","2016-11-04T15:45:03.493","","R4-1610605","","","","","","","","","","","","",""]
["R4-1609252","Updated Simulation Results for NB-IoT NPUSCH Format 2","Nokia, Alcatel-Lucent Shanghai Bell","Ren Da","45542","discussion","Discussion","---","","135","6.3.4.2.3","NPUSCH format 2 [NB_IOT-Perf]",56500000,"noted","2016-11-02T21:32:12.910","2016-11-04T15:45:03.460","","","","","","","","","","","","","","",""]
["R4-1609253","UL 3CC MPR","Qualcomm Incorporated","Prashanth Akula","67450","other","Approval","---","","147","8.1.2","UE RF (36.101) [LTE_CA_R14_intra-Core]",75900000,"noted","2016-11-02T22:27:07.023","2016-11-04T17:07:50.987","","","Rel-14","","","LTE_CA_R14_intra-Core","","","","","","","","",""]
["R4-1609254","PRACH Detection with New PRACH Cyclic Shift Restriction Set","Nokia, Alcatel-Lucent Shanghai Bell","Ren Da","45542","other","Decision","---","","348","8.28.4","BS demodulation (36.104/36.141) [LTE_high_speed]",925400000,"noted","2016-11-02T23:20:45.147","2016-11-04T15:45:03.477","","","","","","","","","","","","","","",""]
["R4-1609255","Correction to Es/Noc, Es/Iot and RSRP values in Idle mode re-selection test in enhanced coverage","Qualcomm Incorporated","Achaleshwar Sahai","63246","CR","Approval","---","","87","6.1.1.3.1","Intra-frequency Cell Re-Selection [LTE_MTCe2_L1-Perf]",925500000,"withdrawn","2016-11-03T00:00:01.683",null,"","","Rel-13","36.133","13.5.0","LTE_MTCe2_L1-Perf","4182","","F","","","","","",""]
["R4-1609256","Correction to Es/Noc, Es/Iot and RSRP values in Idle mode re-selection test in enhanced coverage","Qualcomm Incorporated","Achaleshwar Sahai","63246","CR","Approval","---","","87","6.1.1.3.1","Intra-frequency Cell Re-Selection [LTE_MTCe2_L1-Perf]",925600000,"withdrawn","2016-11-03T00:00:01.807",null,"","","Rel-14","36.133","14.1.0","LTE_MTCe2_L1-Perf","4183","","A","","","","","",""]
["R4-1609257","Applicability rule for eMTC test cases","Qualcomm Incorporated","Achaleshwar Sahai","63246","discussion","Discussion","---","","78","6.1.1.1.1","Test applicability [LTE_MTCe2_L1-Perf]",2360000,"noted","2016-11-03T00:36:09.193","2016-11-07T16:06:18.843","","","","","","","","","","","","","","",""]
["R4-1609258","MIB acquistion delay in Rel-13 eMTC","Qualcomm Incorporated","Achaleshwar Sahai","63246","discussion","Discussion","---","","48","5.5.3.1","Evaluation of MIB and SIB reading delay, and update of requirement for handover and RRC Re-establishment [LTE_MTCe2_L1-Core]",560000,"noted","2016-11-03T00:36:09.210","2016-11-07T16:06:18.843","","","","","","","","","","","","","","",""]
["R4-1609259","Correction to Es/Noc, Es/Iot and RSRP values in Idle mode re-selection test in normal coverage","Qualcomm Incorporated","Achaleshwar Sahai","63246","CR","Approval","---","","85","6.1.1.2.5","Others  [LTE_MTCe2_L1-Perf]",925900000,"agreed","2016-11-03T00:36:09.223","2016-11-07T16:20:16.360","","","Rel-13","36.133","13.5.0","LTE_MTCe2_L1-Perf","4184","","F","RP-162382","","","","",""]
["R4-1609260","Correction to Es/Noc, Es/Iot and RSRP values in Idle mode re-selection test in normal coverage","Qualcomm Incorporated","Achaleshwar Sahai","63246","CR","Approval","---","","85","6.1.1.2.5","Others  [LTE_MTCe2_L1-Perf]",926000000,"agreed","2016-11-03T00:36:09.317","2016-11-19T17:47:25.427","","","Rel-14","36.133","14.1.0","LTE_MTCe2_L1-Perf","4185","","A","RP-162382","","","","",""]
["R4-1609261","Corrections to rsrp-ThresholdsPrach and test requirement in Random Access Test in enhanced coverage","Qualcomm Incorporated","Achaleshwar Sahai","63246","CR","Approval","---","","90","6.1.1.3.4","Random Access [LTE_MTCe2_L1-Perf]",926100000,"agreed","2016-11-03T00:36:09.397","2016-11-07T16:20:16.360","","","Rel-13","36.133","13.5.0","LTE_MTCe2_L1-Perf","4186","","F","RP-162382","","","","",""]
["R4-1609262","Corrections to rsrp-ThresholdsPrach and test requirement in Random Access Test in enhanced coverage","Qualcomm Incorporated","Achaleshwar Sahai","63246","CR","Approval","---","","90","6.1.1.3.4","Random Access [LTE_MTCe2_L1-Perf]",926200000,"agreed","2016-11-03T00:36:09.490","2016-11-24T18:47:27.147","","","Rel-14","36.133","14.1.0","LTE_MTCe2_L1-Perf","4187","","A","RP-162382","","","","",""]
["R4-1609263","Corrections to the RRC re-establishment test cases","Qualcomm Incorporated","Achaleshwar Sahai","63246","CR","Approval","---","","89","6.1.1.3.3","RRC Re-establishment [LTE_MTCe2_L1-Perf]",9143000,"noted","2016-11-03T00:36:09.567","2016-11-07T16:20:16.360","","","Rel-13","36.133","13.5.0","LTE_MTCe2_L1-Perf","4188","","F","","","","","",""]
["R4-1609264","Corrections to the RRC re-establishment test cases","Qualcomm Incorporated","Achaleshwar Sahai","63246","CR","Approval","---","","89","6.1.1.3.3","RRC Re-establishment [LTE_MTCe2_L1-Perf]",9144000,"withdrawn","2016-11-03T00:36:09.660",null,"","","Rel-14","36.133","14.1.0","LTE_MTCe2_L1-Perf","4189","","A","","","","","",""]
["R4-1609265","RLM in CE mode B","Qualcomm Incorporated","Achaleshwar Sahai","63246","discussion","Discussion","---","","93","6.1.1.3.7","RLM  [LTE_MTCe2_L1-Perf]",926500000,"noted","2016-11-03T00:36:09.740","2016-11-07T16:06:18.860","","","","","","LTE_MTCe2_L1-Perf","","","","","","","","",""]
["R4-1609266","PBCH simulation results","Qualcomm Incorporated","Achaleshwar Sahai","63246","discussion","Discussion","---","","97","6.1.2.1","PBCH [LTE_MTCe2_L1-Perf]",926600000,"withdrawn","2016-11-03T00:36:09.757",null,"","","","","","LTE_MTCe2_L1-Perf","","","","","","","","",""]
["R4-1609267","MPDCCH simulation results","Qualcomm Incorporated","Achaleshwar Sahai","63246","discussion","Discussion","---","","98","6.1.2.2","MPDCCH [LTE_MTCe2_L1-Perf]",911600000,"noted","2016-11-03T00:36:09.787","2016-11-07T16:06:18.860","","","","","","LTE_MTCe2_L1-Perf","","","","","","","","",""]
["R4-1609268","MPDSCH simulation results","Qualcomm Incorporated","Achaleshwar Sahai","63246","discussion","Discussion","---","","99","6.1.2.3","MPDSCH [LTE_MTCe2_L1-Perf]",926800000,"noted","2016-11-03T00:36:09.800","2016-11-07T16:06:18.860","","","","","","LTE_MTCe2_L1-Perf","","","","","","","","",""]
["R4-1609269","Some issues on NR ultra-wideband single carrier channel bandwidth","ZTE Corporation","Yuqiang Zhang","43207","discussion","Discussion","This contribution discuss some issues  on NR supports ultra-wideband single carrier channel bandwidth.","","407","11.1","General   [FS_NR_newRAT]",62800000,"noted","2016-11-03T00:47:43.267","2016-11-04T07:11:22.177","","","","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1609270","Further discussion on NR BS Classes","ZTE Corporation","Yuqiang Zhang","43207","discussion","Discussion","This contribution gives some further considerations on NR BS Classes.","","420","11.5.3","BS RF  [FS_NR_newRAT]",973200000,"noted","2016-11-03T00:52:41.430","2016-11-04T07:11:22.177","","","","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1609271","Proposal on the delta TIB,c and delta RIB,c for Band 3, Band 8 and Band 39 3DL/1UL CA","ZTE, Nubia, CMCC","Yuqiang Zhang","43207","other","Approval","For approval. The delta TIB,c and delta RIB,c for 3DL/1UL CA_3A-8A-39A are proposed.","","384","9.1.2","Filter-combiner information [FS_LTE_CA_B3_B39]",4530000,"noted","2016-11-03T00:56:54.167","2016-11-04T07:11:22.177","","","","","","FS_LTE_CA_B3_B39","","","","","","","","",""]
["R4-1609272","Proposal on the delta TIB,c and delta RIB,c for Band 3, Band 39 and Band 41 3DL/1UL CA","ZTE, Nubia, CMCC","Yuqiang Zhang","43207","other","Approval","For approval.  The delta TIB,c and delta RIB,c for 3DL/1UL CA_3A-39A-41A are proposed.","","384","9.1.2","Filter-combiner information [FS_LTE_CA_B3_B39]",927100000,"withdrawn","2016-11-03T01:00:29.213","2016-11-04T07:11:22.177","","R4-1610453","","","","FS_LTE_CA_B3_B39","","","","","","","","",""]
["R4-1609273","5G NR TDD ON-OFF Switching Time Budget","ZTE Corporation","Yuqiang Zhang","43207","discussion","Discussion","In this contribution, we share our initial investigation when deciding on switching time requirements for NR in mm wave systems.","","415","11.5.1","Common issues for UE and BS [FS_NR_newRAT]",935700000,"noted","2016-11-03T01:02:18.600","2016-11-04T07:16:33.820","","","","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1609274","Measurement Requirements for Multipath RSTD reporting","Nokia, Alcatel-Lucent Shanghai Bell","Ren Da","45542","other","Decision","---","","297","8.22.3.1","OTDOA/E-CID enhancement [UTRA_LTE_iPos_enh2]",3390000,"available","2016-11-03T01:06:50.977","2016-11-04T19:29:04.420","","","","","","","","","","","","","","",""]
["R4-1609275","eMTC OTDOA Enhancements with Multipath RSTD Measurements","Nokia, Alcatel-Lucent Shanghai Bell","Ren Da","45542","other","Decision","---","","317","8.25.3.1.2","OTDOA  [LTE_feMTC-Core]",80000,"noted","2016-11-03T01:06:50.990","2016-11-04T19:29:04.420","","","","","","","","","","","","","","",""]
["R4-1609276","Updated eMTC RSTD Simulation Results","Nokia, Alcatel-Lucent Shanghai Bell","Ren Da","45542","discussion","Discussion","---","","317","8.25.3.1.2","OTDOA  [LTE_feMTC-Core]",3420000,"noted","2016-11-03T01:06:51.007","2016-11-04T19:29:04.420","","","","","","","","","","","","","","",""]
["R4-1609277","Definition of UE Rx – Tx time difference","Nokia, Alcatel-Lucent Shanghai Bell","Ren Da","45542","other","Decision","---","","307","8.24.3.1.1","E-CID  [NB_IOTenh-Core]",3280000,"noted","2016-11-03T01:06:51.023","2016-11-04T19:29:04.403","","","","","","","","","","","","","","",""]
["R4-1609278","Simulation results on MPDCCH performance for CEMode B RLM tests","Nokia, Alcatel-Lucent Shanghai Bell","Li Zhang","46368","discussion","Discussion","In this paper, we will provide our simulation results on MPDCCH performance for CEMode B RLM tests based on the new parameter set.","","93","6.1.1.3.7","RLM  [LTE_MTCe2_L1-Perf]",927800000,"noted","2016-11-03T02:38:16.993","2016-11-04T14:30:32.283","","","Rel-13","","","LTE_MTCe2_L1-Perf","","","","","","","","",""]
["R4-1609279","CR for Cat-M1 CEMode B RLM test cases: non-DRX HD-FDD out-of-sync in Rel-13","Nokia, Alcatel-Lucent Shanghai Bell","Li Zhang","46368","CR","Approval","CR for Cat-M1 CEMode B RLM test cases: non-DRX HD-FDD out-of-sync","","93","6.1.1.3.7","RLM  [LTE_MTCe2_L1-Perf]",928000000,"noted","2016-11-03T02:38:17.027","2016-11-04T14:30:32.300","","","Rel-13","36.133","13.5.0","LTE_MTCe2_L1-Perf","4190","","B","","","","","",""]
["R4-1609280","CR for Cat-M1 CEMode B RLM test cases: non-DRX HD-FDD out-of-sync in Rel-14","Nokia, Alcatel-Lucent Shanghai Bell","Li Zhang","46368","CR","Approval","CR for Cat-M1 CEMode B RLM test cases: non-DRX HD-FDD out-of-sync","","93","6.1.1.3.7","RLM  [LTE_MTCe2_L1-Perf]",928100000,"withdrawn","2016-11-03T02:38:17.180",null,"","","Rel-14","36.133","14.1.0","LTE_MTCe2_L1-Perf","4191","","A","","","","","",""]
["R4-1609281","CR for Cat-M1 CEMode B RLM test cases: non-DRX HD-FDD in-sync in Rel-13","Nokia, Alcatel-Lucent Shanghai Bell","Li Zhang","46368","CR","Approval","CR for Cat-M1 CEMode B RLM test cases: non-DRX HD-FDD in-sync","","93","6.1.1.3.7","RLM  [LTE_MTCe2_L1-Perf]",928200000,"noted","2016-11-03T02:38:17.337","2016-11-04T14:30:32.300","","","Rel-13","36.133","13.5.0","LTE_MTCe2_L1-Perf","4192","","B","","","","","",""]
["R4-1609282","CR for Cat-M1 CEMode B RLM test cases: non-DRX HD-FDD in-sync in Rel-14","Nokia, Alcatel-Lucent Shanghai Bell","Li Zhang","46368","CR","Approval","CR for Cat-M1 CEMode B RLM test cases: non-DRX HD-FDD in-sync","","93","6.1.1.3.7","RLM  [LTE_MTCe2_L1-Perf]",969700000,"withdrawn","2016-11-03T02:38:17.463",null,"","","Rel-14","36.133","14.1.0","LTE_MTCe2_L1-Perf","4193","","A","","","","","",""]
["R4-1609283","Introduction of Band 48 to 25.123","Nokia, Ericsson","Li Zhang","46368","CR","Approval","CR for introduction of Band 48 to 25.123","","201","8.10.4","RRM (36.133) [LTE_TDD_3550_CBRS_US]",928300000,"agreed","2016-11-03T02:38:17.557","2016-11-04T14:30:32.300","","","Rel-14","25.123","14.1.0","LTE_TDD_3550_CBRS_US-Perf","0568","","B","RP-162405","","","","",""]
["R4-1609284","Introduction of Band 48 to 25.133","Nokia, Ericsson","Li Zhang","46368","CR","Approval","CR for introduction of Band 48 to 25.133","","201","8.10.4","RRM (36.133) [LTE_TDD_3550_CBRS_US]",928400000,"agreed","2016-11-03T02:38:17.650","2016-11-04T14:30:32.300","","","Rel-14","25.133","14.0.0","LTE_TDD_3550_CBRS_US-Core","1427","","B","RP-162405","","","","",""]
["R4-1609285","Introduction of Band 48 to 36.133","Nokia, Ericsson","Li Zhang","46368","CR","Approval","CR for introduction of Band 48 to 36.133","","201","8.10.4","RRM (36.133) [LTE_TDD_3550_CBRS_US]",928500000,"agreed","2016-11-03T02:38:17.743","2016-11-04T14:30:32.300","","","Rel-14","36.133","14.1.0","LTE_TDD_3550_CBRS_US-Core","4194","","B","RP-162405","","","","",""]
["R4-1609286","Introduction of reliability definition and side condition for GNSS timing requirements","Nokia, Alcatel-Lucent Shanghai Bell","Li Zhang","46368","CR","Approval","CR for introduction of reliability definition and side condition for GNSS timing requirements","","264","8.19.2","RRM core maintenance (36.133)  [LTE_SL_V2V-Core]",976500000,"noted","2016-11-03T02:38:17.837","2016-11-04T14:30:32.300","","","Rel-14","36.133","14.1.0","LTE_SL_V2V-Core","4195","","F","","","","","",""]
["R4-1609287","Discussion on UE transmit timing for V2X","Nokia, Alcatel-Lucent Shanghai Bell","Li Zhang","46368","discussion","Discussion","In this paper, we will discuss the remaining issues in V2V UE TX timing requirements, namely the NTA offset to be applied and the timing error when SynRef UE is used as time reference.","","281","8.20.4.1","UE Transmit timing [LTE_V2X-Core]",9085000,"noted","2016-11-03T02:38:17.930","2016-11-04T14:30:32.313","","","Rel-14","","","LTE_V2X-Core","","","","","","","","",""]
["R4-1609288","Discussion on interruption requirements for V2X","Nokia, Alcatel-Lucent Shanghai Bell","Li Zhang","46368","discussion","Discussion","In this paper, based on the latest RAN1 and RAN4 RF agreements, we will discuss the interruption requirements for V2X.","","282","8.20.4.2","Interruption [LTE_V2X-Core]",99000,"noted","2016-11-03T02:38:17.947","2016-11-04T14:30:32.313","","","Rel-14","","","LTE_V2X-Core","","","","","","","","",""]
["R4-1609289","Discussion on synchronization requirements for V2X","Nokia, Alcatel-Lucent Shanghai Bell","Li Zhang","46368","discussion","Discussion","In this paper, we will discuss the open issues and provide our views on syncronization related requirements for V2X.","","284","8.20.4.4","Requirements related to synchronization [LTE_V2X-Core]",286000,"noted","2016-11-03T02:38:17.960","2016-11-04T14:30:32.313","","","Rel-14","","","LTE_V2X-Core","","","","","","","","",""]
["R4-1609290","Discussion on UE measurement requirements for collision avoidance and congestion control.","Nokia, Alcatel-Lucent Shanghai Bell","Li Zhang","46368","discussion","Discussion","In this paper, based on the latest RAN1 agreements, we will discuss the requirements related to measurements for collision avoidance and congestion control.","","285","8.20.4.5","Autonomous resource selection/reselection [LTE_V2X-Core]",9290000,"noted","2016-11-03T02:38:17.993","2016-11-04T14:30:32.313","","","Rel-14","","","LTE_V2X-Core","","","","","","","","",""]
["R4-1609291","Further discussion on RRM impacts of SRS switching","Nokia, Alcatel-Lucent Shanghai Bell","Li Zhang","46368","discussion","Discussion","In this contribution, based on RAN1 LS, we will provide our further views on the RRM impacts of SRS switching.","","291","8.21.3","RRM core and performance (36.133) [LTE_SRS_switch-Core/Perf]",929100000,"noted","2016-11-03T02:38:18.007","2016-11-04T14:30:32.313","","","Rel-14","","","LTE_SRS_switch-Core","","","","","","","","",""]
["R4-1609292","Discussion on measurement gaps for feMTC","Nokia, Alcatel-Lucent Shanghai Bell","Li Zhang","46368","discussion","Discussion","In this paper, we will provide our views on how to share measurement gaps between intra- and inter-frequency measurements. We will also address RAN1 LS on the need for gaps.","","319","8.25.3.2.1","Measurement [LTE_feMTC-Core]",2480000,"noted","2016-11-03T02:38:18.023","2016-11-04T14:30:32.313","","","Rel-14","","","LTE_feMTC-Core","","","","","","","","",""]
["R4-1609293","RRM/RLM requirements based on MPDCCH monitoring","Nokia, Alcatel-Lucent Shanghai Bell","Li Zhang","46368","discussion","Discussion","In this paper, we will analyze the UE MPDCCH monitoring behavior, and provide our views on how to update RRM/RLM requirements by taking MPDCCH monitoring into account.","","319","8.25.3.2.1","Measurement [LTE_feMTC-Core]",9617000,"noted","2016-11-03T02:38:18.040","2016-11-04T14:30:32.330","","","Rel-14","","","LTE_feMTC-Core","","","","","","","","",""]
["R4-1609294","Discussion on high speed indicator","Nokia, Alcatel-Lucent Shanghai Bell","Li Zhang","46368","discussion","Discussion","In this paper, we will provide our views regarding the usage of HST indicator, and our suggested answers to the questions raised up by RAN2.","","343","8.28.2.3","Others [LTE_high_speed]",9239000,"noted","2016-11-03T02:38:18.070","2016-11-04T14:30:32.330","","","Rel-14","","","LTE_high_speed","","","","","","","","",""]
["R4-1609295","draft Reply LS on performance enhancements indicator for high speed scenarios","Nokia, Alcatel-Lucent Shanghai Bell","Li Zhang","46368","LS out","Approval","LS reply to RAN2 on HST indicator","","343","8.28.2.3","Others [LTE_high_speed]",9553000,"noted","2016-11-03T02:38:18.087","2016-11-04T14:30:32.330","","","Rel-14","","","LTE_high_speed","","","","","","","","",""]
["R4-1609296","Discussion on remaining issues of HST RRM","Nokia, Alcatel-Lucent Shanghai Bell","Li Zhang","46368","discussion","Discussion","In this paper, we will provide our views on the remaining open issues of HST RRM.","","341","8.28.2.1","Enhancement in connected mode (DRX) [LTE_high_speed]",923900000,"noted","2016-11-03T02:38:18.100","2016-11-04T14:30:32.330","","","Rel-14","","","LTE_high_speed","","","","","","","","",""]
["R4-1609297","System level simulation results for HST","Nokia, Alcatel-Lucent Shanghai Bell","Li Zhang","46368","discussion","Discussion","In this paper, we will provide system level simulation results comparing different options from mobility performance perspective, and based on that provide our views on the enhanced HST requirements.","","341","8.28.2.1","Enhancement in connected mode (DRX) [LTE_high_speed]",929400000,"noted","2016-11-03T02:38:18.117","2016-11-04T14:30:32.330","","","Rel-14","","","LTE_high_speed","","","","","","","","",""]
["R4-1609298","Introduction of applicability rule for HST RRM requirements","Nokia, Alcatel-Lucent Shanghai Bell","Li Zhang","46368","CR","Approval","CR for introduction of applicability rule for HST RRM requirements","","341","8.28.2.1","Enhancement in connected mode (DRX) [LTE_high_speed]",952200000,"noted","2016-11-03T02:38:18.147","2016-11-04T14:30:32.347","","","Rel-14","36.133","14.1.0","LTE_high_speed","4196","","B","","","","","",""]
["R4-1609299","Open issues in BS IC study","Nokia, Alcatel-Lucent Shanghai Bell","Li Zhang","46368","discussion","Discussion","In this paper, we will provide our views on those open issues for BS IC study.","","397","9.4.3","Reference receiver [FS_LTE _IC_BS]",998500000,"noted","2016-11-03T02:38:18.243","2016-11-04T14:30:32.347","","","Rel-14","","","FS_LTE_IC_BS","","","","","","","","",""]
["R4-1609300","TP for TR 36.714-00-02: Analysis for CA_3A_5A_7A","SK Telecom","Joonyoung Shin","62013","pCR","Approval","Harmonics and IMD products analysis on 3DL/2UL CA. For approval","","183","8.7.2","UE RF (36.101) [LTE_CA_R14_xDL2UL-Core]",700000,"noted","2016-11-03T08:32:44.770","2016-11-04T04:59:28.433","","","","36.714-00-02","0.4.0","","","","","","","","","",""]
["R4-1609301","TP for TR 36.714-00-02: Analysis for CA_1A_3A_5A_7A","SK Telecom","Joonyoung Shin","62013","pCR","Approval","Harmonic and IMD products analysis on 4DL/2UL CA. For approval","","183","8.7.2","UE RF (36.101) [LTE_CA_R14_xDL2UL-Core]",800000,"noted","2016-11-03T08:35:01.300","2016-11-04T04:59:28.433","","","","36.714-00-02","0.4.0","","","","","","","","","",""]
["R4-1609302","Discussion on B7 NC UL CA","SK Telecom","Joonyoung Shin","62013","other","Discussion","Discussion on B7 NC UL CA","","147","8.1.2","UE RF (36.101) [LTE_CA_R14_intra-Core]",930200000,"noted","2016-11-03T08:37:39.547","2016-11-04T04:59:28.450","","","","36.714-00-00","","","","","","","","","","",""]
["R4-1609303","4 DL CA PCell in FDD FDD-TDD RSRQ for E-UTRAN in Carrier Aggregation","Nokia, Alcatel-Lucent Shanghai Bell","Lars Dalsgaard","69933","CR","Approval","---","","63","5.9.2","RRM [WI code or TEI13]",930300000,"agreed","2016-11-03T10:15:26.707","2016-11-04T18:33:35.363","","","Rel-13","36.133","13.5.0","TEI13","4197","","F","RP-162435","","","","",""]
["R4-1609304","4 DL CA PCell in FDD FDD-TDD RSRQ for E-UTRAN in Carrier Aggregation","Nokia, Alcatel-Lucent Shanghai Bell","Lars Dalsgaard","69933","CR","Approval","---","","63","5.9.2","RRM [WI code or TEI13]",930400000,"agreed","2016-11-03T10:15:26.817","2016-11-24T18:57:26.483","","","Rel-14","36.133","14.1.0","TEI13","4198","","A","RP-162435","","","","",""]
["R4-1609305","4 DL CA PCell in TDD TDD-FDD RSRQ for E-UTRAN in Carrier Aggregation","Nokia, Alcatel-Lucent Shanghai Bell","Lars Dalsgaard","69933","CR","Approval","---","","63","5.9.2","RRM [WI code or TEI13]",930500000,"agreed","2016-11-03T10:15:26.897","2016-11-04T18:33:35.377","","","Rel-13","36.133","13.5.0","TEI13","4199","","F","RP-162435","","","","",""]
["R4-1609306","4 DL CA PCell in TDD TDD-FDD RSRQ for E-UTRAN in Carrier Aggregation","Nokia, Alcatel-Lucent Shanghai Bell","Lars Dalsgaard","69933","CR","Approval","---","","63","5.9.2","RRM [WI code or TEI13]",930600000,"agreed","2016-11-03T10:15:27.003","2016-11-24T18:57:26.527","","","Rel-14","36.133","14.1.0","TEI13","4200","","A","RP-162435","","","","",""]
["R4-1609307","5 DL PCell in FDD RSRQ for E-UTRAN in Carrier Aggregation","Nokia, Alcatel-Lucent Shanghai Bell","Lars Dalsgaard","69933","CR","Approval","---","","63","5.9.2","RRM [WI code or TEI13]",930700000,"agreed","2016-11-03T10:15:27.083","2016-11-04T18:33:35.377","","","Rel-13","36.133","13.5.0","","4201","","F","","","","","",""]
["R4-1609308","5 DL PCell in FDD RSRQ for E-UTRAN in Carrier Aggregation","Nokia, Alcatel-Lucent Shanghai Bell","Lars Dalsgaard","69933","CR","Approval","---","","63","5.9.2","RRM [WI code or TEI13]",930800000,"agreed","2016-11-03T10:15:27.177",null,"","","Rel-14","36.133","14.1.0","","4202","","A","","","","","",""]
["R4-1609309","5 DL PCell in TDD RSRQ for E-UTRAN in Carrier Aggregation","Nokia, Alcatel-Lucent Shanghai Bell","Lars Dalsgaard","69933","CR","Approval","---","","63","5.9.2","RRM [WI code or TEI13]",930900000,"agreed","2016-11-03T10:15:27.287","2016-11-04T18:33:35.377","","","Rel-13","36.133","13.5.0","TEI13","4203","","F","RP-162435","","","","",""]
["R4-1609310","5 DL PCell in TDD RSRQ for E-UTRAN in Carrier Aggregation","Nokia, Alcatel-Lucent Shanghai Bell","Lars Dalsgaard","69933","CR","Approval","---","","63","5.9.2","RRM [WI code or TEI13]",931000000,"agreed","2016-11-03T10:15:27.393","2016-11-24T18:47:27.223","","","Rel-14","36.133","14.1.0","TEI13","4204","","A","RP-162435","","","","",""]
["R4-1609311","Clarification to applicability of NRSRQ for UE category NB1","Nokia, Alcatel-Lucent Shanghai Bell","Lars Dalsgaard","69933","CR","Approval","---","","117","6.3.3","RRM (36.133) [NB_IOT-Perf]",54900000,"revised","2016-11-03T10:15:27.487","2016-11-04T18:33:35.377","","R4-1610549","Rel-13","36.133","13.5.0","","4205","","F","","","","","",""]
["R4-1609312","Clarification to applicability of NRSRQ for UE category NB1","Nokia, Alcatel-Lucent Shanghai Bell","Lars Dalsgaard","69933","CR","Approval","---","","117","6.3.3","RRM (36.133) [NB_IOT-Perf]",931100000,"agreed","2016-11-03T10:15:27.567","2016-11-19T17:47:25.490","","","Rel-14","36.133","14.1.0","NB_IOT-Perf","4206","","A","RP-162379","","","","",""]
["R4-1609313","Introducing agreed measurement period for NB IoT connected mode","Nokia, Alcatel-Lucent Shanghai Bell","Lars Dalsgaard","69933","CR","Approval","---","","56","5.6.4","RRM core (36.133)  [NB_IOT-Core]",3600000,"agreed","2016-11-03T10:15:27.677","2016-11-04T18:34:43.143","","","Rel-13","36.133","13.5.0","NB_IOT-Core","4207","","F","RP-162433","","","","",""]
["R4-1609314","Introducing agreed measurement period for NB IoT connected mode","Nokia, Alcatel-Lucent Shanghai Bell","Lars Dalsgaard","69933","CR","Approval","---","","56","5.6.4","RRM core (36.133)  [NB_IOT-Core]",3700000,"agreed","2016-11-03T10:15:27.767","2016-11-19T17:47:25.507","","","Rel-14","36.133","14.1.0","NB_IOT-Core","4208","","A","RP-162433","","","","",""]
["R4-1609315","Introducing agreed measurement accuracy for UE Category NB1","Nokia, Alcatel-Lucent Shanghai Bell","Lars Dalsgaard","69933","CR","Approval","---","","117","6.3.3","RRM (36.133) [NB_IOT-Perf]",931200000,"revised","2016-11-03T10:15:27.863","2016-11-04T18:34:43.143","","R4-1610550","Rel-13","36.133","13.5.0","","4209","","F","","","","","",""]
["R4-1609316","Introducing agreed measurement accuracy for UE Category NB1","Nokia, Alcatel-Lucent Shanghai Bell","Lars Dalsgaard","69933","CR","Approval","---","","117","6.3.3","RRM (36.133) [NB_IOT-Perf]",931500010,"revised","2016-11-03T10:15:27.970",null,"","R4-1610551","Rel-14","36.133","14.1.0","","4210","","A","","","","","",""]
["R4-1609317","Further discussion on RRM measurements for NB-IoT in-band deployment","Nokia, Alcatel-Lucent Shanghai Bell","Lars Dalsgaard","69933","discussion","","---","","118","6.3.3.1","RRM measurement accuracy [NB_IOT-Perf]",2250000,"noted","2016-11-03T10:15:28.067","2016-11-04T18:34:43.143","","","","","","","","","","","","","","",""]
["R4-1609318","Inband NPBCH Peformance simulation results","Nokia, Alcatel-Lucent Shanghai Bell","Lars Dalsgaard","69933","discussion","","---","","129","6.3.4.1.1","NPBCH  [NB_IOT-Perf]",51400000,"revised","2016-11-03T10:15:28.080","2016-11-04T18:34:43.143","","R4-1610536","","","","","","","","","","","","",""]
["R4-1609319","NPDSCH demodulation performance","Nokia, Alcatel-Lucent Shanghai Bell","Lars Dalsgaard","69933","discussion","","---","","131","6.3.4.1.3","NPDSCH [NB-IOT-Perf]",55800000,"noted","2016-11-03T10:15:28.113","2016-11-04T18:34:43.157","","","","","","","","","","","","","","",""]
["R4-1609320","Inband NPDCCH Peformance simulation results","Nokia, Alcatel-Lucent Shanghai Bell","Lars Dalsgaard","69933","discussion","","---","","130","6.3.4.1.2","NPDCCH [NB_IOT-Perf]",55700000,"revised","2016-11-03T10:15:28.127","2016-11-04T18:35:34.357","","R4-1610537","","","","","","","","","","","","",""]
["R4-1609321","Regarding non-uniform measurement gap","Nokia, Alcatel-Lucent Shanghai Bell","Lars Dalsgaard","69933","discussion","","---","","351","8.29.2","RRM core (36.133) [LTE_meas_gap_enh-Core]",912100000,"noted","2016-11-03T10:15:28.143","2016-11-04T18:35:34.357","","","","","","","","","","","","","","",""]
["R4-1609322","LS on non-uniform gap measurements","Nokia, Alcatel-Lucent Shanghai Bell","Lars Dalsgaard","69933","LS out","Approval","---","","351","8.29.2","RRM core (36.133) [LTE_meas_gap_enh-Core]",954800000,"noted","2016-11-03T10:15:28.173","2016-11-04T18:35:34.357","","","Rel-14","36.133","14.1.0","","","","","","","","","",""]
["R4-1609323","Per-CC based measurement using common gap","Nokia, Alcatel-Lucent Shanghai Bell","Lars Dalsgaard","69933","discussion","","---","","351","8.29.2","RRM core (36.133) [LTE_meas_gap_enh-Core]",9322000,"noted","2016-11-03T10:15:28.190","2016-11-04T18:35:34.357","","","","","","","","","","","","","","",""]
["R4-1609324","Handover delays for mobility enhancements","Nokia, Alcatel-Lucent Shanghai Bell","Lars Dalsgaard","69933","discussion","","---","","327","8.26.3","RRM core (36.133) [LTE_eMob-Core]",910000000,"noted","2016-11-03T10:15:28.207","2016-11-04T18:35:34.357","","","","","","","","","","","","","","",""]
["R4-1609325","Introducing of new handover delay requirements for mobility enhancements","Nokia, Alcatel-Lucent Shanghai Bell","Lars Dalsgaard","69933","CR","Approval","---","","327","8.26.3","RRM core (36.133) [LTE_eMob-Core]",982100000,"noted","2016-11-03T10:15:28.220","2016-11-04T18:51:14.283","","","Rel-14","36.133","14.1.0","","4211","","B","","","","","",""]
["R4-1609326","Discussion on measurements for NR","Nokia, Alcatel-Lucent Shanghai Bell","Lars Dalsgaard","69933","discussion","","---","","425","11.6.1.1","RRM general [FS_NR_newRAT]",93260000,"noted","2016-11-03T10:15:28.360","2016-11-04T18:51:14.283","","","","","","","","","","","","","","",""]
["R4-1609327","Beam measurements in NR","Nokia, Alcatel-Lucent Shanghai Bell","Lars Dalsgaard","69933","discussion","","---","","425","11.6.1.1","RRM general [FS_NR_newRAT]",93270000,"noted","2016-11-03T10:15:28.377","2016-11-04T18:51:14.283","","","","","","","","","","","","","","",""]
["R4-1609328","Measurement gaps for NR","Nokia, Alcatel-Lucent Shanghai Bell","Lars Dalsgaard","69933","discussion","","---","","425","11.6.1.1","RRM general [FS_NR_newRAT]",34900000,"noted","2016-11-03T10:15:28.393","2016-11-04T18:51:14.300","","","","","","","","","","","","","","",""]
["R4-1609329","Power consumption discussion","Nokia, Alcatel-Lucent Shanghai Bell","Lars Dalsgaard","69933","discussion","","---","","425","11.6.1.1","RRM general [FS_NR_newRAT]",32900000,"noted","2016-11-03T10:15:28.423","2016-11-04T18:51:14.300","","","","","","","","","","","","","","",""]
["R4-1609330","Mobility in NR","Nokia, Alcatel-Lucent Shanghai Bell","Lars Dalsgaard","69933","discussion","","---","","425","11.6.1.1","RRM general [FS_NR_newRAT]",93280000,"available","2016-11-03T10:15:28.440","2016-11-04T18:51:56.577","","","","","","","","","","","","","","",""]
["R4-1609331","Discussion on latencies in NR","Nokia, Alcatel-Lucent Shanghai Bell","Lars Dalsgaard","69933","discussion","","---","","425","11.6.1.1","RRM general [FS_NR_newRAT]",93290000,"noted","2016-11-03T10:15:28.457","2016-11-04T18:51:56.593","","","","","","","","","","","","","","",""]
["R4-1609332","MPAC alignment measurement results","Keysight Technologies UK Ltd","Moray Rumney","6630","other","Information","Summary of current MPAC measurements using alignment and performance devices.","","222","8.14.1","General [LTE_MIMO_OTA-Core]",78500000,"noted","2016-11-03T11:50:19.030","2016-11-05T00:42:55.933","","","","","","","","","","","","","","",""]
["R4-1609333","Root cause analysis for MPAC alignment","Keysight Technologies UK Ltd","Moray Rumney","6630","other","Information","Summarizes current investigations into differences between MPAC labs","","222","8.14.1","General [LTE_MIMO_OTA-Core]",91240000,"noted","2016-11-03T11:55:10.093","2016-11-04T22:03:16.277","","","","","","","","","","","","","","",""]
["R4-1609334","Further analysis of starting phase impact on channel model statistics","Keysight Technologies UK Ltd","Moray Rumney","6630","other","Information","---","","222","8.14.1","General [LTE_MIMO_OTA-Core]",91250000,"withdrawn","2016-11-03T11:57:10.527",null,"","","","","","","","","","","","","","",""]
["R4-1609335","CR to 37.977 to add test zone size for RTS","Keysight Technologies UK Ltd","Moray Rumney","6630","CR","Approval","---","","222","8.14.1","General [LTE_MIMO_OTA-Core]",933600000,"revised","2016-11-03T12:00:23.187","2016-11-04T22:05:05.160","","R4-1610785","Rel-14","37.977","14.1.0","UTRA_LTE_MIMO_OTA-Core","0041","","B","","","","","",""]
["R4-1609336","CR to 37.977 add noise floor validation procedure","Keysight Technologies UK Ltd","Moray Rumney","6630","CR","Approval","---","","222","8.14.1","General [LTE_MIMO_OTA-Core]",91570000,"noted","2016-11-03T12:02:03.323","2016-11-04T22:07:48.730","","","Rel-14","37.977","14.1.0","UTRA_LTE_MIMO_OTA-Core","0042","","B","","","","","",""]
["R4-1609337","Draft CR to add V/H spatial correlation validation procedure","Keysight Technologies UK Ltd","Moray Rumney","6630","draftCR","Information","---","","222","8.14.1","General [LTE_MIMO_OTA-Core]",93320000,"noted","2016-11-03T12:03:55.067","2016-11-04T22:08:34.157","","","Rel-14","37.977","14.1.0","UTRA_LTE_MIMO_OTA-Core","","","","","","","","",""]
["R4-1609338","Measuring UE EIRP","Keysight Technologies UK Ltd","Moray Rumney","6630","other","Discussion","---","","417","11.5.2.1","Transmitter characteristics [FS_NR_newRAT]",964800000,"noted","2016-11-03T12:06:42.967","2016-11-04T22:02:18.703","","","","","","","","","","","","","","",""]
["R4-1609339","RC+CE Channel Model Validation Results","Bluetest AB","Christian Lötbäck","45377","discussion","","---","","224","8.14.3","Harmonization [LTE_MIMO_OTA-Core]",959700000,"noted","2016-11-03T12:07:14.497","2016-11-11T08:02:56.750","","","","","","","","","","","","","","",""]
["R4-1609340","CR to TR37.977: RC+CE Channel Model Validation Results","Bluetest AB","Christian Lötbäck","45377","CR","Approval","---","","224","8.14.3","Harmonization [LTE_MIMO_OTA-Core]",992800000,"revised","2016-11-03T12:11:18.480","2016-11-11T08:02:56.750","","R4-1610949","Rel-14","37.977","14.1.0","","0043","","F","","","","","",""]
["R4-1609341","Simulation results for NB-IoT NPRACH","Samsung","Haijie Qiu","46265","discussion","Discussion","---","","133","6.3.4.2.1","NPRACH  [NB_IOT-Perf]",56100000,"noted","2016-11-03T12:46:48.830","2016-11-04T12:40:08.723","","","Rel-13","","","NB_IOT-Perf","","","","","","","","",""]
["R4-1609342","Simulation results for NB-IoT NPUCCH format1","Samsung","Haijie Qiu","46265","discussion","Discussion","---","","134","6.3.4.2.2","NPUSCH format 1 [NB_IOT-Perf]",56400000,"noted","2016-11-03T12:46:48.847","2016-11-04T12:40:08.737","","","Rel-13","","","NB_IOT-Perf","","","","","","","","",""]
["R4-1609343","Simulation results for NB-IoT NPUCCH format2","Samsung","Haijie Qiu","46265","discussion","Discussion","---","","135","6.3.4.2.3","NPUSCH format 2 [NB_IOT-Perf]",56600000,"noted","2016-11-03T12:46:48.877","2016-11-04T12:40:08.753","","","Rel-13","","","NB_IOT-Perf","","","","","","","","",""]
["R4-1609344","Remove square brackets for Rel-13 FD-MIMO performance requirements","Samsung","Haijie Qiu","46265","CR","Approval","---","","64","5.9.3","Demodulation [WI code or TEI13]",934400000,"agreed","2016-11-03T12:46:48.893","2016-11-04T12:40:08.753","","","Rel-13","36.101","13.5.0","LTE_EBF_FDMIMO-Perf","3998","","F","RP-162425","","","","",""]
["R4-1609345","Remove square brackets for FD-MIMO performance requirements","Samsung","Haijie Qiu","46265","CR","Approval","---","","64","5.9.3","Demodulation [WI code or TEI13]",934500000,"agreed","2016-11-03T12:46:49.020","2016-11-19T17:47:25.507","","","Rel-14","36.101","14.1.0","LTE_EBF_FDMIMO-Perf","3999","","A","RP-162425","","","","",""]
["R4-1609346","Consideration on Power Class 1 UEs in B3/20/28 for PS service","Samsung","Haijie Qiu","46265","discussion","Approval","In this contribution we will provide our view on it combined with PS scenario limitation for PC1 UE.","","234","8.16.2","UE RF (36.101)  [LTE_HPUE_B3_B20_B28]",934600000,"noted","2016-11-03T12:46:49.127","2016-11-04T12:40:08.767","","","Rel-14","","","LTE_HPUE_B3_B20_B28","","","","","","","","",""]
["R4-1609347","Consideration on HPUE in B28 for European DTV protection","Samsung","Haijie Qiu","46265","discussion","Discussion","In this contribution, we analyze that how to introduce the European DTV and potential A-MPR for HPUE in B28","","234","8.16.2","UE RF (36.101)  [LTE_HPUE_B3_B20_B28]",934700000,"noted","2016-11-03T12:46:49.160","2016-11-04T12:40:08.783","","","Rel-14","","","LTE_HPUE_B3_B20_B28","","","","","","","","",""]
["R4-1609348","TP for TR 36.714-00-00: REFSENS requirement for CA_3A-3A_BCS2","Samsung","Haijie Qiu","46265","pCR","Approval","---","","147","8.1.2","UE RF (36.101) [LTE_CA_R14_intra-Core]",934800000,"revised","2016-11-03T12:46:49.190","2016-11-04T12:40:08.783","","R4-1610759","","36.714-00-00","0.2.0","LTE_CA_R14_intra-Core","","","","","","","","",""]
["R4-1609349","TP for TR 36.714-00-00: Blocking requirements for CA_3B","Samsung","Haijie Qiu","46265","pCR","Approval","---","","147","8.1.2","UE RF (36.101) [LTE_CA_R14_intra-Core]",982600000,"approved","2016-11-03T12:46:49.207","2016-11-04T12:40:08.800","","","","36.714-00-00","0.2.0","LTE_CA_R14_intra-Core","","","","","","","","",""]
["R4-1609350","Consideration on  operating band unwanted emissions","Samsung","Haijie Qiu","46265","discussion","Approval","---","","421","11.5.3.1","Transmitter characteristics [FS_NR_newRAT]",40300000,"noted","2016-11-03T12:46:49.220","2016-11-04T12:40:08.817","","","Rel-15","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1609351","Further consideration on high power V2X UE","Samsung","Haijie Qiu","46265","discussion","Discussion","Further consideration on high power V2X UE RF requirement based on agreed WF.","","278","8.20.3.1","Tx requirements  [LTE_V2X-Core]",75700000,"noted","2016-11-03T12:46:49.253","2016-11-04T12:40:08.817","","","Rel-14","","","LTE_V2X-Core","","","","","","","","",""]
["R4-1609352","Further discussion on MCC V2X opertion","Samsung","Haijie Qiu","46265","discussion","Discussion","Further discussion on MCC V2X UE RF requirement.","","277","8.20.3","UE RF (36.101) [LTE_V2X-Core]",937900000,"noted","2016-11-03T12:46:49.267","2016-11-04T12:40:08.830","","","Rel-14","","","LTE_V2X-Core","","","","","","","","",""]
["R4-1609353","Simulation results for NR coexistence study in urban macro scenario","Samsung","Haijie Qiu","46265","discussion","Discussion","---","","410","11.3.1","Co-existence [FS_NR_newRAT]",9078000,"noted","2016-11-03T12:46:49.283","2016-11-04T12:40:08.830","","","Rel-15","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1609354","Simulation results for NR coexistence study in dense urban scenario","Samsung","Haijie Qiu","46265","discussion","Discussion","---","","410","11.3.1","Co-existence [FS_NR_newRAT]",9079000,"noted","2016-11-03T12:46:49.317","2016-11-04T12:40:08.847","","","Rel-15","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1609355","Simulation results for NR coexistence study in indoor scenario","Samsung","Haijie Qiu","46265","discussion","Discussion","---","","410","11.3.1","Co-existence [FS_NR_newRAT]",9080000,"noted","2016-11-03T12:46:49.330","2016-11-04T12:40:08.847","","","Rel-15","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1609356","Summary of simulation results and discussion on the remaining issues","Samsung","Haijie Qiu","46265","discussion","Discussion","---","","410","11.3.1","Co-existence [FS_NR_newRAT]",9353000,"noted","2016-11-03T12:46:49.347","2016-11-04T12:40:08.863","","","Rel-15","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1609357","Initial considerations on spectral utilization on NR system with several spectral confinement techniques","Samsung","Haijie Qiu","46265","discussion","Discussion","---","","415","11.5.1","Common issues for UE and BS [FS_NR_newRAT]",922500000,"noted","2016-11-03T12:46:49.363","2016-11-04T12:40:08.863","","","Rel-15","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1609358","TP for TR 36.752: RF Requirement Evaluation for NB-IoT Coexistence with CDMA","Samsung, China Telecom","Haijie Qiu","46265","pCR","Approval","In this contribution, we provide analysis on RF requirement evaluation for NB-IoT Coexistence with CDMA, and corresponding TP for TR 36.752.","","393","9.3.4","RF requirements impact [FS_NB_IOT_CDMA_coex]",954000000,"revised","2016-11-03T12:53:01.530","2016-11-04T12:40:08.877","","R4-1610843","","36.752","0.0.1","FS_NB_IOT_CDMA_coex","","","","","","","","",""]
["R4-1609359","TP for TR 36.752: Conclusion","Samsung, China Telecom","Haijie Qiu","46265","pCR","Approval","In this contribution, we provide TP for conclusion part of TR 36.752.","","393","9.3.4","RF requirements impact [FS_NB_IOT_CDMA_coex]",953900000,"revised","2016-11-03T12:53:01.547","2016-11-04T12:40:08.893","","R4-1610844","","36.752","0.0.1","FS_NB_IOT_CDMA_coex","","","","","","","","",""]
["R4-1609360","Updated Simulation Results for Additional TM2 Demodulation Test with 4RX MMSE-IRC Receiver","Samsung","Haijie Qiu","46265","discussion","Discussion","In this contribution, we provide our simulation with 4RX Type-A MMSE-IRC receivers based on the test TM2/3/3 for both TDD and FDD.","","33","5.2.3.2","UE demodulation and CSI [LTE_4Rx_AP_DL-Perf]",906500000,"noted","2016-11-03T12:53:01.577","2016-11-04T12:40:08.893","","","Rel-13","","","LTE_4Rx_AP_DL-Perf","","","","","","","","",""]
["R4-1609361","Discussion on 4RX UE's test scope and release independence","Samsung","Haijie Qiu","46265","discussion","Discussion","In this contribution, we provided our views on 4RX UE's test scope and release independence","","358","8.30.3.1","Applicability [LTE_4Rx_AP_DL_CA-Perf]",936100000,"noted","2016-11-03T12:53:01.593","2016-11-04T12:40:08.910","","","Rel-14","","","LTE_4Rx_AP_DL_CA-Perf","","","","","","","","",""]
["R4-1609362","Discussion on Enhanced SU-MIMO IM","Samsung","Haijie Qiu","46265","discussion","Discussion","In this contribution, we provided our views on related aspects for enhanced SU-MIMO IM evaluation.","","370","8.31.3.1","Performance evaluation: scenarios and receiver [LTE_eCRSIM_eSUMIMO]",948400000,"noted","2016-11-03T12:53:01.610","2016-11-04T12:40:08.923","","","Rel-14","","","LTE_eCRSIM_eSUMIMO","","","","","","","","",""]
["R4-1609363","Remaining issues on multi-node testing","Huawei","Xiang (Steven) Chen","41576","other","Approval","This contribution is for approval.","","140","7.1.2","Multi-node testing [FS_LTE_LAA_multinode_test]",139000,"available","2016-11-03T13:02:46.033","2016-11-04T17:54:33.020","","","","","","FS_LTE_LAA_multinode_test","","","","","","","","",""]
["R4-1609364","TP for 36.789: Choice of devices","Huawei","Xiang (Steven) Chen","41576","pCR","Approval","---","","139","7.1.1","General  [FS_LTE_LAA_multinode_test]",4610000,"approved","2016-11-03T13:02:46.063","2016-11-04T17:54:33.033","","","","36.789","0.0.1","FS_LTE_LAA_multinode_test","","","","","","","","",""]
["R4-1609365","TP for 36.789: Updates on section 5 and 6.1","Huawei","Xiang (Steven) Chen","41576","pCR","Approval","---","","139","7.1.1","General  [FS_LTE_LAA_multinode_test]",4640000,"revised","2016-11-03T13:02:46.080","2016-11-04T17:54:33.033","","R4-1610812","","36.789","0.0.1","FS_LTE_LAA_multinode_test","","","","","","","","",""]
["R4-1609366","CR on eLAA BS Rx requirements","Huawei, Nokia","Xiang (Steven) Chen","41576","CR","Agreement","---","","250","8.18.3.2","Rx requirements [LTE_eLAA-Core]",73800000,"revised","2016-11-03T13:02:46.093","2016-11-04T12:05:23.003","","R4-1610738","Rel-14","36.104","14.1.0","LTE_eLAA-Core","0889","","B","","","","","",""]
["R4-1609367","On UE core requirements due to SRS switching","Huawei, Hisilicon","Xiang (Steven) Chen","41576","other","Approval","This contribution is for approval.","","290","8.21.2","UE RF (36.101) [LTE_SRS_switch-Core]",4670000,"noted","2016-11-03T13:02:46.237","2016-11-04T12:05:23.017","","","","","","LTE_SRS_switch-Core","","","","","","","","",""]
["R4-1609368","Correction on FRC for V2V in TS 36.101","Huawei, Hisilicon","Xiang (Steven) Chen","41576","CR","Agreement","---","","263","8.19.1.4","Others",936800000,"revised","2016-11-03T13:02:46.267","2016-11-04T12:05:23.017","","R4-1610751","Rel-14","36.101","14.1.0","LTE_SL_V2V-Core","4000","","F","","","","","",""]
["R4-1609369","TP for 36.786: Updated MPR requirements for V2V","Huawei, Hisilicon","Xiang (Steven) Chen","41576","pCR","Approval","---","","260","8.19.1.1","MPR/A-MPR [LTE_SL_V2V-Core]",748000,"revised","2016-11-03T13:02:46.360","2016-11-04T12:05:23.033","","R4-1610748","","36.786","0.0.2","LTE_SL_V2V-Core","","","","","","","","",""]
["R4-1609370","TP for 36.786: Updated A-MPR requirements for V2V","Huawei, Hisilicon","Xiang (Steven) Chen","41576","pCR","Approval","---","","260","8.19.1.1","MPR/A-MPR [LTE_SL_V2V-Core]",27300000,"revised","2016-11-03T13:02:46.377","2016-11-04T12:05:23.047","","R4-1610749","","36.786","0.0.2","LTE_SL_V2V-Core","","","","","","","","",""]
["R4-1609371","Consideration on handling  co-existence requirements with CEN DSRC","Huawei, Hisilicon","Xiang (Steven) Chen","41576","other","Approval","This contribution is for approval.","","259","8.19.1","UE RF core maintenace (36.101)  [LTE_SL_V2V-Core]",42700000,"noted","2016-11-03T13:02:46.407","2016-11-04T12:05:23.047","","","","","","LTE_SL_V2V-Core","","","","","","","","",""]
["R4-1609372","LS on handling co-existence requirements with CEN DSRC","Huawei, Hisilicon","Xiang (Steven) Chen","41576","LS out","Approval","---","","259","8.19.1","UE RF core maintenace (36.101)  [LTE_SL_V2V-Core]",74700000,"revised","2016-11-03T13:02:46.437","2016-11-04T12:05:23.063","","R4-1610746","","","","LTE_SL_V2V-Core","","","","","","RAN2, SA2, CT1","","",""]
["R4-1609373","Discussion on meeting ETSI RX regulatory requirements","Huawei, Hisilicon","Xiang (Steven) Chen","41576","other","Approval","This contribution is for approval.","","261","8.19.1.2","Blocking  [LTE_SL_V2V-Core]",86600,"noted","2016-11-03T13:02:46.470","2016-11-04T12:05:23.080","","","","","","LTE_SL_V2V-Core","","","","","","","","",""]
["R4-1609374","TP for 36.786: Meeting ETSI RX regulatory requirements","Huawei, Hisilicon","Xiang (Steven) Chen","41576","pCR","Approval","---","","261","8.19.1.2","Blocking  [LTE_SL_V2V-Core]",937300000,"revised","2016-11-03T13:02:46.483","2016-11-04T12:05:23.097","","R4-1610750","","36.786","0.0.2","LTE_SL_V2V-Core","","","","","","","","",""]
["R4-1609375","Updated co-existence simulation results for case 1","Huawei, Hisilicon","Xiang (Steven) Chen","41576","discussion","Discussion","---","","276","8.20.2.2","Co-existence study for case 1 and case 2  [LTE_V2X-Core]",75500000,"noted","2016-11-03T13:02:46.500","2016-11-04T12:05:23.097","","","","","","LTE_V2X-Core","","","","","","","","",""]
["R4-1609376","Updated co-existence simulation results for case 2","Huawei, Hisilicon","Xiang (Steven) Chen","41576","discussion","Discussion","---","","276","8.20.2.2","Co-existence study for case 1 and case 2  [LTE_V2X-Core]",937500000,"noted","2016-11-03T13:02:46.530","2016-11-04T12:05:23.110","","","","","","LTE_V2X-Core","","","","","","","","",""]
["R4-1609377","Co-existence simulation results for V2X","Huawei, Hisilicon","Xiang (Steven) Chen","41576","discussion","Discussion","---","","275","8.20.2.1","Co-existence study for High power V2X UE  [LTE_V2X-Core]",937700000,"noted","2016-11-03T13:02:46.547","2016-11-04T12:05:23.127","","","","","","LTE_V2X-Core","","","","","","","","",""]
["R4-1609378","TP for 36.786 Operating bands and channel bandwidth for V2X","Huawei, Hisilicon, CATT","Xiang (Steven) Chen","41576","other","Approval","This contribution is for approval.","","273","8.20.1","General [LTE_V2X-Core]",986700000,"withdrawn","2016-11-03T13:02:46.577",null,"","","","","","","","","","","","","","",""]
["R4-1609379","UE RF requirements for V2X","Huawei, Hisilicon","Xiang (Steven) Chen","41576","other","Approval","This contributiion is for approval.","","277","8.20.3","UE RF (36.101) [LTE_V2X-Core]",949500000,"noted","2016-11-03T13:02:46.593","2016-11-04T12:05:23.127","","","","","","","","","","","","","","",""]
["R4-1609380","Further consideration on inter-band MCC for V2X","Huawei, Hisilicon","Xiang (Steven) Chen","41576","discussion","Discussion","---","","277","8.20.3","UE RF (36.101) [LTE_V2X-Core]",935200000,"noted","2016-11-03T13:02:46.627","2016-11-04T12:05:23.143","","","","","","LTE_V2X-Core","","","","","","","","",""]
["R4-1609381","Overview on BS RF requirements for sTTI","Huawei","Xiang (Steven) Chen","41576","other","Approval","This contribution is for approval.","","404","10.1.3","BS RF (36.104) [LTE_sTTIandPT]",938100000,"approved","2016-11-03T13:02:46.640","2016-11-04T12:05:23.157","","","","","","LTE_sTTIandPT","","","","","","","","",""]
["R4-1609382","Overview on UE RF requirements for sTTI","Huawei, Hisilicon","Xiang (Steven) Chen","41576","other","Approval","This contribution is for approval.","","403","10.1.2","UE RF (36.101) [LTE_sTTIandPT]",938200000,"approved","2016-11-03T13:02:46.670","2016-11-04T12:05:23.157","","","","","","LTE_sTTIandPT","","","","","","","","",""]
["R4-1609383","Discussion on UL ON/OFF time mask","Huawei, Hisilicon","Xiang (Steven) Chen","41576","other","Approval","This contribution is for approval.","","403","10.1.2","UE RF (36.101) [LTE_sTTIandPT]",789000,"noted","2016-11-03T13:02:46.687","2016-11-04T12:05:23.173","","","","","","LTE_sTTIandPT","","","","","","","","",""]
["R4-1609384","Reply LS on UL ON/OFF time mask","Huawei, Hisilicon","Xiang (Steven) Chen","41576","LS out","Approval","---","","403","10.1.2","UE RF (36.101) [LTE_sTTIandPT]",4700000,"noted","2016-11-03T13:02:46.717","2016-11-04T12:05:23.190","","","","","","LTE_sTTIandPT","","","","","RAN1","RAN1","","",""]
["R4-1609385","Necessary changes in 36.101 on new power class for NB-IoT","Huawei, Neul","Xiang (Steven) Chen","41576","discussion","Discussion","---","","304","8.24.2.1","Power Class       [NB_IOTenh-Core]",82900,"noted","2016-11-03T13:02:46.750","2016-11-04T12:15:12.307","","","","","","NB_IOTenh-Core","","","","","","","","",""]
["R4-1609386","NB-IoT UE RF requirements for protection of CDMA","Huawei, Neul","Xiang (Steven) Chen","41576","other","Approval","This contribution is for approval. We provide further discussion on UE RF requirements for co-existence with CDMA.","","393","9.3.4","RF requirements impact [FS_NB_IOT_CDMA_coex]",84500,"noted","2016-11-03T13:02:46.767","2016-11-04T12:15:12.307","","","","","","FS_NB_IOT_CDMA_coex","","","","","","","","",""]
["R4-1609387","CR for 36.141: Multi-band testing with 3 or more bands","Huawei, Ericsson, Nokia","Xiang (Steven) Chen","41576","CR","Agreement","---","","205","8.11.2","BS RF (36.141, 37.141, 25.141) [MB_BS_test_3B-Perf]",74300000,"revised","2016-11-03T13:02:46.797","2016-11-04T12:15:12.307","","R4-1610743","Rel-14","36.141","14.1.0","MB_BS_test_3B-Perf","0922","","B","","","","","",""]
["R4-1609388","CR for 36.141: Introduction of NB-IoT","Huawei","Xiang (Steven) Chen","41576","CR","Agreement","---","","113","6.3.2","BS RF conformance testing (36.141) [NB_IOT-Perf]",54300000,"revised","2016-11-03T13:02:46.890","2016-11-04T12:15:12.323","","R4-1610543","Rel-13","36.141","13.5.0","NB_IOT-Perf","0923","","B","","","","","",""]
["R4-1609389","Introduction of NB-IoT into 36.141","Huawei, Ericsson, Nokia","Xiang (Steven) Chen","41576","CR","Agreement","---","","113","6.3.2","BS RF conformance testing (36.141) [NB_IOT-Perf]",55200000,"agreed","2016-11-03T13:02:46.983","2016-11-19T17:47:25.537","","","Rel-14","36.141","14.1.0","NB_IOT-Perf","0924","","A","RP-162379","","","","",""]
["R4-1609390","CR for 36.113: Introduction of NB-IoT","Huawei","Xiang (Steven) Chen","41576","CR","Agreement","---","","113","6.3.2","BS RF conformance testing (36.141) [NB_IOT-Perf]",56200000,"revised","2016-11-03T13:02:47.107","2016-11-04T12:15:12.323","","R4-1610544","Rel-13","36.113","13.2.0","NB_IOT-Perf","0061","","B","","","","","",""]
["R4-1609391","CR for 36.113: Introduction of NB-IoT","Huawei","Xiang (Steven) Chen","41576","CR","Agreement","---","","113","6.3.2","BS RF conformance testing (36.141) [NB_IOT-Perf]",938800001,"revised","2016-11-03T13:02:47.217","2016-11-19T17:47:25.537","","R4-1611009","Rel-14","36.113","14.0.0","NB_IOT-Perf","0062","","A","","","","","",""]
["R4-1609392","Discussion on frequency error for eMTC","Huawei","Xiang (Steven) Chen","41576","discussion","Discussion","---","","45","5.5.1","UE RF (36.101)  [LTE_MTCe2_L1-Core]",169000,"noted","2016-11-03T13:02:47.310","2016-11-04T12:15:12.323","","","","","","","","","","","","","","",""]
["R4-1609393","CR for 36.101: frequency error for eMTC","Huawei","Xiang (Steven) Chen","41576","CR","Agreement","---","","45","5.5.1","UE RF (36.101)  [LTE_MTCe2_L1-Core]",4580000,"revised","2016-11-03T13:02:47.343","2016-11-04T12:15:12.323","","R4-1610847","Rel-13","36.101","13.5.0","LTE_MTCe2_L1-Core","4001","","F","","","","","",""]
["R4-1609394","CR for 36.101: frequency error for eMTC","Huawei, Intel Corporation, Ericsson","Xiang (Steven) Chen","41576","CR","Agreement","---","","45","5.5.1","UE RF (36.101)  [LTE_MTCe2_L1-Core]",4960000,"agreed","2016-11-03T13:02:47.450","2016-11-19T17:47:25.537","","","Rel-14","36.101","14.1.0","LTE_MTCe2_L1-Core","4002","","A","RP-162431","","","","",""]
["R4-1609395","Further discussion on MPR requirement for contiguous single carrier of UL 256 QAM","Huawei, Hisilicon","Xiang (Steven) Chen","41576","other","Approval","MPR simualtion results on SC for UL 256QAM","","228","8.15.2.1","MPR/A-MPR [LTE_UL_CAP_enh-Core]",77800000,"approved","2016-11-03T13:02:47.560","2016-11-04T15:25:33.677","","","Rel-14","","","LTE_UL_CAP_enh-Core","","","","","","","","",""]
["R4-1609396","MPR requirement on uncontiguous single carrier for UL 256 QAM","Huawei, Hisilicon","Xiang (Steven) Chen","41576","discussion","Discussion","MPR simualtion results on uncontiguous SC for UL 256QAM","","228","8.15.2.1","MPR/A-MPR [LTE_UL_CAP_enh-Core]",77900000,"noted","2016-11-03T13:02:47.607","2016-11-04T15:25:33.677","","","Rel-14","","","LTE_UL_CAP_enh-Core","","","","","","","","",""]
["R4-1609397","MPR requirement on CA for UL 256 QAM","Huawei, Hisilicon","Xiang (Steven) Chen","41576","discussion","Discussion","---","","228","8.15.2.1","MPR/A-MPR [LTE_UL_CAP_enh-Core]",939700000,"noted","2016-11-03T13:02:47.623","2016-11-04T15:25:33.677","","","Rel-14","","","LTE_UL_CAP_enh-Core","","","","","","","","",""]
["R4-1609398","WF on MPR requirment for SC of UL 256QAM","Huawei, Hisilicon","Xiang (Steven) Chen","41576","other","Approval","---","","228","8.15.2.1","MPR/A-MPR [LTE_UL_CAP_enh-Core]",964500000,"revised","2016-11-03T13:02:47.653","2016-11-04T15:25:33.693","","R4-1610778","Rel-14","","","LTE_UL_CAP_enh-Core","","","","","","","","",""]
["R4-1609399","WF on MPR/A-MPR for CA of  UL 256QAM","Huawei, Hisilicon","Xiang (Steven) Chen","41576","other","Approval","---","","228","8.15.2.1","MPR/A-MPR [LTE_UL_CAP_enh-Core]",982300000,"revised","2016-11-03T13:02:47.687","2016-11-04T15:25:33.693","","R4-1610779","Rel-14","","","LTE_UL_CAP_enh-Core","","","","","","","","",""]
["R4-1609400","ACLR requirement for HPUE B3_B20_B28","Huawei, Hisilicon","Xiang (Steven) Chen","41576","discussion","Discussion","---","","234","8.16.2","UE RF (36.101)  [LTE_HPUE_B3_B20_B28]",940000000,"noted","2016-11-03T13:02:47.733","2016-11-07T09:47:13.270","","","Rel-14","","","LTE_HPUE_B3_B20_B28","","","","","","","","",""]
["R4-1609401","Introduction of completed R14 2DL/2UL band combinations to TS 36.101","Huawei, Hisilicon","Xiang (Steven) Chen","41576","CR","Agreement","Big CR for 2DL/2UL","","176","8.6.1","Rapporteur Input (WID/CRs) [LTE_CA_R14_2DL2UL-Core]",940200000,"agreed","2016-11-03T13:02:47.747","2016-11-19T17:47:25.553","","","Rel-14","36.101","14.1.0","LTE_CA_R14_2DL2UL-Core","4003","","B","RP-162403","","","","",""]
["R4-1609402","Revised WID: 2DL 2UL basket WI","Huawei, Hisilicon","Xiang (Steven) Chen","41576","WID revised","Endorsement","2DL/2UL WID revision","","176","8.6.1","Rapporteur Input (WID/CRs) [LTE_CA_R14_2DL2UL-Core]",942100000,"endorsed","2016-11-03T13:02:47.857","2016-11-04T12:11:05.703","","","Rel-14","","","LTE_CA_R14_2DL2UL-Core","","","","","","","","",""]
["R4-1609403","New Work Item LTE Band 42 HPUE","Huawei, Hisilicon","Xiang (Steven) Chen","41576","WID new","Information","---","","430","13","Revision of the Work Plan",916600000,"available","2016-11-03T13:02:47.887","2016-11-04T12:11:05.703","","","","","","","","","","","","","","",""]
["R4-1609404","Motivation for new work item on high power UE for Band 42","Huawei, Hisilicon","Xiang (Steven) Chen","41576","discussion","Discussion","---","","430","13","Revision of the Work Plan",916700000,"available","2016-11-03T13:02:47.903","2016-11-04T12:11:05.717","","","","","","","","","","","","","","",""]
["R4-1609405","NR coexistence calibration results in indoor scenario","Huawei, Hisilicon","Xiang (Steven) Chen","41576","discussion","Discussion","---","","410","11.3.1","Co-existence [FS_NR_newRAT]",156000,"revised","2016-11-03T13:02:47.920","2016-11-04T15:25:33.693","","R4-1610567","","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1609406","Discussion on NR DL coexistence results in urban macro scenario","Huawei, Hisilicon","Xiang (Steven) Chen","41576","discussion","Discussion","---","","410","11.3.1","Co-existence [FS_NR_newRAT]",16000000,"noted","2016-11-03T13:02:47.950","2016-11-04T15:25:33.693","","","","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1609407","Discussion on NR UL coexistence results in urban macro scenario","Huawei, Hisilicon","Xiang (Steven) Chen","41576","discussion","Discussion","---","","410","11.3.1","Co-existence [FS_NR_newRAT]",35400000,"noted","2016-11-03T13:02:47.967","2016-11-04T15:25:33.693","","","","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1609408","NR coexistence calibration results in dense urban scenario","Huawei, Hisilicon","Xiang (Steven) Chen","41576","discussion","Discussion","---","","410","11.3.1","Co-existence [FS_NR_newRAT]",356000,"revised","2016-11-03T13:02:47.997","2016-11-04T15:25:33.710","","R4-1610568","","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1609409","TP for 38.803 SINR vs throughput mapping","Huawei, Hisilicon","Xiang (Steven) Chen","41576","pCR","Discussion","---","","410","11.3.1","Co-existence [FS_NR_newRAT]",941000000,"revised","2016-11-03T13:02:48.030","2016-11-04T15:25:33.710","","R4-1610570","","38.803","0.3.0","FS_NR_newRAT","","","","","","","","",""]
["R4-1609410","Consideration on NF for NR","Huawei, Hisilicon","Xiang (Steven) Chen","41576","other","Approval","This contribution is for approval.","","410","11.3.1","Co-existence [FS_NR_newRAT]",949800000,"noted","2016-11-03T13:02:48.043","2016-11-04T12:14:21.013","","","","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1609411","Further discussion on spectrum utilization","Huawei, Hisilicon","Xiang (Steven) Chen","41576","other","Approval","This contribution is for approval.","","415","11.5.1","Common issues for UE and BS [FS_NR_newRAT]",927300000,"noted","2016-11-03T13:02:48.077","2016-11-04T12:14:21.030","","","","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1609412","Consideration on different guard band for mixed numerologies","Huawei, Hisilicon","Xiang (Steven) Chen","41576","other","Approval","This contribution is for approval.","","415","11.5.1","Common issues for UE and BS [FS_NR_newRAT]",94140000,"noted","2016-11-03T13:02:48.090","2016-11-04T12:14:21.030","","","","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1609413","Consideration on In-band emission requirements for mixed numerologies","Huawei, Hisilicon","Xiang (Steven) Chen","41576","other","Approval","This contribution is for approval.","","415","11.5.1","Common issues for UE and BS [FS_NR_newRAT]",48600000,"noted","2016-11-03T13:02:48.123","2016-11-04T12:14:21.047","","","","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1609414","Consideration on In-band selectivity requirements for mixed numerologies","Huawei, Hisilicon","Xiang (Steven) Chen","41576","other","Approval","This contribution is for approval.","","415","11.5.1","Common issues for UE and BS [FS_NR_newRAT]",48800000,"noted","2016-11-03T13:02:48.137","2016-11-04T12:14:21.060","","","","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1609415","On EU update on 3400-3800MHz","Huawei, Hisilicon","Xiang (Steven) Chen","41576","discussion","Discussion","---","","407","11.1","General   [FS_NR_newRAT]",941600010,"noted","2016-11-03T13:02:48.170","2016-11-04T12:14:21.060","","","","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1609416","Reply LS on Suitability of technical conditions of ECC DEC (11) 06 for 5G","Huawei, Hisilicon","Xiang (Steven) Chen","41576","LS out","Approval","---","","407","11.1","General   [FS_NR_newRAT]",962900000,"withdrawn","2016-11-03T13:02:48.187",null,"","","","","","FS_NR_newRAT","","","","","ECC PT1","ECC PT1","","",""]
["R4-1609417","Discussion on RF parameters for WP5D","Huawei, Hisilicon","Xiang (Steven) Chen","41576","discussion","Discussion","We provide discussion on the details of RF parameters for the response to WP5D.","","411","11.3.2","RF parameters not related co-existence [FS_NR_newRAT]",941700000,"noted","2016-11-03T13:02:48.217","2016-11-04T12:15:12.323","","","","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1609418","Further consideration on spectrum emission mask","Huawei, Hisilicon","Xiang (Steven) Chen","41576","discussion","Discussion","---","","421","11.5.3.1","Transmitter characteristics [FS_NR_newRAT]",44100000,"noted","2016-11-03T13:02:48.230","2016-11-04T12:14:21.077","","","","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1609419","On wider bandwidth operation for NR","Huawei, Hisilicon","Xiang (Steven) Chen","41576","other","Approval","This contribution is for approval.","","407","11.1","General   [FS_NR_newRAT]",59000000,"noted","2016-11-03T13:02:48.263","2016-11-04T12:14:21.077","","","","","","","","","","","","","","",""]
["R4-1609420","Discussion on SINR range for WP5D","Huawei, Hisilicon","Xiang (Steven) Chen","41576","discussion","Discussion","---","","410","11.3.1","Co-existence [FS_NR_newRAT]",940900000,"noted","2016-11-03T13:02:48.277","2016-11-04T15:25:33.710","","","","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1609421","TR 36.714-02-02: 2DL/2UL inter-band CA R14 v0.5.0","Huawei","Ye Liu","57639","draft TR","","2DL/2UL inter-band CA TR v0.5.0","","176","8.6.1","Rapporteur Input (WID/CRs) [LTE_CA_R14_2DL2UL-Core]",98300,"approved","2016-11-03T13:19:43.213","2016-11-04T11:21:06.277","","","Rel-14","36.714-02-02","0.5.0","LTE_CA_R14_2DL2UL-Core","","","","","","","","",""]
["R4-1609422","Test method limitations for the One Dimensional Compact Range Chamber method","KATHREIN-Werke KG","Christiane Dietrich","61230","CR","Approval","The test method limitation section creates the wrong impression that the One Dimensional Compact Range Chamber is only useable for DUTs with one column. The usage of the chamber is with certain restrictions also usable for DUTs with more than one column.","","22","5.1.1","Technical Report (37.842) [AAS_BS_LTE_UTRA-Core]",3600000,"noted","2016-11-03T14:44:19.453","2016-11-03T14:47:08.653","","R4-1700464","Rel-13","37.842","13.0.0","AAS_BS_LTE_UTRA-Core","0007","","F","","","","","",""]
["R4-1609423","Discussion on eLAA demodulation test","Huawei, Hisilicon","Xiang (Steven) Chen","41576","discussion","Discussion","In this contribution, we discuss the Rel-14 eLAA demodulation test","","257","8.18.6","UE/BS demodulation and CSI (36.101/36.104) [LTE_eLAA-Perf]",942400000,"noted","2016-11-03T14:56:36.290","2016-11-07T11:36:01.743","","","","","","LTE_eLAA-Perf","","","","","","","","",""]
["R4-1609424","Simulation assumptions for eLAA","Huawei, Hisilicon","Xiang (Steven) Chen","41576","other","Approval","This contribution will try to provide the simulation assumptions for eLAA.","","257","8.18.6","UE/BS demodulation and CSI (36.101/36.104) [LTE_eLAA-Perf]",975300000,"noted","2016-11-03T14:56:36.307","2016-11-07T11:36:01.743","","","","","","LTE_eLAA-Perf","","","","","","","","",""]
["R4-1609425","Scope for finalization of Rel-13 LAA performance part","Huawei, Hisilicon","Xiang (Steven) Chen","41576","discussion","Discussion","In this contribution, we propose to move discussion on extension of LAA demodulation performance requirements for 3 or more than 3 CC to TEI.","","107","6.2.4.1","General [LTE_LAA-Perf]",9425000,"noted","2016-11-03T14:56:36.320","2016-11-07T11:36:01.743","","","","","","LTE_LAA-Perf","","","","","","","","",""]
["R4-1609426","Discussion on the extension of LAA demodulation performance requirements to cover 3 or more CCs","Huawei, Hisilicon","Xiang (Steven) Chen","41576","discussion","Discussion","This paper gives our view about the extension of LAA demodulation requirements with new LAA band combinations introducation in Rel-14 that have 3 or more CCs including more licensed CCs and/or licensed CCs, includes test applcaibility, release independenc","","107","6.2.4.1","General [LTE_LAA-Perf]",917600000,"noted","2016-11-03T14:56:36.337","2016-11-07T11:36:01.760","","","","","","TEI14","","","","","","","","",""]
["R4-1609427","Discussion on burst transmission pattern for LAA demodulation requirements with more LAA SCells","Huawei, Hisilicon","Xiang (Steven) Chen","41576","discussion","Discussion","With new LAA band combinations introducation in Rel-14 that have more than one LAA SCell, the current agreed burst transmisson pattern that is applicable to one LAA Scell needs to be updated","","107","6.2.4.1","General [LTE_LAA-Perf]",917800000,"noted","2016-11-03T14:56:36.350","2016-11-07T11:36:01.760","","","","","","TEI14","","","","","","","","",""]
["R4-1609428","Update simulation results for LAA PDSCH","Huawei, Hisilicon","Xiang (Steven) Chen","41576","discussion","Discussion","In this contribution, we provides our updated simulation results about LAA PDSCH.","","108","6.2.4.2","PDSCH [LTE_LAA-Perf]",13400000,"noted","2016-11-03T14:56:36.383","2016-11-07T11:36:01.760","","","","","","LTE_LAA-Perf","","","","","","","","",""]
["R4-1609429","Update simulation results for LAA PDCCH","Huawei, Hisilicon","Xiang (Steven) Chen","41576","discussion","Discussion","In this contribution, we provides our updated simulation results for LAA PDCCH.","","109","6.2.4.3","PDCCH [LTE_LAA-Perf]",64300000,"noted","2016-11-03T14:56:36.397","2016-11-07T11:36:01.760","","","","","","","","","","","","","","",""]
["R4-1609430","Simulation results for NPBCH","Huawei, Hisilicon","Xiang (Steven) Chen","41576","discussion","Discussion","In this contribution, we share our simulation results about NPBCH, includes multiple decoding trying for case 2","","129","6.3.4.1.1","NPBCH  [NB_IOT-Perf]",52100000,"noted","2016-11-03T14:56:36.413","2016-11-07T11:36:01.777","","","","","","NB_IOT-Perf","","","","","","","","",""]
["R4-1609431","Simulation results for NPDCCH","Huawei, Hisilicon","Xiang (Steven) Chen","41576","discussion","Discussion","In this contribution, we share our simulation results about NPDCCH with impairment after taking into account the DC leakage.","","130","6.3.4.1.2","NPDCCH [NB_IOT-Perf]",932000000,"noted","2016-11-03T14:56:36.430","2016-11-07T11:36:01.777","","","","","","NB_IOT-Perf","","","","","","","","",""]
["R4-1609432","Discussion on transmission signal pattern for NPDSCH","Huawei, Hisilicon","Xiang (Steven) Chen","41576","discussion","Discussion","In this contribution, we give our view about the 3% NPDCCH BLER impact to NPDSCH performance as per the agreed WF R4-168948:\nOption 1: Multiply NPDSCH throughput results with [97]% to account for [3%] NPDCCH BLER\nOther options are not precluded.","","131","6.3.4.1.3","NPDSCH [NB-IOT-Perf]",967400000,"revised","2016-11-03T14:56:36.460","2016-11-07T11:36:01.777","","R4-1610538","","","","NB_IOT-Perf","","","","","","","","",""]
["R4-1609433","Simulation results for NPDSCH","Huawei, Hisilicon","Xiang (Steven) Chen","41576","discussion","Discussion","In this contribution, we share our simulation results about NPDSCH with impairment after taking into account the DC leakage.","","131","6.3.4.1.3","NPDSCH [NB-IOT-Perf]",911100000,"noted","2016-11-03T14:56:36.477","2016-11-07T11:36:01.777","","","","","","","","","","","","","","",""]
["R4-1609434","Updates to CR for NPDSCH (Rel-13)","Huawei, Hisilicon","Xiang (Steven) Chen","41576","CR","Agreement","This CR updates the existing NPDSCH perf test in Rel-13: including those endorsed R4-168741 in RAN4#80Bis and content related the signal transmission pattern agreed in WF R4-168948 and possible SNR requirements","","131","6.3.4.1.3","NPDSCH [NB-IOT-Perf]",943400000,"revised","2016-11-03T14:56:36.493","2016-11-07T11:36:01.790","","R4-1610558","Rel-13","36.101","13.5.0","NB_IOT-Perf","4004","","F","","","","","",""]
["R4-1609435","CR: Updates to NPDSCH demodulation requirements for NB-IoT (Rel-14)","Huawei, Hisilicon","Xiang (Steven) Chen","41576","CR","Agreement","This CR updates the existing NPDSCH perf test in Rel-14: including those endorsed R4-168741 in RAN4#80Bis and content related the signal transmission pattern agreed in WF R4-168948 and possible SNR requirements","","131","6.3.4.1.3","NPDSCH [NB-IOT-Perf]",951900000,"agreed","2016-11-03T14:56:36.587","2016-11-19T17:47:25.553","","","Rel-14","36.101","14.1.0","NB_IOT-Perf","4005","","A","RP-162379","","","","",""]
["R4-1609436","Updates to CR for NPDCCH (Rel-13)","Huawei, Hisilicon","Xiang (Steven) Chen","41576","CR","Agreement","Resubmission the endorsed R4-167573","","130","6.3.4.1.2","NPDCCH [NB_IOT-Perf]",967600000,"noted","2016-11-03T14:56:36.663","2016-11-07T11:36:01.680","","","Rel-13","36.101","13.5.0","NB_IOT-Perf","4006","","F","","","","","",""]
["R4-1609437","Updates to CR for NPDCCH (Rel-14)","Huawei, Hisilicon","Xiang (Steven) Chen","41576","CR","Agreement","Resubmission the endorsed R4-167573","","130","6.3.4.1.2","NPDCCH [NB_IOT-Perf]",977700000,"withdrawn","2016-11-03T14:56:36.773",null,"","","Rel-14","36.101","14.1.0","NB_IOT-Perf","4007","","A","","","","","",""]
["R4-1609438","Summary for NB-IoT BS simulation results","Huawei","Xiang (Steven) Chen","41576","other","Information","This contribution collects the simulation results about NPRACH, NPUSCH format 1 and NPUSCH format 2","","132","6.3.4.2","BS Demodulation  [NB_IOT-Perf]",60600000,"noted","2016-11-03T14:56:36.867","2016-11-19T17:47:25.567","","","","","","NB_IOT-Perf","","","","","","","","",""]
["R4-1609439","Simulation results for NPRACH","Huawei","Xiang (Steven) Chen","41576","discussion","Discussion","In this contribution, we share our simulation results with the newly agreed WF R4-168745 in RAN4#80Bis with Timing limit = 3.646us and Timing Offset = 30us","","133","6.3.4.2.1","NPRACH  [NB_IOT-Perf]",924300000,"noted","2016-11-03T14:56:36.883","2016-11-07T11:36:01.680","","","","","","NB_IOT-Perf","","","","","","","","",""]
["R4-1609440","Simulation results for NPUSCH format 1","Huawei","Xiang (Steven) Chen","41576","discussion","Discussion","In this contribution, we share our simulation results about NPUSCH format 1 with impairment","","134","6.3.4.2.2","NPUSCH format 1 [NB_IOT-Perf]",924700000,"noted","2016-11-03T14:56:36.897","2016-11-07T11:36:01.697","","","","","","NB_IOT-Perf","","","","","","","","",""]
["R4-1609441","Simulation results for NPUSCH format 2","Huawei","Xiang (Steven) Chen","41576","discussion","Discussion","In this contribution, we share our simulation results about NPUSCH format 2 with impairment","","135","6.3.4.2.3","NPUSCH format 2 [NB_IOT-Perf]",934300000,"noted","2016-11-03T14:56:36.913","2016-11-07T11:36:01.697","","","","","","NB_IOT-Perf","","","","","","","","",""]
["R4-1609442","CR for NPRACH demod perf requirement(Rel-13)","Huawei","Xiang (Steven) Chen","41576","CR","Agreement","This is the resubmisson of endorsed CR R4-168777 in RAN4#80Bis.","","133","6.3.4.2.1","NPRACH  [NB_IOT-Perf]",924600000,"revised","2016-11-03T14:56:36.943","2016-11-07T11:36:01.697","","R4-1610560","Rel-13","36.104","13.5.0","NB_IOT-Perf","0890","","B","","","","","",""]
["R4-1609443","CR: Demodulation requirements for NPRACH (Rel-14)","Huawei","Xiang (Steven) Chen","41576","CR","Agreement","This is the mirror CR for NPRACH in Rel-14.","","133","6.3.4.2.1","NPRACH  [NB_IOT-Perf]",943900000,"agreed","2016-11-03T14:56:37.037","2016-11-19T17:47:25.567","","","Rel-14","36.104","14.1.0","NB_IOT-Perf","0891","","A","RP-162379","","","","",""]
["R4-1609444","Updates to NPUSCH format 1 demod perf requirements(Rel-13)","Huawei","Xiang (Steven) Chen","41576","CR","Agreement","This CR updates the SNR value for NPUSCH format 1 demodulation performance requirements defined in TS 36.104 Release 13 as per the aligned simulation results.","","134","6.3.4.2.2","NPUSCH format 1 [NB_IOT-Perf]",944000000,"revised","2016-11-03T14:56:37.117","2016-11-07T11:36:01.697","","R4-1610563","Rel-13","36.104","13.5.0","NB_IOT-Perf","0892","","F","","","","","",""]
["R4-1609445","CR: Updates to demodulation requirements for NPUSCH format 1 (Rel-14)","Huawei","Xiang (Steven) Chen","41576","CR","Agreement","This is the mirror CR for NPUSCH format 1 demodulation performance requirements defined in TS 36.104 Release 14","","134","6.3.4.2.2","NPUSCH format 1 [NB_IOT-Perf]",944500000,"agreed","2016-11-03T14:56:37.227","2016-11-19T17:47:25.583","","","Rel-14","36.104","14.1.0","NB_IOT-Perf","0893","","A","RP-162379","","","","",""]
["R4-1609446","Updates to NPUSCH format 1 demod conformance test(Rel-13)","Huawei","Xiang (Steven) Chen","41576","CR","Agreement","This CR updates the SNR value for NPUSCH format 1 demod conformance test defined in TS 36.141 Release 13","","134","6.3.4.2.2","NPUSCH format 1 [NB_IOT-Perf]",944600000,"revised","2016-11-03T14:56:37.303","2016-11-07T11:36:01.713","","R4-1610564","Rel-13","36.141","13.5.0","NB_IOT-Perf","0925","","F","","","","","",""]
["R4-1609447","CR: Updates to NPUSCH format 1 demodulation conformance test (Rel-14)","Huawei","Xiang (Steven) Chen","41576","CR","Agreement","This is the mirror CR for NPUSCH format 1 demod conformance test defined in TS 36.141 Release 14","","134","6.3.4.2.2","NPUSCH format 1 [NB_IOT-Perf]",978000000,"agreed","2016-11-03T14:56:37.397","2016-11-19T17:47:25.583","","","Rel-14","36.141","14.1.0","NB_IOT-Perf","0926","","A","RP-162379","","","","",""]
["R4-1609448","Updates to NPUSCH format 2 demod perf requirements(Rel-13)","Huawei","Xiang (Steven) Chen","41576","CR","Agreement","This CR updates the SNR value for NPUSCH format 2 demodulation performance requirements defined in TS 36.104 Release 13  as per the aligned simulation results.","","135","6.3.4.2.3","NPUSCH format 2 [NB_IOT-Perf]",944100000,"revised","2016-11-03T14:56:37.490","2016-11-07T11:36:01.713","","R4-1610565","Rel-13","36.104","13.5.0","NB_IOT-Perf","0894","","F","","","","","",""]
["R4-1609449","Updates to NPUSCH format 2 demod perf requirements(Rel-14)","Huawei","Xiang (Steven) Chen","41576","CR","Agreement","This is the mirror CR for NPUSCH format 2 demodulation performance requirements defined in TS 36.104 Release 14","","135","6.3.4.2.3","NPUSCH format 2 [NB_IOT-Perf]",944900000,"revised","2016-11-03T14:56:37.567","2016-11-19T17:47:25.583","","R4-1610631","Rel-14","36.104","14.1.0","NB_IOT-Perf","0895","","A","","","","","",""]
["R4-1609450","Updates to NPUSCH format 2 demod conformance test(Rel-13)","Huawei","Xiang (Steven) Chen","41576","CR","Agreement","This CR updates the SNR value for NPUSCH format 2 demod conformance test defined in TS 36.141 Release 13  as per the aligned simulation results.","","135","6.3.4.2.3","NPUSCH format 2 [NB_IOT-Perf]",945000000,"revised","2016-11-03T14:56:37.663","2016-11-07T11:36:01.713","","R4-1610566","Rel-13","36.141","13.5.0","NB_IOT-Perf","0927","","F","","","","","",""]
["R4-1609451","CR: Updates to NPUSCH format 2 demodulation conformance test (Rel-14)","Huawei","Xiang (Steven) Chen","41576","CR","Agreement","This is the mirror CR for NPUSCH format 2 demod conformance test defined in TS 36.141 Release 14","","135","6.3.4.2.3","NPUSCH format 2 [NB_IOT-Perf]",978100000,"agreed","2016-11-03T14:56:37.757","2016-11-19T17:47:25.600","","","Rel-14","36.141","14.1.0","NB_IOT-Perf","0928","","A","RP-162379","","","","",""]
["R4-1609452","Discussion and Simulation on PHICH demod performance for Cat.1 UE with 1Rx","Huawei, Hisilicon","Xiang (Steven) Chen","41576","discussion","Discussion","This contribution discuss on FRC definition for PHICH to facilitate the simulation results for Cat.1 like UE with 1Rx as per the agreed WF R4-168673 in RAN4#80Bis","","336","8.27.5","UE demodulation (36.101) [LTE_UE_cat_1RX-Perf]",970100000,"noted","2016-11-03T14:56:37.833","2016-11-07T11:36:01.713","","","","","","LTE_UE_cat_1RX-Perf","","","","","","","","",""]
["R4-1609453","Discussion and simulation on PDSCH TM2, TM4 and TM9 demod performance","Huawei, Hisilicon","Xiang (Steven) Chen","41576","discussion","Discussion","This contribution discuss the PDSCH demod performance requirements introduction and the reated FRC for TM2/TM4/TM9 PDSCH demod perf for Cat.1 like UE with 1Rx as per the agreed WF R4-168673 in RAN4#80Bis","","336","8.27.5","UE demodulation (36.101) [LTE_UE_cat_1RX-Perf]",969800000,"noted","2016-11-03T14:56:37.867","2016-11-07T11:36:01.727","","","","","","LTE_UE_cat_1RX-Perf","","","","","","","","",""]
["R4-1609454","Discussion on deployment scenarios in BS IC","Huawei","Xiang (Steven) Chen","41576","discussion","Discussion","In this contribution, we will further discuss the deployment scenarios for BS-IC.","","396","9.4.2","Deployment scenario [FS_LTE _IC_BS]",929900000,"noted","2016-11-03T14:56:37.880","2016-11-07T11:33:55.430","","","","","","FS_LTE_IC_BS","","","","","","","","",""]
["R4-1609455","TP: deploymenet scenarios for BS-IC","Huawei","Xiang (Steven) Chen","41576","other","Approval","This TP provides the deployment scenarios for BS-IC.","","396","9.4.2","Deployment scenario [FS_LTE _IC_BS]",945400000,"revised","2016-11-03T14:56:37.897","2016-11-07T11:33:55.430","","R4-1610864","","","","","","","","","","","","",""]
["R4-1609456","Discussion on reference receiver to be used for BS IC in this SI","Huawei","Xiang (Steven) Chen","41576","discussion","Discussion","In this contribution, we will further discuss the reference receiver for BS-IC.","","397","9.4.3","Reference receiver [FS_LTE _IC_BS]",945500000,"noted","2016-11-03T14:56:37.927","2016-11-07T11:33:55.447","","","","","","FS_LTE_IC_BS","","","","","","","","",""]
["R4-1609457","Discussion on interference model","Huawei","Xiang (Steven) Chen","41576","discussion","Discussion","According to the approved WF R4-168976, this contribution provides our view on the intra-cell interference model and the inter-cell interference model.","","398","9.4.4","Interference model [FS_LTE _IC_BS]",945700000,"noted","2016-11-03T14:56:37.943","2016-11-07T11:33:55.447","","","","","","FS_LTE_IC_BS","","","","","","","","",""]
["R4-1609458","Discussion on the link evaluation parameters","Huawei","Xiang (Steven) Chen","41576","discussion","Discussion","This contribution gives our view about the link evaluation paramters to be used in the following simulations.","","399","9.4.5","Link level evaluation [FS_LTE _IC_BS]",945800000,"noted","2016-11-03T14:56:37.957","2016-11-07T11:33:55.417","","","","","","FS_LTE_IC_BS","","","","","","","","",""]
["R4-1609459","CR on cleaning up Rel-13 eMTC PUSCH performance requirements","Huawei","Xiang (Steven) Chen","41576","CR","Agreement","This CR will clean up the requirements for PUSCH.","","101","6.1.4","Maintenance of BS performance (36.104, 36.141) [LTE_MTCe2_L1-Perf]",945900000,"agreed","2016-11-03T14:56:37.990","2016-11-07T11:30:26.890","","","Rel-13","36.104","13.5.0","LTE_MTCe2_L1-Perf","0896","","F","RP-162382","","","","",""]
["R4-1609460","CR on cleaning up Rel-14 eMTC PUSCH performance requirements","Huawei","Xiang (Steven) Chen","41576","CR","Agreement","This CR will clean up the requirements for PUSCH.","","101","6.1.4","Maintenance of BS performance (36.104, 36.141) [LTE_MTCe2_L1-Perf]",946000000,"agreed","2016-11-03T14:56:38.083","2016-11-19T17:47:25.600","","","Rel-14","36.104","14.1.0","LTE_MTCe2_L1-Perf","0897","","A","RP-162382","","","","",""]
["R4-1609461","CR on cleaning up Rel-13 eMTC PUSCH conformance test","Huawei","Xiang (Steven) Chen","41576","CR","Agreement","This CR will clean up the conformance test for PUSCH.","","101","6.1.4","Maintenance of BS performance (36.104, 36.141) [LTE_MTCe2_L1-Perf]",946100000,"revised","2016-11-03T14:56:38.193","2016-11-07T11:30:26.890","","R4-1610674","Rel-13","36.141","13.5.0","LTE_MTCe2_L1-Perf","0929","","F","","","","","",""]
["R4-1609462","CR on cleaning up Rel-14 eMTC PUSCH conformance test","Huawei","Xiang (Steven) Chen","41576","CR","Agreement","This CR will clean up the conformance test for PUSCH.","","101","6.1.4","Maintenance of BS performance (36.104, 36.141) [LTE_MTCe2_L1-Perf]",946200000,"agreed","2016-11-03T14:56:38.287","2016-11-22T12:17:26.953","","","Rel-14","36.141","14.1.0","LTE_MTCe2_L1-Perf","0930","","A","RP-162382","","","","",""]
["R4-1609463","Evaluation for eMTC PBCH performance requirements","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","Discussion","In this contribution, we provide the simulation results and view on reqiurements for eMTC PBCH demodulation performance requirements based on the agreed WF R4-164608 .","","97","6.1.2.1","PBCH [LTE_MTCe2_L1-Perf]",911400000,"noted","2016-11-03T14:56:38.410","2016-11-07T11:30:26.907","","","","","","LTE_MTCe2_L1-Perf","","","","","","","","",""]
["R4-1609464","CR for Rel-13 eMTC PBCH demodulation requirement for enhanced coverage","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","Agreement","This CR will introduce the PBCH performance requirements value for 40ms.","","97","6.1.2.1","PBCH [LTE_MTCe2_L1-Perf]",946300000,"revised","2016-11-03T14:56:38.443","2016-11-07T11:30:26.907","","R4-1610863","Rel-13","36.101","13.5.0","LTE_MTCe2_L1-Perf","4008","","F","","","","","",""]
["R4-1609465","CR for Rel-14 eMTC PBCH demodulation requirement for enhanced coverage","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","Agreement","This CR will introduce the PBCH performance requirements value for 40ms.","","97","6.1.2.1","PBCH [LTE_MTCe2_L1-Perf]",946400000,"agreed","2016-11-03T14:56:38.537","2016-11-19T17:47:25.600","","","Rel-14","36.101","14.1.0","LTE_MTCe2_L1-Perf","4009","","A","RP-162382","","","","",""]
["R4-1609466","Simulation results for MPDCCH performance","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","Discussion","This contribution resubmits ideal and impairment simulation results for FDD mode  and provide the simulation results for TDD mode.","","98","6.1.2.2","MPDCCH [LTE_MTCe2_L1-Perf]",926700000,"noted","2016-11-03T14:56:38.630","2016-11-07T11:30:26.907","","","","","","LTE_MTCe2_L1-Perf","","","","","","","","",""]
["R4-1609467","Discussion and evaluation for PDSCH performance requirements","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","Discussion","In this paper, we will discuss the open issuses for the PDSCH and provide our simualtion reuslts for PDSCH.","","99","6.1.2.3","MPDSCH [LTE_MTCe2_L1-Perf]",946700000,"noted","2016-11-03T14:56:38.647","2016-11-07T11:30:26.827","","","","","","LTE_MTCe2_L1-Perf","","","","","","","","",""]
["R4-1609468","Discussion on CQI definition test","Huawei, Hisilicon","Xiang (Steven) Chen","41576","discussion","Discussion","This contribution give the view on CQI definition test.","","100","6.1.3","UE CSI reporting (36.101) [LTE_MTCe2_L1-Perf]",946800000,"noted","2016-11-03T14:56:38.660","2016-11-07T11:30:26.827","","","","","","LTE_MTCe2_L1-Perf","","","","","","","","",""]
["R4-1609469","Collection of simulation results for UE enhancement","Huawei, HiSilicon","Xiang (Steven) Chen","41576","other","Information","This contribution update the collection of simulation results for UE enhancement","","345","8.28.3.1","Enhancement for bi-directional RRH arrangement [LTE_high_speed]",946900000,"revised","2016-11-03T14:56:38.690","2016-11-19T17:47:25.613","","R4-1610681","","","","LTE_high_speed","","","","","","","","",""]
["R4-1609470","Simulation results for UE enhancement in SFN scenario.","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","Discussion","In this contribution, we resubmit the simulation results for alignment.","","345","8.28.3.1","Enhancement for bi-directional RRH arrangement [LTE_high_speed]",947100000,"noted","2016-11-03T14:56:38.707","2016-11-07T11:30:26.843","","","","","","LTE_high_speed","","","","","","","","",""]
["R4-1609471","CR for UE enhancement in SFN scenario","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","Agreement","This CR provides the framework for SFN demodulation performance requirements based on the endorsed CR in last meeting.","","345","8.28.3.1","Enhancement for bi-directional RRH arrangement [LTE_high_speed]",992600000,"revised","2016-11-03T14:56:38.737","2016-11-07T11:30:26.843","","R4-1610696","Rel-14","36.101","14.1.0","LTE_high_speed","4010","","B","","","","","",""]
["R4-1609472","Evaluation and discusion on CSI test for UE enhancement in SFN scenario.","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","Discussion","In this paper, we will evaluate and discuss  the CSI test.","","347","8.28.3.3","CQI reporting [LTE_high_speed]",990000000,"noted","2016-11-03T14:56:38.817","2016-11-07T11:30:26.860","","","","","","LTE_high_speed","","","","","","","","",""]
["R4-1609473","Further discussion on unidirectional  SFN scenario","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","Discussion","In this contribution,we further discuss the UE performance in the unidirectional deployment and give our view on unidirectional deployment.","","346","8.28.3.2","Unidirectional RRH arrangement [LTE_high_speed]",990100000,"noted","2016-11-03T14:56:38.847","2016-11-07T11:30:26.860","","","","","","LTE_high_speed","","","","","","","","",""]
["R4-1609474","Discussion on new PRACH performance requirements","Huawei","Xiang (Steven) Chen","41576","discussion","Discussion","Since RAN1 reached agreement on new PRACH sequence, RAN4 needs to specify the new requirements correspondingly. In this contribution, we would like to trigger the discussion.","","348","8.28.4","BS demodulation (36.104/36.141) [LTE_high_speed]",947400000,"noted","2016-11-03T14:56:38.863","2016-11-07T11:30:26.860","","","","","","LTE_high_speed","","","","","","","","",""]
["R4-1609475","WF on new PRACH performance requirements","Huawei","Xiang (Steven) Chen","41576","other","Approval","In this WF, we try to capture the conclusions for PRACH requirements","","348","8.28.4","BS demodulation (36.104/36.141) [LTE_high_speed]",947500000,"approved","2016-11-03T14:56:38.893","2016-11-07T11:30:26.873","","","","","","LTE_high_speed","","","","","","","","",""]
["R4-1609476","Discussion on the PSCCH demodulation requirements for V2V","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","Discussion","In this contribution, we will discussion PSCCH demodulation requirements for V2V.","","269","8.19.4.1","Single-link PSSCH and PSCCH  [LTE_SL_V2V-Perf]",908400000,"noted","2016-11-03T14:56:38.910","2016-11-07T11:32:15.047","","","","","","LTE_SL_V2V-Perf","","","","","","","","",""]
["R4-1609477","Discussion on the PSSCH demodulation requirements for V2V","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","Discussion","In this contribution, we will discussion PSSCH demodulation requirements for V2V.","","269","8.19.4.1","Single-link PSSCH and PSCCH  [LTE_SL_V2V-Perf]",918000000,"noted","2016-11-03T14:56:38.927","2016-11-07T11:32:15.060","","","","","","LTE_SL_V2V-Perf","","","","","","","","",""]
["R4-1609478","Discussion on  power imbalance test for V2V","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","Discussion","In this contribution, we will discussion power imbalance test for V2V.","","270","8.19.4.2","Multi-link PSSCH and PSCCH [LTE_SL_V2V-Perf]",976200000,"noted","2016-11-03T14:56:38.957","2016-11-07T11:32:15.060","","","","","","LTE_SL_V2V-Perf","","","","","","","","",""]
["R4-1609479","Discussion on maximum sidelink processes test for V2V","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","Discussion","In this contribution, we will discussion  maximum sidelink processes test for V2V.","","271","8.19.4.3","Maximum process test [LTE_SL_V2V-Perf]",976300000,"noted","2016-11-03T14:56:38.973","2016-11-07T11:32:15.060","","","","","","LTE_SL_V2V-Perf","","","","","","","","",""]
["R4-1609480","Discussion on the resource pool configuration for V2V tests","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","Discussion","In this contribution, we will discussion the resource pool configuration for V2V tests.","","269","8.19.4.1","Single-link PSSCH and PSCCH  [LTE_SL_V2V-Perf]",947600000,"noted","2016-11-03T14:56:38.987","2016-11-07T11:32:15.077","","","","","","LTE_SL_V2V-Perf","","","","","","","","",""]
["R4-1609481","Simulation assumptions for V2V demodulation requiremetns","Huawei, HiSilicon, LG Electronics","Xiang (Steven) Chen","41576","other","Approval","In this contribution, we try to capture the simulation parameters for V2V demodulation tests.","","268","8.19.4","UE demodulation (36.101)  [LTE_SL_V2V-Perf]",94810000,"revised","2016-11-03T14:56:39.020","2016-11-07T11:32:15.077","","R4-1610853","","","","","","","","","","","","",""]
["R4-1609482","Evaluations on feasibility test scenarios and reference receiver for enhanced SU-MIMO","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","Discussion","In this contribution, we will present the guidelines for the test case selection for eSU-MIMO.","","370","8.31.3.1","Performance evaluation: scenarios and receiver [LTE_eCRSIM_eSUMIMO]",948500000,"noted","2016-11-03T14:56:39.037","2016-11-07T11:32:15.077","","","","","","LTE_eCRSIM_eSUMIMO","","","","","","","","",""]
["R4-1609483","Evaluations on the rank 2 with lower MCS for enhanced SU-MIMO","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","Discussion","In this contribution, we will evaluate on the rank 2 with lower MCS for enhanced SU-MIMO.","","370","8.31.3.1","Performance evaluation: scenarios and receiver [LTE_eCRSIM_eSUMIMO]",948600000,"noted","2016-11-03T14:56:39.050","2016-11-07T11:32:15.090","","","","","","LTE_eCRSIM_eSUMIMO","","","","","","","","",""]
["R4-1609484","Evaluations on the rank 2 with 256QAM for enhanced SU-MIMO","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","Discussion","In this contribution, we will evaluate on the rank 2 with 256QAM for enhanced SU-MIMO.","","370","8.31.3.1","Performance evaluation: scenarios and receiver [LTE_eCRSIM_eSUMIMO]",948700000,"noted","2016-11-03T14:56:39.080","2016-11-07T11:32:15.090","","","","","","LTE_eCRSIM_eSUMIMO","","","","","","","","",""]
["R4-1609485","Evaluations on the rank 3/4 with low MCS for enhanced SU-MIMO","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","Discussion","In this contribution, we will evaluate on the rank 3/4 with lower MCS for enhanced SU-MIMO.","","370","8.31.3.1","Performance evaluation: scenarios and receiver [LTE_eCRSIM_eSUMIMO]",970900000,"noted","2016-11-03T14:56:39.113","2016-11-07T11:32:15.090","","","","","","LTE_eCRSIM_eSUMIMO","","","","","","","","",""]
["R4-1609486","Evaluations on the rank 3/4 with 256QAM for enhanced SU-MIMO","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","Discussion","In this contribution, we will evaluate on the rank 3/4 with 256QAM for enhanced SU-MIMO.","","370","8.31.3.1","Performance evaluation: scenarios and receiver [LTE_eCRSIM_eSUMIMO]",975800000,"noted","2016-11-03T14:56:39.127","2016-11-07T11:32:15.013","","","","","","LTE_eCRSIM_eSUMIMO","","","","","","","","",""]
["R4-1609487","Simulation assumptions for enhanced SU-MIMO demodulation requiremetns","Huawei, HiSilicon","Xiang (Steven) Chen","41576","other","Approval","In this contribution, we try to capture the simulation parameters for enhanced SU-MIMO demodulation tests.","","370","8.31.3.1","Performance evaluation: scenarios and receiver [LTE_eCRSIM_eSUMIMO]",70000000,"revised","2016-11-03T14:56:39.143","2016-11-07T11:32:15.030","","R4-1610715","","","","","","","","","","","","",""]
["R4-1609488","Simulation results for IRC TM2 tests with 4Rx","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","Discussion","In this contribution, we will present simulation results for IRC TM2 tests.","","33","5.2.3.2","UE demodulation and CSI [LTE_4Rx_AP_DL-Perf]",906600000,"noted","2016-11-03T14:56:39.177","2016-11-07T11:32:15.030","","","","","","","","","","","","","","",""]
["R4-1609489","Simulation results for TM9 tests with 4Rx","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","Discussion","In this contribution, we will present simulation results for TM9 tests.","","33","5.2.3.2","UE demodulation and CSI [LTE_4Rx_AP_DL-Perf]",976400000,"noted","2016-11-03T14:56:39.190","2016-11-07T11:32:15.030","","","","","","","","","","","","","","",""]
["R4-1609490","CR: Corrections for bandwidth combination sets defined for inter-band DC (Rel-13)","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","Agreement","In this CR, we will correct the wrong references for DC since the definetion of DC has been changed.","","15","4.2.4","UE demodulation performance  [WI code or TEI12]",9212000,"agreed","2016-11-03T14:56:39.223","2016-11-07T11:32:15.030","","","Rel-13","36.101","13.5.0","TEI13","4011","","F","RP-162435","","","","",""]
["R4-1609491","CR: Corrections for bandwidth combination sets defined for inter-band DC (Rel-14)","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","Agreement","In this CR, we will correct the wrong references for DC since the definetion of DC has been changed.","","15","4.2.4","UE demodulation performance  [WI code or TEI12]",13500000,"agreed","2016-11-03T14:56:39.300","2016-11-22T12:17:26.970","","","Rel-14","36.101","14.1.0","TEI14","4012","","A","RP-162408","","","","",""]
["R4-1609492","Motivation paper for downlink 8Rx antennas","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","Discussion","This contribution provides the motivation of new WI proposal for downlink 8Rx antennas","","430","13","Revision of the Work Plan",940300000,"available","2016-11-03T14:56:39.393","2016-11-07T11:33:55.430","","","","","","","","","","","","","","",""]
["R4-1609493","New WI for downlink 8Rx antennas","Huawei, HiSilicon","Xiang (Steven) Chen","41576","WID new","Information","This is the WID for downlink 8Rx antennas.","","430","13","Revision of the Work Plan",940400000,"available","2016-11-03T14:56:39.427","2016-11-07T11:33:55.430","","","","","","","","","","","","","","",""]
["R4-1609494","Band 11 PA measurements on EESS protection","Skyworks Solutions Inc.","Dominique Brunel","65099","discussion","Approval","This contribution provides inputs to the EESS band protection based on measurements of a band 11 PA","","388","9.2.2","UE RF (36.101) [FS_LTE_B11_B21_global]",949400001,"noted","2016-11-03T15:05:04.023","2016-11-04T19:15:47.910","","","Rel-14","","","","","","","","","","","",""]
["R4-1609495","Further discussion on V2X MCC first priority scenarios","CATT","Xuhua Tao","62863","discussion","Discussion","The three scenarios listed as the first priority of V2X MCC operation are discussed in terms of working scenarios and operating bands.","","277","8.20.3","UE RF (36.101) [LTE_V2X-Core]",938000000,"noted","2016-11-03T15:11:29.140","2016-11-04T14:40:37.330","","","Rel-14","","","LTE_V2X-Core","","","","","","","","",""]
["R4-1609496","Futher calibration results for 5G NR co-existence study","CATT","Xuhua Tao","62863","discussion","Information","---","","410","11.3.1","Co-existence [FS_NR_newRAT]",1640000,"noted","2016-11-03T15:11:29.170","2016-11-04T14:40:37.330","","","Rel-15","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1609497","On throughput model of dense urban and indoor hotspot","CATT","Xuhua Tao","62863","discussion","Approval","throughput model of dense urban and indoor hotspot based on the simulation results","","410","11.3.1","Co-existence [FS_NR_newRAT]",940700000,"approved","2016-11-03T15:11:29.187","2016-11-04T14:40:37.330","","","Rel-15","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1609498","Discussion on the UL co-existence performance of urban macro","CATT","Xuhua Tao","62863","discussion","Discussion","---","","410","11.3.1","Co-existence [FS_NR_newRAT]",905500000,"noted","2016-11-03T15:11:29.203","2016-11-04T14:40:37.330","","","Rel-15","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1609499","Discussion on the DL co-existence performance of dense urban","CATT","Xuhua Tao","62863","discussion","Discussion","---","","410","11.3.1","Co-existence [FS_NR_newRAT]",15500000,"noted","2016-11-03T15:11:29.217","2016-11-04T14:40:37.347","","","Rel-15","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1609500","Discussion on the DL co-existence performance of indoor hotspot","CATT","Xuhua Tao","62863","discussion","Discussion","---","","410","11.3.1","Co-existence [FS_NR_newRAT]",15700000,"noted","2016-11-03T15:11:29.233","2016-11-04T14:40:37.347","","","Rel-15","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1609501","Discussion on ON/OFF time mask for sTTI","CATT","Xuhua Tao","62863","discussion","Discussion","In this contribution, the relation of UL power ON/OFF transmit time periods with sTTI performance is discussed. Following observation and proposal are presented.\nObservation 1: The UL ON/OFF time mask has some implication to the sTTI performance.\nObservat","","403","10.1.2","UE RF (36.101) [LTE_sTTIandPT]",95300,"noted","2016-11-03T15:11:29.250","2016-11-04T14:40:37.347","","","Rel-15","36.101","","LTE_sTTIandPT","","","","","","","","",""]
["R4-1609502","Discussion on V2X transmission chain","CATT","Xuhua Tao","62863","discussion","Discussion","In this contribution, we discussed transmitter structure for inter-band operation, and some considerations for output power. The paper gives following proposal and observations.\nProposal 1: Current RF requirements for licensed bands should be reused in in","","277","8.20.3","UE RF (36.101) [LTE_V2X-Core]",950200000,"noted","2016-11-03T15:11:29.263","2016-11-04T14:40:37.347","","","Rel-14","36.101","","LTE_V2X-Core","","","","","","","","",""]
["R4-1609503","Discussion on Tx RF requirements for inter-band E-UTRA_V2X operation and higher power class","CATT","Xuhua Tao","62863","discussion","Discussion","In this contribution, we discussed defining V2x transmitter RF requirements for inter-band operation, and higher output power class. The paper gives following proposals.\nProposal 1: Current RF requirements for licensed bands should be reused in inter-band","","278","8.20.3.1","Tx requirements  [LTE_V2X-Core]",75600000,"noted","2016-11-03T15:11:29.280","2016-11-04T14:40:37.347","","","Rel-14","36.101","","LTE_V2X-Core","","","","","","","","",""]
["R4-1609504","TP for Tx RF requirements for inter-band E-UTRA_V2X operation and higher power class","CATT","Xuhua Tao","62863","other","Approval","TP for Tx RF requirements for inter-band E-UTRA_V2X operation and higher power class","","278","8.20.3.1","Tx requirements  [LTE_V2X-Core]",950300000,"revised","2016-11-03T15:11:29.297","2016-11-04T14:40:37.363","","R4-1610756","Rel-14","36.786","","LTE_V2X-Core","","","","","","","","",""]
["R4-1609505","Discussion on ON/OFF time mask for NR","CATT","Xuhua Tao","62863","other","Approval","Discussion on ON/OFF time mask for NR","","415","11.5.1","Common issues for UE and BS [FS_NR_newRAT]",941100000,"noted","2016-11-03T15:11:29.310","2016-11-04T14:40:37.363","","","Rel-15","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1609506","UE transmission timing accuracy test for V2V","CATT","Xuhua Tao","62863","discussion","Discussion","---","","266","8.19.3.1","UE transmission timing accuracy test [LTE_SL_V2V-Perf]",63700000,"noted","2016-11-03T15:11:29.343","2016-11-04T14:40:37.363","","","Rel-14","","","LTE_SL_V2V-Perf","","","","","","","","",""]
["R4-1609507","CR on UE transmission timing accuracy test for V2V","CATT","Xuhua Tao","62863","CR","Approval","---","","266","8.19.3.1","UE transmission timing accuracy test [LTE_SL_V2V-Perf]",95060000,"noted","2016-11-03T15:11:29.357","2016-11-04T14:40:37.363","","R4-1610635","Rel-14","36.133","14.1.0","LTE_SL_V2V-Perf","4212","","B","","","","","",""]
["R4-1609508","Discussion on UE transmission timing requirements for V2X","CATT","Xuhua Tao","62863","discussion","Discussion","---","","281","8.20.4.1","UE Transmit timing [LTE_V2X-Core]",9287000,"noted","2016-11-03T15:11:29.450","2016-11-04T14:40:37.363","","","Rel-14","","","LTE_V2X-Core","","","","","","","","",""]
["R4-1609509","CR on UE transmission timing requirements for V2X","CATT","Xuhua Tao","62863","CR","Approval","---","","281","8.20.4.1","UE Transmit timing [LTE_V2X-Core]",24500000,"revised","2016-11-03T15:11:29.483","2016-11-04T14:40:37.363","","R4-1610874","Rel-14","36.133","14.1.0","LTE_V2X-Core","4213","","B","","","","","",""]
["R4-1609510","Simulation results of S-RSRP measurement requirements for V2X","CATT","Xuhua Tao","62863","discussion","Discussion","---","","283","8.20.4.3","Initiation/cease of SLSS requirement [LTE_V2X-Core]",9510000,"noted","2016-11-03T15:11:29.560","2016-11-04T14:40:37.377","","","Rel-14","","","LTE_V2X-Core","","","","","","","","",""]
["R4-1609511","CR on S-RSRP measurement accuracy requirements for V2X","CATT","Xuhua Tao","62863","CR","Approval","---","","283","8.20.4.3","Initiation/cease of SLSS requirement [LTE_V2X-Core]",68400000,"noted","2016-11-03T15:11:29.577","2016-11-04T14:40:37.377","","","Rel-14","36.133","14.1.0","LTE_V2X-Core","4214","","B","","","","","",""]
["R4-1609512","Simulation results of PSSCH-RSRP measurement","CATT","Xuhua Tao","62863","discussion","Discussion","---","","285","8.20.4.5","Autonomous resource selection/reselection [LTE_V2X-Core]",908600000,"noted","2016-11-03T15:11:29.670","2016-11-04T14:40:37.377","","","Rel-14","","","LTE_V2X-Core","","","","","","","","",""]
["R4-1609513","CR on PSSCH-RSRP measurement accuracy requirement","CATT","Xuhua Tao","62863","CR","Approval","---","","285","8.20.4.5","Autonomous resource selection/reselection [LTE_V2X-Core]",977200000,"noted","2016-11-03T15:11:29.687","2016-11-04T14:40:37.377","","","Rel-14","36.133","14.1.0","LTE_V2X-Core","4215","","B","","","","","",""]
["R4-1609514","Initiation/cease of SLSS requirements for V2X UE","CATT","Xuhua Tao","62863","discussion","Discussion","---","","283","8.20.4.3","Initiation/cease of SLSS requirement [LTE_V2X-Core]",951100000,"noted","2016-11-03T15:11:29.763","2016-11-04T14:40:37.377","","","Rel-14","","","","","","","","","","","",""]
["R4-1609515","RRM interruptions requirements for V2X","CATT","Xuhua Tao","62863","discussion","Discussion","---","","282","8.20.4.2","Interruption [LTE_V2X-Core]",24000000,"withdrawn","2016-11-03T15:11:29.797",null,"","","Rel-14","","","","","","","","","","","",""]
["R4-1609516","Discussion on measurements requirement for congestion control for V2X","CATT","Xuhua Tao","62863","discussion","Discussion","---","","286","8.20.4.6","Congestion control [LTE_V2X-Core]",951600000,"noted","2016-11-03T15:11:29.810","2016-11-04T14:43:30.537","","","Rel-14","","","","","","","","","","","",""]
["R4-1609517","Impairment results of NPBCH Demodulation for NB-IoT","CATT","Xuhua Tao","62863","discussion","Discussion","simulation results of NPBCH Demodulation for NB-IoT","","129","6.3.4.1.1","NPBCH  [NB_IOT-Perf]",52200000,"noted","2016-11-03T15:11:29.827","2016-11-04T14:40:37.393","","","Rel-13","","","NB_IOT-Perf","","","","","","","","",""]
["R4-1609518","Impairment  results of NPDCCH Demodulation for NB-IoT","CATT","Xuhua Tao","62863","discussion","Discussion","simulation results of NPDCCH Demodulation for NB-IoT","","130","6.3.4.1.2","NPDCCH [NB_IOT-Perf]",943600000,"noted","2016-11-03T15:11:29.840","2016-11-04T14:40:37.393","","","Rel-13","","","NB_IOT-Perf","","","","","","","","",""]
["R4-1609519","Impairment  results of NPDSCH Demodulation for NB-IoT","CATT","Xuhua Tao","62863","discussion","Discussion","simulation results of NPDSCH Demodulation for NB-IoT","","131","6.3.4.1.3","NPDSCH [NB-IOT-Perf]",931900000,"noted","2016-11-03T15:11:29.873","2016-11-04T14:40:37.393","","","Rel-13","","","NB_IOT-Perf","","","","","","","","",""]
["R4-1609520","Simulation results for UE demodulation performance under bidirectional SFN scenarios","CATT","Xuhua Tao","62863","discussion","Discussion","Updated simulation results for UE demodulation performance under bidirectional SFN scenarios","","345","8.28.3.1","Enhancement for bi-directional RRH arrangement [LTE_high_speed]",952000000,"noted","2016-11-03T15:11:29.887","2016-11-04T14:40:37.393","","","Rel-14","","","LTE_high_speed","","","","","","","","",""]
["R4-1609521","Discussion on CQI reporting requirements under SFN scenarios","CATT","Xuhua Tao","62863","discussion","Discussion","Discussion on CQI reporting requirements under SFN scenarios","","347","8.28.3.3","CQI reporting [LTE_high_speed]",952100000,"noted","2016-11-03T15:11:29.903","2016-11-04T14:40:37.393","","","Rel-14","","","LTE_high_speed","","","","","","","","",""]
["R4-1609522","RRM requirements enhancement for high speed scenarios","CATT","Xuhua Tao","62863","discussion","Discussion","Discussion on RRM requirements enhancement for high speed scenarios","","341","8.28.2.1","Enhancement in connected mode (DRX) [LTE_high_speed]",929500000,"noted","2016-11-03T15:11:29.920","2016-11-04T14:40:37.410","","","Rel-14","","","LTE_high_speed","","","","","","","","",""]
["R4-1609523","CR for RRM requirements  in RRC connected mode  for high speed conditions","CATT","Xuhua Tao","62863","CR","Approval","CR for RRM requirements  in RRC connected mode  for high speed conditions","","341","8.28.2.1","Enhancement in connected mode (DRX) [LTE_high_speed]",929800000,"noted","2016-11-03T15:11:29.950","2016-11-04T14:40:37.410","","","Rel-14","36.133","14.1.0","LTE_high_speed","4216","","B","","","","","",""]
["R4-1609524","CR for RRM requirements  in idle mode  for high speed conditions","CATT","Xuhua Tao","62863","CR","Approval","CR for RRM requirements  in idle mode  for high speed conditions","","342","8.28.2.2","Enhancement in idle mode [LTE_high_speed]",955200000,"revised","2016-11-03T15:11:30.043","2016-11-04T14:40:37.410","","R4-1610676","Rel-14","36.133","14.1.0","LTE_high_speed","4217","","B","","","","","",""]
["R4-1609525","Discussions on UE demodulation performance requirements for V2V","CATT","Xuhua Tao","62863","discussion","Discussion","Discussions on UE demodulation performance requirements for V2V","","269","8.19.4.1","Single-link PSSCH and PSCCH  [LTE_SL_V2V-Perf]",908300000,"noted","2016-11-03T15:11:30.123","2016-11-04T14:40:37.410","","","Rel-14","","","LTE_SL_V2V-Perf","","","","","","","","",""]
["R4-1609526","Discussion on OTA EVM requirement","CATT","Xuhua Tao","62863","discussion","Discussion","Discussion on OTA EVM requirement","","209","8.12.2.1","In band requirements [AASenh_BS_LTE_UTRA]",5000000,"noted","2016-11-03T15:11:30.153","2016-11-04T14:40:37.410","","","Rel-14","","","AASenh_BS_LTE_UTRA","","","","","","","","",""]
["R4-1609527","TP for NR Rel-14 TR 38.803: TDD timing budget","Ericsson","Magnus Larsson","43293","pCR","Approval","TDD timing budget formulas.","","415","11.5.1","Common issues for UE and BS [FS_NR_newRAT]",950500000,"revised","2016-11-03T15:21:27.337","2016-11-07T16:06:26.410","","R4-1610617","","38.803","0.3.0","FS_NR_newRAT","","","","","","","","",""]
["R4-1609528","Observations regarding NR timing budget","Ericsson","Magnus Larsson","43293","discussion","Discussion","Observations regarding NR timing budget, like uncertainty vs holdover times.","","415","11.5.1","Common issues for UE and BS [FS_NR_newRAT]",941200000,"noted","2016-11-03T15:21:27.353","2016-11-07T16:06:47.207","","","","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1609529","CR for TS 37.141: Multi-band testing with 3 or more bands.","Ericsson","Magnus Larsson","43293","CR","Approval","Conformance testing procedures for 3 bands or more multiband MSR based on approved TR.","","205","8.11.2","BS RF (36.141, 37.141, 25.141) [MB_BS_test_3B-Perf]",938700000,"revised","2016-11-03T15:21:27.367","2016-11-07T16:07:00.857","","R4-1610744","Rel-14","37.141","14.1.0","MB_BS_test_3B-Perf","0475","","B","","","","","",""]
["R4-1609530","BS synchronization for eMBMS","Ericsson","Magnus Larsson","43293","discussion","Discussion","eNB sync requirements.","","373","8.32.1","Inter-cell Synchronization for MBMS/eMBMS [WI code or TEI14]",92000,"noted","2016-11-03T15:21:27.510","2016-11-07T16:07:19.840","","","Rel-14","","","TEI14","","","","","","","","",""]
["R4-1609531","Ideal Simulation assumptions for 256QAM","Ericsson","Magnus Larsson","43293","other","Approval","Ideal simulation assumptions for alignment of simulators.","","231","8.15.3","Other specifications [LTE_UL_CAP_enh-Core]",953100000,"available","2016-11-03T15:21:27.523","2016-11-07T16:07:33.770","","","Rel-14","","","LTE_UL_CAP_enh","","","","","","","","",""]
["R4-1609532","CR to TS 37.141 Rel 13 - Introduction of NB-IoT","Ericsson","Dominique Everaere","63414","CR","Approval","CR to TS 37.141 Rel 13 - Introduction of NB-IoT","","113","6.3.2","BS RF conformance testing (36.141) [NB_IOT-Perf]",938900000,"revised","2016-11-03T15:21:42.187","2016-11-04T14:42:55.047","","R4-1610562","Rel-13","37.141","13.4.0","NB_IOT-Perf","0476","","B","","","","","",""]
["R4-1609533","CR to TS 37.141 introducing NB-IoT","Ericsson, Nokia, Alcatel-Lucent Shanghai Bell, Huawei","Dominique Everaere","63414","CR","Approval","CR to TS 37.141 Rel 14 - Introduction of NB-IoT","","113","6.3.2","BS RF conformance testing (36.141) [NB_IOT-Perf]",953200000,"agreed","2016-11-03T15:21:42.313","2016-11-19T17:47:25.647","","","Rel-14","37.141","14.1.0","NB_IOT-Perf","0477","","A","RP-162379","","","","",""]
["R4-1609534","CR to TS 37.113 Rel 13 - Introduction of NB-IoT","Ericsson","Dominique Everaere","63414","CR","Approval","CR to TS 37.113 Rel 13 - Introduction of NB-IoT","","113","6.3.2","BS RF conformance testing (36.141) [NB_IOT-Perf]",953300000,"revised","2016-11-03T15:21:42.423","2016-11-04T14:42:55.060","","R4-1610552","Rel-13","37.113","13.2.0","NB_IOT-Perf","0053","","B","","","","","",""]
["R4-1609535","CR to TS 37.113 Rel 14 - Introduction of NB-IoT","Ericsson","Dominique Everaere","63414","CR","Approval","CR to TS 37.113 Rel 14 - Introduction of NB-IoT","","113","6.3.2","BS RF conformance testing (36.141) [NB_IOT-Perf]",953500000,"agreed","2016-11-03T15:21:42.547","2016-11-19T17:47:25.647","","","Rel-14","37.113","14.0.0","NB_IOT-Perf","0054","","A","RP-162379","","","","",""]
["R4-1609536","NB-IoT UL Timing error evaluation - simulation results","Ericsson","Dominique Everaere","63414","discussion","Discussion","NB-IoT UL Timing error evaluation - simulation results  - resubmission from RAN4#80b under other agenda item","","56","5.6.4","RRM core (36.133)  [NB_IOT-Core]",3900000,"noted","2016-11-03T15:21:42.657","2016-11-04T14:43:20.647","","","Rel-13","","","NB_IOT-Core","","","","","","","","",""]
["R4-1609537","CR to TS 36.133 Rel-13 section 7.20 - UL timing error requirement","Ericsson","Dominique Everaere","63414","CR","Approval","CR to TS 36.133 Rel-13 section 7.20 - UL timing error requirement","","56","5.6.4","RRM core (36.133)  [NB_IOT-Core]",4000000,"noted","2016-11-03T15:21:42.687","2016-11-04T14:43:20.647","","","Rel-13","36.133","13.5.0","NB_IOT-Core","4218","","C","","","","","",""]
["R4-1609538","CR to TS 36.133 Rel-14 section 7.20 - UL timing error requirement","Ericsson","Dominique Everaere","63414","CR","Approval","CR to TS 36.133 Rel-14 section 7.20 - UL timing error requirement","","56","5.6.4","RRM core (36.133)  [NB_IOT-Core]",9145000,"withdrawn","2016-11-03T15:21:42.797",null,"","","Rel-14","36.133","14.1.0","NB_IOT-Core","4219","","A","","","","","",""]
["R4-1609539","NB-IoT and CMDA coexistence conclusions","Ericsson","Dominique Everaere","63414","discussion","Approval","NB-IoT and CMDA coexistence conclusions","","393","9.3.4","RF requirements impact [FS_NB_IOT_CDMA_coex]",935800000,"noted","2016-11-03T15:21:42.890","2016-11-05T15:17:08.560","","","Rel-14","","","FS_NB_IOT_CDMA_coex","","","","","","","","",""]
["R4-1609540","TP to TR 36.752","Ericsson","Dominique Everaere","63414","other","Approval","TP to TR 36.752","","393","9.3.4","RF requirements impact [FS_NB_IOT_CDMA_coex]",935900000,"noted","2016-11-03T15:21:42.907","2016-11-05T15:17:08.577","","","Rel-14","36.752","0.0.1","FS_NB_IOT_CDMA_coex","","","","","","","","",""]
["R4-1609541","Overview of shorten TTI feature impacts on BS RF requirements TS 36.104","Ericsson","Dominique Everaere","63414","discussion","Discussion","Overview of the shorten TTI feature impacts on BS RF requirements TS 36.104","","404","10.1.3","BS RF (36.104) [LTE_sTTIandPT]",954100000,"noted","2016-11-03T15:21:42.937","2016-11-05T15:17:29.213","","","Rel-15","","","LTE_sTTIandPT","","","","","","","","",""]
["R4-1609542","Way Forward BS RF requirements impact for shorten TTI feature","Ericsson","Dominique Everaere","63414","discussion","Approval","Way Forward on BS RF requirements introducing shorten TTI feature","","404","10.1.3","BS RF (36.104) [LTE_sTTIandPT]",954200000,"revised","2016-11-03T15:21:42.953","2016-11-05T15:17:29.213","","R4-1610788","Rel-15","","","LTE_sTTIandPT","","","","","","","","",""]
["R4-1609543","Conclusion on NPUSCH requirements","Ericsson","Dominique Everaere","63414","discussion","Approval","Conclusion on NPUSCH requirements","","132","6.3.4.2","BS Demodulation  [NB_IOT-Perf]",55900000,"noted","2016-11-03T15:21:42.967","2016-11-04T14:43:20.647","","","Rel-13","","","NB_IOT-Perf","","","","","","","","",""]
["R4-1609544","Lower Maximum Transmit Power Class for Enhanced NB-IoT UE","u-blox AG, Neul","Sylvia Lu","48273","discussion","Approval","---","","304","8.24.2.1","Power Class       [NB_IOTenh-Core]",938500000,"noted","2016-11-03T15:39:31.710","2016-11-04T15:44:57.877","","","Rel-14","","","","","","","","","","","",""]
["R4-1609545","Low densty gap patterns for measurement gap enhancement","Ericsson","Christopher Callender","58614","discussion","Discussion","Discussion on low densty gap patterns for measurement gap enhancement","","351","8.29.2","RRM core (36.133) [LTE_meas_gap_enh-Core]",932100000,"noted","2016-11-03T15:43:31.857","2016-11-04T15:31:13.087","","","Rel-14","","","LTE_meas_gap_enh-Core","","","","","","","","",""]
["R4-1609546","Further discussion on RAN4 related signalling aspects for measurement gaps","Ericsson","Christopher Callender","58614","discussion","Discussion","Further discussion on RAN4 related signalling aspects for measurement gaps","","351","8.29.2","RRM core (36.133) [LTE_meas_gap_enh-Core]",932200000,"noted","2016-11-03T15:43:31.870","2016-11-04T15:31:13.180","","","Rel-14","","","LTE_meas_gap_enh-Core","","","","","","","","",""]
["R4-1609547","Liaison statement on measurement gaps","Ericsson","Christopher Callender","58614","LS out","Approval","Reply and further information on measurement gaps for RAN2","","351","8.29.2","RRM core (36.133) [LTE_meas_gap_enh-Core]",954700000,"revised","2016-11-03T15:43:31.887","2016-11-04T15:31:13.213","","R4-1610888","Rel-14","","","LTE_meas_gap_enh-Core","","","","","R2-167317","RAN WG2","RAN WG1","",""]
["R4-1609548","Parallel measurement capability for measurement gap enhancement","Ericsson","Christopher Callender","58614","discussion","Discussion","Discusses parallel measurement gap capability and requirements for gap enhancement WI","","351","8.29.2","RRM core (36.133) [LTE_meas_gap_enh-Core]",912000000,"noted","2016-11-03T15:43:31.917","2016-11-04T15:31:13.227","","","Rel-14","","","LTE_meas_gap_enh-Core","","","","","","","","",""]
["R4-1609549","RAN4 requirements for measurement gap enhancement","Ericsson","Christopher Callender","58614","discussion","Discussion","Discussion on 36.133 updates to include measurement gap enhancement including TPs for 36.133","","351","8.29.2","RRM core (36.133) [LTE_meas_gap_enh-Core]",954900000,"noted","2016-11-03T15:43:31.950","2016-11-04T15:31:13.227","","","Rel-14","","","LTE_meas_gap_enh-Core","","","","","","","","",""]
["R4-1609550","Requirements for RRC connected state","Ericsson","Christopher Callender","58614","discussion","Discussion","Discusion on enhanced requirements for RRC connected state for high speed scenarios","","341","8.28.2.1","Enhancement in connected mode (DRX) [LTE_high_speed]",907600000,"noted","2016-11-03T15:43:31.963","2016-11-04T15:31:12.790","","","Rel-14","","","LTE_high_speed","","","","","","","","",""]
["R4-1609551","Requirements for RRC idle state","Ericsson","Christopher Callender","58614","discussion","Discussion","Discusion on enhanced requirements for RRC idle state for high speed scenarios","","342","8.28.2.2","Enhancement in idle mode [LTE_high_speed]",9524000,"noted","2016-11-03T15:43:31.980","2016-11-04T15:31:12.807","","","Rel-14","","","LTE_high_speed","","","","","","","","",""]
["R4-1609552","Discussions on RAN2 questions related to high speed indicator","Ericsson","Christopher Callender","58614","discussion","Discussion","Discussion on questions asked by RAN2 on high speed indicator","","343","8.28.2.3","Others [LTE_high_speed]",9295000,"noted","2016-11-03T15:43:32.010","2016-11-04T15:31:12.823","","","Rel-14","","","LTE_high_speed","","","","","","","","",""]
["R4-1609553","Reply LS on performance enhancements indicator for high speed scenarios","Ericsson","Christopher Callender","58614","LS out","Approval","Reply LS on high speed indicator","","343","8.28.2.3","Others [LTE_high_speed]",955300000,"noted","2016-11-03T15:43:32.027","2016-11-04T15:31:12.837","","","Rel-14","","","LTE_high_speed","","","","","R2-167308","RAN WG2","","",""]
["R4-1609554","Further  Mobility Enhancement Requirements","Ericsson","Christopher Callender","58614","discussion","Discussion","Discussion on Further Mobility Enhancement Requirements","","327","8.26.3","RRM core (36.133) [LTE_eMob-Core]",932400000,"noted","2016-11-03T15:43:32.057","2016-11-04T15:31:12.900","","","Rel-14","","","LTE_eMob-Core","","","","","","","","",""]
["R4-1609555","Power Allocation in Uplink Multicarrier scenarios for UMTS including 10ms TTI and Mixed TTI configurations","Ericsson","Christopher Callender","58614","discussion","Discussion","Discussion on impacts to 25.133 from WI on multicarrier enhancements including introduction of 10ms TTI and mixed 2/10ms TTI scenarios","","375","8.32.3","RRM  [WI code or TEI14]",955500000,"noted","2016-11-03T15:43:32.073","2016-11-04T15:31:12.930","","","Rel-14","","","UTRA_MCe","","","","","","","","",""]
["R4-1609556","Power Allocation in Uplink Multicarrier scenarios for UMTS including 10ms TTI and Mixed TTI configurations","Ericsson","Christopher Callender","58614","CR","Approval","CR for 25.133 from WI on multicarrier enhancements including introduction of 10ms TTI and mixed 2/10ms TTI scenarios","","375","8.32.3","RRM  [WI code or TEI14]",955600000,"revised","2016-11-03T15:43:32.090","2016-11-04T15:31:12.947","","R4-1611014","Rel-14","25.133","14.0.0","UTRA_MCe","1428","","B","","","","","",""]
["R4-1609557","Workplan for RRM core work on shortened TTI and reduced processing time for LTE","Ericsson","Christopher Callender","58614","discussion","Discussion","Workplan for RRM core work on shortened TTI and processing time for LTE","","405","10.1.4","RRM core (36.133)  [LTE_sTTIandPT]",112000,"revised","2016-11-03T15:43:32.230","2016-11-04T15:31:12.947","","R4-1610730","Rel-15","","","LTE_sTTIandPT","","","","","","","","",""]
["R4-1609558","Initial views on RRM requirements impacted by shortened TTI and processing time reduction","Ericsson","Christopher Callender","58614","discussion","Discussion","Discussion on RRM requirements impacted by shortened TTI and processing time reduction","","405","10.1.4","RRM core (36.133)  [LTE_sTTIandPT]",955700000,"noted","2016-11-03T15:43:32.247","2016-11-04T15:31:12.947","","","Rel-15","","","LTE_sTTIandPT","","","","","","","","",""]
["R4-1609559","RRM bandwidth considerations for NR","Ericsson","Christopher Callender","58614","discussion","Discussion","RRM bandwidth considerations for NR","","425","11.6.1.1","RRM general [FS_NR_newRAT]",933000000,"available","2016-11-03T15:43:32.260","2016-11-04T15:31:12.963","","","Rel-14","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1609560","RRM power consumption considerations for NR","Ericsson","Christopher Callender","58614","discussion","Discussion","RRM power consumption considerations for NR","","425","11.6.1.1","RRM general [FS_NR_newRAT]",9238000,"noted","2016-11-03T15:43:32.277","2016-11-04T15:31:12.963","","","Rel-14","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1609561","RRM test considerations for NR","Ericsson","Christopher Callender","58614","discussion","Discussion","RRM test considerations for NR","","426","11.6.1.2","Testability [FS_NR_newRAT]",956100000,"noted","2016-11-03T15:43:32.307","2016-11-04T15:31:12.963","","","Rel-14","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1609562","Text proposal on RRM bandwidth for NR","Ericsson","Christopher Callender","58614","pCR","Approval","Text proposal on RRM bandwidth for NR","","425","11.6.1.1","RRM general [FS_NR_newRAT]",981700000,"approved","2016-11-03T15:43:32.323","2016-11-04T15:31:12.963","","","","38.803","0.3.0","FS_NR_newRAT","","","","","","","","",""]
["R4-1609563","Text proposal on RRM power consumption for NR","Ericsson","Christopher Callender","58614","pCR","Approval","Text proposal on RRM power consumption for NR","","425","11.6.1.1","RRM general [FS_NR_newRAT]",15800000,"noted","2016-11-03T15:43:32.340","2016-11-04T15:31:12.977","","","","38.803","0.3.0","FS_NR_newRAT","","","","","","","","",""]
["R4-1609564","Text proposal on RRM testing for NR","Ericsson","Christopher Callender","58614","pCR","Approval","Text proposal on RRM testingfor NR","","426","11.6.1.2","Testability [FS_NR_newRAT]",956400000,"revised","2016-11-03T15:43:32.370","2016-11-04T15:31:12.977","","R4-1610625","","38.803","0.3.0","FS_NR_newRAT","","","","","","","","",""]
["R4-1609565","Way forward for NR RRM","Ericsson","Christopher Callender","58614","other","Approval","Outcomes and WF of RAN4#81 for NR RRM","","425","11.6.1.1","RRM general [FS_NR_newRAT]",933100000,"approved","2016-11-03T15:43:32.387","2016-11-22T12:17:26.987","","","Rel-14","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1609566","Transmitter requirements in transient periods","Ericsson","Christian Bergljung","21143","other","Approval","In this contribution we propose to make clear the applicability of the core transmitter requirements in transient periods: all requirements except EVM and power control","","12","4.2.1","UE RF (core / EMC)  [WI code or TEI12]",4540000,"noted","2016-11-03T16:09:03.790","2016-11-06T19:58:46.997","","","Rel-10","","","LTE-RF","","","","","","","","",""]
["R4-1609567","Applicability of core transmitter requirements in transient periods","Ericsson","Christian Bergljung","21143","CR","Approval","CR to make clear the applicability of the core transmitter requirements in transient periods","","12","4.2.1","UE RF (core / EMC)  [WI code or TEI12]",4550000,"noted","2016-11-03T16:09:03.823","2016-11-06T20:01:45.693","","","Rel-10","36.101","10.23.0","LTE-RF","4013","","F","","","","","",""]
["R4-1609568","Applicability of core transmitter requirements in transient periods","Ericsson","Christian Bergljung","21143","CR","Approval","CR to make clear the applicability of the core transmitter requirements in transient periods","","12","4.2.1","UE RF (core / EMC)  [WI code or TEI12]",4560000,"withdrawn","2016-11-03T16:09:03.917",null,"","","Rel-11","36.101","11.18.0","LTE-RF","4014","","A","","","","","",""]
["R4-1609569","Applicability of core transmitter requirements in transient periods","Ericsson","Christian Bergljung","21143","CR","Approval","CR to make clear the applicability of the core transmitter requirements in transient periods","","12","4.2.1","UE RF (core / EMC)  [WI code or TEI12]",42400000,"withdrawn","2016-11-03T16:09:04.010",null,"","","Rel-12","36.101","12.13.0","LTE-RF","4015","","A","","","","","",""]
["R4-1609570","Applicability of core transmitter requirements in transient periods","Ericsson","Christian Bergljung","21143","CR","Approval","CR to make clear the applicability of the core transmitter requirements in transient periods","","12","4.2.1","UE RF (core / EMC)  [WI code or TEI12]",76400000,"withdrawn","2016-11-03T16:09:04.087",null,"","","Rel-13","36.101","13.5.0","LTE-RF","4016","","A","","","","","",""]
["R4-1609571","Applicability of core transmitter requirements in transient periods","Ericsson","Christian Bergljung","21143","CR","Approval","CR to make clear the applicability of the core transmitter requirements in transient periods","","12","4.2.1","UE RF (core / EMC)  [WI code or TEI12]",956600000,"withdrawn","2016-11-03T16:09:04.197",null,"","","Rel-14","36.101","14.1.0","LTE-RF","4017","","A","","","","","",""]
["R4-1609572","RMCs and applicabilility of core RF requirements","Ericsson","Christian Bergljung","21143","CR","Approval","CR to remove the restriction of the applicability of the core RF requirements to RMCs only (requirements apply generally if not otherwise stated)","","12","4.2.1","UE RF (core / EMC)  [WI code or TEI12]",956700000,"agreed","2016-11-03T16:09:04.307","2016-11-06T20:03:42.460","","","Rel-10","36.101","10.23.0","LTE-RF","4018","","F","RP-162411","","","","",""]
["R4-1609573","RMCs and applicabilility of core RF requirements","Ericsson","Christian Bergljung","21143","CR","Approval","CR to remove the restriction of the applicability of the core RF requirements to RMCs only (requirements apply generally if not otherwise stated)","","12","4.2.1","UE RF (core / EMC)  [WI code or TEI12]",956800000,"agreed","2016-11-03T16:09:04.417","2016-11-22T09:27:26.103","","","Rel-11","36.101","11.18.0","LTE-RF","4019","","A","RP-162411","","","","",""]
["R4-1609574","RMCs and applicabilility of core RF requirements","Ericsson","Christian Bergljung","21143","CR","Approval","CR to remove the restriction of the applicability of the core RF requirements to RMCs only (requirements apply generally if not otherwise stated)","","12","4.2.1","UE RF (core / EMC)  [WI code or TEI12]",956900000,"agreed","2016-11-03T16:09:04.523","2016-11-22T09:27:26.150","","","Rel-12","36.101","12.13.0","LTE-RF","4020","","A","RP-162411","","","","",""]
["R4-1609575","RMCs and applicabilility of core RF requirements","Ericsson","Christian Bergljung","21143","CR","Approval","CR to remove the restriction of the applicability of the core RF requirements to RMCs only (requirements apply generally if not otherwise stated)","","12","4.2.1","UE RF (core / EMC)  [WI code or TEI12]",957000000,"agreed","2016-11-03T16:09:04.633","2016-11-22T09:27:26.150","","","Rel-13","36.101","13.5.0","LTE-RF","4021","","A","RP-162411","","","","",""]
["R4-1609576","RMCs and applicabilility of core RF requirements","Ericsson","Christian Bergljung","21143","CR","Approval","CR to remove the restriction of the applicability of the core RF requirements to RMCs only (requirements apply generally if not otherwise stated)","","12","4.2.1","UE RF (core / EMC)  [WI code or TEI12]",957100000,"agreed","2016-11-03T16:09:04.743","2016-11-22T09:27:26.167","","","Rel-14","36.101","14.1.0","LTE-RF","4022","","A","RP-162411","","","","",""]
["R4-1609577","Modification to UL RMC for covering PUSCH FH and multi-clustered PUSCH","Ericsson","Christian Bergljung","21143","CR","Approval","CR to modify the general definition of the UL RMCs to allow PUSCH FH and multi-clustered PUSCH","","12","4.2.1","UE RF (core / EMC)  [WI code or TEI12]",957200000,"noted","2016-11-03T16:09:04.837","2016-11-06T20:06:07.337","","","Rel-11","36.101","11.18.0","LTE-RF","4023","","F","","","","","",""]
["R4-1609578","Modification to UL RMC for covering PUSCH FH and multi-clustered PUSCH","Ericsson","Christian Bergljung","21143","CR","Approval","CR to modify the general definition of the UL RMCs to allow PUSCH FH and multi-clustered PUSCH","","12","4.2.1","UE RF (core / EMC)  [WI code or TEI12]",957300000,"withdrawn","2016-11-03T16:09:04.930",null,"","","Rel-12","36.101","12.13.0","LTE-RF","4024","","A","","","","","",""]
["R4-1609579","Modification to UL RMC for covering PUSCH FH and multi-clustered PUSCH","Ericsson","Christian Bergljung","21143","CR","Approval","CR to modify the general definition of the UL RMCs to allow PUSCH FH and multi-clustered PUSCH","","12","4.2.1","UE RF (core / EMC)  [WI code or TEI12]",957400000,"withdrawn","2016-11-03T16:09:05.023",null,"","","Rel-13","36.101","13.5.0","LTE-RF","4025","","A","","","","","",""]
["R4-1609580","Modification to UL RMC for covering PUSCH FH and multi-clustered PUSCH","Ericsson","Christian Bergljung","21143","CR","Approval","CR to modify the general definition of the UL RMCs to allow PUSCH FH and multi-clustered PUSCH","","12","4.2.1","UE RF (core / EMC)  [WI code or TEI12]",957500000,"withdrawn","2016-11-03T16:09:05.133",null,"","","Rel-14","36.101","14.1.0","LTE-RF","4026","","A","","","","","",""]
["R4-1609581","Correction of spurious emissions requirements for Band 9 range and intra-band CA","Ericsson","Christian Bergljung","21143","CR","Approval","CR to correct notes on applicability of spurious emissions requirements for intra-band CA and remove redunant protection requirements for the Band 9 range","","12","4.2.1","UE RF (core / EMC)  [WI code or TEI12]",957600000,"agreed","2016-11-03T16:09:05.227","2016-11-06T20:14:29.280","","","Rel-10","36.101","10.23.0","LTE-RF","4027","","F","RP-162411","","","","",""]
["R4-1609582","Correction of spurious emissions requirements for Band 9 range and intra-band CA","Ericsson","Christian Bergljung","21143","CR","Approval","CR to correct notes on applicability of spurious emissions requirements for intra-band CA and remove redunant protection requirements for the Band 9 range","","12","4.2.1","UE RF (core / EMC)  [WI code or TEI12]",957700000,"agreed","2016-11-03T16:09:05.337","2016-11-22T09:27:26.183","","","Rel-11","36.101","11.18.0","LTE-RF","4028","","A","RP-162411","","","","",""]
["R4-1609583","Correction of spurious emissions requirements for Band 9 range and intra-band CA","Ericsson","Christian Bergljung","21143","CR","Approval","CR to correct notes on applicability of spurious emissions requirements for intra-band CA and remove redunant protection requirements for the Band 9 range","","12","4.2.1","UE RF (core / EMC)  [WI code or TEI12]",957800000,"agreed","2016-11-03T16:09:05.430","2016-11-22T09:27:26.183","","","Rel-12","36.101","12.13.0","LTE-RF","4029","","A","RP-162411","","","","",""]
["R4-1609584","Correction of spurious emissions requirements for Band 9 range and intra-band CA","Ericsson","Christian Bergljung","21143","CR","Approval","CR to correct notes on applicability of spurious emissions requirements for intra-band CA and remove redunant protection requirements for the Band 9 range","","12","4.2.1","UE RF (core / EMC)  [WI code or TEI12]",957900000,"agreed","2016-11-03T16:09:05.523","2016-11-22T09:27:26.183","","","Rel-13","36.101","13.5.0","LTE-RF","4030","","A","RP-162411","","","","",""]
["R4-1609585","Correction of spurious emissions requirements for Band 9 range and intra-band CA","Ericsson","Christian Bergljung","21143","CR","Approval","CR to correct notes on applicability of spurious emissions requirements for intra-band CA and remove redunant protection requirements for the Band 9 range","","12","4.2.1","UE RF (core / EMC)  [WI code or TEI12]",958000000,"agreed","2016-11-03T16:09:05.600","2016-11-22T09:27:26.197","","","Rel-14","36.101","14.1.0","LTE-RF","4031","","A","RP-162411","","","","",""]
["R4-1609586","Introduction of UE transmitter requirements for LAA Scell operation in Band 46","Ericsson","Christian Bergljung","21143","CR","Approval","CR to introduce transmitter characteristics for uplink operations in Band 46 (clause 6 except the actual E-UTRA CA configurations addressed in basket CRs)","","243","8.18.2","UE RF (36.101) [LTE_eLAA-Core]",4590000,"revised","2016-11-03T16:09:05.693","2016-11-06T20:16:51.227","","R4-1610735","Rel-14","36.101","14.1.0","LTE_eLAA-Core","4032","","B","","","","","",""]
["R4-1609587","Alignment with Wi-Fi channel bonding in 36.104","Ericsson","Christian Bergljung","21143","discussion","Discussion","In this contribution we show how the Wi-Fi channel bonding concept can be introduced in 36.104 (for Rel-15) in case the Type 2 channel access procedure is used","","248","8.18.3","BS RF (36.104) [LTE_eLAA-Core]",960600000,"withdrawn","2016-11-03T16:09:05.787",null,"","","Rel-14","","","LTE_eLAA-Core","","","","","","","","",""]
["R4-1609588","MPR and A-MPR for eLAA UL","Ericsson","Christian Bergljung","21143","discussion","Discussion","In this contribution we discuss the specification of MPR and A-MPR for eLAA","","244","8.18.2.1","MPR [LTE_eLAA-Core]",958800000,"noted","2016-11-03T16:09:05.803","2016-11-06T20:17:58.400","","","Rel-14","","","LTE_eLAA-Core","","","","","","","","",""]
["R4-1609589","Time masks for eLAA UL","Ericsson","Christian Bergljung","21143","other","Approval","In this contribution we propose time masks and power templates for eLAA","","247","8.18.2.4","Other requirements [LTE_eLAA-Core]",198000,"noted","2016-11-03T16:09:05.833","2016-11-06T20:20:12.057","","","Rel-14","","","LTE_eLAA-Core","","","","","","","","",""]
["R4-1609590","UE reference architecture for NR","Ericsson, Sony","Christian Bergljung","21143","discussion","Discussion","In this contribution we discuss a UE reference architecture for devising UE TX and RX requirements at 30 GHz","","416","11.5.2","UE RF  [FS_NR_newRAT]",923700000,"noted","2016-11-03T16:09:05.850","2016-11-06T20:28:29.933","","","Rel-14","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1609591","On mm-wave UE ACLR for 30, 45 and 70 GHz","Ericsson","Christian Bergljung","21143","other","Approval","In this contribution we propose UE ACLR levels for the example frequency ranges of 30 GHz, 45 GHz and 70 GHz.","","417","11.5.2.1","Transmitter characteristics [FS_NR_newRAT]",995100000,"noted","2016-11-03T16:09:05.867","2016-11-06T20:29:51.457","","","Rel-14","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1609592","TP for 38.803: UE beamforming and number of UE transmitter antennas","Ericsson, Sony","Christian Bergljung","21143","pCR","Approval","In this text proposal we address the number of UE (transmit) antennas to be considered for NR requirements and the UL beamforming gains thus achievable","","417","11.5.2.1","Transmitter characteristics [FS_NR_newRAT]",972200000,"revised","2016-11-03T16:09:05.880","2016-11-06T20:32:42.743","","R4-1610594","","38.803","0.3.0","FS_NR_newRAT","","","","","","","","",""]
["R4-1609593","Correction to Band 70 reference to notes in 5.7.3","Dish Network","Farhad Tchoubineh","66686","CR","Approval","Reference to the Note 6 is needed to be specified for Band 70 in 5.7.3","","374","8.32.2","RF  [WI code or TEI14]",83200,"agreed","2016-11-03T17:17:27.090","2016-11-03T18:24:42.247","","","Rel-14","36.101","14.1.0","TEI14","4033","","F","RP-162408","","","","",""]
["R4-1609594","CR:Updates to LAA PDSCH demodulation performance requirements (Rel-13)","Huawei, HiSilicon","Xiang Li","56874","CR","Agreement","This CR updates the existing LAA PDSCH perf test in Rel-13 by including the final requirements based on the agreed R4-168678 in RAN4#80Bis, timing offset 15us and other possible updates","","108","6.2.4.2","PDSCH [LTE_LAA-Perf]",918100000,"revised","2016-11-03T17:35:07.767","2016-11-10T09:52:26.507","R4-168678","R4-1610642","Rel-13","36.101","13.5.0","LTE_LAA-Perf","3878","2","F","","","","","",""]
["R4-1609595","CR: Updates to LAA PDSCH demodulation performance requirements (Rel-14)","Huawei,HiSilicon","Xiang Li","56874","CR","Agreement","This is a mirroe CR, updates the existing LAA PDSCH perf test in Rel-14, including typo correction, SNR as per the simulation results etc.,","","108","6.2.4.2","PDSCH [LTE_LAA-Perf]",959400000,"agreed","2016-11-03T17:36:55.267","2016-11-19T17:47:25.723","R4-167563","","Rel-14","36.101","14.1.0","LTE_LAA-Perf","3879","1","A","RP-162386","","","","",""]
["R4-1609596","Proposal for MPAC alignment pass/fail limits","ROHDE & SCHWARZ","Thorsten Hertel","60675","discussion","Approval","This contribution proposes the pass/fail limit for the MPAC alignment efforts.","","223","8.14.2","Performance requirements [LTE_MIMO_OTA-Core]",52900000,"revised","2016-11-03T18:50:12.110","2016-11-07T16:09:14.813","","R4-1610960","","37.977","","","","","","","","","","",""]
["R4-1609597","Proposal following UMi decision to declare RTS harmonized","ROHDE & SCHWARZ","Thorsten Hertel","60675","discussion","Approval","Following the decision to use the UMi channel model for the TRMS test cases, it is proposed to declare the Radiated Two-Stage Method harmonized based on the very close correlation from the previous harmonization campaign.","","224","8.14.3","Harmonization [LTE_MIMO_OTA-Core]",934000000,"noted","2016-11-03T18:57:45.243","2016-11-07T16:06:43.913","","","","37.977","","","","","","","","","","",""]
["R4-1609598","Overview of NR UE Test Proposals in NF and FF","ROHDE & SCHWARZ","Thorsten Hertel","60675","discussion","Discussion","This contribution provides an overview of different approaches suitable for NR UE testing as well as pros and cons of NF vs FF approaches","","419","11.5.2.3","Testability [FS_NR_newRAT]",12800000,"noted","2016-11-03T18:59:54.677","2016-11-07T20:15:58.213","","","","","","","","","","","","","","",""]
["R4-1609599","36.101 CR:  Addition of Band 25 to M1 bands","SPRINT Corporation","George Cummings","45981","CR","Approval","36.101 CR:  Addition of Band 25 to M1 bands","","45","5.5.1","UE RF (36.101)  [LTE_MTCe2_L1-Core]",969500000,"endorsed","2016-11-03T19:30:16.710","2016-11-04T16:36:32.727","","","Rel-13","36.101","13.5.0","TEI13","4034","","B","","","","","",""]
["R4-1609600","TP for TR 36.714-02-01: CA_2DL_13A-46A_1UL_BCS0 with MSD","Nokia, Verizon Wireless","Bartlomiej Golebiowski","61448","other","Approval","---","","154","8.2.3","BS RF(36.104) [LTE_CA_R14_2DL1UL-Core]",960000000,"approved","2016-11-03T19:45:03.210","2016-11-04T22:10:10.347","","","","","","","","","","","","","","",""]
["R4-1609601","TP for TR 36.714-03-01: CA_3DL_13A-46C_1UL_BCS0 with MSD","Nokia, Verizon Wireless","Bartlomiej Golebiowski","61448","other","Approval","---","","160","8.3.3","BS RF(36.104) [LTE_CA_R14_3DL1UL-Core]",960100000,"approved","2016-11-03T19:45:03.227","2016-11-04T22:10:10.360","","","","","","","","","","","","","","",""]
["R4-1609602","TP for TR 36.714-04-01: CA_4DL_13A-46D_1UL_BCS0 with MSD","Nokia, Verizon Wireless","Bartlomiej Golebiowski","61448","other","Approval","---","","166","8.4.3","BS RF(36.104) [LTE_CA_R14_4DL1UL-Core]",960200000,"approved","2016-11-03T19:45:03.240","2016-11-04T22:10:10.360","","","","","","","","","","","","","","",""]
["R4-1609603","TP for TR 36.714-05-01: CA_5DL_13A-46E_1UL_BCS0 with MSD","Nokia, Verizon Wireless","Bartlomiej Golebiowski","61448","other","Approval","---","","172","8.5.3","BS RF(36.104) [LTE_CA_R14_5DL1UL-Core]",960300000,"approved","2016-11-03T19:45:03.273","2016-11-04T22:10:10.360","","","","","","","","","","","","","","",""]
["R4-1609604","Simulation results for eLAA BS Rx requirements","Nokia, Alcatel-Lucent Shanghai Bell","Bartlomiej Golebiowski","61448","other","Approval","This contribution provide SNR simulation results for eLAA","","249","8.18.3.1","SNR and NF  [LTE_eLAA-Core]",960400000,"approved","2016-11-03T19:45:03.287","2016-11-04T22:10:10.360","","","","","","","","","","","","","","",""]
["R4-1609605","LAA BS unwanted emission mask for 10 MHz carrier in 36.141","Nokia, Alcatel-Lucent Shanghai Bell, Ericsson","Bartlomiej Golebiowski","61448","CR","Approval","---","","248","8.18.3","BS RF (36.104) [LTE_eLAA-Core]",958700000,"agreed","2016-11-03T19:45:03.320","2016-11-04T22:10:10.360","","","Rel-14","36.141","14.1.0","LTE_eLAA-Perf","0931","","B","RP-162387","","","","",""]
["R4-1609606","ACLR for Band 46 for 10 MHz carrier in 36.141","Nokia, Alcatel-Lucent Shanghai Bell","Bartlomiej Golebiowski","61448","CR","Approval","---","","248","8.18.3","BS RF (36.104) [LTE_eLAA-Core]",960500000,"agreed","2016-11-03T19:45:03.397","2016-11-04T22:10:10.377","","","Rel-14","36.141","14.1.0","LTE_eLAA-Perf","0932","","B","RP-162387","","","","",""]
["R4-1609607","On Multi-node tests pass/fail criteria","Nokia, Alcatel-Lucent Shanghai Bell","Bartlomiej Golebiowski","61448","other","Approval","Further considerations on Multi-node tests details","","140","7.1.2","Multi-node testing [FS_LTE_LAA_multinode_test]",936500000,"noted","2016-11-03T19:45:03.477","2016-11-04T22:10:10.377","","","","","","","","","","","","","","",""]
["R4-1609608","Power Class 1 HPUE ACLR","Motorola Solutions UK Ltd.","Xiaowei Jin","45982","discussion","Approval","---","","234","8.16.2","UE RF (36.101)  [LTE_HPUE_B3_B20_B28]",960800000,"noted","2016-11-03T20:05:23.707","2016-11-04T15:12:14.787","","","","","","LTE_HPUE_B3_B20_B28-Core","","","","","","","","",""]
["R4-1609609","Power Class 1 UE emission requirements","Motorola Solutions UK Ltd.","Xiaowei Jin","45982","discussion","","---","","234","8.16.2","UE RF (36.101)  [LTE_HPUE_B3_B20_B28]",960900000,"noted","2016-11-03T20:06:31.863","2016-11-04T15:12:14.787","","","","","","LTE_HPUE_B3_B20_B28-Core","","","","","","","","",""]
["R4-1609610","Release 12.13.0 CR to 36.101 to add Band 25 and Band 26 to Category 0","SPRINT Corporation","John Humbert","40476","CR","Approval","Release 12.13.0 CR to 36.101 to add Band 25 and Band 26 to Category 0","","5","4.1.1","UE RF (core / EMC) [WI code or TEI12]",961000000,"endorsed","2016-11-03T20:16:28.597","2016-11-04T16:07:53.837","","","Rel-12","36.101","12.13.0","","4035","","B","","","","","",""]
["R4-1609611","CR: E-UTRAN FDD-FDD Intra frequency handover for Cat-M1 UEs in CEModeB (Rel-13)","Nokia, Alcatel-Lucent Shanghai Bell","Ren Da","45542","CR","Approval","---","","88","6.1.1.3.2","Intra-frequency Handover [LTE_MTCe2_L1-Perf]",961100000,"revised","2016-11-03T20:19:39.580","2016-11-04T16:06:22.657","","R4-1610678","Rel-13","36.133","13.5.0","LTE_MTCe2_L1-Perf","4220","","B","","","","","",""]
["R4-1609612","CR: E-UTRAN FDD-FDD Intra frequency handover for Cat-M1 UEs in CEModeB (Rel-14)","Nokia, Alcatel-Lucent Shanghai Bell","Ren Da","45542","CR","Approval","---","","88","6.1.1.3.2","Intra-frequency Handover [LTE_MTCe2_L1-Perf]",961200000,"agreed","2016-11-03T20:19:39.687","2016-11-25T01:57:27.113","","","Rel-14","36.133","14.1.0","LTE_MTCe2_L1-Perf","4221","","A","RP-162382","","","","",""]
["R4-1609613","CR: E-UTRAN HD-FDD Intra frequency handover for Cat-M1 UEs in CEModeB (Rel-13)","Nokia, Alcatel-Lucent Shanghai Bell","Ren Da","45542","CR","Approval","---","","88","6.1.1.3.2","Intra-frequency Handover [LTE_MTCe2_L1-Perf]",961300000,"revised","2016-11-03T20:19:39.797","2016-11-04T16:06:22.673","","R4-1610679","Rel-13","36.133","13.5.0","LTE_MTCe2_L1-Perf","4222","","B","","","","","",""]
["R4-1609614","CR: E-UTRAN HD-FDD Intra frequency handover for Cat-M1 UEs in CEModeB (Rel-14)","Nokia, Alcatel-Lucent Shanghai Bell","Ren Da","45542","CR","Approval","---","","88","6.1.1.3.2","Intra-frequency Handover [LTE_MTCe2_L1-Perf]",961400000,"agreed","2016-11-03T20:19:39.877","2016-11-25T01:57:27.157","","","Rel-14","36.133","14.1.0","LTE_MTCe2_L1-Perf","4223","","A","RP-162382","","","","",""]
["R4-1609615","CR: E-UTRAN TDD-TDD Intra frequency handover for Cat-M1 UEs in CEModeB (Rel-13)","Nokia, Alcatel-Lucent Shanghai Bell","Ren Da","45542","CR","Approval","---","","88","6.1.1.3.2","Intra-frequency Handover [LTE_MTCe2_L1-Perf]",961500000,"revised","2016-11-03T20:19:39.987","2016-11-04T16:06:22.673","","R4-1610680","Rel-13","36.133","13.5.0","LTE_MTCe2_L1-Perf","4224","","B","","","","","",""]
["R4-1609616","CR: E-UTRAN TDD-TDD Intra frequency handover for Cat-M1 UEs in CEModeB (Rel-14)","Nokia, Alcatel-Lucent Shanghai Bell","Ren Da","45542","CR","Approval","---","","88","6.1.1.3.2","Intra-frequency Handover [LTE_MTCe2_L1-Perf]",961600000,"agreed","2016-11-03T20:19:40.093","2016-11-25T01:57:27.157","","","Rel-14","36.133","14.1.0","LTE_MTCe2_L1-Perf","4225","","A","RP-162382","","","","",""]
["R4-1609617","eMTC intra- and inter-frequency measurements without measurement gap","Nokia, Alcatel-Lucent Shanghai Bell","Ren Da","45542","other","Approval","---","","319","8.25.3.2.1","Measurement [LTE_feMTC-Core]",2540000,"noted","2016-11-03T20:19:40.187","2016-11-04T16:06:22.687","","","","","","LTE_feMTC-Core","","","","","","","","",""]
["R4-1609618","LS: eMTC intra- and inter-frequency measurements without measurement gap","Nokia, Alcatel-Lucent Shanghai Bell","Ren Da","45542","LS out","Approval","---","","319","8.25.3.2.1","Measurement [LTE_feMTC-Core]",4950000,"noted","2016-11-03T20:19:40.203","2016-11-04T16:06:22.610","","","","","","","","","","","","","","",""]
["R4-1609619","UE transmit timing requirement for NB-IoT in normal coverage","Nokia, Alcatel-Lucent Shanghai Bell","Ren Da","45542","other","Approval","---","","56","5.6.4","RRM core (36.133)  [NB_IOT-Core]",3900010,"noted","2016-11-03T20:19:40.220","2016-11-04T16:06:22.610","","","","","","NB_IOT-Core","","","","","","","","",""]
["R4-1609620","CR: UE transmit timing requirement for NB-IoT in normal coverage (Rel-13)","Nokia, Alcatel-Lucent Shanghai Bell","Ren Da","45542","CR","Approval","---","","56","5.6.4","RRM core (36.133)  [NB_IOT-Core]",9313000,"revised","2016-11-03T20:19:40.250","2016-11-04T16:06:22.657","","R4-1610546","Rel-13","36.133","13.5.0","NB_IOT-Core","4226","","F","","","","","",""]
["R4-1609621","CR: UE transmit timing requirement for NB-IoT in normal coverage (Rel-14)","Nokia, Alcatel-Lucent Shanghai Bell","Ren Da","45542","CR","Approval","---","","56","5.6.4","RRM core (36.133)  [NB_IOT-Core]",9536000,"withdrawn","2016-11-03T20:19:40.360",null,"","","Rel-14","36.133","14.1.0","NB_IOT-Core","4227","","A","","","","","",""]
["R4-1609622","Proposed WID to add Power Class 2 to band 41 intra-band contiguous carrier aggregation.","SPRINT Corporation","John Humbert","40476","discussion","Information","Proposed WID to add Power Class 2 to band 41 intra-band contiguous carrier aggregation.","","430","13","Revision of the Work Plan",949200000,"available","2016-11-03T20:36:52.747","2016-11-04T16:07:53.837","","","Rel-15","36.101","","","","","","","","","","",""]
["R4-1609623","Discuss the effect of a lower Maximum Transmit Power on physical and protocol layers, and on increase in outage and repetitions","Qualcomm Incorporated","Prashanth Akula","67450","other","Approval","---","","304","8.24.2.1","Power Class       [NB_IOTenh-Core]",954400000,"noted","2016-11-03T20:53:43.327","2016-11-04T16:26:32.753","","","Rel-14","","","NB_IOTenh-Core","","","","","","","","",""]
["R4-1609624","IMT parameters for response to ITU-R WP5D","Ericsson","Johan Skold","10425","other","Approval","For the response to ITU-R, the paper goes through the IMT parameters and makes further proposals for how to respond, based on the present input on those parameters.","","412","11.3.3","others  [FS_NR_newRAT]",962400000,"noted","2016-11-03T21:10:10.560","2016-11-07T21:03:14.637","","","Rel-14","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1609625","Re-use of requirements below 6 GHz","Ericsson","Johan Skold","10425","discussion","Discussion","Based on the way forward agreed for requirement below 6 GHz, a walk-through is made of the RF parameters and the possibility to re-use existing requirements.","","415","11.5.1","Common issues for UE and BS [FS_NR_newRAT]",962700000,"available","2016-11-03T21:10:10.590","2016-11-07T21:03:14.653","","","Rel-14","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1609626","TP for TR 38.903: Re-use of requirements below 6 GHz","Ericsson","Johan Skold","10425","pCR","Approval","Text proposal with a walk-through of the RF parameters and the possibility to re-use existing requirements.","","415","11.5.1","Common issues for UE and BS [FS_NR_newRAT]",964700000,"noted","2016-11-03T21:10:10.607","2016-11-07T21:03:14.653","","","","38.803","0.3.0","FS_NR_newRAT","","","","","","","","",""]
["R4-1609627","NR unwanted emissions for BS and UE","Ericsson","Johan Skold","10425","other","Approval","The paper discusses the options for unwanted emission requirements, in particular for the out-of-band domain.","","415","11.5.1","Common issues for UE and BS [FS_NR_newRAT]",952800000,"noted","2016-11-03T21:10:10.620","2016-11-07T21:03:14.620","","","Rel-14","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1609628","Spectrum emission mask for NR BS in mm-wave bands","Ericsson","Johan Skold","10425","discussion","Discussion","The paper makes proposals for a spectrum emission mask for NR BS.","","421","11.5.3.1","Transmitter characteristics [FS_NR_newRAT]",44300000,"noted","2016-11-03T21:10:10.653","2016-11-07T21:03:14.637","","","Rel-14","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1609629","LS response to ECC PT1 on Suitability of technical conditions of ECC DEC (11) 06 for 5G","Ericsson","Johan Skold","10425","LS out","Agreement","The LS responds to the questions from ECC PT1 regarding RF parameters for the bands in 3400-3800 MHz.","","407","11.1","General   [FS_NR_newRAT]",965800000,"revised","2016-11-03T21:10:10.667","2016-11-07T21:03:14.637","","R4-1610592","Rel-14","","","FS_NR_newRAT","","","","","R4-1609013","ECC PT1","ETSI ERM","",""]
["R4-1609630","LTE UE TRP and TRS Requirements for North American Bands","SPRINT, Verizon, AT&T, SouthernLINC. T-Mobile USA, Bell Canada","John Humbert","40476","other","Approval","LTE UE TRP and TRS Requirements for North American Bands","","218","8.13.2","Hand phantom for smartphones [LTE_UTRA_TRP_TRS-Core]",5040000,"revised","2016-11-03T21:40:51.733","2016-11-04T16:07:53.837","","R4-1610787","Rel-14","","","LTE_UTRA_TRP_TRS, LTE_UTRA_TRP_TRS-Core","","","","","","","","",""]
["R4-1609631","Further Co-existence simulation results for licensed band V2V","Ericsson","Gary Boudreau","43498","other","Approval","This contribution provides additional co-existence simulation results for V2V licensed bands","","276","8.20.2.2","Co-existence study for case 1 and case 2  [LTE_V2X-Core]",963100000,"noted","2016-11-03T21:42:35.893","2016-11-04T19:30:48.643","","","Rel-14","","","LTE_V2X-Core","","","","","","","","",""]
["R4-1609632","RF Requirements for V2V in unlicensed Bands","Ericsson","Gary Boudreau","43498","other","Approval","This contribution provides proposals to address the open V2V RF requirements for unlicensed bands.","","261","8.19.1.2","Blocking  [LTE_SL_V2V-Core]",4260000,"noted","2016-11-03T21:42:35.910","2016-11-07T16:59:04.830","","","Rel-14","","","LTE_SL_V2V-Core","","","","","","","","",""]
["R4-1609633","Co-existence simulation results for 33 dBm V2V UEs and band 47","Ericsson","Gary Boudreau","43498","other","Approval","This contribution provides  co-existence simulation results for 33 dBm V2V UEs and band 47.","","275","8.20.2.1","Co-existence study for High power V2X UE  [LTE_V2X-Core]",963300000,"noted","2016-11-03T21:42:35.927","2016-11-04T19:30:48.643","","","Rel-14","","","LTE_V2X-Core","","","","","","","","",""]
["R4-1609634","UE RF architecture for multicarrier V2X","Ericsson","Gary Boudreau","43498","other","Approval","This contribution proposes architectures for V2X multicarrier operation.","","277","8.20.3","UE RF (36.101) [LTE_V2X-Core]",963400000,"noted","2016-11-03T21:42:35.957","2016-11-07T16:59:46.200","","","Rel-14","","","LTE_V2X-Core","","","","","","","","",""]
["R4-1609635","UE RF Tx requirements in  V2X licensed bands","Ericsson","Gary Boudreau","43498","other","Approval","This contribution addresses UE RF transmit requirements for V2X in licensed bands.","","278","8.20.3.1","Tx requirements  [LTE_V2X-Core]",935100000,"noted","2016-11-03T21:42:35.973","2016-11-07T16:59:46.200","","","Rel-14","","","LTE_V2X-Core","","","","","","","","",""]
["R4-1609636","UE RF Rx requirements in V2X licensed bands","Ericsson","Gary Boudreau","43498","other","Approval","This contribution addresses UE RF receive requirements for V2X in licensed bands.","","279","8.20.3.2","Rx requirements  [LTE_V2X-Core]",963600000,"noted","2016-11-03T21:42:36.003","2016-11-07T16:59:46.200","","","Rel-14","","","LTE_V2X-Core","","","","","","","","",""]
["R4-1609637","Power Control for V2V Adjacent Channel Co-existence in Licensed Bands","Ericsson","Gary Boudreau","43498","other","Approval","This contribution further discusses the impact of UL power control on V2V performance","","276","8.20.2.2","Co-existence study for case 1 and case 2  [LTE_V2X-Core]",963700000,"noted","2016-11-03T21:42:36.037","2016-11-04T19:29:18.990","","","Rel-14","","","LTE_V2X-Core","","","","","","","","",""]
["R4-1609638","LS to RAN1 on UL PC for V2V","Ericsson","Gary Boudreau","43498","LS out","Approval","This LS to RAN1 recommends that open loop UL PC be supported in V2V UE's to address adjacent channel interference to legacy UE's.","","276","8.20.2.2","Co-existence study for case 1 and case 2  [LTE_V2X-Core]",963800000,"revised","2016-11-03T21:42:36.050","2016-11-04T19:29:58.443","","R4-1610755","Rel-14","","","LTE_V2X-Core","","","","","","RAN1","","",""]
["R4-1609639","Release 13 CR to add Band 25 to the list of 4RX supported Bands","SPRINT Corporation","John Humbert","40476","CR","Approval","Release 13 CR to Add Band 25 to the list of 4RX supported Bands","","29","5.2.1","UE RF (36.101)  [LTE_4Rx_AP_DL-Core]",991600000,"endorsed","2016-11-03T21:57:35.297","2016-11-04T16:07:53.837","","","Rel-13","36.101","13.5.0","","4036","","B","","","","","",""]
["R4-1609640","Introduction of completed R14 2DL band combinations to TS 36.101","Qualcomm Incorporated","Ville Vintola","44963","CR","Agreement","---","","152","8.2.1","Rapporteur Input (WID/CRs) [LTE_CA_R14_2DL1UL-Core]",904100000,"agreed","2016-11-03T23:24:53.887","2016-11-19T17:47:25.757","","","Rel-14","36.101","14.1.0","LTE_CA_R14_2DL1UL-Core","4037","","B","RP-162399","","","","",""]
["R4-1609641","Introduction of completed R14 2DL band combinations to TS 36.104","Qualcomm Incorporated","Ville Vintola","44963","CR","Agreement","---","","152","8.2.1","Rapporteur Input (WID/CRs) [LTE_CA_R14_2DL1UL-Core]",964000000,"agreed","2016-11-03T23:24:54.010","2016-11-19T17:47:25.770","","","Rel-14","36.104","14.1.0","LTE_CA_R14_2DL1UL-Core","0898","","B","RP-162399","","","","",""]
["R4-1609642","Introduction of completed R14 2DL band combinations to TS 36.141","Qualcomm Incorporated","Ville Vintola","44963","CR","Agreement","---","","152","8.2.1","Rapporteur Input (WID/CRs) [LTE_CA_R14_2DL1UL-Core]",964100000,"agreed","2016-11-03T23:24:54.120","2016-11-19T17:47:25.770","","","Rel-14","36.141","14.1.0","LTE_CA_R14_2DL1UL-Core","0933","","B","RP-162399","","","","",""]
["R4-1609643","Introduction of completed R14 2DL band combinations to TS 36.104","Qualcomm Incorporated","Ville Vintola","44963","LS out","Approval","DRAFT LS reply for UL256QAM capability","","226","8.15.1","UE capability for UL256QAM  [LTE_UL_CAP_enh-Core]",964400000,"revised","2016-11-03T23:24:54.213","2016-11-19T17:47:25.787","","R4-1610991","Rel-14","","","LTE_UL_CAP_enh","","","","","R4-163125","TSG RAN WG1, TSG RAN WG2","","R1-163915",""]
["R4-1609644","Introduction of completed R14 2DL band combinations to TS 36.141","Qualcomm Incorporated, CMCC, Sprint, Verizon, DISH, Softbank, Huawei, Mediatek, Intel, Motorola Mobility, Sony, OPPO, Vivo, Xiaomi, Coolpad, Blackberry, LGE, Interdigital","Ville Vintola","44963","other","Approval","WF on  UL256QAM capability","","226","8.15.1","UE capability for UL256QAM  [LTE_UL_CAP_enh-Core]",96500000,"noted","2016-11-03T23:24:54.247","2016-11-07T21:27:16.727","","","Rel-14","","","LTE_UL_CAP_enh","","","","","","","","",""]
["R4-1609645","PA simulations vs. Measurement for EVM","Qualcomm Incorporated","Ville Vintola","44963","discussion","","This paper discusses PA simulation and model accuracy for EVM","","228","8.15.2.1","MPR/A-MPR [LTE_UL_CAP_enh-Core]",939600000,"noted","2016-11-03T23:24:54.260","2016-11-07T03:27:31.080","","","Rel-14","","","LTE_UL_CAP_enh","","","","","","","","",""]
["R4-1609646","2UL CA MPR for UL 256QAM","Qualcomm Incorporated","Ville Vintola","44963","discussion","","This paper discusses 2 UL CA MPR for UL 256 QAM","","228","8.15.2.1","MPR/A-MPR [LTE_UL_CAP_enh-Core]",939800000,"approved","2016-11-03T23:24:54.290","2016-11-07T03:27:31.063","","","Rel-14","","","LTE_UL_CAP_enh","","","","","","","","",""]
["R4-1609647","Guardband for NR, waveform, OFDM & WOLA","Qualcomm Incorporated","Ville Vintola","44963","other","Approval","This paper discusses waveforms for NR, differences between F-OFDM and WOLA and their impact to guardband.","","415","11.5.1","Common issues for UE and BS [FS_NR_newRAT]",99500000,"noted","2016-11-03T23:24:54.307","2016-11-07T19:26:00.190","","","","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1609648","Non-contiguous allocations and MPR with OFDM","Qualcomm Incorporated","Ville Vintola","44963","discussion","Discussion","This paper discusses possible need to MPR with OFMD waveforms","","417","11.5.2.1","Transmitter characteristics [FS_NR_newRAT]",986800000,"noted","2016-11-03T23:24:54.323","2016-11-07T22:06:45.893","","","","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1609649","How to define EIS over different beam angles","Qualcomm Incorporated","Ville Vintola","44963","discussion","","This paper discusses how to define OTA requirements with devices with beamforming","","418","11.5.2.2","Receiver characteristics [FS_NR_newRAT]",600000,"noted","2016-11-03T23:24:54.353","2016-11-07T21:21:18.150","","","","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1609650","UL256 QAM Feasibility of grouping for capability","Qualcomm Incorporated","Ville Vintola","44963","discussion","Discussion","Analysis of grouping proposal in R4-167965","","226","8.15.1","UE capability for UL256QAM  [LTE_UL_CAP_enh-Core]",28400000,"noted","2016-11-03T23:24:54.370","2016-11-07T03:27:31.063","","","Rel-14","","","LTE_UL_CAP_enh","","","","","","","","",""]
["R4-1609651","Optional Pcell indocation","Qualcomm Incorporated","Ville Vintola","44963","CR","Agreement","Adding Pcell note according to agreed paper R4-165193. Rel-12 Cat-F CR","","12","4.2.1","UE RF (core / EMC)  [WI code or TEI12]",958100000,"agreed","2016-11-03T23:24:54.387","2016-11-07T03:27:31.093","","","Rel-12","36.101","12.13.0","TEI12","4038","","F","RP-162420","","","","",""]
["R4-1609652","Optional Pcell indocation","Qualcomm Incorporated","Ville Vintola","44963","CR","Agreement","Adding Pcell note according to agreed paper R4-165193. Rel-13 Cat-F CR. Note is added, therefore Cat-F","","12","4.2.1","UE RF (core / EMC)  [WI code or TEI12]",958200000,"agreed","2016-11-03T23:24:54.510","2016-11-07T03:27:31.093","","","Rel-13","36.101","13.5.0","TEI13","4039","","F","RP-162435","","","","",""]
["R4-1609653","Optional Pcell indocation","Qualcomm Incorporated","Ville Vintola","44963","CR","Agreement","Adding Pcell note according to agreed paper R4-165193. Rel-14 Cat-A CR","","12","4.2.1","UE RF (core / EMC)  [WI code or TEI12]",958300000,"agreed","2016-11-03T23:24:54.620","2016-11-19T17:47:25.803","","","Rel-14","36.101","14.1.0","TEI13","4040","","A","RP-162435","","","","",""]
["R4-1609654","New WID: Lower Complexity Higher Order MIMO for LTE","Qualcomm Incorporated","Ville Vintola","44963","WID new","Information","New WID proposal: Low complexity higher order MIMO_x00B_. Current 4rx requirement lead to a very complex implementation especially if  CA is considered. We introduce a new method to implement higher order diversity and 4x4 MIMO with simplified UE implemen","","430","13","Revision of the Work Plan",205000,"available","2016-11-03T23:24:54.713","2016-11-07T03:27:31.080","","","Rel-14","","","","","","","","","","","",""]
["R4-1609655","Motivation for the New WID: Low complexity higher order MIMO","Qualcomm Incorporated","Ville Vintola","44963","discussion","Information","This is motivation document for proposed new work item \"Low complexity higher order MIMO\"","","430","13","Revision of the Work Plan",2820000,"available","2016-11-03T23:24:54.743","2016-11-07T03:27:31.093","","","Rel-14","","","","","","","","","","","",""]
["R4-1609656","B46 REFSENS test exclusion range for 10-MHz carrier","MediaTek Inc.","James Wang","56966","other","Approval","In this contribution, we propose that the B46 REFSENS test frequency exclusion ranges defined for 20-MHz carrier can also be applied for 10-MHz carrier.","","40","5.4.1","UE RF and EMC [LTE_LAA-Core]",4230000,"noted","2016-11-04T00:12:21.353","2016-11-04T21:34:30.507","","","Rel-14","36.101","14.1.0","LTE_LAA-Core","","","","","","","","",""]
["R4-1609657","Phase noise impact in mm-Wave NR","MediaTek Inc.","James Wang","56966","other","Discussion","In this contribution, we discuss the potential LO phase noise impact to mm-Wave signal quality and its implication to the applicable highest order modulation.","","415","11.5.1","Common issues for UE and BS [FS_NR_newRAT]",27900000,"noted","2016-11-04T00:21:01.507","2016-11-04T21:34:57.077","","","","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1609658","NR wideband carrier consideration","MediaTek Inc.","James Wang","56966","other","Discussion","In this contribution, we provide the UE receiver power consumption comparison between single-carrier and CCA of the same RF carrier bandwidth up to 800 MHz. Based on our preliminary analysis, it is expected that CCA would be less favourable than single-ca","","407","11.1","General   [FS_NR_newRAT]",98190000,"noted","2016-11-04T00:25:20.387","2016-11-04T21:35:18.260","","","","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1609659","UE receiver SNDR versus carrier bandwidth","MediaTek Inc.","James Wang","56966","other","Discussion","In this contribution, we evaluate the UE receiver SNDR performance versus carrier bandwidth. The analysis results indicate that the highest modulation order applicable for the radio would be lowered for wider carrier bandwidth if phase noise would not dom","","407","11.1","General   [FS_NR_newRAT]",905600000,"noted","2016-11-04T00:28:53.700","2016-11-04T21:35:37.260","","","","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1609660","On BS Output Power Requirement for NR","Sumitomo Elec. Industries, Ltd","Li Yue","58006","other","Approval","This contribution studies what metric, EIRP or TRP or both, should be used in specifying the output power accuracy of NR BSs and in defining the BS class power limit, and proposes: \nProposal 1 BS Output power accuracy requirement is specified with EIRP\nPr","","421","11.5.3.1","Transmitter characteristics [FS_NR_newRAT]",93500000,"noted","2016-11-04T00:53:37.480","2016-11-04T01:10:20.030","","","Rel-14","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1609661","On spatial coverage requirement for mmWave NR UE","Sumitomo Elec. Industries, Ltd","Li Yue","58006","other","Approval","This contribution discusses whether the whole spatial coverage of EIRP/EIS requirement should be specified for mmWave NR UEs. Taking into account that there would be wide variety of UE types in 5G era, we have the following proposal and observation\nPropos","","416","11.5.2","UE RF  [FS_NR_newRAT]",966100000,"noted","2016-11-04T01:00:41.410","2016-11-04T01:10:20.090","","","Rel-14","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1609662","Considerations on NR spectrum utilization and usage of fractional RB","ZTE, ZTE Microelectronics","Yuqiang Zhang","43207","discussion","","In this contribution we discuss the NR spectrum utilization Y and usage of fractional PRB. It has been discussed to use fractional PRB method to increase the band edge utilization to increase carrier spectrum utilization Y, and also use fractional PRB met","","415","11.5.1","Common issues for UE and BS [FS_NR_newRAT]",94130000,"noted","2016-11-04T01:02:14.603","2016-11-04T10:05:02.573","","","","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1609663","NPDCCH/NPDSCH simulation results","Samsung","Haijie Qiu","46265","discussion","Discussion","In this document, we provide NPDCCH/NPDSCH simulation results.","","130","6.3.4.1.2","NPDCCH [NB_IOT-Perf]",943700000,"noted","2016-11-04T01:04:20.340","2016-11-04T12:40:11.297","","","Rel-13","","","NB_IOT-Perf","","","","","","","","",""]
["R4-1609664","MPDCCH/MPDSCH simulation results","Samsung","Haijie Qiu","46265","discussion","Discussion","In this document, we provide MPDCCH/MPDSCH simulation results.","","98","6.1.2.2","MPDCCH [LTE_MTCe2_L1-Perf]",966800000,"noted","2016-11-04T01:04:20.370","2016-11-04T12:40:11.310","","","Rel-13","","","LTE_MTCe2_L1-Perf","","","","","","","","",""]
["R4-1609665","On Introducing High EIRP UE for NR","Sumitomo Elec. Industries, Ltd","Li Yue","58006","other","Approval","This contribution proposes that the high EIRP classes should be specified for NR UEs.\nProposal 1 Different EIRP classes should be specified for NR UE and high EIRP classes should be allowed","","417","11.5.2.1","Transmitter characteristics [FS_NR_newRAT]",966500,"noted","2016-11-04T01:04:45.470","2016-11-04T01:10:20.123","","","Rel-14","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1609666","Considerations on EVM requirement in NR","ZTE, ZTE Microelectronics","Yuqiang Zhang","43207","discussion","","In this contribution, we discuss the potential impacts from an unevenly distributed EVM among the allocated resources and then propose to address the EVM requirement issue independent from any specific waveform.","","415","11.5.1","Common issues for UE and BS [FS_NR_newRAT]",92270000,"noted","2016-11-04T01:07:21.517","2016-11-04T10:05:02.573","","","","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1609667","The impact of IM3 and input PSD on ACLR","ZTE Corporation","Yuqiang Zhang","43207","discussion","","In this paper we provide an analytical insight into how IM3 and input PSD impact on ACLR and propose the following accordingly:\nUnder realistic PA with large signal input, the impact of PSD of an input new waveform on ACLR is trivial if the roll-off of th","","415","11.5.1","Common issues for UE and BS [FS_NR_newRAT]",962600000,"noted","2016-11-04T01:10:59.513","2016-11-04T10:05:02.587","","","","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1609668","CR for Rel-13 eMTC MPDCCH demodulation requirements","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","Agreement","In this CR will update MPDCCH performance requirements value based on the agreed CR R4-168683  in RAN4 #80 bis meeting.","","98","6.1.2.2","MPDCCH [LTE_MTCe2_L1-Perf]",966900000,"revised","2016-11-04T01:13:28.947","2016-11-07T11:30:26.873","R4-167594","R4-1610671","Rel-13","36.101","13.5.0","LTE_MTCe2_L1-Perf","3884","2","F","","","","","",""]
["R4-1609669","CR for Rel-14 eMTC MPDCCH demodulation requirements","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","Agreement","In this CR will update MPDCCH performance requirements value based on the agreed CR R4-168683  in RAN4 #80 bis meeting.","","98","6.1.2.2","MPDCCH [LTE_MTCe2_L1-Perf]",968300000,"agreed","2016-11-04T01:13:29.070","2016-11-22T12:17:27.017","R4-167595","","Rel-14","36.101","14.1.0","LTE_MTCe2_L1-Perf","3885","1","A","RP-162382","","","","",""]
["R4-1609670","Correction of directions diagram in TR 37.842","CATT","Xuhua Tao","62863","CR","Approval","The oriention of ? in some figures is not aligned with definition of term “directions diagram”.Modifying the oriention of ? in some figures to be aligned with definiton of term “directions diagram”.","","22","5.1.1","Technical Report (37.842) [AAS_BS_LTE_UTRA-Core]",942200000,"revised","2016-11-04T01:15:52.760","2016-11-04T14:40:37.330","","R4-1610793","Rel-13","37.842","13.0.0","AAS_BS_LTE_UTRA-Core","0008","","F","","","","","",""]
["R4-1609671","NPRACH simulation result","Ericsson","Kazuyoshi Uesaka","46968","discussion","Discussion","This contribution provides the simulation result for NPRACH demodulation requirements.","","133","6.3.4.2.1","NPRACH  [NB_IOT-Perf]",924500000,"noted","2016-11-04T01:34:57.053","2016-11-04T15:02:33.377","","","Rel-13","","","NB_IOT-Perf","","","","","","","","",""]
["R4-1609672","NPBCH simulation result","Ericsson","Kazuyoshi Uesaka","46968","discussion","Discussion","This contribution provides the simulation result for NPBCH demodulation requirements, and discuss the multiple window size.","","129","6.3.4.1.1","NPBCH  [NB_IOT-Perf]",55500000,"noted","2016-11-04T01:34:57.067","2016-11-04T15:02:33.390","","","Rel-13","","","NB_IOT-Perf","","","","","","","","",""]
["R4-1609673","NPDCCH simulation result","Ericsson","Kazuyoshi Uesaka","46968","discussion","Discussion","This contribution provides the simulation result for NPDCCH demodulation requirements.","","130","6.3.4.1.2","NPDCCH [NB_IOT-Perf]",951800000,"noted","2016-11-04T01:34:57.083","2016-11-04T15:02:33.407","","","Rel-13","","","NB_IOT-Perf","","","","","","","","",""]
["R4-1609674","NPDSCH simulation result","Ericsson","Kazuyoshi Uesaka","46968","discussion","Discussion","This contribution provides the simulation result for NPDSCH demodulation requirements.","","131","6.3.4.1.3","NPDSCH [NB-IOT-Perf]",943200000,"noted","2016-11-04T01:34:57.100","2016-11-04T15:02:33.420","","","Rel-13","","","NB_IOT-Perf","","","","","","","","",""]
["R4-1609675","Correction of NPDCCH demodulation requirements","Ericsson","Kazuyoshi Uesaka","46968","CR","Approval","This CR finalizes the NPDCCH demodulation requirements. (R4-168739)","","130","6.3.4.1.2","NPDCCH [NB_IOT-Perf]",966300000,"revised","2016-11-04T01:34:57.117","2016-11-04T15:02:33.420","","R4-1610557","Rel-13","36.101","13.5.0","NB_IOT-Perf","4041","","F","","","","","",""]
["R4-1609676","Correction of NPDCCH demodulation requirements","Ericsson","Kazuyoshi Uesaka","46968","CR","Approval","This CR finalizes the NPDCCH demodulation requirements. (R4-168739)","","130","6.3.4.1.2","NPDCCH [NB_IOT-Perf]",967500000,"agreed","2016-11-04T01:34:57.223","2016-11-19T17:47:25.803","","","Rel-14","36.101","14.1.0","NB_IOT-Perf","4042","","A","RP-162379","","","","",""]
["R4-1609677","Simulation summary of NB-IoT UE demodulation requirements","Ericsson","Kazuyoshi Uesaka","46968","other","Information","This sheet summarizes the simulation results for NB-IoT UE demodulation requirements.","","128","6.3.4.1","UE Demodulation  [NB_IOT-Perf]",55300000,"noted","2016-11-04T01:34:57.303","2016-11-19T17:47:25.817","","R4-1610553","Rel-13","","","NB_IOT-Perf","","","","","","","","",""]
["R4-1609678","Way forward on NB-IoT UE demodulation requirements","Ericsson","Kazuyoshi Uesaka","46968","discussion","Discussion","This WF discusses the remaining issues to finalized NB-IoT UE demodulation requirements such as NPBCH windows size and common margin.","","128","6.3.4.1","UE Demodulation  [NB_IOT-Perf]",967700000,"revised","2016-11-04T01:34:57.317","2016-11-19T17:47:25.833","","R4-1610554","Rel-13","","","NB_IOT-Perf","","","","","","","","",""]
["R4-1609679","Simulation assumptions for SI acquisition for NB-IoT","Ericsson","Kazuyoshi Uesaka","46968","discussion","Discussion","This contribution provides the simulation assumption for MIB-NB/SIB-NB acquisition time. This is the correction of R4-168805.","","56","5.6.4","RRM core (36.133)  [NB_IOT-Core]",9619000,"noted","2016-11-04T01:34:57.333","2016-11-04T15:02:33.437","","","Rel-13","","","NB_IOT-Core","","","","","","","","",""]
["R4-1609680","Simulation result of MIB-NB/SIB1-NB/SIB2-NB acquisition time","Ericsson","Kazuyoshi Uesaka","46968","discussion","Discussion","This contribution provides the simulation results for MIB-NB and SIB-NB acquisition times.","","56","5.6.4","RRM core (36.133)  [NB_IOT-Core]",54700000,"noted","2016-11-04T01:34:57.350","2016-11-04T15:02:33.453","","","Rel-13","","","NB_IOT-Core","","","","","","","","",""]
["R4-1609681","Simulation summary of eMTC UE demodulation requirements","Ericsson","Kazuyoshi Uesaka","46968","other","Information","This sheet summarizes the simulation results for eMTC UE demodulation requirements.","","96","6.1.2","UE performance (36.101) [LTE_MTCe2_L1-Perf]",968100000,"revised","2016-11-04T01:34:57.367","2016-11-19T17:47:25.847","","R4-1610662","Rel-13","","","LTE_MTCe2_L1-Perf","","","","","","","","",""]
["R4-1609682","eMTC PBCH simulation result","Ericsson","Kazuyoshi Uesaka","46968","discussion","Discussion","This contribution provides the simulation result for PBCH demodulation requirements, and discuss the multiple window size.","","97","6.1.2.1","PBCH [LTE_MTCe2_L1-Perf]",911500000,"noted","2016-11-04T01:34:57.397","2016-11-04T15:02:33.453","","","Rel-13","","","LTE_MTCe2_L1-Perf","","","","","","","","",""]
["R4-1609683","eMTC MPDCCH simulation result","Ericsson","Kazuyoshi Uesaka","46968","discussion","Discussion","This contribution provides the simulation results for MPDCCH demodulation requirements.","","98","6.1.2.2","MPDCCH [LTE_MTCe2_L1-Perf]",946600000,"noted","2016-11-04T01:34:57.410","2016-11-04T15:02:33.467","","","Rel-13","","","LTE_MTCe2_L1-Perf","","","","","","","","",""]
["R4-1609684","eMTC PDSCH simulation result","Ericsson","Kazuyoshi Uesaka","46968","discussion","Discussion","This contribution provides the simulation results for PDSCH demodulation requirements.","","99","6.1.2.3","MPDSCH [LTE_MTCe2_L1-Perf]",968500000,"noted","2016-11-04T01:34:57.443","2016-11-04T15:02:33.483","","","Rel-13","","","LTE_MTCe2_L1-Perf","","","","","","","","",""]
["R4-1609685","Open issues for PDSCH demodulation requirements","Ericsson","Kazuyoshi Uesaka","46968","discussion","Discussion","This contribution discusses the remaining open issues for eMTC PDSCH demodulation requirements.","","99","6.1.2.3","MPDSCH [LTE_MTCe2_L1-Perf]",911700000,"noted","2016-11-04T01:34:57.457","2016-11-04T15:02:33.483","","","Rel-13","","","LTE_MTCe2_L1-Perf","","","","","","","","",""]
["R4-1609686","Correction of PDCSH demodulation requirements for eMTC","Ericsson","Kazuyoshi Uesaka","46968","CR","Approval","This CR finalizes the eMTC PDSCH demodulation requirements.","","99","6.1.2.3","MPDSCH [LTE_MTCe2_L1-Perf]",968600000,"revised","2016-11-04T01:34:57.490","2016-11-04T15:02:33.483","R4-168684","R4-1610672","Rel-13","36.101","13.5.0","LTE_MTCe2_L1-Perf","3928","2","F","","","","","",""]
["R4-1609687","Correction of PDCSH demodulation requirements for eMTC","Ericsson","Kazuyoshi Uesaka","46968","CR","Approval","This CR finalizes the eMTC PDSCH demodulation requirements.","","99","6.1.2.3","MPDSCH [LTE_MTCe2_L1-Perf]",968700000,"agreed","2016-11-04T01:34:57.600","2016-11-19T17:47:25.847","R4-168217","","Rel-14","36.101","14.1.0","LTE_MTCe2_L1-Perf","3929","1","A","RP-162382","","","","",""]
["R4-1609688","eMTC CQI tests","Ericsson","Kazuyoshi Uesaka","46968","discussion","Discussion","This contribution discusses the open issues on CQI test for eMTC and provides the simulation results.","","100","6.1.3","UE CSI reporting (36.101) [LTE_MTCe2_L1-Perf]",968800000,"noted","2016-11-04T01:34:57.723","2016-11-04T15:02:33.500","","","Rel-13","","","LTE_MTCe2_L1-Perf","","","","","","","","",""]
["R4-1609689","Finalizing CQI definition test for eMTC","Ericsson","Kazuyoshi Uesaka","46968","CR","Approval","This CR finalizes the CQI definition test for eMTC.","","100","6.1.3","UE CSI reporting (36.101) [LTE_MTCe2_L1-Perf]",968900000,"revised","2016-11-04T01:34:57.740","2016-11-04T15:02:33.500","","R4-1610673","Rel-13","36.101","13.5.0","LTE_MTCe2_L1-Perf","4043","","F","","","","","",""]
["R4-1609690","Finalizing CQI definition test for eMTC","Ericsson","Kazuyoshi Uesaka","46968","CR","Approval","This CR finalizes the CQI definition test for eMTC.","","100","6.1.3","UE CSI reporting (36.101) [LTE_MTCe2_L1-Perf]",969000000,"agreed","2016-11-04T01:34:57.833","2016-11-19T17:47:25.847","","","Rel-14","36.101","14.1.0","LTE_MTCe2_L1-Perf","4044","","A","RP-162382","","","","",""]
["R4-1609691","Finalizing UE-selected subband CQI test for eMTC","Ericsson","Kazuyoshi Uesaka","46968","CR","Approval","This CR finalizes the UE-selected subband CQI test for eMTC.","","100","6.1.3","UE CSI reporting (36.101) [LTE_MTCe2_L1-Perf]",969100000,"revised","2016-11-04T01:34:57.927","2016-11-04T15:02:33.500","","R4-1610685","Rel-13","36.101","13.5.0","LTE_MTCe2_L1-Perf","4045","","F","","","","","",""]
["R4-1609692","Finalizing UE-selected subband CQI test for eMTC","Ericsson","Kazuyoshi Uesaka","46968","CR","Approval","This CR finalizes the UE-selected subband CQI test for eMTC.","","100","6.1.3","UE CSI reporting (36.101) [LTE_MTCe2_L1-Perf]",969200000,"revised","2016-11-04T01:34:58.003","2016-11-19T17:47:25.863","","R4-1611017","Rel-14","36.101","14.1.0","LTE_MTCe2_L1-Perf","4046","","A","","","","","",""]
["R4-1609693","Discussion on REFSENS RMC table for Cat-M1 UE","Ericsson","Kazuyoshi Uesaka","46968","discussion","Discussion","This contribution discusses the scheduling for REFSENS test for Cat-M1 UE.","","45","5.5.1","UE RF (36.101)  [LTE_MTCe2_L1-Core]",924000000,"noted","2016-11-04T01:34:58.097","2016-11-04T15:02:33.500","","","Rel-13","","","LTE_MTCe2_L1-Core","","","","","","","","",""]
["R4-1609694","Correction of REFSENS RMC table for Cat-M1 UE","Ericsson","Kazuyoshi Uesaka","46968","CR","Approval","This CR corrects the RMC table for eMTC REFSENS test.","","45","5.5.1","UE RF (36.101)  [LTE_MTCe2_L1-Core]",939200000,"revised","2016-11-04T01:34:58.130","2016-11-04T15:02:33.517","","R4-1610849","Rel-13","36.101","13.5.0","LTE_MTCe2_L1-Core","4047","","F","","","","","",""]
["R4-1609695","Correction of REFSENS RMC table for Cat-M1 UE","Ericsson, Anritsu","Kazuyoshi Uesaka","46968","CR","Approval","This CR corrects the RMC table for eMTC REFSENS test.","","45","5.5.1","UE RF (36.101)  [LTE_MTCe2_L1-Core]",939300000,"agreed","2016-11-04T01:34:58.207","2016-11-22T12:17:27.033","","","Rel-14","36.101","14.1.0","LTE_MTCe2_L1-Core","4048","","A","RP-162430","","","","",""]
["R4-1609696","Simulation result of MIB-BR/SIB1-BR/SIB2 acquisition time","Ericsson","Kazuyoshi Uesaka","46968","discussion","Discussion","This contribution provides the simulation results for MIB and SIB acquisition times.","","48","5.5.3.1","Evaluation of MIB and SIB reading delay, and update of requirement for handover and RRC Re-establishment [LTE_MTCe2_L1-Core]",51000,"noted","2016-11-04T01:34:58.300","2016-11-04T15:02:33.517","","","Rel-13","","","LTE_MTCe2_L1-Core","","","","","","","","",""]
["R4-1609697","Simulation result of RLM with Cat-M1 CE Mode B","Ericsson","Kazuyoshi Uesaka","46968","discussion","Discussion","This contribution provides the simulation results for RLM with Cat-M1 CE Mode B.","","93","6.1.1.3.7","RLM  [LTE_MTCe2_L1-Perf]",927900000,"noted","2016-11-04T01:34:58.317","2016-11-04T15:02:33.517","","","Rel-13","","","LTE_MTCe2_L1-Perf","","","","","","","","",""]
["R4-1609698","Discussion on the demodulation requirements for single Rx Cat-1 UE","Ericsson","Kazuyoshi Uesaka","46968","discussion","Discussion","This contribution discusses the demodulation requirements for the single Rx Cat-1 UE.","","336","8.27.5","UE demodulation (36.101) [LTE_UE_cat_1RX-Perf]",945300000,"noted","2016-11-04T01:34:58.347","2016-11-04T15:02:33.530","","","Rel-14","","","LTE_UE_cat_1RX-Perf","","","","","","","","",""]
["R4-1609699","Simulation assumption for CQI tests for Cat.1 UE with single receiver chain","Qualcomm Incorporated","Jaeho Ryu","47148","other","Approval","This documents summarizes simulation assumption for CQI tests for Cat.1 UE with single receiver chain.","","337","8.27.6","UE CSI (36.101) [LTE_UE_cat_1RX-Perf]",970000000,"approved","2016-11-04T01:38:46.187","2016-11-04T20:39:12.163","","","","","","","","","","","","","","",""]
["R4-1609700","CQI tests for Cat.1 UE with single receiver chain","Qualcomm Incorporated","Jaeho Ryu","47148","other","Discussion","In this contribution, we provide our view on open issues on CQI tests for Cat.1 UE with single receiver chain.","","337","8.27.6","UE CSI (36.101) [LTE_UE_cat_1RX-Perf]",969900000,"noted","2016-11-04T01:38:46.200","2016-11-04T20:39:12.163","","","","","","","","","","","","","","",""]
["R4-1609701","Simulation assumption for demodulation tests for Cat.1 UE with single receiver chain","Qualcomm Incorporated","Jaeho Ryu","47148","other","Approval","This documents summarizes simulation assumption for demodulation tests for Cat.1 UE with single receiver chain.","","336","8.27.5","UE demodulation (36.101) [LTE_UE_cat_1RX-Perf]",970200000,"approved","2016-11-04T01:38:46.217","2016-11-04T20:39:12.163","","","","","","","","","","","","","","",""]
["R4-1609702","Demodulation tests for Cat.1 UE with single receiver chain","Qualcomm Incorporated","Jaeho Ryu","47148","other","Discussion","In this contribution, we provide our view on open issues on demodulation performance requirements for Cat.1 UE with single receiver chain.","","336","8.27.5","UE demodulation (36.101) [LTE_UE_cat_1RX-Perf]",907200000,"noted","2016-11-04T01:38:46.247","2016-11-04T20:39:12.177","","","","","","","","","","","","","","",""]
["R4-1609703","Further discussion on RRM core requirements for Cat.1 UE with single receiver chain","Qualcomm Incorporated","Jaeho Ryu","47148","other","Discussion","In this contribution, we will provide further analyses on open issues in RRM core requirements for Cat.1 UE with single receiver chain.","","334","8.27.3","RRM core (36.133) [LTE_UE_cat_1RX-Core]",42000,"noted","2016-11-04T01:38:46.263","2016-11-04T20:39:12.177","","","","","","","","","","","","","","",""]
["R4-1609704","Simulation assumption for RSTD measurement accuracy for Cat.1 UE with single receiver chain","Qualcomm Incorporated","Jaeho Ryu","47148","other","Approval","This documents summarizes simulation assumption for RSTD measurement accuracy for Cat.1 UE with single receiver chain.","","335","8.27.4","RRM performance (36.133) [LTE_UE_cat_1RX-Perf]",970400000,"approved","2016-11-04T01:38:46.280","2016-11-04T20:39:12.177","","R4-1610729","","","","","","","","","","","","",""]
["R4-1609705","CR for rank 4 CA SDR tests with CA","Qualcomm Incorporated","Jaeho Ryu","47148","CR","Approval","Modify rank 4 CA SDR tests in a generic way to cover all possible UE implementation.","","363","8.30.3.6","SDR test [LTE_4Rx_AP_DL_CA-Perf]",970500000,"endorsed","2016-11-04T01:38:46.297","2016-11-04T20:39:12.177","","","Rel-14","36.101","14.1.0","LTE_4Rx_AP_DL_CA-Perf","4049","","F","","","","","",""]
["R4-1609706","Control channel performance of enhanced CRS-IM receiver UE","Qualcomm Incorporated","Jaeho Ryu","47148","other","Discussion","In this contribution, we provide simulation results for PDCCH based on WF and our view on performance benefits and feasibility of enhanced CRS-IM receiver for control channel.","","367","8.31.2.1","Performance evaluation: scenarios and receiver [LTE_eCRSIM_eSUMIMO]",970700000,"noted","2016-11-04T01:38:46.387","2016-11-04T20:39:12.193","","","","","","","","","","","","","","",""]
["R4-1609707","PDSCH demodulation performance of enhanced CRS-IM receiver UE","Qualcomm Incorporated","Jaeho Ryu","47148","other","Discussion","In this contribution, we provide simulation results for PDSCH based on WF and our view on performance benefits and feasibility of enhanced CRS-IM receiver.","","367","8.31.2.1","Performance evaluation: scenarios and receiver [LTE_eCRSIM_eSUMIMO]",909000000,"noted","2016-11-04T01:38:46.403","2016-11-04T20:39:12.193","","","","","","","","","","","","","","",""]
["R4-1609708","On performance requirements for Rel-14 eLAA","Qualcomm Incorporated","Jaeho Ryu","47148","other","Discussion","In this contribution, we will review key aspect of eLAA design to support UL carrier aggregation for LAA SCell and provide our view on UE and BS performance requirements.","","257","8.18.6","UE/BS demodulation and CSI (36.101/36.104) [LTE_eLAA-Perf]",917900000,"noted","2016-11-04T01:38:46.437","2016-11-04T20:39:12.193","","","","","","","","","","","","","","",""]
["R4-1609709","PDSCH demodulation performance of enhanced SU-MIMO receiver UE","Qualcomm Incorporated","Jaeho Ryu","47148","other","Discussion","In this contribution, we provide simulation results based on WF and our view on performance benefits and feasibility of enhanced SU-MIMO receiver.","","370","8.31.3.1","Performance evaluation: scenarios and receiver [LTE_eCRSIM_eSUMIMO]",948300000,"noted","2016-11-04T01:38:46.450","2016-11-04T20:39:12.210","","","","","","","","","","","","","","",""]
["R4-1609710","Aperiodic CSI report triggering in LAA CQI test","Qualcomm Incorporated","Jaeho Ryu","47148","other","Discussion","In this contribution, we provide our view on how to configure aperiodic CSI reporting in LAA CQI test based on RAN1 specification change.","","110","6.2.5","UE CSI reporting (36.101) [LTE_LAA-Perf]",917000000,"noted","2016-11-04T01:38:46.467","2016-11-04T20:39:12.210","","","","","","","","","","","","","","",""]
["R4-1609711","LAA performance requirements with multiple LAA Scells","Qualcomm Incorporated","Jaeho Ryu","47148","other","Discussion","In this contribution, we provide our view on high level framework for LAA performance requirements with multiple LAA SCells.","","107","6.2.4.1","General [LTE_LAA-Perf]",916900000,"noted","2016-11-04T01:38:46.483","2016-11-04T20:39:12.210","","","","","","","","","","","","","","",""]
["R4-1609712","Test framework for CA MMSE-IRC test","Qualcomm Incorporated","Jaeho Ryu","47148","other","Discussion","In this contribution, we provide our view on open issues on general test framework for MMSE-IRC test for CA.","","360","8.30.3.3","Extend MMSE-IRC requirement from 2Rx to 4Rx [LTE_4Rx_AP_DL_CA-Perf]",1000000000,"noted","2016-11-04T01:38:46.497","2016-11-04T20:39:12.210","","","","","","","","","","","","","","",""]
["R4-1609713","CA demodulation test for 4 Rx UE","Qualcomm Incorporated","Jaeho Ryu","47148","other","Discussion","In this contribution, we provide initial simulation results for TM4 and TM9 demodulation test and our view on other WI objectives for CA demodulation test.","","358","8.30.3.1","Applicability [LTE_4Rx_AP_DL_CA-Perf]",999700000,"noted","2016-11-04T01:38:46.513","2016-11-04T20:39:12.223","","","","","","","","","","","","","","",""]
["R4-1609714","TM9 MU-MIMO demodulation test with channel output duplication","Qualcomm Incorporated","Jaeho Ryu","47148","other","Discussion","In this contribution, we provide simulation results based on WF and propose a solution to the issue raised in [2].","","33","5.2.3.2","UE demodulation and CSI [LTE_4Rx_AP_DL-Perf]",974400000,"noted","2016-11-04T01:38:46.543","2016-11-04T20:39:12.223","","","","","","","","","","","","","","",""]
["R4-1609715","Correction to interfering signal for Narrowband blocking requirement for NB-IOT (Rel-13)","ZTE, ZTE Microelectronics","Zhifeng Ma","61569","CR","","The position of interfering signal for Narrowband blocking requirement for NB-IOT should be corrected","","55","5.6.3","BS RF (36.104) [NB_IOT-Core]",9715000,"agreed","2016-11-04T01:48:44.307","2016-11-04T06:00:00.133","","","Rel-13","36.104","13.5.0","NB_IOT-Core","0899","","F","RP-162433","","","","",""]
["R4-1609716","Correction to interfering signal for Narrowband blocking requirement for NB-IOT (Rel-14)","ZTE, ZTE Microelectronics","Zhifeng Ma","61569","CR","","The position of interfering signal for Narrowband blocking requirement for NB-IOT should be corrected","","55","5.6.3","BS RF (36.104) [NB_IOT-Core]",9716000,"agreed","2016-11-04T01:59:49.817","2016-11-19T17:47:25.863","","","Rel-14","36.104","14.1.0","NB_IOT-Core","0900","","A","RP-162433","","","","",""]
["R4-1609717","TR 36.714-03-01: 3DL/1UL inter-band CA R14 v0.5.0","Huawei, HiSilicon","Huiping Shan","56652","draft TR","Approval","3DL/1UL TR v0.5.0","","158","8.3.1","Rapporteur Input (WID/CRs) [LTE_CA_R14_3DL1UL-Core]",971700000,"approved","2016-11-04T02:12:49.427","2016-11-04T08:49:51.117","","","Rel-14","36.714-03-01","0.5.0","LTE_CA_R14_3DL1UL-Core","","","","","","","","",""]
["R4-1609718","Revised WID: 3DL 1UL basket WI","Huawei, HiSilicon","Huiping Shan","56652","WID revised","Endorsement","3DL/1UL WID revision","","158","8.3.1","Rapporteur Input (WID/CRs) [LTE_CA_R14_3DL1UL-Core]",972100000,"endorsed","2016-11-04T02:12:51.487","2016-11-19T17:47:25.880","","","Rel-14","","","LTE_CA_R14_3DL1UL-Core","","","","","","","","",""]
["R4-1609719","Introduction of completed R14 3DL band combinations to TS 36.101","Huawei, HiSilicon","Huiping Shan","56652","CR","Agreement","Big CR for 3DL/1UL","","158","8.3.1","Rapporteur Input (WID/CRs) [LTE_CA_R14_3DL1UL-Core]",971800000,"agreed","2016-11-04T02:12:51.500","2016-11-19T17:47:25.897","","","Rel-14","36.101","14.1.0","LTE_CA_R14_3DL1UL-Core","4050","","B","RP-162400","","","","",""]
["R4-1609720","Introduction of completed R14 3DL band combinations to TS 36.104","Huawei, HiSilicon","Huiping Shan","56652","CR","Agreement","Big CR for 3DL/1UL","","158","8.3.1","Rapporteur Input (WID/CRs) [LTE_CA_R14_3DL1UL-Core]",971900000,"agreed","2016-11-04T02:12:51.610","2016-11-19T17:47:25.897","","","Rel-14","36.104","14.1.0","LTE_CA_R14_3DL1UL-Core","0901","","B","RP-162400","","","","",""]
["R4-1609721","Introduction of completed R14 3DL band combinations to TS 36.141","Huawei, HiSilicon","Huiping Shan","56652","CR","Agreement","Big CR for 3DL/1UL","","158","8.3.1","Rapporteur Input (WID/CRs) [LTE_CA_R14_3DL1UL-Core]",972000000,"agreed","2016-11-04T02:12:51.720","2016-11-19T17:47:25.910","","","Rel-14","36.141","14.1.0","LTE_CA_R14_3DL1UL-Core","0934","","B","RP-162400","","","","",""]
["R4-1609722","mmWave UE MOP consideration","Huawei, HiSilicon","Huiping Shan","56652","discussion","Discussion","This contribution privides the consideration of mmWave ouput power requirement and test.","","417","11.5.2.1","Transmitter characteristics [FS_NR_newRAT]",959200000,"noted","2016-11-04T02:12:51.797","2016-11-04T08:49:50.443","","","Rel-14","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1609723","mmWave UE REFSENS consideration","Huawei, HiSilicon","Huiping Shan","56652","discussion","Discussion","This contribution privides the consideration of mmWave REFSENS requirement and test.","","418","11.5.2.2","Receiver characteristics [FS_NR_newRAT]",964900,"noted","2016-11-04T02:12:51.813","2016-11-04T08:49:50.443","","","Rel-14","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1609724","Discussion on release independent of performance enhancement for HST","CMCC","jingjing chen","59689","discussion","Discussion","---","","339","8.28.1","General [LTE_high_speed]",972400000,"noted","2016-11-04T02:19:01.800","2016-11-04T09:52:12.713","","","","","","","","","","","","","","",""]
["R4-1609725","Draft reply LS on NB-IoT RRC Re-establishment test configurations","CMCC","jingjing chen","59689","LS out","Approval","---","","121","6.3.3.4","RRC Re-establishment test [NB_IOT-Perf]",1700,"revised","2016-11-04T02:19:01.860","2016-11-04T09:52:12.713","","R4-1610810","","","","","","","","","","","","",""]
["R4-1609726","Discussion on side lobe suppression ratio defining for 5G","CMCC","jingjing chen","59689","discussion","Discussion","---","","421","11.5.3.1","Transmitter characteristics [FS_NR_newRAT]",966000000,"noted","2016-11-04T02:19:01.923","2016-11-04T12:42:26.970","","","Rel-14","","","","","","","","","","","",""]
["R4-1609727","Considerations on ACLR OTA testability for 5G NR above 6GHz","CMCC","jingjing chen","59689","discussion","Discussion","---","","423","11.5.3.3","Testability [FS_NR_newRAT]",972700000,"noted","2016-11-04T02:19:01.970","2016-11-04T12:42:26.970","","","Rel-14","","","","","","","","","","","",""]
["R4-1609728","Unwanted emission requirements associated with beam steering","NTT DOCOMO, INC.","Suguru Okuyama","61038","other","Approval","---","","209","8.12.2.1","In band requirements [AASenh_BS_LTE_UTRA]",3880000,"noted","2016-11-04T02:19:44.637","2016-11-04T09:45:25.553","","","Rel-14","37.105","","AASenh_BS_LTE_UTRA","","","","","","","","",""]
["R4-1609729","Consideration on reducing the measurement point for TRP ALCR","NTT DOCOMO, INC.","Suguru Okuyama","61038","other","Approval","---","","209","8.12.2.1","In band requirements [AASenh_BS_LTE_UTRA]",3900000,"noted","2016-11-04T02:19:44.653","2016-11-04T09:45:25.567","","","Rel-14","37.105","","AASenh_BS_LTE_UTRA","","","","","","","","",""]
["R4-1609730","How to specify OTA OBUE and spurious emission requirement for eAAS","NTT DOCOMO, INC.","Suguru Okuyama","61038","other","Approval","---","","209","8.12.2.1","In band requirements [AASenh_BS_LTE_UTRA]",3620000,"noted","2016-11-04T02:19:44.667","2016-11-04T09:45:25.567","","","Rel-14","37.105","","AASenh_BS_LTE_UTRA","","","","","","","","",""]
["R4-1609731","OTA requirements compliance range","NTT DOCOMO, INC.","Suguru Okuyama","61038","other","Approval","---","","209","8.12.2.1","In band requirements [AASenh_BS_LTE_UTRA]",80100,"noted","2016-11-04T02:19:44.700","2016-11-04T09:45:25.567","","","Rel-14","37.105","","AASenh_BS_LTE_UTRA","","","","","","","","",""]
["R4-1609732","Discussion of NR specific new requirements","NTT DOCOMO, INC.","Suguru Okuyama","61038","other","Approval","---","","420","11.5.3","BS RF  [FS_NR_newRAT]",973600000,"noted","2016-11-04T02:19:44.713","2016-11-04T09:45:25.897","","","Rel-14","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1609733","Necessity of conducted requirements for below 6GHz","NTT DOCOMO, INC.","Suguru Okuyama","61038","other","Approval","---","","420","11.5.3","BS RF  [FS_NR_newRAT]",994100000,"noted","2016-11-04T02:19:44.730","2016-11-04T09:45:25.897","","","Rel-14","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1609734","Metric on NR BS Output power (for accuracy and other perspectives)","NTT DOCOMO, INC.","Suguru Okuyama","61038","other","Approval","---","","421","11.5.3.1","Transmitter characteristics [FS_NR_newRAT]",94180000,"noted","2016-11-04T02:19:44.747","2016-11-04T09:45:25.897","","","Rel-14","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1609735","ACLR requirement associated with beam steering","NTT DOCOMO, INC.","Suguru Okuyama","61038","other","Approval","---","","421","11.5.3.1","Transmitter characteristics [FS_NR_newRAT]",972600000,"noted","2016-11-04T02:19:44.760","2016-11-04T09:45:25.913","","","Rel-14","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1609736","NR BS requirements for multiple beam capable BS","NTT DOCOMO, INC.","Suguru Okuyama","61038","other","Approval","---","","420","11.5.3","BS RF  [FS_NR_newRAT]",985700000,"noted","2016-11-04T02:19:44.793","2016-11-04T09:45:25.913","","","Rel-14","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1609737","Necessity of EVM and in-band emission and its testability for NR BS","NTT DOCOMO, INC.","Suguru Okuyama","61038","other","Approval","---","","415","11.5.1","Common issues for UE and BS [FS_NR_newRAT]",92190000,"noted","2016-11-04T02:19:44.807","2016-11-04T09:45:25.927","","","Rel-14","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1609738","Add Narrowband blocking requirement for NB-IOT in TS36.141(Rel-13)","ZTE, ZTE Microelectronics","Zhifeng Ma","61569","CR","","The Narrowband blocking requirement for NB-IOT should be added.","","116","6.3.2.3","Receiver characteristics  [NB_IOT-Perf]",973800000,"noted","2016-11-04T02:24:27.947","2016-11-04T06:00:00.133","","","Rel-13","36.141","13.5.0","NB_IOT-Perf","0935","","F","","","","","",""]
["R4-1609739","Add Narrowband blocking requirement for NB-IOT in TS36.141(Rel-14)","ZTE, ZTE Microelectronics","Zhifeng Ma","61569","CR","","The Narrowband blocking requirement for NB-IOT should be added.","","116","6.3.2.3","Receiver characteristics  [NB_IOT-Perf]",973900000,"withdrawn","2016-11-04T02:35:10.043",null,"","","Rel-14","36.141","14.1.0","","0936","","A","","","","","",""]
["R4-1609740","TR 36.752 Study of NB-IoT RF requirement for coexistence with CDMA v0.1.0","China Telecom","Dong Zhao","46407","draft TR","Approval","This presents to RAN4, for approval, the updated version of TR 36.752 incorporating the approved TPs from RAN4#80Bis meeting.","","389","9.3","Study on NB-IoT RF requirement for coexistence with CDMA [FS_NB_IOT_CDMA_coex]",84600,"approved","2016-11-04T02:43:21.477","2016-11-04T10:42:00.427","","","Rel-14","36.752","0.1.0","FS_NB_IOT_CDMA_coex","","","","","","","","",""]
["R4-1609741","Summary of coexistence results","China Telecom","Dong Zhao","46407","discussion","Discussion","Table for simulation results collection.","","392","9.3.3","Co-existence study [FS_NB_IOT_CDMA_coex]",974200000,"revised","2016-11-04T02:47:47.907","2016-11-04T10:42:00.427","","R4-1610841","","","","FS_NB_IOT_CDMA_coex","","","","","","","","",""]
["R4-1609742","TP for 36.752 coexistence simulation results","China Telecom","Dong Zhao","46407","pCR","Approval","This contribution provides a text proposal on summary of simulatoin results for the TR36.752.","","392","9.3.3","Co-existence study [FS_NB_IOT_CDMA_coex]",982000000,"revised","2016-11-04T02:53:21.530","2016-11-04T10:42:00.427","","R4-1610842","","36.752","0.1.0","FS_NB_IOT_CDMA_coex","","","","","","","","",""]
["R4-1609743","Operating band for single Rx Category 1","China Telecom","Dong Zhao","46407","discussion","Approval","This document intends to propose new operating bands for single Rx Category 1.","","331","8.27.2","UE RF (36.101) [LTE_UE_cat_1RX-Core]",186000,"approved","2016-11-04T02:58:12.377","2016-11-04T10:42:00.440","","","","","","LTE_UE_cat_1RX","","","","","","","","",""]
["R4-1609744","Simulation results for TM2 IRC test on 4Rx","ZTE, ZTE Microelectronics","Qian Yang","45032","discussion","Discussion","In this contribution, we update the simulation results for 4Rx TM2 IRC demodulation with one interference cell.","","33","5.2.3.2","UE demodulation and CSI [LTE_4Rx_AP_DL-Perf]",906600001,"noted","2016-11-04T03:22:33.660","2016-11-04T13:00:21.840","","","Rel-13","","","LTE_4Rx_AP_DL-Perf","","","","","","","","",""]
["R4-1609745","Simulation results for SFN demodulation on HST","ZTE, ZTE Microelectronics","Qian Yang","45032","discussion","Discussion","In this contribution, we provide the simulation results for SFN demodulation on high speed scenario.","","345","8.28.3.1","Enhancement for bi-directional RRH arrangement [LTE_high_speed]",974500000,"noted","2016-11-04T03:22:33.673","2016-11-04T13:00:21.857","","","Rel-14","","","LTE_high_speed","","","","","","","","",""]
["R4-1609746","PDSCH demodulation on enhanced CRS-IM","ZTE, ZTE Microelectronics","Qian Yang","45032","discussion","Discussion","In this contribution, we provide the simulation results and proposals for PDSCH demodulation on enhanced CRS-IM.","","367","8.31.2.1","Performance evaluation: scenarios and receiver [LTE_eCRSIM_eSUMIMO]",909100000,"noted","2016-11-04T03:22:33.690","2016-11-04T13:00:21.857","","","Rel-14","","","LTE_eCRSIM_eSUMIMO","","","","","","","","",""]
["R4-1609747","Control channel demodulation on enhanced CRS-IM","ZTE, ZTE Microelectronics","Qian Yang","45032","discussion","Discussion","In this contribution, we provide the simulation results and proposals for eCRS-IM control channel demodulation","","367","8.31.2.1","Performance evaluation: scenarios and receiver [LTE_eCRSIM_eSUMIMO]",974700000,"noted","2016-11-04T03:22:33.707","2016-11-04T13:00:21.870","","","Rel-14","","","LTE_eCRSIM_eSUMIMO","","","","","","","","",""]
["R4-1609748","Further discussion on requirements for mobility enhancement solutions","ZTE, ZTE Microelectronics","Qian Yang","45032","discussion","Discussion","---","","327","8.26.3","RRM core (36.133) [LTE_eMob-Core]",69200000,"noted","2016-11-04T03:22:33.720","2016-11-04T13:00:21.887","","","Rel-14","","","LTE_eMob-Core","","","","","","","","",""]
["R4-1609749","CR to introduce handover requirements for mobility enhancement_R14","ZTE, ZTE Microelectronics","Qian Yang","45032","CR","Agreement","---","","327","8.26.3","RRM core (36.133) [LTE_eMob-Core]",974900000,"revised","2016-11-04T03:22:33.753","2016-11-04T13:00:21.887","","R4-1610857","Rel-14","36.133","14.1.0","LTE_eMob-Core","4228","","B","","","","","",""]
["R4-1609750","Support of FS3-only TAGs","Nokia, Alcatel-Lucent Shanghai Bell","Riikka Nurminen","70015","discussion","Discussion","Discussion on FS3-cell only sTAG support in eLAA.","","255","8.18.4.3","Others [LTE_eLAA-Core]",3360000,"noted","2016-11-04T03:34:38.513","2016-11-04T19:02:22.717","","","","","","","","","","","","","","",""]
["R4-1609751","Draft LS Response on Timing Reference for LAA SCell","Nokia, Alcatel-Lucent Shanghai Bell","Riikka Nurminen","70015","LS out","Approval","Draft LS response to RAN2 about LAA Scell reliability as TA reference.","","255","8.18.4.3","Others [LTE_eLAA-Core]",33700000,"noted","2016-11-04T03:34:38.543","2016-11-04T19:02:22.733","","","","","","","","","","","","","","",""]
["R4-1609752","RRM requirements and scaling","Nokia, Alcatel-Lucent Shanghai Bell","Riikka Nurminen","70015","discussion","Discussion","Discussion on scaling the LAA RRM requirements.","","253","8.18.4.1","Measurement with multiple cells [LTE_eLAA-Core]",975200000,"noted","2016-11-04T03:34:38.560","2016-11-04T19:02:22.670","","","","","","","","","","","","","","",""]
["R4-1609753","On eLAA BS demodulation","Nokia, Alcatel-Lucent Shanghai Bell","Riikka Nurminen","70015","discussion","Discussion","Initial discussion on simulation assumptions for eLAA PUSCH.","","257","8.18.6","UE/BS demodulation and CSI (36.101/36.104) [LTE_eLAA-Perf]",942300000,"noted","2016-11-04T03:34:38.577","2016-11-04T19:02:22.687","","","","","","","","","","","","","","",""]
["R4-1609754","On shortened TTI RRM impacts","Nokia, Alcatel-Lucent Shanghai Bell","Riikka Nurminen","70015","discussion","Discussion","Discussion on possible RRM impacts due to RAN1 agreements on short TTI.","","405","10.1.4","RRM core (36.133)  [LTE_sTTIandPT]",955800000,"noted","2016-11-04T03:34:38.653","2016-11-04T19:02:22.703","","","","","","","","","","","","","","",""]
["R4-1609755","SNR and Noise-Figures of phased-array receivers","Qualcomm Incorporated","Raju Hormis","67308","SID new","Discussion","---","","418","11.5.2.2","Receiver characteristics [FS_NR_newRAT]",986900000,"withdrawn","2016-11-04T04:07:54.470",null,"","","","","","","","","","","","","","",""]
["R4-1609756","Out-of-band blockers in the mm-wave spectrum","Qualcomm Incorporated","Raju Hormis","67308","SID new","Discussion","Millimeter wave blockers (or jammers) will have significant impact on transceiver design and network performance at mm-wave bands. This paper is preliminary data that lists the major sources of blocking in the United States.","","418","11.5.2.2","Receiver characteristics [FS_NR_newRAT]",980800000,"noted","2016-11-04T04:13:18.327","2016-11-07T15:40:32.667","","","","","","","","","","","","","","",""]
["R4-1609757","Discussion on demodulation performance for enhanced CRS-IM","LG Electronics Inc.","Jin-yup Hwang","47026","discussion","Discussion","---","","367","8.31.2.1","Performance evaluation: scenarios and receiver [LTE_eCRSIM_eSUMIMO]",71800000,"noted","2016-11-04T04:38:06.147","2016-11-04T09:00:29.187","","","","","","","","","","","","","","",""]
["R4-1609758","Discussion on feasibility test scenarios and reference receiver for enhanced SU-MIMO","LG Electronics Inc.","Jin-yup Hwang","47026","discussion","Discussion","---","","370","8.31.3.1","Performance evaluation: scenarios and receiver [LTE_eCRSIM_eSUMIMO]",909200000,"noted","2016-11-04T04:39:27.920","2016-11-04T09:00:29.453","","","","","","","","","","","","","","",""]
["R4-1609759","Discussion on performance and complexity for RML receiver","LG Electronics Inc.","Jin-yup Hwang","47026","discussion","Discussion","---","","370","8.31.3.1","Performance evaluation: scenarios and receiver [LTE_eCRSIM_eSUMIMO]",909300000,"noted","2016-11-04T04:40:16.077","2016-11-04T09:00:29.467","","","","","","","","","","","","","","",""]
["R4-1609760","Update simulation results for LAA demodulation performance","LG Electronics Inc.","Jin-yup Hwang","47026","discussion","Discussion","---","","108","6.2.4.2","PDSCH [LTE_LAA-Perf]",64200000,"noted","2016-11-04T04:41:03.330","2016-11-04T08:10:17.980","","","","","","","","","","","","","","",""]
["R4-1609761","Discussion about single-link demodulation requirements for Rel-14 V2V","LG Electronics Inc.","Jin-yup Hwang","47026","discussion","Discussion","---","","269","8.19.4.1","Single-link PSSCH and PSCCH  [LTE_SL_V2V-Perf]",42900000,"revised","2016-11-04T04:41:59.707","2016-11-04T09:00:29.483","","R4-1610708","","","","","","","","","","","","",""]
["R4-1609762","Discussion about multi-link demodulation requirements for Rel-14 V2V","LG Electronics Inc.","Jin-yup Hwang","47026","discussion","Discussion","---","","270","8.19.4.2","Multi-link PSSCH and PSCCH [LTE_SL_V2V-Perf]",947800000,"noted","2016-11-04T04:42:49.287","2016-11-04T09:00:29.483","","","","","","","","","","","","","","",""]
["R4-1609763","Discussion about maximum process tests for Rel-14 V2V","LG Electronics Inc.","Jin-yup Hwang","47026","discussion","Discussion","---","","271","8.19.4.3","Maximum process test [LTE_SL_V2V-Perf]",947900000,"noted","2016-11-04T04:43:33.807","2016-11-04T09:00:29.497","","","","","","","","","","","","","","",""]
["R4-1609764","Simulation results for PDSCH with IRC TM2/3/3 test with 4Rx","LG Electronics Inc.","Jin-yup Hwang","47026","discussion","Discussion","---","","33","5.2.3.2","UE demodulation and CSI [LTE_4Rx_AP_DL-Perf]",906700000,"noted","2016-11-04T04:44:29.517","2016-11-04T09:00:29.513","","","","","","","","","","","","","","",""]
["R4-1609765","CR on reliability of GNSS","LG Electronics Inc.","YOONOH YANG","47033","CR","Approval","It is CR to add reliability of GNSS in UE transmision timing.","","264","8.19.2","RRM core maintenance (36.133)  [LTE_SL_V2V-Core]",63600000,"revised","2016-11-04T04:48:57.133","2016-11-04T06:52:48.057","","R4-1610636","Rel-14","36.133","14.1.0","","4229","","F","","","","","",""]
["R4-1609766","CR on UE transmission timing accuracy test","LG Electronics Inc.","YOONOH YANG","47033","CR","Approval","It is CR of test case for UE transmission timining accuracy.","","266","8.19.3.1","UE transmission timing accuracy test [LTE_SL_V2V-Perf]",976600000,"noted","2016-11-04T04:51:57.127","2016-11-04T06:52:48.073","","","Rel-14","36.133","14.1.0","","4230","","B","","","","","",""]
["R4-1609767","UE transmission timing for V2X","LG Electronics Inc.","YOONOH YANG","47033","discussion","Discussion","It discusses NTA,offset and TE for SyncRefUE .","","281","8.20.4.1","UE Transmit timing [LTE_V2X-Core]",960000,"noted","2016-11-04T04:54:12.737","2016-11-04T06:52:48.090","","","Rel-14","36.133","","","","","","","","","","",""]
["R4-1609768","Initiation or Cease of SLSS transmission","LG Electronics Inc.","YOONOH YANG","47033","discussion","Discussion","It discusses initiation/cease of SLSS transmission.","","283","8.20.4.3","Initiation/cease of SLSS requirement [LTE_V2X-Core]",951400000,"noted","2016-11-04T04:55:37.477","2016-11-04T06:52:48.090","","","Rel-14","36.133","","","","","","","","","","",""]
["R4-1609769","SLSS detection requirement","LG Electronics Inc.","YOONOH YANG","47033","discussion","Discussion","It discusses SLSS detection requirement based on simulation result and agreed WF.","","284","8.20.4.4","Requirements related to synchronization [LTE_V2X-Core]",1730000,"noted","2016-11-04T05:00:24.063","2016-11-04T06:52:48.103","","","Rel-14","36.133","","","","","","","","","","",""]
["R4-1609770","Interruption for V2X","LG Electronics Inc.","YOONOH YANG","47033","discussion","Discussion","It  discusses interruption of V2X based on agreements of RAN4 and RAN1.","","282","8.20.4.2","Interruption [LTE_V2X-Core]",1740000,"noted","2016-11-04T05:03:31.687","2016-11-04T06:52:48.103","","","Rel-14","36.133","","","","","","","","","","",""]
["R4-1609771","Cell detection requirements in OoC","LG Electronics Inc.","YOONOH YANG","47033","discussion","Discussion","It discusses cell detection in OoC for V-UE.","","284","8.20.4.4","Requirements related to synchronization [LTE_V2X-Core]",24200000,"noted","2016-11-04T05:04:51.290","2016-11-04T06:52:48.103","","","Rel-14","","","","","","","","","","","",""]
["R4-1609772","Measurement accuracy for PSSCH-RSRP and S-RSSI","LG Electronics Inc.","YOONOH YANG","47033","discussion","Discussion","It discusses measurement accuracy of PSSCH-RSRP based on simulation result and S-RSSI based on analysis.","","285","8.20.4.5","Autonomous resource selection/reselection [LTE_V2X-Core]",951200000,"revised","2016-11-04T05:06:16.157","2016-11-04T06:52:48.103","","R4-1610675","Rel-14","","","","","","","","","","","",""]
["R4-1609773","Simulation results for NR coexistence study in Urban Macro scenario","ZTE Corporation","Fei Xue","59676","discussion","","---","","410","11.3.1","Co-existence [FS_NR_newRAT]",15000000,"noted","2016-11-04T05:17:39.863","2016-11-04T10:22:56.087","","","","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1609774","Simulation results for NR coexistence study in dense urban scenario","ZTE Corporation","Fei Xue","59676","discussion","","---","","410","11.3.1","Co-existence [FS_NR_newRAT]",15100000,"noted","2016-11-04T05:19:23.027","2016-11-04T10:22:56.087","","","","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1609775","Simulation results for NR coexistence study in indoor hotspot scenario","ZTE Corporation","Fei Xue","59676","discussion","","---","","410","11.3.1","Co-existence [FS_NR_newRAT]",15200000,"noted","2016-11-04T05:20:40.867","2016-11-04T10:22:56.087","","","","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1609776","Practical simulation results for NPBCH","ZTE Corporation","Fei Xue","59676","discussion","","---","","129","6.3.4.1.1","NPBCH  [NB_IOT-Perf]",55600000,"noted","2016-11-04T05:22:37.927","2016-11-04T10:22:56.087","","","","","","NB_IOT-Perf","","","","","","","","",""]
["R4-1609777","Practical simulation results for NPDCCH","ZTE Corporation","Fei Xue","59676","discussion","","---","","130","6.3.4.1.2","NPDCCH [NB_IOT-Perf]",943100000,"noted","2016-11-04T05:23:42.250","2016-11-04T10:22:56.103","","","","","","NB_IOT-Perf","","","","","","","","",""]
["R4-1609778","Practical Simulation results for NPDSCH","ZTE Corporation","Fei Xue","59676","discussion","","---","","131","6.3.4.1.3","NPDSCH [NB-IOT-Perf]",943300000,"noted","2016-11-04T05:24:58.490","2016-11-04T10:22:56.103","","","","","","NB_IOT-Perf","","","","","","","","",""]
["R4-1609779","Discussion for NR band defining","KT Corporation","ILWHAN KIM","48721","discussion","Discussion","---","","408","11.2","Spectrum  [FS_NR_newRAT]",95100,"revised","2016-11-04T05:26:11.443","2016-11-04T14:20:38.997","","R4-1610159","","","","","","","","","","","","",""]
["R4-1609780","Practical simulation results for NPUSCH Format 1","ZTE Corporation","Fei Xue","59676","discussion","","---","","134","6.3.4.2.2","NPUSCH format 1 [NB_IOT-Perf]",924800000,"noted","2016-11-04T05:26:14.780","2016-11-04T10:22:56.103","","","","","","NB_IOT-Perf","","","","","","","","",""]
["R4-1609781","Practical simulation results for NPUSCH Format 2","ZTE Corporation","Fei Xue","59676","discussion","","---","","135","6.3.4.2.3","NPUSCH format 2 [NB_IOT-Perf]",925200000,"noted","2016-11-04T05:28:18.870","2016-11-04T10:22:56.117","","","","","","NB_IOT-Perf","","","","","","","","",""]
["R4-1609782","Simulation results for RRM measurement for in-band& Guard band NB-IoT","ZTE Corporation","Fei Xue","59676","discussion","","---","","118","6.3.3.1","RRM measurement accuracy [NB_IOT-Perf]",25900000,"noted","2016-11-04T05:29:28.410","2016-11-04T10:22:56.117","","","","","","NB_IOT-Perf","","","","","","","","",""]
["R4-1609783","Updated TR36.714-00-02 v0.5.0","LG Electronics Inc.","Suhwan Lim","46654","draft TR","Approval","This is draft TR 36.714-00-02 v0.5.0 for xDL/2UL inter-band CA","","182","8.7.1","Rapporteur Input (WID/CRs) [LTE_CA_R14_xDL2UL-Core]",978300000,"approved","2016-11-04T05:29:44.587","2016-11-04T07:23:10.590","","","Rel-14","36.714-00-02","0.5.0","LTE_CA_R14_xDL2UL-Core","","","","","","","","",""]
["R4-1609784","Revised WID for xDL/UL inter-band CA with x=3,4,5 in Rel-14","LG Electronics Inc.","Suhwan Lim","46654","WID revised","Approval","This is revised WID for xDL/2UL CA to add new CA band combination and change the status.","","182","8.7.1","Rapporteur Input (WID/CRs) [LTE_CA_R14_xDL2UL-Core]",979400000,"revised","2016-11-04T05:32:55.790","2016-11-04T07:30:33.287","","R4-1610962","Rel-14","36.714-00-02","","LTE_CA_R14_xDL2UL, LTE_CA_R14_xDL2UL-Core, LTE_CA_R14_xDL2UL-Perf","","","","","","","","",""]
["R4-1609785","RAN1 agreement impact on DL Tx EVM requirements","MediaTek Inc.","Tsang-wei Yu","60138","discussion","Discussion","Provide RAN1 agreements, discussion and proposals","","299","8.23","Downlink Multiuser Superposition Transmission [LTE_MUST]",978500000,"noted","2016-11-04T05:33:55.460","2016-11-04T05:39:25.520","","","Rel-14","","","LTE_MUST","","","","","","","","",""]
["R4-1609786","Discussion on SI acquisition time of NB-IoT UE","ZTE Corporation","Fei Xue","59676","discussion","","---","","56","5.6.4","RRM core (36.133)  [NB_IOT-Core]",54800000,"noted","2016-11-04T05:34:22.387","2016-11-04T10:22:56.117","","","","","","NB_IOT-Core","","","","","","","","",""]
["R4-1609787","Discussion on RAN1 agreements","MediaTek Inc.","Tsang-wei Yu","60138","discussion","Discussion","---","","299","8.23","Downlink Multiuser Superposition Transmission [LTE_MUST]",978700000,"available","2016-11-04T05:35:33.847","2016-11-04T05:39:25.520","","","Rel-14","","","LTE_MUST","","","","","","","","",""]
["R4-1609788","MSD test results for xDL/2UL CA with self-desense problems","LG Electronics Inc.","Suhwan Lim","46654","discussion","Approval","In this paper, we propose MSD levels for xDL/2UL CA with self-desense problems.","","183","8.7.2","UE RF (36.101) [LTE_CA_R14_xDL2UL-Core]",930000,"noted","2016-11-04T05:36:12.847","2016-11-04T08:03:05.267","","","Rel-14","36.714-00-02","","LTE_CA_R14_xDL2UL-Core","","","","","","","","",""]
["R4-1609789","CR for Inter-frequency event triggered reporting","MediaTek, Nokia","Chiao-yao Chuang","47023","CR","","---","","105","6.2.3","RRM performance maintenance (36.133)  [LTE_LAA-Perf]",64500000,"agreed","2016-11-04T05:38:37.690","2016-11-04T11:01:28.133","","","Rel-13","36.133","13.5.0","LTE_LAA-Perf","4231","","F","RP-162386","","","","",""]
["R4-1609790","TP on MSD results for xDL/2UL CA with B46","LG Electronics Inc.","Suhwan Lim","46654","pCR","Approval","For xDL/2UL CA with B46, the MSD do not define in TS36.101, RAN4 agreed just add MSD test results in TR36.714-00-02 as information. So we provide the MSD simulation results in TR36.714-00-02","","183","8.7.2","UE RF (36.101) [LTE_CA_R14_xDL2UL-Core]",930100,"revised","2016-11-04T05:40:23.863","2016-11-04T08:02:35.177","","R4-1610771","","36.714-00-02","0.5.0","LTE_CA_R14_xDL2UL-Core","","","","","","","","",""]
["R4-1609791","Introduction of additional 3DL/2UL CA band combinations in Rel-14","LG Electronics, NTT DoCoMo, KT, TELUS, Softbank, LG Uplus, SK Telecom","Suhwan Lim","46654","CR","Approval","In this CR, new 3DL/2UL CA band combinations are introduced in Rel-14.","","182","8.7.1","Rapporteur Input (WID/CRs) [LTE_CA_R14_xDL2UL-Core]",978400000,"agreed","2016-11-04T05:43:22.937","2016-11-19T17:47:25.927","","","Rel-14","36.101","14.1.0","LTE_CA_R14_xDL2UL-Core","4051","","B","RP-162404","","","","",""]
["R4-1609792","CR for Inter-frequency event triggered reporting","MediaTek Inc.","Chiao-yao Chuang","47023","CR","","---","","105","6.2.3","RRM performance maintenance (36.133)  [LTE_LAA-Perf]",978900000,"revised","2016-11-04T05:46:08.607","2016-11-04T11:01:28.133","","R4-1610645","Rel-14","36.133","14.1.0","","4232","","F","","","","","",""]
["R4-1609793","Introduction of additional 4DL/2UL CA band combination in Rel-14","LG Electronics, NTT DoCoMo, LG Uplus, SKT, KT, TELUS, Softbank","Suhwan Lim","46654","CR","Approval","In this CR, new 4DL/2UL CA band combinations are introduced in Rel-14.","","182","8.7.1","Rapporteur Input (WID/CRs) [LTE_CA_R14_xDL2UL-Core]",979100000,"agreed","2016-11-04T05:47:00.820","2016-11-19T17:47:25.943","","","Rel-14","36.101","14.1.0","LTE_CA_R14_xDL2UL-Core","4052","","B","RP-162404","","","","",""]
["R4-1609794","Introduction of additional 5DL/2UL CA band combination in Rel-14","LG Electronics, NTT DoCoMo","Suhwan Lim","46654","CR","Approval","In this CA, new 5DL/2UL CA band combinations are introduced in Rel-14","","182","8.7.1","Rapporteur Input (WID/CRs) [LTE_CA_R14_xDL2UL-Core]",979300000,"agreed","2016-11-04T05:50:03.623","2016-11-19T17:47:25.957","","","Rel-14","36.101","14.1.0","LTE_CA_R14_xDL2UL-Core","4053","","B","RP-162404","","","","",""]
["R4-1609795","Updated TR 36.786 v0.1.0","LG Electronics Inc.","Suhwan Lim","46654","draft TR","Approval","This is updated TR36.786 v0.1.0 to add agreed TP and WF at last RAN4 meeting.","","273","8.20.1","General [LTE_V2X-Core]",27400000,"revised","2016-11-04T05:54:52.643","2016-11-04T07:26:35.403","","R4-1610752","Rel-14","36.786","0.1.0","LTE_V2X-Core","","","","","","","","",""]
["R4-1609796","LTE-based V2X UE Transmitter requirements","LG Electronics Inc.","Suhwan Lim","46654","pCR","Approval","In pthis paper, we provide our views on how to define general TX requirements based on the previous RAN4 agreements to support up to 33dBm high power and multi-carrier operations for LTE-based V2X UE.","","278","8.20.3.1","Tx requirements  [LTE_V2X-Core]",963500000,"revised","2016-11-04T06:00:03.677","2016-11-04T08:06:44.057","","R4-1610757","","36.786","0.1.0","LTE_V2X-Core","","","","","","","","",""]
["R4-1609797","LTE-based V2X UE receiver requirements","LG Electronics Inc.","Suhwan Lim","46654","pCR","Approval","In this paper, we provide our views on how to define general RX requirements to support high power V2X UE and con-current V2X operation.","","279","8.20.3.2","Rx requirements  [LTE_V2X-Core]",979700000,"revised","2016-11-04T06:04:05.023","2016-11-04T08:06:44.043","","R4-1610911","","36.786","0.1.0","LTE_V2X-Core","","","","","","","","",""]
["R4-1609798","WF on V2X RRM requirement","LG Electronics Inc.","YOONOH YANG","47033","discussion","Approval","It is WF for V2X RRM requirement.","","280","8.20.4","RRM core (36.133) (dedicated, shared, or multi-carrier operations) [LTE_V2X-Core]",72100000,"revised","2016-11-04T06:05:59.323","2016-11-04T06:52:48.103","","R4-1610693","","","","","","","","","","","","",""]
["R4-1609799","Comparison of Conducted power between UMTS and LTE","NTT DOCOMO INC.","Takayuki Furuta","58008","other","Discussion","this contribution is for discussion.","","217","8.13.1","General  [LTE_UTRA_TRP_TRS-Core]",78100000,"noted","2016-11-04T06:06:30.213","2016-11-04T08:23:39.337","","","Rel-14","","","","","","","","","","","",""]
["R4-1609800","MPR simulation results for SA/Data FDM transmission and 3dB boosting for V2V UE","LG Electronics Inc.","Suhwan Lim","46654","discussion","Discussion","In this contribution, we provide MPR simulation results to keep the reasonable PAPR and cubic metric levels for FDM transmission with 3dB boosting between PSCCH and PSSCH.","","260","8.19.1.1","MPR/A-MPR [LTE_SL_V2V-Core]",2750000,"noted","2016-11-04T06:09:12.453","2016-11-04T15:05:48.797","","","Rel-14","","","LTE_SL_V2V-Core","","","","","","","","",""]
["R4-1609801","On NR band structure","Huawei, Hisilicon","Xiang (Steven) Chen","41576","discussion","Discussion","---","","408","11.2","Spectrum  [FS_NR_newRAT]",980100000,"noted","2016-11-04T06:09:57.897","2016-11-04T17:54:33.033","","","","","","","","","","","","","","",""]
["R4-1609802","Measurement results of BHH and tablet TRP/TRS for Band 21","NTT DOCOMO INC.","Takayuki Furuta","58008","other","Discussion","This document is for discussion.","","218","8.13.2","Hand phantom for smartphones [LTE_UTRA_TRP_TRS-Core]",51300000,"noted","2016-11-04T06:10:58.627","2016-11-04T08:23:39.337","","","","","","","","","","","","","","",""]
["R4-1609803","A-MPR simulation results to meet European regulation for V2V UE","LG Electronics Inc.","Suhwan Lim","46654","discussion","Discussion","In this contribution, we provide how to define A-MPR requirements based on European regulation for LTE-based V2V UE to cover the remaining issue 2 and 3.","","260","8.19.1.1","MPR/A-MPR [LTE_SL_V2V-Core]",98000000,"noted","2016-11-04T06:12:24.037","2016-11-04T15:05:48.797","","","Rel-14","36.101","","LTE_SL_V2V-Core","","","","","","","","",""]
["R4-1609804","Proposal for BHH LTETRP/TRS requirement","NTT DOCOMO INC.","Takayuki Furuta","58008","other","Approval","This document is for approval.","","218","8.13.2","Hand phantom for smartphones [LTE_UTRA_TRP_TRS-Core]",98020000,"noted","2016-11-04T06:13:50.977","2016-11-04T08:23:39.353","","","Rel-14","","","","","","","","","","","",""]
["R4-1609805","CR on correction of V2X UE RF requirements","LG Electronics Inc.","Suhwan Lim","46654","CR","Approval","This CR is for Cat. F correction for MPR/A-MPR requirements to align the RAN1 final agreement.","","259","8.19.1","UE RF core maintenace (36.101)  [LTE_SL_V2V-Core]",996700000,"agreed","2016-11-04T06:18:09.530","2016-11-19T17:47:25.973","","","Rel-14","36.101","14.1.0","LTE_SL_V2V-Core","4054","","F","RP-162409","","","","",""]
["R4-1609806","Proposal for tablet LTE TRP/TRS requirement","NTT DOCOMO INC.","Takayuki Furuta","58008","other","Approval","this document is for approval.","","220","8.13.4","Free space for LEE devices [LTE_UTRA_TRP_TRS-Core]",78200000,"noted","2016-11-04T06:20:21.693","2016-11-04T08:23:39.353","","R4-1610782","Rel-14","","","","","","","","","","","",""]
["R4-1609807","Adjacent channel coexistence simulation results for V2V service at 2GHz operating frequency with Power control schemes","LG Electronics Inc.","Suhwan Lim","46654","discussion","Discussion","In this paper, we analyze the adjacent channel coexistence for case1 and cse2 at 2GHz licensed band. we simulated using revised simulation assumption to consider power control schemes.","","276","8.20.2.2","Co-existence study for case 1 and case 2  [LTE_V2X-Core]",937600000,"withdrawn","2016-11-04T06:25:05.970",null,"","","Rel-14","36.786","","LTE_V2X-Core","","","","","","","","",""]
["R4-1609808","EIS definition for UE in mmWave","NTT DOCOMO INC.","Takayuki Furuta","58008","other","Approval","This document is for approval","","418","11.5.2.2","Receiver characteristics [FS_NR_newRAT]",52300000,"noted","2016-11-04T06:26:13.473","2016-11-04T09:01:00.357","","","","","","","","","","","","","","",""]
["R4-1609809","Control Commands for NR UE Testability","Anritsu Corporation","Takeshi Kobayashi","66223","discussion","Discussion","---","","419","11.5.2.3","Testability [FS_NR_newRAT]",13100000,"noted","2016-11-04T06:27:40.333","2016-11-04T11:15:03.060","","","","","","","","","","","","","","",""]
["R4-1609810","Inter-frequency measurements in LAA","Qualcomm Incorporated","Valentin Gheorghiu","43117","discussion","Discussion","In this paper we propose some correction to the Rel.13 LAA core requirements","","42","5.4.3","RRM Core [LTE_LAA-Core]",9810000,"noted","2016-11-04T06:33:45.187","2016-11-04T22:35:07.680","","","Rel-13","","","","","","","","","","","",""]
["R4-1609811","Corrections to LAA Measurement Requirements","Qualcomm Incorporated","Valentin Gheorghiu","43117","CR","Approval","This CR corrects the measurement period requirements by introducing scaling that takes into account the fact that measurements cannot be performed in parallel on the serving cell and inter-frequency.","","42","5.4.3","RRM Core [LTE_LAA-Core]",9811000,"noted","2016-11-04T06:38:38.560","2016-11-04T22:35:07.680","","R4-1610871","Rel-13","36.133","13.5.0","LTE_LAA","4233","","F","","","","","",""]
["R4-1609812","CR on NPBCH Fixed Reference Channel for NB-IoT","Intel Corporation","Yang Tang","56725","CR","Agreement","---","","129","6.3.4.1.1","NPBCH  [NB_IOT-Perf]",967200000,"noted","2016-11-04T06:41:47.820","2016-11-07T21:57:54.650","","","Rel-13","36.101","13.5.0","","4055","","F","","","","","",""]
["R4-1609813","CR on NPBCH Fixed Reference Channel for NB-IoT","Intel Corporation","Yang Tang","56725","CR","Agreement","---","","129","6.3.4.1.1","NPBCH  [NB_IOT-Perf]",977600000,"withdrawn","2016-11-04T06:41:47.990",null,"","","Rel-14","36.101","14.1.0","","4056","","A","","","","","",""]
["R4-1609814","Measurements for LAA with multiple Scells","Qualcomm Incorporated","Valentin Gheorghiu","43117","other","Approval","This paper proposes to introduce scaling of CA intra-frequency measurement periods based on the equation measurement period=min(3, NconfiguredLAASCells","","253","8.18.4.1","Measurement with multiple cells [LTE_eLAA-Core]",9814000,"noted","2016-11-04T06:41:59.893","2016-11-04T22:35:07.697","","","Rel-14","","","","","","","","","","","",""]
["R4-1609815","Simulation results of PDSCH performance for bidirectional HST","LG Electronics Inc.","Jin-yup Hwang","47026","discussion","Discussion","---","","345","8.28.3.1","Enhancement for bi-directional RRH arrangement [LTE_high_speed]",981500000,"noted","2016-11-04T06:42:49.937","2016-11-04T09:00:29.780","","","","","","","","","","","","","","",""]
["R4-1609816","On ACLR with Beamforming","Qualcomm Incorporated","Valentin Gheorghiu","43117","discussion","Discussion","In this paper we present some lab measurements that confirm the assumption that additional channel leakage is beamformed in the same direction as the signal in the main channel","","415","11.5.1","Common issues for UE and BS [FS_NR_newRAT]",952700000,"noted","2016-11-04T06:45:37.497","2016-11-04T22:35:07.697","","","","","","","","","","","","","","",""]
["R4-1609817","Received Signal Strength Measurements for mmWave","Qualcomm Incorporated","Valentin Gheorghiu","43117","discussion","Discussion","In this paper we highlight some problems related to the reference points for defining the requirements and OTA testing","","425","11.6.1.1","RRM general [FS_NR_newRAT]",4700000,"noted","2016-11-04T06:47:45.217","2016-11-04T22:35:07.697","","","","","","","","","","","","","","",""]
["R4-1609818","Test setup for mmWave","Qualcomm Incorporated","Valentin Gheorghiu","43117","discussion","Discussion","In this paper we discuss the basic setup needed for mmWave RF measurements","","419","11.5.2.3","Testability [FS_NR_newRAT]",51200000,"noted","2016-11-04T06:49:57.363","2016-11-04T22:35:07.713","","","","","","","","","","","","","","",""]
["R4-1609819","Wider Single Carrier Channel for NR","Qualcomm Incorporated","Valentin Gheorghiu","43117","discussion","Discussion","In this paper we discussed some aspects related to the proposal of defining a very wide single carrier channel and point out some issues that need further study","","407","11.1","General   [FS_NR_newRAT]",62700000,"noted","2016-11-04T06:52:48.370","2016-11-04T22:35:07.713","","","","","","","","","","","","","","",""]
["R4-1609820","Simulatin Results for NB-IoT co-existence with CDMA","Qualcomm Incorporated","Valentin Gheorghiu","43117","discussion","Discussion","In this paper we present updated simulation results on the co-existence between NB-IoT and CDMA","","392","9.3.3","Co-existence study [FS_NB_IOT_CDMA_coex]",974100000,"noted","2016-11-04T06:55:15.400","2016-11-04T22:35:07.713","","","","","","","","","","","","","","",""]
["R4-1609821","Requirements for Mobility Enhancements","Qualcomm Incorporated","Valentin Gheorghiu","43117","discussion","","In this paper we discuss the requirements for make before break","","327","8.26.3","RRM core (36.133) [LTE_eMob-Core]",955400000,"noted","2016-11-04T06:59:01.600","2016-11-04T22:35:07.727","","","","","","","","","","","","","","",""]
["R4-1609822","UE CR for CBRS band","Nokia, Qualcomm Incorporated","Petri Vasenkari","69954","CR","Approval","UE CR for CBRS band","","199","8.10.2","UE RF (36.101) [LTE_TDD_3550_CBRS_US]",77600000,"revised","2016-11-04T07:05:37.387","2016-11-04T13:27:46.533","","R4-1610776","Rel-14","36.101","14.1.0","LTE_TDD_3550_CBRS_US","4057","","B","","","","","",""]
["R4-1609823","Uplink 256-QAM MPR simulations","Nokia, Alcatel-Lucent Shanghai Bell","Petri Vasenkari","69954","other","Approval","Uplink 256-QAM MPR simulation results for single carrier","","228","8.15.2.1","MPR/A-MPR [LTE_UL_CAP_enh-Core]",939500000,"noted","2016-11-04T07:05:37.527","2016-11-04T13:27:46.533","","","","","","LTE_UL_CAP_enh-Core","","","","","","","","",""]
["R4-1609824","NB-IoT aggregate power control Rel-13","Nokia, Alcatel-Lucent Shanghai Bell","Petri Vasenkari","69954","CR","","Rel-13 CR for NB-IoT aggregate power control requriements","","54","5.6.2","UE RF (36.101) [NB_IOT-Core]",54100000,"revised","2016-11-04T07:05:37.543","2016-11-04T13:27:46.517","","R4-1610541","Rel-13","36.101","13.5.0","NB_IOT-Core","4058","","F","","","","","",""]
["R4-1609825","NB-IoT aggregate power control Rel-14","Nokia, Alcatel-Lucent Shanghai Bell","Petri Vasenkari","69954","CR","","Rel-14 CR for NB-IoT aggregate power control requriements","","54","5.6.2","UE RF (36.101) [NB_IOT-Core]",59600001,"agreed","2016-11-04T07:05:37.683","2016-11-19T17:47:26.003","","","Rel-14","36.101","14.1.0","NB_IOT-Core","4059","","A","RP-162433","","","","",""]
["R4-1609826","Uplink 3CC contigous intraband CA MPR studies","Nokia, Alcatel-Lucent Shanghai Bell","Petri Vasenkari","69954","other","Approval","---","","147","8.1.2","UE RF (36.101) [LTE_CA_R14_intra-Core]",919200000,"noted","2016-11-04T07:05:37.777","2016-11-04T13:27:46.517","","","","","","LTE_CA_R14_intra-Core","","","","","","","","",""]
["R4-1609827","On coverage level selection related matters","Nokia, Alcatel-Lucent Shanghai Bell","Petri Vasenkari","69954","other","Approval","---","","304","8.24.2.1","Power Class       [NB_IOTenh-Core]",962300000,"noted","2016-11-04T07:05:37.793","2016-11-04T13:27:46.517","","","","","","NB_IOTenh-Core","","","","","","","","",""]
["R4-1609828","LS On coverage level selection related matters","Nokia, Alcatel-Lucent Shanghai Bell","Petri Vasenkari","69954","LS out","Approval","---","","304","8.24.2.1","Power Class       [NB_IOTenh-Core]",982700000,"revised","2016-11-04T07:05:37.807","2016-11-04T13:28:22.257","","R4-1610828","","","","NB_IOTenh-Core","","","","","","","","",""]
["R4-1609829","Discussion on RAN5 LS relating to NB-IoT","Nokia, Alcatel-Lucent Shanghai Bell","Petri Vasenkari","69954","other","Approval","---","","54","5.6.2","UE RF (36.101) [NB_IOT-Core]",982400000,"noted","2016-11-04T07:05:37.840","2016-11-04T13:28:22.257","","","","","","NB_IOT-Core","","","","","","","","",""]
["R4-1609830","Draft Reply LS on RF requirements for category NB1 UEs","Nokia, Alcatel-Lucent Shanghai Bell","Petri Vasenkari","69954","LS out","Approval","---","","54","5.6.2","UE RF (36.101) [NB_IOT-Core]",982500000,"revised","2016-11-04T07:05:37.857","2016-11-04T13:28:22.240","","R4-1610542","","","","NB_IOT-Core","","","","","","","","",""]
["R4-1609831","Correction to NB-IoT ON/OFF power measurement period Rel-13","Nokia, Alcatel-Lucent Shanghai Bell","Petri Vasenkari","69954","CR","","---","","54","5.6.2","UE RF (36.101) [NB_IOT-Core]",983100000,"revised","2016-11-04T07:05:37.887","2016-11-04T13:28:22.257","","R4-1610535","Rel-13","36.101","13.5.0","NB_IOT-Core","4060","","F","","","","","",""]
["R4-1609832","Correction to NB-IoT ON/OFF power measurement period  Rel-14","Nokia, Alcatel-Lucent Shanghai Bell","Petri Vasenkari","69954","CR","","---","","54","5.6.2","UE RF (36.101) [NB_IOT-Core]",988200000,"agreed","2016-11-04T07:05:37.980","2016-11-19T17:47:26.020","","","Rel-14","36.101","14.1.0","NB_IOT-Core","4061","","A","RP-162433","","","","",""]
["R4-1609833","CAT 1 single Rx REFSENS definition","Nokia, Alcatel-Lucent Shanghai Bell","Petri Vasenkari","69954","other","Approval","---","","332","8.27.2.1","REFSENS  [LTE_UE_cat_1RX-Core]",187000,"noted","2016-11-04T07:05:38.073","2016-11-04T13:28:22.257","","","Rel-14","","","","","","","","","","","",""]
["R4-1609834","Corrections to CA table reference and header","Nokia, Alcatel-Lucent Shanghai Bell","Petri Vasenkari","69954","CR","","---","","12","4.2.1","UE RF (core / EMC)  [WI code or TEI12]",958400000,"revised","2016-11-04T07:05:38.090","2016-11-04T13:30:58.070","","R4-1610903","Rel-11","36.101","11.18.0","TEI11","4062","","F","","","","","",""]
["R4-1609835","Corrections to CA table reference and header","Nokia, Alcatel-Lucent Shanghai Bell","Petri Vasenkari","69954","CR","","---","","12","4.2.1","UE RF (core / EMC)  [WI code or TEI12]",958500000,"revised","2016-11-04T07:05:38.183","2016-11-19T17:47:26.020","","R4-1611025","Rel-12","36.101","12.13.0","TEI12","4063","","A","","","","","",""]
["R4-1609836","Corrections to CA table reference and header and CA REFSENS table","Nokia, Alcatel-Lucent Shanghai Bell","Petri Vasenkari","69954","CR","","---","","67","5.10.1.1","RF  [WI code]",3180000,"revised","2016-11-04T07:05:38.293","2016-11-04T13:30:58.023","","R4-1610815","Rel-13","36.101","13.5.0","TEI13","4064","","F","","","","","",""]
["R4-1609837","Corrections to CA table reference and header and CA REFSENS table","Nokia, Alcatel-Lucent Shanghai Bell","Petri Vasenkari","69954","CR","","---","","67","5.10.1.1","RF  [WI code]",3190000,"agreed","2016-11-04T07:05:38.400","2016-11-22T12:17:27.047","","","Rel-14","36.101","14.1.0","TEI14","4065","","A","RP-162408","","","","",""]
["R4-1609838","eLAA MPR study","Nokia, Alcatel-Lucent Shanghai Bell","Petri Vasenkari","69954","other","Approval","---","","244","8.18.2.1","MPR [LTE_eLAA-Core]",983800000,"noted","2016-11-04T07:05:38.497","2016-11-04T13:30:58.037","","","","","","LTE_eLAA-Core","","","","","","","","",""]
["R4-1609839","Band 68 modifications for PPDR use in Europe","Nokia","Petri Vasenkari","69954","other","Approval","---","","374","8.32.2","RF  [WI code or TEI14]",188000,"noted","2016-11-04T07:05:38.510","2016-11-04T13:30:58.037","","","","","","TEI14","","","","","","","","",""]
["R4-1609840","V2X S-RSRP simulation results","Ericsson","Joakim Axmon","62375","discussion","Discussion","In this contribution we provide updates results for S-RSRP measurements under the simulation assumptions agreed at RAN4#80bis.","","283","8.20.4.3","Initiation/cease of SLSS requirement [LTE_V2X-Core]",20900000,"noted","2016-11-04T07:31:43.050","2016-11-04T08:47:28.033","","","Rel-14","","","LTE_V2X-Core","","","","","","","","",""]
["R4-1609841","GNSS synchronization source selection time","Ericsson","Joakim Axmon","62375","other","Approval","In this contribution we are proposing requirements on GNSS synchronization source selection times in order to allow UEs to continue to receive and broadcast safety critical information when losing RAN coverage.","","284","8.20.4.4","Requirements related to synchronization [LTE_V2X-Core]",9800000,"noted","2016-11-04T07:31:43.067","2016-11-04T08:47:28.047","","","Rel-14","","","LTE_V2X-Core","","","","","","","","",""]
["R4-1609842","Correction of TA application rule in eMTC","Ericsson","Joakim Axmon","62375","other","Approval","In this contribution we address the timing advance application rule regarding eMTC in HD-FDD operation.","","49","5.5.3.2","UE transmit timing [LTE_MTCe2_L1-Core]",590000,"noted","2016-11-04T07:31:43.080","2016-11-04T08:47:28.047","","","Rel-13","","","LTE_MTCe2_L1-Core","","","","","","","","",""]
["R4-1609843","Correction of TA application rule in eMTC","Ericsson","Joakim Axmon","62375","CR","Approval","The TA application rule is corrected in order to avoid confusion about when in time a timing advance is to be applied when repetition is used.","","49","5.5.3.2","UE transmit timing [LTE_MTCe2_L1-Core]",6000000,"noted","2016-11-04T07:31:43.097","2016-11-04T08:47:28.047","","","Rel-13","36.133","13.5.0","LTE_MTCe2_L1-Core","4234","","F","","","","","",""]
["R4-1609844","Correction of TA application rule in eMTC","Ericsson","Joakim Axmon","62375","CR","Approval","The TA application rule is corrected in order to avoid confusion about when in time a timing advance is to be applied when repetition is used.","","49","5.5.3.2","UE transmit timing [LTE_MTCe2_L1-Core]",6100000,"noted","2016-11-04T07:31:43.190","2016-11-04T08:47:28.017","","","Rel-14","36.133","14.1.0","LTE_MTCe2_L1-Core","4235","","A","","","","","",""]
["R4-1609845","UE Tx timing requirements for 5 MHz under normal and enhanced coverage","Ericsson","Joakim Axmon","62375","other","Approval","In this contribution we are discussing the UE Tx timing tolerance for feMTC with 24 RBs bandwidth.","","321","8.25.3.2.3","UE Tx timing [LTE_feMTC-Core]",984500000,"noted","2016-11-04T07:31:43.300","2016-11-04T08:47:28.033","","","Rel-14","","","LTE_feMTC-Core","","","","","","","","",""]
["R4-1609846","Requirements on measurements for congestion control in V2X","Ericsson","Joakim Axmon","62375","discussion","Discussion","In this contribution we are proposing simulation work on channel busy ratio measurements for congestion control in V2X.","","286","8.20.4.6","Congestion control [LTE_V2X-Core]",9846000,"noted","2016-11-04T07:31:43.317","2016-11-04T08:47:28.033","","","Rel-14","","","LTE_V2X-Core","","","","","","","","",""]
["R4-1609847","TP for 36.714-04-01: CA_3A-3A-7A-8A operating bands, channel bandwidths and BS co-existence studies","CHTTL","Bo-Han Hsieh","61837","pCR","Approval","---","","165","8.4.2","UE RF (36.101) [LTE_CA_R14_4DL1UL-Core]",30800000,"approved","2016-11-04T07:53:35.510","2016-11-04T17:45:09.797","","","","36.714-04-01","0.2.0","","","","","","","","","",""]
["R4-1609848","TP for 36.714-04-01: UE requirements for CA_3A-3A-7A-8A","CHTTL","Bo-Han Hsieh","61837","pCR","Approval","---","","165","8.4.2","UE RF (36.101) [LTE_CA_R14_4DL1UL-Core]",91980000,"approved","2016-11-04T07:56:50.243","2016-11-04T17:45:09.797","","","","36.714-04-01","0.2.0","","","","","","","","","",""]
["R4-1609849","On the need to capture OTA testing aspects in TS 37.145-2","Ericsson","Torbjorn Elfstrom","44796","discussion","Discussion","At last meeting (RAN4#80bis in Ljubljana) two CRs for adding informative text describing newly introduced test procedures better in 37.145-2 was presented [1, 2]. Currently, OTA test methods and procedures are described at a very high abstraction level. H","","26","5.1.3.2","Maintenance for TS37.145-2 [AAS_BS_LTE_UTRA-Perf]",4340000,"noted","2016-11-04T08:05:18.820","2016-11-04T15:44:57.280","","","Rel-13","","","AAS_BS_LTE_UTRA-Perf","","","","","","","","",""]
["R4-1609850","CR to TS 37.145 part 2: Addition of descriptive text on test methods","Ericsson","Torbjorn Elfstrom","44796","CR","Approval","This CR adds descriptive information for applicable test methods in Annex E.","","26","5.1.3.2","Maintenance for TS37.145-2 [AAS_BS_LTE_UTRA-Perf]",984900000,"noted","2016-11-04T08:05:18.837","2016-11-04T15:44:57.297","","","Rel-13","37.145-2","13.0.0","AAS_BS_LTE_UTRA-Perf","0004","","F","","","","","",""]
["R4-1609851","On finding a minimum requirement level for OTA sensitivity","Ericsson","Torbjorn Elfstrom","44796","discussion","Discussion","RAN4 have since the beginning of the AAS WI discussed details of OTA sensitivity. Currently in Release 13, the requirement designed around a declaration of EIS, which should be met within a certain spatial region. This means that one EIS value is declared","","209","8.12.2.1","In band requirements [AASenh_BS_LTE_UTRA]",985300000,"noted","2016-11-04T08:05:18.930","2016-11-04T15:44:57.297","","","Rel-14","","","AASenh_BS_LTE_UTRA","","","","","","","","",""]
["R4-1609852","On OTA frequency error requirement and testing aspects","Ericsson","Torbjorn Elfstrom","44796","discussion","Discussion","At last meeting the discussion on how to defined a RF core requirement for carrier frequency error was initiated in [1]. This contribution presents some aspects on how to test frequency error in an OTA environment.","","209","8.12.2.1","In band requirements [AASenh_BS_LTE_UTRA]",973000000,"noted","2016-11-04T08:05:18.977","2016-11-04T15:44:57.297","","","Rel-14","","","AASenh_BS_LTE_UTRA","","","","","","","","",""]
["R4-1609853","On aspects related to OTA timing alignment error","Ericsson","Torbjorn Elfstrom","44796","discussion","Discussion","For enhanced AAS (eAAS) part of Release 14 WI the work of defining an all OTA specification have started. So far, requirements for radiated transmit power and OTA sensitivity have been defined and captured in specifications (TS 37.105 and TS 37.145). In e","","209","8.12.2.1","In band requirements [AASenh_BS_LTE_UTRA]",985100000,"noted","2016-11-04T08:05:18.990","2016-11-04T15:44:57.297","","","Rel-14","","","AASenh_BS_LTE_UTRA","","","","","","","","",""]
["R4-1609854","On aspects related to OTA testing and occupied bandwidth","Ericsson","Torbjorn Elfstrom","44796","discussion","Discussion","In Release 13, two OTA requirements was introduced for AAS base stations; Radiated transmit power and OTA sensitivity. The work related to find all remaining OTA requirements for AAS base stations is ongoing in RAN4 eAAS WI. This contribution elaborates a","","209","8.12.2.1","In band requirements [AASenh_BS_LTE_UTRA]",3640000,"noted","2016-11-04T08:05:19.023","2016-11-04T15:44:57.297","","","Rel-14","","","AASenh_BS_LTE_UTRA","","","","","","","","",""]
["R4-1609855","Further elaboration on NR BS requirement applicability","Ericsson","Torbjorn Elfstrom","44796","discussion","Discussion","At the last RAN4 meeting (RAN4#80bis) NR BS requirements applicability and conformance testing aspects was discussed. The outcome was capture part of the agreed way-forward  [1]. In RAN4 a specification for MSR base stations have been developed in TS 37.1","","420","11.5.3","BS RF  [FS_NR_newRAT]",99430000,"noted","2016-11-04T08:05:19.037","2016-11-04T15:44:57.313","","","Rel-14","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1609856","On test setups applicable for NR base stations","Ericsson","Torbjorn Elfstrom","44796","discussion","Discussion","NR base station RF core requirements and conformance testing requirements will be developed for base stations converging a frequency range from today’s band up to millimetre-wave frequencies. The requirement can be divided into three main categories, as d","","423","11.5.3.3","Testability [FS_NR_newRAT]",985600000,"noted","2016-11-04T08:05:19.053","2016-11-04T15:44:57.313","","","Rel-14","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1609857","TP for TR 38.803: Micro-wave and millimetre-wave antenna considerations","Ericsson","Torbjorn Elfstrom","44796","pCR","Approval","At the last meeting a set of contributions on micro-wave and millimetre-wave technology aspects for base stations was presented [2, 3, 4, 5, 6]. The contributions presented as text proposals for TR 38.803 with the intention to capture aspects relevant for","","420","11.5.3","BS RF  [FS_NR_newRAT]",994900000,"revised","2016-11-04T08:05:19.087","2016-11-04T15:44:57.313","","R4-1610604","","38.803","0.3.0","FS_NR_newRAT","","","","","","","","",""]
["R4-1609858","On TRP testing for UE emissions","Ericsson","Torbjorn Elfstrom","44796","discussion","Discussion","At last meeting (RAN4#80bis in Ljubljana) some practical issues regarding measuring UE OTA emission was discussed. This contribution will elaborate around possibilities and challenges related to measure UE OTA emission.","","419","11.5.2.3","Testability [FS_NR_newRAT]",1000000,"noted","2016-11-04T08:05:19.100","2016-11-04T15:44:57.313","","","Rel-14","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1609859","New NS value for Band 28","Ericsson","Patrizia Testa","66129","discussion","Discussion","This contribution gives a justification on the possibility to define a new NS value for B28 without creating problem  to legacy PC3 UEs","","234","8.16.2","UE RF (36.101)  [LTE_HPUE_B3_B20_B28]",985900000,"noted","2016-11-04T08:34:55.537","2016-11-04T12:21:31.917","","","Rel-14","","","LTE_HPUE_B3_B20_B28","","","","","","","","",""]
["R4-1609860","TP for TR 36.744: Additional regulatory requirements for Section 5","Ericsson","Patrizia Testa","66129","pCR","Approval","This TP proposes to complete the list of regulatory requirements relevant to RAN 4  by adding power limits.","","198","8.10.1","General [LTE_TDD_3550_CBRS_US]",3000000,"approved","2016-11-04T08:34:55.550","2016-11-04T09:09:39.803","","","","36.744","0.1.0","LTE_TDD_3550_CBRS_US","","","","","","","","",""]
["R4-1609861","Draft CR to 25.104: Introduction of Band 48","Ericsson, Nokia","Patrizia Testa","66129","draftCR","Endorsement","Changes for the introduction of Band 48 to 25.104","","202","8.10.5","Other specifications [LTE_TDD_3550_CBRS_US]",2940000,"endorsed","2016-11-04T08:34:55.567","2016-11-04T09:32:00.780","","","Rel-14","25.104","14.0.0","LTE_TDD_3550_CBRS_US","","","B","","","","","",""]
["R4-1609862","Draft CR to 25.141: Introduction of Band 48","Ericsson, Nokia","Patrizia Testa","66129","draftCR","Endorsement","Changes for the introduction of Band 48 to 25.141","","202","8.10.5","Other specifications [LTE_TDD_3550_CBRS_US]",2970000,"noted","2016-11-04T08:34:55.583","2016-11-04T10:22:42.280","","","Rel-14","25.141","14.0.0","LTE_TDD_3550_CBRS_US","","","B","","","","","",""]
["R4-1609863","Draft CR to 37.104: Introduction of Band 48","Ericsson, Nokia","Patrizia Testa","66129","draftCR","Endorsement","Changes for the introduction of Band 48 to 37.104","","202","8.10.5","Other specifications [LTE_TDD_3550_CBRS_US]",2980000,"noted","2016-11-04T08:34:55.597","2016-11-04T10:33:25.423","","","Rel-14","37.104","14.1.0","LTE_TDD_3550_CBRS_US","","","B","","","","","",""]
["R4-1609864","Draft CR to 37.113: Introduction of Band 48","Ericsson, Nokia","Patrizia Testa","66129","draftCR","Endorsement","Changes for the introduction of Band 48 to 37.113","","202","8.10.5","Other specifications [LTE_TDD_3550_CBRS_US]",3270000,"noted","2016-11-04T08:34:55.627","2016-11-04T10:40:34.873","","","Rel-14","37.113","14.0.0","LTE_TDD_3550_CBRS_US","","","B","","","","","",""]
["R4-1609865","Draft CR to 37.141: Introduction of Band 48","Ericsson, Nokia","Patrizia Testa","66129","draftCR","Endorsement","Changes for the introduction of Band 48 to 37.141","","202","8.10.5","Other specifications [LTE_TDD_3550_CBRS_US]",29900000,"noted","2016-11-04T08:34:55.643","2016-11-04T10:47:42.207","","","Rel-14","37.141","14.1.0","LTE_TDD_3550_CBRS_US","","","B","","","","","",""]
["R4-1609866","Discussion on introducing new enhanced performance requirements type","Huawei,HiSilicon","Xiang (Steven) Chen","41576","discussion","Discussion","In this contribution, we will discuss on introducing new enhanced performance requirements type.","","345","8.28.3.1","Enhancement for bi-directional RRH arrangement [LTE_high_speed]",910700000,"noted","2016-11-04T08:35:28.637","2016-11-07T11:30:26.890","","","","","","LTE_high_speed","","","","","","","","",""]
["R4-1609867","TP for 36.786 Operating bands and channel bandwidth for V2X","Huawei, Hisilicon","Xiang (Steven) Chen","41576","pCR","","---","","273","8.20.1","General [LTE_V2X-Core]",97950000,"revised","2016-11-04T08:48:26.517","2016-11-04T12:05:23.203","","R4-1610753","","36.786","0.1.0","","","","","","","","","",""]
["R4-1609868","Metric on UE RF Tx requirements in mmWave","NTT DOCOMO, INC.","Kei Ando","57164","other","Approval","---","","417","11.5.2.1","Transmitter characteristics [FS_NR_newRAT]",987000000,"noted","2016-11-04T09:07:55.813","2016-11-04T12:10:34.580","","","","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1609869","Metric on UE RF Rx requirements in mmWave","NTT DOCOMO, INC.","Kei Ando","57164","other","Approval","---","","418","11.5.2.2","Receiver characteristics [FS_NR_newRAT]",975500000,"noted","2016-11-04T09:07:55.847","2016-11-04T12:10:34.580","","","","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1609870","UE to UE coexistence between below 6 GHz and mmWave","NTT DOCOMO, INC.","Kei Ando","57164","other","Approval","This contribution discusses UE to UE coexistence between below 6 GHz and mmWave.","","417","11.5.2.1","Transmitter characteristics [FS_NR_newRAT]",991700000,"noted","2016-11-04T09:07:55.860","2016-11-04T12:10:34.597","","","","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1609871","P-Max related requirements for HPUE","NTT DOCOMO, INC.","Kei Ando","57164","other","Approval","---","","234","8.16.2","UE RF (36.101)  [LTE_HPUE_B3_B20_B28]",987100000,"revised","2016-11-04T09:07:55.877","2016-11-04T12:10:34.567","","R4-1610825","","","","LTE_HPUE_B3_B20_B28","","","","","","","","",""]
["R4-1609872","Draft CR for HPUE for operating bands other than Band 41","NTT DOCOMO, INC.","Kei Ando","57164","draftCR","Endorsement","---","","234","8.16.2","UE RF (36.101)  [LTE_HPUE_B3_B20_B28]",987200000,"revised","2016-11-04T09:07:55.893","2016-11-04T12:10:34.580","","R4-1610826","Rel-14","36.101","14.1.0","LTE_HPUE_B3_B20_B28","","","B","","","","","",""]
["R4-1609873","Introduction of 4Rx requirement (non-CA) for Band 21 (Rel-13)","NTT DOCOMO, INC.","Kei Ando","57164","CR","Agreement","---","","29","5.2.1","UE RF (36.101)  [LTE_4Rx_AP_DL-Core]",963900000,"endorsed","2016-11-04T09:07:55.923","2016-11-04T12:10:34.550","","","Rel-13","36.101","13.5.0","LTE_4Rx_AP_DL-Core","4066","","F","","","","","",""]
["R4-1609874","Introduction of 4Rx requirement (non-CA and CA) for Band 21 (Rel-14)","NTT DOCOMO, INC.","Kei Ando","57164","CR","Agreement","---","","29","5.2.1","UE RF (36.101)  [LTE_4Rx_AP_DL-Core]",987300000,"endorsed","2016-11-04T09:07:56.017","2016-11-04T12:10:34.550","","","Rel-14","36.101","14.1.0","LTE_4Rx_AP_DL-Core","4067","","F","","","","","",""]
["R4-1609875","New Work Item proposal on an FDD band plan in the L-band for LTE","NTT DOCOMO, INC.","Kei Ando","57164","WID new","Information","---","","430","13","Revision of the Work Plan",949300000,"available","2016-11-04T09:07:56.110","2016-11-04T12:10:34.567","","","Rel-14","","","","","","","","","","","",""]
["R4-1609876","Motivation to develop a new FDD band plan in the L-band for LTE","NTT DOCOMO, INC.","Kei Ando","57164","discussion","Discussion","---","","430","13","Revision of the Work Plan",962200000,"available","2016-11-04T09:07:56.127","2016-11-04T12:10:34.567","","","Rel-14","","","","","","","","","","","",""]
["R4-1609877","TP for TR 36.714-02-02 2DL2UL CA_21A-28A_BCS0","NTT DOCOMO, INC.","Kei Ando","57164","pCR","Approval","This TP is reserved to capture the MSD value during the meeting.","","177","8.6.2","UE RF (36.101) [LTE_CA_R14_2DL2UL-Core]",9877000,"approved","2016-11-04T09:07:56.143","2016-11-19T17:47:26.037","","","","36.714-02-02","0.5.0","LTE_CA_R14_2DL2UL-Core","","","","","","","","",""]
["R4-1609878","TP for TR 36.714-02-02 2DL2UL CA_28A-42A_BCS0","NTT DOCOMO, INC.","Kei Ando","57164","pCR","Approval","This TP is reserved to capture the MSD value during the meeting.","","177","8.6.2","UE RF (36.101) [LTE_CA_R14_2DL2UL-Core]",9878000,"approved","2016-11-04T09:07:56.157","2016-11-19T17:47:26.050","","","","36.714-02-02","0.5.0","LTE_CA_R14_2DL2UL-Core","","","","","","","","",""]
["R4-1609879","TP for TR 36.745: EESS protection scheme","NTT DOCOMO, INC.","Kei Ando","57164","pCR","Approval","---","","388","9.2.2","UE RF (36.101) [FS_LTE_B11_B21_global]",904300001,"revised","2016-11-04T09:07:56.190","2016-11-04T12:10:34.567","","R4-1610838","","36.745","0.2.0","FS_LTE_B11_B21_global","","","","","","","","",""]
["R4-1609880","Addition of new operating bands for NB-IoT","Nokia","Petri Vasenkari","69954","CR","","a coverpage revision of an agreed CR R4-168964","","238","8.17.2","UE RF (36.101)  [NB_IOT_R14_bands]",988000000,"agreed","2016-11-04T09:32:24.553","2016-11-04T13:30:58.053","R4-168964","","Rel-14","36.101","14.1.0","NB_IOT-Core","3943","2","B","RP-162433","","","","",""]
["R4-1609881","CR for IRC TM2/3/3 tests with 4Rx in Rel-14","Ericsson","Torgny Palenius","22640","CR","Approval","CR for 4Rx IRC\nthis is a coverpage revision of  agreed CR. 3903","","33","5.2.3.2","UE demodulation and CSI [LTE_4Rx_AP_DL-Perf]",936000000,"revised","2016-11-04T09:44:42.653","2016-11-04T14:15:46.043","R4-167915","R4-1610704","Rel-14","36.101","14.1.0","LTE_4Rx_AP_DL-Perf","3903","1","A","","","","","",""]
["R4-1609882","A-MPR for category NB1","Ericsson","Ali Behravan","45979","CR","Approval","In this CR we clarify the A-MPR for category NB1","","54","5.6.2","UE RF (36.101) [NB_IOT-Core]",53500000,"revised","2016-11-04T09:46:15.130","2016-11-04T14:15:00.383","","R4-1610540","Rel-14","36.101","14.1.0","NB_IOT-Core","4068","","A","","","","","",""]
["R4-1609883","Introduction of new bands for NB-IoT in 36.104","Ericsson","Ali Behravan","45979","CR","Approval","In tis CR we introduce new bands for Rel-14 NB-IoT in Rel independent 36.307","","237","8.17.1","Rapporteur Input [NB_IOT_R14_bands]",95900,"revised","2016-11-04T09:46:15.207","2016-11-04T14:16:01.517","","R4-1610831","Rel-13","36.307","13.5.0","NB_IOT_R14_bands-Core","0718","","B","","","","","",""]
["R4-1609884","REFSENS requirements for furhter enhanced MTC","Ericsson","Ali Behravan","45979","other","Discussion","In this contribution we present an approach for deriving reference sensitivity requirement for FeMTC","","313","8.25.2","High data rate  [LTE_feMTC-Core]",83000,"noted","2016-11-04T09:46:15.287","2016-11-04T15:43:48.600","","","Rel-14","","","LTE_feMTC-Core","","","","","","","","",""]
["R4-1609885","Transmitter requirements for Rel-14 MTC UE","Ericsson","Ali Behravan","45979","other","Discussion","In this contribution we discuss transmitter requirements for Rel-14 MTC UE","","313","8.25.2","High data rate  [LTE_feMTC-Core]",988400000,"approved","2016-11-04T09:46:15.317","2016-11-04T15:43:48.600","","","Rel-14","","","LTE_feMTC-Core","","","","","","","","",""]
["R4-1609886","Simulation results for UL 256QAM MPR","Ericsson","Ali Behravan","45979","other","Discussion","In this contribution we present simulation results for MPR of UL 256QAM","","228","8.15.2.1","MPR/A-MPR [LTE_UL_CAP_enh-Core]",939900000,"noted","2016-11-04T09:46:15.333","2016-11-04T15:00:35.003","","","Rel-14","","","LTE_UL_CAP_enh-Core","","","","","","","","",""]
["R4-1609887","WF on MPR and A-MPR for UL 256QAM","Ericsson","Ali Behravan","45979","other","Approval","This is a way forward for MPR and A-MPR of UL 256QAM","","228","8.15.2.1","MPR/A-MPR [LTE_UL_CAP_enh-Core]",988700000,"withdrawn","2016-11-04T09:46:15.347",null,"","","Rel-14","","","LTE_UL_CAP_enh-Core","","","","","","","","",""]
["R4-1609888","Requirements Supporting Resource Selection/Reselection","Qualcomm Europe Inc.(France)","TIen Viet NGUYEN","67205","discussion","Approval","---","","285","8.20.4.5","Autonomous resource selection/reselection [LTE_V2X-Core]",9500000,"noted","2016-11-04T09:49:39.023","2016-11-06T18:56:26.020","","","Rel-14","","","LTE_V2X-Core","","","","","","","","",""]
["R4-1609889","CR to TR 37.842: Clarifications, definitions alignment and text improvements","Huawei","Michal Szydelko","65553","CR","Approval","this is a coverpage revision of an agreed CR.","","22","5.1.1","Technical Report (37.842) [AAS_BS_LTE_UTRA-Core]",967000000,"agreed","2016-11-04T09:50:11.640","2016-11-04T10:11:09.813","R4-168879","","Rel-13","37.842","13.0.0","AAS_BS_LTE_UTRA-Core","0004","2","D","RP-162422","","","","",""]
["R4-1609890","Addition of new operating bands for NB-IoT","Nokia","Petri Vasenkari","69954","CR","","coverpage revision of an agreed CR R4-168251","","238","8.17.2","UE RF (36.101)  [NB_IOT_R14_bands]",989000000,"withdrawn","2016-11-04T09:52:16.910",null,"R4-168251","","Rel-14","36.101","14.1.0","NB_IOT_R14_bands-Core","3943","3","A","","","","","",""]
["R4-1609891","Simulation results for IRC TM2/3/3 test with 4Rx","Ericsson","Torgny Palenius","22640","discussion","Discussion","This contribution contains Ericsson simulation results for new testcase based on IRC TM2/3/3","","33","5.2.3.2","UE demodulation and CSI [LTE_4Rx_AP_DL-Perf]",906700001,"noted","2016-11-04T09:54:59.523","2016-11-04T14:15:46.043","","","Rel-13","","","LTE_4Rx_AP_DL-Perf","","","","","","","","",""]
["R4-1609892","Summary results for IRC TM2/3/3 test with 4Rx","Ericsson","Torgny Palenius","22640","discussion","Discussion","This contribution contains a summary sheet for results for new testcase based on IRC TM2/3/3","","33","5.2.3.2","UE demodulation and CSI [LTE_4Rx_AP_DL-Perf]",64100000,"revised","2016-11-04T09:54:59.540","2016-11-04T14:15:46.057","","R4-1610702","Rel-13","","","LTE_4Rx_AP_DL-Perf","","","","","","","","",""]
["R4-1609893","CR for IRC TM2/3/3 tests with 4Rx in Rel-13","Ericsson","Torgny Palenius","22640","CR","Approval","This contribution contains a CR for new testcase based on IRC TM2/3/3","","33","5.2.3.2","UE demodulation and CSI [LTE_4Rx_AP_DL-Perf]",906800000,"revised","2016-11-04T09:54:59.570","2016-11-04T14:15:46.057","","R4-1610703","Rel-13","36.101","13.5.0","LTE_4Rx_AP_DL-Perf","4069","","F","","","","","",""]
["R4-1609894","CR for IRC TM2/3/3 tests with 4Rx in Rel-14","Ericsson","Torgny Palenius","22640","CR","Approval","This contribution contains a CR for new testcase based on IRC TM2/3/3","","33","5.2.3.2","UE demodulation and CSI [LTE_4Rx_AP_DL-Perf]",906900001,"withdrawn","2016-11-04T09:54:59.680",null,"","","Rel-14","36.101","14.1.0","LTE_4Rx_AP_DL-Perf","4070","","A","","","","","",""]
["R4-1609895","Simulation results for TM9 8.3.1.1 and 8.3.2.1A  test 2 with 4Rx","Ericsson","Torgny Palenius","22640","discussion","Discussion","This contribution contains Ericsson simulation results for the TM9 testcase in 8.3.1.1 and 8.3.2.1A for a 4Rx UE","","33","5.2.3.2","UE demodulation and CSI [LTE_4Rx_AP_DL-Perf]",988100000,"noted","2016-11-04T09:54:59.790","2016-11-04T14:15:46.057","","","Rel-13","","","LTE_4Rx_AP_DL-Perf","","","","","","","","",""]
["R4-1609896","Summary results for TM9 8.3.1.1 and 8.3.2.1A test 2","Ericsson","Torgny Palenius","22640","discussion","Discussion","This contribution contains a summary sheet for the TM9 testcase in 8.3.1.1 and 8.3.2.1A for a 4Rx UE","","33","5.2.3.2","UE demodulation and CSI [LTE_4Rx_AP_DL-Perf]",948900000,"noted","2016-11-04T09:54:59.803","2016-11-04T14:15:46.057","","","","","","","","","","","","","","",""]
["R4-1609897","Discussion on revisiting antenna connection requirements  for Type 2 UEs","Ericsson","Torgny Palenius","22640","discussion","Discussion","This contribution discusses the margins for Type 2 Ues when testing legacy tests","","32","5.2.3.1","Applicability [LTE_4Rx_AP_DL-Perf]",989700000,"noted","2016-11-04T09:54:59.820","2016-11-04T14:15:46.073","","","Rel-13","","","LTE_4Rx_AP_DL-Perf","","","","","","","","",""]
["R4-1609898","CR for correcting applicability rules for 4Rx tests in Rel-13","Ericsson","Torgny Palenius","22640","CR","Approval","This contribution contains a CR for correcting the applicability rules for Type 2 4Rx Ues.","","32","5.2.3.1","Applicability [LTE_4Rx_AP_DL-Perf]",989800000,"noted","2016-11-04T09:54:59.837","2016-11-04T14:15:46.073","","","Rel-13","36.101","13.5.0","LTE_4Rx_AP_DL-Perf","4071","","F","","","","","",""]
["R4-1609899","CR for correcting applicability rules for 4Rx tests in Rel-14","Ericsson","Torgny Palenius","22640","CR","Approval","This contribution contains a CR for correcting the applicability rules for Type 2 4Rx Ues.","","32","5.2.3.1","Applicability [LTE_4Rx_AP_DL-Perf]",989900000,"withdrawn","2016-11-04T09:54:59.947",null,"","","Rel-14","36.101","14.1.0","LTE_4Rx_AP_DL-Perf","4072","","A","","","","","",""]
["R4-1609900","Discussion on HST CQI requirements","Ericsson","Torgny Palenius","22640","discussion","Discussion","This contribution analyze the proposed CQI requirements for HST Ues.","","347","8.28.3.3","CQI reporting [LTE_high_speed]",947200000,"noted","2016-11-04T09:55:00.087","2016-11-04T14:15:46.073","","","Rel-14","","","LTE_high_speed","","","","","","","","",""]
["R4-1609901","Discussion on HST unidirectional performance","Ericsson","Torgny Palenius","22640","discussion","Discussion","This contribution propose a new testcase for HST Unidirectional deployment at 500 km/h","","346","8.28.3.2","Unidirectional RRH arrangement [LTE_high_speed]",947300000,"noted","2016-11-04T09:55:00.117","2016-11-04T14:15:46.090","","","Rel-14","","","LTE_high_speed","","","","","","","","",""]
["R4-1609902","CR on unidirectional RRH arrangement","Ericsson","Torgny Palenius","22640","CR","Approval","This contribution contains a CR to introduce a new testcase for high speed train unidirectional deployment.","","346","8.28.3.2","Unidirectional RRH arrangement [LTE_high_speed]",990200000,"noted","2016-11-04T09:55:00.133","2016-11-04T14:15:46.090","","","Rel-14","36.101","14.1.0","LTE_high_speed","4073","","B","","","","","",""]
["R4-1609903","Introduction of Rel-14 5DL inter-band combinations in 36.101","Nokia","Hisashi Onozawa","70298","CR","Approval","This contribution is a big CR to include Rel-14 5DL/1UL CA into TS36.101.","","170","8.5.1","Rapporteur Input (WID/CRs)  [LTE_CA_R14_5DL1UL-Core]",2910000,"agreed","2016-11-04T09:55:25.153","2016-11-19T17:47:26.067","","","Rel-14","36.101","14.1.0","LTE_CA_R14_5DL1UL-Core","4074","","B","RP-162402","","","","",""]
["R4-1609904","Corrections of CA Refsens exceptions in 7.3.1A (Rel-12)","Nokia, Alcatel-Lucent Shanghai Bell, Huawei","Hisashi Onozawa","70298","CR","Approval","This CR is to revise 7.3.1A  to align with the change of Rel-13 spec.","","12","4.2.1","UE RF (core / EMC)  [WI code or TEI12]",965100000,"revised","2016-11-04T09:55:25.297","2016-11-04T11:04:49.277","","R4-1610904","Rel-12","36.101","12.13.0","TEI12","4075","","F","","","","","",""]
["R4-1609905","Corrections of CA Refsens exceptions in 7.3.1A (Rel-13)","Nokia, Alcatel-Lucent Shanghai Bell, Ericsson, Huawei","Hisashi Onozawa","70298","CR","Approval","This is a merged CR of endorsed CR (R4-167410,\nR4-167981, R4-168288, R4-168289, R4-168291) from 80bis.\nA few more changes are added after offline discussion.","","67","5.10.1.1","RF  [WI code]",983600000,"revised","2016-11-04T09:55:25.387","2016-11-04T11:04:49.293","","R4-1610816","Rel-13","36.101","13.5.0","TEI13","4076","","F","","","","","",""]
["R4-1609906","Corrections of CA Refsens exceptions in 7.3.1A (Cat A)","Nokia, Alcatel-Lucent Shanghai Bell, Ericsson, Huawei","Hisashi Onozawa","70298","CR","Approval","Cat A CR (if Rel-14 CR is accepted, this is not needed.)","","67","5.10.1.1","RF  [WI code]",983700000,"withdrawn","2016-11-04T09:55:25.497",null,"","","Rel-14","36.101","14.1.0","TEI13","4077","","A","","","","","",""]
["R4-1609907","Corrections of CA Refsens exceptions in 7.3.1A (Rel-14)","Nokia, Alcatel-Lucent Shanghai Bell","Hisashi Onozawa","70298","CR","Approval","This is a mirror CR of R4-1609905 together  with additional changes for new CAs introduced in Rel-14.","","67","5.10.1.1","RF  [WI code]",990500000,"revised","2016-11-04T09:55:25.590","2016-11-04T11:04:49.293","","R4-1610817","Rel-14","36.101","14.1.0","TEI14, TEI13","4078","","F","","","","","",""]
["R4-1609908","DeltaRIB for SDL CA","Nokia, Alcatel-Lucent Shanghai Bell","Hisashi Onozawa","70298","CR","Approval","This CR is add DeltaRib for the CA with SDL bands in order to align with the change of Rel-13 spec.","","12","4.2.1","UE RF (core / EMC)  [WI code or TEI12]",965200000,"revised","2016-11-04T09:55:25.700","2016-11-04T11:04:49.293","","R4-1610905","Rel-12","36.101","12.13.0","TEI12","4079","","F","","","","","",""]
["R4-1609909","DeltaRIB for SDL and LAA CA","Nokia, Alcatel-Lucent Shanghai Bell","Hisashi Onozawa","70298","CR","Approval","This is a formal CR of the endorsed CR (R4-168290) from 80bis.\nA few errors in DRib are fixed after 80bis.","","67","5.10.1.1","RF  [WI code]",990600000,"revised","2016-11-04T09:55:25.810","2016-11-04T11:04:49.293","","R4-1610818","Rel-13","36.101","13.5.0","TEI13","4080","","F","","","","","",""]
["R4-1609910","DeltaRIB for SDL and LAA CA","Nokia, Alcatel-Lucent Shanghai Bell","Hisashi Onozawa","70298","CR","Approval","Cat A CR","","67","5.10.1.1","RF  [WI code]",990700000,"agreed","2016-11-04T09:55:25.903","2016-11-19T17:47:26.083","","","Rel-14","36.101","14.1.0","TEI13","4081","","A","RP-162435","","","","",""]
["R4-1609911","AAS ACLR absolute limit","Nokia, Alcatel-Lucent Shanghai Bell","Hisashi Onozawa","70298","CR","Approval","ACLR/CACLR absolute limit scaling is clarified.","","22","5.1.1","Technical Report (37.842) [AAS_BS_LTE_UTRA-Core]",2810000,"revised","2016-11-04T09:55:26.027","2016-11-04T18:50:13.880","","R4-1610791","Rel-13","37.842","13.0.0","AAS_BS_LTE_UTRA-Core","0009","","F","","","","","",""]
["R4-1609912","AAS ACLR absolute limit","Nokia, Alcatel-Lucent Shanghai Bell","Hisashi Onozawa","70298","CR","Approval","ACLR/CACLR absolute limit scaling is clarified.","","23","5.1.2","BS RF(37.105) [AAS_BS_LTE_UTRA-Core]",79600,"revised","2016-11-04T09:55:26.123","2016-11-04T18:50:31.993","","R4-1610794","Rel-13","37.105","13.2.0","AAS_BS_LTE_UTRA-Core","0024","","F","","","","","",""]
["R4-1609913","CR to TS 37.105: Clarifications, definitions alignment and text improvements","Huawei","Michal Szydelko","65553","CR","Approval","This is a coverpage revision of an agreed CR.","","23","5.1.2","BS RF(37.105) [AAS_BS_LTE_UTRA-Core]",4300000,"agreed","2016-11-04T09:58:57.360","2016-11-04T10:11:09.797","R4-168884","","Rel-13","37.105","13.2.0","AAS_BS_LTE_UTRA-Core","0020","2","D","RP-162422","","","","",""]
["R4-1609914","Impacts on BS transmitter requirements","Ericsson","Patrizia Testa","66129","discussion","Discussion","This contribution analyzes possible impacts of larger extended CP on BS Requirements","","380","8.33.3","BS RF [MBMS_LTE_enh2-Core]",991400000,"noted","2016-11-04T10:01:26.653","2016-11-07T14:26:14.763","","","Rel-14","","","MBMS_LTE_enh2-Core","","","","","","","","",""]
["R4-1609915","36.104 changes related to EVM due to new extended cyclic prefix","Ericsson","Patrizia Testa","66129","discussion","Discussion","This contribution analyzes impacts of larger cyclic prefix on BS EVM","","380","8.33.3","BS RF [MBMS_LTE_enh2-Core]",991500000,"noted","2016-11-04T10:01:26.683","2016-11-04T16:05:19.633","","","Rel-14","","","MBMS_LTE_enh2-Core","","","","","","","","",""]
["R4-1609916","Introduction 4Rx feature for B40 single carrier and CA_3-40","Huawei, HiSilicon","Huiping Shan","56652","CR","Agreement","This is a coverpage revision of an agreed CR.","","29","5.2.1","UE RF (36.101)  [LTE_4Rx_AP_DL-Core]",987400000,"endorsed","2016-11-04T10:06:07.313","2016-11-04T11:00:30.880","R4-167408","","Rel-14","36.101","14.1.0","LTE_4Rx_AP_DL-Core","3862","1","F","","","","","",""]
["R4-1609917","Consideration of spatial domain on EIRP","DOCOMO Communications Lab.","Kunihiko Teshima","57760","other","Approval","This contribution is for approval.\nIn this contribution, we provide our consideration on how to consider EIRP requirements from a spatial domain point of view.","","417","11.5.2.1","Transmitter characteristics [FS_NR_newRAT]",933800000,"noted","2016-11-04T10:14:48.027","2016-11-04T15:25:23.740","","","","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1609918","CR on UE Transmit Timing Accuracy Tests for NB-IoT UE","NTT DOCOMO, INC.","Kunihiko Teshima","57760","CR","","Endorsed draft CR in #80bis meeting is R4-168800.","","123","6.3.3.6","UE Transmit timing test [NB_IOT-Perf]",991800000,"agreed","2016-11-04T10:25:14.193","2016-11-04T15:25:23.740","","","Rel-13","36.133","13.5.0","NB_IOT-Perf","4236","","B","RP-162379","","","","",""]
["R4-1609919","CR on UE Transmit Timing Accuracy Tests for NB-IoT UE","NTT DOCOMO, INC.","Kunihiko Teshima","57760","CR","","This is a Cat. A CR on UE Transmit Timing Accuracy Tests for NB-IoT UE","","123","6.3.3.6","UE Transmit timing test [NB_IOT-Perf]",991900000,"agreed","2016-11-04T10:28:11.003","2016-11-19T17:47:26.097","","","Rel-14","36.133","14.1.0","NB_IOT-Perf","4237","","A","RP-162379","","","","",""]
["R4-1609920","Licensed band de-sense in eLAA CA combinations","Skyworks Solutions Inc.","Dominique Brunel","65099","discussion","Approval","Propasal to include licensed band spurious harmonic response and IMD2 related de-sense in eLAA CA combination studies.","","246","8.18.2.3","REFSENS [LTE_eLAA-Core]",992000000,"noted","2016-11-04T10:29:39.427","2016-11-04T19:52:40.207","","","Rel-14","","","","","","","","","","","",""]
["R4-1609921","Exclusion range for 10MHz LAA CA combinations","Skyworks Solutions Inc.","Dominique Brunel","65099","discussion","Approval","Proposal for REFSENS exclusion range for B46 10MHz channel LAA CA combinations.","","40","5.4.1","UE RF and EMC [LTE_LAA-Core]",4500000,"withdrawn","2016-11-04T10:32:47.390","2016-11-04T20:24:15.970","","","Rel-14","","","","","","","","","","","",""]
["R4-1609922","Simulation results of TM4 PDSCH for 4Rx CA demodulation tests","NTT DOCOMO INC.","Takuma Takada","64526","discussion","Discussion","This contribution provides our simulation result of TM4 PDSCH for 4Rx CA.","","359","8.30.3.2","Extend existing 2Rx CA requirement to 4Rx [LTE_4Rx_AP_DL_CA-Perf]",992200000,"noted","2016-11-04T10:47:43.033","2016-11-04T13:25:33.933","","","Rel-14","36.101","","LTE_4Rx_AP_DL_CA-Perf","","","","","","","","",""]
["R4-1609923","Discussion on CQI reporting requirements under SFN scenario","NTT DOCOMO INC.","Takuma Takada","64526","other","Approval","This contribution provides our view on the necessity of CQI reporting reuirement under SFN scenario.","","347","8.28.3.3","CQI reporting [LTE_high_speed]",992300000,"noted","2016-11-04T10:53:18.353","2016-11-04T13:25:33.947","","","Rel-14","36.101","","LTE_high_speed-Perf","","","","","","","","",""]
["R4-1609924","Discussion on network assisted signaling of neighbor cell list information","NTT DOCOMO INC.","Takuma Takada","64526","other","Approval","This contribution provides our view on network assisted signaling for neighbor cell list.","","341","8.28.2.1","Enhancement in connected mode (DRX) [LTE_high_speed]",955000000,"noted","2016-11-04T10:57:51.480","2016-11-04T13:25:33.933","","","Rel-14","","","LTE_high_speed-Core","","","","","","","","",""]
["R4-1609925","Corrections to Antenna connection for 4 Rx capable UEs","Ericsson","Christopher Callender","58614","CR","Approval","Coverpage revision of an agreed CR","","30","5.2.2","RRM (36.133) [LTE_4Rx_AP_DL-Core]",992500000,"agreed","2016-11-04T11:01:00.347","2016-11-04T15:31:12.977","R4-167652","","Rel-14","36.133","14.1.0","LTE_4Rx_AP_DL-Perf","3997","1","A","RP-162423","","","","",""]
["R4-1609926","CR for introducing definition of Type-D receiver","NTT DOCOMO INC.","Takuma Takada","64526","CR","Approval","This is CR for introducing new definition of advanced receiver under SFN scenario as Type-D receiver.","","345","8.28.3.1","Enhancement for bi-directional RRH arrangement [LTE_high_speed]",4070000,"revised","2016-11-04T11:02:34.337","2016-11-04T13:25:33.933","","R4-1610713","Rel-14","36.101","14.1.0","LTE_high_speed-Perf","4082","","B","","","","","",""]
["R4-1609927","On Handling CEN DSRC Protection Requirements in Region 1","Qualcomm Europe Inc.(France)","TIen Viet NGUYEN","67205","discussion","Approval","---","","259","8.19.1","UE RF core maintenace (36.101)  [LTE_SL_V2V-Core]",74600000,"noted","2016-11-04T11:07:30.130","2016-11-06T18:59:37.217","","","Rel-14","","","LTE_SL_V2V-Core","","","","","","","","",""]
["R4-1609928","Rayleigh Validation Measurements for the EMITE RC+CE Test Setup with different number of output ports (2/4/5/6/8)","CTTC","David Sanchez-hernandez","44508","other","Discussion","The project plan for completing the RC+CE validation procedures was approved at the 3GPP RAN4#78bis meeting [1]. At the RAN4#79 meeting, an update on the Rayleigh fading validation procedure which includes test tolerances for the Reverberation Chamber met","","224","8.14.3","Harmonization [LTE_MIMO_OTA-Core]",933900000,"noted","2016-11-04T11:08:45.773","2016-11-04T21:26:19.993","","","Rel-13","37.977","","","","","","","","","","",""]
["R4-1609929","Improvement of REFSENS requirement specification for band 46 CA combos","QUALCOMM UK Ltd","Marco Papaleo","49190","CR","Agreement","Coverpage revision of an agreed CR","","40","5.4.1","UE RF and EMC [LTE_LAA-Core]",992900000,"agreed","2016-11-04T11:19:33.050","2016-11-04T11:25:57.153","R4-168824","","Rel-13","36.101","13.5.0","LTE_LAA-Core","3866","2","F","RP-162428","","","","",""]
["R4-1609930","Improvement of REFSENS requirement specification for band 46 CA combos","Qualcomm Incorporated","Marco Papaleo","49190","CR","Agreement","Coverpage revision of an agreed CR","","40","5.4.1","UE RF and EMC [LTE_LAA-Core]",993000000,"agreed","2016-11-04T11:27:06.090","2016-11-04T11:29:58.813","R4-168825","","Rel-14","36.101","14.1.0","LTE_LAA-Core","3868","2","F","RP-162428","","","","",""]
["R4-1609931","Addition of missing source of IMD for 2UL-2DL CA","Qualcomm Incorporated","Antti Immonen","62092","CR","","Cover page revision of agreed CR","","177","8.6.2","UE RF (36.101) [LTE_CA_R14_2DL2UL-Core]",17800000,"agreed","2016-11-04T11:30:07.953","2016-11-04T11:35:12.887","R4-168343","","Rel-14","36.101","14.1.0","LTE_CA_R14_2DL2UL","3949","1","F","RP-162403","","","","",""]
["R4-1609932","Clarification of note6 for 3DL/2UL and 4DL/2UL CA","Huawei, Hisilicon, KDDI","Antti Immonen","62092","CR","","Cover page revision of agreed CR","","183","8.7.2","UE RF (36.101) [LTE_CA_R14_xDL2UL-Core]",77300000,"agreed","2016-11-04T11:33:29.333","2016-11-04T11:35:12.870","R4-168963","","Rel-14","36.101","14.1.0","LTE_CA_R14_xDL2UL","3946","3","F","RP-162404","","","","",""]
["R4-1609933","Receiver blocking requirement","Ericsson","Thomas Chapman","46692","other","Discussion","Follow up discussion document on RX blocking after discussions at RAN4#80bis","","209","8.12.2.1","In band requirements [AASenh_BS_LTE_UTRA]",993900000,"noted","2016-11-04T11:49:15.317","2016-11-04T16:47:20.467","","","Rel-14","","","AASenh_BS_LTE_UTRA","","","","","","","","",""]
["R4-1609934","RX intermodulation requirement","Ericsson","Thomas Chapman","46692","other","Discussion","Follow up discussion document on RX intermodulation after discussions at RAN4#80bis","","209","8.12.2.1","In band requirements [AASenh_BS_LTE_UTRA]",998100000,"noted","2016-11-04T11:49:15.333","2016-11-04T16:47:20.467","","","Rel-14","","","AASenh_BS_LTE_UTRA","","","","","","","","",""]
["R4-1609935","TP to 37.843: Background information on conducted ACLR requirement","Ericsson","Thomas Chapman","46692","other","Approval","Background information on how the conducted ALCR is structured and decided","","209","8.12.2.1","In band requirements [AASenh_BS_LTE_UTRA]",3990000,"revised","2016-11-04T11:49:15.350","2016-11-04T16:47:20.467","","R4-1610802","","","","AASenh_BS_LTE_UTRA","","","","","","","","",""]
["R4-1609936","TP to 37.843: Background information on conducted EVM requirement","Ericsson","Thomas Chapman","46692","other","Approval","Background information on how the conducted EVM is structured and decided","","209","8.12.2.1","In band requirements [AASenh_BS_LTE_UTRA]",972800000,"noted","2016-11-04T11:49:15.367","2016-11-04T16:47:20.467","","R4-1610806","","","","AASenh_BS_LTE_UTRA","","","","","","","","",""]
["R4-1609937","TP to 37.843: Background information on conducted RX blocking requirement","Ericsson","Thomas Chapman","46692","other","Approval","Background information on how the conducted RX blocking is structured and decided","","209","8.12.2.1","In band requirements [AASenh_BS_LTE_UTRA]",998000000,"noted","2016-11-04T11:49:15.397","2016-11-04T16:47:20.467","","","","","","AASenh_BS_LTE_UTRA","","","","","","","","",""]
["R4-1609938","TP to 37.843: Background information on conducted RX sensitivity requirement","Ericsson","Thomas Chapman","46692","other","Approval","Background information on how the conducted RX sensitivity is structured and decided","","209","8.12.2.1","In band requirements [AASenh_BS_LTE_UTRA]",993500000,"approved","2016-11-04T11:49:15.413","2016-11-04T16:47:20.483","","","","","","AASenh_BS_LTE_UTRA","","","","","","","","",""]
["R4-1609939","BS output power requirement","Ericsson","Thomas Chapman","46692","other","Approval","Metrics needed for BS output power requirement","","209","8.12.2.1","In band requirements [AASenh_BS_LTE_UTRA]",137000,"noted","2016-11-04T11:49:15.427","2016-11-04T16:47:20.483","","","Rel-14","","","AASenh_BS_LTE_UTRA","","","","","","","","",""]
["R4-1609940","Further consideration on BS ACS aspects","Ericsson","Thomas Chapman","46692","other","Discussion","Consideration about ACS spatial aspects and blocking","","422","11.5.3.2","Receiver characteristics [FS_NR_newRAT]",35800000,"noted","2016-11-04T11:49:15.457","2016-11-04T16:47:20.450","","","Rel-14","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1609941","BS classes for NR","Ericsson","Thomas Chapman","46692","other","Approval","Considerations and proposals on BS classes","","420","11.5.3","BS RF  [FS_NR_newRAT]",927000000,"noted","2016-11-04T11:49:15.473","2016-11-04T16:47:20.437","","","Rel-14","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1609942","On UE ACLR metric","Ericsson","Thomas Chapman","46692","other","Discussion","Aspects to consider for UE ACLR metric","","417","11.5.2.1","Transmitter characteristics [FS_NR_newRAT]",994200000,"noted","2016-11-04T11:49:15.507","2016-11-04T16:47:20.437","","","Rel-14","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1609943","Review of NR and eAAS synergies","Ericsson","Thomas Chapman","46692","other","Approval","Proposal on what to discuss in eAAS and what in NR","","420","11.5.3","BS RF  [FS_NR_newRAT]",57500000,"noted","2016-11-04T11:49:15.537","2016-11-04T16:47:20.450","","","Rel-14","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1609944","TP to 38.803: ACLR & ACS assumptions for simulation","Ericsson","Thomas Chapman","46692","pCR","Approval","Additions to the text on ACLR/ACS assumption","","412","11.3.3","others  [FS_NR_newRAT]",994400000,"revised","2016-11-04T11:49:15.553","2016-11-04T16:47:20.450","","R4-1610573","","38.803","0.3.0","FS_NR_newRAT","","","","","","","","",""]
["R4-1609945","Further elaboration on NR guard","Ericsson","Thomas Chapman","46692","other","Discussion","Considerations on windowing & guard band","","415","11.5.1","Common issues for UE and BS [FS_NR_newRAT]",922300000,"noted","2016-11-04T11:49:15.567","2016-11-04T16:37:37.510","","","Rel-14","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1609946","On LS for maximum carrier bandwidths for NR","Ericsson","Thomas Chapman","46692","other","Discussion","Considerations on how to support a wider bandwidth","","407","11.1","General   [FS_NR_newRAT]",926900000,"noted","2016-11-04T11:49:15.600","2016-11-04T16:37:37.573","","","Rel-14","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1609947","Draft reply LS on wider bandwidth operation for NR","Ericsson","Thomas Chapman","46692","LS out","Approval","Reply to the RAN1 incoming LS","","407","11.1","General   [FS_NR_newRAT]",941500000,"revised","2016-11-04T11:49:15.613","2016-11-04T16:47:20.450","","R4-1610591","Rel-14","","","FS_NR_newRAT","","","","","R1-1610655","RAN1","RAN2","R1-1610655",""]
["R4-1609948","On mm wave ACLR for 45 and 70 GHZ","Ericsson","Thomas Chapman","46692","other","Approval","ACLR supported by feasible technologies","","415","11.5.1","Common issues for UE and BS [FS_NR_newRAT]",994800000,"withdrawn","2016-11-04T11:49:15.647","2016-11-04T16:37:37.573","","","Rel-14","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1609949","NR BS requirement overview for mm wave","Ericsson","Thomas Chapman","46692","other","Approval","Further discussion on requirement applicability","","420","11.5.3","BS RF  [FS_NR_newRAT]",61900000,"noted","2016-11-04T11:49:15.660","2016-11-04T16:37:37.590","","","Rel-14","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1609950","On mm wave phase noise","Ericsson","Thomas Chapman","46692","other","Discussion","Discussions on phase noise","","415","11.5.1","Common issues for UE and BS [FS_NR_newRAT]",48300000,"noted","2016-11-04T11:49:15.677","2016-11-04T16:37:37.590","","","Rel-14","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1609951","RF testing of NR mobile devices","Sony Mobile Communications","Thomas Bolin","58174","other","Approval","It is proposed mobile UE RF testing (OTA) to be conducted such that the entire sphere surrounding the UE is covered rather than at just one direction only.","","417","11.5.2.1","Transmitter characteristics [FS_NR_newRAT]",959100000,"noted","2016-11-04T11:50:58.153","2016-11-04T16:37:48.960","","","","","","","","","","","","","","",""]
["R4-1609952","Remaining Issues in V2V RF Specifications","Qualcomm Europe Inc.(France)","TIen Viet NGUYEN","67205","discussion","Approval","---","","263","8.19.1.4","Others",75100000,"noted","2016-11-04T11:52:39.303","2016-11-07T21:15:32.237","","","Rel-14","","","LTE_SL_V2V-Core","","","","","","","","",""]
["R4-1609953","MSD for 3+8 2UL CA","Huawei, Hisilicon","Antti Immonen","62092","other","Approval","This contribution discusses MSD requirements for 3+8 UL CA.","","12","4.2.1","UE RF (core / EMC)  [WI code or TEI12]",129000,"revised","2016-11-04T11:54:53.293","2016-11-04T12:46:51.233","","R4-1610764","","","","","","","","","","","","",""]
["R4-1609954","MSD for 28+42 2UL CA","Huawei, Hisilicon","Antti Immonen","62092","other","Approval","This contribution discusses MSD requirements for 28+42 UL CA.","","177","8.6.2","UE RF (36.101) [LTE_CA_R14_2DL2UL-Core]",18200000,"revised","2016-11-04T11:56:57.390","2016-11-04T12:46:51.233","","R4-1610765","","","","","","","","","","","","",""]
["R4-1609955","MSD for 21+28 2UL CA","Huawei, Hisilicon","Antti Immonen","62092","other","Approval","This contribution discusses MSD requirements for 21+28 UL CA.","","177","8.6.2","UE RF (36.101) [LTE_CA_R14_2DL2UL-Core]",76600000,"revised","2016-11-04T11:58:35.513","2016-11-04T12:46:51.233","","R4-1610768","","","","","","","","","","","","",""]
["R4-1609956","MSD for 5+66 2UL CA","Huawei, Hisilicon","Antti Immonen","62092","other","Approval","This contribution discusses MSD requirements for 5+66 UL CA.","","177","8.6.2","UE RF (36.101) [LTE_CA_R14_2DL2UL-Core]",77000000,"noted","2016-11-04T12:00:31.767","2016-11-04T12:46:51.247","","","","","","","","","","","","","","",""]
["R4-1609957","CR for fixing errors for 4Rx tests in Rel-13","Ericsson","Maomao Chen","46060","CR","Approval","Second revision to fix the cover sheet","","33","5.2.3.2","UE demodulation and CSI [LTE_4Rx_AP_DL-Perf]",995700000,"agreed","2016-11-04T12:01:32.557","2016-11-04T13:54:50.710","R4-168633","","Rel-13","36.101","13.5.0","LTE_4Rx_AP_DL-Perf","3956","2","F","RP-162423","","","","",""]
["R4-1609958","Way forward on aligning the AAS and non-AAS BS specifications","Ericsson","Aurelian Bria","40914","discussion","Agreement","Proposal for a strategy to align AAS and non-AAS BS specifications.","","21","5.1","Base Station (BS) RF requirements for Active Antenna System (AAS) [AAS_BS_LTE_UTRA-Core]",3850000,"noted","2016-11-04T12:01:52.947","2016-11-04T18:35:55.540","","","Rel-13","","","AAS_BS_LTE_UTRA","","","","","","","","",""]
["R4-1609959","TS 37.105: Removal of operating band unwanted emissions for Band 46","Ericsson","Aurelian Bria","40914","CR","Agreement","LAA operation in Band 46 is not fully supported in TS 37.105 and section 6.6.5.4.6 was probably added by mistake","","23","5.1.2","BS RF(37.105) [AAS_BS_LTE_UTRA-Core]",4320000,"revised","2016-11-04T12:01:52.963","2016-11-04T18:35:55.557","","R4-1610795","Rel-13","37.105","13.2.0","AAS_BS_LTE_UTRA","0021","","F","","","","","",""]
["R4-1609960","TS 37.105: Corrections","Ericsson","Aurelian Bria","40914","CR","Approval","Corrections","","23","5.1.2","BS RF(37.105) [AAS_BS_LTE_UTRA-Core]",991200001,"noted","2016-11-04T12:01:53.040","2016-11-04T18:35:55.527","","","Rel-13","37.105","13.2.0","AAS_BS_LTE_UTRA","0022","","F","","","","","",""]
["R4-1609961","TS 37.105:Introduction of rel-13 bands: 45,65, 66, 67 and 68","Ericsson","Aurelian Bria","40914","CR","Approval","Introduction of rel-13 bands: 45, 65, 66, 67 and 68","","23","5.1.2","BS RF(37.105) [AAS_BS_LTE_UTRA-Core]",991300000,"noted","2016-11-04T12:01:53.137","2016-11-04T18:35:55.527","","","Rel-13","37.105","13.2.0","AAS_BS_LTE_UTRA","0023","","B","","","","","",""]
["R4-1609962","TS 37.145-1: Corrections","Ericsson","Aurelian Bria","40914","CR","Approval","Corrections","","25","5.1.3.1","Maintenance for TS37.145-1 [AAS_BS_LTE_UTRA-Perf]",4330000,"revised","2016-11-04T12:01:53.227","2016-11-04T18:35:55.540","","R4-1610797","Rel-13","37.145-1","13.0.0","AAS_BS_LTE_UTRA","0006","","F","","","","","",""]
["R4-1609963","MSD for 2+66 2UL CA","Huawei, Hisilicon","Antti Immonen","62092","other","Approval","This contribution discusses MSD requirements for 2+66 UL CA.","","177","8.6.2","UE RF (36.101) [LTE_CA_R14_2DL2UL-Core]",995600000,"revised","2016-11-04T12:02:29.407","2016-11-04T12:46:51.247","","R4-1610770","","","","","","","","","","","","",""]
["R4-1609964","UE E-UTRA bands TRP/TRS requirements proposal","Sony Mobile Communications","Thomas Bolin","58174","discussion","Approval","UE TRP/TRS requirements are proposed","","218","8.13.2","Hand phantom for smartphones [LTE_UTRA_TRP_TRS-Core]",27700000,"withdrawn","2016-11-04T12:02:46.957","2016-11-04T16:37:48.960","","","","","","","","","","","","","","",""]
["R4-1609965","CR for fixing errors for 4Rx tests in Rel-14","Ericsson","Maomao Chen","46060","CR","Approval","CR","","33","5.2.3.2","UE demodulation and CSI [LTE_4Rx_AP_DL-Perf]",996500000,"agreed","2016-11-04T12:03:09.480","2016-11-04T13:54:50.710","R4-168439","","Rel-14","36.101","14.1.0","LTE_4Rx_AP_DL-Perf","3957","1","A","RP-162423","","","","",""]
["R4-1609966","TP for TR36.714-02-02: UL CA analysis results","Huawei Tech.(UK) Co., Ltd","Antti Immonen","62092","pCR","","This is a TP to include MSD analysis for all approved 2Ul/2DL CA combinations","","177","8.6.2","UE RF (36.101) [LTE_CA_R14_2DL2UL-Core]",996600000,"withdrawn","2016-11-04T12:06:39.300",null,"","","","36.714-02-02","0.5.0","","","","","","","","","",""]
["R4-1609967","CR for V2V UE RF requirements to support CEN DSRC protection techniques","Qualcomm Europe Inc.(France)","TIen Viet NGUYEN","67205","draftCR","Approval","---","","259","8.19.1","UE RF core maintenace (36.101)  [LTE_SL_V2V-Core]",937200000,"revised","2016-11-04T12:08:08.190","2016-11-06T19:25:59.227","","R4-1610747","Rel-14","36.101","14.1.0","LTE_SL_V2V-Core","","","","","","","","",""]
["R4-1609968","Remaining issues in multi-node tests for LAA Wi-Fi coexistence","Broadcom, CableLabs, Hewlett Packard Enterprise, Marvell, Microsoft, Orange","Shubhodeep Adhikari","62546","discussion","Decision","This contribution contains proposals for the important unresolved issues in the LAA – Wi-Fi coexistence tests.","","140","7.1.2","Multi-node testing [FS_LTE_LAA_multinode_test]",4620000,"noted","2016-11-04T12:09:02.197","2016-11-07T19:04:43.953","","","","","","","","","","","","","","",""]
["R4-1609969","TP for TR36.714-00-02: xDL/2UL CA analysis results","Huawei, Hisilicon","Antti Immonen","62092","pCR","","This TP includes MSD analysis results from all approved xDL/2UL CA combinations","","183","8.7.2","UE RF (36.101) [LTE_CA_R14_xDL2UL-Core]",77400000,"approved","2016-11-04T12:09:45.737","2016-11-19T17:47:26.097","","","","36.714-00-02","0.5.0","","","","","","","","","",""]
["R4-1609970","MSD for 1+5+46 2UL/3DL CA","Huawei, Hisilicon","Antti Immonen","62092","other","Approval","This contribution discusses MSD requirements for 1+5+46 2UL/3DL CA.","","183","8.7.2","UE RF (36.101) [LTE_CA_R14_xDL2UL-Core]",978800000,"noted","2016-11-04T12:11:33.597","2016-11-04T12:46:51.247","","","","","","","","","","","","","","",""]
["R4-1609971","MSD for 1+7+46 2UL/3DL CA","Huawei, Hisilicon","Antti Immonen","62092","other","Approval","This contribution discusses MSD requirements for 1+7+46 2UL/3DL CA.","","183","8.7.2","UE RF (36.101) [LTE_CA_R14_xDL2UL-Core]",77200000,"noted","2016-11-04T12:13:13.357","2016-11-04T12:46:51.247","","","","","","","","","","","","","","",""]
["R4-1609972","MSD for 5+7+46 2UL/3DL CA","Huawei, Hisilicon","Antti Immonen","62092","other","","This contribution discusses MSD requirements for 5+7+46 2UL/3DL CA.","","183","8.7.2","UE RF (36.101) [LTE_CA_R14_xDL2UL-Core]",979000000,"noted","2016-11-04T12:14:58.767","2016-11-04T12:46:51.263","","","","","","","","","","","","","","",""]
["R4-1609973","Device selection and configuration for LAA multi-node tests","BROADCOM CORPORATION","Shubhodeep Adhikari","62546","discussion","","LAA multi-node tests are being studied by RAN4. A WF on some fundamental aspects of device selection and configuration for the multi-node tests has been approved in RAN4#80BIS. In this contribution, we propose additional details which build on these agree","","140","7.1.2","Multi-node testing [FS_LTE_LAA_multinode_test]",960700000,"available","2016-11-04T12:15:14.053","2016-11-07T19:04:43.953","","","","","","","","","","","","","","",""]
["R4-1609974","MSD for 3+5+7 2UL/3DL CA","Huawei, Hisilicon","Antti Immonen","62092","other","","This contribution discusses MSD requirements for 3+5+7 2UL/3DL CA.","","183","8.7.2","UE RF (36.101) [LTE_CA_R14_xDL2UL-Core]",993200000,"revised","2016-11-04T12:16:37.983","2016-11-04T12:46:51.263","","R4-1610772","","","","","","","","","","","","",""]
["R4-1609975","MSD for 1+3+42 2UL/3DL CA","Huawei, Hisilicon","Antti Immonen","62092","other","Approval","This contribution discusses MSD requirements for 1+3+42 2UL/3DL CA.","","183","8.7.2","UE RF (36.101) [LTE_CA_R14_xDL2UL-Core]",997000000,"revised","2016-11-04T12:18:52.440","2016-11-04T12:46:51.263","","R4-1610912","","","","","","","","","","","","",""]
["R4-1609976","MSD for 3+19+21 2UL/3DL CA","Huawei, Hisilicon","Antti Immonen","62092","other","","This contribution discusses MSD requirements for 3+19+21 2UL/3DL CA.","","183","8.7.2","UE RF (36.101) [LTE_CA_R14_xDL2UL-Core]",997100000,"revised","2016-11-04T12:20:38.847","2016-11-04T12:46:51.263","","R4-1610773","","","","","","","","","","","","",""]
["R4-1609977","Non-user specific beams and EVM","Ericsson","Esther Sienkiewicz","59234","discussion","Approval","During the last meeting RAN4#80bis in Ljubljana, a WF on EVM was agreed. The following aspects have been agreed for OTA EVM:\n• Manufacturer declares the intended EVM directions range.\n• The BS shall meet the OTA EVM requirement across the declared EVM dir","","209","8.12.2.1","In band requirements [AASenh_BS_LTE_UTRA]",4990000,"noted","2016-11-04T12:22:10.653","2016-11-04T19:00:01.723","","","Rel-14","","","AASenh_BS_LTE_UTRA","","","","","","","","",""]
["R4-1609978","CR to TS 37.842: Replacement of factor for independent contributions","Ericsson","Esther Sienkiewicz","59234","CR","Approval","This CR adds the description for the factor Ci used in uncertainty budget calculations","","22","5.1.1","Technical Report (37.842) [AAS_BS_LTE_UTRA-Core]",988900000,"noted","2016-11-04T12:22:10.667","2016-11-04T18:49:16.627","","","Rel-13","37.842","13.0.0","AAS_BS_LTE_UTRA-Perf","0010","","F","","","","","",""]
["R4-1609979","Further elaboration on practical measurement Grids for ACLR and unwanted emissions","Ericsson","Esther Sienkiewicz","59234","discussion","Discussion","During the last meeting RAN4#80bis in Ljubljana, a discussion regarding TRP sampling grid for spatial ACLR was discussed [1].  The background and definition of TRP was described whilst showing the effect of removal of measurement points for EIRP to provid","","209","8.12.2.1","In band requirements [AASenh_BS_LTE_UTRA]",3910000,"noted","2016-11-04T12:22:10.763","2016-11-04T19:39:28.283","","","Rel-14","","","AASenh_BS_LTE_UTRA","","","","","","","","",""]
["R4-1609980","On the measurement grid density needs for estimating TRP for different types of unwanted emissions","Ericsson","Esther Sienkiewicz","59234","discussion","Discussion","During the last meeting RAN4#80bis in Ljubljana, a WF on OTA ACLR definition was approved.  Within this way forward a list of open issues was defined for consideration for coming meetings.  Specifically, to “determine if the measurement sampling grid for","","209","8.12.2.1","In band requirements [AASenh_BS_LTE_UTRA]",3930000,"noted","2016-11-04T12:22:10.777","2016-11-04T19:39:28.283","","","Rel-14","","","AASenh_BS_LTE_UTRA","","","","","","","","",""]
["R4-1609981","Proposal on how to restrict measurement directions for TRP estimation of a wanted carrier","Ericsson","Esther Sienkiewicz","59234","discussion","Approval","During the last meeting RAN4#80bis in Ljubljana, a WF [1] on OTA ACLR definition was approved.  During which time several open issues were to be considered for the coming meetings.  More specifically the need to:","","209","8.12.2.1","In band requirements [AASenh_BS_LTE_UTRA]",3950000,"noted","2016-11-04T12:22:10.793","2016-11-04T19:40:59.887","","","Rel-14","","","AASenh_BS_LTE_UTRA","","","","","","","","",""]
["R4-1609982","Spurious emissions measurement grid","Ericsson","Esther Sienkiewicz","59234","discussion","Discussion","Current requirements for in band spurious emissions require measurements at the connector.  For eAAS, OTA measurements for spurious emissions shall be considered using (approximated) TRP as the metric.","","209","8.12.2.1","In band requirements [AASenh_BS_LTE_UTRA]",3960000,"noted","2016-11-04T12:22:10.823","2016-11-04T19:40:59.900","","","Rel-14","","","AASenh_BS_LTE_UTRA","","","","","","","","",""]
["R4-1609983","Received SIR in multi-node tests for LAA Wi-Fi coexistence","BROADCOM CORPORATION","Shubhodeep Adhikari","62546","discussion","","This contribution discusses the appropriate value of the received Signal-to-Interference (SIR) at the victim receiver for use in the LAA – Wi-Fi coexistence tests.","","140","7.1.2","Multi-node testing [FS_LTE_LAA_multinode_test]",996800000,"available","2016-11-04T12:22:20.230","2016-11-07T19:04:43.953","","","","","","","","","","","","","","",""]
["R4-1609984","MSD for 3+19+42 2UL/3DL CA","Huawei, Hisilicon","Antti Immonen","62092","other","Approval","This contribution discusses MSD requirements for 3+19+42 2UL/3DL CA.","","183","8.7.2","UE RF (36.101) [LTE_CA_R14_xDL2UL-Core]",997400000,"noted","2016-11-04T12:22:20.840","2016-11-04T12:46:51.263","","","","","","","","","","","","","","",""]
["R4-1609985","Discussion on reference receiver for BS IC","ZTE","Qian Yang","45032","discussion","Discussion","---","","397","9.4.3","Reference receiver [FS_LTE _IC_BS]",945600000,"noted","2016-11-04T12:22:24.427","2016-11-04T13:00:23.120","","","Rel-14","","","FS_LTE_IC_BS","","","","","","","","",""]
["R4-1609986","Discussion on interference model for BS IC","ZTE","Qian Yang","45032","discussion","Discussion","---","","398","9.4.4","Interference model [FS_LTE _IC_BS]",998600000,"noted","2016-11-04T12:22:24.457","2016-11-04T13:00:23.137","","","Rel-14","","","FS_LTE_IC_BS","","","","","","","","",""]
["R4-1609987","MSD for 19+21+42 2UL/3DL CA","Huawei, Hisilicon","Antti Immonen","62092","other","Approval","This contribution discusses MSD requirements for 19+21+42 2UL/3DL CA.","","183","8.7.2","UE RF (36.101) [LTE_CA_R14_xDL2UL-Core]",997500000,"revised","2016-11-04T12:24:01.273","2016-11-04T12:46:51.280","","R4-1610774","","","","","","","","","","","","",""]
["R4-1609988","B46 MOP tolerance","Huawei, Hisilicon","Antti Immonen","62092","other","Approval","This contribution analyses B46 MOP (Maximum Output Power) tolerance according to WF [1] and proposes which value should be used.","","247","8.18.2.4","Other requirements [LTE_eLAA-Core]",4740000,"noted","2016-11-04T12:26:52.623","2016-11-10T09:49:29.917","","","","","","","","","","","","","","",""]
["R4-1609989","CA_3A-3A REFSENS","Huawei, Hisilicon","Antti Immonen","62092","other","Approval","This contribution analyses REFSENS for intra-band non-contiguous CA on B3 (CA_3A-3A).","","147","8.1.2","UE RF (36.101) [LTE_CA_R14_intra-Core]",998900000,"noted","2016-11-04T12:28:17.423","2016-11-04T12:46:51.280","","","","","","","","","","","","","","",""]
["R4-1609990","Summary results for TDD-FDD CA soft buffer tests","Ericsson","Maomao Chen","46060","discussion","Discussion","Discussion","","15","4.2.4","UE demodulation performance  [WI code or TEI12]",37600000,"noted","2016-11-04T12:33:49.657","2016-11-04T13:54:50.727","","","Rel-12","","","TEI12","","","","","","","","",""]
["R4-1609991","CR for fixing soft buffer test for TDD-FDD CA in Rel-12","Ericsson","Maomao Chen","46060","CR","Approval","CR","","15","4.2.4","UE demodulation performance  [WI code or TEI12]",37700000,"revised","2016-11-04T12:33:49.673","2016-11-04T13:54:50.727","","R4-1610858","Rel-12","36.101","12.13.0","TEI12","4083","","F","","","","","",""]
["R4-1609992","CR for fixing soft buffer management test for TDD-FDD CA in Rel-13","Ericsson","Maomao Chen","46060","CR","Approval","CR","","15","4.2.4","UE demodulation performance  [WI code or TEI12]",37800000,"agreed","2016-11-04T12:33:49.797","2016-11-22T09:27:26.277","","","Rel-13","36.101","13.5.0","TEI12","4084","","A","RP-162420","","","","",""]
["R4-1609993","CR for fixing soft buffer test for TDD-FDD CA in Rel-14","Ericsson","Maomao Chen","46060","CR","Approval","CR","","15","4.2.4","UE demodulation performance  [WI code or TEI12]",38200000,"revised","2016-11-04T12:33:49.907","2016-11-22T09:27:26.277","","R4-1611018","Rel-14","36.101","14.1.0","TEI12","4085","","A","","","","","",""]
["R4-1609994","CR for fixing editorial errors in Rel-13","Ericsson","Maomao Chen","46060","CR","Approval","CR","","15","4.2.4","UE demodulation performance  [WI code or TEI12]",94910000,"revised","2016-11-04T12:33:50","2016-11-04T13:54:50.727","","R4-1610720","Rel-13","36.101","13.5.0","TEI13","4086","","F","","","","","",""]
["R4-1609995","CR for fixing editorial errors in Rel-14","Ericsson","Maomao Chen","46060","CR","Approval","CR","","15","4.2.4","UE demodulation performance  [WI code or TEI12]",99900000,"revised","2016-11-04T12:33:50.093","2016-11-22T09:27:26.277","","R4-1611015","Rel-14","36.101","14.1.0","TEI13","4087","","A","","","","","",""]
["R4-1609996","Work plan for performance part of Rel-14 4Rx CA WI","Ericsson","Maomao Chen","46060","other","Approval","Approval","","357","8.30.3","UE demodulation (36.101) [LTE_4Rx_AP_DL_CA-Perf]",971300000,"approved","2016-11-04T12:33:50.187","2016-11-04T13:54:50.727","","","Rel-14","","","LTE_4Rx_AP_DL_CA","","","","","","","","",""]
["R4-1609997","General test structure and applicability rule for normal demod and CSI tests with 4Rx CA","Ericsson","Maomao Chen","46060","discussion","Discussion","Discussion","","358","8.30.3.1","Applicability [LTE_4Rx_AP_DL_CA-Perf]",906300000,"noted","2016-11-04T12:33:50.220","2016-11-04T13:54:50.743","","","Rel-14","","","LTE_4Rx_AP_DL_CA-Perf","","","","","","","","",""]
["R4-1609998","Simulation results for normal demod tests for 4Rx CA","Ericsson","Maomao Chen","46060","discussion","Discussion","Discussion","","359","8.30.3.2","Extend existing 2Rx CA requirement to 4Rx [LTE_4Rx_AP_DL_CA-Perf]",999800000,"noted","2016-11-04T12:33:50.233","2016-11-04T13:54:50.743","","","Rel-14","","","LTE_4Rx_AP_DL_CA-Perf","","","","","","","","",""]
["R4-1609999","Summary of alignment and impairment results for normal demod tests for 4Rx CA","Ericsson","Maomao Chen","46060","discussion","Discussion","Discussion","","359","8.30.3.2","Extend existing 2Rx CA requirement to 4Rx [LTE_4Rx_AP_DL_CA-Perf]",5240000,"revised","2016-11-04T12:33:50.267","2016-11-04T13:54:50.743","","R4-1610705","Rel-14","","","LTE_4Rx_AP_DL_CA-Perf","","","","","","","","",""]
["R4-1610000","CR for introducing new demod tests for 4Rx CA in Rel-14","Ericsson, Qualcomm","Maomao Chen","46060","CR","Approval","CR","","359","8.30.3.2","Extend existing 2Rx CA requirement to 4Rx [LTE_4Rx_AP_DL_CA-Perf]",999900000,"revised","2016-11-04T12:33:50.280","2016-11-04T13:54:50.743","","R4-1610856","Rel-14","36.101","14.1.0","LTE_4Rx_AP_DL_CA-Perf","4088","","B","","","","","",""]
["R4-1610001","General test structure and applicability rule for IRC tests with 4Rx CA","Ericsson","Maomao Chen","46060","discussion","Discussion","Discussion","","360","8.30.3.3","Extend MMSE-IRC requirement from 2Rx to 4Rx [LTE_4Rx_AP_DL_CA-Perf]",906200000,"noted","2016-11-04T12:33:50.390","2016-11-04T13:54:50.743","","","Rel-14","","","LTE_4Rx_AP_DL_CA-Perf","","","","","","","","",""]
["R4-1610002","Test structure and applicability rule for 256QAM 1/2 layers and high layer tests for 4Rx CA","Ericsson","Maomao Chen","46060","discussion","Discussion","Discussion","","361","8.30.3.4","3/4-layer 4Rx CA requirement [LTE_4Rx_AP_DL_CA-Perf]",5250000,"noted","2016-11-04T12:33:50.407","2016-11-04T13:54:50.757","","","Rel-14","","","LTE_4Rx_AP_DL_CA-Perf","","","","","","","","",""]
["R4-1610003","Evaluation results for eSU-MIMO","Ericsson","Maomao Chen","46060","discussion","Discussion","Discussion","","370","8.31.3.1","Performance evaluation: scenarios and receiver [LTE_eCRSIM_eSUMIMO]",975900000,"withdrawn","2016-11-04T12:33:50.423",null,"","","Rel-14","","","LTE_eCRSIM_eSUMIMO","","","","","","","","",""]
["R4-1610004","Evaluation results for eCRS-IM","Ericsson","Maomao Chen","46060","discussion","Discussion","Discussion","","367","8.31.2.1","Performance evaluation: scenarios and receiver [LTE_eCRSIM_eSUMIMO]",975700000,"withdrawn","2016-11-04T12:33:50.453",null,"","","Rel-14","","","LTE_eCRSIM_eSUMIMO","","","","","","","","",""]
["R4-1610005","Performance requirements for SRS switching","Ericsson","Maomao Chen","46060","discussion","Discussion","Discussion","","292","8.21.4","UE/BS demodulation (36.101/36.104/36.141) [LTE_SRS_switch-Perf]",500,"noted","2016-11-04T12:33:50.467","2016-11-04T13:54:50.757","","","Rel-14","","","LTE_SRS_switch-Perf","","","","","","","","",""]
["R4-1610006","NR blocking requirements for mmWave","Huawei, Hisilicon","Antti Immonen","62092","discussion","","This contribution discusses NR blocking requirements for mmWave.","","418","11.5.2.2","Receiver characteristics [FS_NR_newRAT]",975600000,"noted","2016-11-04T12:34:55.520","2016-11-04T12:46:51.280","","","","","","","","","","","","","","",""]
["R4-1610007","TP for TR 36.714-00-02: MSD for CA_3A-7A-8A 3DL with CA_3A-7A and CA_3A-8A 2UL CA","CHTTL","Bo-Han Hsieh","61837","pCR","Approval","Text proposal for TR 36.714-00-02 to capture and summarize the current MSD study for this combination.","","183","8.7.2","UE RF (36.101) [LTE_CA_R14_xDL2UL-Core]",998400000,"approved","2016-11-04T12:50:44.733","2016-11-07T06:04:21.590","","","","36.714-00-02","0.5.0","","","","","","","","","",""]
["R4-1610008","TP for TR 36.714-00-02: MSD for CA_3A-7A-8A 3DL with CA_3A-7A and CA_3A-8A 2UL CA","CHTTL","Bo-Han Hsieh","61837","pCR","Approval","Text proposal for TR 36.714-00-02 to capture and summarize the current MSD studies for this combination.","","183","8.7.2","UE RF (36.101) [LTE_CA_R14_xDL2UL-Core]",998700000,"withdrawn","2016-11-04T12:50:49.320",null,"","","","36.714-00-02","0.5.0","","","","","","","","","",""]
["R4-1610009","5G NR coexistence calibration in urban macro scenario","HuaWei Technologies Co., Ltd","Xiang (Steven) Chen","41576","other","Discussion","---","","410","11.3.1","Co-existence [FS_NR_newRAT]",568000,"noted","2016-11-04T12:51:39.223","2016-11-04T15:25:33.710","","","Rel-14","","","","","","","","","","","",""]
["R4-1610010","Link budget considerations for radiated modulation quality measurements","ROHDE & SCHWARZ","Johannes Koebele","49481","discussion","Discussion","This contribution is focusing on the measurement link budget that is required for EUT (equipment under test) transmit signal quality measurements.","","419","11.5.2.3","Testability [FS_NR_newRAT]",916100000,"noted","2016-11-04T12:53:47.083","2016-11-04T18:15:28.603","","","","","","","","","","","","","","",""]
["R4-1610011","CR on PHR requirement for NB-IoT","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","Approval","remove [] in endorsed CR: R4-168782","","119","6.3.3.2","Power headroom [NB_IOT-Perf]",1100,"revised","2016-11-04T12:58:30.567","2016-11-07T19:39:39.970","","R4-1610577","Rel-13","36.133","13.5.0","","4238","","F","","","","","",""]
["R4-1610012","CR on PHR requirement for NB-IoT R14","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","Approval","---","","119","6.3.3.2","Power headroom [NB_IOT-Perf]",57700,"agreed","2016-11-04T12:58:30.673","2016-11-22T12:17:27.080","","","Rel-14","36.133","14.1.0","NB_IOT-Perf","4239","","A","RP-162379","","","","",""]
["R4-1610013","CR on NPDCCH RMC","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","Approval","endorsed CR R4-167786 with no change","","126","6.3.3.9","Others  [NB_IOT-Perf]",58800,"agreed","2016-11-04T12:58:30.753","2016-11-07T19:39:39.970","","","Rel-13","36.133","13.5.0","NB_IOT-Perf","4240","","F","RP-162379","","","","",""]
["R4-1610014","CR on NPDCCH RMC R14","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","Approval","---","","126","6.3.3.9","Others  [NB_IOT-Perf]",140000,"agreed","2016-11-04T12:58:30.830","2016-11-19T17:47:26.147","","","Rel-14","36.133","14.1.0","NB_IOT-Perf","4241","","A","RP-162379","","","","",""]
["R4-1610015","CR on NPDSCH RMC","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","Approval","endorsed CR R4-167785 with no change","","126","6.3.3.9","Others  [NB_IOT-Perf]",1400,"revised","2016-11-04T12:58:30.923","2016-11-07T19:39:39.643","","R4-1610545","Rel-13","36.133","13.5.0","","4242","","F","","","","","",""]
["R4-1610016","CR on NPDSCH RMC R14","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","Approval","---","","126","6.3.3.9","Others  [NB_IOT-Perf]",1900,"agreed","2016-11-04T12:58:31.003","2016-11-22T12:17:27.080","","","Rel-14","36.133","14.1.0","NB_IOT-Perf","4243","","A","RP-162380","","","","",""]
["R4-1610017","CR on test parameter for RRC re-establishment","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","Approval","remove TBD in SI delay based on endorsed CR: R4-168944","","121","6.3.3.4","RRC Re-establishment test [NB_IOT-Perf]",1800,"revised","2016-11-04T12:58:31.097","2016-11-07T19:39:39.643","","R4-1610598","Rel-13","36.133","13.5.0","","4244","","F","","","","","",""]
["R4-1610018","CR on test parameter for RRC re-establishment R14","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","Approval","remove TBD in SI delay based on endorsed CR: R4-168949","","121","6.3.3.4","RRC Re-establishment test [NB_IOT-Perf]",1800000,"revised","2016-11-04T12:58:31.207","2016-11-07T19:39:39.643","","R4-1610603","Rel-14","36.133","14.1.0","","4245","","F","","","","","",""]
["R4-1610019","CR on NB-IoT measurement conditions R14","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","Approval","Rel-13 CR was agreed in R4-168808. This is corresponding CR for Rel-14","","126","6.3.3.9","Others  [NB_IOT-Perf]",190000,"agreed","2016-11-04T12:58:31.283","2016-11-07T19:39:39.643","","","Rel-14","36.133","14.1.0","NB_IOT-Perf","4246","","F","RP-162380","","","","",""]
["R4-1610020","HD-FDD Radio Link Monitoring Test for Out-of-sync in DRX for UE category NB1 under normal coverage R13","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","Approval","Remove TBD values based on the endorsed CR in R4-168933","","125","6.3.3.8","Radio Link Monitoring test [NB_IOT-Perf]",22000,"agreed","2016-11-04T12:58:31.377","2016-11-07T19:39:39.643","","","Rel-13","36.133","13.5.0","NB_IOT-Perf","4247","","B","RP-162380","","","","",""]
["R4-1610021","HD-FDD Radio Link Monitoring Test for Out-of-sync in DRX for UE category NB1 under normal coverage R14","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","Approval","---","","125","6.3.3.8","Radio Link Monitoring test [NB_IOT-Perf]",23000,"agreed","2016-11-04T12:58:31.470","2016-11-19T17:47:26.160","","","Rel-14","36.133","14.1.0","NB_IOT-Perf","4248","","A","RP-162380","","","","",""]
["R4-1610022","HD-FDD Radio Link Monitoring Test for Out-of-sync in DRX for UE category NB1 under enhanced coverage R13","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","Approval","Remove TBD values based on the endorsed CR in R4-168934","","125","6.3.3.8","Radio Link Monitoring test [NB_IOT-Perf]",26000,"agreed","2016-11-04T12:58:31.563","2016-11-07T19:39:39.657","","","Rel-13","36.133","13.5.0","NB_IOT-Perf","4249","","B","RP-162380","","","","",""]
["R4-1610023","HD-FDD Radio Link Monitoring Test for Out-of-sync in DRX for UE category NB1 under enhanced coverage R14","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","Approval","---","","125","6.3.3.8","Radio Link Monitoring test [NB_IOT-Perf]",26100,"agreed","2016-11-04T12:58:31.643","2016-11-19T17:47:26.160","","","Rel-14","36.133","14.1.0","NB_IOT-Perf","4250","","A","RP-162380","","","","",""]
["R4-1610024","correction on test parameter in RSRP Intra frequency case for Cat-M1 UE in CEModeA","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","Approval","---","","79","6.1.1.1.2","Others  [LTE_MTCe2_L1-Perf]",24000,"revised","2016-11-04T12:58:31.737","2016-11-07T19:39:39.657","","R4-1610648","Rel-13","36.133","13.5.0","","4251","","F","","","","","",""]
["R4-1610025","correction on test parameter in RSRP Intra frequency case for Cat-M1 UE in CEModeA R14","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","Approval","---","","79","6.1.1.1.2","Others  [LTE_MTCe2_L1-Perf]",26000,"agreed","2016-11-04T12:58:31.860","2016-11-19T17:47:26.177","","","Rel-14","36.133","14.1.0","LTE_MTCe2_L1-Perf","4252","","A","RP-162382","","","","",""]
["R4-1610026","correction on test parameter in RSRP Intra frequency case for Cat-M1 UE in CEModeB","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","Approval","---","","79","6.1.1.1.2","Others  [LTE_MTCe2_L1-Perf]",27000,"revised","2016-11-04T12:58:31.937","2016-11-07T19:39:39.657","","R4-1610649","Rel-13","36.133","13.5.0","","4253","","F","","","","","",""]
["R4-1610027","correction on test parameter in RSRP Intra frequency case for Cat-M1 UE in CEModeB R14","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","Approval","---","","79","6.1.1.1.2","Others  [LTE_MTCe2_L1-Perf]",29000,"agreed","2016-11-04T12:58:32.017","2016-11-19T17:47:26.177","","","Rel-14","36.133","14.1.0","LTE_MTCe2_L1-Perf","4254","","A","RP-162382","","","","",""]
["R4-1610028","Introduce RSRP accuracy test case for Band 31 for Cat-M1 UE","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","Approval","---","","79","6.1.1.1.2","Others  [LTE_MTCe2_L1-Perf]",30000,"revised","2016-11-04T12:58:32.110","2016-11-07T19:39:39.657","","R4-1610650","Rel-13","36.133","13.5.0","","4255","","F","","","","","",""]
["R4-1610029","Introduce RSRP accuracy test case for Band 31 for Cat-M1 UE R14","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","Approval","---","","79","6.1.1.1.2","Others  [LTE_MTCe2_L1-Perf]",32000,"agreed","2016-11-04T12:58:32.187","2016-11-19T17:47:26.193","","","Rel-14","36.133","14.1.0","LTE_MTCe2_L1-Perf","4256","","A","RP-162382","","","","",""]
["R4-1610030","Introduce 5MHz Bandwidth MPDCCH Reference Channel for Cat-M1 UE","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","Approval","---","","79","6.1.1.1.2","Others  [LTE_MTCe2_L1-Perf]",33000,"revised","2016-11-04T12:58:32.280","2016-11-07T19:39:39.673","","R4-1610895","Rel-13","36.133","13.5.0","","4257","","F","","","","","",""]
["R4-1610031","Introduce 5MHz Bandwidth MPDCCH Reference Channel for Cat-M1 UE R14","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","Approval","---","","79","6.1.1.1.2","Others  [LTE_MTCe2_L1-Perf]",34000,"agreed","2016-11-04T12:58:32.377","2016-11-19T17:47:26.193","","","Rel-14","36.133","14.1.0","LTE_MTCe2_L1-Perf","4258","","A","RP-162382","","","","",""]
["R4-1610032","Introduce 5MHz Bandwidth MPDSCH Reference Channel for Cat-M1 UE","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","Approval","---","","79","6.1.1.1.2","Others  [LTE_MTCe2_L1-Perf]",35000,"revised","2016-11-04T12:58:32.453","2016-11-07T19:39:39.673","","R4-1610896","Rel-13","36.133","13.5.0","","4259","","F","","","","","",""]
["R4-1610033","Introduce 5MHz Bandwidth MPDSCH Reference Channel for Cat-M1 UE R14","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","Approval","---","","79","6.1.1.1.2","Others  [LTE_MTCe2_L1-Perf]",648000,"agreed","2016-11-04T12:58:32.547","2016-11-19T17:47:26.207","","","Rel-14","36.133","14.1.0","LTE_MTCe2_L1-Perf","4260","","A","RP-162382","","","","",""]
["R4-1610034","Introduce 5MHz Bandwidth OCNG for Cat-M1 UE","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","Approval","---","","79","6.1.1.1.2","Others  [LTE_MTCe2_L1-Perf]",649000,"revised","2016-11-04T12:58:32.623","2016-11-07T19:39:39.673","","R4-1610897","Rel-13","36.133","13.5.0","","4261","","F","","","","","",""]
["R4-1610035","Introduce 5MHz Bandwidth OCNG for Cat-M1 UE R14","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","Approval","---","","79","6.1.1.1.2","Others  [LTE_MTCe2_L1-Perf]",650000,"agreed","2016-11-04T12:58:32.703","2016-11-19T17:47:26.207","","","Rel-14","36.133","14.1.0","LTE_MTCe2_L1-Perf","4262","","A","RP-162382","","","","",""]
["R4-1610036","Simulation result of MIB and SI acquisition delay for NB-IoT","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","Discussion","---","","56","5.6.4","RRM core (36.133)  [NB_IOT-Core]",59700000,"noted","2016-11-04T12:58:32.780","2016-11-07T19:39:39.673","","","","","","","","","","","","","","",""]
["R4-1610037","CR on RRC re-establishment RRM requirement","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","Approval","---","","56","5.6.4","RRM core (36.133)  [NB_IOT-Core]",953800000,"revised","2016-11-04T12:58:32.813","2016-11-07T19:39:39.673","","R4-1610548","Rel-13","36.133","13.5.0","","4263","","F","","","","","",""]
["R4-1610038","CR on RRC re-establishment RRM requirement R14","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","Approval","---","","56","5.6.4","RRM core (36.133)  [NB_IOT-Core]",962100000,"agreed","2016-11-04T12:58:32.890","2016-11-22T12:17:27.080","","","Rel-14","36.133","14.1.0","NB_IOT-Core","4264","","A","RP-162433","","","","",""]
["R4-1610039","CR on paging interruption for NB-IoT","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","Approval","---","","56","5.6.4","RRM core (36.133)  [NB_IOT-Core]",967900000,"revised","2016-11-04T12:58:32.983","2016-11-07T19:39:39.690","","R4-1610589","Rel-13","36.133","13.5.0","","4265","","F","","","","","",""]
["R4-1610040","CR on paging interruption for NB-IoT R14","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","Approval","---","","56","5.6.4","RRM core (36.133)  [NB_IOT-Core]",978600000,"agreed","2016-11-04T12:58:33.060","2016-11-22T12:17:27.097","","","Rel-14","36.133","14.1.0","NB_IOT-Core","4266","","A","RP-162433","","","","",""]
["R4-1610041","discussion on positioning for Cat-1 UE with 1 Rx","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","","---","","334","8.27.3","RRM core (36.133) [LTE_UE_cat_1RX-Core]",910300000,"noted","2016-11-04T12:58:33.170","2016-11-07T19:39:39.690","","","","","","","","","","","","","","",""]
["R4-1610042","WF on Cat-1 UE with 1 Rx positioning","Huawei, HiSilicon","Xiang (Steven) Chen","41576","other","","Way forward","","334","8.27.3","RRM core (36.133) [LTE_UE_cat_1RX-Core]",970300000,"noted","2016-11-04T12:58:33.187","2016-11-07T19:39:39.690","","","","","","","","","","","","","","",""]
["R4-1610043","Discussion on RRM requirements for Cat-1 UE with 1 Rx","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","Discussion","---","","334","8.27.3","RRM core (36.133) [LTE_UE_cat_1RX-Core]",72800000,"noted","2016-11-04T12:58:33.203","2016-11-07T19:39:39.690","","","","","","","","","","","","","","",""]
["R4-1610044","simulation assumption for cell identification for UE Category 1 with 1Rx","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","Approval","---","","334","8.27.3","RRM core (36.133) [LTE_UE_cat_1RX-Core]",910200000,"noted","2016-11-04T12:58:33.233","2016-11-07T19:39:39.690","","","","","","","","","","","","","","",""]
["R4-1610045","Discussion on handover requirement for mobility enhancement","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","Discussion","---","","327","8.26.3","RRM core (36.133) [LTE_eMob-Core]",932500000,"noted","2016-11-04T12:58:33.717","2016-11-07T19:39:39.703","","","","","","","","","","","","","","",""]
["R4-1610046","Discussion on mobility and non-anchor carrier enhancement in NB-IoT enhancement","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","Discussion","---","","309","8.24.3.2","Mobility enhancement [NB_IOTenh-Core]",212000,"noted","2016-11-04T12:58:33.733","2016-11-07T19:39:39.703","","","","","","","","","","","","","","",""]
["R4-1610047","RRM Consideration on beam management in NR","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","Discussion","---","","425","11.6.1.1","RRM general [FS_NR_newRAT]",955900000,"available","2016-11-04T12:58:33.747","2016-11-07T19:39:39.703","","","","","","","","","","","","","","",""]
["R4-1610048","RRM consideration on initial access in NR","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","Discussion","---","","425","11.6.1.1","RRM general [FS_NR_newRAT]",9075000,"noted","2016-11-04T12:58:33.780","2016-11-07T19:39:39.703","","","","","","","","","","","","","","",""]
["R4-1610049","Discussion on RSRQ requirement for eMTC","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","","---","","50","5.5.3.3","Measurement requirement [LTE_MTCe2_L1-Core]",50000,"available","2016-11-04T12:58:33.793","2016-11-07T19:39:39.720","","","","","","","","","","","","","","",""]
["R4-1610050","Way forward on measurement requirement for eMTC","Huawei, HiSilicon","Xiang (Steven) Chen","41576","other","","Way forward","","50","5.5.3.3","Measurement requirement [LTE_MTCe2_L1-Core]",49000,"noted","2016-11-04T12:58:33.827","2016-11-07T19:39:39.737","","","","","","","","","","","","","","",""]
["R4-1610051","Discussion on SI reading for eMTC","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","","---","","48","5.5.3.1","Evaluation of MIB and SIB reading delay, and update of requirement for handover and RRC Re-establishment [LTE_MTCe2_L1-Core]",2210000,"noted","2016-11-04T12:58:33.857","2016-11-07T19:39:39.737","","","","","","","","","","","","","","",""]
["R4-1610052","Discussion on eMTC measurement requirement","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","","---","","50","5.5.3.3","Measurement requirement [LTE_MTCe2_L1-Core]",53000,"noted","2016-11-04T12:58:33.873","2016-11-07T19:39:39.737","","","","","","","","","","","","","","",""]
["R4-1610053","CR on eMTC measurement requirement R13","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","","---","","50","5.5.3.3","Measurement requirement [LTE_MTCe2_L1-Core]",54000,"noted","2016-11-04T12:58:33.887","2016-11-07T19:39:39.737","","","Rel-13","36.133","13.5.0","","4267","","F","","","","","",""]
["R4-1610054","CR on eMTC measurement requirement R14","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","","---","","50","5.5.3.3","Measurement requirement [LTE_MTCe2_L1-Core]",65700000,"withdrawn","2016-11-04T12:58:34.027",null,"","","Rel-14","36.133","14.1.0","","4268","","A","","","","","",""]
["R4-1610055","CR on CGI reading of eMTC R13","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","Approval","---","","48","5.5.3.1","Evaluation of MIB and SIB reading delay, and update of requirement for handover and RRC Re-establishment [LTE_MTCe2_L1-Core]",2550000,"revised","2016-11-04T12:58:34.123","2016-11-07T19:39:39.750","","R4-1610653","Rel-13","36.133","13.5.0","","4269","","F","","","","","",""]
["R4-1610056","CR on CGI reading of eMTC R14","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","Approval","---","","48","5.5.3.1","Evaluation of MIB and SIB reading delay, and update of requirement for handover and RRC Re-establishment [LTE_MTCe2_L1-Core]",2560000,"agreed","2016-11-04T12:58:34.310","2016-11-22T12:17:27.097","","","Rel-14","36.133","14.1.0","LTE_MTCe2_L1-Core","4270","","A","RP-162430","","","","",""]
["R4-1610057","CR on handover of eMTC R13","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","Approval","---","","48","5.5.3.1","Evaluation of MIB and SIB reading delay, and update of requirement for handover and RRC Re-establishment [LTE_MTCe2_L1-Core]",9696000,"revised","2016-11-04T12:58:34.403","2016-11-07T19:39:39.750","","R4-1610654","Rel-13","36.133","13.5.0","","4271","","F","","","","","",""]
["R4-1610058","CR on  handover of eMTC R14","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","Approval","---","","48","5.5.3.1","Evaluation of MIB and SIB reading delay, and update of requirement for handover and RRC Re-establishment [LTE_MTCe2_L1-Core]",41500000,"agreed","2016-11-04T12:58:34.480","2016-11-22T12:17:27.110","","","Rel-14","36.133","14.1.0","LTE_MTCe2_L1-Core","4272","","A","RP-162430","","","","",""]
["R4-1610059","Discussion on eMTC transmission timing requirement","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","","---","","49","5.5.3.2","UE transmit timing [LTE_MTCe2_L1-Core]",9842000,"noted","2016-11-04T12:58:34.573","2016-11-07T19:39:39.750","","","","","","","","","","","","","","",""]
["R4-1610060","CR on eMTC transmission timing requirement for CEModeB R13","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","","---","","49","5.5.3.2","UE transmit timing [LTE_MTCe2_L1-Core]",9843000,"endorsed","2016-11-04T12:58:34.607","2016-11-07T19:39:39.750","","","Rel-13","36.133","13.5.0","","4273","","F","","","","","",""]
["R4-1610061","CR on eMTC transmission timing requirement for CEModeB R14","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","","---","","49","5.5.3.2","UE transmit timing [LTE_MTCe2_L1-Core]",9844000,"endorsed","2016-11-04T12:58:34.730","2016-11-07T19:39:39.750","","","Rel-14","36.133","14.1.0","","4274","","F","","","","","",""]
["R4-1610062","CR on modification of re estalbishment test case R13","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","","---","","89","6.1.1.3.3","RRC Re-establishment [LTE_MTCe2_L1-Perf]",926300000,"noted","2016-11-04T12:58:34.823","2016-11-07T19:39:39.767","","","Rel-13","36.133","13.5.0","","4275","","F","","","","","",""]
["R4-1610063","CR on modification of re estalbishment test case R14","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","","---","","89","6.1.1.3.3","RRC Re-establishment [LTE_MTCe2_L1-Perf]",926400000,"withdrawn","2016-11-04T12:58:34.933",null,"","","Rel-14","36.133","14.1.0","","4276","","A","","","","","",""]
["R4-1610064","CR on modification of handover test case R13","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","Approval","---","","81","6.1.1.2.1","Intra-frequency Handover [LTE_MTCe2_L1-Perf]",640000,"noted","2016-11-04T12:58:35.043","2016-11-07T19:39:39.767","","","Rel-13","36.133","13.5.0","","4277","","F","","","","","",""]
["R4-1610065","CR on modification of handover test case R14","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","Approval","---","","81","6.1.1.2.1","Intra-frequency Handover [LTE_MTCe2_L1-Perf]",650000,"withdrawn","2016-11-04T12:58:35.153",null,"","","Rel-14","36.133","14.1.0","","4278","","A","","","","","",""]
["R4-1610066","CR on modification of cell reselection test case R13","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","","---","","87","6.1.1.3.1","Intra-frequency Cell Re-Selection [LTE_MTCe2_L1-Perf]",66000,"revised","2016-11-04T12:58:35.247","2016-11-07T19:39:39.767","","R4-1610891","Rel-13","36.133","13.5.0","","4279","","F","","","","","",""]
["R4-1610067","CR on modification of cell reselection test case R14","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","","---","","87","6.1.1.3.1","Intra-frequency Cell Re-Selection [LTE_MTCe2_L1-Perf]",67000,"agreed","2016-11-04T12:58:35.340","2016-11-19T17:47:26.237","","","Rel-14","36.133","14.1.0","LTE_MTCe2_L1-Perf","4280","","A","RP-162382","","","","",""]
["R4-1610068","CR on modification of CGI reading test case R13","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","Approval","---","","94","6.1.1.3.8","CGI reading [LTE_MTCe2_L1-Perf]",68000,"withdrawn","2016-11-04T12:58:35.417","2016-11-07T19:39:39.767","","","Rel-13","36.133","13.5.0","","4281","","F","","","","","",""]
["R4-1610069","CR on modification of CGI reading test case R14","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","Approval","---","","94","6.1.1.3.8","CGI reading [LTE_MTCe2_L1-Perf]",69000,"withdrawn","2016-11-04T12:58:35.510",null,"","","Rel-14","36.133","14.1.0","","4282","","A","","","","","",""]
["R4-1610070","Discussion on gap enhancement of per CC and NCSG","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","","---","","351","8.29.2","RRM core (36.133) [LTE_meas_gap_enh-Core]",9549000,"noted","2016-11-04T12:58:35.620","2016-11-07T19:39:39.767","","","","","","","","","","","","","","",""]
["R4-1610071","Discussion on  gap enhancement of short gap","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","","---","","351","8.29.2","RRM core (36.133) [LTE_meas_gap_enh-Core]",932300000,"noted","2016-11-04T12:58:35.650","2016-11-07T19:39:39.783","","","","","","","","","","","","","","",""]
["R4-1610072","WF on RRM impact of gap enhancements","Huawei, HiSilicon","Xiang (Steven) Chen","41576","other","","Way forward","","350","8.29.1","General [LTE_meas_gap_enh-Core]",911900000,"noted","2016-11-04T12:58:35.683","2016-11-07T19:39:39.783","","","","","","","","","","","","","","",""]
["R4-1610073","Discussion on RRM requirement for RAT-dependent indoor positioning","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","","---","","297","8.22.3.1","OTDOA/E-CID enhancement [UTRA_LTE_iPos_enh2]",87600,"noted","2016-11-04T12:58:35.697","2016-11-07T19:39:39.783","","","","","","","","","","","","","","",""]
["R4-1610074","Discussion on RRM requirement for RAT-independent indoor positioning","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","","---","","298","8.22.3.2","RAT-independent enhancement [UTRA_LTE_iPos_enh2]",74000,"noted","2016-11-04T12:58:35.730","2016-11-07T19:39:39.783","","","","","","","","","","","","","","",""]
["R4-1610075","CR on clarification of RRM requirement for indoor positioning","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","","---","","297","8.22.3.1","OTDOA/E-CID enhancement [UTRA_LTE_iPos_enh2]",7500001,"revised","2016-11-04T12:58:35.743","2016-11-07T19:39:39.797","","R4-1610875","Rel-14","36.133","14.1.0","","4283","","F","","","","","",""]
["R4-1610076","CR on Bluetooth Wifi requirement for indoor positioning","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","","---","","298","8.22.3.2","RAT-independent enhancement [UTRA_LTE_iPos_enh2]",76000,"revised","2016-11-04T12:58:35.870","2016-11-07T19:39:39.797","","R4-1610646","Rel-14","36.133","14.1.0","","4284","","B","","","","","",""]
["R4-1610077","Evaluation on FeMTC RRM requirements","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","","---","","319","8.25.3.2.1","Measurement [LTE_feMTC-Core]",790000,"noted","2016-11-04T12:58:35.947","2016-11-07T19:39:39.797","","","","","","","","","","","","","","",""]
["R4-1610078","Discussion on FeMTC RRM requirements","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","","---","","319","8.25.3.2.1","Measurement [LTE_feMTC-Core]",2520000,"noted","2016-11-04T12:58:35.977","2016-11-07T19:39:39.797","","","","","","","","","","","","","","",""]
["R4-1610079","CR on FeMTC RRM requirements","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","","---","","319","8.25.3.2.1","Measurement [LTE_feMTC-Core]",66900000,"noted","2016-11-04T12:58:35.993","2016-11-07T19:39:39.797","","","Rel-14","36.133","14.1.0","","4285","","B","","","","","",""]
["R4-1610080","Discussion and evaluation on UE RSTD measurement for FeMTC","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","","---","","317","8.25.3.1.2","OTDOA  [LTE_feMTC-Core]",927500000,"noted","2016-11-04T12:58:36.087","2016-11-07T19:39:39.813","","","","","","","","","","","","","","",""]
["R4-1610081","Discussion and evaluation on UE Rx-Tx measurement for FeMTC","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","","---","","316","8.25.3.1.1","E-CID  [LTE_feMTC-Core]",81000,"noted","2016-11-04T12:58:36.120","2016-11-07T19:39:39.813","","","","","","","","","","","","","","",""]
["R4-1610082","WF on FeMTC positioning","Huawei, HiSilicon","Xiang (Steven) Chen","41576","other","","Way forward","","315","8.25.3.1","Positioning [LTE_feMTC-Core]",82000,"revised","2016-11-04T12:58:36.150","2016-11-07T19:39:39.813","","R4-1610667","","","","","","","","","","","","",""]
["R4-1610083","Discussion on UE RSTD measurement requirement for eNB-IOT","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","","---","","308","8.24.3.1.2","UTODA/OTDOA [NB_IOTenh-Core]",83000,"noted","2016-11-04T12:58:36.180","2016-11-07T19:39:39.813","","","","","","","","","","","","","","",""]
["R4-1610084","Discussion on UE Rx-Tx time different requirement for eNB-IOT","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","","---","","307","8.24.3.1.1","E-CID  [NB_IOTenh-Core]",34400000,"noted","2016-11-04T12:58:36.197","2016-11-07T19:39:39.830","","","","","","","","","","","","","","",""]
["R4-1610085","Discussion on UTDOA requirement for eNB-IOT","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","","---","","308","8.24.3.1.2","UTODA/OTDOA [NB_IOTenh-Core]",347000,"noted","2016-11-04T12:58:36.227","2016-11-07T19:39:39.830","","","","","","","","","","","","","","",""]
["R4-1610086","Simulation assumption for UE Rx-Tx time different measurement","Huawei, HiSilicon","Xiang (Steven) Chen","41576","other","","Simulation assumption","","307","8.24.3.1.1","E-CID  [NB_IOTenh-Core]",34500000,"revised","2016-11-04T12:58:36.260","2016-11-07T19:39:39.830","","R4-1610698","","","","","","","","","","","","",""]
["R4-1610087","Simulation assumption for UTDOA measurement","Huawei, HiSilicon","Xiang (Steven) Chen","41576","other","","Simulation assumption","","308","8.24.3.1.2","UTODA/OTDOA [NB_IOTenh-Core]",870000,"noted","2016-11-04T12:58:36.290","2016-11-07T19:39:39.830","","","","","","","","","","","","","","",""]
["R4-1610088","WF on NB-IOT positioning","Huawei, HiSilicon","Xiang (Steven) Chen","41576","other","","Way forward","","306","8.24.3.1","Positioning [NB_IOTenh-Core]",88000,"noted","2016-11-04T12:58:36.307","2016-11-07T19:39:39.830","","","","","","","","","","","","","","",""]
["R4-1610089","Corrections on DC interruption test cases R12","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","Approval","Endorsed CR in R4-167757","","14","4.2.3","RRM (Radio Resource Management)  [WI code or TEI12]",4900000,"agreed","2016-11-04T12:58:36.337","2016-11-07T19:39:39.847","","","Rel-12","36.133","12.13.0","TEI12","4286","","F","RP-162420","","","","",""]
["R4-1610090","Corrections on DC interruption test cases R13","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","Approval","Endorsed CR in R4-167758","","14","4.2.3","RRM (Radio Resource Management)  [WI code or TEI12]",4910000,"revised","2016-11-04T12:58:36.430","2016-11-07T19:39:39.847","","R4-1611004","Rel-13","36.133","13.5.0","","4287","","F","","","","","",""]
["R4-1610091","Corrections on DC interruption test cases R14","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","Approval","---","","14","4.2.3","RRM (Radio Resource Management)  [WI code or TEI12]",9209000,"agreed","2016-11-04T12:58:36.523","2016-11-19T17:47:26.253","","","Rel-14","36.133","14.1.0","TEI12","4288","","A","RP-162420","","","","",""]
["R4-1610092","CR on introducing inter-cell synchronization requirements for MBMS R14","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","Approval","---","","373","8.32.1","Inter-cell Synchronization for MBMS/eMBMS [WI code or TEI14]",953000000,"revised","2016-11-04T12:58:36.603","2016-11-07T19:39:39.847","","R4-1610883","Rel-14","36.133","14.1.0","","4289","","B","","","","","",""]
["R4-1610093","CR on introducing UE transmission timing accuracy test based on GNSS timing in V2V","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","Approval","---","","266","8.19.3.1","UE transmission timing accuracy test [LTE_SL_V2V-Perf]",9300000,"noted","2016-11-04T12:58:36.697","2016-11-07T19:39:39.847","","","Rel-14","36.133","14.1.0","","4290","","B","","","","","",""]
["R4-1610094","Evaluation on S-RSRP measurements accuracy for V2X","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","Discussion","---","","283","8.20.4.3","Initiation/cease of SLSS requirement [LTE_V2X-Core]",9700000,"noted","2016-11-04T12:58:36.790","2016-11-07T19:39:39.860","","","","","","","","","","","","","","",""]
["R4-1610095","Evaluation on PSSCH-RSRP measurements accuracy for V2X","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","Discussion","---","","285","8.20.4.5","Autonomous resource selection/reselection [LTE_V2X-Core]",951300010,"noted","2016-11-04T12:58:36.820","2016-11-07T19:39:39.860","","","","","","","","","","","","","","",""]
["R4-1610096","Discussion on UE Tx timing requirement in V2X","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","Discussion","---","","281","8.20.4.1","UE Transmit timing [LTE_V2X-Core]",9767000,"noted","2016-11-04T12:58:36.837","2016-11-07T19:39:39.860","","","","","","","","","","","","","","",""]
["R4-1610097","Discussion on SLSS related requirements in V2X","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","Discussion","---","","283","8.20.4.3","Initiation/cease of SLSS requirement [LTE_V2X-Core]",976800000,"noted","2016-11-04T12:58:36.867","2016-11-07T19:39:39.860","","","","","","","","","","","","","","",""]
["R4-1610098","Discussion on GNSS related requirements","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","Discussion","---","","284","8.20.4.4","Requirements related to synchronization [LTE_V2X-Core]",24100000,"noted","2016-11-04T12:58:36.913","2016-11-07T19:39:39.860","","","","","","","","","","","","","","",""]
["R4-1610099","Discussion on interruption for V2X","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","Discussion","---","","282","8.20.4.2","Interruption [LTE_V2X-Core]",9288000,"noted","2016-11-04T12:58:36.930","2016-11-07T19:39:39.893","","","","","","","","","","","","","","",""]
["R4-1610100","Discussion on autonomous resource selection/reselection in V2X","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","Discussion","---","","285","8.20.4.5","Autonomous resource selection/reselection [LTE_V2X-Core]",9888000,"noted","2016-11-04T12:58:36.960","2016-11-07T19:39:39.893","","","","","","","","","","","","","","",""]
["R4-1610101","Discussion on CBR measurements inV2X","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","Discussion","---","","286","8.20.4.6","Congestion control [LTE_V2X-Core]",10100000,"noted","2016-11-04T12:58:36.993","2016-11-07T19:39:39.907","","","","","","","","","","","","","","",""]
["R4-1610102","Discussion on  performance enhancements indicator for high speed scenarios","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","Discussion","---","","343","8.28.2.3","Others [LTE_high_speed]",103000,"noted","2016-11-04T12:58:37.007","2016-11-07T19:39:39.907","","","","","","","","","","","","","","",""]
["R4-1610103","Reply LS on performance enhancements indicator for high speed scenarios","Huawei, HiSilicon","Xiang (Steven) Chen","41576","LS out","Approval","---","","343","8.28.2.3","Others [LTE_high_speed]",992400000,"revised","2016-11-04T12:58:37.040","2016-11-07T19:39:39.907","","R4-1610677","","","","","","","","","","ran2","","",""]
["R4-1610104","Discussion on the leftover issues in connected mode under high speed scenarios","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","Discussion","---","","341","8.28.2.1","Enhancement in connected mode (DRX) [LTE_high_speed]",99240000,"noted","2016-11-04T12:58:37.057","2016-11-07T19:39:39.907","","","","","","","","","","","","","","",""]
["R4-1610105","Discussion on the leftover issues in idle mode under high speed scenarios","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","Discussion","---","","342","8.28.2.2","Enhancement in idle mode [LTE_high_speed]",952400000,"noted","2016-11-04T12:58:37.087","2016-11-07T19:39:39.907","","","","","","","","","","","","","","",""]
["R4-1610106","CR on the enhanced RRM requirements in connected mode under high speed scenario","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","Approval","---","","341","8.28.2.1","Enhancement in connected mode (DRX) [LTE_high_speed]",929700000,"revised","2016-11-04T12:58:37.117","2016-11-07T19:39:39.923","","R4-1610860","Rel-14","36.133","14.1.0","","4291","","B","","","","","",""]
["R4-1610107","CR on the enhanced RRM requirements in idle mode under high speed scenario","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","Approval","---","","342","8.28.2.2","Enhancement in idle mode [LTE_high_speed]",955100000,"noted","2016-11-04T12:58:37.210","2016-11-07T19:39:39.923","","","Rel-14","36.133","14.1.0","","4292","","B","","","","","",""]
["R4-1610108","Further discussion on interruption requirements on SRS switching","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","Discussion","---","","291","8.21.3","RRM core and performance (36.133) [LTE_SRS_switch-Core/Perf]",108000,"noted","2016-11-04T12:58:37.303","2016-11-07T19:39:39.923","","","","","","","","","","","","","","",""]
["R4-1610109","CR on interruption requirements in SRS switching","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","Approval","---","","291","8.21.3","RRM core and performance (36.133) [LTE_SRS_switch-Core/Perf]",10900000,"revised","2016-11-04T12:58:37.337","2016-11-07T19:39:39.923","","R4-1610861","Rel-14","36.133","14.1.0","","4293","","B","","","","","",""]
["R4-1610110","Discussion on other RRM requirements in SRS switching","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","Discussion","---","","291","8.21.3","RRM core and performance (36.133) [LTE_SRS_switch-Core/Perf]",110000,"noted","2016-11-04T12:58:37.413","2016-11-07T19:39:39.923","","","","","","","","","","","","","","",""]
["R4-1610111","Clarification on the measurement gap restriction in SRS switching","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","Approval","---","","291","8.21.3","RRM core and performance (36.133) [LTE_SRS_switch-Core/Perf]",11100000,"noted","2016-11-04T12:58:37.447","2016-11-07T19:39:39.937","","","Rel-14","36.133","14.1.0","","4294","","B","","","","","",""]
["R4-1610112","Overview on RRM impact on shortened TTI and processing time","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","Discussion","---","","405","10.1.4","RRM core (36.133)  [LTE_sTTIandPT]",975400000,"noted","2016-11-04T12:58:37.537","2016-11-07T19:39:39.937","","","","","","","","","","","","","","",""]
["R4-1610113","Discussion on interruption requirements in eLAA","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","Discussion","---","","254","8.18.4.2","Interruption [LTE_eLAA-Core]",113000,"noted","2016-11-04T12:58:37.570","2016-11-07T19:39:39.937","","","","","","","","","","","","","","",""]
["R4-1610114","Scaling RRM requirements with the number of component carriers in eLAA","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","Discussion","---","","253","8.18.4.1","Measurement with multiple cells [LTE_eLAA-Core]",1140000,"noted","2016-11-04T12:58:37.600","2016-11-07T19:39:39.937","","","","","","","","","","","","","","",""]
["R4-1610115","Discussion on Inter-frequency RSSI measurement requirements in LAA","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","Discussion","---","","42","5.4.3","RRM Core [LTE_LAA-Core]",115000,"noted","2016-11-04T12:58:37.633","2016-11-07T19:39:39.937","","","","","","","","","","","","","","",""]
["R4-1610116","Clarification on Inter-frequency RSSI measurements in LAA R13","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","Approval","---","","42","5.4.3","RRM Core [LTE_LAA-Core]",11600000,"noted","2016-11-04T12:58:37.647","2016-11-07T19:39:39.953","","R4-1610872","Rel-13","36.133","13.5.0","","4295","","F","","","","","",""]
["R4-1610117","Clarification on Inter-frequency RSSI measurements in LAA R14","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","Approval","---","","42","5.4.3","RRM Core [LTE_LAA-Core]",11700000,"withdrawn","2016-11-04T12:58:37.740","2016-11-22T12:17:27.110","","","Rel-14","36.133","14.1.0","","4296","","A","","","","","",""]
["R4-1610118","Correction on SCE test cases R12","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","Approval","---","","14","4.2.3","RRM (Radio Resource Management)  [WI code or TEI12]",1220000,"agreed","2016-11-04T12:58:37.837","2016-11-07T19:39:39.953","","","Rel-12","36.133","12.13.0","LTE_SC_enh_L1-Perf","4297","","F","RP-162418","","","","",""]
["R4-1610119","Correction on SCE test cases R13","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","Approval","---","","14","4.2.3","RRM (Radio Resource Management)  [WI code or TEI12]",1230000,"agreed","2016-11-04T12:58:37.927","2016-11-22T12:17:27.127","","","Rel-13","36.133","13.5.0","LTE_SC_enh_L1-Perf","4298","","A","RP-162418","","","","",""]
["R4-1610120","Correction on SCE test cases R14","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","Approval","---","","14","4.2.3","RRM (Radio Resource Management)  [WI code or TEI12]",4890000,"agreed","2016-11-04T12:58:38.023","2016-11-22T12:17:27.127","","","Rel-14","36.133","14.1.0","LTE_SC_enh_L1-Perf","4299","","A","RP-162418","","","","",""]
["R4-1610121","Correction on the test cases of RSTD Mesaurement in R12","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","Approval","---","","14","4.2.3","RRM (Radio Resource Management)  [WI code or TEI12]",9216000,"agreed","2016-11-04T12:58:38.130","2016-11-07T19:39:39.953","","","Rel-12","36.133","12.13.0","TEI12","4300","","F","RP-162420","","","","",""]
["R4-1610122","Correction on the test cases of RSTD Mesaurement in R13","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","Approval","---","","14","4.2.3","RRM (Radio Resource Management)  [WI code or TEI12]",9217000,"agreed","2016-11-04T12:58:38.240","2016-11-19T17:47:26.270","","","Rel-13","36.133","13.5.0","TEI12","4301","","A","RP-162420","","","","",""]
["R4-1610123","Correction on the test cases of RSTD Mesaurement in R14","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","Approval","---","","14","4.2.3","RRM (Radio Resource Management)  [WI code or TEI12]",9218000,"agreed","2016-11-04T12:58:38.350","2016-11-19T17:47:26.287","","","Rel-14","36.133","14.1.0","TEI12","4302","","A","RP-162420","","","","",""]
["R4-1610124","Corrections on the test cases of UE measurement procedures and measurement performance requirements in R12","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","Approval","---","","14","4.2.3","RRM (Radio Resource Management)  [WI code or TEI12]",27800000,"agreed","2016-11-04T12:58:38.460","2016-11-07T19:39:39.953","","","Rel-12","36.133","12.13.0","TEI12","4303","","F","RP-162420","","","","",""]
["R4-1610125","Corrections on the test cases of UE measurement procedures and measurement performance requirements in R13","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","Approval","---","","14","4.2.3","RRM (Radio Resource Management)  [WI code or TEI12]",41900000,"agreed","2016-11-04T12:58:38.583","2016-11-19T17:47:26.287","","","Rel-13","36.133","13.5.0","TEI12","4304","","A","RP-162420","","","","",""]
["R4-1610126","Corrections on the test cases of UE measurement procedures and measurement performance requirements in R14","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","Approval","---","","14","4.2.3","RRM (Radio Resource Management)  [WI code or TEI12]",42000000,"agreed","2016-11-04T12:58:38.677","2016-11-19T17:47:26.300","","","Rel-14","36.133","14.1.0","TEI12","4305","","A","RP-162420","","","","",""]
["R4-1610127","Soft buffer issue for TDD-FDD CA tests","Ericsson GmbH, Eurolab","Maomao Chen","46060","discussion","Discussion","Discussion","","15","4.2.4","UE demodulation performance  [WI code or TEI12]",37500000,"noted","2016-11-04T13:08:53.520","2016-11-04T13:54:50.757","","","Rel-12","","","","","","","","","","","",""]
["R4-1610128","Effect of Antenna Array Coupling at mmWaves","MVG Industries, Sony Mobile","Alessandro Scannavini","52688","discussion","Discussion","During RAN4#80 –bis, R4-168320 was discussed. It was mainly highlighted that in order to fulfil the FF criteria, 2D^2/lambda, the dimension of the antenna array could have been used as D instead of the dimension of the device under test (DUT).\nThis contri","","419","11.5.2.3","Testability [FS_NR_newRAT]",916000000,"noted","2016-11-04T13:09:56.200","2016-11-04T21:52:26.353","","","Rel-15","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1610129","Introduction of MSD requirement for IMD5 on band3 of CA_3A-8A 2UL CA","CHTTL","Bo-Han Hsieh","61837","CR","Approval","---","","12","4.2.1","UE RF (core / EMC)  [WI code or TEI12]",179000,"revised","2016-11-04T13:14:41.617","2016-11-07T02:19:59.630","","R4-1610767","Rel-12","36.101","12.13.0","LTE_CA_R14_xDL2UL-Core","4089","","F","","","","","",""]
["R4-1610130","Introduction of MSD requirement for IMD5 on band3 of CA_3A-8A 2UL CA","CHTTL","Bo-Han Hsieh","61837","CR","Approval","---","","12","4.2.1","UE RF (core / EMC)  [WI code or TEI12]",181000,"agreed","2016-11-04T13:16:54.373","2016-11-19T17:47:26.300","","","Rel-13","36.101","13.5.0","LTE_CA_R14_xDL2UL-Core","4090","","A","RP-162404","","","","",""]
["R4-1610131","5G NR Testability – Near Field Test Range","MVG Industries","Alessandro Scannavini","52688","discussion","Discussion","During RAN4#80 –bis, R4-168320 was discussed. This contribution highlighted pros and cons for the Far Field and Near Field test method and concluded that Far Field can be the only solution when it comes of 5G NR testability.  This contribution will addres","","419","11.5.2.3","Testability [FS_NR_newRAT]",91590000,"noted","2016-11-04T13:17:29.460","2016-11-04T21:26:37.747","","","Rel-15","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1610132","Introduction of MSD requirement for IMD5 on band3 of CA_3A-8A 2UL CA","CHTTL","Bo-Han Hsieh","61837","CR","Approval","","","12","4.2.1","UE RF (core / EMC)  [WI code or TEI12]",767000,"agreed","2016-11-04T13:19:43.433","2016-11-19T17:47:26.300","","","Rel-14","36.101","14.1.0","LTE_CA_R14_xDL2UL-Core","4091","","A","RP-162404","","","","",""]
["R4-1610133","Updates to burst transmission model for LAA performance requirements (Rel-13)","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","Agreement","Updates to the existing burst transmission model for one LAA Scell and add the burst transmission model for more than 1 LAA Scells","","108","6.2.4.2","PDSCH [LTE_LAA-Perf]",959500000,"revised","2016-11-04T13:25:57.253","2016-11-07T11:36:01.727","","R4-1610865","Rel-13","36.101","13.5.0","LTE_LAA-Perf","4092","","F","","","","","",""]
["R4-1610134","CR: Updates to burst transmission model for LAA performance requirements (Rel-14)","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","Agreement","This is the mirror CR for updates to burst transmission model in Rel-14","","108","6.2.4.2","PDSCH [LTE_LAA-Perf]",976000000,"agreed","2016-11-04T13:25:57.333","2016-11-19T17:47:26.317","","","Rel-14","36.101","14.1.0","LTE_LAA-Perf","4093","","A","RP-162386","","","","",""]
["R4-1610135","CR for correction on OCNG pattern (Rel-13)","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","Agreement","This is the revision of agreed R4-167626 in RAN4#80bis with coversheet updates to the clauses affected empty","","15","4.2.4","UE demodulation performance  [WI code or TEI12]",99910000,"agreed","2016-11-04T13:25:57.457","2016-11-07T11:36:01.727","R4-167626","","Rel-13","36.101","13.5.0","TEI13","3886","1","F","RP-162435","","","","",""]
["R4-1610136","CR for correction on OCNG pattern (Rel-14)","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","Agreement","This is the revision of agreed R4-167627 in RAN4#80bis with coversheet updates to the clauses affected empty","","15","4.2.4","UE demodulation performance  [WI code or TEI12]",99920000,"revised","2016-11-04T13:25:57.630","2016-11-07T11:36:01.743","R4-167627","R4-1611005","Rel-14","36.101","14.1.0","TEI14","3887","1","A","","","","","",""]
["R4-1610137","TRP Uncertainty – Sampling grid vs Beamwidth dimension","MVG Industries","Alessandro Scannavini","52688","discussion","Discussion","During RAN4#80 [1], a way forward on ACLR OTA was approved [1]. ACLR OTA would be defined as the ratio between TRP calculated for the wanted signal and the TRP calculated for the adjacent channel. It was agreed to study test complexity in terms of the tot","","209","8.12.2.1","In band requirements [AASenh_BS_LTE_UTRA]",3940000,"noted","2016-11-04T13:29:43.517","2016-11-07T20:57:54.323","","","Rel-14","","","AASenh_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-1610138","Sets of EARFCN for multiple Scell operation in Band 46","Ericsson","Christian Bergljung","21143","CR","Approval","CR to introduce the Wi-Fi channel bonding for the case in which this is applicable","","248","8.18.3","BS RF (36.104) [LTE_eLAA-Core]",1380000,"revised","2016-11-04T13:37:19.380","2016-11-06T20:34:28.900","","R4-1610984","Rel-14","36.104","14.1.0","LTE_eLAA-Core","0902","","F","","","","","",""]
["R4-1610139","Traffic type in LAA multi-node test","Nokia, Alcatel-Lucent Shanghai Bell","Bartlomiej Golebiowski","61448","other","Approval","---","","140","7.1.2","Multi-node testing [FS_LTE_LAA_multinode_test]",997300000,"available","2016-11-04T13:47:54.830","2016-11-04T22:10:10.377","","","Rel-13","","","","","","","","","","","",""]
["R4-1610140","Simulation results in support of SIR levels for LAA multi-node tests","Nokia, Alcatel-Lucent Shanghai Bell","Bartlomiej Golebiowski","61448","other","Approval","---","","140","7.1.2","Multi-node testing [FS_LTE_LAA_multinode_test]",998300000,"available","2016-11-04T13:50:46.290","2016-11-04T22:10:10.393","","","","","","","","","","","","","","",""]
["R4-1610141","Removal of redundant figure in clause 3.2","Nokia, Alcatel-Lucent Shanghai Bell","Man Hung Ng","68815","CR","Agreement","Delete the redundant figure in clause 3.2.","","19","4.3.1","BS RF (core / conformance / EMC)  [WI code or TEI12]",141000,"agreed","2016-11-04T14:11:28.657","2016-11-04T20:07:43.420","","","Rel-12","37.104","12.11.0","MB_MSR_RF-Core","0310","","F","RP-162413","","","","",""]
["R4-1610142","Removal of redundant figure in clause 3.2","Nokia, Alcatel-Lucent Shanghai Bell","Man Hung Ng","68815","CR","Agreement","Delete the redundant figure in clause 3.2.","","19","4.3.1","BS RF (core / conformance / EMC)  [WI code or TEI12]",142000,"agreed","2016-11-04T14:11:28.767","2016-11-19T17:47:26.317","","","Rel-13","37.104","13.3.0","MB_MSR_RF-Core","0311","","A","RP-162413","","","","",""]
["R4-1610143","Removal of redundant figure in clause 3.2","Nokia, Alcatel-Lucent Shanghai Bell","Man Hung Ng","68815","CR","Agreement","Delete the redundant figure in clause 3.2.","","19","4.3.1","BS RF (core / conformance / EMC)  [WI code or TEI12]",143000,"agreed","2016-11-04T14:11:28.860","2016-11-19T17:47:26.333","","","Rel-14","37.104","14.1.0","MB_MSR_RF-Core","0312","","A","RP-162413","","","","",""]
["R4-1610144","Correction of Fixed Reference Channels for NB-IOT reference sensitivity and dynamic range","Nokia, Alcatel-Lucent Shanghai Bell","Man Hung Ng","68815","CR","Agreement","Indicate the Channel estimation length in NPUSCH Fixed Reference Channels is for information only.","","55","5.6.3","BS RF (36.104) [NB_IOT-Core]",14400000,"agreed","2016-11-04T14:11:28.940","2016-11-04T20:07:43.420","","","Rel-13","36.104","13.5.0","NB_IOT-Core","0903","","F","RP-162433","","","","",""]
["R4-1610145","Correction of Fixed Reference Channels for NB-IOT reference sensitivity and dynamic range","Nokia, Alcatel-Lucent Shanghai Bell","Man Hung Ng","68815","CR","Agreement","Indicate the Channel estimation length in NPUSCH Fixed Reference Channels is for information only.","","55","5.6.3","BS RF (36.104) [NB_IOT-Core]",14500000,"agreed","2016-11-04T14:11:29.033","2016-11-04T20:07:43.420","","","Rel-14","36.104","14.1.0","NB_IOT-Core","0904","","A","RP-162433","","","","",""]
["R4-1610146","TR 37.871 V1.1.0 clean-up","Nokia, Alcatel-Lucent Shanghai Bell, Ericsson, Huawei","Man Hung Ng","68815","pCR","Approval","This contribution provides for approval a text proposal to correct the identified errors.","","203","8.11","Multi-Band Base Station testing with three or more bands  [MB_BS_test_3B]",739000,"revised","2016-11-04T14:11:29.127","2016-11-04T20:07:43.420","","R4-1610739","","37.871","1.1.0","MB_BS_test_3B-Core","","","","","","","","",""]
["R4-1610147","TR 37.871 V1.2.0","Nokia","Man Hung Ng","68815","draft TR","Approval","This contribution provides for approval the updated TR including the approved text proposals in RAN4#80bis.","","203","8.11","Multi-Band Base Station testing with three or more bands  [MB_BS_test_3B]",745000,"revised","2016-11-04T14:11:29.143","2016-11-04T20:07:43.403","","R4-1610740","Rel-14","37.871","1.2.0","MB_BS_test_3B-Core","","","","","","","","",""]
["R4-1610148","Necessary changes to the core requirements for Multi-Band Base Station testing with three or more bands","Nokia, Alcatel-Lucent Shanghai Bell, Ericsson, Huawei","Man Hung Ng","68815","CR","Agreement","Implement the necessary changes to the core requirements for Multi-Band Base Station testing with three or more bands, according to the approved TR 37.871.","","204","8.11.1","BS RF (36.104,37.104, 25.104) [MB_BS_test_3B-Core]",148000,"revised","2016-11-04T14:11:31.047","2016-11-04T20:07:42.653","","R4-1610741","Rel-14","36.104","14.1.0","MB_BS_test_3B-Core","0905","","B","","","","","",""]
["R4-1610149","Necessary changes to the core requirements for Multi-Band Base Station testing with three or more bands","Nokia, Alcatel-Lucent Shanghai Bell, Ericsson, Huawei","Man Hung Ng","68815","CR","Agreement","Implement the necessary changes to the core requirements for Multi-Band Base Station testing with three or more bands, according to the approved TR 37.871.","","204","8.11.1","BS RF (36.104,37.104, 25.104) [MB_BS_test_3B-Core]",741000,"revised","2016-11-04T14:11:31.153","2016-11-04T20:07:42.653","","R4-1610742","Rel-14","37.104","14.1.0","MB_BS_test_3B-Core","0313","","B","","","","","",""]
["R4-1610150","Proposal on simulated UE noise figure for coexistence study for WP5D on new radio access technology","Nokia, Alcatel-Lucent Shanghai Bell","Man Hung Ng","68815","other","Approval","This contribution provides the simulation results using the agreed assumptions (with the necessary correction on the constant in the UMa LOS probability formula from ‘36’ to ‘63’), and proposes refined assumptions on the simulated UE noise figure (NF) for","","410","11.3.1","Co-existence [FS_NR_newRAT]",949900000,"noted","2016-11-04T14:11:31.247","2016-11-04T20:07:42.653","","","","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1610151","Proposal on urban marco indoor UE ratio for coexistence study for WP5D on new radio access technology","Nokia, Alcatel-Lucent Shanghai Bell","Man Hung Ng","68815","other","Approval","This contribution provides the simulation results using the agreed assumptions (with the necessary correction on the constant in the UMa LOS probability formula from ‘36’ to ‘63’), and proposes refined assumptions on the indoor UE ratio in the urban macro","","410","11.3.1","Co-existence [FS_NR_newRAT]",48000000,"noted","2016-11-04T14:11:31.263","2016-11-04T20:07:43.433","","","","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1610152","Proposal on simulated Indoor BS ACLR for coexistence study for WP5D on new radio access technology","Nokia, Alcatel-Lucent Shanghai Bell","Man Hung Ng","68815","other","Approval","This contribution provides the simulation results using the agreed assumptions, and proposes refined assumptions on the simulated Indoor BS ACLR for the coexistence study for WP5D in order to facilitate the calibration process and final output of the stud","","410","11.3.1","Co-existence [FS_NR_newRAT]",62100000,"noted","2016-11-04T14:11:31.297","2016-11-04T20:07:43.433","","","","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1610153","Proposal on dense urban network layout for coexistence study for WP5D on new radio access technology","Nokia, Alcatel-Lucent Shanghai Bell","Man Hung Ng","68815","other","Approval","This contribution provides the simulation results using the agreed assumptions, and proposes refined assumptions on the network layout for the dense urban scenario for the coexistence study for WP5D in order to facilitate the calibration process and final","","410","11.3.1","Co-existence [FS_NR_newRAT]",62200000,"approved","2016-11-04T14:11:31.310","2016-11-04T20:07:43.433","","","","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1610154","Proposal on dense urban BS position for coexistence study for WP5D on new radio access technology","Nokia, Alcatel-Lucent Shanghai Bell","Man Hung Ng","68815","other","Approval","This contribution provides the simulation results using the agreed assumptions, and proposes refined assumptions on the BS position in the dense urban scenario for the coexistence study for WP5D in order to facilitate the calibration process and final out","","410","11.3.1","Co-existence [FS_NR_newRAT]",97730000,"noted","2016-11-04T14:11:31.327","2016-11-04T20:07:43.420","","","","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1610155","Proposal on simulated urban macro UL transmission bandwidth for coexistence study for WP5D on new radio access technology","Nokia, Alcatel-Lucent Shanghai Bell","Man Hung Ng","68815","other","Approval","This contribution provides the simulation results using the agreed assumptions, and proposes refined assumptions on the simulated urban macro UL transmission bandwidth for the coexistence study for WP5D in order to facilitate the calibration process and f","","410","11.3.1","Co-existence [FS_NR_newRAT]",940600000,"noted","2016-11-04T14:11:31.357","2016-11-04T21:07:25.010","","","","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1610156","Simulation results for coexistence study for WP5D on new radio access technology","Nokia, Alcatel-Lucent Shanghai Bell","Man Hung Ng","68815","other","Discussion","This contribution provides the simulation results using the agreed assumptions. The results are provided using the step and number terminologies agreed for the calibration phase.","","410","11.3.1","Co-existence [FS_NR_newRAT]",1620000,"noted","2016-11-04T14:11:31.373","2016-11-04T20:07:43.420","","","","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1610157","Summary of simulation results for calibration on NR coexistence study for WP5D","DOCOMO Communications Lab.","Kunihiko Teshima","57760","other","Information","This is for information.\nThis contribution provide the summary of simulation results for calibration on NR coexistence study for WP5D.\"","","410","11.3.1","Co-existence [FS_NR_newRAT]",950000000,"revised","2016-11-04T14:13:16.237","2016-11-19T17:47:26.333","","R4-1610571","","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1610158","Measurement GAP for NR UE","DOCOMO Communications Lab.","Kunihiko Teshima","57760","other","Approval","This contribution is for approval. In this contribution, we provide our preliminary consideration on measurement GAP for NSA operation.","","425","11.6.1.1","RRM general [FS_NR_newRAT]",34800000,"noted","2016-11-04T14:16:16.603","2016-11-04T17:27:53.867","","","","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1610159","Discussion for NR band defining","KT Corporation","ILWHAN KIM","48721","discussion","Approval","In this paper, we propose how to identify spectrum that RAN4 will work for NR band","","408","11.2","Spectrum  [FS_NR_newRAT]",95200,"withdrawn","2016-11-04T14:18:31.683",null,"R4-1609779","","","","","","","","","","","","","",""]
["R4-1610160","TP on Co-existence simulation scenario, assumption, and methodology for TR 38.803","DOCOMO Communications Lab.","Kunihiko Teshima","57760","pCR","","This contribution is a text proposal for TR 38.803 to add Co-existence simulation scenario, assumption, and methodology.","","410","11.3.1","Co-existence [FS_NR_newRAT]",16000,"revised","2016-11-04T14:19:32.383","2016-11-04T15:25:23.740","","R4-1610572","","38.803","0.3.0","FS_NR_newRAT","","","","","","","","",""]
["R4-1610161","Simulation results for NR coexistence study: urban macro deployment at 30GHz","Qualcomm Incorporated","Marco Papaleo","49190","other","Discussion","Simulation results for urban macro scenario at 30GHz. Both DL and UL data are considered.","","410","11.3.1","Co-existence [FS_NR_newRAT]",9354000,"noted","2016-11-04T14:26:07.083","2016-11-07T20:56:39.893","","","","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1610162","Simulation results for NR coexistence study: dense urban deployment at 30GHz","Qualcomm Incorporated","Marco Papaleo","49190","other","Discussion","Simulation results for dense urban scenario at 30GHz. Both DL and UL data are considered.","","410","11.3.1","Co-existence [FS_NR_newRAT]",9355000,"noted","2016-11-04T14:26:07.100","2016-11-07T20:57:45.007","","","","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1610163","Simulation results for NR coexistence study: indoor deployment at 30GHz","Qualcomm Incorporated","Marco Papaleo","49190","other","Discussion","Simulation results for indoor scenario at 30GHz. Both DL and UL data are considered.","","410","11.3.1","Co-existence [FS_NR_newRAT]",9356000,"noted","2016-11-04T14:26:07.113","2016-11-07T20:58:52.400","","","","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1610164","Simulation results for NR coexistence study: dense urban deployment at 70GHz","Qualcomm Incorporated","Marco Papaleo","49190","other","Discussion","Simulation results for dense urban scenario at 70GHz. Both DL and UL data are considered.","","410","11.3.1","Co-existence [FS_NR_newRAT]",9405000,"noted","2016-11-04T14:26:07.130","2016-11-07T20:59:44.317","","","","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1610165","Simulation results for NR coexistence study: indoor deployment at 70GHz","Qualcomm Incorporated","Marco Papaleo","49190","other","Discussion","Simulation results for indoor scenario at 70GHz. Both DL and UL data are considered.","","410","11.3.1","Co-existence [FS_NR_newRAT]",9408000,"noted","2016-11-04T14:26:07.147","2016-11-07T21:01:02.257","","","","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1610166","Simulation of results for NR coexistence study: summary and ACIR proposals","Qualcomm Incorporated","Marco Papaleo","49190","other","Approval","This contribution presents a summary of the simulation results for the NR adjacent channel coexistence study. Proposals for ACIR are also included.","","410","11.3.1","Co-existence [FS_NR_newRAT]",9496000,"noted","2016-11-04T14:26:07.177","2016-11-07T21:06:01.073","","","","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1610167","Introduction of new bands for NB-IoT in 37.104","Ericsson","Ali Behravan","45979","CR","Approval","In tis CR we introduce new bands for Rel-14 NB-IoT in 36.104","","237","8.17.1","Rapporteur Input [NB_IOT_R14_bands]",988300000,"revised","2016-11-04T14:28:37.763","2016-11-04T14:56:29.333","","R4-1610852","Rel-14","37.104","14.1.0","NB_IOT_R14_bands-Core","0314","","B","","","","","",""]
["R4-1610168","Addition of 1.4 and 3 MHz Channel Bandwidth to E-UTRA operating band 65 for CGC (Complementary Ground Component) operations in Region 1","HUGHES Network Systems Ltd","Pasquale Amodio","61328","WID new","Information","---","","70","5.10.2","New spectrum [WI code]",906000000,"noted","2016-11-04T14:37:14.020","2016-11-04T20:52:29.407","","","Rel-13","36.101","","","","","","","","","","",""]
["R4-1610169","UE cat M1 out of band blocking, Removal of Range 4","Sony","Olof Zander","57059","CR","Approval","---","","45","5.5.1","UE RF (36.101)  [LTE_MTCe2_L1-Core]",913500000,"agreed","2016-11-04T14:39:33.980","2016-11-19T17:47:26.347","","","Rel-14","36.101","14.1.0","LTE_MTCe2_L1-Core","4094","","A","RP-162430","","","","",""]
["R4-1610170","Study on specification impact of new CBW concept from view point of UE RF requirements","DOCOMO Communications Lab.","Kunihiko Teshima","57760","other","","This contribution is for approval. In this contribution, we provide our preliminary analysis on specification impact of the new concept from view point of UE RF requirements.","","407","11.1","General   [FS_NR_newRAT]",15900000,"noted","2016-11-04T14:53:37.890","2016-11-04T15:25:23.740","","","","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1610171","Addition of power class 2","Nokia, Sprint","John Humbert","40476","CR","","This is a cover page revision of an agreed CR.  The change swaps the \"Source to WG\" and \"Source to TSG\" field values.","","193","8.9","Band 41 power class 2 operation [LTE_B41_UE_PC2]",171000,"agreed","2016-11-04T14:57:42.013","2016-11-04T16:07:53.837","R4-168257","","Rel-10","36.307","10.20.0","LTE_B41_UE_PC2-Core","0712","1","F","RP-162406","","","","",""]
["R4-1610172","Addition of CA bandwidth Class F","Nokia, Alcatel-Lucent Shanghai Bell","Petri Vasenkari","69954","CR","","coverpage revision of an agreed CR R4-168253","","17","4.2.6","Other specifications  [WI code or TEI12]",172000,"agreed","2016-11-04T15:04:35.350","2016-11-04T15:54:32.150","R4-168253","","Rel-12","36.307","12.13.0","LTE_CA_R14_intra-Core","0709","1","B","RP-162398","","","","",""]
["R4-1610173","Discussion on V2X RRM Core requirements","Intel Corporation","Yang Tang","56725","discussion","Discussion","---","","284","8.20.4.4","Requirements related to synchronization [LTE_V2X-Core]",9769000,"noted","2016-11-04T15:12:47.360","2016-11-07T18:58:24.047","","","Rel-14","","","LTE_V2X-Core","","","","","","","","",""]
["R4-1610174","V2X UE RRM Interruption Requirements","Intel Corporation","Yang Tang","56725","discussion","Discussion","---","","282","8.20.4.2","Interruption [LTE_V2X-Core]",9770000,"noted","2016-11-04T15:12:47.377","2016-11-07T18:58:24.047","","","Rel-14","","","LTE_V2X-Core","","","","","","","","",""]
["R4-1610175","Addition of power class 2","Nokia, Sprint","John Humbert","40476","CR","Approval","This is a cover page revision of an agreed CR.  The change swaps the \"Source to WG\" and \"Source to TSG\" field values.","","193","8.9","Band 41 power class 2 operation [LTE_B41_UE_PC2]",175000,"withdrawn","2016-11-04T15:13:20.400",null,"R4-168257","","Rel-10","36.307","10.20.0","LTE_B41_UE_PC2-Core","0712","2","F","","","","","",""]
["R4-1610176","Addition of CA bandwidth Class F","Nokia, Alcatel-Lucent Shanghai Bell","Petri Vasenkari","69954","CR","","coverpage revision of an agreed CR R4-168254","","17","4.2.6","Other specifications  [WI code or TEI12]",176000,"agreed","2016-11-04T15:13:44.160","2016-11-04T15:54:32.137","R4-168254","","Rel-13","36.307","13.5.0","LTE_CA_R14_intra-Core","0710","1","A","RP-162398","","","","",""]
["R4-1610177","Addition of CA bandwidth Class F","Nokia, Alcatel-Lucent Shanghai Bell","Petri Vasenkari","69954","CR","","coverpage revision of an agreed CR R4-168255","","17","4.2.6","Other specifications  [WI code or TEI12]",177000,"agreed","2016-11-04T15:19:40.167","2016-11-04T15:54:32.150","R4-168255","","Rel-14","36.307","14.0.0","LTE_CA_R14_intra-Core","0711","1","A","RP-162398","","","","",""]
["R4-1610178","MSD analysis for CA_B5A_B66A with UL on CA_B5A_B66A","Qualcomm Incorporated","Prashanth Akula","67450","other","Approval","---","","177","8.6.2","UE RF (36.101) [LTE_CA_R14_2DL2UL-Core]",99310000,"revised","2016-11-04T15:25:06.690","2016-11-07T14:42:01.653","","R4-1610769","Rel-14","","","LTE_CA_R14_2DL2UL-Core","","","","","","","","",""]
["R4-1610179","Further correction of CA REFSENS harmonic formula R12","Huawei, HiSilicon","Sanjun Feng","40915","CR","Agreement","---","","12","4.2.1","UE RF (core / EMC)  [WI code or TEI12]",965300000,"withdrawn","2016-11-04T15:25:41.680","2016-11-04T15:32:34.317","","","Rel-12","36.101","12.13.0","TEI12","4095","","F","","","","","",""]
["R4-1610180","Further correction of CA REFSENS harmonic formula R13","Huawei, HiSilicon","Sanjun Feng","40915","CR","Agreement","---","","12","4.2.1","UE RF (core / EMC)  [WI code or TEI12]",983400000,"withdrawn","2016-11-04T15:25:41.977","2016-11-04T15:32:34.317","","","Rel-13","36.101","13.5.0","TEI12","4096","","F","","","","","",""]
["R4-1610181","Further correction of CA REFSENS harmonic formula R14","Huawei, HiSilicon","Sanjun Feng","40915","CR","Agreement","---","","12","4.2.1","UE RF (core / EMC)  [WI code or TEI12]",983500000,"withdrawn","2016-11-04T15:25:44.740","2016-11-04T15:32:34.333","","","Rel-14","36.101","14.1.0","TEI12","4097","","F","","","","","",""]
["R4-1610182","MSD analysis for CA_B5A_B66A with UL on CA_B5A_B66A","Qualcomm Incorporated","Prashanth Akula","67450","discussion","","---","","177","8.6.2","UE RF (36.101) [LTE_CA_R14_2DL2UL-Core]",995500000,"withdrawn","2016-11-04T15:25:56.813",null,"","","Rel-14","","","LTE_CA_R14_2DL2UL-Core","","","","","","","","",""]
["R4-1610183","Addition of power class 2 and correction to UE category applicability","Nokia, Sprint","John Humbert","40476","CR","Approval","Request from MCC to revise cover page, this was approved as R4-168924","","193","8.9","Band 41 power class 2 operation [LTE_B41_UE_PC2]",183000,"agreed","2016-11-04T15:27:25.187","2016-11-04T16:07:53.853","R4-168926","","Rel-11","36.307","11.17.0","LTE_B41_UE_PC2-Core","0713","2","F","RP-162406","","","","",""]
["R4-1610184","Addition of power class 2 and correction to UE category applicability Rel-11","Nokia, Sprint","John Humbert","40476","CR","Approval","Request from MCC to revise cover page, this was approved as R4-168924","","193","8.9","Band 41 power class 2 operation [LTE_B41_UE_PC2]",184000,"withdrawn","2016-11-04T15:28:03.547",null,"R4-168926","","Rel-11","36.307","11.17.0","LTE_B41_UE_PC2-Core","0713","3","F","","","","","",""]
["R4-1610185","Correction to UE category applicability","Nokia, Alcatel-Lucent Shanghai Bell","Petri Vasenkari","69954","CR","","coverpage revision of an agreed CR R4-168259","","17","4.2.6","Other specifications  [WI code or TEI12]",185000,"agreed","2016-11-04T15:32:39.637","2016-11-04T15:54:32.150","R4-168259","","Rel-12","36.307","12.13.0","TEI12","0714","1","F","RP-162420","","","","",""]
["R4-1610186","Initial bands for single Rx category 1","Qualcomm Incorporated","Gene Fong","42643","other","","For approval.  Proposal on the initial set of bands to be included in the specifications for 1RxCat1.","","331","8.27.2","UE RF (36.101) [LTE_UE_cat_1RX-Core]",974300000,"revised","2016-11-04T15:42:16.560","2016-11-04T21:04:12.113","","R4-1610822","","","","","","","","","","","","",""]
["R4-1610187","Single Rx Cat 1 reference sensitivity","Qualcomm Incorporated","Gene Fong","42643","other","","For approval. Proposal for reference sensitivity for single Rx device.","","332","8.27.2.1","REFSENS  [LTE_UE_cat_1RX-Core]",983300000,"approved","2016-11-04T15:42:16.683","2016-11-04T21:04:12.113","","","","","","","","","","","","","","",""]
["R4-1610188","Band 68 UE conditions to meet ECC emission requirements","Qualcomm Incorporated","Gene Fong","42643","discussion","","Discussion of how to meet ECC DTV protection requirements and preliminary results","","374","8.32.2","RF  [WI code or TEI14]",2380000,"noted","2016-11-04T15:42:16.700","2016-11-04T21:04:12.113","","","","","","","","","","","","","","",""]
["R4-1610189","Versioning bit indicator for NS_04 A-MPR table","Qualcomm Incorporated","Gene Fong","42643","CR","","Add versioning bit for NS_04 A-MPR table since the table was modified in Rel-14","","195","8.9.2","UE RF (36.101) [LTE_B41_UE_PC2-Core]",189000,"agreed","2016-11-04T15:42:16.730","2016-11-04T21:04:12.130","","","Rel-10","36.101","10.23.0","LTE_B41_UE_PC2","4098","","F","RP-162406","","","","",""]
["R4-1610190","Versioning bit indicator for NS_04 A-MPR table","Qualcomm Incorporated","Gene Fong","42643","CR","","Add versioning bit for NS_04 A-MPR table since the table was modified in Rel-14","","195","8.9.2","UE RF (36.101) [LTE_B41_UE_PC2-Core]",190000,"agreed","2016-11-04T15:42:17.107","2016-11-19T17:47:26.410","","","Rel-11","36.101","11.18.0","LTE_B41_UE_PC2","4099","","A","RP-162406","","","","",""]
["R4-1610191","Versioning bit indicator for NS_04 A-MPR table","Qualcomm Incorporated","Gene Fong","42643","CR","","Add versioning bit for NS_04 A-MPR table since the table was modified in Rel-14","","195","8.9.2","UE RF (36.101) [LTE_B41_UE_PC2-Core]",191000,"agreed","2016-11-04T15:42:17.200","2016-11-19T17:47:26.440","","","Rel-12","36.101","12.13.0","LTE_B41_UE_PC2","4100","","A","RP-162406","","","","",""]
["R4-1610192","Versioning bit indicator for NS_04 A-MPR table","Qualcomm Incorporated","Gene Fong","42643","CR","","Add versioning bit for NS_04 A-MPR table since the table was modified in Rel-14","","195","8.9.2","UE RF (36.101) [LTE_B41_UE_PC2-Core]",192000,"agreed","2016-11-04T15:42:17.277","2016-11-19T17:47:26.440","","","Rel-13","36.101","13.5.0","LTE_B41_UE_PC2","4101","","A","RP-162406","","","","",""]
["R4-1610193","Versioning bit indicator for NS_04 A-MPR table","Qualcomm Incorporated","Gene Fong","42643","CR","","Add versioning bit for NS_04 A-MPR table since the table was modified in Rel-14","","195","8.9.2","UE RF (36.101) [LTE_B41_UE_PC2-Core]",193000,"revised","2016-11-04T15:42:17.357",null,"","R4-1610823","Rel-14","36.101","14.1.0","","4102","","A","","","","","",""]
["R4-1610194","Band 68 NS_26 A-MPR correction","Qualcomm Incorporated","Gene Fong","42643","CR","","A-MPR for 5 MHz is not captured correctly.","","71","5.10.2.1","RF  [WI code]",194000,"revised","2016-11-04T15:42:17.433","2016-11-04T21:04:12.050","","R4-1610821","Rel-13","36.101","13.5.0","","4103","","F","","","","","",""]
["R4-1610195","Band 68 NS_26 A-MPR correction","Qualcomm Incorporated","Gene Fong","42643","CR","","A-MPR for 5 MHz is not captured correctly.","","71","5.10.2.1","RF  [WI code]",195000,"agreed","2016-11-04T15:42:17.527","2016-11-19T17:47:26.457","","","Rel-14","36.101","14.1.0","LTE_FDD_700_ARAB-Core","4104","","A","RP-162427","","","","",""]
["R4-1610196","A-MPR for eLAA in Band 46","Qualcomm Incorporated","Gene Fong","42643","discussion","","Simulation results for US, Europe, and Japan","","245","8.18.2.2","Additional spurious emissions  [LTE_eLAA-Core]",196000,"noted","2016-11-04T15:42:17.653","2016-11-04T21:04:12.067","","","","","","","","","","","","","","",""]
["R4-1610197","In-band emission requirement for eLAA","Qualcomm Incorporated","Gene Fong","42643","other","","For approval.  This contribution provides a proposal for the IBE requirement extending the existing requirement to the interlaced waveform","","247","8.18.2.4","Other requirements [LTE_eLAA-Core]",4750000,"noted","2016-11-04T15:42:17.667","2016-11-04T21:04:12.083","","","","","","","","","","","","","","",""]
["R4-1610198","Maximum output power for eLAA in Band 46","Qualcomm Incorporated","Gene Fong","42643","other","","For approval.  This contribution proposes the maximum output power tolerance be defined as +2/-2.5 dB.","","247","8.18.2.4","Other requirements [LTE_eLAA-Core]",1970000,"noted","2016-11-04T15:42:17.683","2016-11-04T21:04:12.097","","","","","","","","","","","","","","",""]
["R4-1610199","Addition of ?PPowerClass to list of symbols","Qualcomm Incorporated","Gene Fong","42643","CR","","Add DPPowerClass to list of symbols","","195","8.9.2","UE RF (36.101) [LTE_B41_UE_PC2-Core]",199000,"agreed","2016-11-04T15:42:17.700","2016-11-04T21:04:12.097","","","Rel-14","36.101","14.1.0","LTE_B41_UE_PC2","4105","","D","RP-162406","","","","",""]
["R4-1610200","Correction UE category applicability","Nokia, Alcatel-Lucent Shanghai Bell","Petri Vasenkari","69954","CR","","coverpage revision of an agreed CR R4-168260","","17","4.2.6","Other specifications  [WI code or TEI12]",200000,"revised","2016-11-04T15:42:42.153","2016-11-04T15:54:32.150","R4-168260","R4-1610909","Rel-13","36.307","13.5.0","TEI13","0715","1","A","","","","","",""]
["R4-1610201","Correction to UE category applicability","Nokia, Alcatel-Lucent Shanghai Bell","Petri Vasenkari","69954","CR","","coverpage revision of an agreed CR R4-168261","","17","4.2.6","Other specifications  [WI code or TEI12]",201000,"revised","2016-11-04T15:45:31.863","2016-11-04T15:54:56.457","R4-168261","R4-1610910","Rel-14","36.307","14.0.0","TEI14","0716","1","A","","","","","",""]
["R4-1610202","TR skeleton (V0.1.0) for Enhanced CRS and 4Rx SU-MIMO interference Mitigation","Huawei, HiSilicon, LGE, Intel","Xiang (Steven) Chen","41576","TS or TR cover","Approval","In this contribution, we provide TR skeleton for Enhanced CRS and 4Rx SU-MIMO interference Mitigation.","","366","8.31.2","CRS-IM [LTE_eCRSIM_eSUMIMO]",970600000,"approved","2016-11-04T15:46:45.960","2016-11-07T11:32:15.047","","","","","","LTE_eCRSIM_eSUMIMO","","","","","","","","",""]
["R4-1610203","Corrections for MIMO correlation matrics (Rel-14)","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","Agreement","In this CR, we provide corrections for MIMO correlation matrices for 2x4 medium and 4x4 medium A.","","371","8.31.3.2","UE demodulation  [LTE_eCRSIM_eSUMIMO]",20300,"noted","2016-11-04T15:46:45.973","2016-11-07T11:32:15.047","","","Rel-14","36.101","14.1.0","LTE_eCRSIM_eSUMIMO","4106","","F","","","","","",""]
["R4-1610204","Simulation Results for MPR of V2V Waveforms","Qualcomm Europe Inc.(France)","TIen Viet NGUYEN","67205","discussion","Approval","---","","260","8.19.1.1","MPR/A-MPR [LTE_SL_V2V-Core]",9369000,"noted","2016-11-04T16:15:12.997","2016-11-06T19:27:54.697","","","Rel-14","","","LTE_SL_V2V-Core","","","","","","","","",""]
["R4-1610205","New WI: LTE Extended 1.5GHz SDL band (1427 – 1518 MHz) and LTE Carrier Aggregation (2DL/1UL) with Band 20","ORANGE, Telecom Italia, Telia Company","Atoosa Hatefi","62064","WID new","Information","---","","430","13","Revision of the Work Plan",965400000,"available","2016-11-04T16:15:34.727","2016-11-07T18:00:40.130","","","Rel-14","","","","","","","","","","","",""]
["R4-1610206","Discussion on interruptions requirements for V2X","Ericsson","Santhan Thangarasa","59137","discussion","Discussion","In this contribution we discuss interruption requirements based on latest RAN1/RAN2 agreements, and provide our view on their impact on RAN4 requirements.","","282","8.20.4.2","Interruption [LTE_V2X-Core]",20600000,"noted","2016-11-04T16:21:38.680","2016-11-04T20:45:57.093","","","Rel-14","","","LTE_V2X-Core","","","","","","","","",""]
["R4-1610207","Discussion on measurement requirements for V2X","Ericsson","Santhan Thangarasa","59137","discussion","Discussion","In this contribution we discuss the measurement capabilities and the requirements of V2X UEs.","","284","8.20.4.4","Requirements related to synchronization [LTE_V2X-Core]",2080000,"noted","2016-11-04T16:21:38.693","2016-11-04T20:45:57.093","","","Rel-14","","","LTE_V2X-Core","","","","","","","","",""]
["R4-1610208","Discussions on silience period for V2X","Ericsson","Santhan Thangarasa","59137","discussion","Discussion","We discuss the silience period for V2X and provide our view on how the corresponding requirements should be captured.","","284","8.20.4.4","Requirements related to synchronization [LTE_V2X-Core]",9289000,"noted","2016-11-04T16:21:38.727","2016-11-04T20:45:57.093","","","Rel-14","","","LTE_V2X-Core","","","","","","","","",""]
["R4-1610209","Discussions on synchronization requirements for V2X UEs","Ericsson","Santhan Thangarasa","59137","discussion","Discussion","In this contribution we discuss the SLSS based on latest RAN1 agreements and based on the agreed way forward from last RAN4 meeting [4].","","283","8.20.4.3","Initiation/cease of SLSS requirement [LTE_V2X-Core]",984000000,"noted","2016-11-04T16:21:38.740","2016-11-04T20:45:57.093","","","Rel-14","","","LTE_V2X-Core","","","","","","","","",""]
["R4-1610210","Further discussions on handling timing mismatch between GNSS and WAN timing references","Ericsson","Santhan Thangarasa","59137","discussion","Discussion","In this contribution we provide further discussions taking into account the progress in other working groups","","281","8.20.4.1","UE Transmit timing [LTE_V2X-Core]",950900000,"noted","2016-11-04T16:21:38.757","2016-11-04T20:45:57.110","","","Rel-14","","","LTE_V2X-Core","","","","","","","","",""]
["R4-1610211","V2X UE Tx timing requirements","Ericsson","Santhan Thangarasa","59137","discussion","Discussion","In this paper we provide our view to resolve the remaining FFS, when SyncRefUE is used as time reference.","","281","8.20.4.1","UE Transmit timing [LTE_V2X-Core]",21000000,"noted","2016-11-04T16:21:38.787","2016-11-04T20:45:57.110","","","Rel-14","","","LTE_V2X-Core","","","","","","","","",""]
["R4-1610212","Discussions on enhanced RLM for NB-IOT","Ericsson","Santhan Thangarasa","59137","discussion","Discussion","In this contribution we discuss enhanced RLM for NB-IOT","","309","8.24.3.2","Mobility enhancement [NB_IOTenh-Core]",2130000,"noted","2016-11-04T16:21:38.803","2016-11-04T20:45:57.110","","","Rel-14","","","NB_IOTenh-Core","","","","","","","","",""]
["R4-1610213","Draft LS on new event reporting for enhanced RLM for NB-IOT","Ericsson","Santhan Thangarasa","59137","LS out","Approval","Missing abstract","","309","8.24.3.2","Mobility enhancement [NB_IOTenh-Core]",2460000,"noted","2016-11-04T16:21:38.820","2016-11-04T20:45:57.110","","","Rel-14","","","NB_IOTenh-Core","","","","","","RAN2","","",""]
["R4-1610214","Discussion on FeMTC VoLTE enhancements","Ericsson","Santhan Thangarasa","59137","discussion","Discussion","During last RAN4#80bis meeting, RAN4 received an LS from RAN1 regarding VoLTE operation for FeMTC UEs [2]. In this contribution, we discuss this LS and provide motivation for the our draft LS response in [x].","","312","8.25.1","General [LTE_feMTC-Core]",214000,"noted","2016-11-04T16:21:38.850","2016-11-04T20:45:57.127","","","Rel-14","","","LTE_feMTC-Core","","","","","","","","",""]
["R4-1610215","Draft LS on FeMTC VoLTE enhancements","Ericsson","Santhan Thangarasa","59137","LS out","Approval","Missing abstract","","312","8.25.1","General [LTE_feMTC-Core]",2150000,"revised","2016-11-04T16:21:38.867","2016-11-07T08:09:19.680","","R4-1610666","Rel-14","","","LTE_feMTC-Core","","","","","","RAN1","","",""]
["R4-1610216","Discussions on enhanced RLM for feMTC","Ericsson","Santhan Thangarasa","59137","discussion","Discussion","In this contribution, we discuss enhanced RLM for FeMTC","","320","8.25.3.2.2","RLM  [LTE_feMTC-Core]",2170000,"noted","2016-11-04T16:21:38.880","2016-11-04T20:45:57.127","","","Rel-14","","","LTE_feMTC-Core","","","","","","","","",""]
["R4-1610217","Draft LS on new event reporting for enhanced RLM for feMTC","Ericsson","Santhan Thangarasa","59137","LS out","Approval","Missing abstract","","320","8.25.3.2.2","RLM  [LTE_feMTC-Core]",2500000,"noted","2016-11-04T16:21:38.913","2016-11-04T20:45:57.127","","","Rel-14","","","LTE_feMTC-Core","","","","","","RAN2","","",""]
["R4-1610218","Discussions on gap sharing for RRM measurement for Rel-14 feMTC","Ericsson","Santhan Thangarasa","59137","discussion","Discussion","In this contribution we provide some discussions on how both types of measurements can be supported and what needs to be considered when developing these requirements.","","319","8.25.3.2.1","Measurement [LTE_feMTC-Core]",2530000,"noted","2016-11-04T16:21:38.927","2016-11-04T20:45:57.140","","","Rel-14","","","LTE_feMTC-Core","","","","","","","","",""]
["R4-1610219","RRM measurements simulation results for feMTC","Ericsson","Santhan Thangarasa","59137","discussion","Discussion","At last meeting, a way forward capturing the agreements was agreed in [4] and simulation assumptions were captured in [5]. In this contribution we provide the simulation results based on these assumptions.","","319","8.25.3.2.1","Measurement [LTE_feMTC-Core]",218000,"noted","2016-11-04T16:21:38.960","2016-11-04T20:45:57.140","","","Rel-14","","","LTE_feMTC-Core","","","","","","","","",""]
["R4-1610220","Way Forward RRM measurement requirements for feMTC","Ericsson","Santhan Thangarasa","59137","other","Approval","WF on RRM requirements for FeMTC","","318","8.25.3.2","Mobility enhancement [LTE_feMTC-Core]",2200000,"noted","2016-11-04T16:21:38.977","2016-11-04T20:45:57.140","","R4-1610668","Rel-14","","","LTE_feMTC-Core","","","","","","","","",""]
["R4-1610221","Correction to SI reading requirements for eMTC","Ericsson","Santhan Thangarasa","59137","CR","Approval","This CR contains correction to SI reading reuirements based on new simulation results.","","48","5.5.3.1","Evaluation of MIB and SIB reading delay, and update of requirement for handover and RRC Re-establishment [LTE_MTCe2_L1-Core]",4170000,"noted","2016-11-04T16:21:38.990","2016-11-04T20:45:57.157","","","Rel-13","36.133","13.5.0","LTE_MTCe2_L1-Core","4306","","F","","","","","",""]
["R4-1610222","Correction to SI reading requirements for eMTC","Ericsson","Santhan Thangarasa","59137","CR","Approval","This CR contains correction to SI reading reuirements based on new simulation results.","","48","5.5.3.1","Evaluation of MIB and SIB reading delay, and update of requirement for handover and RRC Re-establishment [LTE_MTCe2_L1-Core]",5700000,"withdrawn","2016-11-04T16:21:39.117","2016-11-04T20:45:57.157","","","Rel-14","36.133","14.1.0","LTE_MTCe2_L1-Core","4307","","A","","","","","",""]
["R4-1610223","Correction to eMTC SI reading test","Ericsson","Santhan Thangarasa","59137","CR","Approval","This CR contains correction to SI reading test based on the simulation new simulation results.","","94","6.1.1.3.8","CGI reading [LTE_MTCe2_L1-Perf]",2230000,"revised","2016-11-04T16:21:39.193","2016-11-07T20:54:45.140","","R4-1610664","Rel-13","36.133","13.5.0","LTE_MTCe2_L1-Perf","4308","","B","","","","","",""]
["R4-1610224","Correction to eMTC SI reading test","Ericsson","Santhan Thangarasa","59137","CR","Approval","This CR contains correction to SI reading test based on the simulation new simulation results.","","94","6.1.1.3.8","CGI reading [LTE_MTCe2_L1-Perf]",2240000,"revised","2016-11-04T16:21:39.303","2016-11-07T20:54:45.140","","R4-1610665","Rel-14","36.133","14.1.0","LTE_MTCe2_L1-Perf","4309","","A","","","","","",""]
["R4-1610225","RRM measurement simulation results based on revised simulation assumptions","Ericsson","Santhan Thangarasa","59137","discussion","Discussion","This contribution contains RRM measurement simulation results.","","118","6.3.3.1","RRM measurement accuracy [NB_IOT-Perf]",51900000,"noted","2016-11-04T16:21:39.397","2016-11-04T20:45:57.157","","","Rel-13","","","NB_IOT-Perf","","","","","","","","",""]
["R4-1610226","RLM in-sync test DRX under enhanced coverage","Ericsson","Santhan Thangarasa","59137","CR","Approval","This CR is a revision to already endorsed CR with Tdoc number R4-168945.","","125","6.3.3.8","Radio Link Monitoring test [NB_IOT-Perf]",2310010,"revised","2016-11-04T16:21:39.427","2016-11-04T20:45:57.157","","R4-1610583","Rel-13","36.133","13.5.0","NB_IOT-Perf","4310","","B","","","","","",""]
["R4-1610227","RLM in-sync test with DRX under normal coverage","Ericsson","Santhan Thangarasa","59137","CR","Approval","This CR is a revision to already endorsed CR with Tdoc number R4-168946.","","125","6.3.3.8","Radio Link Monitoring test [NB_IOT-Perf]",2260000,"revised","2016-11-04T16:21:39.520","2016-11-04T20:45:57.173","","R4-1610582","Rel-13","36.133","13.5.0","NB_IOT-Perf","4311","","B","","","","","",""]
["R4-1610228","Inter-frequency cell reselection under enhanced coverage for NB-IOT","Ericsson","Santhan Thangarasa","59137","CR","Approval","Test cases for cell reselection in IDLE state are missing in current specification.","","120","6.3.3.3","Cell Re-selection test [NB_IOT-Perf]",2300000,"revised","2016-11-04T16:21:39.617","2016-11-04T20:45:57.173","","R4-1610579","Rel-13","36.133","13.5.0","NB_IOT-Perf","4312","","B","","","","","",""]
["R4-1610229","Intra-frequency cell reselection under enhanced coverage for NB-IOT","Ericsson","Santhan Thangarasa","59137","CR","Approval","Test cases for cell reselection in IDLE state are missing in current specification.","","120","6.3.3.3","Cell Re-selection test [NB_IOT-Perf]",2330000,"revised","2016-11-04T16:21:39.707","2016-11-04T20:45:57.173","","R4-1610580","Rel-13","36.133","13.5.0","NB_IOT-Perf","4313","","B","","","","","",""]
["R4-1610230","Intra-frequency cell reselection under normal coverage for NB-IOT","Ericsson","Santhan Thangarasa","59137","CR","Approval","Test cases for cell reselection in IDLE state are missing in current specification.","","120","6.3.3.3","Cell Re-selection test [NB_IOT-Perf]",2340000,"revised","2016-11-04T16:21:39.817","2016-11-04T20:45:57.187","","R4-1610578","Rel-13","36.133","13.5.0","NB_IOT-Perf","4314","","B","","","","","",""]
["R4-1610231","RLM in-sync test DRX under enhanced coverage","Ericsson","Santhan Thangarasa","59137","CR","Approval","This CR is a revision to already endorsed CR with Tdoc number R4-168945.","","125","6.3.3.8","Radio Link Monitoring test [NB_IOT-Perf]",2320000,"revised","2016-11-04T16:21:39.927","2016-11-04T20:45:57.187","","R4-1610611","Rel-14","36.133","14.1.0","NB_IOT-Perf","4315","","A","","","","","",""]
["R4-1610232","RLM in-sync test with DRX under normal coverage","Ericsson","Santhan Thangarasa","59137","CR","Approval","This CR is a revision to already endorsed CR with Tdoc number R4-168946.","","125","6.3.3.8","Radio Link Monitoring test [NB_IOT-Perf]",2310000,"revised","2016-11-04T16:21:40.037","2016-11-04T20:56:55.887","","R4-1610609","Rel-14","36.133","14.1.0","NB_IOT-Perf","4316","","A","","","","","",""]
["R4-1610233","Inter-frequency cell reselection under enhanced coverage for NB-IOT","Ericsson","Santhan Thangarasa","59137","CR","Approval","Test cases for cell reselection in IDLE state are missing in current specification.","","120","6.3.3.3","Cell Re-selection test [NB_IOT-Perf]",2630000,"noted","2016-11-04T16:21:40.147","2016-11-04T20:45:57.187","","","Rel-14","36.133","14.1.0","NB_IOT-Perf","4317","","A","","","","","",""]
["R4-1610234","Intra-frequency cell reselection under enhanced coverage for NB-IOT","Ericsson","Santhan Thangarasa","59137","CR","Approval","Test cases for cell reselection in IDLE state are missing in current specification.","","120","6.3.3.3","Cell Re-selection test [NB_IOT-Perf]",2630001,"noted","2016-11-04T16:21:40.240","2016-11-04T20:45:57.187","","","Rel-14","36.133","14.1.0","NB_IOT-Perf","4318","","A","","","","","",""]
["R4-1610235","Intra-frequency cell reselection under normal coverage for NB-IOT","Ericsson","Santhan Thangarasa","59137","CR","Approval","Test cases for cell reselection in IDLE state are missing in current specification.","","120","6.3.3.3","Cell Re-selection test [NB_IOT-Perf]",2350000,"revised","2016-11-04T16:21:40.333","2016-11-04T20:45:57.203","","R4-1610602","Rel-14","36.133","14.1.0","NB_IOT-Perf","4319","","A","","","","","",""]
["R4-1610236","Applicability rule for eMTC test cases in CEModeA and CEModeB","Ericsson","Santhan Thangarasa","59137","CR","Approval","This CR contains applicability rules for eMTC test cases.","","78","6.1.1.1.1","Test applicability [LTE_MTCe2_L1-Perf]",23700000,"revised","2016-11-04T16:21:40.440","2016-11-04T20:45:57.203","","R4-1610658","Rel-13","36.133","13.5.0","LTE_MTCe2_L1-Perf","4320","","B","","","","","",""]
["R4-1610237","Applicability rule for eMTC test cases in CEModeA and CEModeB","Ericsson","Santhan Thangarasa","59137","CR","Approval","This CR contains applicability rules for eMTC test cases.","","78","6.1.1.1.1","Test applicability [LTE_MTCe2_L1-Perf]",27000000,"revised","2016-11-04T16:21:40.537","2016-11-04T20:58:51.250","","R4-1610659","Rel-14","36.133","14.1.0","LTE_MTCe2_L1-Perf","4321","","A","","","","","",""]
["R4-1610238","Band 68 compliance with ECC Decision (16)02: Simulation assumptions for normal environmental conditions","Airbus DS SLC","Eric Georgeaux","38175","discussion","Approval","The objective of this contribution is to propose simulation assumptions to derive the A-MPR requirements for band 68 to meet the European requirements defined in ECC Decision (16)02 [1].","","374","8.32.2","RF  [WI code or TEI14]",2760000,"noted","2016-11-04T16:25:09.963","2016-11-04T16:46:32.763","","","","","","","","","","","","","","",""]
["R4-1610239","NR studies on frequency range 6-24 GHz","ORANGE","Atoosa Hatefi","62064","other","Approval","---","","413","11.4","Co-existence study not related WP5D [FS_NR_newRAT]",92400,"noted","2016-11-04T16:28:51.967","2016-11-07T18:00:40.130","","","","","","","","","","","","","","",""]
["R4-1610240","Discussion on interruptions requirements for V2X","Ericsson","Santhan Thangarasa","59137","discussion","Discussion","In this contribution we discuss interruption requirements based on latest RAN1/RAN2 agreements, and provide our view on their impact on RAN4 requirements.","","282","8.20.4.2","Interruption [LTE_V2X-Core]",951500000,"withdrawn","2016-11-04T16:30:52.837",null,"","","Rel-14","","","LTE_V2X-Core","","","","","","","","",""]
["R4-1610241","Discussion on measurement requirements for V2X","Ericsson","Santhan Thangarasa","59137","discussion","Discussion","In this contribution we discuss the measurement capabilities and the requirements of V2X UEs.","","284","8.20.4.4","Requirements related to synchronization [LTE_V2X-Core]",24300000,"noted","2016-11-04T16:30:52.850",null,"","","Rel-14","","","LTE_V2X-Core","","","","","","","","",""]
["R4-1610242","Discussions on silience period for V2X","Ericsson","Santhan Thangarasa","59137","discussion","Discussion","We discuss the silience period for V2X and provide our view on how the corresponding requirements should be captured.","","284","8.20.4.4","Requirements related to synchronization [LTE_V2X-Core]",98410000,"withdrawn","2016-11-04T16:30:52.867",null,"","","Rel-14","","","LTE_V2X-Core","","","","","","","","",""]
["R4-1610243","Discussions on synchronization requirements for V2X UEs","Ericsson","Santhan Thangarasa","59137","discussion","Discussion","In this contribution we discuss the SLSS based on latest RAN1 agreements and based on the agreed way forward from last RAN4 meeting [4].","","284","8.20.4.4","Requirements related to synchronization [LTE_V2X-Core]",977100000,"withdrawn","2016-11-04T16:30:52.913",null,"","","Rel-14","","","LTE_V2X-Core","","","","","","","","",""]
["R4-1610244","Further discussions on handling timing mismatch between GNSS and WAN timing references","Ericsson","Santhan Thangarasa","59137","discussion","Discussion","In this contribution we provide further discussions taking into account the progress in other working groups","","281","8.20.4.1","UE Transmit timing [LTE_V2X-Core]",36500000,"withdrawn","2016-11-04T16:30:52.947",null,"","","Rel-14","","","LTE_V2X-Core","","","","","","","","",""]
["R4-1610245","V2X UE Tx timing requirements","Ericsson","Santhan Thangarasa","59137","discussion","Discussion","In this paper we provide our view to resolve the remaining FFS, when SyncRefUE is used as time reference.","","281","8.20.4.1","UE Transmit timing [LTE_V2X-Core]",95080000,"withdrawn","2016-11-04T16:30:52.960",null,"","","Rel-14","","","LTE_V2X-Core","","","","","","","","",""]
["R4-1610246","Discussions on enhanced RLM for NB-IOT","Ericsson","Santhan Thangarasa","59137","discussion","Discussion","In this contribution we discuss enhanced RLM for NB-IOT","","309","8.24.3.2","Mobility enhancement [NB_IOTenh-Core]",9152000,"withdrawn","2016-11-04T16:30:52.993",null,"","","Rel-14","","","NB_IOTenh-Core","","","","","","","","",""]
["R4-1610247","Draft LS on new event reporting for enhanced RLM for NB-IOT","Ericsson","Santhan Thangarasa","59137","LS out","Approval","Missing abstract","","309","8.24.3.2","Mobility enhancement [NB_IOTenh-Core]",24700000,"withdrawn","2016-11-04T16:30:53.007",null,"","","Rel-14","","","NB_IOTenh-Core","","","","","","RAN2","","",""]
["R4-1610248","Discussion on FeMTC VoLTE enhancements","Ericsson","Santhan Thangarasa","59137","discussion","Discussion","During last RAN4#80bis meeting, RAN4 received an LS from RAN1 regarding VoLTE operation for FeMTC UEs [2]. In this contribution, we discuss this LS and provide motivation for the our draft LS response in [x].","","319","8.25.3.2.1","Measurement [LTE_feMTC-Core]",929200000,"withdrawn","2016-11-04T16:30:53.040",null,"","","Rel-14","","","LTE_feMTC-Core","","","","","","","","",""]
["R4-1610249","Draft LS on FeMTC VoLTE enhancements","Ericsson","Santhan Thangarasa","59137","LS out","Approval","Missing abstract","","312","8.25.1","General [LTE_feMTC-Core]",2490000,"withdrawn","2016-11-04T16:30:53.053",null,"","","Rel-14","","","LTE_feMTC-Core","","","","","","RAN1","","",""]
["R4-1610250","Discussions on enhanced RLM for feMTC","Ericsson","Santhan Thangarasa","59137","discussion","Discussion","In this contribution, we discuss enhanced RLM for FeMTC","","320","8.25.3.2.2","RLM  [LTE_feMTC-Core]",91490000,"withdrawn","2016-11-04T16:30:53.087",null,"","","Rel-14","","","LTE_feMTC-Core","","","","","","","","",""]
["R4-1610251","Draft LS on new event reporting for enhanced RLM for feMTC","Ericsson","Santhan Thangarasa","59137","LS out","Approval","Missing abstract","","320","8.25.3.2.2","RLM  [LTE_feMTC-Core]",914900000,"withdrawn","2016-11-04T16:30:53.147",null,"","","Rel-14","","","LTE_feMTC-Core","","","","","","RAN2","","",""]
["R4-1610252","Discussions on gap sharing for RRM measurement for Rel-14 feMTC","Ericsson","Santhan Thangarasa","59137","discussion","Discussion","In this contribution we provide some discussions on how both types of measurements can be supported and what needs to be considered when developing these requirements.","","319","8.25.3.2.1","Measurement [LTE_feMTC-Core]",929300000,"withdrawn","2016-11-04T16:30:53.180",null,"","","Rel-14","","","LTE_feMTC-Core","","","","","","","","",""]
["R4-1610253","RRM measurements simulation results for feMTC","Ericsson","Santhan Thangarasa","59137","discussion","Discussion","At last meeting, a way forward capturing the agreements was agreed in [4] and simulation assumptions were captured in [5]. In this contribution we provide the simulation results based on these assumptions.","","319","8.25.3.2.1","Measurement [LTE_feMTC-Core]",961700000,"withdrawn","2016-11-04T16:30:53.210",null,"","","Rel-14","","","LTE_feMTC-Core","","","","","","","","",""]
["R4-1610254","Way Forward RRM measurement requirements for feMTC","Ericsson","Santhan Thangarasa","59137","other","Approval","WF on RRM requirements for FeMTC","","319","8.25.3.2.1","Measurement [LTE_feMTC-Core]",961800000,"withdrawn","2016-11-04T16:30:53.227",null,"","","Rel-14","","","LTE_feMTC-Core","","","","","","","","",""]
["R4-1610255","Correction to SI reading requirements for eMTC","Ericsson","Santhan Thangarasa","59137","CR","Approval","This CR contains correction to SI reading reuirements based on new simulation results.","","48","5.5.3.1","Evaluation of MIB and SIB reading delay, and update of requirement for handover and RRC Re-establishment [LTE_MTCe2_L1-Core]",5800000,"withdrawn","2016-11-04T16:30:53.257",null,"","","Rel-13","36.133","13.5.0","LTE_MTCe2_L1-Core","4322","","F","","","","","",""]
["R4-1610256","Correction to SI reading requirements for eMTC","Ericsson","Santhan Thangarasa","59137","CR","Approval","This CR contains correction to SI reading reuirements based on new simulation results.","","48","5.5.3.1","Evaluation of MIB and SIB reading delay, and update of requirement for handover and RRC Re-establishment [LTE_MTCe2_L1-Core]",9113000,"withdrawn","2016-11-04T16:30:53.383",null,"","","Rel-14","36.133","14.1.0","LTE_MTCe2_L1-Core","4323","","A","","","","","",""]
["R4-1610257","Correction to eMTC SI reading test","Ericsson","Santhan Thangarasa","59137","CR","Approval","This CR contains correction to SI reading test based on the simulation new simulation results.","","94","6.1.1.3.8","CGI reading [LTE_MTCe2_L1-Perf]",2570000,"withdrawn","2016-11-04T16:30:53.553",null,"","","Rel-13","36.133","13.5.0","LTE_MTCe2_L1-Perf","4324","","B","","","","","",""]
["R4-1610258","Correction to eMTC SI reading test","Ericsson","Santhan Thangarasa","59137","CR","Approval","This CR contains correction to SI reading test based on the simulation new simulation results.","","94","6.1.1.3.8","CGI reading [LTE_MTCe2_L1-Perf]",2580000,"withdrawn","2016-11-04T16:30:53.677",null,"","","Rel-14","36.133","14.1.0","LTE_MTCe2_L1-Perf","4325","","A","","","","","",""]
["R4-1610259","RRM measurement simulation results based on revised simulation assumptions","Ericsson","Santhan Thangarasa","59137","discussion","Discussion","This contribution contains RRM measurement simulation results.","","118","6.3.3.1","RRM measurement accuracy [NB_IOT-Perf]",93170000,"withdrawn","2016-11-04T16:30:53.773",null,"","","Rel-13","","","NB_IOT-Perf","","","","","","","","",""]
["R4-1610260","RLM in-sync test DRX under enhanced coverage","Ericsson","Santhan Thangarasa","59137","CR","Approval","This CR is a revision to already endorsed CR with Tdoc number R4-168945.","","125","6.3.3.8","Radio Link Monitoring test [NB_IOT-Perf]",5170000,"withdrawn","2016-11-04T16:30:53.803",null,"","","Rel-13","36.133","13.5.0","NB_IOT-Perf","4326","","B","","","","","",""]
["R4-1610261","RLM in-sync test with DRX under normal coverage","Ericsson","Santhan Thangarasa","59137","CR","Approval","This CR is a revision to already endorsed CR with Tdoc number R4-168946.","","125","6.3.3.8","Radio Link Monitoring test [NB_IOT-Perf]",5180000,"withdrawn","2016-11-04T16:30:53.913",null,"","","Rel-13","36.133","13.5.0","NB_IOT-Perf","4327","","B","","","","","",""]
["R4-1610262","Inter-frequency cell reselection under enhanced coverage for NB-IOT","Ericsson","Santhan Thangarasa","59137","CR","Approval","Test cases for cell reselection in IDLE state are missing in current specification.","","120","6.3.3.3","Cell Re-selection test [NB_IOT-Perf]",2640000,"withdrawn","2016-11-04T16:30:54.020",null,"","","Rel-13","36.133","13.5.0","NB_IOT-Perf","4328","","B","","","","","",""]
["R4-1610263","Intra-frequency cell reselection under enhanced coverage for NB-IOT","Ericsson","Santhan Thangarasa","59137","CR","Approval","Test cases for cell reselection in IDLE state are missing in current specification.","","120","6.3.3.3","Cell Re-selection test [NB_IOT-Perf]",2670000,"withdrawn","2016-11-04T16:30:54.130",null,"","","Rel-13","36.133","13.5.0","NB_IOT-Perf","4329","","B","","","","","",""]
["R4-1610264","Intra-frequency cell reselection under normal coverage for NB-IOT","Ericsson","Santhan Thangarasa","59137","CR","Approval","Test cases for cell reselection in IDLE state are missing in current specification.","","120","6.3.3.3","Cell Re-selection test [NB_IOT-Perf]",2680000,"withdrawn","2016-11-04T16:30:54.223",null,"","","Rel-13","36.133","13.5.0","NB_IOT-Perf","4330","","B","","","","","",""]
["R4-1610265","RLM in-sync test DRX under enhanced coverage","Ericsson","Santhan Thangarasa","59137","CR","Approval","This CR is a revision to already endorsed CR with Tdoc number R4-168945.","","125","6.3.3.8","Radio Link Monitoring test [NB_IOT-Perf]",5160000,"withdrawn","2016-11-04T16:30:54.350",null,"","","Rel-14","36.133","14.1.0","NB_IOT-Perf","4331","","A","","","","","",""]
["R4-1610266","RLM in-sync test with DRX under normal coverage","Ericsson","Santhan Thangarasa","59137","CR","Approval","This CR is a revision to already endorsed CR with Tdoc number R4-168946.","","125","6.3.3.8","Radio Link Monitoring test [NB_IOT-Perf]",5160010,"withdrawn","2016-11-04T16:30:54.443",null,"","","Rel-14","36.133","14.1.0","NB_IOT-Perf","4332","","A","","","","","",""]
["R4-1610267","Inter-frequency cell reselection under enhanced coverage for NB-IOT","Ericsson","Santhan Thangarasa","59137","CR","Approval","Test cases for cell reselection in IDLE state are missing in current specification.","","120","6.3.3.3","Cell Re-selection test [NB_IOT-Perf]",2690000,"withdrawn","2016-11-04T16:30:54.520",null,"","","Rel-14","36.133","14.1.0","NB_IOT-Perf","4333","","A","","","","","",""]
["R4-1610268","Intra-frequency cell reselection under enhanced coverage for NB-IOT","Ericsson","Santhan Thangarasa","59137","CR","Approval","Test cases for cell reselection in IDLE state are missing in current specification.","","120","6.3.3.3","Cell Re-selection test [NB_IOT-Perf]",91470000,"withdrawn","2016-11-04T16:30:54.630",null,"","","Rel-14","36.133","14.1.0","NB_IOT-Perf","4334","","A","","","","","",""]
["R4-1610269","Intra-frequency cell reselection under normal coverage for NB-IOT","Ericsson","Santhan Thangarasa","59137","CR","Approval","Test cases for cell reselection in IDLE state are missing in current specification.","","120","6.3.3.3","Cell Re-selection test [NB_IOT-Perf]",91480000,"withdrawn","2016-11-04T16:30:54.723",null,"","","Rel-14","36.133","14.1.0","NB_IOT-Perf","4335","","A","","","","","",""]
["R4-1610270","Applicability rule for eMTC test cases in CEModeA and CEModeB","Ericsson","Santhan Thangarasa","59137","CR","Approval","This CR contains applicability rules for eMTC test cases.","","78","6.1.1.1.1","Test applicability [LTE_MTCe2_L1-Perf]",27100000,"withdrawn","2016-11-04T16:30:54.817",null,"","","Rel-13","36.133","13.5.0","LTE_MTCe2_L1-Perf","4336","","B","","","","","",""]
["R4-1610271","Applicability rule for eMTC test cases in CEModeA and CEModeB","Ericsson","Santhan Thangarasa","59137","CR","Approval","This CR contains applicability rules for eMTC test cases.","","78","6.1.1.1.1","Test applicability [LTE_MTCe2_L1-Perf]",92570000,"withdrawn","2016-11-04T16:30:54.910",null,"","","Rel-14","36.133","14.1.0","LTE_MTCe2_L1-Perf","4337","","A","","","","","",""]
["R4-1610272","Simulation Results for A-MPR of V2V Waveforms","Qualcomm Europe Inc.(France)","TIen Viet NGUYEN","67205","discussion","Approval","---","","260","8.19.1.1","MPR/A-MPR [LTE_SL_V2V-Core]",937000000,"noted","2016-11-04T16:35:31.373","2016-11-07T21:15:32.237","","","Rel-14","","","","","","","","","","","",""]
["R4-1610273","Simulation Results for A-MPR of V2V Waveforms","Qualcomm Europe Inc.(France)","TIen Viet NGUYEN","67205","discussion","Approval","---","","260","8.19.1.1","MPR/A-MPR [LTE_SL_V2V-Core]",980300000,"withdrawn","2016-11-04T16:37:33.720",null,"","","Rel-14","","","","","","","","","","","",""]
["R4-1610274","Licensed frequency bands for V2X MCC operation","ORANGE","Atoosa Hatefi","62064","other","Approval","---","","273","8.20.1","General [LTE_V2X-Core]",75300000,"noted","2016-11-04T16:48:56.330","2016-11-07T18:00:40.147","","","","","","","","","","","","","","",""]
["R4-1610275","Simulation Results for MPR of V2V Waveforms","Qualcomm Europe Inc.(France)","TIen Viet NGUYEN","67205","discussion","Approval","---","","260","8.19.1.1","MPR/A-MPR [LTE_SL_V2V-Core]",27200000,"withdrawn","2016-11-04T17:07:20.333",null,"","","Rel-14","","","","","","","","","","","",""]
["R4-1610276","Running CR for introduction of European requirements in band 68 and 28 according to ECC Decision (16)02","Airbus DS SLC","Eric Georgeaux","38175","discussion","Discussion","---","","374","8.32.2","RF  [WI code or TEI14]",2850000,"noted","2016-11-04T17:15:04.637","2016-11-04T18:33:48.480","","","","","","","","","","","","","","",""]
["R4-1610277","LTE smartphone TRP and TRS measurements for Bands 3, 7 and 20","ORANGE","Atoosa Hatefi","62064","other","Discussion","---","","218","8.13.2","Hand phantom for smartphones [LTE_UTRA_TRP_TRS-Core]",98040000,"noted","2016-11-04T17:15:52.090","2016-11-07T18:00:40.130","","","","","","","","","","","","","","",""]
["R4-1610278","PCFICH/PDCCH/PHICH Reference channel in UE Cat 0 new CGI RRM test cases","ANRITSU LTD","Ian Rose","9381","CR","","For RRM test cases A.8.1.19, A.8.1.20, A.8.1.21, A.8.1.22, A.8.2.7 and A.8.2.8, change the PCFICH/PDCCH/PHICH Reference channel to one with 2Tx antennas.","","14","4.2.3","RRM (Radio Resource Management)  [WI code or TEI12]",12400000,"agreed","2016-11-04T17:16:25.037","2016-11-04T21:18:23.037","","","Rel-12","36.133","12.13.0","LC_MTC_LTE-Perf","4338","","F","RP-162414","","","","",""]
["R4-1610279","On mm wave ACLR for 45GHz and 70GHz","Ericsson France S.A.S","Thomas Chapman","46692","other","Approval","---","","415","11.5.1","Common issues for UE and BS [FS_NR_newRAT]",962500000,"noted","2016-11-04T17:17:20.700","2016-11-04T17:26:31.907","","","Rel-14","","","","","","","","","","","",""]
["R4-1610280","LTE smartphone TRP and TRS measurements for Bands 3, 7 and 20","ORANGE","Atoosa Hatefi","62064","other","Discussion","---","","218","8.13.2","Hand phantom for smartphones [LTE_UTRA_TRP_TRS-Core]",980200000,"withdrawn","2016-11-04T17:17:49.357",null,"","","","","","","","","","","","","","",""]
["R4-1610281","CR to TR 37.842: Appendix of test method uncertainty descriptions","Ericsson","Esther Sienkiewicz","59234","CR","Approval","coverpage revision of an endorsed CR","","22","5.1.1","Technical Report (37.842) [AAS_BS_LTE_UTRA-Core]",991100000,"agreed","2016-11-04T17:20:54.250","2016-11-07T14:53:16.087","","","Rel-13","37.842","13.0.0","AAS_BS_LTE_UTRA-Perf","0011","","F","RP-162422","","","","",""]
["R4-1610282","New WI proposal: 450MHz E-UTRA FDD Band for BB-PPDR in Europe","Airbus DS SLC","Eric Georgeaux","38175","WID new","Discussion","---","","430","13","Revision of the Work Plan",965500000,"available","2016-11-04T17:25:27.623","2016-11-04T18:33:48.497","","","","","","","","","","","","","","",""]
["R4-1610283","Band 68 compliance with ECC Decision (16)02: A-MPR simulations for normal and extreme environmental conditions","Airbus DS SLC","Eric Georgeaux","38175","discussion","Discussion","In this contribution, A-MPR simulation results for extreme and normal environmental conditions are presented for a 5MHz LTE signal in the frequency range 698-703MHz.","","374","8.32.2","RF  [WI code or TEI14]",959300000,"withdrawn","2016-11-04T17:27:20.610",null,"","","","","","","","","","","","","","",""]
["R4-1610284","Way forward on UL 256QAM UE capability","VODAFONE Group Plc","Tim Frost","28235","discussion","Approval","---","","226","8.15.1","UE capability for UL256QAM  [LTE_UL_CAP_enh-Core]",964300000,"noted","2016-11-04T17:27:36.693","2016-11-07T17:56:09.220","","","Rel-14","","","","","","","","","","","",""]
["R4-1610285","Band 68 compliance with ECC Decision (16)02: A-MPR simulations for normal and extreme environmental conditions","Airbus DS SLC","Eric Georgeaux","38175","discussion","Discussion","In this contribution, A-MPR simulation results for extreme and normal environmental conditions are presented for a 5MHz LTE signal in the frequency range 698-703MHz.","","374","8.32.2","RF  [WI code or TEI14]",983900000,"noted","2016-11-04T17:34:55.207","2016-11-04T17:47:52.550","","","","","","","","","","","","","","",""]
["R4-1610286","Sync Source Detection","Qualcomm Europe Inc.(France)","TIen Viet NGUYEN","67205","discussion","Approval","---","","284","8.20.4.4","Requirements related to synchronization [LTE_V2X-Core]",2070000,"noted","2016-11-04T17:35:25.877","2016-11-06T19:29:26.190","","","","","","","","","","","","","","",""]
["R4-1610287","Timing and Interruption Performance Tests for V2V","Qualcomm Europe Inc.(France)","TIen Viet NGUYEN","67205","discussion","Approval","---","","266","8.19.3.1","UE transmission timing accuracy test [LTE_SL_V2V-Perf]",2870000,"noted","2016-11-04T17:46:33.100","2016-11-06T19:32:24","","","","","","","","","","","","","","",""]
["R4-1610288","Timing and Interruption Performance Tests for V2V","Qualcomm Europe Inc.(France)","TIen Viet NGUYEN","67205","discussion","Approval","---","","266","8.19.3.1","UE transmission timing accuracy test [LTE_SL_V2V-Perf]",28800000,"withdrawn","2016-11-04T17:46:46.423",null,"","","","","","","","","","","","","","",""]
["R4-1610289","Revised WI: LTE Advanced inter-band CA Rel-14 for 5DL/1UL","Nokia","Iwajlo Angelow","34448","WID revised","Approval","---","","170","8.5.1","Rapporteur Input (WID/CRs)  [LTE_CA_R14_5DL1UL-Core]",99030000,"endorsed","2016-11-04T18:33:12.493","2016-11-04T20:52:47.783","","","","","","LTE_CA_R14_5DL1UL","","","","","","","","",""]
["R4-1610290","TR 36.714-05-01 v0.4.0","Nokia","Iwajlo Angelow","34448","draft TR","Approval","---","","170","8.5.1","Rapporteur Input (WID/CRs)  [LTE_CA_R14_5DL1UL-Core]",2900000,"approved","2016-11-04T18:33:12.510","2016-11-04T20:52:48.517","","","Rel-14","36.714-05-01","0.4.0","LTE_CA_R14_5DL1UL-Core","","","","","","","","",""]
["R4-1610291","Introduction of 5DL CA combinations to 36.104","Nokia","Iwajlo Angelow","34448","CR","Approval","---","","170","8.5.1","Rapporteur Input (WID/CRs)  [LTE_CA_R14_5DL1UL-Core]",2920000,"agreed","2016-11-04T18:33:15.037","2016-11-19T17:47:26.583","","","Rel-14","36.104","14.1.0","LTE_CA_R14_5DL1UL-Core","0906","","B","RP-162402","","","","",""]
["R4-1610292","Introduction of 5DL CA combinations to 36.141","Nokia","Iwajlo Angelow","34448","CR","Approval","---","","170","8.5.1","Rapporteur Input (WID/CRs)  [LTE_CA_R14_5DL1UL-Core]",28900000,"agreed","2016-11-04T18:33:15.207","2016-11-19T17:47:26.583","","","Rel-14","36.141","14.1.0","LTE_CA_R14_5DL1UL-Perf","0937","","B","RP-162402","","","","",""]
["R4-1610293","TR 36.744 v0.3.0","Nokia","Iwajlo Angelow","34448","draft TR","Approval","---","","198","8.10.1","General [LTE_TDD_3550_CBRS_US]",2930000,"approved","2016-11-04T18:33:15.317","2016-11-19T17:47:26.583","","","Rel-14","36.744","0.3.0","LTE_TDD_3550_CBRS_US-Core","","","","","","","","",""]
["R4-1610294","Introduction of Band 48","Nokia","Iwajlo Angelow","34448","draftCR","Endorsement","---","","202","8.10.5","Other specifications [LTE_TDD_3550_CBRS_US]",32300000,"endorsed","2016-11-04T18:33:17.453","2016-11-04T20:52:48.533","","","Rel-14","25.461","14.0.0","LTE_TDD_3550_CBRS_US","","","","","","","","",""]
["R4-1610295","Introduction of Band 48","Nokia","Iwajlo Angelow","34448","draftCR","Endorsement","---","","202","8.10.5","Other specifications [LTE_TDD_3550_CBRS_US]",32400000,"endorsed","2016-11-04T18:33:17.487","2016-11-04T20:52:48.533","","","Rel-14","25.466","14.0.0","LTE_TDD_3550_CBRS_US","","","","","","","","",""]
["R4-1610296","Introduction of Band 48","Nokia, Ericsson","Iwajlo Angelow","34448","CR","Approval","---","","200","8.10.3","BS RF (36.104) [LTE_TDD_3550_CBRS_US]",2960000,"agreed","2016-11-04T18:33:17.500","2016-11-04T20:52:48.533","","","Rel-14","36.104","14.1.0","LTE_TDD_3550_CBRS_US-Core","0907","","B","RP-162405","","","","",""]
["R4-1610297","Introduction of Band 48","Nokia, Ericsson","Iwajlo Angelow","34448","CR","Approval","---","","202","8.10.5","Other specifications [LTE_TDD_3550_CBRS_US]",32500000,"agreed","2016-11-04T18:33:17.580","2016-11-04T20:52:48.533","","","Rel-14","36.141","14.1.0","LTE_TDD_3550_CBRS_US-Perf","0938","","B","RP-162405","","","","",""]
["R4-1610298","Introduction of Band 48","Nokia","Iwajlo Angelow","34448","CR","Approval","---","","202","8.10.5","Other specifications [LTE_TDD_3550_CBRS_US]",32600000,"agreed","2016-11-04T18:33:17.673","2016-11-04T20:52:48.547","","","Rel-14","36.113","14.0.0","LTE_TDD_3550_CBRS_US-Core","0063","","B","RP-162405","","","","",""]
["R4-1610299","Introduction of Band 48","Nokia","Iwajlo Angelow","34448","CR","Approval","---","","202","8.10.5","Other specifications [LTE_TDD_3550_CBRS_US]",77700000,"agreed","2016-11-04T18:33:17.750","2016-11-04T20:52:48.547","","","Rel-14","36.124","14.0.0","LTE_TDD_3550_CBRS_US-Core","0036","","B","RP-162405","","","","",""]
["R4-1610300","TP to TR 36.744: Updates on required changes to specifications","Nokia","Iwajlo Angelow","34448","other","Approval","---","","198","8.10.1","General [LTE_TDD_3550_CBRS_US]",31600000,"approved","2016-11-04T18:33:17.827","2016-11-19T17:47:26.597","","","","","","","","","","","","","","",""]
["R4-1610301","TP to 36.714-05-01: Introduction of CA_2A-2A-5A-12A-66A","Nokia, U.S. Cellular","Iwajlo Angelow","34448","other","Approval","---","","171","8.5.2","UE RF (36.101) [LTE_CA_R14_5DL1UL-Core]",3010000,"approved","2016-11-04T18:33:17.843","2016-11-04T20:52:48.547","","","","","","","","","","","","","","",""]
["R4-1610302","TP to 36.714-05-01: Introduction of CA_2A-2A-12B-66A","Nokia, U.S. Cellular","Iwajlo Angelow","34448","other","Approval","---","","171","8.5.2","UE RF (36.101) [LTE_CA_R14_5DL1UL-Core]",3020000,"approved","2016-11-04T18:33:17.877","2016-11-04T20:52:48.547","","","","","","","","","","","","","","",""]
["R4-1610303","TP to 36.714-05-01: Introduction of CA_2A-12B-66A-66A","Nokia, U.S. Cellular","Iwajlo Angelow","34448","other","Approval","---","","171","8.5.2","UE RF (36.101) [LTE_CA_R14_5DL1UL-Core]",3030000,"approved","2016-11-04T18:33:17.890","2016-11-04T20:52:48.563","","","","","","","","","","","","","","",""]
["R4-1610304","TP to 36.714-04-01: Introduction of CA_2A-2A-12A-12A","Nokia, U.S. Cellular","Iwajlo Angelow","34448","other","Approval","---","","165","8.4.2","UE RF (36.101) [LTE_CA_R14_4DL1UL-Core]",91990000,"approved","2016-11-04T18:33:17.907","2016-11-04T20:52:48.563","","","","","","","","","","","","","","",""]
["R4-1610305","TP to 36.714-04-01: Introduction of CA_2A-4A-12A-12A","Nokia, U.S. Cellular","Iwajlo Angelow","34448","other","Approval","---","","165","8.4.2","UE RF (36.101) [LTE_CA_R14_4DL1UL-Core]",92000000,"approved","2016-11-04T18:33:17.923","2016-11-04T20:52:48.563","","","","","","","","","","","","","","",""]
["R4-1610306","TP to 36.714-04-01: Introduction of CA_2A-5A-12A-12A","Nokia, U.S. Cellular","Iwajlo Angelow","34448","other","Approval","---","","165","8.4.2","UE RF (36.101) [LTE_CA_R14_4DL1UL-Core]",92030000,"approved","2016-11-04T18:33:17.953","2016-11-04T20:52:48.563","","","","","","","","","","","","","","",""]
["R4-1610307","TP to 36.714-04-01: Introduction of CA_4A-4A-12A-12A","Nokia, U.S. Cellular","Iwajlo Angelow","34448","other","Approval","---","","165","8.4.2","UE RF (36.101) [LTE_CA_R14_4DL1UL-Core]",98470000,"approved","2016-11-04T18:33:17.970","2016-11-04T20:52:48.563","","","","","","","","","","","","","","",""]
["R4-1610308","TP to 36.714-04-01: Introduction of CA_4A-5A-12A-12A","Nokia, U.S. Cellular","Iwajlo Angelow","34448","other","Approval","---","","165","8.4.2","UE RF (36.101) [LTE_CA_R14_4DL1UL-Core]",984800000,"approved","2016-11-04T18:33:17.983","2016-11-04T20:52:48.580","","","","","","","","","","","","","","",""]
["R4-1610309","Correction to dynamic range requirement","Nokia, Alcatel-Lucent Shanghai Bell","Iwajlo Angelow","34448","CR","Approval","---","","13","4.2.2","BS and Repeater RF (core / conformance / EMC)  [WI code or TEI12]",3090000,"agreed","2016-11-04T18:33:18.017","2016-11-04T20:52:48.580","","","Rel-8","36.104","8.13.0","TEI8","0908","","F","RP-162411","","","","",""]
["R4-1610310","Correction to dynamic range requirement","Nokia, Alcatel-Lucent Shanghai Bell","Iwajlo Angelow","34448","CR","Approval","---","","13","4.2.2","BS and Repeater RF (core / conformance / EMC)  [WI code or TEI12]",3100000,"revised","2016-11-04T18:33:18.127","2016-11-04T20:52:48.580","","R4-1611029","Rel-9","36.104","9.13.0","TEI9","0909","","F","","","","","",""]
["R4-1610311","Correction to dynamic range requirement","Nokia, Alcatel-Lucent Shanghai Bell","Iwajlo Angelow","34448","CR","Approval","---","","13","4.2.2","BS and Repeater RF (core / conformance / EMC)  [WI code or TEI12]",3110000,"revised","2016-11-04T18:33:18.233","2016-11-19T17:47:26.597","","R4-1611024","Rel-10","36.104","10.11.0","TEI10","0910","","A","","","","","",""]
["R4-1610312","Correction to dynamic range requirement","Nokia, Alcatel-Lucent Shanghai Bell","Iwajlo Angelow","34448","CR","Approval","---","","13","4.2.2","BS and Repeater RF (core / conformance / EMC)  [WI code or TEI12]",3120000,"agreed","2016-11-04T18:33:18.327","2016-11-04T20:52:48.597","","","Rel-11","36.104","11.15.0","TEI11","0911","","F","RP-162413","","","","",""]
["R4-1610313","Correction to dynamic range requirement","Nokia, Alcatel-Lucent Shanghai Bell","Iwajlo Angelow","34448","CR","Approval","---","","13","4.2.2","BS and Repeater RF (core / conformance / EMC)  [WI code or TEI12]",3130000,"revised","2016-11-04T18:33:18.420","2016-11-19T17:47:26.613","","R4-1611026","Rel-12","36.104","12.11.0","TEI12","0912","","A","","","","","",""]
["R4-1610314","Correction to dynamic range requirement","Nokia, Alcatel-Lucent Shanghai Bell","Iwajlo Angelow","34448","CR","Approval","---","","13","4.2.2","BS and Repeater RF (core / conformance / EMC)  [WI code or TEI12]",3140000,"revised","2016-11-04T18:33:18.500","2016-11-19T17:47:26.613","","R4-1611027","Rel-13","36.104","13.5.0","TEI13","0913","","A","","","","","",""]
["R4-1610315","Correction to dynamic range requirement","Nokia, Alcatel-Lucent Shanghai Bell","Iwajlo Angelow","34448","CR","Approval","---","","13","4.2.2","BS and Repeater RF (core / conformance / EMC)  [WI code or TEI12]",3150000,"revised","2016-11-04T18:33:18.593","2016-11-19T17:47:26.613","","R4-1611028","Rel-14","36.104","14.1.0","TEI14","0914","","A","","","","","",""]
["R4-1610316","TP to TR 36.744: Updates to BS specific aspects","Nokia","Iwajlo Angelow","34448","other","Approval","---","","198","8.10.1","General [LTE_TDD_3550_CBRS_US]",98600000,"approved","2016-11-04T18:33:18.687","2016-11-04T20:52:48.597","","","","","","","","","","","","","","",""]
["R4-1610317","CR on RLM in-sync test without DRX under normal coverage","QUALCOMM UK Ltd","Amith Chincholi","58403","CR","Approval","This is a CR with Editorial updates to CR on RLM in-sync test without DRX under normal coverage","","125","6.3.3.8","Radio Link Monitoring test [NB_IOT-Perf]",2610000,"revised","2016-11-04T18:34:53.593","2016-11-07T19:42:48.217","","R4-1610584","Rel-13","36.133","13.5.0","","4339","","B","","","","","",""]
["R4-1610318","Further correction of CA_42-42 sub-block CA configuration R13","Huawei, HiSilicon","Sanjun Feng","40915","CR","Agreement","---","","67","5.10.1.1","RF  [WI code]",990900000,"withdrawn","2016-11-04T19:09:54.907","2016-11-04T19:19:41.617","","","Rel-13","36.101","13.5.0","LTE_CA_NC_B42_3DL-Core","4107","","F","","","","","",""]
["R4-1610319","Further correction of CA_42-42 sub-block CA configuration R14","Huawei, HiSilicon","Sanjun Feng","40915","CR","Agreement","---","","67","5.10.1.1","RF  [WI code]",991000000,"withdrawn","2016-11-04T19:09:55.030","2016-11-04T19:19:41.630","","","Rel-14","36.101","14.1.0","LTE_CA_NC_B42_3DL-Core","4108","","A","","","","","",""]
["R4-1610320","Correction of uplink power control setting","Keysight Technologies UK Ltd, Spirent","Moray Rumney","6630","CR","Approval","---","","222","8.14.1","General [LTE_MIMO_OTA-Core]",93330000,"revised","2016-11-04T19:28:36.387","2016-11-04T22:06:43.540","","R4-1610784","Rel-14","37.977","14.1.0","UTRA_LTE_MIMO_OTA-Core","0044","","B","","","","","",""]
["R4-1610321","Correction of uplink power control setting","Keysight Technologies UK Ltd","Moray Rumney","6630","CR","Approval","---","","222","8.14.1","General [LTE_MIMO_OTA-Core]",933500000,"withdrawn","2016-11-04T19:28:52.860",null,"","","Rel-14","37.977","14.1.0","UTRA_LTE_MIMO_OTA-Core","0045","","B","","","","","",""]
["R4-1610322","Correction to WLAN measurement configuration","MediaTek Inc.","Pavan Nuggehalli","60166","CR","Approval","Removes support of periodic WLAN measurements in Release 13, as per RAN2 agreement.","","63","5.9.2","RRM [WI code or TEI13]",3220000,"revised","2016-11-04T19:33:47.123","2016-11-04T21:21:50.517","","R4-1610851","Rel-13","36.133","13.5.0","LTE_WLAN_radio-Perf","4340","","F","","","","","",""]
["R4-1610323","Introduction of Band 48","Nokia, Ericsson","Iwajlo Angelow","34448","CR","Approval","---","","202","8.10.5","Other specifications [LTE_TDD_3550_CBRS_US]",98610000,"revised","2016-11-04T19:55:32.757","2016-11-04T20:52:48.610","","R4-1610777","Rel-14","37.141","14.1.0","LTE_TDD_3550_CBRS_US-Perf","0478","","B","","","","","",""]
["R4-1610324","Introduction of Band 48","Ericsson, Nokia","Iwajlo Angelow","34448","CR","Approval","---","","202","8.10.5","Other specifications [LTE_TDD_3550_CBRS_US]",98630000,"agreed","2016-11-04T19:55:32.867","2016-11-04T20:52:48.610","","","Rel-14","37.113","14.0.0","LTE_TDD_3550_CBRS_US-Core","0055","","B","RP-162405","","","","",""]
["R4-1610325","Introduction of Band 48","Ericsson, Nokia","Iwajlo Angelow","34448","CR","Approval","---","","202","8.10.5","Other specifications [LTE_TDD_3550_CBRS_US]",98640000,"agreed","2016-11-04T19:55:32.977","2016-11-04T20:52:48.627","","","Rel-14","37.104","14.1.0","LTE_TDD_3550_CBRS_US-Core","0315","","B","RP-162405","","","","",""]
["R4-1610326","Introduction of Band 48","Ericsson, Nokia","Iwajlo Angelow","34448","CR","Approval","---","","202","8.10.5","Other specifications [LTE_TDD_3550_CBRS_US]",98650000,"agreed","2016-11-04T19:55:33.070","2016-11-04T20:52:48.610","","","Rel-14","25.141","14.0.0","LTE_TDD_3550_CBRS_US-Perf","0773","","B","RP-162405","","","","",""]
["R4-1610327","Introduction of Band 48","Ericsson, Nokia","Iwajlo Angelow","34448","CR","Approval","---","","202","8.10.5","Other specifications [LTE_TDD_3550_CBRS_US]",2950000,"agreed","2016-11-04T19:55:33.163","2016-11-04T20:52:48.627","","","Rel-14","25.104","14.0.0","LTE_TDD_3550_CBRS_US-Core","0745","","B","RP-162405","","","","",""]
["R4-1610328","LS on Definition of eNB and UE Rx – Tx time differences","Nokia, Alcatel-Lucent Shanghai Bell","Ren Da","45542","LS out","Approval","---","","307","8.24.3.1.1","E-CID  [NB_IOTenh-Core]",9104000,"noted","2016-11-04T20:06:37.570","2016-11-04T20:30:17.127","","","","","","","","","","","","RAN1","","",""]
["R4-1610329","RRM Requirements supporting NR beam management","Nokia, Alcatel-Lucent Shanghai Bell","Ren Da","45542","discussion","Discussion","---","","425","11.6.1.1","RRM general [FS_NR_newRAT]",956000000,"available","2016-11-04T20:06:37.603","2016-11-04T20:30:17.127","","","","","","","","","","","","","","",""]
["R4-1610330","On UE Cat M1 requirements in DRX","Ericsson","Iana Siomina","42857","other","Discussion","On UE Cat M1 requirements in DRX","","47","5.5.3","RRM Core (36.133) [LTE_MTCe2_L1-Core]",3300000,"noted","2016-11-04T20:16:25.907","2016-11-07T21:58:02.340","","","Rel-13","","","LTE_MTCe2_L1-Core","","","","","","","","",""]
["R4-1610331","Requirements clarification for UE Cat M1","Ericsson","Iana Siomina","42857","CR","Approval","Requirements clarification for UE Cat M1","","47","5.5.3","RRM Core (36.133) [LTE_MTCe2_L1-Core]",3310000,"noted","2016-11-04T20:16:25.923","2016-11-07T21:58:02.340","","","Rel-13","36.133","13.5.0","LTE_MTCe2_L1-Core","4341","","F","","","","","",""]
["R4-1610332","Requirements clarification for UE Cat M1","Ericsson","Iana Siomina","42857","CR","Approval","Requirements clarification for UE Cat M1","","47","5.5.3","RRM Core (36.133) [LTE_MTCe2_L1-Core]",3320000,"noted","2016-11-04T20:16:26.017",null,"","","Rel-14","36.133","14.1.0","LTE_MTCe2_L1-Core","4342","","A","","","","","",""]
["R4-1610333","On measurement requirements for multiple SCells in FS3","Ericsson","Iana Siomina","42857","other","Discussion","On measurement requirements for multiple SCells in FS3","","253","8.18.4.1","Measurement with multiple cells [LTE_eLAA-Core]",33300000,"noted","2016-11-04T20:16:26.110","2016-11-07T16:28:58.883","","","Rel-14","","","LTE_eLAA-Core","","","","","","","","",""]
["R4-1610334","eLAA requirements corrections","Ericsson","Iana Siomina","42857","CR","Approval","eLAA requirements corrections","","255","8.18.4.3","Others [LTE_eLAA-Core]",97510000,"revised","2016-11-04T20:16:26.127","2016-11-07T16:28:58.883","","R4-1610732","Rel-14","36.133","14.1.0","LTE_eLAA-Core","4343","","B","","","","","",""]
["R4-1610335","Remaining issues with eLAA RRM requirements","Ericsson","Iana Siomina","42857","CR","Approval","Remaining issues with eLAA RRM requirements","","254","8.18.4.2","Interruption [LTE_eLAA-Core]",3350000,"revised","2016-11-04T20:16:26.220","2016-11-07T16:28:58.900","","R4-1610731","Rel-14","36.133","14.1.0","LTE_eLAA-Core","4344","","F","","","","","",""]
["R4-1610336","On Timing reference for FS3 SCell","Ericsson","Iana Siomina","42857","other","Discussion","On Timing reference for FS3 SCell","","255","8.18.4.3","Others [LTE_eLAA-Core]",33400000,"noted","2016-11-04T20:16:26.330","2016-11-07T16:28:58.900","","","Rel-14","","","LTE_eLAA-Core","","","","","","","","",""]
["R4-1610337","Response on Timing reference for FS3 SCell","Ericsson","Iana Siomina","42857","LS out","Approval","Response on Timing reference for FS3 SCell","","255","8.18.4.3","Others [LTE_eLAA-Core]",97500000,"revised","2016-11-04T20:16:26.360","2016-11-07T16:28:58.900","","R4-1610733","Rel-14","","","LTE_eLAA-Core","","","","","R2-165965","RAN2","RAN1","R2-165965",""]
["R4-1610338","On RRM requirements with SRS carrier based switching","Ericsson","Iana Siomina","42857","other","Discussion","On RRM requirements with SRS carrier based switching","","291","8.21.3","RRM core and performance (36.133) [LTE_SRS_switch-Core/Perf]",338000,"noted","2016-11-04T20:16:26.377","2016-11-07T20:39:28.717","","","Rel-14","","","LTE_SRS_switch-Core","","","","","","","","",""]
["R4-1610339","Impact on requiremets for RSTD in shared cell","Ericsson","Iana Siomina","42857","other","Discussion","Impact on requiremets for RSTD in shared cell","","297","8.22.3.1","OTDOA/E-CID enhancement [UTRA_LTE_iPos_enh2]",7500000,"noted","2016-11-04T20:16:26.407","2016-11-07T16:28:58.900","","","Rel-14","","","UTRA_LTE_iPos_enh2-Core","","","","","","","","",""]
["R4-1610340","RSTD measurements in shared cells","Ericsson","Iana Siomina","42857","CR","Approval","RSTD measurements in shared cells","","297","8.22.3.1","OTDOA/E-CID enhancement [UTRA_LTE_iPos_enh2]",34000000,"revised","2016-11-04T20:16:26.423","2016-11-07T16:28:58.913","","R4-1610854","Rel-14","36.133","14.1.0","UTRA_LTE_iPos_enh2-Core","4345","","B","","","","","",""]
["R4-1610341","Simulation results for UE Rx-Tx in FeMTC","Ericsson","Iana Siomina","42857","other","Discussion","Simulation results for UE Rx-Tx for FeMTC","","316","8.25.3.1.1","E-CID  [LTE_feMTC-Core]",3410000,"noted","2016-11-04T20:16:26.533","2016-11-07T16:28:58.913","","","Rel-14","","","LTE_feMTC-Core","","","","","","","","",""]
["R4-1610342","Simulation results for RSTD in FeMTC","Ericsson","Iana Siomina","42857","other","Discussion","Simulation results for RSTD for FeMTC","","317","8.25.3.1.2","OTDOA  [LTE_feMTC-Core]",927600000,"noted","2016-11-04T20:16:26.563","2016-11-07T16:28:58.913","","","Rel-14","","","LTE_feMTC-Core","","","","","","","","",""]
["R4-1610343","WF on positioning requirements for FeMTC","Ericsson","Iana Siomina","42857","other","Approval","WF on positioning requirements for FeMTC","","315","8.25.3.1","Positioning [LTE_feMTC-Core]",3430000,"noted","2016-11-04T20:16:26.580","2016-11-07T16:28:58.930","","","Rel-14","","","LTE_feMTC-Core","","","","","","","","",""]
["R4-1610344","On E-CID measurements for NB-IoT","Ericsson","Iana Siomina","42857","other","Discussion","On E-CID measurements for NB-IoT","","307","8.24.3.1.1","E-CID  [NB_IOTenh-Core]",91050000,"noted","2016-11-04T20:16:26.597","2016-11-07T16:28:58.930","","","Rel-14","","","NB_IOTenh-Core","","","","","","","","",""]
["R4-1610345","LS on E-CID measurements for NB-IoT","Ericsson","Iana Siomina","42857","LS out","Approval","LS on E-CID measurements for NB-IoT","","307","8.24.3.1.1","E-CID  [NB_IOTenh-Core]",92770000,"revised","2016-11-04T20:16:26.627","2016-11-07T16:28:58.853","","R4-1610855","Rel-14","","","NB_IOTenh-Core","","","","","","RAN2, RAN3","","",""]
["R4-1610346","Simulation assumptions for UE Rx-Tx in NB-IoT","Ericsson","Iana Siomina","42857","other","Approval","Simulation assumptions for UE Rx-Tx time difference in NB-IoT","","307","8.24.3.1.1","E-CID  [NB_IOTenh-Core]",34600000,"noted","2016-11-04T20:16:26.640","2016-11-07T16:28:58.853","","","Rel-14","","","NB_IOTenh-Core","","","","","","","","",""]
["R4-1610347","Simulation results for RSTD in NB-IoT","Ericsson","Iana Siomina","42857","other","Discussion","Simulation results for RSTD with NB-IoT","","308","8.24.3.1.2","UTODA/OTDOA [NB_IOTenh-Core]",85000,"noted","2016-11-04T20:16:26.673","2016-11-07T16:28:58.867","","","Rel-14","","","NB_IOTenh-Core","","","","","","","","",""]
["R4-1610348","On RRM measurements for NR","Ericsson","Iana Siomina","42857","other","Discussion","On RRM measurements for NR","","425","11.6.1.1","RRM general [FS_NR_newRAT]",956200000,"available","2016-11-04T20:16:26.687","2016-11-07T16:28:58.867","","","Rel-15","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1610349","On RRM and mobility support for NR","Ericsson","Iana Siomina","42857","other","Discussion","On RRM and mobility support for NR","","425","11.6.1.1","RRM general [FS_NR_newRAT]",956300000,"available","2016-11-04T20:16:26.720","2016-11-07T16:28:58.867","","","Rel-15","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1610350","TP on mobility and measurements for NR","Ericsson","Iana Siomina","42857","pCR","Approval","TP on mobility and measurements for NR","","425","11.6.1.1","RRM general [FS_NR_newRAT]",956500000,"noted","2016-11-04T20:16:26.737","2016-11-07T16:28:58.883","","","","38.803","0.3.0","FS_NR_newRAT","","","","","","","","",""]
["R4-1610351","New Work Item on UE requirements for network-based CRS mitigation for LTE","Ericsson","Iana Siomina","42857","other","Information","New Work Item on UE requirements for network-based CRS mitigation for LTE","","430","13","Revision of the Work Plan",987500000,"available","2016-11-04T20:16:26.767","2016-11-07T16:28:58.883","","","Rel-15","","","","","","","","","","","",""]
["R4-1610352","Motivation for New Work Item on Network Based CRS Mitigation","Ericsson","Iana Siomina","42857","other","Information","Motivation for New Work Item on Network Based CRS Mitigation","","430","13","Revision of the Work Plan",987600000,"available","2016-11-04T20:16:26.783","2016-11-07T16:31:21.390","","","Rel-15","","","","","","","","","","","",""]
["R4-1610353","Downlink simulation results for NR coexistence study","NEC","Nader Zein","27226","discussion","Discussion","In RAN4#80-bis, the simulation assumptions of co-existence study for WP 5D has been approved. In this contribution, we provide the downlink simulation results according to the agreements.","","410","11.3.1","Co-existence [FS_NR_newRAT]",15300000,"noted","2016-11-04T20:29:30.777","2016-11-07T12:20:30.163","","","Rel-14","38.803","0.0.1","FS_NR_newRAT","","","","","","","","",""]
["R4-1610354","Uplink simulation results for NR coexistence study","NEC","Nader Zein","27226","discussion","Discussion","In RAN4#80-bis, the simulation assumptions of co-existence study for WP 5D has been approved. In this contribution, we provide the uplink simulation results according to the agreements.","","410","11.3.1","Co-existence [FS_NR_newRAT]",15400000,"noted","2016-11-04T20:29:30.793","2016-11-07T12:20:30.163","","","Rel-14","38.803","0.0.1","FS_NR_newRAT","","","","","","","","",""]
["R4-1610355","Coordinate system for NR","NEC","Nader Zein","27226","other","Approval","In NR discussion, it is observed that companies do not have common coordinate system and submit contributions with their own coordinate system. \nIt is beneficial to have a reference coordinate system. It would make the technical discussion easier and prev","","407","11.1","General   [FS_NR_newRAT]",965900010,"noted","2016-11-04T20:29:30.827","2016-11-07T12:20:30.180","","","Rel-14","38.803","0.0.1","FS_NR_newRAT","","","","","","","","",""]
["R4-1610356","Calibration results for NR co-existence study","NEC","Nader Zein","27226","other","Discussion","In RAN4#80, the work plan on NR co-existence study for WP 5D[1] was approved. \nIn the work plan, it was agreed to check results from companies for calibration purpose at RAN4#81 meeting.\nThis contribution provides simulation results from NEC for calibrati","","410","11.3.1","Co-existence [FS_NR_newRAT]",1630000,"noted","2016-11-04T20:29:30.840","2016-11-07T12:20:30.180","","","Rel-14","38.803","0.0.1","FS_NR_newRAT","","","","","","","","",""]
["R4-1610357","BS OTA EVM requirement for NR","NEC","Nader Zein","27226","other","Approval","RAN4 has discussed BS RF requirements for NR during the past meetings. During the last meeting, a Way Forward on BS RF requirements for NR was agreed. The Way Forward includes agreements on BS EVM requirements. \nIn this contribution, NEC further considers","","421","11.5.3.1","Transmitter characteristics [FS_NR_newRAT]",973500000,"noted","2016-11-04T20:29:30.857","2016-11-07T12:20:30.180","","","Rel-14","38.803","0.0.1","FS_NR_newRAT","","","","","","","","",""]
["R4-1610358","BS OTA Receiver Sensitivity for NR","NEC","Nader Zein","27226","other","Approval","In the NR SI, BS RF requirements for NR are being considered. While there are some transmitter characteristics already discussed and some basic principles agreed, receiver characteristics have not yet been discussed. Some receiver requirements have been i","","422","11.5.3.2","Receiver characteristics [FS_NR_newRAT]",35900000,"noted","2016-11-04T20:29:30.887","2016-11-07T12:20:30.180","","","Rel-14","38.803","0.0.1","FS_NR_newRAT","","","","","","","","",""]
["R4-1610359","BS OTA Blocking Requirement for NR","NEC","Nader Zein","27226","other","Approval","In the NR SI, BS RF requirements for NR are being considered. While there are some transmitter characteristics already discussed and some basic principles agreed, receiver characteristics have not yet been discussed. Some receiver requirements have been i","","422","11.5.3.2","Receiver characteristics [FS_NR_newRAT]",99400000,"noted","2016-11-04T20:29:30.903","2016-11-07T12:20:30.180","","","Rel-14","38.803","0.0.1","FS_NR_newRAT","","","","","","","","",""]
["R4-1610360","Correction on coordinate system","NEC","Nader Zein","27226","CR","Approval","In TR37.842, two coordinate systems are adopted. One is represented by spherical angles (?,f) and used in clause 5 for co-existence study. The other one is represented by (T,F) and is used in other clauses. \n (?,f) and (T,F) are wrongly used.\nDirection of","","22","5.1.1","Technical Report (37.842) [AAS_BS_LTE_UTRA-Core]",4310000,"revised","2016-11-04T20:29:30.933","2016-11-07T12:20:30.193","","R4-1610792","Rel-13","37.842","13.0.0","AAS_BS_LTE_UTRA-Core","0012","","F","","","","","",""]
["R4-1610361","Coordinate system for eAAS","NEC","Nader Zein","27226","other","Approval","In Rel-14 AAS discussion, it is beneficial to agree a coordinate system in the earlier stage of WI. It would make the technical discussion easier and prevent delegates misunderstanding contributions from other companies.\nIn this contribution, we propose a","","209","8.12.2.1","In band requirements [AASenh_BS_LTE_UTRA]",80700,"approved","2016-11-04T20:29:31.073","2016-11-07T12:20:30.193","","","Rel-14","","","AASenh_BS_LTE_UTRA","","","","","","","","",""]
["R4-1610362","OTA EVM requirement for eAAS","NEC","Nader Zein","27226","other","Approval","RAN4 has discussed OTA EVM requirements for AAS BS during the past meetings. During the last meeting, a Way Forward was agreed on the OTA EVM requirement to be across the declared EVM directions range. In addition, the Way Forward identified some open iss","","209","8.12.2.1","In band requirements [AASenh_BS_LTE_UTRA]",4980000,"noted","2016-11-04T20:29:31.090","2016-11-07T12:20:30.193","","","Rel-14","","","AASenh_BS_LTE_UTRA","","","","","","","","",""]
["R4-1610363","OTA Receiver Sensitivity for eAAS","NEC","Nader Zein","27226","other","Approval","Receiver Sensitivity requirement for AAS Rel-14 has been discussed by RAN4. A Way Forward was agreed at the last RAN4#81bis meeting to specify the OTA sensitivity based on the conducted reference sensitivity taking into consideration losses and the Direct","","209","8.12.2.1","In band requirements [AASenh_BS_LTE_UTRA]",985400000,"noted","2016-11-04T20:29:31.107","2016-11-07T12:20:30.193","","","Rel-14","","","AASenh_BS_LTE_UTRA","","","","","","","","",""]
["R4-1610364","OTA Blocking Requirement for eAAS","NEC","Nader Zein","27226","other","Approval","During the last RAN4#80bis meeting a WF on blocking requirement was agreed to have the wanted signal and blocking interferer present simultaneously and their directions to be aligned. However, blocking signal level and metrics are still being discussed.\nI","","209","8.12.2.1","In band requirements [AASenh_BS_LTE_UTRA]",993700000,"noted","2016-11-04T20:29:31.167","2016-11-07T12:20:30.210","","","Rel-14","","","AASenh_BS_LTE_UTRA","","","","","","","","",""]
["R4-1610365","Timing and Interruption Requirements for V2X","Qualcomm Europe Inc.(France)","TIen Viet NGUYEN","67205","discussion","Approval","---","","281","8.20.4.1","UE Transmit timing [LTE_V2X-Core]",24400000,"noted","2016-11-04T20:42:12.907","2016-11-07T21:15:32.250","","","Rel-14","","","","","","","","","","","",""]
["R4-1610366","RRM: Correction to TCs A.7.1.7A and A.7.1.7B (Rel-12)","Rohde & Schwarz","Bledar Karajani","41759","CR","","---","","14","4.2.3","RRM (Radio Resource Management)  [WI code or TEI12]",367000,"agreed","2016-11-04T20:43:35.837","2016-11-04T20:55:39.947","","","Rel-12","36.133","12.13.0","TEI12","4346","","F","RP-162420","","","","",""]
["R4-1610367","RRM: Correction to TCs A.7.1.7A and A.7.1.7B (Rel-13)","Rohde & Schwarz","Bledar Karajani","41759","CR","","---","","14","4.2.3","RRM (Radio Resource Management)  [WI code or TEI12]",368000,"agreed","2016-11-04T20:43:35.930","2016-11-22T12:17:27.267","","","Rel-13","36.133","13.5.0","TEI12","4347","","A","RP-162420","","","","",""]
["R4-1610368","RRM: Correction to TCs A.7.1.7A and A.7.1.7B (Rel-14)","Rohde & Schwarz","Bledar Karajani","41759","CR","","---","","14","4.2.3","RRM (Radio Resource Management)  [WI code or TEI12]",890000,"agreed","2016-11-04T20:43:36.037","2016-11-22T12:17:27.267","","","Rel-14","36.133","14.1.0","TEI12","4348","","A","RP-162420","","","","",""]
["R4-1610369","RF: Pb setting in power imbalance TCs (Rel-12)","Rohde & Schwarz","Bledar Karajani","41759","CR","","---","","15","4.2.4","UE demodulation performance  [WI code or TEI12]",99930000,"agreed","2016-11-04T20:43:36.117","2016-11-04T20:55:13.583","","","Rel-12","36.101","12.13.0","TEI12","4109","","F","RP-162420","","","","",""]
["R4-1610370","RF: Pb setting in power imbalance TCs (Rel-13)","Rohde & Schwarz","Bledar Karajani","41759","CR","","---","","15","4.2.4","UE demodulation performance  [WI code or TEI12]",999400000,"agreed","2016-11-04T20:43:36.227","2016-11-19T17:47:26.627","","","Rel-13","36.101","13.5.0","TEI12","4110","","A","RP-162420","","","","",""]
["R4-1610371","RF: Pb setting in power imbalance TCs (Rel-14)","Rohde & Schwarz","Bledar Karajani","41759","CR","","---","","15","4.2.4","UE demodulation performance  [WI code or TEI12]",999500000,"agreed","2016-11-04T20:43:36.350","2016-11-19T17:47:26.643","","","Rel-14","36.101","14.1.0","TEI12","4111","","A","RP-162420","","","","",""]
["R4-1610372","RF: Correction to RMC for UE Category 1 in CSI tests (Rel-12)","Rohde & Schwarz","Bledar Karajani","41759","CR","","---","","15","4.2.4","UE demodulation performance  [WI code or TEI12]",38300000,"agreed","2016-11-04T20:43:36.443","2016-11-04T20:55:13.583","","","Rel-12","36.101","12.13.0","TEI12","4112","","F","RP-162420","","","","",""]
["R4-1610373","RF: Correction to RMC for UE Category 1 in CSI tests (Rel-13)","Rohde & Schwarz","Bledar Karajani","41759","CR","","---","","15","4.2.4","UE demodulation performance  [WI code or TEI12]",38400000,"agreed","2016-11-04T20:43:36.567","2016-11-19T17:47:26.643","","","Rel-13","36.101","13.5.0","TEI12","4113","","A","RP-162420","","","","",""]
["R4-1610374","RF: Correction to RMC for UE Category 1 in CSI tests (Rel-14)","Rohde & Schwarz","Bledar Karajani","41759","CR","","---","","15","4.2.4","UE demodulation performance  [WI code or TEI12]",92130000,"agreed","2016-11-04T20:43:36.693","2016-11-19T17:47:26.643","","","Rel-14","36.101","14.1.0","TEI12","4114","","A","RP-162420","","","","",""]
["R4-1610375","RF: Beamforming model missing in chapter 9 TM9 receiver Type A tests (Rel-11)","Rohde & Schwarz","Bledar Karajani","41759","CR","","---","","15","4.2.4","UE demodulation performance  [WI code or TEI12]",92240000,"revised","2016-11-04T20:43:36.803","2016-11-04T20:55:13.597","","R4-1610695","Rel-11","36.101","11.18.0","TEI11","4115","","F","","","","","",""]
["R4-1610376","RF: Beamforming model missing in chapter 9 TM9 receiver Type A tests (Rel-12)","Rohde & Schwarz","Bledar Karajani","41759","CR","","---","","15","4.2.4","UE demodulation performance  [WI code or TEI12]",92260000,"agreed","2016-11-04T20:43:36.897","2016-11-19T17:47:26.660","","","Rel-12","36.101","12.13.0","TEI11","4116","","F","RP-162413","","","","",""]
["R4-1610377","RF: Beamforming model missing in chapter 9 TM9 receiver Type A tests (Rel-13)","Rohde & Schwarz","Bledar Karajani","41759","CR","","---","","15","4.2.4","UE demodulation performance  [WI code or TEI12]",92290000,"agreed","2016-11-04T20:43:36.990","2016-11-19T17:47:26.660","","","Rel-13","36.101","13.5.0","TEI11","4117","","A","RP-162413","","","","",""]
["R4-1610378","RF: Beamforming model missing in chapter 9 TM9 receiver Type A tests (Rel-14)","Rohde & Schwarz","Bledar Karajani","41759","CR","","---","","15","4.2.4","UE demodulation performance  [WI code or TEI12]",94900000,"agreed","2016-11-04T20:43:37.083","2016-11-19T17:47:26.660","","","Rel-14","36.101","14.1.0","TEI11","4118","","A","RP-162413","","","","",""]
["R4-1610379","RF: Wrong Imcs value in MCS.11B/MCS.12B (Rel-12)","Rohde & Schwarz","Bledar Karajani","41759","CR","","---","","15","4.2.4","UE demodulation performance  [WI code or TEI12]",379000,"revised","2016-11-04T20:43:37.177","2016-11-04T20:55:13.597","","R4-1610726","Rel-12","36.101","12.13.0","TEI12","4119","","F","","","","","",""]
["R4-1610380","RF: Wrong Imcs value in MCS.11B/MCS.12B (Rel-13)","Rohde & Schwarz","Bledar Karajani","41759","CR","","---","","15","4.2.4","UE demodulation performance  [WI code or TEI12]",380000,"withdrawn","2016-11-04T20:43:37.287",null,"","","Rel-13","36.101","13.5.0","TEI12","4120","","A","","","","","",""]
["R4-1610381","RF: Wrong Imcs value in MCS.11B/MCS.12B (Rel-14)","Rohde & Schwarz","Bledar Karajani","41759","CR","","---","","15","4.2.4","UE demodulation performance  [WI code or TEI12]",381000,"withdrawn","2016-11-04T20:43:37.397",null,"","","Rel-14","36.101","14.1.0","TEI12","4121","","A","","","","","",""]
["R4-1610382","RF: Incorrect Number of EREGs per ECCE for special subframe mentioned for TC 8.7.4 (Rel-12)","Rohde & Schwarz","Bledar Karajani","41759","CR","","---","","15","4.2.4","UE demodulation performance  [WI code or TEI12]",92140000,"agreed","2016-11-04T20:43:37.503","2016-11-04T20:55:13.597","","","Rel-12","36.101","12.13.0","TEI12","4122","","F","RP-162421","","","","",""]
["R4-1610383","RF: Incorrect Number of EREGs per ECCE for special subframe mentioned for TC 8.7.4 (Rel-13)","Rohde & Schwarz","Bledar Karajani","41759","CR","","---","","15","4.2.4","UE demodulation performance  [WI code or TEI12]",92200000,"agreed","2016-11-04T20:43:37.597","2016-11-19T17:47:26.677","","","Rel-13","36.101","13.5.0","TEI12","4123","","A","RP-162421","","","","",""]
["R4-1610384","RF: Incorrect Number of EREGs per ECCE for special subframe mentioned for TC 8.7.4 (Rel-14)","Rohde & Schwarz","Bledar Karajani","41759","CR","","---","","15","4.2.4","UE demodulation performance  [WI code or TEI12]",92220000,"agreed","2016-11-04T20:43:37.677","2016-11-19T17:47:26.677","","","Rel-14","36.101","14.1.0","TEI12","4124","","A","RP-162421","","","","",""]
["R4-1610385","On updating Rel-13 AAS with latest non-AAS features","Huawei","Richard Kybett","47339","discussion","Discussion","Discusses approach on updating  AAS BS specifications to the latest releases of non-AAS","","21","5.1","Base Station (BS) RF requirements for Active Antenna System (AAS) [AAS_BS_LTE_UTRA-Core]",995800000,"noted","2016-11-04T20:44:21.417","2016-11-04T21:38:06.787","","","","","","","","","","","","","","",""]
["R4-1610386","CR to TS 37.105: Missing section 6.6.5.3","Huawei","Richard Kybett","47339","CR","Approval","Correct error in document, the indicated sub-clause has been omitted in previous version","","23","5.1.2","BS RF(37.105) [AAS_BS_LTE_UTRA-Core]",3860001,"noted","2016-11-04T20:44:21.450","2016-11-04T21:37:19.147","","","Rel-13","37.105","13.2.0","AAS_BS_LTE_UTRA-Core","0025","","F","","","","","",""]
["R4-1610387","Ad-hoc minutes","Huawei","Richard Kybett","47339","discussion","Discussion","Ad-hoc minutes","","207","8.12.1","General [AASenh_BS_LTE_UTRA]",3870000,"approved","2016-11-04T20:44:21.560","2016-11-19T17:47:26.690","","","","","","","","","","","","","","",""]
["R4-1610388","Estimating antenna gain using 3dB beam width","Huawei","Richard Kybett","47339","report","Approval","Information showing how the 36000+ estimate equation for directivity was derived.","","209","8.12.2.1","In band requirements [AASenh_BS_LTE_UTRA]",985200000,"noted","2016-11-04T20:44:21.590","2016-11-04T21:37:19.147","","","","","","","","","","","","","","",""]
["R4-1610389","Further discussion on Minimum EIS","Huawei","Richard Kybett","47339","discussion","Discussion","Discussing option between table and equation approach for deriving directivity and the antenna Loss figure","","209","8.12.2.1","In band requirements [AASenh_BS_LTE_UTRA]",993300000,"noted","2016-11-04T20:44:21.620","2016-11-04T21:37:19.160","","","","","","","","","","","","","","",""]
["R4-1610390","TP to TR 37.843 on min EIS","Huawei","Richard Kybett","47339","pCR","Approval","TP capturing agreements on minimum EIS","","209","8.12.2.1","In band requirements [AASenh_BS_LTE_UTRA]",993600000,"revised","2016-11-04T20:44:21.637","2016-11-04T21:37:19.160","","R4-1610808","","37.843","0.0.1","AASenh_BS_LTE_UTRA","","","","","","","","",""]
["R4-1610391","Discussion on Rx blocking","Huawei","Richard Kybett","47339","discussion","Discussion","Further discussion on Blocking signal with respect to the options in WF","","209","8.12.2.1","In band requirements [AASenh_BS_LTE_UTRA]",993800000,"noted","2016-11-04T20:44:21.653","2016-11-04T21:37:19.097","","","","","","","","","","","","","","",""]
["R4-1610392","Further Discussion on EVM","Huawei","Richard Kybett","47339","discussion","Approval","Response to open issues from last meeting WF.","","209","8.12.2.1","In band requirements [AASenh_BS_LTE_UTRA]",952600000,"noted","2016-11-04T20:44:21.683","2016-11-04T21:37:19.097","","","","","","","","","","","","","","",""]
["R4-1610393","TP to TR 37.843 on EVM","Huawei","Richard Kybett","47339","pCR","Approval","TP capturing agreements on EVM","","209","8.12.2.1","In band requirements [AASenh_BS_LTE_UTRA]",972900001,"approved","2016-11-04T20:44:21.700","2016-11-04T21:37:19.113","","","","37.843","0.0.1","AASenh_BS_LTE_UTRA","","","","","","","","",""]
["R4-1610394","In band spurious emissions requirements","Huawei","Richard Kybett","47339","discussion","Discussion","discussion on inband absolute requirements, testing and scaling.","","209","8.12.2.1","In band requirements [AASenh_BS_LTE_UTRA]",3630000,"noted","2016-11-04T20:44:21.730","2016-11-04T21:37:19.113","","","","","","","","","","","","","","",""]
["R4-1610395","Further Discussion on ACLR measurement","Huawei","Richard Kybett","47339","discussion","Discussion","Response to open issues relating to measuremet grid.","","209","8.12.2.1","In band requirements [AASenh_BS_LTE_UTRA]",3920000,"noted","2016-11-04T20:44:21.747","2016-11-04T21:37:19.113","","","","","","","","","","","","","","",""]
["R4-1610396","TP to TR 37.843 on ACLR","Huawei","Richard Kybett","47339","pCR","Approval","TP capturing agreements on ACLR","","209","8.12.2.1","In band requirements [AASenh_BS_LTE_UTRA]",4370000,"revised","2016-11-04T20:44:21.777","2016-11-04T21:37:19.130","","R4-1610803","","37.843","0.0.1","AASenh_BS_LTE_UTRA","","","","","","","","",""]
["R4-1610397","Discussion on merging conducted and radiated requirements","Huawei","Richard Kybett","47339","discussion","Discussion","Discussion on how to handle the existing AAS BS requirements and the new OTA requirements propose using hybrid specification as suggested in NR","","207","8.12.1","General [AASenh_BS_LTE_UTRA]",3970000,"noted","2016-11-04T20:44:21.793","2016-11-04T21:37:19.130","","","","","","","","","","","","","","",""]
["R4-1610398","Transmitter IMD requirements","Huawei","Richard Kybett","47339","discussion","Discussion","Investigate location based method of specifying interferer in IMD requirements","","210","8.12.2.2","Out of band requirements [AASenh_BS_LTE_UTRA]",4380000,"noted","2016-11-04T20:44:21.823","2016-11-04T21:37:19.130","","","","","","","","","","","","","","",""]
["R4-1610399","Estimating antenna gain for EIS and blocking requirements","Huawei","Richard Kybett","47339","discussion","Discussion","Looking at how declarations can be used for antenna gain estimates","","209","8.12.2.1","In band requirements [AASenh_BS_LTE_UTRA]",997900000,"noted","2016-11-04T20:44:21.840","2016-11-04T21:37:19.130","","","","","","","","","","","","","","",""]
["R4-1610400","TP to TR 37.843 definitions and abbreviations","Huawei","Richard Kybett","47339","pCR","Approval","Adding the definitions and abbreviations from 37.842 to 37.843","","207","8.12.1","General [AASenh_BS_LTE_UTRA]",4000000,"approved","2016-11-04T20:44:21.857","2016-11-04T21:37:19.147","","","","37.843","0.0.1","AASenh_BS_LTE_UTRA","","","","","","","","",""]
["R4-1610401","Alternative name for TRP","Huawei","Richard Kybett","47339","discussion","Approval","Propose SRP as alternative name for TRP","","209","8.12.2.1","In band requirements [AASenh_BS_LTE_UTRA]",80000,"noted","2016-11-04T20:44:21.887","2016-11-04T21:37:19.147","","","","","","","","","","","","","","",""]
["R4-1610402","Output power requirements","Huawei","Richard Kybett","47339","discussion","Discussion","Further discussion on TRP and EIRP requirements, focus on EIRP for Output power accuracy.","","421","11.5.3.1","Transmitter characteristics [FS_NR_newRAT]",96280000,"noted","2016-11-04T20:44:21.903","2016-11-04T21:38:42.263","","","","","","","","","","","","","","",""]
["R4-1610403","Unwanted emission scaling","Huawei","Richard Kybett","47339","discussion","Discussion","Discuss the scaling used in AAS and how to apply to NR (or not)","","421","11.5.3.1","Transmitter characteristics [FS_NR_newRAT]",92280000,"noted","2016-11-04T20:44:21.917","2016-11-04T21:38:42.263","","","","","","","","","","","","","","",""]
["R4-1610404","BS classes","Huawei","Richard Kybett","47339","discussion","Discussion","Further discuss what needs to be captured in specification on BS classes.","","420","11.5.3","BS RF  [FS_NR_newRAT]",973300000,"noted","2016-11-04T20:44:21.950","2016-11-04T21:38:42.263","","","","","","","","","","","","","","",""]
["R4-1610405","Views on CQI test in birdirectional HST SFN channel","Qualcomm Incorporated","Achaleshwar Sahai","63246","discussion","Discussion","---","","347","8.28.3.3","CQI reporting [LTE_high_speed]",910800000,"noted","2016-11-04T21:06:54.713","2016-11-07T16:06:18.877","","","","","","","","","","","","","","",""]
["R4-1610406","On enhanced RRM requirements in HST","Qualcomm Incorporated","Achaleshwar Sahai","63246","discussion","Discussion","---","","341","8.28.2.1","Enhancement in connected mode (DRX) [LTE_high_speed]",929600000,"noted","2016-11-04T21:06:54.730","2016-11-07T22:27:55.513","","","","","","","","","","","","","","",""]
["R4-1610407","Updated simulation results in bidirectional HST SFN channel","Qualcomm Incorporated","Achaleshwar Sahai","63246","discussion","Discussion","---","","345","8.28.3.1","Enhancement for bi-directional RRH arrangement [LTE_high_speed]",986600000,"noted","2016-11-04T21:06:54.760","2016-11-07T16:06:18.877","","","","","","","","","","","","","","",""]
["R4-1610408","On intra cell mobility enhancement in Rel-14 FeMTC","Qualcomm Incorporated","Achaleshwar Sahai","63246","discussion","Discussion","---","","320","8.25.3.2.2","RLM  [LTE_feMTC-Core]",2160000,"noted","2016-11-04T21:06:54.777","2016-11-07T16:06:18.860","","","","","","","","","","","","","","",""]
["R4-1610409","Handover enhancement via indication of System Frame Number and Repetition of PBCH in Rel-14 FeMTC","Qualcomm Incorporated","Achaleshwar Sahai","63246","discussion","Discussion","---","","322","8.25.3.2.4","Others  [LTE_feMTC-Core]",4090000,"noted","2016-11-04T21:06:54.790","2016-11-07T16:06:18.860","","","","","","","","","","","","","","",""]
["R4-1610410","Correction to EsNoc EsIot and RSRP values in Idle mode re-selection test in enhanced coverage","Qualcomm Incorporated","Achaleshwar Sahai","63246","CR","Approval","---","","87","6.1.1.3.1","Intra-frequency Cell Re-Selection [LTE_MTCe2_L1-Perf]",91390000,"noted","2016-11-04T21:06:54.807","2016-11-07T16:20:16.360","","","Rel-13","36.133","13.5.0","LTE_MTCe2_L1-Perf","4349","","F","","","","","",""]
["R4-1610411","Correction to EsNoc EsIot and RSRP values in Idle mode re-selection test in enhanced coverage","Qualcomm Incorporated","Achaleshwar Sahai","63246","CR","Approval","---","","87","6.1.1.3.1","Intra-frequency Cell Re-Selection [LTE_MTCe2_L1-Perf]",91400000,"withdrawn","2016-11-04T21:06:54.933",null,"","","Rel-14","36.133","14.1.0","LTE_MTCe2_L1-Perf","4350","","A","","","","","",""]
["R4-1610412","Correction to the handover test case in CE mode A","Qualcomm Incorporated","Achaleshwar Sahai","63246","CR","Approval","---","","81","6.1.1.2.1","Intra-frequency Handover [LTE_MTCe2_L1-Perf]",412000,"revised","2016-11-04T21:06:55.027","2016-11-07T16:20:16.360","","R4-1610660","Rel-13","36.133","13.5.0","LTE_MTCe2_L1-Perf","4351","","F","","","","","",""]
["R4-1610413","Correction to the handover test case in CE mode A","Qualcomm Incorporated, Anritsu","Achaleshwar Sahai","63246","CR","Approval","---","","81","6.1.1.2.1","Intra-frequency Handover [LTE_MTCe2_L1-Perf]",413000,"agreed","2016-11-04T21:06:55.120","2016-11-19T17:47:26.690","","","Rel-14","36.133","14.1.0","LTE_MTCe2_L1-Perf","4352","","A","RP-162382","","","","",""]
["R4-1610414","Correction to RSRP bias in idle mode reselection requirement in enhanced coverage","Qualcomm Incorporated","Achaleshwar Sahai","63246","CR","Approval","Cover page correction. Category changed to A.","","51","5.5.3.4","Others [LTE_MTCe2_L1-Core]",4140000,"revised","2016-11-04T21:06:55.243","2016-11-07T16:06:18.827","R4-168117","R4-1610722","Rel-14","36.133","14.1.0","LTE_MTCe2_L1-Core","4094","1","A","","","","","",""]
["R4-1610415","Modification to Handover Delay in CE ModeA","Qualcomm Incorporated","Achaleshwar Sahai","63246","CR","Approval","Cover page correction. Category changed to A.","","48","5.5.3.1","Evaluation of MIB and SIB reading delay, and update of requirement for handover and RRC Re-establishment [LTE_MTCe2_L1-Core]",9258000,"revised","2016-11-04T21:06:55.370","2016-11-07T16:06:18.843","R4-168129","R4-1611006","Rel-14","36.133","14.1.0","LTE_MTCe2_L1-Core","4104","1","A","","","","","",""]
["R4-1610416","Modification to Handover Delay in CE ModeB","Qualcomm Incorporated","Achaleshwar Sahai","63246","CR","Approval","Cover page correction. Category changed to A.","","48","5.5.3.1","Evaluation of MIB and SIB reading delay, and update of requirement for handover and RRC Re-establishment [LTE_MTCe2_L1-Core]",41600000,"agreed","2016-11-04T21:06:55.510","2016-11-07T16:06:18.843","R4-168134","","Rel-14","36.133","14.1.0","LTE_MTCe2_L1-Core","4108","1","A","RP-162430","","","","",""]
["R4-1610417","Modification to Handover Delay in CE ModeA","Qualcomm Incorporated","Achaleshwar Sahai","63246","CR","Approval","Cover page correction. Revision number is corrected","","48","5.5.3.1","Evaluation of MIB and SIB reading delay, and update of requirement for handover and RRC Re-establishment [LTE_MTCe2_L1-Core]",9136000,"agreed","2016-11-04T21:06:55.633","2016-11-07T16:38:56.253","R4-168649","","Rel-13","36.133","13.5.0","LTE_MTCe2_L1-Core","4103","2","F","RP-162430","","","","",""]
["R4-1610418","UE Tranmsit timing accuracy in CE mode B","Qualcomm Incorporated","Achaleshwar Sahai","63246","CR","Approval","Cover page correction. Revision number is corrected","","49","5.5.3.2","UE transmit timing [LTE_MTCe2_L1-Core]",41800000,"revised","2016-11-04T21:06:55.773","2016-11-07T16:38:56.237","R4-168652","R4-1610656","Rel-13","36.133","13.5.0","LTE_MTCe2_L1-Core","4156","2","F","","","","","",""]
["R4-1610419","PCFICH/PDCCH/PHICH Reference channel in UE Cat 0 new CGI RRM test cases","ANRITSU LTD","Ian Rose","9381","CR","","For RRM test cases A.8.1.19, A.8.1.20, A.8.1.21, A.8.1.22, A.8.2.7 and A.8.2.8, change the PCFICH/PDCCH/PHICH Reference channel to one with 2Tx antennas.","","14","4.2.3","RRM (Radio Resource Management)  [WI code or TEI12]",12500000,"agreed","2016-11-04T21:20:58.943","2016-11-19T17:47:26.723","","","Rel-13","36.133","13.5.0","LC_MTC_LTE-Perf","4353","","A","RP-162414","","","","",""]
["R4-1610420","PCFICH/PDCCH/PHICH Reference channel in UE Cat 0 new CGI RRM test cases","ANRITSU LTD","Ian Rose","9381","CR","","For RRM test cases A.8.1.19, A.8.1.20, A.8.1.21, A.8.1.22, A.8.2.7 and A.8.2.8, change the PCFICH/PDCCH/PHICH Reference channel to one with 2Tx antennas.","","14","4.2.3","RRM (Radio Resource Management)  [WI code or TEI12]",12600000,"agreed","2016-11-04T21:23:17.503","2016-11-19T17:47:26.723","","","Rel-14","36.133","14.1.0","LC_MTC_LTE-Perf","4354","","A","RP-162414","","","","",""]
["R4-1610421","eLAA UE MPR","MediaTek Inc.","James Wang","56966","other","Discussion","In this contribution, we evaluate the MPR for eLAA interlaced waveforms to meet E-UTRA ACLR 30 dB requirement with a 5 GHz WiFi PA","","244","8.18.2.1","MPR [LTE_eLAA-Core]",42100000,"noted","2016-11-04T21:29:09.240","2016-11-07T06:02:14.090","","","Rel-14","36.101","14.1.0","LTE_eLAA-Core","","","","","","","","",""]
["R4-1610422","Requirements with SRS carrier based switching","Ericsson","Iana Siomina","42857","CR","Approval","Requirements with SRS carrier based switching","","291","8.21.3","RRM core and performance (36.133) [LTE_SRS_switch-Core/Perf]",42200000,"revised","2016-11-04T21:31:54.600","2016-11-07T20:39:28.733","","R4-1610734","Rel-14","36.133","14.1.0","LTE_SRS_switch-Core","4355","","B","","","","","",""]
["R4-1610423","Exclusion range for 10MHz LAA CA combinations","Skyworks Solutions Inc.","Dominique Brunel","65099","discussion","Approval","This contribution makes proposals for REFSENS exclusion range for LAA CA combinations using 10MHz channels in band 46 based on previous work on 20MHz channels.","","40","5.4.1","UE RF and EMC [LTE_LAA-Core]",45100000,"noted","2016-11-04T21:37:35.323","2016-11-04T21:41:10.150","","","Rel-14","","","","","","","","","","","",""]
["R4-1610424","2UL CA_3A-8A MSD and test configuration for B3","MediaTek Inc.","James Wang","56966","other","Approval","In this contribution, we derive the 2UL CA_3A-8A MSD level for B3 caused by IMD5 and propose a new test configuration for consideration.","","12","4.2.1","UE RF (core / EMC)  [WI code or TEI12]",132000,"noted","2016-11-05T00:22:54.653","2016-11-07T06:02:34.057","","","","36.101","","TEI12","","","","","","","","",""]
["R4-1610425","LTE TRP and TRS BHH measurement results summary for B3, B7, B20","VODAFONE Group Plc, Telecom Italia","Tim Frost","28235","discussion","Discussion","---","","218","8.13.2","Hand phantom for smartphones [LTE_UTRA_TRP_TRS-Core]",2770000,"revised","2016-11-05T08:08:06.750","2016-11-07T17:56:09.220","","R4-1610780","Rel-14","","","","","","","","","","","",""]
["R4-1610426","Simulation Assumptions for ETSI 302 571 Sensitivity Requirements","Qualcomm Europe Inc.(France)","TIen Viet NGUYEN","67205","discussion","Approval","---","","261","8.19.1.2","Blocking  [LTE_SL_V2V-Core]",42800000,"withdrawn","2016-11-05T16:37:04.120","2016-11-06T19:34:24.963","","","Rel-14","","","","","","","","","","","",""]
["R4-1610427","DRAFT LS to RAN2 on CEN DSRC Protection Procedure in Region 1","Qualcomm Europe Inc.(France)","TIen Viet NGUYEN","67205","LS out","","---","","259","8.19.1","UE RF core maintenace (36.101)  [LTE_SL_V2V-Core]",99270000,"noted","2016-11-05T16:38:41.747","2016-11-07T21:15:32.250","","","","","","","","","","","","","","",""]
["R4-1610428","CR for meeting ETSI harmonize standard Rx requirements","Qualcomm Europe Inc.(France)","TIen Viet NGUYEN","67205","draftCR","Approval","ETSI harmornized standard defines additional RX requirements, including sensitivity level for multiples modulation and coding rates. We provide analysis that these requirements can be met with current V2V design.","","261","8.19.1.2","Blocking  [LTE_SL_V2V-Core]",963200000,"noted","2016-11-05T16:42:04.390","2016-11-06T19:35:37.567","","","Rel-14","36.785","14.0.0","LTE_SL_V2V-Core","","","","","","","","",""]
["R4-1610429","Discussion on V2V Demodulation Performance","Qualcomm Europe Inc.(France)","TIen Viet NGUYEN","67205","discussion","Approval","---","","269","8.19.4.1","Single-link PSSCH and PSCCH  [LTE_SL_V2V-Perf]",976100000,"noted","2016-11-05T19:15:21.137","2016-11-07T21:15:32.250","","","Rel-14","","","","","","","","","","","",""]
["R4-1610430","Clarification on the Rx diversity branches vs. demodulation branches terminology","Huawei","Michal Szydelko","65553","discussion","Approval","In this contribution, correction to the definition of number of active receiver units is proposed, clarifying on the Rx diversity branches vs. demodulation branches terminology.","","23","5.1.2","BS RF(37.105) [AAS_BS_LTE_UTRA-Core]",995900000,"approved","2016-11-06T10:43:52.887","2016-11-06T12:16:16.010","","","","","","AAS_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-1610431","Draft CR to TR 37.842: Merged CRs","Huawei","Michal Szydelko","65553","draftCR","Information","This Draft CR captures all CRs from the RAN4#80bis meetings, which were Agreed for the TR 37.842. This Draft CR was shared in the AAS BS reflector in order to ease work on further specification improvements and avoid \"changes of changes\". It is presented","","22","5.1.1","Technical Report (37.842) [AAS_BS_LTE_UTRA-Core]",997800000,"noted","2016-11-06T10:43:52.900","2016-11-06T12:16:15.947","","","Rel-13","37.842","13.0.0","AAS_BS_LTE_UTRA-Core","","","F","","","","","",""]
["R4-1610432","Draft CR to TS 37.105: Merged CRs","Huawei","Michal Szydelko","65553","draftCR","Information","This Draft CR captures all CRs from the RAN4#80bis meetings, which were Agreed for the TS 37.105. This Draft CR was shared in the AAS BS reflector in order to ease work on further specification improvements and avoid \"changes of changes\". It is presented","","23","5.1.2","BS RF(37.105) [AAS_BS_LTE_UTRA-Core]",996100000,"noted","2016-11-06T10:43:52.933","2016-11-06T12:16:15.963","","","Rel-13","37.105","13.2.0","AAS_BS_LTE_UTRA-Core","","","F","","","","","",""]
["R4-1610433","Draft CR to TS 37.145-1: Merged CRs","Huawei","Michal Szydelko","65553","draftCR","Information","This Draft CR captures all CRs from the RAN4#80bis meetings, which were Agreed for the TS 37.145-1. This Draft CR was shared in the AAS BS reflector in order to ease work on further specification improvements and avoid \"changes of changes\". It is presente","","25","5.1.3.1","Maintenance for TS37.145-1 [AAS_BS_LTE_UTRA-Perf]",4350000,"noted","2016-11-06T10:43:52.947","2016-11-06T12:16:15.963","","","Rel-13","37.145-1","13.0.0","AAS_BS_LTE_UTRA-Perf","","","F","","","","","",""]
["R4-1610434","Draft CR to TS 37.145-2: Merged CRs","Huawei","Michal Szydelko","65553","draftCR","Information","This Draft CR captures all CRs from the RAN4#80bis meetings, which were Agreed for the TS 37.145-2. This Draft CR was shared in the AAS BS reflector in order to ease work on further specification improvements and avoid \"changes of changes\". It is presente","","26","5.1.3.2","Maintenance for TS37.145-2 [AAS_BS_LTE_UTRA-Perf]",985000000,"noted","2016-11-06T10:43:52.963","2016-11-06T12:16:15.980","","","Rel-13","37.145-2","13.0.0","AAS_BS_LTE_UTRA-Perf","","","F","","","","","",""]
["R4-1610435","CR to TS 37.145-1: Frequency error corrections","Huawei","Michal Szydelko","65553","CR","Approval","This CR to TS37.145-1 proposes text improvements and corrections related to the frequency error requirement.","","25","5.1.3.1","Maintenance for TS37.145-1 [AAS_BS_LTE_UTRA-Perf]",4390000,"revised","2016-11-06T10:43:52.977","2016-11-06T12:16:15.980","","R4-1610798","Rel-13","37.145-1","13.0.0","AAS_BS_LTE_UTRA-Perf","0007","","D","","","","","",""]
["R4-1610436","OTA frequency error requirement for eAAS BS","Huawei","Michal Szydelko","65553","discussion","Discussion","In this contribution, discussion on the OTA frequency error requirement for the AAS BS is continued.","","209","8.12.2.1","In band requirements [AASenh_BS_LTE_UTRA]",973100000,"noted","2016-11-06T10:43:53.133","2016-11-06T12:16:15.980","","","","","","AASenh_BS_LTE_UTRA","","","","","","","","",""]
["R4-1610437","TP to TR 37.843: Remaining OTA requirements for eAAS BS","Huawei","Michal Szydelko","65553","pCR","Approval","In this contribution, TP to the TR 37.843 is proposed, extending the list of the OTA requirements to be completed in the eAAS WI.","","207","8.12.1","General [AASenh_BS_LTE_UTRA]",4010000,"revised","2016-11-06T10:43:53.167","2016-11-06T12:16:15.980","","R4-1610799","","37.843","0.0.1","AASenh_BS_LTE_UTRA","","","","","","","","",""]
["R4-1610438","Spurious emissions requirement’s frequency range for eAAS","Huawei","Michal Szydelko","65553","discussion","Discussion","In this contribution, it is proposed to align the transmitter’s spurious emission measurement lower limit for the AAS BS, with the measurement limit of the frequency range in SM.329 recommendation.","","210","8.12.2.2","Out of band requirements [AASenh_BS_LTE_UTRA]",998200000,"noted","2016-11-06T10:43:53.180","2016-11-06T12:16:15.993","","","","","","AASenh_BS_LTE_UTRA","","","","","","","","",""]
["R4-1610439","AAS BS Rx spurious emissions requirement correction","Huawei","Michal Szydelko","65553","discussion","Approval","In this contribution, we propose introduction of additional manufactures declaration in order to clarify the applicability of the Rx spurious emissions requirement and its implication on the AAS BS conformance testing.","","25","5.1.3.1","Maintenance for TS37.145-1 [AAS_BS_LTE_UTRA-Perf]",4400000,"noted","2016-11-06T10:43:53.197","2016-11-06T12:16:15.993","","","","","","AAS_BS_LTE_UTRA-Perf","","","","","","","","",""]
["R4-1610440","Clarification on the frequency error testing - data clock and frequency source","Huawei","Michal Szydelko","65553","discussion","Approval","In this contribution, we propose to address the issue observed in the frequency error definition, related to the RF frequency and the data clock source.","","25","5.1.3.1","Maintenance for TS37.145-1 [AAS_BS_LTE_UTRA-Perf]",996200000,"noted","2016-11-06T10:43:53.213","2016-11-06T12:16:15.993","","","","","","AAS_BS_LTE_UTRA-Perf","","","","","","","","",""]
["R4-1610441","Frequency error requirement for NR","Huawei","Michal Szydelko","65553","discussion","Discussion","In this contribution, discussion on the OTA frequency error requirement for the NR BS is initiated.","","421","11.5.3.1","Transmitter characteristics [FS_NR_newRAT]",973400000,"noted","2016-11-06T10:43:53.243","2016-11-06T12:16:15.993","","","","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1610442","OTA BS demodulation requirements: consideration of the eAAS and NR","Huawei","Michal Szydelko","65553","discussion","Discussion","In this contribution, we are collecting thoughts related to the work arrangement for the eAAS BS demodulation requirements application in OTA manner, considering also the ongoing discussion on the NR in RAN4.","","215","8.12.3.3","Demodulation requirements [AASenh_BS_LTE_UTRA]",4440000,"noted","2016-11-06T10:43:53.260","2016-11-06T12:16:16.010","","","","","","AASenh_BS_LTE_UTRA","","","","","","","","",""]
["R4-1610443","Spurious emissions requirement’s frequency range for NR","Huawei","Michal Szydelko","65553","discussion","Discussion","In this contribution, discussion on the NR spurious emissions requirements is continued.","","421","11.5.3.1","Transmitter characteristics [FS_NR_newRAT]",92300000,"noted","2016-11-06T10:43:53.290","2016-11-06T12:16:16.010","","","","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1610444","Overview of the eAAS BS demodulation requirements discussion","Huawei","Michal Szydelko","65553","discussion","Discussion","In this contribution, we are summarizing the discussion papers which were presented so far on the RF room, on the eAAS BS demodulation requirements application in OTA manner.","","215","8.12.3.3","Demodulation requirements [AASenh_BS_LTE_UTRA]",4420000,"noted","2016-11-06T10:43:53.307","2016-11-06T12:16:16.010","","","","","","AASenh_BS_LTE_UTRA","","","","","","","","",""]
["R4-1610445","RAN4 progress with MIMO OTA","GCF PAG, Panasonic Corporation","Valerie Townsend","9493","LS in","","---","","2","3","Letters / reports from other groups / meetings",44500000,"noted","2016-11-06T19:36:04.617","2016-11-06T19:39:09.053","","","","","","","","","","","","RAN4, CTIA MOSG","GCF PAG","CAG-16-462r2",""]
["R4-1610446","EMC Field Strength estimation for AAS","Ericsson","Asif Ali Khan","56794","other","Approval","This paper provides an estimation of the field strength levels for an AAS BS within an EMC chamber.","","211","8.12.2.3","EMC requirements [AASenh_BS_LTE_UTRA]",81100,"noted","2016-11-06T22:05:43.953","2016-11-07T14:16:15.037","","","Rel-14","","","AASenh_BS_LTE_UTRA","","","","","","","","",""]
["R4-1610447","Spurious Emissions & EMC Radiated Emission requirements for AAS","Ericsson","Asif Ali Khan","56794","other","Approval","This pape provides a proposal on how to handle the spurious emission requirements and EMC radiated emission requirements for AAS BS.","","211","8.12.2.3","EMC requirements [AASenh_BS_LTE_UTRA]",4460000,"noted","2016-11-06T22:05:43.983","2016-11-07T14:16:15.053","","","Rel-14","","","AASenh_BS_LTE_UTRA","","","","","","","","",""]
["R4-1610448","RF Blocking and EMC radiated immunity aspects for AAS","Ericsson","Asif Ali Khan","56794","other","Approval","This pape provides a proposal on how to handle the RF blocking and EMC radiated immunity requirements for AAS BS.","","211","8.12.2.3","EMC requirements [AASenh_BS_LTE_UTRA]",4470000,"noted","2016-11-06T22:05:44","2016-11-07T14:16:15.037","","","Rel-14","","","AASenh_BS_LTE_UTRA","","","","","","","","",""]
["R4-1610449","Regulatory EMC requirements for AAS","Ericsson","Asif Ali Khan","56794","discussion","Discussion","This paper provides an overview of the EMC related regulatory requirements that are applicable for AAS BS","","211","8.12.2.3","EMC requirements [AASenh_BS_LTE_UTRA]",4480000,"noted","2016-11-06T22:05:44.030","2016-11-07T14:16:15.037","","","Rel-14","","","AASenh_BS_LTE_UTRA","","","","","","","","",""]
["R4-1610450","REFSENS exclusion region specification for 10MHz LAA channels","QUALCOMM UK Ltd","Marco Papaleo","49190","other","Approval","This contribution addresses the extension of LAA exlusion region and MSD requirements for 10MHz B46","","40","5.4.1","UE RF and EMC [LTE_LAA-Core]",45200000,"noted","2016-11-07T01:53:22.017","2016-11-07T21:10:40.173","","","Rel-13","","","LTE_LAA-Core","","","","","","","","",""]
["R4-1610451","MSD and exclusion region specification for 10MHz LAA channels","QUALCOMM UK Ltd","Marco Papaleo","49190","CR","Agreement","CR to implement MSD and exclusion region requirements for 10MHz LAA channels","","40","5.4.1","UE RF and EMC [LTE_LAA-Core]",96560000,"revised","2016-11-07T01:58:46.607","2016-11-19T17:47:26.737","","R4-1611019","Rel-13","36.101","13.5.0","LTE_LAA-Core","4125","","F","","","","","",""]
["R4-1610452","MSD and exclusion region specification for 10MHz LAA channels","QUALCOMM UK Ltd","Marco Papaleo","49190","CR","Agreement","CR to implement MSD and exclusion region requirements for 10MHz LAA channels","","40","5.4.1","UE RF and EMC [LTE_LAA-Core]",99210000,"revised","2016-11-07T02:02:03.433","2016-11-19T17:47:26.737","","R4-1611020","Rel-14","36.101","14.1.0","LTE_LAA-Core","4126","","F","","","","","",""]
["R4-1610453","Proposal on the delta TIB,c and delta RIB,c for Band 3, Band 39 and Band 41 3DL/1UL CA","ZTE, Nubia, CMCC, Qorvo","Yuqiang Zhang","43207","other","Approval","In this paper, the delta TIB,c and delta RIB,c for 3DL/1UL CA_3A-39A-41A are proposed to approval.","","384","9.1.2","Filter-combiner information [FS_LTE_CA_B3_B39]",927200000,"approved","2016-11-07T03:10:33.907","2016-11-07T08:28:43.707","R4-1609272","","","","","FS_LTE_CA_B3_B39","","","","","","","","",""]
["R4-1610454","Clarification on UE MOP","CATT","Xuhua Tao","62863","CR","Approval","this is a coverpage revision of an agreed CR","","12","4.2.1","UE RF (core / EMC)  [WI code or TEI12]",0,"agreed","2016-11-07T05:52:04.753","2016-11-07T10:27:55.293","R4-168921","","Rel-12","36.101","12.13.0","","3874","2","F","RP-162459","","","","",""]
["R4-1610455","Clarification on UE MOP","CATT","Xuhua Tao","62863","CR","Approval","This is a coverpage revision of an agreed CR","","12","4.2.1","UE RF (core / EMC)  [WI code or TEI12]",990800000,"revised","2016-11-07T05:56:49.860","2016-11-07T10:27:55.293","R4-168922","R4-1610906","Rel-12","36.101","12.13.0","","3875","2","F","","","","","",""]
["R4-1610456","Clarification on UE MOP","CATT","Xuhua Tao","62863","CR","Approval","This is a coverpage revision of an agreed CR","","12","4.2.1","UE RF (core / EMC)  [WI code or TEI12]",995300000,"revised","2016-11-07T06:00:00.413","2016-11-07T10:27:55.277","R4-167530","R4-1610907","Rel-12","36.101","12.13.0","","3876","1","A","","","","","",""]
["R4-1610457","Proposed frequency bands for single Rx category 1","KDDI Corporation","Masaaki Obara","46347","other","Approval","In RAN4#80-bis, which frequency bands should be standardized for single Rx category 1 was discussed.  This paper summarizes possible bands so far.","","330","8.27.1","General [LTE_UE_cat_1RX]",4570000,"available","2016-11-07T06:16:01.140","2016-11-07T09:09:21.597","","","Rel-14","","","","","","","","","","","",""]
["R4-1610458","Missing requirements for eMTC/NB IoT UE","KDDI Corporation","Masaaki Obara","46347","CR","Agreement","In UE-UE co-existence table of Band 5, Japanese requirements are missing.","","45","5.5.1","UE RF (36.101)  [LTE_MTCe2_L1-Core]",939400000,"withdrawn","2016-11-07T06:41:29.800",null,"","","Rel-14","36.101","14.1.0","","4127","","F","","","","","",""]
["R4-1610459","TP for TR36.714-02-02: UE co-existence table for eLAA example band combinations","KDDI Corporation","Masaaki Obara","46347","pCR","Approval","In order to reduce the number of bug fix CRs, it is beneficial to capture UE co-existence table into TR.  This work was approved in R4-164676, which were handled in RAN4#79.","","243","8.18.2","UE RF (36.101) [LTE_eLAA-Core]",73500000,"noted","2016-11-07T06:57:59.963","2016-11-07T09:09:21.597","","","","36.714-02-02","0.5.0","","","","","","","","","",""]
["R4-1610460","Updated TR 36.789 v0.0.2: Multi-node tests for LAA","Ericsson","Rahman Imadur","57720","draft TR","Approval","Updated TR 36.789 v0.0.2: Multi-node tests for LAA","","139","7.1.1","General  [FS_LTE_LAA_multinode_test]",4600000,"approved","2016-11-07T08:16:32.363","2016-11-07T17:24:26.893","","","Rel-13","36.789","0.0.1","FS_LTE_LAA_multinode_test","","","","","","","","",""]
["R4-1610461","TP for TR 36.789 v0.0.2: Cleanup of section 6 of TR 36.789","Ericsson","Rahman Imadur","57720","pCR","Approval","Cleanup of section 6 of TR 36.789 to reflect that we will design two types of tests for LAA BS","","139","7.1.1","General  [FS_LTE_LAA_multinode_test]",936300000,"approved","2016-11-07T08:16:32.440","2016-11-07T17:22:46.007","","","","36.789","0.0.1","FS_LTE_LAA_multinode_test","","","","","","","","",""]
["R4-1610462","Remaining issues related to multi-node throughput tests","Ericsson, Qualcomm, Nokia, Alcatel-Lucent Shanghai Bell","Rahman Imadur","57720","other","Approval","Remaining issues for throughput tests","","140","7.1.2","Multi-node testing [FS_LTE_LAA_multinode_test]",140000,"noted","2016-11-07T08:16:32.457","2016-11-07T17:22:46.007","","","Rel-13","","","FS_LTE_LAA_multinode_test","","","","","","","","",""]
["R4-1610463","TP for TR 36.789 v0.0.2: Updates in throughput tests procedures","Ericsson","Rahman Imadur","57720","pCR","Approval","TP for TR 36.789 v0.0.2: Updates in throughput tests procedures","","141","7.1.2.1","Throughput Test [FS_LTE_LAA_multinode_test]",4630000,"noted","2016-11-07T08:16:32.487","2016-11-07T17:22:46.007","","R4-1610985","","36.789","0.0.1","FS_LTE_LAA_multinode_test","","","","","","","","",""]
["R4-1610464","TP for TR 36.789 v0.0.2: Tools and approach for Multi-node tests","Ericsson","Rahman Imadur","57720","pCR","Approval","TP for TR 36.789 v0.0.2: Tools and approach for Multi-node tests","","141","7.1.2.1","Throughput Test [FS_LTE_LAA_multinode_test]",936400000,"noted","2016-11-07T08:16:32.503","2016-11-07T17:22:46.023","","","","36.789","0.0.1","FS_LTE_LAA_multinode_test","","","","","","","","",""]
["R4-1610465","Procedures and details of outage tests for multi-node tests","Ericsson","Rahman Imadur","57720","other","Approval","Procedures and details of outage tests for multi-node tests","","142","7.1.2.2","Outage Test [FS_LTE_LAA_multinode_test]",4650000,"withdrawn","2016-11-07T08:16:32.537",null,"","","Rel-13","","","FS_LTE_LAA_multinode_test","","","","","","","","",""]
["R4-1610466","TP for TR 36.789 v0.0.2: Outage tests procedures","Ericsson","Rahman Imadur","57720","pCR","Approval","TP for TR 36.789 v0.0.2: Outage tests procedures","","142","7.1.2.2","Outage Test [FS_LTE_LAA_multinode_test]",4660000,"withdrawn","2016-11-07T08:16:32.550",null,"","","","36.789","0.0.1","FS_LTE_LAA_multinode_test","","","","","","","","",""]
["R4-1610467","UL PC accuracy in SRS carrier based switching for LTE","Ericsson","Rahman Imadur","57720","discussion","Discussion","In this contribution, we describe UE PC accuracy related to SRS carrier based switching.","","290","8.21.2","UE RF (36.101) [LTE_SRS_switch-Core]",46800000,"noted","2016-11-07T08:16:32.580","2016-11-07T16:42:01.787","","","Rel-14","","","LTE_SRS_switch-Core","","","","","","","","",""]
["R4-1610468","PC accuracy in SRS carrier based switching in UE core spec","Ericsson","Rahman Imadur","57720","CR","Approval","Introducing SRS carrier based switching in 36.101. In Section 6.3.5, absolute power tolerance value has been changed when SRS carrier based swithcing is used.","","290","8.21.2","UE RF (36.101) [LTE_SRS_switch-Core]",93670000,"revised","2016-11-07T08:16:32.597","2016-11-07T16:42:01.787","","R4-1611007","Rel-14","36.101","14.1.0","LTE_SRS_switch-Core","4128","","B","","","","","",""]
["R4-1610469","Workplan for RF core work on shortened TTI and processing time for LTE","Ericsson","Rahman Imadur","57720","other","Approval","Workplan for RF core work on shortened TTI and processing time for LTE","","402","10.1.1","General  [LTE_sTTIandPT]",938300000,"approved","2016-11-07T08:16:32.690","2016-11-07T17:03:06.483","","","Rel-15","","","LTE_sTTIandPT","","","","","","","","",""]
["R4-1610470","UL power control issues related to shortened TTI patterns","Ericsson","Rahman Imadur","57720","discussion","Discussion","In this contribution, we describe UE RF issues related to shortened TTI patterns for LTE.","","403","10.1.2","UE RF (36.101) [LTE_sTTIandPT]",4730000,"noted","2016-11-07T08:16:32.723","2016-11-07T17:03:06.483","","","Rel-15","","","LTE_sTTIandPT","","","","","","","","",""]
["R4-1610471","Way forward on UE RF issues for shortened TTI and processing time for LTE","Ericsson","Rahman Imadur","57720","other","Approval","Way forward on UE RF issues for shortened TTI and processing time for LTE","","403","10.1.2","UE RF (36.101) [LTE_sTTIandPT]",938200010,"revised","2016-11-07T08:16:32.737","2016-11-07T17:03:06.483","","R4-1610790","Rel-15","","","LTE_sTTIandPT","","","","","","","","",""]
["R4-1610472","Implication of sTTI operation on UL ON/OFF time mask","Ericsson","Rahman Imadur","57720","other","Approval","Discussions on RAN1 LS on implication of sTTI operation on UL ON/OFF time mask","","403","10.1.2","UE RF (36.101) [LTE_sTTIandPT]",4690000,"noted","2016-11-07T08:16:32.770","2016-11-07T19:50:21.957","","","Rel-15","","","LTE_sTTIandPT","","","","","","","","",""]
["R4-1610473","Reply LS to RAN1 on implication of sTTI operation on UL ON/OFF time mask","Ericsson","Rahman Imadur","57720","LS out","Approval","LS on implication of sTTI operation on UL ON/OFF time mask","","403","10.1.2","UE RF (36.101) [LTE_sTTIandPT]",4710000,"noted","2016-11-07T08:16:32.800","2016-11-07T19:50:21.957","","","Rel-15","","","LTE_sTTIandPT","","","","","","RAN1","","",""]
["R4-1610474","LBT functionality requirements for UE in Rel-14 eLAA","Ericsson","Rahman Imadur","57720","other","Approval","Discussions related to UL LBT core requirements for UE in Rel-14 eLAA.","","247","8.18.2.4","Other requirements [LTE_eLAA-Core]",9589000,"withdrawn","2016-11-07T08:16:32.817",null,"","","Rel-14","","","LTE_eLAA-Core","","","","","","","","",""]
["R4-1610475","UL LBT core requiremets in UE spec","Ericsson","Rahman Imadur","57720","CR","Approval","CR on LBT functionality requirements for UE in Rel-14 eLAA","","247","8.18.2.4","Other requirements [LTE_eLAA-Core]",9988000,"agreed","2016-11-07T08:16:32.847","2016-11-07T19:48:59.993","","","Rel-14","36.101","14.1.0","LTE_eLAA-Core","4129","","B","RP-162387","","","","",""]
["R4-1610476","LS to RAN5 on parameters for UL LBT functionalities tests","RAN4","Rahman Imadur","57720","LS out","Approval","LS on implication of sTTI operation on UL ON/OFF time mask","","247","8.18.2.4","Other requirements [LTE_eLAA-Core]",47600000,"approved","2016-11-07T08:16:32.970","2016-11-19T17:47:26.753","","","Rel-15","","","LTE_sTTIandPT","","","","","","RAN5","","",""]
["R4-1610477","Simulations results for coexistence studies in 30GHz","Ericsson","Rahman Imadur","57720","discussion","Discussion","Simulation results for 30GHz spectrum NR coexistence","","410","11.3.1","Co-existence [FS_NR_newRAT]",47700000,"noted","2016-11-07T08:16:32.987","2016-11-07T17:05:52.200","","","Rel-14","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1610478","Simulations results for coexistence studies in 45GHz","Ericsson","Rahman Imadur","57720","discussion","Discussion","Simulation results for 45GHz spectrum NR coexistence","","410","11.3.1","Co-existence [FS_NR_newRAT]",47800000,"noted","2016-11-07T08:16:33.017","2016-11-07T17:05:52.200","","","Rel-14","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1610479","Simulations results for coexistence studies in 70GHz","Ericsson","Rahman Imadur","57720","discussion","Discussion","Simulation results for 70GHz spectrum NR coexistence","","410","11.3.1","Co-existence [FS_NR_newRAT]",47900000,"noted","2016-11-07T08:16:33.033","2016-11-07T17:05:52.200","","","Rel-14","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1610480","Impact of different UL deployment cases for UMa 30GHz simulations","Ericsson","Rahman Imadur","57720","discussion","Discussion","Impact of different NF assumptions in mmwave sysem performance","","410","11.3.1","Co-existence [FS_NR_newRAT]",97750000,"withdrawn","2016-11-07T08:16:33.067",null,"","","Rel-14","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1610481","Impact of different NF assumptions in mmwave sysem performance","Ericsson","Rahman Imadur","57720","discussion","Discussion","Impact of different NF assumptions in mmwave sysem performance","","410","11.3.1","Co-existence [FS_NR_newRAT]",942000000,"noted","2016-11-07T08:16:33.097","2016-11-07T17:05:52.200","","","Rel-14","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1610482","Impact of grid shift for UMa Simulations in 30GHz","Ericsson","Rahman Imadur","57720","other","Approval","Simulation results for 30GHz spectrum NR coexistence","","410","11.3.1","Co-existence [FS_NR_newRAT]",97740000,"noted","2016-11-07T08:16:33.113","2016-11-07T17:05:52.213","","","Rel-14","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1610483","TP for NR Rel-14 TR 38.803: LO generation and phase noise aspects for mm-wave technologies","Ericsson","Rahman Imadur","57720","pCR","Approval","In this contribution, we propose texts related to LO generation and phase noise aspects of mmwave technologies for TR 38.803.","","415","11.5.1","Common issues for UE and BS [FS_NR_newRAT]",966200000,"noted","2016-11-07T08:16:33.127","2016-11-07T17:05:04.480","","","","38.803","0.3.0","FS_NR_newRAT","","","","","","","","",""]
["R4-1610484","TP for NR Rel-14 TR 38.803: PA considerations for mm-wave technologies","Ericsson","Rahman Imadur","57720","pCR","Approval","In this contribution, we propose texts related to PA considerations for TR 38.803.","","415","11.5.1","Common issues for UE and BS [FS_NR_newRAT]",966600000,"noted","2016-11-07T08:16:33.173","2016-11-07T17:05:04.463","","","","38.803","0.3.0","FS_NR_newRAT","","","","","","","","",""]
["R4-1610485","TP for NR Rel-14 TR 38.803: Noise figure for mm-wave technologies","Ericsson","Rahman Imadur","57720","pCR","Approval","In this contribution, we propose texts related to noise figure and other related aspects of mmwave technologies for TR 38.803.","","415","11.5.1","Common issues for UE and BS [FS_NR_newRAT]",966700000,"noted","2016-11-07T08:16:33.190","2016-11-07T17:05:04.463","","","","38.803","0.3.0","FS_NR_newRAT","","","","","","","","",""]
["R4-1610486","TP for NR Rel-14 TR 38.803: Carrier frequency and mm-wave technology aspects","Ericsson","Rahman Imadur","57720","pCR","Approval","TP for TR38.803","","415","11.5.1","Common issues for UE and BS [FS_NR_newRAT]",973700000,"noted","2016-11-07T08:16:33.220","2016-11-07T17:05:04.480","","","","38.803","0.3.0","FS_NR_newRAT","","","","","","","","",""]
["R4-1610487","TP for NR Rel-14 TR 38.803: Filtering aspects in mm-wave technology","Ericsson","Rahman Imadur","57720","pCR","Approval","TP for TR38.803","","415","11.5.1","Common issues for UE and BS [FS_NR_newRAT]",981600000,"noted","2016-11-07T08:16:33.237","2016-11-07T17:05:04.480","","","","38.803","0.3.0","FS_NR_newRAT","","","","","","","","",""]
["R4-1610488","TP for NR Rel-14 TR 38.803: Noise figure in mm-wave systems","Ericsson","Rahman Imadur","57720","pCR","Approval","In this contribution, we propose texts related to nosie figure of mmwave technologies for TR 38.803.","","415","11.5.1","Common issues for UE and BS [FS_NR_newRAT]",994500000,"noted","2016-11-07T08:16:33.267","2016-11-07T17:05:04.480","","","","38.803","0.3.0","FS_NR_newRAT","","","","","","","","",""]
["R4-1610489","Correction to RRM tests on dual connectivity","Ericsson, Bureau Veritas, Anritsu","Muhammad Kazmi","31117","CR","Approval","This CR defines missing values of Noc and Io in the DC test cases","","14","4.2.3","RRM (Radio Resource Management)  [WI code or TEI12]",9210000,"agreed","2016-11-07T08:29:55.170","2016-11-07T18:48:18.300","","","Rel-12","36.133","12.13.0","LTE_SC_enh_dualC-Perf","4356","","F","RP-162417","","","","",""]
["R4-1610490","Correction to RRM tests on dual connectivity","Ericsson, Bureau Veritas, Anritsu","Muhammad Kazmi","31117","CR","Approval","This CR defines missing values of Noc and Io in the DC test cases","","14","4.2.3","RRM (Radio Resource Management)  [WI code or TEI12]",9211000,"agreed","2016-11-07T08:29:55.280","2016-11-25T16:07:27.697","","","Rel-13","36.133","13.5.0","LTE_SC_enh_dualC-Perf","4357","","A","RP-162417","","","","",""]
["R4-1610491","Correction to RRM tests on dual connectivity","Ericsson, Bureau Veritas, Anritsu","Muhammad Kazmi","31117","CR","Approval","This CR defines missing values of Noc and Io in the DC test cases","","14","4.2.3","RRM (Radio Resource Management)  [WI code or TEI12]",9215000,"agreed","2016-11-07T08:29:55.420","2016-11-25T16:07:27.743","","","Rel-14","36.133","14.1.0","LTE_SC_enh_dualC-Perf","4358","","A","RP-162417","","","","",""]
["R4-1610492","Requirements for WLAN RSSI Measurement for Positioning","Ericsson","Muhammad Kazmi","31117","CR","Approval","This CR defines requirements for WLAN RSSI for positioning","","298","8.22.3.2","RAT-independent enhancement [UTRA_LTE_iPos_enh2]",4920000,"revised","2016-11-07T08:29:55.513","2016-11-07T18:48:18.313","","R4-1610647","Rel-14","36.133","14.1.0","UTRA_LTE_iPos_enh2-Core","4359","","B","","","","","",""]
["R4-1610493","Requirements for WLAN RTT Measurement for Positioning","Ericsson","Muhammad Kazmi","31117","discussion","Discussion","This paper discusses requirements for WLAN RTT for positioning","","298","8.22.3.2","RAT-independent enhancement [UTRA_LTE_iPos_enh2]",4940000,"withdrawn","2016-11-07T08:29:55.607",null,"","","Rel-14","","","UTRA_LTE_iPos_enh2-Core","","","","","","","","",""]
["R4-1610494","Requirements for Bluetooth RSSI Measurement for Positioning","Ericsson","Muhammad Kazmi","31117","discussion","Discussion","This paper discusses requirements for BT RSSI for positioning","","298","8.22.3.2","RAT-independent enhancement [UTRA_LTE_iPos_enh2]",6470000,"withdrawn","2016-11-07T08:29:55.623",null,"","","Rel-14","","","UTRA_LTE_iPos_enh2-Core","","","","","","","","",""]
["R4-1610495","Measurement requirements under MDPCCH monitoring","Ericsson","Muhammad Kazmi","31117","discussion","Discussion","This paper discusses requirements for FeMTC under MPDCCH monitoring window","","319","8.25.3.2.1","Measurement [LTE_feMTC-Core]",96180000,"withdrawn","2016-11-07T08:29:55.653",null,"","","Rel-14","","","LTE_feMTC-Core","","","","","","","","",""]
["R4-1610496","Missing requirements for eMTC/NB IoT UE","KDDI Corporation","Masaaki Obara","46347","CR","Agreement","In UE-UE co-existence table of Band 5, Japanese requirements are missing.","","45","5.5.1","UE RF (36.101)  [LTE_MTCe2_L1-Core]",959900000,"noted","2016-11-07T08:47:52.583","2016-11-07T09:09:21.613","","","Rel-13","36.101","13.5.0","","4130","","F","","","","","",""]
["R4-1610497","Missing requirements for eMTC/NB IoT UE","KDDI Corporation","Masaaki Obara","46347","CR","Agreement","In UE-UE co-existence table of Band 5, Japanese requirements are missing.","","45","5.5.1","UE RF (36.101)  [LTE_MTCe2_L1-Core]",969400001,"agreed","2016-11-07T08:51:30.937","2016-11-22T12:17:27.313","","","Rel-14","36.101","14.1.0","LTE_MTCe2_L1-Core, NB_IOT-Core","4131","","A","RP-162431","","","","",""]
["R4-1610498","On OTA eAAS receiver blocking requirements","Nokia, Alcatel-Lucent Shanghai Bell","Anthony Lo","65879","other","Approval","This document continues the discussion in [1] and clarifies the blocking signal direction.","","209","8.12.2.1","In band requirements [AASenh_BS_LTE_UTRA]",997700000,"noted","2016-11-07T09:01:04.080","2016-11-07T19:14:32.447","","","Rel-14","","","AASenh_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-1610499","OTA EVM requirements of eAAS","Nokia, Alcatel-Lucent Shanghai Bell","Anthony Lo","65879","other","Approval","In this document, we address the open issues captured in the way forward on OTA EVM for eAAS.","","209","8.12.2.1","In band requirements [AASenh_BS_LTE_UTRA]",5010000,"noted","2016-11-07T09:06:06.863","2016-11-07T19:14:54.053","","","Rel-14","","","AASenh_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-1610500","OTA ACLR: on the AAS base station coverage for measuring wanted/unwanted power emissions","Nokia, Alcatel-Lucent Shanghai Bell","Anthony Lo","65879","other","Approval","In this document, we address the open issues captured in the way forward on OTA ACLR definition.","","209","8.12.2.1","In band requirements [AASenh_BS_LTE_UTRA]",3890000,"noted","2016-11-07T09:10:17.477","2016-11-07T19:15:14.677","","","","","","AASenh_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-1610501","On power sampling grid for OTA ACLR and in-band unwanted emissions","Nokia, Alcatel-Lucent Shanghai Bell","Anthony Lo","65879","other","Approval","In this document, we present new findings of our measurement campaign and address the open issues captured in the way forward on OTA ACLR definition.","","209","8.12.2.1","In band requirements [AASenh_BS_LTE_UTRA]",3980000,"noted","2016-11-07T09:14:30.540","2016-11-07T19:15:29.310","","","Rel-14","","","AASenh_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-1610502","TP for TR36.714-02-02: Delta values for eLAA example combinations","KDDI Corporation","Masaaki Obara","46347","pCR","Approval","This contribution proposes delta values for dual uplink CA of B1+B46, B41+B46 and B42+B46.  Some editorial corrections are included as well.","","247","8.18.2.4","Other requirements [LTE_eLAA-Core]",920700000,"approved","2016-11-07T09:24:10.407","2016-11-07T09:58:31.837","","","","36.714-02-02","0.5.0","","","","","","","","","",""]
["R4-1610503","Correct InformationBitPayload for Sub-Frame 1, 6 and Max T-put of TDD PDSCH RMC","ANRITSU LTD","Ian Rose","9381","CR","","Corrects the Information Bit Payload for Sub-Frames 1, 6 of PDSCH Reference channel R.4 TDD.","","14","4.2.3","RRM (Radio Resource Management)  [WI code or TEI12]",50300000,"agreed","2016-11-07T09:26:12.990","2016-11-07T10:20:29.430","","","Rel-12","36.133","12.13.0","TEI12","4360","","F","RP-162421","","","","",""]
["R4-1610504","UE E-UTRA bands TRP/TRS requirements proposal","Sony Mobile Communications","Thomas Bolin","58174","other","Approval","UE LTE-bands TRP/TRS requirements are proposed","","218","8.13.2","Hand phantom for smartphones [LTE_UTRA_TRP_TRS-Core]",28000000,"noted","2016-11-07T09:49:35.230","2016-11-07T11:35:25.757","","","","","","","","","","","","","","",""]
["R4-1610505","Discussion on RAN5 incoming LS on NPDSCH RMC","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","Approval","---","","126","6.3.3.9","Others  [NB_IOT-Perf]",1300,"noted","2016-11-07T09:59:04.067","2016-11-07T19:39:39.953","","","","","","","","","","","","","","",""]
["R4-1610506","Reply LS on RRM NPDSCH Reference Channel for UE category NB1","Huawei, HiSilicon","Xiang (Steven) Chen","41576","LS out","Approval","---","","126","6.3.3.9","Others  [NB_IOT-Perf]",50600,"revised","2016-11-07T09:59:04.097","2016-11-07T19:39:39.970","","R4-1610588","","","","","","","","","R5-167204","RAN5","","R5-167204",""]
["R4-1610507","Proposed frequency bands for single Rx category 1","KDDI Corporation","Masaaki Obara","46347","other","Approval","NOTE: R4-1610457 was uploaded with empty so this is just resubmission of it.  If chairman simply notes R4-1610457, it would be appreciated.\n\nAbstract: In RAN4#80-bis, which frequency bands should be standardized for single Rx category 1 was discussed.  Th","","330","8.27.1","General [LTE_UE_cat_1RX]",5070000,"approved","2016-11-07T10:08:16.057","2016-11-07T10:31:19.060","","","","","","","","","","","","","","",""]
["R4-1610508","Missing requirements for eMTC/NB IoT UE","KDDI Corporation","Masaaki Obara","46347","CR","Agreement","NOTE: R4-1610496 was uploaded with empty so this is just resubmission of it.  If chairman simply notes R4-1610496, it would be appreciated.\n\nAbstract: In UE co-existence table of Band 5, Japanese requirements are missing.","","45","5.5.1","UE RF (36.101)  [LTE_MTCe2_L1-Core]",969300000,"revised","2016-11-07T10:21:54.060","2016-11-07T10:31:19.060","","R4-1610850","Rel-13","36.101","13.5.0","","4132","","F","","","","","",""]
["R4-1610509","TP for TR36.714-02-02: UE co-existence table for eLAA example band combinations","KDDI Corporation","Masaaki Obara","46347","pCR","Approval","Note: R4-1610459 was uploaded with empty so this is just resubmission of it.  If chairman simply notes R4-1610459, it would be appreciated.\n\nAbstract: In order to reduce the number of bug fix CRs, it is beneficial to capture UE co-existence table into TR.","","243","8.18.2","UE RF (36.101) [LTE_eLAA-Core]",95860000,"approved","2016-11-07T10:27:21.580","2016-11-07T10:31:19.060","","","","36.714-02-02","0.5.0","","","","","","","","","",""]
["R4-1610510","Correction of paging interruption for eMTC","Intel Corporation","Yang Tang","56725","CR","Agreement","---","","51","5.5.3.4","Others [LTE_MTCe2_L1-Core]",5100001,"agreed","2016-11-07T17:08:28.463","2016-11-07T22:52:34.130","","","Rel-14","36.133","14.1.0","LTE_MTCe2_L1-Core","4361","","A","RP-162430","","","","",""]
["R4-1610511","Correction of TRMS test case parameters","Intel Corporation","Yang Tang","56725","CR","Agreement","---","","223","8.14.2","Performance requirements [LTE_MIMO_OTA-Core]",53100000,"agreed","2016-11-07T17:08:28.570","2016-11-07T22:52:34.130","","","Rel-14","37.144","14.1.0","LTE_MIMO_OTA-Core","0004","","F","RP-162389","","","","",""]
["R4-1610512","TP on NR UE RF testability","Intel Corporation, CATR","Yang Tang","56725","other","Approval","---","","419","11.5.2.3","Testability [FS_NR_newRAT]",959800000,"noted","2016-11-07T17:08:28.680","2016-11-07T22:52:34.147","","R4-1610618","Rel-14","38.803","14.1.0","FS_NR_newRAT","","","","","","","","",""]
["R4-1610513","LTE handset TRP/TRS measurements","Intel Corporation","Yang Tang","56725","discussion","Discussion","---","","218","8.13.2","Hand phantom for smartphones [LTE_UTRA_TRP_TRS-Core]",980400000,"noted","2016-11-07T17:08:28.697","2016-11-07T22:52:34.147","","","Rel-14","37.144","14.1.0","LTE_UTRA_TRP_TRS-Core","","","","","","","","",""]
["R4-1610514","CR on NPBCH Fixed Reference Channel for NB-IoT","QUALCOMM UK Ltd","Amith Chincholi","58403","CR","Approval","This is a CR on NPBCH Fixed Reference Channel for NB-IoT","","129","6.3.4.1.1","NPBCH  [NB_IOT-Perf]",981200000,"withdrawn","2016-11-07T17:29:55.803","2016-11-07T19:29:22.350","","","Rel-13","36.101","13.5.0","","4133","","B","","","","","",""]
["R4-1610515","CR on NPBCH Fixed Reference Channel for NB-IoT","QUALCOMM UK Ltd","Amith Chincholi","58403","CR","Approval","This is a Cat A CR on NPBCH Fixed Reference Channel for NB-IoT","","129","6.3.4.1.1","NPBCH  [NB_IOT-Perf]",981300000,"withdrawn","2016-11-07T17:31:41.760","2016-11-07T19:29:22.350","","","Rel-14","36.101","14.1.0","","4134","","A","","","","","",""]
["R4-1610516","CR on RLM in-sync test without DRX under normal coverage","QUALCOMM UK Ltd","Amith Chincholi","58403","CR","Approval","This is a Cat A CR on RLM in-sync test without DRX under normal coverage","","125","6.3.3.8","Radio Link Monitoring test [NB_IOT-Perf]",2650000,"revised","2016-11-07T17:33:44.530","2016-11-07T19:42:48.230","","R4-1610587","Rel-14","36.133","14.1.0","","4362","","A","","","","","",""]
["R4-1610517","CR on RLM in-sync test without DRX under enhanced coverage","QUALCOMM UK Ltd","Amith Chincholi","58403","CR","Approval","This is a CR on RLM in-sync test without DRX under enhanced coverage","","125","6.3.3.8","Radio Link Monitoring test [NB_IOT-Perf]",2660000,"revised","2016-11-07T17:35:47.833","2016-11-07T20:11:53.230","","R4-1610586","Rel-13","36.133","13.5.0","","4363","","B","","","","","",""]
["R4-1610518","CR on RLM in-sync test without DRX under enhanced coverage","QUALCOMM UK Ltd","Amith Chincholi","58403","CR","Approval","This is a Cat A CR on RLM in-sync test without DRX under enhanced coverage","","125","6.3.3.8","Radio Link Monitoring test [NB_IOT-Perf]",3170000,"revised","2016-11-07T17:37:26.893","2016-11-07T20:11:53.230","","R4-1610585","Rel-14","36.133","14.1.0","","4364","","A","","","","","",""]
["R4-1610519","NRSRP/NRSRQ Measurement Accuracy","QUALCOMM UK Ltd","Amith Chincholi","58403","other","Approval","This is a paper with proposals on NRSRP/NRSRQ Measurement Accuracy","","118","6.3.3.1","RRM measurement accuracy [NB_IOT-Perf]",97820000,"noted","2016-11-07T17:39:56.980","2016-11-07T20:12:23.900","","","Rel-13","36.133","","","","","","","","","","",""]
["R4-1610520","Addition of TDD RMC for UL-DL configuration 0","Ericsson","Christian Bergljung","21143","CR","Approval","CR to introduce RMCs for UL-DL configuration 0 to be used for verifying that PC2 capable UEs meet PC3 requirements when configuration 0 or 6 is indicated","","195","8.9.2","UE RF (36.101) [LTE_B41_UE_PC2-Core]",5200000,"revised","2016-11-07T19:44:20.707","2016-11-07T19:48:43.193","","R4-1610824","Rel-14","36.101","14.1.0","LTE_B41_UE_PC2-Core","4135","","F","","","","","",""]
["R4-1610521","CR on NPBCH Fixed Reference Channel for NB-IoT","QUALCOMM UK Ltd","Amith Chincholi","58403","CR","Approval","This is a CR on NPBCH Fixed Reference Channel for NB-IoT","","129","6.3.4.1.1","NPBCH  [NB_IOT-Perf]",91090000,"revised","2016-11-07T19:57:02.470","2016-11-07T20:02:59.603","","R4-1610555","Rel-13","36.101","13.5.0","","4136","","B","","","","","",""]
["R4-1610522","CR on NPBCH Fixed Reference Channel for NB-IoT","QUALCOMM UK Ltd","Amith Chincholi","58403","CR","Approval","This is a Cat A CR on NPBCH Fixed Reference Channel for NB-IoT","","129","6.3.4.1.1","NPBCH  [NB_IOT-Perf]",94300000,"revised","2016-11-07T19:59:28.923","2016-11-07T20:02:59.617","","R4-1610556","Rel-14","36.101","14.1.0","","4137","","A","","","","","",""]
["R4-1610523","SNR of a phased-array receiver","Qualcomm Incorporated","Raju Hormis","67308","discussion","Discussion","The SNR of phased-array receivers are key figures-of-merit of the receiver. In this paper, we show that, if the beam-forming is performed accurately by the array, the output SNR of a phased-array  increases linearly with number of antennas.","","418","11.5.2.2","Receiver characteristics [FS_NR_newRAT]",97230000,"noted","2016-11-07T20:31:17.177","2016-11-07T22:41:51.923","","","","","","","","","","","","","","",""]
["R4-1610524","Discussion on extension of existing 2Rx CA demodulation performance requirements to 4Rx","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","Discussion","In this contribution, we would like to have further discussion on normal demodulation tests under fading condition for 4Rx UE.","","359","8.30.3.2","Extend existing 2Rx CA requirement to 4Rx [LTE_4Rx_AP_DL_CA-Perf]",524000,"noted","2016-11-07T20:54:09.557","2016-11-07T21:04:00.017","","","","","","","","","","","","","","",""]
["R4-1610525","Discussion on 3/4-layer 4Rx CA demodulation performance requirements","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","Discussion","The agreements are related to normal demodulation tests and IRC tests and there was no agreement on 3/4-layer CA tests. In this contribution, we would like to further discuss 3/4-layer CA tests.","","361","8.30.3.4","3/4-layer 4Rx CA requirement [LTE_4Rx_AP_DL_CA-Perf]",2000000000,"noted","2016-11-07T20:57:04.120","2016-11-07T21:04:00.017","","","","","","","","","","","","","","",""]
["R4-1610526","Discussion on 256QAM CA demodulation performance requirements","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","Discussion","In RAN4#80bis meeting, the agreements on 4Rx CA demodulation performance requirements were captured in [1]. But the agreements are related to normal demodulation tests and IRC tests and there was no agreement on 256QAM CA tests. In this contribution, we w","","362","8.30.3.5","4Rx 256QAM CA requirement [LTE_4Rx_AP_DL_CA-Perf]",5260000,"noted","2016-11-07T21:01:30.913","2016-11-07T21:04:00.017","","","","","","","","","","","","","","",""]
["R4-1610527","Evaluation of Phase Offsets for Channel Models","Spirent Communications","Alfonso Rodriguez-Herrera","61486","discussion","Discussion","A number of contributions have shown that phase offsets for the channel model in 25.996 produce variations in TP.  However, we observe that the some of phase offsets violate the channel model by producing significant V to H correlation.  This is discussed","","222","8.14.1","General [LTE_MIMO_OTA-Core]",91260000,"withdrawn","2016-11-07T22:14:20.227",null,"","","Rel-12","","","","","","","","","","","",""]
["R4-1610528","MPAC SCME UMi V/H Limits","Spirent Communications","Alfonso Rodriguez-Herrera","61486","discussion","Approval","The MPAC SCME UMi PDP is defined in [1], but there are currently no defined performance bounds to validate the acceptable performance.\n\nProposal 1 RAN4 accepts the presented bounds for V/H ratio of ±0.9 dB.","","223","8.14.2","Performance requirements [LTE_MIMO_OTA-Core]",923600000,"withdrawn","2016-11-07T22:23:29.660",null,"","","","","","","","","","","","","","",""]
["R4-1610529","MPAC SCME UMi PDP Limits","Spirent Communications","Alfonso Rodriguez-Herrera","61486","discussion","Approval","The MPAC SCME UMi PDP is defined in [1], but there are currently no defined performance bounds to validate the acceptable performance.  \nProposal 1: Performance bounds of (cluster power ±0.85dB and excess delay ±11ns).\nProposal 2: Performance bounds inclu","","223","8.14.2","Performance requirements [LTE_MIMO_OTA-Core]",959600000,"withdrawn","2016-11-07T22:35:48.443",null,"","","","","","","","","","","","","","",""]
["R4-1610530","Evaluation of Phase Offsets for Channel Models","Spirent Communications","Doug Reed","40990","discussion","Decision","Random seeds will create variations in 25.996 channel model, however we show that this is due to correlation between V & H components.","","222","8.14.1","General [LTE_MIMO_OTA-Core]",91560000,"noted","2016-11-07T22:54:09.243","2016-11-07T22:55:09.880","","","","","","","","","","","","","","",""]
["R4-1610531","MPAC SCME UMi V/H Limits","Spirent Communications","Doug Reed","40990","discussion","Approval","The MPAC SCME UMi V to H ratio is defined in [1], but there are currently no defined performance bounds to validate the acceptable performance.  \nProposal 1 RAN4 accepts the presented bounds for V/H ratio of ±0.9 dB.","","223","8.14.2","Performance requirements [LTE_MIMO_OTA-Core]",53200000,"approved","2016-11-07T22:56:22.827","2016-11-07T22:57:00.857","","","","","","","","","","","","","","",""]
["R4-1610532","MPAC SCME UMi PDP Limits","Spirent Communications","Doug Reed","40990","discussion","Approval","The MPAC SCME UMi PDP is defined in [1], but there are currently no defined performance bounds to validate the acceptable performance.\nProposal 1: Performance bounds of (cluster power ±0.85dB and excess delay ±11ns).\nProposal 2: Performance bounds include","","223","8.14.2","Performance requirements [LTE_MIMO_OTA-Core]",91550000,"approved","2016-11-07T22:58:26.237","2016-11-07T22:59:00.823","","","","","","","","","","","","","","",""]
["R4-1610533","Response to 3GPP RAN 4 liaison on RTT on round trip time (RTT) measurement accuracy","IEEE P802.11 Wireless LANs, Intel","Jonathan Segev","45193","LS in","","","","2","3","Letters / reports from other groups / meetings",53300000,"noted","2016-11-13T22:43:30.217","2016-11-13T22:45:39.713","","","","","","","","","","","R4-168579","RAN4","","11-16-1535-02-00az-proposed-liaison-response-to-3gpp-ran4-on-rtt",""]
["R4-1610534","Followup liaison response to 3GPP R4-164767","IEEE P802.11 WLANs, Cisco","Peter Ecclesine","56396","LS in","","","","2","3","Letters / reports from other groups / meetings",53400000,"available","2016-11-14T14:27:07.200","2016-11-14T17:53:15.833","","","","","","LTE_WLAN_radio-Perf","","","","","R4-164767","RAN4","WiFi Alliance, RAN2","11-16-1518-01-0000-followup-liaison-response-to-3gpp-r4-164767",""]
["R4-1610535","Correction to NB-IoT ON/OFF power measurement period Rel-13","Nokia, Alcatel-Lucent Shanghai Bell","Juha Korhonen","21609","CR","","","","54","5.6.2","UE RF (36.101) [NB_IOT-Core]",983200000,"revised","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609831","R4-1610595","Rel-13","36.101","13.5.0","NB_IOT-Core","4060","1","F","","","","","",""]
["R4-1610536","Inband NPBCH Peformance simulation results","Nokia, Alcatel-Lucent Shanghai Bell","Juha Korhonen","21609","discussion","","","","129","6.3.4.1.1","NPBCH  [NB_IOT-Perf]",51500000,"noted","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609318","","","","","","","","","","","","","",""]
["R4-1610537","Inband NPDCCH Peformance simulation results","Nokia, Alcatel-Lucent Shanghai Bell","Juha Korhonen","21609","discussion","","","","130","6.3.4.1.2","NPDCCH [NB_IOT-Perf]",911000000,"noted","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609320","","","","","","","","","","","","","",""]
["R4-1610538","Discussion on transmission signal pattern for NPDSCH","Huawei, Hisilicon","Juha Korhonen","21609","discussion","Discussion","","","131","6.3.4.1.3","NPDSCH [NB-IOT-Perf]",977800000,"noted","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609432","","","","","NB_IOT-Perf","","","","","","","","",""]
["R4-1610539","Way forward on NB-IoT BS demodulation performance","Huawei","Juha Korhonen","21609","discussion","Approval","","","132","6.3.4.2","BS Demodulation  [NB_IOT-Perf]",943800000,"revised","2016-11-18T23:00:00","2016-11-18T23:00:00","","R4-1610559","","","","","","","","","","","","",""]
["R4-1610540","A-MPR for NB-IoT","Ericsson","Juha Korhonen","21609","CR","Approval","","","54","5.6.2","UE RF (36.101) [NB_IOT-Core]",54000000,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609882","","Rel-14","36.101","14.1.0","NB_IOT-Core","4068","1","A","RP-162433","","","","",""]
["R4-1610541","NB-IoT aggregate power control Rel-13","Nokia, Alcatel-Lucent Shanghai Bell","Juha Korhonen","21609","CR","","","","54","5.6.2","UE RF (36.101) [NB_IOT-Core]",54200000,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609824","","Rel-13","36.101","13.5.0","NB_IOT-Core","4058","1","F","RP-162433","","","","",""]
["R4-1610542","Draft Reply LS on RF requirements for category NB1 UEs","Nokia, Alcatel-Lucent Shanghai Bell","Juha Korhonen","21609","LS out","Approval","","","54","5.6.2","UE RF (36.101) [NB_IOT-Core]",982900000,"revised","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609830","R4-1610596","","","","NB_IOT-Core","","","","","","","","",""]
["R4-1610543","Introduction of NB-IoT into 36.141","Huawei, Ericsson, Nokia","Juha Korhonen","21609","CR","Agreement","","","113","6.3.2","BS RF conformance testing (36.141) [NB_IOT-Perf]",54400000,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609388","","Rel-13","36.141","13.5.0","NB_IOT-Perf","0923","1","B","RP-162380","","","","",""]
["R4-1610544","CR for 36.113: Introduction of NB-IoT","Huawei","Juha Korhonen","21609","CR","Agreement","","","113","6.3.2","BS RF conformance testing (36.141) [NB_IOT-Perf]",938800000,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609390","","Rel-13","36.113","13.2.0","NB_IOT-Perf","0061","1","B","RP-162380","","","","",""]
["R4-1610545","CR on NPDSCH RMC","Huawei, HiSilicon","Juha Korhonen","21609","CR","Approval","","","126","6.3.3.9","Others  [NB_IOT-Perf]",1600,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610015","","Rel-13","36.133","13.5.0","NB_IOT-Perf","4242","1","F","RP-162380","","","","",""]
["R4-1610546","CR: UE transmit timing requirement for NB-IoT in normal coverage (Rel-13)","Nokia, Alcatel-Lucent Shanghai Bell","Juha Korhonen","21609","CR","Approval","","","56","5.6.4","RRM core (36.133)  [NB_IOT-Core]",9314000,"withdrawn","2016-11-24T01:31:49.810",null,"R4-1609620","","Rel-13","36.133","13.5.0","NB_IOT-Core","4226","1","F","","","","","",""]
["R4-1610547","Summary of NB-IoT SI acquisition delay simulation results","Intel Corporation","Juha Korhonen","21609","discussion","Discussion","","","56","5.6.4","RRM core (36.133)  [NB_IOT-Core]",953700000,"noted","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609146","","Rel-13","36.133","","NB_IOT-Perf","","","","","","","","",""]
["R4-1610548","CR on RRC re-establishment RRM requirement","Huawei, HiSilicon","Juha Korhonen","21609","CR","Approval","","","56","5.6.4","RRM core (36.133)  [NB_IOT-Core]",962000000,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610037","","Rel-13","36.133","13.5.0","NB_IOT-Core","4263","1","F","RP-162433","","","","",""]
["R4-1610549","Clarification to applicability of NRSRQ for UE category NB1","Nokia, Alcatel-Lucent Shanghai Bell","Juha Korhonen","21609","CR","Approval","","","117","6.3.3","RRM (36.133) [NB_IOT-Perf]",54900001,"revised","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609311","R4-1610630","Rel-13","36.133","13.5.0","","4205","1","F","","","","","",""]
["R4-1610550","Introducing agreed measurement accuracy for UE Category NB1","Nokia, Alcatel-Lucent Shanghai Bell","Juha Korhonen","21609","CR","Approval","","","117","6.3.3","RRM (36.133) [NB_IOT-Perf]",0,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609315","","Rel-13","36.133","13.5.0","NB_IOT-Perf","4209","1","F","RP-162456","","","","",""]
["R4-1610551","Introducing agreed measurement accuracy for UE Category NB1","Nokia, Alcatel-Lucent Shanghai Bell","Juha Korhonen","21609","CR","Approval","","","117","6.3.3","RRM (36.133) [NB_IOT-Perf]",931500011,"revised","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609316","R4-1611021","Rel-14","36.133","14.1.0","","4210","1","A","","","","","",""]
["R4-1610552","CR to TS 37.113 - Introduction of NB-IoT","Ericsson","Juha Korhonen","21609","CR","Approval","","","113","6.3.2","BS RF conformance testing (36.141) [NB_IOT-Perf]",953400000,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609534","","Rel-13","37.113","13.2.0","NB_IOT-Perf","0053","1","B","RP-162380","","","","",""]
["R4-1610553","Simulation summary of NB-IoT UE demodulation requirements","Ericsson","Juha Korhonen","21609","other","Information","","","128","6.3.4.1","UE Demodulation  [NB_IOT-Perf]",55400000,"noted","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609677","","Rel-13","","","NB_IOT-Perf","","","","","","","","",""]
["R4-1610554","Way forward on NB-IoT UE demodulation requirements","Ericsson","Juha Korhonen","21609","discussion","Discussion","","","128","6.3.4.1","UE Demodulation  [NB_IOT-Perf]",967800000,"withdrawn","2016-11-24T01:31:51.697",null,"R4-1609678","","Rel-13","","","NB_IOT-Perf","","","","","","","","",""]
["R4-1610555","CR on NPBCH Fixed Reference Channel for NB-IoT","QUALCOMM UK Ltd","Juha Korhonen","21609","CR","Approval","","","129","6.3.4.1.1","NPBCH  [NB_IOT-Perf]",93180000,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610521","","Rel-13","36.101","13.5.0","NB_IOT-Perf","4136","1","B","RP-162380","","","","",""]
["R4-1610556","CR on NPBCH Fixed Reference Channel for NB-IoT","QUALCOMM UK Ltd","Juha Korhonen","21609","CR","Approval","","","129","6.3.4.1.1","NPBCH  [NB_IOT-Perf]",95170000,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610522","","Rel-14","36.101","14.1.0","NB_IOT-Perf","4137","1","A","RP-162380","","","","",""]
["R4-1610557","Correction of NPDCCH demodulation requirements","Ericsson","Juha Korhonen","21609","CR","Approval","","","130","6.3.4.1.2","NPDCCH [NB_IOT-Perf]",967300000,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609675","","Rel-13","36.101","13.5.0","NB_IOT-Perf","4041","1","F","RP-162380","","","","",""]
["R4-1610558","Updates to CR for NPDSCH (Rel-13)","Huawei, Hisilicon","Juha Korhonen","21609","CR","Agreement","","","131","6.3.4.1.3","NPDSCH [NB-IOT-Perf]",943500000,"revised","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609434","R4-1610614","Rel-13","36.101","13.5.0","NB_IOT-Perf","4004","1","F","","","","","",""]
["R4-1610559","Way forward on NB-IoT BS demodulation performance","Huawei","Juha Korhonen","21609","discussion","Approval","","","132","6.3.4.2","BS Demodulation  [NB_IOT-Perf]",954300000,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610539","","","","","","","","","","","","","",""]
["R4-1610560","CR: Demodulation requirements for NPRACH (Rel-13)","Huawei","Juha Korhonen","21609","CR","Agreement","","","133","6.3.4.2.1","NPRACH  [NB_IOT-Perf]",934100000,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609442","","Rel-13","36.104","13.5.0","NB_IOT-Perf","0890","1","B","RP-162380","","","","",""]
["R4-1610561","CR: NPRACH performance requirements (Rel-13, TS36.141)","Nokia, Alcatel-Lucent Shanghai Bell","Juha Korhonen","21609","CR","Approval","","","133","6.3.4.2.1","NPRACH  [NB_IOT-Perf]",944300000,"revised","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609244","R4-1611013","Rel-13","36.104","13.5.0","NB_IOT-Perf","0885","1","B","","","","","",""]
["R4-1610562","CR to TS 37.141 Rel 13 - Introduction of NB-IoT","Ericsson","Juha Korhonen","21609","CR","Approval","","","113","6.3.2","BS RF conformance testing (36.141) [NB_IOT-Perf]",939000000,"revised","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609532","R4-1610607","Rel-13","37.141","13.4.0","NB_IOT-Perf","0476","1","B","","","","","",""]
["R4-1610563","Updates to NPUSCH format 1 demod perf requirements(Rel-13)","Huawei","Juha Korhonen","21609","CR","Agreement","","","134","6.3.4.2.2","NPUSCH format 1 [NB_IOT-Perf]",944400000,"revised","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609444","R4-1610623","Rel-13","36.104","13.5.0","NB_IOT-Perf","0892","1","F","","","","","",""]
["R4-1610564","Updates to NPUSCH format 1 demod conformance test(Rel-13)","Huawei","Juha Korhonen","21609","CR","Agreement","","","134","6.3.4.2.2","NPUSCH format 1 [NB_IOT-Perf]",944600001,"revised","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609446","R4-1610624","Rel-13","36.141","13.5.0","NB_IOT-Perf","0925","1","F","","","","","",""]
["R4-1610565","CR: Updates to demodulation requirements for NPUSCH format 2 (Rel-13)","Huawei","Juha Korhonen","21609","CR","Agreement","","","135","6.3.4.2.3","NPUSCH format 2 [NB_IOT-Perf]",944800000,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609448","","Rel-13","36.104","13.5.0","NB_IOT-Perf","0894","1","F","RP-162380","","","","",""]
["R4-1610566","Updates to NPUSCH format 2 demod conformance test(Rel-13)","Huawei","Juha Korhonen","21609","CR","Agreement","","","135","6.3.4.2.3","NPUSCH format 2 [NB_IOT-Perf]",945100000,"revised","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609450","R4-1610615","Rel-13","36.141","13.5.0","NB_IOT-Perf","0927","1","F","","","","","",""]
["R4-1610567","NR coexistence calibration results in indoor scenario","Huawei, Hisilicon","Juha Korhonen","21609","discussion","Discussion","","","410","11.3.1","Co-existence [FS_NR_newRAT]",161000,"noted","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609405","","","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1610568","NR coexistence calibration results in dense urban scenario","Huawei, Hisilicon","Juha Korhonen","21609","discussion","Discussion","","","410","11.3.1","Co-existence [FS_NR_newRAT]",567000,"noted","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609408","","","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1610569","WF on urban marco scenario for coexistence study for WP5D on new radio access technology","Nokia, Alcatel-Lucent Shanghai Bell, Qualcomm, Samsung, CATT, ZTE, NTT DOCOMO, Intel, Ericsson","Juha Korhonen","21609","other","Approval","","","410","11.3.1","Co-existence [FS_NR_newRAT]",48200000,"revised","2016-11-18T23:00:00","2016-11-18T23:00:00","","R4-1610634","","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1610570","TP for 38.803 SINR vs throughput mapping","Huawei, Hisilicon","Juha Korhonen","21609","pCR","Discussion","","","410","11.3.1","Co-existence [FS_NR_newRAT]",941000010,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609409","","","38.803","0.3.0","FS_NR_newRAT","","","","","","","","",""]
["R4-1610571","Summary of simulation results for calibration on NR coexistence study for WP5D","DOCOMO Communications Lab.","Juha Korhonen","21609","other","Information","","","410","11.3.1","Co-existence [FS_NR_newRAT]",950000010,"noted","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610157","","","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1610572","TP on Co-existence simulation scenario, assumption, and methodology for TR 38.803","DOCOMO Communications Lab.","Juha Korhonen","21609","pCR","","","","410","11.3.1","Co-existence [FS_NR_newRAT]",0,"withdrawn","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610160","","","38.803","0.3.0","FS_NR_newRAT","","","","","","","","",""]
["R4-1610573","TP to 38.803: ACLR & ACS assumptions for simulation","Ericsson","Juha Korhonen","21609","pCR","Approval","","","412","11.3.3","others  [FS_NR_newRAT]",994400010,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609944","","","38.803","0.3.0","FS_NR_newRAT","","","","","","","","",""]
["R4-1610574","Guidance on how to contribute to each session for NR and eAAS","Ericsson","Juha Korhonen","21609","discussion","Approval","","","420","11.5.3","BS RF  [FS_NR_newRAT]",57600000,"revised","2016-11-18T23:00:00","2016-11-18T23:00:00","","R4-1610632","","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1610575","Way forward on NR BS requirements prioritization for mm wave","Ericsson","Juha Korhonen","21609","discussion","Endorsement","","","420","11.5.3","BS RF  [FS_NR_newRAT]",62900000,"revised","2016-11-18T23:00:00","2016-11-18T23:00:00","","R4-1610633","","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1610576","Way forward on NR BS specific new requirements","NTT DOCOMO, INC.","Juha Korhonen","21609","discussion","Endorsement","","","420","11.5.3","BS RF  [FS_NR_newRAT]",985500000,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","","","","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1610577","CR on PHR requirement for NB-IoT","Huawei, HiSilicon","Juha Korhonen","21609","CR","Approval","","","119","6.3.3.2","Power headroom [NB_IOT-Perf]",1200,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610011","","Rel-13","36.133","13.5.0","NB_IOT-Perf","4238","1","F","RP-162380","","","","",""]
["R4-1610578","Intra-frequency cell reselection under normal coverage for NB-IOT","Ericsson","Juha Korhonen","21609","CR","Approval","","","120","6.3.3.3","Cell Re-selection test [NB_IOT-Perf]",2340010,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610230","","Rel-13","36.133","13.5.0","NB_IOT-Perf","4314","1","B","RP-162380","","","","",""]
["R4-1610579","Inter-frequency cell reselection under enhanced coverage for NB-IOT","Ericsson","Juha Korhonen","21609","CR","Approval","","","120","6.3.3.3","Cell Re-selection test [NB_IOT-Perf]",2300010,"withdrawn","2016-11-24T01:31:57.407",null,"R4-1610228","","Rel-13","36.133","13.5.0","NB_IOT-Perf","4312","1","B","","","","","",""]
["R4-1610580","Intra-frequency cell reselection under enhanced coverage for NB-IOT","Ericsson","Juha Korhonen","21609","CR","Approval","","","120","6.3.3.3","Cell Re-selection test [NB_IOT-Perf]",2330010,"withdrawn","2016-11-24T01:31:57.657",null,"R4-1610229","","Rel-13","36.133","13.5.0","NB_IOT-Perf","4313","1","B","","","","","",""]
["R4-1610581","nn","NB-IoT_and_NR","Juha Korhonen","21609","other","Discussion","","","432","15","Any other business",58100000,"reserved","2016-11-24T01:31:57.907",null,"","","","","","","","","","","","","","",""]
["R4-1610582","RLM in-sync test with DRX under normal coverage","Ericsson","Juha Korhonen","21609","CR","Approval","","","125","6.3.3.8","Radio Link Monitoring test [NB_IOT-Perf]",2270000,"revised","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610227","R4-1610608","Rel-13","36.133","13.5.0","NB_IOT-Perf","4311","1","B","","","","","",""]
["R4-1610583","RLM in-sync test DRX under enhanced coverage","Ericsson","Juha Korhonen","21609","CR","Approval","","","125","6.3.3.8","Radio Link Monitoring test [NB_IOT-Perf]",2310011,"revised","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610226","R4-1610610","Rel-13","36.133","13.5.0","NB_IOT-Perf","4310","1","B","","","","","",""]
["R4-1610584","CR on RLM in-sync test without DRX under normal coverage","QUALCOMM UK Ltd","Juha Korhonen","21609","CR","Approval","","","125","6.3.3.8","Radio Link Monitoring test [NB_IOT-Perf]",2610010,"revised","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610317","R4-1610613","Rel-13","36.133","13.5.0","","4339","1","B","","","","","",""]
["R4-1610585","CR on RLM in-sync test without DRX under enhanced coverage","Qualcomm Incorporated","Juha Korhonen","21609","CR","Approval","","","125","6.3.3.8","Radio Link Monitoring test [NB_IOT-Perf]",3170010,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610518","","Rel-14","36.133","14.1.0","NB_IOT-Perf","4364","1","A","RP-162380","","","","",""]
["R4-1610586","CR on RLM in-sync test without DRX under enhanced coverage","QUALCOMM UK Ltd","Juha Korhonen","21609","CR","Approval","","","125","6.3.3.8","Radio Link Monitoring test [NB_IOT-Perf]",2660010,"revised","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610517","R4-1610612","Rel-13","36.133","13.5.0","","4363","1","B","","","","","",""]
["R4-1610587","CR on RLM in-sync test without DRX under normal coverage","Qualcomm Incorporated","Juha Korhonen","21609","CR","Approval","","","125","6.3.3.8","Radio Link Monitoring test [NB_IOT-Perf]",2650010,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610516","","Rel-14","36.133","14.1.0","NB_IOT-Perf","4362","1","A","RP-162380","","","","",""]
["R4-1610588","Reply LS on RRM NPDSCH Reference Channel for UE category NB1","Qualcomm Incorporated","Juha Korhonen","21609","LS out","Approval","","","126","6.3.3.9","Others  [NB_IOT-Perf]",54500,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610506","","Rel-13","","","NB_IOT-Perf","","","","","R5-167204","RAN5","","R5-167204",""]
["R4-1610589","CR on paging interruption for NB-IoT","Huawei, HiSilicon","Juha Korhonen","21609","CR","Approval","","","56","5.6.4","RRM core (36.133)  [NB_IOT-Core]",968000000,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610039","","Rel-13","36.133","13.5.0","","4265","1","F","RP-162433","","","","",""]
["R4-1610590","WF on channel bandwidth and transmission bandwidth configuration for NR","DOCOMO Communications Lab.","Juha Korhonen","21609","discussion","Endorsement","This contribution is for approval. In this contribution, we provide our preliminary analysis on specification impact of the new concept from view point of UE RF requirements.","","407","11.1","General   [FS_NR_newRAT]",35500000,"revised","2016-11-18T23:00:00","2016-11-18T23:00:00","","R4-1610920","","","","","","","","","","","","",""]
["R4-1610591","Draft reply LS on wider bandwidth operation for NR","Ericsson","Juha Korhonen","21609","LS out","Approval","","","407","11.1","General   [FS_NR_newRAT]",941600000,"withdrawn","2016-11-24T01:32:00.307",null,"R4-1609947","","Rel-14","","","FS_NR_newRAT","","","","","R1-1610655","RAN1","RAN2","R1-1610655",""]
["R4-1610592","LS on Suitability of technical conditions of ECC DEC (11) 06 for 5G","Ericsson","Juha Korhonen","21609","LS out","Agreement","","","407","11.1","General   [FS_NR_newRAT]",965900000,"revised","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609629","R4-1610994","Rel-14","","","FS_NR_newRAT","","","","","R4-1609013","ECC PT1","ETSI ERM","",""]
["R4-1610593","Way forward on in-band requirement for NR","Nokia, Alcatel-Lucent Shanghai Bell","Juha Korhonen","21609","discussion","Endorsement","","","415","11.5.1","Common issues for UE and BS [FS_NR_newRAT]",92410000,"revised","2016-11-18T23:00:00","2016-11-18T23:00:00","","R4-1610921","","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1610594","TP for 38.803: UE beamforming and number of UE transmitter antennas","Ericsson, Sony","Juha Korhonen","21609","pCR","Approval","","","417","11.5.2.1","Transmitter characteristics [FS_NR_newRAT]",972200001,"available","2016-11-24T01:32:00.837","2016-11-24T01:37:26.613","R4-1609592","","","38.803","0.3.0","FS_NR_newRAT","","","","","","","","",""]
["R4-1610595","Correction to NB-IoT ON/OFF power measurement period Rel-13","Nokia, Alcatel-Lucent Shanghai Bell","Juha Korhonen","21609","CR","","","","54","5.6.2","UE RF (36.101) [NB_IOT-Core]",983200001,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610535","","Rel-13","36.101","13.5.0","NB_IOT-Core","4060","2","F","RP-162433","","","","",""]
["R4-1610596","Draft Reply LS on RF requirements for category NB1 UEs","Nokia, Alcatel-Lucent Shanghai Bell","Juha Korhonen","21609","LS out","Approval","","","54","5.6.2","UE RF (36.101) [NB_IOT-Core]",983000000,"revised","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610542","R4-1610809","","","","NB_IOT-Core","","","","","","","","",""]
["R4-1610597","Way forward on simulation assumptions for SI acquisition for NB-IoT","Ericsson","Juha Korhonen","21609","discussion","Endorsement","","","56","5.6.4","RRM core (36.133)  [NB_IOT-Core]",54600000,"revised","2016-11-18T23:00:00","2016-11-18T23:00:00","","R4-1610599","","","","NB_IOT-Core","","","","","","","","",""]
["R4-1610598","CR on test parameter for RRC re-establishment","Huawei, HiSilicon","Juha Korhonen","21609","CR","Approval","","","121","6.3.3.4","RRC Re-establishment test [NB_IOT-Perf]",1801,"revised","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610017","R4-1610600","Rel-13","36.133","13.5.0","","4244","1","F","","","","","",""]
["R4-1610599","Way forward on simulation assumptions for SI acquisition for NB-IoT","Ericsson","Juha Korhonen","21609","discussion","Endorsement","","","56","5.6.4","RRM core (36.133)  [NB_IOT-Core]",54600001,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610597","","","","","NB_IOT-Core","","","","","","","","",""]
["R4-1610600","CR on test parameter for RRC re-establishment","Huawei, HiSilicon","Juha Korhonen","21609","CR","Approval","","","121","6.3.3.4","RRC Re-establishment test [NB_IOT-Perf]",1802,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610598","","Rel-13","36.133","13.5.0","NB_IOT-Perf","4244","2","F","RP-162380","","","","",""]
["R4-1610601","nn","NB-IoT_and_NR","Juha Korhonen","21609","other","Discussion","","","432","15","Any other business",60100000,"reserved","2016-11-24T01:32:02.320",null,"","","","","","","","","","","","","","",""]
["R4-1610602","Intra-frequency cell reselection under normal coverage for NB-IOT","Ericsson","Juha Korhonen","21609","CR","Approval","","","120","6.3.3.3","Cell Re-selection test [NB_IOT-Perf]",2620000,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610235","","Rel-14","36.133","14.1.0","NB_IOT-Perf","4319","1","A","RP-162381","","","","",""]
["R4-1610603","CR on test parameter for RRC re-establishment R14","Huawei, HiSilicon","Juha Korhonen","21609","CR","Approval","","","121","6.3.3.4","RRC Re-establishment test [NB_IOT-Perf]",1800001,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610018","","Rel-14","36.133","14.1.0","NB_IOT-Perf","4245","1","F","RP-162381","","","","",""]
["R4-1610604","TP for TR 38.803: Micro-wave and millimetre-wave antenna considerations","Ericsson","Juha Korhonen","21609","pCR","Approval","","","420","11.5.3","BS RF  [FS_NR_newRAT]",994900001,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609857","","","38.803","0.3.0","FS_NR_newRAT","","","","","","","","",""]
["R4-1610605","Updated Simulation Results for NB-IoT NPUSCH Format 1","Nokia, Alcatel-Lucent Shanghai Bell","Juha Korhonen","21609","discussion","Discussion","","","134","6.3.4.2.2","NPUSCH format 1 [NB_IOT-Perf]",56300001,"noted","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609251","","","","","","","","","","","","","",""]
["R4-1610606","Updated summary for NB-IoT BS simulation results","Nokia","Juha Korhonen","21609","discussion","Information","","","132","6.3.4.2","BS Demodulation  [NB_IOT-Perf]",924200000,"noted","2016-11-18T23:00:00","2016-11-18T23:00:00","","","","","","NB_IOT-Perf","","","","","","","","",""]
["R4-1610607","CR to TS 37.141 introducing NB-IoT","Ericsson, Alcatel-Lucent Shanghai Bell, Huawei","Juha Korhonen","21609","CR","Approval","","","113","6.3.2","BS RF conformance testing (36.141) [NB_IOT-Perf]",939100000,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610562","","Rel-13","37.141","13.4.0","NB_IOT-Perf","0476","2","B","RP-162381","","","","",""]
["R4-1610608","RLM in-sync test with DRX under normal coverage","Ericsson","Juha Korhonen","21609","CR","Approval","","","125","6.3.3.8","Radio Link Monitoring test [NB_IOT-Perf]",2270001,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610582","","Rel-13","36.133","13.5.0","NB_IOT-Perf","4311","2","B","RP-162381","","","","",""]
["R4-1610609","RLM in-sync test with DRX under normal coverage","Ericsson","Juha Korhonen","21609","CR","Approval","","","125","6.3.3.8","Radio Link Monitoring test [NB_IOT-Perf]",2310001,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610232","","Rel-14","36.133","14.1.0","NB_IOT-Perf","4316","1","A","RP-162381","","","","",""]
["R4-1610610","RLM in-sync test DRX under enhanced coverage","Ericsson","Juha Korhonen","21609","CR","Approval","","","125","6.3.3.8","Radio Link Monitoring test [NB_IOT-Perf]",2310012,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610583","","Rel-13","36.133","13.5.0","NB_IOT-Perf","4310","2","B","RP-162381","","","","",""]
["R4-1610611","RLM in-sync test DRX under enhanced coverage","Ericsson","Juha Korhonen","21609","CR","Approval","","","125","6.3.3.8","Radio Link Monitoring test [NB_IOT-Perf]",2320001,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610231","","Rel-14","36.133","14.1.0","NB_IOT-Perf","4315","1","A","RP-162381","","","","",""]
["R4-1610612","CR on RLM in-sync test without DRX under enhanced coverage","Qualcomm Incorporated","Juha Korhonen","21609","CR","Approval","","","125","6.3.3.8","Radio Link Monitoring test [NB_IOT-Perf]",2660011,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610586","","Rel-13","36.133","13.5.0","NB_IOT-Perf","4363","2","B","RP-162381","","","","",""]
["R4-1610613","CR on RLM in-sync test without DRX under normal coverage","Qualcomm Incorporated","Juha Korhonen","21609","CR","Approval","","","125","6.3.3.8","Radio Link Monitoring test [NB_IOT-Perf]",2610011,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610584","","Rel-13","36.133","13.5.0","NB_IOT-Perf","4339","2","B","RP-162381","","","","",""]
["R4-1610614","CR: Updates to NPDSCH demodulation requirements for NB-IoT (Rel-13)","Huawei, Hisilicon","Juha Korhonen","21609","CR","Agreement","","","131","6.3.4.1.3","NPDSCH [NB-IOT-Perf]",943500001,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610558","","Rel-13","36.101","13.5.0","NB_IOT-Perf","4004","2","F","RP-162381","","","","",""]
["R4-1610615","CR: Updates to NPUSCH format 2 demodulation conformance test (Rel-13)","Huawei","Juha Korhonen","21609","CR","Agreement","","","135","6.3.4.2.3","NPUSCH format 2 [NB_IOT-Perf]",945100001,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610566","","Rel-13","36.141","13.5.0","NB_IOT-Perf","0927","2","F","RP-162381","","","","",""]
["R4-1610616","Way forward on IMT paramters WP 5D","Ericsson","Juha Korhonen","21609","discussion","Endorsement","","","411","11.3.2","RF parameters not related co-existence [FS_NR_newRAT]",61600000,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","","","","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1610617","TP for NR Rel-14 TR 38.803: TDD timing budget","Ericsson","Juha Korhonen","21609","pCR","Approval","","","415","11.5.1","Common issues for UE and BS [FS_NR_newRAT]",950500001,"noted","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609527","","","38.803","0.3.0","FS_NR_newRAT","","","","","","","","",""]
["R4-1610618","TP on NR UE RF testability","Intel Corporation, CATR","Juha Korhonen","21609","other","Approval","","","419","11.5.2.3","Testability [FS_NR_newRAT]",959800001,"withdrawn","2016-11-24T01:32:06.437",null,"R4-1610512","","Rel-14","38.803","14.1.0","FS_NR_newRAT","","","","","","","","",""]
["R4-1610619","Way forward on BS RF requirementss for NR","Nokia","Juha Korhonen","21609","discussion","Endorsement","","","420","11.5.3","BS RF  [FS_NR_newRAT]",40400000,"revised","2016-11-18T23:00:00","2016-11-18T23:00:00","","R4-1610923","","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1610620","Way forward on NR UE RF requirements","Qualcomm","Juha Korhonen","21609","discussion","Approval","","","416","11.5.2","UE RF  [FS_NR_newRAT]",62000000,"revised","2016-11-18T23:00:00","2016-11-18T23:00:00","","R4-1610925","","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1610621","WF on how to derive ACLR/ACS from ACIR for WP 5D","NTT DOCOMO, INC.","Juha Korhonen","21609","discussion","Endorsement","","","410","11.3.1","Co-existence [FS_NR_newRAT]",56900000,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","","","","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1610622","WF on dense urban marco scenario for coexistence study for WP5D on new radio access technology","Nokia, Alcatel-Lucent Shanghai Bell","Juha Korhonen","21609","discussion","Endorsement","This contribution provides the simulation results using the agreed assumptions (with the necessary correction on the constant in the UMa LOS probability formula from ‘36’ to ‘63’), and proposes refined assumptions on the indoor UE ratio in the urban macro","","410","11.3.1","Co-existence [FS_NR_newRAT]",48100000,"noted","2016-11-18T23:00:00","2016-11-18T23:00:00","","","","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1610623","CR: Updates to demodulation requirements for NPUSCH format 1 (Rel-13)","Huawei","Juha Korhonen","21609","CR","Agreement","","","134","6.3.4.2.2","NPUSCH format 1 [NB_IOT-Perf]",944400001,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610563","","Rel-13","36.104","13.5.0","NB_IOT-Perf","0892","2","F","RP-162381","","","","",""]
["R4-1610624","CR: Updates to NPUSCH format 1 demodulation conformance test (Rel-13)","Huawei","Juha Korhonen","21609","CR","Agreement","","","134","6.3.4.2.2","NPUSCH format 1 [NB_IOT-Perf]",944600002,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610564","","Rel-13","36.141","13.5.0","NB_IOT-Perf","0925","2","F","RP-162381","","","","",""]
["R4-1610625","Text proposal on RRM testing for NR","Ericsson","Juha Korhonen","21609","pCR","Approval","","","426","11.6.1.2","Testability [FS_NR_newRAT]",956400001,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609564","","","38.803","0.3.0","FS_NR_newRAT","","","","","","","","",""]
["R4-1610626","Way forward on NR spectrum utilization","Huawei, Hisilicon","Juha Korhonen","21609","discussion","Endorsement","","","415","11.5.1","Common issues for UE and BS [FS_NR_newRAT]",96570000,"revised","2016-11-18T23:00:00","2016-11-18T23:00:00","","R4-1610922","","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1610627","NR AH Meeting minutes","Qualcomm Incorporated.","Juha Korhonen","21609","report","Discussion","","","407","11.1","General   [FS_NR_newRAT]",9419000,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","","","","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1610628","Evening AH minutes for NR on Wednesday","NTT DOCOMO, INC.","Juha Korhonen","21609","report","Discussion","","","407","11.1","General   [FS_NR_newRAT]",170000,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","","","","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1610629","Way forward on BS unwanted emissions for IMT parameters","Ericsson","Juha Korhonen","21609","discussion","Agreement","","","420","11.5.3","BS RF  [FS_NR_newRAT]",57400000,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","","","","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1610630","Clarification to applicability of NRSRQ for UE category NB1","Nokia, Alcatel-Lucent Shanghai Bell","Juha Korhonen","21609","CR","Approval","","","117","6.3.3","RRM (36.133) [NB_IOT-Perf]",55100000,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610549","","Rel-13","36.133","13.5.0","NB_IOT-Perf","4205","2","F","RP-162381","","","","",""]
["R4-1610631","CR: Updates to demodulation requirements for NPUSCH format 2 (Rel-14)","Huawei","Juha Korhonen","21609","CR","Agreement","","","135","6.3.4.2.3","NPUSCH format 2 [NB_IOT-Perf]",944900001,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609449","","Rel-14","36.104","14.1.0","NB_IOT-Perf","0895","1","A","RP-162381","","","","",""]
["R4-1610632","Guidance on how to contribute to each session for NR and eAAS","Ericsson","Juha Korhonen","21609","discussion","Approval","","","420","11.5.3","BS RF  [FS_NR_newRAT]",57600001,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610574","","","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1610633","Way forward on NR BS requirements prioritization for mm wave","Ericsson","Juha Korhonen","21609","discussion","Endorsement","","","420","11.5.3","BS RF  [FS_NR_newRAT]",62900001,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610575","","","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1610634","WF on urban marco scenario for coexistence study for WP5D on new radio access technology","Nokia, Alcatel-Lucent Shanghai Bell, Qualcomm, Samsung, CATT, ZTE, NTT DOCOMO, Intel, Ericsson","Juha Korhonen","21609","other","Approval","","","410","11.3.1","Co-existence [FS_NR_newRAT]",48200001,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610569","","","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1610635","CR on UE transmission timing accuracy test for V2V","CATT","Juha Korhonen","21609","CR","Approval","","","266","8.19.3.1","UE transmission timing accuracy test [LTE_SL_V2V-Perf]",950700000,"withdrawn","2016-11-24T01:32:09.900",null,"R4-1609507","","Rel-14","36.133","14.1.0","LTE_SL_V2V-Perf","4212","1","B","","","","","",""]
["R4-1610636","CR on reliability of GNSS","LG Electronics, Huawei, CATT, Qualcomm, Nokia, Alcatel-Lucent Shanghai Bell","Juha Korhonen","21609","CR","Approval","","","264","8.19.2","RRM core maintenance (36.133)  [LTE_SL_V2V-Core]",928600000,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609765","","Rel-14","36.133","14.1.0","LTE_SL_V2V-Core","4229","1","F","RP-162409","","","","",""]
["R4-1610637","Way forward on open issues for test setup for V2V RRM test","Huawei, Qualcomm","Juha Korhonen","21609","other","Endorsement","","","266","8.19.3.1","UE transmission timing accuracy test [LTE_SL_V2V-Perf]",63500000,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","","","","","","LTE_SL_V2V-Perf","","","","","","","","",""]
["R4-1610638","V2X PSSCH-RSRP measurements accuracy analysis","Intel Corporation","Juha Korhonen","21609","discussion","Discussion","","","285","8.20.4.5","Autonomous resource selection/reselection [LTE_V2X-Core]",68300000,"noted","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609086","","Rel-14","","","LTE_V2X-Core","","","","","","","","",""]
["R4-1610639","Way forward on LAA demodulation performance requirement extension","Huawei, HiSilicon, =, Qualcomm, Intel","Juha Korhonen","21609","other","Approval","","","107","6.2.4.1","General [LTE_LAA-Perf]",86200,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","","","","","","LTE_LAA-Perf","","","","","","","","",""]
["R4-1610640","Simulations on 4RX+ CA tests","Intel Corporation","Juha Korhonen","21609","other","Discussion","","","359","8.30.3.2","Extend existing 2Rx CA requirement to 4Rx [LTE_4Rx_AP_DL_CA-Perf]",906100100,"noted","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609061","","","","","LTE_4Rx_AP_DL_CA-Perf","","","","","","","","",""]
["R4-1610641","Way forward on TM9 Test 8.3.1.1#2 with 4Rx","Intel","Juha Korhonen","21609","other","Endorsement","","","33","5.2.3.2","UE demodulation and CSI [LTE_4Rx_AP_DL-Perf]",948800001,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","","","","","","LTE_4Rx_AP_DL-Perf","","","","","","","","",""]
["R4-1610642","CR:Updates to LAA PDSCH demodulation performance requirements (Rel-13)","Huawei, HiSilicon","Juha Korhonen","21609","CR","Agreement","","","108","6.2.4.2","PDSCH [LTE_LAA-Perf]",942800000,"revised","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609594","R4-1610964","Rel-13","36.101","13.5.0","LTE_LAA-Perf","3878","3","F","","","","","",""]
["R4-1610643","Add PDCCH performance requirements for LAA demodulation","Ericsson","Juha Korhonen","21609","CR","Approval","","","109","6.2.4.3","PDCCH [LTE_LAA-Perf]",917300000,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609172","","Rel-13","36.101","13.5.0","LTE_LAA-Perf","3982","1","F","RP-162386","","","","",""]
["R4-1610644","Clean up and clarification for LAA CSI requirements","Ericsson","Juha Korhonen","21609","CR","Approval","","","110","6.2.5","UE CSI reporting (36.101) [LTE_LAA-Perf]",917400000,"revised","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609170","R4-1610885","Rel-13","36.101","13.5.0","LTE_LAA-Perf","3980","1","F","","","","","",""]
["R4-1610645","CR for Inter-frequency event triggered reporting","MediaTek, Nokia","Juha Korhonen","21609","CR","","","","105","6.2.3","RRM performance maintenance (36.133)  [LTE_LAA-Perf]",979200000,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609792","","Rel-14","36.133","14.1.0","LTE_LAA-Perf","4232","1","A","RP-162386","","","","",""]
["R4-1610646","CR on Bluetooth Wifi requirement for indoor positioning","Huawei, HiSilicon","Juha Korhonen","21609","CR","","","","298","8.22.3.2","RAT-independent enhancement [UTRA_LTE_iPos_enh2]",646000,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610076","","Rel-14","37.171","13.0.0","UTRA_LTE_iPos_enh2","0002","","B","RP-162396","","","","",""]
["R4-1610647","Requirements for WLAN RSSI Measurement for Positioning","Ericsson","Juha Korhonen","21609","CR","Approval","","","298","8.22.3.2","RAT-independent enhancement [UTRA_LTE_iPos_enh2]",4930000,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610492","","Rel-14","37.171","13.0.0","UTRA_LTE_iPos_enh2-Core","0003","","B","RP-162396","","","","",""]
["R4-1610648","Correction on test parameter in RSRP Intra frequency case for Cat-M1 UE in CE mode A","Huawei, HiSilicon","Juha Korhonen","21609","CR","Approval","","","79","6.1.1.1.2","Others  [LTE_MTCe2_L1-Perf]",25000,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610024","","Rel-13","36.133","13.5.0","LTE_MTCe2_L1-Perf","4251","1","F","RP-162383","","","","",""]
["R4-1610649","Correction on test parameter in RSRP Intra frequency case for Cat-M1 UE in CE mode B","Huawei, HiSilicon","Juha Korhonen","21609","CR","Approval","","","79","6.1.1.1.2","Others  [LTE_MTCe2_L1-Perf]",28000,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610026","","Rel-13","36.133","13.5.0","LTE_MTCe2_L1-Perf","4253","1","F","RP-162383","","","","",""]
["R4-1610650","Introduce RSRP accuracy test case for Band 31 for Cat-M1 UE","Huawei, HiSilicon","Juha Korhonen","21609","CR","Approval","","","79","6.1.1.1.2","Others  [LTE_MTCe2_L1-Perf]",31000,"revised","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610028","R4-1610894","Rel-13","36.133","13.5.0","","4255","1","F","","","","","",""]
["R4-1610651","Correction on random access requirement for SRS switching","Intel, Huawei, Ericsson","Juha Korhonen","21609","CR","Agreement","","","291","8.21.3","RRM core and performance (36.133) [LTE_SRS_switch-Core/Perf]",65100000,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","","","Rel-14","36.133","14.1.0","LTE_SRS_switch-Core","4365","1","F","RP-162392","","","","",""]
["R4-1610652","Summary of eMTC MIB acquisition delay simulation results","Intel Corporation","Juha Korhonen","21609","discussion","Discussion","","","48","5.5.3.1","Evaluation of MIB and SIB reading delay, and update of requirement for handover and RRC Re-establishment [LTE_MTCe2_L1-Core]",2220010,"noted","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609136","","Rel-13","","","LTE_MTCe2_L1-Core","","","","","","","","",""]
["R4-1610653","CR on CGI reading of eMTC R13","Huawei, HiSilicon","Juha Korhonen","21609","CR","Approval","","","48","5.5.3.1","Evaluation of MIB and SIB reading delay, and update of requirement for handover and RRC Re-establishment [LTE_MTCe2_L1-Core]",2550010,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610055","","Rel-13","36.133","13.5.0","LTE_MTCe2_L1-Core","4269","1","F","RP-162430","","","","",""]
["R4-1610654","CR on handover of eMTC R13","Huawei, HiSilicon","Juha Korhonen","21609","CR","Approval","","","48","5.5.3.1","Evaluation of MIB and SIB reading delay, and update of requirement for handover and RRC Re-establishment [LTE_MTCe2_L1-Core]",9696010,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610057","","Rel-13","36.133","13.5.0","LTE_MTCe2_L1-Core","4271","1","F","RP-162430","","","","",""]
["R4-1610655","Correction of transmit timing for category M1","Intel Corporation, Ericsson, Nokia, Qualcomm, Sony, Sierra Wireless, Verizon Wireless","Juha Korhonen","21609","CR","Endorsement","","","49","5.5.3.2","UE transmit timing [LTE_MTCe2_L1-Core]",65500000,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","","","Rel-14","36.133","14.1.0","LTE_MTCe2_L1-Core","3980","2","A","RP-162430","","","","",""]
["R4-1610656","UE Tranmsit timing accuracy in CE mode B","Qualcomm, Intel, Huawei, HiSilicon","Juha Korhonen","21609","CR","Approval","","","49","5.5.3.2","UE transmit timing [LTE_MTCe2_L1-Core]",41800010,"revised","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610418","R4-1611022","Rel-13","36.133","13.5.0","LTE_MTCe2_L1-Core","4156","3","F","","","","","",""]
["R4-1610657","LS on RSRQ measurement for cell reselection","Huawei","Juha Korhonen","21609","LS out","Approval","","","50","5.5.3.3","Measurement requirement [LTE_MTCe2_L1-Core]",52000,"revised","2016-11-18T23:00:00","2016-11-18T23:00:00","","R4-1610995","Rel-13","","","LTE_MTCe2_L1-Core","","","","","","RAN2","","",""]
["R4-1610658","Applicability rule for eMTC test cases in CEModeA and CEModeB","Ericsson, Nokia, Qualcomm, Verizon","Juha Korhonen","21609","CR","Approval","","","78","6.1.1.1.1","Test applicability [LTE_MTCe2_L1-Perf]",23700010,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610236","","Rel-13","36.133","13.5.0","LTE_MTCe2_L1-Perf","4320","1","B","RP-162383","","","","",""]
["R4-1610659","Applicability rule for eMTC test cases in CEModeA and CEModeB","Ericsson, Nokia, Qualcomm, Verizon","Juha Korhonen","21609","CR","Approval","","","78","6.1.1.1.1","Test applicability [LTE_MTCe2_L1-Perf]",27000010,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610237","","Rel-14","36.133","14.1.0","LTE_MTCe2_L1-Perf","4321","1","A","RP-162383","","","","",""]
["R4-1610660","Correction to the handover test case in CE mode A","Qualcomm Incorporated, Anritsu","Juha Korhonen","21609","CR","Approval","","","81","6.1.1.2.1","Intra-frequency Handover [LTE_MTCe2_L1-Perf]",412010,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610412","","Rel-13","36.133","13.5.0","LTE_MTCe2_L1-Perf","4351","1","F","RP-162383","","","","",""]
["R4-1610661","WF on link-level simulation assumptions for BS-IC","China Telecom","Juha Korhonen","21609","discussion","Endorsement","","","399","9.4.5","Link level evaluation [FS_LTE _IC_BS]",66100000,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","","","","","","","","","","","","","","",""]
["R4-1610662","Simulation summary of eMTC UE demodulation requirements","Ericsson","Juha Korhonen","21609","other","Information","","","96","6.1.2","UE performance (36.101) [LTE_MTCe2_L1-Perf]",968100010,"revised","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609681","R4-1610709","Rel-13","","","LTE_MTCe2_L1-Perf","","","","","","","","",""]
["R4-1610663","Summary of simulation results for eMTC CEMode B RLM","Nokia","Juha Korhonen","21609","discussion","Information","","","93","6.1.1.3.7","RLM  [LTE_MTCe2_L1-Perf]",66300000,"noted","2016-11-18T23:00:00","2016-11-18T23:00:00","","","","","","","","","","","","","","",""]
["R4-1610664","SI reading tests for eMTC UEs in CEModeB","Ericsson","Juha Korhonen","21609","CR","Approval","","","94","6.1.1.3.8","CGI reading [LTE_MTCe2_L1-Perf]",2230010,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610223","","Rel-13","36.133","13.5.0","LTE_MTCe2_L1-Perf","4308","1","B","RP-162383","","","","",""]
["R4-1610665","SI reading tests for eMTC UEs in CEModeB","Ericsson","Juha Korhonen","21609","CR","Approval","","","94","6.1.1.3.8","CGI reading [LTE_MTCe2_L1-Perf]",2240010,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610224","","Rel-14","36.133","14.1.0","LTE_MTCe2_L1-Perf","4309","1","A","RP-162383","","","","",""]
["R4-1610666","LS response on FeMTC VoLTE enhancements","Ericsson","Juha Korhonen","21609","LS out","Approval","","","312","8.25.1","General [LTE_feMTC-Core]",2150010,"revised","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610215","R4-1610996","Rel-14","","","LTE_feMTC-Core","","","","","","RAN1","RAN2","",""]
["R4-1610667","WF on FeMTC positioning","Huawei, HiSilicon","Juha Korhonen","21609","other","","","","315","8.25.3.1","Positioning [LTE_feMTC-Core]",82010,"noted","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610082","","","","","","","","","","","","","",""]
["R4-1610668","Way Forward RRM measurement requirements for feMTC","Ericsson","Juha Korhonen","21609","other","Approval","","","318","8.25.3.2","Mobility enhancement [LTE_feMTC-Core]",2200010,"withdrawn","2016-11-24T01:32:18.543",null,"R4-1610220","","Rel-14","","","LTE_feMTC-Core","","","","","","","","",""]
["R4-1610669","Way forward on measurement on MPDCCH monitoring","Nokia, Alcatel-Lucent Shanghai Bell, Qualcomm, Huawei, HiSilicon","Juha Korhonen","21609","discussion","Endorsement","","","319","8.25.3.2.1","Measurement [LTE_feMTC-Core]",9293000,"noted","2016-11-18T23:00:00","2016-11-18T23:00:00","","","","","","","","","","","","","","",""]
["R4-1610670","LS to RAN1, RAN2 on PBCH demodulation performance","Intel Corporation","Juha Korhonen","21609","LS out","Approval","","","323","8.25.4","Other specifications [LTE_feMTC-Core]",915100010,"revised","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609151","R4-1610899","Rel-14","","","LTE_feMTC-Core","","","","","","RAN1, RAN2","","",""]
["R4-1610671","CR for Rel-13 eMTC MPDCCH demodulation requirements","Huawei, HiSilicon","Juha Korhonen","21609","CR","Agreement","","","98","6.1.2.2","MPDCCH [LTE_MTCe2_L1-Perf]",966900010,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609668","","Rel-13","36.101","13.5.0","LTE_MTCe2_L1-Perf","3884","3","F","RP-162383","","","","",""]
["R4-1610672","Correction of PDCSH demodulation requirements for eMTC","Ericsson","Juha Korhonen","21609","CR","Approval","","","99","6.1.2.3","MPDSCH [LTE_MTCe2_L1-Perf]",968600010,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609686","","Rel-13","36.101","13.5.0","LTE_MTCe2_L1-Perf","3928","3","F","RP-162383","","","","",""]
["R4-1610673","Finalizing CQI definition test for eMTC","Ericsson","Juha Korhonen","21609","CR","Approval","","","100","6.1.3","UE CSI reporting (36.101) [LTE_MTCe2_L1-Perf]",968900010,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609689","","Rel-13","36.101","13.5.0","LTE_MTCe2_L1-Perf","4043","1","F","RP-162383","","","","",""]
["R4-1610674","CR on cleaning up Rel-13 eMTC PUSCH conformance test","Huawei","Juha Korhonen","21609","CR","Agreement","","","101","6.1.4","Maintenance of BS performance (36.104, 36.141) [LTE_MTCe2_L1-Perf]",946100010,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609461","","Rel-13","36.141","13.5.0","LTE_MTCe2_L1-Perf","0929","1","F","RP-162383","","","","",""]
["R4-1610675","Measurement accuracy for PSSCH-RSRP and S-RSSI","LG Electronics Inc.","Juha Korhonen","21609","discussion","Discussion","","","285","8.20.4.5","Autonomous resource selection/reselection [LTE_V2X-Core]",951300000,"noted","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609772","","Rel-14","","","","","","","","","","","",""]
["R4-1610676","CR for RRM requirements  in idle mode  for high speed conditions","CATT","Juha Korhonen","21609","CR","Approval","","","342","8.28.2.2","Enhancement in idle mode [LTE_high_speed]",955200010,"revised","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609524","R4-1610882","Rel-14","36.133","14.1.0","LTE_high_speed","4217","1","B","","","","","",""]
["R4-1610677","Reply LS on performance enhancements indicator for high speed scenarios","RAN4","Juha Korhonen","21609","LS out","Approval","","","343","8.28.2.3","Others [LTE_high_speed]",992400010,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610103","","Rel-14","","","LTE_high_speed","","","","","R2-167308","RAN2","","",""]
["R4-1610678","CR: E-UTRAN FDD-FDD Intra frequency handover for Cat-M1 UEs in CEModeB (Rel-13)","Nokia, Alcatel-Lucent Shanghai Bell","Juha Korhonen","21609","CR","Approval","","","88","6.1.1.3.2","Intra-frequency Handover [LTE_MTCe2_L1-Perf]",961100010,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609611","","Rel-13","36.133","13.5.0","LTE_MTCe2_L1-Perf","4220","1","B","RP-162383","","","","",""]
["R4-1610679","CR: E-UTRAN HD-FDD Intra frequency handover for Cat-M1 UEs in CEModeB (Rel-13)","Nokia, Alcatel-Lucent Shanghai Bell","Juha Korhonen","21609","CR","Approval","","","88","6.1.1.3.2","Intra-frequency Handover [LTE_MTCe2_L1-Perf]",961300010,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609613","","Rel-13","36.133","13.5.0","LTE_MTCe2_L1-Perf","4222","1","B","RP-162383","","","","",""]
["R4-1610680","CR: E-UTRAN TDD-TDD Intra frequency handover for Cat-M1 UEs in CEModeB (Rel-13)","Nokia, Alcatel-Lucent Shanghai Bell","Juha Korhonen","21609","CR","Approval","","","88","6.1.1.3.2","Intra-frequency Handover [LTE_MTCe2_L1-Perf]",961500010,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609615","","Rel-13","36.133","13.5.0","LTE_MTCe2_L1-Perf","4224","1","B","RP-162383","","","","",""]
["R4-1610681","Collection of simulation results for UE enhancement","Huawei, HiSilicon","Juha Korhonen","21609","other","Information","","","345","8.28.3.1","Enhancement for bi-directional RRH arrangement [LTE_high_speed]",946900001,"noted","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609469","","","","","LTE_high_speed","","","","","","","","",""]
["R4-1610682","V2X S-RSRP measurements accuracy analysis","Intel Corporation","Juha Korhonen","21609","discussion","Discussion","","","283","8.20.4.3","Initiation/cease of SLSS requirement [LTE_V2X-Core]",9087001,"noted","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609087","","Rel-14","","","LTE_V2X-Core","","","","","","","","",""]
["R4-1610683","Simulation result summary for PSSCH-RSRP measurement","Intel","Juha Korhonen","21609","discussion","Discussion","","","285","8.20.4.5","Autonomous resource selection/reselection [LTE_V2X-Core]",10000000,"noted","2016-11-18T23:00:00","2016-11-18T23:00:00","","","","","","LTE_V2X-Core","","","","","","","","",""]
["R4-1610684","Simulation result summary for S-RSRP measurements","Intel","Juha Korhonen","21609","discussion","Discussion","","","283","8.20.4.3","Initiation/cease of SLSS requirement [LTE_V2X-Core]",94000,"noted","2016-11-18T23:00:00","2016-11-18T23:00:00","","","","","","LTE_V2X-Core","","","","","","","","",""]
["R4-1610685","Finalizing UE-selected subband CQI test for eMTC","Ericsson","Juha Korhonen","21609","CR","Approval","","","100","6.1.3","UE CSI reporting (36.101) [LTE_MTCe2_L1-Perf]",969100001,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609691","","Rel-13","36.101","13.5.0","LTE_MTCe2_L1-Perf","4045","1","F","RP-162383","","","","",""]
["R4-1610686","CR on 4-RX TM9 MU test","Intel Corporation","Juha Korhonen","21609","CR","Agreement","","","33","5.2.3.2","UE demodulation and CSI [LTE_4Rx_AP_DL-Perf]",989200000,"revised","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609066","R4-1611011","Rel-13","36.101","13.5.0","LTE_4Rx_AP_DL-Perf","3970","1","F","","","","","",""]
["R4-1610687","CR on 4-RX TM9 MU test","Intel Corporation","Juha Korhonen","21609","CR","Agreement","","","33","5.2.3.2","UE demodulation and CSI [LTE_4Rx_AP_DL-Perf]",989400000,"revised","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609067","R4-1611012","Rel-14","36.101","14.1.0","LTE_4Rx_AP_DL-Perf","3971","1","A","","","","","",""]
["R4-1610688","Ad hoc minutes for LAA and eLAA RRM and demodulation","Huawei","Juha Korhonen","21609","report","Approval","","","105","6.2.3","RRM performance maintenance (36.133)  [LTE_LAA-Perf]",68800000,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","","","","","","LTE_LAA-Perf","","","","","","","","",""]
["R4-1610689","Ad hoc minutes for eMTC RRM and demodulation performance","Ericsson","Juha Korhonen","21609","report","Approval","","","76","6.1.1","RRM performance (36.133) [LTE_MTCe2_L1-Perf]",68900000,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","","","","","","LTE_MTCe2_L1-Perf","","","","","","","","",""]
["R4-1610690","LS on measurement gap enhancement","Intel Corporation","Juha Korhonen","21609","LS out","Approval","","","351","8.29.2","RRM core (36.133) [LTE_meas_gap_enh-Core]",954600000,"revised","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609121","R4-1610997","Rel-14","","","LTE_meas_gap_enh-Core","","","","","","RAN2","RAN1","",""]
["R4-1610691","WF on measurement gap enhancement","Intel, Ericsson, Nokia, Huawei","Juha Korhonen","21609","other","Approval","","","350","8.29.1","General [LTE_meas_gap_enh-Core]",911800001,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609119","","","","","","","","","","","","","",""]
["R4-1610692","Way forward on mobility enhancement RRM","ZTE, ZTE Microelectronics, China Telecom, Ericsson, Samsung, Intel, Huawei, Nokia, Qualcomm","Juha Korhonen","21609","discussion","Endorsement","","","327","8.26.3","RRM core (36.133) [LTE_eMob-Core]",9325000,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","","","","","","LTE_eMob-Core","","","","","","","","",""]
["R4-1610693","WF on V2X RRM requirement","LG Electronics Inc, CATT","Juha Korhonen","21609","discussion","Approval","","","280","8.20.4","RRM core (36.133) (dedicated, shared, or multi-carrier operations) [LTE_V2X-Core]",72400000,"revised","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609798","R4-1610966","","","","","","","","","","","","",""]
["R4-1610694","Way forward on determination of PRACH CE levels","Nokia, Alcatel-Lucent Shanghai Bell","Juha Korhonen","21609","discussion","Endorsement","","","51","5.5.3.4","Others [LTE_MTCe2_L1-Core]",69400000,"noted","2016-11-18T23:00:00","2016-11-18T23:00:00","","","","","","LTE_MTCe2_L1-Core","","","","","","","","",""]
["R4-1610695","RF: Beamforming model missing in chapter 9 TM9 receiver Type A tests (Rel-11)","Rohde & Schwarz","Juha Korhonen","21609","CR","","","","15","4.2.4","UE demodulation performance  [WI code or TEI12]",92240001,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610375","","Rel-11","36.101","11.18.0","TEI11","4115","1","F","RP-162413","","","","",""]
["R4-1610696","CR for UE enhancement in SFN scenario","Huawei, HiSilicon, NTT DOCOMO, CMCC, ZTE, CATT, Qualcomm, LG","Juha Korhonen","21609","CR","Agreement","","","345","8.28.3.1","Enhancement for bi-directional RRH arrangement [LTE_high_speed]",992600001,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609471","","Rel-14","36.101","14.1.0","LTE_high_speed","4010","1","B","RP-162388","","","","",""]
["R4-1610697","LS on ECID measurement quantity for NB-IoT","Intel Corporation","Juha Korhonen","21609","LS out","Approval","","","307","8.24.3.1.1","E-CID  [NB_IOTenh-Core]",8600001,"revised","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609105","R4-1610877","Rel-14","","","","","","","","","","","",""]
["R4-1610698","Simulation assumption for UE Rx-Tx time different measurement","Huawei, HiSilicon","Juha Korhonen","21609","other","","","","307","8.24.3.1.1","E-CID  [NB_IOTenh-Core]",34500001,"revised","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610086","R4-1610892","","","","","","","","","","","","",""]
["R4-1610699","LS to RAN1, RAN2 on NPBCH demodulation performance","Intel Corporation","Juha Korhonen","21609","LS out","Approval","","","310","8.24.4","Other specifications [NB_IOTenh-Core]",915400001,"revised","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609154","R4-1610900","Rel-14","","","NB_IOTenh-Core","","","","","","","","",""]
["R4-1610700","Way forward on demodulation performance for enhanced SU-MIMO","LG Electronics, Huawei, HiSilicon, Intel, Samsung, Ericsson, Qualcomm","Juha Korhonen","21609","discussion","Endorsement","","","370","8.31.3.1","Performance evaluation: scenarios and receiver [LTE_eCRSIM_eSUMIMO]",20300000,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","","","","","","LTE_eCRSIM_eSUMIMO","","","","","","","","",""]
["R4-1610701","Way forward on V2V power imbalance tests","LGE","Juha Korhonen","21609","discussion","Endorsement","","","268","8.19.4","UE demodulation (36.101)  [LTE_SL_V2V-Perf]",70100000,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","","","","","","LTE_SL_V2V-Perf","","","","","","","","",""]
["R4-1610702","Summary results for IRC TM2/3/3 test with 4Rx","Ericsson","Juha Korhonen","21609","discussion","Discussion","","","33","5.2.3.2","UE demodulation and CSI [LTE_4Rx_AP_DL-Perf]",64100001,"noted","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609892","","Rel-13","","","LTE_4Rx_AP_DL-Perf","","","","","","","","",""]
["R4-1610703","CR for IRC TM2/3/3 tests with 4Rx in Rel-13","Ericsson","Juha Korhonen","21609","CR","Approval","","","33","5.2.3.2","UE demodulation and CSI [LTE_4Rx_AP_DL-Perf]",906900000,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609893","","Rel-13","36.101","13.5.0","LTE_4Rx_AP_DL-Perf","3902","2","F","RP-162423","","","","",""]
["R4-1610704","CR for IRC TM2/3/3 tests with 4Rx in Rel-14","Ericsson","Juha Korhonen","21609","CR","Approval","","","33","5.2.3.2","UE demodulation and CSI [LTE_4Rx_AP_DL-Perf]",948800000,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609881","","Rel-14","36.101","14.1.0","LTE_4Rx_AP_DL-Perf","3903","2","A","RP-162423","","","","",""]
["R4-1610705","Summary of alignment and impairment results for normal demod tests for 4Rx CA","Ericsson","Juha Korhonen","21609","discussion","Discussion","","","359","8.30.3.2","Extend existing 2Rx CA requirement to 4Rx [LTE_4Rx_AP_DL_CA-Perf]",5240001,"noted","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609999","","Rel-14","","","LTE_4Rx_AP_DL_CA-Perf","","","","","","","","",""]
["R4-1610706","Way forward on eLAA demodulation performance","Huawei","Juha Korhonen","21609","discussion","Endorsement","","","257","8.18.6","UE/BS demodulation and CSI (36.101/36.104) [LTE_eLAA-Perf]",70600000,"noted","2016-11-18T23:00:00","2016-11-18T23:00:00","","","","","","LTE_eLAA-Perf","","","","","","","","",""]
["R4-1610707","WF on BS IC deployment scenarios and inter-cell interference mode","Huawei, China Telecom, Nokia, ZTE","Juha Korhonen","21609","discussion","Endorsement","","","396","9.4.2","Deployment scenario [FS_LTE _IC_BS]",70700000,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","","","","","","FS_LTE_IC_BS","","","","","","","","",""]
["R4-1610708","Discussion about single-link demodulation requirements for Rel-14 V2V","LG Electronics Inc.","Juha Korhonen","21609","discussion","Discussion","","","269","8.19.4.1","Single-link PSSCH and PSCCH  [LTE_SL_V2V-Perf]",42900001,"noted","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609761","","","","","","","","","","","","","",""]
["R4-1610709","Simulation summary of eMTC UE demodulation requirements","Ericsson","Juha Korhonen","21609","other","Information","","","96","6.1.2","UE performance (36.101) [LTE_MTCe2_L1-Perf]",968100011,"noted","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610662","","Rel-13","","","LTE_MTCe2_L1-Perf","","","","","","","","",""]
["R4-1610710","Way forward on eMTC UE demodulation and CQI","Ericsson","Juha Korhonen","21609","discussion","Endorsement","","","96","6.1.2","UE performance (36.101) [LTE_MTCe2_L1-Perf]",71000000,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","","","","","","LTE_MTCe2_L1-Perf","","","","","","","","",""]
["R4-1610711","Way forward on intra-cell interference model","ZTE","Juha Korhonen","21609","discussion","Endorsement","","","398","9.4.4","Interference model [FS_LTE _IC_BS]",71100000,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","","","","","","FS_LTE_IC_BS","","","","","","","","",""]
["R4-1610712","Way forward on baseline and reference receiver for BS-IC","Nokia, China Telecom, ZTE, Huawei","Juha Korhonen","21609","discussion","Endorsement","","","397","9.4.3","Reference receiver [FS_LTE _IC_BS]",71200000,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","","","","","","FS_LTE_IC_BS","","","","","","","","",""]
["R4-1610713","CR for introducing definition of Type-D receiver","NTT DOCOMO INC.","Juha Korhonen","21609","CR","Approval","","","345","8.28.3.1","Enhancement for bi-directional RRH arrangement [LTE_high_speed]",4070001,"revised","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609926","R4-1610967","Rel-14","36.101","14.1.0","LTE_high_speed-Perf","4082","1","B","","","","","",""]
["R4-1610714","Way forward on CQI reporting performance under SFN scenario","NTT DOCOMO Inc., Huawei","Juha Korhonen","21609","discussion","Endorsement","","","347","8.28.3.3","CQI reporting [LTE_high_speed]",4050000,"noted","2016-11-18T23:00:00","2016-11-18T23:00:00","","","","","","LTE_high_speed","","","","","","","","",""]
["R4-1610715","Simulation assumptions for enhanced SU-MIMO demodulation requiremetns","Huawei, HiSilicon, LG Electronics, Intel","Juha Korhonen","21609","other","Approval","","","370","8.31.3.1","Performance evaluation: scenarios and receiver [LTE_eCRSIM_eSUMIMO]",70000001,"revised","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609487","R4-1610969","","","","","","","","","","","","",""]
["R4-1610716","Way forward on enhanced CRS-IM performance","Intel Corporation, Huawei, HiSilicon, LGE, Ericsson","Juha Korhonen","21609","discussion","Endorsement","","","367","8.31.2.1","Performance evaluation: scenarios and receiver [LTE_eCRSIM_eSUMIMO]",974700,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","","","","","","LTE_eCRSIM_eSUMIMO","","","","","","","","",""]
["R4-1610717","Way forward on simulation assumptions for CRS-IM enhancement","Intel Corporation, Huawei, HiSilicon, LGE, Ericsson","Juha Korhonen","21609","discussion","Endorsement","","","367","8.31.2.1","Performance evaluation: scenarios and receiver [LTE_eCRSIM_eSUMIMO]",71600000,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","","","","","","LTE_eCRSIM_eSUMIMO","","","","","","","","",""]
["R4-1610718","Ad hoc minutes for eCRS-IM and eSU-MIMO IM","Intel","Juha Korhonen","21609","report","Approval","","","367","8.31.2.1","Performance evaluation: scenarios and receiver [LTE_eCRSIM_eSUMIMO]",4000,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","","","","","","LTE_eCRSIM_eSUMIMO","","","","","","","","",""]
["R4-1610719","Ad hoc minutes on 4Rx performance","Ericsson","Juha Korhonen","21609","discussion","Endorsement","","","357","8.30.3","UE demodulation (36.101) [LTE_4Rx_AP_DL_CA-Perf]",71900000,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","","","","","","LTE_4Rx_AP_DL_CA-Perf","","","","","","","","",""]
["R4-1610720","CR for fixing editorial errors in Rel-13","Ericsson","Juha Korhonen","21609","CR","Approval","","","15","4.2.4","UE demodulation performance  [WI code or TEI12]",94910001,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609994","","Rel-13","36.101","13.5.0","TEI13","4086","1","F","RP-162435","","","","",""]
["R4-1610721","Ad hoc minutes for V2V and V2X RRM","Huawei","Juha Korhonen","21609","report","Agreement","","","280","8.20.4","RRM core (36.133) (dedicated, shared, or multi-carrier operations) [LTE_V2X-Core]",9798000,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","","","","","","LTE_V2X-Core","","","","","","","","",""]
["R4-1610722","Correction to RSRP bias in idle mode reselection requirement in enhanced coverage","Qualcomm Incorporated","Juha Korhonen","21609","CR","Approval","","","51","5.5.3.4","Others [LTE_MTCe2_L1-Core]",5100000,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610414","","Rel-14","36.133","14.1.0","LTE_MTCe2_L1-Core","4094","2","A","RP-162430","","","","",""]
["R4-1610723","Correction to RSRP bias in idle mode reselection requirement in enhanced coverage","Qualcomm Incorporated, Anritsu","Juha Korhonen","21609","CR","Agreement","","","51","5.5.3.4","Others [LTE_MTCe2_L1-Core]",88600,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","","","Rel-13","36.133","13.5.0","LTE_MTCe2_L1-Core","4093","2","F","RP-162430","","","","",""]
["R4-1610724","LS on V2X TA offset","Huawei","Juha Korhonen","21609","LS out","Approval","","","280","8.20.4","RRM core (36.133) (dedicated, shared, or multi-carrier operations) [LTE_V2X-Core]",9798001,"noted","2016-11-18T23:00:00","2016-11-18T23:00:00","","","","","","LTE_V2X-Core","","","","","","","","",""]
["R4-1610725","PCC and SCC assignment in 20MHz+10MHz test cases A.8.20.2B and A.9.2.27","ANRITSU LTD","Juha Korhonen","21609","CR","","","","15","4.2.4","UE demodulation performance  [WI code or TEI12]",118001,"reserved","2016-11-24T01:32:31.867",null,"R4-1609209","","Rel-12","36.133","12.13.0","LTE_CA_B39_B41-Perf","4173","1","F","","","","","",""]
["R4-1610726","RF: Wrong Imcs value in MCS.11B/MCS.12B (Rel-12)","Rohde & Schwarz","Juha Korhonen","21609","CR","","","","15","4.2.4","UE demodulation performance  [WI code or TEI12]",379001,"noted","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610379","","Rel-12","36.101","12.13.0","TEI12","4119","1","F","","","","","",""]
["R4-1610727","Correction to cell mapping for periodic CQI reporting on multiple cells","ANRITSU LTD","Juha Korhonen","21609","CR","","","","15","4.2.4","UE demodulation performance  [WI code or TEI12]",13600001,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609224","","Rel-12","36.101","12.13.0","LTE_CA_B39_B41-Perf, LTE_CA_B1_B3-Perf","3994","1","F","RP-162415","","","","",""]
["R4-1610728","Way forward on RRM requirement for Cat 1 UE with 1 Rx","Qualcomm","Juha Korhonen","21609","discussion","Endorsement","","","334","8.27.3","RRM core (36.133) [LTE_UE_cat_1RX-Core]",41000,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","","","","","","LTE_UE_cat_1RX-Core","","","","","","","","",""]
["R4-1610729","Simulation assumption for RSTD measurement accuracy for Cat.1 UE with single receiver chain","Qualcomm Incorporated","Juha Korhonen","21609","other","Approval","","","335","8.27.4","RRM performance (36.133) [LTE_UE_cat_1RX-Perf]",970400001,"withdrawn","2016-11-24T01:32:32.910",null,"R4-1609704","","","","","","","","","","","","","",""]
["R4-1610730","Workplan for RRM core work on shortened TTI and reduced processing time for LTE","Ericsson","Juha Korhonen","21609","discussion","Discussion","","","405","10.1.4","RRM core (36.133)  [LTE_sTTIandPT]",112001,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609557","","Rel-15","","","LTE_sTTIandPT","","","","","","","","",""]
["R4-1610731","Remaining issues with eLAA RRM requirements","Ericsson","Juha Korhonen","21609","CR","Approval","","","254","8.18.4.2","Interruption [LTE_eLAA-Core]",3350001,"noted","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610335","","Rel-14","36.133","14.1.0","LTE_eLAA-Core","4344","1","F","","","","","",""]
["R4-1610732","eLAA requirements corrections","Ericsson","Juha Korhonen","21609","CR","Approval","","","255","8.18.4.3","Others [LTE_eLAA-Core]",0,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610334","","Rel-14","36.133","14.1.0","LTE_eLAA-Core","4343","1","F","RP-162387","","","","",""]
["R4-1610733","Response on Timing reference for FS3 SCell","Ericsson","Juha Korhonen","21609","LS out","Approval","","","255","8.18.4.3","Others [LTE_eLAA-Core]",97500001,"noted","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610337","","Rel-14","","","LTE_eLAA-Core","","","","","R2-165965","RAN2","RAN1","R2-165965",""]
["R4-1610734","Requirements with SRS carrier based switching","Ericsson","Juha Korhonen","21609","CR","Approval","","","291","8.21.3","RRM core and performance (36.133) [LTE_SRS_switch-Core/Perf]",42200001,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610422","","Rel-14","36.133","14.1.0","LTE_SRS_switch-Core","4355","1","B","RP-162392","","","","",""]
["R4-1610735","Introduction of UE transmitter requirements for LAA Scell operation in Band 46","Ericsson","Juha Korhonen","21609","CR","Approval","","","243","8.18.2","UE RF (36.101) [LTE_eLAA-Core]",5090000,"noted","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609586","","Rel-14","36.101","14.1.0","LTE_eLAA-Core","4032","1","B","","","","","",""]
["R4-1610736","Requirements for eLAA dual uplink 2A-46A","Ericsson","Juha Korhonen","21609","pCR","Approval","","","247","8.18.2.4","Other requirements [LTE_eLAA-Core]",73600000,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609204","","","36.714-02-02","0.5.0","LTE_eLAA-Core","","","","","","","","",""]
["R4-1610737","Requirements for eLAA dual uplink 7A-46A","Ericsson","Juha Korhonen","21609","pCR","Approval","","","247","8.18.2.4","Other requirements [LTE_eLAA-Core]",920500000,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609206","","","36.714-02-02","0.5.0","LTE_eLAA-Core","","","","","","","","",""]
["R4-1610738","CR on eLAA BS Rx requirements","Huawei, Nokia","Juha Korhonen","21609","CR","Agreement","","","250","8.18.3.2","Rx requirements [LTE_eLAA-Core]",936600000,"endorsed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609366","","Rel-14","36.104","14.1.0","LTE_eLAA-Core","0889","1","B","","","","","",""]
["R4-1610739","TR 37.871 V1.1.0 clean-up","Nokia, Alcatel-Lucent Shanghai Bell, Ericsson, Huawei","Juha Korhonen","21609","pCR","Approval","","","203","8.11","Multi-Band Base Station testing with three or more bands  [MB_BS_test_3B]",740000,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610146","","","37.871","2.0.0","MB_BS_test_3B-Core","","","","","","","","",""]
["R4-1610740","TR 37.871 V1.2.0","Nokia, Alcatel-Lucent Shanghai Bell, Ericsson, Huawei","Juha Korhonen","21609","draft TR","Approval","","","203","8.11","Multi-Band Base Station testing with three or more bands  [MB_BS_test_3B]",14700000,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610147","","Rel-14","37.871","1.2.0","MB_BS_test_3B-Core","","","","","","","","",""]
["R4-1610741","Necessary changes to the core requirements for Multi-Band Base Station testing with three or more bands","Nokia, Alcatel-Lucent Shanghai Bell, Ericsson, Huawei","Juha Korhonen","21609","CR","Agreement","","","204","8.11.1","BS RF (36.104,37.104, 25.104) [MB_BS_test_3B-Core]",149000,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610148","","Rel-14","36.104","14.1.0","MB_BS_test_3B-Core","0905","1","B","RP-162395","","","","",""]
["R4-1610742","Necessary changes to the core requirements for Multi-Band Base Station testing with three or more bands","Nokia, Alcatel-Lucent Shanghai Bell, Ericsson, Huawei","Juha Korhonen","21609","CR","Agreement","","","204","8.11.1","BS RF (36.104,37.104, 25.104) [MB_BS_test_3B-Core]",742000,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610149","","Rel-14","37.104","14.1.0","MB_BS_test_3B-Core","0313","1","B","RP-162395","","","","",""]
["R4-1610743","CR for 36.141: Multi-band testing with 3 or more bands","Huawei, Ericsson, Nokia","Juha Korhonen","21609","CR","Agreement","","","205","8.11.2","BS RF (36.141, 37.141, 25.141) [MB_BS_test_3B-Perf]",74400000,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609387","","Rel-14","36.141","14.1.0","MB_BS_test_3B-Perf","0922","1","B","RP-162395","","","","",""]
["R4-1610744","CR for TS 37.141: Multi-band testing with 3 or more bands.","Ericsson, Nokia, Huawei","Juha Korhonen","21609","CR","Approval","","","205","8.11.2","BS RF (36.141, 37.141, 25.141) [MB_BS_test_3B-Perf]",952900000,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609529","","Rel-14","37.141","14.1.0","MB_BS_test_3B-Perf","0475","1","B","RP-162395","","","","",""]
["R4-1610745","TR 37.871","Nokia","Juha Korhonen","21609","draft TR","Agreement","","","203","8.11","Multi-Band Base Station testing with three or more bands  [MB_BS_test_3B]",146000,"revised","2016-11-18T23:00:00","2016-11-18T23:00:00","","R4-1610914","Rel-14","37.871","2.0.0","MB_BS_test_3B-Core","","","","","","","","",""]
["R4-1610746","LS on handling co-existence requirements with CEN DSRC","Huawei, Hisilicon","Juha Korhonen","21609","LS out","Approval","","","259","8.19.1","UE RF core maintenace (36.101)  [LTE_SL_V2V-Core]",93710000,"revised","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609372","R4-1610998","Rel-14","","","LTE_SL_V2V-Core","","","","","","RAN2","RAN1","",""]
["R4-1610747","CR for V2V UE RF requirements to support CEN DSRC protection techniques","Qualcomm Europe Inc.(France)","Juha Korhonen","21609","draftCR","Approval","","","259","8.19.1","UE RF core maintenace (36.101)  [LTE_SL_V2V-Core]",980500000,"withdrawn","2016-11-24T01:32:37.653",null,"R4-1609967","","Rel-14","36.101","14.1.0","LTE_SL_V2V-Core","","","","","","","","",""]
["R4-1610748","TP for 36.786: Updated MPR requirements for V2V","Huawei, Hisilicon","Juha Korhonen","21609","pCR","Approval","","","260","8.19.1.1","MPR/A-MPR [LTE_SL_V2V-Core]",2040000,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609369","","","36.786","0.1.0","LTE_SL_V2V-Core","","","","","","","","",""]
["R4-1610749","TP for 36.786: Updated A-MPR requirements for V2V","Huawei, Hisilicon","Juha Korhonen","21609","pCR","Approval","","","260","8.19.1.1","MPR/A-MPR [LTE_SL_V2V-Core]",74900000,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609370","","","36.786","0.1.0","LTE_SL_V2V-Core","","","","","","","","",""]
["R4-1610750","TP for 36.786: Meeting ETSI RX regulatory requirements","Huawei, Hisilicon","Juha Korhonen","21609","pCR","Approval","","","261","8.19.1.2","Blocking  [LTE_SL_V2V-Core]",937400000,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609374","","","36.786","0.1.0","LTE_SL_V2V-Core","","","","","","","","",""]
["R4-1610751","Correction on FRC for V2V in TS 36.101","Huawei, Hisilicon","Juha Korhonen","21609","CR","Agreement","","","263","8.19.1.4","Others",995200000,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609368","","Rel-14","36.101","14.1.0","LTE_SL_V2V-Core","4000","1","F","RP-162409","","","","",""]
["R4-1610752","Updated TR 36.786 v0.1.0","LG Electronics Inc.","Juha Korhonen","21609","draft TR","Approval","","","273","8.20.1","General [LTE_V2X-Core]",75200000,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609795","","Rel-14","36.786","0.1.0","LTE_V2X-Core","","","","","","","","",""]
["R4-1610753","TP for 36.786 Operating bands and channel bandwidth for V2X","Huawei, Hisilicon","Juha Korhonen","21609","pCR","","","","273","8.20.1","General [LTE_V2X-Core]",937800000,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609867","","","36.786","0.1.0","","","","","","","","","",""]
["R4-1610754","TP on the conclusion of co-existence results for V2V UEs","LGE","Juha Korhonen","21609","pCR","Approval","","","276","8.20.2.2","Co-existence study for case 1 and case 2  [LTE_V2X-Core]",75400000,"revised","2016-11-18T23:00:00","2016-11-18T23:00:00","","R4-1610956","","36.786","0.1.0","LTE_V2X-Core","","","","","","","","",""]
["R4-1610755","LS to RAN1 on UL PC for V2V","Ericsson","Juha Korhonen","21609","LS out","Approval","","","276","8.20.2.2","Co-existence study for case 1 and case 2  [LTE_V2X-Core]",980700000,"withdrawn","2016-11-24T01:32:39.463",null,"R4-1609638","","Rel-14","","","LTE_V2X-Core","","","","","","RAN1","","",""]
["R4-1610756","TP for Tx RF requirements for inter-band E-UTRA_V2X operation and higher power class","CATT","Juha Korhonen","21609","other","Approval","","","278","8.20.3.1","Tx requirements  [LTE_V2X-Core]",950400000,"revised","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609504","R4-1610957","Rel-14","36.786","","LTE_V2X-Core","","","","","","","","",""]
["R4-1610757","LTE-based V2X UE Transmitter requirements","LG Electronics Inc.","Juha Korhonen","21609","pCR","Approval","","","278","8.20.3.1","Tx requirements  [LTE_V2X-Core]",979600000,"noted","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609796","","","36.786","0.1.0","LTE_V2X-Core","","","","","","","","",""]
["R4-1610758","Requirements to complete the 3DL CA combination 2A-12A-12A","Ericsson, US Cellular","Juha Korhonen","21609","pCR","Approval","","","159","8.3.2","UE RF (36.101) [LTE_CA_R14_3DL1UL-Core]",904800000,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609193","","","36.714-03-01","0.5.0","LTE_CA_R14_3DL1UL-Core","","","","","","","","",""]
["R4-1610759","TP for TR 36.714-00-00: REFSENS requirement for CA_3A-3A_BCS2","Samsung","Juha Korhonen","21609","pCR","Approval","","","147","8.1.2","UE RF (36.101) [LTE_CA_R14_intra-Core]",934900000,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609348","","","36.714-00-00","0.2.0","LTE_CA_R14_intra-Core","","","","","","","","",""]
["R4-1610760","Requirements to complete the 3DL CA combination 4A-12A-12A","Ericsson, US Cellular","Juha Korhonen","21609","pCR","Approval","","","159","8.3.2","UE RF (36.101) [LTE_CA_R14_3DL1UL-Core]",912800000,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609194","","","36.714-03-01","0.5.0","LTE_CA_R14_3DL1UL-Core","","","","","","","","",""]
["R4-1610761","Requirements to complete the 3DL CA combination 5A-12A-12A","Ericsson, US Cellular","Juha Korhonen","21609","pCR","Approval","","","159","8.3.2","UE RF (36.101) [LTE_CA_R14_3DL1UL-Core]",919300000,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609195","","","36.714-03-01","0.5.0","LTE_CA_R14_3DL1UL-Core","","","","","","","","",""]
["R4-1610762","Requirements to complete the 3DL CA combination 5A-12A-66A","Ericsson, US Cellular","Juha Korhonen","21609","pCR","Approval","","","159","8.3.2","UE RF (36.101) [LTE_CA_R14_3DL1UL-Core]",919500000,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609196","","","36.714-03-01","0.5.0","LTE_CA_R14_3DL1UL-Core","","","","","","","","",""]
["R4-1610763","Requirements to complete the 3DL CA combination 12B-66A","Ericsson, US Cellular","Juha Korhonen","21609","pCR","Approval","","","159","8.3.2","UE RF (36.101) [LTE_CA_R14_3DL1UL-Core]",919700000,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609197","","","36.714-03-01","0.5.0","LTE_CA_R14_3DL1UL-Core","","","","","","","","",""]
["R4-1610764","MSD for 3+8 2UL CA","Huawei, Hisilicon","Juha Korhonen","21609","other","Approval","","","12","4.2.1","UE RF (core / EMC)  [WI code or TEI12]",130000,"noted","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609953","","","","","","","","","","","","","",""]
["R4-1610765","MSD for 28+42 2UL CA","Huawei, Hisilicon","Juha Korhonen","21609","other","Approval","","","177","8.6.2","UE RF (36.101) [LTE_CA_R14_2DL2UL-Core]",76500000,"noted","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609954","","","","","","","","","","","","","",""]
["R4-1610766","MSD for 28 + 42 and 21 +28 2UL CA","Qualcomm","Juha Korhonen","21609","other","Discussion","","","177","8.6.2","UE RF (36.101) [LTE_CA_R14_2DL2UL-Core]",76900000,"noted","2016-11-18T23:00:00","2016-11-18T23:00:00","","","","","","","","","","","","","","",""]
["R4-1610767","Introduction of MSD requirement for IMD5 on band3 of CA_3A-8A 2UL CA","CHTTL","Juha Korhonen","21609","CR","Approval","---","","12","4.2.1","UE RF (core / EMC)  [WI code or TEI12]",180000,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610129","","Rel-12","36.101","12.13.0","LTE_CA_R14_xDL2UL-Core","4089","1","F","RP-162404","","","","",""]
["R4-1610768","MSD for 21+28 2UL CA","Huawei, Hisilicon","Juha Korhonen","21609","other","Approval","","","177","8.6.2","UE RF (36.101) [LTE_CA_R14_2DL2UL-Core]",76800000,"noted","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609955","","","","","","","","","","","","","",""]
["R4-1610769","MSD analysis for CA_B5A_B66A with UL on CA_B5A_B66A","Qualcomm Incorporated","Juha Korhonen","21609","other","Approval","","","177","8.6.2","UE RF (36.101) [LTE_CA_R14_2DL2UL-Core]",995400000,"noted","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610178","","Rel-14","","","LTE_CA_R14_2DL2UL-Core","","","","","","","","",""]
["R4-1610770","MSD for 2+66 2UL CA","Huawei, Hisilicon","Juha Korhonen","21609","other","Approval","","","177","8.6.2","UE RF (36.101) [LTE_CA_R14_2DL2UL-Core]",996300000,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609963","","","","","","","","","","","","","",""]
["R4-1610771","TP on MSD results for xDL/2UL CA with B46","LG Electronics Inc.","Juha Korhonen","21609","pCR","Approval","","","183","8.7.2","UE RF (36.101) [LTE_CA_R14_xDL2UL-Core]",77100000,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609790","","","36.714-00-02","0.5.0","LTE_CA_R14_xDL2UL-Core","","","","","","","","",""]
["R4-1610772","MSD for 3+5+7 2UL/3DL CA","Huawei, Hisilicon","Juha Korhonen","21609","other","","","","183","8.7.2","UE RF (36.101) [LTE_CA_R14_xDL2UL-Core]",996900000,"withdrawn","2016-11-24T01:32:43.083",null,"R4-1609974","","","","","","","","","","","","","",""]
["R4-1610773","MSD for 3+19+21 2UL/3DL CA","Huawei, Hisilicon","Juha Korhonen","21609","other","","","","183","8.7.2","UE RF (36.101) [LTE_CA_R14_xDL2UL-Core]",997200000,"withdrawn","2016-11-24T01:32:43.270",null,"R4-1609976","","","","","","","","","","","","","",""]
["R4-1610774","MSD for 19+21+42 2UL/3DL CA","Huawei, Hisilicon","Juha Korhonen","21609","other","Approval","","","183","8.7.2","UE RF (36.101) [LTE_CA_R14_xDL2UL-Core]",997600000,"withdrawn","2016-11-24T01:32:43.473",null,"R4-1609987","","","","","","","","","","","","","",""]
["R4-1610775","Requirements for eLAA dual uplink 3A-46A","Ericsson","Juha Korhonen","21609","pCR","Approval","","","247","8.18.2.4","Other requirements [LTE_eLAA-Core]",77500000,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609205","","","36.714-02-02","0.5.0","LTE_eLAA-Core","","","","","","","","",""]
["R4-1610776","UE CR for CBRS band","Nokia, Qualcomm Incorporated","Juha Korhonen","21609","CR","Approval","","","199","8.10.2","UE RF (36.101) [LTE_TDD_3550_CBRS_US]",982200000,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609822","","Rel-14","36.101","14.1.0","LTE_TDD_3550_CBRS_US","4057","1","B","RP-162405","","","","",""]
["R4-1610777","Introduction of Band 48","Nokia, Ericsson","Juha Korhonen","21609","CR","Approval","","","202","8.10.5","Other specifications [LTE_TDD_3550_CBRS_US]",98620000,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610323","","Rel-14","37.141","14.1.0","LTE_TDD_3550_CBRS_US-Perf","0478","1","B","RP-162405","","","","",""]
["R4-1610778","WF on MPR requirment for SC of UL 256QAM","Huawei, HiSilicon, Skyworks, Nokia, Qorvo, Qualcomm, Ericsson, CMCC","Juha Korhonen","21609","other","Approval","","","228","8.15.2.1","MPR/A-MPR [LTE_UL_CAP_enh-Core]",964600000,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609398","","Rel-14","","","LTE_UL_CAP_enh-Core","","","","","","","","",""]
["R4-1610779","WF on MPR/A-MPR for CA of  UL 256QAM","Huawei, HiSilicon, Skyworks, Nokia, Qorvo, Qualcomm, Ericsson, CMCC\n, Nokia, Qorvo, Qualcomm, Ericsson","Juha Korhonen","21609","other","Approval","","","228","8.15.2.1","MPR/A-MPR [LTE_UL_CAP_enh-Core]",988600000,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609399","","Rel-14","","","LTE_UL_CAP_enh-Core","","","","","","","","",""]
["R4-1610780","LTE TRP and TRS BHH measurement results summary forB1, B3, B7, B20","VODAFONE Group Plc, Telecom Italia","Juha Korhonen","21609","discussion","Discussion","","","218","8.13.2","Hand phantom for smartphones [LTE_UTRA_TRP_TRS-Core]",2800000,"noted","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610425","","Rel-14","","","","","","","","","","","",""]
["R4-1610781","WF on LTE TRP and TRS framework improvement","Oppo","Juha Korhonen","21609","discussion","Endorsement","","","217","8.13.1","General  [LTE_UTRA_TRP_TRS-Core]",97990000,"noted","2016-11-18T23:00:00","2016-11-18T23:00:00","","","","","","","","","","","","","","",""]
["R4-1610782","Proposal for tablet LTE TRP/TRS requirement","NTT DOCOMO INC.","Juha Korhonen","21609","other","Approval","","","220","8.13.4","Free space for LEE devices [LTE_UTRA_TRP_TRS-Core]",980600000,"revised","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609806","R4-1610827","Rel-14","","","","","","","","","","","",""]
["R4-1610783","3GPP MIMO OTA data template for performance requirement phase","ROHDE & SCHWARZ","Juha Korhonen","21609","discussion","Approval","","","222","8.14.1","General [LTE_MIMO_OTA-Core]",52700000,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609124","","Rel-14","37.977","","","","","","","","","","",""]
["R4-1610784","Correction of uplink power control setting","Keysight Technologies UK Ltd, Spirent","Juha Korhonen","21609","CR","Approval","","","222","8.14.1","General [LTE_MIMO_OTA-Core]",93340000,"noted","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610320","","Rel-14","37.977","14.1.0","UTRA_LTE_MIMO_OTA-Core","0044","1","B","","","","","",""]
["R4-1610785","CR to 37.977 to add test zone size for RTS","Keysight Technologies UK Ltd","Juha Korhonen","21609","CR","Approval","","","222","8.14.1","General [LTE_MIMO_OTA-Core]",933700000,"noted","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609335","","Rel-14","37.977","14.1.0","UTRA_LTE_MIMO_OTA-Core","0041","1","B","","","","","",""]
["R4-1610786","Lab alignment test plan","Intel Corporation","Juha Korhonen","21609","other","Approval","","","223","8.14.2","Performance requirements [LTE_MIMO_OTA-Core]",51100000,"revised","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609155","R4-1610987","Rel-14","","","LTE_MIMO_OTA-Core","","","","","","","","",""]
["R4-1610787","LTE UE TRP and TRS Requirements for North American Bands","SPRINT, Verizon, AT&T, SouthernLINC. T-Mobile USA, Bell Canada","Juha Korhonen","21609","other","Approval","","","218","8.13.2","Hand phantom for smartphones [LTE_UTRA_TRP_TRS-Core]",5130000,"noted","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609630","","Rel-14","","","LTE_UTRA_TRP_TRS, LTE_UTRA_TRP_TRS-Core","","","","","","","","",""]
["R4-1610788","Way Forward BS RF requirements impact for shorten TTI feature","Ericsson","Juha Korhonen","21609","discussion","Approval","","","404","10.1.3","BS RF (36.104) [LTE_sTTIandPT]",954200100,"revised","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609542","R4-1610961","Rel-15","","","LTE_sTTIandPT","","","","","","","","",""]
["R4-1610789","WF on UL on/of massk for sTTI operation","Ericsson","Juha Korhonen","21609","other","Endorsement","","","403","10.1.2","UE RF (36.101) [LTE_sTTIandPT]",4720000,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","","","","","","LTE_sTTIandPT","","","","","","","","",""]
["R4-1610790","Way forward on UE RF issues for shortened TTI and processing time for LTE","Ericsson","Juha Korhonen","21609","other","Approval","","","403","10.1.2","UE RF (36.101) [LTE_sTTIandPT]",938400000,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610471","","Rel-15","","","LTE_sTTIandPT","","","","","","","","",""]
["R4-1610791","AAS ACLR absolute limit","Nokia, Ericsson","Juha Korhonen","21609","CR","Agreement","","","22","5.1.1","Technical Report (37.842) [AAS_BS_LTE_UTRA-Core]",2810001,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609911","","Rel-13","37.842","13.0.0","AAS_BS_LTE_UTRA-Core","0009","1","F","RP-162422","","","","",""]
["R4-1610792","Correction on coordinate system","NEC","Juha Korhonen","21609","CR","Approval","","","22","5.1.1","Technical Report (37.842) [AAS_BS_LTE_UTRA-Core]",4310001,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610360","","Rel-13","37.842","13.0.0","AAS_BS_LTE_UTRA-Core","0012","1","F","RP-162422","","","","",""]
["R4-1610793","Correction of directions diagram in TR 37.842","CATT","Juha Korhonen","21609","CR","Approval","","","22","5.1.1","Technical Report (37.842) [AAS_BS_LTE_UTRA-Core]",942200001,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609670","","Rel-13","37.842","13.0.0","AAS_BS_LTE_UTRA","0008","1","F","RP-162422","","","","",""]
["R4-1610794","AAS ACLR absolute limit","Nokia, Ericsson","Juha Korhonen","21609","CR","Approval","","","23","5.1.2","BS RF(37.105) [AAS_BS_LTE_UTRA-Core]",3860000,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609912","","Rel-13","37.105","13.2.0","AAS_BS_LTE_UTRA-Core","0024","1","F","RP-162422","","","","",""]
["R4-1610795","TS 37.105: Removal of operating band unwanted emissions for Band 46","Ericsson","Juha Korhonen","21609","CR","Agreement","","","23","5.1.2","BS RF(37.105) [AAS_BS_LTE_UTRA-Core]",991200000,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609959","","Rel-13","37.105","13.2.0","AAS_BS_LTE_UTRA","0021","1","F","RP-162422","","","","",""]
["R4-1610796","Clarification on the Rx diversity branches vs. demodulation branches terminology","Huawei","Juha Korhonen","21609","CR","Agreement","","","23","5.1.2","BS RF(37.105) [AAS_BS_LTE_UTRA-Core]",996000000,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","","","Rel-13","37.105","13.2.0","AAS_BS_LTE_UTRA-Core","0026","","F","RP-162422","","","","",""]
["R4-1610797","TS 37.145-1: Corrections","Ericsson","Juha Korhonen","21609","CR","Approval","","","25","5.1.3.1","Maintenance for TS37.145-1 [AAS_BS_LTE_UTRA-Perf]",4330001,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609962","","Rel-13","37.145-1","13.0.0","AAS_BS_LTE_UTRA","0006","1","F","RP-162422","","","","",""]
["R4-1610798","CR to TS 37.145-1: Frequency error corrections","Huawei","Juha Korhonen","21609","CR","Approval","","","25","5.1.3.1","Maintenance for TS37.145-1 [AAS_BS_LTE_UTRA-Perf]",4390001,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610435","","Rel-13","37.145-1","13.0.0","AAS_BS_LTE_UTRA-Perf","0007","1","D","RP-162422","","","","",""]
["R4-1610799","TP to TR 37.843: Remaining OTA requirements for eAAS BS","Huawei","Juha Korhonen","21609","pCR","Approval","","","207","8.12.1","General [AASenh_BS_LTE_UTRA]",4010001,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610437","","","37.843","0.0.1","AASenh_BS_LTE_UTRA","","","","","","","","",""]
["R4-1610800","WF on OTA requirements compliance range","NTT DOCOMO, INC.","Juha Korhonen","21609","discussion","Endorsement","","","209","8.12.2.1","In band requirements [AASenh_BS_LTE_UTRA]",80400,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","","","","","","AASenh_BS_LTE_UTRA","","","","","","","","",""]
["R4-1610801","WF on BS output power requirement","Ericsson","Juha Korhonen","21609","discussion","Endorsement","","","209","8.12.2.1","In band requirements [AASenh_BS_LTE_UTRA]",3610000,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","","","","","","AASenh_BS_LTE_UTRA","","","","","","","","",""]
["R4-1610802","TP to 37.843: Background information on conducted ACLR requirement","Ericsson","Juha Korhonen","21609","other","Approval","","","209","8.12.2.1","In band requirements [AASenh_BS_LTE_UTRA]",4360000,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609935","","","","","AASenh_BS_LTE_UTRA","","","","","","","","",""]
["R4-1610803","TP to TR 37.843 on ACLR","Huawei","Juha Korhonen","21609","pCR","Approval","","","209","8.12.2.1","In band requirements [AASenh_BS_LTE_UTRA]",4370001,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610396","","","37.843","0.0.1","AASenh_BS_LTE_UTRA","","","","","","","","",""]
["R4-1610804","WF on the measurement grid for ACLR","Ericsson","Juha Korhonen","21609","discussion","Endorsement","","","209","8.12.2.1","In band requirements [AASenh_BS_LTE_UTRA]",4980001,"revised","2016-11-18T23:00:00","2016-11-18T23:00:00","","R4-1610989","","","","AASenh_BS_LTE_UTRA","","","","","","","","",""]
["R4-1610805","WF on the hydrid requirements","Huawei","Juha Korhonen","21609","discussion","Endorsement","","","209","8.12.2.1","In band requirements [AASenh_BS_LTE_UTRA]",80500,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","","","","","","AASenh_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-1610806","TP to 37.843: Background information on conducted EVM requirement","Ericsson","Juha Korhonen","21609","other","Approval","","","209","8.12.2.1","In band requirements [AASenh_BS_LTE_UTRA]",972900000,"withdrawn","2016-11-24T01:32:51.990",null,"R4-1609936","","","","","AASenh_BS_LTE_UTRA","","","","","","","","",""]
["R4-1610807","WF on OTA sensitivity","NEC","Juha Korhonen","21609","discussion","Endorsement","","","209","8.12.2.1","In band requirements [AASenh_BS_LTE_UTRA]",993400000,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","","","","","","AASenh_BS_LTE_UTRA","","","","","","","","",""]
["R4-1610808","TP to TR 37.843 on min EIS","Huawei","Juha Korhonen","21609","pCR","Approval","","","209","8.12.2.1","In band requirements [AASenh_BS_LTE_UTRA]",993600001,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610390","","","37.843","0.0.1","AASenh_BS_LTE_UTRA","","","","","","","","",""]
["R4-1610809","Reply LS on RF requirements for category NB1 UEs","RAN4","Juha Korhonen","21609","LS out","Approval","","","54","5.6.2","UE RF (36.101) [NB_IOT-Core]",983000001,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610596","","Rel-13","","","NB_IOT-Core","","","","","","RAN5","","",""]
["R4-1610810","Reply LS on NB-IoT RRC Re-establishment test configurations","RAN4","Juha Korhonen","21609","LS out","Approval","","","121","6.3.3.4","RRC Re-establishment test [NB_IOT-Perf]",1800001,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609725","","Rel-13","","","NB_IOT-Perf","","","","","","RAN5","","",""]
["R4-1610811","WF on EMC requirements for AAS","Ericsson","Juha Korhonen","21609","discussion","Endorsement","","","211","8.12.2.3","EMC requirements [AASenh_BS_LTE_UTRA]",4490000,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","","","","","","","","","","","","","","",""]
["R4-1610812","TP for 36.789: Updates on section 5 and 6.1","Huawei","Juha Korhonen","21609","pCR","Approval","","","139","7.1.1","General  [FS_LTE_LAA_multinode_test]",4640001,"noted","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609365","","","36.789","0.0.1","FS_LTE_LAA_multinode_test","","","","","","","","",""]
["R4-1610813","New performance Item MIMO OTA","GCF-PAC","Juha Korhonen","21609","LS in","Action","","","2","3","Letters / reports from other groups / meetings",81300,"noted","2016-11-18T23:00:00","2016-11-18T23:00:00","","","","","","UTRA_LTE_MIMO_OTA-Core","","","","","","RAN4","RAN, GCF SG","10DCR-General-044-PAG-16-060r1_-_LS_to_RAN4_on_New_Performance_Item_MIMO_OTA",""]
["R4-1610814","Reply LS on RAN2 agreements for NR DL-based mobility and cell definition","RAN1","Juha Korhonen","21609","LS in","Information","","","2","3","Letters / reports from other groups / meetings",81400,"available","2016-11-24T01:32:53.690","2016-11-24T01:37:26.707","","","Rel-14","","","FS_NR_newRAT","","","","","","RAN2","RAN3, RAN4","R1-1613348",""]
["R4-1610815","Corrections to CA table reference and header and CA REFSENS table","Nokia, Alcatel-Lucent Shanghai Bell","Juha Korhonen","21609","CR","","","","67","5.10.1.1","RF  [WI code]",3180001,"revised","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609836","R4-1610958","Rel-13","36.101","13.5.0","TEI13","4064","1","F","","","","","",""]
["R4-1610816","Corrections of CA Refsens exceptions in 7.3.1A (Rel-13)","Nokia, Alcatel-Lucent Shanghai Bell, Ericsson, Huawei","Juha Korhonen","21609","CR","Approval","","","67","5.10.1.1","RF  [WI code]",983600001,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609905","","Rel-13","36.101","13.5.0","TEI13","4076","1","F","RP-162435","","","","",""]
["R4-1610817","Corrections of CA Refsens exceptions in 7.3.1A (Rel-14)","Nokia, Alcatel-Lucent Shanghai Bell, Huawei, Ericsson","Juha Korhonen","21609","CR","Approval","","","67","5.10.1.1","RF  [WI code]",990500001,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609907","","Rel-14","36.101","14.1.0","TEI13, TEI14","4078","1","F","RP-162435","","","","",""]
["R4-1610818","DeltaRIB for SDL and LAA CA","Nokia, Alcatel-Lucent Shanghai Bell","Juha Korhonen","21609","CR","Approval","","","67","5.10.1.1","RF  [WI code]",990600001,"revised","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609909","R4-1611030","Rel-13","36.101","13.5.0","TEI13","4080","1","F","","","","","",""]
["R4-1610819","Addition of 1.4 and 3 MHz channel bandwidths for BAND 65 in TS36.101 (Rel-13)","HUGHES Network Systems Ltd","Juha Korhonen","21609","CR","Endorsement","","","70","5.10.2","New spectrum [WI code]",168001,"revised","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609059","R4-1610915","Rel-13","36.101","13.5.0","","3968","1","B","","","","","",""]
["R4-1610820","Addition of 1.4 and 3 MHz channel bandwidths for BAND 65 in TS36.101 (Rel-14)","HUGHES Network Systems Ltd","Juha Korhonen","21609","CR","Endorsement","","","70","5.10.2","New spectrum [WI code]",905900001,"revised","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609060","R4-1610916","Rel-14","36.101","14.1.0","","3969","1","B","","","","","",""]
["R4-1610821","Band 68 NS_26 A-MPR correction","Qualcomm Incorporated","Juha Korhonen","21609","CR","","","","71","5.10.2.1","RF  [WI code]",194001,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610194","","Rel-13","36.101","13.5.0","LTE_FDD_700_ARAB-Core","4103","1","F","RP-162427","","","","",""]
["R4-1610822","Initial bands for single Rx category 1","Qualcomm Incorporated","Juha Korhonen","21609","other","","","","331","8.27.2","UE RF (36.101) [LTE_UE_cat_1RX-Core]",974300001,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610186","","","","","","","","","","","","","",""]
["R4-1610823","Versioning bit indicator for NS_04 A-MPR table","Qualcomm Incorporated","Juha Korhonen","21609","CR","","","","195","8.9.2","UE RF (36.101) [LTE_B41_UE_PC2-Core]",193001,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610193","","Rel-14","36.101","14.1.0","LTE_B41_UE_PC2","4102","1","F","RP-162406","","","","",""]
["R4-1610824","Addition of TDD RMC for UL-DL configuration 0","Ericsson","Juha Korhonen","21609","CR","Approval","","","195","8.9.2","UE RF (36.101) [LTE_B41_UE_PC2-Core]",5200001,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610520","","Rel-14","36.101","14.1.0","LTE_B41_UE_PC2-Core","4135","1","F","RP-162406","","","","",""]
["R4-1610825","P-Max related requirements for HPUE","NTT DOCOMO, INC.","Juha Korhonen","21609","other","Approval","","","234","8.16.2","UE RF (36.101)  [LTE_HPUE_B3_B20_B28]",987100001,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609871","","","","","LTE_HPUE_B3_B20_B28","","","","","","","","",""]
["R4-1610826","Draft CR for HPUE for operating bands other than Band 41","NTT DOCOMO, INC.","Juha Korhonen","21609","draftCR","Endorsement","","","234","8.16.2","UE RF (36.101)  [LTE_HPUE_B3_B20_B28]",987200001,"endorsed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609872","","Rel-14","36.101","14.1.0","LTE_HPUE_B3_B20_B28","","","B","","","","","",""]
["R4-1610827","Proposal for tablet LTE TRP/TRS requirement","NTT DOCOMO INC.","Juha Korhonen","21609","other","Approval","","","220","8.13.4","Free space for LEE devices [LTE_UTRA_TRP_TRS-Core]",980600001,"withdrawn","2016-11-24T01:32:57.373",null,"R4-1610782","","Rel-14","","","","","","","","","","","",""]
["R4-1610828","Ls on New power class","Nokia, Alcatel-Lucent Shanghai Bell","Juha Korhonen","21609","LS out","Approval","","","304","8.24.2.1","Power Class       [NB_IOTenh-Core]",982800000,"noted","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609828","","","","","NB_IOTenh-Core","","","","","","","","",""]
["R4-1610829","WF on new power class for NB-IoT","Qualcomm, U-Blox","Juha Korhonen","21609","discussion","Endorsement","","","304","8.24.2.1","Power Class       [NB_IOTenh-Core]",982800001,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","","","","","","NB_IOTenh-Core","","","","","","","","",""]
["R4-1610830","WF on frequency bands for FeMTC","Ericsson","Juha Korhonen","21609","discussion","Endorsement","","","313","8.25.2","High data rate  [LTE_feMTC-Core]",988500000,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","","","","","","LTE_feMTC-Core","","","","","","","","",""]
["R4-1610831","Introduction of new bands for NB-IoT in 36.307","Ericsson","Juha Korhonen","21609","CR","Approval","","","237","8.17.1","Rapporteur Input [NB_IOT_R14_bands]",167000,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609883","","Rel-13","36.307","13.5.0","NB_IOT_R14_bands-Core","0718","1","B","RP-162407","","","","",""]
["R4-1610832","WF on A-MPR simulation assumptions for Band 68","Airbus DS SLC","Juha Korhonen","21609","discussion","Endorsement","","","374","8.32.2","RF  [WI code or TEI14]",2830000,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","","","","","","","","","","","","","","",""]
["R4-1610833","LS on UE RF Bandwidth Adaptation in NR","RAN1","Juha Korhonen","21609","LS in","Discussion","","","2","3","Letters / reports from other groups / meetings",83300,"available","2016-11-24T01:32:58.697","2016-11-24T01:37:26.707","","","Rel-14","","","FS_NR_newRAT","","","","","","RAN4","","R1-1613663",""]
["R4-1610834","RAN4#81 evening adhoc meeting report","Ericsson","Juha Korhonen","21609","report","Approval","","","242","8.18.1","General [LTE_eLAA-Core]",83400,"revised","2016-11-18T23:00:00","2016-11-18T23:00:00","","R4-1610835","","","","","","","","","","","","",""]
["R4-1610835","RAN4#81 evening adhoc meeting report","Ericsson","Juha Korhonen","21609","report","Approval","","","242","8.18.1","General [LTE_eLAA-Core]",83401,"noted","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610834","","","","","","","","","","","","","",""]
["R4-1610836","WF on eLAA uplink requirements","Ericsson","Juha Korhonen","21609","discussion","Endorsement","","","242","8.18.1","General [LTE_eLAA-Core]",83600,"revised","2016-11-18T23:00:00","2016-11-18T23:00:00","","R4-1610913","","","","","","","","","","","","",""]
["R4-1610837","TP for TR36.745: Evaluation results and conclusion (section 6 and 7)","SoftBank Corp.","Juha Korhonen","21609","pCR","Approval","","","388","9.2.2","UE RF (36.101) [FS_LTE_B11_B21_global]",904300000,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609043","","","36.745","1.0.0","","","","","","","","","",""]
["R4-1610838","TP for TR 36.745: EESS protection scheme","NTT DOCOMO, INC.","Juha Korhonen","21609","pCR","Approval","","","388","9.2.2","UE RF (36.101) [FS_LTE_B11_B21_global]",949400000,"withdrawn","2016-11-24T01:32:59.777",null,"R4-1609879","","","36.745","1.0.0","FS_LTE_B11_B21_global","","","","","","","","",""]
["R4-1610839","Technical Report of B11/B21 Globalization(TR36.745 v0.3.0)","SoftBank Corp.","Juha Korhonen","21609","draft TR","Approval","","","388","9.2.2","UE RF (36.101) [FS_LTE_B11_B21_global]",987900000,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","","","Rel-14","36.745","0.3.0","FS_LTE_B11_B21_global","","","","","","","","",""]
["R4-1610840","Ad-hoc meeting minutes for V2V/V2X UE RF","LGE","Juha Korhonen","21609","report","Approval","","","272","8.20","LTE based V2X  [LTE_V2X]",84000,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","","","","","","LTE_V2X-Core","","","","","","","","",""]
["R4-1610841","Summary of coexistence results","China Telecom","Juha Korhonen","21609","discussion","Discussion","","","392","9.3.3","Co-existence study [FS_NB_IOT_CDMA_coex]",974200001,"noted","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609741","","","","","FS_NB_IOT_CDMA_coex","","","","","","","","",""]
["R4-1610842","TP for 36.752 coexistence simulation results","China Telecom","Juha Korhonen","21609","pCR","Approval","","","392","9.3.3","Co-existence study [FS_NB_IOT_CDMA_coex]",982000001,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609742","","","36.752","1.0.0","FS_NB_IOT_CDMA_coex","","","","","","","","",""]
["R4-1610843","TP for TR 36.752: RF Requirement Evaluation for NB-IoT Coexistence with CDMA","Samsung, China Telecom","Juha Korhonen","21609","pCR","Approval","","","393","9.3.4","RF requirements impact [FS_NB_IOT_CDMA_coex]",938600000,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609358","","","36.752","1.0.0","FS_NB_IOT_CDMA_coex","","","","","","","","",""]
["R4-1610844","TP for TR 36.752: Conclusion","Samsung, China Telecom","Juha Korhonen","21609","pCR","Approval","","","393","9.3.4","RF requirements impact [FS_NB_IOT_CDMA_coex]",953900001,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609359","","","36.752","1.0.0","FS_NB_IOT_CDMA_coex","","","","","","","","",""]
["R4-1610845","TP for TR 36.752: Description of simulation methodology","Samsung, China Telecom","Juha Korhonen","21609","pCR","Approval","","","393","9.3.4","RF requirements impact [FS_NB_IOT_CDMA_coex]",954000001,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","","","","36.752","1.0.0","FS_NB_IOT_CDMA_coex","","","","","","","","",""]
["R4-1610846","TR 36.752 Study of NB-IoT RF requirement for coexistence with CDMA v0.2.0","China Telecom","Juha Korhonen","21609","draft TR","Approval","","","389","9.3","Study on NB-IoT RF requirement for coexistence with CDMA [FS_NB_IOT_CDMA_coex]",974000000,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","","","Rel-14","36.752","0.2.0","FS_NB_IOT_CDMA_coex","","","","","","","","",""]
["R4-1610847","CR for 36.101: frequency error for eMTC","Huawei, Intel Corporation, Ericsson","Juha Korhonen","21609","CR","Agreement","","","45","5.5.1","UE RF (36.101)  [LTE_MTCe2_L1-Core]",4580001,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609393","","Rel-13","36.101","13.5.0","LTE_MTCe2_L1-Core","4001","1","F","RP-162430","","","","",""]
["R4-1610848","Correction of power control for category M1","Intel Corporation, Ericsson, Qualcomm, Sony, Sierra Wireless, Verizon Wireless","Juha Korhonen","21609","CR","Agreement","","","45","5.5.1","UE RF (36.101)  [LTE_MTCe2_L1-Core]",913200001,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609134","","Rel-13","36.101","13.5.0","LTE_MTCe2_L1-Core","3977","1","F","RP-162430","","","","",""]
["R4-1610849","Correction of REFSENS RMC table for Cat-M1 UE","Ericsson, Anritsu","Juha Korhonen","21609","CR","Approval","","","45","5.5.1","UE RF (36.101)  [LTE_MTCe2_L1-Core]",939200001,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609694","","Rel-13","36.101","13.5.0","LTE_MTCe2_L1-Core","4047","1","F","RP-162430","","","","",""]
["R4-1610850","Missing requirements for eMTC/NB IoT UE","KDDI Corporation","Juha Korhonen","21609","CR","Agreement","","","45","5.5.1","UE RF (36.101)  [LTE_MTCe2_L1-Core]",969400000,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610508","","Rel-13","36.101","13.5.0","LTE_MTCe2_L1-Core, NB_IOT-Core","4132","1","F","RP-162431","","","","",""]
["R4-1610851","Correction to WLAN measurement configuration","MediaTek Inc.","Juha Korhonen","21609","CR","Approval","","","63","5.9.2","RRM [WI code or TEI13]",3220001,"revised","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610322","R4-1610873","Rel-13","36.133","13.5.0","LTE_WLAN_radio-Perf","4340","1","F","","","","","",""]
["R4-1610852","Introduction of new bands for NB-IoT in 36.133","Ericsson","Juha Korhonen","21609","CR","Approval","","","237","8.17.1","Rapporteur Input [NB_IOT_R14_bands]",0,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610167","","Rel-14","36.133","14.1.0","NB_IOT_R14_bands-Core","4366","","B","RP-162407","","","","",""]
["R4-1610853","Simulation assumptions for V2V demodulation requiremetns","Huawei, HiSilicon","Juha Korhonen","21609","other","Approval","","","268","8.19.4","UE demodulation (36.101)  [LTE_SL_V2V-Perf]",94810001,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609481","","","","","","","","","","","","","",""]
["R4-1610854","RSTD measurements in shared cells","Ericsson","Juha Korhonen","21609","CR","Approval","","","297","8.22.3.1","OTDOA/E-CID enhancement [UTRA_LTE_iPos_enh2]",34000001,"noted","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610340","","Rel-14","36.133","14.1.0","UTRA_LTE_iPos_enh2-Core","4345","1","B","","","","","",""]
["R4-1610855","LS on E-CID measurements for NB-IoT","Ericsson","Juha Korhonen","21609","LS out","Approval","","","307","8.24.3.1.1","E-CID  [NB_IOTenh-Core]",92770001,"noted","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610345","","Rel-14","","","NB_IOTenh-Core","","","","","","RAN2, RAN3","","",""]
["R4-1610856","CR for introducing new demod tests for 4Rx CA","Ericsson, Qualcomm","Juha Korhonen","21609","CR","Approval","","","359","8.30.3.2","Extend existing 2Rx CA requirement to 4Rx [LTE_4Rx_AP_DL_CA-Perf]",999900001,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610000","","Rel-14","36.101","14.1.0","LTE_4Rx_AP_DL_CA-Perf","4088","1","B","RP-162394","","","","",""]
["R4-1610857","CR to introduce handover requirements for mobility enhancement_R14","ZTE, ZTE Microelectronics","Juha Korhonen","21609","CR","Agreement","","","327","8.26.3","RRM core (36.133) [LTE_eMob-Core]",974900001,"revised","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609749","R4-1610878","Rel-14","36.133","14.1.0","LTE_eMob-Core","4228","1","B","","","","","",""]
["R4-1610858","CR for fixing soft buffer management test for TDD-FDD CA in Rel-12","Ericsson","Juha Korhonen","21609","CR","Approval","","","15","4.2.4","UE demodulation performance  [WI code or TEI12]",37700001,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609991","","Rel-12","36.101","12.13.0","TEI12","4083","1","F","RP-162421","","","","",""]
["R4-1610859","WF on HST unidirectional test","Ericsson, Vodafone, Telecom Italia, NTT DOCOMO","Juha Korhonen","21609","discussion","Endorsement","","","346","8.28.3.2","Unidirectional RRH arrangement [LTE_high_speed]",85900,"revised","2016-11-18T23:00:00","2016-11-18T23:00:00","","R4-1610968","","","","LTE_high_speed","","","","","","","","",""]
["R4-1610860","CR on the enhanced RRM requirements in connected mode under high speed scenario","Huawei, HiSilicon","Juha Korhonen","21609","CR","Approval","","","341","8.28.2.1","Enhancement in connected mode (DRX) [LTE_high_speed]",929700001,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610106","","Rel-14","36.133","14.1.0","LTE_high_speed","4291","1","B","RP-162388","","","","",""]
["R4-1610861","CR on interruption requirements in SRS switching","Huawei, HiSilicon","Juha Korhonen","21609","CR","Approval","","","291","8.21.3","RRM core and performance (36.133) [LTE_SRS_switch-Core/Perf]",10900001,"revised","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610109","R4-1610963","Rel-14","36.133","14.1.0","","4293","1","B","","","","","",""]
["R4-1610862","Way forward on SDR test for extension of LAA demodulation","Ericsson","Juha Korhonen","21609","discussion","Endorsement","","","107","6.2.4.1","General [LTE_LAA-Perf]",639000,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","","","","","","LTE_LAA-Perf","","","","","","","","",""]
["R4-1610863","CR for Rel-13 eMTC PBCH demodulation requirement for enhanced coverage","Huawei, HiSilicon","Juha Korhonen","21609","CR","Agreement","","","97","6.1.2.1","PBCH [LTE_MTCe2_L1-Perf]",946300001,"revised","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609464","R4-1610893","Rel-13","36.101","13.5.0","LTE_MTCe2_L1-Perf","4008","1","F","","","","","",""]
["R4-1610864","TP: deploymenet scenarios for BS-IC","Huawei","Juha Korhonen","21609","other","Approval","","","396","9.4.2","Deployment scenario [FS_LTE _IC_BS]",945400001,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609455","","","","","","","","","","","","","",""]
["R4-1610865","Updates to burst transmission model for LAA performance requirements (Rel-13)","Huawei, HiSilicon","Juha Korhonen","21609","CR","Agreement","","","108","6.2.4.2","PDSCH [LTE_LAA-Perf]",959500001,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610133","","Rel-13","36.101","13.5.0","LTE_LAA-Perf","4092","1","F","RP-162386","","","","",""]
["R4-1610866","Way forward on V2V single-link performance requirements","Huawei, HiSilicon","Juha Korhonen","21609","discussion","Endorsement","","","268","8.19.4","UE demodulation (36.101)  [LTE_SL_V2V-Perf]",75000000,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","","","","","","LTE_SL_V2V-Perf","","","","","","","","",""]
["R4-1610867","CR on RRC re-establishment test case for Cat-M1 in CE Mode A","Intel Corporation","Juha Korhonen","21609","CR","Agreement","","","84","6.1.1.2.4","RRC Re-establishment [LTE_MTCe2_L1-Perf]",914100001,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609141","","Rel-13","36.133","13.5.0","LTE_MTCe2_L1-Perf","4166","1","F","RP-162382","","","","",""]
["R4-1610868","CR on RRC re-establishment test case for Cat-M1 in CE Mode A","Intel Corporation","Juha Korhonen","21609","CR","Agreement","","","84","6.1.1.2.4","RRC Re-establishment [LTE_MTCe2_L1-Perf]",914200001,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609142","","Rel-14","36.133","14.1.0","LTE_MTCe2_L1-Perf","4167","1","A","RP-162382","","","","",""]
["R4-1610869","CR on cell re-selection test case for Cat-M1 in normal coverage","Intel Corporation","Juha Korhonen","21609","CR","Agreement","","","85","6.1.1.2.5","Others  [LTE_MTCe2_L1-Perf]",913700001,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609137","","Rel-13","36.133","13.5.0","LTE_MTCe2_L1-Perf","4162","1","F","RP-162384","","","","",""]
["R4-1610870","CR on cell re-selection test case for Cat-M1 in normal coverage","Intel Corporation","Juha Korhonen","21609","CR","Agreement","","","85","6.1.1.2.5","Others  [LTE_MTCe2_L1-Perf]",913800001,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609138","","Rel-14","36.133","14.1.0","LTE_MTCe2_L1-Perf","4163","1","A","RP-162384","","","","",""]
["R4-1610871","Corrections to LAA Measurement Requirements","Qualcomm Incorporated","Juha Korhonen","21609","CR","Approval","","","42","5.4.3","RRM Core [LTE_LAA-Core]",9811001,"withdrawn","2016-11-24T01:33:10.257",null,"R4-1609811","","Rel-13","36.133","13.5.0","LTE_LAA","4233","1","F","","","","","",""]
["R4-1610872","Clarification on Inter-frequency RSSI measurements in LAA R13","Huawei, HiSilicon","Juha Korhonen","21609","CR","Approval","","","42","5.4.3","RRM Core [LTE_LAA-Core]",11600001,"withdrawn","2016-11-24T01:33:10.570",null,"R4-1610116","","Rel-13","36.133","13.5.0","","4295","1","F","","","","","",""]
["R4-1610873","Correction to WLAN measurement configuration","MediaTek Inc.","Juha Korhonen","21609","CR","Approval","","","63","5.9.2","RRM [WI code or TEI13]",3220002,"revised","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610851","R4-1610889","Rel-13","36.133","13.5.0","LTE_WLAN_radio-Perf","4340","2","F","","","","","",""]
["R4-1610874","CR on UE transmission timing requirements for V2X","CATT","Juha Korhonen","21609","CR","Approval","","","281","8.20.4.1","UE Transmit timing [LTE_V2X-Core]",24500001,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609509","","Rel-14","36.133","14.1.0","LTE_V2X-Core","4213","1","B","RP-162393","","","","",""]
["R4-1610875","CR on clarification of RRM requirement for indoor positioning","Huawei, HiSilicon","Juha Korhonen","21609","CR","","","","297","8.22.3.1","OTDOA/E-CID enhancement [UTRA_LTE_iPos_enh2]",9101000,"noted","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610075","","Rel-14","36.133","14.1.0","","4283","1","F","","","","","",""]
["R4-1610876","WF on closing further indoor positioning WI core part in RAN4","Huawei","Juha Korhonen","21609","discussion","Agreement","","","297","8.22.3.1","OTDOA/E-CID enhancement [UTRA_LTE_iPos_enh2]",92740000,"noted","2016-11-18T23:00:00","2016-11-18T23:00:00","","","","","","UTRA_LTE_iPos_enh2","","","","","","","","",""]
["R4-1610877","LS on ECID measurement quantity for NB-IoT","RAN4","Juha Korhonen","21609","LS out","Approval","","","307","8.24.3.1.1","E-CID  [NB_IOTenh-Core]",8600002,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610697","","Rel-14","","","NB_IOTenh-Core","","","","","","RAN1","","","R1-1704000"]
["R4-1610878","CR to introduce handover requirements for mobility enhancement","ZTE, ZTE Microelectronics, Nokia, Samsung, Ericsson, Intel, Qualcomm","Juha Korhonen","21609","CR","Agreement","","","327","8.26.3","RRM core (36.133) [LTE_eMob-Core]",974900002,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610857","","Rel-14","36.133","14.1.0","LTE_eMob-Core","4228","2","B","RP-162391","","","","",""]
["R4-1610879","WF on demodulation performance for Cat 1 UE with 1 Rx","Qualcomm","Juha Korhonen","21609","discussion","Approval","","","336","8.27.5","UE demodulation (36.101) [LTE_UE_cat_1RX-Perf]",87900,"revised","2016-11-18T23:00:00","2016-11-18T23:00:00","","R4-1610881","","","","LTE_UE_cat_1RX-Perf","","","","","","","","",""]
["R4-1610880","WF on CSI requirements for Cat 1 UE with 1Rx","Qualcomm","Juha Korhonen","21609","discussion","Approval","","","337","8.27.6","UE CSI (36.101) [LTE_UE_cat_1RX-Perf]",88000,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","","","","","","LTE_UE_cat_1RX-Perf","","","","","","","","",""]
["R4-1610881","WF on demodulation performance for Cat 1 UE with 1 Rx","Qualcomm","Juha Korhonen","21609","discussion","Approval","","","336","8.27.5","UE demodulation (36.101) [LTE_UE_cat_1RX-Perf]",87901,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610879","","","","","LTE_UE_cat_1RX-Perf","","","","","","","","",""]
["R4-1610882","CR for RRM requirements  in idle mode  for high speed conditions","CATT","Juha Korhonen","21609","CR","Approval","","","342","8.28.2.2","Enhancement in idle mode [LTE_high_speed]",955200011,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610676","","Rel-14","36.133","14.1.0","LTE_high_speed","4217","2","B","RP-162388","","","","",""]
["R4-1610883","CR on introducing inter-cell synchronization requirements for MBMS R14","Huawei, HiSilicon","Juha Korhonen","21609","CR","Approval","","","373","8.32.1","Inter-cell Synchronization for MBMS/eMBMS [WI code or TEI14]",953000001,"noted","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610092","","Rel-14","36.133","14.1.0","","4289","1","B","","","","","",""]
["R4-1610884","WF on Rel-12 SU-MIMIO multi-cell test","Qualcomm","Juha Korhonen","21609","discussion","Agreement","","","376","8.32.4","Demodulation [WI code or TEI14]",88400,"noted","2016-11-18T23:00:00","2016-11-18T23:00:00","","","","","","TEI14","","","","","","","","",""]
["R4-1610885","Clean up and clarification for LAA CSI requirements","Ericsson","Juha Korhonen","21609","CR","Approval","","","110","6.2.5","UE CSI reporting (36.101) [LTE_LAA-Perf]",917400001,"revised","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610644","R4-1610965","Rel-13","36.101","13.5.0","LTE_LAA-Perf","3980","2","F","","","","","",""]
["R4-1610886","LS on starting PRACH CE level selection for BL/CE UEs","Nokia, Alcatel-Lucent Shanghai Bell","Juha Korhonen","21609","LS out","Approval","","","51","5.5.3.4","Others [LTE_MTCe2_L1-Core]",72300000,"noted","2016-11-18T23:00:00","2016-11-18T23:00:00","","","Rel-14","","","LTE_MTCe2_L1-Core","","","","","","","","",""]
["R4-1610887","CR on eMTC PBCH requirements correction","Intel Corporation","Juha Korhonen","21609","CR","","","","97","6.1.2.1","PBCH [LTE_MTCe2_L1-Perf]",946500001,"endorsed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609115","","Rel-13","36.101","13.5.0","","3974","1","F","","","","","",""]
["R4-1610888","Liaison statement on measurement gaps","Ericsson","Juha Korhonen","21609","LS out","Approval","","","351","8.29.2","RRM core (36.133) [LTE_meas_gap_enh-Core]",954700001,"revised","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609547","R4-1610999","Rel-14","","","LTE_meas_gap_enh-Core","","","","","R2-167317","RAN2","RAN1","",""]
["R4-1610889","Correction to WLAN measurement configuration","MediaTek Inc.","Juha Korhonen","21609","CR","Approval","","","63","5.9.2","RRM [WI code or TEI13]",3220003,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610873","","Rel-13","36.133","13.5.0","LTE_WLAN_radio-Perf","4340","3","F","RP-162432","","","","",""]
["R4-1610890","CR on RRC re-establishment test case for Cat-M1 in CE Mode B","Intel Corporation","Juha Korhonen","21609","CR","Agreement","","","89","6.1.1.3.3","RRC Re-establishment [LTE_MTCe2_L1-Perf]",6200001,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609143","","Rel-13","36.133","13.5.0","LTE_MTCe2_L1-Perf","4168","1","F","RP-162384","","","","",""]
["R4-1610891","CR on modification of cell reselection test case R13","Huawei, HiSilicon","Juha Korhonen","21609","CR","","","","87","6.1.1.3.1","Intra-frequency Cell Re-Selection [LTE_MTCe2_L1-Perf]",66001,"revised","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610066","R4-1610898","Rel-13","36.133","13.5.0","","4279","1","F","","","","","",""]
["R4-1610892","Simulation assumption for UE Rx-Tx time different measurement","Huawei, HiSilicon","Juha Korhonen","21609","other","","","","307","8.24.3.1.1","E-CID  [NB_IOTenh-Core]",34500002,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610698","","","","","","","","","","","","","",""]
["R4-1610893","CR for Rel-13 eMTC PBCH demodulation requirement for enhanced coverage","Huawei, HiSilicon","Juha Korhonen","21609","CR","Agreement","","","97","6.1.2.1","PBCH [LTE_MTCe2_L1-Perf]",946300002,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610863","","Rel-13","36.101","13.5.0","LTE_MTCe2_L1-Perf","4008","2","F","RP-162384","","","","",""]
["R4-1610894","Introduce RSRP accuracy test case for Band 31 for Cat-M1 UE","Huawei, HiSilicon","Juha Korhonen","21609","CR","Approval","","","79","6.1.1.1.2","Others  [LTE_MTCe2_L1-Perf]",31001,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610650","","Rel-13","36.133","13.5.0","LTE_MTCe2_L1-Perf","4255","2","B","RP-162384","","","","",""]
["R4-1610895","Introduce 5MHz Bandwidth MPDCCH Reference Channel for Cat-M1 UE","Huawei, HiSilicon","Juha Korhonen","21609","CR","Approval","","","79","6.1.1.1.2","Others  [LTE_MTCe2_L1-Perf]",33001,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610030","","Rel-13","36.133","13.5.0","LTE_MTCe2_L1-Perf","4257","1","B","RP-162384","","","","",""]
["R4-1610896","Introduce 5MHz Bandwidth MPDSCH Reference Channel for Cat-M1 UE","Huawei, HiSilicon","Juha Korhonen","21609","CR","Approval","","","79","6.1.1.1.2","Others  [LTE_MTCe2_L1-Perf]",35001,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610032","","Rel-13","36.133","13.5.0","LTE_MTCe2_L1-Perf","4259","1","B","RP-162384","","","","",""]
["R4-1610897","Introduce 5MHz Bandwidth OCNG for Cat-M1 UE","Huawei, HiSilicon","Juha Korhonen","21609","CR","Approval","","","79","6.1.1.1.2","Others  [LTE_MTCe2_L1-Perf]",649001,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610034","","Rel-13","36.133","13.5.0","LTE_MTCe2_L1-Perf","4261","1","B","RP-162384","","","","",""]
["R4-1610898","CR on modification of cell reselection test case R13","Huawei, HiSilicon","Juha Korhonen","21609","CR","","","","87","6.1.1.3.1","Intra-frequency Cell Re-Selection [LTE_MTCe2_L1-Perf]",66002,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610891","","Rel-13","36.133","13.5.0","LTE_MTCe2_L1-Perf","4279","2","F","RP-162384","","","","",""]
["R4-1610899","LS to RAN1, RAN2 on PBCH demodulation performance","Intel Corporation","Juha Korhonen","21609","LS out","Approval","","","323","8.25.4","Other specifications [LTE_feMTC-Core]",915100011,"revised","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610670","R4-1610970","Rel-14","","","LTE_feMTC-Core","","","","","","RAN1, RAN2","","",""]
["R4-1610900","LS to RAN1, RAN2 on NPBCH demodulation performance","Intel Corporation","Juha Korhonen","21609","LS out","Approval","","","310","8.24.4","Other specifications [NB_IOTenh-Core]",915400002,"revised","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610699","R4-1610972","Rel-14","","","NB_IOTenh-Core","","","","","","","","",""]
["R4-1610901","Simulation assumptions for A-MPR of V2V waveform","Qualcomm","Juha Korhonen","21609","discussion","Approval","","","259","8.19.1","UE RF core maintenace (36.101)  [LTE_SL_V2V-Core]",90100,"revised","2016-11-18T23:00:00","2016-11-18T23:00:00","","R4-1610955","","","","","","","","","","","","",""]
["R4-1610902","Clarifications on some issues for V2X","Huaweii","Juha Korhonen","21609","discussion","Approval","","","272","8.20","LTE based V2X  [LTE_V2X]",90200,"available","2016-11-24T01:33:19.027","2016-11-24T01:37:26.723","","","","","","LTE_V2X-Core","","","","","","","","",""]
["R4-1610903","Corrections to CA table reference and header","Nokia, Alcatel-Lucent Shanghai Bell","Juha Korhonen","21609","CR","","","","12","4.2.1","UE RF (core / EMC)  [WI code or TEI12]",958400001,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609834","","Rel-11","36.101","11.18.0","TEI11","4062","1","F","RP-162413","","","","",""]
["R4-1610904","Corrections of CA Refsens exceptions in 7.3.1A (Rel-12)","Nokia, Alcatel-Lucent Shanghai Bell, Huawei","Juha Korhonen","21609","CR","Approval","","","12","4.2.1","UE RF (core / EMC)  [WI code or TEI12]",965100001,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609904","","Rel-12","36.101","12.13.0","TEI12","4075","1","F","RP-162421","","","","",""]
["R4-1610905","DeltaRIB for SDL CA","Nokia, Alcatel-Lucent Shanghai Bell","Juha Korhonen","21609","CR","Approval","","","12","4.2.1","UE RF (core / EMC)  [WI code or TEI12]",965200001,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609908","","Rel-12","36.101","12.13.0","TEI12","4079","1","F","RP-162421","","","","",""]
["R4-1610906","Clarification on UE maximum output power","CATT","Juha Korhonen","21609","CR","Approval","","","12","4.2.1","UE RF (core / EMC)  [WI code or TEI12]",990800001,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610455","","Rel-13","36.101","13.5.0","TEI13","3875","3","F","RP-162435","","","","",""]
["R4-1610907","Clarification on UE maximum output power","CATT","Juha Korhonen","21609","CR","Approval","","","12","4.2.1","UE RF (core / EMC)  [WI code or TEI12]",995300001,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610456","","Rel-14","36.101","14.1.0","TEI13","3876","2","A","RP-162435","","","","",""]
["R4-1610908","Revision of WID: LTE Advanced inter-band CA Rel-14 for 2DL1UL","Qualcomm Incorporated","Juha Korhonen","21609","WID revised","Endorsement","","","152","8.2.1","Rapporteur Input (WID/CRs) [LTE_CA_R14_2DL1UL-Core]",964200001,"endorsed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609040","","Rel-14","","","LTE_CA_R14_2DL1UL","","","","","","","","",""]
["R4-1610909","Correction UE category applicability","Nokia, Alcatel-Lucent Shanghai Bell","Juha Korhonen","21609","CR","","","","17","4.2.6","Other specifications  [WI code or TEI12]",200001,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610200","","Rel-13","36.307","13.5.0","TEI12","0715","2","A","RP-162421","","","","",""]
["R4-1610910","Correction to UE category applicability","Nokia, Alcatel-Lucent Shanghai Bell","Juha Korhonen","21609","CR","","","","17","4.2.6","Other specifications  [WI code or TEI12]",201001,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610201","","Rel-14","36.307","14.0.0","TEI12","0716","2","A","RP-162421","","","","",""]
["R4-1610911","LTE-based V2X UE receiver requirements","LG Electronics Inc.","Juha Korhonen","21609","pCR","Approval","","","279","8.20.3.2","Rx requirements  [LTE_V2X-Core]",979700001,"noted","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609797","","","36.786","0.1.0","LTE_V2X-Core","","","","","","","","",""]
["R4-1610912","MSD for 1+3+42 2UL/3DL CA","Huawei, Hisilicon","Juha Korhonen","21609","other","Approval","","","183","8.7.2","UE RF (36.101) [LTE_CA_R14_xDL2UL-Core]",997000001,"noted","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609975","","","","","","","","","","","","","",""]
["R4-1610913","WF on eLAA uplink requirements","Ericsson","Juha Korhonen","21609","discussion","Endorsement","","","242","8.18.1","General [LTE_eLAA-Core]",83601,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610836","","","","","","","","","","","","","",""]
["R4-1610914","TR 37.871","Nokia","Juha Korhonen","21609","draft TR","Agreement","","","203","8.11","Multi-Band Base Station testing with three or more bands  [MB_BS_test_3B]",146001,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610745","","Rel-14","37.871","1.3.0","MB_BS_test_3B-Core","","","","","","","","",""]
["R4-1610915","Addition of 1.4 and 3 MHz channel bandwidths for BAND 65 in TS36.101 (Rel-13)","HUGHES Network Systems Ltd","Juha Korhonen","21609","CR","Endorsement","","","70","5.10.2","New spectrum [WI code]",168002,"endorsed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610819","","Rel-13","36.101","13.5.0","","3968","2","B","","","","","",""]
["R4-1610916","Addition of 1.4 and 3 MHz channel bandwidths for BAND 65 in TS36.101 (Rel-14)","HUGHES Network Systems Ltd","Juha Korhonen","21609","CR","Endorsement","","","70","5.10.2","New spectrum [WI code]",905900002,"endorsed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610820","","Rel-14","36.101","14.1.0","","3969","2","B","","","","","",""]
["R4-1610917","Addition of UE category 0 to release independence specification","Nokia","Juha Korhonen","21609","CR","Agreement","","","17","4.2.6","Other specifications  [WI code or TEI12]",91700,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","","","Rel-12","36.307","12.13.0","TEI12","0719","","F","RP-162390","","","","",""]
["R4-1610918","Addition of UE category 0 and M1 to release independence specification","Nokia","Juha Korhonen","21609","CR","Agreement","","","17","4.2.6","Other specifications  [WI code or TEI12]",91800,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","","","Rel-13","36.307","13.5.0","TEI13","0720","","F","RP-162390","","","","",""]
["R4-1610919","Addition of UE category 0 and M1 to release independence specification","Nokia","Juha Korhonen","21609","CR","Agreement","","","17","4.2.6","Other specifications  [WI code or TEI12]",91900,"revised","2016-11-18T23:00:00","2016-11-18T23:00:00","","R4-1611008","Rel-14","36.307","14.0.0","TEI13","0721","","A","","","","","",""]
["R4-1610920","WF on channel bandwidth and transmission bandwidth configuration for NR","DOCOMO Communications Lab.","Juha Korhonen","21609","discussion","Endorsement","","","407","11.1","General   [FS_NR_newRAT]",35500001,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610590","","","","","","","","","","","","","",""]
["R4-1610921","Way forward on in-band requirement for NR","Nokia, Alcatel-Lucent Shanghai Bell","Juha Korhonen","21609","discussion","Endorsement","","","415","11.5.1","Common issues for UE and BS [FS_NR_newRAT]",92410001,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610593","","","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1610922","Way forward on NR spectrum utilization","Huawei, Hisilicon","Juha Korhonen","21609","discussion","Endorsement","","","415","11.5.1","Common issues for UE and BS [FS_NR_newRAT]",96570001,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610626","","","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1610923","Way forward on BS RF requirementss for NR","Nokia","Juha Korhonen","21609","discussion","Endorsement","","","420","11.5.3","BS RF  [FS_NR_newRAT]",40400001,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610619","","","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1610924","Way forward on NR studies on frequency range 6-24 GHz","Orange","Juha Korhonen","21609","discussion","Agreement","","","413","11.4","Co-existence study not related WP5D [FS_NR_newRAT]",2390000,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","","","","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1610925","Way forward on NR UE RF requirements","Qualcomm","Juha Korhonen","21609","discussion","Approval","","","416","11.5.2","UE RF  [FS_NR_newRAT]",62000001,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610620","","","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1610926","Way Forward on NR UE testability","Intel Corporation, CATR","Juha Korhonen","21609","other","Approval","","","419","11.5.2.3","Testability [FS_NR_newRAT]",981800001,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609162","","Rel-14","","","FS_NR_newRAT","","","","","","","","",""]
["R4-1610927","nn","NB-IoT and NR","Juha Korhonen","21609","other","Discussion","","","432","15","Any other business",92700,"reserved","2016-11-24T01:33:33.423",null,"","","","","","","","","","","","","","",""]
["R4-1610928","nn","NB-IoT and NR","Juha Korhonen","21609","other","Discussion","","","432","15","Any other business",92800,"reserved","2016-11-24T01:33:33.643",null,"","","","","","","","","","","","","","",""]
["R4-1610929","nn","NB-IoT and NR","Juha Korhonen","21609","other","Discussion","","","432","15","Any other business",92900,"reserved","2016-11-24T01:33:33.877",null,"","","","","","","","","","","","","","",""]
["R4-1610930","nn","NB-IoT and NR","Juha Korhonen","21609","other","Discussion","","","432","15","Any other business",93000,"reserved","2016-11-24T01:33:34.097",null,"","","","","","","","","","","","","","",""]
["R4-1610931","nn","NB-IoT and NR","Juha Korhonen","21609","other","Discussion","","","432","15","Any other business",93100,"reserved","2016-11-24T01:33:34.313",null,"","","","","","","","","","","","","","",""]
["R4-1610932","nn","NB-IoT and NR","Juha Korhonen","21609","other","Discussion","","","432","15","Any other business",93200,"reserved","2016-11-24T01:33:34.547",null,"","","","","","","","","","","","","","",""]
["R4-1610933","nn","NB-IoT and NR","Juha Korhonen","21609","other","Discussion","","","432","15","Any other business",93300,"reserved","2016-11-24T01:33:34.750",null,"","","","","","","","","","","","","","",""]
["R4-1610934","nn","NB-IoT and NR","Juha Korhonen","21609","other","Discussion","","","432","15","Any other business",93400,"reserved","2016-11-24T01:33:34.967",null,"","","","","","","","","","","","","","",""]
["R4-1610935","nn","NB-IoT and NR","Juha Korhonen","21609","other","Discussion","","","432","15","Any other business",93500,"reserved","2016-11-24T01:33:35.217",null,"","","","","","","","","","","","","","",""]
["R4-1610936","nn","NB-IoT and NR","Juha Korhonen","21609","other","Discussion","","","432","15","Any other business",93600,"reserved","2016-11-24T01:33:35.437",null,"","","","","","","","","","","","","","",""]
["R4-1610937","nn","NB-IoT and NR","Juha Korhonen","21609","other","Discussion","","","432","15","Any other business",93700,"reserved","2016-11-24T01:33:35.687",null,"","","","","","","","","","","","","","",""]
["R4-1610938","nn","NB-IoT and NR","Juha Korhonen","21609","other","Discussion","","","432","15","Any other business",93800,"reserved","2016-11-24T01:33:35.903",null,"","","","","","","","","","","","","","",""]
["R4-1610939","nn","NB-IoT and NR","Juha Korhonen","21609","other","Discussion","","","432","15","Any other business",93900,"reserved","2016-11-24T01:33:36.123",null,"","","","","","","","","","","","","","",""]
["R4-1610940","nn","NB-IoT and NR","Juha Korhonen","21609","other","Discussion","","","432","15","Any other business",94000,"reserved","2016-11-24T01:33:36.357",null,"","","","","","","","","","","","","","",""]
["R4-1610941","nn","NB-IoT and NR","Juha Korhonen","21609","other","Discussion","","","432","15","Any other business",94100,"reserved","2016-11-24T01:33:36.670",null,"","","","","","","","","","","","","","",""]
["R4-1610942","nn","NB-IoT and NR","Juha Korhonen","21609","other","Discussion","","","432","15","Any other business",94200,"reserved","2016-11-24T01:33:36.903",null,"","","","","","","","","","","","","","",""]
["R4-1610943","nn","NB-IoT and NR","Juha Korhonen","21609","other","Discussion","","","432","15","Any other business",94300,"reserved","2016-11-24T01:33:37.183",null,"","","","","","","","","","","","","","",""]
["R4-1610944","nn","NB-IoT and NR","Juha Korhonen","21609","other","Discussion","","","432","15","Any other business",94400,"reserved","2016-11-24T01:33:37.403",null,"","","","","","","","","","","","","","",""]
["R4-1610945","nn","NB-IoT and NR","Juha Korhonen","21609","other","Discussion","","","432","15","Any other business",94500,"reserved","2016-11-24T01:33:37.607",null,"","","","","","","","","","","","","","",""]
["R4-1610946","nn","NB-IoT and NR","Juha Korhonen","21609","other","Discussion","","","432","15","Any other business",94600,"reserved","2016-11-24T01:33:37.823",null,"","","","","","","","","","","","","","",""]
["R4-1610947","The minutes of evening adhoc on multi-node testing","Ericsson","Juha Korhonen","21609","discussion","Endorsement","","","139","7.1.1","General  [FS_LTE_LAA_multinode_test]",94700,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","","","","","","","","","","","","","","",""]
["R4-1610948","Response LS to GCF on MIMO OTA progress","Ericsson","Juha Korhonen","21609","LS out","Discussion","","","222","8.14.1","General [LTE_MIMO_OTA-Core]",94800,"revised","2016-11-18T23:00:00","2016-11-18T23:00:00","","R4-1611000","Rel-14","","","LTE_MIMO_OTA-Core","","","","","","GCF","","",""]
["R4-1610949","CR to TR37.977: RC+CE Channel Model Validation Results","Bluetest, ETS","Juha Korhonen","21609","CR","Approval","","","224","8.14.3","Harmonization [LTE_MIMO_OTA-Core]",992800001,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609340","","Rel-14","37.977","14.1.0","UTRA_LTE_MIMO_OTA-Core","0043","1","F","RP-162436","","","","",""]
["R4-1610950","WF on remaining issues on multi-node testing for LAA","Ericsson","Juha Korhonen","21609","discussion","Agreement","","","139","7.1.1","General  [FS_LTE_LAA_multinode_test]",95000,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","","","","","","FS_LTE_LAA_multinode_test","","","","","","","","",""]
["R4-1610951","WF on NR bands","Huawei, HiSilicon","Juha Korhonen","21609","discussion","Endorsement","","","408","11.2","Spectrum  [FS_NR_newRAT]",980100001,"noted","2016-11-18T23:00:00","2016-11-18T23:00:00","","","","","","","","","","","","","","",""]
["R4-1610952","WF on NR bands","KT","Juha Korhonen","21609","other","Discussion","","","408","11.2","Spectrum  [FS_NR_newRAT]",994600000,"revised","2016-11-18T23:00:00","2016-11-18T23:00:00","","R4-1610992","","","","","","","","","","","","",""]
["R4-1610953","Reply LS to RAN1 on implication of sTTI operation on UL ON/OFF time mask","RAN4","Juha Korhonen","21609","LS out","Approval","","","403","10.1.2","UE RF (36.101) [LTE_sTTIandPT]",950100000,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","","","Rel-15","","","LTE_sTTIandPT","","","","","","RAN1","","","R1-1703277, R1-1703578, R1-1703580, R1-1703581"]
["R4-1610954","TP for TR36.714-01: CA_1A_46A_BC1 operating bands and channel bandwidths","Vodafone","Juha Korhonen","21609","pCR","Approval","","","153","8.2.2","UE RF (36.101) [LTE_CA_R14_2DL1UL-Core]",95400,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","","","","36.714-02-01","0.4.0","LTE_CA_R14_2DL1UL-Core","","","","","","","","",""]
["R4-1610955","Simulation assumptions for A-MPR of V2V waveform","Qualcomm","Juha Korhonen","21609","discussion","Approval","","","259","8.19.1","UE RF core maintenace (36.101)  [LTE_SL_V2V-Core]",90101,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610901","","","","","","","","","","","","","",""]
["R4-1610956","TP on the conclusion of co-existence results for V2V UEs","LGE, Huawei","Juha Korhonen","21609","pCR","Approval","","","276","8.20.2.2","Co-existence study for case 1 and case 2  [LTE_V2X-Core]",75400001,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610754","","","36.786","0.1.0","LTE_V2X-Core","","","","","","","","",""]
["R4-1610957","TP for Tx RF requirements for inter-band E-UTRA_V2X operation and higher power class","CATT","Juha Korhonen","21609","pCR","Approval","","","278","8.20.3.1","Tx requirements  [LTE_V2X-Core]",950400001,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610756","","","36.786","0.1.0","LTE_V2X-Core","","","","","","","","",""]
["R4-1610958","Corrections to CA table reference and header and CA REFSENS table","Nokia, Alcatel-Lucent Shanghai Bell","Juha Korhonen","21609","CR","","","","67","5.10.1.1","RF  [WI code]",3180002,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610815","","Rel-13","36.101","13.5.0","TEI13","4064","2","F","RP-162435","","","","",""]
["R4-1610959","Introduction of new bands for NB-IoT in 36.307","Ericsson","Juha Korhonen","21609","CR","Agreement","","","237","8.17.1","Rapporteur Input [NB_IOT_R14_bands]",167001,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","","","Rel-14","36.307","14.0.0","NB_IOT_R14_bands-Core","0722","","A","RP-162407","","","","",""]
["R4-1610960","Proposal for MPAC alignment pass/fail limits","ROHDE & SCHWARZ","Juha Korhonen","21609","discussion","Approval","","","223","8.14.2","Performance requirements [LTE_MIMO_OTA-Core]",52900001,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609596","","","37.977","","","","","","","","","","",""]
["R4-1610961","Way Forward BS RF requirements impact for shorten TTI feature","Ericsson","Juha Korhonen","21609","discussion","Approval","","","404","10.1.3","BS RF (36.104) [LTE_sTTIandPT]",954200101,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610788","","Rel-15","","","LTE_sTTIandPT","","","","","","","","",""]
["R4-1610962","Revised WID for xDL/UL inter-band CA with x=3,4,5 in Rel-14","LG Electronics Inc.","Juha Korhonen","21609","WID revised","Approval","","","182","8.7.1","Rapporteur Input (WID/CRs) [LTE_CA_R14_xDL2UL-Core]",979400001,"endorsed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609784","","Rel-14","36.714-00-02","","LTE_CA_R14_xDL2UL, LTE_CA_R14_xDL2UL-Core, LTE_CA_R14_xDL2UL-Perf","","","","","","","","",""]
["R4-1610963","CR on interruption requirements in SRS switching","Huawei, HiSilicon","Juha Korhonen","21609","CR","Approval","","","291","8.21.3","RRM core and performance (36.133) [LTE_SRS_switch-Core/Perf]",10900002,"revised","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610861","R4-1610971","Rel-14","36.133","14.1.0","","4293","2","B","","","","","",""]
["R4-1610964","CR:Updates to LAA PDSCH demodulation performance requirements (Rel-13)","Huawei, HiSilicon","Juha Korhonen","21609","CR","Agreement","","","108","6.2.4.2","PDSCH [LTE_LAA-Perf]",942800001,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610642","","Rel-13","36.101","13.5.0","LTE_LAA-Perf","3878","4","F","RP-162386","","","","",""]
["R4-1610965","Clean up and clarification for LAA CSI requirements","Ericsson","Juha Korhonen","21609","CR","Approval","","","110","6.2.5","UE CSI reporting (36.101) [LTE_LAA-Perf]",917400002,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610885","","Rel-13","36.101","13.5.0","LTE_LAA-Perf","3980","3","F","RP-162386","","","","",""]
["R4-1610966","WF on V2X RRM requirement","LG Electronics Inc.","Juha Korhonen","21609","discussion","Approval","","","280","8.20.4","RRM core (36.133) (dedicated, shared, or multi-carrier operations) [LTE_V2X-Core]",72400001,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610693","","","","","","","","","","","","","",""]
["R4-1610967","CR for introducing definition of Type-D receiver","NTT DOCOMO INC.","Juha Korhonen","21609","CR","Approval","","","345","8.28.3.1","Enhancement for bi-directional RRH arrangement [LTE_high_speed]",4070002,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610713","","Rel-14","36.101","14.1.0","LTE_high_speed-Perf","4082","2","B","RP-162388","","","","",""]
["R4-1610968","WF on HST unidirectional test","Ericsson, Vodafone, Telecom Italia, NTT DOCOMO","Juha Korhonen","21609","discussion","Endorsement","","","346","8.28.3.2","Unidirectional RRH arrangement [LTE_high_speed]",85901,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610859","","","","","LTE_high_speed","","","","","","","","",""]
["R4-1610969","Simulation assumptions for enhanced SU-MIMO demodulation requiremetns","Huawei, HiSilicon","Juha Korhonen","21609","other","Approval","","","370","8.31.3.1","Performance evaluation: scenarios and receiver [LTE_eCRSIM_eSUMIMO]",70000002,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610715","","","","","","","","","","","","","",""]
["R4-1610970","LS to RAN1, RAN2 on FeMTC SI acquisition delay","Intel Corporation","Juha Korhonen","21609","LS out","Approval","","","323","8.25.4","Other specifications [LTE_feMTC-Core]",915100012,"revised","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610899","R4-1611001","Rel-14","","","LTE_feMTC-Core","","","","","","RAN1, RAN2","","",""]
["R4-1610971","CR on interruption requirements in SRS switching","Huawei, HiSilicon","Juha Korhonen","21609","CR","Approval","","","291","8.21.3","RRM core and performance (36.133) [LTE_SRS_switch-Core/Perf]",10900003,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610963","","Rel-14","36.133","14.1.0","LTE_SRS_switch","4293","3","B","RP-162392","","","","",""]
["R4-1610972","LS to RAN1, RAN2 on eNB-IoT SI acquisition delay","Intel Corporation","Juha Korhonen","21609","LS out","Approval","","","310","8.24.4","Other specifications [NB_IOTenh-Core]",915400003,"revised","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610900","R4-1611002","Rel-14","","","NB_IOTenh-Core","","","","","","RAN1, RAN2","","",""]
["R4-1610973","nn","RRM","Juha Korhonen","21609","other","Discussion","","","432","15","Any other business",97300,"reserved","2016-11-24T01:33:47.167",null,"","","","","","","","","","","","","","",""]
["R4-1610974","nn","RRM","Juha Korhonen","21609","other","Discussion","","","432","15","Any other business",97400,"reserved","2016-11-24T01:33:47.387",null,"","","","","","","","","","","","","","",""]
["R4-1610975","nn","RRM","Juha Korhonen","21609","other","Discussion","","","432","15","Any other business",97500,"reserved","2016-11-24T01:33:47.603",null,"","","","","","","","","","","","","","",""]
["R4-1610976","nn","RRM","Juha Korhonen","21609","other","Discussion","","","432","15","Any other business",97600,"reserved","2016-11-24T01:33:47.837",null,"","","","","","","","","","","","","","",""]
["R4-1610977","nn","RRM","Juha Korhonen","21609","other","Discussion","","","432","15","Any other business",97700,"reserved","2016-11-24T01:33:48.073",null,"","","","","","","","","","","","","","",""]
["R4-1610978","nn","RRM","Juha Korhonen","21609","other","Discussion","","","432","15","Any other business",97800,"reserved","2016-11-24T01:33:48.290",null,"","","","","","","","","","","","","","",""]
["R4-1610979","nn","RRM","Juha Korhonen","21609","other","Discussion","","","432","15","Any other business",97900,"reserved","2016-11-24T01:33:48.510",null,"","","","","","","","","","","","","","",""]
["R4-1610980","nn","RRM","Juha Korhonen","21609","other","Discussion","","","432","15","Any other business",98000,"reserved","2016-11-24T01:33:48.727",null,"","","","","","","","","","","","","","",""]
["R4-1610981","nn","RRM","Juha Korhonen","21609","other","Discussion","","","432","15","Any other business",98100,"reserved","2016-11-24T01:33:48.947",null,"","","","","","","","","","","","","","",""]
["R4-1610982","nn","RRM","Juha Korhonen","21609","other","Discussion","","","432","15","Any other business",98200,"reserved","2016-11-24T01:33:49.180",null,"","","","","","","","","","","","","","",""]
["R4-1610983","WF on BCS for CA 3A_28A","NTT DOCOMO","Juha Korhonen","21609","discussion","Approval","","","176","8.6.1","Rapporteur Input (WID/CRs) [LTE_CA_R14_2DL2UL-Core]",940100000,"revised","2016-11-18T23:00:00","2016-11-18T23:00:00","","R4-1610988","","","","LTE_CA_R14_2DL2UL-Core","","","","","","","","",""]
["R4-1610984","Sets of EARFCN for multiple Scell operation in Band 46","Ericsson","Juha Korhonen","21609","CR","Approval","","","248","8.18.3","BS RF (36.104) [LTE_eLAA-Core]",1380001,"agreed","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610138","","Rel-14","36.104","14.1.0","LTE_eLAA-Core","0902","1","F","RP-162387","","","","",""]
["R4-1610985","TP for TR 36.789 v0.0.2: Updates in throughput tests procedures","Ericsson","Juha Korhonen","21609","pCR","Approval","","","141","7.1.2.1","Throughput Test [FS_LTE_LAA_multinode_test]",4630001,"withdrawn","2016-11-24T01:33:50.070",null,"R4-1610463","","","36.789","0.0.1","FS_LTE_LAA_multinode_test","","","","","","","","",""]
["R4-1610986","LS on Reduced Power Class for eNB-IoT","RAN2","Juha Korhonen","21609","LS in","Action","","","2","3","Letters / reports from other groups / meetings",98600,"available","2016-11-24T01:33:50.350","2016-11-24T01:37:26.800","","","","","","NB_IOTenh-Core","","","","","","RAN4","RAN1","R2-169110",""]
["R4-1610987","Lab alignment test plan","Intel Corporation","Juha Korhonen","21609","other","Approval","","","223","8.14.2","Performance requirements [LTE_MIMO_OTA-Core]",51100001,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610786","","Rel-14","","","LTE_MIMO_OTA-Core","","","","","","","","",""]
["R4-1610988","WF on BCS for CA 3A_28A","NTT DOCOMO","Juha Korhonen","21609","discussion","Approval","","","176","8.6.1","Rapporteur Input (WID/CRs) [LTE_CA_R14_2DL2UL-Core]",940100001,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610983","","","","","LTE_CA_R14_2DL2UL-Core","","","","","","","","",""]
["R4-1610989","WF on the measurement grid for ACLR","Ericsson, NTT DOCOMO, Huawei","Juha Korhonen","21609","discussion","Approval","","","209","8.12.2.1","In band requirements [AASenh_BS_LTE_UTRA]",4980001,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610804","","","","","AASenh_BS_LTE_UTRA","","","","","","","","",""]
["R4-1610990","Way Forward: Further working assumptions and agreements on eLAA Tx requirements","Ericsson, Skyworks","Juha Korhonen","21609","discussion","Approval","","","208","8.12.2","Core Requirements [AASenh_BS_LTE_UTRA]",99000,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","","","","","","AASenh_BS_LTE_UTRA","","","","","","","","",""]
["R4-1610991","LS Reply on UL256QAM capability","Qualcomm Incorporated","Juha Korhonen","21609","LS out","Approval","","","226","8.15.1","UE capability for UL256QAM  [LTE_UL_CAP_enh-Core]",964400001,"revised","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1609643","R4-1610993","Rel-14","","","LTE_UL_CAP_enh","","","","","R4-163125","TSG RAN WG1, TSG RAN WG2","","R1-163915",""]
["R4-1610992","WF on NR bands","KT","Juha Korhonen","21609","other","Discussion","","","408","11.2","Spectrum  [FS_NR_newRAT]",994700000,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610952","","","","","","","","","","","","","",""]
["R4-1610993","LS reply on UE/band specific support of UL 256QAM","RAN4","Juha Korhonen","21609","LS out","Approval","","","226","8.15.1","UE capability for UL256QAM  [LTE_UL_CAP_enh-Core]",964400002,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610991","","Rel-14","","","LTE_UL_CAP_enh-Core","","","","","R1-163463","RAN1, RAN2","","R1-163915",""]
["R4-1610994","LS on Suitability of technical conditions of ECC DEC (11) 06 for 5G","RAN4","Juha Korhonen","21609","LS out","Agreement","","","407","11.1","General   [FS_NR_newRAT]",965900000,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610592","","Rel-14","","","FS_NR_newRAT","","","","","R4-1609013","ECC PT1","ETSI ERM","",""]
["R4-1610995","LS on RSRQ measurement for cell reselection","RAN4","Juha Korhonen","21609","LS out","Approval","","","50","5.5.3.3","Measurement requirement [LTE_MTCe2_L1-Core]",52000,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610657","","Rel-13","","","LTE_MTCe2_L1-Core","","","","","","RAN2","","",""]
["R4-1610996","LS response on FeMTC VoLTE enhancements","RAN4","Juha Korhonen","21609","LS out","Approval","","","312","8.25.1","General [LTE_feMTC-Core]",2150010,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610666","","Rel-14","","","LTE_feMTC-Core","","","","","","RAN1","RAN2","",""]
["R4-1610997","LS on measurement gap enhancement","RAN4","Juha Korhonen","21609","LS out","Approval","","","351","8.29.2","RRM core (36.133) [LTE_meas_gap_enh-Core]",954600000,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610690","","Rel-14","","","LTE_meas_gap_enh-Core","","","","","","RAN2","RAN1","",""]
["R4-1610998","LS on handling co-existence requirements with CEN DSRC","RAN4","Juha Korhonen","21609","LS out","Approval","","","259","8.19.1","UE RF core maintenace (36.101)  [LTE_SL_V2V-Core]",93710000,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610746","","Rel-14","","","LTE_SL_V2V-Core","","","","","","RAN2","RAN1","","R2-1702065, R2-1702075"]
["R4-1610999","LS on Measurement gap enhancement","RAN4","Juha Korhonen","21609","LS out","Approval","","","351","8.29.2","RRM core (36.133) [LTE_meas_gap_enh-Core]",954700001,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610888","","Rel-14","","","LTE_meas_gap_enh-Core","","","","","R2-167317","RAN2","RAN1","",""]
["R4-1611000","Response LS to GCF on MIMO OTA progress","RAN4","Juha Korhonen","21609","LS out","Approval","","","222","8.14.1","General [LTE_MIMO_OTA-Core]",0,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610948","","Rel-14","","","LTE_MIMO_OTA-Core","","","","","","GCF CAG, GCF PAG","CTIA MOSG","",""]
["R4-1611001","LS to RAN1, RAN2 on FeMTC SI acquisition delay","RAN4","Juha Korhonen","21609","LS out","Approval","","","323","8.25.4","Other specifications [LTE_feMTC-Core]",915100012,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610970","","Rel-14","","","LTE_feMTC-Core","","","","","","RAN1, RAN2","","","R1-1703960, R1-1704067"]
["R4-1611002","LS to RAN1, RAN2 on eNB-IoT SI acquisition delay","RAN4","Juha Korhonen","21609","LS out","Approval","","","310","8.24.4","Other specifications [NB_IOTenh-Core]",915400003,"approved","2016-11-18T23:00:00","2016-11-18T23:00:00","R4-1610972","","Rel-14","","","NB_IOTenh-Core","","","","","","RAN1, RAN2","","","R1-1703961, R1-1704068"]
["R4-1611003","Introduction of new bands for NB-IoT in 36.133","Ericsson","Juha Korhonen","21609","CR","Approval","In tis CR we introduce new bands for Rel-14 NB-IoT in 36.133","","240","8.17.4","Other specifications [NB_IOT_R14_bands]",0,"agreed","2016-12-03T03:45:20.277","2016-12-03T03:47:27.900","R4-167900","","Rel-14","36.133","14.1.0","NB_IOT_R14_bands-Core","4064","1","B","RP-162407","","","","",""]
["R4-1611004","Corrections on DC interruption test cases R13","Huawei, HiSilicon","Juha Korhonen","21609","CR","Approval","Endorsed CR in R4-167758","","14","4.2.3","RRM (Radio Resource Management)  [WI code or TEI12]",0,"agreed","2016-12-03T03:52:14.567","2016-12-03T03:57:27.673","R4-1610090","","Rel-13","36.133","13.5.0","TEI12","4287","1","A","RP-162421","","","","",""]
["R4-1611005","CR for correction on OCNG pattern (Rel-14)","Huawei, HiSilicon","Juha Korhonen","21609","CR","Agreement","This is the revision of agreed R4-167627 in RAN4#80bis with coversheet updates to the clauses affected empty","","15","4.2.4","UE demodulation performance  [WI code or TEI12]",0,"agreed","2016-12-03T03:55:45.460","2016-12-03T03:57:27.720","R4-1610136","","Rel-14","36.101","14.1.0","TEI13","3887","2","A","RP-162435","","","","",""]
["R4-1611006","Modification to Handover Delay in CE ModeA","Qualcomm Incorporated","Juha Korhonen","21609","CR","Approval","Cover page correction. Category changed to A.","","48","5.5.3.1","Evaluation of MIB and SIB reading delay, and update of requirement for handover and RRC Re-establishment [LTE_MTCe2_L1-Core]",0,"agreed","2016-12-03T03:57:33.007","2016-12-03T04:07:27.850","R4-1610415","","Rel-14","36.133","14.1.0","LTE_MTCe2_L1-Core","4104","2","A","RP-162430","","","","",""]
["R4-1611007","PC accuracy in SRS carrier based switching in UE core spec","Ericsson","Juha Korhonen","21609","CR","Approval","Introducing SRS carrier based switching in 36.101. In Section 6.3.5, absolute power tolerance value has been changed when SRS carrier based swithcing is used.","","290","8.21.2","UE RF (36.101) [LTE_SRS_switch-Core]",0,"agreed","2016-12-03T03:59:15.110","2016-12-03T04:07:27.897","R4-1610468","","Rel-14","36.101","14.1.0","LTE_SRS_switch-Core","4128","1","B","RP-162392","","","","",""]
["R4-1611008","Addition of UE category 0 and M1 to release independence specification","Nokia","Juha Korhonen","21609","CR","Agreement","","","17","4.2.6","Other specifications  [WI code or TEI12]",0,"agreed","2016-12-03T04:00:57.383","2016-12-03T04:07:27.897","R4-1610919","","Rel-14","36.307","14.0.0","TEI13","0721","1","A","RP-162390","","","","",""]
["R4-1611009","CR for 36.113: Introduction of NB-IoT","Huawei","Juha Korhonen","21609","CR","Agreement","---","","113","6.3.2","BS RF conformance testing (36.141) [NB_IOT-Perf]",0,"agreed","2016-12-03T04:02:20.890","2016-12-03T04:07:27.913","R4-1609391","","Rel-14","36.113","14.0.0","NB_IOT-Perf","0062","1","A","RP-162381","","","","",""]
["R4-1611010","Removal of square brackets from MBS measurement accuracy requirements","NextNav, AT&T, Broadcom","Juha Korhonen","21609","CR","Agreement","Category F CR. Removes the square brackets from the MBS Measurement accuracy requirements","","63","5.9.2","RRM [WI code or TEI13]",0,"revised","2016-12-03T04:03:35.490","2016-12-03T04:07:27.913","R4-1609058","R4-1611023","Rel-13","37.171","13.0.0","UTRA_LTE_iPos_enh-Perf","0001","1","F","","","","","",""]
["R4-1611011","CR on 4-RX TM9 MU test","Intel Corporation","Juha Korhonen","21609","CR","Agreement","","","33","5.2.3.2","UE demodulation and CSI [LTE_4Rx_AP_DL-Perf]",0,"agreed","2016-12-03T04:04:47.077","2016-12-03T04:07:27.913","R4-1610686","","Rel-13","36.101","13.5.0","LTE_4Rx_AP_DL-Perf","3970","2","F","RP-162423","","","","",""]
["R4-1611012","CR on 4-RX TM9 MU test","Intel Corporation","Juha Korhonen","21609","CR","Agreement","","","33","5.2.3.2","UE demodulation and CSI [LTE_4Rx_AP_DL-Perf]",0,"agreed","2016-12-03T04:05:44.173","2016-12-03T04:07:27.913","R4-1610687","","Rel-14","36.101","14.1.0","LTE_4Rx_AP_DL-Perf","3971","2","A","RP-162423","","","","",""]
["R4-1611013","CR: NPRACH performance requirements (Rel-13, TS36.141)","Nokia, Alcatel-Lucent Shanghai Bell","Juha Korhonen","21609","CR","Approval","","","133","6.3.4.2.1","NPRACH  [NB_IOT-Perf]",0,"agreed","2016-12-03T04:13:14.733","2016-12-03T04:17:27","R4-1610561","","Rel-13","36.104","13.5.0","NB_IOT-Perf","0885","2","B","RP-162381","","","","",""]
["R4-1611014","Power Allocation in Uplink Multicarrier scenarios for UMTS including 10ms TTI and Mixed TTI configurations","Ericsson","Juha Korhonen","21609","CR","Approval","CR for 25.133 from WI on multicarrier enhancements including introduction of 10ms TTI and mixed 2/10ms TTI scenarios","","375","8.32.3","RRM  [WI code or TEI14]",0,"agreed","2016-12-03T04:14:16.353","2016-12-03T04:17:27.047","R4-1609556","","Rel-14","25.133","14.0.0","UTRA_MCe","1428","1","F","RP-162410","","","","",""]
["R4-1611015","CR for fixing editorial errors in Rel-14","Ericsson","Juha Korhonen","21609","CR","Approval","CR","","15","4.2.4","UE demodulation performance  [WI code or TEI12]",0,"agreed","2016-12-03T04:15:18.957","2016-12-03T04:17:27.063","R4-1609995","","Rel-14","36.101","14.1.0","TEI13","4087","1","A","RP-162435","","","","",""]
["R4-1611016","Clean up and clarification for LAA CSI requirements","Ericsson","Juha Korhonen","21609","CR","Approval","clean up and make some clarification for LAA CSI requirements","","110","6.2.5","UE CSI reporting (36.101) [LTE_LAA-Perf]",0,"agreed","2016-12-03T04:18:14.190","2016-12-03T04:27:25.917","R4-1609171","","Rel-14","36.101","14.1.0","LTE_LAA-Perf","3981","1","A","RP-162386","","","","",""]
["R4-1611017","Finalizing UE-selected subband CQI test for eMTC","Ericsson","Juha Korhonen","21609","CR","Approval","This CR finalizes the UE-selected subband CQI test for eMTC.","","100","6.1.3","UE CSI reporting (36.101) [LTE_MTCe2_L1-Perf]",0,"agreed","2016-12-03T04:21:14.823","2016-12-03T04:27:25.963","R4-1609692","","Rel-14","36.101","14.1.0","LTE_MTCe2_L1-Perf","4046","1","A","RP-162384","","","","",""]
["R4-1611018","CR for fixing soft buffer management test for TDD-FDD CA in Rel-14","Ericsson","Juha Korhonen","21609","CR","Approval","CR","","15","4.2.4","UE demodulation performance  [WI code or TEI12]",0,"agreed","2016-12-03T04:22:14.167","2016-12-03T04:27:25.963","R4-1609993","","Rel-14","36.101","14.1.0","TEI12","4085","1","A","RP-162421","","","","",""]
["R4-1611019","MSD and exclusion region specification for 10MHz LAA channels","Qualcomm Incorporated","Juha Korhonen","21609","CR","Agreement","CR to implement MSD and exclusion region requirements for 10MHz LAA channels","","40","5.4.1","UE RF and EMC [LTE_LAA-Core]",0,"agreed","2016-12-03T04:23:44.647","2016-12-03T04:27:25.977","R4-1610451","","Rel-13","36.101","13.5.0","LTE_LAA-Core","4125","1","F","RP-162428","","","","",""]
["R4-1611020","MSD and exclusion region specification for 10MHz LAA channels","Qualcomm Incorporated","Juha Korhonen","21609","CR","Agreement","CR to implement MSD and exclusion region requirements for 10MHz LAA channels","","40","5.4.1","UE RF and EMC [LTE_LAA-Core]",0,"agreed","2016-12-03T04:25:06.997","2016-12-03T04:27:25.977","R4-1610452","","Rel-14","36.101","14.1.0","LTE_LAA-Core","4126","1","F","RP-162428","","","","",""]
["R4-1611021","Introducing agreed measurement accuracy for NB IoT","Nokia, Alcatel-Lucent Shanghai Bell","Juha Korhonen","21609","CR","Approval","","","117","6.3.3","RRM (36.133) [NB_IOT-Perf]",0,"agreed","2016-12-03T04:25:57.447","2016-12-03T04:27:25.977","R4-1610551","","Rel-14","36.133","14.1.0","NB_IOT-Perf","4210","2","A","RP-162381","","","","",""]
["R4-1611022","UE Tranmsit timing accuracy in CE mode B","Qualcomm, Intel, Huawei, HiSilicon","Juha Korhonen","21609","CR","Approval","","","49","5.5.3.2","UE transmit timing [LTE_MTCe2_L1-Core]",0,"agreed","2016-12-03T04:27:39.707","2016-12-03T04:37:26.593","R4-1610656","","Rel-13","36.133","13.5.0","LTE_MTCe2_L1-Core","4156","4","F","RP-162430","","","","",""]
["R4-1611023","Removal of square brackets from MBS measurement accuracy requirements","NextNav, AT&T, Broadcom","Juha Korhonen","21609","CR","Agreement","Category F CR. Removes the square brackets from the MBS Measurement accuracy requirements","","63","5.9.2","RRM [WI code or TEI13]",0,"agreed","2016-12-03T04:28:43.573","2016-12-03T04:37:26.640","R4-1611010","","Rel-13","37.171","13.0.0","UTRA_LTE_iPos_enh-Perf","0001","2","F","RP-162396","","","","",""]
["R4-1611024","Correction to dynamic range requirement","Nokia, Alcatel-Lucent Shanghai Bell","Juha Korhonen","21609","CR","Approval","---","","13","4.2.2","BS and Repeater RF (core / conformance / EMC)  [WI code or TEI12]",0,"agreed","2016-12-03T04:30:37.390","2016-12-03T04:47:05.620","R4-1610311","","Rel-10","36.104","10.11.0","TEI8","0910","1","A","RP-162411","","","","",""]
["R4-1611025","Corrections to CA table reference and header","Nokia, Alcatel-Lucent Shanghai Bell","Juha Korhonen","21609","CR","","---","","12","4.2.1","UE RF (core / EMC)  [WI code or TEI12]",0,"agreed","2016-12-03T04:32:22.177","2016-12-03T04:47:05.620","R4-1609835","","Rel-12","36.101","12.13.0","TEI11","4063","1","A","RP-162413","","","","",""]
["R4-1611026","Correction to dynamic range requirement","Nokia, Alcatel-Lucent Shanghai Bell","Juha Korhonen","21609","CR","Approval","---","","13","4.2.2","BS and Repeater RF (core / conformance / EMC)  [WI code or TEI12]",0,"agreed","2016-12-03T04:33:53.497","2016-12-03T04:47:05.637","R4-1610313","","Rel-12","36.104","12.11.0","TEI11","0912","1","A","RP-162413","","","","",""]
["R4-1611027","Correction to dynamic range requirement","Nokia, Alcatel-Lucent Shanghai Bell","Juha Korhonen","21609","CR","Approval","---","","13","4.2.2","BS and Repeater RF (core / conformance / EMC)  [WI code or TEI12]",0,"agreed","2016-12-03T04:35:22.607","2016-12-03T04:47:05.637","R4-1610314","","Rel-13","36.104","13.5.0","TEI11","0913","1","A","RP-162413","","","","",""]
["R4-1611028","Correction to dynamic range requirement","Nokia, Alcatel-Lucent Shanghai Bell","Juha Korhonen","21609","CR","Approval","---","","13","4.2.2","BS and Repeater RF (core / conformance / EMC)  [WI code or TEI12]",0,"agreed","2016-12-03T04:36:36.940","2016-12-03T04:47:05.637","R4-1610315","","Rel-14","36.104","14.1.0","TEI11","0914","1","A","RP-162413","","","","",""]
["R4-1611029","Correction to dynamic range requirement","Nokia, Alcatel-Lucent Shanghai Bell","Juha Korhonen","21609","CR","Approval","---","","13","4.2.2","BS and Repeater RF (core / conformance / EMC)  [WI code or TEI12]",0,"agreed","2016-12-03T04:44:19.090","2016-12-03T04:47:05.637","R4-1610310","","Rel-9","36.104","9.13.0","TEI8","0909","1","F","RP-162411","","","","",""]
["R4-1611030","DeltaRIB for SDL and LAA CA","Nokia, Alcatel-Lucent Shanghai Bell","Juha Korhonen","21609","CR","Approval","","","67","5.10.1.1","RF  [WI code]",0,"agreed","2016-12-03T04:46:06.760","2016-12-03T04:47:05.637","R4-1610818","","Rel-13","36.101","13.5.0","TEI13","4080","2","F","RP-162435","","","","",""]

{"sheet":"CR_Packs_List","index":1,"n_rows":1,"n_cols":11,"rows_kept":1,"cut":false,"hidden":false,"merged":[]}
["CR Pack TDoc","WG Tdoc","WG TDoc decision","CR Individual TSG decision","Spec","CR","CR revision","CR category","Release","Version","CR title"]

{"sheet":"Parameters","index":2,"n_rows":25,"n_cols":4,"rows_kept":25,"cut":false,"hidden":true,"merged":[]}
["Types of Tdocs","Possible statuses of Tdocs","Categories"]
[]
["agenda","reserved","A","Decision"]
["Work Plan","available","B","Agreement"]
["LS in","revised","C","Approval"]
["LS out","agreed","D","Information"]
["pCR","conditionally agreed","E","Discussion"]
["draftCR","approved","F","Action"]
["CR","conditionally approved",null,"Endorsement"]
["CR pack","partially approved",null,"Presentation"]
["ToR","treated"]
["WID new","endorsed"]
["WID revised","replied to"]
["SID new","merged"]
["SID revised","not pursued"]
["WI status report","postponed"]
["WI exception request","noted"]
["TS or TR cover","not concluded"]
["draft TS","withdrawn"]
["draft TR","reissued"]
["report","not treated"]
["discussion"]
["response"]
["other"]
["WI summary"]