**3GPP TSG-RAN WG4 Meeting #94-e R4-****2002202**

**E-meeting, February 24th – March 6th, 2020**

**Title: LS on UE reporting criteria**

**Response to:** -

**Release:** Release 15

**Work Item:** NR\_newRAT-Core

**Source:** Nokia (TSG RAN WG4)

**To:** TSG RAN WG2

**Cc:**

**Contact Person:**

#### Name: Lars Dalsgaard

E-mail Address: [lars.dalsgaard@nokia.com](mailto:lars.dalsgaard@nokia.com)

**Send any reply LS to: 3GPP Liaisons Coordinator,** [**mailto:3GPPLiaison@etsi.org**](mailto:3GPPLiaison@etsi.org)

**Attachments:** -

**1. Overall Description:**

RAN4 thanks RAN2 for the LS R2-1916595 LS on measurement reporting criteria for EN-DC in which RAN2 asks RAN4 following:

Question 1: RAN2 asks RAN4 to confirm whether the changes to UE capabilities for measurements reporting criteria in [R4-1907862](https://portal.3gpp.org/ngppapp/CreateTdoc.aspx?mode=view&contributionUid=R4-1907862) imply that the component in needs to be coordinated between the MN and the SN.

RAN4 has been discussing the question raised in the LS and has concluded that regarding question 1:

* there is a need to exchange information between MN and SN related to configurations impacting the component in ., which follows from that in TS 38.133 is the *total* number of NR reporting criteria configured by PSCell and E-UTRA PCell,
* the above was implied by the existing TS 38.133 and TS 36.133 specifications even before the CR in R4-1907862, rather this approach had been already in both TS 38.133 and TS 36.133.

**2. Actions:**

**To RAN2 group.**

**ACTION:** RAN4 respectfully asks RAN2 to take above into consideration.

**3. Date of Next TSG-RAN WG4 Meetings:**

3GPP RAN4#94bis 20 – 24 Apr 2020 Canada

3GPP RAN4#95 25 – 29 May 2020 Athens