MSG #337 2021-10-26 11:15:14.415

    enobeB PCAP frame

    {
      "layers": {
        "frame": {
          "frame.encap_type": "45",
          "frame.time": "Oct 26, 2021 11:15:14.415227000 CEST",
          "frame.offset_shift": "0.000000000",
          "frame.time_epoch": "1635239714.415227000",
          "frame.time_delta": "0.004981000",
          "frame.time_delta_displayed": "0.008001000",
          "frame.time_relative": "127.175126000",
          "frame.number": "11598",
          "frame.len": "66",
          "frame.cap_len": "66",
          "frame.marked": "0",
          "frame.ignored": "0",
          "frame.protocols": "user_dlt:mac-lte-framed:mac-lte:rlc-lte:pdcp-lte:ip:tcp"
        },
        "user_dlt": "DLT: 147, Payload: mac-lte-framed (mac-lte-framed)",
        "mac-lte": {
          "mac-lte.context": "",
          "mac-lte.context_tree": {
            "mac-lte.radio-type": "1",
            "mac-lte.direction": "0",
            "mac-lte.ueid": "19",
            "mac-lte.sfn": "421",
            "mac-lte.subframe": "6",
            "mac-lte.rnti": "79",
            "mac-lte.rnti-type": "3",
            "mac-lte.is-predefined-frame": "0",
            "mac-lte.length": "41",
            "mac-lte.ul-grant-size": "41",
            "mac-lte.crc-status": "1",
            "mac-lte.carrier-id": "0",
            "mac-lte.ul-tti-count": "1"
          },
          "mac-lte.ul-phy": "",
          "mac-lte.ul-phy_tree": {
            "mac-lte.ul-phy.modulation-type": "4",
            "mac-lte.ul-phy.tbs-index": "16",
            "mac-lte.ul-phy.resource-block-length": "1",
            "mac-lte.ul-phy.resource-block-start": "7",
            "mac-lte.ul-phy.harq-id": "0",
            "mac-lte.ul-phy.ndi": "1"
          },
          "mac-lte.ulsch.header": "",
          "mac-lte.ulsch.header_tree": {
            "mac-lte.sch.subheader": "",
            "mac-lte.sch.subheader_tree": {
              "mac-lte.sch.reserved": "0x00000000",
              "mac-lte.sch.format2": "0",
              "mac-lte.sch.extended": "0x00000000",
              "mac-lte.ulsch.lcid": "0x0000001f"
            }
          },
          "mac-lte.control.bsr": "",
          "mac-lte.control.bsr_tree": {
            "mac-lte.control.bsr.buffer-size-0": "0",
            "mac-lte.control.bsr.buffer-size-1": "0",
            "mac-lte.control.bsr.buffer-size-2": "0",
            "mac-lte.control.bsr.buffer-size-3": "0"
          },
          "mac-lte.sch.header-only": "0",
          "mac-lte.sch.sdu": "b0:77:64:f3:71:e9:3a:d2:05:7c:1c:57:ea:5d:b8:4d:d0:87:02:f7",
          "rlc-lte": {
            "rlc-lte.context": "",
            "rlc-lte.context_tree": {
              "rlc-lte.direction": "0",
              "rlc-lte.mode": "4",
              "rlc-lte.ueid": "19",
              "rlc-lte.priority": "4",
              "rlc-lte.channel-type": "5",
              "rlc-lte.channel-id": "1",
              "rlc-lte.pdu-length": "20",
              "rlc-lte.am-seqnum-length": "10"
            },
            "rlc-lte.am": "",
            "rlc-lte.am.header": "",
            "rlc-lte.am.header_tree": {
              "rlc-lte.am.frame-type": "0x00000001",
              "rlc-lte.am.rf": "0x00000000",
              "rlc-lte.am.p": "0x00000001",
              "rlc-lte.am.fi": "0x00000002",
              "rlc-lte.am.fixed.e": "0x00000000",
              "rlc-lte.am.fixed.sn": "119"
            },
            "rlc-lte.sequence-analysis": "",
            "rlc-lte.sequence-analysis_tree": {
              "rlc-lte.sequence-analysis.previous-frame": "11596",
              "rlc-lte.sequence-analysis.ok": "1"
            },
            "rlc-lte.am.data": "64:f3:71:e9:3a:d2:05:7c:1c:57:ea:5d:b8:4d:d0:87:02:f7",
            "rlc-lte.reassembly-info": "",
            "rlc-lte.reassembly-info_tree": {
              "rlc-lte.reassembly-info.number-of-segments": "2",
              "rlc-lte.reassembly-info.total-length": "62",
              "rlc-lte.reassembly-info.segment": {
                "rlc-lte.reassembly-info.segment.sn": "119",
                "rlc-lte.reassembly-info.segment.frame": "11598",
                "rlc-lte.reassembly-info.segment.length": "18"
              }
            },
            "pdcp-lte": {
              "pdcp-lte.configuration": "",
              "pdcp-lte.configuration_tree": {
                "pdcp-lte.direction": "0",
                "pdcp-lte.plane": "2",
                "pdcp-lte.ueid": "19",
                "pdcp-lte.channel-type": "1",
                "pdcp-lte.channel-id": "1",
                "pdcp-lte.no-header_pdu": "0",
                "pdcp-lte.seqnum_length": "12",
                "pdcp-lte.rohc.compression": "0"
              },
              "pdcp-lte.security-config": "",
              "pdcp-lte.security-config_tree": {
                "pdcp-lte.security-config.setup-frame": "8363",
                "pdcp-lte.security-config.ciphering": "2",
                "pdcp-lte.security-config.integrity": "2",
                "pdcp-lte.security-config.bearer": "0",
                "pdcp-lte.security-config.direction": "0",
                "pdcp-lte.security-config.count": "122",
                "pdcp-lte.security-config.cipher-key": "fa4c5985ff6d3c3cc5fd92f66d6ad62d"
              },
              "pdcp-lte.pdu-type": "1",
              "pdcp-lte.reserved3": "0x00000000",
              "pdcp-lte.seq-num": "122",
              "pdcp-lte.sequence-analysis": "",
              "pdcp-lte.sequence-analysis_tree": {
                "pdcp-lte.sequence-analysis.previous-frame": "11596",
                "pdcp-lte.sequence-analysis.expected-sn": "122",
                "pdcp-lte.sequence-analysis.ok": "1"
              },
              "ip": {
                "ip.version": "4",
                "ip.hdr_len": "20",
                "ip.dsfield": "0x00000000",
                "ip.dsfield_tree": {
                  "ip.dsfield.dscp": "0",
                  "ip.dsfield.ecn": "0"
                },
                "ip.len": "60",
                "ip.id": "0x0000345e",
                "ip.flags": "0x00000040",
                "ip.flags_tree": {
                  "ip.flags.rb": "0",
                  "ip.flags.df": "1",
                  "ip.flags.mf": "0"
                },
                "ip.frag_offset": "0",
                "ip.ttl": "64",
                "ip.proto": "6",
                "ip.checksum": "0x00008008",
                "ip.checksum.status": "2",
                "ip.src": "192.168.3.2",
                "ip.addr": "192.168.2.3",
                "ip.src_host": "192.168.3.2",
                "ip.host": "192.168.2.3",
                "ip.dst": "192.168.2.3",
                "ip.dst_host": "192.168.2.3"
              },
              "tcp": {
                "tcp.srcport": "39370",
                "tcp.dstport": "8100",
                "tcp.port": "8100",
                "tcp.stream": "9",
                "tcp.len": "0",
                "tcp.seq": "0",
                "tcp.seq_raw": "3532954569",
                "tcp.nxtseq": "1",
                "tcp.ack": "0",
                "tcp.ack_raw": "0",
                "tcp.hdr_len": "40",
                "tcp.flags": "0x00000002",
                "tcp.flags_tree": {
                  "tcp.flags.res": "0",
                  "tcp.flags.ns": "0",
                  "tcp.flags.cwr": "0",
                  "tcp.flags.ecn": "0",
                  "tcp.flags.urg": "0",
                  "tcp.flags.ack": "0",
                  "tcp.flags.push": "0",
                  "tcp.flags.reset": "0",
                  "tcp.flags.syn": "1",
                  "tcp.flags.syn_tree": {
                    "_ws.expert": {
                      "tcp.connection.syn": "",
                      "_ws.expert.message": "Connection establish request (SYN): server port 8100",
                      "_ws.expert.severity": "2097152",
                      "_ws.expert.group": "33554432"
                    }
                  },
                  "tcp.flags.fin": "0",
                  "tcp.flags.str": "\u00b7\u00b7\u00b7\u00b7\u00b7\u00b7\u00b7\u00b7\u00b7\u00b7S\u00b7"
                },
                "tcp.window_size_value": "65535",
                "tcp.window_size": "65535",
                "tcp.checksum": "0x0000de6a",
                "tcp.checksum.status": "2",
                "tcp.urgent_pointer": "0",
                "tcp.options": "02:04:05:6e:04:02:08:0a:ff:ff:bb:b6:00:00:00:00:01:03:03:09",
                "tcp.options_tree": {
                  "tcp.options.mss": "02:04:05:6e",
                  "tcp.options.mss_tree": {
                    "tcp.option_kind": "2",
                    "tcp.option_len": "4",
                    "tcp.options.mss_val": "1390"
                  },
                  "tcp.options.sack_perm": "04:02",
                  "tcp.options.sack_perm_tree": {
                    "tcp.option_kind": "4",
                    "tcp.option_len": "2"
                  },
                  "tcp.options.timestamp": "08:0a:ff:ff:bb:b6:00:00:00:00",
                  "tcp.options.timestamp_tree": {
                    "tcp.option_kind": "8",
                    "tcp.option_len": "10",
                    "tcp.options.timestamp.tsval": "4294949814",
                    "tcp.options.timestamp.tsecr": "0"
                  },
                  "tcp.options.nop": "01",
                  "tcp.options.nop_tree": {
                    "tcp.option_kind": "1"
                  },
                  "tcp.options.wscale": "03:03:09",
                  "tcp.options.wscale_tree": {
                    "tcp.option_kind": "3",
                    "tcp.option_len": "3",
                    "tcp.options.wscale.shift": "9",
                    "tcp.options.wscale.multiplier": "512"
                  }
                },
                "Timestamps": {
                  "tcp.time_relative": "0.000000000",
                  "tcp.time_delta": "0.000000000"
                }
              }
            }
          },
          "mac-lte.padding-data": "00:00:00:00:00:00:00:00:00:00:00:00:00:00",
          "mac-lte.padding-length": "14"
        },
        "mac-lte.ulsch": "",
        "_ws.lua.fake": "",
        "_ws.col.Info": "UEId=19    [UL] [AM] DRB:1  [DATA] (P) sn=119   ..18-bytes]",
        "_ws.col.Protocol": "TCP"
      }
    }