MSG #218 2021-12-17 08:56:17.272

SIP REGISTER message at 08:56:17.272

    REGISTER sip:mcstaasting.com SIP/2.0
    Via: SIP/2.0/UDP 192.168.3.2:49054;branch=z9hG4bK-475322294;rport
    From: <sip:PublicUserId-A@mcstaasting.com>;tag=1597691910
    To: <sip:PublicUserId-A@mcstaasting.com>
    Contact: <sip:PublicUserId-A@192.168.3.2:49054;transport=udp>;expires=600000;audio;text;+g.3gpp.cs-voice;+g.3gpp.mcptt;+g.3gpp.mcdata;+g.3gpp.mcdata.sds;+g.3gpp.icsi-ref="urn%3Aurn-7%3A3gpp-service.ims.icsi.mcptt";+g.3gpp.icsi-ref="urn%3Aurn-7%3A3gpp-service.ims.icsi.mcdata";+g.3gpp.icsi-ref="urn%3Aurn-7%3A3gpp-service.ims.icsi.mcdata.sds"
    Call-ID: 1147b073-fcbb-2117-eeaa-ce2862165570
    CSeq: 458190210 REGISTER
    Content-Length: 0
    Max-Forwards: 70
    Authorization: Digest username="PrivateUserId-A@mcstaasting.com",realm="mcstaasting.com",nonce="o94MbTY+MMNkpAePG/jVd24yOzbEbAAAo98ObjI7NsQ=",uri="sip:mcstaasting.com",response="21a725fa6c9a7bdcaca14e3e7fa90c64",algorithm=AKAv1-MD5,cnonce="97f41ed45fd3ffb337fff0c144b45f6b",opaque="5ccc069c403ebaf9f0171e9517f40e41",qop=auth,nc=00000001
    Allow: INVITE, ACK, CANCEL, BYE, MESSAGE, OPTIONS, NOTIFY, PRACK, UPDATE, REFER
    Privacy: none
    P-Access-Network-Info: 3GPP-E-UTRAN-FDD;utran-cell-id-3gpp=0000000000000000
    User-Agent: MCS CLIENT SDK Nemergent 1.0 /v 7.2.6
    P-Preferred-Identity: <sip:PublicUserId-A@mcstaasting.com>
    Supported: path
    Supported: timer
    Security-Client: ipsec-3gpp;alg=hmac-sha-1-96;ealg=aes-cbc;prot=esp;mod=trans;spi-c=1659061855;spi-s=1811560146;port-c=42240;port-s=49054;q=0.9
    Security-Verify: ipsec-3gpp;alg=hmac-sha-1-96;ealg=aes-cbc;spi-c=257;spi-s=256;port-c=5061;port-s=5062;q=0.9
    Security-Verify: ipsec-3gpp;alg=hmac-md5-96;ealg=aes-cbc;spi-c=257;spi-s=256;port-c=5061;port-s=5062;q=0.7
    Require: sec-agree
    Proxy-Require: sec-agree