MSG #382 2023-06-16 15:32:46.222

SIP 200 OK message at 15:32:46.222

    SIP/2.0 200 OK
    Via: SIP/2.0/UDP 192.168.3.2:47744;branch=z9hG4bK-763834550;rport
    From: <sip:PublicUserId-A@mcstaasting.com>;tag=1282482549
    To: <sip:mcptt-server-A@mcstaasting.com>;tag=abc-INVITE-Totag
    CSeq: 616960040 INVITE
    Call-ID: 81ff723e-e3fe-99ea-109b-1642df197647
    Contact: <sip:mcptt-session-A@cf.mcstaasting.com>;+g.3gpp.mcptt;+g.3gpp.icsi-ref="urn%3Aurn-7%3A3gpp-service.ims.icsi.mcptt";audio;isfocus
    Content-Type: application/sdp
    Session-Expires: 3600;refresher=uac
    Supported: norefersub,tdialog,explicitsub,nosub
    Require: timer
    Record-Route: <sip:pcscf.other.com;lr>,<sip:scscf.other.com;lr>,<sip:orig@scscf.3gpp.org;lr>,<sip:192.168.16.111:5062;lr>
    Feature-Caps: *;g.3gpp.mcptt.ambient-listening-call-release
    Content-Length: 378

    v=0
    o=- 1111111111 1111111111 IN IP4 192.168.16.111
    s=
    b=AS:38
    t=0 0
    m=audio 60350 RTP/SAVP 114
    i=speech
    c=IN IP4 192.168.16.111
    b=AS:38
    b=RS:0
    b=RR:2000
    a=rtpmap:114 AMR-WB/16000/1
    a=fmtp:114 mode-change-capability=2;max-red=0
    a=ptime:20
    a=maxptime:240
    a=sendonly
    m=application 60354 udp MCPTT
    c=IN IP4 192.168.16.111
    a=fmtp:MCPTT mc_queueing;mc_priority=3