**3GPP TSG-SA3 Meeting #108e *draft\_S3-221853-r4***

**e-meeting, 22 - 26 August 2022**

**Source: Nokia, Nokia Shanghai Bell, Huawei, HiSilicon**

**Title: KI3 EN resolution on requirements for subscribe notify**

**Document for: Approval**

**Agenda Item: 5.24**

# 1 Decision/action requested

***EN resolution on requirements for subscribe notify key issue***

# 2 References

[1] 3GPP TR 33.875

# 3 Rationale

*Resolution of "Editor’s Note: It is ffs whether these are the correct requirements." is proposed by clarifying the text.*

# 4 Detailed proposal

*\*\*\*\*\*\*\*\*\*\*\* START OF CHANGE*

### 5.3.3 Potential security requirements

It shall be possible for 5G system to ensure notification service is only provided to an authorized NF routed by the URI in the subscribe request message.

It shall be possible for the 5G system to ensure that the notification service is only provided to an NF that has authorized the subscriber to subscribe on its behalf for notifications.

It shall be possible for the 5G system to prevent information disclosure to an unauthorized NF routed by the URI in the subscribe request message.

Editor’s Note: It is ffs whether these are the correct requirements.

*\*\*\*\*\*\*\*\*\*\*\* END OF CHANGE*