**3GPP TSG-SA5 Meeting #141-e *S5-221086rev1***

**e-meeting, 17 -26 January** **2022**

**Source: Huawei**

**Title: Use case of collecting UE related data**

**Document for: Approval**

**Agenda Item: 6.4.1**

# 1 Decision/action requested

***Discuss and approve on the proposal.***

# 2 References

[1] TS 28.557 Management of non-public networks; Stage 1 and stage 2 v1.2.0

# 3 Rationale

It is proposed to add use case to support collecting UE related data in draft TS 28.557 [1] according to the meeting discussion in SA5#140e.

# 4 Detailed proposal

This document proposes the following changes in TS 28.557 [1].

|  |
| --- |
| **1st Change** |

### 5.1.1 Generic use cases

#### 5.1.1.x Collecting UE related data

In some NPN scenarios, the NPN-SC may need to deploy a new vertical service or supervise NPN service SLA based on the UE related data (e.g. UE measurement, etc).

Therefore, 3GPP management system should collect UE related data and provide them to authorized NPN-SC, for example, the vertical customer consumes the management capability exposed by MNO to obtain UE related data.

|  |
| --- |
| **End of change** |