**3GPP TSG-SA5 Meeting #141-e *S5-221229rev1***

**e-meeting, 17 -26 January 2022**

**Source: MATRIXX Software**

**Title: pCR TR 32.847 Conclusions for KI#3**

**Document for: Approval**

**Agenda Item: 7.5.2**

# 1 Decision/action requested

***This*** ***pCR is to introduce conclusions for Key issue#3***

# 2 References

[1] 3GPP TR 32.847 "Study on Charging Aspects for Network Slicing Phase 2"

# 3 Rationale

This pCR is to introduce conclusions for Key issue#3

# 4 Detailed proposal

The following changes are proposed to be incorporated into TR 32.847 [1]

|  |
| --- |
| **First change** |

### 6.3.5 Conclusions

It is concluded on solution #3.1 for Key issue #3, to be specified in two steps:

- In Rel-17 to cover the Combined UE CCS - Tenant CCS solution option for when the Communication Service Provider (CSP) and Network Slice Provider (NSP) are the same. The internal structure for this combined CCS will not be detailed.

- the full solution with charging architecture split between UE CCS and Tenant CCS to be specified.

|  |
| --- |
| **End of changes** |