Agenda Item:	
Source:			Anritsu Corp. , NTT DoCoMo
Title:			Table of Contents for Signalling Test Procedures
Document for:	Discussion and Approval

•	Summary

This document provides a proposal for Table of Contents for Signalling Test Procedures (FDD). 
The structure of this proposal are based on GSM 11.10 and modified for 3G system.
Contents of this proposal is an example. We should study more detail of contents.

Signalling Test Procedures
1	Layer 2
1.1	MAC
1.1.1	Normal procedures
1.1.1.1	MAC PDU receive
1.1.1.2	MAC PDU send / receive
1.1.1.3	MAC SPU mapping to MAC PDU
1.1.2	Abnormal cases
1.2	LAC
1.2.1	Normal procedures
1.2.1.1	LAC PDU receive
1.2.1.2	LAC PDU send / receive
1.2.1.3	LAC SPU mapping to LAC PDU
1.2.2	Abnormal cases
1.3	Layer-to layer communications
1.3.1	Layer1 – MAC
1.3.2	MAC – LAC
1.3.3	LAC – Layer3

2	Layer 3
2.1	Radio Resource Control (RRC)
2.1.1	RRC Connection
2.1.1.1	RRC Connection : Establishment
2.1.1.2	RRC Connection : Failure
2.1.1.3	RRC Connection : Release
2.1.1.4	RRC Connection : Re-establishment
2.1.2	Ciphering
2.1.2.1	Ciphering : Start
2.1.3	Connected Mode Procedures
2.1.3.1	Connected Mode Procedures : Radio Access Bearer Establishment
2.1.3.2	Connected Mode Procedures : Radio Access Bearer Release
2.1.3.3	Connected Mode Procedures : Radio Access Bearer Reconfiguration
2.1.3.4	Connected Mode Procedures : Transport Channel Reconfiguration
2.1.3.5	Connected Mode Procedures : Transport Format Combination(TFC) Control
2.1.3.6	Connected Mode Procedures : Physical Channel Reconfiguration
2.1.4	Mobility Related Procedures
2.1.4.1	Mobility Related Procedures : RRC State Transition
2.1.4.2	Mobility Related Procedures : Active Set Modification/Soft Handover
2.1.4.3	Mobility Related Procedures : Hard Handover
2.1.4.4	Mobility Related Procedures : Inter-system Hard Handover
2.1.4.5	Mobility Related Procedures : URA Update
2.1.4.6	Mobility Related Procedures : Cell Update
2.1.5	Procedures Related to Measurement and Monitoring
2.1.5.1	Procedures Related to Measurement and Monitoring : Measurement Control
2.1.5.2	Procedures Related to Measurement and Monitoring : Measurement Reporting
2.1.6	Miscelleneous Procedures
2.1.6.1	Miscelleneous Procedures : UE Capability Transmission
2.1.6.2	Miscelleneous Procedures : Direct Transfer
2.2	Mobility Management (MM)
2.2.1	Authentication
2.2.1.1	Authentication : Accepted
2.2.1.2	Authentication : Rejected
2.2.2	Connection Management(CM)
2.2.2.1	CM : Request
2.2.2.2	CM : Accepted
2.2.2.3	CM : Prompted
2.2.2.4	CM : Rejected
2.2.2.5	CM : Abortted
2.2.2.6	CM : Re-establishment
2.2.3	Identification
2.2.3.1	Identification : Success
2.2.3.2	Identification : Failure
2.2.4	Location Updating
2.2.4.1	Location Updating : Request
2.2.4.2	Location Updating : Accepted
2.2.4.3	Location Updating : Rejected
2.2.5	TMUI Reallocation
2.2.5.1	TMUI Reallocation : Success
2.2.5.2	TMUI Reallocation : Failure
2.2.6	IMUI Detach
2.2.6.1	IMUI Detach : Indication
2.2.7	Paging
2.2.7.1	Paging : Response
2.2.8	Notification
2.2.8.1	Notification : Response
2.2.9	Aborting
2.2.9.1	Aborting
2.2.10	Miscelleneous Messages
2.2.10.1	Subscriber Specific Information Sending
2.2.10.2	MM Error Status Reporting
2.2.10.3	Null Message
2.3	Circuit Switched Call Control (CC)
2.3.1	Outgoing Call : U0 Null State
2.3.2	Outgoing Call : U0.1 MM Connection Pending
2.3.3	Outgoing Call : U0.2 CC Prompt Present
2.3.4	Outgoing Call : U0.3 Wait for Network Information
2.3.5	Outgoing Call : U0.4 CC-Establishment Present
2.3.6	Outgoing Call : U0.5 CC-Establishment Confirmed
2.3.7	Outgoing Call : U1 Call Initiated
2.3.8	Outgoing Call : U3 Mobile Originating Call Proceeding
2.3.9	Outgoing Call : U4 Call Delivered
2.3.10	Incoming Call : U6 Call Present
2.3.11	Incoming Call : U7 Call Received
2.3.12	Incoming Call : U8 Connect Request
2.3.13	Incoming Call : U9 Mobile Terminating Call Confirmed
2.3.14	U10 Active
2.3.15	U11 Disconnect Request
2.3.16	U12 Disconnect Indication
2.3.17	U19 Release Request
2.3.18	U26 Mobile Originating Modify
2.3.19	U27 Mobile Terminating Modify
2.4	Session Management
2.5	Test Procedures
2.6	SMS

3	Service
3.1	Voice Service
3.1.1	Origination
3.1.2	Termination
3.1.3	Disconnection
3.2	Circuit Switching Service 
3.2.1	Origination
3.2.2	Termination
3.2.3	Disconnection
3.3	Packet Connection Service
3.3.1	Origination
3.3.2	Termination
3.3.3	Disconnection
3.4	Message Services
3.4.1	Origination
3.4.2	Termination
3.4.3	Disconnection
3.5	Supplementary Service
3.6	Multi service
3.6.1	Service addition
3.6.2	Service deletion

4	ME-USIM interface
This should be wrote based on GSM 11.10’s structure.