{"text_format":"1","workbook":"xlsx","n_sheets":6,"sheets":["Simulation assumption","Generalization Parameters(FR1)","KPIs","Frequency combination","UMa_UMi","Sheet2"],"not_rendered":{"charts":1,"images":0,"macros":1,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Simulation assumption","index":0,"n_rows":30,"n_cols":6,"rows_kept":30,"cut":false,"hidden":false,"merged":[[0,0,0,1],[4,0,8,0]]}
["SLS simulation assumption",null,"NTT DOCOMO","Huawei","Mediatek","vivo"]
["Parameter","Values"]
["Frequency Range","FR1@{4GHz,30KHz} as one frequency\nFR1@{2GHz, 15/30KHz} as another frequency"]
["Deployment","\n2-tier model with wrap-around (7 sites, 3 sectors/cells per site)\n"]
["Channel model","UMa with distance-dependent LoS probability function defined in Table 7.4.2-1 in TR 38.901.\nFast fading is necessary. \nOxygen absorption, Time-varying Doppler shift , Explicit ground reflection model and blockage are not considered."]
[null,"Inter-frequency correlation assumption in general (yes or no)","Yes","No","Yes","Yes"]
[null,"Inter-frequency shadow fading correction (e.g. full, partial, no)","Full","No","Full","Full"]
[null,"Whether LOSsoft is modeled or not","No","No","Yes","No"]
[null,"spatial consistency option (A or B)","A","B","A","A"]
["System BW","20MHz"]
["UE Speed","30km/h (baseline), 60km/h (optional), 90km/h (optional)\nOther values are not precluded",90,"30, 60, 90, 120 km/hr","30, 60, 90 km/hr","30km/h"]
["UE distribution","100% outdoor"]
["BS Antenna Configuration"," Companies need to report which option(s) are used between\n- 32 ports: (8,8,2,1,1,2,8), (dH,dV) = (0.5, 0.8)λ\n- 16 ports: (8,4,2,1,1,2,4), (dH,dV) = (0.5, 0.8)λ\nOther configurations are not precluded.","32 ports: (8,8,2,1,1,2,8), (dH,dV) = (0.5, 0.8)λ","32 ports: (8,8,2,1,1,2,8), (dH,dV) = (0.5, 0.8)λ",null,"32 ports: (8,8,2,1,1,2,8), (dH,dV) = (0.5, 0.8)λ\n"]
["BS Antenna radiation pattern","3-sector antenna radiation pattern, 8 dBi"]
["UE Antenna Configuration","4RX: (1,2,2,1,1,1,2), (dH,dV) = (0.5, 0.5)λ for (rank 1-4)\n2RX: (1,1,2,1,1,1,1), (dH,dV) = (0.5, 0.5)λ for (rank 1,2)\nOther configuration is not precluded.","2RX: (1,1,2,1,1,1,1), (dH,dV) = (0.5, 0.5)λ for (rank 1,2)","4RX: (1,2,2,1,1,1,2), (dH,dV) = (0.5, 0.5)λ for (rank 1-4)",null,"2RX: (1,1,2,1,1,1,1), (dH,dV) = (0.5, 0.5)λ \n"]
["UE Antenna radiation pattern","Omni-direction"]
["BS Tx Power","44dBm"]
["Maximum UE Tx Power","23 dBm"]
["BS receiver Noise Figure","5 dB"]
["UE receiver Noise Figure","9 dB"]
["Inter site distance","500m ISD for FR1"]
["BS Antenna height","25m"]
["UE Antenna height","1.5 m"]
["UE trajectory model","Option #1, Option #2, or option #3\nReported by companies","Option 3","Option1","Option1","Option1"]
["UE trajectory boundary processing","Option #1, Option #2, or option #3 \nReported by companies","Option 3","Option1","Option2","Option2"]
["L1/L3 filtering","Option #Sliding, Option #Non-sliding\nReported by companies","No-sliding","Non-sliding","both","Option1"]
["measurement period","200ms"]
["FilterCoefficient",4]
["Number of Tx beams","Reported by companies",4,4,1,1]
["Number of Rx beams","Reported by companies",1,1,1,1]

{"sheet":"Generalization Parameters(FR1)","index":1,"n_rows":6,"n_cols":3,"rows_kept":6,"cut":false,"hidden":false,"merged":[[0,0,0,2]]}
["Generalization Parameters for FR1"]
["Parameter","Configuration #1","Configuration #2"]
["Deployment scenario ","UMi","UMa"]
["ISD","200m","500m"]
["BS antenna height","10m","25m"]
["BS Tx power","40dBm","44dBm"]

{"sheet":"KPIs","index":2,"n_rows":2,"n_cols":5,"rows_kept":2,"cut":false,"hidden":false,"merged":[]}
["Intermediate KPIs","Description/Definition","NTT DOCOMO","vivo","Mediatek"]
["Average L3 cell RSRP difference  (dB)","Average L3 RSRP difference between predicted and ideal L3 cell-level measurement result","Method: Average cross multiple cells","Method: Average cross multiple cells","Method: Average cross multiple cells"]

{"sheet":"Frequency combination","index":3,"n_rows":46,"n_cols":29,"rows_kept":46,"cut":false,"hidden":false,"merged":[[0,0,0,2],[0,3,0,4],[0,5,0,7],[0,8,0,16],[0,17,0,25]]}
["General",null,null,"Generalization Setting",null,"Variable Settings",null,null,"Configurable/Selectable Simulation Assumption",null,null,null,null,null,null,null,null,"Model Related Information",null,null,null,null,null,null,null,null,"Performance Metrics (Baseline)","Performance Metrics (GC#1)","Performance Metrics (GC#2)"]
["Company","Sub case","Other factors","Configuration #A","Configuration #B","Observation window\n(ms)","Channel correlation coefficient between two frequency layers","UE speed\n(km/h)","Spatial consistency","Whether LOSsoft is modeled or not","Inter-frequency correlation ","Inter-frequency shadow fading correlation","UE trajectory model","UE trajectory boundary processing","L1/L3 filtering\n(Sliding/Non-sliding)","Number of Tx beams","Number of Rx beams","Model input","Model output/label","Model type","Detail of model","Model complexity\nin a number of model parameters (K)","Model complexity\nin a number of model size (KByte)","Computational complexity [FLOPs] (M)","Training data size in number of samples (K)","Testing data size in number of samples (K)","Average L3 cell RSRP difference (dB)","Average L3 cell RSRP difference (dB)","Average L3 cell RSRP difference (dB)"]
["Name","1/2/3","Additional consideration\n(e.g. Cluster-based)","Dataset with configuration #A(e.g., 2GHz=>4GHz/4GHz=>2GHz)","Dataset with configuration #B(e.g., 4GHz=>2GHz)","XX"," PCC (Pearson Correlation Coefficient)[TBD]","XX","A/B","YES/NO","YES/NO","FULL/PARTIAL/NO","1/2/3","1/2/3","Sliding/Non-sliding","XX","XX","Number of cell(s),\nMesurement quantity (L1 beam-level, L1-filterd beam-level, L3 cell-level, L3 beam-level measurement results)","Number of cell(s),\nMesurement quantity(L1 beam-level, L1-filterd beam-level, L3 cell-level, L3 beam-level measurement results)","AI/Non-AI: Method (e.g. RNN,CNN, Sample and hold, Decision tree)","e.g.,model structure and description","XX","XX","XX","XX","XX","XX","XX","XX"]
["NTT DOCOMO",3,"Cluster-based","4GHz=>2GHz","4GHz=>2GHz",40,null,90,"A ","No","YES","FULL",3,3,"Sliding",4,1,"7 cells, L1 cell-level RSRP  ","7 cells, L3 cell-level RSRP  ","AI: Transformer",null,null,null,null,1613,403,0.19700000000000001]
["NTT DOCOMO",3,"Cluster-based","2GHz=>4GHz","4GHz=>2GHz",40,null,90,"A ","No","YES","FULL",3,3,"Sliding",4,1,"7 cells, L1 cell-level RSRP  ","7 cells, L3 cell-level RSRP  ","AI: Transformer",null,null,null,null,1613,403,null,1.4407000000000001]
["NTT DOCOMO",3,"Cluster-based","Mix","4GHz=>2GHz",40,null,90,"A ","No","YES","FULL",3,3,"Sliding",4,1,"7 cells, L1 cell-level RSRP  ","7 cells, L3 cell-level RSRP  ","AI: Transformer",null,null,null,null,1613,403,null,null,1.1856]
["NTT DOCOMO",3,"Cluster-based","2GHz=>4GHz","2GHz=>4GHz",40,null,90,"A ","No","YES","FULL",3,3,"Sliding",4,1,"7 cells, L1 cell-level RSRP  ","7 cells, L3 cell-level RSRP  ","AI: Transformer",null,null,null,null,1613,403,0.18079999999999999]
["NTT DOCOMO",3,"Cluster-based","4GHz=>2GHz","2GHz=>4GHz",40,null,90,"A ","No","YES","FULL",3,3,"Sliding",4,1,"7 cells, L1 cell-level RSRP  ","7 cells, L3 cell-level RSRP  ","AI: Transformer",null,null,null,null,1613,403,null,1.6895]
["NTT DOCOMO",3,"Cluster-based","Mix","2GHz=>4GHz",40,null,90,"A ","No","YES","FULL",3,3,"Sliding",4,1,"7 cells, L1 cell-level RSRP  ","7 cells, L3 cell-level RSRP  ","AI: Transformer",null,null,null,null,1613,403,null,null,1.2121999999999999]
["Ericsson",2,"Cluster-based, UMA, during training and inference model DOES NOT knows which samples belong to 2GHz and which belong to 4GHz","2GHz=>4GHz","4GHz=>2GHz","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"9 cells, L3 Cell-Level RSRP","9 cells, L3 Cell-Level RSRP","xgboost","1000 estimators, max_depth=7",292,"7300.0 KB",51,29576,7394,0.120316493691184,19.587450220924101,4.5905178431169098]
["Ericsson",2,"Cluster-based, UMA, during training and inference model knows which samples belong to 2GHz and which belong to 4GHz","2GHz=>4GHz","4GHz=>2GHz","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"15 cells, L3 Cell-Level RSRP","15 cells, L3 Cell-Level RSRP","xgboost","1000 estimators, max_depth=7",292,"7300.0 KB",51,29576,7394,0.10587581198004201,19.912117209772699,2.2350567908132701]
["Ericsson",2,"Cluster-based, UMA, during training and inference model DOES NOT knows which samples belong to 2GHz and which belong to 4GHz","2GHz=>4GHz","4GHz=>2GHz","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"15 cells, L3 Cell-Level RSRP","15 cells, L3 Cell-Level RSRP","xgboost","1000 estimators, max_depth=7",292,"7300.0 KB",51,29576,7394,0.10587581198004201,19.912117209772699,4.1501088421452597]
["Ericsson",2,"Cluster-based, UMA, during training and inference model knows which samples belong to 2GHz and which belong to 4GHz","2GHz=>4GHz","4GHz=>2GHz","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"21 cells, L3 Cell-Level RSRP","21 cells, L3 Cell-Level RSRP","xgboost","1000 estimators, max_depth=7",292,"7300.0 KB",51,29576,7394,9.9950445495688905E-2,20.5883388839841,2.4063629789229299]
["Ericsson",2,"Cluster-based, UMA, during training and inference model DOES NOT knows which samples belong to 2GHz and which belong to 4GHz","2GHz=>4GHz","4GHz=>2GHz","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"21 cells, L3 Cell-Level RSRP","21 cells, L3 Cell-Level RSRP","xgboost","1000 estimators, max_depth=7",292,"7300.0 KB",51,29576,7394,9.9950445495688905E-2,20.5883388839841,4.3811513872272698]
["Ericsson",2,"Cluster-based, UMA, during training and inference model knows which samples belong to 2GHz and which belong to 4GHz","2GHz=>4GHz","4GHz=>2GHz","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"2 cells, L3 Cell-Level RSRP","2 cells, L3 Cell-Level RSRP","xgboost","1000 estimators, max_depth=7",292,"7300.0 KB",51,29576,7394,0.57225400635422596,19.678011695242301,2.56201338522466]
["Ericsson",2,"Cluster-based, UMA, during training and inference model DOES NOT knows which samples belong to 2GHz and which belong to 4GHz","2GHz=>4GHz","4GHz=>2GHz","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"2 cells, L3 Cell-Level RSRP","2 cells, L3 Cell-Level RSRP","xgboost","1000 estimators, max_depth=7",292,"7300.0 KB",51,29576,7394,0.57225400635422596,19.678011695242301,6.6222878164056702]
["Ericsson",2,"Cluster-based, UMI, during training and inference model knows which samples belong to 2GHz and which belong to 4GHz","2GHz=>4GHz","4GHz=>2GHz","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"2 cells, L3 Cell-Level RSRP","2 cells, L3 Cell-Level RSRP","xgboost","1000 estimators, max_depth=7",292,"7300.0 KB",51,29576,7394,0.815184238881422,16.197066272222699,1.91017545151169]
["Ericsson",2,"Cluster-based, UMI, during training and inference model DOES NOT knows which samples belong to 2GHz and which belong to 4GHz","2GHz=>4GHz","4GHz=>2GHz","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"2 cells, L3 Cell-Level RSRP","2 cells, L3 Cell-Level RSRP","xgboost","1000 estimators, max_depth=7",292,"7300.0 KB",51,29576,7394,0.815184238881422,16.197066272222699,8.5800209680529296]
["Ericsson",2,"Cluster-based, UMI, during training and inference model knows which samples belong to 2GHz and which belong to 4GHz","2GHz=>4GHz","4GHz=>2GHz","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"15 cells, L3 Cell-Level RSRP","15 cells, L3 Cell-Level RSRP","xgboost","1000 estimators, max_depth=7",292,"7300.0 KB",51,29576,7394,0.14996768976008501,15.339888261099199,2.1419568499311898]
["Ericsson",2,"Cluster-based, UMI, during training and inference model DOES NOT knows which samples belong to 2GHz and which belong to 4GHz","2GHz=>4GHz","4GHz=>2GHz","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"15 cells, L3 Cell-Level RSRP","15 cells, L3 Cell-Level RSRP","xgboost","1000 estimators, max_depth=7",292,"7300.0 KB",51,29576,7394,0.14996768976008501,15.339888261099199,6.1885177913952001]
["Ericsson",2,"Cluster-based, UMI, during training and inference model knows which samples belong to 2GHz and which belong to 4GHz","2GHz=>4GHz","4GHz=>2GHz","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"9 cells, L3 Cell-Level RSRP","9 cells, L3 Cell-Level RSRP","xgboost","1000 estimators, max_depth=7",292,"7300.0 KB",51,29576,7394,0.16940130790881999,15.622548736311799,1.9845642682498601]
["Ericsson",2,"Cluster-based, UMI, during training and inference model DOES NOT knows which samples belong to 2GHz and which belong to 4GHz","2GHz=>4GHz","4GHz=>2GHz","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"9 cells, L3 Cell-Level RSRP","9 cells, L3 Cell-Level RSRP","xgboost","1000 estimators, max_depth=7",292,"7300.0 KB",51,29576,7394,0.16940130790881999,15.622548736311799,7.4434598565177597]
["Ericsson",2,"Cluster-based, UMI, during training and inference model knows which samples belong to 2GHz and which belong to 4GHz","4GHz=>2GHz","2GHz=>4GHz","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"9 cells, L3 Cell-Level RSRP","9 cells, L3 Cell-Level RSRP","xgboost","1000 estimators, max_depth=7",292,"7300.0 KB",51,29576,7394,0.146901128807016,17.210781823846201,2.0381703850456701]
["Ericsson",2,"Cluster-based, UMI, during training and inference model DOES NOT knows which samples belong to 2GHz and which belong to 4GHz","4GHz=>2GHz","2GHz=>4GHz","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"9 cells, L3 Cell-Level RSRP","9 cells, L3 Cell-Level RSRP","xgboost","1000 estimators, max_depth=7",292,"7300.0 KB",51,29576,7394,0.146901128807016,17.210781823846201,11.3731496795785]
["Ericsson",2,"Cluster-based, UMI, during training and inference model knows which samples belong to 2GHz and which belong to 4GHz","4GHz=>2GHz","2GHz=>4GHz","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"21 cells, L3 Cell-Level RSRP","21 cells, L3 Cell-Level RSRP","xgboost","1000 estimators, max_depth=7",292,"7300.0 KB",51,29576,7394,0.12151091080957201,16.959681615678001,1.93251894908486]
["Ericsson",2,"Cluster-based, UMI, during training and inference model DOES NOT knows which samples belong to 2GHz and which belong to 4GHz","4GHz=>2GHz","2GHz=>4GHz","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"21 cells, L3 Cell-Level RSRP","21 cells, L3 Cell-Level RSRP","xgboost","1000 estimators, max_depth=7",292,"7300.0 KB",51,29576,7394,0.12151091080957201,16.959681615678001,11.1133975064051]
["Ericsson",2,"Cluster-based","2GHz=>4GHz @ UMA","4GHz=>2GHz @ UMI","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"6 cells, L3 Cell-Level RSRP","6 cells, L3 Cell-Level RSRP","xgboost","1000 estimators, max_depth=7",292,"7300.0 KB",51,29576,7394,0.16,18.88,2.5]
["Ericsson",2,"Cluster-based","2GHz=>4GHz @ UMI","4GHz=>2GHz @ UMA","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"6 cells, L3 Cell-Level RSRP","6 cells, L3 Cell-Level RSRP","xgboost","1000 estimators, max_depth=7",292,"7300.0 KB",51,29576,7394,0.2,19,3.9]
["Huawei",2,"Cell-based","4GHz=>2GHz","2GHz=>4GHz",200,0.9,30,"B","NO","NO","NO",1,1,"Non-sliding",4,1,"1 cell,  L3 cell-level RSRP ","1 cell,  L3 cell-level RSRP ","AI: LSTM","3 LSTM layers and 1 full-connectivity layer",80,350,1.03,30,0.5,0.4,0.43,0.41]
["Huawei",2,"Cell-based","2GHz=>4GHz","4GHz=>2GHz",200,0.9,30,"B","NO","NO","NO",1,1,"Non-sliding",4,1,"1 cell,  L3 cell-level RSRP ","1 cell,  L3 cell-level RSRP ","AI: LSTM","3 LSTM layers and 1 full-connectivity layer",80,350,1.03,30,0.5,0.26,0.3,0.28000000000000003]
["Huawei",2,"Cell-based","4GHz=>2GHz","2GHz=>4GHz",200,0.9,60,"B","NO","NO","NO",1,1,"Non-sliding",4,1,"1 cell,  L3 cell-level RSRP ","1 cell,  L3 cell-level RSRP ","AI: LSTM","3 LSTM layers and 1 full-connectivity layer",80,350,1.03,30,0.5,0.21,0.25,0.22]
["Huawei",2,"Cell-based","2GHz=>4GHz","4GHz=>2GHz",200,0.9,60,"B","NO","NO","NO",1,1,"Non-sliding",4,1,"1 cell,  L3 cell-level RSRP ","1 cell,  L3 cell-level RSRP ","AI: LSTM","3 LSTM layers and 1 full-connectivity layer",80,350,1.03,30,0.5,0.19,0.2,0.19]
["Huawei",2,"Cell-based","4GHz=>2GHz","2GHz=>4GHz",200,0.9,90,"B","NO","NO","NO",1,1,"Non-sliding",4,1,"1 cell,  L3 cell-level RSRP ","1 cell,  L3 cell-level RSRP ","AI: LSTM","3 LSTM layers and 1 full-connectivity layer",80,350,1.03,30,0.5,0.55000000000000004,0.56000000000000005,0.55000000000000004]
["Huawei",2,"Cell-based","2GHz=>4GHz","4GHz=>2GHz",200,0.9,90,"B","NO","NO","NO",1,1,"Non-sliding",4,1,"1 cell,  L3 cell-level RSRP ","1 cell,  L3 cell-level RSRP ","AI: LSTM","3 LSTM layers and 1 full-connectivity layer",80,350,1.03,30,0.5,0.42,0.67,0.55000000000000004]
["Mediatek",2,"Cluster-based","4GHz=>2GHz","2GHz=>4GHz",40,null,60,"A ","YES","YES","FULL",1,2,"Sliding",4,1,"21 cells,  L3 cell-level RSRP ","21 cells, L3 cell-level RSRP","AI: CNN","2 layers of convolution layer and 1 FNN layer",50,201,3,160,40,1.589,11.92,2.61]
["Mediatek",2,"Cluster-based","2GHz=>4GHz","4GHz=>2GHz",40,null,60,"A ","YES","YES","FULL",1,2,"Sliding",4,1,"21 cells,  L3 cell-level RSRP ","21 cells, L3 cell-level RSRP","AI: CNN","2 layers of convolution layer and 1 FNN layer",50,201,3,160,40,1.52,11.432,2.08]
["ZTE",2,"Cell-based","2GHz=>4GHz","4GHz=>2GHz",null,0.97699999999999998,90,"A","YES","YES","FULL",3,2,"Non-sliding",4,1,"1 cell, L3 cell-level RSRP","1 cell, L3 cell-level RSRP","AI: Full connection network","7 hidden layers",1.486,7.02,0.01,90,5,0.97,11.92,1]
["ZTE",2,"Cell-based","4GHz=>2GHz","2GHz=>4GHz",null,0.97699999999999998,90,"A","NO","YES","FULL",3,2,"Non-sliding",4,1,"1 cell, L3 cell-level RSRP","1 cell, L3 cell-level RSRP","AI: Full connection network","7 hidden layers",1.486,7.02,0.01,90,5,0.96,11.28,1]
["vivo",2,"Cell-based","4GHz=>2GHz","2GHz=>4GHz",2000,0.92300000000000004,30,"A ","NO","YES","FULL",1,2,"Sliding",1,1,"1 cell, L3 cell-level RSRP and cell id","1 cell, L3 cell-level RSRP","RandomForest","n_estimators = 2\nmax_depth = 20",0.29399999999999998,5.1100000000000003,7.0000000000000001E-3,160,40,0.7,6.38,0.83]
["vivo",2,"Cell-based","2GHz=>4GHz","4GHz=>2GHz",2000,0.92300000000000004,30,"A ","NO","YES","FULL",1,2,"Sliding",1,1,"1 cell, L3 cell-level RSRP and cell id","1 cell, L3 cell-level RSRP","RandomForest","n_estimators = 2\nmax_depth = 20",0.29299999999999998,4.76,7.0000000000000001E-3,160,40,0.76,6.2,0.83]
["vivo",2,"Cell-based","4GHz=>2GHz","2GHz=>4GHz",2000,0.92300000000000004,30,"A ","NO","YES","FULL",1,2,"Sliding",1,1,"1 cell, L3 cell-level RSRP and cell id, input associated with frequency","1 cell, L3 cell-level RSRP","RandomForest","n_estimators = 2\nmax_depth = 20",0.30599999999999999,4.83,8.0000000000000002E-3,160,40,0.64,6.43,0.73]
["vivo",2,"Cell-based","2GHz=>4GHz","4GHz=>2GHz",2000,0.92300000000000004,30,"A ","NO","YES","FULL",1,2,"Sliding",1,1,"2 cell, L3 cell-level RSRP and cell id, input associated with frequency","1 cell, L3 cell-level RSRP","RandomForest","n_estimators = 2\nmax_depth = 20",0.30099999999999999,4.78,8.0000000000000002E-3,160,40,0.74,6.24,0.77]
["CATT",2,"Cluster-based;","2GHz=>4GHz","4GHz=>2GHz",null,0.99,0,"A ","YES","NO","FULL",1,2,"Non-sliding",4,1,"21 cells,  L3 cell-level RSRP, input associated with frequency","21 cells, L3 cell-level RSRP, output associated with frequency","AI: ResNet","1 layers of AI: ResNet layer and 1 DNN layer","17K","65KB","0.286M",13,1.625,0.2009,0.3947,0.25559999999999999]
["CATT",2,"Cluster-based;","2GHz=>4GHz","4GHz=>2GHz",null,0.99,0,"A ","YES","NO","FULL",1,2,"Non-sliding",4,1,"21 cells,  L3 cell-level RSRP, input associated with frequency","21 cells, L3 cell-level RSRP, output associated with frequency","AI: MLP","3 layers of MLP-Mixer","912K","3497KB","19.68M",13,1.625,0.13170000000000001,0.36609999999999998,0.2258]
["CATT",2,"Cluster-based;","4GHz=>2GHz","2GHz=>4GHz",null,0.99,0,"A ","YES","NO","FULL",1,2,"Non-sliding",4,1,"21 cells,  L3 cell-level RSRP, input associated with frequency","21 cells, L3 cell-level RSRP, output associated with frequency","AI: ResNet","1 layers of AI: ResNet layer and 1 DNN layer","17K","65KB","0.286M",13,1.625,0.21310000000000001,0.34870000000000001,0.27]
["CATT",2,"Cluster-based;","4GHz=>2GHz","2GHz=>4GHz",null,0.99,0,"A ","YES","NO","FULL",1,2,"Non-sliding",4,1,"21 cells,  L3 cell-level RSRP, input associated with frequency","21 cells, L3 cell-level RSRP, output associated with frequency","AI: MLP","3 layers of MLP-Mixer","912K","3497KB","19.68M",13,1.625,0.12540000000000001,0.33600000000000002,0.2185]

{"sheet":"UMa_UMi","index":4,"n_rows":25,"n_cols":29,"rows_kept":25,"cut":false,"hidden":false,"merged":[[0,0,0,2],[0,3,0,4],[0,5,0,7],[0,8,0,16],[0,17,0,25]]}
["General",null,null,"Generalization Setting",null,"Variable Settings",null,null,"Configurable/Selectable Simulation Assumption",null,null,null,null,null,null,null,null,"Model Related Information",null,null,null,null,null,null,null,null,"Performance Metrics (Baseline)","Performance Metrics (GC#1)","Performance Metrics (GC#2)"]
["Company","Sub-use case","Other factors","Configuration #A","Configuration #B","Observation window\n(ms)","Channel correlation coefficient between two frequency layers","UE speed\n(km/h)","Spatial consistency","Whether LOSsoft is modeled or not","Inter-frequency correlation ","Inter-frequency shadow fading correlation","UE trajectory model","UE trajectory boundary processing","L1/L3 filtering\n(Sliding/Non-sliding)","Number of Tx beams","Number of Rx beams","Model input","Model output/label","Model type","Detail of model","Model complexity\nin a number of model parameters (K)","Model complexity\nin a number of model size (KByte)","Computational complexity [FLOPs] (M)","Training data size in number of samples (K)","Testing data size in number of samples (K)","Average L3 cell RSRP difference (dB)","Average L3 cell RSRP difference (dB)","Average L3 cell RSRP difference (dB)"]
["Name","1/2/3","Additional consideration\n(e.g. Cluster-based)","Configuration #1/2","Configuration #1/2","XX"," PCC (Pearson Correlation Coefficient)[TBD]","XX","A/B","YES/NO","YES/NO","FULL/PARTIAL/NO","1/2/3","1/2/3","Sliding/Non-sliding","XX","XX","Number of cell(s),\nMesurement quantity (L1 beam-level, L1-filterd beam-level, L3 cell-level, L3 beam-level measurement results)","Number of cell(s),\nMesurement quantity(L1 beam-level, L1-filterd beam-level, L3 cell-level, L3 beam-level measurement results)","AI/Non-AI: Method (e.g. RNN,CNN, Sample and hold, Decision tree)","e.g.,model structure and description","XX","XX","XX","XX","XX","XX","XX","XX"]
["Ericsson","2","UMi-to-UMa, \nVariable BW==> 20Mhz@2GH, 100MHz@4GHz","Configuration #1","Configuration #2","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"21 cell, L3 cell-level RSRP ","21 cell, L3 cell-level RSRP ","AI: xgboost","n_estimators=1000, max_depth=7",292,7300,51,29576,7394,0.12953772289412299,19.844308762323202,3.4129433291299001]
["Ericsson","2","UMi-to-UMa, \nVariable BW==> 20Mhz@2GH, 100MHz@4GHz","Configuration #1","Configuration #2","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"9 cell, L3 cell-level RSRP ","21 cell, L3 cell-level RSRP ","AI: xgboost","n_estimators=1000, max_depth=7",292,7300,51,29576,7394,0.20728552625292801,19.469794046311101,6.9265720163072801]
["Ericsson","2","UMi-to-UMa, \nVariable BW==> 20Mhz@2GH, 100MHz@4GHz","Configuration #1","Configuration #2","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"9 cell, L3 cell-level RSRP ","9 cell, L3 cell-level RSRP ","AI: xgboost","n_estimators=1000, max_depth=7",292,7300,51,29576,7394,0.15131418572531799,19.629387113783,3.1453015009562102]
["Ericsson","2","UMi-to-UMa, \nVariable BW==> 20Mhz@2GH, 100MHz@4GHz","Configuration #1","Configuration #2","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"9 cell, L3 cell-level RSRP ","3 cell, L3 cell-level RSRP ","AI: xgboost","n_estimators=1000, max_depth=7",292,7300,51,29576,7394,0.144995475808779,19.895285924275701,3.1671120325724198]
["Ericsson","2","UMi-to-UMa, \nVariable BW==> 20Mhz@2GH, 100MHz@4GHz","Configuration #1","Configuration #2","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"9 cell, L3 cell-level RSRP ","1 cell, L3 cell-level RSRP ","AI: xgboost","n_estimators=1000, max_depth=7",292,7300,51,29576,7394,0.15091586112975999,20.055461883544901,3.1909370422363201]
["Ericsson","2","UMi-to-UMa, \nVariable BW==> 20Mhz@2GH, 100MHz@4GHz","Configuration #1","Configuration #2","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"21 cell, L3 cell-level RSRP ","21 cell, L3 cell-level RSRP ","AI: Conv2D","1 Conv2D, BN, DropOut, Linear, ",6.7,30,0.06,29576,7394,1.8489953733625799,19.9525955745152,3.0435533637092198]
["Ericsson","2","UMi-to-UMa, \nVariable BW==> 20Mhz@2GH, 100MHz@4GHz","Configuration #1","Configuration #2","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"9 cell, L3 cell-level RSRP ","21 cell, L3 cell-level RSRP ","AI: Conv2D","1 Conv2D, BN, DropOut, Linear, ",6.7,30,0.06,29576,7394,4.1580012866428904,19.624311265491301,5.9759969257172996]
["Ericsson","2","UMi-to-UMa, \nVariable BW==> 20Mhz@2GH, 100MHz@4GHz","Configuration #1","Configuration #2","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"9 cell, L3 cell-level RSRP ","9 cell, L3 cell-level RSRP ","AI: Conv2D","1 Conv2D, BN, DropOut, Linear, ",6.7,30,0.06,29576,7394,2.1265985965728702,19.532007429334801,2.6588056087493799]
["Ericsson","2","UMi-to-UMa, \nVariable BW==> 20Mhz@2GH, 100MHz@4GHz","Configuration #1","Configuration #2","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"9 cell, L3 cell-level RSRP ","3 cell, L3 cell-level RSRP ","AI: Conv2D","1 Conv2D, BN, DropOut, Linear, ",6.7,30,0.06,29576,7394,2.1047019163767402,19.204488754272401,2.7556858857472699]
["Ericsson","2","UMi-to-UMa, \nVariable BW==> 20Mhz@2GH, 100MHz@4GHz","Configuration #1","Configuration #2","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"9 cell, L3 cell-level RSRP ","1 cell, L3 cell-level RSRP ","AI: Conv2D","1 Conv2D, BN, DropOut, Linear, ",6.7,30,0.06,29576,7394,1.8807646036148,19.9992771148681,2.5903682708740199]
["Ericsson","2","UMi-to-UMa, \nFixed BW==> 20Mhz@2GH, 20MHz@4GHz","Configuration #1","Configuration #2","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"21 cell, L3 cell-level RSRP ","21 cell, L3 cell-level RSRP ","AI: xgboost","n_estimators=1000, max_depth=7",292,7300,51,29576,7394,7.5087656222638605E-2,2.19389762764885,0.785992639405386]
["Ericsson","2","UMi-to-UMa, \nFixed BW==> 20Mhz@2GH, 20MHz@4GHz","Configuration #1","Configuration #2","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"21 cell, L3 cell-level RSRP ","21 cell, L3 cell-level RSRP ","AI: Conv2D","1 Conv2D, BN, DropOut, Linear, ",6.7,30,0.06,29576,7394,1.41927737849099,1.74870727175758,0.79899933792295896]
["Ericsson","2","UMi-to-UMa, \nFixed BW==> 20Mhz@2GH, 20MHz@4GHz","Configuration #1","Configuration #2","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"9 cell, L3 cell-level RSRP ","21 cell, L3 cell-level RSRP ","AI: Conv2D","1 Conv2D, BN, DropOut, Linear, ",6.7,30,0.06,29576,7394,4.57605811527797,7.3035481089637297,4.9332485795021004]
["Ericsson","2","UMi-to-UMa, \nFixed BW==> 20Mhz@2GH, 20MHz@4GHz","Configuration #1","Configuration #2","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"9 cell, L3 cell-level RSRP ","21 cell, L3 cell-level RSRP ","AI: xgboost","n_estimators=1000, max_depth=7",292,7300,51,29576,7394,0.15701307640189199,7.7722702139899802,5.54307674226306]
["Ericsson","2","UMi-to-UMa, \nFixed BW==> 20Mhz@2GH, 20MHz@4GHz","Configuration #1","Configuration #2","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"9 cell, L3 cell-level RSRP ","9 cell, L3 cell-level RSRP ","AI: xgboost","n_estimators=1000, max_depth=7",292,7300,51,29576,7394,8.7154998547501E-2,2.3153272999657499,0.96453410387039096]
["Ericsson","2","UMi-to-UMa, \nFixed BW==> 20Mhz@2GH, 20MHz@4GHz","Configuration #1","Configuration #2","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"9 cell, L3 cell-level RSRP ","1 cell, L3 cell-level RSRP ","AI: xgboost","n_estimators=1000, max_depth=7",292,7300,51,29576,7394,8.6389072239398901E-2,2.37794661521911,1.413792014122]
["Ericsson","2","UMi-to-UMa, \nFixed BW==> 20Mhz@2GH, 20MHz@4GHz","Configuration #1","Configuration #2","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"9 cell, L3 cell-level RSRP ","1 cell, L3 cell-level RSRP ","AI: Conv2D","1 Conv2D, BN, DropOut, Linear, ",6.7,30,0.06,29576,7394,1.4072116613387999,2.0070555210113499,0.74950885772705]
["Ericsson","2","UMi-to-UMa, \nFixed BW==> 20Mhz@2GH, 20MHz@4GHz","Configuration #1","Configuration #2","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"9 cell, L3 cell-level RSRP ","9 cell, L3 cell-level RSRP ","AI: Conv2D","1 Conv2D, BN, DropOut, Linear, ",6.7,30,0.06,29576,7394,1.4993192354838001,2.2528410752614301,0.78465145826339699]
["Ericsson","2","UMa-to-UMi, \nFixed BW==> 20Mhz@2GH, 20MHz@4GHz","Configuration #2","Configuration #1","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"21 cell, L3 cell-level RSRP ","21 cell, L3 cell-level RSRP ","AI: Conv2D","1 Conv2D, BN, DropOut, Linear, ",6.7,30,0.06,29576,7394,1.20188009171258,2.0020449842725401,1.5727905829747499]
["Ericsson","2","UMa-to-UMi, \nFixed BW==> 20Mhz@2GH, 20MHz@4GHz","Configuration #2","Configuration #1","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"21 cell, L3 cell-level RSRP ","21 cell, L3 cell-level RSRP ","AI: xgboost","n_estimators=1000, max_depth=7",292,7300,51,29576,7394,3.2882280292965103E-2,2.3868934654054099,1.5757788135891799]
["Ericsson","2","UMa-to-UMi, \nFixed BW==> 20Mhz@2GH, 20MHz@4GHz","Configuration #2","Configuration #1","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"9 cell, L3 cell-level RSRP ","21 cell, L3 cell-level RSRP ","AI: xgboost","n_estimators=1000, max_depth=7",292,7300,51,29576,7394,8.0863951040165694E-2,6.9965534777868301,6.4224226645060902]
["Ericsson","2","UMa-to-UMi, \nFixed BW==> 20Mhz@2GH, 20MHz@4GHz","Configuration #2","Configuration #1","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"9 cell, L3 cell-level RSRP ","3 cell, L3 cell-level RSRP ","AI: xgboost","n_estimators=1000, max_depth=7",292,7300,51,29576,7394,3.5162438948949097E-2,2.50633939107259,1.67726357777913]

{"sheet":"Sheet2","index":5,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}