{"text_format":"1","workbook":"xlsx","n_sheets":4,"sheets":["Simulation assumption","KPIs","Results","Sheet1"],"not_rendered":{"charts":2,"images":0,"macros":0,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Simulation assumption","index":0,"n_rows":30,"n_cols":9,"rows_kept":30,"cut":false,"hidden":false,"merged":[[0,0,0,1],[4,0,8,0]]}
["SLS simulation assumption",null,"CATT","NTT DOCOMO","Mediatek","Huawei","OPPO","vivo","Samsung"]
["Parameter","Values"]
["Frequency Range","FR1@{4GHz,30KHz} as one frequency\nFR1@{2GHz, 15/30KHz} as another frequency"]
["Deployment","\n2-tier model with wrap-around (7 sites, 3 sectors/cells per site)\n"]
["Channel model","UMa with distance-dependent LoS probability function defined in Table 7.4.2-1 in TR 38.901.\nFast fading is necessary. \nOxygen absorption, Time-varying Doppler shift , Explicit ground reflection model and blockage are not considered."]
[null,"Inter-frequency correlation assumption in general (yes or no)","No","Yes","Yes","No","No","Yes","Yes"]
[null,"Inter-frequency shadow fading correction (e.g. full, partial, no)","Full","Full","Full","No","Full","Full","Full"]
[null,"Whether LOSsoft is modeled or not","Yes","No","Yes","No",null,"No","Yes"]
[null,"spatial consistency option (A or B)","A","A","A","B","A","A","B"]
["System BW","20MHz"]
["UE Speed","30km/h (baseline), 60km/h (optional), 90km/h (optional)\nOther values are not precluded","0, 90 km/hr",90,"30, 60, 90 km/hr","30, 60, 90, 120 km/hr"," 30, 60 km/h","30, 60, 90 km/hr","120 km/hr"]
["UE distribution","100% outdoor"]
["BS Antenna Configuration"," Companies need to report which option(s) are used between\n- 32 ports: (8,8,2,1,1,2,8), (dH,dV) = (0.5, 0.8)λ\n- 16 ports: (8,4,2,1,1,2,4), (dH,dV) = (0.5, 0.8)λ\nOther configurations are not precluded.","16 ports: (8,4,2,1,1,2,4), (dH,dV) = (0.5, 0.8)λ","32 ports: (8,8,2,1,1,2,8), (dH,dV) = (0.5, 0.8)λ",null,"32 ports: (8,8,2,1,1,2,8), (dH,dV) = (0.5, 0.8)λ","32 ports: (8,8,2,1,1,2,8), (dH,dV) = (0.5, 0.8)λ","32 ports: (8,8,2,1,1,2,8), (dH,dV) = (0.5, 0.8)λ\n"]
["BS Antenna radiation pattern","3-sector antenna radiation pattern, 8 dBi"]
["UE Antenna Configuration","4RX: (1,2,2,1,1,1,2), (dH,dV) = (0.5, 0.5)λ for (rank 1-4)\n2RX: (1,1,2,1,1,1,1), (dH,dV) = (0.5, 0.5)λ for (rank 1,2)\nOther configuration is not precluded.","2RX: (1,1,2,1,1,1,1), (dH,dV) = (0.5, 0.5)λ for (rank 1,2)","2RX: (1,1,2,1,1,1,1), (dH,dV) = (0.5, 0.5)λ for (rank 1,2)",null,"4RX: (1,2,2,1,1,1,2), (dH,dV) = (0.5, 0.5)λ for (rank 1-4)","4RX: (1,2,2,1,1,1,2), (dH,dV) = (0.5, 0.5)λ for (rank 1-4)","2RX: (1,1,2,1,1,1,1), (dH,dV) = (0.5, 0.5)λ \n"]
["UE Antenna radiation pattern","Omni-direction"]
["BS Tx Power","44dBm"]
["Maximum UE Tx Power","23 dBm"]
["BS receiver Noise Figure","5 dB"]
["UE receiver Noise Figure","9 dB"]
["Inter site distance","500m ISD for FR1"]
["BS Antenna height","25m"]
["UE Antenna height","1.5 m"]
["UE trajectory model","Option #1, Option #2, or option #3\nReported by companies","Option1","Option 3","Option1","Option1","Option1","Option1","Option3"]
["UE trajectory boundary processing","Option #1, Option #2, or option #3 \nReported by companies","Option2","Option 3","Option2","Option1","Option3","Option2","Option3"]
["L1/L3 filtering","Option #Sliding, Option #Non-sliding\nReported by companies","Option #Non-sliding","No-sliding","both","Non-sliding","both","Option1","Sliding"]
["measurement period","200ms"]
["FilterCoefficient",4]
["Number of Tx beams","Reported by companies",4,4,1,4,1,1,1]
["Number of Rx beams","Reported by companies",1,1,1,1,1,1,1]

{"sheet":"KPIs","index":1,"n_rows":2,"n_cols":5,"rows_kept":2,"cut":false,"hidden":false,"merged":[]}
["Intermediate KPIs","Description/Definition","NTT DOCOMO","Mediatek","Samsung"]
["Average L3 cell RSRP difference  (dB)","Average L3 RSRP difference between predicted and ideal L3 cell-level measurement result","Method: Average cross multiple cells","Method: Average cross multiple cells","Method: Average cross multiple cells (i.e., serving cell + 1st-tier 6 neighbor cells)"]

{"sheet":"Results","index":2,"n_rows":259,"n_cols":25,"rows_kept":259,"cut":false,"hidden":false,"merged":[[0,0,0,2],[0,3,0,5],[0,6,0,14],[0,15,0,23]]}
["General",null,null,"Variable Settings",null,null,"Configurable/Selectable Simulation Assumption",null,null,null,null,null,null,null,null,"Model Related Information",null,null,null,null,null,null,null,null,"Performance Metrics"]
["Company","Sub case","Other factors","Observation window\n(ms)","Channel correlation coefficient between two frequency layers","UE speed\n(km/h)","Spatial consistency","Whether LOSsoft is modeled or not","Inter-frequency correlation ","Inter-frequency shadow fading correlation","UE trajectory model","UE trajectory boundary processing","L1/L3 filtering\n(Sliding/Non-sliding)","Number of Tx beams","Number of Rx beams","Model input","Model output/label","Model type","Detail of model","Model complexity\nin a number of model parameters (K)","Model complexity\nin a number of model size (KByte)","Computational complexity [FLOPs] (M)","Training data size in number of samples (K)","Testing data size in number of samples (K)","Average L3 cell RSRP difference (dB)"]
["Name","1/2/3","Additional consideration\n(e.g. 2G->4G/4G->2G, Cell/Cluster-based)","XX"," PCC (Pearson Correlation Coefficient)[TBD]","XX","A/B","YES/NO","YES/NO","FULL/PARTIAL/NO","1/2/3","1/2/3","Sliding/Non-sliding","XX","XX","Number of cell(s),\nMesurement quantity (L1 beam-level, L1-filterd beam-level, L3 cell-level, L3 beam-level measurement results)","Number of cell(s),\nMesurement quantity(L1 beam-level, L1-filterd beam-level, L3 cell-level, L3 beam-level measurement results)","AI/Non-AI: Method (e.g. RNN,CNN, Sample and hold, Decision tree)","e.g.,model structure and description","XX","XX","XX","XX","XX","XX"]
["CATT",2,"2G->4G, Cluster-based",200,0.99,0,"A ","YES","NO","FULL",1,2,"Non-sliding",4,1,"21 cells,  L3 cell-level RSRP ","21 cells, L3 cell-level RSRP","AI: ResNet","1 layers of AI: ResNet layer and 1 DNN layer",17.041,66.56,0.28599999999999998,13,1.625,0.20830000000000001]
["CATT",2,"2G->4G, Cluster-based",200,0.99,90,"A ","YES","NO","FULL",1,2,"Non-sliding",4,1,"21 cells,  L3 cell-level RSRP ","21 cells, L3 cell-level RSRP","AI: ResNet","1 layers of AI: ResNet layer and 1 DNN layer",17.041,66.56,0.28599999999999998,13,1.625,0.2056]
["CATT",2,"4G->2G, Cluster-based",200,0.99,0,"A ","YES","NO","FULL",1,2,"Non-sliding",4,1,"21 cells,  L3 cell-level RSRP ","21 cells, L3 cell-level RSRP","AI: ResNet","1 layers of AI: ResNet layer and 1 DNN layer",17.041,66.56,0.28599999999999998,13,1.625,0.1963]
["CATT",2,"4G->2G, Cluster-based",200,0.99,90,"A ","YES","NO","FULL",1,2,"Non-sliding",4,1,"21 cells,  L3 cell-level RSRP ","21 cells, L3 cell-level RSRP","AI: ResNet","1 layers of AI: ResNet layer and 1 DNN layer",17.041,66.56,0.28599999999999998,13,1.625,0.19969999999999999]
["NTT DOCOMO",1,"2G->4G, Cluster-based",200,null,90,"A ","No","YES","FULL",3,3,"Non-sliding",4,1,"7 cells, L1 beam-level RSRP ","7 cells, L1 beam-level RSRP ","AI: Transformer",null,null,null,null,null,null,1.5]
["NTT DOCOMO",2,"2G->4G, Cluster-based",200,null,90,"A ","No","YES","FULL",3,3,"Non-sliding",4,1,"7 cells,  L3 cell-level RSRP ","7 cells,  L3 cell-level RSRP ","AI: Transformer",null,null,null,null,null,null,0.7]
["NTT DOCOMO",3,"2G->4G, Cluster-based",200,null,90,"A ","No","YES","FULL",3,3,"Non-sliding",4,1,"7 cells, L1 beam-level RSRP ","7 cells,  L3 cell-level RSRP ","AI: Transformer",null,null,null,null,null,null,0.6]
["NTT DOCOMO","/","2G->4G, Cluster-based",200,null,90,"A ","No","YES","FULL",3,3,"Non-sliding",4,1,"L3 cell-level RSRP","L3 cell-level RSRP","Non-AI: RSRP offset",null,"/","/","/","/","/",0.8]
["NTT DOCOMO",1,"4G->2G, Cluster-based",200,null,90,"A ","No","YES","FULL",3,3,"Non-sliding",4,1,"7 cells, L1 beam-level RSRP ","7 cells, L1 beam-level RSRP ","AI: Transformer",null,null,null,null,null,null,1.4]
["NTT DOCOMO",2,"4G->2G, Cluster-based",200,null,90,"A ","No","YES","FULL",3,3,"Non-sliding",4,1,"7 cells,  L3 cell-level RSRP ","7 cells,  L3 cell-level RSRP ","AI: Transformer",null,null,null,null,null,null,0.7]
["NTT DOCOMO",3,"4G->2G, Cluster-based",200,null,90,"A ","No","YES","FULL",3,3,"Non-sliding",4,1,"7 cells, L1 beam-level RSRP ","7 cells,  L3 cell-level RSRP ","AI: Transformer",null,null,null,null,null,null,0.6]
["NTT DOCOMO","/","4G->2G, Cluster-based",200,null,90,"A ","No","YES","FULL",3,3,"Non-sliding",4,1,"L3 cell-level RSRP","L3 cell-level RSRP","Non-AI: RSRP offset",null,"/","/","/","/","/",0.8]
["Ericsson","2","2G->4G, Cell based, L3 Cell-Level Input, and L3 Cell-Level Output, Cluster\nUMA, No-Sorting","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"15 cells, L3 Cell-Level RSRP","15 cells, L3 Cell-Level RSRP","xgboost","1000 estimators, max_depth=7",292,"7300.0 KB",51,29576,7394,0.11517659007306599]
["Ericsson","2","2G->4G, Cell based, L3 Cell-Level Input, and L3 Cell-Level Output, Cluster\nUMA, No-Sorting","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"9 cells, L3 Cell-Level RSRP","9 cells, L3 Cell-Level RSRP","xgboost","1001 estimators, max_depth=7",293,"7300.0 KB",52,29576,7394,0.130937553295253]
["Ericsson","2","2G->4G, Cell based, L3 Cell-Level Input, and L3 Cell-Level Output, Cluster\nUMA, No-Sorting","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"3 cells, L3 Cell-Level RSRP","3 cells, L3 Cell-Level RSRP","xgboost","1002 estimators, max_depth=7",294,"7300.0 KB",53,29576,7394,0.33332163879553101]
["Ericsson","2","2G->4G, Cell based, L3 Cell-Level Input, and L3 Cell-Level Output, Cluster\nUMA, No-Sorting","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"2 cells, L3 Cell-Level RSRP","2 cells, L3 Cell-Level RSRP","xgboost","1003 estimators, max_depth=7",295,"7300.0 KB",54,29576,7394,0.68420230176056196]
["Ericsson","2","2G->4G, Cell based, L3 Cell-Level Input, and L3 Cell-Level Output, Cluster\nUMI, No-Sorting","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"15 cells, L3 Cell-Level RSRP","15 cells, L3 Cell-Level RSRP","xgboost","1004 estimators, max_depth=7",296,"7300.0 KB",55,29576,7394,0.16096127765593099]
["Ericsson","2","2G->4G, Cell based, L3 Cell-Level Input, and L3 Cell-Level Output, Cluster\nUMI, No-Sorting","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"9 cells, L3 Cell-Level RSRP","9 cells, L3 Cell-Level RSRP","xgboost","1005 estimators, max_depth=7",297,"7300.0 KB",56,29576,7394,0.18591691584367501]
["Ericsson","2","2G->4G, Cell based, L3 Cell-Level Input, and L3 Cell-Level Output, Cluster\nUMI, No-Sorting","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"3 cells, L3 Cell-Level RSRP","3 cells, L3 Cell-Level RSRP","xgboost","1006 estimators, max_depth=7",298,"7300.0 KB",57,29576,7394,0.52836864176561804]
["Ericsson","2","2G->4G, Cell based, L3 Cell-Level Input, and L3 Cell-Level Output, Cluster\nUMI, No-Sorting","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"2 cells, L3 Cell-Level RSRP","2 cells, L3 Cell-Level RSRP","xgboost","1007 estimators, max_depth=7",299,"7300.0 KB",58,29576,7394,0.91597266031027802]
["Ericsson","2","2G->4G, Cell based, L3 Cell-Level Input, and L3 Cell-Level Output, Cluster\nUMI, Sorting","XX","xx",30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"15 cells, L3 Cell-Level RSRP","15 cells, L3 Cell-Level RSRP","xgboost","1008 estimators, max_depth=7",300,"7300.0 KB",59,29576,7394,0.169696054757279]
["Ericsson","2","2G->4G, Cell based, L3 Cell-Level Input, and L3 Cell-Level Output, Cluster\nUMI, Sorting","XX","xx",30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"9 cells, L3 Cell-Level RSRP","9 cells, L3 Cell-Level RSRP","xgboost","1009 estimators, max_depth=7",301,"7300.0 KB",60,29576,7394,0.20155992086889701]
["Ericsson","2","2G->4G, Cell based, L3 Cell-Level Input, and L3 Cell-Level Output, Cluster\nUMI, Sorting","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"3 cells, L3 Cell-Level RSRP","3 cells, L3 Cell-Level RSRP","xgboost","1010 estimators, max_depth=7",302,"7300.0 KB",61,29576,7394,0.70560260677870401]
["Ericsson","2","2G->4G, Cell based, L3 Cell-Level Input, and L3 Cell-Level Output, Cluster\nUMI, Sorting","XX",0.8,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"2 cells, L3 Cell-Level RSRP","2 cells, L3 Cell-Level RSRP","xgboost","1011 estimators, max_depth=7",303,"7300.0 KB",62,29576,7394,1.32845686219984]
["Ericsson","2","2G->4G, Cell based, L3 Cell-Level Input, and L3 Cell-Level Output, Cluster\nUMA, Sorting","XX","xx",30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"15 cells, L3 Cell-Level RSRP","15 cells, L3 Cell-Level RSRP","xgboost","1012 estimators, max_depth=7",304,"7300.0 KB",63,29576,7394,0.114410424249013]
["Ericsson","2","2G->4G, Cell based, L3 Cell-Level Input, and L3 Cell-Level Output, Cluster\nUMA, Sorting","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"9 cells, L3 Cell-Level RSRP","9 cells, L3 Cell-Level RSRP","xgboost","1013 estimators, max_depth=7",305,"7300.0 KB",64,29576,7394,0.13266735898548601]
["Ericsson","2","2G->4G, Cell based, L3 Cell-Level Input, and L3 Cell-Level Output, Cluster\nUMA, Sorting","XX",0.8,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"3 cells, L3 Cell-Level RSRP","3 cells, L3 Cell-Level RSRP","xgboost","1014 estimators, max_depth=7",306,"7300.0 KB",65,29576,7394,0.39903812841014502]
["Ericsson","2","2G->4G, Cell based, L3 Cell-Level Input, and L3 Cell-Level Output, Cluster\nUMA, Sorting","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"2 cells, L3 Cell-Level RSRP","2 cells, L3 Cell-Level RSRP","xgboost","1015 estimators, max_depth=7",307,"7300.0 KB",66,29576,7394,0.85526567625677996]
["Ericsson","2","2G->4G, Cell based, L3 Cell-Level Input, and L3 Cell-Level Output, Cluster\nUMI, Sorting","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"21 cells, L3 Cell-Level RSRP","21 cells, L3 Cell-Level RSRP","xgboost","1016 estimators, max_depth=7",308,"7300.0 KB",66,29576,7394,0.155432302804103]
["Ericsson","2","2G->4G, Cell based, L3 Cell-Level Input, and L3 Cell-Level Output, Cluster\nUMI, Sorting","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"18 cells, L3 Cell-Level RSRP","21 cells, L3 Cell-Level RSRP","xgboost","1017 estimators, max_depth=7",309,"7300.0 KB",66,29576,7394,0.18573405961561301]
["Ericsson","2","2G->4G, Cell based, L3 Cell-Level Input, and L3 Cell-Level Output, Cluster\nUMI, Sorting","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"15 cells, L3 Cell-Level RSRP","21 cells, L3 Cell-Level RSRP","xgboost","1018 estimators, max_depth=7",310,"7300.0 KB",66,29576,7394,0.22148113871681499]
["Ericsson","2","2G->4G, Cell based, L3 Cell-Level Input, and L3 Cell-Level Output, Cluster\nUMI, Sorting","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"12 cells, L3 Cell-Level RSRP","21 cells, L3 Cell-Level RSRP","xgboost","1019 estimators, max_depth=7",311,"7300.0 KB",66,29576,7394,0.26676838760496902]
["Ericsson","2","2G->4G, Cell based, L3 Cell-Level Input, and L3 Cell-Level Output, Cluster\nUMI, Sorting","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"9 cells, L3 Cell-Level RSRP","21 cells, L3 Cell-Level RSRP","xgboost","1020 estimators, max_depth=7",312,"7300.0 KB",66,29576,7394,0.34626000294352599]
["Ericsson","2","2G->4G, Cell based, L3 Cell-Level Input, and L3 Cell-Level Output, Cluster\nUMI, Sorting","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"6 cells, L3 Cell-Level RSRP","21 cells, L3 Cell-Level RSRP","xgboost","1021 estimators, max_depth=7",313,"7300.0 KB",66,29576,7394,0.57727796740488502]
["Ericsson","2","2G->4G, Cell based, L3 Cell-Level Input, and L3 Cell-Level Output, Cluster\nUMI, Sorting","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"3 cells, L3 Cell-Level RSRP","21 cells, L3 Cell-Level RSRP","xgboost","1022 estimators, max_depth=7",314,"7300.0 KB",66,29576,7394,2.16559787394544]
["Ericsson","2","2G->4G, Cell based, L3 Cell-Level Input, and L3 Cell-Level Output, Cluster\nUMI, Sorting","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"1 cells, L3 Cell-Level RSRP","21 cells, L3 Cell-Level RSRP","xgboost","1023 estimators, max_depth=7",315,"7300.0 KB",66,29576,7394,7.7488877578414401]
["Ericsson","2","2G->4G, Cell based, L3 Cell-Level Input, and L3 Cell-Level Output, Cluster\nUMA, Sorting","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"21 cells, L3 Cell-Level RSRP","21 cells, L3 Cell-Level RSRP","xgboost","1024 estimators, max_depth=7",316,"7300.0 KB",66,29576,7394,0.10820612095531799]
["Ericsson","2","2G->4G, Cell based, L3 Cell-Level Input, and L3 Cell-Level Output, Cluster\nUMA, Sorting","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"18 cells, L3 Cell-Level RSRP","21 cells, L3 Cell-Level RSRP","xgboost","1025 estimators, max_depth=7",317,"7300.0 KB",66,29576,7394,0.12208984343919101]
["Ericsson","2","2G->4G, Cell based, L3 Cell-Level Input, and L3 Cell-Level Output, Cluster\nUMA, Sorting","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"15 cells, L3 Cell-Level RSRP","21 cells, L3 Cell-Level RSRP","xgboost","1026 estimators, max_depth=7",318,"7300.0 KB",66,29576,7394,0.13798217610348701]
["Ericsson","2","2G->4G, Cell based, L3 Cell-Level Input, and L3 Cell-Level Output, Cluster\nUMA, Sorting","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"12 cells, L3 Cell-Level RSRP","21 cells, L3 Cell-Level RSRP","xgboost","1027 estimators, max_depth=7",319,"7300.0 KB",66,29576,7394,0.161024431024748]
["Ericsson","2","2G->4G, Cell based, L3 Cell-Level Input, and L3 Cell-Level Output, Cluster\nUMA, Sorting","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"9 cells, L3 Cell-Level RSRP","21 cells, L3 Cell-Level RSRP","xgboost","1028 estimators, max_depth=7",320,"7300.0 KB",66,29576,7394,0.19573451724901]
["Ericsson","2","2G->4G, Cell based, L3 Cell-Level Input, and L3 Cell-Level Output, Cluster\nUMA, Sorting","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"6 cells, L3 Cell-Level RSRP","21 cells, L3 Cell-Level RSRP","xgboost","1029 estimators, max_depth=7",321,"7300.0 KB",66,29576,7394,0.28814867497466901]
["Ericsson","2","2G->4G, Cell based, L3 Cell-Level Input, and L3 Cell-Level Output, Cluster\nUMA, Sorting","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"3 cells, L3 Cell-Level RSRP","21 cells, L3 Cell-Level RSRP","xgboost","1030 estimators, max_depth=7",322,"7300.0 KB",66,29576,7394,1.13214804991316]
["Ericsson","2","2G->4G, Cell based, L3 Cell-Level Input, and L3 Cell-Level Output, Cluster\nUMA, Sorting","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"1 cells, L3 Cell-Level RSRP","21 cells, L3 Cell-Level RSRP","xgboost","1031 estimators, max_depth=7",323,"7300.0 KB",66,29576,7394,7.4034816212225598]
["Ericsson","2","2G->4G, Cell based, L3 Cell-Level Input, and L3 Cell-Level Output, Cluster\nUMA, No-Sorting","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"21 cells, L3 Cell-Level RSRP","21 cells, L3 Cell-Level RSRP","xgboost","1032 estimators, max_depth=7",324,"7300.0 KB",66,29576,7394,0.10681541087077701]
["Ericsson","2","2G->4G, Cell based, L3 Cell-Level Input, and L3 Cell-Level Output, Cluster\nUMA, No-Sorting","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"18 cells, L3 Cell-Level RSRP","21 cells, L3 Cell-Level RSRP","xgboost","1033 estimators, max_depth=7",325,"7300.0 KB",66,29576,7394,0.11789612641486601]
["Ericsson","2","2G->4G, Cell based, L3 Cell-Level Input, and L3 Cell-Level Output, Cluster\nUMA, No-Sorting","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"15 cells, L3 Cell-Level RSRP","21 cells, L3 Cell-Level RSRP","xgboost","1034 estimators, max_depth=7",326,"7300.0 KB",66,29576,7394,0.13063744165761401]
["Ericsson","2","2G->4G, Cell based, L3 Cell-Level Input, and L3 Cell-Level Output, Cluster\nUMA, No-Sorting","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"12 cells, L3 Cell-Level RSRP","21 cells, L3 Cell-Level RSRP","xgboost","1035 estimators, max_depth=7",327,"7300.0 KB",66,29576,7394,0.15279757020573101]
["Ericsson","2","2G->4G, Cell based, L3 Cell-Level Input, and L3 Cell-Level Output, Cluster\nUMA, No-Sorting","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"9 cells, L3 Cell-Level RSRP","21 cells, L3 Cell-Level RSRP","xgboost","1036 estimators, max_depth=7",328,"7300.0 KB",66,29576,7394,0.18065584184543099]
["Ericsson","2","2G->4G, Cell based, L3 Cell-Level Input, and L3 Cell-Level Output, Cluster\nUMA, No-Sorting","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"6 cells, L3 Cell-Level RSRP","21 cells, L3 Cell-Level RSRP","xgboost","1037 estimators, max_depth=7",329,"7300.0 KB",66,29576,7394,0.25441615680483798]
["Ericsson","2","2G->4G, Cell based, L3 Cell-Level Input, and L3 Cell-Level Output, Cluster\nUMA, No-Sorting","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"3 cells, L3 Cell-Level RSRP","21 cells, L3 Cell-Level RSRP","xgboost","1038 estimators, max_depth=7",330,"7300.0 KB",66,29576,7394,0.92351079261600999]
["Ericsson","2","2G->4G, Cell based, L3 Cell-Level Input, and L3 Cell-Level Output, Cluster\nUMA, No-Sorting","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"1 cells, L3 Cell-Level RSRP","21 cells, L3 Cell-Level RSRP","xgboost","1039 estimators, max_depth=7",331,"7300.0 KB",66,29576,7394,8.0246495016706891]
["Ericsson","2","2G->4G, Cell based, L3 Cell-Level Input, and L3 Cell-Level Output, Cluster\nUMI, No-Sorting","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"21 cells, L3 Cell-Level RSRP","21 cells, L3 Cell-Level RSRP","xgboost","1040 estimators, max_depth=7",332,"7300.0 KB",66,29576,7394,0.151781208951592]
["Ericsson","2","2G->4G, Cell based, L3 Cell-Level Input, and L3 Cell-Level Output, Cluster\nUMI, No-Sorting","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"18 cells, L3 Cell-Level RSRP","21 cells, L3 Cell-Level RSRP","xgboost","1041 estimators, max_depth=7",333,"7300.0 KB",66,29576,7394,0.17324718810775899]
["Ericsson","2","2G->4G, Cell based, L3 Cell-Level Input, and L3 Cell-Level Output, Cluster\nUMI, No-Sorting","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"15 cells, L3 Cell-Level RSRP","21 cells, L3 Cell-Level RSRP","xgboost","1042 estimators, max_depth=7",334,"7300.0 KB",66,29576,7394,0.20779717031664099]
["Ericsson","2","2G->4G, Cell based, L3 Cell-Level Input, and L3 Cell-Level Output, Cluster\nUMI, No-Sorting","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"12 cells, L3 Cell-Level RSRP","21 cells, L3 Cell-Level RSRP","xgboost","1042 estimators, max_depth=7",334,"7300.0 KB",66,29576,7394,0.25688945510004402]
["Ericsson","2","2G->4G, Cell based, L3 Cell-Level Input, and L3 Cell-Level Output, Cluster\nUMI, No-Sorting","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"9 cells, L3 Cell-Level RSRP","21 cells, L3 Cell-Level RSRP","xgboost","1042 estimators, max_depth=7",334,"7300.0 KB",66,29576,7394,0.31743852387079702]
["Ericsson","2","2G->4G, Cell based, L3 Cell-Level Input, and L3 Cell-Level Output, Cluster\nUMI, No-Sorting","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"6 cells, L3 Cell-Level RSRP","21 cells, L3 Cell-Level RSRP","xgboost","1042 estimators, max_depth=7",334,"7300.0 KB",66,29576,7394,0.49013040082743697]
["Ericsson","2","2G->4G, Cell based, L3 Cell-Level Input, and L3 Cell-Level Output, Cluster\nUMI, No-Sorting","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"3 cells, L3 Cell-Level RSRP","21 cells, L3 Cell-Level RSRP","xgboost","1042 estimators, max_depth=7",334,"7300.0 KB",66,29576,7394,2.0248247660772898]
["Ericsson","2","2G->4G, Cell based, L3 Cell-Level Input, and L3 Cell-Level Output, Cluster\nUMI, No-Sorting","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"1 cells, L3 Cell-Level RSRP","21 cells, L3 Cell-Level RSRP","xgboost","1042 estimators, max_depth=7",334,"7300.0 KB",66,29576,7394,8.1592697564270296]
["Ericsson","2","2G->4G, Cell based, L3 Cell-Level Input, and L3 Cell-Level Output, Cluster\nUMI, No-Sorting","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"21 cells, L3 Cell-Level RSRP","4 cells, L3 Cell-Level RSRP","xgboost","1042 estimators, max_depth=7",334,"7300.0 KB",66,29576,7394,0.14579257414466901]
["Ericsson","2","2G->4G, Cell based, L3 Cell-Level Input, and L3 Cell-Level Output, Cluster\nUMI, No-Sorting","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"15 cells, L3 Cell-Level RSRP","4 cells, L3 Cell-Level RSRP","xgboost","1042 estimators, max_depth=7",334,"7300.0 KB",66,29576,7394,0.15842586683160101]
["Ericsson","2","2G->4G, Cell based, L3 Cell-Level Input, and L3 Cell-Level Output, Cluster\nUMI, No-Sorting","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"12 cells, L3 Cell-Level RSRP","4 cells, L3 Cell-Level RSRP","xgboost","1042 estimators, max_depth=7",334,"7300.0 KB",66,29576,7394,0.16685800102757301]
["Ericsson","2","2G->4G, Cell based, L3 Cell-Level Input, and L3 Cell-Level Output, Cluster\nUMI, No-Sorting","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"9 cells, L3 Cell-Level RSRP","4 cells, L3 Cell-Level RSRP","xgboost","1042 estimators, max_depth=7",334,"7300.0 KB",66,29576,7394,0.18308544006212299]
["Ericsson","2","2G->4G, Cell based, L3 Cell-Level Input, and L3 Cell-Level Output, Cluster\nUMI, No-Sorting","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"6 cells, L3 Cell-Level RSRP","4 cells, L3 Cell-Level RSRP","xgboost","1042 estimators, max_depth=7",334,"7300.0 KB",66,29576,7394,0.22876262595411201]
["Ericsson","2","2G->4G, Cell based, L3 Cell-Level Input, and L3 Cell-Level Output, Cluster\nUMI, No-Sorting","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"3 cells, L3 Cell-Level RSRP","4 cells, L3 Cell-Level RSRP","xgboost","1042 estimators, max_depth=7",334,"7300.0 KB",66,29576,7394,1.01550134122363]
["Ericsson","2","2G->4G, Cell based, L3 Cell-Level Input, and L3 Cell-Level Output, Cluster\nUMI, No-Sorting","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"1 cells, L3 Cell-Level RSRP","4 cells, L3 Cell-Level RSRP","xgboost","1042 estimators, max_depth=7",334,"7300.0 KB",66,29576,7394,5.9548121949673698]
["Ericsson","2","2G->4G, Cell based, L3 Cell-Level Input, and L3 Cell-Level Output, Cluster\nUMA, No-Sorting","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"21 cells, L3 Cell-Level RSRP","4 cells, L3 Cell-Level RSRP","xgboost","1042 estimators, max_depth=7",334,"7300.0 KB",66,29576,7394,0.110673439387247]
["Ericsson","2","2G->4G, Cell based, L3 Cell-Level Input, and L3 Cell-Level Output, Cluster\nUMA, No-Sorting","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"15 cells, L3 Cell-Level RSRP","4 cells, L3 Cell-Level RSRP","xgboost","1042 estimators, max_depth=7",334,"7300.0 KB",66,29576,7394,0.116784678237638]
["Ericsson","2","2G->4G, Cell based, L3 Cell-Level Input, and L3 Cell-Level Output, Cluster\nUMA, No-Sorting","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"12 cells, L3 Cell-Level RSRP","4 cells, L3 Cell-Level RSRP","xgboost","1042 estimators, max_depth=7",334,"7300.0 KB",66,29576,7394,0.12320423947242699]
["Ericsson","2","2G->4G, Cell based, L3 Cell-Level Input, and L3 Cell-Level Output, Cluster\nUMA, No-Sorting","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"9 cells, L3 Cell-Level RSRP","4 cells, L3 Cell-Level RSRP","xgboost","1042 estimators, max_depth=7",334,"7300.0 KB",66,29576,7394,0.13323763857318399]
["Ericsson","2","2G->4G, Cell based, L3 Cell-Level Input, and L3 Cell-Level Output, Cluster\nUMA, No-Sorting","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"6 cells, L3 Cell-Level RSRP","4 cells, L3 Cell-Level RSRP","xgboost","1042 estimators, max_depth=7",334,"7300.0 KB",66,29576,7394,0.15585987112446001]
["Ericsson","2","2G->4G, Cell based, L3 Cell-Level Input, and L3 Cell-Level Output, Cluster\nUMA, No-Sorting","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"3 cells, L3 Cell-Level RSRP","4 cells, L3 Cell-Level RSRP","xgboost","1042 estimators, max_depth=7",334,"7300.0 KB",66,29576,7394,0.51687861971308502]
["Ericsson","2","2G->4G, Cell based, L3 Cell-Level Input, and L3 Cell-Level Output, Cluster\nUMA, No-Sorting","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"1 cells, L3 Cell-Level RSRP","4 cells, L3 Cell-Level RSRP","xgboost","1042 estimators, max_depth=7",334,"7300.0 KB",66,29576,7394,6.3944778196762702]
["Ericsson","2","2G->4G, Cell based, L3 Cell-Level Input, and L3 Cell-Level Output, Cluster\nUMA, Sorting","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"15 cells, L3 Cell-Level RSRP","4 cells, L3 Cell-Level RSRP","xgboost","1042 estimators, max_depth=7",334,"7300.0 KB",66,29576,7394,0.113582861913189]
["Ericsson","2","2G->4G, Cell based, L3 Cell-Level Input, and L3 Cell-Level Output, Cluster\nUMA, Sorting","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"12 cells, L3 Cell-Level RSRP","4 cells, L3 Cell-Level RSRP","xgboost","1042 estimators, max_depth=7",334,"7300.0 KB",66,29576,7394,0.11691761473553899]
["Ericsson","2","2G->4G, Cell based, L3 Cell-Level Input, and L3 Cell-Level Output, Cluster\nUMA, Sorting","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"6 cells, L3 Cell-Level RSRP","4 cells, L3 Cell-Level RSRP","xgboost","1042 estimators, max_depth=7",334,"7300.0 KB",66,29576,7394,0.154988526366962]
["Ericsson","2","2G->4G, Cell based, L3 Cell-Level Input, and L3 Cell-Level Output, Cluster\nUMA, Sorting","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"3 cells, L3 Cell-Level RSRP","4 cells, L3 Cell-Level RSRP","xgboost","1042 estimators, max_depth=7",334,"7300.0 KB",66,29576,7394,0.52697060361563797]
["Ericsson","2","2G->4G, Cell based, L3 Cell-Level Input, and L3 Cell-Level Output, Cluster\nUMA, Sorting","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"1 cells, L3 Cell-Level RSRP","4 cells, L3 Cell-Level RSRP","xgboost","1042 estimators, max_depth=7",334,"7300.0 KB",66,29576,7394,5.5441028068592004]
["Ericsson","2","2G->4G, Cell based, L3 Cell-Level Input, and L3 Cell-Level Output, Cluster\nUMI, Sorting","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"21 cells, L3 Cell-Level RSRP","4 cells, L3 Cell-Level RSRP","xgboost","1042 estimators, max_depth=7",334,"7300.0 KB",66,29576,7394,0.16400902957043401]
["Ericsson","2","2G->4G, Cell based, L3 Cell-Level Input, and L3 Cell-Level Output, Cluster\nUMI, Sorting","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"12 cells, L3 Cell-Level RSRP","4 cells, L3 Cell-Level RSRP","xgboost","1042 estimators, max_depth=7",334,"7300.0 KB",66,29576,7394,0.18838683116807201]
["Ericsson","2","2G->4G, Cell based, L3 Cell-Level Input, and L3 Cell-Level Output, Cluster\nUMI, Sorting","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"9 cells, L3 Cell-Level RSRP","4 cells, L3 Cell-Level RSRP","xgboost","1042 estimators, max_depth=7",334,"7300.0 KB",66,29576,7394,0.212022762080009]
["Ericsson","2","2G->4G, Cell based, L3 Cell-Level Input, and L3 Cell-Level Output, Cluster\nUMI, Sorting","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"6 cells, L3 Cell-Level RSRP","4 cells, L3 Cell-Level RSRP","xgboost","1042 estimators, max_depth=7",334,"7300.0 KB",66,29576,7394,0.27585003513865702]
["Ericsson","2","2G->4G, Cell based, L3 Cell-Level Input, and L3 Cell-Level Output, Cluster\nUMI, Sorting","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"3 cells, L3 Cell-Level RSRP","4 cells, L3 Cell-Level RSRP","xgboost","1042 estimators, max_depth=7",334,"7300.0 KB",66,29576,7394,0.91360984343004503]
["Ericsson","2","2G->4G, Cell based, L3 Cell-Level Input, and L3 Cell-Level Output, Cluster\nUMI, Sorting","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"1 cells, L3 Cell-Level RSRP","4 cells, L3 Cell-Level RSRP","xgboost","1042 estimators, max_depth=7",334,"7300.0 KB",66,29576,7394,6.5353789319017297]
["Ericsson","2","2G->4G, Cell based, L3 Cell-Level Input, and L3 Cell-Level Output, Cluster\nUMI, Sorting","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"11 cells, L3 Cell-Level RSRP","5 cells, L3 Cell-Level RSRP","xgboost","1042 estimators, max_depth=7",334,"7300.0 KB",66,29576,7394,0.192062404389401]
["Ericsson","2","2G->4G, Cell based, L3 Cell-Level Input, and L3 Cell-Level Output, Cluster\nUMI, Sorting","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"11 cells, L3 Cell-Level RSRP","8 cells, L3 Cell-Level RSRP","xgboost","1042 estimators, max_depth=7",334,"7300.0 KB",66,29576,7394,0.18804551446508899]
["Ericsson","2","2G->4G, Cell based, L3 Cell-Level Input, and L3 Cell-Level Output, Cluster\nUMI, Sorting","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"11 cells, L3 Cell-Level RSRP","10 cells, L3 Cell-Level RSRP","xgboost","1042 estimators, max_depth=7",334,"7300.0 KB",66,29576,7394,0.18573838889284899]
["Ericsson","2","2G->4G, Cell based, L3 Cell-Level Input, and L3 Cell-Level Output, Cluster\nUMI, Sorting","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"11 cells, L3 Cell-Level RSRP","12 cells, L3 Cell-Level RSRP","xgboost","1042 estimators, max_depth=7",334,"7300.0 KB",66,29576,7394,0.19732456777486301]
["Ericsson","2","2G->4G, Cell based, L3 Cell-Level Input, and L3 Cell-Level Output, Cluster\nUMI, Sorting","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"11 cells, L3 Cell-Level RSRP","15 cells, L3 Cell-Level RSRP","xgboost","1042 estimators, max_depth=7",334,"7300.0 KB",66,29576,7394,0.23675772794477301]
["Ericsson","2","2G->4G, Cell based, L3 Cell-Level Input, and L3 Cell-Level Output, Cluster\nUMI, Sorting","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"11 cells, L3 Cell-Level RSRP","17 cells, L3 Cell-Level RSRP","xgboost","1042 estimators, max_depth=7",334,"7300.0 KB",66,29576,7394,0.25523732933846199]
["Ericsson","2","2G->4G, Cell based, L3 Cell-Level Input, and L3 Cell-Level Output, Cluster\nUMI, Sorting","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"11 cells, L3 Cell-Level RSRP","19 cells, L3 Cell-Level RSRP","xgboost","1042 estimators, max_depth=7",334,"7300.0 KB",66,29576,7394,0.27301213606831298]
["Ericsson","2","2G->4G, Cell based, L3 Cell-Level Input, and L3 Cell-Level Output, Cluster\nUMI, Sorting","XX",0.88,30,"B","YES","YES","Partial",3,1,"Sliding",4,1,"11 cells, L3 Cell-Level RSRP","21 cells, L3 Cell-Level RSRP","xgboost","1042 estimators, max_depth=7",334,"7300.0 KB",66,29576,7394,0.28455242221335397]
["Huawei",2,"2G->4G, Cell-based",200,0.9,30,"B","NO","NO","NO",1,1,"Non-sliding",4,1,"1 cell,  L3 cell-level RSRP ","1 cell,  L3 cell-level RSRP ","AI: LSTM","3 LSTM layers and 1 full-connectivity layer",80,350,1.03,30,0.5,0.52]
["Huawei",2,"2G->4G, Cell-based",400,0.9,30,"B","NO","NO","NO",1,1,"Non-sliding",4,1,"1 cell,  L3 cell-level RSRP ","1 cell,  L3 cell-level RSRP ","AI: LSTM","3 LSTM layers and 1 full-connectivity layer",80,350,1.03,30,0.5,0.53]
["Huawei",2,"2G->4G, Cell-based",600,0.9,30,"B","NO","NO","NO",1,1,"Non-sliding",4,1,"1 cell,  L3 cell-level RSRP ","1 cell,  L3 cell-level RSRP ","AI: LSTM","3 LSTM layers and 1 full-connectivity layer",80,350,1.03,30,0.5,0.54]
["Huawei",2,"2G->4G, Cell-based",800,0.9,30,"B","NO","NO","NO",1,1,"Non-sliding",4,1,"1 cell,  L3 cell-level RSRP ","1 cell,  L3 cell-level RSRP ","AI: LSTM","3 LSTM layers and 1 full-connectivity layer",80,350,1.03,30,0.5,0.59]
["Huawei",2,"2G->4G, Cell-based",1000,0.9,30,"B","NO","NO","NO",1,1,"Non-sliding",4,1,"1 cell,  L3 cell-level RSRP ","1 cell,  L3 cell-level RSRP ","AI: LSTM","3 LSTM layers and 1 full-connectivity layer",80,350,1.03,30,0.5,0.69]
["Huawei",2,"2G->4G, Cell-based",200,0.9,60,"B","NO","NO","NO",1,1,"Non-sliding",4,1,"1 cell,  L3 cell-level RSRP ","1 cell,  L3 cell-level RSRP ","AI: LSTM","3 LSTM layers and 1 full-connectivity layer",80,350,1.03,30,0.5,0.56000000000000005]
["Huawei",2,"2G->4G, Cell-based",400,0.9,60,"B","NO","NO","NO",1,1,"Non-sliding",4,1,"1 cell,  L3 cell-level RSRP ","1 cell,  L3 cell-level RSRP ","AI: LSTM","3 LSTM layers and 1 full-connectivity layer",80,350,1.03,30,0.5,0.57999999999999996]
["Huawei",2,"2G->4G, Cell-based",600,0.9,60,"B","NO","NO","NO",1,1,"Non-sliding",4,1,"1 cell,  L3 cell-level RSRP ","1 cell,  L3 cell-level RSRP ","AI: LSTM","3 LSTM layers and 1 full-connectivity layer",80,350,1.03,30,0.5,0.57999999999999996]
["Huawei",2,"2G->4G, Cell-based",800,0.9,60,"B","NO","NO","NO",1,1,"Non-sliding",4,1,"1 cell,  L3 cell-level RSRP ","1 cell,  L3 cell-level RSRP ","AI: LSTM","3 LSTM layers and 1 full-connectivity layer",80,350,1.03,30,0.5,0.59]
["Huawei",2,"2G->4G, Cell-based",1000,0.9,60,"B","NO","NO","NO",1,1,"Non-sliding",4,1,"1 cell,  L3 cell-level RSRP ","1 cell,  L3 cell-level RSRP ","AI: LSTM","3 LSTM layers and 1 full-connectivity layer",80,350,1.03,30,0.5,0.7]
["Huawei",2,"2G->4G, Cell-based",200,0.9,90,"B","NO","NO","NO",1,1,"Non-sliding",4,1,"1 cell,  L3 cell-level RSRP ","1 cell,  L3 cell-level RSRP ","AI: LSTM","3 LSTM layers and 1 full-connectivity layer",80,350,1.03,30,0.5,0.79]
["Huawei",2,"2G->4G, Cell-based",400,0.9,90,"B","NO","NO","NO",1,1,"Non-sliding",4,1,"1 cell,  L3 cell-level RSRP ","1 cell,  L3 cell-level RSRP ","AI: LSTM","3 LSTM layers and 1 full-connectivity layer",80,350,1.03,30,0.5,0.79]
["Huawei",2,"2G->4G, Cell-based",600,0.9,90,"B","NO","NO","NO",1,1,"Non-sliding",4,1,"1 cell,  L3 cell-level RSRP ","1 cell,  L3 cell-level RSRP ","AI: LSTM","3 LSTM layers and 1 full-connectivity layer",80,350,1.03,30,0.5,0.81]
["Huawei",2,"2G->4G, Cell-based",800,0.9,90,"B","NO","NO","NO",1,1,"Non-sliding",4,1,"1 cell,  L3 cell-level RSRP ","1 cell,  L3 cell-level RSRP ","AI: LSTM","3 LSTM layers and 1 full-connectivity layer",80,350,1.03,30,0.5,0.83]
["Huawei",2,"2G->4G, Cell-based",1000,0.9,90,"B","NO","NO","NO",1,1,"Non-sliding",4,1,"1 cell,  L3 cell-level RSRP ","1 cell,  L3 cell-level RSRP ","AI: LSTM","3 LSTM layers and 1 full-connectivity layer",80,350,1.03,30,0.5,0.86]
["Huawei",2,"2G->4G, Cell-based",200,0.9,120,"B","NO","NO","NO",1,1,"Non-sliding",4,1,"1 cell,  L3 cell-level RSRP ","1 cell,  L3 cell-level RSRP ","AI: LSTM","3 LSTM layers and 1 full-connectivity layer",80,350,1.03,30,0.5,0.82]
["Huawei",2,"2G->4G, Cell-based",400,0.9,120,"B","NO","NO","NO",1,1,"Non-sliding",4,1,"1 cell,  L3 cell-level RSRP ","1 cell,  L3 cell-level RSRP ","AI: LSTM","3 LSTM layers and 1 full-connectivity layer",80,350,1.03,30,0.5,0.85]
["Huawei",2,"2G->4G, Cell-based",600,0.9,120,"B","NO","NO","NO",1,1,"Non-sliding",4,1,"1 cell,  L3 cell-level RSRP ","1 cell,  L3 cell-level RSRP ","AI: LSTM","3 LSTM layers and 1 full-connectivity layer",80,350,1.03,30,0.5,0.86]
["Huawei",2,"2G->4G, Cell-based",800,0.9,120,"B","NO","NO","NO",1,1,"Non-sliding",4,1,"1 cell,  L3 cell-level RSRP ","1 cell,  L3 cell-level RSRP ","AI: LSTM","3 LSTM layers and 1 full-connectivity layer",80,350,1.03,30,0.5,0.89]
["Huawei",2,"2G->4G, Cell-based",1000,0.9,120,"B","NO","NO","NO",1,1,"Non-sliding",4,1,"1 cell,  L3 cell-level RSRP ","1 cell,  L3 cell-level RSRP ","AI: LSTM","3 LSTM layers and 1 full-connectivity layer",80,350,1.03,30,0.5,0.97]
["Huawei",2,"4G->2G, Cell-based",200,0.9,30,"B","NO","NO","NO",1,1,"Non-sliding",4,1,"1 cell,  L3 cell-level RSRP ","1 cell,  L3 cell-level RSRP ","AI: LSTM","3 LSTM layers and 1 full-connectivity layer",80,350,1.03,30,0.5,0.46]
["Huawei",2,"4G->2G, Cell-based",400,0.9,30,"B","NO","NO","NO",1,1,"Non-sliding",4,1,"1 cell,  L3 cell-level RSRP ","1 cell,  L3 cell-level RSRP ","AI: LSTM","3 LSTM layers and 1 full-connectivity layer",80,350,1.03,30,0.5,0.51]
["Huawei",2,"4G->2G, Cell-based",600,0.9,30,"B","NO","NO","NO",1,1,"Non-sliding",4,1,"1 cell,  L3 cell-level RSRP ","1 cell,  L3 cell-level RSRP ","AI: LSTM","3 LSTM layers and 1 full-connectivity layer",80,350,1.03,30,0.5,0.52]
["Huawei",2,"4G->2G, Cell-based",800,0.9,30,"B","NO","NO","NO",1,1,"Non-sliding",4,1,"1 cell,  L3 cell-level RSRP ","1 cell,  L3 cell-level RSRP ","AI: LSTM","3 LSTM layers and 1 full-connectivity layer",80,350,1.03,30,0.5,0.56999999999999995]
["Huawei",2,"4G->2G, Cell-based",1000,0.9,30,"B","NO","NO","NO",1,1,"Non-sliding",4,1,"1 cell,  L3 cell-level RSRP ","1 cell,  L3 cell-level RSRP ","AI: LSTM","3 LSTM layers and 1 full-connectivity layer",80,350,1.03,30,0.5,0.68]
["Huawei",2,"4G->2G, Cell-based",200,0.9,60,"B","NO","NO","NO",1,1,"Non-sliding",4,1,"1 cell,  L3 cell-level RSRP ","1 cell,  L3 cell-level RSRP ","AI: LSTM","3 LSTM layers and 1 full-connectivity layer",80,350,1.03,30,0.5,0.55000000000000004]
["Huawei",2,"4G->2G, Cell-based",400,0.9,60,"B","NO","NO","NO",1,1,"Non-sliding",4,1,"1 cell,  L3 cell-level RSRP ","1 cell,  L3 cell-level RSRP ","AI: LSTM","3 LSTM layers and 1 full-connectivity layer",80,350,1.03,30,0.5,0.56000000000000005]
["Huawei",2,"4G->2G, Cell-based",600,0.9,60,"B","NO","NO","NO",1,1,"Non-sliding",4,1,"1 cell,  L3 cell-level RSRP ","1 cell,  L3 cell-level RSRP ","AI: LSTM","3 LSTM layers and 1 full-connectivity layer",80,350,1.03,30,0.5,0.56999999999999995]
["Huawei",2,"4G->2G, Cell-based",800,0.9,60,"B","NO","NO","NO",1,1,"Non-sliding",4,1,"1 cell,  L3 cell-level RSRP ","1 cell,  L3 cell-level RSRP ","AI: LSTM","3 LSTM layers and 1 full-connectivity layer",80,350,1.03,30,0.5,0.59]
["Huawei",2,"4G->2G, Cell-based",1000,0.9,60,"B","NO","NO","NO",1,1,"Non-sliding",4,1,"1 cell,  L3 cell-level RSRP ","1 cell,  L3 cell-level RSRP ","AI: LSTM","3 LSTM layers and 1 full-connectivity layer",80,350,1.03,30,0.5,0.69]
["Huawei",2,"4G->2G, Cell-based",200,0.9,90,"B","NO","NO","NO",1,1,"Non-sliding",4,1,"1 cell,  L3 cell-level RSRP ","1 cell,  L3 cell-level RSRP ","AI: LSTM","3 LSTM layers and 1 full-connectivity layer",80,350,1.03,30,0.5,0.78]
["Huawei",2,"4G->2G, Cell-based",400,0.9,90,"B","NO","NO","NO",1,1,"Non-sliding",4,1,"1 cell,  L3 cell-level RSRP ","1 cell,  L3 cell-level RSRP ","AI: LSTM","3 LSTM layers and 1 full-connectivity layer",80,350,1.03,30,0.5,0.79]
["Huawei",2,"4G->2G, Cell-based",600,0.9,90,"B","NO","NO","NO",1,1,"Non-sliding",4,1,"1 cell,  L3 cell-level RSRP ","1 cell,  L3 cell-level RSRP ","AI: LSTM","3 LSTM layers and 1 full-connectivity layer",80,350,1.03,30,0.5,0.82]
["Huawei",2,"4G->2G, Cell-based",800,0.9,90,"B","NO","NO","NO",1,1,"Non-sliding",4,1,"1 cell,  L3 cell-level RSRP ","1 cell,  L3 cell-level RSRP ","AI: LSTM","3 LSTM layers and 1 full-connectivity layer",80,350,1.03,30,0.5,0.82]
["Huawei",2,"4G->2G, Cell-based",1000,0.9,90,"B","NO","NO","NO",1,1,"Non-sliding",4,1,"1 cell,  L3 cell-level RSRP ","1 cell,  L3 cell-level RSRP ","AI: LSTM","3 LSTM layers and 1 full-connectivity layer",80,350,1.03,30,0.5,0.83]
["Huawei",2,"4G->2G, Cell-based",200,0.9,120,"B","NO","NO","NO",1,1,"Non-sliding",4,1,"1 cell,  L3 cell-level RSRP ","1 cell,  L3 cell-level RSRP ","AI: LSTM","3 LSTM layers and 1 full-connectivity layer",80,350,1.03,30,0.5,0.8]
["Huawei",2,"4G->2G, Cell-based",400,0.9,120,"B","NO","NO","NO",1,1,"Non-sliding",4,1,"1 cell,  L3 cell-level RSRP ","1 cell,  L3 cell-level RSRP ","AI: LSTM","3 LSTM layers and 1 full-connectivity layer",80,350,1.03,30,0.5,0.82]
["Huawei",2,"4G->2G, Cell-based",600,0.9,120,"B","NO","NO","NO",1,1,"Non-sliding",4,1,"1 cell,  L3 cell-level RSRP ","1 cell,  L3 cell-level RSRP ","AI: LSTM","3 LSTM layers and 1 full-connectivity layer",80,350,1.03,30,0.5,0.84]
["Huawei",2,"4G->2G, Cell-based",800,0.9,120,"B","NO","NO","NO",1,1,"Non-sliding",4,1,"1 cell,  L3 cell-level RSRP ","1 cell,  L3 cell-level RSRP ","AI: LSTM","3 LSTM layers and 1 full-connectivity layer",80,350,1.03,30,0.5,0.84]
["Huawei",2,"4G->2G, Cell-based",1000,0.9,120,"B","NO","NO","NO",1,1,"Non-sliding",4,1,"1 cell,  L3 cell-level RSRP ","1 cell,  L3 cell-level RSRP ","AI: LSTM","3 LSTM layers and 1 full-connectivity layer",80,350,1.03,30,0.5,0.95]
["Huawei",1,"2G->4G, Cell-based",200,0.9,30,"B","NO","NO","NO",1,1,"Non-sliding",4,1,"1 cell,  L3 cell-level RSRP ","1 cell,  L3 cell-level RSRP ","AI: LSTM","3 LSTM layers and 1 full-connectivity layer",80,350,1.03,30,0.5,0.24]
["Huawei",1,"2G->4G, Cell-based",400,0.9,30,"B","NO","NO","NO",1,1,"Non-sliding",4,1,"1 cell,  L1 beam-level RSRP ","1 cell,  L1 beam-level RSRP ","AI: LSTM","3 LSTM layers and 1 full-connectivity layer",80,350,1.03,30,0.5,0.31]
["Huawei",1,"2G->4G, Cell-based",600,0.9,30,"B","NO","NO","NO",1,1,"Non-sliding",4,1,"1 cell,  L1 beam-level RSRP ","1 cell,  L1 beam-level RSRP ","AI: LSTM","3 LSTM layers and 1 full-connectivity layer",80,350,1.03,30,0.5,0.35]
["Huawei",1,"2G->4G, Cell-based",800,0.9,30,"B","NO","NO","NO",1,1,"Non-sliding",4,1,"1 cell,  L1 beam-level RSRP ","1 cell,  L1 beam-level RSRP ","AI: LSTM","3 LSTM layers and 1 full-connectivity layer",80,350,1.03,30,0.5,0.48]
["Huawei",1,"2G->4G, Cell-based",1000,0.9,30,"B","NO","NO","NO",1,1,"Non-sliding",4,1,"1 cell,  L1 beam-level RSRP ","1 cell,  L1 beam-level RSRP ","AI: LSTM","3 LSTM layers and 1 full-connectivity layer",80,350,1.03,30,0.5,0.68]
["Huawei",1,"2G->4G, Cell-based",200,0.9,60,"B","NO","NO","NO",1,1,"Non-sliding",4,1,"1 cell,  L1 beam-level RSRP ","1 cell,  L1 beam-level RSRP ","AI: LSTM","3 LSTM layers and 1 full-connectivity layer",80,350,1.03,30,0.5,0.24]
["Huawei",1,"2G->4G, Cell-based",400,0.9,60,"B","NO","NO","NO",1,1,"Non-sliding",4,1,"1 cell,  L1 beam-level RSRP ","1 cell,  L1 beam-level RSRP ","AI: LSTM","3 LSTM layers and 1 full-connectivity layer",80,350,1.03,30,0.5,0.32]
["Huawei",1,"2G->4G, Cell-based",600,0.9,60,"B","NO","NO","NO",1,1,"Non-sliding",4,1,"1 cell,  L1 beam-level RSRP ","1 cell,  L1 beam-level RSRP ","AI: LSTM","3 LSTM layers and 1 full-connectivity layer",80,350,1.03,30,0.5,0.39]
["Huawei",1,"2G->4G, Cell-based",800,0.9,60,"B","NO","NO","NO",1,1,"Non-sliding",4,1,"1 cell,  L1 beam-level RSRP ","1 cell,  L1 beam-level RSRP ","AI: LSTM","3 LSTM layers and 1 full-connectivity layer",80,350,1.03,30,0.5,0.5]
["Huawei",1,"2G->4G, Cell-based",1000,0.9,60,"B","NO","NO","NO",1,1,"Non-sliding",4,1,"1 cell,  L1 beam-level RSRP ","1 cell,  L1 beam-level RSRP ","AI: LSTM","3 LSTM layers and 1 full-connectivity layer",80,350,1.03,30,0.5,0.68]
["Huawei",1,"2G->4G, Cell-based",200,0.9,90,"B","NO","NO","NO",1,1,"Non-sliding",4,1,"1 cell,  L1 beam-level RSRP ","1 cell,  L1 beam-level RSRP ","AI: LSTM","3 LSTM layers and 1 full-connectivity layer",80,350,1.03,30,0.5,0.65]
["Huawei",1,"2G->4G, Cell-based",400,0.9,90,"B","NO","NO","NO",1,1,"Non-sliding",4,1,"1 cell,  L1 beam-level RSRP ","1 cell,  L1 beam-level RSRP ","AI: LSTM","3 LSTM layers and 1 full-connectivity layer",80,350,1.03,30,0.5,0.71]
["Huawei",1,"2G->4G, Cell-based",600,0.9,90,"B","NO","NO","NO",1,1,"Non-sliding",4,1,"1 cell,  L1 beam-level RSRP ","1 cell,  L1 beam-level RSRP ","AI: LSTM","3 LSTM layers and 1 full-connectivity layer",80,350,1.03,30,0.5,0.74]
["Huawei",1,"2G->4G, Cell-based",800,0.9,90,"B","NO","NO","NO",1,1,"Non-sliding",4,1,"1 cell,  L1 beam-level RSRP ","1 cell,  L1 beam-level RSRP ","AI: LSTM","3 LSTM layers and 1 full-connectivity layer",80,350,1.03,30,0.5,0.8]
["Huawei",1,"2G->4G, Cell-based",1000,0.9,90,"B","NO","NO","NO",1,1,"Non-sliding",4,1,"1 cell,  L1 beam-level RSRP ","1 cell,  L1 beam-level RSRP ","AI: LSTM","3 LSTM layers and 1 full-connectivity layer",80,350,1.03,30,0.5,0.83]
["Huawei",1,"2G->4G, Cell-based",200,0.9,120,"B","NO","NO","NO",1,1,"Non-sliding",4,1,"1 cell,  L1 beam-level RSRP ","1 cell,  L1 beam-level RSRP ","AI: LSTM","3 LSTM layers and 1 full-connectivity layer",80,350,1.03,30,0.5,0.81]
["Huawei",1,"2G->4G, Cell-based",400,0.9,120,"B","NO","NO","NO",1,1,"Non-sliding",4,1,"1 cell,  L1 beam-level RSRP ","1 cell,  L1 beam-level RSRP ","AI: LSTM","3 LSTM layers and 1 full-connectivity layer",80,350,1.03,30,0.5,0.82]
["Huawei",1,"2G->4G, Cell-based",600,0.9,120,"B","NO","NO","NO",1,1,"Non-sliding",4,1,"1 cell,  L1 beam-level RSRP ","1 cell,  L1 beam-level RSRP ","AI: LSTM","3 LSTM layers and 1 full-connectivity layer",80,350,1.03,30,0.5,0.84]
["Huawei",1,"2G->4G, Cell-based",800,0.9,120,"B","NO","NO","NO",1,1,"Non-sliding",4,1,"1 cell,  L1 beam-level RSRP ","1 cell,  L1 beam-level RSRP ","AI: LSTM","3 LSTM layers and 1 full-connectivity layer",80,350,1.03,30,0.5,0.89]
["Huawei",1,"2G->4G, Cell-based",1000,0.9,120,"B","NO","NO","NO",1,1,"Non-sliding",4,1,"1 cell,  L1 beam-level RSRP ","1 cell,  L1 beam-level RSRP ","AI: LSTM","3 LSTM layers and 1 full-connectivity layer",80,350,1.03,30,0.5,0.95]
["Huawei",1,"4G->2G, Cell-based",200,0.9,30,"B","NO","NO","NO",1,1,"Non-sliding",4,1,"1 cell,  L1 beam-level RSRP ","1 cell,  L1 beam-level RSRP ","AI: LSTM","3 LSTM layers and 1 full-connectivity layer",80,350,1.03,30,0.5,0.23]
["Huawei",1,"4G->2G, Cell-based",400,0.9,30,"B","NO","NO","NO",1,1,"Non-sliding",4,1,"1 cell,  L1 beam-level RSRP ","1 cell,  L1 beam-level RSRP ","AI: LSTM","3 LSTM layers and 1 full-connectivity layer",80,350,1.03,30,0.5,0.3]
["Huawei",1,"4G->2G, Cell-based",600,0.9,30,"B","NO","NO","NO",1,1,"Non-sliding",4,1,"1 cell,  L1 beam-level RSRP ","1 cell,  L1 beam-level RSRP ","AI: LSTM","3 LSTM layers and 1 full-connectivity layer",80,350,1.03,30,0.5,0.33]
["Huawei",1,"4G->2G, Cell-based",800,0.9,30,"B","NO","NO","NO",1,1,"Non-sliding",4,1,"1 cell,  L1 beam-level RSRP ","1 cell,  L1 beam-level RSRP ","AI: LSTM","3 LSTM layers and 1 full-connectivity layer",80,350,1.03,30,0.5,0.48]
["Huawei",1,"4G->2G, Cell-based",1000,0.9,30,"B","NO","NO","NO",1,1,"Non-sliding",4,1,"1 cell,  L1 beam-level RSRP ","1 cell,  L1 beam-level RSRP ","AI: LSTM","3 LSTM layers and 1 full-connectivity layer",80,350,1.03,30,0.5,0.67]
["Huawei",1,"4G->2G, Cell-based",200,0.9,60,"B","NO","NO","NO",1,1,"Non-sliding",4,1,"1 cell,  L1 beam-level RSRP ","1 cell,  L1 beam-level RSRP ","AI: LSTM","3 LSTM layers and 1 full-connectivity layer",80,350,1.03,30,0.5,0.23]
["Huawei",1,"4G->2G, Cell-based",400,0.9,60,"B","NO","NO","NO",1,1,"Non-sliding",4,1,"1 cell,  L1 beam-level RSRP ","1 cell,  L1 beam-level RSRP ","AI: LSTM","3 LSTM layers and 1 full-connectivity layer",80,350,1.03,30,0.5,0.32]
["Huawei",1,"4G->2G, Cell-based",600,0.9,60,"B","NO","NO","NO",1,1,"Non-sliding",4,1,"1 cell,  L1 beam-level RSRP ","1 cell,  L1 beam-level RSRP ","AI: LSTM","3 LSTM layers and 1 full-connectivity layer",80,350,1.03,30,0.5,0.38]
["Huawei",1,"4G->2G, Cell-based",800,0.9,60,"B","NO","NO","NO",1,1,"Non-sliding",4,1,"1 cell,  L1 beam-level RSRP ","1 cell,  L1 beam-level RSRP ","AI: LSTM","3 LSTM layers and 1 full-connectivity layer",80,350,1.03,30,0.5,0.5]
["Huawei",1,"4G->2G, Cell-based",1000,0.9,60,"B","NO","NO","NO",1,1,"Non-sliding",4,1,"1 cell,  L1 beam-level RSRP ","1 cell,  L1 beam-level RSRP ","AI: LSTM","3 LSTM layers and 1 full-connectivity layer",80,350,1.03,30,0.5,0.68]
["Huawei",1,"4G->2G, Cell-based",200,0.9,90,"B","NO","NO","NO",1,1,"Non-sliding",4,1,"1 cell,  L1 beam-level RSRP ","1 cell,  L1 beam-level RSRP ","AI: LSTM","3 LSTM layers and 1 full-connectivity layer",80,350,1.03,30,0.5,0.7]
["Huawei",1,"4G->2G, Cell-based",400,0.9,90,"B","NO","NO","NO",1,1,"Non-sliding",4,1,"1 cell,  L1 beam-level RSRP ","1 cell,  L1 beam-level RSRP ","AI: LSTM","3 LSTM layers and 1 full-connectivity layer",80,350,1.03,30,0.5,0.7]
["Huawei",1,"4G->2G, Cell-based",600,0.9,90,"B","NO","NO","NO",1,1,"Non-sliding",4,1,"1 cell,  L1 beam-level RSRP ","1 cell,  L1 beam-level RSRP ","AI: LSTM","3 LSTM layers and 1 full-connectivity layer",80,350,1.03,30,0.5,0.73]
["Huawei",1,"4G->2G, Cell-based",800,0.9,90,"B","NO","NO","NO",1,1,"Non-sliding",4,1,"1 cell,  L1 beam-level RSRP ","1 cell,  L1 beam-level RSRP ","AI: LSTM","3 LSTM layers and 1 full-connectivity layer",80,350,1.03,30,0.5,0.8]
["Huawei",1,"4G->2G, Cell-based",1000,0.9,90,"B","NO","NO","NO",1,1,"Non-sliding",4,1,"1 cell,  L1 beam-level RSRP ","1 cell,  L1 beam-level RSRP ","AI: LSTM","3 LSTM layers and 1 full-connectivity layer",80,350,1.03,30,0.5,0.81]
["Huawei",1,"4G->2G, Cell-based",200,0.9,120,"B","NO","NO","NO",1,1,"Non-sliding",4,1,"1 cell,  L1 beam-level RSRP ","1 cell,  L1 beam-level RSRP ","AI: LSTM","3 LSTM layers and 1 full-connectivity layer",80,350,1.03,30,0.5,0.76]
["Huawei",1,"4G->2G, Cell-based",400,0.9,120,"B","NO","NO","NO",1,1,"Non-sliding",4,1,"1 cell,  L1 beam-level RSRP ","1 cell,  L1 beam-level RSRP ","AI: LSTM","3 LSTM layers and 1 full-connectivity layer",80,350,1.03,30,0.5,0.78]
["Huawei",1,"4G->2G, Cell-based",600,0.9,120,"B","NO","NO","NO",1,1,"Non-sliding",4,1,"1 cell,  L1 beam-level RSRP ","1 cell,  L1 beam-level RSRP ","AI: LSTM","3 LSTM layers and 1 full-connectivity layer",80,350,1.03,30,0.5,0.81]
["Huawei",1,"4G->2G, Cell-based",800,0.9,120,"B","NO","NO","NO",1,1,"Non-sliding",4,1,"1 cell,  L1 beam-level RSRP ","1 cell,  L1 beam-level RSRP ","AI: LSTM","3 LSTM layers and 1 full-connectivity layer",80,350,1.03,30,0.5,0.89]
["Huawei",1,"4G->2G, Cell-based",1000,0.9,120,"B","NO","NO","NO",1,1,"Non-sliding",4,1,"1 cell,  L1 beam-level RSRP ","1 cell,  L1 beam-level RSRP ","AI: LSTM","3 LSTM layers and 1 full-connectivity layer",80,350,1.03,30,0.5,0.91]
["Mediatek",2,"2G->4G, Cluster-based",400,null,30,"A ","YES","YES","FULL",1,2,"Sliding",1,1,"21 cells,  L3 cell-level RSRP ","21 cells, L3 cell-level RSRP","AI: CNN","2 layers of convolution layer and 1 FNN layer",50,201,3,160,40,1.64]
["Mediatek",3,"2G->4G, Cluster-based",400,null,30,"A ","YES","YES","FULL",1,2,"Sliding",1,1,"21 cells,  L3 cell-level RSRP ","21 cells, L3 cell-level RSRP","AI: CNN","2 layers of convolution layer and 1 FNN layer",50,201,3,160,40,1.93]
["Mediatek",1,"2G->4G, Cluster-based",400,null,30,"A ","YES","YES","FULL",1,2,"Sliding",1,1,"21 cells,  L3 cell-level RSRP ","21 cells, L3 cell-level RSRP","AI: CNN","2 layers of convolution layer and 1 FNN layer",50,201,3,160,40,1.97]
["Mediatek",2,"2G->4G, Cell-based",400,null,30,"A ","YES","YES","FULL",1,2,"Sliding",1,1,"1 cell,  L3 cell-level RSRP ","1 cell, L3 cell-level RSRP","AI: CNN","2 layers of convolution layer and 1 FNN layer",50,201,3,160,40,2.29]
["Mediatek",3,"2G->4G, Cell-based",400,null,30,"A ","YES","YES","FULL",1,2,"Sliding",1,1,"1 cell,  L3 cell-level RSRP ","1 cell, L3 cell-level RSRP","AI: CNN","2 layers of convolution layer and 1 FNN layer",50,201,3,160,40,3.26]
["Mediatek",1,"2G->4G, Cell-based",400,null,30,"A ","YES","YES","FULL",1,2,"Sliding",1,1,"1 cell,  L3 cell-level RSRP ","1 cell, L3 cell-level RSRP","AI: CNN","2 layers of convolution layer and 1 FNN layer",50,201,3,160,40,2.5299999999999998]
["Mediatek",2,"2G->4G, Cluster-based",400,null,30,"A ","YES","YES","FULL",1,2,"Sliding",1,1,"21 cells,  L3 cell-level RSRP ","21 cells, L3 cell-level RSRP","AI: CNN","2 layers of convolution layer and 1 FNN layer",50,201,3,160,40,1.64]
["Mediatek",2,"2G->4G, Cluster-based",400,null,60,"A ","YES","YES","FULL",1,2,"Sliding",1,1,"21 cells,  L3 cell-level RSRP ","21 cells, L3 cell-level RSRP","AI: CNN","2 layers of convolution layer and 1 FNN layer",50,201,3,160,40,1.55]
["Mediatek",2,"2G->4G, Cluster-based",400,null,90,"A ","YES","YES","FULL",1,2,"Sliding",1,1,"21 cells,  L3 cell-level RSRP ","21 cells, L3 cell-level RSRP","AI: CNN","2 layers of convolution layer and 1 FNN layer",50,201,3,160,40,1.49]
["Mediatek",2,"2G->4G, Cluster-based",400,null,120,"A ","YES","YES","FULL",1,2,"Sliding",1,1,"21 cells,  L3 cell-level RSRP ","21 cells, L3 cell-level RSRP","AI: CNN","2 layers of convolution layer and 1 FNN layer",50,201,3,160,40,1.4]
["Mediatek",2,"2G->4G, non-AI",400,null,30,"A ","YES","YES","FULL",1,2,"Sliding",1,1,null,null,"Non-AI: 2GHz measurement + pathloss modification"," Derive 4GHz measurement by the  2GHz cell measurements minus the path loss difference",null,null,null,null,null,2.34]
["Mediatek",2,"2G->4G, non-AI",400,null,60,"A ","YES","YES","FULL",1,2,"Sliding",1,1,null,null,"Non-AI: 2GHz measurement + pathloss modification"," Derive 4GHz measurement by the  2GHz cell measurements minus the path loss difference",null,null,null,null,null,2.2999999999999998]
["Mediatek",2,"2G->4G, non-AI",400,null,90,"A ","YES","YES","FULL",1,2,"Sliding",1,1,null,null,"Non-AI: 2GHz measurement + pathloss modification"," Derive 4GHz measurement by the  2GHz cell measurements minus the path loss difference",null,null,null,null,null,2.31]
["Mediatek",2,"2G->4G, non-AI",400,null,120,"A ","YES","YES","FULL",1,2,"Sliding",1,1,null,null,"Non-AI: 2GHz measurement + pathloss modification"," Derive 4GHz measurement by the  2GHz cell measurements minus the path loss difference",null,null,null,null,null,2.21]
["OPPO",2,"2G->4G, Cell-based",400,0.99,30,"A","NO","YES","FULL",1,3,"Non-sliding",1,1,"1 cell, L3 cell-level RSRP","1 cell, L3 cell-level RSRP","AI: LSTM","2LSTM layer+1 dense layer",170,670,0.4,52,12,0.28000000000000003]
["OPPO",2,"2G->4G, Cluster-based",400,0.99,30,"A","NO","YES","FULL",1,3,"Non-sliding",1,1,"3 cell, L3 cell-level RSRP","3 cell, L3 cell-level RSRP","AI: LSTM","2LSTM layer+1 dense layer",180,670,0.41,52,12,0.43]
["OPPO",2,"2G->4G, Cell-based",800,0.99,30,"A","NO","YES","FULL",1,3,"Non-sliding",1,1,"1 cell, L3 cell-level RSRP","1 cell, L3 cell-level RSRP","AI: LSTM","2LSTM layer+1 dense layer",180,670,0.41,26,6,0.8]
["OPPO",2,"2G->4G, Cluster-based",800,0.99,30,"A","NO","YES","FULL",1,3,"Non-sliding",1,1,"3 cell, L3 cell-level RSRP","3 cell, L3 cell-level RSRP","AI: LSTM","2LSTM layer+1 dense layer",180,670,0.41,26,6,1.49]
["OPPO",2,"2G->4G, Cluster-based",400,0.99,30,"A","NO","YES","FULL",1,3,"Non-sliding",1,1,"21 cell, L3 cell-level RSRP","21 cell, L3 cell-level RSRP","AI: LSTM","2LSTM layer+1 dense layer",190,710,0.42,52,12,0.78]
["OPPO",2,"2G->4G, Cluster-based",800,0.99,30,"A","NO","YES","FULL",1,3,"Non-sliding",1,1,"21 cell, L3 cell-level RSRP","21 cell, L3 cell-level RSRP","AI: LSTM","2LSTM layer+1 dense layer",190,910,0.42,26,6,2.78]
["OPPO",2,"2G->4G, Cell-based",160,0.99,30,"A","NO","YES","FULL",1,3,"Sliding",1,1,"1 cell, L3 cell-level RSRP","1 cell, L3 cell-level RSRP","AI: LSTM","2LSTM layer+1 dense layer",180,690,0.4,1020,260,0.33]
["OPPO",2,"2G->4G, Cell-based",160,0.99,60,"A","NO","YES","FULL",1,3,"Sliding",1,1,"1 cell, L3 cell-level RSRP","1 cell, L3 cell-level RSRP","AI: LSTM","2LSTM layer+1 dense layer",180,690,0.4,1020,260,0.33]
["OPPO",2,"4G->2G, Cell-based",160,0.99,30,"A","NO","YES","FULL",1,3,"Sliding",1,1,"1 cell, L3 cell-level RSRP","1 cell, L3 cell-level RSRP","AI: LSTM","2LSTM layer+1 dense layer",180,690,0.4,1020,260,0.39]
["OPPO",2,"4G->2G, Cell-based",160,0.99,60,"A","NO","YES","FULL",1,3,"Sliding",1,1,"1 cell, L3 cell-level RSRP","1 cell, L3 cell-level RSRP","AI: LSTM","2LSTM layer+1 dense layer",180,690,0.4,1020,260,0.38]
["vivo",2,"2G->4G, Cell-based",2000,0.91500000000000004,60,"A ","NO","YES","FULL",1,2,"Sliding",1,1,"1 cell,L3 cell-level RSRP ","1 cell, L3 cell-level RSRP","Non-AI: 2GHz measurement + mean difference"," Derive 4GHz measurement by the  2GHz cell measurements minus the mean difference",null,null,null,160,40,3.3170000000000002]
["vivo",2,"2G->4G, Cell-based",2000,0.92600000000000005,90,"A ","NO","YES","FULL",1,2,"Sliding",1,1,"1 cell, L3 cell-level RSRP and cell id","1 cell, L3 cell-level RSRP","RandomForest","n_estimators = 2\nmax_depth = 20",0.29399999999999998,5.03,7.0000000000000001E-3,160,40,1.3560000000000001]
["vivo",2,"2G->4G, Cell-based",2000,0.92600000000000005,90,"A ","NO","YES","FULL",1,2,"Sliding",1,1,"1 cell,L3 cell-level RSRP ","1 cell, L3 cell-level RSRP","Non-AI: 2GHz measurement + mean difference"," Derive 4GHz measurement by the  2GHz cell measurements minus the mean difference",null,null,null,160,40,3.2360000000000002]
["vivo",2,"4G->2G, Cell-based",2000,0.92300000000000004,30,"A ","NO","YES","FULL",1,2,"Sliding",1,1,"1 cell, L3 cell-level RSRP and cell id","1 cell, L3 cell-level RSRP","RandomForest","n_estimators = 2\nmax_depth = 20",0.29299999999999998,4.76,7.0000000000000001E-3,160,40,0.81799999999999995]
["vivo",2,"4G->2G, Cell-based",2000,0.92300000000000004,30,"A ","NO","YES","FULL",1,2,"Sliding",1,1,"1 cell,  L3 cell-level RSRP ","1 cell, L3 cell-level RSRP","Non-AI: 4GHz measurement + mean difference"," Derive 2GHz measurement by the  4GHz cell measurements minus the mean difference",null,null,null,160,40,3.3460000000000001]
["vivo",2,"4G->2G, Cell-based",2000,0.91500000000000004,60,"A ","NO","YES","FULL",1,2,"Sliding",1,1,"1 cell, L3 cell-level RSRP and cell id","1 cell, L3 cell-level RSRP","RandomForest","n_estimators = 2\nmax_depth = 20",0.29299999999999998,4.7699999999999996,7.0000000000000001E-3,160,40,1.2130000000000001]
["vivo",2,"4G->2G, Cell-based",2000,0.91500000000000004,60,"A ","NO","YES","FULL",1,2,"Sliding",1,1,"1 cell,L3 cell-level RSRP ","1 cell, L3 cell-level RSRP","Non-AI: 4GHz measurement + mean difference"," Derive 2GHz measurement by the  4GHz cell measurements minus the mean difference",null,null,null,160,40,3.3170000000000002]
["vivo",2,"4G->2G, Cell-based",2000,0.92600000000000005,90,"A ","NO","YES","FULL",1,2,"Sliding",1,1,"1 cell, L3 cell-level RSRP and cell id","1 cell, L3 cell-level RSRP","RandomForest","n_estimators = 2\nmax_depth = 20",0.29299999999999998,4.8499999999999996,7.0000000000000001E-3,160,40,1.4359999999999999]
["vivo",2,"4G->2G, Cell-based",2000,0.92600000000000005,90,"A ","NO","YES","FULL",1,2,"Sliding",1,1,"1 cell, L3 cell-level RSRP ","1 cell, L3 cell-level RSRP","Non-AI: 4GHz measurement + mean difference"," Derive 2GHz measurement by the  4GHz cell measurements minus the mean difference",null,null,null,160,40,3.2360000000000002]
["vivo","2","2G->4G, Cluster-based",2000,0.92300000000000004,30,"A","NO","YES","FULL",1,2,"Sliding",1,1,"21 cells, L3 cell-level RSRP and cell id","1 cell, L3 cell-level RSRP","RandomForest","n_estimators = 2\nmax_depth = 20",0.23,7.02,1.2E-2,160,40,0.36]
["vivo","2","2G->4G, Cluster-based",2000,0.92300000000000004,30,"A","NO","YES","FULL",1,2,"Sliding",1,1,"3 cells of co-located station, L3 cell-level RSRP and cell id","1 cell, L3 cell-level RSRP","RandomForest","n_estimators = 2\nmax_depth = 20",0.317,8.32,1.2E-2,160,40,0.35]
["vivo","2","2G->4G, Cluster-based",2000,0.92300000000000004,30,"A","NO","YES","FULL",1,2,"Sliding",1,1,"18 cells (exclude 3 cells of co-located station), L3 cell-level RSRP and cell id","1 cell, L3 cell-level RSRP","RandomForest","n_estimators = 2\nmax_depth = 20",0.254,6.67,7.0000000000000007E-2,160,40,1.42]
["vivo","2","2G->4G, Cluster-based",2000,0.92300000000000004,30,"A","NO","YES","FULL",1,2,"Sliding",1,1,"3 cells with highest RSRP, L3 cell-level RSRP and cell id","1 cell, L3 cell-level RSRP","RandomForest","n_estimators = 2\nmax_depth = 20",0.221,5.78,1.0999999999999999E-2,160,40,0.24]
["Xiaomi",2,"4G->2G, Cell-based","XX",0.93200000000000005,30,"A ","NO","NO","NO",1,2,"Sliding",1,1,"1 serving cell, L3 cell-level RSRP  ","1 cell, L3 cell-level RSRP  ","AI:Single-branch MLP","MLP with three hidden layers in a decreasing neurons",14.189,212,0.1394,39.984000000000002,4.9980000000000002,4.54]
["Xiaomi",2,"4G->2G, Cluster-based","XX",0.93200000000000005,30,"A ","NO","NO","NO",1,2,"Sliding",1,1,"1 serving cell+6 neighboring cells, L3 cell-level RSRP  ","1 cell, L3 cell-level RSRP  ","AI:Double-branch MLP","MLP with two branches, where one branch handles target cell with a single hidden layer but more neurons, and the other branch handles neighboring cells with two hidden layers but fewer neurons",56.817,724,0.56264000000000003,39.984000000000002,4.9980000000000002,3.52]
["Xiaomi",2,"4G->2G, Cluster-based","XX",0.93200000000000005,30,"A ","NO","NO","NO",1,2,"Sliding",1,1,"1 serving cell+2 collocated cells, L3 cell-level RSRP  ","1 cell, L3 cell-level RSRP  ","AI:Double-branch MLP","MLP with two branches, where one branch handles target cells with one hidden layer, and the other branch handles  collocated cells with one hidden layer but fewer neurons.",27.236999999999998,369,0.26888000000000001,39.984000000000002,4.9980000000000002,4.05]
["Xiaomi",2,"4G->2G, Cluster-based","XX",0.93200000000000005,30,"A ","NO","NO","NO",1,2,"Sliding",1,1,"1 serving cell+6 neighboring cells, L3 cell-level RSRP,Using UE coordinates  ","1 cell, L3 cell-level RSRP  ","AI:Triple-branch MLP","The MLP has three branches, where one branch with a single hidden layer and the most neurons handles the target cell, one with a single hidden layer and the fewest neurons handles UE coordinates, and one with two hidden layers and decreasing neurons handles neighboring cells.",33.728999999999999,466,0.33272000000000002,39.984000000000002,4.9980000000000002,3.5]
["Xiaomi",2,"4G->2G, Cluster-based","XX",0.93200000000000005,30,"A ","NO","NO","NO",1,2,"Sliding",1,1,"1 servg cell+2 collocated cells, L3 cell-level RSRP,Using UE coordinates","1 cell, L3 cell-level RSRP  ","AI:Triple-branch MLP","The MLP has three branches, where one branch with a single hidden layer and the most neurons handles the target cell, one with a single hidden layer and the fewest neurons handles UE coordinates, and one with two hidden layers and decreasing neurons handles collocated cells.",33.377000000000002,463,0.32888000000000001,39.984000000000002,4.9980000000000002,3.56]
["Xiaomi",2,"4G->2G, Cell-based",120,0.93200000000000005,30,"A ",null,null,null,null,null,null,1,1,"1serving  cell, historic L3 cell-level RSRP","1 cell, L3 cell-level RSRP  ","AI:GRU","1 layer of GRU  based on encoder-decoder with 1 layer of FNN handle  previous measurements, and the other branch handles target cell",218.517,2634,3.8697599999999999,39.984000000000002,4.9980000000000002,4.28]
["InterDigital",2,"2G->4G",1000,null,30,"A","Yes",null,null,1,3,"Non-sliding",4,1,"1 cell, L3 cell-level RSRPs","1 cell, L3 cell-level RSRPs","AI: ResNet",null,1840,null,2.38,16.8,4.2,1.0009999999999999]
["Samsung",2,"4G -> 2G, Cell-based","800 ms",0.89900000000000002,30,"B","YES","YES","FULL",3,3,"Sliding",1,1,"1 cell, L3 cell-level RSRP","1 cell, L3 cell-level RSRP","LSTM autoencoder","2 LSTM layers for encoder \n2 LSTEM layers + 3 dense layers for decoder",4.5,200,0.02,39,24,4.1440000000000001]
["Samsung",2,"4G -> 2G, Cluster-based","800 ms",0.89900000000000002,30,"B","YES","YES","FULL",3,3,"Sliding",1,1,"21 cells, L3 cell-level RSRP","21 cells, L3 cell-level RSRP","LSTM autoencoder","2 LSTM layers for encoder \n2 LSTEM layers + 3 dense layers for decoder",300,3500,0.6,39,24,3.1080000000000001]
["Samsung",2,"4G -> 2G, Cell-based","800 ms",0.90200000000000002,60,"B","YES","YES","FULL",3,3,"Sliding",1,1,"1 cell, L3 cell-level RSRP","1 cell, L3 cell-level RSRP","LSTM autoencoder","2 LSTM layers for encoder \n2 LSTEM layers + 3 dense layers for decoder",4.5,200,0.02,19,12,3.907]
["Samsung",2,"4G -> 2G, Cluster-based","800 ms",0.90200000000000002,60,"B","YES","YES","FULL",3,3,"Sliding",1,1,"21 cells, L3 cell-level RSRP","21 cells, L3 cell-level RSRP","LSTM autoencoder","2 LSTM layers for encoder \n2 LSTEM layers + 3 dense layers for decoder",300,3500,0.6,19,12,3.222]
["Samsung",2,"4G -> 2G, Cell-based","800 ms",0.91800000000000004,120,"B","YES","YES","FULL",3,3,"Sliding",1,1,"1 cell, L3 cell-level RSRP","1 cell, L3 cell-level RSRP","LSTM autoencoder","2 LSTM layers for encoder \n2 LSTEM layers + 3 dense layers for decoder",4.5,200,0.02,18,11,3.61]
["Samsung",2,"4G -> 2G, Cluster-based","800 ms",0.91800000000000004,120,"B","YES","YES","FULL",3,3,"Sliding",1,1,"21 cells, L3 cell-level RSRP","21 cells, L3 cell-level RSRP","LSTM autoencoder","2 LSTM layers for encoder \n2 LSTEM layers + 3 dense layers for decoder",300,3500,0.6,18,11,2.94]
["Samsung",2,"4G -> 2G, Non-AI","40 ms",0.89900000000000002,30,"B","YES","YES","FULL",3,3,"Sliding",1,1,"1 cell, L3 cell-level RSRP","1 cell, L3 cell-level RSRP","Non-AI: Freq. offset based on training dataset",null,null,null,null,39,24,4.22]
["Samsung",2,"4G -> 2G, Non-AI","40 ms",0.90200000000000002,60,"B","YES","YES","FULL",3,3,"Sliding",1,1,"1 cell, L3 cell-level RSRP","1 cell, L3 cell-level RSRP","Non-AI: Freq. offset based on training dataset",null,null,null,null,19,12,4.3259999999999996]
["Samsung",2,"4G -> 2G, Non-AI","40 ms",0.91800000000000004,120,"B","YES","YES","FULL",3,3,"Sliding",1,1,"1 cell, L3 cell-level RSRP","1 cell, L3 cell-level RSRP","Non-AI: Freq. offset based on training dataset",null,null,null,null,18,11,4.1310000000000002]
["Apple",2," (0.8, 1.8, 2.6)->2.6, Cluster-based",200,"it's not a scalar but a matrix, not clear how to report",30,"A ","YES","YES","FULL",1,3,"non-sliding",1,1," 3 cells, L3 cell-level RSRP ","L3 cell-level RSRP","AR",null,3,"24bytes",2,"560K","140K",1.006]
["Apple",2," (0.8, 1.8, 2.6)->2.6, Cluster-based",200,"it's not a scalar but a matrix, not clear how to report",30,"A ","YES","YES","FULL",1,3,"non-sliding",1,1," 3 cells, L3 cell-level RSRP ","L3 cell-level RSRP","XGBoost","number of estimators t=10, max depth d=7",63600,"0.25MB",800,"560K","140K",1.0218]
["Apple",2," (0.8, 1.8, 2.6)->2.6, Cluster-based",200,"it's not a scalar but a matrix, not clear how to report",30,"A ","YES","YES","FULL",1,3,"non-sliding",1,1," 3 cells, L3 cell-level RSRP ","L3 cell-level RSRP","Random Forest","number of trees t = 100, average tree depth: d = 10",102300,"~1.37MB","~1 KFLOPs","560K","140K",1.1772]
["Apple",2," (0.8, 1.8, 2.6)->2.6, Cluster-based",200,"it's not a scalar but a matrix, not clear how to report",30,"A ","YES","YES","FULL",1,3,"non-sliding",1,1," 3 cells, L3 cell-level RSRP ","L3 cell-level RSRP","FNN","hidden layer size 64",129,"~1KB","~320","560K","140K",1.0056]
["Apple",2," (0.8, 1.8, 2.6)->2.6, Cluster-based",200,"it's not a scalar but a matrix, not clear how to report",30,"A ","YES","YES","FULL",1,3,"non-sliding",1,1," 3 cells, L3 cell-level RSRP ","L3 cell-level RSRP","AR",null,3,"24bytes",2,"560K","140K",1.0194000000000001]
["Apple",2," (0.8, 1.8, 2.6)->2.6, Cluster-based",200,"it's not a scalar but a matrix, not clear how to report",30,"A ","YES","YES","FULL",1,3,"non-sliding",1,1," 3 cells, L3 cell-level RSRP ","L3 cell-level RSRP","XGBoost","number of estimators t=10, max depth d=7",63600,"0.25MB",800,"560K","140K",1.0315000000000001]
["Apple",2," (0.8, 1.8, 2.6)->2.6, Cluster-based",200,"it's not a scalar but a matrix, not clear how to report",30,"A ","YES","YES","FULL",1,3,"non-sliding",1,1," 3 cells, L3 cell-level RSRP ","L3 cell-level RSRP","Random Forest","number of trees t = 100, average tree depth: d = 10",102300,"~1.37MB","~1 KFLOPs","560K","140K",1.1957]
["Apple",2," (0.8, 1.8, 2.6)->2.6, Cluster-based",200,"it's not a scalar but a matrix, not clear how to report",30,"A ","YES","YES","FULL",1,3,"non-sliding",1,1," 3 cells, L3 cell-level RSRP ","L3 cell-level RSRP","FNN","hidden layer size 64",129,"~1KB","~320","560K","140K",1.0141]
["Qualcomm",2,"2G->4G, Cell-based","<=1280",0.96599999999999997,60,"A ","YES","YES","FULL",2,3,"Sliding",1,1,"1 cell,  L3 cell-level RSRP ","1 cell,  L3 cell-level RSRP ","AI: Transformer","Transfomer encoder",160,1220,null,"2644 trajectories","660 trajectories",2.1800000000000002]
["Qualcomm",2,"2G->4G, Cell-based, M1P4 sparse measurements on 4GHz","<=1280",0.96599999999999997,30,"A ","YES","YES","FULL",2,3,"Sliding",1,1,"1 cell,  L3 cell-level RSRP ","1 cell,  L3 cell-level RSRP ","AI: Transformer","Transfomer encoder",160,1220,null,"2644 trajectories","660 trajectories",1.51]
["China Telecom",2,"2G->4G, Cell-based",400,0.99,30,"A","NO","YES","FULL",1,3,"Non-sliding",1,1,"1 cell,  L3 cell-level RSRP ","1 cell,  L3 cell-level RSRP ","AI: LSTM","1 LSTM layers and 1 full-connectivity layer",31.05,121.29,0.06,207.4,51.8,0.27]
["China Telecom",2,"2G->4G, Cell-based",600,0.99,30,"A","NO","YES","FULL",1,3,"Non-sliding",1,1,"1 cell,  L3 cell-level RSRP ","1 cell,  L3 cell-level RSRP ","AI: LSTM","1 LSTM layers and 1 full-connectivity layer",31.05,121.29,0.1,207,51.7,0.24]
["China Telecom",2,"2G->4G, Cell-based",800,0.99,30,"A","NO","YES","FULL",1,3,"Non-sliding",1,1,"1 cell,  L3 cell-level RSRP ","1 cell,  L3 cell-level RSRP ","AI: LSTM","1 LSTM layers and 1 full-connectivity layer",31.05,121.29,0.13,206.6,51.6,0.27]
["China Telecom",2,"2G->4G, Cell-based",400,0.99,60,"A","NO","YES","FULL",1,3,"Non-sliding",1,1,"1 cell,  L3 cell-level RSRP ","1 cell,  L3 cell-level RSRP ","AI: LSTM","1 LSTM layers and 1 full-connectivity layer",31.05,121.29,0.06,92.6,23.2,0.31]
["China Telecom",2,"2G->4G, Cell-based",600,0.99,60,"A","NO","YES","FULL",1,3,"Non-sliding",1,1,"1 cell,  L3 cell-level RSRP ","1 cell,  L3 cell-level RSRP ","AI: LSTM","1 LSTM layers and 1 full-connectivity layer",31.05,121.29,0.1,92.2,23.1,0.3]
["China Telecom",2,"2G->4G, Cell-based",800,0.99,60,"A","NO","YES","FULL",1,3,"Non-sliding",1,1,"1 cell,  L3 cell-level RSRP ","1 cell,  L3 cell-level RSRP ","AI: LSTM","1 LSTM layers and 1 full-connectivity layer",31.05,121.29,0.13,91.8,23,0.31]
["China Telecom",2,"4G->2G, Cell-based",400,0.99,30,"A","NO","YES","FULL",1,3,"Non-sliding",1,1,"1 cell,  L3 cell-level RSRP ","1 cell,  L3 cell-level RSRP ","AI: LSTM","1 LSTM layers and 1 full-connectivity layer",31.05,121.29,0.06,207.4,51.8,0.26]
["China Telecom",2,"4G->2G, Cell-based",600,0.99,30,"A","NO","YES","FULL",1,3,"Non-sliding",1,1,"1 cell,  L3 cell-level RSRP ","1 cell,  L3 cell-level RSRP ","AI: LSTM","1 LSTM layers and 1 full-connectivity layer",31.05,121.29,0.1,207,51.7,0.22]
["China Telecom",2,"4G->2G, Cell-based",800,0.99,30,"A","NO","YES","FULL",1,3,"Non-sliding",1,1,"1 cell,  L3 cell-level RSRP ","1 cell,  L3 cell-level RSRP ","AI: LSTM","1 LSTM layers and 1 full-connectivity layer",31.05,121.29,0.13,206.6,51.6,0.26]
["China Telecom",2,"4G->2G, Cell-based",400,0.99,60,"A","NO","YES","FULL",1,3,"Non-sliding",1,1,"1 cell,  L3 cell-level RSRP ","1 cell,  L3 cell-level RSRP ","AI: LSTM","1 LSTM layers and 1 full-connectivity layer",31.05,121.29,0.06,92.6,23.2,0.32]
["China Telecom",2,"4G->2G, Cell-based",600,0.99,60,"A","NO","YES","FULL",1,3,"Non-sliding",1,1,"1 cell,  L3 cell-level RSRP ","1 cell,  L3 cell-level RSRP ","AI: LSTM","1 LSTM layers and 1 full-connectivity layer",31.05,121.29,0.1,92.2,23.1,0.31]
["China Telecom",2,"4G->2G, Cell-based",800,0.99,60,"A","NO","YES","FULL",1,3,"Non-sliding",1,1,"1 cell,  L3 cell-level RSRP ","1 cell,  L3 cell-level RSRP ","AI: LSTM","1 LSTM layers and 1 full-connectivity layer",31.05,121.29,0.13,91.8,23,0.3]
["ZTE",2,"2G->4G, cell based",null,0.98399999999999999,"30","A","NO","YES","YES",3,2,"Non-sliding",4,1,"1 cell, L3 cell-level RSRP","1 cell, L3 cell-level RSRP","AI: Full connection network","7 hidden layers",0.48599999999999999,2.048,5.0000000000000001E-3,90,5,0.99]
["ZTE",2,"2G->4G, cell based",null,0.97799999999999998,"30","A","NO","YES","NO",3,2,"Non-sliding",4,1,"1 cell, L3 cell-level RSRP","1 cell, L3 cell-level RSRP","AI: Full connection network","7 hidden layers",0.48599999999999999,2.048,5.0000000000000001E-3,90,5,1.38]
["ZTE",2,"2G->4G, cell based ",null,0.98399999999999999,"90","A","NO","YES","YES",3,2,"Non-sliding",4,1,"1 cell, L3 cell-level RSRP","1 cell, L3 cell-level RSRP","AI: Full connection network","7 hidden layers",0.48599999999999999,2.048,5.0000000000000001E-3,90,5,0.99]
["ZTE",2,"2G->4G, cell based",null,0.97699999999999998,"90","A","NO","YES","NO",3,2,"Non-sliding",4,1,"1 cell, L3 cell-level RSRP","1 cell, L3 cell-level RSRP","AI: Full connection network","7 hidden layers",0.48599999999999999,2.048,5.0000000000000001E-3,90,5,1.4]
["ZTE",2,"4G->2G, cell based",null,0.98399999999999999,"30","A","NO","YES","YES",3,2,"Non-sliding",4,1,"1 cell, L3 cell-level RSRP","1 cell, L3 cell-level RSRP","AI: Full connection network","7 hidden layers",0.48599999999999999,2.048,5.0000000000000001E-3,90,5,1]
["ZTE",2,"4G->2G, cell based",null,0.97799999999999998,"30","A","NO","YES","NO",3,2,"Non-sliding",4,1,"1 cell, L3 cell-level RSRP","1 cell, L3 cell-level RSRP","AI: Full connection network","7 hidden layers",0.48599999999999999,2.048,5.0000000000000001E-3,90,5,1.39]
["ZTE",2,"4G->2G, cell based",null,0.98399999999999999,"90","A","NO","YES","YES",3,2,"Non-sliding",4,1,"1 cell, L3 cell-level RSRP","1 cell, L3 cell-level RSRP","AI: Full connection network","7 hidden layers",0.48599999999999999,2.048,5.0000000000000001E-3,90,5,1]
["ZTE",2,"4G->2G, cell based",null,0.97699999999999998,"90","A","NO","YES","NO",3,2,"Non-sliding",4,1,"1 cell, L3 cell-level RSRP","1 cell, L3 cell-level RSRP","AI: Full connection network","7 hidden layers",0.48599999999999999,2.048,5.0000000000000001E-3,90,5,1.43]

{"sheet":"Sheet1","index":3,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}