**3GPP TSG RAN2 Meeting #116bis-eR2-2xxxxx**

**Online, 17 – 25 January 2022**

**Title:** LS on MBS issues

**Response to:**

**Release:** Rel-17

**Work Item:** NR\_MBS-Core

**Source:** RAN2

**To:** RAN1

**Cc:** -

**Contact Person:**

**Name:** Dawid Koziol

**E-mail:** dawid.koziol@huawei.com

**Send any reply LS to: 3GPP Liaisons Coordinator,** **mailto:3GPPLiaison@etsi.org**

**1. Overall Description:**

RAN2 would like to thank RAN1 for providing the list of L1 parameters to be configured with RRC signalling. RAN2 has discussed some aspects related to this topic and would like to ask RAN1 the following question.

**Question:** Currently, RAN2 running RRC design assumes that only a single CFR (defined by location and bandwidth) is configured for MCCH/MTCH reception of MBS broadcast and it is common for MCCH and all MTCHs. RAN2 would like to confirm this understanding with RAN1.

Furthermore, RAN2 has decided to include MCCH/MTCH search space configuration of MBS broadcast as part of PDCCH-ConfigCommon, to have a unified configuration framework for all common search spaces.

**2. Actions:**

**To RAN1 group:**

**ACTION:** RAN2 respectfully asks RAN1 to take the above into account and answer the above question.

**3. Dates of next TSG-RAN WG2 meetings:**

RAN2#117-e 21 February – 3 March 2022 Online

RAN2#118-e 16 – 27 May 2022 Online