**3GPP TSG-CT WG1 Meeting #128-eC1-21yyyy**

**Electronic meeting, 25 February – 5 March 2021 rev of C1-210640**

|  |
| --- |
| *CR-Form-v12.1* |
| **CHANGE REQUEST** |
|  |
|  | **24.302** | **CR** | **0723** | **rev** | **1** | **Current version:** | **17.0.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | Inclusive language review – TS 24.302 |
|  |  |
| ***Source to WG:*** | OPPO |
| ***Source to TSG:*** | C1 |
|  |  |
| ***Work item code:*** | TEI17 |  | ***Date:*** | 2021-02-26 |
|  |  |  |  |  |
| ***Category:*** | **D** |  | ***Release:*** | Rel-17 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)...Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)* |
|  |  |
| ***Reason for change:*** | In [SP-201143](https://www.3gpp.org/ftp/tsg_sa/TSG_SA/TSGs_90E_Electronic/Docs/SP-201143.zip), from SA#90e, SA has suggested that all TSG WGs should align their TS to more inclusive and neutral language.In [C1-210516](https://apc01.safelinks.protection.outlook.com/?url=https%3A%2F%2Fwww.3gpp.org%2Fftp%2Ftsg_ct%2FWG1_mm-cc-sm_ex-CN1%2FTSGC1_128e%2FDocs%2FC1-210516.zip&data=04%7C01%7Cchin.chenho%40OPPO.COM%7Cbdbd70f8a54249e2372f08d8cddcfe2d%7Cf1905eb1c35341c5951662b4a54b5ee6%7C0%7C0%7C637485697948643352%7CUnknown%7CTWFpbGZsb3d8eyJWIjoiMC4wLjAwMDAiLCJQIjoiV2luMzIiLCJBTiI6Ik1haWwiLCJXVCI6Mn0%3D%7C3000&sdata=vbrJ7ACNTfcKUoFasz2QPBTYcFiLWVhlYmHy5iIZBFY%3D&reserved=0), RAN2 has indicated the inclusive language they have used and suggested that CT1 might use those same terms.  |
|  |  |
| ***Summary of change:*** | Exclusive language changed to inclusive language |
|  |  |
| ***Consequences if not approved:*** | Non-inclusive language exist in TS 24.302 |
|  |  |
| ***Clauses affected:*** | 8.1.4.17.2 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

\* \* \* First Change \* \* \* \*

##### 8.1.4.17.2 Access causes

Access cause #2- Non-3GPP access to EPC not allowed

 This cause is used by the network to indicate that the requested service was rejected due to the user subscription data does not support EPS services from non-3GPP access.

Access cause #3- RAT type not allowed

This cause is used by the network to indicate that the requested service was rejected due to the WLAN is not allowed.

Access cause #6- Illegal ME

 This cause is sent to the UE if the ME used is not acceptable to the network, e.g. prohibit listed.

Access cause #11- PLMN not allowed

 This cause is used by the network to indicate that the requested service was rejected due to the PLMN where the UE is roaming into is not allowed.

\* \* \* End of Changes \* \* \* \*