Documents for TSGN1 meeting #12, Ihilani, Hawaii	Yellow cells indicate an allocated but not available Tdoc	
Agenda item	Agenda item title	Tdoc 3GPP N1-00	Title	Spec.	Source	Result	
1	Opening						
2	Agenda & Reports	0567	Agenda		N1 Chairman	Noted.	
		0568	TSGN#7 meeting report		MCC	Noted.	
		0569	S2/CN1 meeting report		MCC	Noted.
SIP was chosen as the multimedia protocol for R00	
		0570	S2/CN meeting report		MCC	Noted.	
		0574	D R A F T meeting report v. 1.0.0. ( 3GPP Workshop on TrFO and TFO harmonization/ Stockholm, Sweden 8 May 2000)		MCC	Noted.	

							
3	Input Liaison statements						
		0576	LS on RRC Connection Re-establishment mechanism		R2	Noted.
Originally N1 decided that a reply is needed, tdoc N1-000695 was allocated, editor Koshimizu san.
Later it was confirmed by R2 that the questions they ask have already been answered and no LS is needed.
Questions regarding the SERVICE REQUEST retransmission. A retransmission timer and the max. time = retransmission timer * max. number of attempts is also being asked.	
		0577	Correction for mobile stations staying in GMM READY virtually for ever		SMG2	N1 reply needed. CRs in tdocs 648 to 657 to be discussed first. Reply LS by Monica in tdoc N1-000696.
Discussion on whether the correction should apply to R99 only or R97 and R98 too.
SMG2 propose the change of READY timer behaviour in order to save network resources and MS battery capacity.
Related CRs are in tdocs 648 – 657	
		0578	Introduction of 3G MS capabilities in MS Classmark 3 (Introduction of 3G MS capabilities in MS Classmark 3)	24.008	SMG2WPA, SMG2	N1 reply in tdoc N1-000698 (Duncan)
The attached CR was separated to a standalone CR in tdoc N1-000697.
Proposal to add FDD, TDD, CDMA2000 radio technology indication to MS CM.	
		0579	Reply to N1 on ACS and ICM (Active Codec Set and Initial Codec Mode for the Adaptive Multi Rate speech codec)		S4	Noted.
S4 accepts and agrees with N1's proposal that ICM is not needed.
Linked with N1-000588.	
		0580	Response to LS (N1-99F55) on Maximum size of N-PDU		CN3	Noted.
TSG CN3 has studied the increase of 1500 to 1502 octets for the PDP type PPP and has concluded that there is no impact on their specifications for the R reference point (27.060) and the Gi interface (29.061).
The matter needs to be revisited if the N-PDU size is further increased for later releases.	
		0581	LS on additional impacts on Q.931		CN3	Noted.
N3 proposes change to Q.931 (ITU-T's ISDN-spec) to avoid modem code point collision with ETS 300 102. For N1 info.	
		0582	LS on Service Modification without Pre-notification		CN3	N1 action and reply is needed. Tdoc N1-000691 is a CR proposing the change. LS to N3 in Tdoc N1-000699 (Igarashi san)
N3 ask N1 to incorporate "Bearer Modification between Speech and FAX and between Speech and modem during no TrFO (Transcoder Free Operation)" to 24.008 etc. 	
		0583	Response Liaison on new Specification “Application Part (RANAP) on the E-interface”; 29.108		CN4	Noted.
N4 reply to our LS N1-000511 and agree that a new specification for RANAP on the E-interface is needed but are not convinced that they are the right group for its maintenance. N4 propose the responsibility for R3. LS was also sent to R3 proposing this. No N1 action required.
R3 reply is in N1-000596	
		0584	Response (to TSG-SA WG2, copy TSG-SA WG1, TSG-RAN WG3, TSG-CN WG1 and TSG-CN WG2) to LS (S2-000302) on RAB information and Lossless RNS relocation signalling		R2	Noted.
RAN WG2 especially considered the suggestion from SA WG2 to keep the PDCP Sequence Number range of 0 to 255 but came to the conclusion that for high data rates this range may be insufficient. Consequently R2 decided to increase the range to 0 – 65565.
S2 reply in N1-000598.	
		0585	Response on LS (R3-000917) on Paging cause in UTRAN protocols		R2	Noted.
The original R3 LS proposes action to R2 and N1. This needs to be distributed to N1 also.
Paging cause discussion is still ongoing in R2 and they would like to hold the related R3 CR to come to a common decision.	
		0586	Response to LS (N1-000493) on MS initiated signaling connection release		R2	Reply LS by Hannu back to R2 in tdoc N1-000700. The contents depends on the decision on CR in N1-000632.
This LS is the reply to N1-000493 on UE initiated signaling connection release. R2 say they will do their part on 25.331 for R99.
Related N1 CR is in tdoc N1-000632.	
		0587	Response to LS (N1-000542) on Support of Idle mode DRX control in GMM Proposed LS on idle mode DRX  control in GMM		R2	N1 action is needed, Per's LS in tdoc N1-000701 will summarise the decisions on N1-000616.
Related R3 reply is in tdoc N1-000594.
Related CR is in tdoc N1-000616	
		0588	Response to LS (N1-000553) on Transport of Codec Information during the Codec Negotiation between UE and MSC		R2	Phil to draft a reply LS in N1-000702. The contents will be based on the discussion of document N1-000636.
R2 sees a backward compatibility problem if R99 does not support codec negotiation but later releases do, and ask N1 to work further on codec negotiation. 
Relocation from R00 to R99 with change of codec would require changes to RANAP protocol.
Linked with N1-000636.	
		0589	Response to LS (S1-000103) on UE/MS idle mode operation		R2	Olivier to draft a reply to N1-000589, 597 and 624 in N1-000703 following the discussion on CR N1-000630.
3GPP workshop on PLMN and cell selection decided that "the PLMN selection should be performed prior to the mode selection and the cell selection, i.e. the PLMN is chosen first and, once the PLMN is selected, the choice of the mode has to be decided among the ones offered by the chosen PLMN."
Linked with LS in N1-000597 and 624	
		0590	LS on coding of RAB ID		R3- IU SWG	Noted.
R3 asks N1 to remove the coding of NAS Binding Information from 24.008.	
		0591	Response to N1 Liaison Statement “Question about Idle-mode DRX control”		R3- Iu SWG	Withdrawn.
This document was already handled in Umeå.
N1 action is needed, decide on CR N1-000616 first.
Related R2 LS in in tdoc N1-000587 and R3 LS in N1-000594.
Related CR is in tdoc N1-000616	
		0592	LS on timing between RAB Assignment Response and user data		R3	Noted.
	
		0593	Response Liaison to SA4 on Harmonization of TFO and TrFO		R3	Noted.
R3  asks S2 to organize a workshop on TFO/TrFO. For info.	
		0594	Respond to LS "Support of Idle-mode DRX control in GMM"		R3	N1 action is needed, Per's LS in tdoc N1-000701 will summarise the decisions on N1-000616.
Related other LSs are in tdoc N1-000587.
Related CR is in tdoc N1-000616	
		0595	LS to N1 on including the SAI into the Gs-i/f BSSAP+-LOCATION-UPDATE-REQUEST message as requested in N1-000543.		R3	Uda san's LS in N1-000639
SAI as an mandatory parameter to the Gs-i/f BSSAP+-LOCATION-UPDATE-REQUEST message, N1-000543. R3 would like to ask us to reconsider this CR. 	
		0596	Response LS to N4 on new specification 29.108 “Application of the Radio Access Network Application Part (RANAP) on the E-interface”		R3	Noted already.
R3 reply to N1-000583 from N4.
RAN WG3 received the LS from CN WG4 (N4-000084 resp. R3-001014) on the new specification TS 29.108 and whould like to inform them, that we decided to take over the responsibility for it.	
		0597	LS on UE/MS idle mode operation		S1	Olivier to draft a reply to N1-000589, 597 and 624 in N1-000703 following the discussion on CR N1-000630.

S1 would like to stress the fact that two different technologies corresponding to two licenses belonging to the same operator in the same country might (following a regulatory choice) be accessed via two different PLMN.

S1 would also like to clarify the fact that the PLMN selection procedure for Release 99 was modified. The modifications were accepted during SA#6 and are reflected in 22.011 v3.1. Among these modifications, a technology flag was introduced for each entry in the PLMN selector fields which allows for selection of a preferred technology along with the selection of a preferred PLMN. Thus PLMN selection is not performed prior to the mode selection, but concurrently.
Related LS in Tdoc N1-000589 and 624.	
		0598	Liaison statement on RAB information and Lossless RNS relocation signalling		S2	Noted.
S2 have seen R2 decision to extend the PDCP sequence number beyond one octet length. They would like to get some more evidence from R2 that the way they have chosen can work and for SNDCP use one octet sequence numbering is still being proposed.
S2 response to R2 LS in N1-000584.	
		0599	LS on UE triggered authentication and key agreement during connections		S3	N1 reply in tdoc N1-000709 (Duncan)
N1 agreed that this security related work could be carried out as R00 work item. IGC contact person Chris Pudney / Vodafone to define which WG would need to originate the WI description for TSG #8 approval.
Mobile can trigger authentication after the old CK and IK have been used for the maximum allowed time.
This is a R00 proposal but we are asked to study if it would be feasible as a late R99 change.	
		0600	Reply to LS on Requirements for Network Selection		T1	Noted.
T1 are warning that they are reaching the limit of PLMN selection test cases.
"Due to resource limitations, it is felt by T1 that it will not be possible to include further test cases, to cover these new requirements, in the release 99 documents.
T1 would however welcome relevant contributions from the member companies who feel that test coverage of these issues in release 99 is important."	
		0601	Liaison statement on usage of terms GSM, UMTS and GERAN		S1	N1 reply in Hannu's LS, tdoc N1-000710.
"TSG SA WG1 has certain concerns on usage of the terms UMTS and GSM as proposed by the TSG CN WG1. The S1 view is that when specifications refer to different access technologies (like GERAN/UTRAN) those names should be used."
Later on the email discussion pointed out that even these are not the best alternatives and so 2G mode of operation and 3G mode of operation is being suggested.
Related CRsin tdoc N1-000631, 694, 711	
		0602	Modem type code points		SPAN5	Noted.
LS response with no reference. Same issue as in 581? N1 (or N3?) concern recognized, but some errors in the original LS clarified. For N1 info (and N3 action)?
Reply to N1-000581
Related CR N1-000610	
		0611	Request for feedback on TR22.976 Study on Release 2000 services and capabilities	22.976	S1 Release 2000 adhoc	Noted.
22.976 review is requested by S1 R00 adhoc group.
If there are comments during this meeting let's note them and if ask the delegations to take this into account in their R00 contributions.
"TR22.976 identifies the Release 2000 services requirements.  The report identifies the high level vision of Release 2000"	
		0612	Call control between the UE and CSCF within the R00 architecture		S2-CN1 joint meeting	Noted.
This LS states the decisions of S2 – CN R00 joint meeting in April.	
		0613	Terminal capability negotiation including codecs		T2- SWG3 MMS adHoc	Edgar's LS in tdoc N1-000712
T2 SWG 3 MMS adHoc group ask some (basic) questions about indication/negotiation of terminal (codec ) capabilities.	
		0621	LS on the introduction of  a user controlled switch of the priority of the user and operator preferred PLMN list		S1	Olivier's LS in N1-000713 to reply to S1.
What is the real issue here? Is it to ensure that if the user controlled PLMN selector list is empty then the operator controlled list will not be skipped or is it to really provide the user the chance to change the priority?
N1 is of the opinion that the problem pointed out by S1 does not exist. An empty user controlled list does not mean skipping the operator controlled list. 
The change only works if none of the PLMN selector lists is empty. The reason for the 22.011 CR to be clarified by Dieter.
By default the user controlled PLMN selector list takes higher priority than the operator controlled PLMN selector list. S1 have agreed that the user may change this priority order of the two selector lists.	
		0622	Deletion of PDP types X.25 and OSP		S1	Noted.
In this reply S1 promised to N3 to make the CRs on Deletion of X.25 and Interworking with ISDN / PSTN.
Possible N1 action (Radio IF code points!) should follow the stage 1 changes made by S1.	
		0623	Liaison statement on Global "Cause of no ID"		S1	Ohtsuki san's LS to reply to S1 and N4 in N1-000714.
The reply should state N1 decisions on N1-000673 and 674.
S1 states requirements for "Cause of no ID" – a globally compatible solution.
Linked CR and discussion document in N1-000673 and 674.	
		0624	LS on PLMN selection		S1	Olivier to draft a reply to N1-000589, 597 and 624 in N1-000703 following the discussion on CR N1-000630.
S1 asks R2 (and others to take the requirements in 22.011 as working assumption.
Related LS in Tdoc N1-000589 and 597.	
		0625	Liaison statement on hexadecimal IMEI format		S1	Hannu's LS in N1-000715.
Proposal to change at least the SNR part of the IMEI from BCD to hex coding for R00 to increase the  maximum length of terminal production series using single TAC and FAC.
S1 ask the WGs to study the technical impact of the proposal and also to check if it would be feasible to approve a late R99 change at this stage.
•	N1 needs to make a change to 24.008 but we need S3 decision on dummy IMEI first.
•	For R00 the support of hex IMEI should be mandatory for the network while it was suggested that the R99 change would be more acceptable if it was optional for the network or only applies after a certain date.	
		0690	GPRS ciphering		S3	Reply in Monica's LS N1-000778	
		0752	LS on Service Modification without Pre-notification		T2	Noted.	
		0753	LS on Race conditions avoidance		N4	Noted.	
		0754	LS response on Service Modification without Pre-notification		N4	Noted.	
		0776	LS about hexadecimal coding of IMEI		S3	Reply in N1-000715.
Related CR in Tdoc N1-000779.	
		0777	LS on paging cause in UTRAN protocols			R3		Noted.
Related LS in N1-000585	
		0800	Proposal of exchange of the terms “in GSM“ and “in UMTS“		S2	Noted. 
Forwared to the next TSGN1 meeting	
		0801	GPRS connection set up by SIM to create a channel between SIM and the end point destination		T3	Noted. 
Forwared to the next TSGN1 meeting	
		0802	Answer to LS on Removal of Service Accept		S2	Noted. 
Forwared to the next TSGN1 meeting	

							
							
4	Maintenance of R98 and older releases						
4.1	Corrections						
		0618	Network initiated DETACH REQUEST sent unciphered	04.08	Ericsson/ Per	Rejected
	
		0648	Discussion paper - Operation of the GPRS READY timer at Cell Update		Ericsson/ Monica Wifvesson	Revised to N1-000723	
		0649	Change of the GMM Ready Timer behaviour 	04.07	Ericsson /Monica Wifvesson	Revised to N1-000724	
		0650	Change of the GMM Ready Timer behaviour 	04.07	Ericsson/ Monica Wifvesson	Revised to N1-000725	
		0651	Change of the GMM Ready Timer behaviour 	24.007	Ericsson/ Monica Wifvesson	Revised to N1-000726	
		0652	Change of the GMM Ready Timer behaviour 	04.08	Ericsson/ Monica Wifvesson	Revised to N1-000727	
		0653	Change of the GMM Ready Timer behaviour 	04.08	Ericsson/ Monica Wifvesson	Revised to N1-000728	
		0654	Change of the GMM Ready Timer behaviour 	24.008	Ericsson/ Monica Wifvesson	Revised to N1-000729	
		0655	Change of the GMM Ready Timer behaviour 	03.60	Ericsson/ Monica Wifvesson	Revised to N1-000730	
		0656	Change of the GMM Ready Timer behaviour	03.60	Ericsson/ Monica Wifvesson	Revised to N1-000731	
		0657	Change of the GMM Ready Timer behaviour	23.060	Ericsson/ Monica Wifvesson	Revised to N1-000732	
		0687	Clarification on TLLI management	04.08	Alcatel/ Tony Huynh-Quang	Revised to N1-000760
	
		0688	Clarification on TLLI management	04.08	Alcatel/ Tony Huynh-Quang	Revised to N1-000761	
		0689	Clarification on TLLI management	24.008	Alcatel/ Tony Huynh-Quang	Revised to N1-000762	
		0723	Discussion paper - Operation of the GPRS READY timer at Cell Update		Ericsson/ WifesonSiemens	Noted.
Analysis that due to frequent cell updates in dense network the MS may stay in READY state consuming network resources much longer than indicated by the READY timer.
•	It was agreed that it is now too late to change R97 or R98 for this. R99 can be considered.
•	No objection against the principle in R99.
•	In order to work at all the feature must be made mandatory from R99 onwards.
Revision of N1-000648	
		0724	Change of the GMM Ready Timer behaviour	04.07	Ericsson/Wifeson, Siemens /Schramm	Rejected.

Revision of N1-000649	
		0725	Change of the GMM Ready Timer behaviour	04.07	Ericsson/Wifeson, Siemens /Schramm	Rejected.

Revision of N1-000650	
		0726	Change of the GMM Ready Timer behaviour	24.007	Ericsson/Wifeson, Siemens /Schramm	Revised to N1-000764

Revision of N1-000651	
		0727	Change of the GMM Ready Timer behaviour	04.08	Ericsson/Wifeson, Siemens /Schramm	Rejected.

Revision of N1-000652	
		0728	Change of the GMM Ready Timer behaviour	04.08	Ericsson/Wifeson, Siemens /Schramm	Rejected.

Revision of N1-000653	
		0729	Change of the GMM Ready Timer behaviour	24.008	Ericsson/Wifeson, Siemens /Schramm	Revised to N1-000765

Revision of N1-000654	
		0730	Change of the GMM Ready Timer behaviour	03.60	Ericsson/Wifeson, Siemens /Schramm	Rejected.

Revision of N1-000655	
		0731	Change of the GMM Ready Timer behaviour	03.60	Ericsson/Wifeson, Siemens /Schramm	Rejected.

Revision of N1-000656	
		0732	Change of the GMM Ready Timer behaviour	23.060	Ericsson/Wifeson, Siemens /Schramm	Revised to N1-000766

Revision of N1-000657	
		0733	Change of the GMM Ready Timer behaviour	04.64	Ericsson/Wifeson, Siemens /Schramm	Rejected.	
		0734	Change of the GMM Ready Timer behaviour	04.64	Ericsson/ Wifeson, Siemens /Schramm	Rejected.	
		0735	Change of the GMM Ready Timer behaviour	04.64	Ericsson/ Wifeson, Siemens /Schramm	Revised to N1-000767
Now go back to 577 and discuss the reply LS!	
		0760	Clarification on TLLI management	04.08	Alcatel/ Tony Huynh-Quang	Agreed.
Revision of N1-000687	
		0761	Clarification on TLLI management	04.08	Alcatel/ Tony Huynh-Quang	Agreed.
Revision of N1-000688	
		0762	Clarification on TLLI management	24.008	Alcatel/ Tony Huynh-Quang	Agreed.
Revision of N1-000689	
		0763	Change of the GMM Ready Timer behaviour	24.007	Ericsson/Wifeson, Siemens /Schramm	Agreed.

Revision of N1-000726	
		0764	Change of the GMM Ready Timer behaviour	24.008	Ericsson/Wifeson, Siemens /Schramm	Revised to N1-000791

Revision of N1-000729	
		0765	Change of the GMM Ready Timer behaviour	23.060	Ericsson/Wifeson, Siemens /Schramm	Revised to N1-000793

Revision of N1-000732	
		0766	Change of the GMM Ready Timer behaviour	04.64	Ericsson/ Wifeson, Siemens /Schramm	Revised to N1-000792
Tdoc number and revision (r1) to be changed by Ban
Now go back to 577 and discuss the reply LS!
Revision of N1-000735	
		0791	Change of the GMM Ready Timer behaviour	24.008	Ericsson/Wifeson, Siemens /Schramm	Agreed.

Revision of N1-000764	
		0792	Change of the GMM Ready Timer behaviour	04.64	Ericsson/ Wifeson, Siemens /Schramm	Agreed.

Revision of N1-000766	

We need rapporteurs for our specifications!!!

5 	Work Plan for TSGN WG1 for 2000					TSGN1 #10 11.-14.1.2000 (Abiko, Japan/NEC)
GPRS Ad-Hoc  19.-20.1.2000 (Oslo/ Motorola)
SMG#31 14.-18.2.2000
TSGN1 #11 28.2.-3.3.2000 (Umeå, Sweden/Telia)
TSGN#7  13.-15.3.2000
TSGS2 – TSGN1 Ad-hoc on CC and Architecture 11.-13.4.2000
TSGS2 – TSGN ad-hoc on R00 work planning 13.-14.4.2000
TSGN1 #12 22.-26.5.2000 (Hawaii, U.S./T1P1)
TSGN – S3 ad-hoc on R00 requirements 
    13-14.6.2000
TSGN – S2 WI R00 WI drafting 14.-15.6.2000
SMG#32 19.-20.6.2000
TSGN#8  21.-23.6.2000
TSGN1 #13 14.-18.8.2000 (U.S./T1P1)
Please not new meeting date. 
TSGN#9  20.-22.9.2000
SMG#33 6.-10.11.2000
TSGN1 #14 20.11 – 24.11.2000 (UK, Lucent) 
TSGN#10  6.-8.12.2000	
		0571	List of specs/ Rapporteurs		MCC	Revised to N1-000718	
		0572	Features, Building Blocks and Work Tasks - V.1.0		MCC/IGC	Revised to N1-000782.
	
		0575	Open Issues for Release 99 List		MCC/SA	Noted.	
		0662	Change of rapporteur for GSM 03.60, 04.64, 04.65, and 3G TS 23.060		Hans Petter Naper / Motorola	Noted
Hans is resigning from his rapporteurships and we need to nominate new rapporteur for 04.64 and 04.65. Apostolis Salkintzis is being proposed for the task.	
		0718	List of specs/ Rapporteurs		MCC	Noted.
Revision of N1-000571	
		0782	Open Issues for Release 99 List		MCC/SA	Agreed.
R99 open items list from SA
•	The list was updated to current status.
•	Further updates should be provided to the rapporteurs of IGCs.
Revision of N1-000572.	
							
5.1	Election of TSGN1 Vice Chairman					Andrew Howell from Motorola was elected vice chairman of TSGN1.	
		0573	Election of Vice-chair procedure		MCC	Noted.	
		0680	Candidate - Andrew Howell		MCC	Noted.	
							
6	Release 99						
6.1	Multicall						
		0634	Clarification of the Description for Multicall	24.008	Ericsson/ Eiko	Withdrawn.	
		0638	CR to 23.009 on Handover scenario for Multicall	23.009	NTT Comware/ Nobuyuki Uda	Agreed.	
		0641	Clarifications for the description of Multicall	24.008	Ericsson/ Eiko Kato	Revised to 717	
		0717	Clarifications for the description of Multicall	24.008	Ericsson/ Eiko Kato	Withdrawn
Revision of 641	
		0781	N1 Work Item Status: Multicall	23.009	NTT Comware/Nobuyuki Uda	Agreed.	
							
6.2	Multimedia call		Frozen for R99			N1 Rapporteur: Timo Kauhanen / Nokia	
		0609	Applicability of circuit switched multimedia to GSM	24.008	Ericsson/ Rouzbeh Farhoumand	Withdrawn	
		0633	Applicability of CS Multimedia to GSM	24.008	Ericsson/ Rouzbeh	Agreed.	

6.3	GSM / UMTS interworking		Frozen for R99			N1 Rapporteur: Hannu Hietalahti / Nokia	
		0607	Clean-up of 3G_MSC-A_HO SDLs	23.009	Ericsson/Telelogic- Rouzbeh Farhoumand	Agreed.
Ask for approval on Thursday
All SDLs in 23.009 have now been changed, at least for the SDL tool part. The delegations are requested to check the latest versions of the SDLs.	
		0608	Clean-up of 3G_MSC-B_HO SDLs	23.009	Ericsson/Telelogic- Rouzbeh Farhoumand	Agreed.
Ask for approval on Thursday
All SDLs in 23.009 have now been changed, at least for the SDL tool part. The delegations are requested to check the latest versions of the SDLs.	
		0616	DRX value 0000 clarification and R97 compatibility issue	24.008	Ericsson/ Per	Revised to N1-000755.
Decide now on LSs in N1-000587 and 594 -> N1 reply in N1-000701.	
		0617	Compatibility issue due to deletion of SM cause #35	24.008	Ericsson/ Per	Revised to N1-000756	
		0619	Remove GRR primitive descriptions and make reference to other document	24.007	Ericsson/ Francesco	Agreed.	
		0620	Updating SM for R99	24.007	Ericsson/ Francesco	Agreed but the section numbering (VOID) to be corrected by the secretary.	
		0642	SAPs and Service primitives for UMTS	24.007	Ericsson/ Monica Wifvesson	Revised to N1-000757	
		0643	Editorial corrections to MM and GMM in 24.008	24.008	Ericsson/ Monica Wifvesson	Agreed.	
		0644	Removal of P-TMSI signature in Service Request message	24.008	Ericsson/ Monica Wifvesson	Rejected.
•	N1 can not decided whether P-TMSI signature should be included in the SERVICE REQUEST even though S2 have agreed a CR on 23.060 on this issue. BT, Lucent are objecting the proposal in this document.
Postponed, see the outcome of 683 and 790 first.	
		0645	P-TMSI and optionally P-TMSI signature sent in Detach Request in UMTS only	24.008	Ericsson/ Monica Wifvesson	Rejected.	
		0646	Removal of Service Accept message	24.008	Ericsson/ Monica Wifvesson	Could not be agreed but must go to TSGN #8 for plenary decision. The N1 LS N1-000758 and S2 LS N1-000802 along with the original S2 23.060 CR to be attached.
•	Related with S2 CR but N1 disagreed on the concept of implicit response to SERVICE REQUEST and deletion of SERVICE ACCEPT message as this would cause unnecessary inter-layer interfaces and provide little benefit in lover signalling load.
•	S2 LS in N1-000802: they have considered the removal of SERVICE ACCEPT and they still keep their original decision to remove it. 
•	This causes more complex implementation because of inter-layer primitives to indicate the implicit service acceptance.
•	Analogically CM SERVICE ACCEPT is most often omitted and implicit MM establishment is used instead by means of security procedure. But this can not be done for emergency calls with no SIM card as security procedures can not be applied. -> The same problem does exist with VoIP emergency calls without SIM. No answer to this problem could be given by N1.
Related LS out in N1-000758	
		0670	Correction of references in protocol error handling for SM	24.008	Siemens/ R.Zaus	Agreed.	
		0681	Immediate cancellation of PDP context activation	24.008	Fujitsu/Fumihiko Yokota	Revised to N1-000786
	
		0682	Modification of QoS to support max 0kbps	24.008	Fujitsu/Fumihiko Yokota	Revised to N1-000759
Work item is missing!	
		0683	Necessity of P-TMSI signature in SERVICE REQUEST	24.008	Fujitsu/Fumihiko Yokota	Noted.
If SERVICE REQ is sent in order to perform a re-establishment of a lost radio connection then this request should be authenticated and thus it would be useful have the P-TMSI signature included in SERVICE REQUEST. Three alternatives were seen:
•	P-TMSI never included in SERVICE REQUEST (S2 decision, 23.060 CR approved) causes additional signalling when auth. is needed.
•	P-TMSI always included in SERVICE REQ. (additional signalling for P-TMSI reallocation)
•	P-TMSI included in SERVICE REQ when necessary, either specified for re-est. or implementation option	
		0684	PDP context synchronisation procedure	24.008	Fujitsu/Fumihiko Yokota	Noted.	
		0685	Recovery from PDP context inconsistency 	24.008	Fujitsu/Fumihiko Yokota	Revised to N1-000775	
		0694	Use of the terms GSM and UMTS in 23.060, 24.008 etc.	24.008	Ericsson/ Monica Wifvesson	Noted, provided for information.	
		0697	Introduction of 3G MS capabilities in MS Classmark 3 (Introduction of 3G MS capabilities in MS Classmark 3)	24.008		Agreed.	
		0755	DRX value 0000 clarification and R97 compatibility issue	24.008	Ericsson/ Per	Agreed.
Decide now on LSs in N1-000701.
Revision of N1-000616.	
		0756	Compatibility issue due to deletion of SM cause #35	24.008	Ericsson/ Per	Agreed.
Revision of N1-000617.	
		0757	SAPs and Service primitives for UMTS	24.007	Ericsson/ Monica Wifvesson	Withdrawn.

Revision of N1-000642.	
		0759	Modification of QoS to support max 0kbps	24.008	Fujitsu/Fumihiko Yokota	Agreed.
Revision of N1-000682.	
		0775	Recovery from PDP context inconsistency 	24.008	Fujitsu/Fumihiko Yokota	Revised to N1-000807
Revision of N1-000685	
		0783	Architecture proposal regarding UMTS (MS side)	24.007	Siemens /Schramm	Withdrawn.	
		0786	Immediate cancellation of PDP context activation	24.008	Fujitsu/Fumihiko Yokota	Withdrawn.
•	The meeting analysed R99 specification and  agreed that it does not cover the issue of this CR.
•	It was agreed that the matter must be studied further in order to find a solution not just for R00 but also for R99.
Revision of N1-000681.	
		0790	P-TMSI signature in SERVICE REQUEST	24.008, 23.060 / R99, R00	Lucent Technologies/ Sudeep Palat	Noted.	
		0807	Recovery from PDP context inconsistency 	24.008	Fujitsu/Fumihiko Yokota	Agreed.
Ban to update the revision number to r2.
Revision of N1-000775	
							
6.4	MS Classmark		Frozen for R99			N1 Rapporteur: Fumihiko Yokota / Fujitsu
N1 part is complete	

6.5	Security		Security related issues which were completed by TSGN #7 were frozen for R99. 
Two more tasks can still be completed for R99 by TSGN #8:
•	MS reaction after failure of the network authentication by the MS 
•	Integrity protection of emergency calls 			N1 Rapporteur: Duncan Mills / Vodafone Airtouch
R99 status sheet to be provided for TSGN #8 presentation.	
		0647	Integrity checking of MM/GMM messages and integrity protection during emergency call	24.008	Vodafone- Ericsson/ Monica Wifvesson	Revised to N1-000744	
		0663	Network Authentication Failure	24.008	Duncan Mills / Vodafone AirTouch	Agreed.	
		0664	Alignment of CC and SM protocols with current MM/GMM integrity protection rules	24.008	Duncan Mills / Vodafone AirTouch	Revised to N1-000745	
		0665	Alignment of SS protocol with current MM/GMM integrity protection rules	24.010	Duncan Mills / Vodafone AirTouch	Revised to N1-000746	
		0666	Alignment of SMS protocol with current MM/GMM integrity protection rules	24.011	Duncan Mills / Vodafone AirTouch	Revised to N1-000747	
		0671	Correction of the MM Authentication procedure	24.008	Siemens/ R.Zaus	Revised to N1-000748	
		0672	Correction of the GMM Authentication and ciphering procedure	24.008	Siemens/ R.Zaus	Revised to N1-000749	
		0744	Integrity checking of MM/GMM messages and integrity protection during emergency call	24.008	Vodafone- Ericsson/ Monica Wifvesson	Agreed.

Revision of N1-000647.	
		0745	Alignment of CC and SM protocols with current MM/GMM integrity protection rules	24.008	Duncan Mills / Vodafone AirTouch	Agreed.

Revision of N1-000664	
		0746	Alignment of SS protocol with current MM/GMM integrity protection rules	24.010	Duncan Mills / Vodafone AirTouch	Agreed.

Revision of N1-000665	
		0747	Alignment of SMS protocol with current MM/GMM integrity protection rules	24.011	Duncan Mills / Vodafone AirTouch	Agreed.

Revision of N1-000666	
		0748	Correction of the MM Authentication procedure	24.008	Siemens/ R.Zaus	Revised to N1-000785
Revision of N1-000671	
		0749	Correction of the GMM Authentication and ciphering procedure	24.008	Siemens/ R.Zaus	Agreed.
Revision of N1-000672	
		0785	Correction of the MM Authentication procedure	24.008	Siemens/ R.Zaus	Agreed.
Revision of N1-000748	
		0789	Support of GEA/2 Encryption Algorithm	04.08	Ericsson/ Monica Wifvesson	Revised to N1-000798	
		0798	Support of GEA/2 Encryption Algorithm	04.08	Ericsson/ Monica Wifvesson	Agreed.
•	There was strong reservations from one company (BT) on whether this R98 CR should be acceptable. At least it must be clear that the support of the new ciphering algorithms is optional for R98 mobiles.
•	To be marked as strategic for TSGN #8 
•	The concern that this change makes R97 and R98 GPRS different was shared by several delegations.
•	To be forwarded to plenary together with N1-000722 separated from the other documents.
•	Category to be changed to B by the secretary	
		 0803	WI status sheet for security		Duncan 	Agreed.	
							
6.6	QoS		Frozen for R99				
		0614	Additional SDU error rate value	24.008	Ericsson/ Per	Revised to N1-000720	
		0615	TFT IE length and editorials	24.008	Ericsson/ Per	Agreed.	
		0660	Inclusion of PFC Feature Mode in MS Network Capability IE	24.008	Motorola/ Apostolis Salkintzis	Revised to N1-000722	
		0661	Reserve one bit in PFI	24.008	Motorola/ Apostolis Salkintzis	Agreed.	
		0720	Additional SDU error rate value	24.008	Ericsson/ Per	Agreed.
Revision of N1-000614	
		0722	Inclusion of PFC Feature Mode in MS Network Capability IE	24.008	Motorola/ Apostolis Salkintzis	Agreed.

Revision of N1-000660	

6.7	Out-of-Band Transcoder Control		AMR codec part frozen for R99			N1 Rapporteur: Rouzbeh Farhoumand / Ericsson
	
		0635	CR on 24008 for Uplink Supported Codecs	24.008	Ericsson/ Phil	Withdrawn.
	
		0636	Contribution on how to proceed with Downlink Selected Codec 	24.008	Ericsson/ Phil	Noted.
LS to R2 in N1-000795	
		0637	Codec Negotiation at Handover/Relocation	24.008	Ericsson/ Phil	Noted.
Presented for information. Email comments to the originator are invited.	
		0693	ACS(Active Codec Set) negotiation and notification		NTT DoCoMo	Noted.
Presented for information. Email comments to the originator are invited.	
		0808	Draft Report of the joint TSG-RAN WG2 / WG3 / TSG-CN WG1 meeting		TSG-RAN WG2	Noted.	
6.8	CC related Items		NOTE: Agenda item, not a work item. Please indicate also WI on your CR!				
							
6.9	R99 PLMN Selection
And EDGE		NOTE: Agenda item, not a work item. Please indicate also WI on your CR!			This item needs to be brought up early as PLMN selection is still under discussion  between T3 and R2.
N1-R2 ad-hoc meeting on PLMN selection 23.5.2000:
•	When searching for the RPLMN is the MS limited to indicated RAT or is it an educated guess where to start?
•	First the indicated RAT but if RPLMN is not found, then continue search through all supported RATs and Freq. Bands.
•	When searching for RPLMN in case of no indication of the RAT related with RPLMN is available is the default RAT the only one to be searched or is it just the first RAT to be searched?
•	Again this should be just the starting point to speed up the search in the successful case
•	The same principles shall apply when searching for HPLMN with or without an indication of the RAT(s)
•	Continuing this same principle to PLMN selector list search would mean scanning all RATs for each PLMN on the lists and that does not seem to be what N1 and R2 would propose. In this case we propose to limit the search to the RATs that are associated with each PLMN, if RATs have been indicated.
•	There will be 2 PLMN selector lists, user controlled and operator controlled. By default the user list is used for search first and the operator controlled after that. This priority order must be also user controlled.
•	After the search using the PLMN selector lists has failed the MS must search for any network in random order and here the first RAT to be searched should be an implementation option. But all RATs must be searched.
Improvement ideas:
•	How about the network broadcasting all of its RATs for the mobile to store at switch-off for the next RPLMN search? This would require updating also the old part of a multimode network to indicate the presence of the new network.
•	What is the point of having RAT in PLMN selector list at all? If RPLMN and HPLMN search have already been performed, then all supported RATs have already been searched and the results are readily available?
•	PLMN selector list search should be limited to the indicated RATs, if the indication is available.
•	For the search of PLMNs in descending order of signal strength the "exchange rate" between GERAN and UTRAN signal quality must be defined.	
		0630	Modification of PLMN Selection Procedures to support UMTS+COMPACT Network Selection	23.122	Ericsson/ Olivier Irac	Revised to N1-000719
•	If no RAT is indicated in PLMN / RAT list then is what is the default (GSM?) Does the MS limit the search to default only or does it start from the default RAT?
•	Registration via "all supported RATs" is not intended, but search on all RATs and then registration via the chosen one.
•	Which one takes higher priority, PLMN or RAT?
•	Is the MS limited to search only the indicated RATs e.g. when searching for HPLMN or is it allowed to continue from the other supported RATs after this search?
•	If no, how to update a GSM network to multimode? Change all USIMs?	
		0719	Modification of PLMN Selection Procedures to support UMTS+COMPACT Network Selection	23.122	Ericsson/ Olivier Irac	Revised to N1-000796

Revision of N1-000630.	
		0796	Modification of PLMN Selection Procedures to support UMTS+COMPACT Network Selection	23.122	Ericsson/ Olivier Irac	Agreed.	

6.10	Other R99 Issues		NOTE: Agenda item, not a work item. Please indicate also WI on your CR!				
		0667	Modification of MS Classmark 3 and modification of MS RA Capabilities, for DTM mobile stations.	24.008	Duncan Mills / Vodafone AirTouch	Agreed.
	
		0668	Protocol Discriminator to route packet data sent by a DTM mobile from BSC to PCU	24.007	Duncan Mills / Vodafone AirTouch	Agreed.	

6.11	TEI						
		0603	Alignment on ISDN BC Coding	24.008	T-Mobil, Jacobsohn	Agreed.
N1-000603 – 606 to be provided to TSGN #8 in separate document with the request for the manufacturers to check once more that they have not implemented this code point.	
		0604	Alignment on ISDN BC Coding	04.08	T-Mobil, Jacobsohn	Agreed.	
		0605	Alignment on ISDN BC Coding	04.08	T-Mobil, Jacobsohn	Agreed.	
		0606	Alignment on ISDN BC Coding	04.08	T-Mobil, Jacobsohn	Agreed.	
		0610	Clarification of reference to Q.931 for LLC IE	24.008	Ericsson/ Rouzbeh Farhoumand	Agreed.	
		0627	IMEI hex coding	24.008	Nokia/ Hannu Hietalahti	Revised to N1-000779
Corresponding N4 23.003 CR is subject to email approval in N4.	
		0669	Services provided by the Radio Resource Management entity	24.007	Motorola / A. Howell	Agreed. 
WI GSM – UMTS to be added by Ban.
What is flow identifier meant for?
For Thursday ad-hoc meeting with R2.	
		0673	Addition of “Cause of No ID” IE in SETUP message	24.008	NIPPON TELECOMMUNI-CATIONS CONSULTING/ Katsunobu OHTSUKI	Revised to N1-000716.
CR number and stategic / non-strategic not indicated
Incoming LS in N1-000623.
Linked discussion document in N1-000674.
	
		0674	Addition of ‘Cause of no ID’ description	24.008	NIPPON TELECOMMUNI-CATIONS CONSULTING/ Katsunobu OHTSUKI	Noted.
This is a discussion paper giving the reasoning for the linked CR in N1-000673. 	
		0716	Addition of “Cause of No ID” IE in SETUP message	24.008	NIPPON TELECOMMUNI-CATIONS CONSULTING/ Katsunobu OHTSUKI	Revised to N1-000742
CR number and stategic / non-strategic not indicated
Incoming LS in N1-000623.
Linked discussion document in N1-000674.
Revised from 673.	
		0742	Addition of “Cause of No ID” IE in SETUP message	24.008	NIPPON TELECOMMUNI-CATIONS CONSULTING/ Katsunobu OHTSUKI	Revised to N1-000750

Revised from N1-000716.	
		0750	Addition of “Cause of No CLI” IE in SETUP message	24.008	NIPPON TELECOMMUNI-CATIONS CONSULTING/ Katsunobu OHTSUKI	Provisionally agreed, subject to N4 decision on SS Stage 2 and Stage 3.

Revised from N1-000742.	
		0779	IMEI hex coding	24.008	Nokia/ Hannu Hietalahti	Agreed with editorial comments.
Corresponding N4 23.003 CR is subject to email approval in N4.
Revision of N1-000627	

6.12	R99 Corrections						
		0626	References and editorial corrections to 24.008	24.008	Nokia/ Hannu Hietalahti	Agreed.	
		0628	MODIFY PDP CONTEXT REJECT –message definition	24.008	Nokia/ Hannu Hietalahti	Revised to N1-000721	
		0629	Clarifications on GSM – UMTS interoperability	24.008	Nokia/ Hannu Hietalahti	Revised to N1-000736	
		0631	Alignment of 2G / 3G terminology in 23.122	23.122	Nokia / Hannu Hietalahti	Revised to N1-000711.	
		0632	MS behavior if RAU attempt counter is greater than or equal to 5	24.008	Nokia / Hannu Hietalahti	Revised to N1-000737
	
		0640	COMPACT Mobile Station Interference Measurements Capability	24.008	UWCC, Nokia / Hannu Hietalahti	Revised to N1-000780	
		0658	Network behaviour, abnormal cases detach	24.008	Siemens/ R.Zaus	Agreed.
WI GPRS (was not available for TdocList)	
		0659	IEI value of the 'Tear down indicator' IE	24.008	Siemens/ R.Zaus	Agreed.
WI GPRS (was not available for TdocList)	
		0711	Alignment of 2G / 3G terminology in 23.122	23.122	Nokia / Hannu Hietalahti	Withdrawn, 
needs S1, S2 definition of the correct terms.
Revision of N1-000631.	
		0721	MODIFY PDP CONTEXT REJECT –message definition	24.008	Nokia/ Hannu Hietalahti	Agreed.
Revision of N1-000628	
		0736	Clarifications on GSM – UMTS interoperability	24.008	Nokia/ Hannu Hietalahti	Agreed.
Revision of N1-000629	
		0737	MS behavior if RAU attempt counter is greater than or equal to 5	24.008	Nokia / Hannu Hietalahti	Revised to N1-000794.
Now we can decide upon the reply to LS N1-000586
Revision of N1-000632	
		0738	Call Release clarification at the Relay MSC		Nortel Networks	Agreed.
03.68 / ASCI	
		0739	Speech transmission architecture clarification		Nortel Networks	Agreed.
03.68 / ASCI	
		0740	Clarification of anchor MSC address format		Siemens AG	Agreed.
03.68 / ASCI. 	
		0741	Clarification of anchor MSC address format	03.69	Siemens AG	Agreed.
ASCI. 	
		0780	COMPACT Mobile Station Interference Measurements Capability	24.008	UWCC, Nokia / Hannu Hietalahti	Agreed.

Revision of N1-000640	
		0794	MS behavior if RAU attempt counter is greater than or equal to 5	24.008	Nokia / Hannu Hietalahti	Agreed.
Now we can decide upon the reply to LS N1-000586
Revision of N1-000737	

7	Release 2000						
7.1	L3 Segmentation		WI exists				

7.2	Turbocharger		WI exists, checkpoint at TSGN #8				

7.3	TEI		Which TSG should initiate this WI?				

7.4	Other R00 issues						
		0675	Originator-to-Dispatcher Information for VGCS and VBS		STF 139 	ASCI
•	Question about the compatibility, how does a R00 mobile know whether it is being served by a new or old network?
N1-000675, 676, 677, 678 and 679 are linked	
		0676	Introduction of Originator-to-dispatcher information into VGCS	03.68	STF 139 	Agreed.
N1-000675, 676, 677, 678 and 679 are linked and they will all be forwarded to TSGN #8 if the CRs and the transfer of the WI to 3GPP is approved by SMG #32.	
		0677	Introduction of Originator-to-dispatcher information into VGCS	04.68	STF 139	Agreed.
N1-000675, 676, 677, 678 and 679 are linked and they will all be forwarded to TSGN #8 if the CRs and the transfer of the WI to 3GPP is approved by SMG #32.	
		0678	Introduction of Originator-to-dispatcher information into VBS	03.69	STF 139 	Agreed.
N1-000675, 676, 677, 678 and 679 are linked and they will all be forwarded to TSGN #8 if the CRs and the transfer of the WI to 3GPP is approved by SMG #32.	
		0679	Introduction of Originator-to-dispatcher information into VBS	04.69	STF 139	Agreed.
N1-000675, 676, 677, 678 and 679 are linked and they will all be forwarded to TSGN #8 if the CRs and the transfer of the WI to 3GPP is approved by SMG #32.	
		0686	Protocol supporting LCS in PS-domain	24.008	Fujitsu/Fumihiko Yokota	Noted.
N1 working assumptions need to be established. 	
		0691	BC IE parameter negotiation	24.008
	NEC, NTT DoCoMo	Noted.
It was proposed that the possibility to use the existing messages MODIFY, MODIFY COMPLETE and MODIFY REJECT with no additional messages should be studied.	
		0692	CR for BC IE parameter negotiation	24.008	NEC, NTT DoCoMo	Withdrawn.
Service modification without pre-notification.	
		0704	Proposed acceleration of Emergency Call work based on Category	24.008	NEC/Masahiko Yahagi	Rejected.
•	Clarification on S1 working assumption on the category method was requested.
•	It was clarified that the latest version of 22.101 already contains the requirements.
•	Encoding / decoding requirements for service category IE in case of multiple services are requested -> 8 bit long bitmap was preferred.
•	What is octet 4 needed for if multiple indications can be given in octet 3?
•	Max len of the service category IE is needed
•	Default service to be indicated by no bits set in the bitmap
•	Is 4 octets the right length considering SIM datafield length.	
		0705	Bearer modification without pre-notification	24.008/ 23.108	NEC/Masahiko Yahagi	Noted.
The proposal to discuss the concept was supported but there were several comments on the technical proposals.	
		0706	Bearer modification without pre-notification(TS24.008)	24.008	NEC/Masahiko Yahagi	Noted.
Provided for information	
		0707	Bearer modification without pre-notification(TS23.108)	23.108	NEC/Masahiko Yahagi	Noted.
Provided for information	
		0708	BC IE parameter negotiation during the call		NEC,NTT DoCoMo/Masahiko Yahagi, Dasisuke Igarashi	Withdrawn.	
		0767	VGCS service accessibility	03.68	Nortel Networks/ Sonia	Agreed.
ASCI CR which is agreed subject to approval of the R00 WI in TSGN #8.	
		0768	VBS service accessibility	03.69	Nortel Networks Sonia	Agreed.
ASCI CR which is agreed subject to approval of the R00 WI in TSGN #8.	
		0769	talker outside Group Call Area	03.68	Nortel Networks Sonia	Agreed.
ASCI CR which is agreed subject to approval of the R00 WI in TSGN #8.	
		0770	Originator outside Group Call Area	03.69	Nortel Networks Sonia	Agreed.
ASCI CR which is agreed subject to approval of the R00 WI in TSGN #8.	
		0771	Notification response & uplink reply procedure definition	03.68	Nortel Networks Sonia	Agreed.
ASCI CR which is agreed subject to approval of the R00 WI in TSGN #8.	
		0772	Notification response & uplink reply procedure definition	03.69	Nortel Networks Sonia	Agreed.
ASCI CR which is agreed subject to approval of the R00 WI in TSGN #8.	
		0773	Release dataFlow correction	03.68	Nortel Networks Sonia	Agreed.
ASCI CR which is agreed subject to approval of the R00 WI in TSGN #8.	
		0774	Release dataFlow correction	03.69	Nortel Networks Sonia	Agreed.
ASCI CR which is agreed subject to approval of the R00 WI in TSGN #8.	
		0788	CR to 24.008 on Codec Negotiation 	24.008	Ericsson/ Phil Hodges	Noted.
Presented for information. Comments are invited in order to present a new version of the CR based on R00 specification in the next meeting.	

							
							
8	Output Liaison Statements						
		0639	Proposed response to LS to N1 on including the SAI into the Gs-i/f BSSAP+-LOCATION-UPDATE-REQUEST message as requested in N1-000543	29.018	NTT Comware/ Nobuyuki Uda	Agreed.

Linked with N1-000595	
		0695			Koshimizu san	Withdrawn
Reply to N1-000576.	
		0696	Reply to LS on Correction for mobile stations staying in GMM READY virtually for ever		Monica	Revised to N1-000804
Discuss CR in Tdoc N1-000763-766
Reply to N1-000577	
		0698	Liaison Statement on the introduction of 3G MS capabilities in MS classmark 3		Duncan	Is this tdoc Revised to N1-000784 ???
Reply to N1-000578	
		0699			Igarashi san	
Reply to N1-000582	
		0700	Response to LS (R2-000667 / N1-000586) on MS initiated signaling connection release		Hannu	Rejected
See CR in N1-000737 first
Reply to N1-000586	
		0701	Proposed LS on clarifications to DRX parameter for GMM		Per	Agreed.
Related CR in tdoc N1-000755
Reply to N1-000587 and N1-000594	
		0702	LS on Transport of Codec Information during the Codec Negotiation between MS and MSC		Phil	Revised to N1-000795
Reply to N1-000588	
		0703	Response to LS (R2-000945), LS TSG S1 (00) 103 on UE/MS idle mode operation and LS TSG S1 (00) 368 on PLMN selection		Olivier	Agreed.
Reply to N1-000589, N1-000597, N1-000624
Related CR in N1-000719.	
		0709	LS on UE triggered authentication and key agreement during connections		Duncan	Revised to N1-000797
Reply to N1-000599	
		0710	Liaison statement on usage of terms GSM, UMTS and GERAN		Hannu	Agreed with editorial modification.
Reply to N1-000601	
		0712	Terminal capability negotiation including codecs (reply)		Edgar	Agreed.
Reply to N1-000613	
		0713			Olivier	Agreed.
Reply to N1-000621	
		0714	LS on global solution of "Cause of no CLI"		Ohtsuki san	Revised to N1-000751
Reply to N1-000623	
		0715	Response to LS on hexadecimal IMEI format		Hannu	Agreed.
Related CR in N1-000779
Reply to N1-000625	
		0743	Duplicated SIM and USIM data fields		Ericsson/
Olivier Irac	Withdrawn.	
		0751	LS on global solution of "Cause of no CLI"		Ohtsuki san / Hannu	Agreed.
Reply to N1-000623
Revision of N1-000714	
		0758	LS on removal of service accept		Sudeep	Agreed.
LS to S2 on N1 and S2 disagreeing about N1-000646.	
		0778	Reply on GPRS ciphering		Monica	Revised to N1-000799
Reply to N1-000690	
		0784	LS on the introduction of 3G MS capabilities in MS CM		Duncan	Revised to N1-000805
CR N1-000697 is attached	
		0787	Codec Lists from Ue for different Access technologies	24.008	Phil Hdoges	Agreed.	
		0793	Reply to LS on Correction for mobile stations staying in GMM READY virtually for ever		Monica	Agreed.
Reply to N1-000577
Revision of N1-000696	
		0795	LS on Transport of Codec Information during the Codec Negotiation between MS and MSC		Phil	Agreed.
Reply to N1-000588
Revision of N1-000702	
		0797	LS on UE triggered authentication and key agreement during connections		Duncan	Agreed.
Revision of N1-000709
Reply to N1-000599	
		0799	Reply to GPRS ciphering		Monica	Revised to N1-000806
Reply to N1-000690
Revision of N1-000778	
		0804	Reply to LS on Correction for mobile stations staying in GMM READY virtually for ever		Monica	Agreed.
CRs in Tdoc N1-000763, 791 and 792 need to be attached.
Reply to N1-000577
Revision of N1-000696	
		0805	LS on the introduction of 3G MS capabilities in MS CM		Duncan	Agreed.
CR N1-000697 is attached.
Revision of N1-000784	
		0806	Reply to GPRS ciphering		Monica	Agreed.
Reply to N1-000690
Revision of N1-000799	
							
9	A.O.B.						
			Do we need an additional meeting for SIP issues in July / August or do we go the S2 reqular meeting?			AP for Hannu to organise together with TJ a SIP meeting with N1 – S2. Proposal 2 days on week 29 or 30 / 2000.