**3GPP TSG-CT WG1 Meeting #125-eC1-20wxyz**

**Electronic meeting, 20-28 August 2020**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.0* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **29.379** | **CR** | **CR#** | **rev** | **-** | **Current version:** | **16.0.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network |  | Core Network | **X** |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Correct XML schema | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | FirstNet | | | | | | | | | |
| ***Source to TSG:*** | C1 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | MCCI-CT | | | | |  | ***Date:*** | | | 20 August 2020 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **F** |  | | | | | ***Release:*** | | | Rel-16 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) Rel-12 (Release 12)* *Rel-13 (Release 13) Rel-14 (Release 14) Rel-15 (Release 15) Rel-16 (Release 16)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | The XML schema in subclause A.2.1 has incorrect references to the mcpttinfo namespace. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | Removed the external references to mcpttinfo, as the type declarations are self-contained. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | Incorrect XML schema that is unusable. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | A.2.1 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

##### **\* \* \* \* \* FIRST CHANGE \* \* \* \* \***

## A.2.1 XML schema

The XML schema elements for private call parameters in the present clause extend the mcpttinfo schema in 3GPP TS 24.379 [29].

<?xml version="1.0" encoding="UTF-8"?>

<xs:schema

xmlns:xs="http://www.w3.org/2001/XMLSchema"

elementFormDefault="qualified"

attributeFormDefault="unqualified"

xmlns:xenc="http://www.w3.org/2001/04/xmlenc#"

xmlns:mgktp="urn:3gpp:ns:mcpttGKTP:1.0">

<xs:element name="private-call-params" type="private-call-params-type"/>

<xs:complexType name="private-call-params-type">

<xs:sequence>

<xs:choice minOccurs="0">

<xs:element name="floor-control" type="emptyType"/>

<xs:element name="without-floor-control" type="emptyType"/>

</xs:choice>

<xs:choice minOccurs="0">

<xs:element name="implicit-floor" type="emptyType"/>

<xs:element name="without-implicit-floor" type="emptyType"/>

</xs:choice>

<xs:choice minOccurs="0">

<xs:element name="manual-commencement" type="emptyType"/>

<xs:element name="automatic-commencement" type="emptyType"/>

</xs:choice>

</xs:sequence>

<xs:anyAttribute namespace="##any" processContents="lax"/>

</xs:complexType>

<!-- empty complex type -->

<xs:complexType name="emptyType"/>

</xs:schema>

Editor's Note: Need to register and add a namespace to the schema that's specific to interworking.

##### **\* \* \* \* \* END CHANGES \* \* \* \* \***