**3GPP TSG-CT WG1 Meeting #137-eC1-224585**

**E-Meeting, 18th – 26th August 2022**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.2* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **24.483** | **CR** | **0157** | **rev** | **1** | **Current version:** | **17.7.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **x** | Radio Access Network |  | Core Network | **x** |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Correcting MCData user profile MO below IPInformation | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | , Nokia, Nokia Shanghai Bell | | | | | | | | | |
| ***Source to TSG:*** | C1 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | MCProtoc18 | | | | |  | ***Date:*** | | | 2022-08-03 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **D** |  | | | | | ***Release:*** | | | Rel-18 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18) Rel-19 (Release 19)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | In the headings of the management objects of /<x>/<x>/Common/OnetoOne/UserList/<x>/Entry/  IPInformation/<x>/Entry the "/" in front of the last "Entry" is missing. This CR adds the missing "/" to all the affeced headings. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | Adding the missing "/" to the headings of clauses 10.2.16L, 10.2.16M, 10.2.16N, 10.2.16O | | | | | | | | |
| ***To*** | |  | | | | | | | | |
| ***Consequences if not approved:*** | | Errors in the heading of the MO of these entries remain wrong. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 10.2.16L, 10.2.16M, 10.2.16N, 10.2.16O | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **x** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **x** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **x** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

\* \* \* First Change \* \* \* \*

### 10.2.16L /<x>/<x>/Common/OnetoOne/UserList/<x>/Entry/ IPInformation/<x>/Entry

Table 10.2.16L.1: /<x>/<x>/Common/OnetoOne/UserList/<x>/Entry/IPInformation/<x>/Entry

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/OnetoOne/UserList/<x>/Entry/IPInformation/<x>/Entry | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for one or more list of IPInformation data that can be used in the setup of an IP Connectivity session for a specific MCData user in a one-to-one communication. | | | | |

### 10.2.16M /<x>/<x>/Common/OnetoOne/UserList/<x>/Entry/ IPInformation/<x>/Entry/IPv4Information

Table 10.2.16M.1: /<x>/<x>/Common/OnetoOne/UserList/<x>/Entry/IPInformation/<x>/Entry/  
IPv4Information

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/OnetoOne/UserList/<x>/Entry/IPInformation/<x>/Entry/IPv4Information | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | chr | Get, Replace |  |
|  | This leaf node indicates an IPv4 host address or an IPv4 network that can be addressed on an IP Connectivity session in a one-to-one communication for a specific MCData ID. | | | | |

### 10.2.16N /<x>/<x>/Common/OnetoOne/UserList/<x>/Entry/ IPInformation/<x>/Entry/IPv6Information

Table 10.2.16N.1: /<x>/<x>/Common/OnetoOne/UserList/<x>/Entry/IPInformation/<x>/Entry/  
IPv6Information

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/OnetoOne/UserList/<x>/Entry/IPInformation/<x>/Entry/IPv6Information | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | chr | Get, Replace |  |
|  | This leaf node indicates an IPv6 host address or an IPv6 network that can be addressed on an IP Connectivity session in a one-to-one communication for a specific MCData ID. | | | | |

### 10.2.16O /<x>/<x>/Common/OnetoOne/UserList/<x>/Entry/ IPInformation/<x>/Entry/FQDN

Table 10.2.16O.1: /<x>/<x>/Common/OnetoOne/UserList/<x>/Entry/IPInformation/<x>/Entry/FQDN

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/OnetoOne/UserList/<x>/Entry/IPInformation/<x>/Entry/FQDN | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | chr | Get, Replace |  |
|  | This leaf node indicates a fully qualified domain name for a specific host or domain that can be addressed on an IP Connectivity session in a one-to-one communication for a specific MCData ID. | | | | |

\* \* \* End of Changes \* \* \* \*