{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["TDoc_List","CR_Packs_List","Parameters"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":5,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"TDoc_List","index":0,"n_rows":451,"n_cols":31,"rows_kept":451,"cut":false,"hidden":false,"merged":[]}
["TDoc #","Title","Source","Contact","Contact ID","Type","Type supplement","For","Abstract","Agenda item sort order","Agenda item #","Agenda item description","TDoc sort order within agenda item","TDoc Status","Reservation date","Uploaded","Is revision of","Revised to","Release","Spec #","Version","Related WIs","CR #","CR revision #","CR category","TSG CR Pack","Reply to","To","Cc","Original LS","Reply in"]
["C3-150001","Draft Agenda for the CT3#80 Meeting","CT3 Chairman","Mathieu Mangion",27904,"agenda","","","","2","2.1","Approval of the agenda.",10,"Approved","2015-01-23T11:27:59.607","2015-01-23T11:24:57.893","","","","","","","","","","","","","","",""]
["C3-150002","Proposed Schedule for CT3#80","CT3 Chairman","Mathieu Mangion",27904,"other","","","","3","2.2","Proposed schedule",20,"Revised","2015-01-23T11:27:59.617","2015-02-10T16:22:03.343","","C3-150434","","","","","","","","","","","","",""]
["C3-150003","Allocation of documents to agenda items (at Deadline)","CT3 Chairman","Mathieu Mangion",27904,"other","","","","4","3","Registration of documents",30,"Noted","2015-01-23T11:27:59.623","2015-02-10T16:22:03.343","","","","","","","","","","","","","","",""]
["C3-150004","Allocation of documents to agenda items (Start of Day 1)","CT3 Chairman","Mathieu Mangion",27904,"other","","","","4","3","Registration of documents",40,"Noted","2015-01-23T11:27:59.633","2015-02-10T16:22:03.350","","","","","","","","","","","","","","",""]
["C3-150005","Allocation of documents to agenda items (Start of Day 2)","CT3 Chairman","Mathieu Mangion",27904,"other","","","","4","3","Registration of documents",50,"Noted","2015-01-23T11:27:59.640","2015-02-10T16:22:03.350","","","","","","","","","","","","","","",""]
["C3-150006","Allocation of documents to agenda items (Start of Day 3)","CT3 Chairman","Mathieu Mangion",27904,"other","","","","4","3","Registration of documents",60,"Noted","2015-01-23T11:27:59.647","2015-02-10T16:22:03.353","","","","","","","","","","","","","","",""]
["C3-150007","Allocation of documents to agenda items (Start of Day 4)","CT3 Chairman","Mathieu Mangion",27904,"other","","","","4","3","Registration of documents",70,"Noted","2015-01-23T11:27:59.657","2015-02-10T16:22:03.363","","","","","","","","","","","","","","",""]
["C3-150008","Allocation of documents to agenda items (Start of Day 5)","CT3 Chairman","Mathieu Mangion",27904,"other","","","","4","3","Registration of documents",80,"Noted","2015-01-23T11:27:59.663","2015-02-10T16:22:03.367","","","","","","","","","","","","","","",""]
["C3-150009","Allocation of documents to agenda items (End of Day 5)","CT3 Chairman","Mathieu Mangion",27904,"other","","","","4","3","Registration of documents",90,"Noted","2015-01-23T11:27:59.673",null,"","","","","","","","","","","","","","",""]
["C3-150010","Summary of CT#66 related to CT3","CT3 Chairman","Mathieu Mangion",27904,"report","","","","7","4.2","Report from previous CT plenary",100,"Noted","2015-01-23T11:27:59.680","2015-02-10T16:22:03.373","","","","","","","","","","","","","","",""]
["C3-150011","Status of CT3 Work Items","CT3 Chairman","Mathieu Mangion",27904,"other","","","","201","15.1","Work Plan Review",110,"Revised","2015-01-23T11:27:59.690","2015-02-10T16:22:03.377","","C3-150442","","","","","","","","","","","","",""]
["C3-150012","LS on TFT for default bearer","SA2","Mathieu Mangion",27904,"LS in","","","This LS is sent by SA2 to CT1 and CT3 asking them to evaluate and decide on the alternative option of applying the same conditions to the TFT of the default bearer similar to a valid TFT state of the PDP Context established with the Secondary PDP Context","13","6","Received Liaison Statements",120,"Noted","2015-01-23T11:27:59.697","2015-01-23T11:24:57.930","C3-143183","","Rel-11","","","","","","","",null,null,null,"S2-141510"]
["C3-150013","LS on Introducing the feature of excluding Usage of a Service/Application from IP-CAN session/TDF session Usage into the specification","SA2","Mathieu Mangion",27904,"LS in","","","SA2 agreed to the attached CR 0921 to 23.203 as part of eUMONC. SA2 would like CT3 to progress the stage 3 work with following understanding:- \nThe indication of exclusion from session level monitoring associated with PCC/ADC rule(s) corresponds to an ind","13","6","Received Liaison Statements",130,"Noted","2015-01-23T11:27:59.713","2015-01-23T11:24:57.940","C3-145170","","Rel-13","","","eUMONC","","","","",null,null,null,"S2-143809"]
["C3-150014","LS on a study on Diameter load control mechanisms","CT4","Mathieu Mangion",27904,"LS in","","","CT4 has approved a new study on Diameter load control mechanisms for which CT4 informs CT3 and SA5. The Study Item document is attached to the LS.","13","6","Received Liaison Statements",140,"Noted","2015-01-23T11:27:59.730","2015-01-23T11:24:58.700","","","Rel-13","","","","","","","",null,null,null,"C4-142346"]
["C3-150015","Reply LS on Maintenance of I-WLAN Solution","CT4","Mathieu Mangion",27904,"LS in","","","This LS is from CT4, where they indicate that from CT4 perspective the task to capture stopping the maintenance of I-WLAN Interworking feature in Rel-12 in CT4 specifications is now completed. CT4 lists the set of related approved CRs.","13","6","Received Liaison Statements",150,"Noted","2015-01-23T11:27:59.740","2015-01-23T11:24:58.703","","","Rel-12","","","TEI12","","","","",null,null,null,"C4-142474"]
["C3-150016","Reply LS on discontinuance of I-WLAN related TS 29.161","CT","Mathieu Mangion",27904,"LS in","","","CT Plenary has discussed this issue and decided to discontinue the I-WLAN related TS 29.161 from Rel-12 onwards, therefore CT kindly asks CT3 to take theis into consideration and update related specifications accordingly. Consequently, any references to T","13","6","Received Liaison Statements",160,"Noted","2015-01-23T11:27:59.750","2015-01-23T11:24:59.440","","","Rel-12","","","","","","","",null,null,null,"CP-141001"]
["C3-150017","LS on Introducing the feature of excluding Usage of a Service/Application from IP-CAN session/TDF session Usage into the specification.","SA2","Mathieu Mangion",27904,"LS in","","","Withdraw, repetition of C3-150013","13","6","Received Liaison Statements",170,"Withdrawn","2015-01-23T11:27:59.760","2015-01-23T11:24:59.443","","","Rel-13","","","eUMONC","","","","",null,null,null,"S2-143809"]
["C3-150018","LS response on introducing new QCI Values","SA2","Mathieu Mangion",27904,"LS in","","","SA2 would like to clarify the intentions on the introduction of the new QCI values, where the new QCIs are intended to be used for Mission Critical or Non-Mission Critical Push To Talk service apart from QCI 70 which is intended to be used for other Missi","13","6","Received Liaison Statements",180,"Noted","2015-01-23T11:27:59.770","2015-01-23T11:25:00.183","","","Rel-12","","","GCSE_LTE","","","","",null,null,null,"S2-144636"]
["C3-150019","LS to SA on 3GPP work organization for Mission Critical Push to Talk","SA","Mathieu Mangion",27904,"LS in","","","3GPP SA5 would like to inform 3GPP SA and OMA about the potential impact on charging framework of 3GPP SA5 while creating the standard for mission critical communication application in the new 3GPP SA6 group and the supporting 3GPP network architecture in","13","6","Received Liaison Statements",190,"Noted","2015-01-23T11:27:59.783","2015-01-23T11:25:00.920","","","Rel-13","","","MCPTT","","","","",null,null,null,"SP-140655/S5-145393"]
["C3-150020","Candidate Release Available","SA","Mathieu Mangion",27904,"LS in","","","The Technical Plenary of oneM2M informing 3GPP that oneM2M, the Global Partnership developing standards for Machine-to-Machine (M2M) communications and the Internet-of-Things (IoT) announced that its initial Candidate Release of Technical Specifications i","13","6","Received Liaison Statements",200,"Noted","2015-01-23T11:27:59.793","2015-01-23T11:25:01.747","","","","","","","","","","",null,null,null,"SP-140657_TP-2014-0511"]
["C3-150021","LS on Establishment of new working group TSG SA WG6","SA","Mathieu Mangion",27904,"LS in","","","This LS is from 3GPP TSG SA#66 informing us that it has formally established a new working group to progress the work on applications for Mission Critical Communications within 3GPP. The approved ToR for 3GPP TSG SA WG6 is enclosed (SP-140645). The LS als","13","6","Received Liaison Statements",210,"Noted","2015-01-23T11:27:59.807","2015-01-23T11:25:01.750","","","","","","MCPTT","","","","",null,null,null,"SP-140884"]
["C3-150022","CT3-79 Draft Meeting report","MCC","Mathieu Mangion",27904,"report","","","The DRAFT Meeting Report for TSG CT WG3 meeting-79, took place in San Francisco, US, 17/11/2014 to 21/11/2014, is presented here for WG approval","6","4.1","Report from previous CT3 meeting",220,"Approved","2015-01-23T11:27:59.817","2015-01-23T11:25:02.497","","","","","","","","","","","","","","",""]
["C3-150023","Draft references in CT3 specifications","Ericsson","Mathieu Mangion",27904,"other","","","This document shows IETF draft references in CT3 technical specifications.","12","5.3","Other items for immediate consideration",230,"Noted","2015-01-23T11:27:59.827","2015-01-23T15:26:37.760","","","","","","","","","","","","","","",""]
["C3-150024","Bugfix: do not send negative-delivery IMDN after sending SIP 4xx/5xx response","Comverse Network Systems","Mathieu Mangion",27904,"CR","","","Bugfix: do not send negative-delivery IMDN after sending SIP 4xx/5xx response","46","8.21","Support of Service-Level Interworking for Messaging Services [MESSIW]",240,"Revised","2015-01-23T11:27:59.837","2015-01-23T11:25:02.503","","C3-150261","Rel-8","29.311","8.3.0","MESSIW","0034","","F","-","","","","",""]
["C3-150025","Bugfix: do not send negative-delivery IMDN after sending SIP 4xx/5xx response","Comverse","Mathieu Mangion",27904,"CR","","","Bugfix: do not send negative-delivery IMDN after sending SIP 4xx/5xx response","46","8.21","Support of Service-Level Interworking for Messaging Services [MESSIW]",250,"Revised","2015-01-23T11:27:59.917","2015-01-23T11:25:03.337","","C3-150262","Rel-9","29.311","9.2.0","MESSIW","0035","","A","-","","","","",""]
["C3-150026","Bugfix: do not send negative-delivery IMDN after sending SIP 4xx/5xx response","Comverse","Mathieu Mangion",27904,"CR","","","Bugfix: do not send negative-delivery IMDN after sending SIP 4xx/5xx response","46","8.21","Support of Service-Level Interworking for Messaging Services [MESSIW]",260,"Revised","2015-01-23T11:27:59.990","2015-01-23T11:25:04.180","","C3-150263","Rel-10","29.311","10.5.0","MESSIW","0036","","A","-","","","","",""]
["C3-150027","Bugfix: do not send negative-delivery IMDN after sending SIP 4xx/5xx response","Comverse","Mathieu Mangion",27904,"CR","","","Bugfix: do not send negative-delivery IMDN after sending SIP 4xx/5xx response","46","8.21","Support of Service-Level Interworking for Messaging Services [MESSIW]",270,"Revised","2015-01-23T11:28:00.067","2015-01-23T11:25:05.057","","C3-150264","Rel-11","29.311","11.1.0","MESSIW","0037","","A","-","","","","",""]
["C3-150028","Bugfix: do not send negative-delivery IMDN after sending SIP 4xx/5xx response","Comverse","Mathieu Mangion",27904,"CR","","","Bugfix: do not send negative-delivery IMDN after sending SIP 4xx/5xx response","46","8.21","Support of Service-Level Interworking for Messaging Services [MESSIW]",280,"Revised","2015-01-23T11:28:00.140","2015-01-23T11:25:05.907","","C3-150265","Rel-12","29.311","12.0.0","MESSIW","0038","","A","-","","","","",""]
["C3-150029","Bugfix: do not send negative-delivery IMDN after sending SIP 4xx/5xx response","Comverse Network Systems","Mathieu Mangion",27904,"CR","","","","46","8.21","Support of Service-Level Interworking for Messaging Services [MESSIW]",290,"Withdrawn","2015-01-23T11:28:00.213",null,"","","Rel-9","29.311","9.2.0","","0039","","A","-","","","","",""]
["C3-150030","Clarification on the II-NNI requirement for CDIV regarding Privacy header field.","NTT","Mathieu Mangion",27904,"CR","","","This CR is trying to clarify the II-NNI requirement regarding Privacy header field when CDIV service is provided over the II-NNI.","65","9.19","Operational Description of the Inter-IMS NNI   [II-NNI]",300,"Revised","2015-01-23T11:28:00.287","2015-01-23T11:25:06.157","","C3-150281","Rel-9","29.165","9.19.0","II-NNI","0709","","F","-","","","","",""]
["C3-150031","Clarification on the II-NNI requirement for CDIV regarding Privacy header field.","NTT","Mathieu Mangion",27904,"CR","","","This CR is trying to clarify the II-NNI requirement regarding Privacy header field when CDIV service is provided over the II-NNI.","65","9.19","Operational Description of the Inter-IMS NNI   [II-NNI]",310,"Revised","2015-01-23T11:28:00.363","2015-01-23T11:25:07.040","","C3-150282","Rel-10","29.165","10.17.0","II-NNI","0710","","A","-","","","","",""]
["C3-150032","Clarification on the II-NNI requirement for CDIV regarding Privacy header field.","NTT","Mathieu Mangion",27904,"CR","","","This CR is trying to clarify the II-NNI requirement regarding Privacy header field when CDIV service is provided over the II-NNI.","65","9.19","Operational Description of the Inter-IMS NNI   [II-NNI]",320,"Revised","2015-01-23T11:28:00.440","2015-01-23T11:25:07.900","","C3-150283","Rel-11","29.165","11.12.0","II-NNI","0711","","A","-","","","","",""]
["C3-150033","Clarification on the II-NNI requirement for CDIV regarding Privacy header field.","NTT","Mathieu Mangion",27904,"CR","","","This CR is trying to clarify the II-NNI requirement regarding Privacy heade\nr field when CDIV service is provided over the II-NNI.","65","9.19","Operational Description of the Inter-IMS NNI   [II-NNI]",330,"Revised","2015-01-23T11:28:00.523","2015-01-23T11:25:08.787","","C3-150284","Rel-12","29.165","12.6.0","II-NNI","0712","","A","-","","","","",""]
["C3-150034","Addition of \"mp\" header field parameter into CDIV section.","NTT","Mathieu Mangion",27904,"CR","","","Add the \"mp\" parameter into the CDIV section of TS 29.165.","175","12.41","Impacts of RFC7044 for introduction of the new History-Info header field [HISTORY_CT]",340,"Revised","2015-01-23T11:28:00.597","2015-01-23T11:25:09.653","","C3-150332","Rel-12","29.165","12.6.0","HISTORY_CT","0713","","F","-","","","","",""]
["C3-150035","Clarification on the II-NNI requirement regarding cause-param URI parameter.","NTT","Mathieu Mangion",27904,"CR","","","This CR is trying to clarify the II-NNI requirement regarding cause-param U.","65","9.19","Operational Description of the Inter-IMS NNI   [II-NNI]",350,"Revised","2015-01-23T11:28:00.677","2015-01-23T11:25:10.513","","C3-150285","Rel-9","29.165","9.19.0","II-NNI","0714","","F","-","","","","",""]
["C3-150036","Clarification on the II-NNI requirement regarding cause-param URI parameter.","NTT","Mathieu Mangion",27904,"CR","","","This CR is trying to clarify the II-NNI requirement regarding cause-param U\nRI parameter when CDIV service is provided over the II-NNI.","65","9.19","Operational Description of the Inter-IMS NNI   [II-NNI]",360,"Revised","2015-01-23T11:28:00.757","2015-01-23T11:25:11.380","","C3-150286","Rel-10","29.165","10.17.0","II-NNI","0715","","A","-","","","","",""]
["C3-150037","Clarification on the II-NNI requirement regarding cause-param URI parameter.","NTT","Mathieu Mangion",27904,"CR","","","This CR is trying to clarify the II-NNI requirement regarding cause-param U\nRI parameter when CDIV service is provided over the II-NNI.","65","9.19","Operational Description of the Inter-IMS NNI   [II-NNI]",370,"Revised","2015-01-23T11:28:00.830","2015-01-23T11:25:12.230","","C3-150287","Rel-11","29.165","11.12.0","II-NNI","0716","","A","-","","","","",""]
["C3-150038","Clarification on the II-NNI requirement regarding cause-param URI parameter.","NTT","Mathieu Mangion",27904,"CR","","","This CR is trying to clarify the II-NNI requirement regarding cause-param U\nRI parameter when CDIV service is provided over the II-NNI.","65","9.19","Operational Description of the Inter-IMS NNI   [II-NNI]",380,"Revised","2015-01-23T11:28:00.910","2015-01-23T11:25:13.090","","C3-150288","Rel-12","29.165","12.6.0","II-NNI","0717","","A","-","","","","",""]
["C3-150039","Addition of an optional capability regarding a new cause-param value for service number translation.","NTT","Mathieu Mangion",27904,"CR","","","This CR is trying to add an optional capability regarding a new cause-param value for service number translation into 29.165.","192","13.8","Interworking of Called IN number and original Called IN number ISUP parameters",390,"Revised","2015-01-23T11:28:00.987","2015-01-23T11:25:13.977","","C3-150366","Rel-13","29.165","12.6.0","660021","0718","","B","-","","","","",""]
["C3-150040","Correction of a minor error in subclause C.3.1.","NTT","Mathieu Mangion",27904,"CR","","","Editorial correction in subclause C.3.1 of TS 29.165.","194","13.9.1","TEI13 for IMS/CS",400,"Agreed","2015-01-23T11:28:01.067","2015-01-23T11:25:14.857","","","Rel-13","29.165","12.6.0","TEI13","0719","","D","CP-150130","","","","",""]
["C3-150041","ICS call: reference correction","MCC","Mathieu Mangion",27904,"CR","","","Omitted Rel-12 CR, it is equivalent to C3-144042. The identity of the reference to subclause \"Support of ICS call\" corrected.The opportunity has also been taken to correct some editorial errors related to support of the \"ICS call\".","193","13.9","Technical Enhancements and Improvements [TEI13]",410,"Agreed","2015-01-23T11:28:01.143","2015-01-23T11:25:15.713","","","Rel-13","29.163","13.0.0","TEI13","0842","","F","CP-150130","","","","",""]
["C3-150042","Announcement suppression for IMS hold request","MCC","Mathieu Mangion",27904,"CR","","","Omitted Rel-12 CR, it is equivalent to C3-144268. Added that for the call identified as the \"ICS call\" the MGCF should not request the IM-MGW to apply an announcement to the held party. The opportunity has also been taken to correct some editorial errors.","193","13.9","Technical Enhancements and Improvements [TEI13]",420,"Agreed","2015-01-23T11:28:01.223","2015-01-23T11:25:16.577","","","Rel-13","29.163","13.0.0","TEI13","0843","","F","CP-150130","","","","",""]
["C3-150043","Adding support for EVS codec","MCC","Mathieu Mangion",27904,"CR","","","Omitted Rel-12 CR, it is equivalent to C3-145221. MGCF and IM-MGW procedures to handle EVS codec parameters are being specified.","193","13.9","Technical Enhancements and Improvements [TEI13]",430,"Withdrawn","2015-01-23T11:28:01.300","2015-01-23T11:25:17.447","","","Rel-13","29.163","13.0.0","EVS_codec","0844","","B","-","","","","",""]
["C3-150044","Note 4 in Table 3 for mapping to CLI parameter","MCC","Mathieu Mangion",27904,"CR","","","Omitted Rel-12 CR, it is equivalent to C3-145223. Delete Note 4 in column for the mapping of Calling Party Number parameter Address signals","193","13.9","Technical Enhancements and Improvements [TEI13]",440,"Agreed","2015-01-23T11:28:01.377","2015-01-23T11:25:18.347","","","Rel-13","29.163","13.0.0","TEI13","0845","","F","CP-150130","","","","",""]
["C3-150045","Appearance of Redirection Number Restriction parameter","MCC","Mathieu Mangion",27904,"CR","","","Omitted Rel-12 CR, it is equivalent to C3-145298. Change description to clarify that only Redirection Number Restriction parameter may appear.","193","13.9","Technical Enhancements and Improvements [TEI13]",450,"Agreed","2015-01-23T11:28:01.450","2015-01-23T11:25:19.217","","","Rel-13","29.163","13.0.0","TEI13","0846","","F","CP-150130","","","","",""]
["C3-150046","Inclusion of RFC7044","MCC","Mathieu Mangion",27904,"CR","","","Omitted Rel-12 CR, it is equivalent to C3-145296. Replace all references through the document","193","13.9","Technical Enhancements and Improvements [TEI13]",460,"Agreed","2015-01-23T11:28:01.523","2015-01-23T11:25:20.127","","","Rel-13","29.163","13.0.0","HISTORY_CT","0847","","C","CP-150130","","","","",""]
["C3-150047","NAS/RAN cause handling","MCC","Mathieu Mangion",27904,"CR","","","Omitted Rel-12 CR, it is equivalent to C3-144305. IP-CAN session termination, bearer termination and PCC rule error handling procedures are modified to specify the handling of the RAN-NAS-Release-Cause AVP and access network information.\nMultiple instance","193","13.9","Technical Enhancements and Improvements [TEI13]",470,"Agreed","2015-01-23T11:28:01.597","2015-01-23T11:25:21.163","","","Rel-13","29.212","13.0.0","NWK-PL2IMS-CT, TEI13","1264","","B","CP-150131","","","","",""]
["C3-150048","Presence Reporting Area Indication on TDF Session","MCC","Mathieu Mangion",27904,"CR","","","Omitted Rel-12 CR, it is equivalent to C3-144311. In current 3GPP TS 23.203 sub-clause 6.4a: Upon the initial interaction with the TDF, the PCRF may provide the Presence Reporting Area Identifier to be used for reporting changes of UE presence in a Presen","193","13.9","Technical Enhancements and Improvements [TEI13]",480,"Merged","2015-01-23T11:28:01.687","2015-01-23T11:25:22.770","","","Rel-13","29.212","13.0.0","CNO_ULI-CT","1265","","F","-","","","","",""]
["C3-150049","Mute-Notification Status on Gx and Sd Session","MCC","Mathieu Mangion",27904,"CR","","","Omitted Rel-12 CR, it is equivalent to C3-144284. To specify more clearly that Mute-Notification AVP status shall not be changed during the lifetime of the PCC/ADC rules.","193","13.9","Technical Enhancements and Improvements [TEI13]",490,"Agreed","2015-01-23T11:28:01.763","2015-01-23T11:25:23.657","","","Rel-13","29.212","13.0.0","SAPP-CT3","1266","","A","CP-150135","","","","",""]
["C3-150050","Correction to the PC to CS handover indication","MCC","Mathieu Mangion",27904,"CR","","","Omitted Rel-12 CR, it is equivalent to C3-144230. The PCEF is mandated to report the PS_TO_CS_HANDOVER if the IP-CAN bearer termination is caused by the PS to CS handover for GPRS","193","13.9","Technical Enhancements and Improvements [TEI13]",500,"Agreed","2015-01-23T11:28:01.837","2015-01-23T11:25:24.513","","","Rel-13","29.212","13.0.0","PCC-Enh","1267","","A","CP-150136","","","","",""]
["C3-150051","RESOURCE_ALLOCATION_FAILURE error response not to be sent upon PCRF-initiated PCC rule","MCC","Mathieu Mangion",27904,"CR","","","Omitted Rel-12 CR, it is equivalent to C3-144203. The RESOURCE_ALLOCATION_FAILURE (10) value of the Rule-Failure-Code AVP shall not be sent in a CCR after an IP-CAN bearer deactivation triggered by a successful PCRF-initiated PCC rule removal.","193","13.9","Technical Enhancements and Improvements [TEI13]",510,"Agreed","2015-01-23T11:28:01.913","2015-01-23T11:25:25.367","","","Rel-13","29.212","13.0.0","SAES-St3-PCC","1268","","A","CP-150132","","","","",""]
["C3-150052","Number of standard QCI values","MCC","Mathieu Mangion",27904,"CR","","","Omitted Rel-12 CR, it is equivalent to C3-144253. Removal of the word “nine”  in the first paragraph of 5.3.17","193","13.9","Technical Enhancements and Improvements [TEI13]",520,"Agreed","2015-01-23T11:28:01.990","2015-01-23T11:25:26.217","","","Rel-13","29.212","13.0.0","GCSE_LTE-CT","1269","","F","CP-150133","","","","",""]
["C3-150053","QCI code values “spare for future use”","MCC","Mathieu Mangion",27904,"CR","","","Omitted Rel-12 CR, it is equivalent to C3-145306. The terminology for reserved values other than 0 and 255 is changed to “Spare”","193","13.9","Technical Enhancements and Improvements [TEI13]",530,"Agreed","2015-01-23T11:28:02.067","2015-01-23T11:25:27.067","","","Rel-13","29.212","13.0.0","GCSE_LTE-CT","1270","","F","CP-150133","","","","",""]
["C3-150054","3GPP2 reference correction","MCC","Mathieu Mangion",27904,"CR","","","Omitted Rel-12 CR, it is equivalent to C3-145210. 3GPP2 X.S0057-0 v2.0 is changed to 3GPP2 X.S0057-B. The version information is removed from all the 3GPP2 references.","193","13.9","Technical Enhancements and Improvements [TEI13]",540,"Agreed","2015-01-23T11:28:02.143","2015-01-23T11:25:27.907","","","Rel-13","29.212","13.0.0","SAES-St3-PCC","1271","","A","CP-150132","","","","",""]
["C3-150055","Support for IPv6 prefix retrieve by the HSGW during the eHRPD pre-registration procedure","MCC","Mathieu Mangion",27904,"CR","","","Omitted Rel-12 CR, it is equivalent to C3-145213. Inclusion of the Framed-Ipv6-Prefix AVP in the CCA command over Gxx interface and add corresponding descriptions in the annex D.2.2.1.","193","13.9","Technical Enhancements and Improvements [TEI13]",550,"Agreed","2015-01-23T11:28:02.220","2015-01-23T11:25:28.750","","","Rel-13","29.212","13.0.0","SAES-St3-PCC, TEI13","1272","","A","CP-150132","","","","",""]
["C3-150056","TFT handling correction","MCC","Mathieu Mangion",27904,"CR","","","Omitted Rel-12 CR, it is equivalent to C3-145218. According to the new requirement of SA2, the PCEF/BBERF derives traffic mapping information based on implementation specific logic whenever this is required for a non-default bearer.","193","13.9","Technical Enhancements and Improvements [TEI13]",560,"Merged","2015-01-23T11:28:02.297","2015-01-23T11:25:30.347","","","Rel-13","29.212","13.0.0","SAES-St3-PCC, TEI13","1273","","A","-","","","","",""]
["C3-150057","Correction of the REVALIDATION_TIMEOUT event trigger","MCC","Mathieu Mangion",27904,"CR","","","Omitted Rel-12 CR, it is equivalent to C3-145310. Correct the time when the PCEF send the PCC rule request before the indicated revalidation should be limited in a preconfigured period, which is aligned with the preconfigured period before the revalidatio","193","13.9","Technical Enhancements and Improvements [TEI13]",570,"Agreed","2015-01-23T11:28:02.377","2015-01-23T11:25:32.007","","","Rel-13","29.212","13.0.0","SAES-St3-PCC","1274","","A","CP-150132","","","","",""]
["C3-150058","IPCAN Session modification after bearer procedure","MCC","Mathieu Mangion",27904,"CR","","","Omitted Rel-12 CR, it is equivalent to C3-144288. A new step 13 is added to cover the case when an IP-CAN session modification is triggered after IP-CAN bearer signaling in step 12 due to access network information retrieval and the PCEF needs to initiate","193","13.9","Technical Enhancements and Improvements [TEI13]",580,"Agreed","2015-01-23T11:28:02.450","2015-01-23T11:25:32.893","","","Rel-13","29.213","13.0.0","NWK-PL2IMS-CT","0579","","A","CP-150131","","","","",""]
["C3-150059","P-CSCF Restoration Procedure for Local Breakout","MCC","Mathieu Mangion",27904,"CR","","","Omitted Rel-12 CR, it is equivalent to C3-144298. Remove the description for the roaming case with local breakout when the P-CSCF is located in the HPLMN.Update the procedure to separately describe each command of the command pairs AAR/AAA and RAR/RAA.","193","13.9","Technical Enhancements and Improvements [TEI13]",590,"Agreed","2015-01-23T11:28:02.530","2015-01-23T11:25:33.760","","","Rel-13","29.213","13.0.0","PCSCF_RES","0580","","B","CP-150134","","","","",""]
["C3-150060","Priority Consideration for Diameter Overload Control","MCC","Mathieu Mangion",27904,"CR","","","Omitted Rel-12 CR, it is equivalent to C3-144304. This CR provides modifications to Diameter overload control procedures in support of priority services (e.g., MPS).","193","13.9","Technical Enhancements and Improvements [TEI13]",600,"Agreed","2015-01-23T11:28:02.607","2015-01-23T11:25:34.620","","","Rel-13","29.213","13.0.0","DOCME-PCC","0581","","F","CP-150136","","","","",""]
["C3-150061","Correction to the Gateway Control Session establishment procedure","MCC","Mathieu Mangion",27904,"CR","","","Omitted Rel-12 CR, it is equivalent to C3-144227. Correct the descritions of the behaviours for the non-roaming case and roaming case.","193","13.9","Technical Enhancements and Improvements [TEI13]",610,"Agreed","2015-01-23T11:28:02.683","2015-01-23T11:25:35.913","","","Rel-13","29.213","13.0.0","SAES-St3-PCC","0582","","A","CP-150132","","","","",""]
["C3-150062","PCRF discovery for the HNB CS Service","MCC","Mathieu Mangion",27904,"CR","","","Omitted Rel-12 CR, it is equivalent to C3-144286. When the DRA receives a request for a certain S15 Session establishment from the HNB GW, the DRA selects a suitable PCRF for the S15 Session based on HNB local IP address .When the S15 Session is terminate","193","13.9","Technical Enhancements and Improvements [TEI13]",620,"Agreed","2015-01-23T11:28:02.763","2015-01-23T11:25:36.810","","","Rel-13","29.213","13.0.0","BBAI_BBI-CT","0583","","A","CP-150136","","","","",""]
["C3-150063","Access network information reporting during the IP-CAN session termination","MCC","Mathieu Mangion",27904,"CR","","","Omitted Rel-12 CR, it is equivalent to C3-144292. If the BBERF in step 2 or PCEF in step 3 reports the access network information and if the AF requested the H-PCRF to report access network information previously or the RAN-NAS-Cause feature is supported,","193","13.9","Technical Enhancements and Improvements [TEI13]",630,"Merged","2015-01-23T11:28:02.843","2015-01-23T11:25:37.680","","","Rel-13","29.213","13.0.0","NWK-PL2IMS-CT","0584","","A","-","","","","",""]
["C3-150064","Reporting RAN/NAS cause during bearer creation/modification failure scenarious","MCC","Mathieu Mangion",27904,"CR","","","Omitted Rel-12 CR, it is equivalent to C3-144306. AF Session Termination IP-CAN session termination, Service Data Flow Deactivation and Notification of Signalling Flow status procedures are modified to specify the handling of the RAN-NAS-Release-Cause AVP","193","13.9","Technical Enhancements and Improvements [TEI13]",640,"Agreed","2015-01-23T11:28:02.923","2015-01-23T11:25:38.563","","","Rel-13","29.214","13.0.0","NWK-PL2IMS-CT, TEI13","0370","","B","CP-150131","","","","",""]
["C3-150065","Removal of Editor’s Note","MCC","Mathieu Mangion",27904,"CR","","","Omitted Rel-12 CR, it is equivalent to C3-144297. Add a new supported feature bit for P-CSCF restoration, and remove the Editor’s Note regarding if a supported-feature is needed for P-CSCF and PCRF to indicate if they support P-CSCF restoration procedure.","193","13.9","Technical Enhancements and Improvements [TEI13]",650,"Agreed","2015-01-23T11:28:03.003","2015-01-23T11:25:40.207","","","Rel-13","29.214","13.0.0","PCSCF_RES","0371","","B","CP-150134","","","","",""]
["C3-150066","Access network information reporting during the IP-CAN session termination","MCC","Mathieu Mangion",27904,"CR","","","Omitted Rel-12 CR, it is equivalent to C3-144290. Add a note to clarify that the PCRF receives the access network information if it is requested by the AF previously or the IP-CAN session/IP-CAN bearer is terminated.Secondly to correct the descriptions to","193","13.9","Technical Enhancements and Improvements [TEI13]",660,"Agreed","2015-01-23T11:28:03.080","2015-01-23T11:25:41.090","","","Rel-13","29.214","13.0.0","NWK-PL2IMS-CT","0372","","F","CP-150131","","","","",""]
["C3-150067","Introduction of a reference to the Rest-Rx interface","MCC","Mathieu Mangion",27904,"CR","","","Omitted Rel-12 CR, it is equivalent to C3-144206. 3GPP TS 29.201 added to the list of references and the scope. A definition for RESTful HTTP is added. An abbreviation for XML is added.","193","13.9","Technical Enhancements and Improvements [TEI13]",670,"Agreed","2015-01-23T11:28:03.160","2015-01-23T11:25:42.017","","","Rel-13","29.214","13.0.0","REST_AF_PC","0373","","F","CP-150136","","","","",""]
["C3-150068","Inclusion of RAN/NAS cause values into SIP signalling by P-CSCF","MCC","Mathieu Mangion",27904,"CR","","","Omitted Rel-12 CR, it is equivalent to C3-144248. P-CSCF can include RAN/NAS release cause information in the corresponding SIP message as specified in 3GPP TS 24.229.","193","13.9","Technical Enhancements and Improvements [TEI13]",680,"Agreed","2015-01-23T11:28:03.243","2015-01-23T11:25:42.897","","","Rel-13","29.214","13.0.0","NWK-PL2IMS-CT, TEI13","0374","","B","CP-150131","","","","",""]
["C3-150069","Precedence derivation for ADC rule","MCC","Mathieu Mangion",27904,"CR","","","Omitted Rel-12 CR, it is equivalent to C3-144235. The V-PCRF sets the Precedence AVP based on the value received in the PCC rule.","193","13.9","Technical Enhancements and Improvements [TEI13]",690,"Agreed","2015-01-23T11:28:03.323","2015-01-23T11:25:44.507","","","Rel-13","29.215","13.0.0","SAPP-CT3","0367","","A","CP-150135","","","","",""]
["C3-150070","Support for IPv6 prefix retrieve by the HSGW during the eHRPD pre-registration procedure","MCC","Mathieu Mangion",27904,"CR","","","Omitted Rel-12 CR, it is equivalent to C3-145216. Inclusion of the Framed-Ipv6-Prefix AVP in the Subsession-Decision-Info, secondly add a new annex to describe the procedure and thirdly include the reference and abbreviations.","193","13.9","Technical Enhancements and Improvements [TEI13]",700,"Agreed","2015-01-23T11:28:03.407","2015-01-23T11:25:45.363","","","Rel-13","29.215","13.0.0","SAES-St3-PCC, TEI13","0368","","A","CP-150132","","","","",""]
["C3-150071","revised WID on IMS Signalling Activated Trace (ISAT)","Vodafone GmbH","Mathieu Mangion",27904,"WID","","","The purpose of this document is a revises WID on IMS Signalling Activated Trace.","196","13.10","Rel-13 contributions on other Work Items",710,"Revised","2015-01-23T11:28:03.487","2015-01-23T16:43:49.863","","C3-150305","Rel-13","","","","","","","","","","","",""]
["C3-150072","Corrections to the Gateway Control and QoS rules Provision procedure","China Telecom,ZTE,Huawei","Mathieu Mangion",27904,"CR","","","Corrections to the Gateway Control and QoS rules Provision procedure in section 4.3.2.1.","30","8.14.1","Signalling flows (29.213)",720,"Agreed","2015-01-23T11:28:03.500","2015-01-23T11:25:46.977","","","Rel-8","29.213","8.17.0","SAES-St3-PCC","0585","","F","CP-150094","","","","",""]
["C3-150073","Corrections to the Gateway Control and QoS rules Provision procedure","China Telecom,ZTE,Huawei","Mathieu Mangion",27904,"CR","","","Gateway Control and QoS rules Provision procedure is initiated by PCRF not by BBERF in step 17 in section 4.3.2.1.","30","8.14.1","Signalling flows (29.213)",730,"Agreed","2015-01-23T11:28:03.580","2015-01-23T11:25:47.823","","","Rel-9","29.213","9.14.0","SAES-St3-PCC","0586","","A","CP-150094","","","","",""]
["C3-150074","Corrections to the Gateway Control and QoS rules Provision procedure","China Telecom,ZTE,Huawei","Mathieu Mangion",27904,"CR","","","Gateway Control and QoS rules Provision procedure is initiated by PCRF not by BBERF in step 17 in section 4.3.2.1.","30","8.14.1","Signalling flows (29.213)",740,"Agreed","2015-01-23T11:28:03.660","2015-01-23T11:25:48.663","","","Rel-10","29.213","10.12.0","SAES-St3-PCC","0587","","A","CP-150094","","","","",""]
["C3-150075","Corrections to the Gateway Control and QoS rules Provision procedure","China Telecom,ZTE,Huawei","Mathieu Mangion",27904,"CR","","","Gateway Control and QoS rules Provision procedure is initiated by PCRF not by BBERF in step 18 in section 4.3.2.1.","30","8.14.1","Signalling flows (29.213)",750,"Agreed","2015-01-23T11:28:03.743","2015-01-23T11:25:49.513","","","Rel-11","29.213","11.13.0","SAES-St3-PCC","0588","","A","CP-150094","","","","",""]
["C3-150076","Corrections to the Gateway Control and QoS rules Provision procedure","China Telecom,ZTE,Huawei","Mathieu Mangion",27904,"CR","","","Gateway Control and QoS rules Provision procedure is initiated by PCRF not by BBERF in step 18 in section 4.3.2.1.","30","8.14.1","Signalling flows (29.213)",760,"Agreed","2015-01-23T11:28:03.823","2015-01-23T11:25:50.367","","","Rel-12","29.213","12.6.0","SAES-St3-PCC","0589","","A","CP-150094","","","","",""]
["C3-150077","Corrections to the Gateway Control and QoS rules Provision procedure","China Telecom,ZTE,Huawei","Mathieu Mangion",27904,"CR","","","Gateway Control and QoS rules Provision procedure is initiated by PCRF not by BBERF in step 18 in section 4.3.2.1.","30","8.14.1","Signalling flows (29.213)",770,"Agreed","2015-01-23T11:28:03.900","2015-01-23T11:25:51.220","","","Rel-13","29.213","13.0.0","SAES-St3-PCC","0590","","A","CP-150094","","","","",""]
["C3-150078","Corrections to the Gateway Control and QoS rules Provision procedure","China Telecom,ZTE,Huawei","Mathieu Mangion",27904,"CR","","","","30","8.14.1","Signalling flows (29.213)",780,"Withdrawn","2015-01-23T11:28:03.980",null,"","","Rel-13","29.213","13.0.0","SAES-St3-PCC","0591","","A","-","","","","",""]
["C3-150079","Corrections to the Used-Service-Unit AVP when UMCH feature is supported","China Telecom,ZTE,Huawei","Mathieu Mangion",27904,"CR","","","Monitoring-Time AVP may be optionally included in Used-Service-Unit AVP if UMCH feature is supported.","135","11.37","Technical Enhancements and Improvements [TEI11]",790,"Revised","2015-01-23T11:28:04.057","2015-01-23T11:25:52.943","","C3-150302","Rel-11","29.212","11.14.0","TEI11","1275","","F","-","","","","",""]
["C3-150080","Corrections to the Used-Service-Unit AVP when UMCH feature is supported","China Telecom,ZTE,Huawei","Mathieu Mangion",27904,"CR","","","Monitoring-Time AVP may be optionally included in Used-Service-Unit AVP if UMCH feature is supported.","135","11.37","Technical Enhancements and Improvements [TEI11]",800,"Revised","2015-01-23T11:28:04.137","2015-01-23T11:25:54.240","","C3-150303","Rel-12","29.212","12.7.0","TEI11","1276","","A","-","","","","",""]
["C3-150081","Corrections to the Used-Service-Unit AVP when UMCH feature is supported","China Telecom,ZTE,Huawei","Mathieu Mangion",27904,"CR","","","Monitoring-Time AVP may be optionally included in Used-Service-Unit AVP if UMCH feature is supported.","135","11.37","Technical Enhancements and Improvements [TEI11]",810,"Revised","2015-01-23T11:28:04.230","2015-01-23T11:25:55.113","","C3-150304","Rel-13","29.212","13.0.0","TEI11","1277","","A","-","","","","",""]
["C3-150082","Enhanced NGCN based MCPTT architecture","Huawei, Hisilicon,TD-Tech","Mathieu Mangion",27904,"pCR","","","This contribution is to discuss how to enhance the NGCN based archtecture to meet the MCPTT application.","184","13","Release 13",820,"Withdrawn","2015-01-23T11:28:04.310",null,"","","Rel-13","","","","","","","","","","","",""]
["C3-150083","DMO/DMO-R Group call setup","Huawei, Hisilicon,TD-Tech","Mathieu Mangion",27904,"pCR","","","This contribution is to provide a method that DMO group call controlled by call originating user","184","13","Release 13",830,"Withdrawn","2015-01-23T11:28:04.327",null,"","","Rel-13","","","","","","","","","","","",""]
["C3-150084","Layer 3 UE-to-network relay solution for NMO-R","Huawei, Hisilicon,TD-Tech","Mathieu Mangion",27904,"pCR","","","This contribution is to provide another possible solution, IP router based (layer-3 relay)","184","13","Release 13",840,"Withdrawn","2015-01-23T11:28:04.347",null,"","","Rel-13","","","","","","","","","","","",""]
["C3-150085","MCPTT deployment scenarios","Huawei, Hisilicon,TD-Tech","Mathieu Mangion",27904,"pCR","","","This contribution describes the main deployment scenarios to be considered by MCPTT application.","184","13","Release 13",850,"Withdrawn","2015-01-23T11:28:04.367",null,"","","Rel-13","","","","","","","","","","","",""]
["C3-150086","Roaming scenarios for MCPTT service","Huawei, Hisilicon,TD-Tech","Mathieu Mangion",27904,"pCR","","","This document povides some roaming scenarios for MCPTT service","184","13","Release 13",860,"Withdrawn","2015-01-23T11:28:04.387",null,"","","Rel-13","","","","","","","","","","","",""]
["C3-150087","SIP over eMBMS bearer","Huawei, Hisilicon,TD-Tech","Mathieu Mangion",27904,"pCR","","","This contribution proposes a method to transmit SIP signalling over pre-established eMBMS bearer.","15","8","Release 8",870,"Withdrawn","2015-01-23T11:28:04.403",null,"","","Rel-13","","","","","","","","","","","",""]
["C3-150088","TDF support for downlink packet marking","Allot Communications Ltd., Huawei","Mathieu Mangion",27904,"CR","","","TDF based packet marking in order to support QoS enforcement in the downlink direction is introduced.","195","13.9.2","TEI13 for Packet Core",880,"Revised","2015-01-23T11:28:04.420","2015-01-23T11:25:55.990","","C3-150325","Rel-13","29.212","13.0.0","SAPP, SAPP-CT3","1278","","C","-","","","","",""]
["C3-150089","Adapt PCC architecture diagrams to include Np reference point","Huawei","Mathieu Mangion",27904,"CR","","","The PCC architecture figures in this specification is adapted to include Np reference point according to the normative work of UPCON.","185","13.1","CT aspects of User Plane Congestion Management (UPCON) for Building Block I",890,"Agreed","2015-01-23T11:28:04.503","2015-01-26T05:16:21.227","","","Rel-13","29.201","12.1.0","UPCON-DOTCON-CT","0019","","B","CP-150125","","","","",""]
["C3-150090","Mitigating RAN user plane congestion over Rest Rx","Huawei","Mathieu Mangion",27904,"CR","","","Deferred transfer of service information from the AF is added in AF session establishment/modification procedure, and XML representation is updated to include RetryInterval element correspondingly.","185","13.1","CT aspects of User Plane Congestion Management (UPCON) for Building Block I",900,"Revised","2015-01-23T11:28:04.577","2015-01-26T05:16:21.247","","C3-150309","Rel-13","29.201","12.1.0","UPCON-DOTCON-CT","0020","","B","-","","","","",""]
["C3-150091","Add missing definition of RAN user plane congestion","Huawei","Mathieu Mangion",27904,"CR","","","Add the definition of RAN user plane congestion according to stage 2 definition in TS 23.203.","185","13.1","CT aspects of User Plane Congestion Management (UPCON) for Building Block I",910,"Agreed","2015-01-23T11:28:04.667","2015-01-26T05:16:21.267","","","Rel-13","29.213","13.0.0","UPCON-DOTCON-CT","0592","","B","CP-150125","","","","",""]
["C3-150092","DRA procedure to support PCRF selection by the RCAF","Huawei","Mathieu Mangion",27904,"CR","","","Add the DRA procedure of PCRF selection by the RCAF under subclause 7.3.","185","13.1","CT aspects of User Plane Congestion Management (UPCON) for Building Block I",920,"Revised","2015-01-23T11:28:04.743","2015-01-26T05:16:21.287","","C3-150310","Rel-13","29.213","13.0.0","UPCON-DOTCON-CT","0593","","B","-","","","","",""]
["C3-150093","Adding UE location information in aggregated RUCI reporting","Huawei","Mathieu Mangion",27904,"pCR","","","Add the Congestion-Location-Id AVP in the Aggregated-RUCI-Report AVP to support UE location information in aggregated RUCI reporting.","185","13.1","CT aspects of User Plane Congestion Management (UPCON) for Building Block I",930,"Revised","2015-01-23T11:28:04.820","2015-01-26T05:16:21.310","","C3-150307","Rel-13","29.217","1.0.0","UPCON-DOTCON-CT","","","","","","","","",""]
["C3-150094","Remove editor's note on optimization of UE identity in aggregated RUCI reporting","Huawei","Mathieu Mangion",27904,"pCR","","","Propose to remove the editor's note without any change of UE identity in aggregated RUCI reporting.","185","13.1","CT aspects of User Plane Congestion Management (UPCON) for Building Block I",940,"Revised","2015-01-23T11:28:04.833","2015-01-26T05:16:21.090","","C3-150306","Rel-13","29.217","1.0.0","UPCON-DOTCON-CT","","","","","","","","",""]
["C3-150095","Clarifying the congestion level value in AVP defintion","Huawei","Mathieu Mangion",27904,"pCR","","","Add the value definition for Congestion-Level-Value AVP.","185","13.1","CT aspects of User Plane Congestion Management (UPCON) for Building Block I",950,"Revised","2015-01-23T11:28:04.847","2015-01-26T05:16:21.107","","C3-150311","Rel-13","29.217","1.0.0","UPCON-DOTCON-CT","","","","","","","","",""]
["C3-150096","Cleanup of definitions and abbreviations","Huawei","Mathieu Mangion",27904,"pCR","","","Add the definition of “RAN user plane congestion” according to stage 2 TS and remove unused abbreviations.","185","13.1","CT aspects of User Plane Congestion Management (UPCON) for Building Block I",960,"Agreed","2015-01-23T11:28:04.860","2015-01-26T05:16:21.130","","","Rel-13","29.217","1.0.0","UPCON-DOTCON-CT","","","","","","","","",""]
["C3-150097","Editor's note cleanup","Huawei","Mathieu Mangion",27904,"pCR","","","Remove 2 editor’s notes based on the progress analysis of the normative work.","185","13.1","CT aspects of User Plane Congestion Management (UPCON) for Building Block I",970,"Revised","2015-01-23T11:28:04.873","2015-01-26T05:16:21.150","","C3-150312","Rel-13","29.217","1.0.0","UPCON-DOTCON-CT","","","","","","","","",""]
["C3-150098","Remove access type attribute in table of Np reused Diameter AVPs","Huawei","Mathieu Mangion",27904,"pCR","","","Remove access type column from Table 5.4.1 based on group agreement.","185","13.1","CT aspects of User Plane Congestion Management (UPCON) for Building Block I",980,"Merged","2015-01-23T11:28:04.887","2015-01-26T05:16:21.170","","","Rel-13","29.217","1.0.0","UPCON-DOTCON-CT","","","","","","","","",""]
["C3-150099","New AVP and experimental result code in TS 29.214","Huawei","Mathieu Mangion",27904,"LS out","","","LS out on request allocate a range of experimental ting CT4 to result codes for representing transient failures in TS 29.214.","185","13.1","CT aspects of User Plane Congestion Management (UPCON) for Building Block I",990,"Withdrawn","2015-01-23T11:28:04.903","2015-01-26T05:16:21.193","","","Rel-13","","","","","","",""]
["C3-150100","Roaming applicability in EPC-level ProSe discovery","Huawei","Mathieu Mangion",27904,"CR","","","Add a note ” For EPC-level ProSe discovery the roaming architecture is not specified in this release.” in subclause 4.1 PC2 reference model.","170","12.36","CT aspects of Proximity-based Services",1000,"Revised","2015-01-23T11:28:04.920","2015-01-23T11:26:06.440","","C3-150350","Rel-12","29.343","12.1.0","630206","0002","","F","-","","","","",""]
["C3-150101","Reference update to align with the published BBF documents","Huawei","Mathieu Mangion",27904,"CR","","","Update BBF document name WT-300 to TR-300 in both reference section and referred normal text.","161","12.27","Policy and Charging Control for supporting traffic from fixed terminals and NSWO traffic from 3GPP Ues in fixed broadband access networks",1010,"Agreed","2015-01-23T11:28:05","2015-01-23T11:26:07.290","","","Rel-12","29.212","12.7.0","P4C-F-CT3","1279","","F","CP-150111","","","","",""]
["C3-150102","Reference update to align with the published BBF documents","Huawei","Mathieu Mangion",27904,"CR","","","Update BBF document name WT-300 to TR-300 in both reference section and referred normal text.","161","12.27","Policy and Charging Control for supporting traffic from fixed terminals and NSWO traffic from 3GPP Ues in fixed broadband access networks",1020,"Agreed","2015-01-23T11:28:05.087","2015-01-23T11:26:08.167","","","Rel-13","29.212","13.0.0","P4C-F-CT3","1280","","A","CP-150111","","","","",""]
["C3-150103","Remove editor's note on access line identifier","Huawei","Mathieu Mangion",27904,"CR","","","Remove editor’s note “in Annex F.5.1 and void BBF WT-134 in the reference clause.","161","12.27","Policy and Charging Control for supporting traffic from fixed terminals and NSWO traffic from 3GPP Ues in fixed broadband access networks",1030,"Agreed","2015-01-23T11:28:05.167","2015-01-23T11:26:09.073","","","Rel-12","29.213","12.6.0","P4C-F-CT3","0594","","F","CP-150111","","","","",""]
["C3-150104","Remove editor's note on access line identifier","Huawei","Mathieu Mangion",27904,"CR","","","Remove editor’s note “in Annex F.5.1 and void BBF WT-134 in the reference clause.","161","12.27","Policy and Charging Control for supporting traffic from fixed terminals and NSWO traffic from 3GPP Ues in fixed broadband access networks",1040,"Agreed","2015-01-23T11:28:05.247","2015-01-23T11:26:10.540","","","Rel-13","29.213","13.0.0","P4C-F-CT3","0595","","A","CP-150111","","","","",""]
["C3-150105","Reference update to align with the published BBF documents","Huawei","Mathieu Mangion",27904,"CR","","","Update BBF document name WT-203 to TR-203, WT-134 to TR-134 and WT-146 to TR-146 in both reference section and referred normal text.","161","12.27","Policy and Charging Control for supporting traffic from fixed terminals and NSWO traffic from 3GPP Ues in fixed broadband access networks",1050,"Revised","2015-01-23T11:28:05.330","2015-01-23T11:26:11.403","","C3-150345","Rel-12","29.215","12.6.0","P4C-F-CT3","0369","","F","-","","","","",""]
["C3-150106","Reference update to align with the published BBF documents","Huawei","Mathieu Mangion",27904,"CR","","","Update BBF document name WT-203 to TR-203, WT-134 to TR-134 and WT-146 to TR-146 in both reference section and referred normal text.","161","12.27","Policy and Charging Control for supporting traffic from fixed terminals and NSWO traffic from 3GPP Ues in fixed broadband access networks",1060,"Revised","2015-01-23T11:28:05.417","2015-01-23T11:26:12.237","","C3-150346","Rel-13","29.215","13.0.0","P4C-F-CT3","0370","","A","-","","","","",""]
["C3-150107","TWAN release cause for trusted WLAN","Huawei","Mathieu Mangion",27904,"CR","","","Add corresponding handling of TWAN-Release-Cause in IP-CAN session termination, bearer termination and PCC rule error handling procedures.","195","13.9.2","TEI13 for Packet Core",1070,"Revised","2015-01-23T11:28:05.497","2015-01-23T11:26:13.077","","C3-150334","Rel-13","29.212","13.0.0","NWK-PL2IMS-CT, TEI13","1281","","B","-","","","","",""]
["C3-150108","TWAN release cause for trusted WLAN","Huawei","Mathieu Mangion",27904,"CR","","","Add corresponding handling of TWAN-Release-Cause in AF session termination, IP-CAN session termination, Service Data Flow Deactivation and Notification of Signalling Path Status.","195","13.9.2","TEI13 for Packet Core",1080,"Revised","2015-01-23T11:28:05.580","2015-01-23T11:26:13.913","","C3-150335","Rel-13","29.214","13.0.0","NWK-PL2IMS-CT, TEI13","0375","","B","-","","","","",""]
["C3-150109","Correction on volumn and time threshold provisioning","Huawei","Mathieu Mangion",27904,"CR","","","Remove the duplicated text description on volume and time threshold provisioning in subclause 4.5.17.5.","182","12.46.2","TEI12 for Packet Core",1090,"Revised","2015-01-23T11:28:05.667","2015-01-23T11:26:14.757","","C3-150358","Rel-12","29.212","12.7.0","TEI12","1282","","F","-","","","","",""]
["C3-150110","Correction on volumn and time threshold provisioning","Huawei","Mathieu Mangion",27904,"CR","","","Remove the duplicated text description on volume and time threshold provisioning in subclause 4.5.17.5.","182","12.46.2","TEI12 for Packet Core",1100,"Revised","2015-01-23T11:28:05.750","2015-01-23T11:26:15.613","","C3-150359","Rel-13","29.212","13.0.0","TEI12","1283","","A","-","","","","",""]
["C3-150111","Paging policy differentiation for IMS voice","Alcatel-Lucent, Verizon","Mathieu Mangion",27904,"CR","","","The stage 2 specification TS 23.401 V13.1.0, subclause 4.9 contains the requirements for paging policy differentiation as an optional feature. TS 24.229 V13.0.0, subclause L.3.2.4 standardizes that the P-CSCF may support paging policy differentiation. Net","186","13.2","CT aspects of voice over E-UTRAN Paging Policy Differentiation",1110,"Revised","2015-01-23T11:28:05.833","2015-01-23T11:26:16.453","","C3-150319","Rel-13","29.061","12.8.0","voE_UTRAN_PPD-CT, 650303","0444","","B","-","","","","",""]
["C3-150112","Correction to attribute “a=inactive” in initial INVITE","Deutsche Telekom AG","Mathieu Mangion",27904,"CR","","","MGCF are not required to include the ”a=inactive” attribute in the initial INVITE requests. Dependent on agreement of related CT1 CR.","146","12.14","IMS Stage-3 IETF Protocol Alignment  [IMSProtoc6]",1120,"Revised","2015-01-23T11:28:05.917","2015-01-23T12:52:12.300","","C3-150327","Rel-12","29.163","12.6.0","IMSProtoc6","0848","","F","-","","","","",""]
["C3-150113","Correction to attribute “a=inactive” in initial INVITE","Deutsche Telekom AG","Mathieu Mangion",27904,"CR","","","MGCF are not required to include the ”a=inactive” attribute in the initial INVITE requests. Dependent on agreement of related CT1 CR.","146","12.14","IMS Stage-3 IETF Protocol Alignment  [IMSProtoc6]",1130,"Revised","2015-01-23T11:28:05.990","2015-01-23T12:52:12.277","","C3-150328","Rel-13","29.163","13.0.0","IMSProtoc6","0849","","A","-","","","","",""]
["C3-150114","Introducing EVS over 3G CS networks – CT impacts","Qualcomm Incorporated","Mathieu Mangion",27904,"other","","","This document is a discussion paper analyzing the CT impacts of introducing EVS over 3G CS networks.","196","13.10","Rel-13 contributions on other Work Items",1140,"Noted","2015-01-23T11:28:06.067","2015-01-24T20:56:52.750","","","Rel-13","","","650305","","","","","","","","",""]
["C3-150115","New WID on CT aspects of EVS in 3G Circuit-Switched Networks","Qualcomm Incorporated","Mathieu Mangion",27904,"WID","","","This document is a new Rel-13 WID on CT aspects of EVS in 3G Circuit-Switched Networks.","196","13.10","Rel-13 contributions on other Work Items",1150,"Revised","2015-01-23T11:28:06.083","2015-01-24T20:56:52.787","","C3-150258","Rel-13","","","","","","","","","","","",""]
["C3-150116","Request RAT type reporting over Rx interface","China Telecom, Huawei","Mathieu Mangion",27904,"CR","","","Adding a new Request-RAT-Type AVP and related procedure to implement the requirement that the AF asks the PCRF to report the current RAT type.","195","13.9.2","TEI13 for Packet Core",1160,"Withdrawn","2015-01-23T11:28:06.097","2015-01-23T11:26:20.477","","","Rel-13","29.214","13.0.0","TEI13","0376","","F","-","","","","",""]
["C3-150117","Instance-number value for secondary-realm","Ericsson","Mathieu Mangion",27904,"CR","","","The instance-number value must be assigned when adding a \"secondary-realm\" SDP attribute in an SDP offer but the specification currently does not describe how the IMS-ALG or the UA will assign the instance-number value for the \"secondary-realm\" SDP attrib","82","10.17","Optimal Media Routeing [OMR]",1170,"Agreed","2015-01-23T11:28:06.180","2015-01-23T11:26:21.357","","","Rel-10","29.079","10.6.0","OMR","0034","","F","CP-150100","","","","",""]
["C3-150118","Instance-number value for secondary-realm","Ericsson","Mathieu Mangion",27904,"CR","","","The instance-number value must be assigned when adding a \"secondary-realm\" SDP attribute in an SDP offer but the specification currently does not describe how the IMS-ALG or the UA will assign the instance-number value for the \"secondary-realm\" SDP attrib","82","10.17","Optimal Media Routeing [OMR]",1180,"Agreed","2015-01-23T11:28:06.263","2015-01-23T11:26:22.227","","","Rel-11","29.079","11.5.0","OMR","0035","","A","CP-150100","","","","",""]
["C3-150119","Instance-number value for secondary-realm","Ericsson","Mathieu Mangion",27904,"CR","","","The instance-number value must be assigned when adding a \"secondary-realm\" SDP attribute in an SDP offer but the specification currently does not describe how the IMS-ALG or the UA will assign the instance-number value for the \"secondary-realm\" SDP attrib","82","10.17","Optimal Media Routeing [OMR]",1190,"Agreed","2015-01-23T11:28:06.353","2015-01-23T11:26:23.103","","","Rel-12","29.079","12.1.0","OMR","0036","","A","CP-150100","","","","",""]
["C3-150120","Checksum calculation","Ericsson","Mathieu Mangion",27904,"CR","","","Clarified that media lines containing a \"secondary-realm\" SDP attribute shall be included in the checksum calculation.","82","10.17","Optimal Media Routeing [OMR]",1200,"Agreed","2015-01-23T11:28:06.433","2015-01-23T11:26:23.953","","","Rel-10","29.079","10.6.0","OMR","0037","","F","CP-150100","","","","",""]
["C3-150121","Checksum calculation","Ericsson","Mathieu Mangion",27904,"CR","","","Clarified that media lines containing a \"secondary-realm\" SDP attribute shall be included in the checksum calculation.","82","10.17","Optimal Media Routeing [OMR]",1210,"Agreed","2015-01-23T11:28:06.517","2015-01-23T11:26:24.793","","","Rel-11","29.079","11.5.0","OMR","0038","","A","CP-150100","","","","",""]
["C3-150122","Checksum calculation","Ericsson","Mathieu Mangion",27904,"CR","","","Clarified that media lines containing a \"secondary-realm\" SDP attribute shall be included in the checksum calculation.","82","10.17","Optimal Media Routeing [OMR]",1220,"Agreed","2015-01-23T11:28:06.600","2015-01-23T11:26:25.803","","","Rel-12","29.079","12.1.0","OMR","0039","","A","CP-150100","","","","",""]
["C3-150123","Correcting UA procedure","Ericsson","Mathieu Mangion",27904,"CR","","","The UA behaviour upon reception of the SDP answer with the unspecified connection address and the visited-realm instance is specified.","82","10.17","Optimal Media Routeing [OMR]",1230,"Agreed","2015-01-23T11:28:06.687","2015-01-23T11:26:27.200","","","Rel-10","29.079","10.6.0","OMR","0040","","F","CP-150100","","","","",""]
["C3-150124","Correcting UA procedure","Ericsson","Mathieu Mangion",27904,"CR","","","The UA behaviour upon reception of the SDP answer with the unspecified connection address and the visited-realm instance is specified.","82","10.17","Optimal Media Routeing [OMR]",1240,"Agreed","2015-01-23T11:28:06.780","2015-01-23T11:26:28.043","","","Rel-11","29.079","11.5.0","OMR","0041","","A","CP-150100","","","","",""]
["C3-150125","Correcting UA procedure","Ericsson","Mathieu Mangion",27904,"CR","","","The UA behaviour upon reception of the SDP answer with the unspecified connection address and the visited-realm instance is specified.","82","10.17","Optimal Media Routeing [OMR]",1250,"Agreed","2015-01-23T11:28:06.870","2015-01-23T11:26:28.910","","","Rel-12","29.079","12.1.0","OMR","0042","","A","CP-150100","","","","",""]
["C3-150126","Reference update: draft-ietf-mmusic-sctp-sdp","Ericsson","Mathieu Mangion",27904,"CR","","","A new version of draft-ietf-mmusic-sctp-sdp has been submitted to IETF.","145","12.13","IMS-based Telepresence (Stage 3) [IMS_TELEP]",1260,"Revised","2015-01-23T11:28:06.967","2015-01-23T11:26:29.763","","C3-150326","Rel-12","29.165","12.6.0","580001","0720","","F","-","","","","",""]
["C3-150127","Reference update: draft-holmberg-sipcore-received-realm","Ericsson","Mathieu Mangion",27904,"CR","","","A new version of draft-holmberg-sipcore-received-realm has been submitted to IETF.","146","12.14","IMS Stage-3 IETF Protocol Alignment  [IMSProtoc6]",1270,"Agreed","2015-01-23T11:28:07.053","2015-01-23T11:26:30.670","","","Rel-12","29.165","12.6.0","IMSProtoc6","0721","","F","CP-150108","","","","",""]
["C3-150128","Incorrect implementation of CRs","MCC","Mathieu Mangion",27904,"CR","","","The present CR covers a number of the editorial changes in CR#0694r1, CR#0686 and CR#0695r1 that were not incorporated in to the TS 29.165.","183","12.47","Rel-12 contributions on other Work Items",1280,"Revised","2015-01-23T11:28:07.137","2015-01-23T11:26:32.687","","C3-150260","Rel-12","29.165","12.6.0","TEI12","0722","","D","-","","","","",""]
["C3-150129","Reference update: draft-holmberg-dispatch-iotl","Ericsson","Mathieu Mangion",27904,"CR","","","A new version of draft-holmberg-dispatch-iotl has been submitted to IETF.","162","12.28","Study on Technical aspects on Roaming End-to-end scenarios with VoLTE IMS and other networks [FS_REVOLTE_IMS]",1290,"Revised","2015-01-23T11:28:07.223","2015-01-23T11:26:33.553","","C3-150331","Rel-12","29.949","12.0.0","FS_REVOLTE_IMS","0001","","F","-","","","","",""]
["C3-150130","Annex A corrections","Ericsson LM","Mathieu Mangion",27904,"CR","","","The annex A contains some inconsistent references:\nSometimes the trust domain table is referenced and sometimes TS 24.229 for header fields that appear in the trust domain table.\nThe referencing should be aligned!","194","13.9.1","TEI13 for IMS/CS",1300,"Agreed","2015-01-23T11:28:07.310","2015-01-23T12:52:38.387","","","Rel-13","29.165","12.6.0","TEI13","0723","","F","CP-150130","","","","",""]
["C3-150131","Restoration-Info header field applicability","Ericsson","Mathieu Mangion",27904,"CR","","","The Restoration-Info header field can only appear on the roaming interface hence the Restoration-Info header field  needs to be added to subclause 6.1.1.3.","178","12.44","P-CSCF restoration enhancements [PCSCF_RES]",1310,"Revised","2015-01-23T11:28:07.387","2015-01-23T12:52:38.420","","C3-150333","Rel-12","29.165","12.6.0","PCSCF_RES","0724","","F","-","","","","",""]
["C3-150132","Relayed-Charge header field","Ericsson LM","Mathieu Mangion",27904,"CR","","","A Relayed-Charge header field was created in TS 24.229 in the last meeting.\nTS 29.165 needs to include the Relayed-Charge header field","146","12.14","IMS Stage-3 IETF Protocol Alignment  [IMSProtoc6]",1320,"Revised","2015-01-23T11:28:07.463","2015-01-23T12:52:38.443","","C3-150329","Rel-12","29.165","12.6.0","IMSProtoc6","0725","","F","-","","","","",""]
["C3-150133","Applying drafting rules","Ericsson LM","Mathieu Mangion",27904,"CR","","","The TS 29.165 does not fulfill drafting rules with regards to referencing tables and header levels in annexes","194","13.9.1","TEI13 for IMS/CS",1330,"Revised","2015-01-23T11:28:07.543","2015-01-23T12:52:38.467","","C3-150368","Rel-13","29.165","12.6.0","TEI13","0726","","F","-","","","","",""]
["C3-150134","PS to CS SRVCC after access transfer is completed interworking","Ericsson LM","Mathieu Mangion",27904,"CR","","","At the moment TS 24.237 references 29.292 for 3GPP TS 24.229 [2] and NAS signalling as described in 3GPP TS 24.008 [3] interworking after a PS to CS access transfer is completed. However, since TS 29.292 covers much more than is needed by TS 24.237 some c","194","13.9.1","TEI13 for IMS/CS",1340,"Postponed","2015-01-23T11:28:07.617","2015-01-23T12:52:38.500","","","Rel-13","29.292","12.4.0","TEI13","0106","","F","-","","","","",""]
["C3-150135","Procedures to avoid changes in OMR outcome","Ericsson","Mathieu Mangion",27904,"other","","","This document serves as reading support for the CRs describing the procedures to avoid changes in OMR outcome\".","82","10.17","Optimal Media Routeing [OMR]",1350,"Noted","2015-01-23T11:28:07.710","2015-01-23T12:52:38.537","","","","","","OMR","","","","","","","","",""]
["C3-150136","Procedures for avoiding changes in the OMR algorithm outcome on subsequent SDP offer/answer transactions","Ericsson","Mathieu Mangion",27904,"CR","","","The media anchoring points may change depending on the direction on subsequent SDP offer/answer transactions. This may be OK from the generic OMR procedure point of view. From real life traffic point of view this may result in problems with media going in","82","10.17","Optimal Media Routeing [OMR]",1360,"Revised","2015-01-23T11:28:07.730","2015-01-23T12:52:38.557","","C3-150289","Rel-10","29.079","10.6.0","OMR","0043","","F","-","","","","",""]
["C3-150137","Procedures for avoiding changes in the OMR algorithm outcome on subsequent SDP offer/answer transactions","Ericsson LM","Mathieu Mangion",27904,"CR","","","The media anchoring points may change depending on the direction on subsequent SDP offer/answer transactions. This may be OK from the generic OMR procedure point of view. From real life traffic point of view this may result in problems with media going in","82","10.17","Optimal Media Routeing [OMR]",1370,"Revised","2015-01-23T11:28:07.820","2015-01-23T12:52:38.600","","C3-150290","Rel-11","29.079","11.5.0","OMR","0044","","A","-","","","","",""]
["C3-150138","Procedures for avoiding changes in the OMR algorithm outcom on subsequent SDP offer/answer transactions","Ericsson LM","Mathieu Mangion",27904,"CR","","","The media anchoring points may change depending on the direction on subsequent SDP offer/answer transactions. This may be OK from the generic OMR procedure point of view. From real life traffic point of view this may result in problems with media going in","82","10.17","Optimal Media Routeing [OMR]",1380,"Revised","2015-01-23T11:28:07.900","2015-01-23T12:52:38.630","","C3-150291","Rel-12","29.079","12.1.0","OMR","0045","","A","-","","","","",""]
["C3-150139","Reference update: draft-ietf-insipid-session-id","Ericsson","Mathieu Mangion",27904,"CR","","","A new version of draft-ietf-insipid-session-id has been submitted to IETF.","146","12.14","IMS Stage-3 IETF Protocol Alignment  [IMSProtoc6]",1390,"Revised","2015-01-23T11:28:07.983","2015-01-23T11:26:36.153","","C3-150330","Rel-12","29.165","12.6.0","IMSProtoc6","0727","","F","-","","","","",""]
["C3-150140","Reference update: draft-holmberg-dispatch-iotl","Ericsson","Mathieu Mangion",27904,"CR","","","A new version of draft-holmberg-dispatch-iotl has been submitted to IETF.","150","12.17.1","Indication of NNI Routeing scenarios in SIP requests [NNI_RS]",1400,"Agreed","2015-01-23T11:28:08.077","2015-01-23T11:26:37.017","","","Rel-12","29.165","12.6.0","NNI_RS","0728","","F","CP-150109","","","","",""]
["C3-150141","Reference update: draft-holmberg-dispatch-iotl","Ericsson","Mathieu Mangion",27904,"CR","","","A new version of draft-holmberg-dispatch-iotl has been submitted to IETF.","150","12.17.1","Indication of NNI Routeing scenarios in SIP requests [NNI_RS]",1410,"Agreed","2015-01-23T11:28:08.167","2015-01-23T11:26:37.870","","","Rel-12","29.079","12.1.0","NNI_RS","0046","","F","CP-150109","","","","",""]
["C3-150142","LS on new cause URI parameter value for IN numbers interworking","ORANGE","Mathieu Mangion",27904,"LS out","","","LS from CT3 to SA5 (cc: CT1) to check if there is any charging aspects impacted by the introduction of the new parameter value.","192","13.8","Interworking of Called IN number and original Called IN number ISUP parameters",1420,"Revised","2015-01-23T11:28:08.257","2015-01-23T12:09:39.777","","C3-150370","Rel-13","","","INNB_IW","","","","",null,"SA5","CT1"]
["C3-150143","Reference update: draft-mohali-dispatch-cause-for-service-number","ORANGE","Mathieu Mangion",27904,"CR","","","Update of the IETF draft version number in references.","192","13.8","Interworking of Called IN number and original Called IN number ISUP parameters",1430,"Revised","2015-01-23T11:28:08.273","2015-01-23T12:09:39.797","","C3-150367","Rel-13","29.163","13.0.0","INNB_IW","0850","","F","-","","","","",""]
["C3-150144","Correction to the usage monitoring control for sponsored data connectivity","ZTE","Mathieu Mangion",27904,"CR","","","Add a new condition where all the service data flows of the AF session are terminated in the case that PCRF report the accumulated usage to the AF","93","10.26","CT3 Aspects of Policy Enhancements for Sponsored Connectivity and Coherent Access to Policy related Data Bases [PEST-CT3]",1440,"Agreed","2015-01-23T11:28:08.353","2015-01-24T06:24:16.607","","","Rel-10","29.214","10.13.0","PEST-CT3","0377","","F","CP-150101","","","","",""]
["C3-150145","Correction to the usage monitoring control for sponsored data connectivity","ZTE","Mathieu Mangion",27904,"CR","","","Add a new condition where all the service data flows of the AF session are terminated in the case that PCRF report the accumulated usage to the AF","93","10.26","CT3 Aspects of Policy Enhancements for Sponsored Connectivity and Coherent Access to Policy related Data Bases [PEST-CT3]",1450,"Agreed","2015-01-23T11:28:08.433","2015-01-24T06:24:16.637","","","Rel-11","29.214","11.14.0","PEST-CT3","0378","","A","CP-150101","","","","",""]
["C3-150146","Correction to the usage monitoring control for sponsored data connectivity","ZTE","Mathieu Mangion",27904,"CR","","","Add a new condition where all the service data flows of the AF session are terminated in the case that PCRF report the accumulated usage to the AF","93","10.26","CT3 Aspects of Policy Enhancements for Sponsored Connectivity and Coherent Access to Policy related Data Bases [PEST-CT3]",1460,"Agreed","2015-01-23T11:28:08.523","2015-01-24T06:24:16.667","","","Rel-12","29.214","12.6.0","PEST-CT3","0379","","A","CP-150101","","","","",""]
["C3-150147","Correction to the usage monitoring control for sponsored data connectivity","ZTE","Mathieu Mangion",27904,"CR","","","Add a new condition where all the service data flows of the AF session are terminated in the case that PCRF report the accumulated usage to the AF","93","10.26","CT3 Aspects of Policy Enhancements for Sponsored Connectivity and Coherent Access to Policy related Data Bases [PEST-CT3]",1470,"Agreed","2015-01-23T11:28:08.607","2015-01-24T06:24:16.697","","","Rel-13","29.214","13.0.0","PEST-CT3","0380","","A","CP-150101","","","","",""]
["C3-150148","Access network information report in case of IP-CAN bearer/IP-CAN session termination","ZTE","Mathieu Mangion",27904,"CR","","","The PCRF shall not report any subsequently received access network information to the AF, unless the related PCC/QoS rules was deactived due to the IP-CAN bearer is terminated or the IP-CAN session is terminated.","128","11.30","CT aspect on Network Provided Location Information for IMS",1480,"Revised","2015-01-23T11:28:08.683","2015-01-24T06:25:00.063","","C3-150298","Rel-11","29.214","11.14.0","NWK-PL2IMS-CT","0381","","F","-","","","","",""]
["C3-150149","Access network information report in case of IP-CAN bearer/IP-CAN session termination","ZTE","Mathieu Mangion",27904,"CR","","","The PCRF shall not report any subsequently received access network information to the AF, unless the related PCC/QoS rules was deactived due to the IP-CAN bearer is terminated or the IP-CAN session is terminated.","128","11.30","CT aspect on Network Provided Location Information for IMS",1490,"Revised","2015-01-23T11:28:08.760","2015-01-24T06:25:00.090","","C3-150299","Rel-12","29.214","12.6.0","NWK-PL2IMS-CT","0382","","A","-","","","","",""]
["C3-150150","Access network information report in case of IP-CAN bearer/IP-CAN session termination","ZTE","Mathieu Mangion",27904,"CR","","","The PCRF shall not report any subsequently received access network information to the AF, unless the related PCC/QoS rules was deactived due to the IP-CAN bearer is terminated or the IP-CAN session is terminated.","128","11.30","CT aspect on Network Provided Location Information for IMS",1500,"Revised","2015-01-23T11:28:08.837","2015-01-24T06:25:00.117","","C3-150300","Rel-13","29.214","13.0.0","NWK-PL2IMS-CT","0383","","A","-","","","","",""]
["C3-150151","Correction to temporary network failure handling","ZTE","Mathieu Mangion",27904,"CR","","","The access network information reporting shall be considered","133","11.35","Enhanced Nodes Restoration for EPC [eNR_EPC]",1510,"Withdrawn","2015-01-23T11:28:08.917","2015-01-24T06:25:00.147","","","Rel-11","29.214","11.14.0","eNR_EPC","0384","","F","-","","","","",""]
["C3-150152","Correction to temporary network failure handling","ZTE","Mathieu Mangion",27904,"CR","","","The access network information reporting shall be considered","133","11.35","Enhanced Nodes Restoration for EPC [eNR_EPC]",1520,"Withdrawn","2015-01-23T11:28:08.993","2015-01-24T06:25:34.537","","","Rel-12","29.214","12.6.0","eNR_EPC","0385","","A","-","","","","",""]
["C3-150153","Correction to temporary network failure handling","ZTE","Mathieu Mangion",27904,"CR","","","The access network information reporting shall be considered","133","11.35","Enhanced Nodes Restoration for EPC [eNR_EPC]",1530,"Revised","2015-01-23T11:28:09.077","2015-01-24T06:25:34.563","","C3-150301","Rel-13","29.214","13.0.0","eNR_EPC","0386","","A","-","","","","",""]
["C3-150154","TWAN supports access network information report","ZTE","Mathieu Mangion",27904,"CR","","","The PCEF determins whether current access network supports the access network information reporting based on the currently used IP-CAN type or the values of RAT-Type AVP and AN-Trusted AVP.","168","12.34","CT aspects of Network Provided Location Information for IMS Trusted WLAN Access Network [NETLOC_TWAN_CT]",1540,"Revised","2015-01-23T11:28:09.157","2015-01-24T06:25:34.590","","C3-150348","Rel-12","29.212","12.7.0","NETLOC_TWAN-CT","1284","","F","-","","","","",""]
["C3-150155","TWAN supports access network information report","ZTE","Mathieu Mangion",27904,"CR","","","The PCEF determins whether current access network supports the access network information reporting based on the currently used IP-CAN type or the values of RAT-Type AVP and AN-Trusted AVP.","168","12.34","CT aspects of Network Provided Location Information for IMS Trusted WLAN Access Network [NETLOC_TWAN_CT]",1550,"Revised","2015-01-23T11:28:09.237","2015-01-24T06:25:34.617","","C3-150349","Rel-13","29.212","13.0.0","NETLOC_TWAN-CT","1285","","A","-","","","","",""]
["C3-150156","TWAN supports access network information report","ZTE","Mathieu Mangion",27904,"CR","","","The 3GPP GPRS, 3GPP EPS and Trusted WLAN support access network information reporting in this release.","168","12.34","CT aspects of Network Provided Location Information for IMS Trusted WLAN Access Network [NETLOC_TWAN_CT]",1560,"Agreed","2015-01-23T11:28:09.327","2015-01-24T06:28:15.103","","","Rel-12","29.214","12.6.0","NETLOC_TWAN-CT","0387","","F","CP-150114","","","","",""]
["C3-150157","TWAN supports access network information report","ZTE","Mathieu Mangion",27904,"CR","","","The 3GPP GPRS, 3GPP EPS and Trusted WLAN support access network information reporting in this release.","168","12.34","CT aspects of Network Provided Location Information for IMS Trusted WLAN Access Network [NETLOC_TWAN_CT]",1570,"Agreed","2015-01-23T11:28:09.443","2015-01-24T06:28:15.130","","","Rel-13","29.214","13.0.0","NETLOC_TWAN-CT","0388","","A","CP-150114","","","","",""]
["C3-150158","Correction to the PRA reporting","ZTE","Mathieu Mangion",27904,"CR","","","PRA reporting descriptions are corrected","171","12.37","CT aspects of Core Network Overload  User Location Information reporting improvements [CNO_ULI-CT]",1580,"Revised","2015-01-23T11:28:09.553","2015-01-24T06:28:15.153","","C3-150351","Rel-12","29.212","12.7.0","CNO_ULI-CT","1286","","F","-","","","","",""]
["C3-150159","Correction to the PRA reporting","ZTE","Mathieu Mangion",27904,"CR","","","PRA reporting descriptions are corrected","171","12.37","CT aspects of Core Network Overload  User Location Information reporting improvements [CNO_ULI-CT]",1590,"Revised","2015-01-23T11:28:09.663","2015-01-24T06:28:15.180","","C3-150352","Rel-13","29.212","13.0.0","CNO_ULI-CT","1287","","A","-","","","","",""]
["C3-150160","Clarify the condition where the RCAF reports the RUCI","ZTE","Mathieu Mangion",27904,"pCR","","","Clarify the condition where the RCAF reports the RUCI","185","13.1","CT aspects of User Plane Congestion Management (UPCON) for Building Block I",1600,"Revised","2015-01-23T11:28:09.747","2015-01-24T06:30:31.343","","C3-150314","Rel-13","29.217","1.0.0","UPCON-DOTCON-CT","","","","","","","","",""]
["C3-150161","M bit set for the specific AVPs","ZTE","Mathieu Mangion",27904,"pCR","","","M bit is clear for the specific AVPs related to report restriction","185","13.1","CT aspects of User Plane Congestion Management (UPCON) for Building Block I",1610,"Revised","2015-01-23T11:28:09.763","2015-01-24T06:30:31.370","","C3-150315","Rel-13","29.217","1.0.0","UPCON-DOTCON-CT","","","","","","","","",""]
["C3-150162","Remove the access capability in re-used AVP table","ZTE","Mathieu Mangion",27904,"pCR","","","Remove the access capability in re-used AVP tablespecific AVPs related to report restriction","185","13.1","CT aspects of User Plane Congestion Management (UPCON) for Building Block I",1620,"Revised","2015-01-23T11:28:09.780","2015-01-24T06:30:31.407","","C3-150313","Rel-13","29.217","1.0.0","UPCON-DOTCON-CT","","","","","","","","",""]
["C3-150163","Remove the redundant references","ZTE","Mathieu Mangion",27904,"pCR","","","Remove the redundant references","185","13.1","CT aspects of User Plane Congestion Management (UPCON) for Building Block I",1630,"Agreed","2015-01-23T11:28:09.800","2015-01-24T06:30:31.437","","","Rel-13","29.217","1.0.0","UPCON-DOTCON-CT","","","","","","","","",""]
["C3-150164","Resolve the editor's notes","ZTE","Mathieu Mangion",27904,"pCR","","","Resolve the editor's notes","185","13.1","CT aspects of User Plane Congestion Management (UPCON) for Building Block I",1640,"Merged","2015-01-23T11:28:09.817","2015-01-24T06:31:32.663","","","Rel-13","29.217","1.0.0","UPCON-DOTCON-CT","","","","","","","","",""]
["C3-150165","Resolve the race conditions related to UE mobility between RCAFs","ZTE","Mathieu Mangion",27904,"pCR","","","Resolve the race conditions related to UE mobility between RCAFs","185","13.1","CT aspects of User Plane Congestion Management (UPCON) for Building Block I",1650,"Revised","2015-01-23T11:28:09.837","2015-01-26T10:45:55.990","","C3-150308","Rel-13","29.217","1.0.0","UPCON-DOTCON-CT","","","","","","","","",""]
["C3-150166","Excluding Usage of a ServiceApplication from IP-CAN sessionTDF session Usage","ZTE, China Telecom, Huawei","Mathieu Mangion",27904,"CR","","","Support excluding Usage of a ServiceApplication from IP-CAN sessionTDF session Usage","190","13.6","CT3 Aspect of Usage Monitoring Control extension",1660,"Revised","2015-01-23T11:28:09.853","2015-01-24T06:31:32.697","","C3-150323","Rel-13","29.212","13.0.0","eUMONC-CT3","1288","","B","-","","","","",""]
["C3-150167","Excluding Usage of a ServiceApplication from IP-CAN sessionTDF session Usage for roaming case","ZTE, China Telecom, Huawei","Mathieu Mangion",27904,"CR","","","Support excluding Usage of a ServiceApplication from IP-CAN sessionTDF session Usage for roaming case","190","13.6","CT3 Aspect of Usage Monitoring Control extension",1670,"Revised","2015-01-23T11:28:09.937","2015-01-24T06:31:32.727","","C3-150324","Rel-13","29.215","13.0.0","eUMONC-CT3","0371","","B","-","","","","",""]
["C3-150168","New WID on Extended Overload Control for PCC based Diameter applications","ZTE","Mathieu Mangion",27904,"WID","","","Propose a new WID Extended Overload Control for PCC based Diameter applications","196","13.10","Rel-13 contributions on other Work Items",1680,"Revised","2015-01-23T11:28:10.013","2015-01-26T07:07:22.470","","C3-150259","Rel-13","","","","","","","","","","","",""]
["C3-150169","Correction of APRI Mapping for Generic Number","Deutsche Telekom, Nokia Networks","Mathieu Mangion",27904,"CR","","","Table 6 contains ambiguous mapping rules for the APRI of the Generic Number Parameter which need to be corrected.","55","9.2","Interworking between IM Subsystem with CS  [IMS-CCR-IWCS]",1690,"Revised","2015-01-23T11:28:10.033","2015-01-23T11:27:00.967","","C3-150215","Rel-9","29.163","9.19.0","IMS-CCR-IWCS","0851","","F","-","","","","",""]
["C3-150170","Correction of APRI Mapping for Generic Number","Deutsche Telekom, Nokia Networks","Mathieu Mangion",27904,"CR","","","Table 6 contains ambiguous mapping rules for the APRI of the Generic Number Parameter which need to be corrected.","55","9.2","Interworking between IM Subsystem with CS  [IMS-CCR-IWCS]",1720,"Revised","2015-01-23T11:28:10.130","2015-01-23T11:27:01.820","","C3-150216","Rel-10","29.163","10.15.0","IMS-CCR-IWCS","0852","","A","-","","","","",""]
["C3-150171","Correction of APRI Mapping for Generic Number","Deutsche Telekom, Nokia Networks","Mathieu Mangion",27904,"CR","","","Table 6 contains ambiguous mapping rules for the APRI of the Generic Number Parameter which need to be corrected.","55","9.2","Interworking between IM Subsystem with CS  [IMS-CCR-IWCS]",2151,"Revised","2015-01-23T11:28:10.220","2015-01-23T11:27:02.707","","C3-150217","Rel-11","29.163","11.12.0","IMS-CCR-IWCS","0853","","A","-","","","","",""]
["C3-150172","Correction of APRI Mapping for Generic Number","Deutsche Telekom, Nokia Networks","Mathieu Mangion",27904,"CR","","","Table 6 contains ambiguous mapping rules for the APRI of the Generic Number Parameter which need to be corrected.","55","9.2","Interworking between IM Subsystem with CS  [IMS-CCR-IWCS]",2170,"Revised","2015-01-23T11:28:10.317","2015-01-23T11:27:03.560","","C3-150218","Rel-12","29.163","12.6.0","IMS-CCR-IWCS","0854","","A","-","","","","",""]
["C3-150173","Correction of APRI Mapping for Generic Number","Deutsche Telekom, Nokia Networks","Mathieu Mangion",27904,"CR","","","Table 6 contains ambiguous mapping rules for the APRI of the Generic Number Parameter which need to be corrected.","55","9.2","Interworking between IM Subsystem with CS  [IMS-CCR-IWCS]",2181,"Revised","2015-01-23T11:28:10.407","2015-01-23T11:27:04.410","","C3-150219","Rel-13","29.163","13.0.0","IMS-CCR-IWCS","0855","","A","-","","","","",""]
["C3-150174","Adding missing abbreviations","Fujitsu Limited","Mathieu Mangion",27904,"CR","","","This CR is trying to add the missing abbreviations.","194","13.9.1","TEI13 for IMS/CS",1740,"Revised","2015-01-23T11:28:10.500","2015-01-26T09:19:06.557","","C3-150369","Rel-13","29.165","12.6.0","TEI13","0729","","F","-","","","","",""]
["C3-150175","Editorial correction and incorrect implementation of CRs","Alcatel-Lucent Deutschland AG","Mathieu Mangion",27904,"CR","","","CR 0012 rev 2 (C3-144293) and CR 0017 rev 5 (C3-145275) are implemented faulty. The style of the text is corrected to \"normal\" in subclause 4.5.1. The heading title \"Type\" (table 5.4.1.3.1, 3rd column) is re-introduced.","152","12.18.1","Representational State Transfer (REST) reference point between Application Function (AF) and Protocol Converter (PC) [REST_AF_PC]",1750,"Revised","2015-01-23T11:28:10.583","2015-01-23T11:27:06.117","","C3-150342","Rel-12","29.201","12.1.0","REST_AF_PC","0021","","D","-","","","","",""]
["C3-150176","Correction of applicability of P-Charging-Vector header field in NOTIFY method","Fujitsu Limited","Mathieu Mangion",27904,"CR","","","This CR is trying to correct the applicability of P-C-V header field in NOTIFY method.","94","10.27","Dynamic View of Headers in Messages for II-NNI [NNI_DV]",1760,"Withdrawn","2015-01-23T11:28:10.680",null,"","","Rel-10","29.165","10.17.0","NNI_DV","0730","","F","-","","","","",""]
["C3-150177","Correction of applicability of P-Charging-Vector header field in NOTIFY method","Fujitsu Limited","Mathieu Mangion",27904,"CR","","","This CR is trying to correct the applicability of P-C-V header field in NOTIFY method.","94","10.27","Dynamic View of Headers in Messages for II-NNI [NNI_DV]",1770,"Withdrawn","2015-01-23T11:28:10.773",null,"","","Rel-11","29.165","11.12.0","NNI_DV","0731","","A","-","","","","",""]
["C3-150178","Correction of applicability of P-Charging-Vector header field in NOTIFY method","Fujitsu Limited","Mathieu Mangion",27904,"CR","","","This CR is trying to correct the applicability of P-C-V header field in NOTIFY method.","183","12.47","Rel-12 contributions on other Work Items",1780,"Revised","2015-01-23T11:28:10.870","2015-01-26T09:19:06.580","","C3-150365","Rel-12","29.165","12.6.0","NNI_DV","0732","","F","-","","","","",""]
["C3-150179","Double resource reuse support over S9","Ericsson","Mathieu Mangion",27904,"CR","","","A new feature has been introduced over Rx and Gx in order to allow resource sharing in the network based on information received over Rx.\nThis functionality is also applicable in roaming scenarios.","189","13.5","CT aspects of Double Resource Reuse for Multiple Media Sessions",1790,"Revised","2015-01-23T11:28:10.950","2015-01-23T11:27:09.577","","C3-150321","Rel-13","29.215","13.0.0","DRuMS-CT","0372","","B","-","","","","",""]
["C3-150180","Completion of Double Resource Reuse support over Gx","Ericsson","Mathieu Mangion",27904,"CR","","","The editor’s note  “it is FFS how to remove rules from resource sharing” is removed due to the lack of requirements. Applicability of the functionality applies to all accesses.","189","13.5","CT aspects of Double Resource Reuse for Multiple Media Sessions",1800,"Agreed","2015-01-23T11:28:11.043","2015-01-23T11:27:10.427","","","Rel-13","29.212","13.0.0","DRuMS-CT","1289","","B","CP-150127","","","","",""]
["C3-150181","Uniqueness of Sharing Key for resource sharing over Rx","Ericsson","Mathieu Mangion",27904,"CR","","","The CR proposes that the sharing key is unique per media and changes the format of the sharing key.","189","13.5","CT aspects of Double Resource Reuse for Multiple Media Sessions",1810,"Revised","2015-01-23T11:28:11.137","2015-01-23T11:27:11.290","","C3-150322","Rel-13","29.214","13.0.0","DRuMS-CT","0389","","B","-","","","","",""]
["C3-150182","LS on New AVPs and range of transient failure result codes in TS 29.214","Ericsson","Mathieu Mangion",27904,"LS out","","","CT3 informs CT4 about the new AVPs defined in Rel-12 and asks for a new range of transient failure result codes.","140","12.3","Policy Control and Charging [PCC]",1820,"Approved","2015-01-23T11:28:11.227","2015-01-23T11:27:12.233","","C3-150257","Rel-12","","","PCC","","","","",null,"CT4"]
["C3-150183","Reply LS on End-to-end QoS handling of MTSI","Ericsson","Mathieu Mangion",27904,"LS out","","","CT3 provides SA4 with feedback related to TR 26.924.","187","13.3","CT Aspects of End-to-End MTSI Extensions",1830,"Revised","2015-01-23T11:28:11.263","2015-01-23T11:27:12.970","","C3-150320","Rel-13","","","E2EMTSI-CT","","","","","C3-150254","SA4","CT1, CT4, SA2"]
["C3-150184","Charging correlation identifier for the IP-CAN session in Gx","Ericsson","Mathieu Mangion",27904,"CR","","","A new AVP, IP-CAN-Charging-Indicator AVP, is introduced over Gx to indicate when the Access-Network-Charging-Identifier-Gx AVP applies at IP-CAN session level.","141","12.4","PCC aspects of SAE [SAES-St3-PCC]",1840,"Revised","2015-01-23T11:28:11.297","2015-01-23T11:27:13.717","","C3-150337","Rel-12","29.212","12.7.0","SAES-St3-PCC, TEI12","1290","","B","-","","","","",""]
["C3-150185","Charging correlation identifier for the IP-CAN session in Gx","Ericsson","Mathieu Mangion",27904,"CR","","","A new AVP, IP-CAN-Charging-Indicator AVP, is introduced over Gx to indicate when the Access-Network-Charging-Identifier-Gx AVP applies at IP-CAN session level.","141","12.4","PCC aspects of SAE [SAES-St3-PCC]",1850,"Merged","2015-01-23T11:28:11.390","2015-01-23T11:27:15.297","","","Rel-13","29.212","13.0.0","SAES-St3-PCC, TEI12","1291","","A","-","","","","",""]
["C3-150186","Charging correlation identifier for the IP-CAN session in S9","Ericsson","Mathieu Mangion",27904,"CR","","","The IP-CAN-Session-Charging-Indicator AVP is included within the Subsession-Enforcement-Info AVP to provide the charging identifier that corresponds to the PDN connection.","141","12.4","PCC aspects of SAE [SAES-St3-PCC]",1860,"Withdrawn","2015-01-23T11:28:11.493","2015-01-23T11:27:16.877","","","Rel-12","29.215","12.6.0","SAES-St3-PCC, TEI12","0373","","B","-","","","","",""]
["C3-150187","Charging correlation identifier for the IP-CAN session in S9","Ericsson","Mathieu Mangion",27904,"CR","","","The IP-CAN-Session-Charging-Indicator AVP is included within the Subsession-Enforcement-Info AVP to provide the charging identifier that corresponds to the PDN connection.","141","12.4","PCC aspects of SAE [SAES-St3-PCC]",1870,"Withdrawn","2015-01-23T11:28:11.587","2015-01-23T11:27:18.623","","","Rel-13","29.215","13.0.0","SAES-St3-PCC, TEI12","0374","","A","-","","","","",""]
["C3-150188","QoS change of default bearer","Ericsson","Mathieu Mangion",27904,"CR","","","Impacts in the bearer binding functionality are introduced for 3GPP-EPS when the default bearer QoS is being changed by the PCRF.","141","12.4","PCC aspects of SAE [SAES-St3-PCC]",1880,"Revised","2015-01-23T11:28:11.683","2015-01-23T11:27:20.230","","C3-150340","Rel-12","29.212","12.7.0","SAES-St3-PCC, TEI12","1292","","B","-","","","","",""]
["C3-150189","QoS change of default bearer","Ericsson","Mathieu Mangion",27904,"CR","","","Impacts in the bearer binding functionality are introduced for 3GPP-EPS when the default bearer QoS is being changed by the PCRF.","141","12.4","PCC aspects of SAE [SAES-St3-PCC]",1890,"Revised","2015-01-23T11:28:11.777","2015-01-23T11:27:21.873","","C3-150341","Rel-13","29.212","13.0.0","SAES-St3-PCC, TEI12","1293","","A","-","","","","",""]
["C3-150190","Correction about conditions for filter restrictions","Ericsson, Huawei","Mathieu Mangion",27904,"CR","","","The definition of the Filter_Restriction cause code is corrected to remove the restriction that the keyword “assigned” shall not be used.","104","11.5","PCC aspects of SAE [SAES-St3-PCC]",1900,"Revised","2015-01-23T11:28:11.913","2015-01-23T11:27:23.537","","C3-150292","Rel-11","29.212","11.14.0","SAES-St3-PCC","1294","","F","-","","","","",""]
["C3-150191","Correction about conditions for filter restrictions","Ericsson, Huawei","Mathieu Mangion",27904,"CR","","","The definition of the Filter_Restriction cause code is corrected to remove the restriction that the keyword “assigned” shall not be used.","104","11.5","PCC aspects of SAE [SAES-St3-PCC]",1910,"Revised","2015-01-23T11:28:12.037","2015-01-23T11:27:24.377","","C3-150293","Rel-12","29.212","12.7.0","SAES-St3-PCC","1295","","A","-","","","","",""]
["C3-150192","Correction about conditions for filter restrictions","Ericsson, Huawei","Mathieu Mangion",27904,"CR","","","The definition of the Filter_Restriction cause code is corrected to remove the restriction that the keyword “assigned” shall not be used.","104","11.5","PCC aspects of SAE [SAES-St3-PCC]",1920,"Revised","2015-01-23T11:28:12.173","2015-01-23T11:27:25.230","","C3-150294","Rel-13","29.212","13.0.0","SAES-St3-PCC","1296","","A","-","","","","",""]
["C3-150193","LS on New AVPs in TS 29.061","Ericsson","Mathieu Mangion",27904,"LS out","","","CT3 informs CT4 about the new AVPs defined in Rel-12 for TS 29.061 with regards to MBMS reference points.","165","12.31","eMBMS restoration procedures [eMBMS_Rest]",1930,"Approved","2015-01-23T11:28:12.267","2015-01-23T11:27:26.090","","","Rel-12","","","eMBMS_Rest","","","","",null,"CT4"]
["C3-150194","Protocol enhancements to indicate support of device recall and replace by SMS-SC","Ericsson, Huawei","Mathieu Mangion",27904,"CR","","","Resubmission of CR0013 which was agreed in the Dubrovnik meeting April 2014 but never implemented in to the TS.","169","12.35","CT aspects of Small Data and Device Triggering Enhancements [MTCe-SDDTE-CT]",1940,"Agreed","2015-01-23T11:28:12.300","2015-01-23T11:27:26.827","","","Rel-12","29.368","12.3.0","MTCe-SDDTE-CT","0018","","B","CP-150115","","","","",""]
["C3-150195","Removal of UE context procedure","Ericsson","Mathieu Mangion",27904,"pCR","","","Removal of UE context procedure is defined as a separate procedure to cover more scenarios than UE mobility scenario.","185","13.1","CT aspects of User Plane Congestion Management (UPCON) for Building Block I",1950,"Revised","2015-01-23T11:28:12.397","2015-01-23T11:27:27.667","","C3-150316","Rel-13","29.217","1.0.0","UPCON-DOTCON-CT","","","","","","","","",""]
["C3-150196","Conditional and Unconditional reporting restrictions","Ericsson","Mathieu Mangion",27904,"pCR","","","The Conditional and Unconditional reporting restrictions functionality is corrected. Also the use of AVPs related to reporting restrictions is detailed.","185","13.1","CT aspects of User Plane Congestion Management (UPCON) for Building Block I",1960,"Revised","2015-01-23T11:28:12.427","2015-01-23T11:27:28.517","","C3-150317","Rel-13","29.217","1.0.0","UPCON-DOTCON-CT","","","","","","","","",""]
["C3-150197","UE context removal in IP-CAN session termination procedure","Ericsson","Mathieu Mangion",27904,"CR","","","IP-CAN session termination subclauses are updated to cover Removal of UE context procedure over Np reference point.","185","13.1","CT aspects of User Plane Congestion Management (UPCON) for Building Block I",1970,"Revised","2015-01-23T11:28:12.460","2015-01-23T11:27:29.380","","C3-150318","Rel-13","29.213","13.0.0","UPCON-DOTCON-CT","0596","","B","-","","","","",""]
["C3-150198","Enable MB2 procedures authorization","Ericsson","Mathieu Mangion",27904,"CR","","","The GCS-Identifier AVP is re-used from TS29.214 to host the GCS AS identity to be used by the BM-SC for authorization.","176","12.42","CT aspects of Group Communication System Enablers for LTE [GCSE_LTE-CT]",1980,"Postponed","2015-01-23T11:28:12.557","2015-01-23T11:27:30.310","","","Rel-12","29.468","12.1.0","GCSE_LTE-CT","0011","","F","-","","","","",""]
["C3-150199","Discussion of  Called-Station-Id","China Mobile Com. Corporation","Mathieu Mangion",27904,"other","","","Discuss weather the full APN-FQDN or only the APN  NI shall be included in the Gx interface.","76","10.3","PCC aspects of SAE [SAES-St3-PCC]",1990,"Postponed","2015-01-23T11:28:12.650","2015-01-26T09:57:14.937","","","Rel-10","29.212","10.16.0","SAES-St3-PCC","","","","","","","","",""]
["C3-150200","Clarification of the Called-Station-Id","China Mobile Com. Corporation","Mathieu Mangion",27904,"CR","","","Clarify that only the APN  NI shall be included in the Gx interface.","76","10.3","PCC aspects of SAE [SAES-St3-PCC]",2000,"Postponed","2015-01-23T11:28:12.670","2015-01-26T09:57:14.960","","","Rel-10","29.212","10.16.0","SAES-St3-PCC","1297","","F","-","","","","",""]
["C3-150201","Clarification of the Called-Station-Id","China Mobile Com. Corporation","Mathieu Mangion",27904,"CR","","","Clarify that only the APN  NI shall be included in the Gx interface.","76","10.3","PCC aspects of SAE [SAES-St3-PCC]",2010,"Postponed","2015-01-23T11:28:12.750","2015-01-26T09:57:14.980","","","Rel-11","29.212","11.14.0","SAES-St3-PCC","1298","","A","-","","","","",""]
["C3-150202","Clarification of the Called-Station-Id","China Mobile Com. Corporation","Mathieu Mangion",27904,"CR","","","Clarify that only the APN  NI shall be included in the Gx interface.","76","10.3","PCC aspects of SAE [SAES-St3-PCC]",2020,"Postponed","2015-01-23T11:28:12.830","2015-01-26T09:57:15.003","","","Rel-12","29.212","12.7.0","SAES-St3-PCC","1299","","A","-","","","","",""]
["C3-150203","Clarification of the Called-Station-Id","China Mobile Com. Corporation","Mathieu Mangion",27904,"CR","","","Clarify that only the APN NI shall be included in the Called-Station-Id","197","13.11","PCC aspects of SAE [SAES-St3-PCC]",2030,"Revised","2015-01-23T11:28:12.913",null,"","C3-150241","Rel-13","29.214","13.0.0","","0390","","A","-","","","","",""]
["C3-150204","AF session termination","Huawei","Mathieu Mangion",27904,"CR","","","Remove the incorrect description of IP-CAN session termination.","152","12.18.1","Representational State Transfer (REST) reference point between Application Function (AF) and Protocol Converter (PC) [REST_AF_PC]",2040,"Agreed","2015-01-23T11:28:12.997","2015-01-26T01:02:17.603","","","Rel-12","29.201","12.1.0","REST_AF_PC","0022","","F","CP-150110","","","","",""]
["C3-150205","Provisioning of Access Network Charging Identifier","Huawei","Mathieu Mangion",27904,"CR","","","Add the description of the indication in PCEF general part.","141","12.4","PCC aspects of SAE [SAES-St3-PCC]",2050,"Merged","2015-01-23T11:28:13.097","2015-01-26T01:02:17.623","","","Rel-12","29.212","12.7.0","SAES-St3-PCC","1300","","F","-","","","","",""]
["C3-150206","Provisioning of Access Network Charging Identifier","Huawei","Mathieu Mangion",27904,"CR","","","Add the description of the indication in PCEF general part.","141","12.4","PCC aspects of SAE [SAES-St3-PCC]",2060,"Revised","2015-01-23T11:28:13.177","2015-01-26T01:02:17.643","","C3-150338","Rel-13","29.212","13.0.0","SAES-St3-PCC","1301","","A","-","","","","",""]
["C3-150207","Correction of TFT handling on default bearer","Huawei","Mathieu Mangion",27904,"CR","","","The description about the PCRF shall add an uplink service data flow filter to the resulting PCC rule that effectively disallows any useful packet flows in uplink direction for PCC rules with service data flow filters for the downlink direction only are r","104","11.5","PCC aspects of SAE [SAES-St3-PCC]",2070,"Revised","2015-01-23T11:28:13.273","2015-01-26T01:02:17.663","","C3-150295","Rel-11","29.212","11.14.0","SAES-St3-PCC","1302","","F","-","","","","",""]
["C3-150208","Correction of TFT handling on default bearer","Huawei","Mathieu Mangion",27904,"CR","","","The description about the PCRF shall add an uplink service data flow filter to the resulting PCC rule that effectively disallows any useful packet flows in uplink direction for PCC rules with service data flow filters for the downlink direction only are r","104","11.5","PCC aspects of SAE [SAES-St3-PCC]",2080,"Revised","2015-01-23T11:28:13.420","2015-01-26T01:02:17.683","","C3-150296","Rel-12","29.212","12.7.0","SAES-St3-PCC","1303","","A","-","","","","",""]
["C3-150209","Correction of TFT handling on default bearer","Huawei","Mathieu Mangion",27904,"CR","","","The description about the PCRF shall add an uplink service data flow filter to the resulting PCC rule that effectively disallows any useful packet flows in uplink direction for PCC rules with service data flow filters for the downlink direction only are r","104","11.5","PCC aspects of SAE [SAES-St3-PCC]",2090,"Revised","2015-01-23T11:28:13.543","2015-01-26T01:02:17.707","","C3-150297","Rel-13","29.212","13.0.0","SAES-St3-PCC","1304","","A","-","","","","",""]
["C3-150210","TMGI and Flow ID Handling","Huawei, Nokia Networks","Mathieu Mangion",27904,"CR","","","Definitions for MBMS bearer service and MBMS bearer are provided and Notes clarifying differences to TS 23.246 are added.","176","12.42","CT aspects of Group Communication System Enablers for LTE [GCSE_LTE-CT]",2103,"Revised","2015-01-23T11:28:13.633","2015-01-26T01:02:17.723","","C3-150354","Rel-12","29.468","12.1.0","GCSE_LTE-CT","0012","","F","-","","","","",""]
["C3-150211","Calendar of forthcoming CT3 meetings","MCC","Mathieu Mangion",27904,"other","","","This document lists the future CT3 meetings.","204","15.4","Calendar",2110,"Noted","2015-01-23T11:28:13.717","2015-01-23T12:44:18.767","","","","","","","","","","","","","","",""]
["C3-150212","TWAN release cause for REST-Rx interface","Alcatel-Lucent, Alcatel-Lucent Shanghai Bell, Huawei","Mathieu Mangion",27904,"CR","","","The TWAN release cause reporting is introduced by the CRs 23.402 # 1329 and 23.203 #0963. As a consequence the reporting is introduced on the Diameter based Rx interface as well. This CR introduces the TWAN release cause on the REST-Rx interface.","195","13.9.2","TEI13 for Packet Core",2120,"Withdrawn","2015-01-23T11:28:13.737","2015-01-23T12:26:44.683","","","Rel-13","29.201","12.1.0","NWK-PL2IMS-CT, TEI13","0023","","B","-","","","","",""]
["C3-150213","WORK PLAN- 3GPP Work Plan extract for CT3","MCC","Mathieu Mangion",27904,"WI status report","","","This file is an extract of the 3GPP work plan, filtered by CT3 WIDs.","201","15.1","Work Plan Review",2130,"Noted","2015-01-23T11:28:13.827","2015-01-23T12:43:43.197","","","","","","","","","","","","","","",""]
["C3-150214","QoS mapping for RS and RR","ZTE Corporation","Mathieu Mangion",27904,"CR","","","RR-Bandwidth and RS-Bandwidth shall not be provided when the RS and RR values are set to 0.","195","13.9.2","TEI13 for Packet Core",2140,"Revised","2015-01-23T11:28:13.850","2015-01-24T06:31:32.757","","C3-150336","Rel-13","29.213","13.0.0","TEI13","0597","","B","-","","","","",""]
["C3-150215","Correction of APRI Mapping for Generic Number","Deutsche Telekom, Nokia Networks, Orange","Mathieu Mangion",27904,"CR","","","Table 6 contains ambiguous mapping rules for the APRI of the Generic Number Parameter which need to be corrected.","55","9.2","Interworking between IM Subsystem with CS  [IMS-CCR-IWCS]",1700,"Revised","2015-01-23T11:28:13.933","2015-01-23T11:27:42.427","C3-150169","C3-150276","Rel-9","29.163","9.19.0","IMS-CCR-IWCS","0851","1","F","-","","","","",""]
["C3-150216","Correction of APRI Mapping for Generic Number","Deutsche Telekom, Nokia Networks, Orange","Mathieu Mangion",27904,"CR","","","Table 6 contains ambiguous mapping rules for the APRI of the Generic Number Parameter which need to be corrected.","55","9.2","Interworking between IM Subsystem with CS  [IMS-CCR-IWCS]",1730,"Revised","2015-01-23T11:28:14.030","2015-01-23T11:27:43.310","C3-150170","C3-150277","Rel-10","29.163","10.15.0","IMS-CCR-IWCS","0852","1","A","-","","","","",""]
["C3-150217","Correction of APRI Mapping for Generic Number","Deutsche Telekom, Nokia Networks, Orange","Mathieu Mangion",27904,"CR","","","Table 6 contains ambiguous mapping rules for the APRI of the Generic Number Parameter which need to be corrected.","55","9.2","Interworking between IM Subsystem with CS  [IMS-CCR-IWCS]",2160,"Revised","2015-01-23T11:28:14.127","2015-01-23T11:27:44.167","C3-150171","C3-150278","Rel-11","29.163","11.12.0","IMS-CCR-IWCS","0853","1","A","-","","","","",""]
["C3-150218","Correction of APRI Mapping for Generic Number","Deutsche Telekom, Nokia Networks, Orange","Mathieu Mangion",27904,"CR","","","Table 6 contains ambiguous mapping rules for the APRI of the Generic Number Parameter which need to be corrected.","55","9.2","Interworking between IM Subsystem with CS  [IMS-CCR-IWCS]",2171,"Revised","2015-01-23T11:28:14.223","2015-01-23T11:27:45.013","C3-150172","C3-150279","Rel-12","29.163","12.6.0","IMS-CCR-IWCS","0854","1","A","-","","","","",""]
["C3-150219","Correction of APRI Mapping for Generic Number","Deutsche Telekom, Nokia Networks, Orange","Mathieu Mangion",27904,"CR","","","Table 6 contains ambiguous mapping rules for the APRI of the Generic Number Parameter which need to be corrected.","55","9.2","Interworking between IM Subsystem with CS  [IMS-CCR-IWCS]",2190,"Revised","2015-01-23T11:28:14.323","2015-01-23T11:27:45.877","C3-150173","C3-150280","Rel-13","29.163","13.0.0","IMS-CCR-IWCS","0855","1","A","-","","","","",""]
["C3-150220","Reference update for UUSIW","Alcatel-Lucent , Alcatel-Lucent Shanghai Bell","Mathieu Mangion",27904,"CR","","","draft-ietf-cuss-sip-uui has now been published as RFC 7433.\ndraft-ietf-cuss-sip-uui-isdn has now been published as RFC 7434.\nThere have been no technical changes in the publication process of either document, i.e. since the current referenced version.","37","8.18","Interworking between User-to-User Signaling (UUS) and SIP [UUSIW]",2200,"Revised","2015-01-23T13:11:28.233","2015-01-23T15:05:42.943","","C3-150266","Rel-8","29.163","8.25.0","UUSIW","0856","","F","-","","","","",""]
["C3-150221","Reference update for UUSIW","Alcatel-Lucent, Alcatel-Lucent Shanghai Bell","Mathieu Mangion",27904,"CR","","","draft-ietf-cuss-sip-uui has now been published as RFC 7433.\ndraft-ietf-cuss-sip-uui-isdn has now been published as RFC 7434.\nThere have been no technical changes in the publication process of either document, i.e. since the current referenced version.","37","8.18","Interworking between User-to-User Signaling (UUS) and SIP [UUSIW]",2210,"Revised","2015-01-23T13:17:23.407","2015-01-23T15:05:42.963","","C3-150267","Rel-9","29.163","9.19.0","UUSIW","0857","","A","-","","","","",""]
["C3-150222","Reference update for UUSIW","Alcatel-Lucent, Alcatel-Lucent Shanghai Bell","Mathieu Mangion",27904,"CR","","","draft-ietf-cuss-sip-uui has now been published as RFC 7433.\ndraft-ietf-cuss-sip-uui-isdn has now been published as RFC 7434.\nThere have been no technical changes in the publication process of either document, i.e. since the current referenced version.","37","8.18","Interworking between User-to-User Signaling (UUS) and SIP [UUSIW]",2220,"Revised","2015-01-23T13:20:51.977","2015-01-23T15:05:43.003","","C3-150268","Rel-10","29.163","10.15.0","UUSIW","0858","","A","-","","","","",""]
["C3-150223","Reference update for UUSIW","Alcatel-Lucent, Alcatel-Lucent Shanghai Bell","Mathieu Mangion",27904,"CR","","","draft-ietf-cuss-sip-uui has now been published as RFC 7433.\ndraft-ietf-cuss-sip-uui-isdn has now been published as RFC 7434.\nThere have been no technical changes in the publication process of either document, i.e. since the current referenced version.","37","8.18","Interworking between User-to-User Signaling (UUS) and SIP [UUSIW]",2230,"Revised","2015-01-23T13:24:25.157","2015-01-23T15:05:42.803","","C3-150269","Rel-11","29.163","11.12.0","UUSIW","0859","","A","-","","","","",""]
["C3-150224","Reference update for UUSIW","Alcatel-Lucent, Alcatel-Lucent Shanghai Bell","Mathieu Mangion",27904,"CR","","","draft-ietf-cuss-sip-uui has now been published as RFC 7433.\ndraft-ietf-cuss-sip-uui-isdn has now been published as RFC 7434.\nThere have been no technical changes in the publication process of either document, i.e. since the current referenced version.","37","8.18","Interworking between User-to-User Signaling (UUS) and SIP [UUSIW]",2240,"Revised","2015-01-23T13:27:32.123","2015-01-23T15:05:42.827","","C3-150270","Rel-12","29.163","12.6.0","UUSIW","0860","","A","-","","","","",""]
["C3-150225","Reference update for UUSIW","Alcatel-Lucent, ALcatel-Lucent Shanghai Bell","Mathieu Mangion",27904,"CR","","","draft-ietf-cuss-sip-uui has now been published as RFC 7433.\ndraft-ietf-cuss-sip-uui-isdn has now been published as RFC 7434.\nThere have been no technical changes in the publication process of either document, i.e. since the current referenced version.","37","8.18","Interworking between User-to-User Signaling (UUS) and SIP [UUSIW]",2250,"Revised","2015-01-23T13:31:01.147","2015-01-23T15:05:42.847","","C3-150271","Rel-13","29.163","13.0.0","UUSIW","0861","","A","-","","","","",""]
["C3-150226","Reference update for UUSIW","Alcatel-Lucent, Alcatel-Lucent Shanghai Bell","Mathieu Mangion",27904,"CR","","","draft-ietf-cuss-sip-uui has now been published as RFC 7433.\ndraft-ietf-cuss-sip-uui-isdn has now been published as RFC 7434.\nThere have been no technical changes in the publication process of either document, i.e. since the current referenced version.","65","9.19","Operational Description of the Inter-IMS NNI   [II-NNI]",2260,"Revised","2015-01-23T14:47:56.830","2015-01-23T15:05:42.863","","C3-150272","Rel-9","29.165","9.19.0","UUSIW, II-NNI","0733","","F","-","","","","",""]
["C3-150227","Reference update for UUSIW","Alcatel-Lucent, Alcatel-Lucent Shanghai Bell","Mathieu Mangion",27904,"CR","","","draft-ietf-cuss-sip-uui has now been published as RFC 7433.\ndraft-ietf-cuss-sip-uui-isdn has now been published as RFC 7434.\nThere have been no technical changes in the publication process of either document, i.e. since the current referenced version.","65","9.19","Operational Description of the Inter-IMS NNI   [II-NNI]",2270,"Revised","2015-01-23T14:52:22.810","2015-01-23T15:05:42.883","","C3-150273","Rel-10","29.165","10.17.0","UUSIW, II-NNI","0734","","A","-","","","","",""]
["C3-150228","Reference update for UUSIW","Alcatel-Lucent, Alcatel-Lucent Shanghai Bell","Mathieu Mangion",27904,"CR","","","draft-ietf-cuss-sip-uui has now been published as RFC 7433.\ndraft-ietf-cuss-sip-uui-isdn has now been published as RFC 7434.\nThere have been no technical changes in the publication process of either document, i.e. since the current referenced version.","65","9.19","Operational Description of the Inter-IMS NNI   [II-NNI]",2280,"Revised","2015-01-23T14:57:45.963","2015-01-23T15:05:42.903","","C3-150274","Rel-11","29.165","11.12.0","UUSIW, II-NNI","0735","","A","-","","","","",""]
["C3-150229","Reference update for UUSIW","Alcatel-Lucent, Alcatel-Lucent Shanghai Bell","Mathieu Mangion",27904,"CR","","","draft-ietf-cuss-sip-uui has now been published as RFC 7433.\ndraft-ietf-cuss-sip-uui-isdn has now been published as RFC 7434.\nThere have been no technical changes in the publication process of either document, i.e. since the current referenced version.","65","9.19","Operational Description of the Inter-IMS NNI   [II-NNI]",2290,"Revised","2015-01-23T15:02:22.457","2015-01-23T15:05:42.923","","C3-150275","Rel-12","29.165","12.6.0","UUSIW, II-NNI","0736","","A","-","","","","",""]
["C3-150230","Correction to the session establishment and notification URIs","Oracle Corporation","Mathieu Mangion",27904,"CR","","","The session establishment URI should not contain the word \"establishment\" as the POST method already implies creation of the resource. \nThe notification URI needs to contain the afsessionid, otherwise the AF will not be able to correlate the notification","152","12.18.1","Representational State Transfer (REST) reference point between Application Function (AF) and Protocol Converter (PC) [REST_AF_PC]",2300,"Revised","2015-01-24T21:32:49.473","2015-01-25T23:48:25.117","","C3-150343","Rel-12","29.201","12.1.0","REST_AF_PC","0024","","F","-","","","","",""]
["C3-150231","Allowing for forward compatibility and miscellaneous corrections","Oracle Corporation","Mathieu Mangion",27904,"CR","","","The XML schema for both the complex types and messages do not allow for future extension. The schema needs to be updated to allow such extensions.\nAlso, some of the XML element names are too long or too brief to understand.","152","12.18.1","Representational State Transfer (REST) reference point between Application Function (AF) and Protocol Converter (PC) [REST_AF_PC]",2310,"Revised","2015-01-24T21:52:46.113","2015-01-25T23:48:25.220","","C3-150344","Rel-12","29.201","12.1.0","REST_AF_PC","0025","","F","-","","","","",""]
["C3-150232","Corrections in the definition of MBMS Service Area AVP","Motorola Solutions Danmark A/S","Mathieu Mangion",27904,"CR","","","This CR aligns the wording for the definition of MBMS-Service-Area AVP with the definition in the stage 2 document 23.003.","176","12.42","CT aspects of Group Communication System Enablers for LTE [GCSE_LTE-CT]",2321,"Revised","2015-01-25T13:48:14.007","2015-01-26T10:06:17.250","","C3-150355","Rel-12","29.061","12.8.0","GCSE_LTE-CT","0445","","F","-","","","","",""]
["C3-150233","The inclusion of Flow Identifier in the MBMS Bearer activation request","Motorola Solutions Danmark A/S","Mathieu Mangion",27904,"CR","","","This CR implements the Stage-2 decision according to which the GCS AS may indicate a Flow Identifier when asking to activate an MBMS bearer.","176","12.42","CT aspects of Group Communication System Enablers for LTE [GCSE_LTE-CT]",2331,"Revised","2015-01-25T13:53:36.710","2015-01-26T10:06:44.147","","C3-150250","Rel-12","29.468","12.0.1","GCSE_LTE-CT","0013","","C","-","","","","",""]
["C3-150234","Opptional MBMS Session Identity","Motorola Solutions Danmark A/S","Mathieu Mangion",27904,"CR","","","This CR adds the possibility for a GSC AS to add optionally a session ID when activation an MBMS bearer as it is stated in the Stage-2 document 23.246.","176","12.42","CT aspects of Group Communication System Enablers for LTE [GCSE_LTE-CT]",2342,"Revised","2015-01-25T13:56:42.777","2015-01-26T10:07:04.717","","C3-150251","Rel-12","29.468","12.0.1","GCSE_LTE-CT","0014","","F","-","","","","",""]
["C3-150235","Enabling the AF for defining the ToS-Traffic-Class AVP","Motorola Solutions Danmark A/S","Mathieu Mangion",27904,"other","","","This contribution introduces the need for enabling the AF to define the value of ToS-Traffic-Class AVP over the Rx interface.","182","12.46.2","TEI12 for Packet Core",2350,"Noted","2015-01-25T14:11:16.933","2015-01-26T10:07:28.027","","","Rel-12","","","TEI12","","","","","","","","",""]
["C3-150236","Add the ToS-Traffic-Class AVP to the message sent by AF over Rx","Motorola Solutions Danmark A/S","Mathieu Mangion",27904,"CR","","","This CR is mentions that, during session establishment an AF may also indicate the ToS-Traffic-Class AVP.","182","12.46.2","TEI12 for Packet Core",2355,"Withdrawn","2015-01-25T14:18:18.197","2015-01-26T14:27:07.600","","","Rel-12","29.213","12.6.0","TEI12","0598","","F","-","","","","",""]
["C3-150237","Add the ToS-Traffic-Class AVP to the Rx to be sent by AF","Motorola Solutions Danmark A/S","Mathieu Mangion",27904,"CR","","","This CR indicates how the ToS-Traffic-Class AVP is optionally used by an AF in the Rx interface.","182","12.46.2","TEI12 for Packet Core",2360,"Withdrawn","2015-01-25T14:22:29.783","2015-01-26T14:27:24.357","","","Rel-12","29.214","12.6.0","TEI12","0391","","F","-","","","","",""]
["C3-150238","Enable the ToS-Traffic-Class AVP to be provided by AF","Motorola Solutions Danmark A/S","Mathieu Mangion",27904,"CR","","","This CR indicates how a value of ToS-Traffic-Class AVP received from the AF via RX interface, is reflected to the Gx interface.","182","12.46.2","TEI12 for Packet Core",2370,"Withdrawn","2015-01-25T14:25:22.483","2015-01-26T14:27:38.040","","","Rel-12","29.212","12.7.0","TEI12","1305","","F","-","","","","",""]
["C3-150239","Location information in case of non-3GPP access","Alcatel-Lucent","Mathieu Mangion",27904,"CR","","","TS 29.214 does not mention the non-3GPP accesses in the definition of the 3GPP-SGSN-MCC-MNC AVP as it is already done in TS 29.212, which states: For 3GPP/non-3GPP accesses the MCC and MNC provided by the serving gateway (SGW, or AGW or TWAG). The definit","182","12.46.2","TEI12 for Packet Core",2390,"Revised","2015-01-26T07:23:46.057","2015-01-26T07:47:16.093","","C3-150361","Rel-12","29.214","12.6.0","TEI12","0392","","F","-","","","","",""]
["C3-150240","Clarification of the Called-Station-Id","China Mobile Com. Corporation, Huawei","Mathieu Mangion",27904,"CR","","","Clarify that only the APN  NI shall be included in the Gx interface.","76","10.3","PCC aspects of SAE [SAES-St3-PCC]",2400,"Postponed","2015-01-26T07:23:54.697","2015-01-26T09:57:15.027","","","Rel-13","29.212","13.0.0","SAES-St3-PCC","1306","","A","-","","","","",""]
["C3-150241","Clarification of the Called-Station-Id","China Mobile Com. Corporation","Mathieu Mangion",27904,"CR","","","Clarify that only the APN NI shall be included in the Called-Station-Id","197","13.11","PCC aspects of SAE [SAES-St3-PCC]",2410,"Postponed","2015-01-26T07:28:28.473","2015-01-26T09:57:15.047","C3-150203","","Rel-13","29.214","13.0.0","SAES-St3-PCC","0390","1","F","-","","","","",""]
["C3-150242","Location information in case of non-3GPP access","Alcatel-Lucent","Mathieu Mangion",27904,"CR","","","TS 29.214 does not mention the non-3GPP accesses in the definition of the 3GPP-SGSN-MCC-MNC AVP as it is already done in TS 29.212, which states: For 3GPP/non-3GPP accesses the MCC and MNC provided by the serving gateway (SGW, or AGW or TWAG). The definit","182","12.46.2","TEI12 for Packet Core",2420,"Revised","2015-01-26T07:30:20.713","2015-01-26T07:47:16.120","","C3-150362","Rel-13","29.214","13.0.0","TEI12","0393","","A","-","","","","",""]
["C3-150243","Clarification of the Called-Station-Id","China Mobile Com. Corporation, Huawei","Mathieu Mangion",27904,"CR","","","Clarify that only the APN NI shall be included in the Called-Station-Id","197","13.11","PCC aspects of SAE [SAES-St3-PCC]",2430,"Postponed","2015-01-26T07:34:00.847","2015-01-26T09:57:15.067","","","Rel-13","29.215","13.0.0","SAES-St3-PCC","0375","","F","-","","","","",""]
["C3-150244","Correction of EVS reference bumber","Nokia Networks","Mathieu Mangion",27904,"CR Pack","","","Reference number of reference to TS 26.445 is corrected","179","12.45","CT Impacts of Codec for Enhanced Voice Services [EVS_codec-CT]",2440,"Withdrawn","2015-01-26T12:03:44.777","2015-02-10T16:25:25.297","","","Rel-12","29.163","12.6.0","","","","","","","","","",""]
["C3-150245","Correction of EVS related reference number","Nokia Networks","Mathieu Mangion",27904,"CR","","","Reference number for TS 26.445 is corrected.","179","12.45","CT Impacts of Codec for Enhanced Voice Services [EVS_codec-CT]",2450,"Agreed","2015-01-26T12:09:08.430","2015-01-26T12:56:23.427","","","Rel-12","29.163","12.6.0","EVS_codec-CT","0862","","F","CP-150121","","","","",""]
["C3-150246","Correction of EVS related reference number","Nokia Networks","Mathieu Mangion",27904,"CR","","","Reference Number to TS 26.445 is corrected","179","12.45","CT Impacts of Codec for Enhanced Voice Services [EVS_codec-CT]",2460,"Withdrawn","2015-01-26T12:12:36.857",null,"","","Rel-13","29.163","13.0.0","","0863","","A","-","","","","",""]
["C3-150247","Adding support for EVS codec","Nokia Networks","Mathieu Mangion",27904,"CR","","","The Rel-12 CR has been agreed at CT3#79, but MCC failed to include the contents into the REl-13 version of TS 29.163 created after the meeting","179","12.45","CT Impacts of Codec for Enhanced Voice Services [EVS_codec-CT]",2470,"Revised","2015-01-26T13:00:53.687","2015-01-26T13:15:07.690","","C3-150339","Rel-13","29.163","13.0.0","EVS_codec-CT","0864","","B","-","","","","",""]
["C3-150248","Note 4 in Table 3 for mapping to CLI parameter","Nokia Networks","Mathieu Mangion",27904,"CR","","","CR 0832 has been agreed for Rel-12 at CT3#79. MCC created a Rel-13 version of TS 29.163 after the meeting, but forgot to include the agreed CR","181","12.46.1","TEI12 for IMS/CS",2480,"Withdrawn","2015-01-26T13:20:55.407","2015-01-26T13:27:15.220","","","Rel-13","29.163","13.0.0","TEI12","0865","","F","-","","","","",""]
["C3-150249","Appearance of Redirection Number Restriction parameter","Nokia Networks","Mathieu Mangion",27904,"CR","","","CR 0833 has been agreed for Rel-12 at CT3#79. MCC created a Rel-13 version of TS 29.163 after the meeting, but forgot to include the agreed CR.","181","12.46.1","TEI12 for IMS/CS",2490,"Withdrawn","2015-01-26T13:50:53.283","2015-01-26T13:56:44.943","","","Rel-13","29.163","13.0.0","TEI12","0866","","F","-","","","","",""]
["C3-150250","The inclusion of Flow Identifier in the MBMS Bearer activation request","Motorola Solutions Danmark A/S","Mathieu Mangion",27904,"CR","","","This CR implements the Stage-2 decision according to which the GCS AS may indicate a Flow Identifier when asking to activate an MBMS bearer.","176","12.42","CT aspects of Group Communication System Enablers for LTE [GCSE_LTE-CT]",2331,"Revised","2015-02-10T16:30:51.837","2015-02-10T16:25:29.020","C3-150233","C3-150356","Rel-12","29.468","12.1.0","GCSE_LTE-CT","0013","1","C","-","","","","",""]
["C3-150251","Opptional MBMS Session Identity","Motorola Solutions Danmark A/S","Mathieu Mangion",27904,"CR","","","This CR adds the possibility for a GSC AS to add optionally a session ID when activation an MBMS bearer as it is stated in the Stage-2 document 23.246.","176","12.42","CT aspects of Group Communication System Enablers for LTE [GCSE_LTE-CT]",2342,"Revised","2015-02-10T16:30:52.020","2015-02-10T16:25:29.987","C3-150234","C3-150357","Rel-12","29.468","12.1.0","GCSE_LTE-CT","0014","1","F","-","","","","",""]
["C3-150252","LS related to Mobile VoIP IMS Roaming","SA3-LI","Mathieu Mangion",27904,"LS in","","","SA3-LI would like to highlight that the IMS/LTE Roaming Architecture could have a significant impact on operators’ abilities to meet LI obligations. SA3-LI kindly requests CT3 to provide SA3-LI with details of Roaming Architecture models. Home routed scen","13","6","Received Liaison Statements",25200,"Noted","2015-02-10T16:30:52.150","2015-02-10T16:25:30.827","","","Rel-12","","","","","","","",null,null,null,"S3i150073","C3-150256"]
["C3-150253","Reply LS on TLS and DTLS terminology","SA3","Mathieu Mangion",27904,"LS in","","","This LS provides answers to ITU-T Q3/16 for the questions in LS on TLS and DTLS terminology.","13","6","Received Liaison Statements",25300,"Noted","2015-02-10T16:30:52.207","2015-02-10T16:25:30.830","","","","","","","","","","",null,null,null,"S3-151138"]
["C3-150254","LS on TR 26.924 Study on improved end-to-end QoS handling","SA4","Mathieu Mangion",27904,"LS in","","","SA4 has progressed the study on improved end-to-end QoS handling and have updated draft TR 26.924. The latest updated version of TR 26.924 (v0.1.7) is attached.","13","6","Received Liaison Statements",25400,"Noted","2015-02-10T16:30:52.260","2015-02-10T16:25:30.833","","","Rel-13","","","QOSE2EMTSI","","","","",null,null,null,"S4-150163","C3-150450"]
["C3-150255","LS on CT Impacts of the ROI WI","SA4","Mathieu Mangion",27904,"LS in","","","The Release 13 work item on “Video Enhancements by Region-of-Interest Information Signaling” (ROI) (WID attached) is progressing at SA4 with a finalized set of requirements and several potential solutions, all documented in the attached permanent document","13","6","Received Liaison Statements",25500,"Postponed","2015-02-10T16:30:52.313","2015-02-10T16:25:31.600","","","Rel-13","","","ROI","","","","",null,null,null,"S4-150250"]
["C3-150256","Reply to: LS related to Mobile VoIP IMS Roaming","Orange","Mathieu Mangion",27904,"LS out","","","","13","6","Received Liaison Statements",25201,"Approved","2015-02-10T16:30:52.363","2015-02-10T16:25:32.350","","","Rel-12","","","","","","","","C3-150252","SA WG3-LI, SA2","CT1, CT4"]
["C3-150257","LS on New AVPs and range of transient failure result codes in TS 29.214","Ericsson","Mathieu Mangion",27904,"LS out","","","CT3 asks CT4 to kindly update TS 29.230 with the new defined AVP in TS 29.214 for Rel-12. CT3 also asks CT4 to kindly assign a new range of 3GPP specific Transient Failure result codes for the same specification for Rel-13 and include the already defined","140","12.3","Policy Control and Charging [PCC]",1821,"Withdrawn","2015-02-10T16:30:52.417","2015-02-10T16:25:32.367","C3-150182","","","","","PCC","","","","",null,"CT4"]
["C3-150258","New WID on CT aspects of EVS in 3G Circuit-Switched Networks","Qualcomm Incorporated","Mathieu Mangion",27904,"WID","","","","196","13.10","Rel-13 contributions on other Work Items",1151,"Technically endorsed","2015-02-10T16:30:52.477","2015-02-10T16:25:33.120","C3-150115","","Rel-13","","","","","","","","","","","",""]
["C3-150259","New WID on Extended Overload Control for PCC based Diameter applications","ZTE","Mathieu Mangion",27904,"WID","","","","196","13.10","Rel-13 contributions on other Work Items",1681,"Revised","2015-02-10T16:30:52.550","2015-02-10T16:25:33.137","C3-150168","C3-150402","Rel-13","","","","","","","","","","","",""]
["C3-150260","Incorrect implementation of CRs","MCC","Mathieu Mangion",27904,"CR","","","","183","12.47","Rel-12 contributions on other Work Items",1281,"Agreed","2015-02-10T16:30:52.617","2015-02-10T16:25:33.263","C3-150128","","Rel-12","29.165","12.6.0","TEI12","0722","1","D","CP-150123","","","","",""]
["C3-150261","Bugfix: do not send negative-delivery IMDN after sending SIP 4xx/5xx response","Comverse Network Systems","Mathieu Mangion",27904,"CR","","","","46","8.21","Support of Service-Level Interworking for Messaging Services [MESSIW]",241,"Revised","2015-02-10T16:30:52.753","2015-02-10T16:25:34.237","C3-150024","C3-150374","Rel-8","29.311","8.3.0","MESSIW","0034","1","F","-","","","","",""]
["C3-150262","Bugfix: do not send negative-delivery IMDN after sending SIP 4xx/5xx response","Comverse","Mathieu Mangion",27904,"CR","","","","46","8.21","Support of Service-Level Interworking for Messaging Services [MESSIW]",251,"Revised","2015-02-10T16:30:52.907","2015-02-10T16:25:35.210","C3-150025","C3-150375","Rel-9","29.311","9.2.0","MESSIW","0035","1","A","-","","","","",""]
["C3-150263","Bugfix: do not send negative-delivery IMDN after sending SIP 4xx/5xx response","Comverse","Mathieu Mangion",27904,"CR","","","","46","8.21","Support of Service-Level Interworking for Messaging Services [MESSIW]",261,"Revised","2015-02-10T16:30:53.040","2015-02-10T16:25:36.163","C3-150026","C3-150376","Rel-10","29.311","10.5.0","MESSIW","0036","1","A","-","","","","",""]
["C3-150264","Bugfix: do not send negative-delivery IMDN after sending SIP 4xx/5xx response","Comverse","Mathieu Mangion",27904,"CR","","","","46","8.21","Support of Service-Level Interworking for Messaging Services [MESSIW]",271,"Revised","2015-02-10T16:30:53.173","2015-02-10T16:25:37.153","C3-150027","C3-150377","Rel-11","29.311","11.1.0","MESSIW","0037","1","A","-","","","","",""]
["C3-150265","Bugfix: do not send negative-delivery IMDN after sending SIP 4xx/5xx response","Comverse","Mathieu Mangion",27904,"CR","","","","46","8.21","Support of Service-Level Interworking for Messaging Services [MESSIW]",281,"Revised","2015-02-10T16:30:53.300","2015-02-10T16:25:38.127","C3-150028","C3-150378","Rel-12","29.311","12.0.0","MESSIW","0038","1","A","-","","","","",""]
["C3-150266","Reference update for UUSIW","Alcatel-Lucent , Alcatel-Lucent Shanghai Bell","Mathieu Mangion",27904,"CR","","","","37","8.18","Interworking between User-to-User Signaling (UUS) and SIP [UUSIW]",2201,"Agreed","2015-02-10T16:30:53.430","2015-02-10T16:25:39.117","C3-150220","","Rel-8","29.163","8.25.0","UUSIW","0856","1","F","CP-150095","","","","",""]
["C3-150267","Reference update for UUSIW","Alcatel-Lucent, Alcatel-Lucent Shanghai Bell","Mathieu Mangion",27904,"CR","","","","37","8.18","Interworking between User-to-User Signaling (UUS) and SIP [UUSIW]",2211,"Agreed","2015-02-10T16:30:53.560","2015-02-10T16:25:40.110","C3-150221","","Rel-9","29.163","9.19.0","UUSIW","0857","1","A","CP-150095","","","","",""]
["C3-150268","Reference update for UUSIW","Alcatel-Lucent, Alcatel-Lucent Shanghai Bell","Mathieu Mangion",27904,"CR","","","","37","8.18","Interworking between User-to-User Signaling (UUS) and SIP [UUSIW]",2221,"Agreed","2015-02-10T16:30:53.690","2015-02-10T16:25:41.113","C3-150222","","Rel-10","29.163","10.15.0","UUSIW","0858","1","A","CP-150095","","","","",""]
["C3-150269","Reference update for UUSIW","Alcatel-Lucent, Alcatel-Lucent Shanghai Bell","Mathieu Mangion",27904,"CR","","","","37","8.18","Interworking between User-to-User Signaling (UUS) and SIP [UUSIW]",2231,"Agreed","2015-02-10T16:30:53.823","2015-02-10T16:25:42.177","C3-150223","","Rel-11","29.163","11.12.0","UUSIW","0859","1","A","CP-150095","","","","",""]
["C3-150270","Reference update for UUSIW","Alcatel-Lucent, Alcatel-Lucent Shanghai Bell","Mathieu Mangion",27904,"CR","","","","37","8.18","Interworking between User-to-User Signaling (UUS) and SIP [UUSIW]",2241,"Agreed","2015-02-10T16:30:53.953","2015-02-10T16:25:43.147","C3-150224","","Rel-12","29.163","12.6.0","UUSIW","0860","1","A","CP-150095","","","","",""]
["C3-150271","Reference update for UUSIW","Alcatel-Lucent, ALcatel-Lucent Shanghai Bell","Mathieu Mangion",27904,"CR","","","","37","8.18","Interworking between User-to-User Signaling (UUS) and SIP [UUSIW]",2251,"Agreed","2015-02-10T16:30:54.087","2015-02-10T16:25:44.127","C3-150225","","Rel-13","29.163","13.0.0","UUSIW","0861","1","A","CP-150095","","","","",""]
["C3-150272","Reference update for UUSIW","Alcatel-Lucent, Alcatel-Lucent Shanghai Bell","Mathieu Mangion",27904,"CR","","","","65","9.19","Operational Description of the Inter-IMS NNI   [II-NNI]",2261,"Agreed","2015-02-10T16:30:54.220","2015-02-10T16:25:45.103","C3-150226","","Rel-9","29.165","9.19.0","UUSIW, II-NNI","0733","1","F","CP-150099","","","","",""]
["C3-150273","Reference update for UUSIW","Alcatel-Lucent, Alcatel-Lucent Shanghai Bell","Mathieu Mangion",27904,"CR","","","","65","9.19","Operational Description of the Inter-IMS NNI   [II-NNI]",2271,"Agreed","2015-02-10T16:30:54.350","2015-02-10T16:25:46.840","C3-150227","","Rel-10","29.165","10.17.0","UUSIW, II-NNI","0734","1","A","CP-150099","","","","",""]
["C3-150274","Reference update for UUSIW","Alcatel-Lucent, Alcatel-Lucent Shanghai Bell","Mathieu Mangion",27904,"CR","","","","65","9.19","Operational Description of the Inter-IMS NNI   [II-NNI]",2281,"Agreed","2015-02-10T16:30:54.487","2015-02-10T16:25:48.587","C3-150228","","Rel-11","29.165","11.12.0","UUSIW, II-NNI","0735","1","A","CP-150099","","","","",""]
["C3-150275","Reference update for UUSIW","Alcatel-Lucent, Alcatel-Lucent Shanghai Bell","Mathieu Mangion",27904,"CR","","","","65","9.19","Operational Description of the Inter-IMS NNI   [II-NNI]",2291,"Agreed","2015-02-10T16:30:54.620","2015-02-10T16:25:50.327","C3-150229","","Rel-12","29.165","12.6.0","UUSIW, II-NNI","0736","1","A","CP-150099","","","","",""]
["C3-150276","Correction of APRI Mapping for Generic Number","Deutsche Telekom, Nokia Networks, Orange","Mathieu Mangion",27904,"CR","","","","55","9.2","Interworking between IM Subsystem with CS  [IMS-CCR-IWCS]",1710,"Agreed","2015-02-10T16:30:54.753","2015-02-10T16:25:52.077","C3-150215","","Rel-9","29.163","9.19.0","IMS-CCR-IWCS","0851","2","F","CP-150097","","","","",""]
["C3-150277","Correction of APRI Mapping for Generic Number","Deutsche Telekom, Nokia Networks, Orange","Mathieu Mangion",27904,"CR","","","","55","9.2","Interworking between IM Subsystem with CS  [IMS-CCR-IWCS]",2150,"Agreed","2015-02-10T16:30:54.887","2015-02-10T16:25:53.060","C3-150216","","Rel-10","29.163","10.15.0","IMS-CCR-IWCS","0852","2","A","CP-150097","","","","",""]
["C3-150278","Correction of APRI Mapping for Generic Number","Deutsche Telekom, Nokia Networks, Orange","Mathieu Mangion",27904,"CR","","","","55","9.2","Interworking between IM Subsystem with CS  [IMS-CCR-IWCS]",2161,"Agreed","2015-02-10T16:30:55.020","2015-02-10T16:25:54.077","C3-150217","","Rel-11","29.163","11.12.0","IMS-CCR-IWCS","0853","2","A","CP-150097","","","","",""]
["C3-150279","Correction of APRI Mapping for Generic Number","Deutsche Telekom, Nokia Networks, Orange","Mathieu Mangion",27904,"CR","","","","55","9.2","Interworking between IM Subsystem with CS  [IMS-CCR-IWCS]",2180,"Agreed","2015-02-10T16:30:55.153","2015-02-10T16:25:55.073","C3-150218","","Rel-12","29.163","12.6.0","IMS-CCR-IWCS","0854","2","A","CP-150097","","","","",""]
["C3-150280","Correction of APRI Mapping for Generic Number","Deutsche Telekom, Nokia Networks, Orange","Mathieu Mangion",27904,"CR","","","","55","9.2","Interworking between IM Subsystem with CS  [IMS-CCR-IWCS]",2191,"Agreed","2015-02-10T16:30:55.290","2015-02-10T16:25:56.120","C3-150219","","Rel-13","29.163","13.0.0","IMS-CCR-IWCS","0855","2","A","CP-150097","","","","",""]
["C3-150281","Clarification on the II-NNI requirement for CDIV regarding Privacy header field.","NTT","Mathieu Mangion",27904,"CR","","","","65","9.19","Operational Description of the Inter-IMS NNI   [II-NNI]",301,"Revised","2015-02-10T16:30:55.423","2015-02-10T16:25:57.130","C3-150030","C3-150387","Rel-9","29.165","9.19.0","II-NNI","0709","1","F","-","","","","",""]
["C3-150282","Clarification on the II-NNI requirement for CDIV regarding Privacy header field.","NTT","Mathieu Mangion",27904,"CR","","","","65","9.19","Operational Description of the Inter-IMS NNI   [II-NNI]",311,"Revised","2015-02-10T16:30:55.557","2015-02-10T16:25:58.170","C3-150031","C3-150388","Rel-10","29.165","10.17.0","II-NNI","0710","1","A","-","","","","",""]
["C3-150283","Clarification on the II-NNI requirement for CDIV regarding Privacy header field.","NTT","Mathieu Mangion",27904,"CR","","","","65","9.19","Operational Description of the Inter-IMS NNI   [II-NNI]",321,"Revised","2015-02-10T16:30:55.693","2015-02-10T16:25:59.160","C3-150032","C3-150389","Rel-11","29.165","11.12.0","II-NNI","0711","1","A","-","","","","",""]
["C3-150284","Clarification on the II-NNI requirement for CDIV regarding Privacy header field.","NTT","Mathieu Mangion",27904,"CR","","","","65","9.19","Operational Description of the Inter-IMS NNI   [II-NNI]",331,"Revised","2015-02-10T16:30:55.827","2015-02-10T16:26:00.153","C3-150033","C3-150390","Rel-12","29.165","12.6.0","II-NNI","0712","1","A","-","","","","",""]
["C3-150285","Clarification on the II-NNI requirement regarding cause-param URI parameter.","NTT","Mathieu Mangion",27904,"CR","","","","65","9.19","Operational Description of the Inter-IMS NNI   [II-NNI]",351,"Agreed","2015-02-10T16:30:55.960","2015-02-10T16:26:01.177","C3-150035","","Rel-9","29.165","9.19.0","II-NNI","0714","1","F","CP-150098","","","","",""]
["C3-150286","Clarification on the II-NNI requirement regarding cause-param URI parameter.","NTT","Mathieu Mangion",27904,"CR","","","","65","9.19","Operational Description of the Inter-IMS NNI   [II-NNI]",361,"Agreed","2015-02-10T16:30:56.090","2015-02-10T16:26:02.157","C3-150036","","Rel-10","29.165","10.17.0","II-NNI","0715","1","A","CP-150098","","","","",""]
["C3-150287","Clarification on the II-NNI requirement regarding cause-param URI parameter.","NTT","Mathieu Mangion",27904,"CR","","","","65","9.19","Operational Description of the Inter-IMS NNI   [II-NNI]",371,"Agreed","2015-02-10T16:30:56.223","2015-02-10T16:26:03.143","C3-150037","","Rel-11","29.165","11.12.0","II-NNI","0716","1","A","CP-150098","","","","",""]
["C3-150288","Clarification on the II-NNI requirement regarding cause-param URI parameter.","NTT","Mathieu Mangion",27904,"CR","","","","65","9.19","Operational Description of the Inter-IMS NNI   [II-NNI]",381,"Agreed","2015-02-10T16:30:56.357","2015-02-10T16:26:04.277","C3-150038","","Rel-12","29.165","12.6.0","II-NNI","0717","1","A","CP-150098","","","","",""]
["C3-150289","Procedures for avoiding changes in the OMR algorithm outcome on subsequent SDP offer/answer transactions","Ericsson","Mathieu Mangion",27904,"CR","","","","82","10.17","Optimal Media Routeing [OMR]",1361,"Postponed","2015-02-10T16:30:56.493",null,"C3-150136","","Rel-10","29.079","10.6.0","OMR","0043","1","F","-","","","","",""]
["C3-150290","Procedures for avoiding changes in the OMR algorithm outcome on subsequent SDP offer/answer transactions","Ericsson LM","Mathieu Mangion",27904,"CR","","","","82","10.17","Optimal Media Routeing [OMR]",1371,"Postponed","2015-02-10T16:30:56.627",null,"C3-150137","","Rel-11","29.079","11.5.0","OMR","0044","1","A","-","","","","",""]
["C3-150291","Procedures for avoiding changes in the OMR algorithm outcom on subsequent SDP offer/answer transactions","Ericsson LM","Mathieu Mangion",27904,"CR","","","","82","10.17","Optimal Media Routeing [OMR]",1381,"Postponed","2015-02-10T16:30:56.760",null,"C3-150138","","Rel-12","29.079","12.1.0","OMR","0045","1","A","-","","","","",""]
["C3-150292","Correction about conditions for filter restrictions","Ericsson, Huawei","Mathieu Mangion",27904,"CR","","","","104","11.5","PCC aspects of SAE [SAES-St3-PCC]",1901,"Revised","2015-02-10T16:30:56.900","2015-02-10T16:26:08.223","C3-150190","C3-150379","Rel-11","29.212","11.14.0","SAES-St3-PCC","1294","1","F","-","","","","",""]
["C3-150293","Correction about conditions for filter restrictions","Ericsson, Huawei","Mathieu Mangion",27904,"CR","","","","104","11.5","PCC aspects of SAE [SAES-St3-PCC]",1911,"Revised","2015-02-10T16:30:57.043","2015-02-10T16:26:09.207","C3-150191","C3-150380","Rel-12","29.212","12.7.0","SAES-St3-PCC","1295","1","A","-","","","","",""]
["C3-150294","Correction about conditions for filter restrictions","Ericsson, Huawei","Mathieu Mangion",27904,"CR","","","","104","11.5","PCC aspects of SAE [SAES-St3-PCC]",1921,"Revised","2015-02-10T16:30:57.173","2015-02-10T16:26:10.180","C3-150192","C3-150381","Rel-13","29.212","13.0.0","SAES-St3-PCC","1296","1","A","-","","","","",""]
["C3-150295","Correction of TFT handling on default bearer","Huawei","Mathieu Mangion",27904,"CR","","","","104","11.5","PCC aspects of SAE [SAES-St3-PCC]",2071,"Revised","2015-02-10T16:30:57.307","2015-02-10T16:26:11.177","C3-150207","C3-150382","Rel-11","29.212","11.14.0","SAES-St3-PCC","1302","1","F","-","","","","",""]
["C3-150296","Correction of TFT handling on default bearer","Huawei","Mathieu Mangion",27904,"CR","","","","104","11.5","PCC aspects of SAE [SAES-St3-PCC]",2081,"Revised","2015-02-10T16:30:57.447","2015-02-10T16:26:12.153","C3-150208","C3-150383","Rel-12","29.212","12.7.0","SAES-St3-PCC","1303","1","A","-","","","","",""]
["C3-150297","Correction of TFT handling on default bearer","Huawei","Mathieu Mangion",27904,"CR","","","","104","11.5","PCC aspects of SAE [SAES-St3-PCC]",2091,"Revised","2015-02-10T16:30:57.580","2015-02-10T16:26:13.150","C3-150209","C3-150384","Rel-13","29.212","13.0.0","SAES-St3-PCC","1304","1","A","-","","","","",""]
["C3-150298","Access network information report in case of IP-CAN bearer/IP-CAN session termination","ZTE","Mathieu Mangion",27904,"CR","","","","128","11.30","CT aspect on Network Provided Location Information for IMS",1481,"Revised","2015-02-10T16:30:57.717","2015-02-10T16:26:14.150","C3-150148","C3-150404","Rel-11","29.214","11.14.0","NWK-PL2IMS-CT","0381","1","F","-","","","","",""]
["C3-150299","Access network information report in case of IP-CAN bearer/IP-CAN session termination","ZTE","Mathieu Mangion",27904,"CR","","","","128","11.30","CT aspect on Network Provided Location Information for IMS",1491,"Revised","2015-02-10T16:30:57.857","2015-02-10T16:26:15.263","C3-150149","C3-150405","Rel-12","29.214","12.6.0","NWK-PL2IMS-CT","0382","1","A","-","","","","",""]
["C3-150300","Access network information report in case of IP-CAN bearer/IP-CAN session termination","ZTE","Mathieu Mangion",27904,"CR","","","","128","11.30","CT aspect on Network Provided Location Information for IMS",1501,"Revised","2015-02-10T16:30:57.997","2015-02-10T16:26:16.230","C3-150150","C3-150406","Rel-13","29.214","13.0.0","NWK-PL2IMS-CT","0383","1","A","-","","","","",""]
["C3-150301","Correction to temporary network failure handling","ZTE","Mathieu Mangion",27904,"CR","","","","133","11.35","Enhanced Nodes Restoration for EPC [eNR_EPC]",1531,"Agreed","2015-02-10T16:30:58.133","2015-02-10T16:26:17.207","C3-150153","","Rel-13","29.214","13.0.0","eNR_EPC","0386","1","F","CP-150136","","","","",""]
["C3-150302","Corrections to the Used-Service-Unit AVP when UMCH feature is supported","China Telecom,ZTE,Huawei","Mathieu Mangion",27904,"CR","","","","135","11.37","Technical Enhancements and Improvements [TEI11]",791,"Revised","2015-02-10T16:30:58.270","2015-02-10T16:26:18.223","C3-150079","C3-150407","Rel-11","29.212","11.14.0","TEI11","1275","1","F","-","","","","",""]
["C3-150303","Corrections to the Used-Service-Unit AVP when UMCH feature is supported","China Telecom,ZTE,Huawei","Mathieu Mangion",27904,"CR","","","","135","11.37","Technical Enhancements and Improvements [TEI11]",801,"Revised","2015-02-10T16:30:58.420","2015-02-10T16:26:19.207","C3-150080","C3-150408","Rel-12","29.212","12.7.0","TEI11","1276","1","A","-","","","","",""]
["C3-150304","Corrections to the Used-Service-Unit AVP when UMCH feature is supported","China Telecom,ZTE,Huawei","Mathieu Mangion",27904,"CR","","","","135","11.37","Technical Enhancements and Improvements [TEI11]",811,"Revised","2015-02-10T16:30:58.560","2015-02-10T16:26:20.227","C3-150081","C3-150409","Rel-13","29.212","13.0.0","TEI11","1277","1","A","-","","","","",""]
["C3-150305","revised WID on IMS Signalling Activated Trace (ISAT)","Vodafone GmbH","Mathieu Mangion",27904,"WID","","","","196","13.10","Rel-13 contributions on other Work Items",711,"Technically endorsed","2015-02-10T16:30:58.697","2015-02-10T16:26:21.110","C3-150071","","Rel-13","","","","","","","","","","","",""]
["C3-150306","Remove editor's note on optimization of UE identity in aggregated RUCI reporting","Huawei","Mathieu Mangion",27904,"pCR","","","","185","13.1","CT aspects of User Plane Congestion Management (UPCON) for Building Block I",941,"Agreed","2015-02-10T16:30:58.763","2015-02-10T16:26:21.127","C3-150094","","Rel-13","29.217","1.0.0","UPCON-DOTCON-CT","","","","","","","","",""]
["C3-150307","Adding UE location information in aggregated RUCI reporting","Huawei","Mathieu Mangion",27904,"pCR","","","","185","13.1","CT aspects of User Plane Congestion Management (UPCON) for Building Block I",931,"Revised","2015-02-10T16:30:58.837","2015-02-10T16:26:22","C3-150093","C3-150392","Rel-13","29.217","1.0.0","UPCON-DOTCON-CT","","","","","","","","",""]
["C3-150308","Resolve the race conditions related to UE mobility between RCAFs","ZTE","Mathieu Mangion",27904,"pCR","","","","185","13.1","CT aspects of User Plane Congestion Management (UPCON) for Building Block I",1651,"Revised","2015-02-10T16:30:58.903","2015-02-10T16:26:22.887","C3-150165","C3-150395","Rel-13","29.217","1.0.0","UPCON-DOTCON-CT","","","","","","","","",""]
["C3-150309","Mitigating RAN user plane congestion over Rest Rx","Huawei, China Telecom, Cisco","Mathieu Mangion",27904,"CR","","","","185","13.1","CT aspects of User Plane Congestion Management (UPCON) for Building Block I",901,"Agreed","2015-02-10T16:30:58.973","2015-02-10T16:26:23.850","C3-150090","","Rel-13","29.201","12.1.0","UPCON-DOTCON-CT","0020","1","B","CP-150125","","","","",""]
["C3-150310","DRA procedure to support PCRF selection by the RCAF","Huawei, China Telecom","Mathieu Mangion",27904,"CR","","","","185","13.1","CT aspects of User Plane Congestion Management (UPCON) for Building Block I",921,"Revised","2015-02-10T16:30:59.110","2015-02-10T16:26:24.813","C3-150092","C3-150391","Rel-13","29.213","13.0.0","UPCON-DOTCON-CT","0593","1","B","-","","","","",""]
["C3-150311","Clarifying the congestion level value in AVP defintion","Huawei","Mathieu Mangion",27904,"pCR","","","","185","13.1","CT aspects of User Plane Congestion Management (UPCON) for Building Block I",951,"Revised","2015-02-10T16:30:59.250","2015-02-10T16:26:25.707","C3-150095","C3-150393","Rel-13","29.217","1.0.0","UPCON-DOTCON-CT","","","","","","","","",""]
["C3-150312","Editor's note cleanup","Huawei","Mathieu Mangion",27904,"pCR","","","","185","13.1","CT aspects of User Plane Congestion Management (UPCON) for Building Block I",971,"Agreed","2015-02-10T16:30:59.323","2015-02-10T16:26:26.597","C3-150097","","Rel-13","29.217","1.0.0","UPCON-DOTCON-CT","","","","","","","","",""]
["C3-150313","Remove the access capability in re-used AVP table","ZTE","Mathieu Mangion",27904,"pCR","","","","185","13.1","CT aspects of User Plane Congestion Management (UPCON) for Building Block I",1621,"Agreed","2015-02-10T16:30:59.393","2015-02-10T16:26:27.543","C3-150162","","Rel-13","29.217","1.0.0","UPCON-DOTCON-CT","","","","","","","","",""]
["C3-150314","Clarify the condition where the RCAF reports the RUCI","ZTE","Mathieu Mangion",27904,"pCR","","","","185","13.1","CT aspects of User Plane Congestion Management (UPCON) for Building Block I",1601,"Revised","2015-02-10T16:30:59.460","2015-02-10T16:26:28.423","C3-150160","C3-150394","Rel-13","29.217","1.0.0","UPCON-DOTCON-CT","","","","","","","","",""]
["C3-150315","M bit set for the specific AVPs","ZTE","Mathieu Mangion",27904,"pCR","","","","185","13.1","CT aspects of User Plane Congestion Management (UPCON) for Building Block I",1611,"Agreed","2015-02-10T16:30:59.533","2015-02-10T16:26:29.297","C3-150161","","","29.217","1.0.0","UPCON-DOTCON-CT","","","","","","","","",""]
["C3-150316","Removal of UE context procedure","Ericsson","Mathieu Mangion",27904,"pCR","","","","185","13.1","CT aspects of User Plane Congestion Management (UPCON) for Building Block I",1951,"Agreed","2015-02-10T16:30:59.603","2015-02-10T16:26:30.170","C3-150195","","Rel-13","29.217","1.0.0","UPCON-DOTCON-CT","","","","","","","","",""]
["C3-150317","Conditional and Unconditional reporting restrictions","Ericsson","Mathieu Mangion",27904,"pCR","","","","185","13.1","CT aspects of User Plane Congestion Management (UPCON) for Building Block I",1961,"Revised","2015-02-10T16:30:59.677","2015-02-10T16:26:31.047","C3-150196","C3-150421","Rel-13","29.217","1.0.0","UPCON-DOTCON-CT","","","","","","","","",""]
["C3-150318","UE context removal in IP-CAN session termination procedure","Ericsson","Mathieu Mangion",27904,"CR","","","","185","13.1","CT aspects of User Plane Congestion Management (UPCON) for Building Block I",1971,"Revised","2015-02-10T16:30:59.753","2015-02-10T16:26:32.040","C3-150197","C3-150431","Rel-13","29.213","13.0.0","UPCON-DOTCON-CT","0596","1","B","-","","","","",""]
["C3-150319","Paging policy differentiation for IMS voice","Alcatel-Lucent, Verizon","Mathieu Mangion",27904,"CR","","","","186","13.2","CT aspects of voice over E-UTRAN Paging Policy Differentiation",1111,"Revised","2015-02-10T16:30:59.940","2015-02-10T16:26:33.067","C3-150111","C3-150396","Rel-13","29.061","12.8.0","voE_UTRAN_PPD-CT, 650303","0444","1","B","-","","","","",""]
["C3-150320","Reply LS on End-to-end QoS handling of MTSI","Ericsson","Mathieu Mangion",27904,"LS out","","","","187","13.3","CT Aspects of End-to-End MTSI Extensions",1831,"Revised","2015-02-10T16:31:00.090","2015-02-10T16:26:34.697","C3-150183","C3-150399","Rel-13","","","QOSE2EMTSI-CT","","","","","C3-150254","SA4","CT1, CT4, SA2"]
["C3-150321","Double resource reuse support over S9","Ericsson","Mathieu Mangion",27904,"CR","","","","189","13.5","CT aspects of Double Resource Reuse for Multiple Media Sessions",1791,"Agreed","2015-02-10T16:31:00.163","2015-02-10T16:26:35.570","C3-150179","","Rel-13","29.215","13.0.0","DRuMS-CT","0372","1","B","CP-150127","","","","",""]
["C3-150322","Uniqueness of Sharing Key for resource sharing over Rx","Ericsson","Mathieu Mangion",27904,"CR","","","","189","13.5","CT aspects of Double Resource Reuse for Multiple Media Sessions",1811,"Revised","2015-02-10T16:31:00.317","2015-02-10T16:26:36.557","C3-150181","C3-150400","Rel-13","29.214","13.0.0","DRuMS-CT","0389","1","B","-","","","","",""]
["C3-150323","Excluding Usage of a ServiceApplication from IP-CAN sessionTDF session Usage","ZTE, China Telecom, Huawei","Mathieu Mangion",27904,"CR","","","","190","13.6","CT3 Aspect of Usage Monitoring Control extension",1661,"Agreed","2015-02-10T16:31:00.457","2015-02-10T16:26:37.523","C3-150166","","Rel-13","29.212","13.0.0","eUMONC-CT3","1288","1","B","CP-150128","","","","",""]
["C3-150324","Excluding Usage of a ServiceApplication from IP-CAN sessionTDF session Usage for roaming case","ZTE, China Telecom, Huawei","Mathieu Mangion",27904,"CR","","","","190","13.6","CT3 Aspect of Usage Monitoring Control extension",1671,"Agreed","2015-02-10T16:31:00.603","2015-02-10T16:26:38.517","C3-150167","","Rel-13","29.215","13.0.0","eUMONC-CT3","0371","1","B","CP-150128","","","","",""]
["C3-150325","TDF support for downlink packet marking","Allot Communications Ltd., Huawei","Mathieu Mangion",27904,"CR","","","","195","13.9.2","TEI13 for Packet Core",881,"Revised","2015-02-10T16:31:00.747","2015-02-10T16:26:39.537","C3-150088","C3-150401","Rel-13","29.212","13.0.0","SAPP, SAPP-CT3","1278","1","C","-","","","","",""]
["C3-150326","Reference update: draft-ietf-mmusic-sctp-sdp","Ericsson","Mathieu Mangion",27904,"CR","","","","145","12.13","IMS-based Telepresence (Stage 3) [IMS_TELEP]",1261,"Agreed","2015-02-10T16:31:00.890","2015-02-10T16:26:41.273","C3-150126","","Rel-12","29.165","12.6.0","580001","0720","1","F","CP-150107","","","","",""]
["C3-150327","Correction to attribute “a=inactive” in initial INVITE","Deutsche Telekom AG, AT&T, Telefonica, NTT","Mathieu Mangion",27904,"CR","","","","146","12.14","IMS Stage-3 IETF Protocol Alignment  [IMSProtoc6]",1121,"Agreed","2015-02-10T16:31:01.037","2015-02-10T16:26:42.250","C3-150112","","Rel-12","29.163","12.6.0","IMSProtoc6","0848","1","F","CP-150108","","","","",""]
["C3-150328","Correction to attribute “a=inactive” in initial INVITE","Deutsche Telekom AG, AT&T, Telefonica, NTT","Mathieu Mangion",27904,"CR","","","","146","12.14","IMS Stage-3 IETF Protocol Alignment  [IMSProtoc6]",1131,"Agreed","2015-02-10T16:31:01.177","2015-02-10T16:26:43.257","C3-150113","","Rel-13","29.163","13.0.0","IMSProtoc6","0849","1","A","CP-150108","","","","",""]
["C3-150329","Relayed-Charge header field","Ericsson LM","Mathieu Mangion",27904,"CR","","","","146","12.14","IMS Stage-3 IETF Protocol Alignment  [IMSProtoc6]",1321,"Revised","2015-02-10T16:31:01.323","2015-02-10T16:26:44.257","C3-150132","C3-150363","Rel-12","29.165","12.6.0","IMSProtoc6","0725","1","F","-","","","","",""]
["C3-150330","Reference update: draft-ietf-insipid-session-id","Ericsson","Mathieu Mangion",27904,"CR","","","","146","12.14","IMS Stage-3 IETF Protocol Alignment  [IMSProtoc6]",1391,"Agreed","2015-02-10T16:31:01.473","2015-02-10T16:26:45.307","C3-150139","","Rel-12","29.165","12.6.0","IMSProtoc6","0727","1","F","CP-150108","","","","",""]
["C3-150331","Reference update: draft-holmberg-dispatch-iotl","Ericsson","Mathieu Mangion",27904,"CR","","","","162","12.28","Study on Technical aspects on Roaming End-to-end scenarios with VoLTE IMS and other networks [FS_REVOLTE_IMS]",1291,"Agreed","2015-02-10T16:31:01.617","2015-02-10T16:26:46.340","C3-150129","","Rel-13","29.949","12.0.0","IMSProtoc7","0001","1","F","CP-150113","","","","",""]
["C3-150332","Addition of \"mp\" header field parameter into CDIV section.","NTT","Mathieu Mangion",27904,"CR","","","","175","12.41","Impacts of RFC7044 for introduction of the new History-Info header field [HISTORY_CT]",341,"Agreed","2015-02-10T16:31:01.760","2015-02-10T16:26:47.350","C3-150034","","Rel-12","29.165","12.6.0","HISTORY_CT","0713","1","F","CP-150118","","","","",""]
["C3-150333","Restoration-Info header field applicability","Ericsson","Mathieu Mangion",27904,"CR","","","","178","12.44","P-CSCF restoration enhancements [PCSCF_RES]",1311,"Agreed","2015-02-10T16:31:01.907","2015-02-10T16:26:48.337","C3-150131","","Rel-12","29.165","12.6.0","PCSCF_RES","0724","1","F","CP-150120","","","","",""]
["C3-150334","TWAN release cause for trusted WLAN","Huawei","Mathieu Mangion",27904,"CR","","","","195","13.9.2","TEI13 for Packet Core",1071,"Postponed","2015-02-10T16:31:02.047","2015-02-10T16:26:49.353","C3-150107","","Rel-13","29.212","13.0.0","NWK-PL2IMS-CT, TEI13","1281","1","B","-","","","","",""]
["C3-150335","TWAN release cause for trusted WLAN","Huawei","Mathieu Mangion",27904,"CR","","","","195","13.9.2","TEI13 for Packet Core",1081,"Postponed","2015-02-10T16:31:02.190","2015-02-10T16:26:51.093","C3-150108","","Rel-13","29.214","13.0.0","NWK-PL2IMS-CT, TEI13","0375","1","B","-","","","","",""]
["C3-150336","QoS mapping for RS and RR","ZTE Corporation","Mathieu Mangion",27904,"CR","","","","195","13.9.2","TEI13 for Packet Core",2141,"Postponed","2015-02-10T16:31:02.347","2015-02-10T16:26:52.827","C3-150214","","Rel-13","29.213","13.0.0","TEI13","0597","1","B","-","","","","",""]
["C3-150337","Charging correlation identifier for the IP-CAN session in Gx","Ericsson, Huawei","Mathieu Mangion",27904,"CR","","","","141","12.4","PCC aspects of SAE [SAES-St3-PCC]",1841,"Revised","2015-02-10T16:31:02.500","2015-02-10T16:26:53.787","C3-150184","C3-150410","Rel-12","29.212","12.7.0","SAES-St3-PCC, TEI12","1290","1","B","-","","","","",""]
["C3-150338","Charging correlation identifier for the IP-CAN session in Gx","Huawei","Mathieu Mangion",27904,"CR","","","","141","12.4","PCC aspects of SAE [SAES-St3-PCC]",2061,"Revised","2015-02-10T16:31:02.643","2015-02-10T16:26:55.560","C3-150206","C3-150411","Rel-13","29.212","13.0.0","SAES-St3-PCC, TEI12","1301","1","A","-","","","","",""]
["C3-150339","Adding support for EVS codec","Nokia Networks","Mathieu Mangion",27904,"CR","","","","179","12.45","CT Impacts of Codec for Enhanced Voice Services [EVS_codec-CT]",2471,"Revised","2015-02-10T16:31:02.783","2015-02-10T16:26:57.333","C3-150247","C3-150436","Rel-13","29.163","13.0.0","EVS_codec-CT","0864","1","B","-","","","","",""]
["C3-150340","QoS change of default bearer","Ericsson","Mathieu Mangion",27904,"CR","","","","141","12.4","PCC aspects of SAE [SAES-St3-PCC]",1881,"Agreed","2015-02-10T16:31:02.927","2015-02-10T16:26:58.307","C3-150188","","Rel-12","29.212","12.7.0","SAES-St3-PCC, TEI12","1292","1","B","CP-150106","","","","",""]
["C3-150341","QoS change of default bearer","Ericsson","Mathieu Mangion",27904,"CR","","","","141","12.4","PCC aspects of SAE [SAES-St3-PCC]",1891,"Agreed","2015-02-10T16:31:03.070","2015-02-10T16:27:00.030","C3-150189","","Rel-13","29.212","13.0.0","SAES-St3-PCC, TEI12","1293","1","A","CP-150106","","","","",""]
["C3-150342","Editorial correction and incorrect implementation of CRs","Alcatel-Lucent Deutschland AG","Mathieu Mangion",27904,"CR","","","","152","12.18.1","Representational State Transfer (REST) reference point between Application Function (AF) and Protocol Converter (PC) [REST_AF_PC]",1751,"Agreed","2015-02-10T16:31:03.213","2015-02-10T16:27:01.757","C3-150175","","Rel-12","29.201","12.1.0","REST_AF_PC","0021","1","F","CP-150110","","","","",""]
["C3-150343","Correction to the session establishment and notification URIs","Oracle Corporation","Mathieu Mangion",27904,"CR","","","","152","12.18.1","Representational State Transfer (REST) reference point between Application Function (AF) and Protocol Converter (PC) [REST_AF_PC]",2301,"Revised","2015-02-10T16:31:03.353","2015-02-10T16:27:02.750","C3-150230","C3-150385","Rel-12","29.201","12.1.0","REST_AF_PC","0024","1","F","-","","","","",""]
["C3-150344","Allowing for forward compatibility and miscellaneous corrections","Oracle Corporation","Mathieu Mangion",27904,"CR","","","","152","12.18.1","Representational State Transfer (REST) reference point between Application Function (AF) and Protocol Converter (PC) [REST_AF_PC]",2311,"Revised","2015-02-10T16:31:03.497",null,"C3-150231","C3-150386","Rel-12","29.201","12.1.0","REST_AF_PC","0025","1","F","-","","","","",""]
["C3-150345","Reference update to align with the published BBF documents","Huawei","Mathieu Mangion",27904,"CR","","","","161","12.27","Policy and Charging Control for supporting traffic from fixed terminals and NSWO traffic from 3GPP Ues in fixed broadband access networks",1051,"Revised","2015-02-10T16:31:03.640","2015-02-10T16:27:04.707","C3-150105","C3-150397","Rel-12","29.215","12.6.0","P4C-F-CT3","0369","1","F","-","","","","",""]
["C3-150346","Reference update to align with the published BBF documents","Huawei","Mathieu Mangion",27904,"CR","","","","161","12.27","Policy and Charging Control for supporting traffic from fixed terminals and NSWO traffic from 3GPP Ues in fixed broadband access networks",1061,"Revised","2015-02-10T16:31:03.780","2015-02-10T16:27:05.673","C3-150106","C3-150398","Rel-13","29.215","13.0.0","P4C-F-CT3","0370","1","A","-","","","","",""]
["C3-150347","Reference update to align with the published BBF documents","Huawei","Mathieu Mangion",27904,"CR","","","","122","11.24","Support for BroadBand Forum Accesses Interworking, Core Network Impacts, Building Block I [BBAI_BBI-CT]",1071,"Agreed","2015-02-10T16:31:03.927","2015-02-10T16:27:06.547","","","Rel-11","29.215","11.15.0","BBAI_BBI-CT","0376","","F","CP-150103","","","","",""]
["C3-150348","TWAN supports access network information report","ZTE","Mathieu Mangion",27904,"CR","","","","168","12.34","CT aspects of Network Provided Location Information for IMS Trusted WLAN Access Network [NETLOC_TWAN_CT]",1541,"Agreed","2015-02-10T16:31:04.057","2015-02-10T16:27:07.523","C3-150154","","Rel-12","29.212","12.7.0","NETLOC_TWAN-CT","1284","1","F","CP-150114","","","","",""]
["C3-150349","TWAN supports access network information report","ZTE","Mathieu Mangion",27904,"CR","","","","168","12.34","CT aspects of Network Provided Location Information for IMS Trusted WLAN Access Network [NETLOC_TWAN_CT]",1551,"Agreed","2015-02-10T16:31:04.200","2015-02-10T16:27:08.507","C3-150155","","Rel-13","29.212","13.0.0","NETLOC_TWAN-CT","1285","1","A","CP-150114","","","","",""]
["C3-150350","Roaming applicability in EPC-level ProSe discovery","Huawei","Mathieu Mangion",27904,"CR","","","","170","12.36","CT aspects of Proximity-based Services",1001,"Agreed","2015-02-10T16:31:04.347","2015-02-10T16:27:09.597","C3-150100","","Rel-12","29.343","12.1.0","630206","0002","1","F","CP-150116","","","","",""]
["C3-150351","Correction to the PRA reporting","ZTE","Mathieu Mangion",27904,"CR","","","","171","12.37","CT aspects of Core Network Overload  User Location Information reporting improvements [CNO_ULI-CT]",1581,"Revised","2015-02-10T16:31:04.490","2015-02-10T16:27:10.577","C3-150158","C3-150413","Rel-12","29.212","12.7.0","CNO_ULI-CT","1286","1","F","-","","","","",""]
["C3-150352","Correction to the PRA reporting","ZTE","Mathieu Mangion",27904,"CR","","","","171","12.37","CT aspects of Core Network Overload  User Location Information reporting improvements [CNO_ULI-CT]",1591,"Revised","2015-02-10T16:31:04.640","2015-02-10T16:27:11.543","C3-150159","C3-150422","Rel-13","29.212","13.0.0","CNO_ULI-CT","1287","1","A","-","","","","",""]
["C3-150353","LS on Enable MB2 procedures authorization","CT3","Mathieu Mangion",27904,"LS out","","","This LS relats to the authorization of the GCS AS and the supported procedures over the MB2-C interface, such as TMGI allocation/deallocation and MBMS bearer procedures.","176","12.42","CT aspects of Group Communication System Enablers for LTE [GCSE_LTE-CT]",2100,"Revised","2015-02-10T16:31:04.793","2015-02-10T16:27:12.407","","C3-150414","Rel-12","","","GCSE_LTE-CT","","","","",null,"SA3","SA2"]
["C3-150354","TMGI and Flow ID Handling","Huawei, Nokia Networks","Mathieu Mangion",27904,"CR","","","","176","12.42","CT aspects of Group Communication System Enablers for LTE [GCSE_LTE-CT]",2104,"Agreed","2015-02-10T16:31:04.863","2015-02-10T16:27:13.250","C3-150210","","Rel-12","29.468","12.1.0","GCSE_LTE-CT","0012","1","F","CP-150119","","","","",""]
["C3-150355","Corrections in the definition of MBMS Service Area AVP","Motorola Solutions Danmark A/S","Mathieu Mangion",27904,"CR","","","","176","12.42","CT aspects of Group Communication System Enablers for LTE [GCSE_LTE-CT]",2330,"Revised","2015-02-10T16:31:05.007","2015-02-10T16:27:14.257","C3-150232","C3-150416","Rel-12","29.061","12.8.0","GCSE_LTE-CT","0445","1","F","-","","","","",""]
["C3-150356","Activation of an additional MBMS Bearer for a TMGI with already an active MBMS Bearer","Motorola Solutions Danmark A/S","Mathieu Mangion",27904,"CR","","","","176","12.42","CT aspects of Group Communication System Enablers for LTE [GCSE_LTE-CT]",2332,"Revised","2015-02-10T16:31:05.150","2015-02-10T16:27:15.133","C3-150250","C3-150417","Rel-12","29.468","12.1.0","GCSE_LTE-CT","0013","2","F","-","","","","",""]
["C3-150357","Opptional MBMS Session Identity","Motorola Solutions Danmark A/S","Mathieu Mangion",27904,"CR","","","","176","12.42","CT aspects of Group Communication System Enablers for LTE [GCSE_LTE-CT]",37100,"Postponed","2015-02-10T16:31:05.280",null,"C3-150251","","Rel-12","29.468","12.1.0","GCSE_LTE-CT","0014","2","F","-","","","","",""]
["C3-150358","Correction on volumn and time threshold provisioning","Huawei","Mathieu Mangion",27904,"CR","","","","182","12.46.2","TEI12 for Packet Core",1091,"Agreed","2015-02-10T16:31:05.410","2015-02-10T16:27:17.007","C3-150109","","Rel-12","29.212","12.7.0","UMONC-CT3","1282","1","F","CP-150122","","","","",""]
["C3-150359","Correction on volumn and time threshold provisioning","Huawei","Mathieu Mangion",27904,"CR","","","","182","12.46.2","TEI12 for Packet Core",1101,"Agreed","2015-02-10T16:31:05.553","2015-02-10T16:27:18.007","C3-150110","","Rel-13","29.212","13.0.0","UMONC-CT3","1283","1","A","CP-150122","","","","",""]
["C3-150360","Add the ToS-Traffic-Class AVP to the Rx to be sent by AF","Motorola Solutions Danmark A/S","Mathieu Mangion",27904,"CR","","","","198","13.12","CT aspects of Group Communication System Enablers for LTE [GCSE_LTE-CT]",37100,"Revised","2015-02-10T16:31:05.703","2015-02-10T16:27:18.877","","C3-150403","Rel-13","29.214","13.0.0","TEI13, GCSE_LTE-CT","0394","","B","-","","","","",""]
["C3-150361","Location information in case of non-3GPP access","Alcatel-Lucent","Mathieu Mangion",27904,"CR","","","","182","12.46.2","TEI12 for Packet Core",2391,"Revised","2015-02-10T16:31:05.840","2015-02-10T16:27:20.577","C3-150239","C3-150418","Rel-12","29.214","12.6.0","TEI12","0392","1","F","-","","","","",""]
["C3-150362","Location information in case of non-3GPP access","Alcatel-Lucent","Mathieu Mangion",27904,"CR","","","","182","12.46.2","TEI12 for Packet Core",2421,"Revised","2015-02-10T16:31:05.993","2015-02-10T16:27:21.550","C3-150242","C3-150419","Rel-13","29.214","13.0.0","TEI12","0393","1","B","-","","","","",""]
["C3-150363","Relayed-Charge header field","Ericsson LM","Mathieu Mangion",27904,"CR","","","","146","12.14","IMS Stage-3 IETF Protocol Alignment  [IMSProtoc6]",1322,"Revised","2015-02-10T16:31:06.147","2015-02-10T16:27:22.417","C3-150329","C3-150435","Rel-12","29.165","12.6.0","IMSProtoc6","0725","2","F","-","","","","",""]
["C3-150364","Removal of duplicated refrence","Nokia Networks","Mathieu Mangion",27904,"CR","","","","179","12.45","CT Impacts of Codec for Enhanced Voice Services [EVS_codec-CT]",37500,"Agreed","2015-02-10T16:31:06.270","2015-02-10T16:27:23.290","","","Rel-12","29.163","12.6.0","EVS_codec-CT","0867","","F","CP-150121","","","","",""]
["C3-150365","Correction of applicability of P-Charging-Vector header field in NOTIFY method","Fujitsu Limited","Mathieu Mangion",27904,"CR","","","","183","12.47","Rel-12 contributions on other Work Items",1781,"Agreed","2015-02-10T16:31:06.397","2015-02-10T16:27:24.277","C3-150178","","Rel-12","29.165","12.6.0","NNI_DV","0732","1","F","CP-150124","","","","",""]
["C3-150366","Addition of an optional capability regarding a new cause-param value for service number translation.","NTT","Mathieu Mangion",27904,"CR","","","","192","13.8","Interworking of Called IN number and original Called IN number ISUP parameters",391,"Agreed","2015-02-10T16:31:06.543","2015-02-10T16:27:25.267","C3-150039","","Rel-13","29.165","12.6.0","660021","0718","1","B","CP-150129","","","","",""]
["C3-150367","Reference update: draft-mohali-dispatch-cause-for-service-number","ORANGE","Mathieu Mangion",27904,"CR","","","","192","13.8","Interworking of Called IN number and original Called IN number ISUP parameters",1431,"Revised","2015-02-10T16:31:06.687","2015-02-10T16:27:26.253","C3-150143","C3-150371","Rel-13","29.163","13.0.0","INNB_IW","0850","1","F","-","","","","",""]
["C3-150368","Applying drafting rules","Ericsson LM","Mathieu Mangion",27904,"CR","","","","194","13.9.1","TEI13 for IMS/CS",1331,"Revised","2015-02-10T16:31:06.853","2015-02-10T16:27:27.213","C3-150133","C3-150373","Rel-13","29.165","12.6.0","TEI13","0726","1","F","-","","","","",""]
["C3-150369","Adding missing abbreviations","Fujitsu Limited, NTT","Mathieu Mangion",27904,"CR","","","","194","13.9.1","TEI13 for IMS/CS",1741,"Agreed","2015-02-10T16:31:07.007","2015-02-10T16:27:28.207","C3-150174","","Rel-13","29.165","12.6.0","TEI13","0729","1","F","CP-150130","","","","",""]
["C3-150370","LS on new cause URI parameter value for IN numbers interworking","ORANGE","Mathieu Mangion",27904,"LS out","","","CT3 and CT1 informing SA5 of the enabling the Interworking of the ISUP parameters Called IN number and Original called IN number with IMS, asking them if there is any impact on their spec.","192","13.8","Interworking of Called IN number and original Called IN number ISUP parameters",1421,"Revised","2015-02-10T16:31:07.157","2015-02-10T16:27:29.103","C3-150142","C3-150372","Rel-13","","","INNB_IW","","","","",null,"SA5","CT1"]
["C3-150371","Reference update: draft-mohali-dispatch-cause-for-service-number","ORANGE","Mathieu Mangion",27904,"CR","","","","192","13.8","Interworking of Called IN number and original Called IN number ISUP parameters",1432,"Agreed","2015-02-10T16:31:07.233","2015-02-10T16:27:29.900","C3-150367","","Rel-13","29.163","13.0.0","660021","0850","2","F","CP-150129","","","","",""]
["C3-150372","LS on new cause URI parameter value for IN numbers interworking","ORANGE","Mathieu Mangion",27904,"LS out","","","","192","13.8","Interworking of Called IN number and original Called IN number ISUP parameters",1422,"Revised","2015-02-10T16:31:07.367","2015-02-10T16:27:30.783","C3-150370","C3-150439","Rel-13","","","INNB_IW","","","","",null,"SA5","CT1"]
["C3-150373","Applying drafting rules","Ericsson LM","Mathieu Mangion",27904,"CR","","","","194","13.9.1","TEI13 for IMS/CS",1332,"Revised","2015-02-10T16:31:07.437","2015-02-10T16:27:31.567","C3-150368","C3-150440","Rel-13","29.165","12.6.0","TEI13","0726","2","F","-","","","","",""]
["C3-150374","Bugfix: do not send negative-delivery IMDN after sending SIP 4xx/5xx response","Comverse Network Systems","Mathieu Mangion",27904,"CR","","","","46","8.21","Support of Service-Level Interworking for Messaging Services [MESSIW]",242,"Agreed","2015-02-10T16:31:07.570","2015-02-10T16:27:32.467","C3-150261","","Rel-8","29.311","8.3.0","MESSIW","0034","2","F","CP-150096","","","","",""]
["C3-150375","Bugfix: do not send negative-delivery IMDN after sending SIP 4xx/5xx response","Comverse","Mathieu Mangion",27904,"CR","","","","46","8.21","Support of Service-Level Interworking for Messaging Services [MESSIW]",252,"Agreed","2015-02-10T16:31:07.707","2015-02-10T16:27:33.357","C3-150262","","Rel-9","29.311","9.2.0","MESSIW","0035","2","A","CP-150096","","","","",""]
["C3-150376","Bugfix: do not send negative-delivery IMDN after sending SIP 4xx/5xx response","Comverse","Mathieu Mangion",27904,"CR","","","","46","8.21","Support of Service-Level Interworking for Messaging Services [MESSIW]",262,"Agreed","2015-02-10T16:31:07.847","2015-02-10T16:27:34.233","C3-150263","","Rel-10","29.311","10.5.0","MESSIW","0036","2","A","CP-150096","","","","",""]
["C3-150377","Bugfix: do not send negative-delivery IMDN after sending SIP 4xx/5xx response","Comverse","Mathieu Mangion",27904,"CR","","","","46","8.21","Support of Service-Level Interworking for Messaging Services [MESSIW]",272,"Agreed","2015-02-10T16:31:07.977","2015-02-10T16:27:35.093","C3-150264","","Rel-11","29.311","11.1.0","MESSIW","0037","2","A","CP-150096","","","","",""]
["C3-150378","Bugfix: do not send negative-delivery IMDN after sending SIP 4xx/5xx response","Comverse","Mathieu Mangion",27904,"CR","","","","46","8.21","Support of Service-Level Interworking for Messaging Services [MESSIW]",282,"Agreed","2015-02-10T16:31:08.110","2015-02-10T16:27:35.960","C3-150265","","Rel-12","29.311","12.0.0","MESSIW","0038","2","A","CP-150096","","","","",""]
["C3-150379","Correction about conditions for filter restrictions","Ericsson, Huawei","Mathieu Mangion",27904,"CR","","","","104","11.5","PCC aspects of SAE [SAES-St3-PCC]",1902,"Agreed","2015-02-10T16:31:08.247","2015-02-10T16:27:36.817","C3-150292","","Rel-11","29.212","11.14.0","SAES-St3-PCC","1294","2","F","CP-150102","","","","",""]
["C3-150380","Correction about conditions for filter restrictions","Ericsson, Huawei","Mathieu Mangion",27904,"CR","","","","104","11.5","PCC aspects of SAE [SAES-St3-PCC]",1912,"Agreed","2015-02-10T16:31:08.383","2015-02-10T16:27:37.683","C3-150293","","Rel-12","29.212","12.7.0","SAES-St3-PCC","1295","2","A","CP-150102","","","","",""]
["C3-150381","Correction about conditions for filter restrictions","Ericsson, Huawei","Mathieu Mangion",27904,"CR","","","","104","11.5","PCC aspects of SAE [SAES-St3-PCC]",1922,"Agreed","2015-02-10T16:31:08.517","2015-02-10T16:27:38.557","C3-150294","","Rel-13","29.212","13.0.0","SAES-St3-PCC","1296","2","A","CP-150102","","","","",""]
["C3-150382","Correction of TFT handling on default bearer","Huawei","Mathieu Mangion",27904,"CR","","","","104","11.5","PCC aspects of SAE [SAES-St3-PCC]",2072,"Agreed","2015-02-10T16:31:08.653","2015-02-10T16:27:39.427","C3-150295","","Rel-11","29.212","11.14.0","SAES-St3-PCC","1302","2","F","CP-150102","","","","",""]
["C3-150383","Correction of TFT handling on default bearer","Huawei","Mathieu Mangion",27904,"CR","","","","104","11.5","PCC aspects of SAE [SAES-St3-PCC]",2082,"Agreed","2015-02-10T16:31:08.790","2015-02-10T16:27:40.317","C3-150296","","Rel-12","29.212","12.7.0","SAES-St3-PCC","1303","2","A","CP-150102","","","","",""]
["C3-150384","Correction of TFT handling on default bearer","Huawei","Mathieu Mangion",27904,"CR","","","","104","11.5","PCC aspects of SAE [SAES-St3-PCC]",2092,"Revised","2015-02-10T16:31:08.923","2015-02-10T16:27:41.213","C3-150297","C3-150423","Rel-13","29.212","13.0.0","SAES-St3-PCC","1304","2","A","-","","","","",""]
["C3-150385","Correction to the session establishment and notification URIs","Oracle Corporation","Mathieu Mangion",27904,"CR","","","","152","12.18.1","Representational State Transfer (REST) reference point between Application Function (AF) and Protocol Converter (PC) [REST_AF_PC]",2302,"Revised","2015-02-10T16:31:09.057","2015-02-10T16:27:42.103","C3-150343","C3-150412","Rel-12","29.201","12.1.0","REST_AF_PC","0024","2","F","-","","","","",""]
["C3-150386","Allowing for forward compatibility and miscellaneous corrections","Oracle Corporation","Mathieu Mangion",27904,"CR","","","","152","12.18.1","Representational State Transfer (REST) reference point between Application Function (AF) and Protocol Converter (PC) [REST_AF_PC]",2312,"Revised","2015-02-10T16:31:09.200","2015-02-10T16:27:42.950","C3-150344","C3-150415","Rel-12","29.201","12.1.0","REST_AF_PC","0025","2","F","-","","","","",""]
["C3-150387","Clarification on the II-NNI requirement for CDIV regarding Privacy header field.","NTT","Mathieu Mangion",27904,"CR","","","","65","9.19","Operational Description of the Inter-IMS NNI   [II-NNI]",302,"Agreed","2015-02-10T16:31:09.340","2015-02-10T16:27:43.827","C3-150281","","Rel-9","29.165","9.19.0","II-NNI","0709","2","F","CP-150098","","","","",""]
["C3-150388","Clarification on the II-NNI requirement for CDIV regarding Privacy header field.","NTT","Mathieu Mangion",27904,"CR","","","","65","9.19","Operational Description of the Inter-IMS NNI   [II-NNI]",312,"Agreed","2015-02-10T16:31:09.477","2015-02-10T16:27:44.700","C3-150282","","Rel-10","29.165","10.17.0","II-NNI","0710","2","A","CP-150098","","","","",""]
["C3-150389","Clarification on the II-NNI requirement for CDIV regarding Privacy header field.","NTT","Mathieu Mangion",27904,"CR","","","","65","9.19","Operational Description of the Inter-IMS NNI   [II-NNI]",322,"Agreed","2015-02-10T16:31:09.610","2015-02-10T16:27:45.580","C3-150283","","Rel-11","29.165","11.12.0","II-NNI","0711","2","A","CP-150098","","","","",""]
["C3-150390","Clarification on the II-NNI requirement for CDIV regarding Privacy header field.","NTT","Mathieu Mangion",27904,"CR","","","","65","9.19","Operational Description of the Inter-IMS NNI   [II-NNI]",332,"Agreed","2015-02-10T16:31:09.760","2015-02-10T16:27:46.457","C3-150284","","Rel-12","29.165","12.6.0","II-NNI","0712","2","A","CP-150098","","","","",""]
["C3-150391","DRA procedure to support PCRF selection by the RCAF","Huawei, China Telecom","Mathieu Mangion",27904,"CR","","","","185","13.1","CT aspects of User Plane Congestion Management (UPCON) for Building Block I",922,"Agreed","2015-02-10T16:31:09.897","2015-02-10T16:27:47.320","C3-150310","","Rel-13","29.213","13.0.0","UPCON-DOTCON-CT","0593","2","B","CP-150125","","","","",""]
["C3-150392","Adding UE location information in aggregated RUCI reporting","Huawei","Mathieu Mangion",27904,"pCR","","","","185","13.1","CT aspects of User Plane Congestion Management (UPCON) for Building Block I",932,"Revised","2015-02-10T16:31:10.037","2015-02-10T16:27:48.180","C3-150307","C3-150420","Rel-13","29.217","1.0.0","UPCON-DOTCON-CT","","","","","","","","",""]
["C3-150393","Clarifying the congestion level value in AVP defintion","Huawei, China Telecom","Mathieu Mangion",27904,"pCR","","","","185","13.1","CT aspects of User Plane Congestion Management (UPCON) for Building Block I",952,"Revised","2015-02-10T16:31:10.113","2015-02-10T16:27:49.027","C3-150311","C3-150427","Rel-13","29.217","1.0.0","UPCON-DOTCON-CT","","","","","","","","",""]
["C3-150394","Clarify the condition where the RCAF reports the RUCI","ZTE","Mathieu Mangion",27904,"pCR","","","","185","13.1","CT aspects of User Plane Congestion Management (UPCON) for Building Block I",1602,"Revised","2015-02-10T16:31:10.187","2015-02-10T16:27:49.890","C3-150314","C3-150428","Rel-13","29.217","1.0.0","UPCON-DOTCON-CT","","","","","","","","",""]
["C3-150395","Resolve the race conditions related to UE mobility between RCAFs","ZTE","Mathieu Mangion",27904,"pCR","","","","185","13.1","CT aspects of User Plane Congestion Management (UPCON) for Building Block I",1652,"Revised","2015-02-10T16:31:10.270","2015-02-10T16:27:50.757","C3-150308","C3-150432","Rel-13","29.217","1.0.0","UPCON-DOTCON-CT","","","","","","","","",""]
["C3-150396","Paging policy differentiation for IMS voice","Alcatel-Lucent, Verizon","Mathieu Mangion",27904,"CR","","","","186","13.2","CT aspects of voice over E-UTRAN Paging Policy Differentiation",1112,"Agreed","2015-02-10T16:31:10.343","2015-02-10T16:27:51.627","C3-150319","","Rel-13","29.061","12.8.0","650303","0444","2","B","CP-150126","","","","",""]
["C3-150397","Reference update to align with the published BBF documents","Huawei","Mathieu Mangion",27904,"CR","","","","161","12.27","Policy and Charging Control for supporting traffic from fixed terminals and NSWO traffic from 3GPP Ues in fixed broadband access networks",1052,"Agreed","2015-02-10T16:31:10.483","2015-02-10T16:27:52.490","C3-150345","","Rel-12","29.215","12.6.0","BBAI_BBI-CT, P4C-F-CT3","0369","2","F","CP-150112","","","","",""]
["C3-150398","Reference update to align with the published BBF documents","Huawei","Mathieu Mangion",27904,"CR","","","","161","12.27","Policy and Charging Control for supporting traffic from fixed terminals and NSWO traffic from 3GPP Ues in fixed broadband access networks",1062,"Agreed","2015-02-10T16:31:10.620","2015-02-10T16:27:54.130","C3-150346","","Rel-13","29.215","13.0.0","BBAI_BBI-CT, P4C-F-CT3","0370","2","A","CP-150112","","","","",""]
["C3-150399","Reply LS on End-to-end QoS handling of MTSI","Ericsson","Mathieu Mangion",27904,"LS out","","","","187","13.3","CT Aspects of End-to-End MTSI Extensions",1832,"Revised","2015-02-10T16:31:10.760","2015-02-10T16:27:55.797","C3-150320","C3-150444","","","","QOSE2EMTSI-CT","","","","","C3-150254","SA4","CT1, CT4, SA2"]
["C3-150400","Uniqueness of Sharing Key for resource sharing over Rx","Ericsson","Mathieu Mangion",27904,"CR","","","","189","13.5","CT aspects of Double Resource Reuse for Multiple Media Sessions",1812,"Agreed","2015-02-10T16:31:10.837","2015-02-10T16:27:56.570","C3-150322","","Rel-13","29.214","13.0.0","DRuMS-CT","0389","2","B","CP-150127","","","","",""]
["C3-150401","TDF support for downlink packet marking","Allot Communications Ltd., Huawei","Mathieu Mangion",27904,"CR","","","","195","13.9.2","TEI13 for Packet Core",882,"Postponed","2015-02-10T16:31:10.977","2015-02-10T16:27:57.437","C3-150325","","Rel-13","29.212","13.0.0","SAPP, SAPP-CT3","1278","2","C","-","","","","",""]
["C3-150402","New WID on Extended Overload Control for PCC based Diameter applications","ZTE","Mathieu Mangion",27904,"WID","","","","196","13.10","Rel-13 contributions on other Work Items",1682,"Agreed","2015-02-10T16:31:11.110","2015-02-10T16:27:59.037","C3-150259","","Rel-13","","","","","","","","","","","",""]
["C3-150403","Add the ToS-Traffic-Class AVP to the Rx to be sent by AF","Motorola Solutions Danmark A/S","Mathieu Mangion",27904,"CR","","","","198","13.12","CT aspects of Group Communication System Enablers for LTE [GCSE_LTE-CT]",37101,"Revised","2015-02-10T16:31:11.187","2015-02-10T16:27:59.050","C3-150360","C3-150429","Rel-13","29.214","13.0.0","TEI13, GCSE_LTE-CT","0394","1","B","-","","","","",""]
["C3-150404","Access network information report in case of IP-CAN bearer/IP-CAN session termination","ZTE","Mathieu Mangion",27904,"CR","","","","128","11.30","CT aspect on Network Provided Location Information for IMS",1482,"Agreed","2015-02-10T16:31:11.327","2015-02-10T16:28:00.690","C3-150298","","Rel-11","29.214","11.14.0","NWK-PL2IMS-CT","0381","2","F","CP-150104","","","","",""]
["C3-150405","Access network information report in case of IP-CAN bearer/IP-CAN session termination","ZTE","Mathieu Mangion",27904,"CR","","","","128","11.30","CT aspect on Network Provided Location Information for IMS",1492,"Agreed","2015-02-10T16:31:11.467","2015-02-10T16:28:01.603","C3-150299","","Rel-12","29.214","12.6.0","NWK-PL2IMS-CT","0382","2","A","CP-150104","","","","",""]
["C3-150406","Access network information report in case of IP-CAN bearer/IP-CAN session termination","ZTE","Mathieu Mangion",27904,"CR","","","","128","11.30","CT aspect on Network Provided Location Information for IMS",1502,"Agreed","2015-02-10T16:31:11.603","2015-02-10T16:28:02.497","C3-150300","","Rel-13","29.214","13.0.0","NWK-PL2IMS-CT","0383","2","A","CP-150104","","","","",""]
["C3-150407","Corrections to the Used-Service-Unit AVP when UMCH feature is supported","China Telecom,ZTE,Huawei","Mathieu Mangion",27904,"CR","","","","135","11.37","Technical Enhancements and Improvements [TEI11]",792,"Agreed","2015-02-10T16:31:11.740","2015-02-10T16:28:03.363","C3-150302","","Rel-11","29.212","11.14.0","TEI11","1275","2","F","CP-150105","","","","",""]
["C3-150408","Corrections to the Used-Service-Unit AVP when UMCH feature is supported","China Telecom,ZTE,Huawei","Mathieu Mangion",27904,"CR","","","","135","11.37","Technical Enhancements and Improvements [TEI11]",802,"Agreed","2015-02-10T16:31:11.880","2015-02-10T16:28:04.210","C3-150303","","Rel-12","29.212","12.7.0","TEI11","1276","2","A","CP-150105","","","","",""]
["C3-150409","Corrections to the Used-Service-Unit AVP when UMCH feature is supported","China Telecom,ZTE,Huawei","Mathieu Mangion",27904,"CR","","","","135","11.37","Technical Enhancements and Improvements [TEI11]",812,"Agreed","2015-02-10T16:31:12.030","2015-02-10T16:28:05.073","C3-150304","","Rel-13","29.212","13.0.0","TEI11","1277","2","A","CP-150105","","","","",""]
["C3-150410","Charging correlation identifier for the IP-CAN session in Gx","Ericsson, Huawei","Mathieu Mangion",27904,"CR","","","","141","12.4","PCC aspects of SAE [SAES-St3-PCC]",1842,"Agreed","2015-02-10T16:31:12.170","2015-02-10T16:28:05.937","C3-150337","","Rel-12","29.212","12.7.0","SAES-St3-PCC, TEI12","1290","2","B","CP-150106","","","","",""]
["C3-150411","Charging correlation identifier for the IP-CAN session in Gx","Huawei","Mathieu Mangion",27904,"CR","","","","141","12.4","PCC aspects of SAE [SAES-St3-PCC]",2062,"Agreed","2015-02-10T16:31:12.317","2015-02-10T16:28:07.530","C3-150338","","Rel-13","29.212","13.0.0","SAES-St3-PCC, TEI12","1301","2","A","CP-150106","","","","",""]
["C3-150412","Correction to the session establishment and notification URIs","Oracle Corporation","Mathieu Mangion",27904,"CR","","","","152","12.18.1","Representational State Transfer (REST) reference point between Application Function (AF) and Protocol Converter (PC) [REST_AF_PC]",2303,"Agreed","2015-02-10T16:31:12.457","2015-02-10T16:28:08.413","C3-150385","","Rel-12","29.201","12.1.0","REST_AF_PC","0024","3","F","CP-150110","","","","",""]
["C3-150413","Correction to the PRA reporting","ZTE","Mathieu Mangion",27904,"CR","","","","171","12.37","CT aspects of Core Network Overload  User Location Information reporting improvements [CNO_ULI-CT]",1582,"Agreed","2015-02-10T16:31:12.597","2015-02-10T16:28:09.267","C3-150351","","Rel-12","29.212","12.7.0","CNO_ULI-CT","1286","2","F","CP-150117","","","","",""]
["C3-150414","LS on Enable MB2 procedures authorization","CT3","Mathieu Mangion",27904,"LS out","","","","176","12.42","CT aspects of Group Communication System Enablers for LTE [GCSE_LTE-CT]",2101,"Revised","2015-02-10T16:31:12.747","2015-02-10T16:28:10.123","C3-150353","C3-150424","Rel-12","","","GCSE_LTE-CT","","","","",null,"SA3","SA2"]
["C3-150415","Allowing for forward compatibility and miscellaneous corrections","Oracle Corporation","Mathieu Mangion",27904,"CR","","","","152","12.18.1","Representational State Transfer (REST) reference point between Application Function (AF) and Protocol Converter (PC) [REST_AF_PC]",2313,"Agreed","2015-02-10T16:31:12.827","2015-02-10T16:28:10.863","C3-150386","","Rel-12","29.201","12.1.0","REST_AF_PC","0025","3","F","CP-150110","","","","",""]
["C3-150416","Corrections in the definition of MBMS Service Area AVP","Motorola Solutions Danmark A/S","Mathieu Mangion",27904,"CR","","","","176","12.42","CT aspects of Group Communication System Enablers for LTE [GCSE_LTE-CT]",2330,"Revised","2015-02-10T16:31:12.970","2015-02-10T16:28:11.727","C3-150355","C3-150425","Rel-12","29.061","12.8.0","GCSE_LTE-CT","0445","2","F","-","","","","",""]
["C3-150417","Activation of an additional MBMS Bearer for a TMGI with already an active MBMS Bearer","Motorola Solutions Danmark A/S","Mathieu Mangion",27904,"CR","","","","176","12.42","CT aspects of Group Communication System Enablers for LTE [GCSE_LTE-CT]",2341,"Agreed","2015-02-10T16:31:13.113","2015-02-10T16:28:12.587","C3-150356","","Rel-12","29.468","12.1.0","GCSE_LTE-CT","0013","3","F","CP-150119","","","","",""]
["C3-150418","Location information in case of non-3GPP access","Alcatel-Lucent","Mathieu Mangion",27904,"CR","","","","182","12.46.2","TEI12 for Packet Core",2392,"Postponed","2015-02-10T16:31:13.250","2015-02-10T16:28:13.463","C3-150361","","Rel-12","29.214","12.6.0","TEI12","0392","2","F","-","","","","",""]
["C3-150419","Location information in case of non-3GPP access","Alcatel-Lucent","Mathieu Mangion",27904,"CR","","","","182","12.46.2","TEI12 for Packet Core",2422,"Postponed","2015-02-10T16:31:13.393",null,"C3-150362","","Rel-13","29.214","13.0.0","TEI13","0393","2","B","-","","","","",""]
["C3-150420","Adding UE location information in aggregated RUCI reporting","Huawei","Mathieu Mangion",27904,"pCR","","","","185","13.1","CT aspects of User Plane Congestion Management (UPCON) for Building Block I",933,"Revised","2015-02-10T16:31:13.543","2015-02-10T16:28:15.197","C3-150392","C3-150426","Rel-13","29.217","1.0.0","UPCON-DOTCON-CT","","","","","","","","",""]
["C3-150421","Conditional and Unconditional reporting restrictions","Ericsson","Mathieu Mangion",27904,"pCR","","","","185","13.1","CT aspects of User Plane Congestion Management (UPCON) for Building Block I",1962,"Agreed","2015-02-10T16:31:13.620","2015-02-10T16:28:16.053","C3-150317","","Rel-13","29.217","1.0.0","UPCON-DOTCON-CT","","","","","","","","",""]
["C3-150422","Correction to the PRA reporting","ZTE","Mathieu Mangion",27904,"CR","","","","171","12.37","CT aspects of Core Network Overload  User Location Information reporting improvements [CNO_ULI-CT]",1592,"Revised","2015-02-10T16:31:13.707","2015-02-10T16:28:16.917","C3-150352","C3-150430","Rel-13","29.212","13.0.0","CNO_ULI-CT","1287","2","F","-","","","","",""]
["C3-150423","Correction of TFT handling on default bearer","Huawei","Mathieu Mangion",27904,"CR","","","","104","11.5","PCC aspects of SAE [SAES-St3-PCC]",2093,"Agreed","2015-02-10T16:31:13.847","2015-02-10T16:28:17.773","C3-150384","","Rel-13","29.212","13.0.0","SAES-St3-PCC","1304","3","F","CP-150102","","","","",""]
["C3-150424","LS on Enable MB2 procedures authorization","CT3","Mathieu Mangion",27904,"LS out","","","","176","12.42","CT aspects of Group Communication System Enablers for LTE [GCSE_LTE-CT]",2102,"Approved","2015-02-10T16:31:13.990","2015-02-10T16:28:18.647","C3-150414","","Rel-12","","","GCSE_LTE-CT","","","","",null,"SA3","SA2"]
["C3-150425","Corrections in the definition of MBMS Service Area AVP","Motorola Solutions Danmark A/S","Mathieu Mangion",27904,"CR","","","","176","12.42","CT aspects of Group Communication System Enablers for LTE [GCSE_LTE-CT]",2330,"Agreed","2015-02-10T16:31:14.073","2015-02-10T16:28:19.397","C3-150416","","Rel-12","29.061","12.8.0","GCSE_LTE-CT","0445","3","F","CP-150119","","","","",""]
["C3-150426","Adding UE location information in aggregated RUCI reporting","Huawei, China Telecom","Mathieu Mangion",27904,"pCR","","","","185","13.1","CT aspects of User Plane Congestion Management (UPCON) for Building Block I",934,"Revised","2015-02-10T16:31:14.220","2015-02-10T16:28:20.253","C3-150420","C3-150445","Rel-13","29.217","1.0.0","UPCON-DOTCON-CT","","","","","","","","",""]
["C3-150427","Clarifying the congestion level value in AVP defintion","Huawei, China Telecom","Mathieu Mangion",27904,"pCR","","","","185","13.1","CT aspects of User Plane Congestion Management (UPCON) for Building Block I",953,"Revised","2015-02-10T16:31:14.300","2015-02-10T16:28:21.107","C3-150393","C3-150441","Rel-13","29.217","1.0.0","UPCON-DOTCON-CT","","","","","","","","",""]
["C3-150428","Clarify the condition where the RCAF reports the RUCI","ZTE","Mathieu Mangion",27904,"pCR","","","","185","13.1","CT aspects of User Plane Congestion Management (UPCON) for Building Block I",1603,"Revised","2015-02-10T16:31:14.387","2015-02-10T16:28:21.980","C3-150394","C3-150437","Rel-13","29.217","1.0.0","UPCON-DOTCON-CT","","","","","","","","",""]
["C3-150429","Add the ToS-Traffic-Class AVP to the Rx to be sent by AF","Motorola Solutions Danmark A/S","Mathieu Mangion",27904,"CR","","","","198","13.12","CT aspects of Group Communication System Enablers for LTE [GCSE_LTE-CT]",37102,"Agreed","2015-02-10T16:31:14.470","2015-02-10T16:28:22.933","C3-150403","","Rel-13","29.214","13.0.0","TEI13, GCSE_LTE-CT","0394","2","B","CP-150133","","","","",""]
["C3-150430","Correction to the PRA reporting","ZTE","Mathieu Mangion",27904,"CR","","","","171","12.37","CT aspects of Core Network Overload  User Location Information reporting improvements [CNO_ULI-CT]",1593,"Agreed","2015-02-10T16:31:14.617","2015-02-10T16:28:24.607","C3-150422","","Rel-13","29.212","13.0.0","CNO_ULI-CT","1287","3","F","CP-150117","","","","",""]
["C3-150431","UE context removal in IP-CAN session termination procedure","Ericsson","Mathieu Mangion",27904,"CR","","","","185","13.1","CT aspects of User Plane Congestion Management (UPCON) for Building Block I",1972,"Agreed","2015-02-10T16:31:14.760","2015-02-10T16:28:25.480","C3-150318","","Rel-13","29.213","13.0.0","NWK-PL2IMS-CT, UPCON-DOTCON-CT","0596","2","B","CP-150125","","","","",""]
["C3-150432","Resolve the race conditions related to UE mobility between RCAFs","ZTE","Mathieu Mangion",27904,"pCR","","","","185","13.1","CT aspects of User Plane Congestion Management (UPCON) for Building Block I",1653,"Revised","2015-02-10T16:31:14.907","2015-02-10T16:28:27.127","C3-150395","C3-150438","Rel-13","29.217","1.0.0","UPCON-DOTCON-CT","","","","","","","","",""]
["C3-150433","LS on Flow ID supplied by AS  for GCSE","Nokia Networks","Mathieu Mangion",27904,"LS out","","","","176","12.42","CT aspects of Group Communication System Enablers for LTE [GCSE_LTE-CT]",43300,"Revised","2015-02-10T16:31:14.993","2015-02-10T16:28:28","","C3-150443","Rel-12","","","","","","","",null,"SA2"]
["C3-150434","Proposed Schedule for CT3#80","CT3 Chairman","Mathieu Mangion",27904,"other","","","","3","2.2","Proposed schedule",21,"Approved","2015-02-10T16:31:15.077",null,"C3-150002","","","","","","","","","","","","","",""]
["C3-150435","Relayed-Charge header field","Ericsson LM","Mathieu Mangion",27904,"CR","","","","146","12.14","IMS Stage-3 IETF Protocol Alignment  [IMSProtoc6]",1323,"Agreed","2015-02-10T16:31:15.170","2015-02-10T16:28:28.023","C3-150363","","Rel-12","29.165","12.6.0","IMSProtoc6","0725","3","F","CP-150108","","","","",""]
["C3-150436","Adding support for EVS codec","Nokia Networks","Mathieu Mangion",27904,"CR","","","","179","12.45","CT Impacts of Codec for Enhanced Voice Services [EVS_codec-CT]",2472,"Agreed","2015-02-10T16:31:15.313","2015-02-10T16:28:28.890","C3-150339","","Rel-13","29.163","13.0.0","EVS_codec-CT","0864","2","B","CP-150121","","","","",""]
["C3-150437","Clarify the condition where the RCAF reports the RUCI","ZTE","Mathieu Mangion",27904,"pCR","","","","185","13.1","CT aspects of User Plane Congestion Management (UPCON) for Building Block I",1604,"Agreed","2015-02-10T16:31:15.457","2015-02-10T16:28:29.807","C3-150428","","Rel-13","29.217","1.0.0","UPCON-DOTCON-CT","","","","","","","","",""]
["C3-150438","Resolve the race conditions related to UE mobility between RCAFs","ZTE","Mathieu Mangion",27904,"pCR","","","","185","13.1","CT aspects of User Plane Congestion Management (UPCON) for Building Block I",1654,"Agreed","2015-02-10T16:31:15.547","2015-02-10T16:28:30.677","C3-150432","","Rel-13","29.217","1.0.0","UPCON-DOTCON-CT","","","","","","","","",""]
["C3-150439","LS on new cause URI parameter value for IN numbers interworking","ORANGE","Mathieu Mangion",27904,"LS out","","","","192","13.8","Interworking of Called IN number and original Called IN number ISUP parameters",1423,"Approved","2015-02-10T16:31:15.630","2015-02-10T16:28:31.560","C3-150372","","Rel-13","","","INNB_IW","","","","",null,"SA5","CT1"]
["C3-150440","Applying drafting rules","Ericsson LM","Mathieu Mangion",27904,"CR","","","","194","13.9.1","TEI13 for IMS/CS",1333,"Agreed","2015-02-10T16:31:15.730","2015-02-10T16:28:32.320","C3-150373","","Rel-13","29.165","12.6.0","TEI13","0726","3","F","CP-150130","","","","",""]
["C3-150441","Clarifying the congestion level value in AVP defintion","Huawei, China Telecom","Mathieu Mangion",27904,"pCR","","","","185","13.1","CT aspects of User Plane Congestion Management (UPCON) for Building Block I",954,"Agreed","2015-02-10T16:31:15.870","2015-02-10T16:28:33.190","C3-150427","","Rel-13","29.217","1.0.0","UPCON-DOTCON-CT","","","","","","","","",""]
["C3-150442","Status of CT3 Work Items","CT3 Chairman","Mathieu Mangion",27904,"other","","","","201","15.1","Work Plan Review",111,"Noted","2015-02-10T16:31:15.953",null,"C3-150011","","","","","","","","","","","","","",""]
["C3-150443","LS on Flow ID supplied by AS  for GCSE","Nokia Networks","Mathieu Mangion",27904,"LS out","","","","176","12.42","CT aspects of Group Communication System Enablers for LTE [GCSE_LTE-CT]",43301,"Revised","2015-02-10T16:31:16.053","2015-02-10T16:28:34.080","C3-150433","C3-150446","Rel-12","","","GCSE_LTE-CT","","","","",null,"SA2"]
["C3-150444","Reply LS on End-to-end QoS handling of MTSI","Ericsson","Mathieu Mangion",27904,"LS out","","","","187","13.3","CT Aspects of End-to-End MTSI Extensions",1833,"Revised","2015-02-10T16:31:16.137","2015-02-10T16:28:34.833","C3-150399","C3-150447","","","","QOSE2EMTSI-CT","","","","","C3-150254","SA4","CT1, CT4, SA2"]
["C3-150445","Adding UE location information in aggregated RUCI reporting","Huawei, China Telecom","Mathieu Mangion",27904,"pCR","","","","185","13.1","CT aspects of User Plane Congestion Management (UPCON) for Building Block I",935,"Agreed","2015-02-10T16:31:16.217","2015-02-10T16:28:35.590","C3-150426","","Rel-13","29.217","1.0.0","UPCON-DOTCON-CT","","","","","","","","",""]
["C3-150446","LS on Flow ID supplied by GCS AS","Nokia Networks","Mathieu Mangion",27904,"LS out","","","","176","12.42","CT aspects of Group Communication System Enablers for LTE [GCSE_LTE-CT]",43302,"Approved","2015-02-10T16:31:16.310","2015-02-10T16:28:36.453","C3-150443","","Rel-12","","","GCSE_LTE-CT","","","","",null,"SA2"]
["C3-150447","Reply LS on End-to-end QoS handling of MTSI","Ericsson","Mathieu Mangion",27904,"LS out","","","","187","13.3","CT Aspects of End-to-End MTSI Extensions",1834,"Revised","2015-02-10T16:31:16.403","2015-02-10T16:28:37.217","C3-150444","C3-150450","","","","QOSE2EMTSI-CT","","","","","C3-150254","SA4","CT1, CT4, SA2"]
["C3-150448","Providing TS 29.217 v2.0.0","Huawei","Mathieu Mangion",27904,"other","","","","185","13.1","CT aspects of User Plane Congestion Management (UPCON) for Building Block I",44800,"Available","2015-02-10T16:31:16.493","2015-03-02T09:18:53.993","","","Rel-13","29.217","2.0.0","","","","","","","","","",""]
["C3-150449","Presentation sheet for TS 29.217","Huawei","Mathieu Mangion",27904,"other","","","","185","13.1","CT aspects of User Plane Congestion Management (UPCON) for Building Block I",44900,"Available","2015-02-10T16:31:16.540","2015-03-02T09:18:54.010","","","Rel-13","29.217","2.0.0","","","","","","","","","",""]
["C3-150450","Reply LS on End-to-end QoS handling of MTSI","Ericsson","Mathieu Mangion",27904,"LS out","","","","187","13.3","CT Aspects of End-to-End MTSI Extensions",1835,"Approved","2015-02-10T16:31:16.590",null,"C3-150447","","","","","QOSE2EMTSI-CT","","","","","C3-150254","SA4","CT1, CT4, SA2"]

{"sheet":"CR_Packs_List","index":1,"n_rows":1,"n_cols":11,"rows_kept":1,"cut":false,"hidden":false,"merged":[]}
["CR Pack TDoc #","WG TDoc #","WG TDoc decision","CR Individual TSG decision","Spec #","CR #","CR revision #","CR category","Release","Version","CR title"]

{"sheet":"Parameters","index":2,"n_rows":16,"n_cols":3,"rows_kept":16,"cut":false,"hidden":true,"merged":[]}
["Types of Tdocs","Possible statuses of Tdocs","Categories"]
[]
["agenda","Reserved","A"]
["LS in","Available","B"]
["LS out","Revised","C"]
["pCR","Approved","D"]
["CR","Agreed","E"]
["CR pack","Postponed","F"]
["WID","Noted"]
["WI status report","Rejected"]
["TS or TR","Withdrawn"]
["report","Treated"]
["other","Partially approved"]
[null,"Technically endorsed"]
[null,"Merged"]
[null,"Reissued"]