{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["TDoc_List","CR_Packs_List","Parameters"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":6,"comments":1,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"TDoc_List","index":0,"n_rows":404,"n_cols":32,"rows_kept":404,"cut":false,"hidden":false,"merged":[]}
["TDoc #","Title","Source","Contact","Contact ID","Type","Type supplement","For","Abstract","Secretary Remarks","Agenda item sort order","Agenda item #","Agenda item description","TDoc sort order within agenda item","TDoc Status","Reservation date","Uploaded","Is revision of","Revised to","Release","Spec #","Version","Related WIs","CR #","CR revision #","CR category","TSG CR Pack","Reply to","To","Cc","Original LS","Reply in"]
["C3-160000","Draft Agenda for the CT3#84 Meeting","CT3 chairman","Saurav Arora",62621,"agenda","","","","","2","2.1","Approval of the agenda",0,"revised","2016-01-12T10:36:38.540","2016-01-13T14:57:22.037","","C3-160016","","","","","","","","","","","","",""]
["C3-160001","INFO    Proposed Schedule for CT3#84","CT3 Chairman","Saurav Arora",62621,"other","","Information","","","3","2.2","Proposed Schedule",10,"revised","2016-01-12T10:36:38.540","2016-02-11T13:00:04.777","","C3-160309","","","","","","","","","","","","",""]
["C3-160002","Allocation of documents to agenda items (at Deadline)","CT3 Chairman","Saurav Arora",62621,"other","","Information","","","4","3","Registration of documents",20,"noted","2016-01-12T10:36:38.540","2016-02-14T11:41:09.860","","","","","","","","","","","","","","",""]
["C3-160003","Allocation of documents to agenda items (Start of Day 1)","CT3 Chairman","Saurav Arora",62621,"other","","Information","","","4","3","Registration of documents",30,"noted","2016-01-12T10:36:38.557","2016-02-11T13:00:04.790","","","","","","","","","","","","","","",""]
["C3-160004","Allocation of documents to agenda items (Start of Day 2)","CT3 Chairman","Saurav Arora",62621,"other","","Information","","","4","3","Registration of documents",40,"noted","2016-01-12T10:36:38.557","2016-03-01T15:03:19.087","","","","","","","","","","","","","","",""]
["C3-160005","Allocation of documents to agenda items (Start of Day 3)","CT3 Chairman","Saurav Arora",62621,"other","","Information","","","4","3","Registration of documents",50,"noted","2016-01-12T10:36:38.557","2016-03-01T15:03:19.103","","","","","","","","","","","","","","",""]
["C3-160006","Allocation of documents to agenda items (Start of Day 4)","CT3 Chairman","Saurav Arora",62621,"other","","Information","","","4","3","Registration of documents",60,"noted","2016-01-12T10:36:38.573","2016-03-01T15:03:19.103","","","","","","","","","","","","","","",""]
["C3-160007","Allocation of documents to agenda items (Start of Day 5)","CT3 Chairman","Saurav Arora",62621,"other","","Information","","","4","3","Registration of documents",70,"noted","2016-01-12T10:36:38.573","2016-03-01T15:03:19.103","","","","","","","","","","","","","","",""]
["C3-160008","Allocation of documents to agenda items (End of Day 5)","CT3 Chairman","Saurav Arora",62621,"other","","Information","","","4","3","Registration of documents",80,"noted","2016-01-12T10:36:38.573","2016-03-01T15:03:19.103","","","","","","","","","","","","","","",""]
["C3-160009","Summary of CT#70 related to CT3","CT3 Chairman","Saurav Arora",62621,"report","","","","","7","4.2","Report from previous CT plenary",90,"noted","2016-01-12T10:36:38.587","2016-02-01T08:53:23.423","","","","","","","","","","","","","","",""]
["C3-160010","Proposed Revision of CT3 ToR","CT3 Chairman","Saurav Arora",62621,"other","","Information","","","12","5.3","Other items for immediate consideration",100,"revised","2016-01-12T10:36:38.587","2016-02-01T08:53:23.470","","C3-160199","","","","","","","","","","","","",""]
["C3-160011","Status of CT3 Work Items","CT3 Chairman","Saurav Arora",62621,"Work Plan","","Information","","","236","15.1","Work Plan Review",110,"revised","2016-01-12T10:36:38.603","2016-02-01T08:53:23.517","","","","","","","","","","","","","","",""]
["C3-160012","Minutes of CT3#83","MCC","Saurav Arora",62621,"report","","","","","6","4.1","Report from previous CT3 meeting",120,"approved","2016-01-12T10:36:38.603","2016-01-29T10:46:29.517","","","","","","","","","","","","","","",""]
["C3-160013","WI status report  from MCC","MCC","Saurav Arora",62621,"Work Plan","","Information","","","236","15.1","Work Plan Review",130,"noted","2016-01-12T10:36:38.603","2016-01-29T10:46:29.627","","","","","","","","","","","","","","",""]
["C3-160014","Meeting Calendar","MCC","Saurav Arora",62621,"other","","Information","","","239","15.4","Calendar",140,"noted","2016-01-12T10:36:38.620","2016-01-29T10:46:29.657","","","","","","","","","","","","","","",""]
["C3-160015","TrGW configuration for end-to-end WebRTC calls (stage 2)","Alcatel-Lucent","Albrecht Schwarz",20164,"CR","","Agreement","","","216","13.25","Enhancements to WEBRTC interoperability stage 3 [eWebRTCi_CT]",150,"withdrawn","2016-01-12T11:07:15.177","2016-02-01T14:29:02.867","","","Rel-13","29.162","13.1.0","eWebRTCi-CT ","0148","","B",null,"","","","",""]
["C3-160016","Draft Agenda for the CT3#84 Meeting","CT3 chairman","Saurav Arora",62621,"agenda","","Information","","","2","2.1","Approval of the agenda",160,"approved","2016-01-13T09:51:36.817","2016-02-01T08:53:23.563","C3-160000","","","","","","","","","","","","","",""]
["C3-160017","Interworking of History-Info Header Field when Original Called Number is not present","Deutsche Telekom / Michael","Michael Kreipl",43940,"CR","","Agreement","When the MGC receives an ISUP IAM with a \"Redirection Information Parameter\" and a \"Redirecting Number Parameter\" but the \"Original Called Number Parameter\" is not included, the Call Diversion information is lost during the ISUP-SIP Interworking.","","15","8.2","Interworking between IM Subsystem with CS  [IMS-CCR-IWCS]",170,"revised","2016-01-21T08:45:23.787","2016-01-21T11:20:30.140","","C3-160221","Rel-8","29.163","8.29.0","IMS-CCR-IWCS","0948","","F",null,"","","","",""]
["C3-160018","Interworking of History-Info Header Field when Original Called Number is not present","Deutsche Telekom / Michael","Michael Kreipl",43940,"CR","","Agreement","When the MGC receives an ISUP IAM with a \"Redirection Information Parameter\" and a \"Redirecting Number Parameter\" but the \"Original Called Number Parameter\" is not included, the Call Diversion information is lost during the ISUP-SIP Interworking.","","15","8.2","Interworking between IM Subsystem with CS  [IMS-CCR-IWCS]",180,"revised","2016-01-21T08:45:23.943","2016-01-21T11:20:30.173","","C3-160222","Rel-9","29.163","9.23.0","IMS-CCR-IWCS","0949","","A",null,"","","","",""]
["C3-160019","Interworking of History-Info Header Field when Original Called Number is not present","Deutsche Telekom / Michael","Michael Kreipl",43940,"CR","","Agreement","When the MGC receives an ISUP IAM with a \"Redirection Information Parameter\" and a \"Redirecting Number Parameter\" but the \"Original Called Number Parameter\" is not included, the Call Diversion information is lost during the ISUP-SIP Interworking.","","15","8.2","Interworking between IM Subsystem with CS  [IMS-CCR-IWCS]",190,"revised","2016-01-21T08:45:24.037","2016-01-21T11:20:30.203","","C3-160223","Rel-10","29.163","10.19.0","IMS-CCR-IWCS","0950","","A",null,"","","","",""]
["C3-160020","Interworking of History-Info Header Field when Original Called Number is not present","Deutsche Telekom / Michael","Michael Kreipl",43940,"CR","","Agreement","When the MGC receives an ISUP IAM with a \"Redirection Information Parameter\" and a \"Redirecting Number Parameter\" but the \"Original Called Number Parameter\" is not included, the Call Diversion information is lost during the ISUP-SIP Interworking.","","15","8.2","Interworking between IM Subsystem with CS  [IMS-CCR-IWCS]",200,"revised","2016-01-21T08:45:24.130","2016-01-21T11:20:30.250","","C3-160224","Rel-11","29.163","11.16.0","IMS-CCR-IWCS","0951","","A",null,"","","","",""]
["C3-160021","Interworking of History-Info Header Field when Original Called Number is not present","Deutsche Telekom / Michael","Michael Kreipl",43940,"CR","","Agreement","When the MGC receives an ISUP IAM with a \"Redirection Information Parameter\" and a \"Redirecting Number Parameter\" but the \"Original Called Number Parameter\" is not included, the Call Diversion information is lost during the ISUP-SIP Interworking.","","15","8.2","Interworking between IM Subsystem with CS  [IMS-CCR-IWCS]",210,"revised","2016-01-21T08:45:24.223","2016-01-21T11:20:30.283","","C3-160225","Rel-12","29.163","12.10.0","IMS-CCR-IWCS","0952","","A",null,"","","","",""]
["C3-160022","Interworking of History-Info Header Field when Original Called Number is not present","Deutsche Telekom / Michael","Michael Kreipl",43940,"CR","","Agreement","When the MGC receives an ISUP IAM with a \"Redirection Information Parameter\" and a \"Redirecting Number Parameter\" but the \"Original Called Number Parameter\" is not included, the Call Diversion information is lost during the ISUP-SIP Interworking.","","15","8.2","Interworking between IM Subsystem with CS  [IMS-CCR-IWCS]",220,"revised","2016-01-21T08:45:24.317","2016-01-21T11:20:30.330","","C3-160226","Rel-13","29.163","13.4.0","IMS-CCR-IWCS","0953","","A",null,"","","","",""]
["C3-160023","Discussion on early media in interconnection case","NTT","Kenjiro Arai",44174,"discussion","","Discussion","This contribution is trying to discuss the issues related to early media traversing the II-NNI.","","198","13.7","IMS Stage-3 IETF Protocol Alignment [IMSProtoc7]",230,"noted","2016-01-26T02:45:49.193","2016-02-01T08:30:33.750","","","Rel-13","","","IMSProtoc7","","","","","","","","",""]
["C3-160024","Draft references in CT3 specifications","Ericsson","Nevenka Biondic",41878,"other","","Information","This document shows IETF draft references in CT3 technical specifications.","","12","5.3","Other items for immediate consideration",240,"noted","2016-01-26T12:56:38.230","2016-02-01T10:21:04.957","","","","","","","","","","","","","","",""]
["C3-160025","Multi-stream Multiparty Conferencing Media Handling","Ericsson","Nevenka Biondic",41878,"discussion","","Discussion","The purpose of this discussion paper is to present an initial analysis of the updates required in CT WGs specifications to enable Multi-stream Multiparty Conferencing Media Handling (MMCMH), and to propose a way forward on the introduction of Multi-stream","","229","14.2","CT aspects of MTSI Extension on Multi-stream Multiparty Conferencing Media Handling [MMCMH-CT]",250,"noted","2016-01-26T12:56:38.247","2016-02-01T10:21:04.987","","","Rel-14","","","","","","","","","","","",""]
["C3-160026","CT aspects of MTSI Extension on Multi-stream Multiparty Conferencing Media Handling","Ericsson","Nevenka Biondic",41878,"WID new","","Agreement","The objective of this work item is to add an optional support for the MTSI extension on Multi-stream Multiparty Conferencing Media Handling to the specifications under CT WGs responsibility.","","229","14.2","CT aspects of MTSI Extension on Multi-stream Multiparty Conferencing Media Handling [MMCMH-CT]",260,"revised","2016-01-26T12:56:38.247","2016-02-01T10:21:05.020","","C3-160212","Rel-14","","","","","","","","","","","",""]
["C3-160027","Bandwidth adjustment for EVS codec","Ericsson","Nevenka Biondic",41878,"CR","","Agreement","Information about bandwidths adjustment for EVS codec if IBCF performs IP version interworking.","","222","13.30.1","TEI13 for IMS/CS",270,"agreed","2016-01-26T12:56:38.247","2016-02-01T10:21:05.067","","","Rel-13","29.162","13.1.0","TEI13","0149","","F","CP-160105","","","","",""]
["C3-160028","Support of enhanced bandwidth negotiation mechanism for MTSI sessions","Ericsson","Nevenka Biondic",41878,"CR","","Agreement","Specification of Ix procedures (stage 2) to support the enhanced bandwidth negotiation mechanism.","","194","13.3","CT Aspects of QoS End to End MTSI extensions [QOSE2EMTSI-CT]",280,"revised","2016-01-26T12:56:38.323","2016-02-01T10:21:05.113","","C3-160231","Rel-13","29.162","13.1.0","QOSE2EMTSI-CT","0150","","B",null,"","","","",""]
["C3-160029","Support of enhanced bandwidth negotiation mechanism for MTSI sessions","Ericsson","Nevenka Biondic",41878,"CR","","Agreement","Specification of Ix procedures (stage 2) to support the enhanced bandwidth negotiation mechanism.","","194","13.3","CT Aspects of QoS End to End MTSI extensions [QOSE2EMTSI-CT]",290,"revised","2016-01-26T12:56:38.400","2016-02-01T10:21:04.927","","C3-160232","Rel-13","29.163","13.4.0","QOSE2EMTSI-CT","0954","","B",null,"","","","",""]
["C3-160030","Adding MBMS usage info and location info procedure","Ericsson","Jan Holm",12624,"CR","","Agreement","","","215","13.24","Mission Critical Push To Talk over LTE protocol aspects [MCPTT-CT]",300,"revised","2016-01-26T14:11:20.317","2016-02-08T11:15:57.197","","C3-160321","Rel-13","29.165","13.3.0","MCPTT-CT","0813","","B",null,"","","","",""]
["C3-160031","Adding \"application/vnd.3gpp.mcptt-info\" MIME body","Ericsson","Jan Holm",12624,"CR","","Agreement","","","215","13.24","Mission Critical Push To Talk over LTE protocol aspects [MCPTT-CT]",310,"revised","2016-01-26T14:14:58.340","2016-02-08T11:15:57.247","","C3-160322","Rel-13","29.165","13.3.0","MCPTT-CT","0814","","F",null,"","","","",""]
["C3-160032","Adding MCPTT as option item in annex C","Ericsson","Jan Holm",12624,"CR","","Agreement","","","215","13.24","Mission Critical Push To Talk over LTE protocol aspects [MCPTT-CT]",320,"revised","2016-01-26T14:17:41.640","2016-02-08T11:15:57.293","","C3-160323","Rel-13","29.165","13.3.0","MCPTT-CT","0815","","B",null,"","","","",""]
["C3-160033","Adding affiliation","Ericsson","Jan Holm",12624,"CR","","Agreement","","","215","13.24","Mission Critical Push To Talk over LTE protocol aspects [MCPTT-CT]",330,"revised","2016-01-26T14:20:55.373","2016-02-08T11:15:57.337","","C3-160324","Rel-13","29.165","13.3.0","MCPTT-CT","0816","","B",null,"","","","",""]
["C3-160034","Withdrawn","Ericsson","Jan Holm",12624,"draftCR","","Agreement","","","198","13.7","IMS Stage-3 IETF Protocol Alignment [IMSProtoc7]",340,"withdrawn","2016-01-26T14:25:01.370",null,"","","Rel-13","29.002","13.2.0","IMSProtoc7","","",null,"","","","","",""]
["C3-160035","Adding \"Timer N\" in the timer table","Ericsson","Jan Holm",12624,"CR","","Agreement","","","198","13.7","IMS Stage-3 IETF Protocol Alignment [IMSProtoc7]",350,"revised","2016-01-26T14:28:10.067","2016-01-31T18:09:38.383","","C3-160275","Rel-13","29.165","13.3.0","IMSProtoc7","0817","","F",null,"","","","",""]
["C3-160036","Updating \"Details for operator choice\" in DRVCC to include the STN","Ericsson","Jan Holm",12624,"CR","","Agreement","","","162","12.9","Dual-Radio VCC Enhancements [eDRVCC]",360,"revised","2016-01-26T14:31:53.143","2016-01-31T18:09:38.417","","C3-160228","Rel-12","29.165","12.10.0","eDRVCC","0818","","F",null,"","","","",""]
["C3-160037","Updating \"Details for operator choice\" in DRVCC to include the STN","Ericsson","Jan Holm",12624,"CR","","Agreement","","","162","12.9","Dual-Radio VCC Enhancements [eDRVCC]",370,"revised","2016-01-26T14:35:11.183","2016-01-31T18:09:38.460","","C3-160229","Rel-13","29.165","13.3.0","eDRVCC","0819","","A",null,"","","","",""]
["C3-160038","Format of Type 1 orig-ioi and term-ioi","Ericsson","Jan Holm",12624,"CR","","Agreement","","","222","13.30.1","TEI13 for IMS/CS",380,"revised","2016-01-26T14:39:19.910","2016-01-31T18:09:38.507","","C3-160280","Rel-13","29.165","13.3.0","TEI13","0820","","F",null,"","","","",""]
["C3-160039","Coding of type 1 and type orig-ioi and term-ioi","Ericsson","Jan Holm",12624,"CR","","Agreement","","","222","13.30.1","TEI13 for IMS/CS",390,"revised","2016-01-26T14:41:58.093","2016-01-31T18:09:38.540","","C3-160281","Rel-13","29.949","13.3.0","TEI13","0011","","F",null,"","","","",""]
["C3-160040","eProSe-Ext-CT impacts","Qualcomm Incorporated","Lena Chaponniere",38080,"discussion","","Discussion","The purpose of this contribution is to provide an analysis of the work left to complete in each CT WG to develop the stage 3 for the stage 2 solutions agreed under the SA2","","206","13.15","CT aspects of enhancements to Proximity-based Services extensions [eProSe-Ext-CT]",400,"noted","2016-01-28T00:43:26.083","2016-01-29T22:54:17.290","","","Rel-13","","","eProSe-Ext-CT","","","","","","","","",""]
["C3-160041","Resolution of Editor’s notes on EVS over UMTS CS","Qualcomm Incorporated","Lena Chaponniere",38080,"CR","","Agreement","","","201","13.10","CT aspects of EVS in 3G Circuit-Switched Networks [EVSoCS-CT]",410,"revised","2016-01-28T00:46:36.370","2016-01-29T22:53:54.093","","C3-160276","Rel-13","29.163","13.4.0","EVSoCS-CT","0955","","B",null,"","","","",""]
["C3-160042","Resolution of Editor’s notes on EVS over UMTS CS","Qualcomm Incorporated","Lena Chaponniere",38080,"CR","","Agreement","","","201","13.10","CT aspects of EVS in 3G Circuit-Switched Networks [EVSoCS-CT]",420,"revised","2016-01-28T00:48:50.827","2016-01-29T22:53:54.140","","C3-160277","Rel-13","29.414","13.0.0","EVSoCS-CT","0040","","B",null,"","","","",""]
["C3-160043","Resolution of Editor’s notes on EVS over UMTS CS","Qualcomm Incorporated","Lena Chaponniere",38080,"CR","","Agreement","","","201","13.10","CT aspects of EVS in 3G Circuit-Switched Networks [EVSoCS-CT]",430,"revised","2016-01-28T00:50:49.027","2016-01-29T22:53:54.170","","C3-160278","Rel-13","29.415","13.0.0","EVSoCS-CT","0018","","B",null,"","","","",""]
["C3-160044","Correction for the SIP-ISUP interworking parameter","FUJITSU, NTT","Tatsuya Toyama",59400,"CR","","Agreement","The interworking parameter about the SIP cause URI parameter to the ISUP Call Diversion Information is unclear in table 7.5.4.2.1.4. It should be corrected.","","15","8.2","Interworking between IM Subsystem with CS  [IMS-CCR-IWCS]",440,"withdrawn","2016-01-28T04:26:26.960","2016-02-01T11:04:03.120","","","Rel-8","29.163","8.29.0","IMS-CCR-IWCS","0956","","F",null,"","","","",""]
["C3-160045","Correction for the SIP-ISUP interworking parameter","FUJITSU, NTT","Tatsuya Toyama",59400,"CR","","Agreement","The interworking parameter about the SIP cause URI parameter to the ISUP Call Diversion Information is unclear in table 7.5.4.2.1.4. It should be corrected.","","15","8.2","Interworking between IM Subsystem with CS  [IMS-CCR-IWCS]",450,"withdrawn","2016-01-28T04:35:12.927","2016-02-01T11:04:03.153","","","Rel-9","29.163","9.23.0","IMS-CCR-IWCS","0957","","A",null,"","","","",""]
["C3-160046","Correction for the SIP-ISUP interworking parameter","FUJITSU, NTT","Tatsuya Toyama",59400,"CR","","Agreement","The interworking parameter about the SIP cause URI parameter to the ISUP Call Diversion Information is unclear in table 7.5.4.2.1.4. It should be corrected.","","15","8.2","Interworking between IM Subsystem with CS  [IMS-CCR-IWCS]",460,"withdrawn","2016-01-28T04:38:22.730","2016-02-01T11:04:03.183","","","Rel-10","29.163","10.19.0","IMS-CCR-IWCS","0958","","A",null,"","","","",""]
["C3-160047","Correction for the SIP-ISUP interworking parameter","FUJITSU, NTT","Tatsuya Toyama",59400,"CR","","Agreement","The interworking parameter about the SIP cause URI parameter to the ISUP Call Diversion Information is unclear in table 7.5.4.2.1.4. It should be corrected.","","15","8.2","Interworking between IM Subsystem with CS  [IMS-CCR-IWCS]",470,"withdrawn","2016-01-28T04:41:46.263","2016-02-01T11:04:03.213","","","Rel-11","29.163","11.16.0","IMS-CCR-IWCS","0959","","A",null,"","","","",""]
["C3-160048","Correction for the SIP-ISUP interworking parameter","FUJITSU, NTT","Tatsuya Toyama",59400,"CR","","Agreement","The interworking parameter about the SIP cause URI parameter to the ISUP Call Diversion Information is unclear in table 7.5.4.2.1.4. It should be corrected.","","15","8.2","Interworking between IM Subsystem with CS  [IMS-CCR-IWCS]",480,"withdrawn","2016-01-28T04:46:15.813","2016-02-01T11:04:03.247","","","Rel-12","29.163","12.10.0","IMS-CCR-IWCS","0960","","A",null,"","","","",""]
["C3-160049","Correction for the SIP-ISUP interworking parameter","FUJITSU, NTT","Tatsuya Toyama",59400,"CR","","Agreement","The interworking parameter about the SIP cause URI parameter to the ISUP Call Diversion Information is unclear in table 7.5.4.2.1.4. It should be corrected.","","15","8.2","Interworking between IM Subsystem with CS  [IMS-CCR-IWCS]",490,"revised","2016-01-28T04:48:45.777","2016-02-01T11:04:03.277","","C3-160227","Rel-13","29.163","13.4.0","IMS-CCR-IWCS","0961","","A",null,"","","","",""]
["C3-160050","Correction of the incorrect ISUP parameter name","FUJITSU, NTT","Tatsuya Toyama",59400,"CR","","Agreement","In Table 7.5.4.2.2.1 and Table 7.5.4.3.3 at TS 29.163, there are some incorrect ISUP parameter name. It should be corrected.","","15","8.2","Interworking between IM Subsystem with CS  [IMS-CCR-IWCS]",500,"withdrawn","2016-01-28T04:55:45.723","2016-02-01T11:04:03.307","","","Rel-8","29.163","8.29.0","IMS-CCR-IWCS","0962","","F",null,"","","","",""]
["C3-160051","Correction of the incorrect ISUP parameter name","FUJITSU, NTT","Tatsuya Toyama",59400,"CR","","Agreement","In Table 7.5.4.2.2.1 and Table 7.5.4.3.3 at TS 29.163, there are some incorrect ISUP parameter name. It should be corrected.","","15","8.2","Interworking between IM Subsystem with CS  [IMS-CCR-IWCS]",510,"withdrawn","2016-01-28T04:57:51.443","2016-02-01T11:04:03.357","","","Rel-9","29.163","9.23.0","IMS-CCR-IWCS","0963","","A",null,"","","","",""]
["C3-160052","Correction of the incorrect ISUP parameter name","FUJITSU, NTT","Tatsuya Toyama",59400,"CR","","Agreement","In Table 7.5.4.2.2.1 and Table 7.5.4.3.3 at TS 29.163, there are some incorrect ISUP parameter name. It should be corrected.","","15","8.2","Interworking between IM Subsystem with CS  [IMS-CCR-IWCS]",520,"withdrawn","2016-01-28T04:59:33.857","2016-02-01T11:04:03.387","","","Rel-10","29.163","10.19.0","IMS-CCR-IWCS","0964","","A",null,"","","","",""]
["C3-160053","Correction of the incorrect ISUP parameter name","FUJITSU, NTT","Tatsuya Toyama",59400,"CR","","Agreement","In Table 7.5.4.2.2.1 and Table 7.5.4.3.3 at TS 29.163, there are some incorrect ISUP parameter name. It should be corrected.","","15","8.2","Interworking between IM Subsystem with CS  [IMS-CCR-IWCS]",530,"withdrawn","2016-01-28T05:01:06.847","2016-02-01T11:04:03.417","","","Rel-11","29.163","11.16.0","IMS-CCR-IWCS","0965","","A",null,"","","","",""]
["C3-160054","Correction of the incorrect ISUP parameter name","FUJITSU, NTT","Tatsuya Toyama",59400,"CR","","Agreement","In Table 7.5.4.2.2.1 and Table 7.5.4.3.3 at TS 29.163, there are some incorrect ISUP parameter name. It should be corrected.","","15","8.2","Interworking between IM Subsystem with CS  [IMS-CCR-IWCS]",540,"withdrawn","2016-01-28T05:02:49.307","2016-02-01T11:04:03.463","","","Rel-12","29.163","12.10.0","IMS-CCR-IWCS","0966","","A",null,"","","","",""]
["C3-160055","Clarification on the setting of the hostportion of SIP URI","NTT","Yoshihiro Inoue",44190,"CR","","Agreement","This CR is to clarify that details how to set the hostportion of SIP URI is outside the scope of TS 29.163.","","222","13.30.1","TEI13 for IMS/CS",550,"revised","2016-01-28T08:18:49.073","2016-01-29T04:02:21.187","","C3-160282","Rel-13","29.163","13.4.0","TEI13, IMS-CCR-IWCS","0967","","F",null,"","","","",""]
["C3-160056","Completion of NBIFOM","Ericsson","Sven-ove Emanuelsson",45992,"CR","","Agreement","","","205","13.14","CT aspects of IP Flow Mobility support for S2a and S2b Interfaces (NBIFOM) [NBIFOM-CT]",560,"revised","2016-01-29T06:45:29.500","2016-02-01T09:53:38.200","","C3-160310","Rel-13","29.212","13.4.0","NBIFOM-CT","1405","","B",null,"","","","",""]
["C3-160057","Time conditioned APN-AMBR handling","Ericsson","Sven-ove Emanuelsson",45992,"CR","","Agreement","","","223","13.30.2","TEI13 for Packet Core",570,"revised","2016-01-29T06:51:47.907","2016-02-01T09:53:38.230","","C3-160294","Rel-13","29.212","13.4.0","TEI13, PCC","1406","","B",null,"","","","",""]
["C3-160058","Support for Non-IP data for CIoT over Sgi","Ericsson","Sven-ove Emanuelsson",45992,"CR","","Agreement","","","220","13.29","CT Aspects of Architecture enhancements for Cellular Internet of Things [CIoT-CT]",580,"agreed","2016-01-29T06:57:34.443","2016-02-01T09:53:38.263","","","Rel-13","29.061","13.2.0","CIoT-CT","0460","","B","CP-160108","","","","",""]
["C3-160059","New WID Representational State Transfer (REST) reference point between Service Capability Exposure Function (SCEF) and Protocol Converter (PC)","ZTE Corporation","Xiaoyun Zhou",38525,"WID new","","Approval","","","230","14.3","Representational State Transfer (REST) reference point between Service Capability Exposure Function (SCEF) and Protocol Converter (PC) [REST_SCEF_PC]",590,"revised","2016-01-29T09:03:08.430","2016-02-01T06:56:06.807","","C3-160210","","","","","","","","","","","","",""]
["C3-160060","New WID Representational State Transfer (REST) reference point between Application Function (AF) and Protocol Converter (PC) enhancement","ZTE Corporation","Xiaoyun Zhou",38525,"WID new","","Endorsement","","","231","14.4","Representational State Transfer (REST) reference point between Application Function (AF) and Protocol Converter (PC) Enhancement [REST_AF_PC_En]",600,"noted","2016-01-29T09:04:02.297","2016-02-01T07:25:07.943","","","","","","","","","","","","","","",""]
["C3-160061","Vendor-Specific-Application-Id AVP for S9/S9a commands","ZTE","Xiaoyun Zhou",38525,"CR","","Agreement","Correct Vendor-Specific-Application-Id AVP for S9/S9a commands","","137","11.24","Support for BroadBand Forum Accesses Interworking, Core Network Impacts, Building Block I [BBAI_BBI-CT]",610,"withdrawn","2016-01-29T09:06:57.063","2016-02-01T07:25:07.990","","","Rel-11","29.215","11.16.0","BBAI_BBI-CT","0396","","F",null,"","","","",""]
["C3-160062","Vendor-Specific-Application-Id AVP for S9/S9a commands","ZTE","Xiaoyun Zhou",38525,"CR","","Agreement","Correct Vendor-Specific-Application-Id AVP for S9/S9a commands","","137","11.24","Support for BroadBand Forum Accesses Interworking, Core Network Impacts, Building Block I [BBAI_BBI-CT]",620,"withdrawn","2016-01-29T09:06:57.220","2016-02-01T07:25:08.020","","","Rel-12","29.215","12.8.0","BBAI_BBI-CT","0397","","A",null,"","","","",""]
["C3-160063","Vendor-Specific-Application-Id AVP for S9/S9a commands","ZTE","Xiaoyun Zhou",38525,"CR","","Agreement","Correct Vendor-Specific-Application-Id AVP for S9/S9a commands","","137","11.24","Support for BroadBand Forum Accesses Interworking, Core Network Impacts, Building Block I [BBAI_BBI-CT]",630,"withdrawn","2016-01-29T09:06:57.313","2016-02-01T07:25:08.067","","","Rel-13","29.215","13.4.0","BBAI_BBI-CT","0398","","A",null,"","","","",""]
["C3-160064","Capability of REST-Rx","ZTE","Xiaoyun Zhou",38525,"CR","","Agreement","Clarify the capability of REST-Rx","","161","12.8.1","Representational State Transfer (REST) reference point between Application Function (AF) and Protocol Converter (PC) [REST_AF_PC]",640,"revised","2016-01-29T09:06:57.423","2016-02-01T07:25:08.100","","C3-160233","Rel-12","29.201","12.3.0","REST_AF_PC","0033","","F",null,"","","","",""]
["C3-160065","Capability of REST-Rx","ZTE","Xiaoyun Zhou",38525,"CR","","Agreement","Clarify the capability of REST-Rx","","161","12.8.1","Representational State Transfer (REST) reference point between Application Function (AF) and Protocol Converter (PC) [REST_AF_PC]",650,"revised","2016-01-29T09:06:57.500","2016-02-01T07:25:08.147","","C3-160234","Rel-13","29.201","13.3.0","REST_AF_PC","0034","","A",null,"","","","",""]
["C3-160066","Application id, command codes and AVP codes","ZTE","Xiaoyun Zhou",38525,"CR","","Agreement","Allocates Application id, command codes and AVP codes","","192","13.1","CT aspects of User Plane Congestion Management (UPCON) for Building Block I [UPCON-DOTCON-CT]",660,"merged","2016-01-29T09:06:57.610","2016-02-01T07:25:43.993","","","Rel-13","29.217","13.2.0","UPCON-DOTCON-CT","0020","","B",null,"","","","",""]
["C3-160067","Include RCAF in the EPC-routed architecture","ZTE","Xiaoyun Zhou",38525,"CR","","Agreement","Include RCAF in the EPC-routed architecture","","192","13.1","CT aspects of User Plane Congestion Management (UPCON) for Building Block I [UPCON-DOTCON-CT]",670,"revised","2016-01-29T09:06:57.703","2016-02-01T07:25:44.040","","C3-160315","Rel-13","29.212","13.4.0","UPCON-DOTCON-CT","1407","","F",null,"","","","",""]
["C3-160068","Include RCAF in the EPC-routed architecture","ZTE","Xiaoyun Zhou",38525,"CR","","Agreement","Include RCAF in the EPC-routed architecture","","192","13.1","CT aspects of User Plane Congestion Management (UPCON) for Building Block I [UPCON-DOTCON-CT]",680,"merged","2016-01-29T09:06:57.797","2016-02-01T07:25:44.087","","","Rel-13","29.215","13.4.0","UPCON-DOTCON-CT","0399","","B",null,"","","","",""]
["C3-160069","Support for UE requested IP Flow Mapping","ZTE","Xiaoyun Zhou",38525,"CR","","Agreement","Defines the procedure of support for UE requested IP Flow Mapping","","205","13.14","CT aspects of IP Flow Mobility support for S2a and S2b Interfaces (NBIFOM) [NBIFOM-CT]",690,"merged","2016-01-29T09:06:57.907","2016-02-01T07:25:44.133","","","Rel-13","29.212","13.4.0","NBIFOM-CT","1408","","B",null,"","","","",""]
["C3-160070","Network-initiated removal of one access from the PDN connection","ZTE","Xiaoyun Zhou",38525,"CR","","Agreement","PCRF initiates the removal of one access from the PDN connection","","205","13.14","CT aspects of IP Flow Mobility support for S2a and S2b Interfaces (NBIFOM) [NBIFOM-CT]",700,"revised","2016-01-29T09:06:58","2016-02-01T07:25:44.167","","C3-160311","Rel-13","29.212","13.4.0","NBIFOM-CT","1409","","F",null,"","","","",""]
["C3-160071","Network-initiated removal of one access from the PDN connection","ZTE","Xiaoyun Zhou",38525,"CR","","Agreement","PCRF initiates the removal of one access from the PDN connection","","205","13.14","CT aspects of IP Flow Mobility support for S2a and S2b Interfaces (NBIFOM) [NBIFOM-CT]",710,"agreed","2016-01-29T09:06:58.107","2016-02-01T07:26:13.383","","","Rel-13","29.213","13.4.0","NBIFOM-CT","0638","","F","CP-160107","","","","",""]
["C3-160072","REST-Rx enhancement for Change of chargeable party","ZTE","Xiaoyun Zhou",38525,"CR","","Agreement","Defines the procedure of Change of chargeable party in REST-Rx","","207","13.16","CT aspects of Architecture Enhancements for Service Capability Exposure [AESE-CT]",720,"revised","2016-01-29T09:06:58.203","2016-02-01T07:26:13.430","","C3-160265","Rel-13","29.201","13.3.0","AESE-CT","0035","","B",null,"","","","",""]
["C3-160073","Rx impact for background data transfer","ZTE","Xiaoyun Zhou",38525,"CR","","Agreement","Defines the procedure of support for backgroud data transfer","","207","13.16","CT aspects of Architecture Enhancements for Service Capability Exposure [AESE-CT]",730,"revised","2016-01-29T09:06:58.310","2016-02-01T07:26:13.463","","C3-160266","Rel-13","29.214","13.4.0","AESE-CT","0435","","B",null,"","","","",""]
["C3-160074","Rx impact for background data transfer","ZTE","Xiaoyun Zhou",38525,"CR","","Agreement","Defines the procedure of support for backgroud data transfer","","207","13.16","CT aspects of Architecture Enhancements for Service Capability Exposure [AESE-CT]",740,"revised","2016-01-29T09:06:58.407","2016-02-01T07:26:13.527","","C3-160267","Rel-13","29.201","13.3.0","AESE-CT","0036","","B",null,"","","","",""]
["C3-160075","ADC rule error handling report initiated by the TSSF","ZTE","Xiaoyun Zhou",38525,"CR","","Agreement","Defines the procedure of ADC rule error handling report initiated by the TSSF","","211","13.20","CT3 Aspect of Flexible Mobile Service Steering [FMSS-CT]",750,"merged","2016-01-29T09:06:58.497","2016-02-01T07:26:13.570","","","Rel-13","29.212","13.4.0","FMSS-CT","1410","","B",null,"","","","",""]
["C3-160076","ADC rule error handling report initiated by the TSSF","ZTE","Xiaoyun Zhou",38525,"CR","","Agreement","Defines the procedure of ADC rule error handling report initiated by the TSSF","","211","13.20","CT3 Aspect of Flexible Mobile Service Steering [FMSS-CT]",760,"revised","2016-01-29T09:06:58.593","2016-02-01T07:28:20.210","","C3-160217","Rel-13","29.213","13.4.0","FMSS-CT","0639","","B",null,"","","","",""]
["C3-160077","IPv4 address provisioning","ZTE","Xiaoyun Zhou",38525,"CR","","Agreement","Defines the procedure of IP address provisioning","","211","13.20","CT3 Aspect of Flexible Mobile Service Steering [FMSS-CT]",770,"revised","2016-01-29T09:06:58.687","2016-02-01T07:28:20.257","","C3-160218","Rel-13","29.212","13.4.0","FMSS-CT","1411","","B",null,"","","","",""]
["C3-160078","IPv4 address provisioning","ZTE","Xiaoyun Zhou",38525,"CR","","Agreement","Defines the procedure of IP address provisioning","","211","13.20","CT3 Aspect of Flexible Mobile Service Steering [FMSS-CT]",780,"agreed","2016-01-29T09:06:58.780","2016-02-01T07:28:20.307","","","Rel-13","29.213","13.4.0","FMSS-CT","0640","","F","CP-160091","","","","",""]
["C3-160079","Include TSSF in the EPC-routed architecture","ZTE","Xiaoyun Zhou",38525,"CR","","Agreement","Include TSSF in the EPC-routed architecture","","211","13.20","CT3 Aspect of Flexible Mobile Service Steering [FMSS-CT]",790,"revised","2016-01-29T09:06:58.857","2016-02-01T08:06:39.917","","C3-160316","Rel-13","29.215","13.4.0","FMSS-CT","0400","","B",null,"","","","",""]
["C3-160080","REST-Rx enhancment for NetLoc-Untrusted-WLAN","ZTE","Xiaoyun Zhou",38525,"CR","","Agreement","Enhances the REST-Rx to support NetLoc-Untrusted-WLAN","","212","13.21","CT aspects of Support of Emergency services over WLAN - phase 1 [SEW1-CT]",800,"revised","2016-01-29T09:06:58.950","2016-02-01T07:28:20.337","","C3-160330","Rel-13","29.201","13.3.0","SEW1-CT","0037","","B",null,"","","","",""]
["C3-160081","Include the AN-Trusted element","ZTE","Xiaoyun Zhou",38525,"CR","","Agreement","Includes the AN-Trusted element in REST-Rx","","223","13.30.2","TEI13 for Packet Core",810,"revised","2016-01-29T09:06:59.030","2016-02-01T07:28:20.383","","C3-160297","Rel-13","29.201","13.3.0","TEI13","0038","","B",null,"","","","",""]
["C3-160082","ICSI format specification over Rx","Ericsson LM","Susana Fernandez",42321,"CR","","Agreement","","","223","13.30.2","TEI13 for Packet Core",820,"agreed","2016-01-29T10:19:04.117","2016-01-29T12:10:34.170","","","Rel-13","29.214","13.4.0","PCC, TEI13","0436","","F","CP-160101","","","","",""]
["C3-160083","Add missing abbreviations","Huawei","Yizhuang Wu",61155,"CR","","Agreement","This contribution proposes to add the missing abbreviations.","","192","13.1","CT aspects of User Plane Congestion Management (UPCON) for Building Block I [UPCON-DOTCON-CT]",830,"withdrawn","2016-01-29T10:25:44.300",null,"","","Rel-13","29.217","13.2.0","UPCON-DOTCON-CT","0021","","F",null,"","","","",""]
["C3-160084","Congestion Level for the specific user id","Huawei","Yizhuang Wu",61155,"CR","","Agreement","Congestion level for specific UE is revised to specific user id.","","192","13.1","CT aspects of User Plane Congestion Management (UPCON) for Building Block I [UPCON-DOTCON-CT]",840,"revised","2016-01-29T10:25:44.397","2016-02-01T10:08:38.003","","C3-160317","Rel-13","29.217","13.2.0","UPCON-DOTCON-CT","0022","","F",null,"","","","",""]
["C3-160085","Add command codes and AVP numbers for Np protocol","Huawei","Yizhuang Wu",61155,"CR","","Agreement","This contribution proposes to add the allocated AVP codes and command codes.","","192","13.1","CT aspects of User Plane Congestion Management (UPCON) for Building Block I [UPCON-DOTCON-CT]",850,"revised","2016-01-29T10:25:44.503","2016-02-01T10:08:38.033","","C3-160314","Rel-13","29.217","13.2.0","UPCON-DOTCON-CT","0023","","F",null,"","","","",""]
["C3-160086","Add the missing abbreviations","Huawei","Yizhuang Wu",61155,"CR","","Agreement","This contribution proposes to add the missing abbreviations and revises several editoral errors.","","207","13.16","CT aspects of Architecture Enhancements for Service Capability Exposure [AESE-CT]",860,"revised","2016-01-29T10:25:44.567","2016-02-01T10:08:38.067","","C3-160268","Rel-13","29.153","13.0.0","AESE-CT","0001","","F",null,"","","","",""]
["C3-160087","Removal of the Ens in subclause 5.5","Huawei","Yizhuang Wu",61155,"CR","","Agreement","This contribution proposes to delete the useless Ens in subcluase 5.5.","","207","13.16","CT aspects of Architecture Enhancements for Service Capability Exposure [AESE-CT]",870,"agreed","2016-01-29T10:25:44.643","2016-02-01T10:08:38.110","","","Rel-13","29.153","13.0.0","AESE-CT","0002","","F","CP-160095","","","","",""]
["C3-160088","Add command codes and AVP numbers for Ns protocol","Huawei","Yizhuang Wu",61155,"CR","","Agreement","This contribution proposes to add the allocated AVP codes and command codes.","","207","13.16","CT aspects of Architecture Enhancements for Service Capability Exposure [AESE-CT]",880,"agreed","2016-01-29T10:25:44.707","2016-02-01T10:08:38.143","","","Rel-13","29.153","13.0.0","AESE-CT","0003","","F","CP-160095","","","","",""]
["C3-160089","Signnalling flows over Ns reference point","Huawei","Yizhuang Wu",61155,"CR","","Agreement","This CR proposes to add the information flows over Ns reference point.","","207","13.16","CT aspects of Architecture Enhancements for Service Capability Exposure [AESE-CT]",890,"revised","2016-01-29T10:25:44.770","2016-02-01T10:08:38.190","","C3-160269","Rel-13","29.153","13.0.0","AESE-CT","0004","","F",null,"","","","",""]
["C3-160090","Add command codes and AVP numbers for Nt protocol","Huawei","Yizhuang Wu",61155,"CR","","Agreement","This contribution proposes to add the allocated AVP codes and command codes.","","207","13.16","CT aspects of Architecture Enhancements for Service Capability Exposure [AESE-CT]",900,"revised","2016-01-29T10:25:44.847","2016-02-01T10:08:38.220","","C3-160270","Rel-13","29.154","13.0.0","AESE-CT","0001","","F",null,"","","","",""]
["C3-160091","Missed Transfer-Request-Type AVP in the commands","Huawei","Yizhuang Wu",61155,"CR","","Agreement","This contribution proposes to add the Transfer-Request-Type AVP into the BTR/BTA commands.","","207","13.16","CT aspects of Architecture Enhancements for Service Capability Exposure [AESE-CT]",910,"revised","2016-01-29T10:25:44.910","2016-02-01T10:08:38.267","","C3-160271","Rel-13","29.154","13.0.0","AESE-CT","0002","","F",null,"","","","",""]
["C3-160092","Some corrections for Nt protocol","Huawei","Yizhuang Wu",61155,"CR","","Agreement","This CR proposes to add the missing abbreviations and correct some typos.","","207","13.16","CT aspects of Architecture Enhancements for Service Capability Exposure [AESE-CT]",920,"revised","2016-01-29T10:25:44.987","2016-02-01T10:08:38.300","","C3-160272","Rel-13","29.154","13.0.0","AESE-CT","0003","","F",null,"","","","",""]
["C3-160093","Update the scope to include the Nt interface","Huawei","Yizhuang Wu",61155,"CR","","Agreement","This CR proposes to update the scope to include Nt reference  point.","","207","13.16","CT aspects of Architecture Enhancements for Service Capability Exposure [AESE-CT]",930,"revised","2016-01-29T10:25:45.080","2016-02-01T10:08:38.347","","C3-160273","Rel-13","29.213","13.4.0","AESE-CT","0641","","B",null,"","","","",""]
["C3-160094","Signalling flows over Nt reference point","Huawei","Yizhuang Wu",61155,"CR","","Agreement","This CR proposes to add the signaling flows over Nt reference pont.","","207","13.16","CT aspects of Architecture Enhancements for Service Capability Exposure [AESE-CT]",940,"merged","2016-01-29T10:25:45.160","2016-02-01T10:08:38.377","","","Rel-13","29.213","13.4.0","AESE-CT","0642","","B",null,"","","","",""]
["C3-160095","Diameter Message Priority over diameter based St interface","Huawei","Yizhuang Wu",61155,"CR","","Agreement","This CR proposes the optional inclusion of the DRMP AVP for the Diameter based St commands, in support of priority treatment associated with these commands.","","219","13.28","Diameter Message Priority [DiaPri]",950,"revised","2016-01-29T10:25:45.253","2016-02-01T10:08:38.423","","C3-160299","Rel-13","29.212","13.4.0","DiaPri","1412","","B",null,"","","","",""]
["C3-160096","Diameter Message Priority over Ns interface","Huawei","Yizhuang Wu",61155,"CR","","Agreement","This CR proposes the optional inclusion of the DRMP AVP for Ns commands, in support of priority treatment associated with these commands.","","219","13.28","Diameter Message Priority [DiaPri]",960,"agreed","2016-01-29T10:25:45.377","2016-02-01T10:08:38.457","","","Rel-13","29.153","13.0.0","DiaPri","0005","","B","CP-160093","","","","",""]
["C3-160097","Diameter Message Priority over Nt interface","Huawei","Yizhuang Wu",61155,"CR","","Agreement","This CR proposes the optional inclusion of the DRMP AVP for Nt commands, in support of priority treatment associated with these commands.","","219","13.28","Diameter Message Priority [DiaPri]",970,"revised","2016-01-29T10:25:45.470","2016-02-01T10:08:37.643","","C3-160300","Rel-13","29.154","13.0.0","DiaPri","0004","","B",null,"","","","",""]
["C3-160098","Diameter Message Priority over Sy interface","Huawei","Yizhuang Wu",61155,"CR","","Agreement","This CR proposes the optional inclusion of the DRMP AVP for Sy commands, in support of priority treatment associated with these commands.","","219","13.28","Diameter Message Priority [DiaPri]",980,"agreed","2016-01-29T10:25:45.567","2016-02-01T10:08:37.690","","","Rel-13","29.219","13.2.0","DiaPri","0047","","B","CP-160093","","","","",""]
["C3-160099","Reference of the Diameter message priority mechanism procedure","Huawei","Yizhuang Wu",61155,"CR","","Agreement","This CR proposes to refer to the Diameter message priority mechanism procedure defined in TS29.213.","","219","13.28","Diameter Message Priority [DiaPri]",990,"agreed","2016-01-29T10:25:45.643","2016-02-01T10:08:37.737","","","Rel-13","29.217","13.2.0","DiaPri","0024","","F","CP-160093","","","","",""]
["C3-160100","Conveying the IMEI of devices to the EPC","Huawei","Yizhuang Wu",61155,"CR","","Agreement","This CR proposes to transfer the IMEI in the IP-CAN session establishment procedre.","","223","13.30.2","TEI13 for Packet Core",1000,"revised","2016-01-29T10:25:45.720","2016-02-01T10:08:37.767","","C3-160298","Rel-13","29.212","13.4.0","TEI13","1413","","F",null,"","","","",""]
["C3-160101","Policy Control for remote UE behind relay UE","Huawei","Yizhuang Wu",61155,"CR","","Agreement","This CR proposes to performing the session binding based on the delegated IPv6 prefix assigned to the relay UE.","","206","13.15","CT aspects of enhancements to Proximity-based Services extensions [eProSe-Ext-CT]",1010,"merged","2016-01-29T10:25:45.800","2016-02-01T10:08:37.800","","","Rel-13","29.213","13.4.0","eProSe-Ext-CT","0644","","B",null,"","","","",""]
["C3-160102","LS to CT4 on allocation of new Diameter Application ID and commands code for PC2 protocol","Huawei, Qualcomm","Yizhuang Wu",61155,"LS out","","Approval","LS on Allocation of new Diameter Application ID and commands code for PC2","","206","13.15","CT aspects of enhancements to Proximity-based Services extensions [eProSe-Ext-CT]",1020,"revised","2016-01-29T10:25:45.893","2016-02-01T10:08:37.830","","C3-160214","Rel-13","","","eProSe-Ext-CT","","","",""]
["C3-160103","Transfer of the serving network identifier","Huawei","Yizhuang Wu",61155,"CR","","Agreement","PCEF provides the serving network identifier in the IP-CAN session establishment procedure.","","212","13.21","CT aspects of Support of Emergency services over WLAN - phase 1 [SEW1-CT]",1030,"agreed","2016-01-29T10:25:45.907","2016-02-01T10:08:37.863","","","Rel-13","29.212","13.4.0","SEW1-CT","1414","","F","CP-160104","","","","",""]
["C3-160104","Missed Fixed-User-Location-Info AVP in CC-request command","Huawei, Ericsson","Yizhuang Wu",61155,"CR","","Agreement","This CR proposes to add the Fixed-User-Location-Info into the CC-Request command.","","170","12.17","Policy and Charging Control for supporting traffic from fixed terminals and NSWO traffic from 3GPP Ues in fixed broadband access networks [P4C-F-CT3]",1040,"agreed","2016-01-29T10:25:45.987","2016-02-01T10:08:37.910","","","Rel-12","29.212","12.11.0","P4C-F-CT3","1415","","F","CP-160099","","","","",""]
["C3-160105","Missed Fixed-User-Location-Info AVP in CC-request command","Huawei, Ericsson","Yizhuang Wu",61155,"CR","","Agreement","This CR proposes to add the Fixed-User-Location-Info into the CC-Request command.","","170","12.17","Policy and Charging Control for supporting traffic from fixed terminals and NSWO traffic from 3GPP Ues in fixed broadband access networks [P4C-F-CT3]",1050,"agreed","2016-01-29T10:25:46.080","2016-02-01T10:08:37.940","","","Rel-13","29.212","13.4.0","P4C-F-CT3","1416","","A","CP-160099","","","","",""]
["C3-160106","Update the scope to include the St interface","Huawei","Yizhuang Wu",61155,"CR","","Agreement","","","211","13.20","CT3 Aspect of Flexible Mobile Service Steering [FMSS-CT]",1060,"revised","2016-01-29T10:25:46.157","2016-02-01T10:08:37.970","","C3-160219","Rel-13","29.213","13.4.0","FMSS-CT","0645","","F",null,"","","","",""]
["C3-160107","Correction of command name for Rx session termination","Ericsson LM","Susana Fernandez",42321,"CR","","Agreement","","","223","13.30.2","TEI13 for Packet Core",1070,"agreed","2016-01-29T10:26:49.790","2016-01-29T12:10:34.217","","","Rel-13","29.213","13.4.0","PCC, TEI13","0646","","D","CP-160101","","","","",""]
["C3-160108","NAS/RAN cause handling at bearer termination failure","Ericsson LM","Susana Fernandez",42321,"CR","","Agreement","","","223","13.30.2","TEI13 for Packet Core",1080,"revised","2016-01-29T10:33:30.707","2016-02-01T10:18:30.643","","C3-160295","Rel-13","29.212","13.4.0","PCC, TEI13","1417","","B",null,"","","","",""]
["C3-160109","Reporting of NAS/RAN cause in the STR command","Ericsson LM","Susana Fernandez",42321,"CR","","Agreement","","","190","12.35.2","TEI12 for Packet Core",1090,"withdrawn","2016-01-29T10:38:04.780","2016-02-01T10:18:30.673","","C3-160200","Rel-12","29.212","12.11.0","PCC, TEI12","1418","","F",null,"","","","",""]
["C3-160110","Reporting of NAS/RAN cause in the STR command","Ericsson LM","Susana Fernandez",42321,"CR","","Agreement","","","190","12.35.2","TEI12 for Packet Core",1100,"revised","2016-01-29T10:43:02.880","2016-02-01T10:18:30.720","","C3-160236","Rel-13","29.214","13.4.0","PCC, TEI12","0437","","A",null,"","","","",""]
["C3-160111","RAN-NAS-Cause handling upon unsuccessful bearer termination over Rx","Ericsson LM","Susana Fernandez",42321,"CR","","Agreement","","","223","13.30.2","TEI13 for Packet Core",1110,"revised","2016-01-29T10:47:11.073","2016-02-01T10:18:30.753","","C3-160296","Rel-13","29.214","13.4.0","PCC, TEI13","0438","","F",null,"","","","",""]
["C3-160112","Completion of RAN-NAS cause handling procedures","Ericsson LM","Susana Fernandez",42321,"CR","","Agreement","","","190","12.35.2","TEI12 for Packet Core",1120,"revised","2016-01-29T10:53:22.297","2016-02-01T10:18:30.783","","C3-160237","Rel-12","29.213","12.10.0","PCC, TEI12","0647","","F",null,"","","","",""]
["C3-160113","LS on NBIFOM procedure in SCM and RAN rules handling parameter","3GPP TSG CT WG1","Xingyue Zhou",42680,"LS in","","Information","","","13","6","Received Liaison Statements",1130,"noted","2016-01-29T10:54:59.003","2016-01-29T11:51:37.437","","","Rel-13","","","NBIFOM-CT","","","","",null,"3GPP TSG SA WG2","3GPP TSG CT WG3, 3GPP TSG CT WG4"]
["C3-160114","LS on EVS over UTRAN","3GPP TSG CT4","Lena Chaponniere",38080,"LS in","","Information","","","13","6","Received Liaison Statements",1140,"noted","2016-01-29T11:04:20.643","2016-01-29T11:51:37.470","","","Rel-13","","","EVSoCS","","","","",null,"TSG SA WG4","RAN WG1, TSG RAN WG2, TSG RAN WG3, TSG CT WG1, TSG CT WG3"]
["C3-160115","Completion of RAN-NAS cause handling procedures","Ericsson LM","Susana Fernandez",42321,"CR","","Agreement","","","223","13.30.2","TEI13 for Packet Core",1150,"revised","2016-01-29T11:05:54.843","2016-02-01T10:18:30.830","","C3-160306","Rel-13","29.213","13.4.0","PCC, TEI13","0648","","F",null,"","","","",""]
["C3-160116","Completion of RAN-NAS cause handling procedures","Ericsson LM","Susana Fernandez",42321,"CR","","Agreement","","","223","13.30.2","TEI13 for Packet Core",1160,"withdrawn","2016-01-29T11:06:00.007",null,"","","Rel-13","29.213","13.4.0","PCC, TEI13","0649","","F",null,"","","","",""]
["C3-160117","LS on progress of the work on Diameter Base Protocol Update","3GPP TSG CT4","Lionel Morand",25150,"LS in","","Discussion","","","13","6","Received Liaison Statements",1170,"noted","2016-01-29T11:07:45.763","2016-01-29T11:51:37.500","","","Rel-13","","","FS_DBPU","","","","",null,"3GPP TSG CT3, 3GPP TSG SA3, 3GPP TSG SA5"]
["C3-160118","Support of background data transfer per UE in the PCRF","Ericsson LM","Susana Fernandez",42321,"CR","","Agreement","","","207","13.16","CT aspects of Architecture Enhancements for Service Capability Exposure [AESE-CT]",1180,"agreed","2016-01-29T11:09:49.047","2016-01-29T12:10:34.250","","","Rel-13","29.213","13.4.0","AESE-CT","0650","","B","CP-160095","","","","",""]
["C3-160119","Reply LS on 3GPP Work on Explicit Congestion Notification for Lower Layer Protocols","RAN2","Soenghun Kim",33371,"LS in","","Information","","","13","6","Received Liaison Statements",1190,"noted","2016-01-29T11:14:28.153","2016-01-29T11:51:37.547","","","Rel-10","","","ECSRA_LAA-CN","","","","",null,"SA","CT, RAN, SA2, SA4, CT1, CT3, CT4"]
["C3-160120","Inclusion of Reference Id over Rx","Ericsson LM","Susana Fernandez",42321,"CR","","Agreement","","","207","13.16","CT aspects of Architecture Enhancements for Service Capability Exposure [AESE-CT]",1200,"merged","2016-01-29T11:17:26.660","2016-01-29T12:10:34.280","","","Rel-13","29.214","13.4.0","AESE-CT","0439","","B",null,"","","","",""]
["C3-160121","Inclusion of Reference Id over Rx","Ericsson LM","Susana Fernandez",42321,"CR","","Agreement","","","207","13.16","CT aspects of Architecture Enhancements for Service Capability Exposure [AESE-CT]",1210,"withdrawn","2016-01-29T11:17:31.997",null,"","","Rel-13","29.214","13.4.0","","0440","","B",null,"","","","",""]
["C3-160122","LS on S1 signalling solutions for non-NB-IoT UEs","RAN","Riikka Susitaival",44957,"LS in","","Information","","","13","6","Received Liaison Statements",1220,"noted","2016-01-29T11:17:42.383","2016-01-29T11:51:37.577","","","Rel-13","","","NB_IOT-Core","","","","",null,"SA2, SA3, SA, CT1, CT3, CT4, RAN2, RAN3","RAN1"]
["C3-160123","Reply LS on NBIFOM Clarifications","3GPP TSG SA WG2","Tricci So",44974,"LS in","","Discussion","","","13","6","Received Liaison Statements",1230,"noted","2016-01-29T11:21:56.210","2016-01-29T11:51:37.610","","","","","","NBIFOM-CT","","","","",null,"3GPP TSG CT WG","3GPP TSG CT WG1, 3GPP TSG SA WG3 and WG4"]
["C3-160124","Reply to CT3’s LS on addition of delivery content over MB2-C reference point","3GPP TSG SA WG2","Val Oprescu",14981,"LS in","","Discussion","","","13","6","Received Liaison Statements",1240,"noted","2016-01-29T11:26:44.527","2016-01-29T11:51:37.640","","","Rel-13","","","","","","","",null,"3GPP TSG CT WG3"]
["C3-160125","UE-to-network relay PCC handling over Rx","Ericsson LM","Susana Fernandez",42321,"CR","","Agreement","","","206","13.15","CT aspects of enhancements to Proximity-based Services extensions [eProSe-Ext-CT]",1250,"revised","2016-01-29T11:28:59.263","2016-01-29T12:10:34.310","","C3-160285","Rel-13","29.214","13.4.0","eProSe-Ext-CT","0441","","B",null,"","","","",""]
["C3-160126","LS on Network asserted WLAN Location Information for PDN connection establishment over S2b","3GPP TSG SA2","Laurent Thiebaut",11066,"LS in","","Information","","","13","6","Received Liaison Statements",1260,"noted","2016-01-29T11:30:45.017","2016-01-29T11:51:37.687","","","Rel-13","","","SEW1-CT","","","","",null,"3GPP TSG CT4","3GPP TSG CT3"]
["C3-160127","UE-to-network relay PCC handling over Gx","Ericsson LM","Susana Fernandez",42321,"CR","","Agreement","","","206","13.15","CT aspects of enhancements to Proximity-based Services extensions [eProSe-Ext-CT]",1270,"revised","2016-01-29T11:33:27.177","2016-01-29T12:10:34.357","","C3-160286","Rel-13","29.212","13.4.0","eProSe-Ext-CT","1419","","B",null,"","","","",""]
["C3-160128","Reply LS on NBIFOM Clarifications","3GPP TSG SA WG2","Huan Li",58261,"LS in","","Discussion","","","13","6","Received Liaison Statements",1280,"noted","2016-01-29T11:34:26.003","2016-01-29T11:51:37.717","","","","","","NBIFOM-CT","","","","",null,"3GPP TSG CT WG3","3GPP TSG CT WG1, 3GPP TSG SA WG3 and WG4"]
["C3-160129","UE-to-network relay PCC handling","Ericsson LM","Susana Fernandez",42321,"CR","","Agreement","","","206","13.15","CT aspects of enhancements to Proximity-based Services extensions [eProSe-Ext-CT]",1290,"revised","2016-01-29T11:36:56.823","2016-01-29T12:10:34.390","","C3-160284","Rel-13","29.213","13.4.0","eProSe-Ext-CT","0651","","B",null,"","","","",""]
["C3-160130","LS on Packet switched conversational multimedia applications TS 26.235 and TS 26.236","3GPP TSG SA WG4","Frederic Gabin",18030,"LS in","","Information","","","13","6","Received Liaison Statements",1300,"noted","2016-01-29T11:37:24.810","2016-01-29T11:51:37.750","","","Rel-13","","","IMS-CODEC","","","","",null,"3GPP TSG CT WG3, 3GPP TSG CT WG4, 3GPP TSG RAN WG5, 3GPP TSG RAN WG2","3GPP TSG SA"]
["C3-160131","LS on New AVPs and Experimental Result Code in TS 29.214","Ericsson LM","Susana Fernandez",42321,"LS out","","Approval","","","223","13.30.2","TEI13 for Packet Core",1310,"approved","2016-01-29T11:40:34.427","2016-01-29T12:10:34.420","","","Rel-13","","","PCC, TEI13","","","","",null,"CT4"]
["C3-160132","LS on recently established new Study Group 20 (SG20)","ITU-T SG20","Saurav Arora",62621,"LS in","","Information","","","13","6","Received Liaison Statements",1320,"noted","2016-01-29T11:44:21.747","2016-01-29T11:51:37.780","","","","","","","","","",""]
["C3-160133","Support of removed filters when SIP Forking applies over Rx","Ericsson LM","Susana Fernandez",42321,"CR","","Agreement","","","223","13.30.2","TEI13 for Packet Core",1330,"revised","2016-01-29T11:44:37.660","2016-01-29T12:10:34.453","","C3-160307","Rel-13","29.214","13.4.0","TEI13, PCC","0442","","F",null,"","","","",""]
["C3-160134","Reply LS on 3GPP Work on Explicit Congestion Notification for Lower Layer Protocols","SA","Erik Guttman",18782,"LS in","","Information","","","13","6","Received Liaison Statements",1340,"noted","2016-01-29T11:46:33.597","2016-01-29T11:51:37.813","","","Rel-10","","","ECSRA_LAA-CN","","","","",null,"IETF tsvwg","CT, RAN, SA2, SA4, RAN2, RAN3, CT1, CT3, CT4"]
["C3-160135","Removal of the reference to draft-ietf-dime-ovli","Ericsson LM","Susana Fernandez",42321,"CR","","Agreement","","","202","13.11","Continuation of the Overload Control for PCC based Diameter applications [cDOCME_PCC]",1350,"agreed","2016-01-29T11:52:07.747","2016-01-29T12:10:34.500","","","Rel-13","29.213","13.4.0","cDOCME_PCC","0652","","D","CP-160106","","","","",""]
["C3-160136","Missing experimental result code value","Ericsson LM","Susana Fernandez",42321,"CR","","Agreement","","","192","13.1","CT aspects of User Plane Congestion Management (UPCON) for Building Block I [UPCON-DOTCON-CT]",1360,"agreed","2016-01-29T11:55:48.860","2016-01-29T12:10:34.530","","","Rel-13","29.214","13.4.0","UPCON-DOTCON-CT","0443","","F","CP-160094","","","","",""]
["C3-160137","Metadata indicator for restricted discovery monitor request procedure","Qualcomm Incorporated","Zhibin Wu",49530,"CR","","Agreement","","","206","13.15","CT aspects of enhancements to Proximity-based Services extensions [eProSe-Ext-CT]",1370,"revised","2016-01-31T15:52:15.990","2016-01-31T23:05:11.320","","C3-160287","Rel-13","29.343","13.1.0","eProSe-Ext-CT","0018","","F",null,"","","","",""]
["C3-160138","Open discovery procedures in PC2 interface for application-controlled extension","Qualcomm Incorporated","Zhibin Wu",49530,"CR","","Agreement","","","206","13.15","CT aspects of enhancements to Proximity-based Services extensions [eProSe-Ext-CT]",1380,"revised","2016-01-31T15:55:54.233","2016-01-31T23:05:11.290","","C3-160288","Rel-13","29.343","13.1.0","eProSe-Ext-CT","0019","","F",null,"","","","",""]
["C3-160139","Traffic Steering Rule Error handling over the REST based St interface","Oracle Corporation","Tarek Abou-assali",58502,"CR","","Agreement","Traffic steering rule error handling procedures over the REST based St.","","211","13.20","CT3 Aspect of Flexible Mobile Service Steering [FMSS-CT]",1390,"revised","2016-01-31T17:44:32.740","2016-02-01T04:35:28.680","","C3-160220","Rel-13","29.155","13.0.0","FMSS-CT","0001","","B",null,"","","","",""]
["C3-160140","Miscellaneous corrections related to the REST based St","Oracle Corporation","Tarek Abou-assali",58502,"CR","","Agreement","Miscellaneous corrections","","211","13.20","CT3 Aspect of Flexible Mobile Service Steering [FMSS-CT]",1400,"revised","2016-01-31T23:32:32.837","2016-02-01T04:35:28.710","","C3-160261","Rel-13","29.155","13.0.0","FMSS-CT","0002","","F",null,"","","","",""]
["C3-160141","Updates to JSON content rules for the notification procedures from the TSSF to the PCRF","Oracle Corporation","Tarek Abou-assali",58502,"CR","","Agreement","","","211","13.20","CT3 Aspect of Flexible Mobile Service Steering [FMSS-CT]",1410,"revised","2016-01-31T23:41:47.067","2016-02-01T04:35:28.743","","C3-160262","Rel-13","29.155","13.0.0","FMSS-CT","0003","","B",null,"","","","",""]
["C3-160142","JSON content rules updates for error responses with traffic steering rule reports over the REST based St interface","Oracle Corporation","Tarek Abou-assali",58502,"CR","","Agreement","JCR updates for error responses related to traffic steering rule provisioning","","211","13.20","CT3 Aspect of Flexible Mobile Service Steering [FMSS-CT]",1420,"revised","2016-01-31T23:49:23.117","2016-02-01T04:35:28.633","","C3-160263","Rel-13","29.155","13.0.0","FMSS-CT","0004","","B",null,"","","","",""]
["C3-160143","Traffic steering rule report JSON Content Rules over St","Oracle Corporation","Tarek Abou-assali",58502,"CR","","Agreement","JCRs for traffic steering rule report","","211","13.20","CT3 Aspect of Flexible Mobile Service Steering [FMSS-CT]",1430,"revised","2016-01-31T23:52:42.903","2016-02-01T04:35:28.773","","C3-160264","Rel-13","29.155","13.0.0","FMSS-CT","0005","","B",null,"","","","",""]
["C3-160144","Correction for the PCEF procedures","Huawei","Youyang Yu",46021,"CR","","Agreement","","","205","13.14","CT aspects of IP Flow Mobility support for S2a and S2b Interfaces (NBIFOM) [NBIFOM-CT]",1440,"revised","2016-02-01T01:16:01.127","2016-02-01T07:21:47.483","","C3-160312","Rel-13","29.212","13.4.0","NBIFOM-CT","1420","","F",null,"","","","",""]
["C3-160145","Editorial correction on DIAMETER_ERROR_NBIFOM_NOT_AUTHORIZED","Huawei","Youyang Yu",46021,"CR","","Agreement","","","205","13.14","CT aspects of IP Flow Mobility support for S2a and S2b Interfaces (NBIFOM) [NBIFOM-CT]",1450,"agreed","2016-02-01T01:16:01.253","2016-02-01T07:21:47.530","","","Rel-13","29.212","13.4.0","NBIFOM-CT","1421","","F","CP-160090","","","","",""]
["C3-160146","NBIFOM routing rule definition","Huawei","Youyang Yu",46021,"CR","","Agreement","","","205","13.14","CT aspects of IP Flow Mobility support for S2a and S2b Interfaces (NBIFOM) [NBIFOM-CT]",1460,"merged","2016-02-01T01:16:01.360","2016-02-01T07:21:47.577","","","Rel-13","29.212","13.4.0","NBIFOM-CT","1422","","F",null,"","","","",""]
["C3-160147","Clarifications regarding Monitoring-Time procedures","Oracle Corporation","Tarek Abou-assali",58502,"CR","","Agreement","Monitoring Time procedures defined in clause 4.5.17.6 are unclear with regards to resetting of the usage threshold","","190","12.35.2","TEI12 for Packet Core",1470,"revised","2016-02-01T03:16:21.787","2016-02-01T04:35:28.820","","C3-160238","Rel-12","29.212","12.11.0","TEI12","1423","","F",null,"","","","",""]
["C3-160148","Network-initiated removal of one access from the PDN connection","ZTE Corporation","Xiaoyun Zhou",38525,"CR","","Agreement","Support of network-initiated removal of one access from the PDN connection","","205","13.14","CT aspects of IP Flow Mobility support for S2a and S2b Interfaces (NBIFOM) [NBIFOM-CT]",1480,"agreed","2016-02-01T03:22:40.037","2016-02-01T07:28:20.430","","","Rel-13","29.215","13.4.0","NBIFOM-CT","0401","","F","CP-160107","","","","",""]
["C3-160149","Correction to NBIFOM handling in roaming case","ZTE Corporation","Xiaoyun Zhou",38525,"CR","","Agreement","","","205","13.14","CT aspects of IP Flow Mobility support for S2a and S2b Interfaces (NBIFOM) [NBIFOM-CT]",1490,"revised","2016-02-01T03:24:11.593","2016-02-01T07:28:20.477","","C3-160313","Rel-13","29.215","13.4.0","NBIFOM-CT","0402","","F",null,"","","","",""]
["C3-160150","LS on AVP codes allocation to CT4","ZTE Corporation","Xiaoyun Zhou",38525,"LS out","","Approval","","","205","13.14","CT aspects of IP Flow Mobility support for S2a and S2b Interfaces (NBIFOM) [NBIFOM-CT]",1500,"merged","2016-02-01T03:26:57.107","2016-02-01T07:28:20.523","","","Rel-13","","","","","","","",null,"CT4"]
["C3-160151","Clarifications regarding Monitoring-Time procedures","Oracle Corporation","Tarek Abou-assali",58502,"CR","","Agreement","","","190","12.35.2","TEI12 for Packet Core",1510,"revised","2016-02-01T03:32:38.077","2016-02-01T04:35:28.603","","C3-160239","Rel-13","29.212","13.4.0","TEI12","1424","","A",null,"","","","",""]
["C3-160152","Rx impact for background data transfer","ZTE Corporation","Xiaoyun Zhou",38525,"CR","","Agreement","Support of the call flow of Rx impact for background data transfer","","207","13.16","CT aspects of Architecture Enhancements for Service Capability Exposure [AESE-CT]",0,"agreed","2016-02-01T07:57:24.017","2016-02-01T08:03:06.683","","","Rel-13","29.213","13.4.0","AESE-CT","0653","","B","CP-160095","","","","",""]
["C3-160153","DRMP over REST Interface","ACS, OEC, AT&T,Alcatel-Lucent, Alcatel-Lucent Shanghai Bell and  Nokia Networks","Viqar Shaikh",43795,"CR","","Agreement","","","219","13.28","Diameter Message Priority [DiaPri]",1530,"revised","2016-02-01T08:12:16.453","2016-02-01T15:30:50.277","","C3-160302","Rel-13","29.201","13.3.0","DiaPri","0039","","B",null,"","","","",""]
["C3-160154","Reservation-Priority AVP and DRMP AVP Interaction","ACS, OEC, AT&T,Alcatel-Lucent, Alcatel-Lucent Shanghai Bell and  Nokia Networks","Viqar Shaikh",56720,"CR","","Agreement","","","219","13.28","Diameter Message Priority [DiaPri]",1540,"revised","2016-02-01T08:14:39.973","2016-02-01T15:25:01.633","","C3-160303","Rel-13","29.213","13.4.0","DiaPri","0654","","B",null,"","","","",""]
["C3-160155","Reservation-Priority AVP and DRMP AVP Interaction","ACS, OEC, AT&T,Alcatel-Lucent, Alcatel-Lucent Shanghai Bell and  Nokia Networks","Viqar Shaikh",56720,"CR","","Agreement","","","219","13.28","Diameter Message Priority [DiaPri]",1550,"withdrawn","2016-02-01T08:16:20.593","2016-02-01T15:25:01.667","","","Rel-13","29.213","13.4.0","DiaPri","0655","","B",null,"","","","",""]
["C3-160156","Removal of references to TS 26.235","Nokia Networks, Alcatel Lucent","Thomas Belling",23293,"CR","","Agreement","References to TS 26.235 are replaced by references to TS 26.114, because SA4 decided to discontinue TS 26.235.","","222","13.30.1","TEI13 for IMS/CS",1560,"agreed","2016-02-01T08:28:47.797","2016-02-01T11:03:10.457","","","Rel-13","29.162","13.1.0","TEI13","0151","","F","CP-160105","","","","",""]
["C3-160157","Removal of references to TS 26.235 and TS 26.236","Nokia Networks, Alcatel_lucent","Thomas Belling",23293,"CR","","Agreement","References to TS 26.235 and to TS 26.236 are replaced by references to TS 26.114, because SA4 decided to discontinue TS  26.235 and TS 26.236.","","222","13.30.1","TEI13 for IMS/CS",1570,"agreed","2016-02-01T08:35:22.537","2016-02-01T11:03:10.503","","","Rel-13","29.163","13.4.0","TEI13","0968","","F","CP-160105","","","","",""]
["C3-160158","Removal of references to TS 26.236","Nokia Networks, Alcatel-Lucent","Thomas Belling",23293,"CR","","Agreement","References to TS 26.236 are replaced by references to TS 26.114, because SA4 decided to discontinue TS 26.236.","","223","13.30.2","TEI13 for Packet Core",1580,"revised","2016-02-01T08:44:18.970","2016-02-01T11:03:10.550","","C3-160308","Rel-13","29.213","13.4.0","TEI13","0656","","F",null,"","","","",""]
["C3-160159","Removal of references to TS 26.235 and TS 26.236","Nokia Networks, Alcatel-Lucent","Thomas Belling",23293,"CR","","Agreement","References to TS 26.235 and to TS 26.236 are replaced by references to TS 26.114, because SA4 decided to discontinue S 26.235 and TS 26.236.","","222","13.30.1","TEI13 for IMS/CS",1590,"agreed","2016-02-01T08:50:20.513","2016-02-01T11:03:10.597","","","Rel-13","29.235","13.0.0","TEI13","0104","","F","CP-160105","","","","",""]
["C3-160160","Removal of references to TS 26.235","Nokia Networks, Alcatel-Lucent","Thomas Belling",23293,"CR","","Agreement","References to TS 26.235 are replaced by references to TS 26.114, because SA4 decided to discontinue TS 26.235.","","222","13.30.1","TEI13 for IMS/CS",1600,"revised","2016-02-01T08:55:41.497","2016-02-01T11:03:10.643","","C3-160283","Rel-13","29.292","13.2.0","TEI13","0130","","F",null,"","","","",""]
["C3-160161","St Diameter Application ID","Nokia Networks","Thomas Belling",23293,"CR","","Agreement","Diameter St application ID is added.","","211","13.20","CT3 Aspect of Flexible Mobile Service Steering [FMSS-CT]",1610,"agreed","2016-02-01T09:01:23.213","2016-02-01T11:03:10.690","","","Rel-13","29.212","13.4.0","FMSS-CT","1425","","F","CP-160091","","","","",""]
["C3-160162","St Supported Feature Mechanism Clarifications","Nokia Networks","Thomas Belling",23293,"CR","","Agreement","Unclear terms \"client\" and \"server\" are replaced by unambiguous \"PCRF\" and \"TSSF\", and term \"post-Rel-13 St functionality\" assuming that supported features are defined in Rel-14 is removed.","","211","13.20","CT3 Aspect of Flexible Mobile Service Steering [FMSS-CT]",1620,"agreed","2016-02-01T09:11:41.577","2016-02-01T11:03:10.720","","","Rel-13","29.212","13.4.0","FMSS-CT","1426","","F","CP-160091","","","","",""]
["C3-160163","Encoding of Diameter St Error Notifications","Nokia Networks","Thomas Belling",23293,"discussion","","Discussion","The discussion paper suggests adding a notification message from TSSF to PCRF that can be used for error handling when traffic steering rules can no longer be enforced, and compares different possible encodings for this Diameter message.","","211","13.20","CT3 Aspect of Flexible Mobile Service Steering [FMSS-CT]",1630,"noted","2016-02-01T09:19:39.497","2016-02-01T11:03:10.767","","","Rel-13","29.212","13.4.0","FMSS-CT","","","","","","","","",""]
["C3-160164","Diameter St Error Notifications","Nokia Networks","Thomas Belling",23293,"CR","","Agreement","","","211","13.20","CT3 Aspect of Flexible Mobile Service Steering [FMSS-CT]",1640,"revised","2016-02-01T09:22:20.737","2016-02-01T11:03:10.800","","C3-160216","Rel-13","29.212","13.4.0","FMSS-CT","1427","","B",null,"","","","",""]
["C3-160165","LS on Request for Diameter Command Code for new St Interface","Nokia Networks","Thomas Belling",23293,"LS out","","Approval","CT3 asks CT4 and their MCC to kindly request a new Diameter Commend code for the Diameter St application from IANA","","211","13.20","CT3 Aspect of Flexible Mobile Service Steering [FMSS-CT]",1650,"approved","2016-02-01T09:27:56.277","2016-02-01T11:03:10.830","","","Rel-13","29.212","","FMSS-CT","","","","",null,"CT4"]
["C3-160166","Support of bitrate variations","Ericsson LM","Susana Fernandez",42321,"CR","","Agreement","","","194","13.3","CT Aspects of QoS End to End MTSI extensions [QOSE2EMTSI-CT]",1660,"revised","2016-02-01T09:37:07.887","2016-02-01T14:27:57.907","","C3-160328","Rel-13","29.212","13.4.0","QOSE2EMTSI-CT","1428","","B",null,"","","","",""]
["C3-160167","Usage of the UDP port for default unicast encapsulation mode at the SGmb interface is required to support SYNC protocol","Nokia Networks, Alcatel-Lucent","Thomas Belling",23293,"CR","","Agreement","If the GGSN selects unicast encapsulation, it shall always allocates a transport plane UDP port number where to receive user plane data and shall signal it to the BM-SC in the MBMS-GW-UDP-Port AVP (as also done on the SGmB interface).","","54","9.4","MBMS [MBMS]",1670,"revised","2016-02-01T09:42:46.780","2016-02-01T11:03:10.860","","C3-160289","Rel-9","29.061","9.15.0","MBMS","0461","","F",null,"","","","",""]
["C3-160168","Usage of the UDP port for default unicast encapsulation mode at the Gmb interface is required to support SYNC protocol","Nokia Networks","Thomas Belling",23293,"CR","","Agreement","If the GGSN selects unicast encapsulation, it shall always allocates a transport plane UDP port number where to receive user plane data and shall signal it to the BM-SC in the MBMS-GW-UDP-Port AVP (as also done on the SGmB interface).","","54","9.4","MBMS [MBMS]",1680,"revised","2016-02-01T10:05:04.253","2016-02-01T11:03:10.893","","C3-160290","Rel-10","29.061","10.13.0","MBMS","0462","","B",null,"","","","",""]
["C3-160169","Location reporting for IMS sessions over S2b","Alcatel-Lucent, Alcatel-Lucent Shanghai Bell, Nokia Networks","Horst Brinkmann",12927,"CR","","Agreement","SA2 enhanced the location reporting for emergency and regular sessions for an untrusted access to the EPC. The CR alligns the Rx interface with stage 2 requirements.","","212","13.21","CT aspects of Support of Emergency services over WLAN - phase 1 [SEW1-CT]",1690,"agreed","2016-02-01T10:08:00.563","2016-02-01T12:23:54.493","","","Rel-13","29.214","13.4.0","SEW1-CT","0444","","F","CP-160104","","","","",""]
["C3-160170","Usage of the UDP port for default unicast encapsulation mode at the Gmb interface is required to support SYNC protocol","Nokia Networks, Alcatel-Lucent","Thomas Belling",23293,"CR","","Agreement","If the GGSN selects unicast encapsulation, it shall always allocates a transport plane UDP port number where to receive user plane data and shall signal it to the BM-SC in the MBMS-GW-UDP-Port AVP (as also done on the SGmB interface).","","54","9.4","MBMS [MBMS]",1700,"revised","2016-02-01T10:11:28.227","2016-02-01T11:03:10.923","","C3-160291","Rel-11","29.061","11.11.0","MBMS","0463","","A",null,"","","","",""]
["C3-160171","Use of Supported-Features AVP","Alcatel-Lucent, Alcatel-Lucent Shanghai Bell, Nokia Networks","Horst Brinkmann",12927,"CR","","Agreement","Subclause 5.1.6 specifies the usage of the Supported-Features AVP, but the Supported-Features AVP is not used on the Sy interface. 3GPP TS 29.219 for 3GPP Release 13 already mentions that subclause 5.6.1 is a placeholder for when any supported features ar","","126","11.17","CT3 aspects of QoS Control Based on Subscriber Spending Limits  [QoS_SSL-CT3]",1710,"withdrawn","2016-02-01T10:15:42.820","2016-02-01T12:23:54.573","","","Rel-11","29.219","11.7.0","QoS_SSL-CT3","0048","","F",null,"","","","",""]
["C3-160172","Usage of the UDP port for default unicast encapsulation mode at the Gmb interface is required to support SYNC protocol","Nokia Networks, Alcatel-Lucent","Thomas Belling",23293,"CR","","Agreement","If the GGSN selects unicast encapsulation, it shall always allocates a transport plane UDP port number where to receive user plane data and shall signal it to the BM-SC in the MBMS-GW-UDP-Port AVP (as also done on the SGmB interface).","","54","9.4","MBMS [MBMS]",1720,"revised","2016-02-01T10:19:37.037","2016-02-01T11:03:10.957","","C3-160292","Rel-12","29.061","12.11.0","MBMS","0464","","A",null,"","","","",""]
["C3-160173","Use of Supported-Features AVP","Alcatel-Lucent, Alcatel-Lucent Shanghai Bell, Nokia Networks","Horst Brinkmann",12927,"CR","","Agreement","Subclause 5.1.6 specifies the usage of the Supported-Features AVP, but the Supported-Features AVP is not used on the Sy interface. 3GPP TS 29.219 for 3GPP Release 13 already mentions that subclause 5.6.1 is a placeholder for when any supported features ar","","126","11.17","CT3 aspects of QoS Control Based on Subscriber Spending Limits  [QoS_SSL-CT3]",1730,"withdrawn","2016-02-01T10:21:13.457","2016-02-01T12:23:54.617","","","Rel-12","29.219","12.3.0","QoS_SSL-CT3","0049","","A",null,"","","","",""]
["C3-160174","Use of Supported-Features AVP","Alcatel-Lucent, Alcatel-Lucent Shanghai Bell, Nokia Networks","Horst Brinkmann",12927,"CR","","Agreement","Subclause 5.1.6 specifies the usage of the Supported-Features AVP, but the Supported-Features AVP is not used on the Sy interface. 3GPP TS 29.219 for 3GPP Release 13 already mentions that subclause 5.6.1 is a placeholder for when any supported features ar","","126","11.17","CT3 aspects of QoS Control Based on Subscriber Spending Limits  [QoS_SSL-CT3]",1740,"withdrawn","2016-02-01T10:26:21.603","2016-02-01T12:23:54.540","","","Rel-13","29.219","13.2.0","QoS_SSL-CT3","0050","","A",null,"","","","",""]
["C3-160175","Usage of the UDP port for default unicast encapsulation mode at the Gmb interface is required to support SYNC protocol","Nokia Networks, Alcatel-Lucent","Thomas Belling",23293,"CR","","Agreement","If the GGSN selects unicast encapsulation, it shall always allocates a transport plane UDP port number where to receive user plane data and shall signal it to the BM-SC in the MBMS-GW-UDP-Port AVP (as also done on the SGmB interface).","","54","9.4","MBMS [MBMS]",1750,"revised","2016-02-01T10:30:16.320","2016-02-01T11:03:11.003","","C3-160293","Rel-13","29.061","13.2.0","MBMS","0465","","B",null,"","","","",""]
["C3-160176","Consequences on Gx and Rx of the RAN/NAS cause inclusion into the Delete Bearer Response message","Alcatel-Lucent, Alcatel-Lucent Shanghai Bell, Nokia Networks, Huawei","Horst Brinkmann",12927,"discussion","","Discussion","This discussion paper proposes to enhance the 3GPP TS 29.212 and 3GPP TS 29.214 in order to effectively improve the end-user’s VoLTE experiences in some poor RF environments.","","223","13.30.2","TEI13 for Packet Core",1760,"noted","2016-02-01T10:44:07.513","2016-02-01T12:23:54.743","","","Rel-13","","","PCC, TEI13","","","","","","","","",""]
["C3-160177","WebRTC media plane optimization procedure","Nokia Networks","Thomas Belling",23293,"CR","","Agreement","Media Plane Optimization procedures for WebRTC are specified. The eIMS-AGW is configured with transport \"UDP\", as all higher protocol layers need to be passed without modification.","","216","13.25","Enhancements to WEBRTC interoperability stage 3 [eWebRTCi_CT]",1770,"revised","2016-02-01T10:50:44.127","2016-02-01T11:03:10.410","","C3-160204","Rel-13","29.162","13.1.0","eWebRTCi-CT ","0152","","B",null,"","","","",""]
["C3-160178","RAN/NAS introduction for session termination","Alcatel-Lucent, Alcatel-Lucent Shanghai Bell, Nokia Networks, Huawei","Horst Brinkmann",12927,"CR","","Agreement","In particular for Voice over PS operations and in case a temporary radio link failure occurs, a special use case arises when the far-end party is not patient enough and hang up the call within an MME safeguard recovering period. In this case a QoE finetun","","223","13.30.2","TEI13 for Packet Core",1780,"merged","2016-02-01T10:51:45.793","2016-02-01T12:23:54.680","","","Rel-13","29.214","13.4.0","PCC, TEI13","0445","","B",null,"","","","",""]
["C3-160179","RAN/NAS introduction for session termination","Alcatel-Lucent, Alcatel-Lucent Shanghai Bell, Nokia Networks, Huawei","Horst Brinkmann",12927,"CR","","Agreement","In particular for Voice over PS operations and in case a temporary radio link failure occurs, a special use case arises when the far-end party is not patient enough and hang up the call within an MME safeguard recovering period. In this case a QoE finetun","","223","13.30.2","TEI13 for Packet Core",1790,"merged","2016-02-01T10:59:03.057","2016-02-01T12:23:54.650","","","Rel-13","29.212","13.4.0","PCC, TEI13","1429","","B",null,"","","","",""]
["C3-160180","LS on new AVPs in TS 29.212","Nokia Networks","Thomas Belling",23293,"LS out","","Approval","CT4 is informed about new AVP codes that need to be documented TS 29.230","","223","13.30.2","TEI13 for Packet Core",1800,"revised","2016-02-01T11:00:16.737","2016-02-01T16:48:07.830","","C3-160213","Rel-13","29.212","","PCC, TEI13","","","",""]
["C3-160181","Add missing abbreviations","HUAWEI TECHNOLOGIES Co. Ltd.","Yizhuang Wu",61155,"CR","","Agreement","","","192","13.1","CT aspects of User Plane Congestion Management (UPCON) for Building Block I [UPCON-DOTCON-CT]",1810,"agreed","2016-02-01T12:30:59.623","2016-02-01T12:38:19.460","","","Rel-13","29.217","13.2.0","UPCON-DOTCON-CT","0025","","F","CP-160094","","","","",""]
["C3-160182","Introduction of YANG model to St reference point","China Mobile Com. Corporation,Huawei","Zhenning Huang",60086,"CR","","Agreement","Replace the current example and JSON schema with RESTCONF+YANG.","","211","13.20","CT3 Aspect of Flexible Mobile Service Steering [FMSS-CT]",1820,"withdrawn","2016-02-01T13:38:36.267","2016-02-01T15:15:48.383","","","Rel-13","29.155","13.0.0","FMSS-CT","0006","","C",null,"","","","",""]
["C3-160183","LS Reply to LS on TSSF Identity Information over Gx","3GPP TSG SA2","Nirav Salot",56645,"LS in","","Information","","","13","6","Received Liaison Statements",1830,"noted","2016-02-01T14:00:09.763","2016-02-01T14:37:24.840","","","Rel-13","","","TEI13, FMSS-CT","","","","",null,"CT3"]
["C3-160184","Reply LS on NBIFOM procedure in SCM and RAN rules handling parameter","3GPP TSG SA WG2","Huan Li",58261,"LS in","","Information","","","13","6","Received Liaison Statements",1840,"noted","2016-02-01T14:03:38.897","2016-02-01T14:37:24.887","","","","","","","","","","",null,"3GPP TSG CT WG1","3GPP TSG CT WG3, 3GPP TSG CT WG4"]
["C3-160185","Reply LS to LS on APN AMBR change at a certain time on Gx","3GPP TSG SA2","Laurent Thiebaut",11066,"LS in","","Discussion","","","13","6","Received Liaison Statements",1850,"noted","2016-02-01T14:07:14.767","2016-02-01T14:37:24.917","","","Rel-13","","","TEI13","","","","",null,"3GPP TSG CT3"]
["C3-160186","LS on potential need of PCC enhancement for MCPTT","3GPP TSG SA WG2","Belen Pancorbo",4022,"LS in","","Information","","","13","6","Received Liaison Statements",1860,"noted","2016-02-01T14:10:05.790","2016-02-01T14:37:24.950","","","Rel-13","","","MCPTT-CT","","","","",null,"3GPP TSG SA WG6","3GPP TSG CT WG3, 3GPP TSG CT WG1"]
["C3-160187","LS on Completion of QOSE2EMTSI work item","SA4","Tomas Frankkila",25766,"LS in","","Discussion","","","13","6","Received Liaison Statements",1870,"postponed","2016-02-01T14:13:07.153","2016-02-01T14:37:24.980","","","Rel-13","","","QOSE2EMTSI-CT","","","","",null,"CT3","CT1, CT4"]
["C3-160188","Reply LS on Multi-stream Multiparty Conferencing Media Handling","SA4","Tomas Frankkila",25766,"LS in","","Discussion","","","13","6","Received Liaison Statements",1880,"noted","2016-02-01T14:15:57.817","2016-02-01T14:37:25.027","","","Rel-13","","","MMCMH","","","","",null,"CT3, CT1","CT4, CT"]
["C3-160189","LS on EVS over CS","SA4","Imre Varga",16587,"LS in","","Discussion","","","13","6","Received Liaison Statements",1890,"replied to","2016-02-01T14:20:29.147","2016-02-01T14:37:25.057","","","Rel-13","","","EVSoCS","","","","",null,"RAN1, RAN2, CT1, CT3, CT4","RAN3, TSG-SA",null,"C3-160393"]
["C3-160190","LS on Charging Id assignment for NBIFOM","SA5","David Shrader",46800,"LS in","","Information","","","13","6","Received Liaison Statements",1900,"noted","2016-02-01T14:24:01.100","2016-02-01T14:37:25.090","","","Rel-13","","","NBIFOM-CT","","","","",null,"3GPP TSG SA WG2","3GPP TSG CT WG3, 3GPP TSG CT WG4"]
["C3-160191","Reply LS to CT4 LS on progress of the work on Diameter Base Protocol Update","3GPP TSG SA5","Maryse Gardella",33757,"LS in","","Discussion","","","13","6","Received Liaison Statements",1910,"noted","2016-02-01T14:35:29.400","2016-02-01T14:37:25.120","","","Rel-14","","","FS_DBPU","","","","",null,"3GPP TSG CT4","3GPP TSG CT3, 3GPP TSG SA3"]
["C3-160192","Adding ENODEB_CHANGE event trigger","China Mobile Com. Corporation, ZTE, Allot Communications, China Unicom, Huawei","Zhenning Huang",60086,"CR","","Agreement","This CR implements a new event trigger ENODEB_CHANGE in Event-Trigger mechanism, and this CR is applicable to macro eNodeB.\nThe PCEF supply the eNodeB ID reusing the ECGI of 3GPP-User-Location-Info AVP and the 20 leftmost bits contained the ID of the eNod","","228","14.1.2","TEI14 for Packet Core",1920,"postponed","2016-02-01T14:48:14.450","2016-02-01T15:15:48.430","C3-155195","C3-161150","Rel-14","29.212","13.4.0","TEI14","1401","1","B",null,"","","","",""]
["C3-160193","Corrections to EVS AMR-WB IO mode-change-capability MIME parameter handling","Nokia Networks","Thomas Belling",23293,"CR","","Agreement","The handling of the EVS AMR-WB IO mode-change-capability MIME parameter  is aligned with recent changes agreed by SA4.","","187","12.34","CT Impacts of Codec for Enhanced Voice Services [EVS_codec-CT]",1930,"agreed","2016-02-01T14:53:39.007","2016-02-01T15:43:06.420","","","Rel-12","29.163","12.10.0","EVS_codec-CT","0969","","F","CP-160111","","","","",""]
["C3-160194","Corrections to EVS AMR-WB IO mode-change-capability MIME parameter handling","Nokia Networks","Thomas Belling",23293,"CR","","Agreement","The handling of the EVS AMR-WB IO mode-change-capability MIME parameter  is aligned with recent changes agreed by SA4.","","187","12.34","CT Impacts of Codec for Enhanced Voice Services [EVS_codec-CT]",1940,"revised","2016-02-01T15:14:45.343","2016-02-01T15:43:06.340","","C3-160230","Rel-13","29.163","13.4.0","EVS_codec-CT","0970","","A",null,"","","","",""]
["C3-160195","Reservation-Priority AVP and DRMP AVP Interaction","ACS, OEC, AT&T,Alcatel-Lucent, Alcatel-Lucent Shanghai Bell and  Nokia Networks","Viqar Shaikh",56720,"CR","","Agreement","","","219","13.28","Diameter Message Priority [DiaPri]",1950,"revised","2016-02-01T15:23:47.253","2016-02-01T15:35:29.047","","C3-160301","Rel-13","29.214","13.4.0","DiaPri","0446","","B",null,"","","","",""]
["C3-160196","Corrections to EVS AMR-WB IO mode-change-capability MIME parameter handling","Nokia Networks","Thomas Belling",23293,"CR","","Agreement","The handling of the EVS AMR-WB IO mode-change-capability MIME parameter  is aligned with recent changes agreed by SA4.","","201","13.10","CT aspects of EVS in 3G Circuit-Switched Networks [EVSoCS-CT]",1960,"merged","2016-02-01T15:31:02.787","2016-02-01T15:43:06.387","","","Rel-13","29.163","13.4.0","EVSoCS-CT","0971","","F",null,"","","","",""]
["C3-160197","New study item on PCRF failure and restoration enhancement","China Mobile Com. Corporation","Zhenning Huang",60086,"SID new","","","study an optional enhanced PCRF restoration procedure to support the scenario that the AF (e.g. P-CSCF) contacts with the PCRF before the PCEF/BBERF contacts with the PCRF after the PCRF failure (e.g. IMS initialing call).","","232","14.5","Study item on PCRF failure and restoration enhancement [FS_PCRF-eFR]",1970,"revised","2016-02-01T17:32:58.967","2016-02-01T17:40:26.640","","C3-160211","Rel-14","","","","","","","","","","","",""]
["C3-160198","MB2 Interface Enhancements","SAMSUNG Electronics Co., Ltd.","Prakash Kolan",63609,"WID new","","Discussion","","","233","14.6","MB2 Interface Enhancements [eMB2]",1980,"noted","2016-02-01T23:41:13.913","2016-02-04T23:35:35.247","","","Rel-14","29.468","","","","","","","","","","",""]
["C3-160199","Proposed Revision of CT3 ToR","3GPP CT3 Chairman","Weihua Qiao",42235,"other","","Information","","","12","5.3","Other items for immediate consideration",1990,"revised","2016-02-04T08:41:19.850","2016-02-08T14:58:46.237","C3-160010","C3-160208","","","","","","","","","","","","",""]
["C3-160200","Reporting of NAS/RAN cause in the STR command","Ericsson LM","Saurav Arora",62621,"CR","","Agreement","","","190","12.35.2","TEI12 for Packet Core",2000,"withdrawn","2016-02-04T13:26:07.833",null,"C3-160109","","Rel-12","29.214","12.10.0","PCC, TEI12","0447","","F",null,"","","","",""]
["C3-160201","Reporting of NAS/RAN cause in the STR command","Ericsson LM","Susana Fernandez",42321,"CR","","Agreement","","","190","12.35.2","TEI12 for Packet Core",2010,"revised","2016-02-04T13:30:07.587","2016-02-04T15:54:49.603","","C3-160235","Rel-12","29.214","12.10.0","PCC, TEI12","0447","1","F",null,"","","","",""]
["C3-160202","Revised WID on Controlling IMS Media Plane with SDP Capability Negotiation","Huawei","Weiwei(Tommy) YANG",55591,"WID revised","","Approval","The SDP capability negotiation, as defined in IETF RFC 5939, enables SDP to provide limited support for indicating capabilities and their associated potential configurations, and negotiate the use of those potential configurations as actual configurations","","203","13.12","Controlling IMS Media Plane with SDP Capability Negotiation [SDPCN_IMS]",2020,"withdrawn","2016-02-04T16:08:33.277","2016-02-04T16:12:57.617","CP-150238","","Rel-13","","","SDPCN_IMS","","","","","","","","",""]
["C3-160203","Diameter message priority over MB2-C","Applied Communication Sciences, OEC, AT&T, Alcatel-Lucent Alcatel-Lucent Shanghai Bell and Nokia Networks","Viqar Shaikh",56720,"CR","","Agreement","Diameter message priority over MB2-C interface is added and refers to the current IETF draft-ietf-dime-drmp-02.","","219","13.28","Diameter Message Priority [DiaPri]",2030,"revised","2016-02-05T16:29:00.227","2016-02-05T19:46:37.553","","C3-160305","Rel-13","29.468","13.0.0","DiaPri","0019","","B",null,"","","","",""]
["C3-160204","WebRTC media plane optimization procedure","Nokia Networks , Alcatel-Lucent","Thomas Belling",23293,"CR","","Agreement","Media Plane Optimization procedures for WebRTC are specified. The eIMS-AGW is configured with transport \"UDP\", as all higher protocol layers need to be passed without modification.","","216","13.25","Enhancements to WEBRTC interoperability stage 3 [eWebRTCi_CT]",2040,"revised","2016-02-08T07:10:27.287","2016-02-08T11:32:57.900","C3-160177","C3-160279","Rel-13","29.162","13.1.0","eWebRTCi-CT ","0152","1","B",null,"","","","",""]
["C3-160205","New subclause to Appendix A for the handling of MCPTT emergency calls","Motorola Solution Inc.","Baruh Hason",58708,"CR","","Agreement","","","215","13.24","Mission Critical Push To Talk over LTE protocol aspects [MCPTT-CT]",2050,"revised","2016-02-08T09:24:59.130","2016-02-11T16:13:18.467","","C3-160318","Rel-13","29.214","13.4.0","MCPTT-CT","0448","","B",null,"","","","",""]
["C3-160206","29.165 rel-13 Addressed MCPTT SIP interfaces","Ericsson Nokia Networks, Alcatel-Lucent, Alcatel-Lucent Shanghai Bell","Jan Holm",12624,"CR","","Agreement","","","215","13.24","Mission Critical Push To Talk over LTE protocol aspects [MCPTT-CT]",2060,"revised","2016-02-08T11:07:26.347","2016-02-08T11:15:57.387","","C3-160325","Rel-13","29.165","13.3.0","MCPTT-CT","0821","","F",null,"","","","",""]
["C3-160207","The value of ARP for MCPTT emergency","Motorola Solutions Danmark A/S","Baruh Hason",58708,"CR","","Agreement","","","215","13.24","Mission Critical Push To Talk over LTE protocol aspects [MCPTT-CT]",2070,"revised","2016-02-11T08:38:51.773","2016-02-11T16:13:18.433","","C3-160320","Rel-13","29.213","13.4.0","MCPTT-CT","0657","","B",null,"","","","",""]
["C3-160208","Proposed Revision of CT3 ToR","3GPP CT3 Chairman","Saurav Arora",62621,"other","","Information","","","12","5.3","Other items for immediate consideration",1991,"revised","2016-02-22T10:24:11.680","2016-03-01T15:03:20.400","C3-160199","C3-160394","","","","","","","","","","","","",""]
["C3-160209","Reply to: LS on EVS over CS","CT3","Saurav Arora",62621,"LS out","","Approval","","","13","6","Received Liaison Statements",1891,"revised","2016-02-22T10:24:11.757","2016-03-01T15:03:20.417","","C3-160393","Rel-13","","","EVSoCS","","","","","C3-160189","SA4","CT4"]
["C3-160210","New WID Representational State Transfer (REST) reference point between Service Capability Exposure Function (SCEF) and Protocol Converter (PC)","ZTE Corporation","Saurav Arora",62621,"WID new","","Endorsement","","","230","14.3","Representational State Transfer (REST) reference point between Service Capability Exposure Function (SCEF) and Protocol Converter (PC) [REST_SCEF_PC]",591,"postponed","2016-02-22T10:24:11.850",null,"C3-160059","","","","","","","","","","","","","",""]
["C3-160211","New study item on PCRF failure and restoration enhancement","China Mobile Com. Corporation","Saurav Arora",62621,"SID new","","Endorsement","","","232","14.5","Study item on PCRF failure and restoration enhancement [FS_PCRF-eFR]",1971,"withdrawn","2016-02-22T10:24:11.927",null,"C3-160197","","Rel-14","","","","","","","","","","","",""]
["C3-160212","CT aspects of MTSI Extension on Multi-stream Multiparty Conferencing Media Handling","Ericsson","Saurav Arora",62621,"WID new","","Endorsement","","","229","14.2","CT aspects of MTSI Extension on Multi-stream Multiparty Conferencing Media Handling [MMCMH-CT]",261,"endorsed","2016-02-22T10:24:12.023","2016-03-01T15:03:20.417","C3-160026","","Rel-14","","","","","","","","","","","",""]
["C3-160213","LS on new AVPs in TS 29.212","Nokia Networks","Saurav Arora",62621,"LS out","","Approval","","","223","13.30.2","TEI13 for Packet Core",1801,"revised","2016-02-22T10:24:12.117","2016-03-01T15:03:20.417","C3-160180","C3-160361","Rel-13","29.212","","PCC, TEI13","","","",""]
["C3-160214","LS to CT4 on allocation of new Diameter Application ID and commands code for PC2 protocol","Huawei, Qualcomm","Saurav Arora",62621,"LS out","","Approval","","","206","13.15","CT aspects of enhancements to Proximity-based Services extensions [eProSe-Ext-CT]",1021,"approved","2016-02-22T10:24:12.193","2016-03-01T15:03:20.433","C3-160102","","Rel-13","","","eProSe-Ext-CT","","","","",null,"CT4",null,null,"C4-162270"]
["C3-160215","CR Incorrect use of the term \"full hexadecimal representation\" to mean binary incoding","Oracle Corporation","Saurav Arora",62621,"CR","","Agreement","","","223","13.30.2","TEI13 for Packet Core",21500,"agreed","2016-02-22T10:24:12.317","2016-03-01T15:03:20.433","","C3-160354","Rel-13","29.212","13.4.0","TEI13, CNO_ULI-CT","1430","","F","CP-160101","","","","",""]
["C3-160216","Diameter St Error Notifications","Nokia Networks,ZTE","Saurav Arora",62621,"CR","","Agreement","","","211","13.20","CT3 Aspect of Flexible Mobile Service Steering [FMSS-CT]",1641,"revised","2016-02-22T10:24:15.143","2016-03-01T15:03:20.433","C3-160164","C3-160370","Rel-13","29.212","13.4.0","FMSS-CT","1427","1","B",null,"","","","",""]
["C3-160217","ADC rule error handling report initiated by the TSSF","ZTE,Nokia Networks","Saurav Arora",62621,"CR","","Agreement","","","211","13.20","CT3 Aspect of Flexible Mobile Service Steering [FMSS-CT]",761,"revised","2016-02-22T10:24:15.297","2016-03-01T15:03:20.433","C3-160076","C3-160340","Rel-13","29.213","13.4.0","FMSS-CT","0639","1","B",null,"","","","",""]
["C3-160218","IPv4 address provisioning","ZTE","Saurav Arora",62621,"CR","","Agreement","","","211","13.20","CT3 Aspect of Flexible Mobile Service Steering [FMSS-CT]",771,"revised","2016-02-22T10:24:15.470","2016-03-01T15:03:20.433","C3-160077","C3-160341","Rel-13","29.212","13.4.0","FMSS-CT","1411","1","F",null,"","","","",""]
["C3-160219","Update the scope to include the St interface","Huawei","Saurav Arora",62621,"CR","","Agreement","","","211","13.20","CT3 Aspect of Flexible Mobile Service Steering [FMSS-CT]",1061,"revised","2016-02-22T10:24:15.703","2016-03-01T15:03:20.433","C3-160106","C3-160342","Rel-13","29.213","13.4.0","FMSS-CT","0645","1","F",null,"","","","",""]
["C3-160220","Traffic Steering Rule Error handling over the REST based St interface","Oracle Corporation","Saurav Arora",62621,"CR","","Agreement","","","211","13.20","CT3 Aspect of Flexible Mobile Service Steering [FMSS-CT]",1391,"revised","2016-02-22T10:24:15.907","2016-03-01T15:03:20.433","C3-160139","C3-160376","Rel-13","29.155","13.0.0","FMSS-CT","0001","1","B",null,"","","","",""]
["C3-160221","Interworking of History-Info Header Field when Original Called Number is not present","Deutsche Telekom / Michael","Saurav Arora",62621,"CR","","Agreement","When the MGC receives an ISUP IAM with a \"Redirection Information Parameter\" and a \"Redirecting Number Parameter\" but the \"Original Called Number Parameter\" is not included, the Call Diversion information is lost during the ISUP-SIP Interworking.","","15","8.2","Interworking between IM Subsystem with CS  [IMS-CCR-IWCS]",22100,"revised","2016-02-22T10:24:16.047","2016-03-01T15:03:20.433","C3-160017","C3-160397","Rel-8","29.163","8.29.0","IMS-CCR-IWCS","0948","1","F",null,"","","","",""]
["C3-160222","Interworking of History-Info Header Field when Original Called Number is not present","Deutsche Telekom / Michael","Saurav Arora",62621,"CR","","Agreement","When the MGC receives an ISUP IAM with a \"Redirection Information Parameter\" and a \"Redirecting Number Parameter\" but the \"Original Called Number Parameter\" is not included, the Call Diversion information is lost during the ISUP-SIP Interworking.","","15","8.2","Interworking between IM Subsystem with CS  [IMS-CCR-IWCS]",22200,"revised","2016-02-22T10:24:16.233","2016-03-01T15:03:20.450","C3-160018","C3-160398","Rel-9","29.163","9.23.0","IMS-CCR-IWCS","0949","1","A",null,"","","","",""]
["C3-160223","Interworking of History-Info Header Field when Original Called Number is not present","Deutsche Telekom / Michael","Saurav Arora",62621,"CR","","Agreement","When the MGC receives an ISUP IAM with a \"Redirection Information Parameter\" and a \"Redirecting Number Parameter\" but the \"Original Called Number Parameter\" is not included, the Call Diversion information is lost during the ISUP-SIP Interworking.","","15","8.2","Interworking between IM Subsystem with CS  [IMS-CCR-IWCS]",22300,"revised","2016-02-22T10:24:16.390","2016-03-01T15:03:20.467","C3-160019","C3-160399","Rel-10","29.163","10.19.0","IMS-CCR-IWCS","0950","1","A",null,"","","","",""]
["C3-160224","Interworking of History-Info Header Field when Original Called Number is not present","Deutsche Telekom / Michael","Saurav Arora",62621,"CR","","Agreement","When the MGC receives an ISUP IAM with a \"Redirection Information Parameter\" and a \"Redirecting Number Parameter\" but the \"Original Called Number Parameter\" is not included, the Call Diversion information is lost during the ISUP-SIP Interworking.","","15","8.2","Interworking between IM Subsystem with CS  [IMS-CCR-IWCS]",22400,"revised","2016-02-22T10:24:16.560","2016-03-01T15:03:20.467","C3-160020","C3-160400","Rel-11","29.163","11.16.0","IMS-CCR-IWCS","0951","1","A",null,"","","","",""]
["C3-160225","Interworking of History-Info Header Field when Original Called Number is not present","Deutsche Telekom / Michael","Saurav Arora",62621,"CR","","Agreement","When the MGC receives an ISUP IAM with a \"Redirection Information Parameter\" and a \"Redirecting Number Parameter\" but the \"Original Called Number Parameter\" is not included, the Call Diversion information is lost during the ISUP-SIP Interworking.","","15","8.2","Interworking between IM Subsystem with CS  [IMS-CCR-IWCS]",22500,"revised","2016-02-22T10:24:16.717","2016-03-01T15:03:20.467","C3-160021","C3-160401","Rel-12","29.163","12.10.0","IMS-CCR-IWCS","0952","1","A",null,"","","","",""]
["C3-160226","Interworking of History-Info Header Field when Original Called Number is not present","Deutsche Telekom / Michael","Saurav Arora",62621,"CR","","Agreement","When the MGC receives an ISUP IAM with a \"Redirection Information Parameter\" and a \"Redirecting Number Parameter\" but the \"Original Called Number Parameter\" is not included, the Call Diversion information is lost during the ISUP-SIP Interworking.","","15","8.2","Interworking between IM Subsystem with CS  [IMS-CCR-IWCS]",22600,"revised","2016-02-22T10:24:16.890","2016-03-01T15:03:20.467","C3-160022","C3-160402","Rel-13","29.163","13.4.0","IMS-CCR-IWCS","0953","1","A",null,"","","","",""]
["C3-160227","Correction for the SIP-ISUP interworking parameter","FUJITSU, NTT","Saurav Arora",62621,"CR","","Agreement","The interworking parameter about the SIP cause URI parameter to the ISUP Call Diversion Information is unclear in table 7.5.4.2.1.4. It should be corrected.","","15","8.2","Interworking between IM Subsystem with CS  [IMS-CCR-IWCS]",22700,"agreed","2016-02-22T10:24:17.060","2016-03-01T15:03:20.480","C3-160049","","Rel-13","29.163","13.4.0","IMS-CCR-IWCS, TEI13","0961","1","F","CP-160105","","","","",""]
["C3-160228","Updating \"Details for operator choice\" in DRVCC to include the STN","Ericsson","Saurav Arora",62621,"CR","","Agreement","","","162","12.9","Dual-Radio VCC Enhancements [eDRVCC]",22800,"agreed","2016-02-22T10:24:17.280","2016-03-01T15:03:20.480","C3-160036","","Rel-12","29.165","12.10.0","eDRVCC","0818","1","F","CP-160096","","","","",""]
["C3-160229","Updating \"Details for operator choice\" in DRVCC to include the STN","Ericsson","Saurav Arora",62621,"CR","","Agreement","","","162","12.9","Dual-Radio VCC Enhancements [eDRVCC]",22900,"agreed","2016-02-22T10:24:17.467","2016-03-01T15:03:20.480","C3-160037","","Rel-13","29.165","13.3.0","eDRVCC","0819","1","A","CP-160096","","","","",""]
["C3-160230","Corrections to EVS AMR-WB IO mode-change-capability MIME parameter handling","Nokia Networks","Saurav Arora",62621,"CR","","Agreement","The handling of the EVS AMR-WB IO mode-change-capability MIME parameter  is aligned with recent changes agreed by SA4.","","187","12.34","CT Impacts of Codec for Enhanced Voice Services [EVS_codec-CT]",23000,"revised","2016-02-22T10:24:17.637","2016-03-01T15:03:20.480","C3-160194","C3-160326","Rel-13","29.163","13.4.0","EVS_codec-CT","0970","1","F",null,"","","","",""]
["C3-160231","Support of enhanced bandwidth negotiation mechanism for MTSI sessions","Ericsson","Saurav Arora",62621,"CR","","Agreement","Specification of Ix procedures (stage 2) to support the enhanced bandwidth negotiation mechanism.","","194","13.3","CT Aspects of QoS End to End MTSI extensions [QOSE2EMTSI-CT]",23100,"revised","2016-02-22T10:24:17.793","2016-03-01T15:03:20.497","C3-160028","C3-160386","Rel-13","29.162","13.1.0","QOSE2EMTSI-CT","0150","1","B",null,"","","","",""]
["C3-160232","Support of enhanced bandwidth negotiation mechanism for MTSI sessions","Ericsson","Saurav Arora",62621,"CR","","Agreement","Specification of Ix procedures (stage 2) to support the enhanced bandwidth negotiation mechanism.","","194","13.3","CT Aspects of QoS End to End MTSI extensions [QOSE2EMTSI-CT]",23200,"revised","2016-02-22T10:24:17.967","2016-03-01T15:03:20.497","C3-160029","C3-160387","Rel-13","29.163","13.4.0","QOSE2EMTSI-CT","0954","1","B",null,"","","","",""]
["C3-160233","Capability of REST-Rx","ZTE","Saurav Arora",62621,"CR","","Agreement","Clarify the capability of REST-Rx","","161","12.8.1","Representational State Transfer (REST) reference point between Application Function (AF) and Protocol Converter (PC) [REST_AF_PC]",23300,"revised","2016-02-22T10:24:18.137","2016-03-01T15:03:20.497","C3-160064","C3-160363","Rel-12","29.201","12.3.0","REST_AF_PC","0033","1","F",null,"","","","",""]
["C3-160234","Capability of REST-Rx","ZTE","Saurav Arora",62621,"CR","","Agreement","Clarify the capability of REST-Rx","","161","12.8.1","Representational State Transfer (REST) reference point between Application Function (AF) and Protocol Converter (PC) [REST_AF_PC]",23400,"revised","2016-02-22T10:24:18.310","2016-03-01T15:03:20.497","C3-160065","C3-160364","Rel-13","29.201","13.3.0","REST_AF_PC","0034","1","A",null,"","","","",""]
["C3-160235","Reporting of NAS/RAN cause in the STR command","Ericsson LM","Saurav Arora",62621,"CR","","Agreement","","","190","12.35.2","TEI12 for Packet Core",23500,"revised","2016-02-22T10:24:18.480","2016-03-01T15:03:20.513","C3-160201","C3-160355","Rel-12","29.214","12.10.0","PCC, TEI12","0447","2","F",null,"","","","",""]
["C3-160236","Reporting of NAS/RAN cause in the STR command","Ericsson LM","Saurav Arora",62621,"CR","","Agreement","","","190","12.35.2","TEI12 for Packet Core",23600,"revised","2016-02-22T10:24:18.667","2016-03-01T15:03:20.513","C3-160110","C3-160356","Rel-13","29.214","13.4.0","PCC, TEI12","0437","1","A",null,"","","","",""]
["C3-160237","Completion of RAN-NAS cause handling procedures","Ericsson LM","Saurav Arora",62621,"CR","","Agreement","","","190","12.35.2","TEI12 for Packet Core",23700,"agreed","2016-02-22T10:24:18.840","2016-03-01T15:03:20.513","C3-160112","","Rel-12","29.213","12.10.0","PCC, TEI12","0647","1","F","CP-160100","","","","",""]
["C3-160238","Clarifications regarding Monitoring-Time procedures","Oracle Corporation","Saurav Arora",62621,"CR","","Agreement","Monitoring Time procedures defined in clause 4.5.17.6 are unclear with regards to resetting of the usage threshold","","190","12.35.2","TEI12 for Packet Core",23800,"agreed","2016-02-22T10:24:19.043","2016-03-01T15:03:20.513","C3-160147","","Rel-12","29.212","12.11.0","TEI12","1423","1","F","CP-160100","","","","",""]
["C3-160239","Clarifications regarding Monitoring-Time procedures","Oracle Corporation","Saurav Arora",62621,"CR","","Agreement","Monitoring Time procedures defined in clause 4.5.17.6 are unclear with regards to resetting of the usage threshold","","190","12.35.2","TEI12 for Packet Core",23900,"agreed","2016-02-22T10:24:19.213","2016-03-01T15:03:20.527","C3-160151","","Rel-13","29.212","13.4.0","TEI12","1424","1","A","CP-160100","","","","",""]
["C3-160240","nn","IMS break Out","Saurav Arora",62621,"other","","Information","","","15","8.2","Interworking between IM Subsystem with CS  [IMS-CCR-IWCS]",24000,"withdrawn","2016-02-22T10:24:19.400",null,"","","","","","","","","","","","","","",""]
["C3-160241","nn","IMS break Out","Saurav Arora",62621,"other","","Information","","","15","8.2","Interworking between IM Subsystem with CS  [IMS-CCR-IWCS]",24100,"withdrawn","2016-02-22T10:24:19.463",null,"","","","","","","","","","","","","","",""]
["C3-160242","nn","IMS break Out","Saurav Arora",62621,"other","","Information","","","15","8.2","Interworking between IM Subsystem with CS  [IMS-CCR-IWCS]",24200,"withdrawn","2016-02-22T10:24:19.540",null,"","","","","","","","","","","","","","",""]
["C3-160243","nn","IMS break Out","Saurav Arora",62621,"other","","Information","","","15","8.2","Interworking between IM Subsystem with CS  [IMS-CCR-IWCS]",24300,"withdrawn","2016-02-22T10:24:19.603",null,"","","","","","","","","","","","","","",""]
["C3-160244","nn","IMS break Out","Saurav Arora",62621,"other","","Information","","","15","8.2","Interworking between IM Subsystem with CS  [IMS-CCR-IWCS]",24400,"withdrawn","2016-02-22T10:24:19.680",null,"","","","","","","","","","","","","","",""]
["C3-160245","nn","IMS break Out","Saurav Arora",62621,"other","","Information","","","15","8.2","Interworking between IM Subsystem with CS  [IMS-CCR-IWCS]",24500,"withdrawn","2016-02-22T10:24:19.760",null,"","","","","","","","","","","","","","",""]
["C3-160246","nn","IMS break Out","Saurav Arora",62621,"other","","Information","","","15","8.2","Interworking between IM Subsystem with CS  [IMS-CCR-IWCS]",24600,"withdrawn","2016-02-22T10:24:19.837",null,"","","","","","","","","","","","","","",""]
["C3-160247","nn","IMS break Out","Saurav Arora",62621,"other","","Information","","","15","8.2","Interworking between IM Subsystem with CS  [IMS-CCR-IWCS]",24700,"withdrawn","2016-02-22T10:24:19.930",null,"","","","","","","","","","","","","","",""]
["C3-160248","nn","IMS break Out","Saurav Arora",62621,"other","","Information","","","15","8.2","Interworking between IM Subsystem with CS  [IMS-CCR-IWCS]",24800,"withdrawn","2016-02-22T10:24:20.010",null,"","","","","","","","","","","","","","",""]
["C3-160249","nn","IMS break Out","Saurav Arora",62621,"other","","Information","","","15","8.2","Interworking between IM Subsystem with CS  [IMS-CCR-IWCS]",24900,"withdrawn","2016-02-22T10:24:20.070",null,"","","","","","","","","","","","","","",""]
["C3-160250","nn","IMS break Out","Saurav Arora",62621,"other","","Information","","","15","8.2","Interworking between IM Subsystem with CS  [IMS-CCR-IWCS]",25000,"withdrawn","2016-02-22T10:24:20.133",null,"","","","","","","","","","","","","","",""]
["C3-160251","nn","IMS break Out","Saurav Arora",62621,"other","","Information","","","15","8.2","Interworking between IM Subsystem with CS  [IMS-CCR-IWCS]",25100,"withdrawn","2016-02-22T10:24:20.213",null,"","","","","","","","","","","","","","",""]
["C3-160252","nn","IMS break Out","Saurav Arora",62621,"other","","Information","","","15","8.2","Interworking between IM Subsystem with CS  [IMS-CCR-IWCS]",25200,"withdrawn","2016-02-22T10:24:20.273",null,"","","","","","","","","","","","","","",""]
["C3-160253","nn","IMS break Out","Saurav Arora",62621,"other","","Information","","","15","8.2","Interworking between IM Subsystem with CS  [IMS-CCR-IWCS]",25300,"withdrawn","2016-02-22T10:24:20.353",null,"","","","","","","","","","","","","","",""]
["C3-160254","nn","IMS break Out","Saurav Arora",62621,"other","","Information","","","15","8.2","Interworking between IM Subsystem with CS  [IMS-CCR-IWCS]",25400,"withdrawn","2016-02-22T10:24:20.417",null,"","","","","","","","","","","","","","",""]
["C3-160255","nn","IMS break Out","Saurav Arora",62621,"other","","Information","","","15","8.2","Interworking between IM Subsystem with CS  [IMS-CCR-IWCS]",25500,"withdrawn","2016-02-22T10:24:20.493",null,"","","","","","","","","","","","","","",""]
["C3-160256","nn","IMS break Out","Saurav Arora",62621,"other","","Information","","","15","8.2","Interworking between IM Subsystem with CS  [IMS-CCR-IWCS]",25600,"withdrawn","2016-02-22T10:24:20.570",null,"","","","","","","","","","","","","","",""]
["C3-160257","nn","IMS break Out","Saurav Arora",62621,"other","","Information","","","15","8.2","Interworking between IM Subsystem with CS  [IMS-CCR-IWCS]",25700,"withdrawn","2016-02-22T10:24:20.663",null,"","","","","","","","","","","","","","",""]
["C3-160258","nn","IMS break Out","Saurav Arora",62621,"other","","Information","","","15","8.2","Interworking between IM Subsystem with CS  [IMS-CCR-IWCS]",25800,"withdrawn","2016-02-22T10:24:20.743",null,"","","","","","","","","","","","","","",""]
["C3-160259","nn","IMS break Out","Saurav Arora",62621,"other","","Information","","","15","8.2","Interworking between IM Subsystem with CS  [IMS-CCR-IWCS]",25900,"withdrawn","2016-02-22T10:24:20.820",null,"","","","","","","","","","","","","","",""]
["C3-160260","nn","IMS break Out","Saurav Arora",62621,"other","","Information","","","15","8.2","Interworking between IM Subsystem with CS  [IMS-CCR-IWCS]",26000,"withdrawn","2016-02-22T10:24:20.897",null,"","","","","","","","","","","","","","",""]
["C3-160261","Miscellaneous corrections related to the REST based St","Oracle Corporation","Saurav Arora",62621,"CR","","Agreement","","","211","13.20","CT3 Aspect of Flexible Mobile Service Steering [FMSS-CT]",1401,"agreed","2016-02-22T10:24:20.977","2016-03-01T15:03:20.560","C3-160140","","Rel-13","29.155","13.0.0","FMSS-CT","0002","1","F","CP-160091","","","","",""]
["C3-160262","Updates to JSON content rules for the notification procedures from the TSSF to the PCRF","Oracle Corporation","Saurav Arora",62621,"CR","","Agreement","","","211","13.20","CT3 Aspect of Flexible Mobile Service Steering [FMSS-CT]",1411,"revised","2016-02-22T10:24:21.163","2016-03-01T15:03:20.560","C3-160141","C3-160373","Rel-13","29.155","13.0.0","FMSS-CT","0003","1","B",null,"","","","",""]
["C3-160263","JSON content rules updates for error responses with traffic steering rule reports over the REST based St interface","Oracle Corporation","Saurav Arora",62621,"CR","","Agreement","","","211","13.20","CT3 Aspect of Flexible Mobile Service Steering [FMSS-CT]",1421,"agreed","2016-02-22T10:24:21.350","2016-03-01T15:03:20.560","C3-160142","","Rel-13","29.155","13.0.0","FMSS-CT","0004","1","B","CP-160091","","","","",""]
["C3-160264","Traffic steering rule report JSON Content Rules over St","Oracle Corporation","Saurav Arora",62621,"CR","","Agreement","","","211","13.20","CT3 Aspect of Flexible Mobile Service Steering [FMSS-CT]",1431,"revised","2016-02-22T10:24:21.553","2016-03-01T15:03:20.577","C3-160143","C3-160374","Rel-13","29.155","13.0.0","FMSS-CT","0005","1","B",null,"","","","",""]
["C3-160265","REST-Rx enhancement for Change of chargeable party","ZTE","Saurav Arora",62621,"CR","","Agreement","","","207","13.16","CT aspects of Architecture Enhancements for Service Capability Exposure [AESE-CT]",721,"agreed","2016-02-22T10:24:21.710","2016-03-01T15:03:20.577","C3-160072","","Rel-13","29.201","13.3.0","AESE-CT","0035","1","B","CP-160095","","","","",""]
["C3-160266","Rx impact for background data transfer","ZTE, Ericsson","Saurav Arora",62621,"CR","","Agreement","","","207","13.16","CT aspects of Architecture Enhancements for Service Capability Exposure [AESE-CT]",731,"revised","2016-02-22T10:24:21.880","2016-03-01T15:03:20.577","C3-160073","C3-160334","Rel-13","29.214","13.4.0","AESE-CT","0435","1","B",null,"","","","",""]
["C3-160267","Rx impact for background data transfer","ZTE","Saurav Arora",62621,"CR","","Agreement","","","207","13.16","CT aspects of Architecture Enhancements for Service Capability Exposure [AESE-CT]",741,"revised","2016-02-22T10:24:22.037","2016-03-01T15:03:20.577","C3-160074","C3-160335","Rel-13","29.201","13.3.0","AESE-CT","0036","1","B",null,"","","","",""]
["C3-160268","Add the missing abbreviations","Huawei","Saurav Arora",62621,"CR","","Agreement","","","207","13.16","CT aspects of Architecture Enhancements for Service Capability Exposure [AESE-CT]",861,"agreed","2016-02-22T10:24:22.210","2016-03-01T15:03:20.577","C3-160086","","Rel-13","29.153","13.0.0","AESE-CT","0001","1","F","CP-160095","","","","",""]
["C3-160269","Signnalling flows over Ns reference point","Huawei","Saurav Arora",62621,"CR","","Agreement","","","207","13.16","CT aspects of Architecture Enhancements for Service Capability Exposure [AESE-CT]",891,"revised","2016-02-22T10:24:22.443","2016-03-01T15:03:20.590","C3-160089","C3-160336","Rel-13","29.153","13.0.0","AESE-CT","0004","1","F",null,"","","","",""]
["C3-160270","Add command codes and AVP numbers for Nt protocol","Huawei","Saurav Arora",62621,"CR","","Agreement","","","207","13.16","CT aspects of Architecture Enhancements for Service Capability Exposure [AESE-CT]",901,"agreed","2016-02-22T10:24:22.630","2016-03-01T15:03:20.590","C3-160090","","Rel-13","29.154","13.0.0","AESE-CT","0001","1","F","CP-160095","","","","",""]
["C3-160271","Missed Transfer-Request-Type AVP in the commands","Huawei","Saurav Arora",62621,"CR","","Agreement","","","207","13.16","CT aspects of Architecture Enhancements for Service Capability Exposure [AESE-CT]",911,"revised","2016-02-22T10:24:22.833","2016-03-01T15:03:20.590","C3-160091","C3-160337","Rel-13","29.154","13.0.0","AESE-CT","0002","1","F",null,"","","","",""]
["C3-160272","Some corrections for Nt protocol","Huawei","Saurav Arora",62621,"CR","","Agreement","","","207","13.16","CT aspects of Architecture Enhancements for Service Capability Exposure [AESE-CT]",921,"revised","2016-02-22T10:24:23.020","2016-03-01T15:03:20.607","C3-160092","C3-160338","Rel-13","29.154","13.0.0","AESE-CT","0003","1","F",null,"","","","",""]
["C3-160273","Update the scope to include the Nt interface","Huawei","Saurav Arora",62621,"CR","","Agreement","","","207","13.16","CT aspects of Architecture Enhancements for Service Capability Exposure [AESE-CT]",931,"revised","2016-02-22T10:24:23.223","2016-03-01T15:03:20.607","C3-160093","C3-160339","Rel-13","29.213","13.4.0","AESE-CT","0641","1","B",null,"","","","",""]
["C3-160274","Correction to wrongly Experimental-Result-Code values for PC2 interface","Huawei","Saurav Arora",62621,"CR","","Agreement","","","206","13.15","CT aspects of enhancements to Proximity-based Services extensions [eProSe-Ext-CT]",27400,"revised","2016-02-22T10:24:23.393","2016-03-01T15:03:20.607","","C3-160329","Rel-13","29.343","13.1.0","eProSe-Ext-CT","0020","","F",null,"","","","",""]
["C3-160275","Adding \"Timer N\" in the timer table","Ericsson","Saurav Arora",62621,"CR","","Agreement","","","198","13.7","IMS Stage-3 IETF Protocol Alignment [IMSProtoc7]",351,"agreed","2016-02-22T10:24:23.847","2016-03-01T15:03:20.607","C3-160035","","Rel-13","29.165","13.3.0","IMSProtoc7","0817","1","F","CP-160098","","","","",""]
["C3-160276","Resolution of Editor’s notes on EVS over UMTS CS","Qualcomm Incorporated","Saurav Arora",62621,"CR","","Agreement","","","201","13.10","CT aspects of EVS in 3G Circuit-Switched Networks [EVSoCS-CT]",411,"agreed","2016-02-22T10:24:24.033","2016-03-01T15:03:20.620","C3-160041","","Rel-13","29.163","13.4.0","EVSoCS-CT","0955","1","B","CP-160112","","","","",""]
["C3-160277","Resolution of Editor’s notes on EVS over UMTS CS","Qualcomm Incorporated","Saurav Arora",62621,"CR","","Agreement","","","201","13.10","CT aspects of EVS in 3G Circuit-Switched Networks [EVSoCS-CT]",421,"agreed","2016-02-22T10:24:24.237","2016-03-01T15:03:20.620","C3-160042","","Rel-13","29.414","13.0.0","EVSoCS-CT","0040","1","B","CP-160112","","","","",""]
["C3-160278","Resolution of Editor’s notes on EVS over UMTS CS","Qualcomm Incorporated","Saurav Arora",62621,"CR","","Agreement","","","201","13.10","CT aspects of EVS in 3G Circuit-Switched Networks [EVSoCS-CT]",431,"agreed","2016-02-22T10:24:24.457","2016-03-01T15:03:20.620","C3-160043","","Rel-13","29.415","13.0.0","EVSoCS-CT","0018","1","B","CP-160112","","","","",""]
["C3-160279","WebRTC media plane optimization procedure","Nokia Networks , Alcatel-Lucent","Saurav Arora",62621,"CR","","Agreement","","","216","13.25","Enhancements to WEBRTC interoperability stage 3 [eWebRTCi_CT]",2041,"revised","2016-02-22T10:24:24.657","2016-03-01T15:03:20.620","C3-160204","C3-160372","Rel-13","29.162","13.1.0","eWebRTCi-CT ","0152","2","B",null,"","","","",""]
["C3-160280","Format of Type 1 orig-ioi and term-ioi","Ericsson","Saurav Arora",62621,"CR","","Agreement","","","222","13.30.1","TEI13 for IMS/CS",381,"postponed","2016-02-22T10:24:24.847","2016-03-01T15:03:20.620","C3-160038","","Rel-13","29.165","13.3.0","TEI13","0820","1","F",null,"","","","",""]
["C3-160281","Coding of type 1 and type orig-ioi and term-ioi","Ericsson","Saurav Arora",62621,"CR","","Agreement","","","222","13.30.1","TEI13 for IMS/CS",391,"postponed","2016-02-22T10:24:25.033","2016-03-01T15:03:20.637","C3-160039","","Rel-13","29.949","13.3.0","TEI13","0011","1","F",null,"","","","",""]
["C3-160282","Clarification on the setting of the SIP message compnents","NTT","Saurav Arora",62621,"CR","","Agreement","","","222","13.30.1","TEI13 for IMS/CS",551,"revised","2016-02-22T10:24:25.237","2016-03-01T15:03:20.637","C3-160055","C3-160327","Rel-13","29.163","13.4.0","TEI13, IMS-CCR-IWCS","0967","1","F",null,"","","","",""]
["C3-160283","Removal of references to TS 26.235","Nokia Networks, Alcatel-Lucent","Saurav Arora",62621,"CR","","Agreement","","","222","13.30.1","TEI13 for IMS/CS",1601,"agreed","2016-02-22T10:24:25.453","2016-03-01T15:03:20.637","C3-160160","","Rel-13","29.292","13.2.0","TEI13","0130","1","F","CP-160105","","","","",""]
["C3-160284","UE-to-network relay PCC handling","Ericsson, Huawei","Saurav Arora",62621,"CR","","Agreement","","","206","13.15","CT aspects of enhancements to Proximity-based Services extensions [eProSe-Ext-CT]",1291,"agreed","2016-02-22T10:24:25.627","2016-03-01T15:03:20.637","C3-160129","","Rel-13","29.213","13.4.0","eProSe-Ext-CT","0651","1","B","CP-160092","","","","",""]
["C3-160285","UE-to-network relay PCC handling over Rx","Ericsson LM","Saurav Arora",62621,"CR","","Agreement","","","206","13.15","CT aspects of enhancements to Proximity-based Services extensions [eProSe-Ext-CT]",1251,"agreed","2016-02-22T10:24:25.797","2016-03-01T15:03:20.653","C3-160125","","Rel-13","29.214","13.4.0","eProSe-Ext-CT","0441","1","B","CP-160092","","","","",""]
["C3-160286","UE-to-network relay PCC handling over Gx","Ericsson LM","Saurav Arora",62621,"CR","","Agreement","","","206","13.15","CT aspects of enhancements to Proximity-based Services extensions [eProSe-Ext-CT]",1271,"revised","2016-02-22T10:24:25.967","2016-03-01T15:03:20.653","C3-160127","C3-160333","Rel-13","29.212","13.4.0","eProSe-Ext-CT","1419","1","B",null,"","","","",""]
["C3-160287","Metadata indicator for restricted discovery monitor request procedure","Qualcomm Incorporated","Saurav Arora",62621,"CR","","Agreement","","","206","13.15","CT aspects of enhancements to Proximity-based Services extensions [eProSe-Ext-CT]",1371,"revised","2016-02-22T10:24:26.140","2016-03-01T15:03:20.653","C3-160137","C3-160359","Rel-13","29.343","13.1.0","eProSe-Ext-CT","0018","1","F",null,"","","","",""]
["C3-160288","Open discovery procedures in PC2 interface for application-controlled extension","Qualcomm Incorporated","Saurav Arora",62621,"CR","","Agreement","","","206","13.15","CT aspects of enhancements to Proximity-based Services extensions [eProSe-Ext-CT]",1381,"agreed","2016-02-22T10:24:26.297","2016-03-01T15:03:20.653","C3-160138","","Rel-13","29.343","13.1.0","eProSe-Ext-CT","0019","1","F","CP-160092","","","","",""]
["C3-160289","Usage of the UDP port for default unicast encapsulation mode at the SGmb interface is required to support SYNC protocol","Nokia Networks, Alcatel-Lucent","Saurav Arora",62621,"CR","","Agreement","","","54","9.4","MBMS [MBMS]",1671,"revised","2016-02-22T10:24:26.453","2016-03-01T15:03:20.667","C3-160167","C3-160346","Rel-9","29.061","9.15.0","MBMS","0461","1","F",null,"","","","",""]
["C3-160290","Usage of the UDP port for default unicast encapsulation mode at the Gmb interface is required to support SYNC protocol","Nokia Networks","Saurav Arora",62621,"CR","","Agreement","","","54","9.4","MBMS [MBMS]",1681,"revised","2016-02-22T10:24:26.623","2016-03-01T15:03:20.667","C3-160168","C3-160347","Rel-10","29.061","10.13.0","MBMS","0462","1","A",null,"","","","",""]
["C3-160291","Usage of the UDP port for default unicast encapsulation mode at the Gmb interface is required to support SYNC protocol","Nokia Networks, Alcatel-Lucent","Saurav Arora",62621,"CR","","Agreement","","","54","9.4","MBMS [MBMS]",1701,"revised","2016-02-22T10:24:26.810","2016-03-01T15:03:20.667","C3-160170","C3-160348","Rel-11","29.061","11.11.0","MBMS","0463","1","A",null,"","","","",""]
["C3-160292","Usage of the UDP port for default unicast encapsulation mode at the Gmb interface is required to support SYNC protocol","Nokia Networks, Alcatel-Lucent","Saurav Arora",62621,"CR","","Agreement","","","54","9.4","MBMS [MBMS]",1721,"revised","2016-02-22T10:24:26.983","2016-03-01T15:03:20.667","C3-160172","C3-160349","Rel-12","29.061","12.11.0","MBMS","0464","1","A",null,"","","","",""]
["C3-160293","Usage of the UDP port for default unicast encapsulation mode at the Gmb interface is required to support SYNC protocol","Nokia Networks, Alcatel-Lucent","Saurav Arora",62621,"CR","","Agreement","","","54","9.4","MBMS [MBMS]",1751,"revised","2016-02-22T10:24:27.170","2016-03-01T15:03:20.683","C3-160175","C3-160350","Rel-13","29.061","13.2.0","MBMS","0465","1","B",null,"","","","",""]
["C3-160294","Time conditioned APN-AMBR handling","Ericsson, Verizon, Nokia Networks, Alcatel-Lucent, Alcatel-Lucent Shanghai Bell, Oracle Corporation","Saurav Arora",62621,"CR","","Agreement","","","223","13.30.2","TEI13 for Packet Core",571,"revised","2016-02-22T10:24:27.340","2016-03-01T15:03:20.683","C3-160057","C3-160345","Rel-13","29.212","13.4.0","PCC, TEI13","1406","1","B",null,"","","","",""]
["C3-160295","NAS/RAN cause handling at bearer termination failure","Ericsson, Alcatel-Lucent, Alcatel-Lucent Shanghai Bell, Nokia Networks, Huawei, ZTE","Saurav Arora",62621,"CR","","Agreement","","","223","13.30.2","TEI13 for Packet Core",1081,"revised","2016-02-22T10:24:27.513","2016-03-01T15:03:20.683","C3-160108","C3-160351","Rel-13","29.212","13.4.0","PCC, TEI13","1417","1","B",null,"","","","",""]
["C3-160296","RAN-NAS-Cause handling upon unsuccessful bearer termination over Rx","Ericsson, Alcatel-Lucent, Alcatel-Lucent Shanghai Bell, Nokia Networks, Huawei, ZTE","Saurav Arora",62621,"CR","","Agreement","","","223","13.30.2","TEI13 for Packet Core",1111,"revised","2016-02-22T10:24:27.700","2016-03-01T15:03:20.683","C3-160111","C3-160352","Rel-13","29.214","13.4.0","PCC, TEI13","0438","1","F",null,"","","","",""]
["C3-160297","Include the AN-Trusted element","ZTE","Saurav Arora",62621,"CR","","Agreement","","","223","13.30.2","TEI13 for Packet Core",811,"agreed","2016-02-22T10:24:27.870","2016-03-01T15:03:20.700","C3-160081","","Rel-13","29.201","13.3.0","TEI13","0038","1","B","CP-160101","","","","",""]
["C3-160298","Conveying the IMEI of devices to the EPC","Huawei","Saurav Arora",62621,"CR","","Agreement","","","223","13.30.2","TEI13 for Packet Core",1001,"agreed","2016-02-22T10:24:28.027","2016-03-01T15:03:20.700","C3-160100","","Rel-13","29.212","13.4.0","TEI13","1413","1","F","CP-160101","","","","",""]
["C3-160299","Diameter Message Priority over diameter based St interface","Huawei","Saurav Arora",62621,"CR","","Agreement","","","219","13.28","Diameter Message Priority [DiaPri]",951,"revised","2016-02-22T10:24:28.217","2016-03-01T15:03:20.700","C3-160095","C3-160343","Rel-13","29.212","13.4.0","DiaPri","1412","1","B",null,"","","","",""]
["C3-160300","Diameter Message Priority over Nt interface","Huawei","Saurav Arora",62621,"CR","","Agreement","","","219","13.28","Diameter Message Priority [DiaPri]",971,"revised","2016-02-22T10:24:28.387","2016-03-01T15:03:20.700","C3-160097","C3-160344","Rel-13","29.154","13.0.0","DiaPri","0004","1","B",null,"","","","",""]
["C3-160301","Reservation-Priority AVP and DRMP AVP Interaction","ACS, OEC, AT&T,Alcatel-Lucent, Alcatel-Lucent Shanghai Bell and  Nokia Networks","Saurav Arora",62621,"CR","","Agreement","","","219","13.28","Diameter Message Priority [DiaPri]",1951,"revised","2016-02-22T10:24:28.557","2016-03-01T15:03:20.717","C3-160195","C3-160391","Rel-13","29.214","13.4.0","DiaPri","0446","1","B",null,"","","","",""]
["C3-160302","DRMP over REST Interface","ACS, OEC, AT&T,Alcatel-Lucent, Alcatel-Lucent Shanghai Bell and  Nokia Networks","Saurav Arora",62621,"CR","","Agreement","","","219","13.28","Diameter Message Priority [DiaPri]",1531,"agreed","2016-02-22T10:24:28.730","2016-03-01T15:03:20.717","C3-160153","","Rel-13","29.201","13.3.0","DiaPri","0039","1","B","CP-160093","","","","",""]
["C3-160303","Reservation-Priority AVP and DRMP AVP Interaction","ACS, OEC, AT&T,Alcatel-Lucent, Alcatel-Lucent Shanghai Bell and  Nokia Networks","Saurav Arora",62621,"CR","","Agreement","","","219","13.28","Diameter Message Priority [DiaPri]",1541,"revised","2016-02-22T10:24:28.900","2016-03-01T15:03:20.717","C3-160154","C3-160390","Rel-13","29.213","13.4.0","DiaPri","0654","1","B",null,"","","","",""]
["C3-160304","Correction to eMPS algorithm","ACS, OEC, AT&T,Alcatel-Lucent, Alcatel-Lucent Shanghai Bell and  Nokia Networks","Saurav Arora",62621,"CR","","Agreement","","","223","13.30.2","TEI13 for Packet Core",30400,"agreed","2016-02-22T10:24:29.073","2016-03-01T15:03:20.717","","","Rel-13","29.213","13.4.0","TEI13, eMPS-CN","0658","","F","CP-160101","","","","",""]
["C3-160305","Diameter message priority over MB2-C","Applied Communication Sciences, OEC, AT&T, Alcatel-Lucent Alcatel-Lucent Shanghai Bell and Nokia Networks","Saurav Arora",62621,"CR","","Agreement","","","219","13.28","Diameter Message Priority [DiaPri]",2031,"revised","2016-02-22T10:24:31.553","2016-03-01T15:03:20.730","C3-160203","C3-160392","Rel-13","29.468","13.0.0","TEI13, GCSE_LTE-CT","0019","1","B",null,"","","","",""]
["C3-160306","Completion of RAN-NAS cause handling procedures","Ericsson LM,Nokia Networks,Alcatel-Lucent","Saurav Arora",62621,"CR","","Agreement","","","223","13.30.2","TEI13 for Packet Core",1151,"revised","2016-02-22T10:24:31.740","2016-03-01T15:03:20.730","C3-160115","C3-160353","Rel-13","29.213","13.4.0","PCC, TEI13","0648","1","F",null,"","","","",""]
["C3-160307","Support of removed filters when SIP Forking applies over Rx","Ericsson LM","Saurav Arora",62621,"CR","","Agreement","","","223","13.30.2","TEI13 for Packet Core",1331,"agreed","2016-02-22T10:24:31.943","2016-03-01T15:03:20.747","C3-160133","","Rel-13","29.214","13.4.0","PCC, TEI13","0442","1","F","CP-160101","","","","",""]
["C3-160308","Removal of references to TS 26.236","Nokia Networks, Alcatel-Lucent","Saurav Arora",62621,"CR","","Agreement","","","223","13.30.2","TEI13 for Packet Core",1581,"agreed","2016-02-22T10:24:32.130","2016-03-01T15:03:20.747","C3-160158","","Rel-13","29.213","13.4.0","TEI13","0656","1","F","CP-160101","","","","",""]
["C3-160309","INFO    Proposed Schedule for CT3#84","CT3 Chairman","Saurav Arora",62621,"other","","Information","","","3","2.2","Proposed Schedule",11,"noted","2016-02-22T10:24:32.317","2016-03-01T15:03:20.747","C3-160001","","","","","","","","","","","","","",""]
["C3-160310","Completion of NBIFOM","Ericsson, ZTE, Huawei","Saurav Arora",62621,"CR","","Agreement","","","205","13.14","CT aspects of IP Flow Mobility support for S2a and S2b Interfaces (NBIFOM) [NBIFOM-CT]",561,"revised","2016-02-22T10:24:32.410","2016-03-01T15:03:20.747","C3-160056","C3-160378","Rel-13","29.212","13.4.0","NBIFOM-CT","1405","1","B",null,"","","","",""]
["C3-160311","Network-initiated removal of one access from the PDN connection","ZTE","Saurav Arora",62621,"CR","","Agreement","","","205","13.14","CT aspects of IP Flow Mobility support for S2a and S2b Interfaces (NBIFOM) [NBIFOM-CT]",701,"revised","2016-02-22T10:24:32.583","2016-03-01T15:03:20.747","C3-160070","C3-160331","Rel-13","29.212","13.4.0","NBIFOM-CT","1409","1","F",null,"","","","",""]
["C3-160312","Correction for the PCEF procedures","Huawei","Saurav Arora",62621,"CR","","Agreement","","","205","13.14","CT aspects of IP Flow Mobility support for S2a and S2b Interfaces (NBIFOM) [NBIFOM-CT]",1441,"agreed","2016-02-22T10:24:32.787","2016-03-01T15:03:20.763","C3-160144","","Rel-13","29.212","13.4.0","NBIFOM-CT","1420","1","F","CP-160090","","","","",""]
["C3-160313","Correction to NBIFOM handling in roaming case","ZTE Corporation","Saurav Arora",62621,"CR","","Agreement","","","205","13.14","CT aspects of IP Flow Mobility support for S2a and S2b Interfaces (NBIFOM) [NBIFOM-CT]",1491,"revised","2016-02-22T10:24:32.987","2016-03-01T15:03:20.763","C3-160149","C3-160332","Rel-13","29.215","13.4.0","NBIFOM-CT","0402","1","F",null,"","","","",""]
["C3-160314","Add command codes and AVP numbers for Np protocol","Huawei","Saurav Arora",62621,"CR","","Agreement","","","192","13.1","CT aspects of User Plane Congestion Management (UPCON) for Building Block I [UPCON-DOTCON-CT]",851,"agreed","2016-02-22T10:24:33.177","2016-03-01T15:03:20.763","C3-160085","","Rel-13","29.217","13.2.0","UPCON-DOTCON-CT","0023","1","F","CP-160094","","","","",""]
["C3-160315","Include RCAF in the EPC-routed architecture","ZTE","Saurav Arora",62621,"CR","","Agreement","","","192","13.1","CT aspects of User Plane Congestion Management (UPCON) for Building Block I [UPCON-DOTCON-CT]",671,"agreed","2016-02-22T10:24:33.377","2016-03-01T15:03:20.763","C3-160067","","Rel-13","29.212","13.4.0","UPCON-DOTCON-CT","1407","1","F","CP-160094","","","","",""]
["C3-160316","Include TSSF and RCAF in the EPC-routed architecture","ZTE","Saurav Arora",62621,"CR","","Agreement","","","211","13.20","CT3 Aspect of Flexible Mobile Service Steering [FMSS-CT]",791,"agreed","2016-02-22T10:24:33.580","2016-03-01T15:03:20.777","C3-160079","","Rel-13","29.215","13.4.0","FMSS-CT, UPCON-DOTCON-CT","0400","1","B","CP-160091","","","","",""]
["C3-160317","Congestion Level for the specific user id","Huawei","Saurav Arora",62621,"CR","","Agreement","","","192","13.1","CT aspects of User Plane Congestion Management (UPCON) for Building Block I [UPCON-DOTCON-CT]",841,"agreed","2016-02-22T10:24:33.767","2016-03-01T15:03:20.777","C3-160084","","Rel-13","29.217","13.2.0","UPCON-DOTCON-CT","0022","1","F","CP-160094","","","","",""]
["C3-160318","New subclause to Appendix A for the handling of MCPTT emergency calls","Motorola Solution Inc.","Saurav Arora",62621,"CR","","Agreement","","","215","13.24","Mission Critical Push To Talk over LTE protocol aspects [MCPTT-CT]",2051,"revised","2016-02-22T10:24:33.970","2016-03-01T15:03:20.777","C3-160205","C3-160389","Rel-13","29.214","13.4.0","MCPTT-CT","0448","1","B",null,"","","","",""]
["C3-160319","LS on MCPTT priorities support over Rx","CT3","Saurav Arora",62621,"LS out","","Approval","","","215","13.24","Mission Critical Push To Talk over LTE protocol aspects [MCPTT-CT]",31900,"revised","2016-02-22T10:24:34.143","2016-03-01T15:03:20.777","","C3-160380","Rel-13","","","MCPTT-CT","","","","",null,"SA2","SA6"]
["C3-160320","The value of ARP for MCPTT emergency","Motorola Solutions Danmark A/S","Saurav Arora",62621,"CR","","Agreement","","","215","13.24","Mission Critical Push To Talk over LTE protocol aspects [MCPTT-CT]",2071,"agreed","2016-02-22T10:24:34.237","2016-03-01T15:03:20.777","C3-160207","","Rel-13","29.213","13.4.0","MCPTT-CT","0657","1","B","CP-160087","","","","",""]
["C3-160321","Adding MBMS usage info and location info procedure","Ericsson","Saurav Arora",62621,"CR","","Agreement","","","215","13.24","Mission Critical Push To Talk over LTE protocol aspects [MCPTT-CT]",301,"revised","2016-02-22T10:24:34.423","2016-03-01T15:03:20.793","C3-160030","C3-160383","Rel-13","29.165","13.3.0","MCPTT-CT","0813","1","B",null,"","","","",""]
["C3-160322","Adding \"application/vnd.3gpp.mcptt-info\" MIME body","Ericsson","Saurav Arora",62621,"CR","","Agreement","","","215","13.24","Mission Critical Push To Talk over LTE protocol aspects [MCPTT-CT]",311,"revised","2016-02-22T10:24:34.627","2016-03-01T15:03:20.793","C3-160031","C3-160384","Rel-13","29.165","13.3.0","MCPTT-CT","0814","1","F",null,"","","","",""]
["C3-160323","Adding MCPTT as option item in annex C","Ericsson","Saurav Arora",62621,"CR","","Agreement","","","215","13.24","Mission Critical Push To Talk over LTE protocol aspects [MCPTT-CT]",321,"revised","2016-02-22T10:24:34.830","2016-03-01T15:03:20.793","C3-160032","C3-160385","Rel-13","29.165","13.3.0","MCPTT-CT","0815","1","B",null,"","","","",""]
["C3-160324","Adding affiliation","Ericsson","Saurav Arora",62621,"CR","","Agreement","","","215","13.24","Mission Critical Push To Talk over LTE protocol aspects [MCPTT-CT]",331,"agreed","2016-02-22T10:24:35.017","2016-03-01T15:03:20.793","C3-160033","","Rel-13","29.165","13.3.0","MCPTT-CT","0816","1","B","CP-160088","","","","",""]
["C3-160325","29.165 rel-13 Addressed MCPTT SIP interfaces","Ericsson Nokia Networks, Alcatel-Lucent, Alcatel-Lucent Shanghai Bell","Saurav Arora",62621,"CR","","Agreement","","","215","13.24","Mission Critical Push To Talk over LTE protocol aspects [MCPTT-CT]",2061,"agreed","2016-02-22T10:24:35.187","2016-03-01T15:03:20.810","C3-160206","","Rel-13","29.165","13.3.0","MCPTT-CT","0821","1","F","CP-160088","","","","",""]
["C3-160326","Corrections to EVS AMR-WB IO mode-change-capability MIME parameter handling","Nokia Networks","Saurav Arora",62621,"CR","","Agreement","","","187","12.34","CT Impacts of Codec for Enhanced Voice Services [EVS_codec-CT]",23001,"agreed","2016-02-22T10:24:35.377","2016-03-01T15:03:20.810","C3-160230","","Rel-13","29.163","13.4.0","EVS_codec-CT","0970","2","A","CP-160111","","","","",""]
["C3-160327","Clarification on the setting of the SIP message components","NTT","Saurav Arora",62621,"CR","","Agreement","","","222","13.30.1","TEI13 for IMS/CS",552,"agreed","2016-02-22T10:24:35.530","2016-03-01T15:03:20.810","C3-160282","","Rel-13","29.163","13.4.0","TEI13, IMS-CCR-IWCS","0967","2","F","CP-160105","","","","",""]
["C3-160328","Support of bitrate variations","Ericsson LM","Saurav Arora",62621,"CR","","Agreement","","","194","13.3","CT Aspects of QoS End to End MTSI extensions [QOSE2EMTSI-CT]",1661,"revised","2016-02-22T10:24:35.733","2016-03-01T15:03:20.810","C3-160166","C3-160367","Rel-13","29.212","13.4.0","QOSE2EMTSI-CT","1428","1","B",null,"","","","",""]
["C3-160329","Correction to wrong Experimental-Result-Code values for PC2 interface","Huawei","Saurav Arora",62621,"CR","","Agreement","","","206","13.15","CT aspects of enhancements to Proximity-based Services extensions [eProSe-Ext-CT]",27401,"agreed","2016-02-22T10:24:35.920","2016-03-01T15:03:20.823","C3-160274","","Rel-13","29.343","13.1.0","eProSe-Ext-CT","0020","1","F","CP-160092","","","","",""]
["C3-160330","REST-Rx enhancement for NetLoc-Untrusted-WLAN","ZTE","Saurav Arora",62621,"CR","","Agreement","","","212","13.21","CT aspects of Support of Emergency services over WLAN - phase 1 [SEW1-CT]",801,"agreed","2016-02-22T10:24:36.107","2016-03-01T15:03:20.823","C3-160080","","Rel-13","29.201","13.3.0","SEW1-CT","0037","1","B","CP-160104","","","","",""]
["C3-160331","Network-initiated removal of one access from the PDN connection","ZTE","Saurav Arora",62621,"CR","","Agreement","","","205","13.14","CT aspects of IP Flow Mobility support for S2a and S2b Interfaces (NBIFOM) [NBIFOM-CT]",702,"revised","2016-02-22T10:24:36.310","2016-03-01T15:03:20.823","C3-160311","C3-160358","Rel-13","29.212","13.4.0","NBIFOM-CT","1409","2","F",null,"","","","",""]
["C3-160332","Correction to NBIFOM handling in roaming case","ZTE Corporation","Saurav Arora",62621,"CR","","Agreement","","","205","13.14","CT aspects of IP Flow Mobility support for S2a and S2b Interfaces (NBIFOM) [NBIFOM-CT]",1492,"revised","2016-02-22T10:24:36.467","2016-03-01T15:03:20.823","C3-160313","C3-160357","Rel-13","29.215","13.4.0","NBIFOM-CT","0402","2","F",null,"","","","",""]
["C3-160333","UE-to-network relay PCC handling over Gx","Ericsson LM","Saurav Arora",62621,"CR","","Agreement","","","206","13.15","CT aspects of enhancements to Proximity-based Services extensions [eProSe-Ext-CT]",1272,"agreed","2016-02-22T10:24:36.623","2016-03-01T15:03:20.840","C3-160286","","Rel-13","29.212","13.4.0","eProSe-Ext-CT","1419","2","B","CP-160092","","","","",""]
["C3-160334","Rx impact for background data transfer","ZTE, Ericsson","Saurav Arora",62621,"CR","","Agreement","","","207","13.16","CT aspects of Architecture Enhancements for Service Capability Exposure [AESE-CT]",732,"agreed","2016-02-22T10:24:36.797","2016-03-01T15:03:20.840","C3-160266","","Rel-13","29.214","13.4.0","AESE-CT","0435","2","B","CP-160095","","","","",""]
["C3-160335","Rx impact for background data transfer","ZTE","Saurav Arora",62621,"CR","","Agreement","","","207","13.16","CT aspects of Architecture Enhancements for Service Capability Exposure [AESE-CT]",742,"agreed","2016-02-22T10:24:36.950","2016-03-01T15:03:20.840","C3-160267","","Rel-13","29.201","13.3.0","AESE-CT","0036","2","B","CP-160095","","","","",""]
["C3-160336","Signnalling flows over Ns reference point","Huawei","Saurav Arora",62621,"CR","","Agreement","","","207","13.16","CT aspects of Architecture Enhancements for Service Capability Exposure [AESE-CT]",892,"agreed","2016-02-22T10:24:37.107","2016-03-01T15:03:20.840","C3-160269","","Rel-13","29.153","13.0.0","AESE-CT","0004","2","F","CP-160095","","","","",""]
["C3-160337","Missed Transfer-Request-Type AVP in the commands","Huawei","Saurav Arora",62621,"CR","","Agreement","","","207","13.16","CT aspects of Architecture Enhancements for Service Capability Exposure [AESE-CT]",912,"agreed","2016-02-22T10:24:37.263","2016-03-01T15:03:20.857","C3-160271","","Rel-13","29.154","13.0.0","AESE-CT","0002","2","F","CP-160095","","","","",""]
["C3-160338","Some corrections for Nt protocol","Huawei","Saurav Arora",62621,"CR","","Agreement","","","207","13.16","CT aspects of Architecture Enhancements for Service Capability Exposure [AESE-CT]",922,"agreed","2016-02-22T10:24:37.420","2016-03-01T15:03:20.857","C3-160272","","Rel-13","29.154","13.0.0","AESE-CT","0003","2","F","CP-160095","","","","",""]
["C3-160339","Update the scope to include the Nt interface","Huawei","Saurav Arora",62621,"CR","","Agreement","","","207","13.16","CT aspects of Architecture Enhancements for Service Capability Exposure [AESE-CT]",932,"agreed","2016-02-22T10:24:37.577","2016-03-01T15:03:20.857","C3-160273","","Rel-13","29.213","13.4.0","AESE-CT","0641","2","B","CP-160095","","","","",""]
["C3-160340","ADC rule error handling report initiated by the TSSF","ZTE,Nokia Networks","Saurav Arora",62621,"CR","","Agreement","","","211","13.20","CT3 Aspect of Flexible Mobile Service Steering [FMSS-CT]",762,"agreed","2016-02-22T10:24:37.730","2016-03-01T15:03:20.857","C3-160217","","Rel-13","29.213","13.4.0","FMSS-CT","0639","2","B","CP-160091","","","","",""]
["C3-160341","IPv4 address provisioning","ZTE","Saurav Arora",62621,"CR","","Agreement","","","211","13.20","CT3 Aspect of Flexible Mobile Service Steering [FMSS-CT]",772,"agreed","2016-02-22T10:24:37.887","2016-03-01T15:03:20.857","C3-160218","","Rel-13","29.212","13.4.0","FMSS-CT","1411","2","F","CP-160091","","","","",""]
["C3-160342","Update the scope to include the St interface","Huawei","Saurav Arora",62621,"CR","","Agreement","","","211","13.20","CT3 Aspect of Flexible Mobile Service Steering [FMSS-CT]",1062,"agreed","2016-02-22T10:24:38.057","2016-03-01T15:03:20.870","C3-160219","","Rel-13","29.213","13.4.0","FMSS-CT","0645","2","F","CP-160091","","","","",""]
["C3-160343","Diameter Message Priority over diameter based St interface","Huawei","Saurav Arora",62621,"CR","","Agreement","","","219","13.28","Diameter Message Priority [DiaPri]",952,"agreed","2016-02-22T10:24:38.230","2016-03-01T15:03:20.870","C3-160299","","Rel-13","29.212","13.4.0","DiaPri","1412","2","B","CP-160093","","","","",""]
["C3-160344","Diameter Message Priority over Nt interface","Huawei","Saurav Arora",62621,"CR","","Agreement","","","219","13.28","Diameter Message Priority [DiaPri]",972,"agreed","2016-02-22T10:24:38.387","2016-03-01T15:03:20.870","C3-160300","","Rel-13","29.154","13.0.0","DiaPri","0004","2","B","CP-160093","","","","",""]
["C3-160345","Time conditioned APN-AMBR handling","Ericsson, Verizon, Nokia Networks, Alcatel-Lucent, Alcatel-Lucent Shanghai Bell, Oracle Corporation","Saurav Arora",62621,"CR","","Agreement","","","223","13.30.2","TEI13 for Packet Core",572,"agreed","2016-02-22T10:24:38.543","2016-03-01T15:03:20.870","C3-160294","","Rel-13","29.212","13.4.0","PCC, TEI13","1406","2","B","CP-160101","","","","",""]
["C3-160346","Usage of the UDP port for default unicast encapsulation mode at the SGmb interface is required to support SYNC protocol","Nokia Networks, Alcatel-Lucent","Saurav Arora",62621,"CR","","Agreement","","","54","9.4","MBMS [MBMS]",1672,"agreed","2016-02-22T10:24:38.697","2016-03-01T15:03:20.887","C3-160289","","Rel-9","29.061","9.15.0","MBMS","0461","2","F","CP-160089","","","","",""]
["C3-160347","Usage of the UDP port for default unicast encapsulation mode at the Gmb interface is required to support SYNC protocol","Nokia Networks","Saurav Arora",62621,"CR","","Agreement","","","54","9.4","MBMS [MBMS]",1682,"revised","2016-02-22T10:24:38.870","2016-03-01T15:03:20.887","C3-160290","C3-160362","Rel-10","29.061","10.13.0","MBMS","0462","2","A",null,"","","","",""]
["C3-160348","Usage of the UDP port for default unicast encapsulation mode at the Gmb interface is required to support SYNC protocol","Nokia Networks, Alcatel-Lucent","Saurav Arora",62621,"CR","","Agreement","","","54","9.4","MBMS [MBMS]",1702,"agreed","2016-02-22T10:24:39.027","2016-03-01T15:03:20.887","C3-160291","","Rel-11","29.061","11.11.0","MBMS","0463","2","A","CP-160089","","","","",""]
["C3-160349","Usage of the UDP port for default unicast encapsulation mode at the Gmb interface is required to support SYNC protocol","Nokia Networks, Alcatel-Lucent","Saurav Arora",62621,"CR","","Agreement","","","54","9.4","MBMS [MBMS]",1722,"agreed","2016-02-22T10:24:39.180","2016-03-01T15:03:20.903","C3-160292","","Rel-12","29.061","12.11.0","MBMS","0464","2","A","CP-160089","","","","",""]
["C3-160350","Usage of the UDP port for default unicast encapsulation mode at the Gmb interface is required to support SYNC protocol","Nokia Networks, Alcatel-Lucent","Saurav Arora",62621,"CR","","Agreement","","","54","9.4","MBMS [MBMS]",1752,"agreed","2016-02-22T10:24:39.353","2016-03-01T15:03:20.903","C3-160293","","Rel-13","29.061","13.2.0","MBMS","0465","2","B","CP-160089","","","","",""]
["C3-160351","NAS/RAN cause handling at bearer termination failure","Ericsson, Alcatel-Lucent, Alcatel-Lucent Shanghai Bell, Nokia Networks, Huawei, ZTE","Saurav Arora",62621,"CR","","Agreement","","","223","13.30.2","TEI13 for Packet Core",1082,"revised","2016-02-22T10:24:39.557","2016-03-01T15:03:20.903","C3-160295","C3-160360","Rel-13","29.212","13.4.0","PCC, TEI13","1417","2","B",null,"","","","",""]
["C3-160352","RAN-NAS-Cause handling upon unsuccessful bearer termination over Rx","Ericsson, Alcatel-Lucent, Alcatel-Lucent Shanghai Bell, Nokia Networks, Huawei, ZTE","Saurav Arora",62621,"CR","","Agreement","","","223","13.30.2","TEI13 for Packet Core",1112,"agreed","2016-02-22T10:24:39.743","2016-03-01T15:03:20.917","C3-160296","","Rel-13","29.214","13.4.0","PCC, TEI13","0438","2","F","CP-160101","","","","",""]
["C3-160353","Completion of RAN-NAS cause handling procedures","Ericsson LM,Nokia Networks,Alcatel-Lucent","Saurav Arora",62621,"CR","","Agreement","","","223","13.30.2","TEI13 for Packet Core",1152,"agreed","2016-02-22T10:24:39.930","2016-03-01T15:03:20.917","C3-160306","","Rel-13","29.213","13.4.0","PCC, TEI13","0648","2","F","CP-160101","","","","",""]
["C3-160354","CR Incorrect use of the term \"full hexadecimal representation\" to mean binary incoding","Oracle Corporation","Saurav Arora",62621,"CR","","Agreement","","","223","13.30.2","TEI13 for Packet Core",21501,"withdrawn","2016-02-22T10:24:40.117",null,"C3-160215","","Rel-13","29.212","13.4.0","TEI13, CNO_ULI-CT","1430","1","F",null,"","","","",""]
["C3-160355","Reporting of NAS/RAN cause in the STA command","Ericsson LM","Saurav Arora",62621,"CR","","Agreement","","","190","12.35.2","TEI12 for Packet Core",23501,"revised","2016-02-22T10:24:40.290","2016-03-01T15:03:20.917","C3-160235","C3-160365","Rel-12","29.214","12.10.0","PCC, TEI12","0447","3","F",null,"","","","",""]
["C3-160356","Reporting of NAS/RAN cause in the STA command","Ericsson LM","Saurav Arora",62621,"CR","","Agreement","","","190","12.35.2","TEI12 for Packet Core",23601,"revised","2016-02-22T10:24:40.493","2016-03-01T15:03:20.933","C3-160236","C3-160366","Rel-13","29.214","13.4.0","PCC, TEI12","0437","2","A",null,"","","","",""]
["C3-160357","Correction to NBIFOM handling in roaming case","ZTE Corporation","Saurav Arora",62621,"CR","","Agreement","","","205","13.14","CT aspects of IP Flow Mobility support for S2a and S2b Interfaces (NBIFOM) [NBIFOM-CT]",1493,"revised","2016-02-22T10:24:40.647","2016-03-01T15:03:20.933","C3-160332","C3-160369","Rel-13","29.215","13.4.0","NBIFOM-CT","0402","3","F",null,"","","","",""]
["C3-160358","Network-initiated removal of one access from the PDN connection","ZTE","Saurav Arora",62621,"CR","","Agreement","","","205","13.14","CT aspects of IP Flow Mobility support for S2a and S2b Interfaces (NBIFOM) [NBIFOM-CT]",703,"revised","2016-02-22T10:24:40.820","2016-03-01T15:03:20.933","C3-160331","C3-160368","Rel-13","29.212","13.4.0","NBIFOM-CT","1409","3","F",null,"","","","",""]
["C3-160359","Metadata indicator for restricted discovery monitor request procedure","Qualcomm Incorporated","Saurav Arora",62621,"CR","","Agreement","","","206","13.15","CT aspects of enhancements to Proximity-based Services extensions [eProSe-Ext-CT]",1372,"agreed","2016-02-22T10:24:40.990","2016-03-01T15:03:20.933","C3-160287","","Rel-13","29.343","13.1.0","eProSe-Ext-CT","0018","2","F","CP-160092","","","","",""]
["C3-160360","NAS/RAN cause handling at bearer termination failure","Ericsson, Alcatel-Lucent, Alcatel-Lucent Shanghai Bell, Nokia Networks, Huawei, ZTE","Saurav Arora",62621,"CR","","Agreement","","","223","13.30.2","TEI13 for Packet Core",1083,"revised","2016-02-22T10:24:41.147","2016-03-01T15:03:20.933","C3-160351","C3-160377","Rel-13","29.212","13.4.0","PCC, TEI13","1417","3","B",null,"","","","",""]
["C3-160361","LS on new AVPs in TS 29.212","Nokia Networks","Saurav Arora",62621,"LS out","","Approval","","","223","13.30.2","TEI13 for Packet Core",1802,"revised","2016-02-22T10:24:41.317","2016-03-01T15:03:20.950","C3-160213","C3-160371","Rel-13","29.212","","PCC, TEI13","","","","",null,"CT4"]
["C3-160362","Usage of the UDP port for default unicast encapsulation mode at the Gmb interface is required to support SYNC protocol","Nokia Networks","Saurav Arora",62621,"CR","","Agreement","","","54","9.4","MBMS [MBMS]",1683,"agreed","2016-02-22T10:24:41.427","2016-03-01T15:03:20.950","C3-160347","","Rel-10","29.061","10.13.0","MBMS","0462","3","A","CP-160089","","","","",""]
["C3-160363","Capability of REST-Rx","ZTE","Saurav Arora",62621,"CR","","Agreement","","","161","12.8.1","Representational State Transfer (REST) reference point between Application Function (AF) and Protocol Converter (PC) [REST_AF_PC]",23301,"agreed","2016-02-22T10:24:41.617","2016-03-01T15:03:20.950","C3-160233","","Rel-12","29.201","12.3.0","REST_AF_PC","0033","2","F","CP-160103","","","","",""]
["C3-160364","Capability of REST-Rx","ZTE","Saurav Arora",62621,"CR","","Agreement","","","161","12.8.1","Representational State Transfer (REST) reference point between Application Function (AF) and Protocol Converter (PC) [REST_AF_PC]",23401,"agreed","2016-02-22T10:24:41.803","2016-03-01T15:03:20.950","C3-160234","","Rel-13","29.201","13.3.0","REST_AF_PC","0034","2","A","CP-160103","","","","",""]
["C3-160365","Reporting of NAS/RAN cause in the STA command","Ericsson LM","Saurav Arora",62621,"CR","","Agreement","","","190","12.35.2","TEI12 for Packet Core",23502,"agreed","2016-02-22T10:24:41.990","2016-03-01T15:03:20.967","C3-160355","","Rel-12","29.214","12.10.0","PCC, TEI12","0447","4","F","CP-160100","","","","",""]
["C3-160366","Reporting of NAS/RAN cause in the STA command","Ericsson LM","Saurav Arora",62621,"CR","","Agreement","","","190","12.35.2","TEI12 for Packet Core",23602,"agreed","2016-02-22T10:24:42.147","2016-03-01T15:03:20.967","C3-160356","","Rel-13","29.214","13.4.0","PCC, TEI12","0437","3","A","CP-160100","","","","",""]
["C3-160367","Support of bitrate variations","Ericsson LM","Saurav Arora",62621,"CR","","Agreement","","","194","13.3","CT Aspects of QoS End to End MTSI extensions [QOSE2EMTSI-CT]",1662,"agreed","2016-02-22T10:24:42.317","2016-03-01T15:03:20.967","C3-160328","","Rel-13","29.212","13.4.0","QOSE2EMTSI-CT","1428","2","B","CP-160110","","","","",""]
["C3-160368","Network-initiated removal of one access from the PDN connection","ZTE","Saurav Arora",62621,"CR","","Agreement","","","205","13.14","CT aspects of IP Flow Mobility support for S2a and S2b Interfaces (NBIFOM) [NBIFOM-CT]",704,"agreed","2016-02-22T10:24:42.487","2016-03-01T15:03:20.967","C3-160358","","Rel-13","29.212","13.4.0","NBIFOM-CT","1409","4","F","CP-160107","","","","",""]
["C3-160369","Correction to NBIFOM handling in roaming case","ZTE Corporation","Saurav Arora",62621,"CR","","Agreement","","","205","13.14","CT aspects of IP Flow Mobility support for S2a and S2b Interfaces (NBIFOM) [NBIFOM-CT]",1494,"agreed","2016-02-22T10:24:42.643","2016-03-01T15:03:20.967","C3-160357","","Rel-13","29.215","13.4.0","NBIFOM-CT","0402","4","F","CP-160090","","","","",""]
["C3-160370","Diameter St Error Notifications","Nokia Networks,ZTE","Saurav Arora",62621,"CR","","Agreement","","","211","13.20","CT3 Aspect of Flexible Mobile Service Steering [FMSS-CT]",1642,"revised","2016-02-22T10:24:42.817","2016-03-01T15:03:20.980","C3-160216","C3-160375","Rel-13","29.212","13.4.0","FMSS-CT","1427","2","B",null,"","","","",""]
["C3-160371","LS on new AVPs in TS 29.212","Nokia Networks","Saurav Arora",62621,"LS out","","Approval","","","223","13.30.2","TEI13 for Packet Core",1803,"approved","2016-02-22T10:24:42.987","2016-03-01T15:03:20.980","C3-160361","","Rel-13","29.212","","PCC, TEI13","","","","",null,"CT4"]
["C3-160372","WebRTC media plane optimization procedure","Nokia Networks , Alcatel-Lucent","Saurav Arora",62621,"CR","","Agreement","","","216","13.25","Enhancements to WEBRTC interoperability stage 3 [eWebRTCi_CT]",2042,"revised","2016-02-22T10:24:43.097","2016-03-01T15:03:20.980","C3-160279","C3-160388","Rel-13","29.162","13.1.0","eWebRTCi-CT ","0152","3","B",null,"","","","",""]
["C3-160373","Updates to JSON content rules for the notification procedures from the TSSF to the PCRF","Oracle Corporation","Saurav Arora",62621,"CR","","Agreement","","","211","13.20","CT3 Aspect of Flexible Mobile Service Steering [FMSS-CT]",1412,"revised","2016-02-22T10:24:43.253","2016-03-01T15:03:20.980","C3-160262","C3-160381","Rel-13","29.155","13.0.0","FMSS-CT","0003","2","B",null,"","","","",""]
["C3-160374","Traffic steering rule report JSON Content Rules over St","Oracle Corporation","Saurav Arora",62621,"CR","","Agreement","","","211","13.20","CT3 Aspect of Flexible Mobile Service Steering [FMSS-CT]",1432,"revised","2016-02-22T10:24:43.423","2016-03-01T15:03:20.997","C3-160264","C3-160382","Rel-13","29.155","13.0.0","FMSS-CT","0005","2","B",null,"","","","",""]
["C3-160375","Diameter St Error Notifications","Nokia Networks,ZTE","Saurav Arora",62621,"CR","","Agreement","","","211","13.20","CT3 Aspect of Flexible Mobile Service Steering [FMSS-CT]",1643,"agreed","2016-02-22T10:24:43.597","2016-03-01T15:03:20.997","C3-160370","","Rel-13","29.212","13.4.0","FMSS-CT","1427","3","B","CP-160091","","","","",""]
["C3-160376","Traffic Steering Rule Error handling over the REST based St interface","Oracle Corporation","Saurav Arora",62621,"CR","","Agreement","","","211","13.20","CT3 Aspect of Flexible Mobile Service Steering [FMSS-CT]",1392,"agreed","2016-02-22T10:24:43.767","2016-03-01T15:03:20.997","C3-160220","","Rel-13","29.155","13.0.0","FMSS-CT","0001","2","B","CP-160091","","","","",""]
["C3-160377","NAS/RAN cause handling at bearer termination failure","Ericsson, Alcatel-Lucent, Alcatel-Lucent Shanghai Bell, Nokia Networks, Huawei, ZTE","Saurav Arora",62621,"CR","","Agreement","","","223","13.30.2","TEI13 for Packet Core",1084,"revised","2016-02-22T10:24:43.940","2016-03-01T15:03:20.997","C3-160360","C3-160379","Rel-13","29.212","13.4.0","PCC, TEI13","1417","4","B",null,"","","","",""]
["C3-160378","Completion of NBIFOM","Ericsson, ZTE, Huawei","Saurav Arora",62621,"CR","","Agreement","","","205","13.14","CT aspects of IP Flow Mobility support for S2a and S2b Interfaces (NBIFOM) [NBIFOM-CT]",562,"agreed","2016-02-22T10:24:44.110","2016-03-01T15:03:21.010","C3-160310","","Rel-13","29.212","13.4.0","NBIFOM-CT","1405","2","B","CP-160090","","","","",""]
["C3-160379","NAS/RAN cause handling at bearer termination failure","Ericsson, Alcatel-Lucent, Alcatel-Lucent Shanghai Bell, Nokia Networks, Huawei, ZTE","Saurav Arora",62621,"CR","","Agreement","","","223","13.30.2","TEI13 for Packet Core",1085,"agreed","2016-02-22T10:24:44.283","2016-03-01T15:03:21.010","C3-160377","","Rel-13","29.212","13.4.0","PCC, TEI13","1417","5","B","CP-160101","","","","",""]
["C3-160380","LS on MCPTT priorities support over Rx","CT3","Saurav Arora",62621,"LS out","","Approval","","","215","13.24","Mission Critical Push To Talk over LTE protocol aspects [MCPTT-CT]",31901,"revised","2016-02-22T10:24:44.470","2016-03-01T15:03:21.010","C3-160319","C3-160395","Rel-13","","","MCPTT-CT","","","","",null,"SA2","SA6"]
["C3-160381","Updates to JSON content rules for the notification procedures from the TSSF to the PCRF","Oracle Corporation","Saurav Arora",62621,"CR","","Agreement","","","211","13.20","CT3 Aspect of Flexible Mobile Service Steering [FMSS-CT]",1413,"agreed","2016-02-22T10:24:44.563","2016-03-01T15:03:21.010","C3-160373","","Rel-13","29.155","13.0.0","FMSS-CT","0003","3","B","CP-160091","","","","",""]
["C3-160382","Traffic steering rule report JSON Content Rules over St","Oracle Corporation","Saurav Arora",62621,"CR","","Agreement","","","211","13.20","CT3 Aspect of Flexible Mobile Service Steering [FMSS-CT]",1433,"agreed","2016-02-22T10:24:44.767","2016-03-01T15:03:21.027","C3-160374","","Rel-13","29.155","13.0.0","FMSS-CT","0005","3","B","CP-160091","","","","",""]
["C3-160383","Adding MBMS usage info and location info procedure","Ericsson","Saurav Arora",62621,"CR","","Agreement","","","215","13.24","Mission Critical Push To Talk over LTE protocol aspects [MCPTT-CT]",302,"agreed","2016-02-22T10:24:44.937","2016-03-01T15:03:21.027","C3-160321","","Rel-13","29.165","13.3.0","MCPTT-CT","0813","2","B","CP-160088","","","","",""]
["C3-160384","Adding \"application/vnd.3gpp.mcptt-info\" MIME body","Ericsson","Saurav Arora",62621,"CR","","Agreement","","","215","13.24","Mission Critical Push To Talk over LTE protocol aspects [MCPTT-CT]",312,"agreed","2016-02-22T10:24:45.110","2016-03-01T15:03:21.027","C3-160322","","Rel-13","29.165","13.3.0","MCPTT-CT","0814","2","F","CP-160088","","","","",""]
["C3-160385","Adding MCPTT as option item in annex C","Ericsson","Saurav Arora",62621,"CR","","Agreement","","","215","13.24","Mission Critical Push To Talk over LTE protocol aspects [MCPTT-CT]",322,"agreed","2016-02-22T10:24:45.313","2016-03-01T15:03:21.027","C3-160323","","Rel-13","29.165","13.3.0","MCPTT-CT","0815","2","B","CP-160088","","","","",""]
["C3-160386","Support of enhanced bandwidth negotiation mechanism for MTSI sessions","Ericsson","Saurav Arora",62621,"CR","","Agreement","","","194","13.3","CT Aspects of QoS End to End MTSI extensions [QOSE2EMTSI-CT]",23101,"agreed","2016-02-22T10:24:45.483","2016-03-01T15:03:21.043","C3-160231","","Rel-13","29.162","13.1.0","QOSE2EMTSI-CT","0150","2","B","CP-160102","","","","",""]
["C3-160387","Support of enhanced bandwidth negotiation mechanism for MTSI sessions","Ericsson","Saurav Arora",62621,"CR","","Agreement","","","194","13.3","CT Aspects of QoS End to End MTSI extensions [QOSE2EMTSI-CT]",23201,"agreed","2016-02-22T10:24:45.657","2016-03-01T15:03:21.043","C3-160232","","Rel-13","29.163","13.4.0","QOSE2EMTSI-CT","0954","2","B","CP-160102","","","","",""]
["C3-160388","WebRTC media plane optimization procedure","Nokia Networks , Alcatel-Lucent","Saurav Arora",62621,"CR","","Agreement","","","216","13.25","Enhancements to WEBRTC interoperability stage 3 [eWebRTCi_CT]",2043,"agreed","2016-02-22T10:24:45.810","2016-03-01T15:03:21.043","C3-160372","","Rel-13","29.162","13.1.0","eWebRTCi-CT ","0152","4","B","CP-160097","","","","",""]
["C3-160389","New subclause to Appendix A for the handling of MCPTT emergency calls","Motorola Solution Inc.","Saurav Arora",62621,"CR","","Agreement","","","215","13.24","Mission Critical Push To Talk over LTE protocol aspects [MCPTT-CT]",2052,"agreed","2016-02-22T10:24:45.983","2016-03-01T15:03:21.043","C3-160318","","Rel-13","29.214","13.4.0","MCPTT-CT","0448","2","B","CP-160087","","","","",""]
["C3-160390","Reservation-Priority AVP and DRMP AVP Interaction","ACS, OEC, AT&T,Alcatel-Lucent, Alcatel-Lucent Shanghai Bell and  Nokia Networks","Saurav Arora",62621,"CR","","Agreement","","","219","13.28","Diameter Message Priority [DiaPri]",1542,"agreed","2016-02-22T10:24:46.153","2016-03-01T15:03:21.043","C3-160303","","Rel-13","29.213","13.4.0","DiaPri","0654","2","B","CP-160093","","","","",""]
["C3-160391","Reservation-Priority AVP and DRMP AVP Interaction","ACS, OEC, AT&T,Alcatel-Lucent, Alcatel-Lucent Shanghai Bell and  Nokia Networks","Saurav Arora",62621,"CR","","Agreement","","","219","13.28","Diameter Message Priority [DiaPri]",1952,"agreed","2016-02-22T10:24:46.327","2016-03-01T15:03:21.057","C3-160301","","Rel-13","29.214","13.4.0","DiaPri","0446","2","B","CP-160093","","","","",""]
["C3-160392","Diameter message priority over MB2-C","Applied Communication Sciences, OEC, AT&T, Alcatel-Lucent Alcatel-Lucent Shanghai Bell and Nokia Networks","Saurav Arora",62621,"CR","","Agreement","","","219","13.28","Diameter Message Priority [DiaPri]",2032,"agreed","2016-02-22T10:24:46.497","2016-03-01T15:03:21.057","C3-160305","","Rel-13","29.468","13.0.0","TEI13, GCSE_LTE-CT","0019","2","B","CP-160101","","","","",""]
["C3-160393","Reply to: LS on EVS over CS","CT3","Saurav Arora",62621,"LS out","","Approval","","","13","6","Received Liaison Statements",1892,"approved","2016-02-22T10:24:46.687","2016-03-01T15:03:21.057","C3-160209","","Rel-13","","","EVSoCS","","","","","C3-160189","SA4","CT4"]
["C3-160394","Proposed Revision of CT3 ToR","3GPP CT3 Chairman","Saurav Arora",62621,"other","","Information","","","12","5.3","Other items for immediate consideration",1992,"revised","2016-02-22T10:24:46.793","2016-03-01T15:03:21.057","C3-160208","C3-160396","","","","","","","","","","","","",""]
["C3-160395","LS on MCPTT priorities support over Rx","CT3","Saurav Arora",62621,"LS out","","Approval","","","215","13.24","Mission Critical Push To Talk over LTE protocol aspects [MCPTT-CT]",31902,"approved","2016-02-22T10:24:46.887","2016-03-01T15:03:21.073","C3-160380","","Rel-13","","","MCPTT-CT","","","","",null,"SA2","SA6"]
["C3-160396","Proposed Revision of CT3 ToR","3GPP CT3 Chairman","Saurav Arora",62621,"other","","Information","","","12","5.3","Other items for immediate consideration",1993,"agreed","2016-02-22T10:24:46.997","2016-03-01T15:03:21.073","C3-160394","","","","","","","","","","","","","",""]
["C3-160397","Interworking of History-Info Header Field when Original Called Number is not present","Deutsche Telekom / Michael","Saurav Arora",62621,"CR","","Agreement","","","15","8.2","Interworking between IM Subsystem with CS  [IMS-CCR-IWCS]",22101,"postponed","2016-02-22T10:24:47.107","2016-03-01T15:03:21.073","C3-160221","C3-161025","Rel-8","29.163","8.29.0","IMS-CCR-IWCS","0948","2","F",null,"","","","",""]
["C3-160398","Interworking of History-Info Header Field when Original Called Number is not present","Deutsche Telekom / Michael","Saurav Arora",62621,"CR","","Agreement","","","15","8.2","Interworking between IM Subsystem with CS  [IMS-CCR-IWCS]",22201,"postponed","2016-02-22T10:24:47.277","2016-03-01T15:03:21.073","C3-160222","C3-161026","Rel-9","29.163","9.23.0","IMS-CCR-IWCS","0949","2","A",null,"","","","",""]
["C3-160399","Interworking of History-Info Header Field when Original Called Number is not present","Deutsche Telekom / Michael","Saurav Arora",62621,"CR","","Agreement","","","15","8.2","Interworking between IM Subsystem with CS  [IMS-CCR-IWCS]",22301,"postponed","2016-02-22T10:24:47.450","2016-03-01T15:03:21.073","C3-160223","C3-161027","Rel-10","29.163","10.19.0","IMS-CCR-IWCS","0950","2","A",null,"","","","",""]
["C3-160400","Interworking of History-Info Header Field when Original Called Number is not present","Deutsche Telekom / Michael","Saurav Arora",62621,"CR","","Agreement","","","15","8.2","Interworking between IM Subsystem with CS  [IMS-CCR-IWCS]",22401,"postponed","2016-02-22T10:24:47.653","2016-03-01T15:03:21.090","C3-160224","C3-161028","Rel-11","29.163","11.16.0","IMS-CCR-IWCS","0951","2","A",null,"","","","",""]
["C3-160401","Interworking of History-Info Header Field when Original Called Number is not present","Deutsche Telekom / Michael","Saurav Arora",62621,"CR","","Agreement","","","15","8.2","Interworking between IM Subsystem with CS  [IMS-CCR-IWCS]",22501,"postponed","2016-02-22T10:24:47.823","2016-03-01T15:03:21.090","C3-160225","C3-161029","Rel-12","29.163","12.10.0","IMS-CCR-IWCS","0952","2","A",null,"","","","",""]
["C3-160402","Interworking of History-Info Header Field when Original Called Number is not present","Deutsche Telekom / Michael","Saurav Arora",62621,"CR","","Agreement","","","15","8.2","Interworking between IM Subsystem with CS  [IMS-CCR-IWCS]",22601,"postponed","2016-02-22T10:24:48.010","2016-03-01T15:03:21.090","C3-160226","C3-161030","Rel-13","29.163","13.4.0","IMS-CCR-IWCS","0953","2","A",null,"","","","",""]

{"sheet":"CR_Packs_List","index":1,"n_rows":1,"n_cols":11,"rows_kept":1,"cut":false,"hidden":false,"merged":[]}
["CR Pack TDoc #","WG TDoc #","WG TDoc decision","CR Individual TSG decision","Spec #","CR #","CR revision #","CR category","Release","Version","CR title"]

{"sheet":"Parameters","index":2,"n_rows":24,"n_cols":4,"rows_kept":24,"cut":false,"hidden":true,"merged":[]}
["Types of Tdocs","Possible statuses of Tdocs","Categories"]
[]
["agenda","reserved","A","Decision"]
["Work Plan","available","B","Agreement"]
["LS in","revised","C","Approval"]
["LS out","agreed","D","Information"]
["pCR","conditionally agreed","E","Discussion"]
["draftCR","approved","F","Action"]
["CR","conditionally approved",null,"Endorsement"]
["CR pack","partially approved",null,"Presentation"]
["ToR","treated"]
["WID new","endorsed"]
["WID revised","replied to"]
["SID new","merged"]
["SID revised","not pursued"]
["WI status report","postponed"]
["WI exception request","noted"]
["TS or TR cover","not concluded"]
["draft TS","withdrawn"]
["draft TR","reissued"]
["report"]
["discussion"]
["response"]
["other"]