{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["TDoc_List","CR_Packs_List","Parameters"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":6,"comments":1,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"TDoc_List","index":0,"n_rows":344,"n_cols":32,"rows_kept":344,"cut":false,"hidden":false,"merged":[]}
["TDoc #","Title","Source","Contact","Contact ID","Type","Type supplement","For","Abstract","Secretary Remarks","Agenda item sort order","Agenda item #","Agenda item description","TDoc sort order within agenda item","TDoc Status","Reservation date","Uploaded","Is revision of","Revised to","Release","Spec #","Version","Related WIs","CR #","CR revision #","CR category","TSG CR Pack","Reply to","To","Cc","Original LS","Reply in"]
["C4-164000","Draft Agenda","CT4 Chairman","Kimmo Kymalainen",19464,"agenda","","Information","","","5","2","Allocation of documents to agenda items",0,"noted","2016-06-22T15:02:09.527","2016-06-22T15:04:45.760","","","","","","","","","","","","","","",""]
["C4-164001","Detailed agenda & time plan for CT4#74: status at document deadline","CT4 Chairman","Nigel. H Berry",68268,"agenda","","Information","","","5","2","Allocation of documents to agenda items",0,"noted","2016-06-22T15:02:09.540","2016-07-16T11:07:27.487","","","","","","","","","","","","","","",""]
["C4-164002","Detailed agenda & time plan for CT4#74: status on eve of meeting","CT4 Chairman","Nigel. H Berry",68268,"agenda","","Information","","","5","2","Allocation of documents to agenda items",0,"noted","2016-06-22T15:02:09.540","2016-07-20T16:40:23.053","","","","","","","","","","","","","","",""]
["C4-164003","Proposed allocation of documents to agenda items for CT4#74: status at document deadline","CT4 Chairman","Nigel. H Berry",68268,"agenda","","Information","","","5","2","Allocation of documents to agenda items",0,"noted","2016-06-22T15:02:09.540","2016-07-16T11:07:08.877","","","","","","","","","","","","","","",""]
["C4-164004","Proposed allocation of documents to agenda items for CT4#74: status on eve of meeting","CT4 Chairman","Nigel. H Berry",68268,"agenda","","Information","","","5","2","Allocation of documents to agenda items",0,"noted","2016-06-22T15:02:09.557","2016-07-20T16:38:49.703","","","","","","","","","","","","","","",""]
["C4-164005","CT4 previous meeting report for approval","MCC","Kimmo Kymalainen",19464,"report","","Approval","","","6","3","Meeting Reports",0,"approved","2016-06-22T15:02:09.557","2016-07-25T06:45:32.277","","","","","","","","","","","","","","",""]
["C4-164006","CT4 Aspect of the Workplan","CT4 Chairman","Nigel. H Berry",68268,"Work Plan","","Agreement","","","188","11","Update of the Work Plan",0,"noted","2016-06-22T15:02:09.557","2016-07-15T19:02:16.657","","C4-164341","","","","","","","","","","","","",""]
["C4-164007","Reply LS on Maximum upper layer data packet size for NB-IoT","CT1","Kimmo Kymalainen",19464,"LS in","","Action","CT1 thanks RAN2 on their LS on Maximum upper layer data packet size for NB-IoT.\nRegarding the maximum PDU size for application layer: \nRAN2 assumes 1500 octets maximum PDU size for application layer. This maximum PDU size applies to: \n-\t IP and non-IP\n-\tuplink and downlink \n-\tCIoT CP optimisation (NAS SDU) and CIoT UP optimisation (PDCP SDU).\nCT1 agrees that it is beneficial to specify the maximum higher layer data size to be supported to minimise buffering requirements in layer 2.","","7","4","Input liaison statements: allocation to agenda items as appropriate",0,"noted","2016-06-22T15:23:40.353","2016-06-22T15:47:51.787","","","Rel-13","","","NB_IOT-Core, CIoT-CT","","","","",null,"CT4, RAN2","SA2","C1-163141"]
["C4-164008","LS on new indication from PGW for the NBIFOM procedures","CT1","Kimmo Kymalainen",19464,"LS in","","Action","SA2 has defined the new messages exchange (see subclause 6.4.1 in 3GPP TS 23.161) between the UE and the SGSN for the UE-initiated NBIFOM procedures (consisting of 4 or 5 NAS messages) when network-initiated mode is used. In order to distinguish this new procedure with the normal procedure (consisting of 2 NAS messages) used in the UE-initiated NBIFOM mode, the SGSN needs information from PGW side. Therefore, CT1 would like to ask CT4 to define a new indication from PGW to the SGSN for the SGSN to perform the different procedures.","","56","7.2.6","IP Flow Mobility support for S2a and S2b Interfaces on stage 3 (CT1) [NBIFOM]",0,"noted","2016-06-22T15:23:40.353","2016-06-22T15:47:51.787","","","Rel-13","","","NBIFOM-CT","","","","",null,"CT4",null,"C1-163142","C4-164215"]
["C4-164009","LS on EVS over CS","CT3","Kimmo Kymalainen",19464,"LS in","","Information","1. Overall Description:\nCT3 thanks SA4 for their LS on EVS over CS.\n\nIn the LS SA4 attached a CR, commented on interworking procedures, and also suggested a work split.\n\n\nRelated to the CR SA4 attached to their LS, CT3 has the following comments and questions:","","7","4","Input liaison statements: allocation to agenda items as appropriate",0,"noted","2016-06-22T15:23:40.370","2016-06-22T15:47:51.787","","","Rel-13","","","EVSoCS","","","","",null,"SA4","CT4","C3-161205"]
["C4-164010","Reply LS on SCS Identity format for device triggering","CT3","Kimmo Kymalainen",19464,"LS in","","Action","","","140","9.13.2","Reach ability Aspects of SIMTC [SIMTC-Reach]",0,"noted","2016-06-22T15:23:40.370","2016-06-22T15:47:51.787","","","Rel-11","","","SIMTC-ReachCSPS","","","","",null,"CT4",null,"C3-161241"]
["C4-164011","Reply LS on progress of the work on Diameter Load Control","CT3","Kimmo Kymalainen",19464,"LS in","","Action","CT3 would like to thank CT4 for their LS on the progress of Diameter Load Control work. \n\nCT3 has reviewed 3GPP TR 29.810 v0.6.0 with focus on CT3 owned interfaces and functions. Below is the feedback:","","7","4","Input liaison statements: allocation to agenda items as appropriate",0,"postponed","2016-06-22T15:23:40.370","2016-06-22T15:47:51.803","","","Rel-14","","","FS_DLoCME","","","","",null,"CT4","SA5","C3-161313"]
["C4-164012","Correction on LS on new AVPs in TS 29.214","CT3","Kimmo Kymalainen",19464,"LS in","","Action","Handled in CT4#73","","7","4","Input liaison statements: allocation to agenda items as appropriate",0,"withdrawn","2016-06-22T15:23:40.370","2016-06-22T15:47:51.743","","","","","","","","","","",null,"CT4",null,"C3-161315"]
["C4-164013","LS about Diameter Application ID for PC2 interface","CT3","Kimmo Kymalainen",19464,"LS in","","Action","CT3 decide to use the Diameter application ID 16777350 for the PC2 interface application in Release 13 version of TS 29.343. The PC2 interface application identifier 16777337 is used in Release 12 version of TS 29.343. For backward-compatibility, the ProSe Application Server in releases later than Rel-12 is encouraged to also support the Rel-12 version and the old application ID 16777337.","","7","4","Input liaison statements: allocation to agenda items as appropriate",0,"noted","2016-06-22T15:23:40.387","2016-06-22T15:47:51.757","","","","","","eProSe-Ext-CT","","","","",null,"CT4",null,"C3-161316"]
["C4-164014","LS on update of definition of BSIC to include Radio frequency Colour Code","Geran Plenary","Kimmo Kymalainen",19464,"LS in","","Action","GERAN has recently updated their specifications to facilitate operation in very tight frequency re-use networks through an extension of the existing Base Station Identification Code (BSIC) with a new 3 bit Radio frequency Colour Code (RCC). This helps the MS distinguish between cells using the same BCCH ARFCN and the same (Network colour code (NCC) and BS colour code (BCC)).\n\nThe attached Draft CR to 23.003 “Update of definition of BSIC to include Radio frequency Colour Code (Rel-13)” was endorsed at GERAN#70.\n\nFinally, please note that GERAN#70 is the final and last GERAN meeting. The responsibility will be taken over by RAN WG6 and any further correspondence should therefore be addressed to RAN WG6.","","70","7.3.5","Addressing and Subscriber Data Handling [TEI13]",0,"noted","2016-06-22T15:23:40.387","2016-06-22T15:47:51.757","","","Rel-13","","","eDRX_GSM, CIoT_EC_GSM","","","","",null,"CT4",null,"GP-160488"]
["C4-164015","LS on RAN2 agreements on eDRX Paging Hyper-frame Calculation","RAN2","Kimmo Kymalainen",19464,"LS in","","Information","RAN2 respectfully asks SA2 and RAN3 to take the RAN2 agreements into account and align the relevant specification.","","7","4","Input liaison statements: allocation to agenda items as appropriate",0,"noted","2016-06-22T15:23:40.387","2016-06-22T15:47:51.757","","","Rel-13","","","LTE_extDRX-Core","","","","",null,"RAN3, SA2","CT4","R2-164575"]
["C4-164016","Reply LS on NB-IOT NAS retransmission timers","RAN2","Kimmo Kymalainen",19464,"LS in","","Information","RAN WG2 would like to ask SA2 and CT1 to take the answer into account.","","7","4","Input liaison statements: allocation to agenda items as appropriate",0,"noted","2016-06-22T15:23:40.400","2016-06-22T15:47:51.757","","","Rel-13","","","NB_IOT-Core","","","","",null,"SA2, CT1","CT4, RAN3","R2-164578"]
["C4-164017","Reply LS on UE context retention at SCTP recovery","RAN3","Kimmo Kymalainen",19464,"LS in","","Action","RAN3 thanks CT4 for reminding in the LS (R3-161040/C4-162256) to also take into account suspended UE Contexts for stage 2 description of the UE context retention at SCTP recovery function and will work on respective normative text for TS 36.300.","","7","4","Input liaison statements: allocation to agenda items as appropriate",0,"noted","2016-06-22T15:23:40.400","2016-06-22T15:47:51.757","","","Rel-13","","","","","","","",null,"CT4","SA2","R3-161500"]
["C4-164018","LS on V2V Authorization","RAN3","Kimmo Kymalainen",19464,"LS in","","Action","Within the scope of V2V services based on LTE sidelink Work Item, RAN3 discussed the normative work on the authorization of UEs supporting V2V Service. \n\nRAN3 believes that the V2V authorization information needs to be provided to the eNB from a trusted node (i.e. the MME or another eNB), and to be extensible in the future (i.e. further considering the possible outcome of the RAN V2X SI). RAN3 has technically endorsed the attached CRs which introduce a Vehicular Services Authorized IE.","","7","4","Input liaison statements: allocation to agenda items as appropriate",0,"noted","2016-06-22T15:23:40.417","2016-06-22T15:47:51.773","","","Rel-14","","","LTE_SL_V2V","","","","",null,"CT4, SA2","RAN2, RAN1, SA1","R3-161540"]
["C4-164019","Reply LS on eDRX Paging Hyper-frame and PTW_Start Calculation","RAN Plenary","Kimmo Kymalainen",19464,"LS in","","Information","On eDRX Paging Hyper-frame and PTW_Start calculation informed by RAN2 in R2-164575, TSG-RAN discussed if PTW_start calculation is modified to ensure uniform distribution of SN used for paging as well as Paging Hyper-frame. However, TSG-RAN was unable to conclude on the modification of PTW_start calculation and decided to postpone the topic together with the RAN2 agreed CR on Paging Hyper-frame calculation in R2-164574.","","7","4","Input liaison statements: allocation to agenda items as appropriate",0,"noted","2016-06-22T15:23:40.417","2016-06-22T15:47:51.773","","","Rel-13","","","LTE_extDRX-Core","","","","",null,"RAN2, RAN3, SA2","CT1, CT4","RP-161311"]
["C4-164020","LS on Support of EAP Re-authentication for WLAN Interworking","SA2","Kimmo Kymalainen",19464,"LS in","","Action","SA2 would like to inform SA3, CT4 and CT1 that the attached Rel-14 CR to TS 23.402 has been approved in order to support EAP re-authentication for interworking with non-3GPP accesses (typically WLANs).","","7","4","Input liaison statements: allocation to agenda items as appropriate",0,"noted","2016-06-22T15:23:40.417","2016-06-22T15:47:51.773","","","Rel-14","","","TEI14","","","","",null,"CT4, SA3, CT1",null,"S2-162796"]
["C4-164021","LS for enhancements required for charging of PDN connection to SCEF","SA5","Kimmo Kymalainen",19464,"LS in","","Action","During the work on Cellular Internet of Things for Rel-13, SA5 has identified a primary set of required enhancements for the starting phase of the CIoT for charging purpose, for the solution based on the Non-IP data delivery to SCS/AS mechanism using a PDN connection towards a SCEF.\n\nThe following information has been considered as needed to be conveyed from the MME towards the SCEF, through the IWK-SCEF in roaming:\n- \tUE identification (i.e. IMEISV) \n- \tserving PLMN identification (i.e. MCC and MNC).\t\n  \nIn addition, SA5 assumed the RAT type is already specified as conveyed towards the SCEF during the initial PDN connection. SA5 sees also the need for the SCEF/IWK-SCEF to be aware on the RAT type change, if not already specified.","","64","7.2.14","CIoT-CT (CT1)  [CIoT-CT]",0,"noted","2016-06-22T15:23:40.430","2016-06-22T15:47:51.773","","","Rel-13","","","CIoT-CH","","","","",null,"CT4, SA2",null,"S5-163259"]
["C4-164022","LS to SA2 on Control Plane CIoT EPS Optimisation Indicator propagated to PGW for charging purpose","SA5","Kimmo Kymalainen",19464,"LS in","","Action","During the work on Cellular Internet of Things for Rel-13, SA5 has introduced an indicator “Control Plane CIoT EPS Optimisation” in order to indicate whether the data transfer occurred over S11-U (i.e. Control Plane CIoT EPS Optimisation is used), or over S1-U, for the data counted.\n\nSA5 believes this is an important aspect from charging perspective, to know whether “Control Plane CIoT EPS Optimisation” has been used or not for the data delivery using PDN connection to PGW.\n\nIt is SA5 understanding this information is available in the S-GW, but not available to the PGW.\nSA5 would like to get confirmation from SA2 on this, and, in such a case to consider specifying conveyance of “Control Plane CIoT EPS Optimisation” use indicator to the PGW for charging purpose.","","64","7.2.14","CIoT-CT (CT1)  [CIoT-CT]",0,"noted","2016-06-22T15:23:40.430","2016-06-22T15:47:51.787","","","Rel-13","","","CIoT-CH","","","","",null,"CT4, SA2",null,"S5-163271"]
["C4-164023","LS to CT3 for PDP type extension to non-IP PDN type","SA5","Kimmo Kymalainen",19464,"LS in","","Information","Non-IP PDN connection to PGW introduced in Rel-13 for Cellular Internet of Things is specified in TS 23.401 with a new “non-IP” PDN type. This new PDN type has been specified in SA5 charging specifications, as an extension of the existing PDN Type. \n\nThe SA5 reference for the encoding of the PDP/PDN Type is TS 29.061, which is now required to be extended for charging purposes.","","64","7.2.14","CIoT-CT (CT1)  [CIoT-CT]",0,"noted","2016-06-22T15:23:40.447","2016-06-22T15:47:51.787","","","Rel-13","","","CIoT-CH","","","","",null,null,"CT4, SA2","S5-163274"]
["C4-164024","CT4 Chairman's Status Report from TSG CT and SA #72","CT4 Chairman","Nigel. H Berry",68268,"discussion","","Information","","","6","3","Meeting Reports",0,"noted","2016-06-22T15:45:15.973","2016-07-15T19:01:12.540","","","","","","","","","","","","","","",""]
["C4-164025","Adding missing result code","Huawei","Peter Schmitt",13753,"CR","","Approval","REsult code   5515 is added in subclause 6.3.3.10","","37","7.1.9","Monitoring Enhancements CT aspects [MONTE-CT]",0,"agreed","2016-06-27T13:41:15.883","2016-07-14T06:27:13.397","","","Rel-13","29.128","13.1.0","MONTE-CT","0020","","F","CP-160427","","","","",""]
["C4-164026","Correction of  Reference for ePCO","Huawei","Peter Schmitt",13753,"CR","","Approval","correction of  an incorrect reference","","64","7.2.14","CIoT-CT (CT1)  [CIoT-CT]",0,"revised","2016-06-28T08:29:41.837","2016-07-14T06:27:13.397","","C4-164255","Rel-13","29.128","13.1.0","CIoT-CT","0021","","F",null,"","","","",""]
["C4-164027","Allocate missing AVP and experimental result codes for  CIoT","Huawei","Peter Schmitt",13753,"CR","","Approval","","","64","7.2.14","CIoT-CT (CT1)  [CIoT-CT]",0,"merged","2016-06-28T08:33:49.640","2016-07-14T06:27:13.397","","C4-164256","Rel-13","29.230","13.5.0","CIoT-CT","0566","","F",null,"","","","",""]
["C4-164028","Alocate missing AVP and experimental result codes for  CIoT","Huawei","Peter Schmitt",13753,"CR","","Approval","","","64","7.2.14","CIoT-CT (CT1)  [CIoT-CT]",0,"merged","2016-06-28T08:36:19.603","2016-07-14T06:27:13.397","","","Rel-14","29.230","14.1.0","CIoT-CT","0567","","A",null,"","","","",""]
["C4-164029","LS on Introduction of simulcast and pause-resume usage into MMCMH","SA4","Bo Burman",16624,"LS in","","Action","At CT#71 it was found that the MMCMH feature introduced in TS 26.114 in Release 13 includes some items that are not yet supported in CT specifications. SA4 was informed that CT4 is planning to add these items in Release 14 in the MMCMH_Enh-CT work item. Alignment is therefore needed. At SA#72, functionality corresponding to Release 14 CT work was removed from TS 26.114 Release 13.","","11","6.1.1","CT aspects of MTSI Extension on Multi-stream Multiparty Conferencing Media Handling [MMCMH-CT]",0,"noted","2016-07-06T08:02:09.777","2016-07-06T08:10:23.733","","","Rel-13","","","MMCMH_Enh, MMCMH_Enh-CT","","","","",null,"CT1, CT3, CT4",null,"S4-160784","C4-164111, C4-164266, C4-164271"]
["C4-164030","Reply LS on EVS over CS","SA4","Imre Varga",16587,"LS in","","Information","SA4 agrees that it is not necessary to do extensive redocumentation and considers it appropriate to work as CT3 proposes.","","7","4","Input liaison statements: allocation to agenda items as appropriate",0,"noted","2016-07-06T08:04:41.567","2016-07-06T08:10:23.750","","","Rel-13","","","EVSoCS","","","","",null,"CT3","CT4","S4-160834"]
["C4-164031","LS on I-WLAN handling and specification withdrawal","SA","Edward Hall",43958,"LS in","","Action","SA asks SA1, SA2, SA3, SA3-LI, SA5, CT1, CT3, CT4, CT6, and CT to note reference to the specific discontinuation of I-WLAN and the future availability of a feature discontinuation process. Please update any existing I-WLAN references to specifically point to the latest versions of the I-WLAN specifications that still contain technical content.","","7","4","Input liaison statements: allocation to agenda items as appropriate",0,"noted","2016-07-06T08:10:02.360","2016-07-06T08:10:23.750","","","Rel-13","","","WLAN-IW","","","","",null,"SA1, SA2, SA3, SA3-LI, SA5, CT1, CT3, CT4, CT6, CT",null,"SP-160508"]
["C4-164032","Discussion on Protocol Selection for Sx Interface of Control / User Plane Separated EPC","Cisco Systems Inc","Sridhar Bhaskaran",58580,"discussion","","Discussion","Discussion paper on protocol selection for Sx interface","","25","6.3.8","CUPS",0,"revised","2016-07-08T08:57:36.223","2016-07-15T05:28:44.727","","C4-164172","Rel-14","","","","","","","","","","","",""]
["C4-164033","Discussion on Mapping of Gx and Sd Features to U Plane","Cisco Systems Inc","Sridhar Bhaskaran",58580,"discussion","","Discussion","Discussion paper on mapping of Gx and Sd features to corresponding feature requirements from U plane.","","25","6.3.8","CUPS",0,"revised","2016-07-08T09:00:17.680","2016-07-15T05:28:44.727","","C4-164173","Rel-14","","","","","","","","","","","",""]
["C4-164034","Define new experimental-result from 3GPP AAA to ePDG to indicate EIR check result","ZTE/Joy","Xingyue Zhou",42680,"CR","","Agreement","","","14","6.1.4","EIR check for WLAN access to EPC [EWE-CT]",0,"withdrawn","2016-07-11T10:14:51.190",null,"","","Rel-14","29.273","13.4.0","EWE-CT","0460","","B",null,"","","","",""]
["C4-164035","Handling of Exception Reports in the Core Network","Huawei, Vodafone","Peter Schmitt",13753,"CR","","Approval","","","64","7.2.14","CIoT-CT (CT1)  [CIoT-CT]",0,"revised","2016-07-11T12:01:05.050","2016-07-15T12:18:32.093","C4-163260","C4-164197","Rel-13","29.274","13.6.0","CIoT-CT","1743","4","F",null,"","","","",""]
["C4-164036","Handling of Exception Reports in the Core Network","Huawei","Peter Schmitt",13753,"CR","","Approval","","","64","7.2.14","CIoT-CT (CT1)  [CIoT-CT]",0,"revised","2016-07-11T12:03:42.047","2016-07-15T12:18:32.093","","C4-164254","Rel-13","29.128","13.1.0","CIoT-CT","0022","","F",null,"","","","",""]
["C4-164037","New. WID on CT aspects of Control and User Plane Separation of EPC nodes (CUPS-CT)","Huawei, , Nokia, Alcatel-Lucent Shanghai Bell","Peter Schmitt",13753,"WID new","","Approval","","","8","5","Work item management",0,"revised","2016-07-11T12:07:02.430","2016-07-15T12:18:32.093","","C4-164170","","","","FS_CUPS, CUPS","","","","","","","","",""]
["C4-164038","Work planning for CUPS","Huawei","Peter Schmitt",13753,"discussion","","Information","","","25","6.3.8","CUPS",0,"revised","2016-07-11T12:09:47.957","2016-07-15T12:18:32.110","","C4-164171","","","","CUPS","","","","","","","","",""]
["C4-164039","S-CSCF Restoration during Registration enhancement","Ericsson","Maria-Cruz Bartolome",44824,"CR","","Action","","","22","6.3.5","IMS [TEI14]",0,"revised","2016-07-12T08:16:16.447","2016-07-15T11:15:29.227","","C4-164199","Rel-13","23.380","13.3.0","TEI14","0088","","B",null,"","","","",""]
["C4-164040","S-CSCF Restoration during Registration enhancement","Ericsson","Maria-Cruz Bartolome",44824,"CR","","Action","","","22","6.3.5","IMS [TEI14]",0,"revised","2016-07-12T08:19:29.217","2016-07-15T11:15:29.227","","C4-164200","Rel-13","29.228","13.2.0","TEI14","0666","","B",null,"","","","",""]
["C4-164041","Notification of changes to RepositoryData for an Alias Public User Identity Set","Ericsson","Maria-Cruz Bartolome",44824,"CR","","Action","","","149","9.21","IMS [TEI11]",0,"revised","2016-07-12T08:29:05.163","2016-07-15T11:15:29.243","","C4-164242","Rel-11","29.328","11.17.0","TEI11","0563","","F",null,"","","","",""]
["C4-164042","CT aspects of Support of Emergency services over WLAN – phase 2","Nokia, Alcatel-Lucent Shanghai Bell","Bruno Landais",68755,"WID new","","Approval","","","8","5","Work item management",0,"revised","2016-07-12T08:34:24.430","2016-07-13T15:47:48.437","","C4-164179","","","","","","","","","","","","",""]
["C4-164043","3GPP AAA Server / Proxy – EIR (S13'') reference point","Nokia, Alcatel-Lucent Shanghai Bell","Bruno Landais",68755,"CR","","Approval","","","14","6.1.4","EIR check for WLAN access to EPC [EWE-CT]",0,"revised","2016-07-12T08:34:24.447","2016-07-13T15:47:48.437","","C4-164220","Rel-14","29.273","13.4.0","EWE-CT","0461","","B",null,"","","","",""]
["C4-164044","STa and SWm extensions for IMEI check","Nokia, Alcatel-Lucent Shanghai Bell","Bruno Landais",68755,"CR","","Approval","","","14","6.1.4","EIR check for WLAN access to EPC [EWE-CT]",0,"revised","2016-07-12T08:34:24.527","2016-07-13T15:47:48.453","","C4-164221","Rel-14","29.273","13.4.0","EWE-CT","0462","","B",null,"","","","",""]
["C4-164045","STa and SWm extensions for IMEI check","Nokia, Alcatel-Lucent Shanghai Bell","Bruno Landais",68755,"CR","","Approval","","","14","6.1.4","EIR check for WLAN access to EPC [EWE-CT]",0,"revised","2016-07-12T08:34:24.603","2016-07-13T15:47:48.453","","C4-164222","Rel-14","29.230","14.1.0","EWE-CT","0568","","B",null,"","","","",""]
["C4-164046","F-TEID allocation principles with CUPS","Nokia, Alcatel-Lucent Shanghai Bell","Bruno Landais",68755,"discussion","","Decision","","","25","6.3.8","CUPS",0,"revised","2016-07-12T08:34:24.667","2016-07-13T15:47:48.453","","C4-164169","Rel-14","","","","","","","","","","","",""]
["C4-164047","Pseudo-CR on CP and UP selection functions","Nokia, Alcatel-Lucent Shanghai Bell","Bruno Landais",68755,"discussion","","Approval","","","25","6.3.8","CUPS",0,"postponed","2016-07-12T08:34:24.680","2016-07-13T15:47:48.453","","","Rel-14","","","","","","","","","","","",""]
["C4-164048","MT SMS handling for extended idle mode DRX – SMS over SGs","Nokia, Alcatel-Lucent Shanghai Bell","Bruno Landais",68755,"CR","","Approval","","","60","7.2.10","Extended DRX cycle for power consumption optimization (CT1) [eDRX]",0,"revised","2016-07-12T08:34:24.680","2016-07-13T15:47:48.470","","C4-164238","Rel-13","29.002","13.4.0","eDRX-CT","1217","","F",null,"","","","",""]
["C4-164049","MT SMS handling for extended idle mode DRX – SMS over SGs","Nokia, Alcatel-Lucent Shanghai Bell","Bruno Landais",68755,"CR","","Approval","","","60","7.2.10","Extended DRX cycle for power consumption optimization (CT1) [eDRX]",0,"revised","2016-07-12T08:34:24.743","2016-07-13T15:47:48.470","","C4-164239","Rel-14","29.002","14.0.0","eDRX-CT","1218","","A",null,"","","","",""]
["C4-164050","CT4 impacts for CIoT","Nokia, Alcatel-Lucent Shanghai Bell","Bruno Landais",68755,"discussion","","Information","","","64","7.2.14","CIoT-CT (CT1)  [CIoT-CT]",0,"noted","2016-07-12T08:34:24.837","2016-07-13T15:47:48.470","","","Rel-13","","","CIoT-CT","","","","","","","","",""]
["C4-164051","CT4 impacts for support of Extended Coverage and NB-IoT","Nokia, Alcatel-Lucent Shanghai Bell","Bruno Landais",68755,"discussion","","Decision","","","64","7.2.14","CIoT-CT (CT1)  [CIoT-CT]",0,"noted","2016-07-12T08:34:24.837","2016-07-13T15:47:48.483","","","Rel-13","","","CIoT-CT","","","","","","","","",""]
["C4-164052","Extended DL Data Buffering for Extended Coverage","Nokia, Alcatel-Lucent Shanghai Bell","Bruno Landais",68755,"CR","","Approval","","","64","7.2.14","CIoT-CT (CT1)  [CIoT-CT]",0,"revised","2016-07-12T08:34:24.853","2016-07-13T15:47:48.483","","C4-164193","Rel-13","29.274","13.6.0","CIoT-CT","1744","","F",null,"","","","",""]
["C4-164053","Extended DL Data Buffering for Extended Coverage","Nokia, Alcatel-Lucent Shanghai Bell","Bruno Landais",68755,"CR","","Approval","","","64","7.2.14","CIoT-CT (CT1)  [CIoT-CT]",0,"revised","2016-07-12T08:34:24.917","2016-07-13T15:47:48.500","","C4-164194","Rel-14","29.274","14.0.0","CIoT-CT","1745","","A",null,"","","","",""]
["C4-164054","Dedicated bearer signalling for a UE using Extended Coverage","Nokia, Alcatel-Lucent Shanghai Bell","Bruno Landais",68755,"CR","","Approval","","","64","7.2.14","CIoT-CT (CT1)  [CIoT-CT]",0,"revised","2016-07-12T08:34:24.993","2016-07-13T15:47:48.500","","C4-164195","Rel-13","29.274","13.6.0","CIoT-CT","1746","","F",null,"","","","",""]
["C4-164055","Dedicated bearer signalling for a UE using Extended Coverage","Nokia, Alcatel-Lucent Shanghai Bell","Bruno Landais",68755,"CR","","Approval","","","64","7.2.14","CIoT-CT (CT1)  [CIoT-CT]",0,"revised","2016-07-12T08:34:25.057","2016-07-13T15:47:48.500","","C4-164196","Rel-14","29.274","14.0.0","CIoT-CT","1747","","A",null,"","","","",""]
["C4-164056","PDN-Connection-Restricted flag","Nokia, Alcatel-Lucent Shanghai Bell, Verizon, Vodafone","Bruno Landais",68755,"CR","","Approval","","","64","7.2.14","CIoT-CT (CT1)  [CIoT-CT]",0,"agreed","2016-07-12T08:34:25.133","2016-07-13T15:47:48.500","","","Rel-13","29.272","13.6.0","CIoT-CT","0644","","F","CP-160423","","","","",""]
["C4-164057","PDN-Connection-Restricted flag","Nokia, Alcatel-Lucent Shanghai Bell, Verizon, Vodafone","Bruno Landais",68755,"CR","","Approval","","","64","7.2.14","CIoT-CT (CT1)  [CIoT-CT]",0,"agreed","2016-07-12T08:34:25.197","2016-07-13T15:47:48.517","","","Rel-14","29.272","14.0.0","CIoT-CT","0645","","A","CP-160423","","","","",""]
["C4-164058","PDN-Connection-Restricted flag","Nokia, Alcatel-Lucent Shanghai Bell, Verizon, Vodafone","Bruno Landais",68755,"CR","","Approval","","","64","7.2.14","CIoT-CT (CT1)  [CIoT-CT]",0,"agreed","2016-07-12T08:34:25.257","2016-07-13T15:47:48.517","","CP-160572","Rel-13","23.008","13.5.0","CIoT-CT","0503","","F","CP-160423","","","","",""]
["C4-164059","Preferred Data Mode for an SGi PDN connection","Nokia, Alcatel-Lucent Shanghai Bell, Verizon","Bruno Landais",68755,"CR","","Approval","","","64","7.2.14","CIoT-CT (CT1)  [CIoT-CT]",0,"revised","2016-07-12T08:34:25.337","2016-07-13T15:47:48.517","","C4-164252","Rel-13","29.272","13.6.0","CIoT-CT","0646","","F",null,"","","","",""]
["C4-164060","Preferred Data Mode for an SGi PDN connection","Nokia, Alcatel-Lucent Shanghai Bell, Verizon","Bruno Landais",68755,"CR","","Approval","","","64","7.2.14","CIoT-CT (CT1)  [CIoT-CT]",0,"revised","2016-07-12T08:34:25.397","2016-07-13T15:47:48.517","","C4-164253","Rel-14","29.272","14.0.0","CIoT-CT","0647","","A",null,"","","","",""]
["C4-164061","Preferred Data Mode for an SGi PDN connection","Nokia, Alcatel-Lucent Shanghai Bell, Verizon","Bruno Landais",68755,"CR","","Approval","","","64","7.2.14","CIoT-CT (CT1)  [CIoT-CT]",0,"agreed","2016-07-12T08:34:25.460","2016-07-13T15:47:48.517","","","Rel-13","23.008","13.5.0","CIoT-CT","0504","","F","CP-160423","","","","",""]
["C4-164062","Data switching from CP to UP without sending a Release Access Bearers Request","Nokia, Alcatel-Lucent Shanghai Bell","Bruno Landais",68755,"CR","","Approval","","","64","7.2.14","CIoT-CT (CT1)  [CIoT-CT]",0,"agreed","2016-07-12T08:34:25.570","2016-07-13T15:47:48.530","","","Rel-13","29.274","13.6.0","CIoT-CT","1748","","F","CP-160423","","","","",""]
["C4-164063","Data switching from CP to UP without sending a Release Access Bearers Request","Nokia, Alcatel-Lucent Shanghai Bell","Bruno Landais",68755,"CR","","Approval","","","64","7.2.14","CIoT-CT (CT1)  [CIoT-CT]",0,"agreed","2016-07-12T08:34:25.663","2016-07-13T15:47:48.530","","","Rel-14","29.274","14.0.0","CIoT-CT","1749","","A","CP-160423","","","","",""]
["C4-164064","S11-U bearers of multiple SGi PDN connections using Data over the Control Plane","Nokia, Alcatel-Lucent Shanghai Bell","Bruno Landais",68755,"CR","","Approval","","","64","7.2.14","CIoT-CT (CT1)  [CIoT-CT]",0,"agreed","2016-07-12T08:34:25.757","2016-07-13T15:47:48.530","","","Rel-13","29.274","13.6.0","CIoT-CT","1750","","F","CP-160423","","","","",""]
["C4-164065","S11-U bearers of multiple SGi PDN connections using Data over the Control Plane","Nokia, Alcatel-Lucent Shanghai Bell","Bruno Landais",68755,"CR","","Approval","","","64","7.2.14","CIoT-CT (CT1)  [CIoT-CT]",0,"agreed","2016-07-12T08:34:25.867","2016-07-13T15:47:48.530","","","Rel-14","29.274","14.0.0","CIoT-CT","1751","","A","CP-160423","","","","",""]
["C4-164066","MT-Data-Request command","MCC, Nokia, Alcatel-Lucent Shanghai Bell","Bruno Landais",68755,"CR","","Approval","","","64","7.2.14","CIoT-CT (CT1)  [CIoT-CT]",0,"agreed","2016-07-12T08:34:25.960","2016-07-13T15:47:48.547","","","Rel-13","29.128","13.1.0","CIoT-CT","0023","","F","CP-160423","","","","",""]
["C4-164067","Sending of ePCO during the T6a connection release procedure","Nokia, Alcatel-Lucent Shanghai Bell","Bruno Landais",68755,"CR","","Approval","","","64","7.2.14","CIoT-CT (CT1)  [CIoT-CT]",0,"revised","2016-07-12T08:34:26.053","2016-07-13T15:47:48.547","","C4-164262","Rel-13","29.128","13.1.0","CIoT-CT","0024","","F",null,"","","","",""]
["C4-164068","Missing AVP codes and Experimental-Result codes for T6a","Nokia, Alcatel-Lucent Shanghai Bell","Bruno Landais",68755,"CR","","Approval","","","64","7.2.14","CIoT-CT (CT1)  [CIoT-CT]",0,"revised","2016-07-12T08:34:26.133","2016-07-13T15:47:48.547","","C4-164261","Rel-13","29.128","13.1.0","CIoT-CT","0025","","F",null,"","","","",""]
["C4-164069","Missing AVP codes and Experimental-Result codes for T6a","Nokia, Alcatel-Lucent Shanghai Bell","Bruno Landais",68755,"CR","","Approval","","","64","7.2.14","CIoT-CT (CT1)  [CIoT-CT]",0,"revised","2016-07-12T08:34:26.193","2016-07-13T15:47:48.547","","C4-164259","Rel-13","29.230","13.5.0","CIoT-CT","0569","","F",null,"","","","",""]
["C4-164070","Missing AVP codes and Experimental-Result codes for T6a","Nokia, Alcatel-Lucent Shanghai Bell","Bruno Landais",68755,"CR","","Approval","","","64","7.2.14","CIoT-CT (CT1)  [CIoT-CT]",0,"revised","2016-07-12T08:34:26.287","2016-07-13T15:47:48.547","","C4-164260","Rel-14","29.230","14.1.0","CIoT-CT","0570","","A",null,"","","","",""]
["C4-164071","APN subscription check in the STa authentication and authorization procedure","Nokia, Alcatel-Lucent Shanghai Bell","Bruno Landais",68755,"CR","","Approval","","","68","7.3.3","EPS AAA interfaces [TEI13]",0,"agreed","2016-07-12T08:34:26.367","2016-07-13T15:47:48.563","","","Rel-13","29.273","13.4.0","TEI13","0463","","F","CP-160418","","","","",""]
["C4-164072","Unaccepted PDN connection during an Intra-MME/SGSN handover","Nokia, Alcatel-Lucent Shanghai Bell","Bruno Landais",68755,"CR","","Approval","","","66","7.3.1","GTP and PMIP [TEI13]",0,"revised","2016-07-12T08:34:26.443","2016-07-13T15:47:48.577","","C4-164225","Rel-13","29.274","13.6.0","TEI13","1752","","F",null,"","","","",""]
["C4-164073","Unaccepted PDN connection during an Intra-MME/SGSN handover","Nokia, Alcatel-Lucent Shanghai Bell","Bruno Landais",68755,"CR","","Approval","","","66","7.3.1","GTP and PMIP [TEI13]",0,"revised","2016-07-12T08:34:26.523","2016-07-13T15:47:48.577","","C4-164226","Rel-14","29.274","14.0.0","TEI13","1753","","A",null,"","","","",""]
["C4-164074","Notification of changes to RepositoryData for an Alias Public User Identity Set","Ericsson","Maria-Cruz Bartolome",44824,"CR","","Action","","","149","9.21","IMS [TEI11]",0,"revised","2016-07-12T08:42:09.167","2016-07-15T11:15:29.227","","C4-164243","Rel-12","29.328","12.12.0","TEI11","0564","","A",null,"","","","",""]
["C4-164075","Notification of changes to RepositoryData for an Alias Public User Identity Set","Ericsson","Maria-Cruz Bartolome",44824,"CR","","Action","","","149","9.21","IMS [TEI11]",0,"revised","2016-07-12T08:45:00.877","2016-07-15T11:15:29.243","","C4-164244","Rel-13","29.328","13.5.0","TEI11","0565","","A",null,"","","","",""]
["C4-164076","Correction on ePCO","Ericsson","Yong Yang",42295,"CR","","Action","","","64","7.2.14","CIoT-CT (CT1)  [CIoT-CT]",0,"revised","2016-07-12T11:10:16.917","2016-07-15T13:25:25.293","","C4-164280","Rel-13","29.274","13.6.0","","1754","","F",null,"","","","",""]
["C4-164077","Clarification on the release of unsuccessful EPC bearer context at mobility procedures when interworking with CIoT","Ericsson","Yong Yang",42295,"CR","","Action","","","64","7.2.14","CIoT-CT (CT1)  [CIoT-CT]",0,"revised","2016-07-12T11:29:09.810","2016-07-15T13:25:25.293","","C4-164202","Rel-13","29.274","13.6.0","CIoT-CT","1755","","F",null,"","","","",""]
["C4-164078","Clarification on the inclusion of the Serving PLMN Rate Control during Inter MME procedure","Ericsson LM","Yong Yang",42295,"CR","","Action","","","64","7.2.14","CIoT-CT (CT1)  [CIoT-CT]",0,"revised","2016-07-12T11:37:04.203","2016-07-15T13:25:25.293","","C4-164205","Rel-13","29.274","13.6.0","CIoT-CT","1756","","F",null,"","","","",""]
["C4-164079","Inclusion of UE TCP Port","Ericsson","Yong Yang",42295,"CR","","Action","","","66","7.3.1","GTP and PMIP [TEI13]",0,"revised","2016-07-12T11:44:10.363","2016-07-15T13:25:25.293","","C4-164230","Rel-13","29.274","13.6.0","TEI13","1757","","F",null,"","","","",""]
["C4-164080","Discussion on the unexpected PDN deletion due to obsoleted command message","Ericsson","Yong Yang",42295,"discussion","","Discussion","","","66","7.3.1","GTP and PMIP [TEI13]",0,"noted","2016-07-12T11:48:51.720","2016-07-15T13:25:25.307","","C4-164232","","","","","","","","","","","","",""]
["C4-164081","Inclusion of Sender' F-TEID in the Command message","Ericsson","Yong Yang",42295,"CR","","Action","","","66","7.3.1","GTP and PMIP [TEI13]",0,"revised","2016-07-12T11:53:55.107","2016-07-15T13:25:25.307","","C4-164233","Rel-13","29.274","13.6.0","TEI13","1758","","F",null,"","","","",""]
["C4-164082","Discussion on the new indication from PGW for NBIFOM","Huawei","Youyang Yu",46021,"discussion","","Discussion","","","56","7.2.6","IP Flow Mobility support for S2a and S2b Interfaces on stage 3 (CT1) [NBIFOM]",0,"noted","2016-07-13T04:35:50.160","2016-07-15T08:47:36.660","","","","","","NBIFOM-CT","","","","","","","","",""]
["C4-164083","New Flag from PGW to SGSN","Huawei","Youyang Yu",46021,"CR","","Action","","","56","7.2.6","IP Flow Mobility support for S2a and S2b Interfaces on stage 3 (CT1) [NBIFOM]",0,"revised","2016-07-13T04:35:50.190","2016-07-15T08:47:36.660","","C4-164211","Rel-13","29.274","13.6.0","NBIFOM-CT","1759","","F",null,"","","","",""]
["C4-164084","New Flag from PGW to SGSN","Huawei","Youyang Yu",46021,"CR","","Action","","","56","7.2.6","IP Flow Mobility support for S2a and S2b Interfaces on stage 3 (CT1) [NBIFOM]",0,"revised","2016-07-13T04:35:50.330","2016-07-15T08:47:36.660","","C4-164212","Rel-14","29.274","14.0.0","NBIFOM-CT","1760","","A",null,"","","","",""]
["C4-164085","Failure case for NBIFOM","Huawei","Youyang Yu",46021,"CR","","Action","","","56","7.2.6","IP Flow Mobility support for S2a and S2b Interfaces on stage 3 (CT1) [NBIFOM]",0,"revised","2016-07-13T04:35:50.440","2016-07-15T08:47:36.673","","C4-164213","Rel-13","23.007","13.5.0","NBIFOM-CT","0342","","F",null,"","","","",""]
["C4-164086","Failure case for NBIFOM","Huawei","Youyang Yu",46021,"CR","","Action","","","56","7.2.6","IP Flow Mobility support for S2a and S2b Interfaces on stage 3 (CT1) [NBIFOM]",0,"revised","2016-07-13T04:35:50.533","2016-07-15T08:47:36.673","","C4-164214","Rel-14","23.007","14.0.0","NBIFOM-CT","0343","","A",null,"","","","",""]
["C4-164087","LS on the new Flag from PGW to SGSN","Huawei","Youyang Yu",46021,"LS out","","Approval","","","56","7.2.6","IP Flow Mobility support for S2a and S2b Interfaces on stage 3 (CT1) [NBIFOM]",0,"revised","2016-07-13T04:35:50.597","2016-07-15T08:47:36.673","","C4-164215","","","","NBIFOM-CT","","","",""]
["C4-164088","Skeleton for TR Study on control and user plane separation of EPC nodes","Huawei","Peter Schmitt",13753,"other","","Decision","","","25","6.3.8","CUPS",0,"revised","2016-07-13T06:04:49.770","2016-07-15T12:18:32.110","","C4-164191","","","","","","","","","","","","",""]
["C4-164089","Pseudo-CR on Solution for PGW-U Failure with Restart – Solution #1","Cisco Systems Inc","Sridhar Bhaskaran",58580,"discussion","","Approval","Stage 2 had identified that the TEID and GTPU address allocation after restoration of the U plane can follow solution #3 given in sub-clause 6.1.1.5.4 but has left the decision upto CT4 to discuss and decide. This is a PCR to the new CUPS TR adding a solution for PGW-U restoration with restart.","","25","6.3.8","CUPS",0,"revised","2016-07-13T06:32:59.427","2016-07-15T05:28:44.727","","C4-164264","Rel-14","","","","","","","","","","","",""]
["C4-164090","Pseudo-CR on Solution for PGW-U Failure without Restart – Solution#1","Cisco Systems Inc","Sridhar Bhaskaran",58580,"discussion","","Approval","Stage 2 had identified that the TEID and GTPU address allocation after restoration of the U plane can follow solution #3 given in sub-clause 6.1.1.5.4 but has left the decision upto CT4 to discuss and decide. This is a PCR to the new CUPS TR adding a solution for PGW-U restoration without restart.","","25","6.3.8","CUPS",0,"revised","2016-07-13T06:34:41.950","2016-07-15T05:28:44.710","","C4-164274","Rel-14","","","","","","","","","","","",""]
["C4-164091","Pseudo-CR on Solution for PGW-U Faillure Without Restart – Solution #2","Cisco Systems Inc","Sridhar Bhaskaran",58580,"discussion","","Approval","Stage 2 had identified that the TEID and GTPU address allocation after restoration of the U plane can follow solution #3 given in sub-clause 6.1.1.5.4 but has left the decision upto CT4 to discuss and decide. This is a PCR to the new CUPS TR adding a solution for PGW-U restoration without restart.","","25","6.3.8","CUPS",0,"revised","2016-07-13T06:37:20.007","2016-07-15T05:28:44.710","","C4-164275","Rel-14","","","","","","","","","","","",""]
["C4-164092","Pseudo-CR on Solution for SGW-U Failure with Restart – Solution #1","Cisco Systems Inc","Sridhar Bhaskaran",58580,"discussion","","Approval","Stage 2 had identified that the TEID and GTPU address allocation after restoration of the U plane can follow solution #3 given in sub-clause 6.1.1.5.4 but has left the decision upto CT4 to discuss and decide. This is a PCR to the new stage 3 CUPS TR adding a solution for SGW-U restoration with restart.","","25","6.3.8","CUPS",0,"revised","2016-07-13T06:39:35.430","2016-07-15T05:29:18.983","","C4-164265","Rel-14","","","","","","","","","","","",""]
["C4-164093","Pseudo-CR on Solution for SGW-U Failure without Restart – Solution#1","Cisco Systems Inc","Sridhar Bhaskaran",58580,"discussion","","Approval","Stage 2 had identified that the TEID and GTPU address allocation after restoration of the U plane can follow solution #3 given in sub-clause 6.1.1.5.4 but has left the decision upto CT4 to discuss and decide. This is a PCR to the new stage 3 CUPS TR adding a solution for SGW-U restoration without restart.","","25","6.3.8","CUPS",0,"revised","2016-07-13T06:41:51.383","2016-07-15T05:28:44.710","","C4-164276","Rel-14","","","","","","","","","","","",""]
["C4-164094","Pseudo-CR on Solution for SGW-U Faillure Without Restart – Solution #2","Cisco Systems Inc","Sridhar Bhaskaran",58580,"discussion","","Approval","Stage 2 had identified that the TEID and GTPU address allocation after restoration of the U plane can follow solution #3 given in sub-clause 6.1.1.5.4 but has left the decision upto CT4 to discuss and decide. This is a PCR to the new stage 3 CUPS TR adding a solution for SGW-U restoration without restart","","25","6.3.8","CUPS",0,"revised","2016-07-13T06:43:48.070","2016-07-15T05:28:44.680","","C4-164277","Rel-14","","","","","","","","","","","",""]
["C4-164095","Pseudo-CR on Solution for SGW-U Faillure Without Restart – Solution #2","Cisco Systems Inc","Sridhar Bhaskaran",58580,"discussion","","Approval","Stage 2 had identified that the TEID and GTPU address allocation after restoration of the U plane can follow solution #3 given in sub-clause 6.1.1.5.4 but has left the decision upto CT4 to discuss and decide. This is a PCR to the new stage 3 CUPS TR adding a solution for SGW-U restoration without restart","","25","6.3.8","CUPS",0,"withdrawn","2016-07-13T06:44:57.850",null,"","","Rel-14","","","","","","","","","","","",""]
["C4-164096","Convery Serving PLMN ID and IMEISV to the SCEF","ZTE","Zhijun Li",39295,"CR","","Approval","As per SA5 (S5-163259) requested, the MME needs to convery the Serving PLMN ID and IMEISV to the SCEF for charging purpose.","","64","7.2.14","CIoT-CT (CT1)  [CIoT-CT]",0,"merged","2016-07-13T06:45:29.737","2016-07-15T07:12:33.187","","","Rel-13","29.128","13.1.0","CIoT-CT","0026","","F",null,"","","","",""]
["C4-164097","SCEF Behavior of Rate Control Handling","ZTE","Zhijun Li",39295,"CR","","Approval","This contribution clarifies the SCEF behavior of handling downlink/uplink Non-IP data if Rate Control is activated.","","64","7.2.14","CIoT-CT (CT1)  [CIoT-CT]",0,"revised","2016-07-13T06:45:29.847","2016-07-15T07:12:33.187","","C4-164282","Rel-13","29.128","13.1.0","CIoT-CT","0027","","F",null,"","","","",""]
["C4-164098","Not Able to Deliver MO Non-IP Data","ZTE","Zhijun Li",39295,"CR","","Approval","If the SCS/AS has requested the SCEF to delete NIDD configuration context, the SCEF is not able to continue forward MO Non-IP data to the SCS/AS. The SCEF shall stop the NIDD delivery procedure and may responds error cause to the MME.","","64","7.2.14","CIoT-CT (CT1)  [CIoT-CT]",0,"revised","2016-07-13T06:45:29.953","2016-07-15T07:12:33.203","","C4-164283","Rel-13","29.128","13.1.0","CIoT-CT","0028","","F",null,"","","","",""]
["C4-164099","Indicating Control Plane CIoT EPS Optimization when Generating CDR","ZTE","Zhijun Li",39295,"CR","","Approval","As per SA5 (S5-163271) requested, the PGW needs to know whether the CP/S11-U is used for generating differentiated CDR. If Control Plane Only indication is set to a PDN, such information can be used by the PGW to indicate Control Plane CIoT EPS Optimization in CDR.","","64","7.2.14","CIoT-CT (CT1)  [CIoT-CT]",0,"postponed","2016-07-13T06:45:30.033","2016-07-15T07:12:33.203","","","Rel-13","29.274","13.6.0","CIoT-CT","1761","","F",null,"","","","",""]
["C4-164100","Indicating Control Plane CIoT EPS Optimization when Generating CDR","ZTE","Zhijun Li",39295,"CR","","Approval","Mirror CR","","64","7.2.14","CIoT-CT (CT1)  [CIoT-CT]",0,"postponed","2016-07-13T06:45:30.110","2016-07-15T07:12:33.187","","","Rel-14","29.274","14.0.0","CIoT-CT","1762","","A",null,"","","","",""]
["C4-164101","Addressing the Editor’s Note on high load resulting from shared subscription data update","Nokia, Alcatel-Lucent Shanghai Bell","Ulrich Wiehe",6963,"CR","","Agreement","","","13","6.1.3","Shared Subscription Data Update [eSDU]",0,"withdrawn","2016-07-13T08:27:35.067","2016-07-15T09:26:56.050","","","Rel-14","29.272","14.0.0","eSDU","0648","","F",null,"","","","",""]
["C4-164102","Removal of Editor’s Note on non shareable subscription data","Nokia, Alcatel-Lucent Shanghai Bell","Ulrich Wiehe",6963,"CR","","Agreement","","","13","6.1.3","Shared Subscription Data Update [eSDU]",0,"revised","2016-07-13T08:30:34.607","2016-07-15T09:26:56.050","","C4-164207","Rel-14","29.272","14.0.0","eSDU","0649","","F",null,"","","","",""]
["C4-164103","Removal of Editor’s Note on detailed checks for shared subscription data update","Nokia, Alcatel-Lucent Shanghai Bell","Ulrich Wiehe",6963,"CR","","Agreement","","","13","6.1.3","Shared Subscription Data Update [eSDU]",0,"agreed","2016-07-13T08:32:55.117","2016-07-15T09:26:56.050","","","Rel-14","29.272","14.0.0","eSDU","0650","","F","CP-160437","","","","",""]
["C4-164104","ASN.1 module version update","Nokia, Alcatel-Lucent Shanghai Bell","Ulrich Wiehe",6963,"CR","","Agreement","","","23","6.3.6","MAP [TEI14]",0,"agreed","2016-07-13T08:39:49.200","2016-07-15T09:26:56.050","","","Rel-14","29.002","14.0.0","TEI14","1219","","F","CP-160430","","","","",""]
["C4-164105","New WID on Diameter Load Control Mechanisms","Nokia, Alcatel-Lucent Shanghai Bell","Ulrich Wiehe",6963,"WID new","","Agreement","","","8","5","Work item management",0,"revised","2016-07-13T08:42:50.517","2016-07-15T09:26:56.067","","C4-164180","","","","","","","","","","","","",""]
["C4-164106","T6a Connection Release after MO Data Answer with permanent error","Nokia,Alcatel-Lucent Shanghai Bell","Ulrich Wiehe",6963,"CR","","Agreement","","","64","7.2.14","CIoT-CT (CT1)  [CIoT-CT]",0,"revised","2016-07-13T08:50:33.507","2016-07-15T09:26:56.033","","C4-164284","Rel-13","29.128","13.1.0","CIoT-CT","0029","","F",null,"","","","",""]
["C4-164107","Addition of Serving PLMN ID and IMEISV to CMR","Nokia, Alcatel-Lucent Shanghai Bell","Ulrich Wiehe",6963,"CR","","Agreement","","","64","7.2.14","CIoT-CT (CT1)  [CIoT-CT]",0,"revised","2016-07-13T08:54:36.553","2016-07-15T09:26:56.033","","C4-164263","Rel-13","29.128","13.1.0","CIoT-CT","0030","","F",null,"","","","",""]
["C4-164108","Restoration procedures for CUPS","Huawei","Youyang Yu",46021,"discussion","","Discussion","","","25","6.3.8","CUPS",0,"revised","2016-07-13T09:20:00.320","2016-07-15T11:24:31.120","","C4-164278","","","","CUPS","","","","","","","","",""]
["C4-164109","Source SGSN behavior if Target does not support CIoT optimizations","ORANGE","Julien Bournelle",41373,"CR","","Action","","","16","6.2.1","CT aspects for Non-IP for Cellular Internet of Things for 2G/3G-GPRS [NonIP_GPRS-CT]",0,"revised","2016-07-13T11:23:25.430","2016-07-13T13:19:25.637","","C4-164216","Rel-14","29.060","14.0.0","NonIP_GPRS-CT","1040","","B",null,"","","","",""]
["C4-164110","Use of DNS to select a GGSN handling Non-IP data","ORANGE","Julien Bournelle",41373,"CR","","Action","","","16","6.2.1","CT aspects for Non-IP for Cellular Internet of Things for 2G/3G-GPRS [NonIP_GPRS-CT]",0,"revised","2016-07-13T11:34:17.910","2016-07-13T13:19:25.637","","C4-164217","Rel-14","29.303","13.4.0","","0090","","B",null,"","","","",""]
["C4-164111","Reply LS on Introduction of simulcast and pause-resume usage into MMCMH","CT4","Nevenka Biondic",41878,"LS out","","Approval","","","11","6.1.1","CT aspects of MTSI Extension on Multi-stream Multiparty Conferencing Media Handling [MMCMH-CT]",0,"revised","2016-07-13T12:28:28.853","2016-07-15T15:52:29.407","","C4-164266","Rel-14","","","MMCMH_Enh-CT","","","","","C4-164029","3GPP SA WG4","3GPP CT WG1, 3GPP CT WG3","S4-160784"]
["C4-164112","SDP offer/answer for TLS and DTLS protected media","Ericsson","Nevenka Biondic",41878,"CR","","Agreement","","","74","7.3.9","H.248 Interfaces",0,"postponed","2016-07-13T12:28:28.853","2016-07-15T15:35:58.393","","C4-165177","Rel-13","23.334","13.5.0","TEI13","0111","","F",null,"","","","",""]
["C4-164113","SDP offer/answer for TLS and DTLS protected media","Ericsson","Nevenka Biondic",41878,"CR","","Agreement","","","74","7.3.9","H.248 Interfaces",0,"postponed","2016-07-13T12:28:28.977","2016-07-15T15:35:58.393","","","Rel-13","29.334","13.5.0","TEI13","0110","","F",null,"","","","",""]
["C4-164114","Mandatory support of RTP/RTCP multiplexing","Ericsson, Nokia","Nevenka Biondic",41878,"CR","","Agreement","","","24","6.3.7","H.248 Interfaces [TEI14]",0,"revised","2016-07-13T12:28:29.087","2016-07-15T15:35:58.407","","C4-164267","Rel-14","23.334","13.5.0","TEI14","0112","","F",null,"","","","",""]
["C4-164115","Mandatory support of RTP/RTCP multiplexing","Ericsson","Nevenka Biondic",41878,"CR","","Agreement","","","24","6.3.7","H.248 Interfaces [TEI14]",0,"revised","2016-07-13T12:28:29.180","2016-07-15T15:35:58.407","","C4-164268","Rel-14","29.334","13.5.0","TEI14","0111","","F",null,"","","","",""]
["C4-164116","Correction on ePCO","Ericsson","Yong Yang",42295,"CR","","Action","","","64","7.2.14","CIoT-CT (CT1)  [CIoT-CT]",0,"revised","2016-07-13T12:45:13.597","2016-07-15T13:25:25.307","","C4-164281","Rel-14","29.274","14.0.0","","1763","","A",null,"","","","",""]
["C4-164117","Clarification on the release of unsuccessful EPC bearer context at mobility procedures when interworking with CIoT","Ericsson","Yong Yang",42295,"CR","","Action","","","64","7.2.14","CIoT-CT (CT1)  [CIoT-CT]",0,"revised","2016-07-13T12:46:52.250","2016-07-15T13:25:25.307","","C4-164203","Rel-14","29.274","14.0.0","","1764","","A",null,"","","","",""]
["C4-164118","Support of EAP Re-authentication Protocol for WLAN Interworking","ORANGE","Julien Bournelle",41373,"WID new","","Agreement","","","8","5","Work item management",0,"revised","2016-07-13T12:47:49.533","2016-07-13T13:17:39.713","","C4-164182","Rel-14","","","","","","","","","","","",""]
["C4-164119","Clarification on the inclusion of the Serving PLMN Rate Control during Inter MME procedure","Ericsson","Yong Yang",42295,"CR","","Action","","","64","7.2.14","CIoT-CT (CT1)  [CIoT-CT]",0,"revised","2016-07-13T12:48:30.513","2016-07-15T13:25:25.307","","C4-164206","Rel-14","29.274","14.0.0","","1765","","A",null,"","","","",""]
["C4-164120","Inclusion of Sender' F-TEID in the Command message","Ericsson","Yong Yang",42295,"CR","","Action","","","66","7.3.1","GTP and PMIP [TEI13]",0,"revised","2016-07-13T12:52:12.517","2016-07-15T13:25:25.323","","C4-164234","Rel-14","29.274","14.0.0","","1766","","A",null,"","","","",""]
["C4-164121","Inclusion of UE TCP Port","Ericsson","Yong Yang",42295,"CR","","Action","","","66","7.3.1","GTP and PMIP [TEI13]",0,"revised","2016-07-13T12:53:50.077","2016-07-15T13:25:25.293","","C4-164231","Rel-14","29.274","14.0.0","","1767","","A",null,"","","","",""]
["C4-164122","CR implementation error on ECR and ECA commands","Ericsson, MCC","Jesus De Gregorio",40423,"CR","","Action","","","48","7.1.20","Diameter Message Priority [DiaPri]",0,"agreed","2016-07-13T13:13:59.833","2016-07-15T12:58:44.430","","","Rel-13","29.272","13.6.0","DiaPri","0651","","F","CP-160428","","","","",""]
["C4-164123","CR implementation error on ECR and ECA commands","Ericsson, MCC","Jesus De Gregorio",40423,"CR","","Action","","","48","7.1.20","Diameter Message Priority [DiaPri]",0,"agreed","2016-07-13T13:17:03.163","2016-07-15T12:58:44.430","","","Rel-14","29.272","14.0.0","DiaPri","0652","","A","CP-160428","","","","",""]
["C4-164124","T6b reference point for NonIP-GPRS","Ericsson","Jesus De Gregorio",40423,"CR","","Action","","","16","6.2.1","CT aspects for Non-IP for Cellular Internet of Things for 2G/3G-GPRS [NonIP_GPRS-CT]",0,"revised","2016-07-13T13:20:42.687","2016-07-15T12:58:44.430","","C4-164223","Rel-14","29.128","13.1.0","NonIP_GPRS-CT","0031","","B",null,"","","","",""]
["C4-164125","Network Access Mode in non-3GPP access","Ericsson","Jesus De Gregorio",40423,"CR","","Action","","","20","6.3.3","EPS AAA interfaces (29.273) [TEI14]",0,"postponed","2016-07-13T13:26:05.150","2016-07-15T12:58:44.447","","","Rel-14","23.008","13.5.0","TEI14","0505","","F",null,"","","","",""]
["C4-164126","Network Access Mode in non-3GPP access","Ericsson","Jesus De Gregorio",40423,"CR","","Action","","","20","6.3.3","EPS AAA interfaces (29.273) [TEI14]",0,"postponed","2016-07-13T13:28:22.837","2016-07-15T12:58:44.447","","","Rel-14","29.273","13.4.0","TEI14","0464","","F",null,"","","","",""]
["C4-164127","SCS identity format","Nokia, Hewlett-Packard Enterprise","Ulrich Wiehe",6963,"CR","","Agreement","","","140","9.13.2","Reach ability Aspects of SIMTC [SIMTC-Reach]",0,"revised","2016-07-13T13:28:36.750","2016-07-15T13:55:18.063","C4-161101","C4-164208","Rel-11","29.336","11.2.0","SIMTC-Reach","0041","1","F",null,"","","","",""]
["C4-164128","Change of Network Access Mode","Ericsson","Jesus De Gregorio",40423,"CR","","Agreement","","","20","6.3.3","EPS AAA interfaces (29.273) [TEI14]",0,"agreed","2016-07-13T13:31:30.797","2016-07-15T12:58:44.447","","","Rel-14","29.272","14.0.0","TEI14","0653","","F","CP-160433","","","","",""]
["C4-164129","SCS identity format","Nokia, Hewlett-Packard Enterprise","Ulrich Wiehe",6963,"CR","","Agreement","","","140","9.13.2","Reach ability Aspects of SIMTC [SIMTC-Reach]",0,"revised","2016-07-13T13:31:45.527","2016-07-15T13:55:18.063","C4-161102","C4-164209","Rel-12","29.336","12.5.0","SIMTC-Reach","0042","1","A",null,"","","","",""]
["C4-164130","SCS identity format","Nokia, Hewlett-Packard Enterprise","Ulrich Wiehe",6963,"CR","","Agreement","","","140","9.13.2","Reach ability Aspects of SIMTC [SIMTC-Reach]",0,"revised","2016-07-13T13:32:56.940","2016-07-15T13:55:18.063","C4-161103","C4-164210","Rel-13","29.336","13.4.0","SIMTC-Reach","0043","1","A",null,"","","","",""]
["C4-164131","Usage of Supported Features","Ericsson","Jesus De Gregorio",40423,"CR","","Agreement","","","21","6.3.4","Diameter based Interfaces (29.272, 29.173) [TEI14]",0,"agreed","2016-07-13T13:34:20.290","2016-07-15T12:58:44.447","","","Rel-14","29.272","14.0.0","TEI14","0654","","F","CP-160432","","","","",""]
["C4-164132","Handling of MSISDN removal from subscription profile","Ericsson","Jesus De Gregorio",40423,"CR","","Agreement","","","21","6.3.4","Diameter based Interfaces (29.272, 29.173) [TEI14]",0,"agreed","2016-07-13T13:38:34.103","2016-07-15T12:58:44.463","","","Rel-14","29.272","14.0.0","TEI14","0655","","B","CP-160432","","","","",""]
["C4-164133","Simultaneous updates not allowed","Ericsson","Maria-Cruz Bartolome",44824,"CR","","Agreement","","","22","6.3.5","IMS [TEI14]",0,"revised","2016-07-13T13:53:24.077","2016-07-15T11:15:29.257","","C4-164201","Rel-13","29.328","13.5.0","TEI14","0566","","B",null,"","","","",""]
["C4-164134","Simultaneous updates not allowed","Ericsson","Maria-Cruz Bartolome",44824,"CR","","Agreement","","","22","6.3.5","IMS [TEI14]",0,"revised","2016-07-13T13:56:05.893","2016-07-15T11:15:29.257","","C4-164273","Rel-13","29.329","13.0.0","TEI14","0228","","B",null,"","","","",""]
["C4-164135","TS Skeleton Interface between Control plane and User plane nodes in Packet System","Huawei","Peter Schmitt",13753,"discussion","","Decision","","","25","6.3.8","CUPS",0,"revised","2016-07-13T13:58:42.207","2016-07-15T12:18:32.110","","C4-164192","Rel-14","","","","","","","","","","","",""]
["C4-164136","Non REGISTER authentication after S-CSCF restart","Ericsson","Maria-Cruz Bartolome",44824,"CR","","Agreement","","","149","9.21","IMS [TEI11]",0,"agreed","2016-07-13T13:59:29.003","2016-07-15T11:15:29.243","","","Rel-11","23.380","11.3.0","TEI11","0089","","F","CP-160415","","","","",""]
["C4-164137","TS Scope for CUPS","Huawei","Peter Schmitt",13753,"discussion","","Decision","","","25","6.3.8","CUPS",0,"revised","2016-07-13T14:00:12.607","2016-07-15T12:18:32.110","","C4-164279","Rel-14","","","","","","","","","","","",""]
["C4-164138","Non REGISTER authentication after S-CSCF restart","Ericsson","Maria-Cruz Bartolome",44824,"CR","","Agreement","","","149","9.21","IMS [TEI11]",0,"agreed","2016-07-13T14:01:37.220","2016-07-15T11:15:29.243","","","Rel-12","23.380","12.3.0","TEI11","0090","","A","CP-160415","","","","",""]
["C4-164139","P-CR, Session management and message structure of messages for CUPS","Huawei","Peter Schmitt",13753,"discussion","","Decision","","","25","6.3.8","CUPS",0,"noted","2016-07-13T14:01:43.007","2016-07-15T12:18:32.110","","","Rel-14","","","","","","","","","","","",""]
["C4-164140","Transferring AAA identifier from the ePDG/TWAN to the PGW","ORANGE","Lionel Morand",25150,"CR","","Agreement","C4-161459 (CR#1693) has introduced in the TS 29.274 the ability for the ePDG and the TWAN to provide over S2a/S2b the selected 3GPP AAA server's identities to the PDN GW. These identities can be used by the PDN GW to address the 3GPP AAA server over S6b for authorization procedure. Ths behaviour is described in the TS 29.273.","","68","7.3.3","EPS AAA interfaces [TEI13]",0,"revised","2016-07-13T14:03:16.467","2016-07-13T14:07:20.090","","C4-164224","Rel-13","29.273","13.4.0","TEI13","0465","","F",null,"","","","",""]
["C4-164141","Non REGISTER authentication after S-CSCF restart","Ericsson","Maria-Cruz Bartolome",44824,"CR","","Agreement","","","149","9.21","IMS [TEI11]",0,"agreed","2016-07-13T14:03:26.403","2016-07-15T11:15:29.243","","","Rel-13","23.380","13.3.0","TEI11","0091","","A","CP-160415","","","","",""]
["C4-164142","Adding supported feature for eNB change reporting","China Mobile Com. Corporation","Zhenning Huang",60086,"CR","","Agreement","Adding supported feature for eNB change reporting","","18","6.3.1","GTP and PMIP [TEI14]",0,"revised","2016-07-13T14:36:03.350","2016-07-15T17:40:17.727","","C4-164236","Rel-14","29.274","14.0.0","TEI14","1768","","B",null,"","","","",""]
["C4-164143","New Work Item for the core network aspects of Extended Architecture support for CIoT","Intel","Vivek Gupta",36134,"WID new","","Endorsement","","","8","5","Work item management",0,"postponed","2016-07-13T14:45:18.423","2016-07-18T05:40:02.070","","","Rel-14","","","","","","","","","","","",""]
["C4-164144","Status report on EnTV","QUALCOMM Incorporated/Amer","Amer Catovic",39766,"report","","Information","Status report on the SA2 study item on EnTV with a preliminary forecast of the scope of work n CT groups for Release 14.","","26","6.3.9","EnTV",0,"noted","2016-07-13T15:24:58.003","2016-07-15T07:17:00.533","","","Rel-14","","","","","","","","","","","",""]
["C4-164145","Solution to avoid high load resulting from shared subscription data update","Ericsson","Maria-Cruz Bartolome",44824,"CR","","Agreement","","","13","6.1.3","Shared Subscription Data Update [eSDU]",0,"revised","2016-07-13T15:50:27.557","2016-07-15T11:15:29.257","","C4-164204","Rel-14","29.272","14.0.0","eSDU","0656","","F",null,"","","","",""]
["C4-164146","New RAT Type for C-IoT","Ericsson","Jesus De Gregorio",40423,"CR","","Agreement","","","64","7.2.14","CIoT-CT (CT1)  [CIoT-CT]",0,"revised","2016-07-13T15:51:10.737","2016-07-15T12:58:44.463","","C4-164250","Rel-13","29.002","13.4.0","CIoT-CT","1220","","F",null,"","","","",""]
["C4-164147","New RAT Type for C-IoT","Ericsson","Jesus De Gregorio",40423,"CR","","Agreement","","","64","7.2.14","CIoT-CT (CT1)  [CIoT-CT]",0,"revised","2016-07-13T15:55:29.010","2016-07-15T12:58:44.463","","C4-164251","Rel-14","29.002","14.0.0","CIoT-CT","1221","","A",null,"","","","",""]
["C4-164148","New Work Item for CT aspects of V2X Services","LG Electronics Inc.","Taehun Kim",58301,"WID new","","Endorsement","","","8","5","Work item management",0,"revised","2016-07-14T00:22:31.307","2016-07-15T07:29:05.117","","C4-164154","Rel-14","","","","","","","","","","","",""]
["C4-164149","Mandatory support for RTP/RTCP multiplexing for WebRTC","Nokia","Thomas Belling",68266,"CR","","Agreement","","","24","6.3.7","H.248 Interfaces [TEI14]",0,"withdrawn","2016-07-14T15:24:57.880",null,"","","Rel-14","23.334","13.5.0","TEI14","0113","","B",null,"","","","",""]
["C4-164150","Transport of T.140 and BFCP within data channels","Nokia","Thomas Belling",68266,"CR","","Agreement","If T.140 is transported over the data channel, then draft-schwarz-mmusic-t140-usage-data-channel shall be used. As T.140 is transported via unreliable RTP/UDP in the IMS core network, some application aware correction of packet loss (as described in ITU-T H.248.94 Appendix II) is required in the eIMS-AGW.\nIf BFCP is transported over the data channel, then draft-schwarz-mmusic-bfcp-usage-data-channel shall be used.","","24","6.3.7","H.248 Interfaces [TEI14]",0,"revised","2016-07-14T15:28:04.190","2016-07-15T12:50:16.560","","C4-164269","Rel-14","23.334","13.5.0","TEI14","0114","","B",null,"","","","",""]
["C4-164151","Transport of T.140 within data channels","Nokia","Thomas Belling",68266,"CR","","Agreement","If T.140 is transported over the data channel, then draft-schwarz-mmusic-t140-usage-data-channel shall be used. As T.140 is transported via unreliable RTP/UDP in the IMS core network, some application aware correction of packet loss (as described in ITU-T H.248.94 Appendix II) is required in the eIMS-AGW.","","22","6.3.5","IMS [TEI14]",0,"revised","2016-07-14T15:33:03.287","2016-07-15T12:50:16.560","","C4-164270","Rel-14","29.334","13.5.0","TEI14","0112","","B",null,"","","","",""]
["C4-164152","ePCO and PCO handling at the PGW","ZTE","Fei Lu",39755,"CR","","Approval","","","64","7.2.14","CIoT-CT (CT1)  [CIoT-CT]",0,"not pursued","2016-07-15T03:28:06.343","2016-07-15T06:45:16.387","","","Rel-13","29.274","13.6.0","","1769","","F",null,"","","","",""]
["C4-164153","ePCO and PCO handling at the PGW","ZTE","Fei Lu",39755,"CR","","Approval","","","64","7.2.14","CIoT-CT (CT1)  [CIoT-CT]",0,"not pursued","2016-07-15T03:29:50.503","2016-07-15T06:45:16.387","","","Rel-14","29.274","14.0.0","","1770","","A",null,"","","","",""]
["C4-164154","New Work Item for CT aspects of V2X Services","LG Electronics Inc.","Taehun Kim",58301,"WID new","","Endorsement","","","8","5","Work item management",0,"revised","2016-07-15T07:34:23.650","2016-07-15T08:08:02.073","C4-164148","C4-164184","Rel-14","","","","","","","","","","","",""]
["C4-164155","AVP codes for 32.299","Nokia, Alcatel-Lucent Shanghai Bell","Ulrich Wiehe",6963,"CR","","Agreement","","","67","7.3.2","Diameter 29.230 CRs [TEI13]",0,"revised","2016-07-15T09:07:13.017","2016-07-15T09:26:56.033","","C4-164227","Rel-13","29.230","13.5.0","CH13, NBIFOM-CH, CIoT-CH","0571","","F",null,"","","","",""]
["C4-164156","AVP codes for 32.299","Nokia, Alcatel-Lucent Shanghai Bell","Ulrich Wiehe",6963,"CR","","Agreement","","","67","7.3.2","Diameter 29.230 CRs [TEI13]",0,"revised","2016-07-15T09:12:56.743","2016-07-15T09:26:56.033","","C4-164228","Rel-14","29.230","14.1.0","CH13, NBIFOM-CH, CH14, CIoT-CH","0572","","F",null,"","","","",""]
["C4-164157","Reply LS for enhancements required for charging of PDN connection to SCEF","SA2","Hannu Hietalahti",69922,"LS in","","Action","SA2 thanks SA5 for their work on CIoT charging aspects, and would like to acknowledge the addition of new parameters (IMEISV and Serving PLMN identity) in T6a, T6b and T7 to make SCEF aware of the ME identity and the Serving PLMN identity. \n\nSA2 confirms that SCEF will already be aware of RAT type. Since Inter-RAT mobility between NB-IoT and other RAT is not supported in Rel-13, this RAT type cannot change between NB-IoT and other RAT during the life time of the PDN connection to SCEF in Rel-13.\n\nSA2 is studying inter-RAT mobility as part of Rel-14 study item FS_CIoT_Ext.","","64","7.2.14","CIoT-CT (CT1)  [CIoT-CT]",0,"noted","2016-07-16T21:36:01.673","2016-07-16T21:52:31.657","","","Rel-13","","","CIoT-CH","","","","",null,"SA5, CT4",null,"S2-163767"]
["C4-164158","Response to SA5 “LS on Control Plane CIoT EPS Optimisation Indicator propagated to PGW for charging purpose”","SA2","Chris Pudney",1122,"LS in","","Action","SA2 thanks SA5 for their LS on the ability to independently record data volumes for data sent over S11-U and that over S1-U.\n\nSA2 agree that the SGW has the information that enables it to do this differentiation. \n\nCurrently SA2 has not specified the means for the PGW to do this differentiation for any PDN connection that one MME can switch between S11-U and S1-U. \n\nSA2 are concerned that it might increase SGW – PGW signalling load considerably. \n\nSA2 also note that the choice between use of S11-U and S1-U (for a device that can use both) is under VPLMN control, hence SA2 are not sure whether or not the HPLMN needs to know which bearer is being used.\n\nSA2 would like to invite CT4 to consider solutions and their associated signalling load before SA2 updates the stage 2 signalling flows.","","64","7.2.14","CIoT-CT (CT1)  [CIoT-CT]",0,"noted","2016-07-16T21:38:55.080","2016-07-16T21:52:31.657","","","Rel-13","","","CIoT-CH","","","","",null,"SA5, CT4",null,"S2-163768","C4-164188, C4-164288"]
["C4-164159","LS on Guidance and requests for work related to control and user plane split EPC architecture","SA2","Nirav Salot",56645,"LS in","","Action","CUPS\nThis is to inform CT4 that SA2 has recently concluded the study phase of CUPS workitem and now starting the normative work for the same.\nSA2 is starting the normative work just now and hence more details and other aspects, e.g. impacts for supporting CIoT architecture, etc., will be available as the normative work progresses. However, CT4’s questions or feedback on any of the aspects will be welcomed by SA2.","","25","6.3.8","CUPS",0,"noted","2016-07-16T21:42:07.133","2016-07-16T21:52:31.657","","","Rel-14","","","CUPS","","","","",null,"CT4","CT3","S2-164014"]
["C4-164160","LS on MT NIDD procedures at the T6a/T6b interface","SA2","Hans Ronneke",25844,"LS in","","Action","Related to alignment of the TS 23.682 stage 2 specification with stage 3 TS 29.128, SA2 discussed the latest rel-13 version which extends the MT NIDD PDUs with new optional parameters “SCEF wait time”, “Maximum Re-transmission Time” and “Requested Re-transmission time”.\nSA2 asks CT4 to decide a way forward for this topic and inform SA2 of the result and clarification of MME handling as needed.","","64","7.2.14","CIoT-CT (CT1)  [CIoT-CT]",0,"noted","2016-07-16T21:45:33.817","2016-07-16T21:52:31.673","","","Rel-13","","","CIoT-CH","","","","",null,"CT4",null,"S2-164073"]
["C4-164161","LS on Retrieval of S1-U SGW F-TEID by MME","SA2","Dario Serafino Tonesi",43468,"LS in","","Action","Since, according to CT4 requirements, it must be possible to set different IP addresses for S1-U and S11-U tunnels, the MME may not be able to obtain the valid S1-U SGW F-TEID(s) when establishing S1-U bearers during the Data Transport in Control Plane CIoT EPS optimisation procedure.\n\n\nOne possible solution that would not change the current “Establishment of S1-U bearer during Data Transport in Control Plane CIoT EPS optimisation” procedure (see TS 23.401) would be to keep the S11-U SGW F-TEID same as the S1-U SGW F-TEID. This would however require to update the CT4 principle described above.","","64","7.2.14","CIoT-CT (CT1)  [CIoT-CT]",0,"noted","2016-07-16T21:48:50.123","2016-07-16T21:52:31.673","","","Rel-13","","","CIoT-CT","","","","",null,"CT4",null,"S2-164076"]
["C4-164162","LS on Improvement to authentication procedure for supporting Emergency Service on WLAN","SA2","Marco Spini",8356,"LS in","","Information","SA2 would like to inform SA3 that the Release 14 normative work related to the support of Emergency Services for voice over WLAN for both Trusted and Untrusted WLAN  for UE without valid IMSI and for Unauthenticated UE (e.g. without IMSI) has been completed.","","7","4","Input liaison statements: allocation to agenda items as appropriate",0,"noted","2016-07-16T21:51:51.113","2016-07-16T21:52:31.673","","","Rel-14","","","SEW2","","","","",null,"SA3","CT1, CT4","S2-164273"]
["C4-164163","TS 29.283 \"User-Data-Id\" AVP datatype","Kodiak Networks","Tom Hiller",60380,"discussion","","Discussion","Discussion on changing the datatype of the 29.383 \"User-Data-ID\" AVP from unsigned 32-bit integer to string.","","61","7.2.11","Mission Critical Push To Talk over LTE protocol aspects (CT1) [MCPTT-CT]",0,"noted","2016-07-17T16:42:14.210","2016-07-17T16:47:04.320","","","Rel-13","29.283","13.1.0","","","","","","","","","",""]
["C4-164164","DP on Rel-14 Impacts on 3GPP specs of ERP","ORANGE","Julien Bournelle",41373,"discussion","","Discussion","","","8","5","Work item management",0,"noted","2016-07-18T11:34:05.113","2016-07-18T11:52:23.033","","","Rel-14","","","","","","","","","","","",""]
["C4-164165","Current Location Retrieval","Nokia, Alcatel-Lucent Shanghai Bell","Ulrich Wiehe",6963,"CR","","Agreement","","","60","7.2.10","Extended DRX cycle for power consumption optimization (CT1) [eDRX]",0,"revised","2016-07-20T10:01:11.420","2016-07-20T10:07:16.130","","C4-164240","Rel-13","29.272","13.6.0","TEI13, eDRX-CT","0657","","F",null,"","","","",""]
["C4-164166","Current Location Retrieval","Nokia, Alcatel-Lucent Shanghai Bell","Ulrich Wiehe",6963,"CR","","Agreement","","","60","7.2.10","Extended DRX cycle for power consumption optimization (CT1) [eDRX]",0,"revised","2016-07-20T10:05:21.983","2016-07-20T10:07:16.130","","C4-164241","Rel-14","29.272","14.0.0","TEI13, eDRX-CT","0658","","A",null,"","","","",""]
["C4-164167","Reference [18] correction","Nokia, Alcatel-Lucent Shanghai Bell","Ulrich Wiehe",6963,"CR","","Agreement","","","73","7.3.8","MAP [TEI13]",0,"withdrawn","2016-07-20T11:10:51.317","2016-07-20T11:16:30.087","","","Rel-13","29.002","13.4.0","TEI13","1222","","F",null,"","","","",""]
["C4-164168","Reference [18] correction","Nokia, Alcatel-Lucent Shanghai Bell","Ulrich Wiehe",6963,"CR","","Agreement","","","73","7.3.8","MAP [TEI13]",0,"withdrawn","2016-07-20T11:13:44.603","2016-07-20T11:16:30.087","","","Rel-14","29.002","14.0.0","TEI13","1223","","A",null,"","","","",""]
["C4-164169","F-TEID allocation principles with CUPS","Nokia, Alcatel-Lucent Shanghai Bell","Bruno Landais",68755,"discussion","","Decision","","","25","6.3.8","CUPS",0,"noted","2016-07-20T15:04:27.140","2016-07-22T15:03:01.383","C4-164046","","Rel-14","","","","","","","","","","","",""]
["C4-164170","New. WID on CT aspects of Control and User Plane Separation of EPC nodes (CUPS-CT)","Huawei, , Nokia, Alcatel-Lucent Shanghai Bell","Peter Schmitt",13753,"WID new","","Approval","","","8","5","Work item management",0,"revised","2016-07-22T11:01:14.990","2016-07-22T11:12:12.713","C4-164037","C4-164178","","","","FS_CUPS, CUPS","","","","","","","","",""]
["C4-164171","Work planning for CUPS","Huawei","Peter Schmitt",13753,"discussion","","Information","","","25","6.3.8","CUPS",0,"noted","2016-07-22T11:02:58.977","2016-07-22T11:12:12.727","C4-164038","","","","","CUPS","","","","","","","","",""]
["C4-164172","Discussion on Protocol Selection for Sx Interface of Control / User Plane Separated EPC","Cisco Systems Inc","Sridhar Bhaskaran",58580,"discussion","","Discussion","Discussion paper on protocol selection for Sx interface","","25","6.3.8","CUPS",0,"noted","2016-07-22T12:10:09.870","2016-07-22T12:45:20.423","C4-164032","","Rel-14","","","","","","","","","","","",""]
["C4-164173","Discussion on Mapping of Gx and Sd Features to U Plane","Cisco Systems Inc","Sridhar Bhaskaran",58580,"discussion","","Discussion","Discussion paper on mapping of Gx and Sd features to corresponding feature requirements from U plane.","","25","6.3.8","CUPS",0,"noted","2016-07-22T12:26:14.800","2016-07-22T14:05:05.740","C4-164033","","Rel-14","","","","","","","","","","","",""]
["C4-164174","Reply LS on MT NIDD procedures at the T6a/T6b interface","Nokia, Alcatel-Lucent Shanghai Bell","Bruno Landais",68755,"LS out","","Approval","","","7","4","Input liaison statements: allocation to agenda items as appropriate",0,"revised","2016-07-22T14:34:12.507","2016-07-22T14:44:42.137","","C4-164218","Rel-13","","","","","","","","S2-164073","SA2"]
["C4-164175","LS reply to LS on Feasibility Study on the Diameter Base Protocol Update","SA5","Maryse Gardella",68914,"LS in","","Action","SA5 will consider this recommendation as decorrelated from the TR 29.819 conclusions and recommendations on Diameter Base Protocol Update from IETF RFC 3588 to the IETF RFC 6733, and can conclude SA5 has no comment on the final TR 29.819 v1.2.0.","","47","7.1.19","Feasibility Study on the Diameter Base Protocol Update [FS_DBPU]",0,"noted","2016-07-24T15:57:05.697","2016-07-24T16:01:26.167","","","Rel-13","","","FS_DBPU","","","","",null,"CT4","CT3","S5-164180"]
["C4-164176","LS on Addition of AVP code definitions","SA5","Maryse Gardella",68914,"LS in","","Action","SA5 kindly asks CT4 to take into account the AVP definitions and update their specifications accordingly.","","64","7.2.14","CIoT-CT (CT1)  [CIoT-CT]",0,"noted","2016-07-24T16:00:53.577","2016-07-24T16:01:26.167","","","Rel-13","","","CH13, NBIFOM-CH, CH14, CIoT-CH","","","","",null,"CT4","CT3","S5-164301"]
["C4-164177","SGW Potential Paging Enhancements","AT&T","Martin Dolly",44313,"discussion","","Discussion","Today, if MME receives the Downlink Data Notification (DDN) message, the MME shall reply the DDN Ack immediately regardless whether the actual paging is successful or not.  Then later if MME goes through the paging cycle and cannot find the UE or due to some other network failure in the middle of the paging, the MME will send the DDN failure indication message to the SGW. That terminates the whole paging process. This is not an optimal architecture.","","18","6.3.1","GTP and PMIP [TEI14]",0,"noted","2016-07-24T16:08:07.787","2016-07-24T16:10:22.070","","","Rel-14","","","","","","","","","","","",""]
["C4-164178","New. WID on CT aspects of Control and User Plane Separation of EPC nodes (CUPS-CT)","Huawei, Nokia, Alcatel-Lucent Shanghai Bell","Peter Schmitt",13753,"WID new","","Approval","","","8","5","Work item management",0,"agreed","2016-07-25T09:45:50.137","2016-07-29T12:03:58.597","C4-164170","","","","","FS_CUPS, CUPS","","","","","","","","",""]
["C4-164179","CT aspects of Support of Emergency services over WLAN – phase 2","Nokia, Alcatel-Lucent Shanghai Bell","Bruno Landais",68755,"WID new","","Approval","","","8","5","Work item management",0,"endorsed","2016-07-25T10:22:43.043","2016-07-29T12:03:58.610","C4-164042","","","","","","","","","","","","","",""]
["C4-164180","New WID on Diameter Load Control Mechanisms","Nokia, Alcatel-Lucent Shanghai Bell","Ulrich Wiehe",6963,"WID new","","Agreement","","","8","5","Work item management",0,"agreed","2016-07-25T10:29:08.877","2016-07-29T12:03:58.610","C4-164105","","","","","","","","","","","","","",""]
["C4-164181","New WID on CT aspects of Enhancements of Dedicated Core Networks selection mechanism","Ericsson","Yong Yang",42295,"WID new","","Endorsement","","","8","5","Work item management",0,"revised","2016-07-25T10:33:23.980","2016-07-29T12:03:58.610","","C4-164185","","","","","","","","","","","","",""]
["C4-164182","Support of EAP Re-authentication Protocol for WLAN Interworking","ORANGE","Julien Bournelle",41373,"WID new","","Agreement","","","8","5","Work item management",0,"revised","2016-07-25T10:39:35.803","2016-07-29T12:03:58.627","C4-164118","C4-164287","Rel-14","","","","","","","","","","","",""]
["C4-164183","WID on MCPTT enhancements","Samsung","Ricky Kaura",36916,"WID new","","Endorsement","","","8","5","Work item management",0,"revised","2016-07-25T10:53:20.243","2016-07-29T12:03:58.627","","C4-164219","Rel-14","","","","","","","","","","","",""]
["C4-164184","New Work Item for CT aspects of V2X Services","LG Electronics Inc.","Taehun Kim",58301,"WID new","","Endorsement","","","8","5","Work item management",0,"endorsed","2016-07-25T11:25:36.863","2016-07-29T12:03:58.627","C4-164154","","Rel-14","","","","","","","","","","","",""]
["C4-164185","New WID on CT aspects of Enhancements of Dedicated Core Networks selection mechanism","Ericsson","Yong Yang",42295,"WID new","","Endorsement","","","8","5","Work item management",0,"endorsed","2016-07-25T11:35:30.360","2016-07-29T12:03:58.627","C4-164181","","","","","","","","","","","","","",""]
["C4-164186","CT Aspects of Improvements of Awareness of User Location Change","HUAWEI","Yizhuang Wu",61155,"WID new","","Endorsement","","","8","5","Work item management",0,"revised","2016-07-25T11:41:59.517","2016-07-29T12:03:58.643","","C4-164187","Rel-14","","","","","","","","","","","",""]
["C4-164187","CT Aspects of Improvements of Awareness of User Location Change","HUAWEI","Yizhuang Wu",61155,"WID new","","Endorsement","","","8","5","Work item management",0,"endorsed","2016-07-25T13:17:35.473","2016-07-29T12:03:58.643","C4-164186","","Rel-14","","","","","","","","","","","",""]
["C4-164188","Reply LS to SA2 on Control Plane CIoT EPS Optimisation Indicator propagated to PGW for charging purpose","CT4","Bruno Landais",68755,"LS out","","Approval","","","64","7.2.14","CIoT-CT (CT1)  [CIoT-CT]",0,"revised","2016-07-25T13:46:36.810","2016-07-29T12:03:58.643","","C4-164288","","","","","","","","","C4-164158","SA2, SA5"]
["C4-164189","CT Aspects of S8 Home Routing Architecture for VoLTE","NTT DOCOMO INC.","Tsuyoshi Takakura",56979,"discussion","","Discussion","","","8","5","Work item management",0,"noted","2016-07-25T14:03:38.620","2016-07-29T12:03:58.643","","","","","","","","","","","","","","",""]
["C4-164190","Reply LS on Retrieval of S1-U SGW F-TEID by MME","CT4","Peter Schmitt",13753,"LS out","","Approval","","","64","7.2.14","CIoT-CT (CT1)  [CIoT-CT]",0,"revised","2016-07-25T14:37:29.493","2016-07-29T12:03:58.657","","C4-164289","Rel-13","","","CIoT-CT","","","","","S2-164076","SA2"]
["C4-164191","Skeleton for TR Study on control and user plane separation of EPC nodes","Huawei","Kimmo Kymalainen",19464,"other","","Decision","","","25","6.3.8","CUPS",0,"revised","2016-07-25T17:11:53.977","2016-07-29T12:03:58.657","C4-164088","C4-164324","","","","","","","","","","","","",""]
["C4-164192","TS Skeleton Interface between Control plane and User plane nodes in Packet System","Huawei","Peter Schmitt",13753,"discussion","","Decision","","","25","6.3.8","CUPS",0,"revised","2016-07-25T17:46:58.013","2016-07-29T12:03:58.657","C4-164135","C4-164326","Rel-14","","","","","","","","","","","",""]
["C4-164193","Extended DL Data Buffering for Extended Coverage","Nokia, Alcatel-Lucent Shanghai Bell","Bruno Landais",68755,"CR","","Approval","","","64","7.2.14","CIoT-CT (CT1)  [CIoT-CT]",0,"revised","2016-07-26T08:52:56.150","2016-07-29T12:03:58.657","C4-164052","C4-164298","Rel-13","29.274","13.6.0","CIoT-CT","1744","1","F",null,"","","","",""]
["C4-164194","Extended DL Data Buffering for Extended Coverage","Nokia, Alcatel-Lucent Shanghai Bell","Bruno Landais",68755,"CR","","Approval","","","64","7.2.14","CIoT-CT (CT1)  [CIoT-CT]",0,"revised","2016-07-26T08:54:18.487","2016-07-29T12:03:58.673","C4-164053","C4-164299","Rel-14","29.274","14.0.0","CIoT-CT","1745","1","A",null,"","","","",""]
["C4-164195","Dedicated bearer signalling for a UE using Extended Coverage","Nokia, Alcatel-Lucent Shanghai Bell","Bruno Landais",68755,"CR","","Approval","","","64","7.2.14","CIoT-CT (CT1)  [CIoT-CT]",0,"agreed","2016-07-26T08:57:43.873","2016-07-29T12:03:58.673","C4-164054","","Rel-13","29.274","13.6.0","CIoT-CT","1746","1","F","CP-160423","","","","",""]
["C4-164196","Dedicated bearer signalling for a UE using Extended Coverage","Nokia, Alcatel-Lucent Shanghai Bell","Bruno Landais",68755,"CR","","Approval","","","64","7.2.14","CIoT-CT (CT1)  [CIoT-CT]",0,"agreed","2016-07-26T08:58:25.510","2016-07-29T12:03:58.673","C4-164055","","Rel-14","29.274","14.0.0","CIoT-CT","1747","1","A","CP-160423","","","","",""]
["C4-164197","Handling of Exception Reports in the Core Network","Huawei, Vodafone","Peter Schmitt",13753,"CR","","Approval","","","64","7.2.14","CIoT-CT (CT1)  [CIoT-CT]",0,"revised","2016-07-26T09:20:32.157","2016-07-29T12:03:58.673","C4-164035","C4-164300","Rel-13","29.274","13.6.0","CIoT-CT","1743","5","F",null,"","","","",""]
["C4-164198","Handling of Exception Reports in the Core Network","Huawei, Vodafone","Peter Schmitt",13753,"CR","","Agreement","","","64","7.2.14","CIoT-CT (CT1)  [CIoT-CT]",0,"revised","2016-07-26T09:21:44.430",null,"","C4-164301","Rel-14","29.274","14.0.0","CIoT-CT","1771","","A",null,"","","","",""]
["C4-164199","S-CSCF Restoration during Registration enhancement","Ericsson","Maria-Cruz Bartolome",44824,"CR","","Agreement","","","22","6.3.5","IMS [TEI14]",0,"agreed","2016-07-26T09:25:51.033","2016-07-27T10:53:01.770","C4-164039","","Rel-14","23.380","13.3.0","TEI14","0088","1","B","CP-160431","","","","",""]
["C4-164200","S-CSCF Restoration during Registration enhancement","Ericsson","Maria-Cruz Bartolome",44824,"CR","","Agreement","","","22","6.3.5","IMS [TEI14]",0,"agreed","2016-07-26T09:27:55.630","2016-07-27T10:53:01.787","C4-164040","","Rel-14","29.228","13.2.1","TEI14","0666","1","B","CP-160431","","","","",""]
["C4-164201","Request to update data while a previous update request is in progress","Ericsson","Maria-Cruz Bartolome",44824,"CR","","Agreement","","","22","6.3.5","IMS [TEI14]",0,"agreed","2016-07-26T09:30:21.007","2016-07-29T12:03:58.690","C4-164133","","Rel-14","29.328","13.5.0","TEI14","0566","1","B","CP-160431","","","","",""]
["C4-164202","Clarification on the release of unsuccessful EPC bearer context at mobility procedures when interworking with CIoT","Ericsson","Yong Yang",42295,"CR","","Agreement","","","64","7.2.14","CIoT-CT (CT1)  [CIoT-CT]",0,"revised","2016-07-26T11:00:27.977","2016-07-29T12:03:58.690","C4-164077","C4-164312","Rel-13","29.274","13.6.0","CIoT-CT","1755","1","F",null,"","","","",""]
["C4-164203","Clarification on the release of unsuccessful EPC bearer context at mobility procedures when interworking with CIoT","Ericsson","Yong Yang",42295,"CR","","Agreement","","","64","7.2.14","CIoT-CT (CT1)  [CIoT-CT]",0,"revised","2016-07-26T11:01:01.923",null,"C4-164117","C4-164313","Rel-14","29.274","14.0.0","CIoT-CT","1764","1","A",null,"","","","",""]
["C4-164204","Solution to avoid high load resulting from shared subscription data update","Ericsson, Nokia, Alcatel-Lucent Shanghai Bell","Maria-Cruz Bartolome",44824,"CR","","Agreement","","","13","6.1.3","Shared Subscription Data Update [eSDU]",0,"revised","2016-07-26T11:02:03.590","2016-07-29T12:03:58.690","C4-164145","C4-164291","Rel-14","29.272","14.0.0","eSDU","0656","1","F",null,"","","","",""]
["C4-164205","Clarification on the inclusion of the Serving PLMN Rate Control during Inter MME procedure","Ericsson LM","Yong Yang",42295,"CR","","Agreement","","","64","7.2.14","CIoT-CT (CT1)  [CIoT-CT]",0,"agreed","2016-07-26T11:12:20.800","2016-07-29T12:03:58.707","C4-164078","","Rel-13","29.274","13.6.0","CIoT-CT","1756","1","F","CP-160423","","","","",""]
["C4-164206","Clarification on the inclusion of the Serving PLMN Rate Control during Inter MME procedure","Ericsson","Yong Yang",42295,"CR","","Agreement","","","64","7.2.14","CIoT-CT (CT1)  [CIoT-CT]",0,"agreed","2016-07-26T11:13:06.960","2016-07-29T12:03:58.707","C4-164119","","Rel-14","29.274","14.0.0","CIoT-CT","1765","1","A","CP-160423","","","","",""]
["C4-164207","Removal of Editor’s Note on non shareable subscription data","Nokia, Alcatel-Lucent Shanghai Bell","Ulrich Wiehe",6963,"CR","","Agreement","","","13","6.1.3","Shared Subscription Data Update [eSDU]",0,"agreed","2016-07-26T11:16:17.577","2016-07-29T12:03:58.707","C4-164102","","Rel-14","29.272","14.0.0","eSDU","0649","1","F","CP-160437","","","","",""]
["C4-164208","SCS identity format","Nokia, Hewlett-Packard Enterprise","Ulrich Wiehe",6963,"CR","","Agreement","","","140","9.13.2","Reach ability Aspects of SIMTC [SIMTC-Reach]",0,"agreed","2016-07-26T13:30:15.440","2016-07-29T12:03:58.707","C4-164127","","Rel-11","29.336","11.2.0","SIMTC-Reach","0041","2","F","CP-160416","","","","",""]
["C4-164209","SCS identity format","Nokia, Hewlett-Packard Enterprise","Ulrich Wiehe",6963,"CR","","Agreement","","","140","9.13.2","Reach ability Aspects of SIMTC [SIMTC-Reach]",0,"agreed","2016-07-26T13:32:06.993","2016-07-29T12:03:58.720","C4-164129","","Rel-12","29.336","12.5.0","SIMTC-Reach","0042","2","A","CP-160416","","","","",""]
["C4-164210","SCS identity format","Nokia, Hewlett-Packard Enterprise","Ulrich Wiehe",6963,"CR","","Agreement","","","140","9.13.2","Reach ability Aspects of SIMTC [SIMTC-Reach]",0,"agreed","2016-07-26T13:33:22.403","2016-07-29T12:03:58.720","C4-164130","","Rel-13","29.336","13.4.0","SIMTC-Reach","0043","2","A","CP-160416","","","","",""]
["C4-164211","New Flag from PGW to SGSN","HuaWei","Youyang Yu",46021,"CR","","Agreement","","","56","7.2.6","IP Flow Mobility support for S2a and S2b Interfaces on stage 3 (CT1) [NBIFOM]",0,"agreed","2016-07-26T13:34:20.187","2016-07-29T12:03:58.720","C4-164083","","Rel-13","29.274","13.6.0","NBIFOM-CT","1759","1","F","CP-160422","","","","",""]
["C4-164212","New Flag from PGW to SGSN","HuaWei Technologies Co., Ltd","Youyang Yu",46021,"CR","","Agreement","","","56","7.2.6","IP Flow Mobility support for S2a and S2b Interfaces on stage 3 (CT1) [NBIFOM]",0,"agreed","2016-07-26T13:34:44.897","2016-07-29T12:03:58.720","C4-164084","","Rel-14","29.274","14.0.0","NBIFOM-CT","1760","1","A","CP-160422","","","","",""]
["C4-164213","Failure case for NBIFOM","HuaWei","Youyang Yu",46021,"CR","","Agreement","","","56","7.2.6","IP Flow Mobility support for S2a and S2b Interfaces on stage 3 (CT1) [NBIFOM]",0,"agreed","2016-07-26T13:52:47.017","2016-07-29T12:03:58.737","C4-164085","","Rel-13","23.007","13.5.0","NBIFOM-CT","0342","1","F","CP-160422","","","","",""]
["C4-164214","Failure case for NBIFOM","HuaWei","Youyang Yu",46021,"CR","","Agreement","","","56","7.2.6","IP Flow Mobility support for S2a and S2b Interfaces on stage 3 (CT1) [NBIFOM]",0,"agreed","2016-07-26T13:53:10.320","2016-07-29T12:03:58.737","C4-164086","","Rel-14","23.007","14.0.0","NBIFOM-CT","0343","1","A","CP-160422","","","","",""]
["C4-164215","LS on the new Flag from PGW to SGSN","CT4","Youyang Yu",46021,"LS out","","Approval","","","56","7.2.6","IP Flow Mobility support for S2a and S2b Interfaces on stage 3 (CT1) [NBIFOM]",0,"revised","2016-07-26T13:56:51.857","2016-07-29T12:03:58.737","C4-164087","C4-164295","","","","","","","","","C4-164008","CT1"]
["C4-164216","Source SGSN behavior if Target does not support CIoT optimizations","ORANGE","Julien Bournelle",41373,"CR","","Agreement","","","16","6.2.1","CT aspects for Non-IP for Cellular Internet of Things for 2G/3G-GPRS [NonIP_GPRS-CT]",0,"revised","2016-07-26T14:06:07.320","2016-07-29T12:03:58.737","C4-164109","C4-164294","Rel-14","29.060","14.0.0","NonIP_GPRS-CT","1040","1","B",null,"","","","",""]
["C4-164217","Use of DNS to select a GGSN handling Non-IP data","ORANGE","Julien Bournelle",41373,"CR","","Agreement","","","16","6.2.1","CT aspects for Non-IP for Cellular Internet of Things for 2G/3G-GPRS [NonIP_GPRS-CT]",0,"agreed","2016-07-26T14:15:39.150","2016-07-29T12:03:58.753","C4-164110","","Rel-14","29.303","13.4.0","NonIP_GPRS-CT","0090","1","B","CP-160435","","","","",""]
["C4-164218","Reply LS on MT NIDD procedures at the T6a/T6b interface","Nokia, Alcatel-Lucent Shanghai Bell","Bruno Landais",68755,"LS out","","Approval","","","7","4","Input liaison statements: allocation to agenda items as appropriate",0,"revised","2016-07-26T14:18:44.417","2016-07-29T12:03:58.753","C4-164174","C4-164329","Rel-13","","","","","","","","S2-164073","SA2"]
["C4-164219","WID on MCPTT enhancements","Samsung","Ricky Kaura",36916,"WID new","","Endorsement","","","8","5","Work item management",0,"endorsed","2016-07-26T15:21:43.913","2016-07-29T12:03:58.753","C4-164183","","Rel-14","","","","","","","","","","","",""]
["C4-164220","3GPP AAA Server / Proxy – EIR (S13'') reference point","Nokia, Alcatel-Lucent Shanghai Bell, Orange, Ericsson, ZTE","Bruno Landais",68755,"CR","","Approval","","","14","6.1.4","EIR check for WLAN access to EPC [EWE-CT]",0,"agreed","2016-07-26T15:58:06.573","2016-07-29T12:03:58.767","C4-164043","","Rel-14","29.273","13.4.0","EWE-CT","0461","1","B","CP-160436","","","","",""]
["C4-164221","STa and SWm extensions for IMEI check","Nokia, Alcatel-Lucent Shanghai Bell, Orange, Ericsson, ZTE","Bruno Landais",68755,"CR","","Approval","","","14","6.1.4","EIR check for WLAN access to EPC [EWE-CT]",0,"revised","2016-07-26T16:11:58.783","2016-07-29T12:03:58.767","C4-164044","C4-164293","Rel-14","29.273","13.4.0","EWE-CT","0462","1","B",null,"","","","",""]
["C4-164222","STa and SWm extensions for IMEI check","Nokia, Alcatel-Lucent Shanghai Bell","Bruno Landais",68755,"CR","","Approval","","","14","6.1.4","EIR check for WLAN access to EPC [EWE-CT]",0,"agreed","2016-07-26T16:44:23.867","2016-07-29T12:03:58.767","C4-164045","","Rel-14","29.230","14.1.0","EWE-CT","0568","1","B","CP-160436","","","","",""]
["C4-164223","T6b reference point for NonIP-GPRS","Ericsson","Jesus De Gregorio",40423,"CR","","Action","","","16","6.2.1","CT aspects for Non-IP for Cellular Internet of Things for 2G/3G-GPRS [NonIP_GPRS-CT]",0,"agreed","2016-07-26T17:20:01.617","2016-07-29T12:03:58.767","C4-164124","","Rel-14","29.128","13.1.0","NonIP_GPRS-CT","0031","1","B","CP-160435","","","","",""]
["C4-164224","Transferring AAA identifier from the ePDG/TWAN to the PGW","ORANGE","Lionel Morand",25150,"CR","","Agreement","C4-161459 (CR#1693) has introduced in the TS 29.274 the ability for the ePDG and the TWAN to provide over S2a/S2b the selected 3GPP AAA server's identities to the PDN GW. These identities can be used by the PDN GW to address the 3GPP AAA server over S6b for authorization procedure. Ths behaviour is described in the TS 29.273.","","68","7.3.3","EPS AAA interfaces [TEI13]",0,"agreed","2016-07-26T17:36:47.527","2016-07-29T12:03:58.783","C4-164140","","Rel-13","29.273","13.4.0","TEI13","0465","1","F","CP-160418","","","","",""]
["C4-164225","Unaccepted PDN connection during an Intra-MME/SGSN handover","Nokia, Alcatel-Lucent Shanghai Bell","Bruno Landais",68755,"CR","","Approval","","","66","7.3.1","GTP and PMIP [TEI13]",0,"revised","2016-07-27T08:10:40.967","2016-07-29T12:03:58.783","C4-164072","C4-164310","Rel-13","29.274","13.6.0","TEI13","1752","1","F",null,"","","","",""]
["C4-164226","Unaccepted PDN connection during an Intra-MME/SGSN handover","Nokia, Alcatel-Lucent Shanghai Bell","Bruno Landais",68755,"CR","","Approval","","","66","7.3.1","GTP and PMIP [TEI13]",0,"revised","2016-07-27T08:11:40.467","2016-07-29T12:03:58.783","C4-164073","C4-164311","Rel-14","29.274","14.0.0","TEI13","1753","1","A",null,"","","","",""]
["C4-164227","AVP codes for 32.299","Nokia, Alcatel-Lucent Shanghai Bell","Ulrich Wiehe",6963,"CR","","Agreement","","","67","7.3.2","Diameter 29.230 CRs [TEI13]",0,"agreed","2016-07-27T08:12:44.037","2016-07-29T12:03:58.783","C4-164155","","Rel-13","29.230","13.5.0","CH13, NBIFOM-CH, CIoT-CH","0571","1","F","CP-160419","","","","",""]
["C4-164228","AVP codes for 32.299","Nokia, Alcatel-Lucent Shanghai Bell","Ulrich Wiehe",6963,"CR","","Agreement","","","67","7.3.2","Diameter 29.230 CRs [TEI13]",0,"agreed","2016-07-27T08:13:50.757","2016-07-29T12:03:58.800","C4-164156","","Rel-14","29.230","14.1.0","CH13, NBIFOM-CH, CH14, CIoT-CH","0572","1","F","CP-160419","","","","",""]
["C4-164229","LS on need to define MCPTT confidentiality protection FQDN","CT1","Ricky Kaura",36916,"LS in","","Action","","","61","7.2.11","Mission Critical Push To Talk over LTE protocol aspects (CT1) [MCPTT-CT]",0,"noted","2016-07-27T08:20:00.863","2016-07-29T12:03:58.800","","","","","","MCPTT-CT","","","","",null,"CT4",null,"C1-163731"]
["C4-164230","Inclusion of UE TCP Port","Ericsson","Yong Yang",42295,"CR","","Action","","","66","7.3.1","GTP and PMIP [TEI13]",0,"agreed","2016-07-27T08:20:58.303","2016-07-29T12:03:58.800","C4-164079","CP-160585","Rel-13","29.274","13.6.0","SEW1-CT","1757","1","F","CP-160420","","","","",""]
["C4-164231","Inclusion of UE TCP Port","Ericsson","Yong Yang",42295,"CR","","Action","","","66","7.3.1","GTP and PMIP [TEI13]",0,"agreed","2016-07-27T08:23:20.090","2016-07-29T12:57:10.727","C4-164121","CP-160586","Rel-14","29.274","14.0.0","SEW1-CT","1767","1","A","CP-160420","","","","",""]
["C4-164232","Discussion on the unexpected PDN deletion due to obsoleted command message","Ericsson","Yong Yang",42295,"discussion","","Discussion","","","66","7.3.1","GTP and PMIP [TEI13]",0,"noted","2016-07-27T08:49:27.817","2016-07-29T12:06:09.853","C4-164080","","","","","","","","","","","","","",""]
["C4-164233","Inclusion of Sender' F-TEID in the Command message","Ericsson","Yong Yang",42295,"CR","","Action","","","66","7.3.1","GTP and PMIP [TEI13]",0,"revised","2016-07-27T08:50:09.220","2016-07-29T12:06:09.853","C4-164081","C4-164314","Rel-13","29.274","13.6.0","TEI13","1758","1","F",null,"","","","",""]
["C4-164234","Inclusion of Sender' F-TEID in the Command message","Ericsson","Yong Yang",42295,"CR","","Action","","","66","7.3.1","GTP and PMIP [TEI13]",0,"revised","2016-07-27T08:50:56.860",null,"C4-164120","C4-164315","Rel-14","29.274","14.0.0","","1766","1","A",null,"","","","",""]
["C4-164235","MCPTT confidentiality protection FQDN","Ericsson","Maria-Cruz Bartolome",44824,"CR","","Agreement","","","61","7.2.11","Mission Critical Push To Talk over LTE protocol aspects (CT1) [MCPTT-CT]",0,"revised","2016-07-27T09:33:38.053","2016-07-27T10:13:34.557","","C4-164246","Rel-13","23.003","13.6.0","MCPTT-CT","0442","","F",null,"","","","",""]
["C4-164236","Adding supported feature for eNB change reporting","China Mobile Com. Corporation","Kimmo Kymalainen",19464,"CR","","Agreement","Adding supported feature for eNB change reporting","","18","6.3.1","GTP and PMIP [TEI14]",0,"revised","2016-07-27T09:34:55.817","2016-07-29T12:06:09.853","C4-164142","C4-164339","Rel-14","29.274","14.0.0","TEI14","1768","1","B",null,"","","","",""]
["C4-164237","MCPTT confidentiality protection FQDN","Ericsson","Maria-Cruz Bartolome",44824,"CR","","Agreement","","","61","7.2.11","Mission Critical Push To Talk over LTE protocol aspects (CT1) [MCPTT-CT]",0,"revised","2016-07-27T09:40:57.580","2016-07-27T10:13:34.557","","C4-164247","Rel-14","23.003","14.0.0","MCPTT-CT","0443","","A",null,"","","","",""]
["C4-164238","MT SMS handling for extended idle mode DRX – SMS over SGs","Nokia, Alcatel-Lucent Shanghai Bell","Bruno Landais",68755,"CR","","Approval","","","60","7.2.10","Extended DRX cycle for power consumption optimization (CT1) [eDRX]",0,"agreed","2016-07-27T10:15:04.287","2016-07-29T12:06:09.870","C4-164048","CP-160582","Rel-13","29.002","13.4.0","eDRX-CT","1217","1","F","CP-160426","","","","",""]
["C4-164239","MT SMS handling for extended idle mode DRX – SMS over SGs","Nokia, Alcatel-Lucent Shanghai Bell","Bruno Landais",68755,"CR","","Approval","","","60","7.2.10","Extended DRX cycle for power consumption optimization (CT1) [eDRX]",0,"agreed","2016-07-27T10:16:09.983","2016-07-29T12:06:09.870","C4-164049","CP-160583","Rel-14","29.002","14.0.0","eDRX-CT","1218","1","A","CP-160426","","","","",""]
["C4-164240","Current Location Retrieval","Nokia, Alcatel-Lucent Shanghai Bell","Ulrich Wiehe",6963,"CR","","Agreement","","","60","7.2.10","Extended DRX cycle for power consumption optimization (CT1) [eDRX]",0,"revised","2016-07-27T10:22:16.490","2016-07-29T12:06:09.870","C4-164165","C4-164296","Rel-13","29.272","13.6.0","TEI13, eDRX-CT","0657","1","F",null,"","","","",""]
["C4-164241","Current Location Retrieval","Nokia, Alcatel-Lucent Shanghai Bell","Ulrich Wiehe",6963,"CR","","Agreement","","","60","7.2.10","Extended DRX cycle for power consumption optimization (CT1) [eDRX]",0,"revised","2016-07-27T10:23:38.760",null,"C4-164166","C4-164297","Rel-14","29.272","14.0.0","TEI13, eDRX-CT","0658","1","A",null,"","","","",""]
["C4-164242","Notification of changes to RepositoryData for an Alias Public User Identity Set","Ericsson","Maria-Cruz Bartolome",44824,"CR","","Action","","","149","9.21","IMS [TEI11]",0,"agreed","2016-07-27T10:49:34.260","2016-07-29T12:06:09.870","C4-164041","","Rel-11","29.328","11.17.0","TEI11","0563","1","F","CP-160415","","","","",""]
["C4-164243","Notification of changes to RepositoryData for an Alias Public User Identity Set","Ericsson","Maria-Cruz Bartolome",44824,"CR","","Action","","","149","9.21","IMS [TEI11]",0,"agreed","2016-07-27T10:57:01.930","2016-07-29T12:06:09.887","C4-164074","","Rel-12","29.328","12.12.0","TEI11","0564","1","A","CP-160415","","","","",""]
["C4-164244","Notification of changes to RepositoryData for an Alias Public User Identity Set","Ericsson","Maria-Cruz Bartolome",44824,"CR","","Action","","","149","9.21","IMS [TEI11]",0,"agreed","2016-07-27T10:58:11.273","2016-07-29T12:06:09.887","C4-164075","","Rel-13","29.328","13.5.0","TEI11","0565","1","A","CP-160415","","","","",""]
["C4-164245","LS on the need to define a Domain Name for MCPTT confidentiality protection","Ericsson","Maria-Cruz Bartolome",44824,"LS out","","Approval","","","61","7.2.11","Mission Critical Push To Talk over LTE protocol aspects (CT1) [MCPTT-CT]",0,"approved","2016-07-27T11:38:30.863","2016-07-28T14:25:43.557","","","Rel-13","","","MCPTT-CT","","","","",null,"GSMA","CT1"]
["C4-164246","Domain Name for theMCPTT confidentiality protection","Ericsson","Ivo Sedlacek",41880,"CR","","Agreement","","","61","7.2.11","Mission Critical Push To Talk over LTE protocol aspects (CT1) [MCPTT-CT]",0,"agreed","2016-07-27T13:16:57.843","2016-07-29T12:06:09.887","C4-164235","","Rel-13","23.003","13.6.0","MCPTT-CT","0442","1","F","CP-160425","","","","",""]
["C4-164247","Domain Name for theMCPTT confidentiality protection","Ericsson","Ivo Sedlacek",41880,"CR","","Agreement","","","61","7.2.11","Mission Critical Push To Talk over LTE protocol aspects (CT1) [MCPTT-CT]",0,"agreed","2016-07-27T13:17:34.767","2016-07-29T12:06:09.887","C4-164237","","Rel-14","23.003","14.0.0","MCPTT-CT","0443","1","A","CP-160425","","","","",""]
["C4-164248","Update of definition of BSIC to include Radio frequency Colour Code","Ericsson","Jesus De Gregorio",40423,"CR","","Agreement","The Base Station Identification Code (BSIC) is extended with a 3 bit Radio frequency Colour Code (RCC) to help the MS distinguish between cells using the same BCCH ARFCN and the same BSIC (Network colour code (NCC) and BS colour code (BCC)) in tight frequency reuse networks.","","70","7.3.5","Addressing and Subscriber Data Handling [TEI13]",0,"agreed","2016-07-27T13:26:32.200","2016-07-29T12:06:09.887","","","Rel-13","23.003","13.6.0","CIoT_EC_GSM","0444","","B","CP-160417","","","","",""]
["C4-164249","3GPP TR 29.819 v1.3.0","ORANGE","Lionel Morand",25150,"draft TR","","Agreement","This version shall be sent for approval in CT#73.","","47","7.1.19","Feasibility Study on the Diameter Base Protocol Update [FS_DBPU]",0,"agreed","2016-07-27T13:42:18.647","2016-07-29T12:06:09.900","","","Rel-13","29.819","1.3.0","","","","","","","","","",""]
["C4-164250","New RAT Type for C-IoT","Ericsson","Jesus De Gregorio",40423,"CR","","Agreement","","","64","7.2.14","CIoT-CT (CT1)  [CIoT-CT]",0,"agreed","2016-07-27T13:42:57.770","2016-07-29T12:06:09.917","C4-164146","","Rel-13","29.002","13.4.0","CIoT-CT","1220","1","F","CP-160423","","","","",""]
["C4-164251","New RAT Type for C-IoT","Ericsson","Jesus De Gregorio",40423,"CR","","Agreement","","","64","7.2.14","CIoT-CT (CT1)  [CIoT-CT]",0,"agreed","2016-07-27T13:43:47.957","2016-07-29T12:06:09.917","C4-164147","","Rel-14","29.002","14.0.0","CIoT-CT","1221","1","A","CP-160423","","","","",""]
["C4-164252","Preferred Data Mode for an SGi PDN connection","Nokia, Alcatel-Lucent Shanghai Bell, Verizon","Bruno Landais",68755,"CR","","Approval","","","64","7.2.14","CIoT-CT (CT1)  [CIoT-CT]",0,"agreed","2016-07-27T14:28:10.670","2016-07-29T12:06:09.930","C4-164059","","Rel-13","29.272","13.6.0","CIoT-CT","0646","1","F","CP-160423","","","","",""]
["C4-164253","Preferred Data Mode for an SGi PDN connection","Nokia, Alcatel-Lucent Shanghai Bell, Verizon","Bruno Landais",68755,"CR","","Approval","","","64","7.2.14","CIoT-CT (CT1)  [CIoT-CT]",0,"agreed","2016-07-27T14:28:48.970","2016-07-29T12:06:09.930","C4-164060","","Rel-14","29.272","14.0.0","CIoT-CT","0647","1","A","CP-160423","","","","",""]
["C4-164254","Handling of Exception Reports in the Core Network","Huawei","Peter Schmitt",13753,"CR","","Approval","","","64","7.2.14","CIoT-CT (CT1)  [CIoT-CT]",0,"revised","2016-07-27T15:30:30.903","2016-07-29T12:06:09.930","C4-164036","C4-164330","Rel-13","29.128","13.1.0","CIoT-CT","0022","1","F",null,"","","","",""]
["C4-164255","Correction of  Reference for ePCO","Huawei","Peter Schmitt",13753,"CR","","Approval","correction of  an incorrect reference","","64","7.2.14","CIoT-CT (CT1)  [CIoT-CT]",0,"agreed","2016-07-27T15:41:03.620","2016-07-29T12:06:09.930","C4-164026","","Rel-13","29.128","13.1.0","CIoT-CT","0021","1","F","CP-160423","","","","",""]
["C4-164256","Allocate missing AVP and experimental result codes for  CIoT","Huawei","Peter Schmitt",13753,"CR","","Approval","","","64","7.2.14","CIoT-CT (CT1)  [CIoT-CT]",0,"withdrawn","2016-07-27T15:50:41.300",null,"C4-164027","","Rel-13","29.230","13.5.0","CIoT-CT","0566","1","F",null,"","","","",""]
["C4-164257","Allocation of AVP Codes","Huawei Tech.(UK) Co., Ltd","Peter Schmitt",13753,"CR","","Agreement","","","64","7.2.14","CIoT-CT (CT1)  [CIoT-CT]",0,"revised","2016-07-27T15:53:54.597","2016-07-29T12:06:09.947","","C4-164331","Rel-13","29.230","13.5.0","CIoT-CT","0573","","F",null,"","","","",""]
["C4-164258","AVP Codes","Huawei Tech.(UK) Co., Ltd","Peter Schmitt",13753,"CR","","Agreement","","","64","7.2.14","CIoT-CT (CT1)  [CIoT-CT]",0,"revised","2016-07-27T15:57:14.497","2016-07-29T12:06:09.947","","C4-164332","Rel-14","29.230","14.1.0","CIoT-CT","0574","","A",null,"","","","",""]
["C4-164259","Missing AVP codes and Experimental-Result codes for T6a","Nokia, Alcatel-Lucent Shanghai Bell, Verizon","Bruno Landais",68755,"CR","","Approval","","","64","7.2.14","CIoT-CT (CT1)  [CIoT-CT]",0,"agreed","2016-07-27T15:58:08.563","2016-07-29T12:06:09.947","C4-164069","","Rel-13","29.272","13.6.0","CIoT-CT","0569","1","F","CP-160423","","","","",""]
["C4-164260","Missing AVP codes and Experimental-Result codes for T6a","Nokia, Alcatel-Lucent Shanghai Bell, Verizon","Bruno Landais",68755,"CR","","Approval","","","64","7.2.14","CIoT-CT (CT1)  [CIoT-CT]",0,"agreed","2016-07-27T15:58:45.520","2016-07-29T12:06:09.947","C4-164070","","Rel-14","29.230","14.1.0","CIoT-CT","0570","1","A","CP-160424","","","","",""]
["C4-164261","Missing AVP codes and Experimental-Result codes for T6a","Nokia, Alcatel-Lucent Shanghai Bell","Bruno Landais",68755,"CR","","Approval","","","64","7.2.14","CIoT-CT (CT1)  [CIoT-CT]",0,"agreed","2016-07-27T16:06:57.917","2016-07-29T12:06:09.963","C4-164068","","Rel-13","29.128","13.1.0","CIoT-CT","0025","1","F","CP-160424","","","","",""]
["C4-164262","Sending of ePCO during the T6a connection release procedure","Nokia, Alcatel-Lucent Shanghai Bell","Bruno Landais",68755,"CR","","Approval","","","64","7.2.14","CIoT-CT (CT1)  [CIoT-CT]",0,"agreed","2016-07-27T16:24:05.543","2016-07-29T12:06:09.963","C4-164067","","Rel-13","29.128","13.1.0","CIoT-CT","0024","1","F","CP-160424","","","","",""]
["C4-164263","Addition of Serving PLMN ID and IMEISV to CMR","Nokia, ZTE, Alcatel-Lucent Shanghai Bell","Ulrich Wiehe",6963,"CR","","Agreement","","","64","7.2.14","CIoT-CT (CT1)  [CIoT-CT]",0,"revised","2016-07-27T16:42:04.433","2016-07-29T12:06:09.963","C4-164107","C4-164333","Rel-13","29.128","13.1.0","CIoT-CT","0030","1","F",null,"","","","",""]
["C4-164264","Pseudo-CR on Solution for PGW-U Failure with Restart – Solution #1","Cisco Systems","Sridhar Bhaskaran",58580,"discussion","","Approval","Stage 2 had identified that the TEID and GTPU address allocation after restoration of the U plane can follow solution #3 given in sub-clause 6.1.1.5.4 but has left the decision upto CT4 to discuss and decide. This is a PCR to the new CUPS TR adding a solution for PGW-U restoration with restart.","","25","6.3.8","CUPS",0,"revised","2016-07-27T18:07:14.447","2016-07-29T12:06:09.963","C4-164089","C4-164321","Rel-14","","","","","","","","","","","",""]
["C4-164265","Pseudo-CR on Solution for SGW-U Failure with Restart – Solution #1","Cisco Systems Belgium","Sridhar Bhaskaran",58580,"discussion","","Approval","Stage 2 had identified that the TEID and GTPU address allocation after restoration of the U plane can follow solution #3 given in sub-clause 6.1.1.5.4 but has left the decision upto CT4 to discuss and decide. This is a PCR to the new stage 3 CUPS TR adding a solution for SGW-U restoration with restart.","","25","6.3.8","CUPS",0,"revised","2016-07-27T18:10:33.920","2016-07-29T12:06:09.977","C4-164092","C4-164322","Rel-14","","","","","","","","","","","",""]
["C4-164266","Reply LS on Introduction of simulcast and pause-resume usage into MMCMH","Ericsson","Nevenka Biondic",41878,"LS out","","Approval","","","11","6.1.1","CT aspects of MTSI Extension on Multi-stream Multiparty Conferencing Media Handling [MMCMH-CT]",0,"revised","2016-07-28T07:05:13.213","2016-07-29T12:06:09.977","C4-164111","C4-164271","Rel-14","","","MMCMH_Enh-CT","","","","","C4-164029","3GPP SA WG4","3GPP CT WG1, 3GPP CT WG3","S4-160784"]
["C4-164267","Mandatory support of RTP/RTCP multiplexing","Ericsson, Nokia","Nevenka Biondic",41878,"CR","","Agreement","","","24","6.3.7","H.248 Interfaces [TEI14]",0,"agreed","2016-07-28T07:13:21.630","2016-07-29T12:06:09.977","C4-164114","","Rel-14","23.334","13.5.0","TEI14","0112","1","F","CP-160429","","","","",""]
["C4-164268","Mandatory support of RTP/RTCP multiplexing","Ericsson","Nevenka Biondic",41878,"CR","","Agreement","","","24","6.3.7","H.248 Interfaces [TEI14]",0,"agreed","2016-07-28T07:18:26.593","2016-07-29T12:06:09.977","C4-164115","","Rel-14","29.334","13.5.0","TEI14","0111","1","F","CP-160429","","","","",""]
["C4-164269","Transport of T.140 and BFCP within data channels","Nokia, Ericsson","Thomas Belling",68266,"CR","","Agreement","If T.140 is transported over the data channel, then draft-schwarz-mmusic-t140-usage-data-channel shall be used. As T.140 is transported via unreliable RTP/UDP in the IMS core network, some application aware correction of packet loss (as described in ITU-T H.248.94 Appendix II) is required in the eIMS-AGW.\nIf BFCP is transported over the data channel, then draft-schwarz-mmusic-bfcp-usage-data-channel shall be used.","","24","6.3.7","H.248 Interfaces [TEI14]",0,"agreed","2016-07-28T07:35:01.697","2016-07-29T12:06:09.977","C4-164150","","Rel-14","23.334","13.5.0","TEI14","0114","1","B","CP-160429","","","","",""]
["C4-164270","Transport of T.140 within data channels","Nokia, Ericsson","Thomas Belling",68266,"CR","","Agreement","If T.140 is transported over the data channel, then draft-schwarz-mmusic-t140-usage-data-channel shall be used. As T.140 is transported via unreliable RTP/UDP in the IMS core network, some application aware correction of packet loss (as described in ITU-T H.248.94 Appendix II) is required in the eIMS-AGW.","","22","6.3.5","IMS [TEI14]",0,"agreed","2016-07-28T07:38:17.130","2016-07-29T12:06:09.993","C4-164151","","Rel-14","29.334","13.5.0","TEI14","0112","1","B","CP-160431","","","","",""]
["C4-164271","Reply LS on Introduction of simulcast and pause-resume usage into MMCMH","CT4","Nevenka Biondic",41878,"LS out","","Approval","","","11","6.1.1","CT aspects of MTSI Extension on Multi-stream Multiparty Conferencing Media Handling [MMCMH-CT]",0,"approved","2016-07-28T08:01:58.530","2016-07-29T12:06:09.993","C4-164266","","Rel-14","","","MMCMH_Enh-CT","","","","","C4-164029","3GPP SA WG4","3GPP CT WG1, 3GPP CT WG3","S4-160784"]
["C4-164272","Update of definition of BSIC to include Radio frequency Colour Code","Ericsson","Jesus De Gregorio",40423,"CR","","Agreement","","","70","7.3.5","Addressing and Subscriber Data Handling [TEI13]",0,"agreed","2016-07-28T08:19:16.627","2016-07-29T12:06:09.993","","","Rel-14","23.003","14.0.0","CIoT_EC_GSM","0445","","A","CP-160417","","","","",""]
["C4-164273","Request to update data while a previous update request is in progress","Ericsson","Maria-Cruz Bartolome",44824,"CR","","Agreement","","","22","6.3.5","IMS [TEI14]",0,"agreed","2016-07-28T10:27:18.843","2016-07-29T12:06:09.993","C4-164134","","Rel-14","29.329","13.0.0","TEI14","0228","1","B","CP-160431","","","","",""]
["C4-164274","Pseudo-CR on Solution for PGW-U Failure without Restart – Solution#1","Cisco","Sridhar Bhaskaran",58580,"discussion","","Approval","Stage 2 had identified that the TEID and GTPU address allocation after restoration of the U plane can follow solution #3 given in sub-clause 6.1.1.5.4 but has left the decision upto CT4 to discuss and decide. This is a PCR to the new CUPS TR adding a solution for PGW-U restoration without restart.","","25","6.3.8","CUPS",0,"revised","2016-07-28T10:45:22.350","2016-07-29T12:06:10.010","C4-164090","C4-164320","Rel-14","","","","","","","","","","","",""]
["C4-164275","Pseudo-CR on Solution for PGW-U Faillure Without Restart – Solution #2","Cisco","Sridhar Bhaskaran",58580,"discussion","","Approval","Stage 2 had identified that the TEID and GTPU address allocation after restoration of the U plane can follow solution #3 given in sub-clause 6.1.1.5.4 but has left the decision upto CT4 to discuss and decide. This is a PCR to the new CUPS TR adding a solution for PGW-U restoration without restart.","","25","6.3.8","CUPS",0,"agreed","2016-07-28T11:02:30.993","2016-07-29T12:06:10.010","C4-164091","","Rel-14","","","","","","","","","","","",""]
["C4-164276","Pseudo-CR on Solution for SGW-U Failure without Restart – Solution#1","Cisco","Sridhar Bhaskaran",58580,"discussion","","Approval","Stage 2 had identified that the TEID and GTPU address allocation after restoration of the U plane can follow solution #3 given in sub-clause 6.1.1.5.4 but has left the decision upto CT4 to discuss and decide. This is a PCR to the new stage 3 CUPS TR adding a solution for SGW-U restoration without restart.","","25","6.3.8","CUPS",0,"revised","2016-07-28T11:08:34.407","2016-07-29T12:06:10.010","C4-164093","C4-164323","Rel-14","","","","","","","","","","","",""]
["C4-164277","Pseudo-CR on Solution for SGW-U Faillure Without Restart – Solution #2","Cisco Systems Inc","Sridhar Bhaskaran",58580,"discussion","","Approval","Stage 2 had identified that the TEID and GTPU address allocation after restoration of the U plane can follow solution #3 given in sub-clause 6.1.1.5.4 but has left the decision upto CT4 to discuss and decide. This is a PCR to the new stage 3 CUPS TR adding a solution for SGW-U restoration without restart","","25","6.3.8","CUPS",0,"agreed","2016-07-28T11:15:40.113","2016-07-29T12:06:10.010","C4-164094","","Rel-14","","","","","","","","","","","",""]
["C4-164278","Restoration procedures for CUPS","HuaWei","Youyang Yu",46021,"discussion","","Discussion","","","25","6.3.8","CUPS",0,"revised","2016-07-28T11:28:16.660","2016-07-29T12:06:10.027","C4-164108","C4-164325","","","","","","","","","","","","",""]
["C4-164279","TS Scope for CUPS","Huawei","Peter Schmitt",13753,"discussion","","Decision","","","25","6.3.8","CUPS",0,"agreed","2016-07-28T11:36:04.363","2016-07-29T12:06:10.027","C4-164137","","Rel-14","","","","","","","","","","","",""]
["C4-164280","Correction on ePCO","Ericsson","Yong Yang",42295,"CR","","Action","","","64","7.2.14","CIoT-CT (CT1)  [CIoT-CT]",0,"revised","2016-07-28T12:59:50.603","2016-07-29T12:06:10.027","C4-164076","C4-164327","Rel-13","29.274","13.6.0","","1754","1","F",null,"","","","",""]
["C4-164281","Correction on ePCO","Ericsson","Yong Yang",42295,"CR","","Action","","","64","7.2.14","CIoT-CT (CT1)  [CIoT-CT]",0,"revised","2016-07-28T13:01:05.420",null,"C4-164116","C4-164328","Rel-14","29.274","14.0.0","","1763","1","A",null,"","","","",""]
["C4-164282","SCEF Behavior of Rate Control Handling","ZTE","Zhijun Li",39295,"CR","","Approval","This contribution clarifies the SCEF behavior of handling downlink/uplink Non-IP data if Rate Control is activated.","","64","7.2.14","CIoT-CT (CT1)  [CIoT-CT]",0,"agreed","2016-07-28T13:15:29.157","2016-07-29T12:56:07.343","C4-164097","","Rel-13","29.128","13.1.0","CIoT-CT","0027","1","F","CP-160424","","","","",""]
["C4-164283","Not Able to Deliver MO Non-IP Data","ZTE","Zhijun Li",39295,"CR","","Approval","If the SCS/AS has requested the SCEF to delete NIDD configuration context, the SCEF is not able to continue forward MO Non-IP data to the SCS/AS. The SCEF shall stop the NIDD delivery procedure and may responds error cause to the MME.","","64","7.2.14","CIoT-CT (CT1)  [CIoT-CT]",0,"revised","2016-07-28T13:31:48.533","2016-07-29T12:56:07.343","C4-164098","C4-164334","Rel-13","29.128","13.1.0","CIoT-CT","0028","1","F",null,"","","","",""]
["C4-164284","T6a Connection Release after MO Data Answer with permanent error","Nokia,Alcatel-Lucent Shanghai Bell","Ulrich Wiehe",6963,"CR","","Agreement","","","64","7.2.14","CIoT-CT (CT1)  [CIoT-CT]",0,"agreed","2016-07-28T13:45:22.723","2016-07-29T12:56:07.360","C4-164106","","Rel-13","29.128","13.1.0","CIoT-CT","0029","1","F","CP-160424","","","","",""]
["C4-164285","3GPP TR 29.8de v001 Study on control and user plane separation of EPC nodes","FSCOM","Kimmo Kymalainen",19464,"other","","Endorsement","","","25","6.3.8","CUPS",0,"agreed","2016-07-28T14:19:37.833","2016-09-01T18:45:31.233","","","Rel-14","","","","","","","","","","","",""]
["C4-164286","3GPP TS 29.abc v001 Interface between the Control Plane and the User Plane of EPS Nodes","Huawei","Peter Schmitt",13753,"other","","Agreement","","","25","6.3.8","CUPS",0,"agreed","2016-07-28T14:20:56.003","2016-08-31T16:09:47.537","","","Rel-14","","","","","","","","","","","",""]
["C4-164287","Support of EAP Re-authentication Protocol for WLAN Interworking","ORANGE","Julien Bournelle",41373,"WID new","","Agreement","","","8","5","Work item management",0,"agreed","2016-07-28T14:27:46.047","2016-07-29T12:56:07.360","C4-164182","","Rel-14","","","","","","","","","","","",""]
["C4-164288","Reply LS to SA2 on Control Plane CIoT EPS Optimisation Indicator propagated to PGW for charging purpose","CT4","Bruno Landais",68755,"LS out","","Approval","","","64","7.2.14","CIoT-CT (CT1)  [CIoT-CT]",0,"approved","2016-07-28T15:34:30.790","2016-07-29T12:56:07.390","C4-164188","","","","","","","","","","C4-164158","SA2, SA5"]
["C4-164289","Reply LS on Retrieval of S1-U SGW F-TEID by MME","CT4","Peter Schmitt",13753,"LS out","","Approval","","","64","7.2.14","CIoT-CT (CT1)  [CIoT-CT]",0,"approved","2016-07-28T15:42:04.687","2016-07-29T12:56:07.407","C4-164190","","Rel-13","","","CIoT-CT","","","","","S2-164076","SA2"]
["C4-164290","Keep the S11-U SGW F-TEID the same as the S1-U SGW F-TEID","Huawei","Peter Schmitt",13753,"CR","","Agreement","","","64","7.2.14","CIoT-CT (CT1)  [CIoT-CT]",0,"revised","2016-07-28T15:49:43.307","2016-07-29T12:56:07.407","","C4-164308","Rel-13","29.274","13.6.0","CIoT-CT","1772","","F",null,"","","","",""]
["C4-164291","Solution to avoid high load resulting from shared subscription data update","Ericsson, Nokia, Alcatel-Lucent Shanghai Bell","Maria-Cruz Bartolome",44824,"CR","","Agreement","","","13","6.1.3","Shared Subscription Data Update [eSDU]",0,"agreed","2016-07-28T15:52:02.507","2016-07-29T12:56:07.407","C4-164204","","Rel-14","29.272","14.0.0","eSDU","0656","2","F","CP-160437","","","","",""]
["C4-164292","Keep the S11-U SGW F-TEID the same as the S1-U SGW F-TEID","Huawei","Peter Schmitt",13753,"CR","","Agreement","","","64","7.2.14","CIoT-CT (CT1)  [CIoT-CT]",0,"revised","2016-07-28T15:52:43.300","2016-07-29T12:56:07.420","","C4-164309","Rel-14","29.274","14.0.0","CIoT-CT","1773","","A",null,"","","","",""]
["C4-164293","STa and SWm extensions for IMEI check","Nokia, Alcatel-Lucent Shanghai Bell, Orange, Ericsson, ZTE","Bruno Landais",68755,"CR","","Approval","","","14","6.1.4","EIR check for WLAN access to EPC [EWE-CT]",0,"agreed","2016-07-28T16:05:38.707","2016-07-29T12:56:07.437","C4-164221","","Rel-14","29.273","13.4.0","EWE-CT","0462","2","B","CP-160436","","","","",""]
["C4-164294","Source SGSN behavior if Target does not support CIoT optimizations","ORANGE","Julien Bournelle",41373,"CR","","Agreement","","","16","6.2.1","CT aspects for Non-IP for Cellular Internet of Things for 2G/3G-GPRS [NonIP_GPRS-CT]",0,"agreed","2016-07-28T16:14:09.837","2016-07-29T12:56:07.453","C4-164216","","Rel-14","29.060","14.0.0","NonIP_GPRS-CT","1040","2","B","CP-160435","","","","",""]
["C4-164295","LS on the new Flag from PGW to SGSN","CT4","Youyang Yu",46021,"LS out","","Approval","","","56","7.2.6","IP Flow Mobility support for S2a and S2b Interfaces on stage 3 (CT1) [NBIFOM]",0,"approved","2016-07-28T17:14:06.597","2016-07-29T12:56:07.453","C4-164215","","","","","","","","","","C1-163142","CT1"]
["C4-164296","Current Location Retrieval","Nokia, Alcatel-Lucent Shanghai Bell","Ulrich Wiehe",6963,"CR","","Agreement","","","60","7.2.10","Extended DRX cycle for power consumption optimization (CT1) [eDRX]",0,"agreed","2016-07-28T17:18:52.437","2016-07-29T12:56:07.453","C4-164240","","Rel-13","29.272","13.6.0","TEI13, eDRX-CT","0657","2","F","CP-160426","","","","",""]
["C4-164297","Current Location Retrieval","Nokia, Alcatel-Lucent Shanghai Bell","Ulrich Wiehe",6963,"CR","","Agreement","","","60","7.2.10","Extended DRX cycle for power consumption optimization (CT1) [eDRX]",0,"agreed","2016-07-28T17:19:50.590","2016-07-29T12:56:07.453","C4-164241","","Rel-14","29.272","14.0.0","TEI13, eDRX-CT","0658","2","A","CP-160426","","","","",""]
["C4-164298","Extended DL Data Buffering for Extended Coverage","Nokia, Alcatel-Lucent Shanghai Bell","Bruno Landais",68755,"CR","","Approval","","","64","7.2.14","CIoT-CT (CT1)  [CIoT-CT]",0,"agreed","2016-07-28T17:28:23.967","2016-07-29T12:56:07.467","C4-164193","","Rel-13","29.274","13.6.0","CIoT-CT","1744","2","F","CP-160424","","","","",""]
["C4-164299","Extended DL Data Buffering for Extended Coverage","Nokia, Alcatel-Lucent Shanghai Bell","Bruno Landais",68755,"CR","","Approval","","","64","7.2.14","CIoT-CT (CT1)  [CIoT-CT]",0,"agreed","2016-07-28T17:28:53.810","2016-07-29T12:56:07.467","C4-164194","","Rel-14","29.274","14.0.0","CIoT-CT","1745","2","A","CP-160424","","","","",""]
["C4-164300","Handling of Exception Reports in the Core Network","Huawei, Vodafone","Peter Schmitt",13753,"CR","","Approval","","","64","7.2.14","CIoT-CT (CT1)  [CIoT-CT]",0,"revised","2016-07-28T17:50:14.080","2016-07-29T12:56:07.467","C4-164197","C4-164335","Rel-13","29.274","13.6.0","CIoT-CT","1743","6","F",null,"","","","",""]
["C4-164301","Handling of Exception Reports in the Core Network","Huawei, Vodafone","Peter Schmitt",13753,"CR","","Agreement","","","64","7.2.14","CIoT-CT (CT1)  [CIoT-CT]",0,"revised","2016-07-28T17:50:49.727","2016-07-29T12:56:07.483","C4-164198","C4-164336","Rel-14","29.274","14.0.0","CIoT-CT","1771","1","A",null,"","","","",""]
["C4-164302","AVP code for 29.214","Nokia, Alcatel-Lucent shanghai Bell Solutions & Networks (S)","Ulrich Wiehe",6963,"CR","","Agreement","","","67","7.3.2","Diameter 29.230 CRs [TEI13]",0,"revised","2016-07-29T06:51:29.037","2016-07-29T12:56:07.483","","C4-164318","Rel-13","29.230","13.5.0","TEI13","0575","","F",null,"","","","",""]
["C4-164303","AVP code for 29.214","Nokia, Alcatel-Lucent Shanghai Bell","Ulrich Wiehe",6963,"CR","","Agreement","","","67","7.3.2","Diameter 29.230 CRs [TEI13]",0,"revised","2016-07-29T06:54:07.923","2016-07-29T12:56:07.500","","C4-164319","Rel-14","29.230","14.1.0","TEI13","0576","","A",null,"","","","",""]
["C4-164304","AVP code for 29.212","Nokia, Alcatel-Lucent Shanghai Bell","Ulrich Wiehe",6963,"CR","","Agreement","","","67","7.3.2","Diameter 29.230 CRs [TEI13]",0,"revised","2016-07-29T06:56:54.810","2016-07-29T12:56:07.500","","C4-164316","Rel-13","29.230","13.5.0","TEI13","0577","","F",null,"","","","",""]
["C4-164305","AVP code for 29.212","Nokia, Alcatel-Lucent Shanghai Bell","Ulrich Wiehe",6963,"CR","","Agreement","","","67","7.3.2","Diameter 29.230 CRs [TEI13]",0,"revised","2016-07-29T07:00:14.850","2016-07-29T12:56:07.517","","C4-164317","Rel-14","29.230","14.1.0","TEI13","0578","","A",null,"","","","",""]
["C4-164306","LS on new AVPs in TS 29.212","CT3","Horst Brinkmann",70091,"LS in","","Action","CT3 would like to request CT4 to update TS 29.230 with the following new AVP used in TS 29.212 starting with Release 13","","67","7.3.2","Diameter 29.230 CRs [TEI13]",0,"noted","2016-07-29T07:19:06.653","2016-07-29T12:56:07.517","","","Rel-13","","","TEI13","","","","",null,"CT4",null,"C3-162199"]
["C4-164307","LS on new AVPs in TS 29.214","CT3","Fernandez alonso Susana",38588,"LS in","","Action","CT3 would like to request CT4 to update TS 29.230 with a new Diameter Code used in TS 29.214.","","67","7.3.2","Diameter 29.230 CRs [TEI13]",0,"noted","2016-07-29T07:22:32.213","2016-07-29T12:56:07.530","","","Rel-13","","","TEI13","","","","",null,"CT4",null,"C3-162255"]
["C4-164308","Keep the S11-U SGW F-TEID the same as the S1-U SGW F-TEID","Huawei","Peter Schmitt",13753,"CR","","Agreement","","","64","7.2.14","CIoT-CT (CT1)  [CIoT-CT]",0,"agreed","2016-07-29T07:44:20.513","2016-07-29T12:56:07.530","C4-164290","","Rel-13","29.274","13.6.0","CIoT-CT","1772","1","F","CP-160424","","","","",""]
["C4-164309","Keep the S11-U SGW F-TEID the same as the S1-U SGW F-TEID","Huawei","Kimmo Kymalainen",19464,"CR","","Agreement","","","64","7.2.14","CIoT-CT (CT1)  [CIoT-CT]",0,"agreed","2016-07-29T07:45:19.340","2016-07-29T12:56:07.530","C4-164292","","Rel-14","29.274","14.0.0","CIoT-CT","1773","1","A","CP-160424","","","","",""]
["C4-164310","Unaccepted PDN connection during an Intra-MME/SGSN handover","Nokia, Alcatel-Lucent Shanghai Bell","Bruno Landais",68755,"CR","","Approval","","","66","7.3.1","GTP and PMIP [TEI13]",0,"agreed","2016-07-29T07:49:41.853","2016-07-29T12:56:07.530","C4-164225","","Rel-13","29.274","13.6.0","TEI13","1752","2","F","CP-160421","","","","",""]
["C4-164311","Unaccepted PDN connection during an Intra-MME/SGSN handover","Nokia, Alcatel-Lucent Shanghai Bell","Bruno Landais",68755,"CR","","Approval","","","66","7.3.1","GTP and PMIP [TEI13]",0,"agreed","2016-07-29T07:50:18.047","2016-07-29T12:56:07.547","C4-164226","","Rel-14","29.274","14.0.0","TEI13","1753","2","A","CP-160421","","","","",""]
["C4-164312","Clarification on the release of unsuccessful EPC bearer context at mobility procedures when interworking with CIoT","Ericsson","Yong Yang",42295,"CR","","Agreement","","","64","7.2.14","CIoT-CT (CT1)  [CIoT-CT]",0,"agreed","2016-07-29T08:03:33.403","2016-07-29T12:56:07.547","C4-164202","","Rel-13","29.274","13.6.0","CIoT-CT","1755","2","F","CP-160424","","","","",""]
["C4-164313","Clarification on the release of unsuccessful EPC bearer context at mobility procedures when interworking with CIoT","Ericsson","Yong Yang",42295,"CR","","Agreement","","","64","7.2.14","CIoT-CT (CT1)  [CIoT-CT]",0,"agreed","2016-07-29T08:04:32.417","2016-07-29T12:56:07.547","C4-164203","","Rel-14","29.274","14.0.0","CIoT-CT","1764","2","A","CP-160424","","","","",""]
["C4-164314","Inclusion of Sender' F-TEID in the Command message","Ericsson","Yong Yang",42295,"CR","","Action","","","66","7.3.1","GTP and PMIP [TEI13]",0,"agreed","2016-07-29T08:05:26.407","2016-07-29T12:56:07.547","C4-164233","","Rel-13","29.274","13.6.0","TEI13","1758","2","F","CP-160421","","","","",""]
["C4-164315","Inclusion of Sender' F-TEID in the Command message","Ericsson","Yong Yang",42295,"CR","","Action","","","66","7.3.1","GTP and PMIP [TEI13]",0,"agreed","2016-07-29T08:06:15.157","2016-07-29T12:56:07.560","C4-164234","","Rel-14","29.274","14.0.0","TEI13","1766","2","A","CP-160421","","","","",""]
["C4-164316","AVP code for 29.212","Nokia, Alcatel-Lucent shanghai Bell","Ulrich Wiehe",6963,"CR","","Agreement","","","67","7.3.2","Diameter 29.230 CRs [TEI13]",0,"agreed","2016-07-29T08:15:01.620","2016-07-29T12:56:07.560","C4-164304","","Rel-13","29.230","13.5.0","TEI13","0577","1","F","CP-160419","","","","",""]
["C4-164317","AVP code for 29.212","Nokia, Alcatel-Lucent shanghai Bell","Ulrich Wiehe",6963,"CR","","Agreement","","","67","7.3.2","Diameter 29.230 CRs [TEI13]",0,"agreed","2016-07-29T08:15:30.497","2016-07-29T12:56:07.560","C4-164305","","Rel-14","29.230","14.1.0","TEI13","0578","1","A","CP-160419","","","","",""]
["C4-164318","AVP code for 29.214","Nokia, Alcatel-Lucent shanghai Bell","Ulrich Wiehe",6963,"CR","","Agreement","","","67","7.3.2","Diameter 29.230 CRs [TEI13]",0,"agreed","2016-07-29T08:20:11.310","2016-07-29T12:56:07.577","C4-164302","","Rel-13","29.230","13.5.0","TEI13","0575","1","F","CP-160419","","","","",""]
["C4-164319","AVP code for 29.214","Nokia, Alcatel-Lucent shanghai Bell","Ulrich Wiehe",6963,"CR","","Agreement","","","67","7.3.2","Diameter 29.230 CRs [TEI13]",0,"agreed","2016-07-29T08:21:01.307","2016-07-29T12:56:07.577","C4-164303","","Rel-14","29.230","14.1.0","TEI13","0576","1","A","CP-160419","","","","",""]
["C4-164320","Pseudo-CR on Solution for PGW-U Failure without Restart – Solution#1","Cisco","Sridhar Bhaskaran",58580,"discussion","","Approval","Stage 2 had identified that the TEID and GTPU address allocation after restoration of the U plane can follow solution #3 given in sub-clause 6.1.1.5.4 but has left the decision upto CT4 to discuss and decide. This is a PCR to the new CUPS TR adding a solution for PGW-U restoration without restart.","","25","6.3.8","CUPS",0,"agreed","2016-07-29T08:41:30.597","2016-07-29T12:56:07.577","C4-164274","","Rel-14","","","","","","","","","","","",""]
["C4-164321","Pseudo-CR on Solution for PGW-U Failure with Restart – Solution #1","Cisco","Sridhar Bhaskaran",58580,"discussion","","Approval","Stage 2 had identified that the TEID and GTPU address allocation after restoration of the U plane can follow solution #3 given in sub-clause 6.1.1.5.4 but has left the decision upto CT4 to discuss and decide. This is a PCR to the new CUPS TR adding a solution for PGW-U restoration with restart.","","25","6.3.8","CUPS",0,"agreed","2016-07-29T08:57:50.330","2016-07-29T12:56:07.593","C4-164264","","Rel-14","","","","","","","","","","","",""]
["C4-164322","Pseudo-CR on Solution for SGW-U Failure with Restart – Solution #1","Cisco","Sridhar Bhaskaran",58580,"discussion","","Approval","Stage 2 had identified that the TEID and GTPU address allocation after restoration of the U plane can follow solution #3 given in sub-clause 6.1.1.5.4 but has left the decision upto CT4 to discuss and decide. This is a PCR to the new stage 3 CUPS TR adding a solution for SGW-U restoration with restart.","","25","6.3.8","CUPS",0,"agreed","2016-07-29T08:59:14.507","2016-07-29T12:56:07.593","C4-164265","","Rel-14","","","","","","","","","","","",""]
["C4-164323","Pseudo-CR on Solution for SGW-U Failure without Restart – Solution#1","Cisco Systems Belgium","Sridhar Bhaskaran",58580,"discussion","","Approval","Stage 2 had identified that the TEID and GTPU address allocation after restoration of the U plane can follow solution #3 given in sub-clause 6.1.1.5.4 but has left the decision upto CT4 to discuss and decide. This is a PCR to the new stage 3 CUPS TR adding a solution for SGW-U restoration without restart.","","25","6.3.8","CUPS",0,"agreed","2016-07-29T09:03:04.357","2016-07-29T12:56:07.593","C4-164276","","","","","","","","","","","","","",""]
["C4-164324","Skeleton for TR Study on control and user plane separation of EPC nodes","Huawei","Peter Schmitt",13753,"other","","Decision","","","25","6.3.8","CUPS",0,"agreed","2016-07-29T09:15:21.547","2016-07-29T12:56:07.593","C4-164191","","","","","","","","","","","","","",""]
["C4-164325","Restoration procedures for CUPS","HuaWei","Youyang Yu",46021,"discussion","","Discussion","","","25","6.3.8","CUPS",0,"agreed","2016-07-29T09:21:49.187","2016-07-29T12:56:07.607","C4-164278","","","","","","","","","","","","","",""]
["C4-164326","TS Skeleton Interface between Control plane and User plane nodes in Packet System","Huawei","Peter Schmitt",13753,"discussion","","Decision","","","25","6.3.8","CUPS",0,"agreed","2016-07-29T09:29:32.333","2016-07-29T12:56:07.607","C4-164192","","Rel-14","","","","","","","","","","","",""]
["C4-164327","Correction on ePCO","Ericsson","Yong Yang",42295,"CR","","Action","","","64","7.2.14","CIoT-CT (CT1)  [CIoT-CT]",0,"revised","2016-07-29T10:07:58.217","2016-07-29T12:56:07.607","C4-164280","C4-164337","Rel-13","29.274","13.6.0","","1754","2","F",null,"","","","",""]
["C4-164328","Correction on ePCO","Ericsson","Yong Yang",42295,"CR","","Action","","","64","7.2.14","CIoT-CT (CT1)  [CIoT-CT]",0,"revised","2016-07-29T10:08:46.857","2016-07-29T12:56:07.607","C4-164281","C4-164338","Rel-14","29.274","14.0.0","","1763","2","A",null,"","","","",""]
["C4-164329","Reply LS on MT NIDD procedures at the T6a/T6b interface","CT4","Bruno Landais",68755,"LS out","","Approval","","","7","4","Input liaison statements: allocation to agenda items as appropriate",0,"approved","2016-07-29T10:20:25.407","2016-07-29T12:56:07.623","C4-164218","","Rel-13","","","","","","","","S2-164073","SA2"]
["C4-164330","Handling of Exception Reports in the Core Network","Huawei","Peter Schmitt",13753,"CR","","Approval","","","64","7.2.14","CIoT-CT (CT1)  [CIoT-CT]",0,"revised","2016-07-29T10:33:27.460","2016-07-29T12:56:07.623","C4-164254","C4-164340","Rel-13","29.128","13.1.0","CIoT-CT","0022","2","F",null,"","","","",""]
["C4-164331","Allocation of AVP Codes","Huawei","Peter Schmitt",13753,"CR","","Agreement","","","64","7.2.14","CIoT-CT (CT1)  [CIoT-CT]",0,"agreed","2016-07-29T10:54:22.393","2016-07-29T12:56:07.623","C4-164257","","Rel-13","29.230","13.5.0","CIoT-CT","0573","1","F","CP-160424","","","","",""]
["C4-164332","AVP Codes","Huawei","Peter Schmitt",13753,"CR","","Agreement","","","64","7.2.14","CIoT-CT (CT1)  [CIoT-CT]",0,"agreed","2016-07-29T10:55:20.473","2016-07-29T12:56:07.640","C4-164258","","Rel-14","29.230","14.1.0","CIoT-CT","0574","1","A","CP-160424","","","","",""]
["C4-164333","Addition of Serving PLMN ID and IMEISV to CMR","Nokia, ZTE, Alcatel-Lucent Shanghai Bell","Ulrich Wiehe",6963,"CR","","Agreement","","","64","7.2.14","CIoT-CT (CT1)  [CIoT-CT]",0,"agreed","2016-07-29T10:59:40.727","2016-07-29T12:56:07.640","C4-164263","","Rel-13","29.128","13.1.0","CIoT-CT","0030","2","F","CP-160424","","","","",""]
["C4-164334","Not Able to Deliver MO Non-IP Data","ZTE","Zhijun Li",39295,"CR","","Approval","If the SCS/AS has requested the SCEF to delete NIDD configuration context, the SCEF is not able to continue forward MO Non-IP data to the SCS/AS. The SCEF shall stop the NIDD delivery procedure and may responds error cause to the MME.","","64","7.2.14","CIoT-CT (CT1)  [CIoT-CT]",0,"agreed","2016-07-29T11:13:26.473","2016-07-29T12:56:07.640","C4-164283","CP-160573","Rel-13","29.128","13.1.0","CIoT-CT","0028","2","F","CP-160424","","","","",""]
["C4-164335","Handling of Exception Reports in the Core Network","Huawei, Vodafone","Peter Schmitt",13753,"CR","","Approval","","","64","7.2.14","CIoT-CT (CT1)  [CIoT-CT]",0,"agreed","2016-07-29T11:19:18.860","2016-07-29T12:56:07.640","C4-164300","","Rel-13","29.274","13.6.0","CIoT-CT","1743","7","F","CP-160424","","","","",""]
["C4-164336","Handling of Exception Reports in the Core Network","Huawei, Vodafone","Peter Schmitt",13753,"CR","","Agreement","","","64","7.2.14","CIoT-CT (CT1)  [CIoT-CT]",0,"agreed","2016-07-29T11:20:08.327","2016-07-29T12:56:07.657","C4-164301","","Rel-14","29.274","14.0.0","CIoT-CT","1771","2","A","CP-160424","","","","",""]
["C4-164337","Correction on ePCO","Ericsson","Yong Yang",42295,"CR","","Action","","","64","7.2.14","CIoT-CT (CT1)  [CIoT-CT]",0,"agreed","2016-07-29T11:32:54.220","2016-07-29T12:56:07.657","C4-164327","","Rel-13","29.274","13.6.0","CIoT-CT","1754","3","F","CP-160424","","","","",""]
["C4-164338","Correction on ePCO","Ericsson","Yong Yang",42295,"CR","","Action","","","64","7.2.14","CIoT-CT (CT1)  [CIoT-CT]",0,"agreed","2016-07-29T11:33:35.217","2016-07-29T12:56:07.657","C4-164328","","Rel-14","29.274","14.0.0","","1763","3","A","CP-160424","","","","",""]
["C4-164339","Adding supported feature for eNB change reporting","China Mobile","Zhenning Huang",60086,"CR","","Agreement","Adding supported feature for eNB change reporting","","18","6.3.1","GTP and PMIP [TEI14]",0,"agreed","2016-07-29T13:04:46.990","2016-07-29T13:42:31.207","C4-164236","","Rel-14","29.274","14.0.0","TEI14","1768","2","B","CP-160434","","","","",""]
["C4-164340","Handling of Exception Reports in the Core Network","Huawei Tech.(UK) Co., Ltd","Peter Schmitt",13753,"CR","","Approval","","","64","7.2.14","CIoT-CT (CT1)  [CIoT-CT]",0,"agreed","2016-07-29T13:12:42.507","2016-07-29T13:42:31.223","C4-164330","","Rel-13","29.128","13.1.0","CIoT-CT","0022","3","F","CP-160424","","","","",""]
["C4-164341","CT4 Aspect of the Workplan","CT4 Chairman","Nigel. H Berry",68268,"Work Plan","","Agreement","","","188","11","Update of the Work Plan",0,"agreed","2016-07-29T13:17:05.007","2016-07-29T13:42:31.223","C4-164006","","","","","","","","","","","","","",""]
["C4-164342","List of output documents","Nokia Networks","Nigel. H Berry",68268,"other","","Information","","","193","14","Check of approved output documents",0,"noted","2016-07-29T13:20:15.327","2016-08-03T15:33:28.650","","","","","","","","","","","","","","",""]

{"sheet":"CR_Packs_List","index":1,"n_rows":1,"n_cols":11,"rows_kept":1,"cut":false,"hidden":false,"merged":[]}
["CR Pack TDoc #","WG TDoc #","WG TDoc decision","CR Individual TSG decision","Spec #","CR #","CR revision #","CR category","Release","Version","CR title"]

{"sheet":"Parameters","index":2,"n_rows":24,"n_cols":4,"rows_kept":24,"cut":false,"hidden":true,"merged":[]}
["Types of Tdocs","Possible statuses of Tdocs","Categories"]
[]
["agenda","reserved","A","Decision"]
["Work Plan","available","B","Agreement"]
["LS in","revised","C","Approval"]
["LS out","agreed","D","Information"]
["pCR","conditionally agreed","E","Discussion"]
["draftCR","approved","F","Action"]
["CR","conditionally approved",null,"Endorsement"]
["CR pack","partially approved",null,"Presentation"]
["ToR","treated"]
["WID new","endorsed"]
["WID revised","replied to"]
["SID new","merged"]
["SID revised","not pursued"]
["WI status report","postponed"]
["WI exception request","noted"]
["TS or TR cover","not concluded"]
["draft TS","withdrawn"]
["draft TR","reissued"]
["report"]
["discussion"]
["response"]
["other"]