{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["TDoc_List","CR_Packs_List","Parameters"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":6,"comments":1,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"TDoc_List","index":0,"n_rows":118,"n_cols":32,"rows_kept":118,"cut":false,"hidden":false,"merged":[]}
["TDoc #","Title","Source","Contact","Contact ID","Type","Type supplement","For","Abstract","Secretary Remarks","Agenda item sort order","Agenda item #","Agenda item description","TDoc sort order within agenda item","TDoc Status","Reservation date","Uploaded","Is revision of","Revised to","Release","Spec #","Version","Related WIs","CR #","CR revision #","CR category","TSG CR Pack","Reply to","To","Cc","Original LS","Reply in"]
["C6-150201","Correction for FDN usage in case of IMS","QUALCOMM Incorporated","Michele Berionne",45196,"CR","","Decision","The existing text for FDN refers explcitly to CS bearer and this would imply that FDN is not applicable for IMS calls.","","51","7.7.3","IMS impacts on UICC Application Aspects (IMS_UApAs)",0,"revised","2015-05-14T19:48:50.193","2015-05-18T14:59:13.490","","C6-150274","Rel-12","31.102","12.7.0","","0625","","F",null,"","","","",""]
["C6-150202","Support for toolkit initiated GBA bootstrap using refresh on ISIM","QUALCOMM Incorporated","Michele Berionne",45196,"CR","","Decision","The current text allows the Toolkit-initiated GBA with refresh only on the USIM application. Anyway, there might be cases where the UICC does not contain the USIM at all or has GBABP file only in the ISIM.","","49","7.7.1","TEI 12 (TEI12)",0,"available","2015-05-14T19:52:39.543","2015-05-18T14:59:13.553","","","Rel-12","31.111","12.7.0","","0427","","F","CP-150388","","","","",""]
["C6-150203","Geographical Area in Direct Communication Radio Parameters","QUALCOMM Incorporated","Michele Berionne",45196,"CR","","Decision","Radio parameters to be used to perform ProSe direct communication when the UE is not served by E-UTRAN always have associated location where they can be used.","","50","7.7.2","CT6 part of CT aspects of Proximity-based Services (ProSe-CT)",0,"available","2015-05-14T19:54:56.683","2015-05-18T14:59:13.600","","","Rel-12","31.102","12.7.0","","0626","","F","CP-150382","","","","",""]
["C6-150204","Update of tags allocated by ETSI SCP","QUALCOMM Incorporated","Michele Berionne",45196,"CR","","Decision","Definition of tags, as specified by ETSI SCP in TS 101 220, and change in the name of tag and COMPREHENSION-TLV for the ProSe Report.","","49","7.7.1","TEI 12 (TEI12)",0,"revised","2015-05-14T19:58:07.113","2015-05-18T14:59:13.663","","C6-150271","Rel-12","31.111","12.7.0","","0428","","F",null,"","","","",""]
["C6-150205","Clarification of text for UE configuration parameters for SM Retry restriction","QUALCOMM Incorporated","Michele Berionne",45196,"CR","","Decision","Text approved in TS 24.368 for UE configuration parameters for SM Retry restriction (CP-150069) is slightly different than what is specified in TS 31.102.","","56","8","Other topics",0,"available","2015-05-14T20:02:26.290","2015-05-18T14:59:13.693","","","Rel-12","31.102","12.7.0","","0627","","F","CP-150383","","","","",""]
["C6-150206","Change of test case for UICC presence detection","QUALCOMM Incorporated","Michele Berionne",45196,"CR","","Decision","The UICC presence detection mechanism was modified in document C6-140109 to take into account the cases where the terminal has an active PDP context or EPS bearer context, but does not exchange data with the network. The corresponding test case needs to be updated accordingly, to reflect this.","","49","7.7.1","TEI 12 (TEI12)",0,"available","2015-05-14T20:04:51.790","2015-05-18T14:59:13.740","","","Rel-12","31.121","12.2.0","","0199","","F","CP-150388","","","","",""]
["C6-150207","CT aspects of enhancements to Proximity-based Services extensions","QUALCOMM Incorporated","Michele Berionne",45196,"WID new","","Decision","CT aspects of enhancements to Proximity-based Services extensions","","55","7.9","New Work Items / Study Items",0,"revised","2015-05-14T21:33:56.580","2015-05-18T14:59:13.787","","C6-150293","Rel-13","","","","","","","","","","","",""]
["C6-150208","Enhancements to Proximity-based Services (ProSe) extensions - Stage 2 status","QUALCOMM Incorporated","Michele Berionne",45196,"other","","Decision","The purpose of this contribution is to present the status of the stage 2 work on enhancements to Proximity-based Services extension (eProSe-Ext) after SA2#108, as supporting information for the discussion on the eProSe-Ext CT WID provided in C6-150207.","","58","8.2","Discussion documents",0,"available","2015-05-15T20:12:09.107","2015-05-18T14:59:13.817","","","Rel-13","","","","","","","","","","","",""]
["C6-150209","Removal of mandatory clause","BlackBerry UK Limited","Adrian Buckley",26735,"CR","","Decision","Removal of clause that makes all features mandatory","","54","7.8.2","Review of dedicated 3GPP UICC features (Red_UCe)",0,"revised","2015-05-17T18:51:25.197","2015-05-17T19:04:02.433","","C6-150295","Rel-13","31.111","12.7.0","Red_UCe","0429","","C",null,"","","","",""]
["C6-150210","Removal of mandatory clause","BlackBerry UK Limited","Adrian Buckley",26735,"CR","","Decision","","","54","7.8.2","Review of dedicated 3GPP UICC features (Red_UCe)",0,"revised","2015-05-17T18:54:43.723","2015-05-17T19:04:02.497","","C6-150296","Rel-13","31.124","12.3.0","Red_UCe","0419","","C",null,"","","","",""]
["C6-150211","Making features optional","BlackBerry UK Limited","Adrian Buckley",26735,"CR","","Decision","","","54","7.8.2","Review of dedicated 3GPP UICC features (Red_UCe)",0,"revised","2015-05-17T18:57:41.783","2015-05-17T19:04:02.543","","C6-150297","Rel-13","31.124","12.3.0","Red_UCe","0420","","C",null,"","","","",""]
["C6-150212","Correction of PDP context activation parameters","Intel","Vivek Gupta",36134,"CR","","Decision","","","33","7.5.1","TEI 10 (TEI10)",0,"available","2015-05-18T01:28:18.203","2015-05-18T01:36:25.920","","","Rel-10","31.111","10.15.0","","0430","","F","CP-150380","","","","",""]
["C6-150213","Correction of PDP context activation parameters","Intel","Vivek Gupta",36134,"CR","","Decision","","","33","7.5.1","TEI 10 (TEI10)",0,"available","2015-05-18T01:31:08.790","2015-05-18T01:36:25.967","","","Rel-11","31.111","11.11.0","","0431","","A","CP-150380","","","","",""]
["C6-150214","Correction of PDP context activation parameters","Intel","Vivek Gupta",36134,"CR","","Decision","","","33","7.5.1","TEI 10 (TEI10)",0,"available","2015-05-18T01:33:20.017","2015-05-18T01:36:25.997","","","Rel-12","31.111","12.7.0","","0432","","A","CP-150380","","","","",""]
["C6-150215","CT WG6#76 agenda with document allocation","LG Electronics France","Paul Jolivet",16261,"agenda","","Decision","","","4","3.1","Agreement of the agenda and the scheduling",0,"revised","2015-05-18T08:52:51.460","2015-05-18T09:16:13.750","","C6-150216","","","","","","","","","","","","",""]
["C6-150216","CT WG6#76 agenda with document allocation","LG Electronics France","Paul Jolivet",16261,"agenda","","Decision","","","4","3.1","Agreement of the agenda and the scheduling",0,"revised","2015-05-18T08:53:49.460","2015-05-21T13:09:10.503","C6-150215","C6-150317","","","","","","","","","","","","",""]
["C6-150217","Call for IPRs and Statement of anti-trust compliance ","MCC","Paul Jolivet",16261,"other","","Decision","","","5","3.2","IPR",0,"available","2015-05-18T08:55:07.913","2015-05-21T13:18:41.440","","","","","","","","","","","","","","",""]
["C6-150218","Draft meeting report of CT6#75","MCC","Paul Jolivet",16261,"report","","Decision","","","6","3.3","Report of previous CT6 meeting",0,"revised","2015-05-18T08:56:10.890","2015-05-24T18:58:39.773","","C6-150219","","","","","","","","","","","","",""]
["C6-150219","Approved meeting report of CT6#75","LG Electronics France","Paul Jolivet",16261,"report","","Decision","","","6","3.3","Report of previous CT6 meeting",0,"available","2015-05-18T08:57:12.993","2015-09-17T09:15:02.723","C6-150218","","","","","","","","","","","","","",""]
["C6-150220","Report from CT plenary #67","LG Electronics France","Paul Jolivet",16261,"report","","Decision","","","10","5.1","Report from TSG plenary meetings",0,"available","2015-05-18T08:57:57.017","2015-05-21T13:11:43.433","","","","","","","","","","","","","","",""]
["C6-150221","Action list after CT6#75 / before CT6#76","LG Electronics France","Paul Jolivet",16261,"other","","Decision","","","13","5.4","Review of action list",0,"revised","2015-05-18T08:58:51.677","2015-05-24T16:11:41.537","","C6-150222","","","","","","","","","","","","",""]
["C6-150222","Action list after CT6#76","LG Electronics France","Paul Jolivet",16261,"other","","Decision","","","13","5.4","Review of action list",0,"available","2015-05-18T08:59:34.187","2015-08-13T07:27:25.837","C6-150221","","","","","","","","","","","","","",""]
["C6-150223","Current status of WIs, specifications, rapporteurs before CT6#76","MCC","Paul Jolivet",16261,"other","","Decision","","","14","5.5","Status of CT6 specifications, rapporteurs & WIs",0,"revised","2015-05-18T08:59:59.927","2015-09-17T09:15:02.940","","C6-150224","","","","","","","","","","","","",""]
["C6-150224","Current status of WIs, specifications, rapporteurs after CT6#76","LG Electronics France","Paul Jolivet",16261,"other","","Decision","","","14","5.5","Status of CT6 specifications, rapporteurs & WIs",0,"available","2015-05-18T09:00:39.893","2015-09-17T09:15:03.113","C6-150223","","","","","","","","","","","","","",""]
["C6-150225","Status report of SCP activities after SCP #68","LG Electronics France","Paul Jolivet",16261,"report","","Decision","","","59","9","Report on ETSI TC SCP activity and review of approved ETSI TC SCP change requests",0,"available","2015-05-18T09:11:12.187","2015-05-19T14:55:31.400","","","","","","","","","","","","","","",""]
["C6-150226","Meeting schedule","LG Electronics France","Paul Jolivet",16261,"other","","Decision","","","60","10","Meeting plan",0,"revised","2015-05-18T09:12:01.357","2015-05-24T16:43:53.187","","C6-150227","","","","","","","","","","","","",""]
["C6-150227","Updated meeting schedule","LG Electronics France","Paul Jolivet",16261,"other","","Decision","","","60","10","Meeting plan",0,"available","2015-05-18T09:12:38.423","2015-09-17T09:15:03.287","C6-150226","","","","","","","","","","","","","",""]
["C6-150228","Correction of handling of Proof of Receipt","Morpho Cards GmbH","Heiko Kruse",12666,"CR","","Decision","Correction of the Proof of receipt handling","","49","7.7.1","TEI 12 (TEI12)",0,"available","2015-05-18T12:53:55.007","2015-05-18T12:56:15.080","","","Rel-12","31.115","12.1.0","","0026","","F","CP-150388","","","","",""]
["C6-150229","Contribution to TR 31.829 Development of conformance requirements for the IP Multimedia Services Identity Module (ISIM) application support in ME","Gemalto N.V.","Ly Thanh Phan",42268,"pCR","","Decision","Review of existing test scenario relative to ME-IMS interface and evaluationof the coverage of these tests to verify whether the contents of the ISIM are correctly read and used by the ME..","","27","7.3.3","Testing the interworking of ISIM Terminals with the IP Multimedia Subsystem (ISIM_IMS_Test)",0,"revised","2015-05-18T14:34:34.767","2015-05-18T14:49:07.807","","C6-150270","","","","","","",null,"","","","","",""]
["C6-150230","URI support by USAT clarification on the interactions with FDN_URI and BDN_URI","Gemalto N.V.","Ly Thanh Phan",42268,"CR","","Decision","CT6 has defined in TS 31.102 URI support by USIM (e.g. FDN_URI and BDN_URI). The interactions between CALL CONTROL commands and the support of URI for FDN and BDN services need be clarified.\n","","51","7.7.3","IMS impacts on UICC Application Aspects (IMS_UApAs)",0,"available","2015-05-18T14:54:56.760","2015-05-18T15:13:16.123","","C6-150273","Rel-12","31.111","12.7.0","","0433","","F",null,"","","","",""]
["C6-150231","URI support by USAT SMS related features","Gemalto N.V.","Ly Thanh Phan",42268,"CR","","Decision","3GPP stage 3 has worked on support of URI in Release 12. In particular, 3GPP TS 24.341 provide the specifications for the support of SMS Over IP networks without MSISDN (clauses 5.3.1.4, 5.3.2.6, 5.3.3.5 and B.7). According to this specification, the SMS over IP networks sender and receiver may use URIs to identify the sender and receiver of the SMS.\nThe USAT SMS related features need be aligned to TS 24.341 in order to support the new addressing mechanism based on URI.","","51","7.7.3","IMS impacts on UICC Application Aspects (IMS_UApAs)",0,"revised","2015-05-18T15:01:23.953","2015-05-18T15:13:16.170","","C6-150276","Rel-13","31.111","12.7.0","","0434","","B",null,"","","","",""]
["C6-150232","URI support for SMS indicator in UST","Gemalto N.V.","Ly Thanh Phan",42268,"CR","","Decision","USIM needs to indicate the ME when it support URI addressing in SMS features.","","51","7.7.3","IMS impacts on UICC Application Aspects (IMS_UApAs)",0,"revised","2015-05-18T15:06:16.377","2015-05-18T15:13:16.200","","C6-150290","Rel-13","31.102","12.7.0","","0628","","B",null,"","","","",""]
["C6-150233","URI support for SMS indicator in ISIM","Gemalto N.V.","Ly Thanh Phan",42268,"CR","","Decision","ISIM needs to indicate the ME when it support URI addressing in SMS features.","","51","7.7.3","IMS impacts on UICC Application Aspects (IMS_UApAs)",0,"revised","2015-05-18T15:09:32.827","2015-05-18T15:13:16.233","","C6-150291","Rel-13","31.103","12.2.0","","0094","","B",null,"","","","",""]
["C6-150234","Enhanced IMS Call Control","Gemalto N.V.","Ly Thanh Phan",42268,"CR","","Decision","SA1 requirements 3GPP TS 22.038 requires that UICC be able to control IMS communication session. However it was discussed in C6-150059 that the current CT6 TS 31.111 does not fulfill the SA1 requirement as a USAT application cannot:\n-\tDifferentiate the type of IMS communication (texting, voice, video)\n-\tSetup a conversational communication to a specified URI with a specified type of media\n-\tBe informed on the cause of a disconnection of an IMS communication","","53","7.8.1","TEI 13 (TEI13)",0,"revised","2015-05-18T15:19:44.713","2015-05-18T15:31:04.277","","C6-150301","Rel-13","31.111","12.7.0","","0435","","B",null,"","","","",""]
["C6-150235","Support of Enhanced IMS Call Control by USIM","Gemalto N.V.","Ly Thanh Phan",42268,"CR","","Decision","USAT enhanced IMS call control requires the USIM to indicate its support of the new Enhanced IMS Call Control feature","","53","7.8.1","TEI 13 (TEI13)",0,"revised","2015-05-18T15:24:25.277","2015-05-18T15:31:04.340","","C6-150302","Rel-13","31.102","12.7.0","","0629","","B",null,"","","","",""]
["C6-150236","Support of Enhanced IMS Call Control by ISIM","Gemalto N.V.","Ly Thanh Phan",42268,"CR","","Decision","USAT enhanced IMS call control requires the ISIM to indicate its support of the new Enhanced IMS Call Control feature","","53","7.8.1","TEI 13 (TEI13)",0,"revised","2015-05-18T15:27:00.480","2015-05-18T15:31:04.373","","C6-150303","Rel-13","31.103","12.2.0","","0095","","B",null,"","","","",""]
["C6-150237","Revised WID on CT aspects of Application specific Congestion control for Data Communication (ACDC)","LG Electronics Inc.","Jaehyun Kim",44912,"WID new","","Decision","","","55","7.9","New Work Items / Study Items",0,"available","2015-05-19T00:30:01.770","2015-05-19T00:35:17.153","","","Rel-13","","","ACDC","","","","","","","","",""]
["C6-150238","Alignement of Provide Local Information for Timing Advance to E-UTRAN radio technology","Gemalto N.V.","Ly Thanh Phan",42268,"CR","","Decision","Timing advance information is available in the ME when it is connected to GERAN or E-UTRAN. However, the Provide Local Information USAT specification restricted the availability of the information to GERAN as the information was not avaialble in UTRAN. It is proposed to align the availability of the information to the support of E-UTRAN technology.","","53","7.8.1","TEI 13 (TEI13)",0,"revised","2015-05-19T09:02:59.790",null,"","C6-150422","Rel-13","31.111","12.7.0","","0436","","B",null,"","","","",""]
["C6-150239","Home ePDG preferred indicator","Gemalto N.V.","Ly Thanh Phan",42268,"CR","","Decision","According to incoming LS on ePDG selection when UE is roaming from GSMA RILTE (C1-151283), in certain VoWiFi deployment scenarios it is preferred to have the UE to connect to the ePDG in home network even when UE is roaming.\nThis CR adds a new indicator “Home ePDG Preferred” indicator in EF_AD file for the MNO ti indicate the ME its preference.","","53","7.8.1","TEI 13 (TEI13)",0,"revised","2015-05-19T09:24:22.297","2015-05-19T09:29:45.923","","C6-150419","Rel-13","31.102","12.7.0","","0630","","B",null,"","","","",""]
["C6-150240","Correct file access conditions to activate/deactivate","LG Electronics France","Paul Jolivet",16261,"CR","","Decision","When the platform part of smart card applications was transferred to ETSI SCP, 3G commands INVALIDATE/REHABILITATE were not transferred and only  ACTIVATE/DEACTIVATE are used.  In some file descriptions, there is still the mention of INVALIDATE/REHABILITATE commands that are not specified.","","25","7.3.1","TEI 8 (TEI8)",0,"revised","2015-05-21T12:27:40.913","2015-05-21T12:55:09.153","","C6-150258","Rel-8","31.102","8.17.0","TEI8","0631","","F",null,"","","","",""]
["C6-150241","Correct file access conditions to activate/deactivate","LG Electronics France","Paul Jolivet",16261,"CR","","Decision","When the platform part of smart card applications was transferred to ETSI SCP, 3G commands INVALIDATE/REHABILITATE were not transferred and only  ACTIVATE/DEACTIVATE are used.  In some file descriptions, there is still the mention of INVALIDATE/REHABILITATE commands that are not specified.","","25","7.3.1","TEI 8 (TEI8)",0,"revised","2015-05-21T12:40:25.027","2015-05-21T12:55:09.183","","C6-150264","Rel-9","31.102","9.14.0","TEI8","0632","","A",null,"","","","",""]
["C6-150242","Correct file access conditions to activate/deactivate","LG Electronics France","Paul Jolivet",16261,"CR","","Decision","When the platform part of smart card applications was transferred to ETSI SCP, 3G commands INVALIDATE/REHABILITATE were not transferred and only  ACTIVATE/DEACTIVATE are used.  In some file descriptions, there is still the mention of INVALIDATE/REHABILITATE commands that are not specified.","","25","7.3.1","TEI 8 (TEI8)",0,"revised","2015-05-21T12:45:46.953","2015-05-21T12:55:09.247","","C6-150265","Rel-10","31.102","10.10.0","TEI8","0633","","A",null,"","","","",""]
["C6-150243","Correct file access conditions to activate/deactivate","LG Electronics France","Paul Jolivet",16261,"CR","","Decision","When the platform part of smart card applications was transferred to ETSI SCP, 3G commands INVALIDATE/REHABILITATE were not transferred and only  ACTIVATE/DEACTIVATE are used.  In some file descriptions, there is still the mention of INVALIDATE/REHABILITATE commands that are not specified.","","25","7.3.1","TEI 8 (TEI8)",0,"revised","2015-05-21T12:49:09.567","2015-05-21T12:55:09.277","","C6-150266","Rel-11","31.102","11.7.0","TEI8","0634","","A",null,"","","","",""]
["C6-150244","Correct file access conditions to activate/deactivate","LG Electronics France","Paul Jolivet",16261,"CR","","Decision","When the platform part of smart card applications was transferred to ETSI SCP, 3G commands INVALIDATE/REHABILITATE were not transferred and only  ACTIVATE/DEACTIVATE are used.  In some file descriptions, there is still the mention of INVALIDATE/REHABILITATE commands that are not specified.","","25","7.3.1","TEI 8 (TEI8)",0,"revised","2015-05-21T12:52:40.077","2015-05-21T12:55:09.293","","C6-150267","Rel-12","31.102","12.7.0","TEI8","0635","","A",null,"","","","",""]
["C6-150245","LS on Specific network availability","GSM Association","Xavier Piednoir",32337,"LS in","","Decision","","","17","6.2","Incoming liaison statements / inputs from other groups",0,"available","2015-05-23T08:31:00.127","2015-05-23T08:39:48.990","","","","","","","","","","",null,null,null,"",""]
["C6-150246","LS on I-WLAN specification maintenance","3GPP SA","Xavier Piednoir",32337,"LS in","","Decision","","","16","6.1","Incoming liaison statements / inputs from 3GPP groups",0,"available","2015-05-23T08:36:36.920","2015-05-23T08:39:49.020","","","","","","","","","","",null,null,null,"",""]
["C6-150247","LS on MAPN TR","3GPP SA1","Xavier Piednoir",32337,"LS in","","Decision","","","16","6.1","Incoming liaison statements / inputs from 3GPP groups",0,"available","2015-05-23T08:39:12.827","2015-05-23T08:39:49.037","","","","","","","","","","",null,null,null,"",""]
["C6-150248","Exception on the SIM Remote File Management","China Mobile","Xavier Piednoir",32337,"CR","","Decision","","","25","7.3.1","TEI 8 (TEI8)",0,"available","2015-05-23T13:42:06.577","2015-05-23T14:07:11.997","","","Rel-8","31.116","8.2.0","TEI8","0028","","F",null,"","","","",""]
["C6-150249","Exception on the SIM Remote File Management","China Mobile","Xavier Piednoir",32337,"CR","","Decision","","","25","7.3.1","TEI 8 (TEI8)",0,"available","2015-05-23T13:46:56.350","2015-05-23T14:07:12.057","","","Rel-9","31.116","9.4.0","TEI8","0029","","A",null,"","","","",""]
["C6-150250","Exception on the SIM Remote File Management","China Mobile","Xavier Piednoir",32337,"CR","","Decision","","","25","7.3.1","TEI 8 (TEI8)",0,"available","2015-05-23T13:48:31.027","2015-05-23T14:07:12.090","","","Rel-10","31.116","10.4.0","TEI8","0030","","A",null,"","","","",""]
["C6-150251","Exception on the SIM Remote File Management","China Mobile","Xavier Piednoir",32337,"CR","","Decision","","","25","7.3.1","TEI 8 (TEI8)",0,"available","2015-05-23T13:52:00.337","2015-05-23T14:07:12.137","","","Rel-11","31.116","11.1.0","TEI8","0031","","A",null,"","","","",""]
["C6-150252","Exception on the SIM Remote File Management","China Mobile","Xavier Piednoir",32337,"CR","","Decision","","","25","7.3.1","TEI 8 (TEI8)",0,"available","2015-05-23T13:54:20.457","2015-05-23T14:07:12.153","","","Rel-12","31.116","12.0.0","","0032","","A",null,"","","","",""]
["C6-150253","Specify the status condition returned  if search pattern can not be found in any of the records","China Mobile","Xavier Piednoir",32337,"CR","","Decision","","","25","7.3.1","TEI 8 (TEI8)",0,"revised","2015-05-23T13:59:51.477","2015-05-23T14:07:12.183","","C6-150448","Rel-8","31.122","8.0.1","TEI8","0052","","F",null,"","","","",""]
["C6-150254","Specify the status condition returned  if search pattern can not be found in any of the records","China Mobile","Xavier Piednoir",32337,"CR","","Decision","","","25","7.3.1","TEI 8 (TEI8)",0,"revised","2015-05-23T13:59:51.557","2015-05-23T14:07:12.230","","C6-150449","Rel-9","31.122","9.2.0","TEI8","0053","","A",null,"","","","",""]
["C6-150255","Specify the status condition returned  if search pattern can not be found in any of the records","China Mobile","Xavier Piednoir",32337,"CR","","Decision","","","25","7.3.1","TEI 8 (TEI8)",0,"revised","2015-05-23T13:59:51.633","2015-05-23T14:07:12.277","","C6-150450","Rel-10","31.122","10.0.0","TEI8","0054","","A",null,"","","","",""]
["C6-150256","Specify the status condition returned  if search pattern can not be found in any of the records","China Mobile","Xavier Piednoir",32337,"CR","","Decision","","","25","7.3.1","TEI 8 (TEI8)",0,"revised","2015-05-23T13:59:51.727","2015-05-23T14:07:12.307","","C6-150451","Rel-11","31.122","11.1.0","TEI8","0055","","A",null,"","","","",""]
["C6-150257","Specify the status condition returned  if search pattern can not be found in any of the records","China Mobile","Xavier Piednoir",32337,"CR","","Decision","","","25","7.3.1","TEI 8 (TEI8)",0,"revised","2015-05-23T13:59:51.790","2015-05-23T14:07:12.370","","C6-150452","Rel-12","31.122","12.0.0","TEI8","0056","","A",null,"","","","",""]
["C6-150258","Correct file access conditions to activate/deactivate","LG Electronics France","Xavier Piednoir",32337,"CR","","Decision","When the platform part of smart card applications was transferred to ETSI SCP, 3G commands INVALIDATE/REHABILITATE were not transferred and only  ACTIVATE/DEACTIVATE are used.  In some file descriptions, there is still the mention of INVALIDATE/REHABILITATE commands that are not specified.","","25","7.3.1","TEI 8 (TEI8)",0,"available","2015-05-25T04:24:23.627","2015-09-17T09:15:03.440","C6-150240","","Rel-8","31.102","8.17.0","TEI8","0631","1","F","CP-150379","","","","",""]
["C6-150259","Update of reference to ETSI TS 102 226","Morpho Cards GmbH","Heiko Kruse",12666,"CR","","Decision","ETSI SCP updated TS 102 226 to include corrections that are also required by 3GPP","","49","7.7.1","TEI 12 (TEI12)",0,"revised","2015-05-25T05:46:44.397","2015-05-25T05:53:14.980","","C6-150272","Rel-12","31.116","12.0.0","TEI12","0033","","F",null,"","","","",""]
["C6-150260","Discussion document on reference update for TS 102 221","QUALCOMM Incorporated","Michele Berionne",45196,"other","","Decision","Discussion document on reference update for TS 102 221","","57","8.1","Update of references to ETSI specifications",0,"available","2015-05-25T05:51:59.490","2015-09-17T09:15:03.613","","","Rel-12","31.101","12.1.0","","","","","","","","","",""]
["C6-150261","Update of reference to ETSI TS 102 221","QUALCOMM Incorporated","Michele Berionne",45196,"CR","","Decision","Update of reference to ESTI TS 102 221","","57","8.1","Update of references to ETSI specifications",0,"revised","2015-05-25T06:03:47.100","2015-09-17T09:15:03.817","","C6-150278","Rel-12","31.101","12.1.0","","0081","","F",null,"","","","",""]
["C6-150262","Discussion document on reference update for TS 102 223","QUALCOMM Incorporated","Michele Berionne",45196,"other","","Decision","Discussion document on reference update for TS 102 223","","57","8.1","Update of references to ETSI specifications",0,"available","2015-05-25T08:31:27.327","2015-09-17T09:15:03.987","","","Rel-12","","","","","","","","","","","",""]
["C6-150263","Update of reference to ETSI TS 102 223","QUALCOMM Incorporated","Michele Berionne",45196,"CR","","Decision","Update of reference to ESTI TS 102 223","","57","8.1","Update of references to ETSI specifications",0,"revised","2015-05-25T08:55:59.533","2015-09-17T09:15:04.267","","C6-150277","Rel-12","31.111","12.7.0","","0437","","F",null,"","","","",""]
["C6-150264","Correct file access conditions to activate/deactivate","LG Electronics France","Xavier Piednoir",32337,"CR","","Decision","When the platform part of smart card applications was transferred to ETSI SCP, 3G commands INVALIDATE/REHABILITATE were not transferred and only  ACTIVATE/DEACTIVATE are used.  In some file descriptions, there is still the mention of INVALIDATE/REHABILITATE commands that are not specified.","","25","7.3.1","TEI 8 (TEI8)",0,"available","2015-05-26T01:08:11.607","2015-09-17T09:15:04.440","C6-150241","","Rel-9","31.102","9.14.0","TEI8","0632","1","A","CP-150379","","","","",""]
["C6-150265","Correct file access conditions to activate/deactivate","LG Electronics France","Xavier Piednoir",32337,"CR","","Decision","When the platform part of smart card applications was transferred to ETSI SCP, 3G commands INVALIDATE/REHABILITATE were not transferred and only  ACTIVATE/DEACTIVATE are used.  In some file descriptions, there is still the mention of INVALIDATE/REHABILITATE commands that are not specified.","","25","7.3.1","TEI 8 (TEI8)",0,"available","2015-05-26T01:09:13.447","2015-09-17T09:15:04.597","C6-150242","","Rel-10","31.102","10.10.0","TEI8","0633","1","A","CP-150379","","","","",""]
["C6-150266","Correct file access conditions to activate/deactivate","LG Electronics France","Xavier Piednoir",32337,"CR","","Decision","When the platform part of smart card applications was transferred to ETSI SCP, 3G commands INVALIDATE/REHABILITATE were not transferred and only  ACTIVATE/DEACTIVATE are used.  In some file descriptions, there is still the mention of INVALIDATE/REHABILITATE commands that are not specified.","","25","7.3.1","TEI 8 (TEI8)",0,"available","2015-05-26T01:10:01.387","2015-09-17T09:15:04.767","C6-150243","","Rel-11","31.102","11.7.0","TEI8","0634","1","A","CP-150379","","","","",""]
["C6-150267","Correct file access conditions to activate/deactivate","LG Electronics France","Xavier Piednoir",32337,"CR","","Decision","When the platform part of smart card applications was transferred to ETSI SCP, 3G commands INVALIDATE/REHABILITATE were not transferred and only  ACTIVATE/DEACTIVATE are used.  In some file descriptions, there is still the mention of INVALIDATE/REHABILITATE commands that are not specified.","","25","7.3.1","TEI 8 (TEI8)",0,"available","2015-05-26T01:10:45.207","2015-09-17T09:15:04.970","C6-150244","","Rel-12","31.102","12.7.0","TEI8","0635","1","A","CP-150379","","","","",""]
["C6-150268","Discussion document on GSMA requirement in the LS in document C6-150245 on Specific network availability","Morpho Cards GmbH","Heiko Kruse",12666,"other","","Decision","In the LS The GSMA ESIM Subgroup asks 3GPP CT6 to evaluate the requirement to create a new mechanism to allow the UICC to request the ME to check the availability of a specific 3GPP network while connected to another 3GPP network. ","","17","6.2","Incoming liaison statements / inputs from other groups",0,"available","2015-05-26T01:34:28.163","2015-05-26T01:40:48.650","","","","","","","","","","","","","","",""]
["C6-150269","LS on SEARCH RECORD command","3GPP CT6","Xavier Piednoir",32337,"LS out","","Decision","","","18","6.3","Outgoing liaison statements",0,"available","2015-05-26T01:59:22.567","2015-09-17T09:15:05.140","","","","","","","","","","","","ETSI TC SCP TEC",""]
["C6-150270","Contribution to TR 31.829 Development of conformance requirements for the IP Multimedia Services Identity Module (ISIM) application support in ME","Gemalto N.V.","Xavier Piednoir",32337,"draft TS","","Decision","Review of existing test scenario relative to ME-IMS interface and evaluationof the coverage of these tests to verify whether the contents of the ISIM are correctly read and used by the ME..","","27","7.3.3","Testing the interworking of ISIM Terminals with the IP Multimedia Subsystem (ISIM_IMS_Test)",0,"revised","2015-05-26T03:12:05.990","2015-09-17T09:15:05.313","C6-150229","C6-150313","Rel-13","31.829","0.1.0","","","","","","","","","",""]
["C6-150271","Update of tags allocated by ETSI SCP","Qualcomm Incorporated","Xavier Piednoir",32337,"CR","","Decision","Definition of tags, as specified by ETSI SCP in TS 101 220, and change in the name of tag and COMPREHENSION-TLV for the ProSe Report.","","49","7.7.1","TEI 12 (TEI12)",0,"available","2015-05-26T03:44:59.213","2015-05-26T03:46:49.663","C6-150204","","Rel-12","31.111","12.7.0","TEI12","0428","1","F","CP-150388","","","","",""]
["C6-150272","Correction of handling of Proof of Receipt","Morpho Cards GmbH, Orange","Xavier Piednoir",32337,"CR","","Decision","Correction of the Proof of receipt handling","","49","7.7.1","TEI 12 (TEI12)",0,"available","2015-05-26T04:10:39.077","2015-05-26T08:40:53.467","C6-150259","","Rel-12","31.115","12.1.0","","0033","1","F","CP-150388","","","","",""]
["C6-150273","URI support by USAT clarification on the interactions with FDN_URI and BDN_URI","Gemato N.V.","Xavier Piednoir",32337,"CR","","Decision","CT6 has defined in TS 31.102 URI support by USIM (e.g. FDN_URI and BDN_URI). The interactions between CALL CONTROL commands and the support of URI for FDN and BDN services need be clarified.\n","","51","7.7.3","IMS impacts on UICC Application Aspects (IMS_UApAs)",0,"available","2015-05-26T06:51:04.283","2015-05-26T08:40:53.513","C6-150230","","Rel-12","31.111","12.7.0","","0433","1","F","CP-150388","","","","",""]
["C6-150274","URI support by USAT clarification on the interactions with FDN_URI and BDN_URI","Qualcomm Incorporated","Xavier Piednoir",32337,"CR","","Decision","CT6 has defined in TS 31.102 URI support by USIM (e.g. FDN_URI and BDN_URI). The interactions between CALL CONTROL commands and the support of URI for FDN and BDN services need be clarified.\n","","51","7.7.3","IMS impacts on UICC Application Aspects (IMS_UApAs)",0,"available","2015-05-26T07:01:16.953","2015-05-26T08:40:53.560","C6-150201","","Rel-12","31.111","12.7.0","","0625","1","F","CP-150384","","","","",""]
["C6-150275","Possible solution with Event for information about other available networks","Morpho Cards GmbH","Heiko Kruse",12666,"other","","Decision","A possible solution to solve the issue of the GSMA ESIM work group related to the incoming LS","","17","6.2","Incoming liaison statements / inputs from other groups",0,"available","2015-05-26T07:34:05.917","2015-09-17T09:15:05.483","","","","","","","","","","","","","","",""]
["C6-150276","URI support by USAT SMS related features","Gemalto N.V.","Xavier Piednoir",32337,"CR","","Decision","3GPP stage 3 has worked on support of URI in Release 12. In particular, 3GPP TS 24.341 provide the specifications for the support of SMS Over IP networks without MSISDN (clauses 5.3.1.4, 5.3.2.6, 5.3.3.5 and B.7). According to this specification, the SMS over IP networks sender and receiver may use URIs to identify the sender and receiver of the SMS.\nThe USAT SMS related features need be aligned to TS 24.341 in order to support the new addressing mechanism based on URI.","","51","7.7.3","IMS impacts on UICC Application Aspects (IMS_UApAs)",0,"revised","2015-05-26T07:36:55.973","2015-05-26T08:40:53.593","C6-150231","C6-150289","Rel-13","31.111","12.7.0","","0434","1","B",null,"","","","",""]
["C6-150277","Update of reference to ETSI TS 102 223","Qualcomm Incorporated","Xavier Piednoir",32337,"CR","","Decision","Update of reference to ESTI TS 102 223","","57","8.1","Update of references to ETSI specifications",0,"available","2015-05-26T08:26:34.257","2015-05-26T08:40:53.623","C6-150263","","Rel-12","31.111","12.7.0","","0437","1","F","CP-150388","","","","",""]
["C6-150278","Update of reference to ETSI TS 102 221","Qualcomm Incorporated","Xavier Piednoir",32337,"CR","","Decision","Update of reference to ESTI TS 102 221","","57","8.1","Update of references to ETSI specifications",0,"available","2015-05-26T08:38:38.887","2015-05-26T08:40:53.657","C6-150261","","Rel-12","31.101","12.1.0","","0081","1","F","CP-150388","","","","",""]
["C6-150279","Correction to information sent to the UICC when communication is established over WLAN","Gemalto","Xavier Piednoir",32337,"CR","","Decision","","","49","7.7.1","TEI 12 (TEI12)",0,"available","2015-05-26T08:44:00.700","2015-09-17T09:15:05.670","C6-150041","","Rel-12","31.111","12.7.0","TEI12","0422","1","F",null,"","","","",""]
["C6-150280","User Controlled and Operator Controlled WLAN for RAN Based WLAN Selection","Gemalto","Xavier Piednoir",32337,"CR","","Decision","","","49","7.7.1","TEI 12 (TEI12)",0,"available","2015-05-26T08:44:00.903","2015-09-17T09:15:05.907","C6-150042","","Rel-12","31.102","12.7.0","TEI12","0618","1","C",null,"","","","",""]
["C6-150281","Barred and authrorized ANID list storage in USIM","Gemalto","Xavier Piednoir",32337,"CR","","Decision","","","49","7.7.1","TEI 12 (TEI12)",0,"available","2015-05-26T08:44:01.090","2015-09-17T09:15:06.093","C6-150043","","Rel-12","31.102","12.7.0","TEI12","0619","1","B",null,"","","","",""]
["C6-150282","Offload Preference Indicator for RAN based WLAN interworking","Gemalto","Xavier Piednoir",32337,"CR","","Decision","","","49","7.7.1","TEI 12 (TEI12)",0,"available","2015-05-26T08:44:01.293","2015-09-17T09:15:06.280","C6-150044","","Rel-12","31.102","12.7.0","TEI12","0620","1","B",null,"","","","",""]
["C6-150283","Provide Local Information requests for network details","Gemalto","Xavier Piednoir",32337,"CR","","Decision","","","49","7.7.1","TEI 12 (TEI12)",0,"revised","2015-05-26T08:44:01.467","2015-08-17T16:37:34.967","C6-150046","C6-150460","Rel-12","31.111","12.7.0","TEI12","0423","1","C",null,"","","","",""]
["C6-150284","Test cases to cover Transaction Id for simultaneous calls","Gemalto","Xavier Piednoir",32337,"CR","","Decision","","","49","7.7.1","TEI 12 (TEI12)",0,"revised","2015-05-26T08:44:01.653","2015-09-17T09:15:06.450","C6-150086","C6-150306","Rel-12","31.124","12.3.0","TEI12","0418","2","B",null,"","","","",""]
["C6-150285","Missing rule for SMS_PP envelope response handling","OBERTHUR TECHNOLOGIES","Xavier Piednoir",32337,"CR","","Decision","","","25","7.3.1","TEI 8 (TEI8)",0,"revised","2015-05-26T08:44:01.840",null,"C6-150103","C6-150453","Rel-10","31.130","10.4.0","TEI8","0068","2","F",null,"","","","",""]
["C6-150286","Missing rule for SMS_PP envelope response handling","OBERTHUR TECHNOLOGIES","Xavier Piednoir",32337,"CR","","Decision","","","25","7.3.1","TEI 8 (TEI8)",0,"revised","2015-05-26T08:44:02.027",null,"C6-150104","C6-150454","Rel-11","31.130","11.0.0","TEI8","0069","2","A",null,"","","","",""]
["C6-150287","Missing rule for SMS_PP envelope response handling","OBERTHUR TECHNOLOGIES","Xavier Piednoir",32337,"CR","","Decision","","","25","7.3.1","TEI 8 (TEI8)",0,"revised","2015-05-26T08:44:02.213",null,"C6-150105","C6-150455","Rel-12","31.130","12.0.0","TEI8","0070","2","A",null,"","","","",""]
["C6-150288","WLAN Bearer alignment of USAT","Gemalto","Xavier Piednoir",32337,"CR","","Decision","","","49","7.7.1","TEI 12 (TEI12)",0,"revised","2015-05-26T08:44:02.400","2015-09-17T09:15:06.623","C6-150106","C6-150304","Rel-12","31.111","12.7.0","TEI12","0424","4","B",null,"","","","",""]
["C6-150289","URI support by USAT SMS related features","Gemalto N.V.","Xavier Piednoir",32337,"CR","","Decision","3GPP stage 3 has worked on support of URI in Release 12. In particular, 3GPP TS 24.341 provide the specifications for the support of SMS Over IP networks without MSISDN (clauses 5.3.1.4, 5.3.2.6, 5.3.3.5 and B.7). According to this specification, the SMS over IP networks sender and receiver may use URIs to identify the sender and receiver of the SMS.\nThe USAT SMS related features need be aligned to TS 24.341 in order to support the new addressing mechanism based on URI.","","51","7.7.3","IMS impacts on UICC Application Aspects (IMS_UApAs)",0,"available","2015-05-26T09:04:24.850","2015-06-02T09:36:33.893","C6-150276","","Rel-13","31.111","12.7.0","","0434","2","B","CP-150381","","","","",""]
["C6-150290","URI support for SMS indicator in UST","Gemalto N.V.","Xavier Piednoir",32337,"CR","","Decision","USIM needs to indicate the ME when it support URI addressing in SMS features.","","51","7.7.3","IMS impacts on UICC Application Aspects (IMS_UApAs)",0,"available","2015-05-26T09:21:18.613","2015-06-02T09:36:33.923","C6-150232","","Rel-13","31.102","12.7.0","","0628","1","B","CP-150381","","","","",""]
["C6-150291","URI support for SMS indicator in ISIM","Gemalto N.V.","Xavier Piednoir",32337,"CR","","Decision","ISIM needs to indicate the ME when it support URI addressing in SMS features.","","51","7.7.3","IMS impacts on UICC Application Aspects (IMS_UApAs)",0,"available","2015-05-26T09:23:00.437","2015-06-02T09:36:33.957","C6-150233","","Rel-13","31.103","12.2.0","","0094","1","B","CP-150381","","","","",""]
["C6-150292","Lack of reference in ENVELOPE (EVENT DOWNLOAD – MT Call) command parameters table","GIESECKE & DEVRIENT GmbH","Sergi Espi",59761,"CR","","Decision","","","49","7.7.1","TEI 12 (TEI12)",0,"available","2015-05-26T17:45:47.613","2015-09-17T09:15:06.810","","","Rel-12","31.111","12.7.0","TEI12","0626","","D",null,"","","","",""]
["C6-150293","CT aspects of enhancements to Proximity-based Services extensions","QUALCOMM Incorporated","Michele Berionne",45196,"WID new","","Decision","CT aspects of enhancements to Proximity-based Services extensions","","55","7.9","New Work Items / Study Items",0,"available","2015-05-27T00:39:14.083","2015-09-17T09:15:06.983","C6-150207","","Rel-13","","","","","","","","","","","",""]
["C6-150294","Replay LS on Specific network availability","QUALCOMM Incorporated","Michele Berionne",45196,"LS out","","Decision","Replay LS on Specific network availability","","18","6.3","Outgoing liaison statements",0,"available","2015-05-27T00:48:02.597","2015-08-19T16:47:03.040","","","","","","","","","","","C6-150245","GSM Association - ESIM Subgroup","3GPP SA1, 3GPP CT1"]
["C6-150295","Removal of mandatory clause","BlackBerry UK Limited","Xavier Piednoir",32337,"CR","","Decision","Removal of clause that makes all features mandatory","","54","7.8.2","Review of dedicated 3GPP UICC features (Red_UCe)",0,"revised","2015-05-27T01:20:50.180","2015-09-17T09:15:07.170","C6-150209","C6-150298","Rel-13","31.111","12.7.0","Red_UCe","0429","1","C",null,"","","","",""]
["C6-150296","Removal of mandatory clause","BlackBerry UK Limited","Xavier Piednoir",32337,"CR","","Decision","","","54","7.8.2","Review of dedicated 3GPP UICC features (Red_UCe)",0,"revised","2015-05-27T01:21:57.027","2015-09-17T09:15:07.340","C6-150210","C6-150299","Rel-13","31.124","12.3.0","Red_UCe","0419","1","C",null,"","","","",""]
["C6-150297","Making features optional","BlackBerry UK Limited","Xavier Piednoir",32337,"CR","","Decision","","","54","7.8.2","Review of dedicated 3GPP UICC features (Red_UCe)",0,"revised","2015-05-27T01:23:57.837","2015-09-17T09:15:07.543","C6-150211","C6-150300","Rel-13","31.124","12.3.0","Red_UCe","0420","1","C",null,"","","","",""]
["C6-150298","Removal of mandatory clause","BlackBerry UK Ltd","Xavier Piednoir",32337,"CR","","Decision","Removal of clause that makes all features mandatory","","54","7.8.2","Review of dedicated 3GPP UICC features (Red_UCe)",0,"revised","2015-05-27T03:16:04.113","2015-06-02T09:36:34.003","C6-150295","C6-150307","Rel-13","31.111","12.7.0","Red_UCe","0429","2","C",null,"","","","",""]
["C6-150299","Removal of mandatory clause","BlackBerry UK Ltd","Xavier Piednoir",32337,"CR","","Decision","","","54","7.8.2","Review of dedicated 3GPP UICC features (Red_UCe)",0,"revised","2015-05-27T03:23:29.483","2015-06-02T09:36:34.033","C6-150296","C6-150308","Rel-13","31.124","12.3.0","Red_UCe","0419","2","C",null,"","","","",""]
["C6-150300","Making features optional","BlackBerry UK Ltd.","Xavier Piednoir",32337,"CR","","Decision","","","54","7.8.2","Review of dedicated 3GPP UICC features (Red_UCe)",0,"revised","2015-05-27T03:53:40.387","2015-06-02T09:36:34.047","C6-150297","C6-150309","Rel-13","31.124","12.3.0","Red_UCe","0420","2","C",null,"","","","",""]
["C6-150301","Enhanced IMS Call Control","Gemalto N.V.","Xavier Piednoir",32337,"CR","","Decision","SA1 requirements 3GPP TS 22.038 requires that UICC be able to control IMS communication session. However it was discussed in C6-150059 that the current CT6 TS 31.111 does not fulfill the SA1 requirement as a USAT application cannot:\n-\tDifferentiate the type of IMS communication (texting, voice, video)\n-\tSetup a conversational communication to a specified URI with a specified type of media\n-\tBe informed on the cause of a disconnection of an IMS communication","","53","7.8.1","TEI 13 (TEI13)",0,"revised","2015-05-27T03:59:12.483","2015-06-02T09:36:34.080","C6-150234","C6-150310","Rel-13","31.111","12.7.0","","0435","1","B",null,"","","","",""]
["C6-150302","Support of Enhanced IMS Call Control by USIM","Gemalto N.V.","Xavier Piednoir",32337,"CR","","Decision","USAT enhanced IMS call control requires the USIM to indicate its support of the new Enhanced IMS Call Control feature","","53","7.8.1","TEI 13 (TEI13)",0,"revised","2015-05-27T04:10:19.767","2015-06-02T09:36:34.127","C6-150235","C6-150311","Rel-13","31.102","12.7.0","","0629","1","B","CP-150385","","","","",""]
["C6-150303","Support of Enhanced IMS Call Control by ISIM","Gemalto N.V.","Xavier Piednoir",32337,"CR","","Decision","USAT enhanced IMS call control requires the ISIM to indicate its support of the new Enhanced IMS Call Control feature","","53","7.8.1","TEI 13 (TEI13)",0,"revised","2015-05-27T04:24:45.687","2015-06-02T09:36:34.143","C6-150236","C6-150312","Rel-13","31.103","12.2.0","","0095","1","B",null,"","","","",""]
["C6-150304","WLAN Bearer alignment of USAT","Gemalto N.V","Xavier Piednoir",32337,"CR","","Decision","","","49","7.7.1","TEI 12 (TEI12)",0,"revised","2015-05-27T04:46:33.357","2015-06-02T09:36:34.190","C6-150288","C6-150315","Rel-12","31.111","12.7.0","TEI12","0424","5","B",null,"","","","",""]
["C6-150305","Technical proposal for Provide Local Information – Network Scan","Morpho Cards GmbH","Xavier Piednoir",32337,"other","","Decision","","","53","7.8.1","TEI 13 (TEI13)",0,"available","2015-05-27T07:10:13.543","2015-06-02T09:36:34.203","","","","","","","","","","","","","","",""]
["C6-150306","Test cases to cover Transaction Id for simultaneous calls","Gemalto N.V.","Xavier Piednoir",32337,"CR","","Decision","","","49","7.7.1","TEI 12 (TEI12)",0,"available","2015-05-27T08:53:12.393","2015-06-02T09:36:34.220","C6-150284","","Rel-12","31.124","12.3.0","TEI12","0418","3","B","CP-150388","","","","",""]
["C6-150307","Removal of mandatory clause","BlackBerry UK Ltd.","Xavier Piednoir",32337,"CR","","Decision","Removal of clause that makes all features mandatory","","54","7.8.2","Review of dedicated 3GPP UICC features (Red_UCe)",0,"available","2015-05-28T01:10:00.867","2015-06-02T09:36:34.250","C6-150298","","Rel-13","31.111","12.7.0","Red_UCe","0429","3","C","CP-150386","","","","",""]
["C6-150308","Removal of mandatory clause","BlackBerry UK Ltd.","Xavier Piednoir",32337,"CR","","Decision","","","54","7.8.2","Review of dedicated 3GPP UICC features (Red_UCe)",0,"available","2015-05-28T01:15:12.387","2015-06-02T09:36:34.283","C6-150299","","Rel-13","31.124","12.3.0","Red_UCe","0419","3","C","CP-150387","","","","",""]
["C6-150309","Making features optional","BlackBerry UK Ltd.","Xavier Piednoir",32337,"CR","","Decision","","","54","7.8.2","Review of dedicated 3GPP UICC features (Red_UCe)",0,"available","2015-05-28T01:20:53.970","2015-06-02T09:36:34.297","C6-150300","","Rel-13","31.124","12.3.0","Red_UCe","0420","3","C","CP-150386","","","","",""]
["C6-150310","Enhanced IMS Call Control","Gemalto N.V.","Xavier Piednoir",32337,"CR","","Decision","SA1 requirements 3GPP TS 22.038 requires that UICC be able to control IMS communication session. However it was discussed in C6-150059 that the current CT6 TS 31.111 does not fulfill the SA1 requirement as a USAT application cannot:\n-\tDifferentiate the type of IMS communication (texting, voice, video)\n-\tSetup a conversational communication to a specified URI with a specified type of media\n-\tBe informed on the cause of a disconnection of an IMS communication","","53","7.8.1","TEI 13 (TEI13)",0,"available","2015-06-01T08:45:00.127","2015-06-02T09:36:34.330","C6-150301","","Rel-13","31.111","12.7.0","","0435","2","B","CP-150385","","","","",""]
["C6-150311","Support of Enhanced IMS Call Control by USIM","Gemalto N.V.","Xavier Piednoir",32337,"CR","","Decision","USAT enhanced IMS call control requires the USIM to indicate its support of the new Enhanced IMS Call Control feature","","53","7.8.1","TEI 13 (TEI13)",0,"available","2015-06-02T07:39:36.080","2015-06-02T09:36:34.360","C6-150302","","Rel-13","31.102","12.7.0","","0629","2","B","CP-150394","","","","",""]
["C6-150312","Support of Enhanced IMS Call Control by ISIM","Gemalto N.V.","Xavier Piednoir",32337,"CR","","Decision","USAT enhanced IMS call control requires the ISIM to indicate its support of the new Enhanced IMS Call Control feature","","53","7.8.1","TEI 13 (TEI13)",0,"available","2015-06-02T07:40:54.347","2015-06-02T09:36:34.377","C6-150303","","Rel-13","31.103","12.2.0","","0095","2","B","CP-150385","","","","",""]
["C6-150313","TR 31.829 v0.2.0","CT6","Xavier Piednoir",32337,"draft TS","","Decision","Review of existing test scenario relative to ME-IMS interface and evaluationof the coverage of these tests to verify whether the contents of the ISIM are correctly read and used by the ME..","","27","7.3.3","Testing the interworking of ISIM Terminals with the IP Multimedia Subsystem (ISIM_IMS_Test)",0,"revised","2015-06-02T07:43:37.680","2015-06-02T09:36:34.423","C6-150270","C6-150314","Rel-13","31.829","0.2.0","FS_ISIM_CR","","","","","","","","",""]
["C6-150314","TR 31.829 v2.0.0","CT6","Xavier Piednoir",32337,"draft TS","","Decision","Review of existing test scenario relative to ME-IMS interface and evaluationof the coverage of these tests to verify whether the contents of the ISIM are correctly read and used by the ME..","","27","7.3.3","Testing the interworking of ISIM Terminals with the IP Multimedia Subsystem (ISIM_IMS_Test)",0,"available","2015-06-02T07:49:25.907","2015-09-17T09:15:07.717","C6-150313","","Rel-13","31.829","2.0.0","FS_ISIM_CR","","","","","","","","",""]
["C6-150315","WLAN Bearer alignment of USAT","Gemalto N.V.","Xavier Piednoir",32337,"CR","","Decision","","","49","7.7.1","TEI 12 (TEI12)",0,"available","2015-06-02T07:50:47.730","2015-06-02T09:36:34.453","C6-150304","","Rel-12","31.111","12.7.0","TEI12","0424","6","B","CP-150385","","","","",""]
["C6-150316","LS on COMPREHENSION TLV tags used by 3GPP","CT6","Xavier Piednoir",32337,"LS out","","Decision","","","18","6.3","Outgoing liaison statements",0,"available","2015-06-02T07:52:39.990","2015-06-02T09:36:34.500","","","Rel-13","","","","","","","","","ETSI TC SCP TEC","ETSI TC SCP"]
["C6-150317","CT WG6 #76 agenda with document allocation (final)","CT6 Chairman","Xavier Piednoir",32337,"agenda","","Decision","","","4","3.1","Agreement of the agenda and the scheduling",0,"available","2015-06-02T07:53:26.683","2015-06-02T09:36:34.547","C6-150216","","","","","","","","","","","","","",""]

{"sheet":"CR_Packs_List","index":1,"n_rows":1,"n_cols":11,"rows_kept":1,"cut":false,"hidden":false,"merged":[]}
["CR Pack TDoc #","WG TDoc #","WG TDoc decision","CR Individual TSG decision","Spec #","CR #","CR revision #","CR category","Release","Version","CR title"]

{"sheet":"Parameters","index":2,"n_rows":24,"n_cols":4,"rows_kept":24,"cut":false,"hidden":true,"merged":[]}
["Types of Tdocs","Possible statuses of Tdocs","Categories"]
[]
["agenda","reserved","A","Decision"]
["Work Plan","available","B","Agreement"]
["LS in","revised","C","Approval"]
["LS out","agreed","D","Information"]
["pCR","conditionally agreed","E","Discussion"]
["draftCR","approved","F","Action"]
["CR","conditionally approved",null,"Endorsement"]
["CR pack","partially approved",null,"Presentation"]
["ToR","treated"]
["WID new","endorsed"]
["WID revised","replied to"]
["SID new","merged"]
["SID revised","not pursued"]
["WI status report","postponed"]
["WI exception request","noted"]
["TS or TR cover","not concluded"]
["draft TS","withdrawn"]
["draft TR","reissued"]
["report"]
["discussion"]
["response"]
["other"]