**3GPP TSG-RAN WG2 Meeting #117-eR2-2nnnnn**

**Online, Feb 21th – March 3th 2022**

**Title:** [Draft] LS on logged MDT configuration at SN in DC scenario

**Response to:**

**Release:** Rel-17

**Work Item:** NR\_ENDC\_SON\_MDT\_enh-Core

**Source:** Ericsson [To be RAN2]

**To:** RAN3

**Cc:** SA5

**Contact Person:**

**Name:**  Ali Parichehreh

**E-mail Address:** ali.parichehreh@ericsson.com

**Send any reply LS to: 3GPP Liaisons Coordinator,**[**mailto:3GPPLiaison@etsi.org**](mailto:3GPPLiaison@etsi.org)

**Attachments:** -

**1. Overall description:**

RAN2 would like to kindly inform RAN3 that according to agreements captured in [1] and further discussions in RAN WG2 meeting #117-e, UE configuration of logged MDT at the SN is not supported for all DC scenarios, including EN-DC, NGEN-DC, NE-DC and NR-DC.

**2. Actions:**

RAN3 is respectfully asked to take the above into account in their discussions on logged MDT signaling in DC scenarios.

**3. Date of next TSG RAN WG2 meetings:**

RAN2#118-e 16 May - 25 May 2022 Online

**4. References:**

[1] R2-2104434: Report of [AT113b-e][804][NR/R17 SON/MDT] Logged MDT (CMCC), CMCC, 12th April – 20th April 2021.