**3GPP TSG-R3 Meeting #108-eR3-20XXXX**

**June 1st – 12th 2020, Online**

**Title:** [Draft] LS on Reply on QoE Measurement Collection

**Response to:** LS S5-202305, S5-202304 (LS on Reply on QoE Measurement Collection)

**Release:** Rel-16

**Work Item:** TEI16

**Source:** TBD (to be RAN3)

**To:** SA5

**Cc:** RAN2, SA4, CT1

**Contact Person:**

#### Name:

**Tel. Number:**

E-mail Address:

**Send any reply LS to: 3GPP Liaisons Coordinator, <mailto:3GPPLiaison@etsi.org>**

**Attachments:** R3-204118, R3-204119

**1. Overall Description:**

RAN3 thanks SA5 for the LS S5-202305 and S5-202304 on QoE Measurement Collection.

RAN3 would like to inform SA5, RAN3, SA4, CT1 that the following has been agreed at the RAN3#108-e meeting:

* add QMC ID in order to support QoE reference parameter (X2AP, RANAP)
* add Recording Session Indication (RANAP), since no streaming indication is currently specified
* add *withinArea* for propagation of QoE measurement collection at handover (X2AP, RANAP)
* add support for “QoE collection entity address” at handover in X2AP

Related contributions to Stage 3:

R3-204118 “CR TS 36.423 on QoE measurement collection support for X2AP”

R3-204119 “CR TS 25.413 on QoE measurement collection support for RANAP”

In addition, RAN3 would like SA5 provide confirmation that QMC ID, withinArea and QoE collection entity address can be supported in S1AP ( e.g. support S1 based Handover ).

**2. Actions:**

**To SA5**

**ACTION:** RAN3 informs SA5 that the requested changes from SA5 have been agreed at the RAN3#108-e meeting and provides response.

**3. Date of Next TSG-RAN WG3 Meetings:**

RAN3#109-e 17 – 28 August 2020 Online