**3GPP TSG-RAN WG3 Meeting #114-e R3-21xxxx**

**E-meeting, 1-11 Nov 2021**

**Title: Draft LS on the support of including slice ID in the QoE reporting container**

**Response to:**

**Release: Rel-17**

**Work Item: NR\_QoE**

Source: Huawei [to be RAN3]

**To: SA4**

**Cc: RAN2**

**Contact person:**

Name: Xudong Yang

Tel. Number: +86-21 3890808

E-mail Address: yangxudong@huawei.com

**Send any reply LS to: 3GPP Liaisons Coordinator,** **mailto:3GPPLiaison@etsi.org**

**Attachments:** **None**

# 1 Overall description

RAN3 thanks SA4 for the reply LS S4-211225 on the mapping between service types and slice at application, which mentions that “*SA4 is considering updates to its QoE report format to also include the S-NSSAI and DNN, whenever available.*”

Based on the above text in the LS S4-211225, RAN3 has made the following agreements in RAN3#114e meeting:

* RAN3 assumes that slice ID is included inside the transparent QoE reporting container, which is up to SA4’s decision.

With the agreements above, RAN3 would also like to ask SA4 the following questions:

**Question 1**: RAN3 would like to check with SA4 if the above agreements (especially the first bullet) is in line with SA4’s understanding; if not, please provide further feedback on SA4’s understanding.

Question 2: RAN3 would like to check with SA4 if there is any corresponding SA4 specification impact, and to provide the necessary specification support, if applicable.

# 2 Actions

**To SA4**

**ACTION:** RAN3 respectfully asks SA4 and RAN2 to take the above agreements into account and also asks SA4 to answer the raised questions.

# 3 Dates of next RAN3 meetings

3GPP TSG RAN3#115e 02/2022 E-Meeting