**3GPP TSG RAN3 meeting #117-bis-e R3-225992**

**E-meeting, 10th – 18th Oct. 2022**

**Title:** LS for the signaling based logged MDT override protection

**Release:** Rel-18

**Work Item:** NR\_ENDC\_SON\_MDT\_enh2-Core

**Source:** RAN3

**To:** RAN2

**Cc:**

**Contact Person:**

**Name: Jiaying Sun**

**E-mail Address:** **sunjiaying (at) catt (dot) cn**

**Send any reply LS to: 3GPP Liaisons Coordinator,** **mailto:3GPPLiaison@etsi.org**

**Attachments:** -

1. **Overall Description:**

The WI objective in Rel-18 for signalling based logged MDT override protection is as follows:

- Support of signalling based logged MDT override protection to address the scenario where the signalling based MDT is configured in E-UTRAN when [RAN2, RAN3]:

- UE reselects to NR while logged measurements are collected

- UE reselects to NR after logged measurements are collected and before uploading the logged MDT report.

Based on the WID description, RAN3 understands that signaling based logged MDT override protection applies only for inter-system inter-RAT scenarios.

RAN3 would like to ask RAN2 to provide feedback in case any different use cases are believed to be in scope of the WID.

**2. Actions:**

**To RAN2**

**ACTION:** RAN3 kindly asks RAN2 take the above information into consideration and feedback if needed.

**3. Date of Next TSG-RAN WG3 Meetings:**

TSG-RAN3 Meeting #118 14th Nov - 18th Nov 2022, France