**3GPP TSG-RAN WG3 #122 R3-237976**

**13th – 17th Nov 2023 Chicago, USA**

**Agenda item: 11.4**

**Source: CATT**

**Title: TP for 38.410 on Introduction of R18 QoE measurement**

**Document for: Approval**

# 1 Introduction

This TP is to specify support the objective in the WID on R18 QoE measurement:

Support the continuity of legacy QoE measurement job for streaming and MTSI service during intra-5GC inter-RAT handover process

# 2 TP for 38.410

**----------------------------Change Begins-------------------------------------------------------------------------**

6.25 The procedures for supporting QMC

The following procedures are used to control the QMC sessions in the UE and to transfer QMC session information to the target NG-RAN node during a UE’s intra-system intra-RAT or intra-system inter-RAT mobility:

- Initial Context Setup;

- UE Context Modification;

- Handover Preparation;

- Handover Resource Allocation.

**------------------------Change Ends----------------------------------------------------------------------------**