{"text_format":"1","workbook":"xlsx","n_sheets":6,"sheets":["Cover","Parameters","PUSCH requirement OCC feature","PDSCH requirement with RedCap","PUSCH requirement 4Rx","PUSCH requirement 8Rx"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Cover","index":0,"n_rows":7,"n_cols":10,"rows_kept":7,"cut":false,"hidden":false,"merged":[]}
[]
[null,"3GPP TSG-RAN WG4 Meeting #116bis",null,null,null,null,null,null,null,"R4-2515040"]
[null,"Prague, Czech, 13th-17th, Oct, 2025"]
[]
[null,"Source: Samsung"]
[null,"Title: Simulation results summary for NTN Phase 3 demodulation"]
[null,"Agenda: 6.23"]

{"sheet":"Parameters","index":1,"n_rows":12,"n_cols":5,"rows_kept":12,"cut":false,"hidden":false,"merged":[[1,2,1,4],[6,2,6,4],[7,2,7,4]]}
[]
[null,null,"Parameters for deriving performance requirements"]
[null,null,"Ideal Span Threshold",2,"dB"]
[null,null,"Impairment Span Threshold",4,"dB"]
[]
[]
[null,"Notes","1. Call function DerivingPerfReq()"]
[null,null,"2. If the ruls does not apply, or fails, -100dB or less will be returned"]
[null,null,null,-100,"Not enough input"]
[null,null,null,-101,"Input should be pairs"]
[null,null,null,-102,"Too large span for impairment"]
[null,null,null,-103,"After removal iteration, not enough input"]

{"sheet":"PUSCH requirement OCC feature","index":2,"n_rows":69,"n_cols":31,"rows_kept":69,"cut":false,"hidden":false,"merged":[[31,13,32,13],[33,3,34,3],[33,4,34,4],[33,5,34,5],[33,6,34,6],[33,7,34,7],[33,8,34,8],[33,9,34,9],[33,10,34,10],[33,11,34,11],[33,12,34,12],[33,13,34,13],[31,3,32,3],[31,4,32,4],[31,5,32,5],[31,6,32,6],[31,8,32,8],[31,9,32,9],[31,10,32,10],[31,11,32,11],[31,12,32,12],[31,7,32,7],[27,13,28,13],[29,3,30,3],[29,4,30,4],[29,5,30,5],[29,6,30,6],[29,7,30,7],[29,8,30,8],[29,9,30,9],[29,10,30,10],[29,11,30,11],[29,12,30,12],[29,13,30,13],[27,3,28,3],[27,4,28,4],[27,5,28,5],[27,6,28,6],[27,8,28,8],[27,9,28,9],[27,10,28,10],[27,11,28,11],[27,12,28,12],[27,7,28,7],[23,13,24,13],[25,3,26,3],[25,4,26,4],[25,5,26,5],[25,6,26,6],[25,7,26,7],[25,8,26,8],[25,9,26,9],[25,10,26,10],[25,11,26,11],[25,12,26,12],[25,13,26,13],[23,3,24,3],[23,4,24,4],[23,5,24,5],[23,6,24,6],[23,8,24,8],[23,9,24,9],[23,10,24,10],[23,11,24,11],[23,12,24,12],[23,7,24,7],[14,7,15,7],[19,13,20,13],[21,3,22,3],[21,4,22,4],[21,5,22,5],[21,6,22,6],[21,7,22,7],[21,8,22,8],[21,9,22,9],[21,10,22,10],[21,11,22,11],[21,12,22,12],[21,13,22,13],[19,3,20,3],[19,4,20,4],[19,5,20,5],[19,6,20,6],[19,8,20,8],[19,9,20,9],[19,10,20,10],[19,11,20,11],[19,12,20,12],[19,7,20,7],[10,5,11,5],[10,6,11,6],[10,7,11,7],[14,13,15,13],[16,3,17,3],[16,4,17,4],[16,5,17,5],[16,6,17,6],[16,7,17,7],[16,8,17,8],[16,9,17,9],[16,10,17,10],[16,11,17,11],[16,12,17,12],[16,13,17,13],[14,8,15,8],[14,9,15,9],[14,10,15,10],[14,11,15,11],[14,12,15,12],[14,3,15,3],[14,4,15,4],[14,5,15,5],[14,6,15,6],[6,3,7,3],[6,4,7,4],[6,5,7,5],[6,6,7,6],[6,7,7,7],[10,13,11,13],[12,3,13,3],[12,4,13,4],[12,5,13,5],[12,6,13,6],[12,7,13,7],[12,8,13,8],[12,9,13,9],[12,10,13,10],[12,11,13,11],[12,12,13,12],[12,13,13,13],[10,8,11,8],[10,9,11,9],[10,10,11,10],[10,11,11,11],[10,12,11,12],[10,3,11,3],[10,4,11,4],[2,4,3,4],[2,3,3,3],[2,6,3,6],[2,8,3,8],[2,5,3,5],[2,12,3,12],[2,13,3,13],[6,13,7,13],[8,3,9,3],[8,4,9,4],[8,5,9,5],[8,6,9,6],[8,7,9,7],[8,8,9,8],[8,9,9,9],[8,10,9,10],[8,11,9,11],[8,12,9,12],[8,13,9,13],[6,8,7,8],[6,9,7,9],[6,10,7,10],[6,11,7,11],[6,12,7,12],[36,3,37,3],[36,4,37,4],[36,5,37,5],[36,6,37,6],[36,7,37,7],[36,8,37,8],[36,9,37,9],[36,10,37,10],[36,11,37,11],[38,3,39,3],[38,4,39,4],[38,5,39,5],[38,6,39,6],[38,7,39,7],[38,8,39,8],[38,9,39,9],[38,10,39,10],[38,11,39,11],[40,3,41,3],[40,4,41,4],[40,5,41,5],[40,6,41,6],[40,7,41,7],[40,8,41,8],[40,9,41,9],[40,10,41,10],[40,11,41,11],[42,3,43,3],[42,4,43,4],[42,5,43,5],[42,6,43,6],[42,7,43,7],[42,8,43,8],[42,9,43,9],[42,10,43,10],[42,11,43,11],[44,3,45,3],[44,4,45,4],[44,5,45,5],[44,6,45,6],[44,7,45,7],[44,8,45,8],[44,9,45,9],[44,10,45,10],[44,11,45,11],[46,3,47,3],[46,4,47,4],[46,5,47,5],[46,6,47,6],[46,7,47,7],[46,8,47,8],[46,9,47,9],[46,10,47,10],[46,11,47,11],[48,3,49,3],[48,4,49,4],[48,5,49,5],[48,6,49,6],[48,7,49,7],[48,8,49,8],[48,9,49,9],[48,10,49,10],[48,11,49,11],[50,3,51,3],[50,4,51,4],[50,5,51,5],[50,6,51,6],[50,7,51,7],[50,8,51,8],[50,9,51,9],[50,10,51,10],[50,11,51,11],[53,3,54,3],[53,4,54,4],[53,5,54,5],[53,6,54,6],[53,7,54,7],[53,8,54,8],[53,9,54,9],[53,10,54,10],[53,11,54,11],[55,3,56,3],[55,4,56,4],[55,5,56,5],[55,6,56,6],[55,7,56,7],[55,8,56,8],[55,9,56,9],[55,10,56,10],[55,11,56,11],[57,3,58,3],[57,4,58,4],[57,5,58,5],[57,6,58,6],[57,7,58,7],[57,8,58,8],[57,9,58,9],[57,10,58,10],[57,11,58,11],[59,3,60,3],[59,4,60,4],[59,5,60,5],[59,6,60,6],[59,7,60,7],[59,8,60,8],[59,9,60,9],[59,10,60,10],[59,11,60,11],[61,3,62,3],[61,4,62,4],[61,5,62,5],[61,6,62,6],[61,7,62,7],[61,8,62,8],[61,9,62,9],[61,10,62,10],[61,11,62,11],[63,3,64,3],[63,4,64,4],[63,5,64,5],[63,6,64,6],[63,7,64,7],[63,8,64,8],[63,9,64,9],[63,10,64,10],[63,11,64,11],[65,3,66,3],[65,4,66,4],[65,5,66,5],[65,6,66,6],[65,7,66,7],[65,8,66,8],[65,9,66,9],[65,10,66,10],[65,11,66,11],[67,3,68,3],[67,4,68,4],[67,5,68,5],[67,6,68,6],[67,7,68,7],[67,8,68,8],[67,9,68,9],[67,10,68,10],[67,11,68,11],[0,25,0,26],[0,23,0,24],[0,21,0,22],[0,19,0,20],[0,17,0,18],[2,2,3,2],[4,2,5,2],[6,2,7,2],[8,2,9,2],[4,12,5,12],[4,13,5,13],[2,10,3,10],[2,11,3,11],[4,3,5,3],[4,4,5,4],[4,5,5,5],[4,6,5,6],[4,7,5,7],[4,8,5,8],[4,9,5,9],[4,10,5,10],[4,11,5,11],[2,9,3,9],[2,7,3,7],[10,2,11,2],[12,2,13,2],[14,2,15,2],[16,2,17,2],[19,2,20,2],[21,2,22,2],[23,2,24,2],[25,2,26,2],[27,2,28,2],[48,2,49,2],[50,2,51,2],[29,2,30,2],[31,2,32,2],[33,2,34,2],[36,2,37,2],[38,2,39,2],[40,2,41,2],[42,2,43,2],[44,2,45,2],[46,2,47,2]]}
[null,null,"Case","Tx","Rx","SCS","BW","Mapping type ","DMRS","Channel Model","MCS","FO (HZ)","No. of Rep","OCC length","OCC index","38.104 req","38.141-1/2 req","Samsung",null,"Ericsson",null,"Huawei",null,"CATT",null,"ZTE",null,"SPAN","SPAN","AVERAGE","AVERAGE"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ideal","Impairment","ideal","Impairment","ideal","Impairment","ideal","Impairment","ideal","Impairment","ideal","Impairment","ideal","Impairment"]
[null,null,1,1,1,"15khZ","5MHz","A","(2,11)","NTN-TDLC5-200 Low","MCS 5 (99/1024)",0,2,2,0,null,null,-7.36,null,-8.27,null,-2.7,null,null,null,null,null,{"$f":"MAX(R3:Z3)-MIN(R3:Z3)","v":5.5699999999999994},null,{"$f":"AVERAGE(R3:Z3)","v":-6.1099999999999994}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,-7.28,null,-8.27,null,-2.7,null,null,null,null,null,{"$f":"MAX(R4:Z4)-MIN(R4:Z4)","v":5.5699999999999994},null,{"$f":"AVERAGE(R4:Z4)","v":-6.083333333333333}]
[null,null,2,1,1,"15khZ","5MHz","A","(2,11)","NTN-TDLC5-200 Low","MCS 5 (99/1024)",200,2,2,0,null,null,-7.14,null,-8.26,null,-2.7,null,null,null,null,null,5.56,null,-6.0333333333333323]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,-7.09,null,-8.26,null,-2.7,null,null,null,null,null,5.56,null,-6.0166666666666666]
[null,null,3,1,2,"15khZ","5MHz","A","(2,11)","NTN-TDLC5-200 Low","MCS 5 (99/1024)",0,2,2,0,null,null,-10.59,null,-11.4,null,-5.7,null,null,null,null,null,5.7,null,-9.23]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,-10.55,null,-11.4,null,-5.7,null,null,null,null,null,5.7,null,-9.2166666666666668]
[null,null,4,1,2,"15khZ","5MHz","A","(2,11)","NTN-TDLC5-200 Low","MCS 5 (99/1024)",200,2,2,0,null,null,-10.4,null,-11.4,null,-5.7,null,null,null,null,null,5.7,null,-9.1666666666666661]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,-10.32,null,-11.4,null,-5.7,null,null,null,null,null,5.7,null,-9.1399999999999988]
[null,null,5,1,1,"15khZ","5MHz","A","(2,11)","NTN-TDLA100-200 Low","MCS 5 (99/1024)",0,2,2,0,null,null,1.7,null,-6.21,null,-2.1,null,null,null,null,null,7.91,null,-2.2033333333333331]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,1.85,null,-6.21,null,-2.1,null,null,null,null,null,8.06,null,-2.1533333333333329]
[null,null,6,1,1,"15khZ","5MHz","A","(2,11)","NTN-TDLA100-200 Low","MCS 5 (99/1024)",200,2,2,0,null,null,1.71,null,-6.23,null,-2.1,null,null,null,null,null,7.94,null,-2.206666666666667]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,1.74,null,-6.23,null,-2.1,null,null,null,null,null,7.9700000000000006,null,-2.1966666666666668]
[null,null,7,1,2,"15khZ","5MHz","A","(2,11)","NTN-TDLA100-200 Low","MCS 5 (99/1024)",0,2,2,0,null,null,-7.44,null,-10,null,-5.7,null,null,null,null,null,4.3,null,-7.7133333333333338]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,-7.36,null,-10,null,-5.7,null,null,null,null,null,4.3,null,-7.6866666666666665]
[null,null,8,1,2,"15khZ","5MHz","A","(2,11)","NTN-TDLA100-200 Low","MCS 5 (99/1024)",200,2,2,0,null,null,-7.27,null,-10,null,-5.7,null,null,null,null,null,4.3,null,-7.6566666666666663]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,-7.24,null,-10,null,-5.7,null,null,null,null,null,4.3,null,-7.6466666666666674]
[]
[null,null,9,1,1,"30khZ","10MHz","A","(2,11)","NTN-TDLC5-200 Low","MCS 5 (99/1024)",0,2,2,0,null,null,-7.32,null,null,null,-2.8,null,null,null,null,null,4.5200000000000005,null,-5.0600000000000005]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,-7.32,null,null,null,-2.8,null,null,null,null,null,4.5200000000000005,null,-5.0600000000000005]
[null,null,10,1,1,"30khZ","10MHz","A","(2,11)","NTN-TDLC5-200 Low","MCS 5 (99/1024)",200,2,2,0,null,null,-6.52,null,null,null,-2.8,null,null,null,null,null,3.7199999999999998,null,-4.66]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,-6.53,null,null,null,-2.8,null,null,null,null,null,3.7300000000000004,null,-4.665]
[null,null,11,1,2,"30khZ","10MHz","A","(2,11)","NTN-TDLC5-200 Low","MCS 5 (99/1024)",0,2,2,0,null,null,-10.54,null,null,null,-5.7,null,null,null,null,null,4.839999999999999,null,-8.1199999999999992]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,-10.58,null,null,null,-5.7,null,null,null,null,null,4.88,null,-8.14]
[null,null,12,1,2,"30khZ","10MHz","A","(2,11)","NTN-TDLC5-200 Low","MCS 5 (99/1024)",200,2,2,0,null,null,-9.75,null,null,null,-5.7,null,null,null,null,null,4.05,null,-7.7249999999999996]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,-9.7899999999999991,null,null,null,-5.7,null,null,null,null,null,4.089999999999999,null,-7.7449999999999992]
[null,null,13,1,1,"30khZ","10MHz","A","(2,11)","NTN-TDLA100-200 Low","MCS 5 (99/1024)",0,2,2,0,null,null,-5.25,null,null,null,-2.1,null,null,null,null,null,3.15,null,-3.6749999999999998]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,-5.26,null,null,null,-2.1,null,null,null,null,null,3.1599999999999997,null,-3.6799999999999997]
[null,null,14,1,1,"30khZ","10MHz","A","(2,11)","NTN-TDLA100-200 Low","MCS 5 (99/1024)",200,2,2,0,null,null,-4.37,null,null,null,-2.1,null,null,null,null,null,2.27,null,-3.2350000000000003]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,-4.38,null,null,null,-2.1,null,null,null,null,null,2.2799999999999998,null,-3.24]
[null,null,15,1,2,"30khZ","10MHz","A","(2,11)","NTN-TDLA100-200 Low","MCS 5 (99/1024)",0,2,2,0,null,null,-9.58,null,null,null,-5.8,null,null,null,null,null,3.7800000000000002,null,-7.6899999999999995]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,-9.56,null,null,null,-5.8,null,null,null,null,null,3.7600000000000007,null,-7.68]
[null,null,16,1,2,"30khZ","10MHz","A","(2,11)","NTN-TDLA100-200 Low","MCS 5 (99/1024)",200,2,2,0,null,null,-8.8800000000000008,null,null,null,-5.8,null,null,null,null,null,3.080000000000001,null,-7.34]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,-8.85,null,null,null,-5.8,null,null,null,null,null,3.05,null,-7.3249999999999993]
[]
[null,null,17,1,1,"15khZ","5MHz","B","(2,11)","NTN-TDLC5-200 Low","MCS 5 (99/1024)",0,null,null,null,null,null,null,null,null,null,-2.7,null,null,null,null,null,0,null,-2.7]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,-2.7,null,null,null,null,null,0,null,-2.7]
[null,null,18,1,1,"15khZ","5MHz","B","(2,11)","NTN-TDLC5-200 Low","MCS 5 (99/1024)",200,null,null,null,null,null,null,null,null,null,-2.7,null,null,null,null,null,0,null,-2.7]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,-2.7,null,null,null,null,null,0,null,-2.7]
[null,null,19,1,2,"15khZ","5MHz","B","(2,11)","NTN-TDLC5-200 Low","MCS 5 (99/1024)",0,null,null,null,null,null,null,null,null,null,-5.7,null,null,null,null,null,0,null,-5.7]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,-5.7,null,null,null,null,null,0,null,-5.7]
[null,null,20,1,2,"15khZ","5MHz","B","(2,11)","NTN-TDLC5-200 Low","MCS 5 (99/1024)",200,null,null,null,null,null,null,null,null,null,-5.7,null,null,null,null,null,0,null,-5.7]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,-5.7,null,null,null,null,null,0,null,-5.7]
[null,null,21,1,1,"15khZ","5MHz","B","(2,11)","NTN-TDLA100-200 Low","MCS 5 (99/1024)",0,null,null,null,null,null,null,null,null,null,-2.1,null,null,null,null,null,0,null,-2.1]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,-2.1,null,null,null,null,null,0,null,-2.1]
[null,null,22,1,1,"15khZ","5MHz","B","(2,11)","NTN-TDLA100-200 Low","MCS 5 (99/1024)",200,null,null,null,null,null,null,null,null,null,-2.1,null,null,null,null,null,0,null,-2.1]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,-2.1,null,null,null,null,null,0,null,-2.1]
[null,null,23,1,2,"15khZ","5MHz","B","(2,11)","NTN-TDLA100-200 Low","MCS 5 (99/1024)",0,null,null,null,null,null,null,null,null,null,-5.7,null,null,null,null,null,0,null,-5.7]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,-5.7,null,null,null,null,null,0,null,-5.7]
[null,null,24,1,2,"15khZ","5MHz","B","(2,11)","NTN-TDLA100-200 Low","MCS 5 (99/1024)",200,null,null,null,null,null,null,null,null,null,-5.7,null,null,null,null,null,0,null,-5.7]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,-5.7,null,null,null,null,null,0,null,-5.7]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[null,null,null,1,1,"30khZ","10MHz","B","(2,11)","NTN-TDLC5-200 Low","MCS 5 (99/1024)",0,null,null,null,null,null,null,null,null,null,-2.8,null,null,null,null,null,0,null,-2.8]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,-2.8,null,null,null,null,null,0,null,-2.8]
[null,null,null,1,1,"30khZ","10MHz","B","(2,11)","NTN-TDLC5-200 Low","MCS 5 (99/1024)",200,null,null,null,null,null,null,null,null,null,-2.8,null,null,null,null,null,0,null,-2.8]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,-2.8,null,null,null,null,null,0,null,-2.8]
[null,null,null,1,2,"30khZ","10MHz","B","(2,11)","NTN-TDLC5-200 Low","MCS 5 (99/1024)",0,null,null,null,null,null,null,null,null,null,-5.7,null,null,null,null,null,0,null,-5.7]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,-5.7,null,null,null,null,null,0,null,-5.7]
[null,null,null,1,2,"30khZ","10MHz","B","(2,11)","NTN-TDLC5-200 Low","MCS 5 (99/1024)",200,null,null,null,null,null,null,null,null,null,-5.7,null,null,null,null,null,0,null,-5.7]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,-5.7,null,null,null,null,null,0,null,-5.7]
[null,null,null,1,1,"30khZ","10MHz","B","(2,11)","NTN-TDLA100-200 Low","MCS 5 (99/1024)",0,null,null,null,null,null,null,null,null,null,-2.1,null,null,null,null,null,0,null,-2.1]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,-2.1,null,null,null,null,null,0,null,-2.1]
[null,null,null,1,1,"30khZ","10MHz","B","(2,11)","NTN-TDLA100-200 Low","MCS 5 (99/1024)",200,null,null,null,null,null,null,null,null,null,-2.1,null,null,null,null,null,0,null,-2.1]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,-2.1,null,null,null,null,null,0,null,-2.1]
[null,null,null,1,2,"30khZ","10MHz","B","(2,11)","NTN-TDLA100-200 Low","MCS 5 (99/1024)",0,null,null,null,null,null,null,null,null,null,-5.7,null,null,null,null,null,0,null,-5.7]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,-5.7,null,null,null,null,null,0,null,-5.7]
[null,null,null,1,2,"30khZ","10MHz","B","(2,11)","NTN-TDLA100-200 Low","MCS 5 (99/1024)",200,null,null,null,null,null,null,null,null,null,-5.7,null,null,null,null,null,{"$f":"MAX(R68:Z68)-MIN(R68:Z68)","v":0},null,{"$f":"AVERAGE(R68:Z68)","v":-5.7}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,-5.7,null,null,null,null,null,0,null,-5.7]

{"sheet":"PDSCH requirement with RedCap","index":3,"n_rows":70,"n_cols":15,"rows_kept":70,"cut":false,"hidden":false,"merged":[[5,1,6,1],[5,2,6,2],[5,3,6,3],[5,4,6,4],[5,5,6,5],[7,1,8,1],[7,2,8,2],[7,3,8,3],[7,4,8,4],[7,5,8,5],[9,1,10,1],[9,2,10,2],[9,3,10,3],[9,4,10,4],[9,5,10,5],[23,1,24,1],[23,2,24,2],[23,3,24,3],[23,4,24,4],[23,5,24,5],[25,1,26,1],[25,2,26,2],[25,3,26,3],[25,4,26,4],[25,5,26,5],[27,1,28,1],[27,2,28,2],[27,3,28,3],[27,4,28,4],[27,5,28,5],[29,1,30,1],[29,2,30,2],[29,3,30,3],[29,4,30,4],[29,5,30,5],[49,1,50,1],[49,2,50,2],[49,3,50,3],[49,4,50,4],[49,5,50,5],[51,7,52,7],[51,1,52,1],[51,2,52,2],[51,3,52,3],[51,4,52,4],[51,5,52,5],[53,1,54,1],[53,2,54,2],[53,3,54,3],[53,4,54,4],[53,5,54,5],[5,8,6,8],[5,9,6,9],[5,10,6,10],[5,11,6,11],[7,7,8,7],[7,8,8,8],[7,9,8,9],[7,10,8,10],[7,11,8,11],[5,7,6,7],[9,8,10,8],[9,9,10,9],[9,10,10,10],[9,11,10,11],[23,7,24,7],[23,8,24,8],[23,9,24,9],[23,10,24,10],[23,11,24,11],[16,9,17,9],[9,7,10,7],[25,8,26,8],[25,9,26,9],[25,10,26,10],[25,11,26,11],[27,7,28,7],[27,8,28,8],[27,9,28,9],[27,10,28,10],[27,11,28,11],[25,7,26,7],[29,8,30,8],[29,9,30,9],[29,10,30,10],[29,11,30,11],[49,7,50,7],[49,8,50,8],[49,9,50,9],[49,10,50,10],[49,11,50,11],[34,8,35,8],[29,7,30,7],[5,13,6,13],[5,14,6,14],[7,12,8,12],[7,13,8,13],[7,14,8,14],[9,12,10,12],[9,13,10,13],[9,14,10,14],[55,7,56,7],[55,8,56,8],[55,9,56,9],[55,10,56,10],[55,11,56,11],[5,12,6,12],[14,8,15,8],[14,9,15,9],[14,10,15,10],[14,11,15,11],[51,8,52,8],[51,9,52,9],[51,10,52,10],[51,11,52,11],[53,7,54,7],[53,8,54,8],[16,13,17,13],[16,14,17,14],[18,1,19,1],[18,2,19,2],[18,3,19,3],[18,4,19,4],[18,5,19,5],[14,12,15,12],[14,13,15,13],[14,14,15,14],[16,1,17,1],[16,2,17,2],[16,3,17,3],[16,4,17,4],[16,5,17,5],[16,7,17,7],[16,8,17,8],[14,1,15,1],[14,2,15,2],[14,3,15,3],[14,4,15,4],[14,5,15,5],[14,7,15,7],[18,7,19,7],[18,8,19,8],[18,9,19,9],[18,10,19,10],[18,11,19,11],[18,12,19,12],[16,10,17,10],[16,11,17,11],[16,12,17,12],[27,12,28,12],[27,13,28,13],[27,14,28,14],[29,12,30,12],[29,13,30,13],[29,14,30,14],[18,13,19,13],[18,14,19,14],[23,12,24,12],[23,13,24,13],[23,14,24,14],[25,12,26,12],[25,13,26,13],[25,14,26,14],[34,9,35,9],[34,10,35,10],[34,11,35,11],[34,12,35,12],[34,13,35,13],[34,14,35,14],[34,1,35,1],[34,2,35,2],[34,3,35,3],[34,4,35,4],[34,5,35,5],[34,7,35,7],[36,14,37,14],[38,1,39,1],[38,2,39,2],[38,3,39,3],[38,4,39,4],[38,5,39,5],[38,7,39,7],[38,8,39,8],[38,9,39,9],[38,10,39,10],[36,8,37,8],[36,9,37,9],[36,10,37,10],[36,11,37,11],[36,12,37,12],[36,13,37,13],[36,1,37,1],[36,2,37,2],[36,3,37,3],[36,4,37,4],[36,5,37,5],[36,7,37,7],[38,11,39,11],[38,12,39,12],[38,13,39,13],[38,14,39,14],[40,1,41,1],[40,2,41,2],[40,3,41,3],[40,4,41,4],[40,5,41,5],[40,7,41,7],[40,14,41,14],[60,1,61,1],[60,2,61,2],[60,3,61,3],[60,4,61,4],[60,5,61,5],[60,7,61,7],[60,8,61,8],[60,9,61,9],[60,10,61,10],[40,8,41,8],[40,9,41,9],[40,10,41,10],[40,11,41,11],[40,12,41,12],[40,13,41,13],[53,9,54,9],[53,10,54,10],[53,11,54,11],[55,1,56,1],[55,2,56,2],[55,3,56,3],[55,4,56,4],[55,5,56,5],[62,1,63,1],[62,2,63,2],[62,3,63,3],[62,4,63,4],[62,5,63,5],[62,7,63,7],[62,8,63,8],[62,9,63,9],[62,10,63,10],[64,1,65,1],[64,2,65,2],[64,3,65,3],[64,4,65,4],[64,5,65,5],[64,7,65,7],[64,8,65,8],[64,9,65,9],[64,10,65,10],[66,1,67,1],[66,2,67,2],[66,3,67,3],[66,4,67,4],[66,5,67,5],[66,7,67,7],[66,8,67,8],[66,9,67,9],[66,10,67,10],[55,12,56,12],[55,13,56,13],[55,14,56,14],[60,12,61,12],[60,13,61,13],[60,14,61,14],[66,11,67,11],[49,12,50,12],[49,13,50,13],[49,14,50,14],[51,12,52,12],[51,13,52,13],[51,14,52,14],[53,12,54,12],[53,13,54,13],[53,14,54,14],[64,11,65,11],[62,11,63,11],[60,11,61,11],[66,12,67,12],[66,13,67,13],[66,14,67,14],[62,12,63,12],[62,13,63,13],[62,14,63,14],[64,12,65,12],[64,13,65,13],[64,14,65,14]]}
[]
[]
[]
[null,"NTN RedCap 1Rx"]
[null,"Test number ","MCS/PRB","Channel model","HARQ process","Antenna configuration","Reference channel","Huawei","Ericsson","Apple","QC","MTK","span","STD","average"]
[null,1,"MCS4, 52PRB","NTN-TDLA100-200",16,"1x1","New FRC for FDD",1.1000000000000001,0.7,2.2000000000000002,null,null,{"$f":"MAX(H6:L6)-MIN(H6:L6)","v":1.5000000000000002},{"$f":"_xlfn.STDEV.S(H6:L6)","v":0.77674534651540328},{"$f":"AVERAGE(H6:L6)","v":1.3333333333333333}]
[null,null,null,null,null,null,"New FRC for HD-FDD"]
[null,2,"MCS4, 52PRB","NTN-TDLC5-200",32,"1x1","New FRC for FDD",0.2,-0.9,0.8,null,null,{"$f":"MAX(H8:L8)-MIN(H8:L8)","v":1.7000000000000002},{"$f":"_xlfn.STDEV.S(H8:L8)","v":0.86216781042517088},{"$f":"AVERAGE(H8:L8)","v":3.3333333333333361E-2}]
[null,null,null,null,null,null,"New FRC for HD-FDD"]
[null,3,"MCS13, 52PRB","NTN-TDLC5-200",16,"1x1","R.PDSCH.1-2.1 FDD",8,7.3,8.3000000000000007,null,null,{"$f":"MAX(H10:L10)-MIN(H10:L10)","v":1.0000000000000009},{"$f":"_xlfn.STDEV.S(H10:L10)","v":0.51316014394468878},{"$f":"AVERAGE(H10:L10)","v":7.8666666666666671}]
[null,null,null,null,null,null,"R.PDSCH. 1-1.2  HD-FDD"]
[]
[null,"NTN RedCap 1Rx"]
[null,"Test number ","MCS/PRB","Channel model","HARQ process","Antenna configuration","Reference channel","Huawei","Ericsson","Apple","QC","MTK","Average","additional margin","SNR"]
[null,1,"MCS4, 52PRB","NTN-TDLA100-200",16,"1x1","New FRC for FDD",1.1000000000000001,0.7,2.2000000000000002,null,null,{"$f":"AVERAGE(H15:L15)","v":1.3333333333333333},0.5,{"$f":"ROUND(M15+N15,1)","v":1.8}]
[null,null,null,null,null,null,"New FRC for HD-FDD"]
[null,2,"MCS4, 52PRB","NTN-TDLC5-200",32,"1x1","New FRC for FDD",0.2,-0.9,0.8,null,null,{"$f":"AVERAGE(H17:L17)","v":3.3333333333333361E-2},0.5,{"$f":"ROUND(M17+N17,1)","v":0.5}]
[null,null,null,null,null,null,"New FRC for HD-FDD"]
[null,3,"MCS13, 52PRB","NTN-TDLC5-200",16,"1x1","R.PDSCH.1-2.1 FDD",8,7.3,8.3000000000000007,null,null,{"$f":"AVERAGE(H19:L19)","v":7.8666666666666671},{"$f":"_xlfn.STDEV.S(H19:L19)","v":0.51316014394468878},{"$f":"ROUND(M19+N19,1)","v":8.4}]
[null,null,null,null,null,null,"R.PDSCH. 1-1.2  HD-FDD"]
[]
[null,"NTN eRedCap 1Rx/2Rx UE without baseband bandwidth reduction capability"]
[null,"Test number ","MCS/PRB","Channel model","HARQ process","Antenna configuration","Reference channel","Huawei","Ericsson","Apple","QC","MTK","SPAN","STD","average"]
[null,1,"MCS4, 52","NTN-TDLA100-200",16,"1x1","New FRC for FDD",1.1000000000000001,0.7,2.2000000000000002,null,null,{"$f":"MAX(H24:L24)-MIN(H24:L24)","v":1.5000000000000002},{"$f":"_xlfn.STDEV.S(H24:L24)","v":0.77674534651540328},{"$f":"AVERAGE(H24:L24)","v":1.3333333333333333}]
[null,null,null,null,null,null,"New FRC for HD-FDD"]
[null,2,"MCS13, 40","NTN-TDLC5-200",16,"1x1","R.PDSCH.1-12.3 FDD",8,7.3,8.3000000000000007,null,null,{"$f":"MAX(H26:L26)-MIN(H26:L26)","v":1.0000000000000009},{"$f":"_xlfn.STDEV.S(H26:L26)","v":0.51316014394468878},{"$f":"AVERAGE(H26:L26)","v":7.8666666666666671}]
[null,null,null,null,null,null,"R.PDSCH.1-2.4 HD-FDD"]
[null,3,"MCS4, 52","NTN-TDLA100-200",16,"1x2","New FRC for FDD",null,-2.7,null,null,null,{"$f":"MAX(H28:L28)-MIN(H28:L28)","v":0}]
[null,null,null,null,null,null,"New FRC for HD-FDD"]
[null,4,"MCS13, 40","NTN-TDLC5-200",16,"1x2","R.PDSCH.1-12.3 FDD",4.8,3.6,4.8,null,null,{"$f":"MAX(H30:L30)-MIN(H30:L30)","v":1.1999999999999997},{"$f":"_xlfn.STDEV.S(H30:L30)","v":0.69282032302755381},{"$f":"AVERAGE(H30:L30)","v":4.3999999999999995}]
[null,null,null,null,null,null,"R.PDSCH.1-2.4 HD-FDD"]
[]
[null,"NTN eRedCap 1Rx/2Rx UE without baseband bandwidth reduction capability"]
[null,"Test number ","MCS/PRB","Channel model","HARQ process","Antenna configuration","Reference channel","Huawei","Ericsson","Apple","QC","MTK","average","additional margin","SNR"]
[null,1,"MCS4, 52","NTN-TDLA100-200",16,"1x1","New FRC for FDD",1.1000000000000001,0.7,2.2000000000000002,null,null,{"$f":"AVERAGE(H35:L35)","v":1.3333333333333333},0.5,{"$f":"ROUND(M35+N35,1)","v":1.8}]
[null,null,null,null,null,null,"New FRC for HD-FDD"]
[null,2,"MCS13, 40","NTN-TDLC5-200",16,"1x1","R.PDSCH.1-12.3 FDD",8,7.3,8.3000000000000007,null,null,{"$f":"AVERAGE(H37:L37)","v":7.8666666666666671},0.5,{"$f":"ROUND(M37+N37,1)","v":8.4}]
[null,null,null,null,null,null,"R.PDSCH.1-2.4 HD-FDD"]
[null,3,"MCS4, 52","NTN-TDLA100-200",16,"1x2","New FRC for FDD",null,-2.7,null,null,null,{"$f":"AVERAGE(H39:L39)","v":-2.7},0.5,-2.2000000000000002]
[null,null,null,null,null,null,"New FRC for HD-FDD"]
[null,4,"MCS13, 40","NTN-TDLC5-200",16,"1x2","R.PDSCH.1-12.3 FDD",4.8,3.6,4.8,null,null,{"$f":"AVERAGE(H41:L41)","v":4.3999999999999995},0.5,{"$f":"ROUND(M41+N41,1)","v":4.9000000000000004}]
[null,null,null,null,null,null,"R.PDSCH.1-2.4 HD-FDD"]
[]
[]
[]
[]
[]
[null,"NTN eRedCap 1Rx/2Rx UE with baseband bandwidth reduction capability"]
[null,"Test number ","MCS/PRB","Channel model","HARQ process","Antenna configuration","Reference channel","Huawei","Ericsson","Apple","QC","MTK","SPAN","STD","average"]
[null,1,"MCS4, 25","NTN-TDLA100-200",16,"1x1","New FRC for FDD",1.4,1.2,2.5,null,null,{"$f":"MAX(H50,L50)","v":1.4},{"$f":"_xlfn.STDEV.S(H50:L50)","v":0.69999999999999951},{"$f":"AVERAGE(H50:L50)","v":1.7}]
[null,null,null,null,null,null,"New FRC for HD-FDD"]
[null,2,"MCS13, 25","NTN-TDLC5-200",16,"1x1","R.PDSCH.1-25.1 FDD",7.6,7.1,7.7,null,null,{"$f":"MAX(H52,L52)","v":7.6},{"$f":"_xlfn.STDEV.S(H52:L52)","v":0.321455025366432},{"$f":"AVERAGE(H52:L52)","v":7.4666666666666659}]
[null,null,null,null,null,null,"R.PDSCH.1-2.3 HD-FDD"]
[null,3,"MCS4, 25","NTN-TDLA100-200",16,"1x2","New FRC for FDD",-2.6,-3.2,-1.6,null,null,{"$f":"MAX(H54,L54)","v":-2.6},{"$f":"_xlfn.STDEV.S(H54:L54)","v":0.80829037686547667},{"$f":"AVERAGE(H54:L54)","v":-2.4666666666666668}]
[null,null,null,null,null,null,"New FRC for HD-FDD"]
[null,4,"MCS13, 25","NTN-TDLC5-200",16,"1x2","R.PDSCH.1-25.1 FDD",4.7,3.4,4.3,null,null,{"$f":"MAX(H56,L56)","v":4.7},{"$f":"_xlfn.STDEV.S(H56:L56)","v":0.6658328118479433},{"$f":"AVERAGE(H56:L56)","v":4.1333333333333329}]
[null,null,null,null,null,null,"R.PDSCH.1-2.3 HD-FDD"]
[]
[null,"NTN eRedCap 1Rx/2Rx UE with baseband bandwidth reduction capability"]
[null,"Test number ","MCS/PRB","Channel model","HARQ process","Antenna configuration","Reference channel","Huawei","Ericsson","Apple","QC","MTK","average","additional margin","SNR"]
[null,1,"MCS4, 25","NTN-TDLA100-200",16,"1x1","New FRC for FDD",1.4,1.2,2.5,null,null,{"$f":"AVERAGE(H61:L61)","v":1.7},0.5,{"$f":"ROUND(M61+N61,1)","v":2.2000000000000002}]
[null,null,null,null,null,null,"New FRC for HD-FDD"]
[null,2,"MCS13, 25","NTN-TDLC5-200",16,"1x1","R.PDSCH.1-25.1 FDD",7.6,7.1,7.7,null,null,{"$f":"AVERAGE(H63:L63)","v":7.4666666666666659},0.5,{"$f":"ROUND(M63+N63,1)","v":8}]
[null,null,null,null,null,null,"R.PDSCH.1-2.3 HD-FDD"]
[null,3,"MCS4, 25","NTN-TDLA100-200",16,"1x2","New FRC for FDD",-2.6,-3.2,-1.6,null,null,{"$f":"AVERAGE(H65:L65)","v":-2.4666666666666668},0.5,{"$f":"ROUND(M65+N65,1)","v":-2}]
[null,null,null,null,null,null,"New FRC for HD-FDD"]
[null,4,"MCS13, 25","NTN-TDLC5-200",16,"1x2","R.PDSCH.1-25.1 FDD",4.7,3.4,4.3,null,null,{"$f":"AVERAGE(H67:L67)","v":4.1333333333333329},0.5,{"$f":"ROUND(M67+N67,1)","v":4.5999999999999996}]
[null,null,null,null,null,null,"R.PDSCH.1-2.3 HD-FDD"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,"Cf. 0.5dB for QPSK/16QAM, 0.8dB for 64QAM/256QAM, and 1dB for 1024QAM (single carrier case)"]

{"sheet":"PUSCH requirement 4Rx","index":4,"n_rows":30,"n_cols":40,"rows_kept":30,"cut":false,"hidden":true,"merged":[[0,28,0,29],[0,30,0,31],[0,32,0,33],[0,34,0,35],[0,36,0,37],[0,38,0,39],[17,14,17,15],[17,16,17,17],[17,18,17,19],[17,20,17,21],[17,22,17,23],[17,24,17,25],[17,26,17,27],[17,28,17,29],[17,30,17,31],[17,32,17,33],[17,34,17,35],[17,36,17,37],[17,38,17,39],[0,14,0,15],[0,16,0,17],[0,18,0,19],[0,20,0,21],[0,22,0,23],[0,24,0,25],[0,26,0,27],[2,1,3,1],[5,1,6,1],[8,1,9,1],[11,1,12,1],[19,1,20,1],[22,1,23,1],[25,1,26,1],[2,3,3,3],[5,3,6,3],[8,3,9,3],[11,3,12,3],[19,3,20,3],[22,3,23,3],[25,3,26,3],[2,6,3,6],[5,6,6,6],[8,6,9,6],[11,6,12,6],[19,6,20,6],[22,6,23,6],[25,6,26,6],[2,8,3,8],[28,1,29,1],[2,2,3,2],[5,2,6,2],[8,2,9,2],[11,2,12,2],[19,2,20,2],[22,2,23,2],[25,2,26,2],[28,2,29,2],[28,3,29,3],[2,4,3,4],[5,4,6,4],[8,4,9,4],[11,4,12,4],[19,4,20,4],[22,4,23,4],[25,4,26,4],[28,4,29,4],[28,6,29,6],[2,7,3,7],[5,7,6,7],[8,7,9,7],[11,7,12,7],[19,7,20,7],[22,7,23,7],[25,7,26,7],[28,7,29,7],[5,8,6,8],[8,8,9,8],[11,8,12,8],[19,8,20,8],[22,8,23,8],[25,8,26,8],[28,8,29,8],[2,9,3,9],[5,9,6,9],[8,9,9,9],[11,9,12,9],[19,9,20,9],[22,9,23,9],[25,9,26,9],[28,9,29,9],[2,10,3,10],[5,10,6,10],[8,10,9,10],[11,10,12,10],[19,10,20,10],[22,10,23,10],[25,10,26,10],[28,10,29,10],[2,11,3,11],[5,11,6,11],[8,11,9,11],[11,11,12,11],[19,11,20,11],[22,11,23,11],[25,11,26,11],[28,11,29,11]]}
["case ","Tx","SCS","Waveform","BW","Mapping Type","MCS for target cell","MCS for interferer cell","Propagation condition for target cell","Propagation conditon for interferer cell ","Number of Interferer cells","DIP set","38.104 req","38.141-1/2 req","Samsung",null,"Huawei",null,"Ericsson",null,"ZTE",null,"Nokia",null,"QC",null,"CATT",null,"CTC",null,"CMCC",null,"Tejas Networks",null,"NTT DOCOMO",null,"SPAN",null,"AVERAGE"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ideal","Impairment","ideal","Impairment","ideal","Impairment","ideal","Impairment","ideal","Impairment","ideal","Impairment","ideal","Impairment","ideal","Impairment","ideal","Impairment","ideal","Impairment","ideal","Impairment","Ideal","Impairment","Ideal","Impairment"]
[1,1,"15kHz","CP-OFDM","5MHz","A",16,"16QAM","TDLC300-100","TDLC300-100",2,"HomNet set1: (-1.11. -10.91)",{"$f":"DerivingPerfReq(O3:AJ3)","v":10.1},{"$f":"IF(M3>-100,M3+0.6,M3)","v":10.7},9.1,11.1,8,10,8.18,10.48,7.4,9.9,7.4,9.9,8.6999999999999993,10.7,7.74,10.24,8,10.5,7.02,9.02,7.7,null,null,null,{"$f":"MAX(O3,Q3,S3,U3,W3,Y3,AA3,AC3,AE3,AG3,AI3)-MIN(O3,Q3,S3,U3,W3,Y3,AA3,AC3,AE3,AG3,AI3)","v":2.08},{"$f":"MAX(P20,R20,T20,V20,X20,Z20,AB20,AD20,AF20,AH20,AJ20)","v":11.6},{"$f":"AVERAGE(O3,Q3,S3,U3,W3,Y3,AA3,AC3,AE3,AG3,AI3)","v":7.9240000000000013},{"$f":"AVERAGE(P3,R3,T3,V3,X3,Z3,AB3,AD3,AF3,AH3,AJ3)","v":10.204444444444443}]
[2,null,null,null,null,"B",null,null,null,null,null,null,{"$f":"DerivingPerfReq(O4:AJ4)","v":10.4},{"$f":"IF(M4>-100,M4+0.6,M4)","v":11},9.1,11.1,null,null,8.24,10.5,7.3,9.8000000000000007,7.5,10,null,null,null,null,8.1999999999999993,10.7,null,null,null,null,null,null,{"$f":"MAX(O4,Q4,S4,U4,W4,Y4,AA4,AC4,AE4,AG4,AI4)-MIN(O4,Q4,S4,U4,W4,Y4,AA4,AC4,AE4,AG4,AI4)","v":1.7999999999999998},{"$f":"MAX(P21,R21,T21,V21,X21,Z21,AB21,AD21,AF21,AH21,AJ21)","v":11.6},{"$f":"AVERAGE(O4,Q4,S4,U4,W4,Y4,AA4,AC4,AE4,AG4,AI4)","v":8.0680000000000014},{"$f":"AVERAGE(P4,R4,T4,V4,X4,Z4,AB4,AD4,AF4,AH4,AJ4)","v":10.420000000000002}]
[]
[3,1,"15kHz","CP-OFDM","5MHz","A",16,"16QAM","TDLA30-10","TDLC300-100",2,"HetNet set2: (-0.43. -13.78)",{"$f":"DerivingPerfReq(O6:AJ6)","v":10.1},10.7,9.1999999999999993,11.2,8.4,10.4,7.55,9.6300000000000008,7,9.5,7,9.5,9.59,11.59,8.5299999999999994,11.03,8.5,11,7.93,9.93,9,null,null,null,2.59,12.37,8.2700000000000014,10.42]
[4,null,null,null,null,"B",null,null,null,null,null,null,{"$f":"DerivingPerfReq(O7:AJ7)","v":10.199999999999999},10.799999999999999,9.1999999999999993,11.2,null,null,7.77,10.16,7.1,9.6,7,9.5,null,null,null,null,8.9,11.4,null,null,null,null,null,null,2.1999999999999993,11.5,7.9939999999999998,10.372]
[]
[5,1,"15kHz","CP-OFDM","20MHz","A",16,"16QAM","TDLC300-100","TDLC300-100",2,"HomNet set1: (-1.11. -10.91)",{"$f":"DerivingPerfReq(O9:AJ9)","v":10.4},11,9.1999999999999993,11.2,8.1999999999999993,10.199999999999999,8.3000000000000007,10.5,8.1999999999999993,10.7,7.6,10.1,8.67,10.67,8.5,11,7.7,10.199999999999999,7.32,9.32,8,null,null,null,1.879999999999999,12.1,8.1690000000000005,10.432222222222224]
[6,null,null,null,null,"B",null,null,null,null,null,null,{"$f":"DerivingPerfReq(O10:AJ10)","v":10.7},11.299999999999999,9.1999999999999993,11.2,null,null,8.33,10.56,8.3000000000000007,10.8,7.6,10.1,null,null,null,null,8.1999999999999993,10.7,null,null,null,null,null,null,1.5999999999999996,11.5,8.3259999999999987,10.672000000000001]
[]
[7,1,"15kHz","CP-OFDM","20MHz","A",16,"16QAM","TDLA30-10","TDLC300-100",2,"HetNet set2: (-0.43. -13.78)",{"$f":"DerivingPerfReq(O12:AJ12)","v":11.1},11.7,9.3000000000000007,11.3,8.8000000000000007,10.8,8.19,10.46,7.5,10,6.8,9.3000000000000007,9.6199999999999992,11.62,9.3000000000000007,11.8,9,11.5,7.91,9.91,9.1999999999999993,null,null,null,2.8199999999999994,12.34,8.5619999999999994,10.743333333333332]
[8,null,null,null,null,"B",null,null,null,null,null,null,{"$f":"DerivingPerfReq(O13:AJ13)","v":10.9},11.5,9.3000000000000007,11.3,null,null,8.31,10.58,7.6,10.1,6.7,9.1999999999999993,null,null,null,null,9,11.7,null,null,null,null,null,null,2.6000000000000005,11.2,8.1819999999999986,10.576000000000002]
[]
[32,null,null,null,null,"B",null,null,null,null,null,null,{"$f":"DerivingPerfReq(O15:AJ15)","v":-100},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[]
[]
["case ","Tx","SCS","Waveform","BW","Mapping Type","MCS for target cell","MCS for interferer cell","Propagation condition for target cell","Propagation conditon for interferer cell ","Number of Interferer cells","DIP set","38.104 req","38.141-1/2 req","Samsung",null,"Huawei",null,"Ericsson",null,"ZTE",null,"Nokia",null,"QC",null,"CATT",null,"CTC",null,"CMCC",null,"Tejas Networks",null,"NTT DOCOMO",null,"SPAN",null,"AVERAGE"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ideal","Impairment","ideal","Impairment","ideal","Impairment","ideal","Impairment","ideal","Impairment","ideal","Impairment","idela ","Impairment","ideal","Impairment","ideal","Impairment","ideal","Impairment","ideal","Impairment","Ideal","Impairment","Ideal","Impairment"]
[1,1,"30kHz","CP-OFDM","10MHz","A",16,"16QAM","TDLC300-100","TDLC300-100",2,"HomNet set1: (-1.11. -10.91)",{"$f":"DerivingPerfReq(O20:AJ20)","v":10.4},{"$f":"IF(M20>-100,M20+0.6,M20)","v":11},9.6,11.6,7.6,9.6,8.2899999999999991,10.7,8.1,10.6,8.1,10.6,9.06,11.06,8.4,10.9,8.1999999999999993,10.7,7.44,9.44,8.4,null,null,null,{"$f":"MAX(O20,Q20,S20,U20,W20,Y20,AA20,AC20,AE20,AG20,AI20)-MIN(O20,Q20,S20,U20,W20,Y20,AA20,AC20,AE20,AG20,AI20)","v":2.1599999999999993},{"$f":"MAX(P20,R20,T20,V20,X20,Z20,AB20,AD20,AF20,AH20,AJ20)-MIN(P20,R20,T20,V20,X20,Z20,AB20,AD20,AF20,AH20,AJ20)","v":2.16},{"$f":"AVERAGE(O20,Q20,S20,U20,W20,Y20,AA20,AC20,AE20,AG20,AI20)","v":8.3189999999999991},{"$f":"AVERAGE(P20,R20,T20,V20,X20,Z20,AB20,AD20,AF20,AH20,AJ20)","v":10.577777777777778}]
[2,null,null,null,null,"B",null,null,null,null,null,null,{"$f":"DerivingPerfReq(O21:AJ21)","v":10.8},{"$f":"IF(M21>-100,M21+0.6,M21)","v":11.4},9.6,11.6,null,null,8.35,10.55,8.1999999999999993,10.7,8.1,10.6,null,null,null,null,8.3000000000000007,10.8,null,null,null,null,null,null,{"$f":"MAX(O21,Q21,S21,U21,W21,Y21,AA21,AC21,AE21,AG21,AI21)-MIN(O21,Q21,S21,U21,W21,Y21,AA21,AC21,AE21,AG21,AI21)","v":1.5},{"$f":"MAX(P21,R21,T21,V21,X21,Z21,AB21,AD21,AF21,AH21,AJ21)-MIN(P21,R21,T21,V21,X21,Z21,AB21,AD21,AF21,AH21,AJ21)","v":1.0499999999999989},{"$f":"AVERAGE(O21,Q21,S21,U21,W21,Y21,AA21,AC21,AE21,AG21,AI21)","v":8.51},{"$f":"AVERAGE(P21,R21,T21,V21,X21,Z21,AB21,AD21,AF21,AH21,AJ21)","v":10.85}]
[]
[3,1,"30kHz","CP-OFDM","10MHz","A",16,"16QAM","TDLA30-10","TDLC300-100",2,"HetNet set2: (-0.43. -13.78)",{"$f":"DerivingPerfReq(O23:AJ23)","v":10.4},11,9.5,11.5,8.1,10.1,8.1300000000000008,10.49,7.7,10.199999999999999,7.2,10.199999999999999,10.37,12.37,8.5,11,8.6,11.1,7.9,9.9,9.3000000000000007,null,null,null,3.169999999999999,2.4699999999999989,8.5300000000000011,10.762222222222224]
[4,null,null,null,null,"B",null,null,null,null,null,null,{"$f":"DerivingPerfReq(O24:AJ24)","v":10.5},11.1,9.5,11.5,null,null,8.18,10.39,7.8,10.3,7.2,10.199999999999999,null,null,null,null,8.5,11,null,null,null,null,null,null,2.2999999999999998,1.3000000000000007,8.2360000000000007,10.678000000000001]
[]
[5,1,"30kHz","CP-OFDM","100MHz","A",16,"16QAM","TDLC300-100","TDLC300-100",2,"HomNet set1: (-1.11. -10.91)",{"$f":"DerivingPerfReq(O26:AJ26)","v":10.8},11.4,9.5,11.5,8.1999999999999993,10.199999999999999,8.06,10.16,8,10.5,8,10.5,8.92,10.92,9.6,12.1,8.6,11.1,8.1199999999999992,10.119999999999999,8.5,null,null,null,1.5999999999999996,1.9800000000000004,8.5500000000000007,10.788888888888888]
[6,null,null,null,null,"B",null,null,null,null,null,null,{"$f":"DerivingPerfReq(O27:AJ27)","v":10.8},11.4,9.5,11.5,null,null,8.1300000000000008,10.33,8.1,10.6,8,10.5,null,null,null,null,8.6,11.1,null,null,null,null,null,null,1.5,1.17,8.4660000000000011,10.806000000000001]
[]
[7,1,"30kHz","CP-OFDM","100MHz","A",16,"16QAM","TDLA30-10","TDLC300-100",2,"HetNet set2: (-0.43. -13.78)",{"$f":"DerivingPerfReq(O29:AJ29)","v":10.8},11.4,9.1999999999999993,11.2,9,11,8.35,10.83,8.1,10.6,7.7,10.199999999999999,10.029999999999999,12.03,9.84,12.34,8.6999999999999993,11.2,8.4,10.4,9.3000000000000007,null,null,null,2.3299999999999992,2.1400000000000006,8.8620000000000001,11.08888888888889]
[8,null,null,null,null,"B",null,null,null,null,null,null,{"$f":"DerivingPerfReq(O30:AJ30)","v":10.8},11.4,9.1999999999999993,11.2,null,null,8.41,10.66,8.1,10.6,7.7,10.199999999999999,null,null,null,null,8.6,11.1,null,null,null,null,null,null,1.4999999999999991,1,8.402000000000001,10.751999999999999]

{"sheet":"PUSCH requirement 8Rx","index":5,"n_rows":31,"n_cols":40,"rows_kept":31,"cut":false,"hidden":true,"merged":[[0,28,0,29],[0,30,0,31],[0,32,0,33],[0,34,0,35],[0,36,0,37],[0,38,0,39],[17,14,17,15],[17,16,17,17],[17,18,17,19],[17,20,17,21],[17,22,17,23],[17,24,17,25],[17,26,17,27],[17,28,17,29],[17,30,17,31],[17,32,17,33],[17,34,17,35],[17,36,17,37],[17,38,17,39],[0,14,0,15],[0,16,0,17],[0,18,0,19],[0,20,0,21],[0,22,0,23],[0,24,0,25],[0,26,0,27],[2,1,3,1],[5,1,6,1],[8,1,9,1],[11,1,12,1],[19,1,20,1],[22,1,23,1],[25,1,26,1],[2,3,3,3],[5,3,6,3],[8,3,9,3],[11,3,12,3],[19,3,20,3],[22,3,23,3],[25,3,26,3],[2,6,3,6],[5,6,6,6],[8,6,9,6],[11,6,12,6],[19,6,20,6],[22,6,23,6],[25,6,26,6],[2,8,3,8],[28,1,30,1],[2,2,3,2],[5,2,6,2],[8,2,9,2],[11,2,12,2],[19,2,20,2],[22,2,23,2],[25,2,26,2],[28,2,30,2],[28,3,30,3],[2,4,3,4],[5,4,6,4],[8,4,9,4],[11,4,12,4],[19,4,20,4],[22,4,23,4],[25,4,26,4],[28,4,30,4],[28,6,29,6],[2,7,3,7],[5,7,6,7],[8,7,9,7],[11,7,12,7],[19,7,20,7],[22,7,23,7],[25,7,26,7],[28,7,30,7],[5,8,6,8],[8,8,9,8],[11,8,12,8],[19,8,20,8],[22,8,23,8],[25,8,26,8],[28,8,30,8],[2,9,3,9],[5,9,6,9],[8,9,9,9],[11,9,12,9],[19,9,20,9],[22,9,23,9],[25,9,26,9],[28,9,30,9],[2,10,3,10],[5,10,6,10],[8,10,9,10],[11,10,12,10],[19,10,20,10],[22,10,23,10],[25,10,26,10],[28,10,30,10],[2,11,3,11],[5,11,6,11],[8,11,9,11],[11,11,12,11],[19,11,20,11],[22,11,23,11],[25,11,26,11],[28,11,30,11]]}
["case ","Tx","SCS","Waveform","BW","Mapping Type","MCS for target cell","MCS for interferer cell","Propagation condition for target cell","Propagation conditon for interferer cell ","Number of Interferer cells","DIP set","38.104 req","38.141-1/2 req","Samsung",null,"Huawei",null,"Ericsson",null,"ZTE",null,"Nokia",null,"CTC",null,"QC",null,"CATT",null,"CMCC",null,"Tejas Networks",null,"NTT DOCOMO",null,"SPAN",null,"AVERAGE"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Ideal","impairment","ideal"," impairment","ideal","impairment","ideal"," impairment"," ideal","impairment","ideal"," impairment"," ideal"," impairment"," ideal"," impairment","ideal","impairment","ideal","impairment"," ideal","impairment","Ideal","impairment","Ideal","Impairment"]
[1,1,"15kHz","CP-OFDM","5MHz","A",16,"16QAM","TDLC300-100","TDLC300-100",2,"HomNet set1: (-1.11. -10.91)",{"$f":"DerivingPerfReq(O3:AJ3)","v":6.9},{"$f":"IF(M3>-100,M3+0.6,M3)","v":7.5},4.7,6.7,4.5999999999999996,6.6,4.1399999999999997,6.28,4.4000000000000004,6.9,3.2,5.7,4.2,6.7,4.62,7.12,5,7.5,2.79,4.79,3.2,null,5.62,7.62,{"$f":"MAX(O3,Q3,S3,U3,W3,Y3,AA3,AC3,AE3,AG3,AI3)-MIN(O3,Q3,S3,U3,W3,Y3,AA3,AC3,AE3,AG3,AI3)","v":2.83},{"$f":"MAX(P3,R3,T3,V3,X3,Z3,AB3,AD3,AF3,AH3,AJ3)-MIN(P3,R3,T3,V3,X3,Z3,AB3,AD3,AF3,AH3,AJ3)","v":2.83},{"$f":"AVERAGE(O3,Q3,S3,U3,W3,Y3,AA3,AC3,AE3,AG3,AI3)","v":4.2245454545454546},{"$f":"AVERAGE(P3,R3,T3,V3,X3,Z3,AB3,AD3,AF3,AH3,AJ3)","v":6.5910000000000011}]
[2,null,null,null,null,"B",null,null,null,null,null,null,{"$f":"DerivingPerfReq(O4:AJ4)","v":6.5},{"$f":"IF(M4>-100,M4+0.6,M4)","v":7.1},4.7,6.7,null,null,4.22,6.42,4.5999999999999996,7.1,3.1,5.6,4,6.5,null,null,null,null,null,null,null,null,8.07,10.07,{"$f":"MAX(O4,Q4,S4,U4,W4,Y4,AA4,AC4,AE4,AG4,AI4)-MIN(O4,Q4,S4,U4,W4,Y4,AA4,AC4,AE4,AG4,AI4)","v":4.9700000000000006},{"$f":"MAX(P4,R4,T4,V4,X4,Z4,AB4,AD4,AF4,AH4,AJ4)-MIN(P4,R4,T4,V4,X4,Z4,AB4,AD4,AF4,AH4,AJ4)","v":4.4700000000000006},{"$f":"AVERAGE(O4,Q4,S4,U4,W4,Y4,AA4,AC4,AE4,AG4,AI4)","v":4.7816666666666672},{"$f":"AVERAGE(P4,R4,T4,V4,X4,Z4,AB4,AD4,AF4,AH4,AJ4)","v":7.0650000000000004}]
[]
[3,1,"15kHz","CP-OFDM","5MHz","A",16,"16QAM","TDLA30-10","TDLC300-100",2,"HetNet set2: (-0.43. -13.78)",{"$f":"DerivingPerfReq(O6:AJ6)","v":6.1},6.6999999999999993,4.5999999999999996,6.6,4.4000000000000004,6.4,3.55,6.02,3.4,5.9,3,5.5,4.0999999999999996,6.6,5.91,8.41,5.05,7.55,3.36,5.36,4,null,6.13,8.1300000000000008,3.13,3.05,4.3181818181818192,6.6470000000000002]
[4,null,null,null,null,"B",null,null,null,null,null,null,{"$f":"DerivingPerfReq(O7:AJ7)","v":6.1},6.6999999999999993,4.5999999999999996,6.6,null,null,3.68,5.91,3.3,5.8,3,5.5,4.2,6.7,null,null,null,null,null,null,null,null,8.6999999999999993,10.7,5.6999999999999993,5.1999999999999993,4.5799999999999992,6.8683333333333323]
[]
[5,1,"15kHz","CP-OFDM","20MHz","A",16,"16QAM","TDLC300-100","TDLC300-100",2,"HomNet set1: (-1.11. -10.91)",{"$f":"DerivingPerfReq(O9:AJ9)","v":6.6},7.1999999999999993,4.8,6.8,4.5,6.5,4.21,6.62,4.8,7.3,3.3,5.8,4.5,7,4.5,7,5.97,8.4700000000000006,3.68,5.68,3.2,null,6.04,8.0399999999999991,2.84,2.7900000000000009,4.5000000000000009,6.9210000000000012]
[6,null,null,null,null,"B",null,null,null,null,null,null,{"$f":"DerivingPerfReq(O10:AJ10)","v":6.7},7.3,4.8,6.8,null,null,4.32,6.65,4.9000000000000004,7.4,3.4,5.9,4.3,6.8,null,null,null,null,null,null,null,null,8.9700000000000006,10.97,5.57,5.07,5.1150000000000011,7.419999999999999]
[]
[7,1,"15kHz","CP-OFDM","20MHz","A",16,"16QAM","TDLA30-10","TDLC300-100",2,"HetNet set2: (-0.43. -13.78)",{"$f":"DerivingPerfReq(O12:AJ12)","v":6.8},7.3999999999999995,4.8,6.8,4.5,6.5,3.79,6.13,3.6,6.1,3,5.5,4.4000000000000004,6.9,5.58,8.08,5.4,7.9,3.9,5.9,4.0999999999999996,null,6.25,8.25,3.25,2.75,4.4836363636363634,6.806]
[8,null,null,null,null,"B",null,null,null,null,null,null,{"$f":"DerivingPerfReq(O13:AJ13)","v":6.2},6.8,4.8,6.8,null,null,3.92,6.09,3.7,6.2,2.9,5.4,4.0999999999999996,6.6,null,null,null,null,null,null,null,null,9.32,11.32,6.42,5.92,4.79,7.0683333333333342]
[]
[]
[]
[]
["case ","Tx","SCS","Waveform ","BW","Mapping Type","MCS for target cell","MCS for interferer cell","Propagation condition for target cell","Propagation conditon for interferer cell ","Number of Interferer cells","DIP set","38.104 req","38.141-1/2 req","Samsung",null,"Huawei",null,"Ericsson",null,"ZTE",null,"Nokia",null,"CTC",null,"QC",null,"CATT",null,"CMCC",null,"Tejas Networks",null,"NTT DOCOMO",null,"SPAN",null,"AVERAGE"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Ideal","impairment","ideal","impairment","ideal","impairment","ideal","impairment","ideal","impairment","ideal","impairment","ideal","impairment"," ideal","impairment","ideal","impairment","ideal","impairment"," ideal","impairment","Ideal","Ideal","Ideal","Impairment"]
[1,1,"30kHz","CP-OFDM","10MHz","A",16,"16QAM","TDLC300-100","TDLC300-100",2,"HomNet set1: (-1.11. -10.91)",{"$f":"DerivingPerfReq(O20:AJ20)","v":6.7},{"$f":"IF(M20>-100,M20+0.6,M20)","v":7.3},5.2,7.2,4.3,6.3,4.34,6.66,4.7,7.2,3.9,6.4,4.3,6.8,4.91,7.41,6.25,8.75,3.27,5.27,3.7,null,5.91,7.91,{"$f":"MAX(O20,Q20,S20,U20,W20,Y20,AA20,AC20,AE20,AG20,AI20)-MIN(O20,Q20,S20,U20,W20,Y20,AA20,AC20,AE20,AG20,AI20)","v":2.98},{"$f":"MAX(P20,R20,T20,V20,X20,Z20,AB20,AD20,AF20,AH20,AJ20)-MIN(P20,R20,T20,V20,X20,Z20,AB20,AD20,AF20,AH20,AJ20)","v":3.4800000000000004},{"$f":"AVERAGE(O20,Q20,S20,U20,W20,Y20,AA20,AC20,AE20,AG20,AI20)","v":4.6163636363636362},{"$f":"AVERAGE(P20,R20,T20,V20,X20,Z20,AB20,AD20,AF20,AH20,AJ20)","v":6.9899999999999993}]
[2,null,null,null,null,"B",null,null,null,null,null,null,{"$f":"DerivingPerfReq(O21:AJ21)","v":6.9},{"$f":"IF(M21>-100,M21+0.6,M21)","v":7.5},5.2,7.2,null,null,4.3600000000000003,6.53,4.8,7.3,3.9,6.4,4.4000000000000004,6.9,null,null,null,null,null,null,null,null,6.39,8.39,{"$f":"MAX(O21,Q21,S21,U21,W21,Y21,AA21,AC21,AE21,AG21,AI21)-MIN(O21,Q21,S21,U21,W21,Y21,AA21,AC21,AE21,AG21,AI21)","v":2.4899999999999998},{"$f":"MAX(P21,R21,T21,V21,X21,Z21,AB21,AD21,AF21,AH21,AJ21)-MIN(P21,R21,T21,V21,X21,Z21,AB21,AD21,AF21,AH21,AJ21)","v":1.9900000000000002},{"$f":"AVERAGE(O21,Q21,S21,U21,W21,Y21,AA21,AC21,AE21,AG21,AI21)","v":4.8416666666666659},{"$f":"AVERAGE(P21,R21,T21,V21,X21,Z21,AB21,AD21,AF21,AH21,AJ21)","v":7.12}]
[]
[3,1,"30kHz","CP-OFDM","10MHz","A",16,"16QAM","TDLA30-10","TDLC300-100",2,"HetNet set2: (-0.43. -13.78)",{"$f":"DerivingPerfReq(O23:AJ23)","v":6.5},7.1,5,7,4.3,6.3,4.09,6.41,4.3,6.8,3.3,5.8,4.2,6.7,6.2,8.6999999999999993,5.0999999999999996,7.6,3.3,5.3,4.8,null,6.33,8.33,3.0300000000000002,3.3999999999999995,4.6290909090909089,6.894000000000001]
[4,null,null,null,null,"B",null,null,null,null,null,null,{"$f":"DerivingPerfReq(O24:AJ24)","v":6.7},7.3,5,8.1,null,null,4.13,6.3,4.4000000000000004,6.9,3.3,5.8,4,6.5,null,null,null,null,null,null,null,null,7.06,9.06,3.76,3.2600000000000007,4.6483333333333325,7.1099999999999994]
[]
[5,1,"30kHz","CP-OFDM","100MHz","A",16,"16QAM","TDLC300-100","TDLC300-100",2,"HomNet set1: (-1.11. -10.91)",{"$f":"DerivingPerfReq(O26:AJ26)","v":6.7},7.3,5.2,7.2,4.5999999999999996,6.6,4.24,6.47,4.2,6.7,3.8,6.3,4.8,7.3,4.67,7.17,7.2,9.6999999999999993,3.49,5.49,3.7,null,5.9,6.9,3.71,4.2099999999999991,4.7090909090909099,6.9829999999999997]
[6,null,null,null,null,"B",null,null,null,null,null,null,{"$f":"DerivingPerfReq(O27:AJ27)","v":6.9},7.5,5.4,7.4,null,null,4.28,6.73,4.2,6.7,3.8,6.3,4.9000000000000004,7.4,null,null,null,null,null,null,null,null,6.42,8.42,2.62,2.12,4.833333333333333,7.1583333333333341]
[]
[7,1,"30kHz","CP-OFDM","100MHz","A",16,"16QAM","TDLA30-10","TDLC300-100",2,"HetNet set2: (-0.43. -13.78)",{"$f":"DerivingPerfReq(O29:AJ29)","v":6.5},7.1,4.5999999999999996,6.6,4.7,6.7,4.24,6.6,4.5,7,3.5,6,4.5999999999999996,7.1,5.63,8.1300000000000008,6.49,8.99,3.48,5.48,4.5999999999999996,null,6.23,8.23,3.0100000000000002,3.51,4.7790909090909084,7.0830000000000011]
[8,null,null,null,null,"B",null,null,null,null,null,null,{"$f":"DerivingPerfReq(O30:AJ30)","v":6.6},7.1999999999999993,4.5,6.5,null,null,4.3099999999999996,6.43,4.5,7,3.6,6.1,4.5,7,null,null,null,null,null,null,null,null,7.34,9.34,3.7399999999999998,3.24,4.791666666666667,7.0616666666666674]
[56,null,null,null,null,"B",null,null,null,null,null,null,null,{"$f":"IF(M31>100,M31+0.6,M31)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]