{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["TDoc_List","CR_Packs_List","Parameters"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":6,"comments":1,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"TDoc_List","index":0,"n_rows":1827,"n_cols":31,"rows_kept":1827,"cut":false,"hidden":false,"merged":[]}
["TDoc","Title","Source","Contact","Contact ID","Type","For","Abstract","Secretary Remarks","Agenda item sort order","Agenda item","Agenda item description","TDoc sort order within agenda item","TDoc Status","Reservation date","Uploaded","Is revision of","Revised to","Release","Spec","Version","Related WIs","CR","CR revision","CR category","TSG CR Pack","Reply to","To","Cc","Original LS","Reply in"]
["R4-1704500","Agenda for RAN4#83","Samsung Electronics Co., Ltd","Xutao Zhou","40317","agenda","Approval","","","2","2","Approval of the agenda",45000,"approved","2017-04-26T13:56:31.357","2017-05-04T13:17:52.297","","","","","","","","","","","","","","",""]
["R4-1704501","RAN4#82bis Meeting Report","MCC","Kyoungseok Oh","70239","report","Approval","","","3","3","Letters / reports from other groups / meetings",45010,"approved","2017-04-26T13:56:31.437","2017-05-11T08:06:51.440","","","","","","","","","","","","","","",""]
["R4-1704502","LS on CRS muting in eFeMTC","RAN1, Nokia","Kyoungseok Oh","70239","LS in","Discussion","","","3","3","Letters / reports from other groups / meetings",45020,"noted","2017-04-26T13:56:31.467","2017-05-02T16:17:51.110","","","Rel-15","","","LTE_eMTC4","","","","","","RAN4","","R1-1706734",""]
["R4-1704503","LS regarding 1024QAM","RAN1, Qualcomm","Kyoungseok Oh","70239","LS in","Discussion","","","3","3","Letters / reports from other groups / meetings",45030,"noted","2017-04-26T13:56:31.513","2017-05-02T16:17:51.127","","","Rel-14","","","LTE_1024QAM_DL-Core","","","","","","RAN4","","R1-1706842",""]
["R4-1704504","LS on RAN1 agreements for FeD2D study item","RAN1, Intel","Kyoungseok Oh","70239","LS in","Discussion","","","3","3","Letters / reports from other groups / meetings",45040,"noted","2017-04-26T13:56:31.547","2017-05-02T16:17:51.127","","","Rel-15","","","FS_feD2D_IoT_relay_wearable","","","","","","RAN2, RAN4","","R1-1706843",""]
["R4-1704505","LS reply on TM10 / FD-MIMO UE capability signalling","RAN1, Intel","Kyoungseok Oh","70239","LS in","Discussion","","","3","3","Letters / reports from other groups / meetings",45050,"noted","2017-04-26T13:56:31.577","2017-05-02T16:17:51.143","","","Rel-14","","","LTE_EBF_FDMIMO-Core","","","","","R1-1704177","RAN2, RAN4","","R1-1706856",""]
["R4-1704506","LS response on applicability of requirements to any category UE with CE support","RAN2, Intel","Kyoungseok Oh","70239","LS in","Discussion","","","3","3","Letters / reports from other groups / meetings",45060,"noted","2017-04-26T13:56:31.623","2017-05-02T16:17:51.143","","","Rel-13","","","LTE_MTCe2_L1-Core","","","","","R4-1702482","RAN4","","R2-1703838",""]
["R4-1704507","Reply LS on new event reporting for enhanced RLM for eNB-IoT and feMTC","RAN2, Intel","Kyoungseok Oh","70239","LS in","Discussion","","","3","3","Letters / reports from other groups / meetings",45070,"noted","2017-04-26T13:56:31.653","2017-05-02T16:17:51.157","","","Rel-14","","","NB_IOTenh-Core, LTE_feMTC-Core","","","","","R4-1702469, R4-1702483","RAN4","","R2-1703841",""]
["R4-1704508","Clarification on NCSG applicability to non-CA cases","RAN2, Qualcomm","Kyoungseok Oh","70239","LS in","Discussion","","","3","3","Letters / reports from other groups / meetings",45080,"noted","2017-04-26T13:56:31.700","2017-05-02T16:17:51.157","","","Rel-14","","","LTE_meas_gap_enh","","","","","","RAN4","","R2-1703948",""]
["R4-1704509","LS on the feasibility of DC-related mobility enhancements in NR","RAN2, Intel","Kyoungseok Oh","70239","LS in","Discussion","","","3","3","Letters / reports from other groups / meetings",45090,"noted","2017-04-26T13:56:31.717","2017-05-02T16:17:51.157","","","Rel-15","","","NR_newRAT-Core","","","","","","RAN1, RAN4","","R2-1703971",""]
["R4-1704510","TP for TR36.714-04-01: the support of CA_4DL_1A-3A-5A-41A_1UL_BCS0","China Telecommunications","Hongliang Bian","45685","pCR","Approval","This paper investigates all the necessary elements to complete CA_1A-3A-5A-41A.","","107","7.4.2","UE RF (36.101) [LTE_CA_R14_4DL1UL-Core]",48930,"approved","2017-04-27T01:36:54.657","2017-05-05T05:53:26.370","","","Rel-14","36.714-04-01","0.6.0","LTE_CA_R14_4DL1UL-Core","","","","","","","","",""]
["R4-1704511","Working Procedure for LTE-NR combinations","KDDI Corporation","Masaaki Obara","46347","other","Approval","This contribution proposes working procedure for LTE-NR combinations in RAN4.","","416","10.2.2","NR-LTE band combinations proposals [NR_newRAT]",47590,"noted","2017-04-27T04:21:49.903","2017-04-28T09:29:35.560","","","Rel-15","","","","","","","","","","","",""]
["R4-1704512","Addition of Band 28 UE category 1bis into TS36.101","Telstra Corporation Limited","Meng Wang","68589","CR","Approval","","","231","7.19.2","UE RF (36.101) [LTE_UE_cat_1RX-Core]",45120,"endorsed","2017-04-27T06:01:00.440","2017-04-27T06:34:33.130","","","Rel-14","36.101","14.3.0","LTE_UE_cat_1RX-Core","4379","","F","","","","","",""]
["R4-1704513","Discussion on the supporting stand-alone and guard-band RRM test for NB-IoT","China Telecommunications","Chen Shuzhen","71976","CR","Discussion","The purpose of the discussion is to adding stand-alone and guard-band mode test cases for NB-IoT RRM test, because the current 3GPP TS 36.133 only defines the in-band mode for NB-IoT RRM test.","","62","5.5.5","RRM Performance (36.133) [NB_IOT-Perf]",574000,"withdrawn","2017-04-27T08:15:20.283",null,"","","Rel-13","36.133","13.7.0","NB_IOT-Perf","4832","","B","","","","","",""]
["R4-1704514","LAA RRM: Correction to test case A.9.11.x and A.9.12.x (Rel-13)","Rohde & Schwarz","Bledar Karajani","41759","CR","Agreement","","","38","5.3.5","RRM Performance (36.133) [LTE_LAA-Perf]",45140,"agreed","2017-04-27T11:22:05.813","2017-05-05T09:53:05.363","","R4-1705974","Rel-13","36.133","13.7.0","LTE_LAA-Perf","4833","","F","RP-171307","","","","",""]
["R4-1704515","LAA RRM: Correction to test case A.9.11.x and A.9.12.x (Rel-14)","Rohde & Schwarz","Bledar Karajani","41759","CR","Agreement","","","38","5.3.5","RRM Performance (36.133) [LTE_LAA-Perf]",45150,"agreed","2017-04-27T11:22:06.750","2017-05-23T15:07:50.570","","","Rel-14","36.133","14.3.0","LTE_LAA-Perf","4834","","A","RP-171307","","","","",""]
["R4-1704516","eMTC RRM: Correction to MPDCCH and PDSCH Reference Measurement Channels (Rel-13)","Rohde & Schwarz","Bledar Karajani","41759","CR","Agreement","","","49","5.4.5","RRM performance (36.133) [LTE_MTCe2_L1-Perf]",45170,"agreed","2017-04-27T11:22:07.623","2017-05-05T11:41:51.867","","","Rel-13","36.133","13.7.0","LTE_MTCe2_L1-Perf","4835","","F","RP-171309","","","","",""]
["R4-1704517","eMTC RRM: Correction to MPDCCH and PDSCH Reference Measurement Channels (Rel-14)","Rohde & Schwarz","Bledar Karajani","41759","CR","Agreement","","","49","5.4.5","RRM performance (36.133) [LTE_MTCe2_L1-Perf]",617500,"agreed","2017-04-27T11:22:08.747","2017-05-23T15:07:50.587","","","Rel-14","36.133","14.3.0","LTE_MTCe2_L1-Perf","4836","","A","RP-171309","","","","",""]
["R4-1704518","InDoPos: Corrections to BT-LE requirements (Rel-14)","Rohde & Schwarz","Bledar Karajani","41759","CR","Agreement","","","252","7.23.2.2","RAT-independent enhancement [UTRA_LTE_iPos_enh2-Perf]",45200,"agreed","2017-04-27T11:22:09.650","2017-05-05T11:11:15.723","","","Rel-14","37.171","14.1.0","UTRA_LTE_iPos_enh2-Perf","0012","","F","RP-171270","","","","",""]
["R4-1704519","InDoPos: New WLAN delay test case in nominal conditions with LTE FDD and TDD (Rel-14)","Rohde & Schwarz","Bledar Karajani","41759","CR","","","","252","7.23.2.2","RAT-independent enhancement [UTRA_LTE_iPos_enh2-Perf]",50060,"revised","2017-04-27T11:22:10.620","2017-05-05T09:53:05.363","","R4-1706027","Rel-14","37.171","14.1.0","UTRA_LTE_iPos_enh2-Perf","0013","","F","","","","","",""]
["R4-1704520","InDoPos: New WLAN delay test case in dynamic range conditions with LTE FDD and TDD (Rel-14)","Rohde & Schwarz","Bledar Karajani","41759","CR","","","","252","7.23.2.2","RAT-independent enhancement [UTRA_LTE_iPos_enh2-Perf]",50070,"revised","2017-04-27T11:22:11.727","2017-05-05T09:53:05.380","","R4-1706028","Rel-14","37.171","14.1.0","UTRA_LTE_iPos_enh2-Perf","0014","","F","","","","","",""]
["R4-1704521","CR on applicability of V2X contiguous intraband multi-carrier  operation requirements.","Qualcomm Inc.","TIen Viet NGUYEN","67205","CR","Approval","Reason for change:Clarify the applicability of V2X contiguous intraband multi-carrier requirements.Summary of change:The current V2X contiguous intraband multi-carrier operation requirements assume that there are multiple active transmissions on al","","177","7.16.2","UE RF Maintenance (36.101) [LTE_V2X-Core]",45210,"revised","2017-04-27T16:09:16.150","2017-05-05T18:44:00.417","","R4-1705879","Rel-14","36.101","14.3.0","LTE_SL_V2V-Core","4380","","F","","","","","",""]
["R4-1704522","CR on side condition for reliability of GNSS","QualcommInc.","TIen Viet NGUYEN","67205","CR","Agreement","Fix the side condition table is missing information. The reference timing is duplicated with RAN2 specification (TS36.331) \n\nFix the side condition table. Fix the reference timing according to TS36.331\n\nSide condition for GNSS reliability is not complete.","","169","7.15.2","RRM core maintenance (36.133) [LTE_SL_V2V-Core]",45220,"agreed","2017-04-27T16:30:13.717","2017-05-05T18:44:00.417","","","Rel-14","36.133","14.3.0","LTE_SL_V2V-Core","4837","","F","RP-171281","","","","",""]
["R4-1704523","Enlarging maximum BWs of Band 8 in NR","SoftBank Corp.","Kenichi Kihara","41094","other","Approval","This paper is resubmission of R4-1702772, mainly to confirm whether Korean Band 8 needs A-MPR against Band 5 or not.","","415","10.2.1.2","Band definition for NR bands [NR_newRAT]",605300,"approved","2017-04-27T23:54:39.810","2017-04-28T00:32:18.337","","","Rel-15","","","NR_newRAT","","","","","","","","",""]
["R4-1704524","On synchronization raster concept in NR","SoftBank Corp.","Kenichi Kihara","41094","other","Approval","This paper is intended to address issues around synchronization raster in RAN4 RF context and propose to  investigate synchronization raster and relevant RF issues as a package.","","419","10.3.2","Channel Raster [NR_newRAT]",46830,"noted","2017-04-28T00:00:29.603","2017-05-02T10:28:59.173","","","Rel-15","","","NR_newRAT","","","","","","","","",""]
["R4-1704525","A-GNSS in V2V performance test","Qualcomm Inc.","TIen Viet NGUYEN","67205","discussion","Approval","Observation 1: In a testing environment, as long as the signal is the replicated signal of the real satellites, there is no need for almanac to obtain a fix.\nObservation 2: With strong enough GNSS reception signal, one can expect that a typical GNSS recei","","170","7.15.3","RRM performance (36.133) [LTE_SL_V2V-Perf]",45250,"noted","2017-04-28T02:23:42.830","2017-05-05T18:44:00.430","","","Rel-14","","","","","","","","","","","",""]
["R4-1704526","Corrections of Table 8.7.5.1-2 and Table 8.7.5.2-2","Korea Testing Laboratory","Song Raphael","38072","CR","Agreement","Add the 10+10 bandwidth combination set into Table 8.7.5.1-2 and Table 8.7.5.2-2","","98","7.2.5","Other Specifications [LTE_CA_R14_2DL1UL-Core]",569300,"revised","2017-04-28T09:37:22.567","2017-05-04T13:18:54.137","","R4-1706011","Rel-13","36.101","13.7.0","LTE_CA_R14_2DL1UL-Core","4381","","F","","","","","",""]
["R4-1704527","Additional information of LTE BHH TRPTRS measurement results","NTT DOCOMO INC.","Takayuki Furuta","72176","other","Discussion","This contribution is for discussion.","","140","7.10.2","Hand phantom for smartphones [LTE_UTRA_TRP_TRS-Core]",45270,"noted","2017-05-01T08:44:14.367","2017-05-05T14:45:42.760","","","","","","","","","","","","","","",""]
["R4-1704528","Measurement results of re-testing PAD devices for lab alignment test activity","NTT DOCOMO INC.","Takayuki Furuta","72176","other","Discussion","This contribution provides measurement results of re-testing.","","145","7.11.2","Performance requirements [LTE_MIMO_OTA-Core]",46580,"noted","2017-05-01T08:47:55.163","2017-05-02T09:34:24.280","","","","","","","","","","","","","","",""]
["R4-1704529","MIMO OTA measurement results for band 1 and 19","NTT DOCOMO INC.","Takayuki Furuta","72176","other","Discussion","This contribution provides measurement results for band 1 and 19.","","145","7.11.2","Performance requirements [LTE_MIMO_OTA-Core]",46590,"noted","2017-05-01T08:49:42.520","2017-05-23T15:07:50.603","","","","","","","","","","","","","","",""]
["R4-1704530","Reference measurement results for band 1 and 19","NTT DOCOMO INC.","Takayuki Furuta","72176","other","Information","","","145","7.11.2","Performance requirements [LTE_MIMO_OTA-Core]",47510,"withdrawn","2017-05-01T08:54:28.043",null,"","","","","","","","","","","","","","",""]
["R4-1704531","NR ? UE Power Class definition for cmW and mmW ranges","InterDigital, Inc.","Virgil Comsa","72096","other","Approval","In this contribution we discussed the Power Class definition for the cmW and mmW :\nProposals:\nProposal 1:  Power class definition should include a testable TRP limit (reachable) which should account generically for multiple simultaneous beams transmission","","427","10.4.3.1","UE power class and MPR/A-MPR [NR_newRAT]",51070,"noted","2017-05-01T15:57:47.073","2017-05-05T16:53:37.977","","","Rel-15","","","","","","","","","","","",""]
["R4-1704532","Discussion on set of configuration values for SS burst set periodicity","LG Electronics Inc.","YOONOH YANG","47033","discussion","Discussion","It proivides our view on potential issues and set of configuration values for SS burst set periodicity.","","411","10.1.2","Topics related to incoming LS from other WG [NR_newRAT]",45320,"noted","2017-05-01T23:15:38.303","2017-05-02T02:13:44.393","","","Rel-15","","","","","","","","","","","",""]
["R4-1704533","Reply LS on set of configuration values for SS burst set periodicity","LG Electronics Inc.","YOONOH YANG","47033","LS out","Approval","","","411","10.1.2","Topics related to incoming LS from other WG [NR_newRAT]",47990,"noted","2017-05-01T23:20:03.217","2017-05-02T02:13:44.393","","","Rel-15","","","","","","","","R4-1704311, ¡°LS on set of configuration values for SS burst set periodicity¡±","RAN1","","",""]
["R4-1704534","Discussion on NR cell identification","LG Electronics Inc.","YOONOH YANG","47033","discussion","Discussion","It provides our view on NR cell detection time and the factors to impact the cell detection time such as searching synchronization signal frequency raster, the number of SS blocks in SS burst set periodicity, UE Rx beam capability and how to design measur","","452","10.6.4","Expected Measurement requirements for NSA [NR_newRAT]",50160,"noted","2017-05-01T23:21:30.030","2017-05-02T02:13:44.393","","","Rel-15","","","","","","","","","","","",""]
["R4-1704535","Motivation for Study of RF measurement methodology for 5G vehicular device","LG Electronics Inc.","YOONOH YANG","47033","SID new","Information","It is motivation to study of RF measurment methodology for 5G vehicle device.","","473","13","Revision of the Work Plan",45630,"noted","2017-05-01T23:24:14.980","2017-05-02T02:13:44.410","","","","","","","","","","","","","","",""]
["R4-1704536","Discussion on GNSS side conditions for V2V performance requirements","LG Electronics Inc.","YOONOH YANG","47033","discussion","Discussion","It provides our view on down-selection between 2 GNSS side conditions and summarizes questions to get input on the 2 GNSS side condtions from RAN4.","","170","7.15.3","RRM performance (36.133) [LTE_SL_V2V-Perf]",56600,"noted","2017-05-01T23:26:26.813","2017-05-02T02:13:44.410","","","Rel-14","","","","","","","","","","","",""]
["R4-1704537","Discussion on V2X RRM test cases","LG Electronics Inc.","YOONOH YANG","47033","discussion","Discussion","It provides our view on V2X RRM test cases based on the agreement in the RAN4 last meeting.","","179","7.16.4","RRM performance (36.133) [LTE_V2X-Perf]",45370,"noted","2017-05-01T23:27:39.397","2017-05-02T02:13:44.410","","","Rel-14","","","","","","","","","","","",""]
["R4-1704538","Initial discussion on intra-frequency measurement for NR","LG Electronics Inc.","Jin-yup Hwang","47026","discussion","Discussion","","","455","10.6.7","UE architecture [NR_newRAT]",45380,"noted","2017-05-01T23:37:55.727","2017-05-04T13:31:48.177","","","","","","","","","","","","","","",""]
["R4-1704539","Necessity of TRP BS output power requirement for NR","NTT DOCOMO, INC.","Suguru Okuyama","61038","other","Approval","","","442","10.5.3.4","Other Tx requirements [NR_newRAT]",49530,"noted","2017-05-02T00:14:24.193","2017-05-02T08:50:32.597","","","Rel-15","","","NR_newRAT","","","","","","","","",""]
["R4-1704540","Target specs for NR BS","NTT DOCOMO, INC.","Suguru Okuyama","61038","other","Approval","","","436","10.5.1","BS RF General (ad-hoc MoM, Plan, Spec structure) [NR_newRAT]",49510,"noted","2017-05-02T00:14:24.210","2017-05-02T08:50:32.627","","","Rel-15","","","NR_newRAT","","","","","","","","",""]
["R4-1704541","Proposal on NR BS beam related requirements","NTT DOCOMO, INC.","Suguru Okuyama","61038","other","Approval","","","436","10.5.1","BS RF General (ad-hoc MoM, Plan, Spec structure) [NR_newRAT]",52980,"noted","2017-05-02T00:14:24.223","2017-05-02T08:50:32.627","","","Rel-15","","","NR_newRAT","","","","","","","","",""]
["R4-1704542","Proposal on below 6GHz NR BS unwanted emission mask requirement","NTT DOCOMO, INC.","Suguru Okuyama","61038","other","Approval","","","440","10.5.3.2","Unwanted emission requirements [NR_newRAT]",52860,"noted","2017-05-02T00:14:24.240","2017-05-02T08:50:32.643","","","Rel-15","","","NR_newRAT","","","","","","","","",""]
["R4-1704543","Proposal on ACLR requirement for NR BS","NTT DOCOMO, INC.","Suguru Okuyama","61038","other","Approval","","","440","10.5.3.2","Unwanted emission requirements [NR_newRAT]",583200,"withdrawn","2017-05-02T00:14:24.270",null,"","","Rel-15","","","NR_newRAT","","","","","","","","",""]
["R4-1704544","Proposal on occupied bandwidth requirement for NR BS","NTT DOCOMO, INC.","Suguru Okuyama","61038","other","Approval","","","440","10.5.3.2","Unwanted emission requirements [NR_newRAT]",583300,"approved","2017-05-02T00:14:24.270","2017-05-02T08:50:32.643","","","Rel-15","","","NR_newRAT","","","","","","","","",""]
["R4-1704545","Proposal on NR BS EVM requirements","NTT DOCOMO, INC.","Suguru Okuyama","61038","other","Approval","","","439","10.5.3.1","EVM requirements [NR_newRAT]",45450,"noted","2017-05-02T00:14:24.287","2017-05-02T08:50:32.643","","","Rel-15","","","NR_newRAT","","","","","","","","",""]
["R4-1704546","TRP accuracy value","NTT DOCOMO, INC.","Suguru Okuyama","61038","other","Approval","","","358","9.12.2.1","TRP accuracy [AASenh_BS_LTE_UTRA-Core]",45460,"noted","2017-05-02T00:14:24.287","2017-05-02T08:50:32.643","","","Rel-15","","","AASenh_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-1704547","TX/RX loss factors for OTA in-band/out-of-band requirements","NTT DOCOMO, INC.","Suguru Okuyama","61038","other","Approval","","","359","9.12.2.2","Tx and Rx loss values [AASenh_BS_LTE_UTRA-Core]",45470,"noted","2017-05-02T00:14:24.303","2017-05-02T08:50:32.657","","","Rel-15","","","AASenh_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-1704548","Introduction of the FDD L-band (Band 74) into TS 36.104","NTT DOCOMO, INC.","Suguru Okuyama","61038","draftCR","Endorsement","This draft CR is for Endorsement. Formal CR will be sumbitted in RAN4#84 based on this endorsed version.","","317","9.4.3","BS RF (36.104, 36.141) [LTE_FDD_L_Band-core/Perf]",45480,"revised","2017-05-02T00:14:24.303","2017-05-02T08:50:32.657","","R4-1705926","Rel-15","36.104","14.3.0","LTE_FDD_L_Band-Core","","","","","","","","",""]
["R4-1704549","Introduction of the FDD L-band (Band 74) into TS 36.141","NTT DOCOMO, INC.","Suguru Okuyama","61038","draftCR","Endorsement","This draft CR is for Endorsement. Formal CR will be sumbitted in RAN4#84 based on this endorsed version.","","317","9.4.3","BS RF (36.104, 36.141) [LTE_FDD_L_Band-core/Perf]",49710,"revised","2017-05-02T00:14:24.317","2017-05-02T08:50:32.673","","R4-1705927","Rel-15","36.141","14.3.0","LTE_FDD_L_Band-Perf","","","","","","","","",""]
["R4-1704550","Introduction of the FDD L-band (Band 74) into TS 36.113","NTT DOCOMO, INC.","Suguru Okuyama","61038","draftCR","Endorsement","This draft CR is for Endorsement. Formal CR will be sumbitted in RAN4#84 based on this endorsed version.","","319","9.4.5","Other specifications [LTE_FDD_L_Band]",45520,"endorsed","2017-05-02T00:14:24.333","2017-05-02T08:50:32.673","","","Rel-15","36.113","14.2.0","LTE_FDD_L_Band","","","","","","","","",""]
["R4-1704551","Introduction of the FDD L-band (Band 74) into TS 25.104","NTT DOCOMO, INC.","Suguru Okuyama","61038","draftCR","Endorsement","This draft CR is for Endorsement. Formal CR will be sumbitted in RAN4#84 based on this endorsed version.","","319","9.4.5","Other specifications [LTE_FDD_L_Band]",45521,"revised","2017-05-02T00:14:24.350","2017-05-02T08:50:32.673","","R4-1705928","Rel-15","25.104","14.1.0","LTE_FDD_L_Band","","","","","","","","",""]
["R4-1704552","Introduction of the FDD L-band (Band 74) into TS 25.141","NTT DOCOMO, INC.","Suguru Okuyama","61038","draftCR","Endorsement","This draft CR is for Endorsement. Formal CR will be sumbitted in RAN4#84 based on this endorsed version.","","319","9.4.5","Other specifications [LTE_FDD_L_Band]",45531,"revised","2017-05-02T00:14:24.350","2017-05-02T08:50:32.673","","R4-1705930","Rel-15","25.141","14.1.0","LTE_FDD_L_Band","","","","","","","","",""]
["R4-1704553","Introduction of the FDD L-band (Band 74) into TS 37.104","NTT DOCOMO, INC.","Suguru Okuyama","61038","draftCR","Endorsement","This draft CR is for Endorsement. Formal CR will be sumbitted in RAN4#84 based on this endorsed version.","","319","9.4.5","Other specifications [LTE_FDD_L_Band]",45541,"revised","2017-05-02T00:14:24.367","2017-05-02T08:50:32.673","","R4-1705931","Rel-15","37.104","14.3.0","LTE_FDD_L_Band","","","","","","","","",""]
["R4-1704554","Introduction of the FDD L-band (Band 74) into TS 37.113","NTT DOCOMO, INC.","Suguru Okuyama","61038","draftCR","Endorsement","This draft CR is for Endorsement. Formal CR will be sumbitted in RAN4#84 based on this endorsed version.","","319","9.4.5","Other specifications [LTE_FDD_L_Band]",45720,"endorsed","2017-05-02T00:14:24.380","2017-05-02T08:50:32.673","","","Rel-15","37.113","14.1.0","LTE_FDD_L_Band","","","","","","","","",""]
["R4-1704555","Introduction of the FDD L-band (Band 74) into TS 37.141","NTT DOCOMO, INC.","Suguru Okuyama","61038","draftCR","Endorsement","This draft CR is for Endorsement. Formal CR will be sumbitted in RAN4#84 based on this endorsed version.","","319","9.4.5","Other specifications [LTE_FDD_L_Band]",45721,"revised","2017-05-02T00:14:24.380","2017-05-02T08:50:32.690","","R4-1705932","Rel-15","37.141","14.3.0","LTE_FDD_L_Band","","","","","","","","",""]
["R4-1704556","Remaining issues for BS IC receiver","China Telecom","Shan Yang","48340","discussion","Discussion","","","298","8.1.1","General [FS_LTE _IC_BS]",600800,"noted","2017-05-02T02:47:56.753","2017-05-04T08:37:51.770","","","Rel-15","","","","","","","","","","","",""]
["R4-1704557","Updated summary of BS IC simulation results without time and frequency offset","China Telecom","Shan Yang","48340","other","Information","","","300","8.1.3","Link level evaluation [FS_LTE _IC_BS]",51750,"noted","2017-05-02T02:47:56.767","2017-05-23T15:07:50.603","","","Rel-15","","","","","","","","","","","",""]
["R4-1704558","Updated summary of BS IC simulation results with time and frequency offset","China Telecom","Shan Yang","48340","other","Information","","","300","8.1.3","Link level evaluation [FS_LTE _IC_BS]",51760,"noted","2017-05-02T02:47:56.783","2017-05-23T15:07:50.617","","","Rel-15","","","","","","","","","","","",""]
["R4-1704559","TR 36.766 V1.1.0: Study on interference cancellation receiver for LTE BS","China Telecom, Huawei","Shan Yang","48340","draft TR","Approval","","","298","8.1.1","General [FS_LTE _IC_BS]",45590,"agreed","2017-05-02T02:47:56.800","2017-05-04T08:32:00.840","","","Rel-15","36.766","1.1.0","FS_LTE_IC_BS","","","","","","","","",""]
["R4-1704560","TP on additional simulation results for BS IC without TO/FO","China Telecom","Shan Yang","48340","pCR","Approval","","","298","8.1.1","General [FS_LTE _IC_BS]",51770,"approved","2017-05-02T02:47:59.950","2017-05-23T15:07:50.617","","","Rel-15","36.766","1.0.0","FS_LTE_IC_BS","","","","","","","","",""]
["R4-1704561","Editorial TP for TR 36.766","China Telecom","Shan Yang","48340","pCR","Approval","","","298","8.1.1","General [FS_LTE _IC_BS]",45600,"approved","2017-05-02T02:47:59.997","2017-05-04T08:32:00.840","","","Rel-15","36.766","1.0.0","FS_LTE_IC_BS","","","","","","","","",""]
["R4-1704562","TP on TR conclusions","China Telecom","Shan Yang","48340","pCR","Approval","","","298","8.1.1","General [FS_LTE _IC_BS]",45610,"revised","2017-05-02T02:48:00.043","2017-05-04T08:32:00.840","","R4-1706007","Rel-15","36.766","1.0.0","FS_LTE_IC_BS","","","","","","","","",""]
["R4-1704563","Motivation for new WI on  Performance requirements of interference cancellation receiver for LTE BS","China Telecom","Shan Yang","48340","other","Information","","","473","13","Revision of the Work Plan",45640,"noted","2017-05-02T02:48:00.077","2017-05-04T08:32:00.840","","","Rel-15","","","","","","","","","","","",""]
["R4-1704564","Draft WID on performance requirements of interference cancellation receiver for LTE BS","China Telecom","Shan Yang","48340","other","Information","","","473","13","Revision of the Work Plan",46490,"noted","2017-05-02T02:48:00.077","2017-05-04T08:32:00.857","","","Rel-15","","","","","","","","","","","",""]
["R4-1704565","On NR Maximum Channel Bandwidth","Qualcomm Incorporated","Valentin Gheorghiu","43117","discussion","Discussion","in this paper we explain the rationale behind the proposals in the NR maximum channel bandwidth way forward","","418","10.3.1","Channel bandwidth and subcarrier spacing [NR_newRAT]",45650,"noted","2017-05-02T07:26:41.943","2017-05-05T13:35:52.117","","","","","","","","","","","","","","",""]
["R4-1704566","WF on Maximum Channel Bandwidth","Qualcomm Incorporated","Valentin Gheorghiu","43117","other","Approval","In this WF we make several proposals related to the maximum channel bandwidth and forward compatibility of introducing new channel bandwidths","","418","10.3.1","Channel bandwidth and subcarrier spacing [NR_newRAT]",52400,"revised","2017-05-02T07:29:11.137","2017-05-05T13:35:52.133","","R4-1706054","Rel-15","","","","","","","","","","","",""]
["R4-1704567","Channel Raster and Synchronization Signal Raster Considerations","Qualcomm Incorporated","Valentin Gheorghiu","43117","other","Approval","In this paper we propose that the channel raster should have a 1 RB granularity to allow 0 guardband intra-band CA and how to down select the synchronization frequency raster","","419","10.3.2","Channel Raster [NR_newRAT]",46140,"noted","2017-05-02T07:32:46.490","2017-05-05T13:35:52.133","","","Rel-15","","","","","","","","","","","",""]
["R4-1704568","Synchronization Block Design Implications on RAN4","Qualcomm Incorporated","Valentin Gheorghiu","43117","other","Approval","In this paper we show that initial system acquisition will be impacted due to the RAN1 agreements on synchronization burst design. We propose to send an LS to RAN1 to ask them to reconsider the PBCH design.","","419","10.3.2","Channel Raster [NR_newRAT]",52660,"revised","2017-05-02T07:37:58.937","2017-05-05T13:35:52.133","","R4-1705825","Rel-15","","","","","","","","","","","",""]
["R4-1704569","Noise Source Time Correlation Impact","Qualcomm Incorporated","Valentin Gheorghiu","43117","discussion","Discussion","In this paper we discuss the impact that the noise source time domain correlation has on SNR predictability","","462","10.7.3","Common to UE RRM and Demodulation [FS_NR_test_methods]",45690,"noted","2017-05-02T07:40:55.557","2017-05-05T13:35:52.150","","","Rel-15","","","","","","","","","","","",""]
["R4-1704570","Beam management requirements","Qualcomm Incorporated","Valentin Gheorghiu","43117","discussion","Discussion","In this paper we discuss the high level framework to be used for deriving beam management requirements","","453","10.6.5","System level and link level Simulation plan [NR_newRAT]",47610,"noted","2017-05-02T07:43:48.777","2017-05-05T13:35:52.150","","","Rel-15","","","","","","","","","","","",""]
["R4-1704571","[draft] Introduction of the FDD L-band (Band 74) into 36.133","DOCOMO Communications Lab.","Takuma Takada","70194","draftCR","Endorsement","This is draft CR on adding Band 74 to spec. This CR is for endorsement. Formal CR will be submitted in RAN4#84.","","318","9.4.4","RRM core (36.133) [LTE_FDD_L_Band-core]",45710,"revised","2017-05-02T11:43:03.277","2017-05-02T12:03:23.407","","R4-1706014","Rel-15","36.133","14.3.0","LTE_FDD_L_Band-Core","","","B","","","","","",""]
["R4-1704572","[draft] Introduction of the FDD L-band (Band 74) into 25.123","DOCOMO Communications Lab.","Takuma Takada","70194","draftCR","Endorsement","This is draft CR on adding Band 74 to spec. This CR is for endorsement. Formal CR will be submitted in RAN4#84.","","319","9.4.5","Other specifications [LTE_FDD_L_Band]",45510,"revised","2017-05-02T11:45:35.267","2017-05-02T12:03:23.393","","R4-1706036","Rel-15","25.123","14.2.0","LTE_FDD_L_Band","","","B","","","","","",""]
["R4-1704573","[draft] Introduction of the FDD L-band (Band 74) into 25.133","DOCOMO Communications Lab.","Takuma Takada","70194","draftCR","Endorsement","This is draft CR on adding Band 74 to spec. This CR is for endorsement. Formal CR will be submitted in RAN4#84.","","319","9.4.5","Other specifications [LTE_FDD_L_Band]",45500,"revised","2017-05-02T11:47:43.337","2017-05-02T12:03:23.393","","R4-1706015","Rel-15","25.133","14.1.0","LTE_FDD_L_Band","","","B","","","","","",""]
["R4-1704574","LS reply Positioning for NB-IoT","RAN1, Ericsson, Intel","Kyoungseok Oh","70239","LS in","Discussion","","","3","3","Letters / reports from other groups / meetings",45740,"noted","2017-05-02T16:00:38.707","2017-05-02T16:17:51.253","","","Rel-14","","","NB_IOTenh-Core","","","","","R2-1702323","RAN2","RAN4","R1-1706859",""]
["R4-1704575","On NR BS spectrum utilization","ZTE","Yonghong Gao","68603","other","Approval","In this contribution, we discuss how to capture spectrum utilization for frequency bands below 6GHz in the NR BS specification, and also how to obtain the RB numbers meanwhile ensure good spectral efficiency.","","420","10.3.3","Spectrum utilization [NR_newRAT]",52810,"noted","2017-05-02T16:15:20.963","2017-05-05T12:22:09.150","","","Rel-15","","","","","","","","","","","",""]
["R4-1704576","Number of ATF Measurements for RTS Isolation Measurement","ROHDE & SCHWARZ, Keysight Technologies","Thorsten Hertel","60675","discussion","Discussion","","","144","7.11.1","General [LTE_MIMO_OTA-Core]",46200,"noted","2017-05-03T04:34:47.020","2017-05-06T18:41:24.053","","","","37.977","","","","","","","","","","",""]
["R4-1704577","CR on Number of ATF Measurements for RTS Isolation Measurement","ROHDE & SCHWARZ, Keysight Technologies","Thorsten Hertel","60675","CR","Approval","","","144","7.11.1","General [LTE_MIMO_OTA-Core]",46570,"rejected","2017-05-03T04:41:10.367","2017-05-06T18:41:24.053","","","Rel-14","37.977","14.3.0","LTE_MIMO_OTA","0055","","F","","","","","",""]
["R4-1704578","Analysis of Harmonization Results","ROHDE & SCHWARZ","Thorsten Hertel","60675","discussion","Discussion","This contribution provides an analysis of the available harmonization results","","146","7.11.3","Harmonization [LTE_MIMO_OTA-Core]",45780,"noted","2017-05-03T04:45:19.650","2017-05-23T15:07:50.617","","","","","","","","","","","","","","",""]
["R4-1704579","Channel model validation procedures for RTS","ROHDE & SCHWARZ, Keysight Technologies","Thorsten Hertel","60675","discussion","Discussion","","","144","7.11.1","General [LTE_MIMO_OTA-Core]",46600,"noted","2017-05-03T04:50:06.153","2017-05-06T18:41:24.053","","","","","","","","","","","","","","",""]
["R4-1704580","Further discussion of co-existence study on LTE450_Reg3 band","China Unicom","Rongyi Hu","70322","discussion","Approval","","","345","9.10.1","General [LTE450_Reg3]",45800,"approved","2017-05-03T07:25:12.343","2017-05-06T06:17:51.410","","","Rel-15","","","","","","","","","","","",""]
["R4-1704581","Correction to RRM 4DL FDD CA test cases","ANRITSU LTD","Ian Rose","9381","CR","Agreement","For A.8.16.55:\n- Correct Test Purpose and Environment.\n- Correct Cell 2 OCNG Pattern\n- Correct RSRP and SCH_RP for Cell 4\n- Correct Cell 5 OCNG Pattern","","74","5.7.1.2","RRM [WI code]",45810,"agreed","2017-05-03T12:21:10.767","2017-05-04T14:14:31.573","","","Rel-13","36.133","13.7.0","LTE_CA_B1_B40-Perf","4838","","F","RP-171298","","","","",""]
["R4-1704582","Correction to RRM 4DL FDD CA test cases","ANRITSU LTD","Ian Rose","9381","CR","","For A.8.16.55:\n- Correct Test Purpose and Environment.\n- Correct Cell 2 OCNG Pattern\n- Correct RSRP and SCH_RP for Cell 4\n- Correct Cell 5 OCNG Pattern","","74","5.7.1.2","RRM [WI code]",45820,"revised","2017-05-03T12:26:24.037","2017-05-23T15:07:50.617","","","Rel-14","36.133","14.3.0","LTE_CA_B1_B40-Perf","4839","","A","","","","","",""]
["R4-1704583","Correction to Table A.4-1 and A.4-16 for Cat M1.","ANRITSU LTD","Ian Rose","9381","CR","Agreement","Correct PDSCH RPB allocation from 6th to 5th at Note 12 in Table A.4-1.\nCorrect Imcs value from 16 to 15 at CQI index=10 in Table A.4-16.\nCorrect Modulation based on TS36.213 Table 7.2.3-3.","","53","5.4.6.1","BL/CE UE [LTE_MTCe2_L1-Perf]",45850,"agreed","2017-05-03T12:36:32.893","2017-05-05T09:42:29.817","","","Rel-13","36.101","13.7.0","LTE_MTCe2_L1-Perf","4382","","F","RP-171309","","","","",""]
["R4-1704584","Correction to Table A.4-1 and A.4-16 for CatM1.","ANRITSU LTD","Ian Rose","9381","CR","Agreement","Correct PDSCH RPB allocation from 6th to 5th at Note 12 in Table A.4-1.\nCorrect Imcs value from 16 to 15 at CQI index=10 in Table A.4-16.\nCorrect Modulation based on TS36.213 Table 7.2.3-3.","","53","5.4.6.1","BL/CE UE [LTE_MTCe2_L1-Perf]",45860,"agreed","2017-05-03T12:40:50.337","2017-05-23T15:07:50.633","","","Rel-14","36.101","14.3.0","LTE_MTCe2_L1-Perf","4383","","A","RP-171309","","","","",""]
["R4-1704585","Correction to minimum requirement for Cat M1 Single-Layer Spatial Multiplexing","ANRITSU LTD","Ian Rose","9381","CR","","Add  cqi-pmi-ConfigIndex=12 in Table 8.11.1.1.1-1.\nChange channel for CQI reporting to PUSCH, and add Note 4 for PUSCH scheduling.\nRemove square brackets in Table 8.11.1.1.1.1-2","","53","5.4.6.1","BL/CE UE [LTE_MTCe2_L1-Perf]",45861,"revised","2017-05-03T12:51:48.253","2017-05-05T10:42:24.753","","R4-1705987","Rel-13","36.101","13.7.0","LTE_MTCe2_L1-Perf","4384","","F","","","","","",""]
["R4-1704586","Correction to minimum requirement for CatM1 Single-Layer Spatial Multiplexing","Anritsu, Rohde & Schwarz","Ian Rose","9381","CR","Agreement","Add  cqi-pmi-ConfigIndex=12 in Table 8.11.1.1.1-1.\nChange channel for CQI reporting to PUSCH, and add Note 4 for PUSCH scheduling.\nRemove square brackets in Table 8.11.1.1.1.1-2","","53","5.4.6.1","BL/CE UE [LTE_MTCe2_L1-Perf]",45880,"agreed","2017-05-03T12:56:24.507","2017-05-23T15:07:50.633","","","Rel-14","36.101","14.3.0","LTE_MTCe2_L1-Perf","4385","","A","RP-171310","","","","",""]
["R4-1704587","Correction to Test Parameters for MPDCCH in Table 8.11.2.1-1","ANRITSU LTD","Ian Rose","9381","CR","","Correct Frequency hopping interval from 4ms to N/A.\nCorrect Precoder update granularity from 4ms to 32ms.\nRemove Reference channel for PDSCH transmission.","","53","5.4.6.1","BL/CE UE [LTE_MTCe2_L1-Perf]",47460,"noted","2017-05-03T13:10:05.707","2017-05-05T13:02:28.240","","","Rel-13","36.101","13.7.0","LTE_MTCe2_L1-Perf","4386","","F","","","","","",""]
["R4-1704588","Correction to Test Parameters for MPDCCH in Table 8.11.2.1-1","ANRITSU LTD","Ian Rose","9381","CR","","Correct Frequency hopping interval from 4ms to N/A.\nCorrect Precoder update granularity from 4ms to 32ms.\nRemove Reference channel for PDSCH transmission.","","53","5.4.6.1","BL/CE UE [LTE_MTCe2_L1-Perf]",47470,"withdrawn","2017-05-03T13:13:10.813",null,"","","Rel-14","36.101","14.3.0","LTE_MTCe2_L1-Perf","4387","","A","","","","","",""]
["R4-1704589","Corrections to LAA Event-triggered reporting Test Cases A.8.26","ANRITSU LTD","Ian Rose","9381","CR","Agreement","Add Antenna Configuration, change Propagation condition to be per cell.\nSpecify Noc to be per carrier, and Io to be per carrier.\nFor fixed BW FS3 cells, specify Io directly and remove scaling with # of RBs.\nSpecify _RA, _RB values to be per cell.\nSpecify","","38","5.3.5","RRM Performance (36.133) [LTE_LAA-Perf]",45890,"agreed","2017-05-03T13:32:18.313","2017-05-04T13:07:47.153","","","Rel-13","36.133","13.7.0","LTE_LAA-Perf","4840","","F","RP-171307","","","","",""]
["R4-1704590","Corrections to LAA Event-triggered reporting Test Cases A.8.26","ANRITSU LTD","Ian Rose","9381","CR","Agreement","Add Antenna Configuration, change Propagation condition to be per cell.\nSpecify Noc to be per carrier, and Io to be per carrier.\nFor fixed BW FS3 cells, specify Io directly and remove scaling with # of RBs.\nSpecify _RA, _RB values to be per cell.\nSpecify","","38","5.3.5","RRM Performance (36.133) [LTE_LAA-Perf]",45900,"agreed","2017-05-03T13:35:42.217","2017-05-23T15:07:50.633","","","Rel-14","36.133","14.3.0","LTE_LAA-Perf","4841","","A","RP-171307","","","","",""]
["R4-1704591","UE RRM test methodologies in NR","ANRITSU LTD","Ian Rose","9381","discussion","Endorsement","This Tdoc looks at some specific aspects of the UE test environment for NR RRM.","","465","10.7.4.1","Baseline measurement setup [FS_NR_test_methods]",54670,"noted","2017-05-03T13:49:06.177","2017-05-05T09:52:38.593","","","","","","","","","","","","","","",""]
["R4-1704592","Revised WI: LTE Advanced inter-band CA Rel-14 for 5DL/1UL","Nokia","Iwajlo Angelow","68260","WID revised","Endorsement","","","112","7.5.1","Rapporteur Input (WID/CRs) [LTE_CA_R14_5DL1UL-Core]",45940,"endorsed","2017-05-03T13:57:32.107","2017-06-06T13:47:53.310","","","Rel-14","","","LTE_CA_R14_5DL1UL","","","","","","","","",""]
["R4-1704593","TR 36.714-05-01 v0.7.0","Nokia","Iwajlo Angelow","68260","draft TR","Approval","","","112","7.5.1","Rapporteur Input (WID/CRs) [LTE_CA_R14_5DL1UL-Core]",45920,"approved","2017-05-03T13:57:32.123","2017-05-06T16:59:02.190","","","Rel-14","36.714-05-01","0.7.0","LTE_CA_R14_5DL1UL","","","","","","","","",""]
["R4-1704594","Introduction of 5DL CA combinations to 36.104","Nokia","Iwajlo Angelow","68260","CR","Approval","","","112","7.5.1","Rapporteur Input (WID/CRs) [LTE_CA_R14_5DL1UL-Core]",45970,"revised","2017-05-03T13:57:35.307","2017-05-23T15:07:50.650","","R4-1706083","Rel-14","36.104","14.3.0","LTE_CA_R14_5DL1UL-Core","4668","","B","","","","","",""]
["R4-1704595","Introduction of 5DL CA combinations to 36.141","Nokia","Iwajlo Angelow","68260","CR","Approval","","","112","7.5.1","Rapporteur Input (WID/CRs) [LTE_CA_R14_5DL1UL-Core]",54440,"revised","2017-05-03T13:57:36.163","2017-05-23T15:07:50.650","","R4-1706084","Rel-14","36.141","14.3.0","LTE_CA_R14_5DL1UL-Perf","1024","","B","","","","","",""]
["R4-1704596","New WI: LTE Advanced inter-band CA Rel-15 for 5DL/1UL","Nokia","Iwajlo Angelow","68260","WID new","Endorsement","","","112","7.5.1","Rapporteur Input (WID/CRs) [LTE_CA_R14_5DL1UL-Core]",45950,"endorsed","2017-05-03T13:57:37.053","2017-06-06T13:47:53.387","","","","","","","","","","","","","","",""]
["R4-1704597","Updated scope of TR: LTE Advanced inter-band CA Rel-14 for 5DL/1UL","Nokia","Iwajlo Angelow","68260","other","Approval","","","112","7.5.1","Rapporteur Input (WID/CRs) [LTE_CA_R14_5DL1UL-Core]",45930,"approved","2017-05-03T13:57:37.067","2017-06-06T13:47:53.403","","","","","","","","","","","","","","",""]
["R4-1704598","TP to 36.714-03-01: Introduction of CA_2A-48A-66A","Nokia, Verizon","Iwajlo Angelow","68260","other","Approval","","","101","7.3.2","UE RF (36.101) [LTE_CA_R14_3DL1UL-Core]",46000,"revised","2017-05-03T13:57:37.083","2017-05-06T17:03:35.627","","R4-1705901","","","","","","","","","","","","",""]
["R4-1704599","TP to 36.714-03-01: Introduction of CA_2A-48C","Nokia, Verizon","Iwajlo Angelow","68260","other","Approval","","","101","7.3.2","UE RF (36.101) [LTE_CA_R14_3DL1UL-Core]",46010,"revised","2017-05-03T13:57:37.100","2017-05-06T17:03:35.627","","R4-1705902","","","","","","","","","","","","",""]
["R4-1704600","TP to 36.714-03-01: Introduction of CA_48A-48A-66A","Nokia, Verizon","Iwajlo Angelow","68260","other","Approval","","","101","7.3.2","UE RF (36.101) [LTE_CA_R14_3DL1UL-Core]",47230,"approved","2017-05-03T13:57:37.117","2017-05-06T17:03:35.627","","","","","","","","","","","","","","",""]
["R4-1704601","TP to 36.714-03-01: Introduction of CA_48C-66A","Nokia, Verizon","Iwajlo Angelow","68260","other","Approval","","","101","7.3.2","UE RF (36.101) [LTE_CA_R14_3DL1UL-Core]",48990,"approved","2017-05-03T13:57:37.130","2017-05-06T17:03:35.627","","","","","","","","","","","","","","",""]
["R4-1704602","Draft CR to 25.104: Introduction of Band 71","Nokia","Iwajlo Angelow","68260","draftCR","Endorsement","","","338","9.8.4","Other specifications [LTE600_US]",46050,"endorsed","2017-05-03T13:57:37.147","2017-05-06T17:03:35.627","","","Rel-14","25.104","14.1.0","LTE600_US-Core","","","","","","","","",""]
["R4-1704603","Draft CR to 36.104: Introduction of Band 71","Nokia","Iwajlo Angelow","68260","draftCR","Endorsement","","","337","9.8.3","BS RF (36.104) [LTE600_US-core]",46030,"endorsed","2017-05-03T13:57:37.177","2017-05-06T17:03:35.643","","","Rel-14","36.104","14.3.0","LTE600_US-Core","","","","","","","","",""]
["R4-1704604","Draft CR to 36.113: Introduction of Band 71","Nokia","Iwajlo Angelow","68260","draftCR","Endorsement","","","338","9.8.4","Other specifications [LTE600_US]",46060,"endorsed","2017-05-03T13:57:37.207","2017-05-06T17:03:35.643","","","Rel-14","36.113","14.2.0","LTE600_US-Core","","","","","","","","",""]
["R4-1704605","Draft CR to 36.124: Introduction of Band 71","Nokia","Iwajlo Angelow","68260","draftCR","Endorsement","","","338","9.8.4","Other specifications [LTE600_US]",46070,"endorsed","2017-05-03T13:57:37.257","2017-05-06T17:03:35.643","","","Rel-14","36.124","14.1.0","LTE600_US-Core","","","","","","","","",""]
["R4-1704606","Draft CR to 36.141: Introduction of Band 71","Nokia","Iwajlo Angelow","68260","draftCR","Endorsement","","","338","9.8.4","Other specifications [LTE600_US]",49580,"endorsed","2017-05-03T13:57:44.463","2017-05-06T17:03:35.643","","","Rel-14","36.141","14.3.0","LTE600_US-Perf","","","","","","","","",""]
["R4-1704607","Draft CR to 37.113: Introduction of Band 71","Nokia","Iwajlo Angelow","68260","draftCR","Endorsement","","","338","9.8.4","Other specifications [LTE600_US]",49590,"endorsed","2017-05-03T13:57:44.493","2017-05-06T17:03:35.643","","","Rel-14","37.113","14.1.0","LTE600_US-Core","","","","","","","","",""]
["R4-1704608","Draft CR to 36.104: Introduction of Band 72","Nokia","Iwajlo Angelow","68260","draftCR","Endorsement","","","309","9.2.3","BS RF (36.104) [LTE450_Europe_PPDR-core]",46080,"endorsed","2017-05-03T13:57:44.510","2017-05-06T17:03:35.657","","","Rel-14","36.104","14.3.0","LTE450_Europe_PPDR-Core","","","","","","","","",""]
["R4-1704609","Expected changes to 36.104: Band 73 introduction","Nokia, Alcatel-Lucent Shanghai Bell","Iwajlo Angelow","68260","other","Approval","","","348","9.10.4","BS RF (36.104) [LTE450_Reg3-core]",46090,"approved","2017-05-03T13:57:44.633","2017-05-06T17:03:35.657","","","","","","","","","","","","","","",""]
["R4-1704610","On LTE extended 1.5GHz SDL band plan","Nokia","Iwajlo Angelow","68260","other","Approval","","","320","9.5","LTE Extended 1.5 GHz SDL band (1427 ? 1518 MHz) and LTE Carrier Aggregation (2DL/1UL) with Band 20 [LTE_SDL_1500ext]",46100,"noted","2017-05-03T13:57:44.633","2017-05-06T17:03:35.657","","","","","","","","","","","","","","",""]
["R4-1704611","L-band RF filter simulations","Nokia","Iwajlo Angelow","68260","discussion","Discussion","","","321","9.5.1","Co-exitence requirements with EESS and MSS [LTE_SDL_1500ext]",46110,"noted","2017-05-03T13:57:44.650","2017-05-06T17:03:35.657","","","","","","","","","","","","","","",""]
["R4-1704612","Far-field distance determination at 28GHz based on power measurements","ROHDE & SCHWARZ","Thorsten Hertel","60675","discussion","Discussion","This contribution is a continuation of the power-based measurement approach to estimate the boundary between the near and far field region of wireless enabled devices","","459","10.7.2","UE RF [FS_NR_test_methods]",566800,"withdrawn","2017-05-03T17:50:09.603",null,"","","","","","","","","","","","","","",""]
["R4-1704613","NR band numbering","Ericsson","Johan Skold","10425","other","Approval","The paper discusses and makes proposals for band numbering principles for NR.","","413","10.2.1","NR frequency range and bands [NR_newRAT]",52940,"revised","2017-05-03T18:52:06.730","2017-05-05T19:34:58.957","","R4-1706051","Rel-15","","","NR_newRAT","","","","","","","","",""]
["R4-1704614","NR Sync channel raster and channel arrangement","Ericsson","Johan Skold","10425","other","Approval","The paper analyses the RAN1 agreements on sync channel and initial access, concluding on some issues for smaller channel bandwidths. It is proposed to send an LS to RAN1 on the topic.","","419","10.3.2","Channel Raster [NR_newRAT]",486301,"revised","2017-05-03T18:52:06.747","2017-05-05T19:34:58.957","","R4-1706057","Rel-15","","","NR_newRAT","","","","","","","","",""]
["R4-1704615","Draft LS to RAN1 on Sync channel raster","Ericsson","Johan Skold","10425","LS out","Approval","Proposed LS response concerning the RAN1 agreements on sync channel and initial access.","","419","10.3.2","Channel Raster [NR_newRAT]",569600,"noted","2017-05-03T18:52:06.760","2017-05-05T19:34:58.957","","","Rel-15","","","NR_newRAT","","","","","R4-1704312","RAN1","","",""]
["R4-1704616","NR BS boundary between out-of-band and spurious domain below 6 Ghz","Ericsson","Johan Skold","10425","other","Approval","Based on analysis and band filter simulations, the paper further discusses and makes proposals for how to set the boundary to the spurious domain for bands below 6 GHz.","","440","10.5.3.2","Unwanted emission requirements [NR_newRAT]",52880,"noted","2017-05-03T18:52:06.823","2017-05-05T19:34:58.940","","","Rel-15","","","NR_newRAT","","","","","","","","",""]
["R4-1704617","NR BS mmWave unwanted emissions","Ericsson","Johan Skold","10425","other","Approval","Baes on the agreements from RAN4#82bis, further proposals are made for how to specify mmWave unwanted emissions limits.","","440","10.5.3.2","Unwanted emission requirements [NR_newRAT]",46160,"noted","2017-05-03T18:52:06.823","2017-05-05T19:34:58.940","","","Rel-15","","","NR_newRAT","","","","","","","","",""]
["R4-1704618","NR BS RF specifications structure","Ericsson","Johan Skold","10425","discussion","Discussion","Two options for specification structure are discussed, one based on the LTE&MSR BS specs and one based on the AAS BS spec.","","436","10.5.1","BS RF General (ad-hoc MoM, Plan, Spec structure) [NR_newRAT]",45410,"noted","2017-05-03T18:52:06.853","2017-05-05T19:34:58.940","","","Rel-15","","","NR_newRAT","","","","","","","","",""]
["R4-1704619","TS 38.104 v0.0.1 NR Base Station (BS) radio transmission and reception (Skeleton)","Ericsson","Johan Skold","10425","draft TS","Approval","Proposed skeleton for the NR BS RF specification.","","436","10.5.1","BS RF General (ad-hoc MoM, Plan, Spec structure) [NR_newRAT]",0,"revised","2017-05-03T18:52:06.870","2017-05-04T07:28:00.010","","R4-1705298, R4-1705332","Rel-15","38.104","0.0.1","NR_newRAT","","","","","","","","",""]
["R4-1704620","CR on Channel model validation procedures for RTS","ROHDE & SCHWARZ, Keysight Technologies","Thorsten Hertel","60675","CR","Approval","","","144","7.11.1","General [LTE_MIMO_OTA-Core]",46630,"revised","2017-05-03T21:27:18.643","2017-05-06T18:41:24.053","","R4-1705918","Rel-14","37.977","14.3.0","LTE_MIMO_OTA","0056","","F","","","","","",""]
["R4-1704621","Demodulation requirements for Rel.13 non-BL/CE UEs","Intel Corporation","Yang Tang","56725","other","Discussion","","","54","5.4.6.2","Non-BL/CE UE [LTE_MTCe2_L1-Perf]",48130,"noted","2017-05-03T23:04:25.677","2017-05-06T17:26:32.740","","","Rel-13","36.101","","LTE_MTCe2_L1-Perf","","","","","","","","",""]
["R4-1704622","Demodulation requirements for Rel.14 non-BL/CE UEs","Intel Corporation","Yang Tang","56725","other","Discussion","","","228","7.18.8.2","Non-BL/CE UE [LTE_feMTC-Perf]",55410,"noted","2017-05-03T23:04:25.707","2017-05-06T17:26:32.757","","","Rel-14","36.101","","LTE_feMTC-Perf","","","","","","","","",""]
["R4-1704623","PDSCH simulation results for Rel.14 FeMTC Cat. M2 UEs","Intel Corporation","Yang Tang","56725","other","Discussion","","","227","7.18.8.1","BL/CE UE [LTE_feMTC-Perf]",48070,"noted","2017-05-03T23:04:25.723","2017-05-06T17:26:32.757","","","Rel-14","36.101","","LTE_feMTC-Perf","","","","","","","","",""]
["R4-1704624","CR for demodulation of NB-IoT correction (Rel.13)","Intel Corporation","Yang Tang","56725","CR","Agreement","","","64","5.5.6.1","UE Demodulation (36.101) [NB_IOT-Perf]",46260,"agreed","2017-05-03T23:04:25.723","2017-05-06T17:26:32.757","","","Rel-13","36.101","13.7.0","NB_IOT-Perf","4388","","F","RP-171300","","","","",""]
["R4-1704625","CR for demodulation of NB-IoT correction (Rel.14)","Intel Corporation","Yang Tang","56725","CR","Agreement","","","64","5.5.6.1","UE Demodulation (36.101) [NB_IOT-Perf]",55800,"agreed","2017-05-03T23:04:28.627","2017-05-23T15:07:50.727","","","Rel-14","36.101","14.3.0","NB_IOT-Perf","4389","","A","RP-171300","","","","",""]
["R4-1704626","Discussion on Rel.13 NPDSCH standalone test case","Intel Corporation","Yang Tang","56725","other","Discussion","","","64","5.5.6.1","UE Demodulation (36.101) [NB_IOT-Perf]",46250,"noted","2017-05-03T23:04:29.420","2017-05-06T17:26:32.757","","","Rel-13","36.101","","NB_IOT-Perf","","","","","","","","",""]
["R4-1704627","NPDSCH simulation results for Rel.14 eNB-IoT","Intel Corporation","Yang Tang","56725","other","Discussion","","","202","7.17.6","UE demodulation(36.101) [NB_IOTenh-Perf]",48090,"noted","2017-05-03T23:04:29.437","2017-05-06T17:26:32.770","","","Rel-14","36.101","","NB_IOTenh-Perf","","","","","","","","",""]
["R4-1704628","Discussion on CQI reporting test","Intel Corporation","Yang Tang","56725","other","Discussion","","","265","7.25.4.3","CQI reporting [LTE_high_speed-Perf]",46280,"noted","2017-05-03T23:04:29.453","2017-05-06T17:26:32.770","","","Rel-14","36.101","","LTE_high_speed-Perf","","","","","","","","",""]
["R4-1704629","CR for LAA TDD test case correction (Rel.13)","Intel Corporation","Yang Tang","56725","CR","Agreement","","","39","5.3.6","UE Demodulation (36.101) [LTE_LAA-Perf]",46290,"agreed","2017-05-03T23:04:29.453","2017-05-06T17:26:32.770","","","Rel-13","36.101","13.7.0","LTE_LAA-Perf","4390","","F","RP-171307","","","","",""]
["R4-1704630","CR for LAA TDD test case correction (Rel.14)","Intel Corporation","Yang Tang","56725","CR","Agreement","","","39","5.3.6","UE Demodulation (36.101) [LTE_LAA-Perf]",46300,"agreed","2017-05-03T23:04:30.327","2017-05-23T15:07:50.757","","","Rel-14","36.101","14.3.0","LTE_LAA-Perf","4391","","A","RP-171307","","","","",""]
["R4-1704631","4RX CA IRC simulation results","Intel Corporation","Yang Tang","56725","discussion","Discussion","","","244","7.21.2","UE demodulation (36.101) [LTE_4Rx_AP_DL_CA-Perf]",51330,"noted","2017-05-03T23:04:31.217","2017-05-06T17:26:32.770","","","Rel-14","","","LTE_4Rx_AP_DL_CA-Perf","","","","","","","","",""]
["R4-1704632","Enhanced CRS-IM performance requirements","Intel Corporation","Yang Tang","56725","discussion","Discussion","","","276","7.27.2","CRS-IM [LTE_eCRSIM_eSUMIMO]",616600,"noted","2017-05-03T23:04:31.230","2017-05-06T17:32:20.957","","","Rel-14","","","LTE_eCRSIM_eSUMIMO","","","","","","","","",""]
["R4-1704633","Summary of Enhanced CRS-IM PDSCH simulation results","Intel Corporation","Yang Tang","56725","other","Information","Summary of alignment and impairements Enhanced CRS-IM PDSCH simulation results","","277","7.27.2.1","PDSCH [LTE_eCRSIM_eSUMIMO]",46330,"noted","2017-05-03T23:04:31.230","2017-05-23T15:07:50.757","","","Rel-14","","","LTE_eCRSIM_eSUMIMO","","","","","","","","",""]
["R4-1704634","Summary of Enhanced CRS-IM PDCCH/PCFICH simulation results","Intel Corporation","Yang Tang","56725","other","Information","Summary of alignment and impairements Enhanced CRS-IM PDCCH/PCFICH simulation results","","278","7.27.2.2","Control channel [LTE_eCRSIM_eSUMIMO]",46390,"noted","2017-05-03T23:04:31.247","2017-05-23T15:07:50.773","","","Rel-14","","","LTE_eCRSIM_eSUMIMO","","","","","","","","",""]
["R4-1704635","Enhanced CRS-IM UE capabilities and network assistance framework","Intel Corporation","Yang Tang","56725","discussion","Discussion","","","275","7.27.1.1","Capability and signaling [LTE_eCRSIM_eSUMIMO]",46350,"noted","2017-05-03T23:04:31.263","2017-05-06T17:32:20.973","","","Rel-14","","","LTE_eCRSIM_eSUMIMO","","","","","","","","",""]
["R4-1704636","TR 36.747 text proposal on Enhanced CRS-IM","Intel Corporation","Yang Tang","56725","other","Approval","TR 36.747 text proposal","","274","7.27.1","General [LTE_eCRSIM_eSUMIMO]",46360,"revised","2017-05-03T23:04:31.277","2017-05-06T17:32:20.973","","R4-1706030","Rel-14","36.747","","LTE_eCRSIM_eSUMIMO","","","","","","","","",""]
["R4-1704637","Draft CR on Enhanced CRS-IM PDSCH performance requirements","Intel Corporation","Yang Tang","56725","draftCR","Endorsement","","","277","7.27.2.1","PDSCH [LTE_eCRSIM_eSUMIMO]",49230,"revised","2017-05-03T23:04:31.277","2017-05-06T17:32:20.973","","R4-1706032","Rel-14","36.101","14.3.0","LTE_eCRSIM_eSUMIMO","","","","","","","","",""]
["R4-1704638","Draft CR on Enhanced CRS-IM PDSCH FRCs","Intel Corporation","Yang Tang","56725","draftCR","Endorsement","","","277","7.27.2.1","PDSCH [LTE_eCRSIM_eSUMIMO]",51730,"endorsed","2017-05-03T23:04:31.293","2017-05-06T17:32:20.973","","","Rel-14","36.101","14.3.0","LTE_eCRSIM_eSUMIMO","","","","","","","","",""]
["R4-1704639","Draft CR on Enhanced CRS-IM PDCCH/PCFICH performance requirements","Intel Corporation","Yang Tang","56725","draftCR","Endorsement","","","278","7.27.2.2","Control channel [LTE_eCRSIM_eSUMIMO]",51740,"revised","2017-05-03T23:04:31.480","2017-05-06T17:32:20.990","","R4-1706033","Rel-14","36.101","14.3.0","LTE_eCRSIM_eSUMIMO","","","","","","","","",""]
["R4-1704640","Enhanced SU-MIMO IM demodulation requirements","Intel Corporation","Yang Tang","56725","discussion","Discussion","","","279","7.27.3","SU-MIMO IM [LTE_eCRSIM_eSUMIMO]",49420,"noted","2017-05-03T23:04:31.497","2017-05-06T17:32:20.990","","","Rel-14","","","LTE_eCRSIM_eSUMIMO","","","","","","","","",""]
["R4-1704641","MUST Case 3 demodulation performance requirements","Intel Corporation","Yang Tang","56725","discussion","Discussion","","","256","7.24.1.2","Case 3 [LTE_MUST-Perf]",46410,"noted","2017-05-03T23:04:31.513","2017-05-06T17:32:20.990","","","Rel-14","","","LTE_MUST-Perf","","","","","","","","",""]
["R4-1704642","Discussion on MUST UE Capabilities","Intel Corporation","Yang Tang","56725","discussion","Discussion","","","257","7.24.2","UE capbility [LTE_MUST]",46420,"noted","2017-05-03T23:04:31.527","2017-05-06T17:32:20.990","","","Rel-14","","","LTE_MUST","","","","","","","","",""]
["R4-1704643","LTE V2V UE demodulation requirements","Intel Corporation","Yang Tang","56725","discussion","Discussion","","","172","7.15.4.1","Single-link PSSCH and PSCCH [LTE_SL_V2V-Perf]",46430,"noted","2017-05-03T23:04:31.543","2017-05-06T17:32:21.007","","","Rel-14","","","LTE_SL_V2V-Perf","","","","","","","","",""]
["R4-1704644","CR on V2V demodulation requirements FRCs","Intel Corporation","Yang Tang","56725","CR","Approval","","","171","7.15.4","UE demodulation (36.101) [LTE_SL_V2V-Perf]",55460,"noted","2017-05-03T23:04:31.543","2017-05-06T17:32:21.007","","","Rel-14","36.101","14.3.0","LTE_SL_V2V-Perf","4392","","F","","","","","",""]
["R4-1704645","LTE V2X UE demodulation requirements: PSSCH/PSCCH maximum processing capability test cases","Intel Corporation","Yang Tang","56725","discussion","Discussion","","","181","7.16.5.1","PSSCH/PSCCH maximum processing capability test [LTE_V2X-Perf]",46450,"noted","2017-05-03T23:04:32.587","2017-05-06T17:32:21.007","","","Rel-14","","","LTE_SL_V2V-Perf","","","","","","","","",""]
["R4-1704646","LTE V2X UE demodulation requirements: PSBCH, eNB sync and WAN SDR test cases","Intel Corporation","Yang Tang","56725","discussion","Discussion","","","182","7.16.5.2","PSBCH, eNB sync and WAN SDR [LTE_V2X-Perf]",49140,"noted","2017-05-03T23:04:32.603","2017-05-06T17:33:19.360","","","Rel-14","","","LTE_SL_V2V-Perf","","","","","","","","",""]
["R4-1704647","On TM10 / FD-MIMO UE capability signalling","Intel Corporation","Yang Tang","56725","discussion","Discussion","","","281","7.28.1","General [LTE_eFDMIMO-Perf]",46480,"noted","2017-05-03T23:04:32.620","2017-05-06T17:33:19.377","","","Rel-14","","","LTE_EBF_FDMIMO-Core","","","","","","","","",""]
["R4-1704648","[Draft] LS reply on TM10 / FD-MIMO UE capability signalling","Intel Corporation","Yang Tang","56725","LS out","Approval","","","281","7.28.1","General [LTE_eFDMIMO-Perf]",47760,"noted","2017-05-03T23:04:32.637","2017-05-06T17:33:19.377","","","Rel-14","","","LTE_EBF_FDMIMO-Core","","","","","R2-1702346","RAN2","RAN1","",""]
["R4-1704649","New WI Proposal: LTE CRS-IM Performance Requirements for Single RX Chain UEs","Intel Corporation","Yang Tang","56725","other","Information","","","473","13","Revision of the Work Plan",46500,"noted","2017-05-03T23:04:32.667","2017-05-06T17:33:19.377","","","Rel-15","","","","","","","","","","","",""]
["R4-1704650","Motivation for WI: LTE CRS-IM Performance Requirements for Single RX Chain UEs","Intel Corporation","Yang Tang","56725","other","Information","","","473","13","Revision of the Work Plan",46510,"noted","2017-05-03T23:04:32.680","2017-05-06T17:33:19.377","","","Rel-15","","","","","","","","","","","",""]
["R4-1704651","New SI proposal: Study on Advanced Receivers for LTE V2X","Intel Corporation","Yang Tang","56725","other","Information","","","473","13","Revision of the Work Plan",46520,"noted","2017-05-03T23:04:32.697","2017-05-06T17:33:19.390","","","Rel-15","","","","","","","","","","","",""]
["R4-1704652","Motivation for SI: Study on Advanced Receivers LTE V2X","Intel Corporation","Yang Tang","56725","other","Approval","","","473","13","Revision of the Work Plan",50990,"noted","2017-05-03T23:04:32.713","2017-05-06T17:33:19.390","","","Rel-15","","","","","","","","","","","",""]
["R4-1704653","Discussion on NR spectrum utilization","Intel Corporation","Yang Tang","56725","discussion","Discussion","","","420","10.3.3","Spectrum utilization [NR_newRAT]",53410,"noted","2017-05-03T23:04:32.713","2017-05-06T17:33:19.407","","","Rel-15","","","NR_newRAT","","","","","","","","",""]
["R4-1704654","LTE handset TRP/TRS measurements","Intel Corporation","Yang Tang","56725","discussion","Discussion","","","140","7.10.2","Hand phantom for smartphones [LTE_UTRA_TRP_TRS-Core]",46540,"noted","2017-05-03T23:04:32.727","2017-05-06T13:27:51.443","","","Rel-14","","","LTE_UTRA_TRP_TRS-Core","","","","","","","","",""]
["R4-1704655","TRP/TRS joint band passing rate worksheet","Intel Corporation","Yang Tang","56725","discussion","Discussion","","","140","7.10.2","Hand phantom for smartphones [LTE_UTRA_TRP_TRS-Core]",53090,"revised","2017-05-03T23:04:32.743","2017-05-06T13:27:51.477","","R4-1706093","Rel-14","","","LTE_UTRA_TRP_TRS-Core","","","","","","","","",""]
["R4-1704656","LTE handset BHH TRP/TRS requirement analysis","Intel Corporation","Yang Tang","56725","other","Approval","","","140","7.10.2","Hand phantom for smartphones [LTE_UTRA_TRP_TRS-Core]",609500,"noted","2017-05-03T23:04:32.760","2017-05-06T13:27:51.477","","","Rel-14","","","LTE_UTRA_TRP_TRS-Core","","","","","","","","",""]
["R4-1704657","MIMO OTA email discussion","Intel Corporation","Yang Tang","56725","report","Approval","","","144","7.11.1","General [LTE_MIMO_OTA-Core]",46640,"noted","2017-05-03T23:04:32.777","2017-05-06T13:27:51.477","","","Rel-14","","","LTE_MIMO_OTA-Core","","","","","","","","",""]
["R4-1704658","LTE handset TRMS measurements","Intel Corporation","Yang Tang","56725","discussion","Discussion","","","145","7.11.2","Performance requirements [LTE_MIMO_OTA-Core]",53130,"noted","2017-05-03T23:04:32.790","2017-05-06T13:27:51.490","","","Rel-14","","","LTE_MIMO_OTA-Core","","","","","","","","",""]
["R4-1704659","MIMO OTA lab alignment analysis","Intel Corporation","Yang Tang","56725","discussion","Discussion","","","145","7.11.2","Performance requirements [LTE_MIMO_OTA-Core]",573400,"noted","2017-05-03T23:04:32.807","2017-05-06T13:17:51.447","","","Rel-14","","","LTE_MIMO_OTA-Core","","","","","","","","",""]
["R4-1704660","On concluding the MIMO OTA Work Item","Intel Corporation","Yang Tang","56725","other","Approval","","","144","7.11.1","General [LTE_MIMO_OTA-Core]",566700,"noted","2017-05-03T23:04:32.837","2017-05-23T15:07:50.773","","","Rel-14","","","LTE_MIMO_OTA-Core","","","","","","","","",""]
["R4-1704661","Harmonization analysis","Intel Corporation","Yang Tang","56725","discussion","Discussion","","","146","7.11.3","Harmonization [LTE_MIMO_OTA-Core]",46610,"noted","2017-05-03T23:04:32.853","2017-05-23T15:07:50.773","","","Rel-14","","","LTE_MIMO_OTA-Core","","","","","","","","",""]
["R4-1704662","CR on harmonization outcome","Intel Corporation, SGS Wireless","Yang Tang","56725","CR","Agreement","","","146","7.11.3","Harmonization [LTE_MIMO_OTA-Core]",46620,"agreed","2017-05-03T23:04:32.853","2017-05-23T15:07:50.790","","","Rel-14","37.977","14.3.0","LTE_MIMO_OTA-Core","0057","","F","RP-171258","","","","",""]
["R4-1704663","LS on MIMO OTA progress","Intel Corporation","Yang Tang","56725","LS out","Approval","","","144","7.11.1","General [LTE_MIMO_OTA-Core]",566900,"revised","2017-05-03T23:04:33.663","2017-05-06T13:17:51.480","","R4-1705922","Rel-14","","","LTE_MIMO_OTA-Core","","","","","","GCF CAG, GCF PAG, CTIA MOSG","RAN5","",""]
["R4-1704664","MIMO OTA evening adhoc notes","Intel Corporation","Yang Tang","56725","report","Approval","","","144","7.11.1","General [LTE_MIMO_OTA-Core]",571100,"approved","2017-05-03T23:04:33.680","2017-05-23T15:07:50.790","","","Rel-14","","","LTE_MIMO_OTA-Core","","","","","","","","",""]
["R4-1704665","On defining the unwanted emissions requirements","Intel Corporation","Yang Tang","56725","discussion","Discussion","","","429","10.4.3.3","Spurious emission [NR_newRAT]",607200,"withdrawn","2017-05-03T23:04:33.697",null,"","","Rel-15","","","NR_newRAT","","","","","","","","",""]
["R4-1704666","TR38.810 v0.0.2","Intel Corporation, CATR","Yang Tang","56725","other","Approval","","","458","10.7.1","General [FS_NR_test_methods]",46700,"approved","2017-05-03T23:04:33.710","2017-05-06T13:17:51.497","","","Rel-15","","","NR_newRAT","","","","","","","","",""]
["R4-1704667","On measurement uncertainty elements for UE RF test setup","Intel Corporation","Yang Tang","56725","discussion","Discussion","","","461","10.7.2.2","Measurement uncertainty and test tolerance [FS_NR_test_methods]",46670,"noted","2017-05-03T23:04:33.727","2017-05-06T13:17:51.497","","","Rel-15","","","NR_newRAT","","","","","","","","",""]
["R4-1704668","On propagation model for RRM and demodulation","Intel Corporation","Yang Tang","56725","discussion","Discussion","","","463","10.7.3.1","Propagation model for RRM and demodulation [FS_NR_test_methods]",46680,"noted","2017-05-03T23:04:33.743","2017-05-06T13:17:51.510","","","Rel-15","","","NR_newRAT","","","","","","","","",""]
["R4-1704669","On baseline measurement setup for RRM","Intel Corporation","Yang Tang","56725","discussion","Discussion","","","465","10.7.4.1","Baseline measurement setup [FS_NR_test_methods]",583100,"noted","2017-05-03T23:04:33.757","2017-05-06T19:07:51.673","","","Rel-15","","","NR_newRAT","","","","","","","","",""]
["R4-1704670","NR testability adhoc meeting notes","Intel Corporation","Yang Tang","56725","report","Approval","","","458","10.7.1","General [FS_NR_test_methods]",46660,"approved","2017-05-03T23:04:33.773","2017-05-23T15:07:50.807","","","Rel-15","","","NR_newRAT","","","","","","","","",""]
["R4-1704671","On absolute power control accuracy requirement for NB-IoT","Intel Corporation","Yang Tang","56725","discussion","Discussion","","","58","5.5.1","UE RF core(36.101) [NB_IOT-Core]",53980,"noted","2017-05-03T23:04:33.790","2017-05-06T13:17:51.510","","","Rel-13","","","NB_IOT-Core","","","","","","","","",""]
["R4-1704672","CR on absolute power control accuracy for NB-IoT","Intel Corporation","Yang Tang","56725","CR","Agreement","","","58","5.5.1","UE RF core(36.101) [NB_IOT-Core]",53990,"withdrawn","2017-05-03T23:04:33.807",null,"","","Rel-13","36.101","13.7.0","NB_IOT-Core","4393","","F","","","","","",""]
["R4-1704673","Rel-13 CR on the applicability of RRC procedures","Intel Corporation","Yang Tang","56725","CR","Agreement","","","60","5.5.3","RRM core (36.133) [NB_IOT-Core]",49800,"agreed","2017-05-03T23:04:34.647","2017-05-06T13:17:51.527","","","Rel-13","36.133","13.7.0","NB_IOT-Core","4842","","F","RP-171299","","","","",""]
["R4-1704674","Rel-14 CR on the applicability of RRC procedures","Intel Corporation","Yang Tang","56725","CR","Agreement","","","60","5.5.3","RRM core (36.133) [NB_IOT-Core]",573600,"agreed","2017-05-03T23:04:35.507","2017-05-23T15:07:50.807","","","Rel-14","36.133","14.3.0","NB_IOT-Core","4843","","A","RP-171299","","","","",""]
["R4-1704675","On power headroom reporting for NB-IoT","Intel Corporation","Yang Tang","56725","discussion","Discussion","","","62","5.5.5","RRM Performance (36.133) [NB_IOT-Perf]",45130,"noted","2017-05-03T23:04:36.333","2017-05-06T13:17:51.527","","","Rel-13","","","NB_IOT-Core","","","","","","","","",""]
["R4-1704676","On absolute power control accuracy requirement for NB-IoT","Intel Corporation","Yang Tang","56725","discussion","Discussion","","","186","7.17.2","UE RF (36.101) [NB_IOTenh-Core]",46760,"noted","2017-05-03T23:04:36.363","2017-05-06T13:17:51.543","","","Rel-14","","","NB_IOTenh-Core","","","","","","","","",""]
["R4-1704677","CR on absolute power control accuracy for eNB-IoT","Intel Corporation","Yang Tang","56725","CR","Agreement","","","186","7.17.2","UE RF (36.101) [NB_IOTenh-Core]",46770,"withdrawn","2017-05-03T23:04:36.380",null,"","","Rel-14","36.101","14.3.0","NB_IOTenh-Core","4394","","F","","","","","",""]
["R4-1704678","On power headroom reporting for eNB-IoT","Intel Corporation","Yang Tang","56725","discussion","Discussion","","","195","7.17.3.2.3","PHR [NB_IOTenh-Core]",49840,"noted","2017-05-03T23:04:37.173","2017-05-06T13:17:51.543","","","Rel-14","","","NB_IOTenh-Core","","","","","","","","",""]
["R4-1704679","Correction to the table of intra-band non-contiguous CA with one uplink configuration for reference sensitivity","Intel Corporation","Yang Tang","56725","CR","Agreement","","","13","4.2.1","UE RF (core / EMC) [WI code or TEI12]",46790,"agreed","2017-05-03T23:04:37.190","2017-05-06T17:33:19.407","","","Rel-13","36.101","13.7.0","LTE_CA-Core","4395","","F","RP-171395","","","","",""]
["R4-1704680","Correction to the table of intra-band non-contiguous CA with one uplink configuration for reference sensitivity","Intel Corporation","Yang Tang","56725","CR","Agreement","","","13","4.2.1","UE RF (core / EMC) [WI code or TEI12]",46800,"agreed","2017-05-03T23:04:38.080","2017-05-06T17:33:19.407","","","Rel-14","36.101","14.3.0","LTE_CA-Core","4396","","A","RP-171395","","","","",""]
["R4-1704681","Correction to the table of intra-band non-contiguous CA with one uplink configuration for reference sensitivity","Intel Corporation","Yang Tang","56725","CR","Agreement","","","13","4.2.1","UE RF (core / EMC) [WI code or TEI12]",46810,"agreed","2017-05-03T23:04:38.890","2017-05-06T17:33:19.407","","","Rel-14","36.101","14.3.0","LTE_CA-Core","4397","","F","RP-171395","","","","",""]
["R4-1704682","On the 450 MHz band for LTE in Region 3 ? UE RF","Intel Corporation","Yang Tang","56725","other","Approval","","","347","9.10.3","UE RF (36.101) [LTE450_Reg3-core]",46820,"revised","2017-05-03T23:04:39.700","2017-05-06T17:33:19.407","","R4-1705898","","","","NR_newRAT","","","","","","","","",""]
["R4-1704683","On NR channel raster and synchronization signal raster","Intel Corporation","Yang Tang","56725","other","Discussion","","","419","10.3.2","Channel Raster [NR_newRAT]",46150,"noted","2017-05-03T23:04:39.717","2017-05-06T17:33:19.407","","","","","","NR_newRAT","","","","","","","","",""]
["R4-1704684","On NR mmWave UE antenna reference architecture","Intel Corporation","Yang Tang","56725","other","Discussion","","","425","10.4.2","Reference architecture [NR_newRAT]",48690,"noted","2017-05-03T23:04:39.733","2017-05-06T17:33:19.423","","","","","","NR_newRAT","","","","","","","","",""]
["R4-1704685","Further study on the feasibility of 3.3 - 4.2 GHz NR spectrum","Intel Corporation","Yang Tang","56725","other","Discussion","","","415","10.2.1.2","Band definition for NR bands [NR_newRAT]",52600,"withdrawn","2017-05-03T23:04:39.763","2017-05-06T09:07:51.903","","","Rel-15","","","NR_newRAT","","","","","","","","",""]
["R4-1704686","On consideration of mmWave UE power class","Intel Corporation","Yang Tang","56725","other","Discussion","","","427","10.4.3.1","UE power class and MPR/A-MPR [NR_newRAT]",51080,"withdrawn","2017-05-03T23:04:39.780","2017-05-06T09:07:51.917","","","Rel-15","","","NR_newRAT","","","","","","","","",""]
["R4-1704687","Transient On/Off Time for NR above-24 GHz","Intel Corporation","Yang Tang","56725","other","Discussion","","","428","10.4.3.2","ON/OFF time mask [NR_newRAT]",51990,"noted","2017-05-03T23:04:39.810","2017-05-06T09:07:51.933","","","Rel-15","","","NR_newRAT","","","","","","","","",""]
["R4-1704688","On supporting CBW and SCS mapping","Intel Corporation","Yang Tang","56725","other","Discussion","","","418","10.3.1","Channel bandwidth and subcarrier spacing [NR_newRAT]",52870,"noted","2017-05-03T23:04:39.827","2017-05-06T09:07:51.950","","","Rel-15","","","NR_newRAT","","","","","","","","",""]
["R4-1704689","E-UTRAN FDD - FDD Intra frequency RACH-less handover","Intel Corporation","Yang Tang","56725","CR","Approval","","","240","7.20.2","RRM performance (36.133) [LTE_eMob-Perf]",46890,"revised","2017-05-03T23:04:39.843","2017-05-06T17:36:28.810","","R4-1706001","Rel-14","36.133","14.3.0","LTE_eMob-Core","4844","","F","","","","","",""]
["R4-1704690","E-UTRAN FDD - FDD Inter frequency RACH-less handover","Intel Corporation","Yang Tang","56725","CR","Approval","","","240","7.20.2","RRM performance (36.133) [LTE_eMob-Perf]",46900,"revised","2017-05-03T23:04:40.623","2017-05-06T17:36:28.810","","R4-1706002","Rel-14","36.133","14.3.0","LTE_eMob-Core","4845","","F","","","","","",""]
["R4-1704691","E-UTRAN TDD - TDD Intra frequency RACH-less handover","Intel Corporation","Yang Tang","56725","CR","Approval","","","240","7.20.2","RRM performance (36.133) [LTE_eMob-Perf]",46910,"revised","2017-05-03T23:04:41.463","2017-05-06T17:36:28.810","","R4-1706003","Rel-14","36.133","14.3.0","LTE_eMob-Core","4846","","F","","","","","",""]
["R4-1704692","E-UTRAN TDD - TDD Inter frequency RACH-less handover","Intel Corporation","Yang Tang","56725","CR","Approval","","","240","7.20.2","RRM performance (36.133) [LTE_eMob-Perf]",46920,"revised","2017-05-03T23:04:42.230","2017-05-06T17:36:28.810","","R4-1706004","Rel-14","36.133","14.3.0","LTE_eMob-Core","4847","","F","","","","","",""]
["R4-1704693","On Maximum Transmission Timing Difference in Carrier Aggregation for sTTI","Intel Corporation","Yang Tang","56725","discussion","Discussion","","","385","9.13.4.3","Maximum reception/transmission timing difference [LTE_sTTIandPT-core]",46930,"noted","2017-05-03T23:04:43.040","2017-05-06T17:36:28.810","","","Rel-15","36.133","","","","","","","","","","",""]
["R4-1704694","LS on Maximum Transmission Timing Difference in CA for sTTI","Intel Corporation","Yang Tang","56725","LS out","Approval","","","385","9.13.4.3","Maximum reception/transmission timing difference [LTE_sTTIandPT-core]",46940,"revised","2017-05-03T23:04:43.057","2017-05-06T17:36:28.810","","R4-1706271","Rel-15","","","","","","","","","RAN2","","",""]
["R4-1704695","Further discussion on TS38.133 skeleton","Intel Corporation","Yang Tang","56725","discussion","Discussion","","","449","10.6.1","RRM General (ad-hoc MoM, Plan, Spec structure) [NR_newRAT]",46950,"noted","2017-05-03T23:04:43.070","2017-05-06T17:36:28.810","","","Rel-15","38.133","","","","","","","","","","",""]
["R4-1704696","Draft of TS38.133 v0.0.1","Intel Corporation","Yang Tang","56725","draft TS","Approval","","","449","10.6.1","RRM General (ad-hoc MoM, Plan, Spec structure) [NR_newRAT]",47600,"revised","2017-05-03T23:04:43.103","2017-05-06T17:36:28.827","","R4-1706324","Rel-15","38.133","0.0.1","NR_newRAT-Perf","","","","","","","","",""]
["R4-1704697","On UE measurement capability for NR","Intel Corporation","Yang Tang","56725","discussion","Discussion","","","450","10.6.2","UE measurement capability [NR_newRAT]",46970,"noted","2017-05-03T23:04:44.507","2017-05-06T17:36:28.827","","","Rel-15","38.133","","","","","","","","","","",""]
["R4-1704698","On set of configuration values for SS burst set periodicity","Intel Corporation","Yang Tang","56725","discussion","Discussion","","","411","10.1.2","Topics related to incoming LS from other WG [NR_newRAT]",45330,"noted","2017-05-03T23:04:44.523","2017-05-06T17:36:28.827","","","Rel-15","38.133","","","","","","","","","","",""]
["R4-1704699","Reply LS on set of configuration values for SS burst set periodicity","Intel Corporation","Yang Tang","56725","LS out","Approval","","","411","10.1.2","Topics related to incoming LS from other WG [NR_newRAT]",48000,"noted","2017-05-03T23:04:44.553","2017-05-06T17:36:28.827","","","Rel-15","","","","","","","","R1-1706708","RAN1","","",""]
["R4-1704700","On the feasibility of DC-related mobility enhancements in NR","Intel Corporation","Yang Tang","56725","discussion","Discussion","","","411","10.1.2","Topics related to incoming LS from other WG [NR_newRAT]",49900,"noted","2017-05-03T23:04:44.583","2017-05-06T17:36:28.843","","","Rel-15","38.133","","","","","","","","","","",""]
["R4-1704701","Reply LS on the feasibility of DC-related mobility enhancements in NR","Intel Corporation","Yang Tang","56725","LS out","Approval","","","411","10.1.2","Topics related to incoming LS from other WG [NR_newRAT]",51550,"noted","2017-05-03T23:04:44.600","2017-05-06T17:36:28.843","","","Rel-15","","","","","","","","R2-1703971","RAN2","RAN1","",""]
["R4-1704702","CR on inter-frequency and inter-RAT measurement requirement in idle mode R13","Intel Corporation","Yang Tang","56725","CR","Approval","","","47","5.4.3.2","Non-BL/CE UE [LTE_MTCe2_L1-Core]",47020,"noted","2017-05-03T23:04:44.630","2017-05-06T17:36:28.843","","","Rel-13","36.133","13.7.0","LTE_MTCe2_L1-Core","4848","","F","","","","","",""]
["R4-1704703","CR on inter-frequency and inter-RAT measurement requirement in CONNECTED mode R13","Intel Corporation","Yang Tang","56725","CR","Approval","","","47","5.4.3.2","Non-BL/CE UE [LTE_MTCe2_L1-Core]",47030,"noted","2017-05-03T23:04:45.503","2017-05-06T17:36:28.843","","","Rel-13","36.133","13.7.0","LTE_MTCe2_L1-Core","4849","","F","","","","","",""]
["R4-1704704","On requirement applicability for R14 non-BL/CE UE","Intel Corporation","Yang Tang","56725","discussion","Discussion","","","219","7.18.4","RRM core for non-BL/CE UE (36.133) [LTE_feMTC-Core]",618300,"noted","2017-05-03T23:04:46.440","2017-05-06T17:36:28.857","","","Rel-14","36.133","","","","","","","","","","",""]
["R4-1704705","CR on requirement applicability for R14 non-BL/CE UE","Intel Corporation","Yang Tang","56725","CR","Approval","","","219","7.18.4","RRM core for non-BL/CE UE (36.133) [LTE_feMTC-Core]",618400,"noted","2017-05-03T23:04:46.473","2017-05-06T17:36:28.857","","","Rel-14","36.133","14.3.0","LTE_feMTC-Core","4850","","F","","","","","",""]
["R4-1704706","Discussion on the RLM requirement for R14 non-BL/CE UE","Intel Corporation","Yang Tang","56725","discussion","Discussion","","","219","7.18.4","RRM core for non-BL/CE UE (36.133) [LTE_feMTC-Core]",572900,"noted","2017-05-03T23:04:47.297","2017-05-06T17:36:28.857","","","Rel-14","36.133","","LTE_feMTC-Core","","","","","","","","",""]
["R4-1704707","Discussion on the SI acquisition requirement for R14 non-BL/CE UE","Intel Corporation","Yang Tang","56725","discussion","Discussion","","","219","7.18.4","RRM core for non-BL/CE UE (36.133) [LTE_feMTC-Core]",47070,"noted","2017-05-03T23:04:47.330","2017-05-06T17:36:28.857","","","Rel-14","36.133","","","","","","","","","","",""]
["R4-1704708","Discussion on the RSRP and RSRQ measurement periods and accuracy for R14 non-BL/CE UE","Intel Corporation","Yang Tang","56725","discussion","Discussion","","","219","7.18.4","RRM core for non-BL/CE UE (36.133) [LTE_feMTC-Core]",48140,"withdrawn","2017-05-03T23:04:47.347",null,"","","Rel-14","36.133","","","","","","","","","","",""]
["R4-1704709","On RLM enhancement for FeMTC UE","Intel Corporation","Yang Tang","56725","discussion","Discussion","","","217","7.18.3.2.5","RLM and timing [LTE_feMTC-Core]",47100,"noted","2017-05-03T23:04:47.360","2017-05-06T17:36:28.857","","","Rel-14","36.133","","","","","","","","","","",""]
["R4-1704710","LS on RLM enhancement for FeMTC UE","Intel Corporation","Yang Tang","56725","LS out","Approval","","","217","7.18.3.2.5","RLM and timing [LTE_feMTC-Core]",50280,"revised","2017-05-03T23:04:47.393","2017-05-06T17:36:28.873","","R4-1705984","Rel-14","","","","","","","","","RAN2","","",""]
["R4-1704711","CR on inter-RAT measurement requirement in idle mode R14","Intel Corporation","Yang Tang","56725","CR","Approval","","","219","7.18.4","RRM core for non-BL/CE UE (36.133) [LTE_feMTC-Core]",47120,"noted","2017-05-03T23:04:47.407","2017-05-06T17:38:10.893","","","Rel-14","36.133","14.3.0","LTE_feMTC-Core","4851","","F","","","","","",""]
["R4-1704712","CR on inter-RAT measurement requirement in CONNECTED mode R14","Intel Corporation","Yang Tang","56725","CR","Approval","","","219","7.18.4","RRM core for non-BL/CE UE (36.133) [LTE_feMTC-Core]",47130,"withdrawn","2017-05-03T23:04:48.313","2017-05-06T17:38:10.893","","","Rel-14","36.133","14.3.0","LTE_feMTC-Core","4852","","F","","","","","",""]
["R4-1704713","On CE level selection for RACH for non-BL/CE UE","Intel Corporation","Yang Tang","56725","discussion","Discussion","","","219","7.18.4","RRM core for non-BL/CE UE (36.133) [LTE_feMTC-Core]",47060,"noted","2017-05-03T23:04:49.247","2017-05-06T17:38:10.910","","","Rel-14","36.133","","LTE_feMTC-Core","","","","","","","","",""]
["R4-1704714","On UE measurement gap for NSA NR","Intel Corporation","Yang Tang","56725","discussion","Discussion","","","452","10.6.4","Expected Measurement requirements for NSA [NR_newRAT]",52280,"noted","2017-05-03T23:04:49.263","2017-05-06T17:38:10.910","","","Rel-15","38.133","","","","","","","","","","",""]
["R4-1704715","CR on reduced MGL test case for FDD-FDD","Intel Corporation","Yang Tang","56725","CR","Approval","","","272","7.26.3","RRM performance (36.133) [LTE_meas_gap_enh-Perf]",47840,"revised","2017-05-03T23:04:49.280","2017-05-06T17:38:10.910","","R4-1705953","Rel-14","36.133","14.3.0","LTE_meas_gap_enh-Perf","4853","","B","","","","","",""]
["R4-1704716","CR on reduced MGL test case for TDD-TDD","Intel Corporation","Yang Tang","56725","CR","Approval","","","272","7.26.3","RRM performance (36.133) [LTE_meas_gap_enh-Perf]",574600,"revised","2017-05-03T23:04:50.217","2017-05-06T17:38:10.910","","R4-1705954","Rel-14","36.133","14.3.0","LTE_meas_gap_enh-Perf","4854","","B","","","","","",""]
["R4-1704717","CR on per-CC measurement gap for FDD-FDD inter-frequency measurements","Intel Corporation","Yang Tang","56725","CR","Approval","","","272","7.26.3","RRM performance (36.133) [LTE_meas_gap_enh-Perf]",575300,"noted","2017-05-03T23:04:51.137","2017-05-06T17:38:10.927","","","Rel-14","36.133","14.3.0","LTE_meas_gap_enh-Perf","4855","","B","","","","","",""]
["R4-1704718","CR  on NCSG for FDD-FDD inter-frequency measurements","Intel Corporation","Yang Tang","56725","CR","Approval","","","272","7.26.3","RRM performance (36.133) [LTE_meas_gap_enh-Perf]",47190,"noted","2017-05-03T23:04:51.977","2017-05-06T17:38:10.927","","","Rel-14","36.133","14.3.0","LTE_meas_gap_enh-Perf","4856","","B","","","","","",""]
["R4-1704719","CR on per-CC measurement gap for TDD-TDD inter-frequency measurements","Intel Corporation","Yang Tang","56725","CR","Approval","","","272","7.26.3","RRM performance (36.133) [LTE_meas_gap_enh-Perf]",575400,"noted","2017-05-03T23:04:52.867","2017-05-06T17:38:10.927","","","Rel-14","36.133","14.3.0","LTE_meas_gap_enh-Perf","4857","","B","","","","","",""]
["R4-1704720","CR  on NCSG for TDD-TDD inter-frequency measurements","Intel Corporation","Yang Tang","56725","CR","Approval","","","272","7.26.3","RRM performance (36.133) [LTE_meas_gap_enh-Perf]",47200,"noted","2017-05-03T23:04:53.727","2017-05-06T17:38:10.927","","","Rel-14","36.133","14.3.0","LTE_meas_gap_enh-Perf","4858","","B","","","","","",""]
["R4-1704721","CA RRM: 4DL CA test parameter correction for A.8.16.51 and A.8.16.52 (Rel-13)","Bureau Veritas, Anritsu","Amy Tao","62771","CR","Agreement","","","74","5.7.1.2","RRM [WI code]",47210,"agreed","2017-05-04T02:30:31.523","2017-05-08T15:16:12.193","","","Rel-13","36.133","13.7.0","LTE_CA_B1_B40-Perf","4859","","F","RP-171298","","","","",""]
["R4-1704722","CA RRM: 4DL CA test parameter correction for A.8.16.51 and A.8.16.52 (Rel-14)","Bureau Veritas, Anritsu","Amy Tao","62771","CR","Agreement","","","74","5.7.1.2","RRM [WI code]",47220,"agreed","2017-05-04T02:33:20.313","2017-05-23T15:07:50.820","","","Rel-14","36.133","14.3.0","LTE_CA_B1_B40-Perf","4860","","A","RP-171298","","","","",""]
["R4-1704723","TP for TR 36.714-03-01 : New BCS 1 for CA_1A_3A_26A","SK Telecom","Joonyoung Shin","62013","pCR","Approval","New BCS suggestion on CA_1A_3A_26A","","101","7.3.2","UE RF (36.101) [LTE_CA_R14_3DL1UL-Core]",51440,"approved","2017-05-04T05:41:55.390","2017-05-05T07:13:39.447","","","Rel-14","36.714-03-01","0.7.0","LTE_CA_R14_3DL1UL-Core","","","","","","","","",""]
["R4-1704724","TP for TR 36.714-04-01: Analysis for CA_1A_3A_7A_26A","SK Telecom","Joonyoung Shin","62013","pCR","","Harmonics/IMD Analysis on CA_1A_3A_7A_26A","","107","7.4.2","UE RF (36.101) [LTE_CA_R14_4DL1UL-Core]",48940,"approved","2017-05-04T05:43:55.320","2017-05-05T07:13:39.447","","","Rel-14","36.714-04-01","0.6.0","LTE_CA_R14_4DL1UL-Core","","","","","","","","",""]
["R4-1704725","TP for TR 36.714-05-01: Analysis for CA_1A_3A_7A_7A_26A","SK Telecom","Joonyoung Shin","62013","pCR","Approval","Harmonics/IMD Analysis on CA_1A_3A_7A_7A_26A","","113","7.5.2","UE RF (36.101) [LTE_CA_R14_5DL1UL-Core]",54330,"approved","2017-05-04T05:45:45.783","2017-05-05T07:13:39.447","","","Rel-14","36.714-05-01","0.7.0","LTE_CA_R14_5DL1UL-Core","","","","","","","","",""]
["R4-1704726","Introducing band 5 into V2X MCC operation","SK Telecom","Joonyoung Shin","62013","other","Approval","Introducing New LTE band 5 into V2X MCC operation","","340","9.9.1","General [LTE_V2X_CA_bands]",47260,"noted","2017-05-04T05:48:06.397","2017-05-05T07:13:39.447","","","Rel-15","","","","","","","","","","","",""]
["R4-1704727","Summary of simulation results for MUST","MediaTek inc.","Tsang-wei Yu","60138","discussion","Information","summary of simulation resutls for alignment","","254","7.24.1","Demodulation performance (36.101) [LTE_MUST-Perf]",47270,"noted","2017-05-04T06:03:23.867","2017-05-23T15:07:50.820","","","Rel-14","","","LTE_MUST-Perf","","","","","","","","",""]
["R4-1704728","CR on performance requirements for MUST Case 1 and Case 2","MediaTek inc.","Tsang-wei Yu","60138","CR","Approval","","","254","7.24.1","Demodulation performance (36.101) [LTE_MUST-Perf]",47280,"revised","2017-05-04T06:03:23.897","2017-05-05T08:31:37.627","","R4-1705955","Rel-14","36.101","14.3.0","LTE_MUST-Perf","4398","","B","","","","","",""]
["R4-1704729","CR on performance requirements for MUST Case 3","MediaTek inc.","Tsang-wei Yu","60138","CR","Approval","","","254","7.24.1","Demodulation performance (36.101) [LTE_MUST-Perf]",47290,"revised","2017-05-04T06:03:24.880","2017-05-05T08:31:37.643","","R4-1705950","Rel-14","36.101","14.3.0","LTE_MUST-Perf","4399","","B","","","","","",""]
["R4-1704730","CR on Fixed Reference Channels for MUST","MediaTek inc.","Tsang-wei Yu","60138","CR","Agreement","","","254","7.24.1","Demodulation performance (36.101) [LTE_MUST-Perf]",47300,"agreed","2017-05-04T06:03:25.757","2017-05-05T08:31:37.643","","","Rel-14","36.101","14.3.0","LTE_MUST-Perf","4400","","B","RP-171263","","","","",""]
["R4-1704731","CR on applicability rule for MUST Case 3","MediaTek inc.","Tsang-wei Yu","60138","CR","Approval","","","254","7.24.1","Demodulation performance (36.101) [LTE_MUST-Perf]",47310,"revised","2017-05-04T06:03:26.583","2017-05-05T08:31:37.643","","R4-1705956","Rel-14","36.101","14.3.0","LTE_MUST-Perf","4401","","B","","","","","",""]
["R4-1704732","CR on Defintions for MUST","MediaTek inc.","Tsang-wei Yu","60138","CR","Approval","","","254","7.24.1","Demodulation performance (36.101) [LTE_MUST-Perf]",47320,"noted","2017-05-04T06:03:27.407","2017-05-05T08:31:37.643","","","Rel-14","36.101","14.3.0","LTE_MUST-Perf","4402","","B","","","","","",""]
["R4-1704733","Discussion on MUST Case 1 and 2","MediaTek inc.","Tsang-wei Yu","60138","discussion","Discussion","Provide views on remaining issues for MUST Case 1 and 2","","255","7.24.1.1","Case1 and Case 2 [LTE_MUST-Perf]",47330,"noted","2017-05-04T06:03:28.297","2017-05-05T08:31:37.657","","","Rel-14","","","LTE_MUST-Perf","","","","","","","","",""]
["R4-1704734","Discussion on MUST Case 3","MediaTek inc.","Tsang-wei Yu","60138","discussion","Discussion","Provide views on remaining issues for MUST Case 3","","256","7.24.1.2","Case 3 [LTE_MUST-Perf]",51320,"noted","2017-05-04T06:03:28.330","2017-05-05T08:31:37.657","","","Rel-14","","","LTE_MUST-Perf","","","","","","","","",""]
["R4-1704735","Discussion on MUST Capability","MediaTek inc.","Tsang-wei Yu","60138","discussion","Discussion","Discuss MUST capability","","257","7.24.2","UE capbility [LTE_MUST]",47360,"noted","2017-05-04T06:03:28.343","2017-05-05T08:31:37.657","","","Rel-14","","","LTE_MUST","","","","","","","","",""]
["R4-1704736","Draft Reply LS on LTE Rel-14 UE feature list for MUST","MediaTek inc.","Tsang-wei Yu","60138","LS out","Approval","reply LS for R4-1702715","","257","7.24.2","UE capbility [LTE_MUST]",55340,"noted","2017-05-04T06:03:28.377","2017-05-05T08:31:37.673","","","Rel-14","","","LTE_MUST","","","","","R4-1702715","RAN2","RAN1","",""]
["R4-1704737","Clarification of NR UE RF terminologies of EIRP and Beam peak","Anritsu Corporation","Osamu Yamashita","66204","discussion","Endorsement","Discussion paper to clarify the definition of the terms ¡°EIRP¡± and ¡°Beam peak¡± in Table 6.2.1-1 in TR38.803.","","410","10.1.1","TR maintenance [NR_newRAT]",47370,"noted","2017-05-04T06:55:56.517","2017-05-05T07:05:10.307","","","Rel-14","38.803","","NR_newRAT-Core","","","","","","","","",""]
["R4-1704738","Addition of notes on EIRP and Beam peak definition for mmW","Anritsu Corporation","Osamu Yamashita","66204","CR","Agreement","Add a note in Table 6.2.1-1 to clarify the definition of the terms ¡°EIRP¡± and ¡°Beam peak¡±.","","410","10.1.1","TR maintenance [NR_newRAT]",47380,"noted","2017-05-04T07:03:13.120","2017-05-05T07:05:10.307","","","Rel-14","38.803","14.0.0","NR_newRAT","0007","","F","","","","","",""]
["R4-1704739","Discussion on Measurement Uncertainty Contributions of OTA Measurements for NR UE","Anritsu Corporation","Osamu Yamashita","66204","discussion","Discussion","Introduction of measurement uncertainty contributions of NR OTA measurements.","","461","10.7.2.2","Measurement uncertainty and test tolerance [FS_NR_test_methods]",47390,"noted","2017-05-04T07:07:59.297","2017-05-05T05:25:13.443","","","Rel-15","","","NR_newRAT-Core","","","","","","","","",""]
["R4-1704740","PCC and SCC assignment in 20MHz+10MHz test case A.8.16.22","ANRITSU LTD","Ian Rose","9381","CR","Agreement","This CR updates test cases A.8.16.22 to also allow the PCell to be 10MHz Channel BW, and the SCell to be 20MHz Channel BW.","","15","4.2.3","RRM (Radio Resource Management) [WI code or TEI12]",47400,"agreed","2017-05-04T07:09:14.237","2017-05-04T13:14:34.883","","","Rel-12","36.133","12.15.0","LTE_CA_B39_B41-Perf","4861","","F","RP-171296","","","","",""]
["R4-1704741","PCC and SCC assignment in 20MHz+10MHz test case A.8.16.22","ANRITSU LTD","Ian Rose","9381","CR","Agreement","This CR updates test cases A.8.16.22 to also allow the PCell to be 10MHz Channel BW, and the SCell to be 20MHz Channel BW.","","15","4.2.3","RRM (Radio Resource Management) [WI code or TEI12]",47410,"agreed","2017-05-04T07:14:17.590","2017-05-23T15:07:50.837","","","Rel-13","36.133","13.7.0","LTE_CA_B39_B41-Perf","4862","","A","RP-171296","","","","",""]
["R4-1704742","Correction of N_RB_agg for CA_41C in Table 7.3.1A-1","Anritsu Corporation","Osamu Yamashita","66204","CR","Agreement","Change N_RB_agg values at CA_41C in Table 7.3.1A-1","","13","4.2.1","UE RF (core / EMC) [WI code or TEI12]",47420,"agreed","2017-05-04T07:16:03.043","2017-05-05T03:11:58.393","","","Rel-12","36.101","12.15.0","TEI12","4403","","F","RP-171297","","","","",""]
["R4-1704743","PCC and SCC assignment in 20MHz+10MHz test case A.8.16.22","ANRITSU LTD","Ian Rose","9381","CR","Agreement","This CR updates test cases A.8.16.22 to also allow the PCell to be 10MHz Channel BW, and the SCell to be 20MHz Channel BW.","","15","4.2.3","RRM (Radio Resource Management) [WI code or TEI12]",47430,"agreed","2017-05-04T07:16:47.220","2017-05-23T15:07:50.837","","","Rel-14","36.133","14.3.0","LTE_CA_B39_B41-Perf","4863","","A","RP-171296","","","","",""]
["R4-1704744","Correction of N_RB_agg for CA_41C and CA_7C in Table 7.3.1A-1","Anritsu Corporation","Osamu Yamashita","66204","CR","Agreement","Change N_RB_agg values at CA_41C and CA_7C in Table 7.3.1A-1.","","13","4.2.1","UE RF (core / EMC) [WI code or TEI12]",47440,"agreed","2017-05-04T07:22:38.217","2017-05-05T03:11:58.393","","","Rel-13","36.101","13.7.0","TEI12","4404","","F","RP-171297","","","","",""]
["R4-1704745","Correction of N_RB_agg for CA_41C and CA_7C in Table 7.3.1A-1","Anritsu Corporation","Osamu Yamashita","66204","CR","Agreement","Change N_RB_agg values at CA_41C and CA_7C in Table 7.3.1A-1","","13","4.2.1","UE RF (core / EMC) [WI code or TEI12]",47450,"agreed","2017-05-04T07:25:35.727","2017-05-23T15:07:50.837","","","Rel-14","36.101","14.3.0","TEI12","4405","","A","RP-171297","","","","",""]
["R4-1704746","Correction to Test Parameters for Testing CDM-multiplexed DM RS","ANRITSU LTD","Ian Rose","9381","CR","","1) Corrected parameters for Downlink power allocation by taking into account of beamforming in Table 8.11.1.1.2.1-1.\n2) Added a parameter of simultaneous transmission in Table 8.11.1.1.2.1-1.","","53","5.4.6.1","BL/CE UE [LTE_MTCe2_L1-Perf]",47480,"noted","2017-05-04T08:01:13.077","2017-05-05T12:21:40.400","","","Rel-13","36.101","13.7.0","LTE_MTCe2_L1-Perf","4406","","F","","","","","",""]
["R4-1704747","Correction to Test Parameters for Testing CDM-multiplexed DM RS","ANRITSU LTD","Ian Rose","9381","CR","","1) Corrected parameters for Downlin power allocation by taking into account of beamforming in Table 8.11.1.1.2.1-1.\n2) Added a parameter of simultaneous transmission in Table 8.11.1.1.2.1-1.","","53","5.4.6.1","BL/CE UE [LTE_MTCe2_L1-Perf]",47490,"withdrawn","2017-05-04T08:04:21.333",null,"","","Rel-14","36.101","14.3.0","LTE_MTCe2_L1-Perf","4407","","A","","","","","",""]
["R4-1704748","Correction to Test Parameters for Cat M1 PUCCH 1-0 static test","ANRITSU LTD","Ian Rose","9381","CR","","1) Corrected Frequency hopping interval from 4 to N/A in Table 9.8.1.1-1.\n2) To avoid the CQI drop, added note 4 and also added parameters to schedule PUSCH.\n3) Corrected OCNG pattern in Note1 to OP.2.","","53","5.4.6.1","BL/CE UE [LTE_MTCe2_L1-Perf]",47491,"noted","2017-05-04T08:13:13.160","2017-05-05T13:21:51.280","","R4-1705998","Rel-13","36.101","13.7.0","LTE_MTCe2_L1-Perf","4408","","F","","","","","",""]
["R4-1704749","Correction to Test Parameters for Cat M1 PUCCH 1-0 static test","ANRITSU LTD","Ian Rose","9381","CR","","1) Corrected Frequency hopping interval from 4 to N/A in Table 9.8.1.1-1.\n2) To avoid the CQI drop, added note 4 and also added parameters to schedule PUSCH.\n3) Corrected OCNG pattern in Note1 to OP.2.","","53","5.4.6.1","BL/CE UE [LTE_MTCe2_L1-Perf]",620400,"withdrawn","2017-05-04T08:16:03.897",null,"","","Rel-14","36.101","14.3.0","LTE_MTCe2_L1-Perf","4409","","A","","","","","",""]
["R4-1704750","MIMO OTA harmonization testing results (part 3)","CATR","Ruixin Wang","64036","other","Discussion","","","146","7.11.3","Harmonization [LTE_MIMO_OTA-Core]",47500,"noted","2017-05-04T08:20:41.787","2017-06-06T13:47:53.497","","","Rel-14","","","LTE_MIMO_OTA-Core","","","","","","","","",""]
["R4-1704751","Noise issue in MPAC system","CATR","Ruixin Wang","64036","discussion","Discussion","","","145","7.11.2","Performance requirements [LTE_MIMO_OTA-Core]",573500,"noted","2017-05-04T08:24:21.180","2017-05-06T16:30:07.093","","","Rel-14","","","LTE_MIMO_OTA-Core","","","","","","","","",""]
["R4-1704752","Correction to Mapping of CQI Index to Modulation coding scheme for 256QAM","ANRITSU LTD","Ian Rose","9381","CR","Agreement","Updates Imcs mapping Tables A.4-14 and Table A.4-15 as per agreements at RAN4#82bis","","16","4.2.4","UE demodulation performance [WI code or TEI12]",47520,"agreed","2017-05-04T08:27:30.107","2017-05-05T15:02:14.400","","","Rel-12","36.101","12.15.0","LTE_SC_enh_L1-Perf","4410","","F","RP-171296","","","","",""]
["R4-1704753","Correction to Mapping of CQI Index to Modulation coding scheme for 256QAM","ANRITSU LTD","Ian Rose","9381","CR","Agreement","Updates Imcs mapping Tables A.4-14 and Table A.4-15 as per agreements at RAN4#82bis","","16","4.2.4","UE demodulation performance [WI code or TEI12]",47530,"agreed","2017-05-04T08:31:23.387","2017-05-23T15:07:50.853","","","Rel-13","36.101","13.7.0","LTE_SC_enh_L1-Perf","4411","","A","RP-171296","","","","",""]
["R4-1704754","Correction to Mapping of CQI Index to Modulation coding scheme for 256QAM","ANRITSU LTD","Ian Rose","9381","CR","Agreement","Updates Imcs mapping Tables A.4-14 and Table A.4-15 as per agreements at RAN4#82bis","","16","4.2.4","UE demodulation performance [WI code or TEI12]",47540,"agreed","2017-05-04T08:34:14.467","2017-05-23T15:07:50.853","","","Rel-14","36.101","14.3.0","LTE_SC_enh_L1-Perf","4412","","A","RP-171296","","","","",""]
["R4-1704755","Discussion on Framework Improvement for LTE BHH OTA","Samsung","Haijie Qiu","46265","discussion","Discussion","","","139","7.10.1","General [LTE_UTRA_TRP_TRS-Core]",51640,"noted","2017-05-04T08:36:47.203","2017-05-05T17:57:51.833","","","Rel-14","","","LTE_UTRA_TRP_TRS-Core","","","","","","","","",""]
["R4-1704756","CR for correction of 4RX demodulation requirements (Rel-13)","Samsung","Haijie Qiu","46265","CR","Approval","","","32","5.2.3","UE demodulation and CSI (36.101) [LTE_4Rx_AP_DL-Perf]",47560,"revised","2017-05-04T08:36:47.220","2017-05-05T17:57:51.863","","R4-1706193","Rel-13","36.101","13.7.0","LTE_4Rx_AP_DL-Perf","4413","","F","","","","","",""]
["R4-1704757","CR for correction of 4RX demodulation requirements (Rel-14)","Samsung","Haijie Qiu","46265","CR","Agreement","","","32","5.2.3","UE demodulation and CSI (36.101) [LTE_4Rx_AP_DL-Perf]",47570,"agreed","2017-05-04T08:36:48","2017-05-23T15:07:50.993","","","Rel-14","36.101","14.3.0","LTE_4Rx_AP_DL-Perf","4414","","A","RP-171304","","","","",""]
["R4-1704758","Discussion on NR UE capability","Samsung","Haijie Qiu","46265","discussion","Discussion","","","450","10.6.2","UE measurement capability [NR_newRAT]",47580,"noted","2017-05-04T08:36:48.797","2017-05-05T17:57:51.863","","","Rel-15","","","NR_newRAT","","","","","","","","",""]
["R4-1704759","Coexistence analysis on LTE-NR band combinations","Samsung","Haijie Qiu","46265","discussion","Discussion","","","416","10.2.2","NR-LTE band combinations proposals [NR_newRAT]",582600,"noted","2017-05-04T08:36:48.810","2017-05-05T17:57:51.863","","","Rel-15","","","NR_newRAT","","","","","","","","",""]
["R4-1704760","RAN1 and RAN2 RRM progress and impact on RAN4 RRM work","Samsung","Haijie Qiu","46265","discussion","Discussion","","","449","10.6.1","RRM General (ad-hoc MoM, Plan, Spec structure) [NR_newRAT]",47630,"noted","2017-05-04T08:36:48.827","2017-05-05T17:57:51.863","","","Rel-15","","","NR_newRAT","","","","","","","","",""]
["R4-1704761","Discussion on mobility measurement accuracy","Samsung","Haijie Qiu","46265","discussion","Discussion","","","453","10.6.5","System level and link level Simulation plan [NR_newRAT]",56120,"noted","2017-05-04T08:36:48.827","2017-05-05T17:57:51.880","","","Rel-15","","","NR_newRAT","","","","","","","","",""]
["R4-1704762","Discussion on cell detection delay","Samsung","Haijie Qiu","46265","discussion","Discussion","","","452","10.6.4","Expected Measurement requirements for NSA [NR_newRAT]",48020,"noted","2017-05-04T08:36:48.840","2017-05-05T17:57:51.880","","","Rel-15","","","NR_newRAT","","","","","","","","",""]
["R4-1704763","RAN1 and RAN2 RRM progress and impact on RAN4 RRM work","Samsung","Haijie Qiu","46265","discussion","Discussion","","","449","10.6.1","RRM General (ad-hoc MoM, Plan, Spec structure) [NR_newRAT]",578400,"withdrawn","2017-05-04T08:36:48.840",null,"","","Rel-15","","","NR_newRAT","","","","","","","","",""]
["R4-1704764","Discussion on mobility measurement accuracy","Samsung","Haijie Qiu","46265","discussion","Discussion","","","453","10.6.5","System level and link level Simulation plan [NR_newRAT]",56140,"withdrawn","2017-05-04T08:36:48.857",null,"","","Rel-15","","","NR_newRAT","","","","","","","","",""]
["R4-1704765","Discussion on cell detection delay","Samsung","Haijie Qiu","46265","discussion","Discussion","","","452","10.6.4","Expected Measurement requirements for NSA [NR_newRAT]",56110,"withdrawn","2017-05-04T08:36:48.873",null,"","","Rel-15","","","NR_newRAT","","","","","","","","",""]
["R4-1704766","WF on NR MU and test tolerance","CATR, Intel Corporation","Ruixin Wang","64036","other","Approval","","","458","10.7.1","General [FS_NR_test_methods]",47660,"approved","2017-05-04T08:39:02.377","2017-06-06T13:47:53.450","","","Rel-15","","","","","","","","","","","",""]
["R4-1704767","On MU for UE RF test setup","CATR","Ruixin Wang","64036","other","Discussion","","","461","10.7.2.2","Measurement uncertainty and test tolerance [FS_NR_test_methods]",47670,"noted","2017-05-04T08:49:50.470","2017-05-23T15:07:51.007","","","Rel-15","","","","","","","","","","","",""]
["R4-1704768","Discussion on Frequency Hopping Interval for Cat-M1 UE","ANRITSU LTD","Ian Rose","9381","discussion","","Aims to clarify whether specific Cat M1 demodulation test intend frequency hopping during the measurement or not.","","53","5.4.6.1","BL/CE UE [LTE_MTCe2_L1-Perf]",45840,"noted","2017-05-04T09:10:32.113","2017-05-04T13:47:24.270","","","Rel-13","","","LTE_MTCe2_L1-Perf","","","","","","","","",""]
["R4-1704769","Introduction of additional gap patterns and measurement capabilities for measurement gap enhancement","Ericsson, Nokia, Huawei","Christopher Callender","58614","CR","Agreement","CR to intrroduce NCSG and short MGL gap patterns in 36.133 chapter 8","","270","7.26.2.1","Gap pattern, signaling and capability (RAN2 related) [LTE_meas_gap_enh-Core]",51150,"revised","2017-05-04T09:48:02.257","2017-05-05T16:51:24.163","","R4-1706211","Rel-14","36.133","14.3.0","LTE_meas_gap_enh-Core","4864","","B","","","","","",""]
["R4-1704770","On band definition for 26.5-29.5GHz","Samsung, SK Telecom, KT Corporation, LG Uplus, NTT DOCOMO, INC.","Haijie Qiu","46265","discussion","Approval","","","415","10.2.1.2","Band definition for NR bands [NR_newRAT]",570000,"approved","2017-05-04T08:36:51.557","2017-05-05T17:57:51.880","","","Rel-15","","","NR_newRAT","","","","","","","","",""]
["R4-1704771","Consideration on Transmission BW configuration and CHBW in NR UE specification","Samsung","Haijie Qiu","46265","discussion","Discussion","","","418","10.3.1","Channel bandwidth and subcarrier spacing [NR_newRAT]",486201,"noted","2017-05-04T08:36:51.570","2017-05-05T17:57:51.897","","","Rel-15","","","NR_newRAT","","","","","","","","",""]
["R4-1704772","Discussion on NR channel raster and sync raster","Samsung","Haijie Qiu","46265","discussion","Discussion","","","419","10.3.2","Channel Raster [NR_newRAT]",47720,"noted","2017-05-04T08:36:51.570","2017-05-05T17:57:51.897","","","Rel-15","","","NR_newRAT","","","","","","","","",""]
["R4-1704773","Discussion on NR wideband operation","Samsung","Haijie Qiu","46265","discussion","Discussion","","","419","10.3.2","Channel Raster [NR_newRAT]",47730,"noted","2017-05-04T08:36:51.587","2017-05-05T17:57:51.897","","","Rel-15","","","NR_newRAT","","","","","","","","",""]
["R4-1704774","Mobile Station RF Front End Performance at 26.5GHz-29.5GHz","Samsung","Haijie Qiu","46265","discussion","Discussion","","","415","10.2.1.2","Band definition for NR bands [NR_newRAT]",570100,"noted","2017-05-04T08:36:51.603","2017-05-05T17:57:51.897","","","Rel-15","","","NR_newRAT","","","","","","","","",""]
["R4-1704775","RF Front End Efficiency Considerations at 26.5GHz-29.5GHz","Samsung","Haijie Qiu","46265","discussion","Discussion","","","415","10.2.1.2","Band definition for NR bands [NR_newRAT]",583500,"noted","2017-05-04T08:36:51.603","2017-05-05T17:57:51.897","","","Rel-15","","","NR_newRAT","","","","","","","","",""]
["R4-1704776","Overview on performance impact on Rel-14 eFD-MIMO WI","Samsung","Haijie Qiu","46265","discussion","Approval","","","281","7.28.1","General [LTE_eFDMIMO-Perf]",626800,"noted","2017-05-04T08:36:51.617","2017-05-05T17:57:51.910","","","Rel-14","","","LTE_eFDMIMO-Perf","","","","","","","","",""]
["R4-1704777","Test case design for CSI-RS enhancement","Samsung","Haijie Qiu","46265","discussion","Approval","","","287","7.28.2.5","CRI-RS Enhancement [LTE_eFDMIMO-Perf]",575100,"noted","2017-05-04T08:36:51.633","2017-05-05T17:57:51.910","","","Rel-14","","","LTE_eFDMIMO-Perf","","","","","","","","",""]
["R4-1704778","Test case design for semi-open-loop transmission","Samsung","Haijie Qiu","46265","discussion","Approval","","","283","7.28.2.1","Semi-open-loop transmission [LTE_eFDMIMO-Perf]",47780,"noted","2017-05-04T08:36:51.633","2017-05-05T17:57:51.910","","","Rel-14","","","LTE_eFDMIMO-Perf","","","","","","","","",""]
["R4-1704779","Test case design for Class A  PMI test case","Samsung","Haijie Qiu","46265","discussion","Approval","","","284","7.28.2.2","Class A PMI [LTE_eFDMIMO-Perf]",48100,"noted","2017-05-04T08:36:51.650","2017-05-05T17:57:51.910","","","Rel-14","","","LTE_eFDMIMO-Perf","","","","","","","","",""]
["R4-1704780","Tes case design for advacned CSI","Samsung","Haijie Qiu","46265","discussion","Approval","","","285","7.28.2.3","Advanced CSI [LTE_eFDMIMO-Perf]",47800,"revised","2017-05-04T08:36:51.650","2017-05-05T17:57:51.910","","R4-1706034","Rel-14","","","LTE_eFDMIMO-Perf","","","","","","","","",""]
["R4-1704781","Test case design for Hybrid CSI mechanism 1","Samsung","Haijie Qiu","46265","discussion","Approval","","","286","7.28.2.4","Hybrid CSI [LTE_eFDMIMO-Perf]",47810,"noted","2017-05-04T08:36:51.667","2017-05-05T17:57:51.927","","","Rel-14","","","LTE_eFDMIMO-Perf","","","","","","","","",""]
["R4-1704782","Test case design for Hybrid CSI mechanism 2","Samsung","Haijie Qiu","46265","discussion","Approval","","","286","7.28.2.4","Hybrid CSI [LTE_eFDMIMO-Perf]",47820,"noted","2017-05-04T08:36:51.680","2017-05-05T17:57:51.927","","","Rel-14","","","LTE_eFDMIMO-Perf","","","","","","","","",""]
["R4-1704783","Carrier Aggregation within NR","Samsung, SK Telecom, KT Corporation, LG Uplus","Haijie Qiu","46265","discussion","Approval","","","412","10.2","NR bands and NR-LTE band combinations [NR_newRAT]",51650,"noted","2017-05-04T08:36:51.697","2017-05-05T17:57:51.927","","","Rel-15","","","NR_newRAT","","","","","","","","",""]
["R4-1704784","Discussion on eGAP RRM tests","Ericsson","Christopher Callender","58614","discussion","Discussion","Consideration on feasibility of per CC and parallel measurement for gap enhancement","","272","7.26.3","RRM performance (36.133) [LTE_meas_gap_enh-Perf]",574800,"noted","2017-05-04T09:48:03.113","2017-05-05T16:51:24.163","","","Rel-14","","","LTE_meas_gap_enh-Perf","","","","","","","","",""]
["R4-1704785","Test cases list for eLAA RRM","Ericsson","Christopher Callender","58614","other","Approval","Test case list for eLAA RRM","","165","7.14.6","RRM performance (36.133) [LTE_eLAA-Perf]",47850,"noted","2017-05-04T09:48:03.113","2017-05-05T16:51:24.163","","","Rel-14","","","LTE_eLAA-Perf","","","","","","","","",""]
["R4-1704786","Test cases for eLAA","Ericsson","Christopher Callender","58614","discussion","Discussion","Discussion on test case list for eLAA RRM","","165","7.14.6","RRM performance (36.133) [LTE_eLAA-Perf]",47860,"noted","2017-05-04T09:48:03.127","2017-05-05T16:51:24.163","","","Rel-14","","","LTE_eLAA-Perf","","","","","","","","",""]
["R4-1704787","Introduction of event triggered reporting LAA test cases for multiple Scells","Ericsson","Christopher Callender","58614","CR","Agreement","event triggered reporting for LAA with multiple Scelols","","165","7.14.6","RRM performance (36.133) [LTE_eLAA-Perf]",47870,"revised","2017-05-04T09:48:03.143","2017-05-05T16:51:24.163","","R4-1705972","Rel-14","36.133","14.3.0","LTE_eLAA-Perf","4865","","B","","","","","",""]
["R4-1704788","MRTD and MTTD for carrier aggregation with sTTI","Ericsson","Christopher Callender","58614","discussion","Discussion","Discussion on maximum receive time difference and maximum transmit time difference for sTTI","","385","9.13.4.3","Maximum reception/transmission timing difference [LTE_sTTIandPT-core]",47880,"noted","2017-05-04T09:48:04.003","2017-05-05T16:51:24.180","","","Rel-15","","","LTE_sTTIandPT-Core","","","","","","","","",""]
["R4-1704789","Draft CR for introduction of requirements for sTTI and reduced processing time","Ericsson","Christopher Callender","58614","draftCR","Discussion","Draft CR for remaining changes needed in sTTI and procesing time reduction","","382","9.13.4","RRM core (36.133) [LTE_sTTIandPT-core]",47940,"noted","2017-05-04T09:48:04.017","2017-05-05T16:51:24.180","","","Rel-15","36.133","14.3.0","LTE_sTTIandPT-Core","","","","","","","","",""]
["R4-1704790","Scell activation and deactivation delay for sTTI and processing time reduction","Ericsson","Christopher Callender","58614","discussion","Discussion","Further discussion on Scell activation delay","","384","9.13.4.2","SCell activation and deactivation [LTE_sTTIandPT-core]",50560,"noted","2017-05-04T09:48:04.033","2017-05-05T16:51:24.180","","","Rel-15","","","LTE_sTTIandPT-Core","","","","","","","","",""]
["R4-1704791","Interruptions in sTTI and processing tme reduction","Ericsson","Christopher Callender","58614","discussion","Discussion","Further discusison on interruptions","","386","9.13.4.4","Interruption [LTE_sTTIandPT-core]",47910,"noted","2017-05-04T09:48:04.033","2017-05-05T16:51:24.180","","","Rel-15","","","LTE_sTTIandPT-Core","","","","","","","","",""]
["R4-1704792","TX timing requirements for sTTI and reduced processing time","Ericsson","Christopher Callender","58614","CR","Endorsement","CR to introduce TX timing requirements for sPUCCH/sPUSCH","","388","9.13.4.6","Others: PHR, measurement, timing [LTE_sTTIandPT-core]",47920,"revised","2017-05-04T09:48:04.050","2017-05-05T16:51:24.180","","R4-1706169","Rel-15","36.133","14.3.0","LTE_sTTIandPT-Core","4866","","B","","","","","",""]
["R4-1704793","TA adjustment delay for sTTI and processing time reduction","Ericsson","Christopher Callender","58614","discussion","Discussion","Further discussion on processing time reduction","","383","9.13.4.1","TA adjustment delay [LTE_sTTIandPT-core]",47930,"noted","2017-05-04T09:48:04.843","2017-05-05T16:51:24.197","","","Rel-15","","","LTE_sTTIandPT-Core","","","","","","","","",""]
["R4-1704794","RRM way forward for sTTI and processing time reduction","Ericsson","Christopher Callender","58614","other","Approval","RRM way forward for sTTI and processing time reduction","","382","9.13.4","RRM core (36.133) [LTE_sTTIandPT-core]",47890,"withdrawn","2017-05-04T09:48:04.860",null,"","","Rel-15","","","LTE_sTTIandPT-Core","","","","","","","","",""]
["R4-1704795","Discussion on NR RRM system level simulation plan","Ericsson","Christopher Callender","58614","discussion","Discussion","System level simulation plan for NR RRM work","","453","10.6.5","System level and link level Simulation plan [NR_newRAT]",45700,"noted","2017-05-04T09:48:04.860","2017-05-05T16:51:24.197","","","Rel-15","","","NR_newRAT","","","","","","","","",""]
["R4-1704796","Specification structure for NR RRM","Ericsson","Christopher Callender","58614","discussion","Discussion","Consideration on specification struture for 38.133","","449","10.6.1","RRM General (ad-hoc MoM, Plan, Spec structure) [NR_newRAT]",46960,"noted","2017-05-04T09:48:04.877","2017-05-05T16:51:24.197","","","Rel-15","","","NR_newRAT","","","","","","","","",""]
["R4-1704797","UE architecture: measurement gaps for inter-frequency and inter-RAT measurements","Ericsson","Christopher Callender","58614","discussion","Discussion","Discussion on measurement gap related aspects of UE architecture for NR","","455","10.6.7","UE architecture [NR_newRAT]",47970,"noted","2017-05-04T09:48:04.890","2017-05-05T16:51:24.197","","","Rel-15","","","NR_newRAT","","","","","","","","",""]
["R4-1704798","UE Architecture: Interruptions for NR RRM","Ericsson","Christopher Callender","58614","discussion","Discussion","Discussion on interruption related aspects of UE architecture for NR","","455","10.6.7","UE architecture [NR_newRAT]",47980,"noted","2017-05-04T09:48:04.907","2017-05-05T16:51:24.133","","","Rel-15","","","NR_newRAT","","","","","","","","",""]
["R4-1704799","SS burst set periodicity","Ericsson","Christopher Callender","58614","discussion","Discussion","Discussion of SS burst set periodicity and specifically on the feasibility of 160ms periodicity","","411","10.1.2","Topics related to incoming LS from other WG [NR_newRAT]",46980,"noted","2017-05-04T09:48:04.923","2017-05-05T16:51:24.133","","","Rel-15","","","NR_newRAT","","","","","","","","",""]
["R4-1704800","Reply LS on set of configuration values for SS burst set periodicity","Ericsson","Christopher Callender","58614","LS out","Approval","Reply LS on set of configuration values for SS burst set periodicity","","411","10.1.2","Topics related to incoming LS from other WG [NR_newRAT]",48050,"noted","2017-05-04T09:48:04.937","2017-05-05T16:51:24.133","","","Rel-15","","","NR_newRAT","","","","","R1-1706708","RAN WG1","","",""]
["R4-1704801","Changes needed to support NSA option 3 operation in 38.133","Ericsson","Christopher Callender","58614","discussion","Discussion","Outline of changes needed to 38.133 to introduce NSA option 3","","452","10.6.4","Expected Measurement requirements for NSA [NR_newRAT]",45340,"noted","2017-05-04T09:48:04.953","2017-05-05T16:51:24.150","","","Rel-15","","","NR_newRAT","","","","","","","","",""]
["R4-1704802","Changes needed to support NSA option 3 operation in 36.133","Ericsson","Christopher Callender","58614","discussion","Discussion","Outline of changes needed to 36.133 to introduce NSA option 3","","452","10.6.4","Expected Measurement requirements for NSA [NR_newRAT]",47620,"noted","2017-05-04T09:48:04.987","2017-05-05T16:51:24.150","","","Rel-15","","","NR_newRAT","","","","","","","","",""]
["R4-1704803","Measurement definition for NR","Ericsson","Christopher Callender","58614","discussion","Discussion","Further discussion on NR measurement definition","","454","10.6.6","Measurement definition and reference point [NR_newRAT]",50140,"noted","2017-05-04T09:48:04.987","2017-05-05T16:51:24.150","","","Rel-15","","","NR_newRAT","","","","","","","","",""]
["R4-1704804","Bandwidth aspects for NR measurements","Ericsson","Christopher Callender","58614","discussion","Discussion","Discussion on bandwidth aspects for NR measurements","","450","10.6.2","UE measurement capability [NR_newRAT]",51570,"noted","2017-05-04T09:48:05","2017-05-05T16:51:24.150","","","Rel-15","","","NR_newRAT","","","","","","","","",""]
["R4-1704805","Considerations on the feasibility of DC-related mobility enhancements in NR","Ericsson","Christopher Callender","58614","discussion","Discussion","Considering the issues raised in liaison statement R2-1703971","","411","10.1.2","Topics related to incoming LS from other WG [NR_newRAT]",49910,"noted","2017-05-04T09:48:05.017","2017-05-05T16:51:24.150","","","Rel-15","","","NR_newRAT","","","","","","","","",""]
["R4-1704806","NR RRM way forward","Ericsson","Christopher Callender","58614","other","Approval","NR RRM way forward","","449","10.6.1","RRM General (ad-hoc MoM, Plan, Spec structure) [NR_newRAT]",48060,"approved","2017-05-04T09:48:05.033","2017-05-23T15:07:51.007","","","Rel-15","","","NR_newRAT","","","","","","","","",""]
["R4-1704807","UE demodulation simulation results for FeMTC","Ericsson","Kazuyoshi Uesaka","46968","discussion","Discussion","This contribution shows the simulation results for PDSCH demodulation for FeMTC.","","227","7.18.8.1","BL/CE UE [LTE_feMTC-Perf]",55400,"noted","2017-05-04T10:18:20.480","2017-05-05T09:53:05.223","","","Rel-14","","","LTE_feMTC-Perf","","","","","","","","",""]
["R4-1704808","UE Demodulation and CQI requirements for Rel-14 non-BL UE supporting coverage enhancements","Ericsson","Kazuyoshi Uesaka","46968","discussion","Discussion","This contribution discusses the UE demodulation and CQI requirements for non-BL UE supporting coverage enhancement in Rel-14.","","228","7.18.8.2","Non-BL/CE UE [LTE_feMTC-Perf]",48080,"noted","2017-05-04T10:18:20.497","2017-05-05T10:02:15.493","","","Rel-14","","","LTE_feMTC-Perf","","","","","","","","",""]
["R4-1704809","UE demodulation simulation results for eNB-IoT","Ericsson","Kazuyoshi Uesaka","46968","discussion","Discussion","This contribution shows the simulation results for NPDSCH demodulation for eNB-IoT.","","202","7.17.6","UE demodulation(36.101) [NB_IOTenh-Perf]",55250,"noted","2017-05-04T10:18:20.513","2017-05-05T10:02:15.493","","","Rel-14","","","NB_IOTenh-Perf","","","","","","","","",""]
["R4-1704810","Discussion on UE requirements for eFD-MIMO CSI-RS Class A test","Ericsson","Kazuyoshi Uesaka","46968","discussion","Discussion","This contribution provides the simulation results for PMI reporting tests with Rel-14 CSI-RS class A codebook and discuss the simulation setup.","","284","7.28.2.2","Class A PMI [LTE_eFDMIMO-Perf]",49260,"noted","2017-05-04T10:18:20.527","2017-05-05T10:02:15.493","","","Rel-14","","","LTE_eFDMIMO-Perf","","","","","","","","",""]
["R4-1704811","Discussion on UE requirements for eFD-MIMO Advanced CSI reporting","Ericsson","Kazuyoshi Uesaka","46968","discussion","Discussion","This contribution shows our view on Advanced-CSI reporting test.","","285","7.28.2.3","Advanced CSI [LTE_eFDMIMO-Perf]",48110,"withdrawn","2017-05-04T10:18:20.543",null,"","","Rel-14","","","LTE_eFDMIMO-Perf","","","","","","","","",""]
["R4-1704812","UE Demodulation and CQI requirements for Rel-13 non-BL UE supporting coverage enhancements","Ericsson","Kazuyoshi Uesaka","46968","discussion","Discussion","This contribution discusses the UE demodulation and CQI requirements for non-BL UE supporting coverage enhancement in Rel-13.","","54","5.4.6.2","Non-BL/CE UE [LTE_MTCe2_L1-Perf]",46210,"noted","2017-05-04T10:18:20.573","2017-05-05T10:02:15.493","","","Rel-13","","","LTE_MTCe2_L1-Perf","","","","","","","","",""]
["R4-1704813","Clarification of demodulation requirements for UE supporting coverage enhancements","Ericsson","Kazuyoshi Uesaka","46968","CR","Approval","This CR clarifies the applicability of demodulation requirements for UE supporting coverage enhancements.","","54","5.4.6.2","Non-BL/CE UE [LTE_MTCe2_L1-Perf]",55420,"noted","2017-05-04T10:18:20.573","2017-05-05T10:02:15.510","","","Rel-13","36.101","13.7.0","LTE_MTCe2_L1-Perf","4415","","F","","","","","",""]
["R4-1704814","SI acquisition requirements for non-BL UE in Rel-14","Ericsson","Kazuyoshi Uesaka","46968","discussion","Discussion","This contribution discusses the SI acquisition requirements for non-BL/CE UE in Rel-14.","","219","7.18.4","RRM core for non-BL/CE UE (36.133) [LTE_feMTC-Core]",47110,"noted","2017-05-04T10:18:23.493","2017-05-05T10:02:15.510","","","Rel-14","","","LTE_feMTC-Core","","","","","","","","",""]
["R4-1704815","RLM requirements for non-BL UE in Rel-14","Ericsson","Kazuyoshi Uesaka","46968","discussion","Discussion","This contribution discusses the RLM requirements for non-BL/CE UE in Rel-14.","","219","7.18.4","RRM core for non-BL/CE UE (36.133) [LTE_feMTC-Core]",48150,"noted","2017-05-04T10:18:23.507","2017-05-05T10:02:15.510","","","Rel-14","","","LTE_feMTC-Core","","","","","","","","",""]
["R4-1704816","Clarification of PRB allocation for PUSCH test for eMTC (Rel-13)","Ericsson","Kazuyoshi Uesaka","46968","CR","Approval","This CR clarifies the PRB allocation and frequency hopping offset for eMTC PUSCH test.","","55","5.4.7","BS performance (36.104/36.141) [LTE_MTCe2_L1-Perf]",572001,"revised","2017-05-04T10:18:23.507","2017-05-05T10:02:15.527","","R4-1706037","Rel-13","36.141","13.7.0","LTE_MTCe2_L1-Perf","1025","","F","","","","","",""]
["R4-1704817","Clarification of PRB allocation for PUSCH test for eMTC (Rel-14)","Ericsson","Kazuyoshi Uesaka","46968","CR","Agreement","This CR clarifies the PRB allocation and frequency hopping offset for eMTC PUSCH test.","","55","5.4.7","BS performance (36.104/36.141) [LTE_MTCe2_L1-Perf]",626300,"agreed","2017-05-04T10:18:24.273","2017-05-23T15:07:51.023","","","Rel-14","36.141","14.3.0","LTE_MTCe2_L1-Perf","1026","","A","RP-171310","","","","",""]
["R4-1704818","Introduction of power class 1 HPUE in Band 3, 20 and 28","Huawei, Nokia, Motorola solutions, NTT DOCOMO","Xiang (Steven) Chen","41576","CR","Agreement","Introduction of power class 1 HPUE feature for Band 3, 20 and 28 into 36.101","","304","9.1.2","UE RF (36.101) [LTE_HPUE_B3_B20_B28]",54410,"revised","2017-05-04T11:00:45.013","2017-05-05T11:41:46.377","","R4-1705881","Rel-15","36.101","14.3.0","LTE_HPUE_B3_B20_B28","4416","","B","","","","","",""]
["R4-1704819","Aspects of Small Batteries for Even Further Enhanced MTC","Sony","Olof Zander","57059","discussion","","","","397","9.15.2.1","Lower power class [LTE_eMTC4-core]",48190,"noted","2017-05-04T11:06:37.537","2017-05-05T12:21:41.553","","","","","","","","","","","","","","",""]
["R4-1704820","Updated TR36.714-00-02 v0.8.0","LG Electronics Inc.","Suhwan Lim","46654","draft TR","","Update TR to captured the approved TPs and WF at last RAN4 meeting","","124","7.7.1","Rapporteur Input (WID/CRs) [LTE_CA_R14_xDL2UL-Core]",48200,"approved","2017-05-04T11:15:29.270","2017-05-04T12:27:33.563","","","Rel-14","36.714-00-02","0.8.0","LTE_CA_R14_xDL2UL-Core, LTE_CA_R14_xDL2UL-Perf","","","","","","","","",""]
["R4-1704821","Revised WID for xDL/UL inter-band CA with x=3,4,5 in Rel-14 for completion","LG Electronics Inc.","Suhwan Lim","46654","WID revised","","Provide revised WID to complete all proposed xDL/2UL CA band combinations in rel-14","","124","7.7.1","Rapporteur Input (WID/CRs) [LTE_CA_R14_xDL2UL-Core]",48210,"endorsed","2017-05-04T11:19:14.840","2017-05-04T13:15:27.920","","","Rel-14","","","LTE_CA_R14_xDL2UL-Core, LTE_CA_R14_xDL2UL-Perf","","","","","","","","",""]
["R4-1704822","New WID for xDL/UL inter-band CA with x=3,4,5 in Rel-15","LG Electronics Inc.","Suhwan Lim","46654","WID new","","Propose new WID for xDL/2UL CA basket WI in rel-15","","124","7.7.1","Rapporteur Input (WID/CRs) [LTE_CA_R14_xDL2UL-Core]",48220,"endorsed","2017-05-04T11:21:06.987","2017-05-23T15:07:51.023","","","Rel-15","","","","","","","","","","","",""]
["R4-1704823","BS RF Receiver NB intermodulation and spurious response issue","Ericsson","Dominique Everaere","63414","discussion","Approval","This contribution discussed the potential spurious response issue for NB intermodulation and general intermodulation requirement.","","59","5.5.2","BS RF core(36.104) [NB_IOT-Core]",54140,"noted","2017-05-04T11:23:49.567","2017-05-05T13:25:30.093","","","Rel-13","","","NB_IOT-Core","","","","","","","","",""]
["R4-1704824","CR NB-IoT FRC clarification","Ericsson","Dominique Everaere","63414","CR","Approval","This CR is a cleanup of FRC for NB-IoT, removing useless item that might be confusing","","59","5.5.2","BS RF core(36.104) [NB_IOT-Core]",48250,"revised","2017-05-04T11:23:49.583","2017-05-05T13:25:47.260","","R4-1705912","Rel-13","36.104","13.7.0","NB_IOT-Core","4669","","F","","","","","",""]
["R4-1704825","CR NB-IoT FRC clarification","Ericsson","Dominique Everaere","63414","CR","Approval","This CR is a cleanup of FRC for NB-IoT, removing useless item that might be confusing","","59","5.5.2","BS RF core(36.104) [NB_IOT-Core]",48280,"withdrawn","2017-05-04T11:23:50.427",null,"","","Rel-14","36.104","14.3.0","NB_IOT-Core","4670","","A","","","","","",""]
["R4-1704826","CR NB-IoT FRC clarification - test","Ericsson","Dominique Everaere","63414","CR","Approval","This CR is a cleanup of FRC for NB-IoT, removing useless item that might be confusing","","61","5.5.4","BS RF Conformance testing (36.141) [NB_IOT-Perf]",48321,"revised","2017-05-04T11:23:51.517","2017-05-05T13:25:47.260","","R4-1705915","Rel-13","36.141","13.7.0","NB_IOT-Perf","1027","","F","","","","","",""]
["R4-1704827","CR NB-IoT FRC clarification - test","Ericsson","Dominique Everaere","63414","CR","Approval","This CR is a cleanup of FRC for NB-IoT, removing useless item that might be confusing","","61","5.5.4","BS RF Conformance testing (36.141) [NB_IOT-Perf]",48340,"withdrawn","2017-05-04T11:23:52.437",null,"","","Rel-14","36.141","14.3.0","NB_IOT-Perf","1028","","A","","","","","",""]
["R4-1704828","CR NB-IoT Missing note Output power","Ericsson","Dominique Everaere","63414","CR","Approval","This CR is to align NB-IoT note related to BS output power in between 36.104 and 37.104","","59","5.5.2","BS RF core(36.104) [NB_IOT-Core]",48290,"revised","2017-05-04T11:23:53.390","2017-05-05T14:02:51.170","","R4-1705913","Rel-13","37.104","13.5.0","NB_IOT-Core","0777","","F","","","","","",""]
["R4-1704829","Missing clarification note related to BS output power when considering NB-IoT","Ericsson","Dominique Everaere","63414","CR","Agreement","This CR is to align NB-IoT note related to BS output power in between 36.104 and 37.104","","59","5.5.2","BS RF core(36.104) [NB_IOT-Core]",48300,"agreed","2017-05-04T11:23:54.217","2017-05-23T15:07:51.040","","","Rel-14","37.104","14.3.0","NB_IOT-Core","0778","","A","RP-171300","","","","",""]
["R4-1704830","CR NB-IoT Remove 1.4 MHz inband support","Ericsson","Dominique Everaere","63414","CR","Approval","This is to remove NB-IoT inband requirement from 1.4MHz which is supposed not to be supported.","","59","5.5.2","BS RF core(36.104) [NB_IOT-Core]",54000,"revised","2017-05-04T11:23:55.107","2017-05-05T15:19:36.787","","R4-1705870","Rel-13","37.104","13.5.0","NB_IOT-Core","0779","","F","","","","","",""]
["R4-1704831","Remove NB-IoT inband support for 1.4 MHz","Ericsson","Dominique Everaere","63414","CR","Agreement","This is to remove NB-IoT inband requirement from 1.4MHz which is supposed not to be supported.","","59","5.5.2","BS RF core(36.104) [NB_IOT-Core]",54010,"agreed","2017-05-04T11:23:55.933","2017-05-23T15:07:51.040","","","Rel-14","37.104","14.3.0","NB_IOT-Core","0780","","A","RP-171299","","","","",""]
["R4-1704832","CR NB-IoT Remove 1.4 MHz inband support - Test","Ericsson","Dominique Everaere","63414","CR","Approval","This is to remove NB-IoT inband requirement from 1.4MHz which is supposed not to be supported.","","61","5.5.4","BS RF Conformance testing (36.141) [NB_IOT-Perf]",48361,"revised","2017-05-04T11:23:56.777","2017-05-06T10:15:14.353","","R4-1705916","Rel-13","37.141","13.6.0","NB_IOT-Perf","0776","","F","","","","","",""]
["R4-1704833","Remove NB-IoT inband support for 1.4 MHz - Tests","Ericsson","Dominique Everaere","63414","CR","Agreement","This is to remove NB-IoT inband requirement from 1.4MHz which is supposed not to be supported.","","61","5.5.4","BS RF Conformance testing (36.141) [NB_IOT-Perf]",54020,"agreed","2017-05-04T11:23:57.697","2017-05-23T15:07:51.053","","","Rel-14","37.141","14.3.0","NB_IOT-Perf","0777","","A","RP-171302","","","","",""]
["R4-1704834","CR NB-IoT v_shift issue and editorials","Ericsson","Dominique Everaere","63414","CR","Approval","This CR is to fix NTM etst model for NB-IoT: cell-ID is not compatible with E-UTRA cell-ID for inband.","","61","5.5.4","BS RF Conformance testing (36.141) [NB_IOT-Perf]",54201,"revised","2017-05-04T11:23:58.553","2017-05-06T10:15:14.353","","R4-1705917","Rel-13","36.141","13.7.0","NB_IOT-Perf","1029","","F","","","","","",""]
["R4-1704835","NB-IoT Cell-ID value in Test Model N-TM and some editorials","Ericsson","Dominique Everaere","63414","CR","Agreement","This CR is to fix NTM etst model for NB-IoT: cell-ID is not compatible with E-UTRA cell-ID for inband.","","61","5.5.4","BS RF Conformance testing (36.141) [NB_IOT-Perf]",54220,"agreed","2017-05-04T11:23:59.380","2017-05-23T15:07:51.053","","","Rel-14","36.141","14.3.0","NB_IOT-Perf","1030","","A","RP-171302","","","","",""]
["R4-1704836","CR NB-IoT Wrong tolerances for NPUSCH format 1","Ericsson","Dominique Everaere","63414","CR","Approval","This CR is to fix NPUSCH format1 modulation requirements and make compatible with agreed tolerance","","65","5.5.6.2","BS Demodulation (36.104) [NB_IOT-Perf]",54230,"revised","2017-05-04T11:24:00.190","2017-05-06T10:15:14.367","","R4-1705966","Rel-13","36.141","13.7.0","NB_IOT-Perf","1031","","F","","","","","",""]
["R4-1704837","Wrong tolerance for NPUSCH format 1","Ericsson","Dominique Everaere","63414","CR","Agreement","This CR is to fix NPUSCH format1 modulation requirements and make compatible with agreed tolerance","","65","5.5.6.2","BS Demodulation (36.104) [NB_IOT-Perf]",54240,"agreed","2017-05-04T11:24:00.957","2017-05-23T15:07:51.053","","","Rel-14","36.141","14.3.0","NB_IOT-Perf","1032","","A","RP-171302","","","","",""]
["R4-1704838","Draft CR sTTI 2OS introduction","Ericsson","Dominique Everaere","63414","draftCR","Endorsement","This draft CR is a proposed draft to introduct sTTI 2OS feature in BS RF requirements","","378","9.13.3","BS RF (36.104) [LTE_sTTIandPT-core]",48380,"revised","2017-05-04T11:24:01.813","2017-05-06T10:16:30.770","","R4-1705933","Rel-14","36.104","14.3.0","LTE_sTTIandPT-Core","","","B","","","","","",""]
["R4-1704839","UE ON/OFF mask","Ericsson","Dominique Everaere","63414","discussion","Approval","This contribution proposes of each use case the corresponding UE ON/OFF mask","","374","9.13.2.2.1","ON/OFF time mask [LTE_sTTIandPT-core]",48400,"noted","2017-05-04T11:24:01.847","2017-05-06T10:16:30.817","","","Rel-15","","","LTE_sTTIandPT-Core","","","","","","","","",""]
["R4-1704840","Reply LS to RAN1 on on-off mask","Ericsson","Dominique Everaere","63414","LS out","Approval","This is a follow-up to previous reply to RAN1 LS regarding UE ON/OFF mask proposing the new specified masks","","374","9.13.2.2.1","ON/OFF time mask [LTE_sTTIandPT-core]",48410,"noted","2017-05-04T11:24:01.877","2017-05-06T10:16:30.833","","","Rel-15","","","LTE_sTTIandPT-Core","","","","","R1-1611054","RAN1","","",""]
["R4-1704841","UE reporting supported transient time parameters","Ericsson","Dominique Everaere","63414","discussion","Approval","This contribution discusses the benefit of UE reporting its supported transient time value and proposes to add this feature.","","374","9.13.2.2.1","ON/OFF time mask [LTE_sTTIandPT-core]",48420,"noted","2017-05-04T11:24:01.907","2017-05-06T10:16:30.833","","","Rel-15","","","LTE_sTTIandPT-Core","","","","","","","","",""]
["R4-1704842","LS to RAN2 on UE reporting its supported transient time parameters","Ericsson","Dominique Everaere","63414","LS out","Approval","This is proposed LS to RAN2 to add the possibility for a UE to report its supported transient time and so optimize performances.","","374","9.13.2.2.1","ON/OFF time mask [LTE_sTTIandPT-core]",48430,"noted","2017-05-04T11:24:01.923","2017-05-06T10:16:30.850","","","Rel-15","","","LTE_sTTIandPT-Core","","","","","","RAN2","RAN1","",""]
["R4-1704843","sTTI ON/OFF Mask: List of use cases","Ericsson","Dominique Everaere","63414","discussion","Approval","This contribution list all use cases to be considered when specifying the UE ON/OFF mask","","374","9.13.2.2.1","ON/OFF time mask [LTE_sTTIandPT-core]",51860,"revised","2017-05-04T11:24:01.987","2017-05-06T10:16:30.850","","R4-1706122","Rel-15","","","LTE_sTTIandPT-Core","","","","","","","","",""]
["R4-1704844","NB-IoT small cells: BS RF requirements","Ericsson","Dominique Everaere","63414","discussion","Discussion","This contribution further adresses BS RF requirements impact when introducing small cell supporting NB-IoT","","392","9.14.2.1","eNB power classes [NB_IOTenh2-core]",48440,"noted","2017-05-04T11:24:02","2017-05-06T10:15:58.867","","","Rel-15","","","NB_IOTenh2-Core","","","","","","","","",""]
["R4-1704845","NB-IoT small cells: coexistence simulations for BS RF requirements","Ericsson","Dominique Everaere","63414","discussion","Approval","This contribution further discusses about the simulations needed when specifying BS RF requirements for NB-IoT small cells","","392","9.14.2.1","eNB power classes [NB_IOTenh2-core]",48460,"noted","2017-05-04T11:24:02.033","2017-05-06T10:15:58.883","","","Rel-15","","","NB_IOTenh2-Core","","","","","","","","",""]
["R4-1704846","NB-IoT small cells: Simulation assumptions for BS RF requirements","Ericsson","Dominique Everaere","63414","discussion","Discussion","This contribution proposes the simulation assumptions for NB-IoT small cells","","392","9.14.2.1","eNB power classes [NB_IOTenh2-core]",54260,"noted","2017-05-04T11:24:02.047","2017-05-06T10:15:58.883","","","Rel-15","","","NB_IOTenh2-Core","","","","","","","","",""]
["R4-1704847","CR to finalize introduction of Band 21 supporting NB-IoT","Ericsson","Dominique Everaere","63414","CR","Approval","This CR finalizes NB-IoT support in band 21 in TS 37.141. This CR was missing in last RAN4#82b meeting when B21 was introduced","","132","7.8.3","BS RF (36.104) [NB_IOT_R14_bands]",48470,"revised","2017-05-04T11:24:02.080","2017-05-06T10:15:34.890","","R4-1705861","Rel-14","37.141","14.3.0","NB_IOT_R14_bands","0778","","B","","","","","",""]
["R4-1704848","MSD test results for xDL/2UL CA with self-desense problems","LG Electronics Inc.","Suhwan Lim","46654","discussion","Approval","We propose the MSD test results for each CA combination with potential IMD problems. The MSD levels can be merged with other MSD test results from interested companies to decide MSD level.","","125","7.7.2","UE RF (36.101) [LTE_CA_R14_xDL2UL-Core]",48560,"noted","2017-05-04T11:24:12.920","2017-05-04T13:15:27.937","","","","","","LTE_CA_R14_xDL2UL-Core","","","","","","","","",""]
["R4-1704849","TP on summay of MSD levels for xDL/2UL CA with self desense issues","LG Electronics Inc.","Suhwan Lim","46654","pCR","Approval","Propose TP to add the MSD test results for xDL/2UL CA band combinations with self-desense problems","","125","7.7.2","UE RF (36.101) [LTE_CA_R14_xDL2UL-Core]",53070,"revised","2017-05-04T11:28:36.977","2017-05-04T13:15:27.937","","R4-1705874","Rel-14","36.714-00-02","0.8.0","LTE_CA_R14_xDL2UL-Core","","","","","","","","",""]
["R4-1704850","A common concept for handling OTA co-location requirements","Ericsson","Torbjorn Elfstrom","44796","other","Approval","This intension with this contribution is give our view on the above given open issues listed in the way-forward agreed last meeting.","","360","9.12.2.3","Co-location requirements [AASenh_BS_LTE_UTRA-Core]",48780,"noted","2017-05-04T11:28:58.473","2017-05-05T15:51:48.987","","","Rel-15","","","AASenh_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-1704851","Draft TS 37.105 specification text for OTA reference sensitivity in sub-clause 10.3","Ericsson","Torbjorn Elfstrom","44796","discussion","Discussion","This contribution presents draft TS 37.105 specification text for OTA reference sensitivity in sub-clause 10.3. The intension is to use the draft as discussion material in the work of developing the CR implementing the new OTA requirements for eAAS base s","","356","9.12.1","General [AASenh_BS_LTE_UTRA]",56530,"noted","2017-05-04T11:28:58.473","2017-05-05T15:51:48.987","","","Rel-15","","","AASenh_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-1704852","Draft TS 37.105 specification text for Transmit signal quality (sub-clause 9.6) and bandwidth (sub-clause 9.7)","Ericsson","Torbjorn Elfstrom","44796","discussion","Discussion","At the end of this contribution draft specification text is attached for discussion.","","356","9.12.1","General [AASenh_BS_LTE_UTRA]",56531,"revised","2017-05-04T11:28:58.490","2017-05-05T15:51:48.987","","R4-1706129","Rel-15","","","AASenh_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-1704853","Conformance test aspects related to OTA unwanted emission","Ericsson","Torbjorn Elfstrom","44796","discussion","Discussion","This intension with this contribution is to summarize all emission requirement and discuss around some potential candidate test methods emission requirements.","","366","9.12.3.1","RF conformance requirements [AASenh_BS_LTE_UTRA-Perf]",48530,"noted","2017-05-04T11:28:58.503","2017-05-05T15:51:49.020","","","Rel-15","","","AASenh_BS_LTE_UTRA-Perf","","","","","","","","",""]
["R4-1704854","On antenna loss factor to be assumed when deriving OTA requirements","Ericsson","Torbjorn Elfstrom","44796","other","Approval","This contribution continues the discussion of the antenna loss factor assumption to be used as a base for defining OTA requirements.","","359","9.12.2.2","Tx and Rx loss values [AASenh_BS_LTE_UTRA-Core]",48540,"noted","2017-05-04T11:28:58.503","2017-05-05T15:51:49.020","","","Rel-15","","","AASenh_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-1704855","On fundamental aspects related to measuring TRP emissions","Ericsson","Torbjorn Elfstrom","44796","discussion","Discussion","This contribution presents some relevant information on fundamental aspects vital for measuring TRP emissions.","","366","9.12.3.1","RF conformance requirements [AASenh_BS_LTE_UTRA-Perf]",48550,"noted","2017-05-04T11:28:58.520","2017-05-05T15:51:48.957","","","Rel-15","","","AASenh_BS_LTE_UTRA-Perf","","","","","","","","",""]
["R4-1704856","Introduction of new 3DL/2UL CA band combinations in rel-14","LG Electronics, CHTTL, SoftBank Corp., KDDI","Suhwan Lim","46654","CR","Agreement","Introduce new CA band combinations for 3DL/2UL CA in Rel-14. \n?\tDL: CA_3A-42C,     UL: CA_42C\n?\tDL: CA_28A-42C,   UL: CA_42C \n?\tDL: CA_41C-42A,   UL: CA_41C\n?\tDL: CA_3A-7A-8A,       UL: CA_3A-7A, CA_3A-8A, CA_7A-8A \n?\tDL: CA_3A-41A-42A,   UL: CA_41A-42A\n?","","125","7.7.2","UE RF (36.101) [LTE_CA_R14_xDL2UL-Core]",48480,"agreed","2017-05-04T11:33:21.907","2017-05-23T15:07:51.053","","","Rel-14","36.101","14.3.0","LTE_CA_R14_xDL2UL-Core","4417","","B","RP-171278","","","","",""]
["R4-1704857","Introduction of test method for OTA unwanted emission","Ericsson","Torbjorn Elfstrom","44796","discussion","Discussion","The measurement equipment in terms of chamber and positioner is similar to traditional chambers used for EMC radiated emission and susceptibility testing. A measurement procedure is developed to capture unwanted emission radiation coming from the test obj","","366","9.12.3.1","RF conformance requirements [AASenh_BS_LTE_UTRA-Perf]",48570,"noted","2017-05-04T11:28:59.767","2017-05-05T15:51:48.957","","","Rel-15","","","AASenh_BS_LTE_UTRA-Perf","","","","","","","","",""]
["R4-1704858","Draft applicability table for TS 38.104","Ericsson","Torbjorn Elfstrom","44796","discussion","Discussion","This intension with this contribution is to stimulate the discussion on how to create the requirement applicability table for TS 38.104.","","436","10.5.1","BS RF General (ad-hoc MoM, Plan, Spec structure) [NR_newRAT]",52360,"noted","2017-05-04T11:28:59.800","2017-05-05T15:51:48.957","","","Rel-15","","","NR_newRAT","","","","","","","","",""]
["R4-1704859","Draft TS 37.105 specification text for requirement applicability table in clause 5.","Ericsson","Torbjorn Elfstrom","44796","discussion","Discussion","An applicability table with BS types is proposed to be introduced in TS 37.105, sub-clause clause 5.1. The BS type in general and selects different types of requirements to be met for different types of AAS base stations. The intension with this contribut","","356","9.12.1","General [AASenh_BS_LTE_UTRA]",53890,"noted","2017-05-04T11:28:59.800","2017-05-05T15:51:48.973","","","Rel-15","","","AASenh_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-1704860","Introduction of new 4DL/2UL CA band combination in Rel-14","LG Electronics, CHTTL, Softbank Mobile, KDDI","Suhwan Lim","46654","CR","Agreement","Introduce new CA band combinations for 4DL/2UL CA in Rel-14.\n?\tDL: CA_41C-42C,               UL: CA_41C\n?\tDL: CA_3C-7C,                   UL: CA_3A-7A\n?\tDL: CA_3A-28A-41A-42A,   UL: CA_41A-42A\n?\tDL: CA_3A-28A-42C,          UL: CA_42C\n?\tDL: CA_3A-41A-42C,","","125","7.7.2","UE RF (36.101) [LTE_CA_R14_xDL2UL-Core]",48490,"agreed","2017-05-04T11:36:57.727","2017-05-23T15:07:51.070","","","Rel-14","36.101","14.3.0","LTE_CA_R14_xDL2UL-Core","4418","","B","RP-171278","","","","",""]
["R4-1704861","A-SE measurement BW in Band 41","LG Electronics Inc.","Suhwan Lim","46654","CR","Agreement","The A-SE requirement for Band 41 with NS_04 is inconsistent with FCC regulation. The measurement BW in 3GPP is define with 1MHz to measure 0MHz offset from the lower edge of Band 41. In case, some UEs do not satisfy the A-SE requirement evenif apply A-MPR","","291","7.29.2","RF [WI code or TEI14]",54470,"revised","2017-05-04T12:00:26.513","2017-05-04T13:15:27.953","","R4-1705864","Rel-14","36.101","14.3.0","LTE_B41_UE_PC2-Core","4419","","F","","","","","",""]
["R4-1704862","NR subcarrier spacing considerations for above 6GHz bands","AT&T","Arun Ghosh","57084","discussion","Decision","","","418","10.3.1","Channel bandwidth and subcarrier spacing [NR_newRAT]",567600,"revised","2017-05-04T12:04:25.220","2017-05-06T22:27:51.487","","R4-1705839","","","","","","","","","","","","",""]
["R4-1704863","NR channel raster for sub 6GHz and above 6GHz bands","AT&T","Arun Ghosh","57084","discussion","Decision","","","419","10.3.2","Channel Raster [NR_newRAT]",48630,"revised","2017-05-04T12:04:25.220","2017-05-06T22:27:51.503","","R4-1705840","","","","","","","","","","","","",""]
["R4-1704864","UE antenna array configuration for mmWave 28GHz","Sony, Ericsson","Olof Zander","57059","discussion","","Two different antenna configurations, patch arrays and linear dipole arrays, for the 28GHz band has been analyzed from a diversity point of view.","","425","10.4.2","Reference architecture [NR_newRAT]",46840,"noted","2017-05-04T12:07:00.293","2017-05-04T17:44:04.130","","","","","","","","","","","","","","",""]
["R4-1704865","CR on V2X duplexer mode and Pumax for non-concurrent operaion","LG Electronics Inc.","Suhwan Lim","46654","CR","Agreement","V2X UE consider Half duplexer for sidelink operation. But this is not noticed in TS 36.101. Also the Pumax for non-current V2X UE definition is not cleared.","","177","7.16.2","UE RF Maintenance (36.101) [LTE_V2X-Core]",48650,"revised","2017-05-04T12:08:22.677","2017-05-04T13:15:27.890","","R4-1706089","Rel-14","36.101","14.3.0","LTE_V2X-Core","4420","","F","","","","","",""]
["R4-1704866","Frequency Response of UE mmWave antennas for the 28GHz band","Sony, Ericsson","Olof Zander","57059","discussion","","Gain versus frequency response is studied for three different antenna types for the 28GHz band.","","425","10.4.2","Reference architecture [NR_newRAT]",48640,"noted","2017-05-04T12:12:32.723","2017-05-04T17:44:04.130","","","","","","","","","","","","","","",""]
["R4-1704867","Updated TR36.787 v0.1.0 for V2X new band combinations","LG Electronics Inc.","Suhwan Lim","46654","draft TR","Approval","Provide update TR v0.1.0 to capture the approved TPs at last RAN4 meeting","","339","9.9","V2X new band combinations [LTE_V2X_CA_bands]",48670,"approved","2017-05-04T12:15:40.450","2017-05-04T12:35:58.477","","","Rel-15","36.787","0.1.0","LTE_V2X_CA_bands, LTE_V2X_CA_bands-Core","","","","","","","","",""]
["R4-1704868","Spatial multiplexing for mmWave 28GHz","Sony, Ericsson","Olof Zander","57059","other","Approval","Proposal 1: Baseline UE DL capability shall be 2x2 MIMO in the 28GHz mmWave range for the smartphone type UE. \nProposal 2: Send an LS to RAN1 with cc to RAN2 informing decision in RAN4.","","425","10.4.2","Reference architecture [NR_newRAT]",48660,"noted","2017-05-04T12:17:11.243","2017-05-04T17:44:04.147","","","","","","","","","","","","","","",""]
["R4-1704869","draft LS on Spatial multiplexing for mmWave NR","Sony, Ericsson","Olof Zander","57059","LS out","","RAN WG4 have decided the minimum UE DL capability of 2x2 MIMO in the 28GHz mmWave range.","","425","10.4.2","Reference architecture [NR_newRAT]",48680,"noted","2017-05-04T12:21:33.817","2017-05-04T17:44:04.147","","","","","","","","","","","","RAN1","RAN2","",""]
["R4-1704870","Candidate solution for Harmonics/IMD problem on own licensed band and ITS band","LG Electronics Inc.","Suhwan Lim","46654","pCR","Approval","we provide our views on how to solve the self-interference problems by harmonics and IMD products from own transmissions of inter-band con-current V2X UE.","","341","9.9.2","UE RF (36.101) [LTE_V2X_CA_bands-core]",48700,"approved","2017-05-04T12:32:33.937","2017-05-04T13:15:27.907","","","Rel-15","36.787","0.1.0","LTE_V2X_CA_bands","","","","","","","","",""]
["R4-1704871","Correction of payload in R.75 TDD","Rohde & Schwarz","Niels Petrovic","49274","CR","Agreement","","","32","5.2.3","UE demodulation and CSI (36.101) [LTE_4Rx_AP_DL-Perf]",48710,"noted","2017-05-04T12:33:51.527","2017-05-04T12:40:19.867","","","Rel-13","36.101","13.7.0","LTE_4Rx_AP_DL-Perf","4421","","F","","","","","",""]
["R4-1704872","Correction of payload in R.75 TDD","Rohde & Schwarz","Niels Petrovic","49274","CR","Agreement","","","32","5.2.3","UE demodulation and CSI (36.101) [LTE_4Rx_AP_DL-Perf]",48720,"withdrawn","2017-05-04T12:33:52.340",null,"","","Rel-14","36.101","14.3.0","LTE_4Rx_AP_DL-Perf","4422","","A","","","","","",""]
["R4-1704873","Correction of test points for Single-antenna port performance TDD FDD CA","Rohde & Schwarz","Niels Petrovic","49274","CR","Agreement","","","70","5.6.3","Demodulation and CSI [WI code or TEI13]",48730,"revised","2017-05-04T12:33:53.213","2017-05-04T12:40:19.867","","R4-1706210","Rel-13","36.101","13.7.0","TEI13","4423","","F","","","","","",""]
["R4-1704874","Correction of test points for Single-antenna port performance TDD FDD CA","Rohde & Schwarz","Niels Petrovic","49274","CR","Agreement","","","70","5.6.3","Demodulation and CSI [WI code or TEI13]",48740,"agreed","2017-05-04T12:33:54.040","2017-05-23T15:07:51.070","","","Rel-14","36.101","14.3.0","TEI13","4424","","A","RP-171311","","","","",""]
["R4-1704875","TP for TR 37.843: Improvements of definitions of spatial angles in sub-clause 4.6","Ericsson","Torbjorn Elfstrom","44796","pCR","Approval","The text proposal is attached for approval at the end of this contribution.","","356","9.12.1","General [AASenh_BS_LTE_UTRA]",48750,"revised","2017-05-04T12:39:46.750","2017-05-05T15:51:48.973","","R4-1706124","Rel-15","37.843","0.2.0","AASenh_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-1704876","TP for TR 37.843: Updating EIS formula and background in sub-clause 6.2","Ericsson","Torbjorn Elfstrom","44796","pCR","Approval","The intension with this contribution is to update the background information in TR 37.843 to be in line with proposals in a companion contribution related to antenna loss factors for AAS base stations.","","363","9.12.2.6","Other Receiver requirements [AASenh_BS_LTE_UTRA-Core]",52330,"noted","2017-05-04T12:39:46.797","2017-05-05T15:51:48.973","","","Rel-15","37.843","0.2.0","AASenh_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-1704877","TP for TR 37.843: Addition of agreements from WF in sub-clause 6.2","Ericsson","Torbjorn Elfstrom","44796","pCR","Approval","This text proposal captures agreements from last meeting in TR 37.843, sub-clause 6.2.2.","","363","9.12.2.6","Other Receiver requirements [AASenh_BS_LTE_UTRA-Core]",52320,"noted","2017-05-04T12:39:46.857","2017-05-05T15:51:48.973","","","Rel-15","37.843","0.2.0","AASenh_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-1704878","TP for TR 37.843: Adding Annex for background information common for co-location requirements","Ericsson","Torbjorn Elfstrom","44796","pCR","Approval","This contribution holds a text proposal to add an annex for common background information for all BS-to-BS co-location requirements.","","360","9.12.2.3","Co-location requirements [AASenh_BS_LTE_UTRA-Core]",613300,"approved","2017-05-04T12:39:46.890","2017-05-05T15:51:48.973","","","Rel-15","37.843","0.2.0","AASenh_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-1704879","TP on the additional ILs level for V2X_20-47 concurrent operation UE","LG Electronics Inc.","Suhwan Lim","46654","pCR","Approval","We propose additional IL for V2X_20A-47A based on commertial HTF. Tib =0.2 dB and Rib =0.2dB for Band 20.","","341","9.9.2","UE RF (36.101) [LTE_V2X_CA_bands-core]",48790,"approved","2017-05-04T12:42:01.687","2017-05-04T13:15:27.907","","","Rel-15","36.787","0.1.0","LTE_V2X_CA_bands, LTE_V2X_CA_bands-Core","","","","","","","","",""]
["R4-1704880","Revised WID: Basket WI for LTE Advanced Intra-band CA Rel-14","Ericsson","Per Lindell","56972","WID revised","Endorsement","Revised WID: Basket WI for LTE Advanced Intra-band Rel-14 CA, including editorial corrections compared to the endorsed version at RAN4 82bis","","88","7.1.1","Rapporteur Input (WID/CRs) [LTE_CA_R14_intra-Core]",48820,"endorsed","2017-05-04T12:45:04.763","2017-06-06T13:47:53.557","","","Rel-14","","","LTE_CA_R14_intra-Core","","","","","","","","",""]
["R4-1704881","Revised WID: Basket WI for LTE Advanced inter-band CA Rel-14 for 4DL/1UL","Ericsson","Per Lindell","56972","WID revised","Endorsement","Revised WID: Basket WI for LTE Advanced 4DL/1UL Rel-14 CA, including editorial corrections compared to the endorsed version at RAN4 82bis","","106","7.4.1","Rapporteur Input (WID/CRs) [LTE_CA_R14_4DL1UL-Core]",48830,"endorsed","2017-05-04T12:45:04.797","2017-06-06T13:47:53.557","","","Rel-14","","","LTE_CA_R14_4DL1UL-Core","","","","","","","","",""]
["R4-1704882","Basket WI for LTE Advanced Intra-band CA Rel-15","Ericsson","Per Lindell","56972","WID new","Endorsement","Basket WI for LTE Advanced Intra-band CA Rel-15, including updates compared to the endorsed version at RAN4 82bis","","88","7.1.1","Rapporteur Input (WID/CRs) [LTE_CA_R14_intra-Core]",48841,"revised","2017-05-04T12:45:04.810","2017-06-06T13:47:53.543","","R4-1705899","","","","","","","","","","","","",""]
["R4-1704883","Basket WI for LTE Advanced inter-band CA Rel-15 for 4DL/1UL","Ericsson","Per Lindell","56972","WID new","Endorsement","Basket WI for LTE Advanced inter-band CA Rel-15 for 4DL/1UL, including updates compared to the endorsed version at RAN4 82bis","","106","7.4.1","Rapporteur Input (WID/CRs) [LTE_CA_R14_4DL1UL-Core]",48850,"endorsed","2017-05-04T12:45:04.827","2017-06-06T13:47:53.557","","","","","","","","","","","","","","",""]
["R4-1704884","Intra-band TR 36.714-00-00 version 0.7.0","Ericsson","Per Lindell","56972","draft TR","Approval","Intra-band TR 36.714-00-00 version 0.7.0 including the approved TP's from RAN4 #82bis","","88","7.1.1","Rapporteur Input (WID/CRs) [LTE_CA_R14_intra-Core]",48800,"approved","2017-05-04T12:45:04.857","2017-05-05T11:21:51.807","","","Rel-14","36.714-00-00","0.6.0","LTE_CA_R14_intra","","","","","","","","",""]
["R4-1704885","4DL/1UL TR 36.714-04-01 version 0.7.0","Ericsson","Per Lindell","56972","draft TR","Approval","4DL/1UL TR 36.714-04-01 version 0.7.0 including the approved TP's from RAN4 #82bis","","106","7.4.1","Rapporteur Input (WID/CRs) [LTE_CA_R14_4DL1UL-Core]",48810,"approved","2017-05-04T12:45:06.200","2017-05-05T11:21:51.840","","","Rel-14","36.714-04-01","0.6.0","LTE_CA_R14_4DL1UL","","","","","","","","",""]
["R4-1704886","Introduction of Rel-14 Intra-band combinations in 36.101","Ericsson","Per Lindell","56972","CR","Approval","Introduction of Intra-band combinations in 36.101 (big CR)","","88","7.1.1","Rapporteur Input (WID/CRs) [LTE_CA_R14_intra-Core]",48860,"revised","2017-05-04T12:45:07.540","2017-05-23T15:07:51.100","","R4-1706099","Rel-14","36.101","14.3.0","LTE_CA_R14_intra-Core","4425","","B","","","","","",""]
["R4-1704887","Introduction of Rel-14 Intra-band combinations in 36.104","Ericsson","Per Lindell","56972","CR","Approval","Introduction of Intra-band combinations in 36.104 (big CR)","","88","7.1.1","Rapporteur Input (WID/CRs) [LTE_CA_R14_intra-Core]",48870,"revised","2017-05-04T12:45:08.417","2017-05-23T15:07:51.100","","R4-1706100","Rel-14","36.104","14.3.0","LTE_CA_R14_intra-Core","4671","","B","","","","","",""]
["R4-1704888","Introduction of Rel-14 Intra-band combinations in 36.141","Ericsson","Per Lindell","56972","CR","Approval","Introduction of Intra-band combinations in 36.141 (big CR)","","88","7.1.1","Rapporteur Input (WID/CRs) [LTE_CA_R14_intra-Core]",48880,"revised","2017-05-04T12:45:09.227","2017-05-23T15:07:51.100","","R4-1706101","Rel-14","36.141","14.3.0","LTE_CA_R14_intra-Core","1033","","B","","","","","",""]
["R4-1704889","Introduction of Rel-14 4DL/1UL combinations in 36.101","Ericsson","Per Lindell","56972","CR","Approval","Introduction of Rel-14 4DL/1UL combinations in 36.101 (big CR)","","106","7.4.1","Rapporteur Input (WID/CRs) [LTE_CA_R14_4DL1UL-Core]",48890,"revised","2017-05-04T12:45:10.053","2017-05-23T15:07:51.117","","R4-1706085","Rel-14","36.101","14.3.0","LTE_CA_R14_4DL1UL","4426","","B","","","","","",""]
["R4-1704890","Introduction of Rel-14 4DL/1UL combinations in 36.104","Ericsson","Per Lindell","56972","CR","Approval","Introduction of Rel-14 4DL/1UL combinations in 36.104 (big CR)","","106","7.4.1","Rapporteur Input (WID/CRs) [LTE_CA_R14_4DL1UL-Core]",48900,"revised","2017-05-04T12:45:10.927","2017-05-23T15:07:51.117","","R4-1706086","Rel-14","36.104","14.3.0","LTE_CA_R14_4DL1UL","4672","","B","","","","","",""]
["R4-1704891","Introduction of Rel-14 4DL/1UL combinations in 36.141","Ericsson","Per Lindell","56972","CR","Approval","Introduction of Rel-14 4DL/1UL combinations in 36.141 (big CR)","","106","7.4.1","Rapporteur Input (WID/CRs) [LTE_CA_R14_4DL1UL-Core]",48910,"revised","2017-05-04T12:45:11.753","2017-05-23T15:07:51.117","","R4-1706087","Rel-14","36.141","14.3.0","LTE_CA_R14_4DL1UL","1034","","B","","","","","",""]
["R4-1704892","CA_4DL_3A-7A-20A-28A_1UL_BCS0","Ericsson","Per Lindell","56972","pCR","Approval","TP to introduce CA_4DL_3A-7A-20A-28A_1UL_BCS0","","107","7.4.2","UE RF (36.101) [LTE_CA_R14_4DL1UL-Core]",48960,"revised","2017-05-04T12:45:12.547","2017-05-05T11:21:51.840","","R4-1705905","Rel-14","36.714-04-01","0.7.0","LTE_CA_R14_4DL1UL-Core","","","","","","","","",""]
["R4-1704893","CA_4DL_1A-7A-20A-28A_1UL_BCS0","Ericsson","Per Lindell","56972","pCR","Approval","TP to introduce CA_4DL_1A-7A-20A-28A_1UL_BCS0","","107","7.4.2","UE RF (36.101) [LTE_CA_R14_4DL1UL-Core]",48970,"revised","2017-05-04T12:45:14.513","2017-05-05T11:21:51.793","","R4-1705906","Rel-14","36.714-04-01","0.7.0","LTE_CA_R14_4DL1UL-Core","","","","","","","","",""]
["R4-1704894","CA_4DL_1A-3A-20A-28A_1UL_BCS0","Ericsson","Per Lindell","56972","pCR","Approval","TP to introduce CA_4DL_1A-3A-20A-28A_1UL_BCS0","","107","7.4.2","UE RF (36.101) [LTE_CA_R14_4DL1UL-Core]",48980,"revised","2017-05-04T12:45:14.577","2017-05-05T11:21:51.793","","R4-1705907","Rel-14","36.714-04-01","0.7.0","LTE_CA_R14_4DL1UL-Core","","","","","","","","",""]
["R4-1704895","CA_5DL_1A-3A-7A-20A-28A_1UL_BCS0","Ericsson","Per Lindell","56972","pCR","Approval","TP to introduce CA_5DL_1A-3A-7A-20A-28A_1UL_BCS0","","113","7.5.2","UE RF (36.101) [LTE_CA_R14_5DL1UL-Core]",54830,"approved","2017-05-04T12:45:14.640","2017-05-05T11:21:51.793","","","Rel-14","36.714-05-01","0.6.0","LTE_CA_R14_5DL1UL-Core","","","","","","","","",""]
["R4-1704896","CA_4DL_2A-48A-48A-66A_1UL_BCS0","Ericsson, Verizon","Per Lindell","56972","pCR","Approval","TP to introduce CA_4DL_2A-48A-48A-66A_1UL_BCS0","","107","7.4.2","UE RF (36.101) [LTE_CA_R14_4DL1UL-Core]",53240,"revised","2017-05-04T12:45:14.687","2017-05-05T11:21:51.793","","R4-1705908","Rel-14","36.714-04-01","0.7.0","LTE_CA_R14_4DL1UL-Core","","","","","","","","",""]
["R4-1704897","CA_4DL_48D-66A _1UL_BCS0","Ericsson, Verizon","Per Lindell","56972","pCR","Approval","TP to introduce CA_4DL_48D-66A _1UL_BCS0","","107","7.4.2","UE RF (36.101) [LTE_CA_R14_4DL1UL-Core]",53280,"approved","2017-05-04T12:45:14.747","2017-05-05T11:21:51.793","","","Rel-14","36.714-04-01","0.7.0","LTE_CA_R14_4DL1UL-Core","","","","","","","","",""]
["R4-1704898","CA_4DL_48A-48C-66A_1UL_BCS0","Ericsson, Verizon","Per Lindell","56972","pCR","Approval","TP to introduce CA_4DL_48A-48C-66A_1UL_BCS0","","107","7.4.2","UE RF (36.101) [LTE_CA_R14_4DL1UL-Core]",53290,"approved","2017-05-04T12:45:14.797","2017-05-05T11:21:51.793","","","Rel-14","36.714-04-01","0.7.0","LTE_CA_R14_4DL1UL-Core","","","","","","","","",""]
["R4-1704899","CA_3DL_2A-48A-48A _1UL_BCS0","Ericsson, Verizon","Per Lindell","56972","pCR","Approval","TP to introduce CA_3DL_2A-48A-48A _1UL_BCS0","","101","7.3.2","UE RF (36.101) [LTE_CA_R14_3DL1UL-Core]",52970,"revised","2017-05-04T12:45:14.857","2017-05-05T11:21:51.807","","R4-1705903","Rel-14","36.714-03-01","0.6.0","LTE_CA_R14_3DL1UL-Core","","","","","","","","",""]
["R4-1704900","Revised WID on V2X new band combinations in Rel-15","LG Electronics Inc.","Suhwan Lim","46654","WID revised","Approval","Provide revised WID to include additonal new V2X band combination for V2X_5A-47A and V2X_34A-47A","","339","9.9","V2X new band combinations [LTE_V2X_CA_bands]",49000,"endorsed","2017-05-04T12:45:43.170","2017-05-23T15:07:51.117","","","Rel-15","","","LTE_V2X_CA_bands, LTE_V2X_CA_bands-Core","","","","","","","","",""]
["R4-1704901","CR on introduction of V2X_20-47 band combination","LG Electronics Inc.","Suhwan Lim","46654","CR","Agreement","Introduce new V2X band combination which has harmonic problems in own Rx band. So RAN4 mandate harmonic trap filter to protect Band 47. RAN4 define additional IL term for the HTF.","","341","9.9.2","UE RF (36.101) [LTE_V2X_CA_bands-core]",49010,"revised","2017-05-04T12:51:10.427","2017-05-04T13:15:27.907","","R4-1705876","Rel-15","36.101","14.3.0","LTE_V2X_CA_bands-Core","4427","","B","","","","","",""]
["R4-1704902","CR on reference configurations for V2X RRM tests","CATT","Xuhua Tao","62863","CR","Approval","","","179","7.16.4","RRM performance (36.133) [LTE_V2X-Perf]",50500,"revised","2017-05-04T12:53:35.080","2017-05-05T15:25:57.133","","R4-1705948","Rel-14","36.133","14.3.0","LTE_V2X-Perf","4867","","F","","","","","",""]
["R4-1704903","Correction on reliability of GNSS singal for V2V","CATT","Xuhua Tao","62863","CR","Approval","","","169","7.15.2","RRM core maintenance (36.133) [LTE_SL_V2V-Core]",49030,"revised","2017-05-04T12:53:35.877","2017-05-05T15:25:57.150","","R4-1705944","Rel-14","36.133","14.3.0","LTE_SL_V2V-Core","4868","","F","","","","","",""]
["R4-1704904","CR on reliability of GNSS singal for V2X","CATT","Xuhua Tao","62863","CR","Approval","","","178","7.16.3","RRM core Maintenance (36.133) [LTE_V2X-Core]",49041,"revised","2017-05-04T12:53:36.750","2017-05-05T15:25:57.150","","R4-1705945","Rel-14","36.133","14.3.0","LTE_V2X-Core","4869","","F","","","","","",""]
["R4-1704905","Test cases for E-UTRAN initiation/cease of SLSS Transmission for V2X sidelink communication","CATT","Xuhua Tao","62863","CR","Approval","","","179","7.16.4","RRM performance (36.133) [LTE_V2X-Perf]",50390,"noted","2017-05-04T12:53:37.623","2017-05-05T15:25:57.150","","","Rel-14","36.133","14.3.0","LTE_V2X-Perf","4870","","F","","","","","",""]
["R4-1704906","Test cases for V2X initiation/cease of SLSS Transmission when GNSS as synchronization source","CATT","Xuhua Tao","62863","CR","Approval","","","179","7.16.4","RRM performance (36.133) [LTE_V2X-Perf]",50400,"noted","2017-05-04T12:53:38.483","2017-05-05T15:25:57.150","","","Rel-14","36.133","14.3.0","LTE_V2X-Perf","4871","","F","","","","","",""]
["R4-1704907","Test cases for V2X UE transmission timing accuracy","CATT","Xuhua Tao","62863","CR","Approval","","","179","7.16.4","RRM performance (36.133) [LTE_V2X-Perf]",49060,"noted","2017-05-04T12:53:39.543","2017-05-05T15:25:57.150","","","Rel-14","36.133","14.3.0","LTE_V2X-Perf","4872","","F","","","","","",""]
["R4-1704908","Further discussion on RRM requirements impact for sTTI and processing time reduction","CATT","Xuhua Tao","62863","discussion","Discussion","","","383","9.13.4.1","TA adjustment delay [LTE_sTTIandPT-core]",50550,"noted","2017-05-04T12:53:41.243","2017-05-05T15:25:57.150","","","Rel-15","","","LTE_sTTIandPT-Core","","","","","","","","",""]
["R4-1704909","Discussion on UE transmit timing requirement for NR","CATT","Xuhua Tao","62863","discussion","Discussion","","","451","10.6.3","UE transmit timing [NR_newRAT]",49090,"noted","2017-05-04T12:53:41.243","2017-05-05T15:25:57.163","","","Rel-15","","","NR_newRAT","","","","","","","","",""]
["R4-1704910","Alignment and Impairment results for V2V single link demodulation performance requirements","CATT","Xuhua Tao","62863","discussion","Discussion","","","172","7.15.4.1","Single-link PSSCH and PSCCH [LTE_SL_V2V-Perf]",55430,"noted","2017-05-04T12:53:41.273","2017-05-05T15:25:57.163","","","Rel-14","","","LTE_SL_V2V-Perf","","","","","","","","",""]
["R4-1704911","Updated results and discussion for V2V power imbalance test","CATT","Xuhua Tao","62863","discussion","Discussion","","","173","7.15.4.2","Multi-link PSSCH and PSCCH [LTE_SL_V2V-Perf]",49110,"noted","2017-05-04T12:53:41.320","2017-05-05T15:25:57.163","","","Rel-14","","","LTE_SL_V2V-Perf","","","","","","","","",""]
["R4-1704912","Discussion on PSSCH/PSCCH maximum processing capability tests","CATT","Xuhua Tao","62863","discussion","Discussion","","","181","7.16.5.1","PSSCH/PSCCH maximum processing capability test [LTE_V2X-Perf]",49120,"noted","2017-05-04T12:53:41.353","2017-05-05T15:25:57.163","","","Rel-14","","","LTE_V2X-Perf","","","","","","","","",""]
["R4-1704913","Evaluation result for PSBCH demodulation test","CATT","Xuhua Tao","62863","discussion","Discussion","","","182","7.16.5.2","PSBCH, eNB sync and WAN SDR [LTE_V2X-Perf]",55510,"noted","2017-05-04T12:53:41.367","2017-05-05T15:25:57.163","","","Rel-14","","","LTE_V2X-Perf","","","","","","","","",""]
["R4-1704914","Discussion on the open issues for V2X demodulation tests","CATT","Xuhua Tao","62863","discussion","Discussion","","","182","7.16.5.2","PSBCH, eNB sync and WAN SDR [LTE_V2X-Perf]",55490,"noted","2017-05-04T12:53:41.400","2017-05-05T15:25:57.163","","","Rel-14","","","LTE_V2X-Perf","","","","","","","","",""]
["R4-1704915","Discussion on the feasibility of DC-related mobility enhancements in NR","CATT","Xuhua Tao","62863","discussion","Decision","","","411","10.1.2","Topics related to incoming LS from other WG [NR_newRAT]",51230,"noted","2017-05-04T12:53:41.460","2017-05-05T15:25:57.180","","","Rel-15","","","NR_newRAT","","","","","","","","",""]
["R4-1704916","Response LS on the feasibility of DC-related mobility enhancements in NR","CATT","Xuhua Tao","62863","discussion","Approval","","","411","10.1.2","Topics related to incoming LS from other WG [NR_newRAT]",52930,"noted","2017-05-04T12:53:41.493","2017-05-05T15:25:57.180","","","Rel-15","","","NR_newRAT","","","","","","","","",""]
["R4-1704917","Discussion on specification structure of TS38.101","CATT","Xuhua Tao","62863","discussion","Discussion","","","424","10.4.1","UE RF General (ad-hoc MoM, Plan, Spec Structure) [NR_newRAT]",615600,"noted","2017-05-04T12:53:41.523","2017-05-05T15:25:57.180","","","Rel-15","","","NR_newRAT","","","","","","","","",""]
["R4-1704918","Discussion on time mask for NR UE","CATT","Xuhua Tao","62863","discussion","Discussion","","","428","10.4.3.2","ON/OFF time mask [NR_newRAT]",567300,"noted","2017-05-04T12:53:41.557","2017-05-05T15:25:57.180","","","Rel-15","","","NR_newRAT","","","","","","","","",""]
["R4-1704919","Draft CR on mutli carriers with high transmit power V2X UE","CATT","Xuhua Tao","62863","other","Endorsement","","","402","9.16.2.2","Mutli carriers with high transmit power [LTE_eV2X-core]",49190,"endorsed","2017-05-04T12:53:41.570","2017-05-05T15:25:57.180","","","Rel-15","36.101","","LTE_eV2X-Core","","","","","","","","",""]
["R4-1704920","Consideration on  beam related new requirement for  NR","CATT","Xuhua Tao","62863","discussion","Discussion","","","436","10.5.1","BS RF General (ad-hoc MoM, Plan, Spec structure) [NR_newRAT]",53320,"noted","2017-05-04T12:53:41.603","2017-05-05T15:25:57.180","","","Rel-15","","","NR_newRAT","","","","","","","","",""]
["R4-1704921","Discussion on  Transmit ON/OFF power OTA requirement","CATT","Xuhua Tao","62863","discussion","Discussion","","","362","9.12.2.5","Other Transmitter Requirements [AASenh_BS_LTE_UTRA-Core]",53150,"noted","2017-05-04T12:53:41.617","2017-05-05T15:25:57.197","","","Rel-14","","","AASenh_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-1704922","Discussion scaling factor for OTA AAS BS","CATT","Xuhua Tao","62863","discussion","Discussion","","","362","9.12.2.5","Other Transmitter Requirements [AASenh_BS_LTE_UTRA-Core]",56510,"revised","2017-05-04T12:53:41.617","2017-05-05T15:25:57.197","","R4-1706137","Rel-14","","","AASenh_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-1704923","PDSCH demodulation performance of Enhanced CRS-IM","CATT","Xuhua Tao","62863","discussion","Discussion","","","277","7.27.2.1","PDSCH [LTE_eCRSIM_eSUMIMO]",46370,"noted","2017-05-04T12:53:41.633","2017-05-05T15:25:57.197","","","Rel-14","","","LTE_eCRSIM_eSUMIMO","","","","","","","","",""]
["R4-1704924","PDCCH demodulation performance of Enhanced CRS-IM","CATT","Xuhua Tao","62863","discussion","Discussion","","","278","7.27.2.2","Control channel [LTE_eCRSIM_eSUMIMO]",46340,"noted","2017-05-04T12:53:41.650","2017-05-05T15:25:57.197","","","Rel-14","","","LTE_eCRSIM_eSUMIMO","","","","","","","","",""]
["R4-1704925","PDSCH demodulation performance of Enhanced SU-MIMO IM","CATT","Xuhua Tao","62863","discussion","Discussion","","","279","7.27.3","SU-MIMO IM [LTE_eCRSIM_eSUMIMO]",49550,"noted","2017-05-04T12:53:41.710","2017-05-05T15:25:57.197","","","Rel-14","","","LTE_eCRSIM_eSUMIMO","","","","","","","","",""]
["R4-1704926","simulation results for PMI test of CSI-RS Class A","CATT","Xuhua Tao","62863","discussion","Discussion","","","284","7.28.2.2","Class A PMI [LTE_eFDMIMO-Perf]",55600,"noted","2017-05-04T12:53:41.727","2017-05-05T15:25:57.197","","","Rel-14","","","LTE_eFDMIMO-Perf","","","","","","","","",""]
["R4-1704927","Clean ups of TS36.101 for V2X requirements","CATT","Xuhua Tao","62863","CR","Agreement","","","177","7.16.2","UE RF Maintenance (36.101) [LTE_V2X-Core]",49270,"agreed","2017-05-04T12:53:41.743","2017-05-05T15:25:57.197","","","Rel-14","36.101","14.3.0","LTE_V2X-Core","4428","","F","RP-171282","","","","",""]
["R4-1704928","draft TP to introduce the band combination of 34/47 for V2X","CATT","Xuhua Tao","62863","discussion","Discussion","","","340","9.9.1","General [LTE_V2X_CA_bands]",49280,"noted","2017-05-04T12:53:42.663","2017-05-05T15:25:57.210","","","Rel-15","","","LTE_V2X_CA_bands","","","","","","","","",""]
["R4-1704929","Co-existence performance for NR_NR co-existence on sub-6GHz","CATT","Xuhua Tao","62863","discussion","Discussion","","","422","10.3.5","ACLR and ACS [NR_newRAT]",570200,"noted","2017-05-04T12:53:42.677","2017-05-05T15:25:57.210","","","Rel-15","","","NR_newRAT","","","","","","","","",""]
["R4-1704930","Discussion on NR BS dynamic range","CATT","Xuhua Tao","62863","discussion","Discussion","","","444","10.5.4.1","Dynamic Range [NR_newRAT]",49300,"noted","2017-05-04T12:53:42.693","2017-05-05T15:25:57.210","","","Rel-15","","","NR_newRAT","","","","","","","","",""]
["R4-1704931","Correction on Duplex mode for Prose operating band","CATT","Xuhua Tao","62863","CR","Approval","","","13","4.2.1","UE RF (core / EMC) [WI code or TEI12]",49310,"revised","2017-05-04T12:53:42.710","2017-05-05T15:25:57.210","","R4-1705909","Rel-12","36.101","12.15.0","TEI","4429","","F","","","","","",""]
["R4-1704932","Correction on Duplex mode for Prose operating band","CATT","Xuhua Tao","62863","CR","Approval","","","13","4.2.1","UE RF (core / EMC) [WI code or TEI12]",49320,"postponed","2017-05-04T12:53:43.583","2017-05-23T15:07:51.117","","","Rel-13","36.101","13.7.0","TEI","4430","","A","","","","","",""]
["R4-1704933","Correction on Duplex mode for Prose operating band","CATT","Xuhua Tao","62863","CR","Approval","","","13","4.2.1","UE RF (core / EMC) [WI code or TEI12]",49330,"postponed","2017-05-04T12:53:44.440","2017-05-23T15:07:51.133","","","Rel-14","36.101","14.3.0","TEI","4431","","A","","","","","",""]
["R4-1704934","Transmitter RF requirements for NR UE","LG Electronics Inc.","Suhwan Lim","46654","discussion","Approval","In this paper, we provide our views on the NR UE Tx requirements for both single and dual connectivity UE since there was no difference for the RF requirements between NSA UE and SA UE.","","426","10.4.3","Transmitter characteristics [NR_newRAT]",49340,"noted","2017-05-04T12:59:10.023","2017-05-05T09:13:12.507","","","Rel-15","","","NR_newRAT-Core","","","","","","","","",""]
["R4-1704935","Transmitter RF requirements for NR UE","LG Electronics Inc.","Suhwan Lim","46654","discussion","Approval","In this paper, we provide our views on the NR UE Tx requirements for both single and dual connectivity UE since there was no difference for the RF requirements between NSA UE and SA UE.","","426","10.4.3","Transmitter characteristics [NR_newRAT]",53400,"withdrawn","2017-05-04T12:59:58.163",null,"","","Rel-15","","","NR_newRAT-Core","","","","","","","","",""]
["R4-1704936","CR for V2V performance requirements","LG Electronics Inc.","Jin-yup Hwang","47026","CR","Approval","","","171","7.15.4","UE demodulation (36.101) [LTE_SL_V2V-Perf]",46441,"revised","2017-05-04T13:01:36.440","2017-05-04T13:31:48.177","","R4-1705949","Rel-14","36.101","14.3.0","LTE_SL_V2V-Perf","4432","","B","","","","","",""]
["R4-1704937","Receiver RF requirements for NR UE","LG Electronics Inc.","Suhwan Lim","46654","discussion","Approval","In this paper, we provide our views on the 5G UE Rx requirements for both single and dual connectivity UE since there was no difference for the RF requirements between NSA UE and SA UE.","","431","10.4.4","Receiver characteristics [NR_newRAT]",49370,"noted","2017-05-04T13:03:10.163","2017-05-05T09:13:12.507","","","Rel-15","","","NR_newRAT-Core","","","","","","","","",""]
["R4-1704938","Simulation results for V2V performance requirements","LG Electronics Inc.","Jin-yup Hwang","47026","discussion","Discussion","","","172","7.15.4.1","Single-link PSSCH and PSCCH [LTE_SL_V2V-Perf]",49380,"noted","2017-05-04T13:04:33.840","2017-05-04T13:31:48.177","","","","","","","","","","","","","","",""]
["R4-1704939","Discussion on V2X demodulation test cases","LG Electronics Inc.","Jin-yup Hwang","47026","discussion","Discussion","","","182","7.16.5.2","PSBCH, eNB sync and WAN SDR [LTE_V2X-Perf]",46460,"noted","2017-05-04T13:05:51.467","2017-05-04T13:31:48.193","","","","","","","","","","","","","","",""]
["R4-1704940","Discussion and simulation results for enhanced SU-MIMO","LG Electronics Inc.","Jin-yup Hwang","47026","discussion","Discussion","","","279","7.27.3","SU-MIMO IM [LTE_eCRSIM_eSUMIMO]",51300,"noted","2017-05-04T13:06:46.407","2017-05-04T13:31:48.193","","","","","","","","","","","","","","",""]
["R4-1704941","Simulation reuslts for enhanced CRS-IM for control channels","LG Electronics Inc.","Jin-yup Hwang","47026","discussion","Discussion","","","278","7.27.2.2","Control channel [LTE_eCRSIM_eSUMIMO]",49240,"noted","2017-05-04T13:07:46.840","2017-05-04T13:31:48.210","","","","","","","","","","","","","","",""]
["R4-1704942","Summary of simulation results for enhanced SU-MIMO","LG Electronics Inc.","Jin-yup Hwang","47026","discussion","Information","","","279","7.27.3","SU-MIMO IM [LTE_eCRSIM_eSUMIMO]",55520,"noted","2017-05-04T13:08:55.853","2017-05-23T15:07:51.133","","","","","","","","","","","","","","",""]
["R4-1704943","AAS OTA CRS and pilot channel requirements","Ericsson","Thomas Chapman","46692","other","Approval","Considerations on how to set requirement for P-CPICH and CRS accuracy","","362","9.12.2.5","Other Transmitter Requirements [AASenh_BS_LTE_UTRA-Core]",49210,"noted","2017-05-04T13:09:05.277","2017-05-05T13:39:13.947","","","Rel-15","","","AASenh_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-1704944","Draft specification text on blocking for eAAS","Ericsson","Thomas Chapman","46692","other","Discussion","Discussion on how to write blocking int he specifications","","363","9.12.2.6","Other Receiver requirements [AASenh_BS_LTE_UTRA-Core]",614500,"noted","2017-05-04T13:09:05.290","2017-05-05T13:39:13.947","","","Rel-15","","","AASenh_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-1704945","TP to 37.843: In band blocking requirement","Ericsson","Thomas Chapman","46692","pCR","Approval","Capturing blocking agreement","","363","9.12.2.6","Other Receiver requirements [AASenh_BS_LTE_UTRA-Core]",56431,"revised","2017-05-04T13:09:05.290","2017-05-05T13:39:13.947","","R4-1706146","Rel-15","37.843","0.2.0","AASenh_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-1704946","Terminology for carrier bandwidth discussions","Ericsson","Thomas Chapman","46692","other","Approval","Clarifying terminology for bandwidths/carriers etc","","418","10.3.1","Channel bandwidth and subcarrier spacing [NR_newRAT]",49460,"noted","2017-05-04T13:09:05.353","2017-05-05T13:39:13.963","","","Rel-15","","","NR_newRAT","","","","","","","","",""]
["R4-1704947","Bandwidth and carrier configurations for NR","Ericsson","Thomas Chapman","46692","other","Approval","Considerations on concept of carrier and CA","","418","10.3.1","Channel bandwidth and subcarrier spacing [NR_newRAT]",49470,"noted","2017-05-04T13:09:05.353","2017-05-05T13:39:13.963","","","Rel-15","","","NR_newRAT","","","","","","","","",""]
["R4-1704948","On the need for multi-numerology related requirements in RAN4","Ericsson","Thomas Chapman","46692","other","Discussion","Considerations on requirement for PSS/SSS and general need for requirement","","421","10.3.4","In-band requirements [NR_newRAT]",52820,"noted","2017-05-04T13:09:05.370","2017-05-05T13:39:13.963","","","Rel-15","","","NR_newRAT","","","","","","","","",""]
["R4-1704949","Further elaboration on multiple numerologies","Ericsson","Thomas Chapman","46692","other","Discussion","Discusses the block filter for various utilization per numerology","","420","10.3.3","Spectrum utilization [NR_newRAT]",52070,"noted","2017-05-04T13:09:05.400","2017-05-05T13:39:54.383","","","Rel-15","","","NR_newRAT","","","","","","","","",""]
["R4-1704950","Further elaboration on NR bandwidths for sub 6 GHz bands","Ericsson","Thomas Chapman","46692","other","Discussion","Further elaboration on NR bandwidths for existing bands in the WID","","418","10.3.1","Channel bandwidth and subcarrier spacing [NR_newRAT]",569900,"noted","2017-05-04T13:09:05.417","2017-05-05T13:39:54.383","","","Rel-15","","","NR_newRAT","","","","","","","","",""]
["R4-1704951","Further elaboration on mm-wave band requirement coverage","Ericsson","Thomas Chapman","46692","other","Approval","Discusses specific requirements which can possibly be excluded for mm-wave bands","","436","10.5.1","BS RF General (ad-hoc MoM, Plan, Spec structure) [NR_newRAT]",615800,"noted","2017-05-04T13:09:05.417","2017-05-05T13:39:54.383","","","Rel-15","","","NR_newRAT","","","","","","","","",""]
["R4-1704952","CR on Sub-carrier spacing for mm-wave bands","Ericsson","Thomas Chapman","46692","CR","Approval","CR to add simulation results for different SCS in mm-wave bands.","","410","10.1.1","TR maintenance [NR_newRAT]",49520,"noted","2017-05-04T13:09:05.433","2017-05-05T13:39:54.397","","","Rel-14","38.803","14.0.0","FS_NR_newRAT","0008","","F","","","","","",""]
["R4-1704953","General discussion on expected radiation pattern","Ericsson","Thomas Chapman","46692","other","Discussion","General discussion on expected radiation pattern","","436","10.5.1","BS RF General (ad-hoc MoM, Plan, Spec structure) [NR_newRAT]",56340,"noted","2017-05-04T13:09:06.213","2017-05-05T13:39:54.397","","","Rel-15","","","NR_newRAT","","","","","","","","",""]
["R4-1704954","Further discussions on radiation patterns: multi-user multi-antenna transmission scheme case","Ericsson","Thomas Chapman","46692","other","Discussion","Further elaboration on radiation patterns for multi-user multi-antenna transmission scheme case","","436","10.5.1","BS RF General (ad-hoc MoM, Plan, Spec structure) [NR_newRAT]",56350,"noted","2017-05-04T13:09:06.227","2017-05-05T13:39:54.367","","","Rel-15","","","NR_newRAT","","","","","","","","",""]
["R4-1704955","Draft CR for test applicability rule for enhanced SU-MIMO","LG Electronics Inc.","Jin-yup Hwang","47026","draftCR","Endorsement","","","279","7.27.3","SU-MIMO IM [LTE_eCRSIM_eSUMIMO]",55530,"endorsed","2017-05-04T13:11:57.620","2017-05-04T13:31:48.210","","R4-1706162","Rel-14","36.101","14.3.0","LTE_eCRSIM_eSUMIMO-Perf","","","","","","","","",""]
["R4-1704956","Discussion about CBW and SCS for NR UE","LG Electronics Inc.","Jin-yup Hwang","47026","discussion","Discussion","","","418","10.3.1","Channel bandwidth and subcarrier spacing [NR_newRAT]",574200,"noted","2017-05-04T13:13:12.843","2017-05-04T13:32:13.777","","","","","","","","","","","","","","",""]
["R4-1704957","Discussion on antenna reference architecture for mmWave","LG Electronics Inc.","Jin-yup Hwang","47026","discussion","Discussion","","","425","10.4.2","Reference architecture [NR_newRAT]",49570,"noted","2017-05-04T13:14:15.837","2017-05-04T13:32:13.777","","","","","","","","","","","","","","",""]
["R4-1704958","Draft CR to 37.104: IIntroduction of Band 71 (600MHz FDD band for US)","Ericsson, Nokia","Patrizia Testa","66129","draftCR","Endorsement","This CR introduces B71 in the specification","","338","9.8.4","Other specifications [LTE600_US]",49600,"endorsed","2017-05-04T13:15:07.877","2017-05-06T11:57:51.640","","","Rel-15","37.104","14.3.0","LTE600_US","","","B","","","","","",""]
["R4-1704959","Draft CR 37.141: Introduction of Band 71 (600MHz FDD band for US)","Ericsson, Nokia","Patrizia Testa","66129","draftCR","Endorsement","This CR introduces B71 in the specification","","338","9.8.4","Other specifications [LTE600_US]",49610,"endorsed","2017-05-04T13:15:07.890","2017-05-06T11:57:51.670","","","Rel-15","37.141","14.3.0","LTE600_US","","","B","","","","","",""]
["R4-1704960","Draft CR 25.141: Introduction of Band 71 (600MHz FDD band for US)","Ericsson, Nokia","Patrizia Testa","66129","draftCR","Endorsement","This CR introduces B71 in the specification","","338","9.8.4","Other specifications [LTE600_US]",49620,"endorsed","2017-05-04T13:15:07.907","2017-05-06T11:57:51.670","","","Rel-15","25.141","14.1.0","LTE600_US","","","B","","","","","",""]
["R4-1704961","Draft CR 36.133: Introduction of Band 71 (600MHz FDD band for US)","Ericsson, Nokia","Patrizia Testa","66129","draftCR","Endorsement","This CR introduces B71 in the specification","","338","9.8.4","Other specifications [LTE600_US]",46020,"endorsed","2017-05-04T13:15:07.923","2017-05-06T11:57:51.670","","","Rel-15","36.133","14.3.0","LTE600_US","","","B","","","","","",""]
["R4-1704962","Draft CR 25.133: Introduction of Band 71 (600MHz FDD band for US)","Ericsson, Nokia","Patrizia Testa","66129","draftCR","Endorsement","This CR introduces B71 in the specification","","338","9.8.4","Other specifications [LTE600_US]",46040,"endorsed","2017-05-04T13:15:07.923","2017-05-06T11:57:51.670","","","Rel-15","25.133","14.1.0","LTE600_US","","","B","","","","","",""]
["R4-1704963","Draft CR 25.123: Introduction of Band 71 (600MHz FDD band for US)","Ericsson, Nokia","Patrizia Testa","66129","draftCR","Endorsement","This CR introduces B71 in the specification","","338","9.8.4","Other specifications [LTE600_US]",49630,"revised","2017-05-04T13:15:07.937","2017-05-06T11:57:51.687","","R4-1705888","Rel-15","25.123","14.2.0","LTE600_US","","","B","","","","","",""]
["R4-1704964","Draft CR 25.461: Introduction of Band 71 (600MHz FDD band for US)","Ericsson, Nokia","Patrizia Testa","66129","draftCR","Endorsement","This CR introduces B71 in the specification","","338","9.8.4","Other specifications [LTE600_US]",49640,"endorsed","2017-05-04T13:15:07.953","2017-05-06T11:57:51.687","","","Rel-15","25.461","14.1.0","LTE600_US","","","B","","","","","",""]
["R4-1704965","Draft CR 25.466: Introduction of Band 71 (600MHz FDD band for US)","Ericsson, Nokia","Patrizia Testa","66129","draftCR","Endorsement","This CR introduces B71 in the specification","","338","9.8.4","Other specifications [LTE600_US]",49650,"noted","2017-05-04T13:15:07.970","2017-05-06T11:57:51.687","","","Rel-15","25.466","14.1.0","LTE600_US","","","B","","","","","",""]
["R4-1704966","TP to TR 36.755 Update of section on Coexistence with WMTS services","Ericsson, Qorvo","Patrizia Testa","66129","other","Approval","The purpose of this text proposal is to update TR 36.755 adding more details on coexistence aspects between 600 MHz services and WMTS operations in Channel 37.","","335","9.8.1","General [LTE600_US]",49660,"revised","2017-05-04T13:15:07.970","2017-05-06T11:57:51.687","","R4-1705885","Rel-15","36.755","","LTE600_US","","","","","","","","",""]
["R4-1704967","TP to TR 36.755 Section 3 (Symbols and Abbreviations)","Ericsson","Patrizia Testa","66129","other","Approval","This document is a text proposal to TR 36.755 section 3.","","335","9.8.1","General [LTE600_US]",49670,"approved","2017-05-04T13:15:07.983","2017-05-06T11:57:51.703","","","Rel-15","36.755","","LTE600_US","","","","","","","","",""]
["R4-1704968","CR to 36.101: Introduction of FeMBMS numerologies","Ericsson","Patrizia Testa","66129","CR","Agreement","This CR extends applicability of requirements to FeMBMS","","153","7.13.1","UE RF(36.101) [MBMS_LTE_enh2-Core]",49680,"agreed","2017-05-04T13:15:08","2017-05-06T11:57:51.703","","","Rel-14","36.101","14.3.0","MBMS_LTE_enh2-Core","4433","","B","RP-171261","","","","",""]
["R4-1704969","UE filter vendor data on Insertion Loss","Ericsson","Patrizia Testa","66129","discussion","Discussion","This contribution presents UE filter vendor data on insertion loss as inputs for discussions, ongoing in RAN4, to agree on reference sensitivity for new SDL band.","","322","9.5.2","UE RF (36.101) [LTE_SDL_1500ext-core]",49690,"noted","2017-05-04T13:15:08.827","2017-05-06T11:57:51.703","","","Rel-15","","","LTE_SDL_1500ext-Core","","","","","","","","",""]
["R4-1704970","Investigation of SDL band plan options in L-band","Ericsson","Patrizia Testa","66129","discussion","Discussion","This paper compares band plan options identified in the Way Forward in terms of BS aspects","","320","9.5","LTE Extended 1.5 GHz SDL band (1427 ? 1518 MHz) and LTE Carrier Aggregation (2DL/1UL) with Band 20 [LTE_SDL_1500ext]",609100,"noted","2017-05-04T13:15:08.843","2017-05-06T11:57:51.703","","","Rel-15","","","LTE_SDL_1500ext-Core","","","","","","","","",""]
["R4-1704971","CR to 36.104: Introduction of FDD Band (1427-1518 MHz)","Ericsson","Patrizia Testa","66129","draftCR","Endorsement","This CR introduces FDD Band (1427-1518 MHz) in the specification","","317","9.4.3","BS RF (36.104, 36.141) [LTE_FDD_L_Band-core/Perf]",45490,"noted","2017-05-04T13:15:08.857","2017-05-06T11:57:51.703","","","Rel-15","36.104","14.3.0","LTE_FDD_L_Band-Core","","","B","","","","","",""]
["R4-1704972","CR on T311 timer in RRC re-establishment test case R14","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","Agreement","","","62","5.5.5","RRM Performance (36.133) [NB_IOT-Perf]",49760,"agreed","2017-05-04T13:55:16.447","2017-05-06T11:56:27.287","","","Rel-14","36.133","14.3.0","NB_IOT-Perf","4873","","A","RP-171301","","","","",""]
["R4-1704973","Introduce NPDCCH RMC with DCI format N0 R13","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","Agreement","","","62","5.5.5","RRM Performance (36.133) [NB_IOT-Perf]",51460,"agreed","2017-05-04T13:55:17.303","2017-05-06T11:56:27.287","","","Rel-13","36.133","13.7.0","NB_IOT-Perf","4874","","F","RP-171300","","","","",""]
["R4-1704974","Introduce NPDCCH RMC with DCI format N0 R14","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","Agreement","","","62","5.5.5","RRM Performance (36.133) [NB_IOT-Perf]",56620,"agreed","2017-05-04T13:55:18.117","2017-05-23T15:07:51.197","","","Rel-14","36.133","14.3.0","NB_IOT-Perf","4875","","A","RP-171300","","","","",""]
["R4-1704975","Correction on UE transmit timing test for NB-IoT R13","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","Agreement","","","62","5.5.5","RRM Performance (36.133) [NB_IOT-Perf]",50720,"revised","2017-05-04T13:55:27.240","2017-05-06T11:56:27.287","","R4-1706203","Rel-13","36.133","13.7.0","NB_IOT-Perf","4876","","F","","","","","",""]
["R4-1704976","Correction on UE transmit timing test for NB-IoT R14","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","Agreement","","","62","5.5.5","RRM Performance (36.133) [NB_IOT-Perf]",50730,"agreed","2017-05-04T13:55:28.177","2017-05-23T15:07:51.197","","","Rel-14","36.133","14.3.0","NB_IOT-Perf","4877","","A","RP-171302","","","","",""]
["R4-1704977","Correction on timing advance test for NB-IoT R13","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","Agreement","","","62","5.5.5","RRM Performance (36.133) [NB_IOT-Perf]",50820,"revised","2017-05-04T13:55:29.127","2017-05-06T11:56:27.287","","R4-1705962","Rel-13","36.133","13.7.0","NB_IOT-Perf","4878","","F","","","","","",""]
["R4-1704978","Correction on timing advance test for NB-IoT R14","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","Agreement","","","62","5.5.5","RRM Performance (36.133) [NB_IOT-Perf]",50830,"agreed","2017-05-04T13:55:30.143","2017-05-23T15:07:51.210","","","Rel-14","36.133","14.3.0","NB_IOT-Perf","4879","","A","RP-171303","","","","",""]
["R4-1704979","Maintenance CR on NB-IoT core requirements R13","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","Agreement","","","60","5.5.3","RRM core (36.133) [NB_IOT-Core]",573700,"agreed","2017-05-04T13:55:30.970","2017-05-06T11:56:27.287","","","Rel-13","36.133","13.7.0","NB_IOT-Core","4880","","F","RP-171299","","","","",""]
["R4-1704980","Maintenance CR on NB-IoT core requirements R14","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","Agreement","","","60","5.5.3","RRM core (36.133) [NB_IOT-Core]",626100,"agreed","2017-05-04T13:55:31.857","2017-05-23T15:07:51.210","","","Rel-14","36.133","14.3.0","NB_IOT-Core","4881","","A","RP-171299","","","","",""]
["R4-1704981","Correction on side condition for RRC re-establishment test cases R13","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","Agreement","","","62","5.5.5","RRM Performance (36.133) [NB_IOT-Perf]",49770,"agreed","2017-05-04T13:55:32.967","2017-05-06T11:56:27.303","","","Rel-13","36.133","13.7.0","NB_IOT-Perf","4882","","F","RP-171302","","","","",""]
["R4-1704982","Correction on side condition for RRC re-establishment test cases R14","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","Agreement","","","62","5.5.5","RRM Performance (36.133) [NB_IOT-Perf]",49780,"agreed","2017-05-04T13:55:34.587","2017-05-23T15:07:51.227","","","Rel-14","36.133","14.3.0","NB_IOT-Perf","4883","","A","RP-171302","","","","",""]
["R4-1704983","Simulation results for PUSCH in UpPTS","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","Discussion","","","150","7.12.3","Demodulation (36.104/36.141) [LTE_UL_CAP_enh-Core/Perf]",53040,"revised","2017-05-04T13:55:36.617","2017-05-06T11:56:27.303","","R4-1706010","","","","LTE_UL_CAP_enh-Perf","","","","","","","","",""]
["R4-1704984","Discussion on PHR mapping for NB-IoT","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","Discussion","","","195","7.17.3.2.3","PHR [NB_IOTenh-Core]",46780,"noted","2017-05-04T13:55:36.633","2017-05-06T11:56:27.303","","","","","","NB_IOTenh-Core","","","","","","","","",""]
["R4-1704985","CR for applicability requirements for NB-IoT","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","Agreement","","","197","7.17.3.2.5","Others [NB_IOTenh-Core]",54700,"withdrawn","2017-05-04T13:55:36.647",null,"","","Rel-14","36.133","14.3.0","NB_IOTenh-Core","4884","","B","","","","","",""]
["R4-1704986","E-UTRAN FDD - UE Transmit Timing Accuracy Test for RACH-less Handover","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","Agreement","","","240","7.20.2","RRM performance (36.133) [LTE_eMob-Perf]",51680,"agreed","2017-05-04T13:55:37.537","2017-05-06T11:56:27.303","","","Rel-14","36.133","14.3.0","LTE_eMob","4885","","B","RP-171259","","","","",""]
["R4-1704987","E-UTRAN TDD - UE Transmit Timing Accuracy Test for RACH-less Handover","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","Agreement","","","240","7.20.2","RRM performance (36.133) [LTE_eMob-Perf]",51690,"agreed","2017-05-04T13:55:38.457","2017-05-06T11:56:27.320","","","Rel-14","36.133","14.3.0","LTE_eMob","4886","","B","RP-171259","","","","",""]
["R4-1704988","Initial consideration on UE measurement capabilities","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","Discussion","","","450","10.6.2","UE measurement capability [NR_newRAT]",48040,"noted","2017-05-04T13:55:39.300","2017-05-06T11:56:27.320","","","","","","NR_newRAT","","","","","","","","",""]
["R4-1704989","RRM consideration on NSA requirements","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","Discussion","","","452","10.6.4","Expected Measurement requirements for NSA [NR_newRAT]",47650,"noted","2017-05-04T13:55:39.330","2017-05-06T11:56:27.320","","","","","","NR_newRAT","","","","","","","","",""]
["R4-1704990","Discussion on incoming LS from RAN2 on DC-related mobility enhancements in NR","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","Discussion","","","411","10.1.2","Topics related to incoming LS from other WG [NR_newRAT]",50540,"noted","2017-05-04T13:55:39.347","2017-05-06T11:56:27.367","","","","","","NR_newRAT","","","","","","","","",""]
["R4-1704991","Reply LS on the feasibility of DC-related mobility enhancements in NR","Huawei, HiSilicon","Xiang (Steven) Chen","41576","LS out","Approval","","","411","10.1.2","Topics related to incoming LS from other WG [NR_newRAT]",52430,"revised","2017-05-04T13:55:39.377","2017-05-06T11:56:27.383","","R4-1706226","","","","NR_newRAT","","","","","R2-1703971","RAN2","RAN1","",""]
["R4-1704992","Correction on transmit timing requirement R13","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","","","","50","5.4.5.1","Test cases for BL/CE UE [LTE_MTCe2_L1-Perf]",49920,"revised","2017-05-04T13:55:39.440","2017-05-06T11:56:27.383","","R4-1705997","Rel-13","36.133","13.7.0","LTE_MTCe2_L1-Perf","4887","","F","","","","","",""]
["R4-1704993","Correction on transmit timing requirement R14","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","Agreement","","","50","5.4.5.1","Test cases for BL/CE UE [LTE_MTCe2_L1-Perf]",49930,"agreed","2017-05-04T13:55:40.267","2017-05-23T15:07:51.227","","","Rel-14","36.133","14.3.0","LTE_MTCe2_L1-Perf","4888","","A","RP-171310","","","","",""]
["R4-1704994","Discussion on RSTD requirement for eNB-IOT","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","","","","191","7.17.3.1.2","UTODA/OTDOA [NB_IOTenh-Core]",49940,"noted","2017-05-04T13:55:41.157","2017-05-06T11:56:27.400","","","","","","","","","","","","","","",""]
["R4-1704995","CR on intra frequency RSTD measurement requirement for eNB-IOT","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","","","","191","7.17.3.1.2","UTODA/OTDOA [NB_IOTenh-Core]",49960,"revised","2017-05-04T13:55:41.203","2017-05-06T11:56:27.400","","R4-1705957","Rel-14","36.133","14.3.0","NB_IOTenh-Core","4889","","B","","","","","",""]
["R4-1704996","CR on inter frequency RSTD measurement requirement for eNB-IOT","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","","","","191","7.17.3.1.2","UTODA/OTDOA [NB_IOTenh-Core]",56060,"revised","2017-05-04T13:55:42.060","2017-05-06T11:56:27.400","","R4-1705958","Rel-14","36.133","14.3.0","NB_IOTenh-Core","4890","","B","","","","","",""]
["R4-1704997","CR on intra frequency RSTD accuracy requirement for eNB-IOT","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","","","","199","7.17.4.1","Positioning [NB_IOTenh-Perf]",49970,"revised","2017-05-04T13:55:42.903","2017-05-06T11:56:27.400","","R4-1706265","Rel-14","36.133","14.3.0","NB_IOTenh-Perf","4891","","B","","","","","",""]
["R4-1704998","CR on inter frequency RSTD accuracy requirement for eNB-IOT","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","","","","199","7.17.4.1","Positioning [NB_IOTenh-Perf]",49980,"revised","2017-05-04T13:55:43.760","2017-05-06T11:56:27.413","","R4-1706276","Rel-14","36.133","14.3.0","NB_IOTenh-Perf","4892","","B","","","","","",""]
["R4-1704999","Discussion on RSTD requirement for FeMTC","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","","","","211","7.18.3.1.2","OTDOA [LTE_feMTC-Core]",49990,"noted","2017-05-04T13:55:44.557","2017-05-06T11:56:27.447","","","","","","","","","","","","","","",""]
["R4-1705000","CR on intra frequency RSTD measurement requirement for FeMTC","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","","","","211","7.18.3.1.2","OTDOA [LTE_feMTC-Core]",56030,"revised","2017-05-04T13:55:44.573","2017-05-06T11:56:27.460","","R4-1705978","Rel-14","36.133","14.3.0","LTE_feMTC-Core","4893","","B","","","","","",""]
["R4-1705001","CR on inter frequency RSTD measurement requirement for FeMTC","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","","","","211","7.18.3.1.2","OTDOA [LTE_feMTC-Core]",56050,"revised","2017-05-04T13:55:45.447","2017-05-06T11:56:27.460","","R4-1706277","Rel-14","36.133","14.3.0","LTE_feMTC-Core","4894","","B","","","","","",""]
["R4-1705002","CR on intra frequency RSTD accuracy requirement for FeMTC","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","","","","221","7.18.5.1","Positioning [LTE_feMTC-Perf]",50020,"noted","2017-05-04T13:55:46.350","2017-05-06T11:56:27.460","","R4-1706266","Rel-14","36.133","14.3.0","LTE_feMTC-Perf","4895","","B","","","","","",""]
["R4-1705003","CR on inter frequency RSTD accuracy requirement for FeMTC","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","","","","221","7.18.5.1","Positioning [LTE_feMTC-Perf]",50030,"noted","2017-05-04T13:55:47.397","2017-05-06T11:56:27.477","","R4-1706278","Rel-14","36.133","14.3.0","LTE_feMTC-Perf","4896","","B","","","","","",""]
["R4-1705004","Discussion on UE Rx-Tx requirement for FeMTC","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","","","","210","7.18.3.1.1","E-CID [LTE_feMTC-Core]",50040,"noted","2017-05-04T13:55:48.347","2017-05-06T11:56:27.477","","","","","","","","","","","","","","",""]
["R4-1705005","CR on UE Rx-Tx  measurement requirement for FeMTC","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","","","","210","7.18.3.1.1","E-CID [LTE_feMTC-Core]",597600,"noted","2017-05-04T13:55:48.377","2017-05-06T11:56:27.477","","","Rel-14","36.133","14.3.0","LTE_feMTC-Core","4897","","B","","","","","",""]
["R4-1705006","discussion on test case for Bluetooth","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","","","","252","7.23.2.2","RAT-independent enhancement [UTRA_LTE_iPos_enh2-Perf]",45180,"noted","2017-05-04T13:55:49.283","2017-05-06T11:56:27.477","","","","","","","","","","","","","","",""]
["R4-1705007","CR on test case for Bluetooth RSSI reporting delay","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","","","","252","7.23.2.2","RAT-independent enhancement [UTRA_LTE_iPos_enh2-Perf]",54740,"withdrawn","2017-05-04T13:55:49.300",null,"","","Rel-14","36.133","14.3.0","UTRA_LTE_iPos_enh2-Perf","4898","","B","","","","","",""]
["R4-1705008","Discussion on RAT-independent test case for indoor positioning","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","","","","251","7.23.2.1","OTDOA/E-CID enhancement [UTRA_LTE_iPos_enh2-Perf]",50080,"noted","2017-05-04T13:55:50.157","2017-05-06T11:56:27.477","","","","","","","","","","","","","","",""]
["R4-1705009","WF on indoor positioning","Huawei, HiSilicon","Xiang (Steven) Chen","41576","other","","","","250","7.23.2","RRM performance (36.133/37.171) [UTRA_LTE_iPos_enh2-Perf]",50090,"approved","2017-05-04T13:55:50.187","2017-05-06T11:56:27.493","","","","","","","","","","","","","","",""]
["R4-1705010","CR on RAT-dependent indoor positioning","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","","","","249","7.23.1","RRM core maintenance (36.133) [UTRA_LTE_iPos_enh2-Core]",50100,"noted","2017-05-04T13:55:50.220","2017-05-06T11:56:27.493","","","Rel-14","36.133","14.3.0","UTRA_LTE_iPos_enh2-Core","4899","","F","","","","","",""]
["R4-1705011","Discussion on RSRP range for eMTC","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","","","","46","5.4.3.1","BL/CE UE [LTE_MTCe2_L1-Core]",51480,"noted","2017-05-04T13:55:51","2017-05-06T11:56:27.493","","","","","","","","","","","","","","",""]
["R4-1705012","CR on RSRP range for eMTC R13","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","","","","46","5.4.3.1","BL/CE UE [LTE_MTCe2_L1-Core]",51490,"noted","2017-05-04T13:55:51.017","2017-05-06T11:56:27.493","","R4-1705995","Rel-13","36.133","13.7.0","LTE_MTCe2_L1-Core","4900","","F","","","","","",""]
["R4-1705013","CR on RSRP range for eMTC R14","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","","","","46","5.4.3.1","BL/CE UE [LTE_MTCe2_L1-Core]",51500,"withdrawn","2017-05-04T13:55:51.887",null,"","","Rel-14","36.133","14.3.0","LTE_MTCe2_L1-Core","4901","","A","","","","","",""]
["R4-1705014","Discussion on NR RRM measurement definitions","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","","","","454","10.6.6","Measurement definition and reference point [NR_newRAT]",50150,"noted","2017-05-04T13:55:52.667","2017-05-06T11:56:27.507","","","","","","","","","","","","","","",""]
["R4-1705015","Discussion on RRM requirement over different numerologies and bandwidth","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","","","","454","10.6.6","Measurement definition and reference point [NR_newRAT]",53230,"noted","2017-05-04T13:55:52.683","2017-05-06T11:56:27.507","","","","","","","","","","","","","","",""]
["R4-1705016","RLM consideration in NR","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","","","","452","10.6.4","Expected Measurement requirements for NSA [NR_newRAT]",56100,"withdrawn","2017-05-04T13:55:52.700",null,"","","","","","NR_newRAT","","","","","","","","",""]
["R4-1705017","CR on conditions for measurements procedures in RRC_CONNECTED State for FeMTC in R14","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","","","","222","7.18.5.2","Mobility enhancement [LTE_feMTC-Perf]",50170,"noted","2017-05-04T13:55:52.717","2017-05-06T11:56:27.507","","","Rel-14","36.133","14.3.0","LTE_feMTC-Perf","4902","","B","","","","","",""]
["R4-1705018","CR on conditions for measurements procedures in RRC_IDLE State for FeMTC in R14","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","","","","222","7.18.5.2","Mobility enhancement [LTE_feMTC-Perf]",50180,"noted","2017-05-04T13:55:53.527","2017-05-06T11:56:27.507","","","Rel-14","36.133","14.3.0","LTE_feMTC-Perf","4903","","B","","","","","",""]
["R4-1705019","RRM test for UE Cat M2","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","","","","223","7.18.5.3","Applicability of requirements and test cases [LTE_feMTC-Perf]",50240,"noted","2017-05-04T13:55:54.307","2017-05-06T11:56:27.507","","","Rel-14","36.133","14.3.0","LTE_feMTC-Perf","4904","","B","","","","","",""]
["R4-1705020","Discussion on enhancement RLM for FeMTC","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","","","","217","7.18.3.2.5","RLM and timing [LTE_feMTC-Core]",50200,"noted","2017-05-04T13:55:55.103","2017-05-06T11:56:27.523","","","","","","LTE_feMTC-Core","","","","","","","","",""]
["R4-1705021","CR on enhanced RLM requirement for FeMTC","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","","","","217","7.18.3.2.5","RLM and timing [LTE_feMTC-Core]",50800,"noted","2017-05-04T13:55:55.117","2017-05-06T11:56:27.523","","","Rel-14","36.133","14.3.0","LTE_feMTC-Core","4905","","B","","","","","",""]
["R4-1705022","Discussion on 2 Tx port RSRP detection for PRACH CE level selection","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","","","","215","7.18.3.2.3","Random access [LTE_feMTC-Core]",54610,"noted","2017-05-04T13:55:55.960","2017-05-06T11:56:27.523","","","","","","","","","","","","","","",""]
["R4-1705023","Discussion on applicability rules for FeMTC","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","","","","223","7.18.5.3","Applicability of requirements and test cases [LTE_feMTC-Perf]",50190,"noted","2017-05-04T13:55:55.977","2017-05-06T11:56:27.523","","","","","","LTE_feMTC-Perf","","","","","","","","",""]
["R4-1705024","CR on applicability rule for FeMTC in R14","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","","","","223","7.18.5.3","Applicability of requirements and test cases [LTE_feMTC-Perf]",50230,"revised","2017-05-04T13:55:55.990","2017-05-06T11:56:27.523","","R4-1706267","Rel-14","36.133","14.3.0","LTE_feMTC-Perf","4906","","B","","","","","",""]
["R4-1705025","Discussion on measurement gap sharing for FeMTC","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","","","","216","7.18.3.2.4","Gap sharing and measurement [LTE_feMTC-Core]",50250,"noted","2017-05-04T13:55:56.787","2017-05-06T11:56:27.540","","","","","","LTE_feMTC-Core","","","","","","","","",""]
["R4-1705026","CR on the measurements requirement for FeMTC in R14","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","","","","216","7.18.3.2.4","Gap sharing and measurement [LTE_feMTC-Core]",50740,"noted","2017-05-04T13:55:56.817","2017-05-06T11:56:27.540","","","Rel-14","36.133","14.3.0","LTE_feMTC-Core","4907","","F","","","","","",""]
["R4-1705027","CR on Timing advance for FeMTC in R14","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","","","","217","7.18.3.2.5","RLM and timing [LTE_feMTC-Core]",572700,"noted","2017-05-04T13:55:57.660","2017-05-06T11:56:27.540","","","Rel-14","36.133","14.3.0","LTE_feMTC-Core","4908","","B","","","","","",""]
["R4-1705028","CR on UE timer accuracy for FeMTC in R14","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","","","","217","7.18.3.2.5","RLM and timing [LTE_feMTC-Core]",598600,"revised","2017-05-04T13:55:58.487","2017-05-06T11:56:27.540","","R4-1705985","Rel-14","36.133","14.3.0","LTE_feMTC-Core","4909","","B","","","","","",""]
["R4-1705029","Absolute and relative RSRQ accuracies in FDD 4DL CA in R13","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","","","","292","7.29.3","RRM [WI code or TEI14]",50290,"revised","2017-05-04T13:55:59.347","2017-05-06T11:56:27.540","","R4-1706041","Rel-13","36.133","13.7.0","TEI14","4910","","F","","","","","",""]
["R4-1705030","4DL FDD RSRQ for E-UTRAN in Carrier Aggregation in R14","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","","","Post-meeting note: It was noted before RAN#76 that there is a cover sheet error. So it was revised to R4-1706296","292","7.29.3","RRM [WI code or TEI14]",50300,"revised","2017-05-04T13:56:00.157","2017-05-23T15:07:51.243","","","Rel-14","36.133","14.3.0","TEI14","4911","","A","","","","","",""]
["R4-1705031","Absolute and relative RSRQ accuracies in TDD 4DL CA in R13","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","","","","292","7.29.3","RRM [WI code or TEI14]",50310,"revised","2017-05-04T13:56:00.967","2017-05-06T11:56:27.557","","R4-1706172","Rel-13","36.133","13.7.0","TEI14","4912","","F","","","","","",""]
["R4-1705032","4DL TDD RSRQ for E-UTRAN in Carrier Aggregation in R14","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","","","Post-meeting note: It was noted before RAN#76 that there is a cover sheet error. So it was revised to R4-1706297","292","7.29.3","RRM [WI code or TEI14]",50320,"revised","2017-05-04T13:56:01.793","2017-05-23T15:07:51.243","","","Rel-14","36.133","14.3.0","TEI14","4913","","A","","","","","",""]
["R4-1705033","Correction on the tests of RLM for Cat-M1 UE in R13","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","","","","292","7.29.3","RRM [WI code or TEI14]",50330,"revised","2017-05-04T13:56:02.933","2017-05-06T11:56:27.557","","R4-1706173","Rel-13","36.133","13.7.0","TEI14","4914","","F","","","","","",""]
["R4-1705034","Correction on the test cases of RLM for Cat-M1 UE in R14","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","","","Post-meeting note: It was noted before RAN#76 that there is a cover sheet error. So it was revised to R4-1706298","292","7.29.3","RRM [WI code or TEI14]",50340,"revised","2017-05-04T13:56:03.743","2017-05-23T15:07:51.257","","","Rel-14","36.133","14.3.0","TEI14","4915","","A","","","","","",""]
["R4-1705035","Discussion on BS synchronization requirements for eMBMS enhancements","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","Discussion","","","155","7.13.3","RRM core (36.133) [MBMS_LTE_enh2-Core]",574500,"noted","2017-05-04T13:56:04.557","2017-05-06T11:56:27.557","","","","","","","","","","","","","","",""]
["R4-1705036","CR on BS synchronization requirements for eMBMS enhancements","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","Agreement","","","155","7.13.3","RRM core (36.133) [MBMS_LTE_enh2-Core]",575000,"revised","2017-05-04T13:56:04.570","2017-05-06T11:56:27.557","","R4-1706009","Rel-14","36.133","14.3.0","MBMS_LTE_enh2-Core","4916","","F","","","","","",""]
["R4-1705037","CR on Modification of Selection/Reselection of V2X Synchronization Reference","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","Agreement","","","178","7.16.3","RRM core Maintenance (36.133) [LTE_V2X-Core]",50371,"revised","2017-05-04T13:56:05.397","2017-05-06T11:56:27.557","","R4-1705946","Rel-14","36.133","14.3.0","LTE_V2X-Core","4917","","F","","","","","",""]
["R4-1705038","List of RRM test cases for V2X requirements","Huawei, HiSilicon","Xiang (Steven) Chen","41576","other","Approval","","","179","7.16.4","RRM performance (36.133) [LTE_V2X-Perf]",49020,"revised","2017-05-04T13:56:06.177","2017-05-06T11:56:27.570","","R4-1706174","","","","","","","","","","","","",""]
["R4-1705039","Discussion on UE Transmission Timing Tests for V2X","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","Discussion","","","179","7.16.4","RRM performance (36.133) [LTE_V2X-Perf]",49050,"noted","2017-05-04T13:56:06.210","2017-05-06T11:56:27.570","","","","","","","","","","","","","","",""]
["R4-1705040","CR on UE Transmission Timing Accuracy Tests for V2X","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","Agreement","","","179","7.16.4","RRM performance (36.133) [LTE_V2X-Perf]",49070,"agreed","2017-05-04T13:56:06.223","2017-05-06T11:56:27.570","","","Rel-14","36.133","14.3.0","LTE_V2X-Perf","4918","","B","RP-171265","","","","",""]
["R4-1705041","Discussion on Initiation/Cease of SLSS Transmission Tests for V2X","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","Discussion","","","179","7.16.4","RRM performance (36.133) [LTE_V2X-Perf]",50380,"noted","2017-05-04T13:56:07.037","2017-05-06T11:56:27.570","","","","","","","","","","","","","","",""]
["R4-1705042","CR on Initiation/Cease of SLSS Transmissions Tests for V2X","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","Agreement","","","179","7.16.4","RRM performance (36.133) [LTE_V2X-Perf]",50410,"noted","2017-05-04T13:56:07.050","2017-05-06T11:56:27.570","","","Rel-14","36.133","14.3.0","LTE_V2X-Perf","4919","","B","","","","","",""]
["R4-1705043","Discussion on SyncRef UE Selection/Reselection Tests for V2X","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","Discussion","","","179","7.16.4","RRM performance (36.133) [LTE_V2X-Perf]",50420,"noted","2017-05-04T13:56:07.940","2017-05-06T11:56:27.587","","","","","","","","","","","","","","",""]
["R4-1705044","CR on Synchronization Reference Selection / Reselection Tests for V2X","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","Agreement","","","179","7.16.4","RRM performance (36.133) [LTE_V2X-Perf]",50430,"noted","2017-05-04T13:56:07.970","2017-05-06T11:56:27.587","","","Rel-14","36.133","14.3.0","LTE_V2X-Perf","4920","","B","","","","","",""]
["R4-1705045","Discussion on Autonomous Resource Selection/Reselection Measurement Tests for V2X","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","Discussion","","","179","7.16.4","RRM performance (36.133) [LTE_V2X-Perf]",50440,"noted","2017-05-04T13:56:08.830","2017-05-06T11:56:27.587","","","","","","","","","","","","","","",""]
["R4-1705046","CR on Autonomous Resource Selection/Reselection Measurement Tests for V2X","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","Agreement","","","179","7.16.4","RRM performance (36.133) [LTE_V2X-Perf]",50450,"noted","2017-05-04T13:56:08.860","2017-05-06T11:56:27.587","","","Rel-14","36.133","14.3.0","LTE_V2X-Perf","4921","","B","","","","","",""]
["R4-1705047","Discussion on Congestion Control Measurement Tests for V2X","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","Discussion","","","179","7.16.4","RRM performance (36.133) [LTE_V2X-Perf]",50460,"noted","2017-05-04T13:56:09.733","2017-05-06T11:56:27.587","","","","","","","","","","","","","","",""]
["R4-1705048","CR on Congestion Control Measurement Tests for V2X","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","Agreement","","","179","7.16.4","RRM performance (36.133) [LTE_V2X-Perf]",50470,"noted","2017-05-04T13:56:09.767","2017-05-06T11:56:27.603","","","Rel-14","36.133","14.3.0","LTE_V2X-Perf","4922","","B","","","","","",""]
["R4-1705049","Discussion on Interruptions Tests for V2X","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","Discussion","","","179","7.16.4","RRM performance (36.133) [LTE_V2X-Perf]",50480,"noted","2017-05-04T13:56:10.700","2017-05-06T11:56:27.617","","","","","","","","","","","","","","",""]
["R4-1705050","CR on Interruptions Tests for V2X","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","Agreement","","","179","7.16.4","RRM performance (36.133) [LTE_V2X-Perf]",50490,"noted","2017-05-04T13:56:10.780","2017-05-06T11:56:27.617","","","Rel-14","36.133","14.3.0","LTE_V2X-Perf","4923","","B","","","","","",""]
["R4-1705051","CR on Test Configurations for V2X","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","Agreement","","","179","7.16.4","RRM performance (36.133) [LTE_V2X-Perf]",50510,"noted","2017-05-04T13:56:11.717","2017-05-06T09:57:52.800","","","Rel-14","36.133","14.3.0","LTE_V2X-Perf","4924","","B","","","","","",""]
["R4-1705052","Discussion on NR UE transmit timing","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","Discussion","","","451","10.6.3","UE transmit timing [NR_newRAT]",50520,"noted","2017-05-04T13:56:12.620","2017-05-06T11:56:27.633","","","","","","","","","","","","","","",""]
["R4-1705053","Discussion on BS synchronization requirements in NR","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","Discussion","","","456","10.6.8","Other requirements [NR_newRAT]",50530,"withdrawn","2017-05-04T13:56:12.667",null,"","","","","","","","","","","","","","",""]
["R4-1705054","Discussion on cell identification in NR","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","Discussion","","","411","10.1.2","Topics related to incoming LS from other WG [NR_newRAT]",46990,"noted","2017-05-04T13:56:12.713","2017-05-06T11:56:27.633","","","","","","","","","","","","","","",""]
["R4-1705055","Discussion on the TA adjustment delay for shortened TTI and reduced processing","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","Discussion","","","383","9.13.4.1","TA adjustment delay [LTE_sTTIandPT-core]",49080,"noted","2017-05-04T13:56:12.760","2017-05-06T11:56:27.227","","","","","","","","","","","","","","",""]
["R4-1705056","Discussion on SCell activation and deactivation delay with Stti","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","Discussion","","","384","9.13.4.2","SCell activation and deactivation [LTE_sTTIandPT-core]",47900,"noted","2017-05-04T13:56:12.793","2017-05-06T11:56:27.227","","","","","","","","","","","","","","",""]
["R4-1705057","Draft CR on  Scell activation and deactivation delay with Stti","Huawei, HiSilicon","Xiang (Steven) Chen","41576","draftCR","Endorsement","","","384","9.13.4.2","SCell activation and deactivation [LTE_sTTIandPT-core]",50570,"withdrawn","2017-05-04T13:56:12.853",null,"","","Rel-15","36.133","14.3.0","LTE_sTTIandPT-Core","","","B","","","","","",""]
["R4-1705058","Further discussion on the RSRP measurement impact by Inter-frequency RSSI measurement in LAA","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","Discussion","","","36","5.3.3","RRM Core (36.133) [LTE_LAA-Core]",50580,"noted","2017-05-04T13:56:12.900","2017-05-06T11:56:27.227","","","","","","","","","","","","","","",""]
["R4-1705059","Modification on LAA measurement considering Inter-frequency RSSI measurement R13","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","Agreement","","","36","5.3.3","RRM Core (36.133) [LTE_LAA-Core]",50590,"agreed","2017-05-04T13:56:12.947","2017-05-06T11:56:27.227","","","Rel-13","36.133","13.7.0","LTE_LAA-Core","4925","","F","RP-171307","","","","",""]
["R4-1705060","Modification on LAA measurement considering Inter-frequency RSSI measurement R14","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","Agreement","","","36","5.3.3","RRM Core (36.133) [LTE_LAA-Core]",50600,"agreed","2017-05-04T13:56:13.820","2017-05-06T11:56:27.227","","","Rel-14","36.133","14.3.0","LTE_eLAA-Core","4926","","F","RP-171285","","","","",""]
["R4-1705061","Corrections on the LAA test cases R13","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","Agreement","","","38","5.3.5","RRM Performance (36.133) [LTE_LAA-Perf]",50610,"revised","2017-05-04T13:56:14.710","2017-05-06T11:56:27.240","","R4-1705973","Rel-13","36.133","13.7.0","LTE_LAA-Perf","4927","","F","","","","","",""]
["R4-1705062","Corrections on the LAA test cases R14","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","Agreement","","","38","5.3.5","RRM Performance (36.133) [LTE_LAA-Perf]",50620,"agreed","2017-05-04T13:56:15.537","2017-05-23T15:07:51.257","","","Rel-14","36.133","14.3.0","LTE_LAA-Perf","4928","","A","RP-171307","","","","",""]
["R4-1705063","Update of some SCE test case","Huawei, HiSilicon, Anritsu","Xiang (Steven) Chen","41576","CR","Agreement","","","15","4.2.3","RRM (Radio Resource Management) [WI code or TEI12]",50630,"agreed","2017-05-04T13:56:16.427","2017-05-06T11:56:27.240","","","Rel-12","36.133","12.15.0","TEI12","4929","","F","RP-171297","","","","",""]
["R4-1705064","Update of some SCE test case","Huawei, HiSilicon, Anritsu","Xiang (Steven) Chen","41576","CR","Agreement","","","15","4.2.3","RRM (Radio Resource Management) [WI code or TEI12]",50640,"agreed","2017-05-04T13:56:17.330","2017-05-23T15:07:51.287","","","Rel-13","36.133","13.7.0","TEI12","4930","","A","RP-171297","","","","",""]
["R4-1705065","Update of some SCE test case","Huawei, HiSilicon, Anritsu","Xiang (Steven) Chen","41576","CR","Agreement","","","15","4.2.3","RRM (Radio Resource Management) [WI code or TEI12]",50650,"agreed","2017-05-04T13:56:18.253","2017-05-23T15:07:51.287","","","Rel-14","36.133","14.3.0","TEI12","4931","","A","RP-171297","","","","",""]
["R4-1705066","Event triggered reporting on deactivated SCells and interruption probability (0.5%) without DRX (FDD-TDD 4DL CA) R13","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","Agreement","","","69","5.6.2","RRM [WI code or TEI13]",50660,"agreed","2017-05-04T13:56:19.407","2017-05-06T11:56:27.240","","","Rel-13","36.133","13.7.0","TEI13","4932","","F","RP-171311","","","","",""]
["R4-1705067","Event triggered reporting on deactivated SCells and interruption probability (0.5%) without DRX (FDD-TDD 4DL CA) R14","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","Agreement","","","69","5.6.2","RRM [WI code or TEI13]",50670,"agreed","2017-05-04T13:56:20.390","2017-05-23T15:07:51.303","","","Rel-14","36.133","14.3.0","TEI13","4933","","A","RP-171311","","","","",""]
["R4-1705068","Event triggered reporting on deactivated SCells and interruption probability (0.5%) without DRX (TDD-FDD 4 DL CA) R13","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","Agreement","","","69","5.6.2","RRM [WI code or TEI13]",50680,"agreed","2017-05-04T13:56:21.433","2017-05-06T11:56:27.273","","","Rel-13","36.133","13.7.0","TEI13","4934","","F","RP-171311","","","","",""]
["R4-1705069","Event triggered reporting on deactivated SCells and interruption probability (0.5%) without DRX (TDD-FDD 4 DL CA) R14","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","Agreement","","","69","5.6.2","RRM [WI code or TEI13]",50690,"agreed","2017-05-04T13:56:22.197","2017-05-23T15:07:51.303","","","Rel-14","36.133","14.3.0","TEI13","4935","","A","RP-171311","","","","",""]
["R4-1705070","Discussion on measurement gaps in NR","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","Discussion","","","452","10.6.4","Expected Measurement requirements for NSA [NR_newRAT]",50700,"noted","2017-05-04T13:56:23.010","2017-05-06T11:56:27.273","","","","","","","","","","","","","","",""]
["R4-1705071","Discussion on system level and link level simulations in NR RRM","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","Approval","","","453","10.6.5","System level and link level Simulation plan [NR_newRAT]",47640,"noted","2017-05-04T13:56:23.057","2017-05-06T11:56:27.273","","","","","","","","","","","","","","",""]
["R4-1705072","Inter-frequency cell reselection under enhanced coverage for NB-IOT","Ericsson","Santhan Thangarasa","59137","CR","Approval","In this contribution we introduce the inter-frequency test case for NB-IOT","","62","5.5.5","RRM Performance (36.133) [NB_IOT-Perf]",51160,"revised","2017-05-04T14:12:01.910","2017-05-05T21:32:47.607","","R4-1705963","Rel-13","36.133","13.7.0","NB_IOT-Perf","4936","","B","","","","","",""]
["R4-1705073","Inter-frequency cell reselection under enhanced coverage for NB-IOT","Ericsson","Santhan Thangarasa","59137","CR","Agreement","In this contribution we introduce the inter-frequency test case for NB-IOT","","62","5.5.5","RRM Performance (36.133) [NB_IOT-Perf]",51170,"agreed","2017-05-04T14:12:02.813","2017-05-30T15:08:22.297","","","Rel-14","36.133","14.3.0","NB_IOT-Perf","4937","","A","RP-171303","","","","",""]
["R4-1705074","Discussions on gap sharing for RSTD measurement for feMTC","Ericsson","Santhan Thangarasa","59137","discussion","Discussion","In this contribution, we discuss gap sharing for RSTD measurement.","","216","7.18.3.2.4","Gap sharing and measurement [LTE_feMTC-Core]",50260,"noted","2017-05-04T14:12:03.670","2017-05-05T21:32:47.620","","","Rel-14","","","LTE_feMTC-Core","","","","","","","","",""]
["R4-1705075","CONNECTED mode requirements for feMTC UEs in CEModeA","Ericsson","Santhan Thangarasa","59137","CR","Approval","This contribution contains CR to RRC_connected mode requirements for CEModeA","","216","7.18.3.2.4","Gap sharing and measurement [LTE_feMTC-Core]",50750,"revised","2017-05-04T14:12:03.687","2017-05-05T21:32:47.620","","R4-1706191","Rel-14","36.133","14.3.0","LTE_feMTC-Core","4938","","B","","","","","",""]
["R4-1705076","CONNECTED mode requirements for feMTC UEs in CEModeB","Ericsson","Santhan Thangarasa","59137","CR","Approval","This contribution contains CR to RRC_connected mode requirements for CEModeB","","216","7.18.3.2.4","Gap sharing and measurement [LTE_feMTC-Core]",50760,"revised","2017-05-04T14:12:04.547","2017-05-05T21:32:47.620","","R4-1706192","Rel-14","36.133","14.3.0","LTE_feMTC-Core","4939","","B","","","","","",""]
["R4-1705077","Timing advance requirements for Cat M1 UEs","Ericsson","Santhan Thangarasa","59137","CR","Approval","This CR contians timing advance requirements for Cat-M1 UEs.","","45","5.4.3","RRM Core (36.133) [LTE_MTCe2_L1-Core]",50770,"revised","2017-05-04T14:12:05.293","2017-05-05T21:32:47.620","","R4-1706197","Rel-13","36.133","13.7.0","LTE_MTCe2_L1-Core","4940","","F","","","","","",""]
["R4-1705078","Timing advance requirements for Cat M1 UEs","Ericsson","Santhan Thangarasa","59137","CR","Approval","This CR contians timing advance requirements for Cat-M1 UEs.","","45","5.4.3","RRM Core (36.133) [LTE_MTCe2_L1-Core]",50780,"revised","2017-05-04T14:12:06.370","2017-05-23T15:07:51.320","","","Rel-14","36.133","14.3.0","LTE_MTCe2_L1-Core","4941","","A","","","","","",""]
["R4-1705079","Introduction of enhanced RLM for feMTC","Ericsson","Santhan Thangarasa","59137","CR","Approval","This CR introduces the enhanced RLM requirements for feMTC.","","217","7.18.3.2.5","RLM and timing [LTE_feMTC-Core]",50810,"revised","2017-05-04T14:12:07.400","2017-05-05T21:32:47.637","","R4-1706189","Rel-14","36.133","14.3.0","LTE_feMTC-Core","4942","","B","","","","","",""]
["R4-1705080","Discussions on remaining issues of enhanced RLM for feMTC","Ericsson","Santhan Thangarasa","59137","discussion","Discussion","This contribution discusses enhanced RLM for feMTC.","","217","7.18.3.2.5","RLM and timing [LTE_feMTC-Core]",47090,"noted","2017-05-04T14:12:08.337","2017-05-05T21:32:47.637","","","Rel-14","","","LTE_feMTC-Core","","","","","","","","",""]
["R4-1705081","Draft LS on agreements on enhanced RLM for feMTC","Ericsson","Santhan Thangarasa","59137","LS out","Approval","This LS contains RAN4 agreements on enhanced RLM.","","217","7.18.3.2.5","RLM and timing [LTE_feMTC-Core]",50790,"noted","2017-05-04T14:12:08.430","2017-05-05T21:32:47.637","","","Rel-14","","","LTE_feMTC-Core","","","","","","RAN2","","",""]
["R4-1705082","Correction on PHR reporting requirements for NB1","Ericsson","Santhan Thangarasa","59137","CR","Approval","This CR contains a correction to the PHR reporting tables for rel-13 NB1 UEs.","","62","5.5.5","RRM Performance (36.133) [NB_IOT-Perf]",48251,"noted","2017-05-04T14:12:08.477","2017-05-05T21:32:47.637","","R4-1705960, R4-1706058","Rel-13","36.133","13.7.0","NB_IOT-Perf","4943","","F","","","","","",""]
["R4-1705083","Correction on PHR reporting requirements for NB1","Ericsson","Santhan Thangarasa","59137","CR","Approval","This CR contains a correction to the PHR reporting tables for rel-13 NB1 UEs.","","62","5.5.5","RRM Performance (36.133) [NB_IOT-Perf]",49720,"withdrawn","2017-05-04T14:12:09.333",null,"","","Rel-14","36.133","14.3.0","NB_IOT-Perf","4944","","A","","","","","",""]
["R4-1705084","Clarification on V2X requirements for V2X UEs in RRC_CONNECTED state","Ericsson","Santhan Thangarasa","59137","CR","Approval","This CR contains a clarification to the current V2X requirements with respect to RRC_CONNECTED mode operation.","","178","7.16.3","RRM core Maintenance (36.133) [LTE_V2X-Core]",50841,"revised","2017-05-04T14:12:10.177","2017-05-05T21:32:47.637","","R4-1705947","Rel-14","36.133","14.3.0","LTE_V2X-Core","4945","","F","","","","","",""]
["R4-1705085","Correction to cat-M1 UE timing test case","Ericsson","Santhan Thangarasa","59137","CR","Approval","In this CR, we correct the refrences to the core requirements used in the cat-M1 test cases.","","50","5.4.5.1","Test cases for BL/CE UE [LTE_MTCe2_L1-Perf]",50850,"noted","2017-05-04T14:12:11.003","2017-05-05T21:32:47.653","","","Rel-13","36.133","13.7.0","LTE_MTCe2_L1-Perf","4946","","F","","","","","",""]
["R4-1705086","Correction to cat-M1 UE timing test case","Ericsson","Santhan Thangarasa","59137","CR","Approval","In this CR, we correct the refrences to the core requirements used in the cat-M1 test cases.","","50","5.4.5.1","Test cases for BL/CE UE [LTE_MTCe2_L1-Perf]",50860,"withdrawn","2017-05-04T14:12:11.860",null,"","","Rel-14","36.133","14.3.0","LTE_MTCe2_L1-Perf","4947","","A","","","","","",""]
["R4-1705087","PHR reporting for NB-IOT low-power class UEs","Ericsson","Santhan Thangarasa","59137","CR","Approval","This CR is revision to already agreed CR at RAN4#83bis meeting with Tdoc number R4-1704253.","","195","7.17.3.2.3","PHR [NB_IOTenh-Core]",50870,"revised","2017-05-04T14:16:20.553","2017-05-05T21:32:47.653","R4-1704253","R4-1706190","Rel-14","36.133","14.3.0","NB_IOTenh-Core","4695","2","B","","","","","",""]
["R4-1705088","Reference sensitivity for the extended L-band","ORANGE","Atoosa Hatefi","62064","other","Approval","","","322","9.5.2","UE RF (36.101) [LTE_SDL_1500ext-core]",50880,"revised","2017-05-04T15:17:00.217","2017-05-05T16:11:52.907","","R4-1706113","Rel-14","","","LTE_SDL_1500ext-Core","","","","","","","","",""]
["R4-1705089","Traffic test cases related to multi-node tests for Rel-13 LAA","Ericsson, Qualcomm, Nokia, Huawei","Rahman Imadur","57720","discussion","Approval","In this contribution, we provide discussions related to different traffic test cases and our proposals related to this for multi-node tests.","","82","6.1.1","General [FS_LTE_LAA_multinode_test]",582300,"noted","2017-05-04T16:32:35.577","2017-05-05T20:57:54.127","","","Rel-13","","","FS_LTE_LAA_multinode_test","","","","","","","","",""]
["R4-1705090","TP for TR 36.789 v0.0.4: Tools and approach for Multi-node tests","Ericsson, Qualcomm, Nokia, Huawei","Rahman Imadur","57720","pCR","Approval","In this TP, we propose to several changes in Section 5, related to tools and approaches for the tests.","","82","6.1.1","General [FS_LTE_LAA_multinode_test]",582400,"noted","2017-05-04T16:32:35.610","2017-05-05T20:57:54.127","","","Rel-13","36.789","0.0.3","FS_LTE_LAA_multinode_test","","","","","","","","",""]
["R4-1705091","PCMAX: UL power control for single UL CC","Ericsson","Rahman Imadur","57720","discussion","Approval","In this contribution, we describe UL power control issues for signle carrier transmission related to shortened TTI patterns for LTE.","","375","9.13.2.2.2","Power control [LTE_sTTIandPT-core]",50910,"noted","2017-05-04T16:32:35.670","2017-05-05T17:12:44.293","","","Rel-15","","","LTE_sTTIandPT-Core","","","","","","","","",""]
["R4-1705092","PCMAX: UL power control for UL CA","Ericsson","Rahman Imadur","57720","discussion","Approval","In this contribution, we describe UL power control issues for UL CA transmission related to shortened TTI patterns for LTE.","","375","9.13.2.2.2","Power control [LTE_sTTIandPT-core]",50920,"noted","2017-05-04T16:32:35.687","2017-05-05T17:12:44.293","","","Rel-15","","","LTE_sTTIandPT-Core","","","","","","","","",""]
["R4-1705093","MPR/A-MPR for single carrier and CA","Ericsson","Rahman Imadur","57720","discussion","Approval","In this contribution, we describe MPR/A-MPR issues related to shortened TTI patterns for LTE.","","375","9.13.2.2.2","Power control [LTE_sTTIandPT-core]",50930,"noted","2017-05-04T16:32:35.703","2017-05-05T17:12:44.293","","","Rel-15","","","LTE_sTTIandPT-Core","","","","","","","","",""]
["R4-1705094","Joint probability for receiver blocking for NR BS","Ericsson","Rahman Imadur","57720","discussion","Approval","In this contribution, we provide a methodology based on joint probability of receiver blocking where probability of both wanted signal and blocking signal above a level are considered.","","445","10.5.4.2","Blocking Requirements [NR_newRAT]",50940,"noted","2017-05-04T16:32:35.717","2017-05-05T17:02:35.813","","","Rel-15","","","NR_newRAT","","","","","","","","",""]
["R4-1705095","Simulation results using joint probability for receiver blocking","Ericsson","Rahman Imadur","57720","discussion","Approval","In this contribution, we provide a simulation results based on joint probability of receiver blocking where probability of both wanted signal and blocking signal above a level are considered.","","445","10.5.4.2","Blocking Requirements [NR_newRAT]",0,"withdrawn","2017-05-04T16:32:35.733",null,"","","Rel-15","","","NR_newRAT","","","","","","","","",""]
["R4-1705096","Further coexistence simulations results on Urban Macro Scenario in 30GHz","Ericsson","Rahman Imadur","57720","discussion","Approval","In last RAN4 meeting, there were discussions related to some of the assumptions that were used for the ITU-R simulations for UMa scenario [8]. In this contribution, we present further coexietnce simulations for Uma scenario by taking these above mentioned","","422","10.3.5","ACLR and ACS [NR_newRAT]",570300,"noted","2017-05-04T16:32:35.750","2017-05-05T17:02:35.813","","","Rel-15","","","NR_newRAT","","","","","","","","",""]
["R4-1705097","Simulation results for receiver dynamic range of NR BS receiver with different deployment scenarios","Ericsson","Rahman Imadur","57720","discussion","Approval","Simulation results for dynamic range and ICS on BS receiver with different deployment scenarios","","444","10.5.4.1","Dynamic Range [NR_newRAT]",50970,"noted","2017-05-04T16:32:35.767","2017-05-05T14:56:57.637","","","Rel-15","","","NR_newRAT","","","","","","","","",""]
["R4-1705098","Introduction of Band 49 LAA operation in UE spec","Ericsson","Rahman Imadur","57720","CR","Approval","Introduction of new band 49 DL LAA operation is not specified in UE spec","","352","9.11.2","UE RF (Downlink only in 3.5GHz) (36.101) [LTE_ 3550_CBRS_US_LAA]",53100,"revised","2017-05-04T16:32:35.780","2017-05-05T14:54:54.067","","R4-1706090","Rel-15","36.101","14.3.0","LTE_3550_CBRS_US_LAA","4434","","B","","","","","",""]
["R4-1705099","Motivation for the new SI on Enhanced Carrier Aggregation Mobility","Intel Corporation","Yang Tang","56725","discussion","Information","","","473","13","Revision of the Work Plan",51000,"noted","2017-05-04T16:44:01.013","2017-05-06T17:38:10.940","","","Rel-15","","","","","","","","","","","",""]
["R4-1705100","New Study Item Proposal Enhanced Carrier Aggregation Mobility SID","Intel Corporation","Yang Tang","56725","SID new","Information","","","473","13","Revision of the Work Plan",52090,"noted","2017-05-04T16:44:01.030","2017-05-06T17:38:10.940","","","Rel-15","","","","","","","","","","","",""]
["R4-1705101","256QAM for eLAA: allowed power reductions and in-band emissions","Ericsson","Christian Bergljung","21143","discussion","Discussion","In this contribution we present simulation results for power reduction and discuss in-band emissions for 256QAM","","161","7.14.2","UE RF Maintenance(36.101) [LTE_eLAA-Core]",51010,"withdrawn","2017-05-04T19:19:54.323",null,"","","Rel-14","","","LTE_eLAA-Core","","","","","","","","",""]
["R4-1705102","Correction to A-MPR tables and in-band emissions for eLAA","Ericsson","Christian Bergljung","21143","CR","Approval","CR to correct (and change the format) of the A-MPR tables and specify the applicability of the in-band emissions for eLAA","","161","7.14.2","UE RF Maintenance(36.101) [LTE_eLAA-Core]",51020,"revised","2017-05-04T19:19:54.337","2017-05-06T04:47:52.877","","R4-1706088","Rel-14","36.101","14.3.0","LTE_eLAA-Core","4435","","F","","","","","",""]
["R4-1705103","OTA measurements in the radiative near field","Ericsson","Christian Bergljung","21143","CR","Agreement","CR to introduce text on OTA measurements of TRP in the radiative near field","","410","10.1.1","TR maintenance [NR_newRAT]",51030,"agreed","2017-05-04T19:19:55.117","2017-05-05T19:39:19.537","","","Rel-14","38.803","14.0.0","FS_NR_newRAT","0009","","F","RP-171254","","","","",""]
["R4-1705104","Sampling grids for UE TRP measurements","Ericsson, Huawei","Christian Bergljung","21143","CR","Agreement","CR to introduce text on the sampling grid","","410","10.1.1","TR maintenance [NR_newRAT]",51040,"agreed","2017-05-04T19:19:55.913","2017-05-05T19:40:11.440","","","Rel-14","38.803","14.0.0","FS_NR_newRAT","0010","","F","RP-171254","","","","",""]
["R4-1705105","Initial radar altimeter coexistence study","Ericsson, Skyworks Solutions Inc.","Christian Bergljung","21143","other","Approval","Initial results on the LTE/NR compatibility with radar altimeters in 4.2-4.4 GHz. It is proposed that RAN4 does not take a decision on compatibility at RAN4#83.","","415","10.2.1.2","Band definition for NR bands [NR_newRAT]",52460,"noted","2017-05-04T19:19:56.693","2017-05-05T19:30:38.707","","","Rel-15","","","NR_newRAT","","","","","","","","",""]
["R4-1705106","Definition of UE power class","Ericsson, Sony","Christian Bergljung","21143","other","Approval","It is proposed that TRP is used for defining the UE power class (with an EIRP requirements is specified in addition for each power class)","","427","10.4.3.1","UE power class and MPR/A-MPR [NR_newRAT]",45310,"noted","2017-05-04T19:19:56.710","2017-05-05T19:36:57.210","","","Rel-15","","","NR_newRAT","","","","","","","","",""]
["R4-1705107","UE power classes for 28 GHz","Ericsson, Sony","Christian Bergljung","21143","discussion","Discussion","UE power classes discussed: TRP around 20 dBm and possibly a lower power class","","427","10.4.3.1","UE power class and MPR/A-MPR [NR_newRAT]",55110,"noted","2017-05-04T19:19:56.723","2017-05-05T19:37:54.527","","","Rel-15","","","NR_newRAT","","","","","","","","",""]
["R4-1705108","Metrics for power reduction, minimum output power and configured output power for mmW bands","Ericsson, Sony","Christian Bergljung","21143","other","Approval","It is proposed to specify requirements on power reduction, minimum output power and configured output power (not excluding additional EIRP requirements)","","427","10.4.3.1","UE power class and MPR/A-MPR [NR_newRAT]",52060,"noted","2017-05-04T19:19:56.723","2017-05-05T19:38:32.767","","","Rel-15","","","NR_newRAT","","","","","","","","",""]
["R4-1705109","IncMon clarification","Nokia, Alcatel-Lucent Shanghai Bell","Lars Dalsgaard","69933","discussion","Discussion","In this paper address a missing requirement for the IncMon feature. It is not clear from current specification what the UE behavior and requirements are when the number of carriers in NPG is higher than current maximum for when IncMon scaling applies.","","15","4.2.3","RRM (Radio Resource Management) [WI code or TEI12]",51090,"noted","2017-05-04T19:54:57.183","2017-05-05T18:55:32.027","","","Rel-12","36.133","","TEI12","","","","","","","","",""]
["R4-1705110","Clarification to IncMon","Nokia, Alcatel-Lucent Shanghai Bell","Lars Dalsgaard","69933","CR","Approval","Clarification of the IncMon feature for the situation when the number of carrier in the NPG is higher than the stated requirements for when the IncMon scaling applies. Correction to section reference.","","15","4.2.3","RRM (Radio Resource Management) [WI code or TEI12]",51100,"noted","2017-05-04T19:59:14.737","2017-05-05T18:55:32.027","","","Rel-12","36.133","12.15.0","TEI12","4948","","F","","","","","",""]
["R4-1705111","Clarification to IncMon","Nokia, Alcatel-Lucent Shanghai Bell","Lars Dalsgaard","69933","CR","Approval","","","15","4.2.3","RRM (Radio Resource Management) [WI code or TEI12]",51110,"withdrawn","2017-05-04T20:01:23.887",null,"","","Rel-13","36.133","13.7.0","TEI12","4949","","A","","","","","",""]
["R4-1705112","Clarification to IncMon","Nokia, Alcatel-Lucent Shanghai Bell","Lars Dalsgaard","69933","CR","Approval","","","15","4.2.3","RRM (Radio Resource Management) [WI code or TEI12]",51120,"withdrawn","2017-05-04T20:03:47.140",null,"","","Rel-14","36.133","14.3.0","TEI12","4950","","A","","","","","",""]
["R4-1705113","NCSG applicability to non-CA","Nokia, Alcatel-Lucent Shanghai Bell","Lars Dalsgaard","69933","discussion","Discussion","In this paper, we have presented our view on NCSG applicability to non-CA cases and how this could be captured in the RAN4 specification","","270","7.26.2.1","Gap pattern, signaling and capability (RAN2 related) [LTE_meas_gap_enh-Core]",47690,"noted","2017-05-04T20:14:40.737","2017-05-05T18:56:33.217","","","Rel-14","36.133","","LTE_meas_gap_enh-Core","","","","","","","","",""]
["R4-1705114","Reply LS on NCSG applicability to non-CA cases","Nokia, Alcatel-Lucent Shanghai Bell","Lars Dalsgaard","69933","LS out","Approval","","","270","7.26.2.1","Gap pattern, signaling and capability (RAN2 related) [LTE_meas_gap_enh-Core]",51140,"noted","2017-05-04T20:18:22.987","2017-05-05T18:56:33.217","","","Rel-14","","","LTE_meas_gap_enh-Core","","","","","R2-1703948","RAN2","","",""]
["R4-1705115","Introduction of interruption control for Network Controlled Short Gap pattern for inter-frequency measurements","Nokia, Alcatel-Lucent Shanghai Bell","Lars Dalsgaard","69933","CR","Approval","Introduction of interruption control for Network Controlled Short Gap pattern for inter-frequency measurements. Additionally also restructuring of the UE interruption control requirements","","271","7.26.2.2","RRM core requirement [LTE_meas_gap_enh-Core]",574900,"revised","2017-05-04T20:21:22.663","2017-05-05T18:56:33.217","","R4-1705952","Rel-14","36.133","14.3.0","LTE_meas_gap_enh-Core","4951","","B","","","","","",""]
["R4-1705116","Contention Based Random Access Test for UE category NB1 UEs in Normal Coverage","Nokia, Alcatel-Lucent Shanghai Bell","Lars Dalsgaard","69933","CR","Approval","Introduction of Contention Based Random Access Test for UE category NB1 UEs in Normal Coverage","","62","5.5.5","RRM Performance (36.133) [NB_IOT-Perf]",51180,"revised","2017-05-04T20:24:39.347","2017-05-05T18:56:33.230","","R4-1705964","Rel-13","36.133","13.7.0","NB_IOT-Perf","4952","","F","","","","","",""]
["R4-1705117","Contention Based Random Access Test for UE category NB1 UEs in Normal Coverage","Nokia, Alcatel-Lucent Shanghai Bell","Lars Dalsgaard","69933","CR","Agreement","","","62","5.5.5","RRM Performance (36.133) [NB_IOT-Perf]",51190,"agreed","2017-05-04T20:27:16.343","2017-05-23T15:07:51.337","","","Rel-14","36.133","14.3.0","NB_IOT-Perf","4953","","A","RP-171303","","","","",""]
["R4-1705118","Contention Based Random Access Test for UE category NB1 UEs in Enhanced Coverage","Nokia, Alcatel-Lucent Shanghai Bell","Lars Dalsgaard","69933","CR","Approval","Introduction of Contention Based Random Access Test for UE category NB1 UEs in Enhanced Coverage","","62","5.5.5","RRM Performance (36.133) [NB_IOT-Perf]",51220,"revised","2017-05-04T20:29:47.557","2017-05-05T18:57:41.233","","R4-1705965","Rel-13","36.133","13.7.0","NB_IOT-Perf","4954","","F","","","","","",""]
["R4-1705119","Contention Based Random Access Test for UE category NB1 UEs in Enhanced Coverage","Nokia, Alcatel-Lucent Shanghai Bell","Lars Dalsgaard","69933","CR","Agreement","","","62","5.5.5","RRM Performance (36.133) [NB_IOT-Perf]",51450,"agreed","2017-05-04T20:31:50.800","2017-05-23T15:07:51.337","","","Rel-14","36.133","14.3.0","NB_IOT-Perf","4955","","A","RP-171303","","","","",""]
["R4-1705120","Discussion on early RLF for eNB-IOT","Nokia, Alcatel-Lucent Shanghai Bell","Lars Dalsgaard","69933","discussion","Discussion","In this paper, we have discussed the issue addressed by the proposed early Qin and Qout reporting and the solution. We propose a solution which addresses the identified problem without the need for reporting and which does not suffer from potentially larg","","193","7.17.3.2.1","Repetition level feedback and RLM [NB_IOTenh-Core]",51200,"noted","2017-05-04T20:34:35.090","2017-05-05T18:57:41.233","","","Rel-14","36.133","","NB_IOTenh-Core","","","","","","","","",""]
["R4-1705121","LS on new parameter configuration for RLM for eNB-IoT","Nokia, Alcatel-Lucent Shanghai Bell","Lars Dalsgaard","69933","LS out","Approval","","","193","7.17.3.2.1","Repetition level feedback and RLM [NB_IOTenh-Core]",51210,"noted","2017-05-04T20:36:26.533","2017-05-05T18:57:41.233","","","Rel-14","","","NB_IOTenh-Core","","","","","","RAN2","","",""]
["R4-1705122","CR: NB-IoT Radio Link Monitoring Performance Test for Out-of-Sync in Enhanced Coverage","Nokia, Alcatel-Lucent Shanghai Bell","Lars Dalsgaard","69933","CR","Agreement","Introduction of NB-IoT Radio Link Monitoring Performance Test for Out-of-Sync in Enhanced Coverage","","62","5.5.5","RRM Performance (36.133) [NB_IOT-Perf]",49750,"agreed","2017-05-04T20:38:41.033","2017-05-05T18:57:41.250","","","Rel-14","36.133","14.3.0","NB_IOT-Perf","4956","","A","RP-171302","","","","",""]
["R4-1705123","SS burst periodicity for initial cell selection in NR","Nokia, Alcatel-Lucent Shanghai Bell","Lars Dalsgaard","69933","discussion","Discussion","In this paper we discussed the incoming LSs [3, 4] from RAN1 regarding default SS burst periodicity for cell selection","","411","10.1.2","Topics related to incoming LS from other WG [NR_newRAT]",49160,"noted","2017-05-04T21:33:54.500","2017-05-05T19:22:04.947","","","Rel-14","","","NR_newRAT-Core","","","","","","","","",""]
["R4-1705124","CR for correction for RRM core requirement for Cat.1bis UE","Qualcomm Incorporated","Jaeho Ryu","47148","CR","Approval","","","232","7.19.3","RRM core (36.133) [LTE_UE_cat_1RX-Core]",51240,"revised","2017-05-04T21:40:04.477","2017-05-06T05:27:52.787","R4-1704123","R4-1706022","Rel-14","36.133","14.3.0","LTE_UE_cat_1RX-Core","4706","2","F","","","","","",""]
["R4-1705125","CR for RRM tests for Cat.1 UE with single receiver chain","Qualcomm Incorporated","Jaeho Ryu","47148","CR","Approval","","","235","7.19.4","RRM performance (36.133) [LTE_UE_cat_1RX-Perf]",51250,"revised","2017-05-04T21:42:41.927","2017-05-06T05:27:52.850","R4-1704125","R4-1706023","Rel-14","36.133","14.3.0","LTE_UE_cat_1RX-Perf","4708","2","B","","","","","",""]
["R4-1705126","Optimization of UE capability signalling","Qualcomm Incorporated","Jaeho Ryu","47148","other","Discussion","","","472","12","Liaison and output to other groups",51260,"noted","2017-05-04T21:44:53.773","2017-05-06T05:27:52.850","","","","","","LTE_EBF_FDMIMO-Core","","","","","","","","",""]
["R4-1705127","Tx EVM and Rx EVM for DL 1025QAM modulation","Qualcomm Incorporated","Jaeho Ryu","47148","other","Discussion","In this contribution, we provide simulation results to evaluate the impact of Tx and Rx EVM on 1024QAM PDSCH demodulation performance and provide our proposal for RAN4¡¯s LS response.","","405","9.17.1","General [LTE_HCS]",51880,"noted","2017-05-04T21:44:53.790","2017-05-06T05:27:52.850","","","","","","LTE_1024QAM_DL-Core","","","","","","","","",""]
["R4-1705128","WF on CRS-IM capability and assistance signalling","Qualcomm Incorporated","Jaeho Ryu","47148","other","Approval","WF on CRS-IM capability and assistance signalling","","275","7.27.1.1","Capability and signaling [LTE_eCRSIM_eSUMIMO]",53670,"revised","2017-05-04T21:44:53.807","2017-05-06T05:27:52.863","","R4-1706031","","","","LTE_eCRSIM_eSUMIMO","","","","","","","","",""]
["R4-1705129","Further simulation results for enhanced CRS-IM PDCCH demodulation test","Qualcomm Incorporated","Jaeho Ryu","47148","other","Discussion","In this contribution, we provide simulation results for test 1 and further analysis for test 3.","","278","7.27.2.2","Control channel [LTE_eCRSIM_eSUMIMO]",49410,"noted","2017-05-04T21:44:53.820","2017-05-06T05:27:52.863","","","","","","LTE_eCRSIM_eSUMIMO","","","","","","","","",""]
["R4-1705130","Further simulation results for PDSCH demodulation tests for enhanced SU-MIMO","Qualcomm Incorporated","Jaeho Ryu","47148","other","Discussion","In this contribution, we provide simulation results for further evaluation scenarios and our view on the feasibility of requirement definition.","","279","7.27.3","SU-MIMO IM [LTE_eCRSIM_eSUMIMO]",49250,"noted","2017-05-04T21:44:53.820","2017-05-06T05:27:52.880","","","","","","LTE_eCRSIM_eSUMIMO","","","","","","","","",""]
["R4-1705131","Simulation results for MUST case 1/2","Qualcomm Incorporated","Jaeho Ryu","47148","other","Discussion","In this contribution, we provide simulation results for candidate test cases for MUST case 1 and 2.","","255","7.24.1.1","Case1 and Case 2 [LTE_MUST-Perf]",51310,"noted","2017-05-04T21:44:53.837","2017-05-06T05:27:52.880","","","","","","LTE_MUST-Perf","","","","","","","","",""]
["R4-1705132","Simulation results for MUST case 3","Qualcomm Incorporated","Jaeho Ryu","47148","other","Discussion","In this contribution, we provide simulation results for candidate test cases for MUST case 3.","","256","7.24.1.2","Case 3 [LTE_MUST-Perf]",52300,"noted","2017-05-04T21:44:53.853","2017-05-06T05:27:52.897","","","","","","LTE_MUST-Perf","","","","","","","","",""]
["R4-1705133","CA demodulation test for 4 Rx UE","Qualcomm Incorporated","Jaeho Ryu","47148","other","Discussion","In this contribution, we provide simulation results for 256QAM and 4 layer MIMO based on simulation assumption circulated on the RAN4 reflector.","","244","7.21.2","UE demodulation (36.101) [LTE_4Rx_AP_DL_CA-Perf]",53590,"noted","2017-05-04T21:44:53.853","2017-05-06T05:27:52.897","","","","","","LTE_4Rx_AP_DL_CA-Perf","","","","","","","","",""]
["R4-1705134","Correction to RSTD test cases for carrier aggregation (R12)","Qualcomm Incorporated","Jaeho Ryu","47148","CR","Approval","for 5 MHz PRS bandwidth, the number of consecutive downlink positioning subframes (NPRS) should be NPRS =2 as per subclause 9.1.10","","15","4.2.3","RRM (Radio Resource Management) [WI code or TEI12]",51340,"revised","2017-05-04T21:44:53.867","2017-05-06T05:27:52.910","","R4-1706207","Rel-12","36.133","12.15.0","TEI12","4957","","F","","","","","",""]
["R4-1705135","Correction to RSTD test cases for carrier aggregation (R13)","Qualcomm Incorporated","Jaeho Ryu","47148","CR","Approval","for 5 MHz PRS bandwidth, the number of consecutive downlink positioning subframes (NPRS) should be NPRS =2 as per subclause 9.1.10","","15","4.2.3","RRM (Radio Resource Management) [WI code or TEI12]",51350,"revised","2017-05-04T21:44:54.633","2017-05-06T05:27:52.910","","R4-1706208","Rel-13","36.133","13.7.0","TEI12","4958","","A","","","","","",""]
["R4-1705136","Correction to RSTD test cases for carrier aggregation (R14)","Qualcomm Incorporated","Jaeho Ryu","47148","CR","Approval","for 5 MHz PRS bandwidth, the number of consecutive downlink positioning subframes (NPRS) should be NPRS =2 as per subclause 9.1.10","","15","4.2.3","RRM (Radio Resource Management) [WI code or TEI12]",51360,"revised","2017-05-04T21:44:55.380","2017-05-06T05:27:52.927","","R4-1706209","Rel-14","36.133","14.3.0","TEI12","4959","","A","","","","","",""]
["R4-1705137","CR for FRC overview table for 4 layer SDR tests (R13)","Qualcomm Incorporated","Jaeho Ryu","47148","CR","Agreement","Add new FRCs for 4 layer SDR tests in FRC overview table.","","32","5.2.3","UE demodulation and CSI (36.101) [LTE_4Rx_AP_DL-Perf]",51370,"agreed","2017-05-04T21:44:56.160","2017-05-06T05:27:52.927","","","Rel-13","36.101","13.7.0","LTE_4Rx_AP_DL-Perf","4436","","D","RP-171304","","","","",""]
["R4-1705138","CR for FRC overview table for 4 layer SDR tests (R14)","Qualcomm Incorporated","Jaeho Ryu","47148","CR","Agreement","Add new FRCs for 4 layer SDR tests in FRC overview table.","","32","5.2.3","UE demodulation and CSI (36.101) [LTE_4Rx_AP_DL-Perf]",51380,"agreed","2017-05-04T21:44:56.940","2017-05-06T05:27:52.927","","","Rel-14","36.101","14.3.0","LTE_4Rx_AP_DL-Perf","4437","","A","RP-171304","","","","",""]
["R4-1705139","Maintenance CR for demodulation and CQI tests for Cat.1bis UE","Qualcomm Incorporated","Jaeho Ryu","47148","CR","Agreement","Remove [] in the in the demodulation and CQI test specification. Add new FRCs for Cat.1bis UE demodulation tests in FRC overview table. Channel bandwidth for R.31-1A TDD is changed to 20MHz.","","236","7.19.5","UE demodulation (36.101) [LTE_UE_cat_1RX-Perf]",51390,"agreed","2017-05-04T21:44:57.690","2017-05-06T05:27:52.943","","","Rel-14","36.101","14.3.0","LTE_UE_cat_1RX-Perf","4438","","D","RP-171269","","","","",""]
["R4-1705140","CR for RSTD measurement requirement for Cat.1bis UE","Qualcomm Incorporated","Jaeho Ryu","47148","CR","Approval","Introduced RSTD measurement requirements for category 1bis UE.","","233","7.19.3.1","E-CID and OTDOA [LTE_UE_cat_1RX-Core]",51400,"revised","2017-05-04T21:44:58.453","2017-05-06T05:27:52.943","","R4-1706024","Rel-14","36.133","14.3.0","LTE_UE_cat_1RX-Core","4960","","B","","","","","",""]
["R4-1705141","CR for correcting transmit timing requirement of eLAA","Qualcomm Incorporated","Jaeho Ryu","47148","CR","Approval","Clarify UE transmit timing requirement for eLAA.","","164","7.14.5","RRM core Maintenance (36.133) [LTE_eLAA-Core]",54980,"noted","2017-05-04T21:44:59.297","2017-05-06T05:27:52.943","","","Rel-14","36.133","14.3.0","LTE_eLAA-Core","4961","","F","","","","","",""]
["R4-1705142","Maintenance CR for LLA demodulation tests","Qualcomm Incorporated","Jaeho Ryu","47148","CR","Approval","Add FRCs for LAA demodulation tests in FRC overview table. Specify FRC number for LAA SDR tests.","","39","5.3.6","UE Demodulation (36.101) [LTE_LAA-Perf]",51420,"revised","2017-05-04T21:45:00.077","2017-05-06T05:27:52.943","","R4-1705942","Rel-13","36.101","13.7.0","LTE_LAA-Perf","4439","","D","","","","","",""]
["R4-1705143","Maintenance CR for LLA demodulation tests","Qualcomm Incorporated","Jaeho Ryu","47148","CR","Approval","Add FRCs for LAA demodulation tests in FRC overview table. Specify FRC number for LAA SDR tests.","","39","5.3.6","UE Demodulation (36.101) [LTE_LAA-Perf]",51430,"revised","2017-05-04T21:45:00.840","2017-05-06T05:27:52.957","","R4-1705943","Rel-14","36.101","14.3.0","LTE_LAA-Perf","4440","","A","","","","","",""]
["R4-1705144","Correction on uplink limitation of 3DL CA 8A-11A-28A","SoftBank Corp.","Kenichi Kihara","41094","CR","Agreement","This CR is to add notes on uplink limitation.","","101","7.3.2","UE RF (36.101) [LTE_CA_R14_3DL1UL-Core]",45980,"agreed","2017-05-04T21:48:52.220","2017-05-04T21:53:42.187","","","Rel-14","36.101","14.3.0","LTE_CA_R14_3DL1UL-Core","4441","","F","RP-171274","","","","",""]
["R4-1705145","Correction to inter-frequency RRC re-establishment test case in NB-IOT","Qualcomm Incorporated","Achaleshwar Sahai","63246","CR","Approval","The PRB location of nCell2 is modified such that the OCNG patttern fits","","62","5.5.5","RRM Performance (36.133) [NB_IOT-Perf]",49810,"revised","2017-05-04T21:49:31.780","2017-05-06T09:57:52.910","","R4-1705961","Rel-13","36.133","13.7.0","NB_IOT-Perf","4962","","F","","","","","",""]
["R4-1705146","Correction to inter-frequency RRC re-establishment test case in NB-IOT","Qualcomm Incorporated","Achaleshwar Sahai","63246","CR","Agreement","The PRB location of nCell2 is modified such that the OCNG patttern fits","","62","5.5.5","RRM Performance (36.133) [NB_IOT-Perf]",49820,"agreed","2017-05-04T21:49:32.683","2017-05-23T15:17:51.113","","","Rel-14","36.133","14.3.0","NB_IOT-Perf","4963","","A","RP-171302","","","","",""]
["R4-1705147","CR to cleanup Handover Requirements in eMTC","Qualcomm Incorporated","Achaleshwar Sahai","63246","CR","Approval","CE mode A and mode B requirements are merged into one section","","46","5.4.3.1","BL/CE UE [LTE_MTCe2_L1-Core]",55080,"noted","2017-05-04T21:49:33.463","2017-05-06T09:57:52.927","","","Rel-13","36.133","13.7.0","LTE_MTCe2_L1-Core","4964","","D","","","","","",""]
["R4-1705148","CR to cleanup Handover Requirements in Cat-M1","Qualcomm Incorporated","Achaleshwar Sahai","63246","CR","Approval","CE mode A and mode B requirements are merged into one section","","46","5.4.3.1","BL/CE UE [LTE_MTCe2_L1-Core]",571300,"withdrawn","2017-05-04T21:49:34.197",null,"","","Rel-14","36.133","14.3.0","LTE_MTCe2_L1-Core","4965","","A","","","","","",""]
["R4-1705149","CR to cleanup Random access  Requirements for Cat-M1","Qualcomm Incorporated","Achaleshwar Sahai","63246","CR","Approval","New (independent) section for Random access requirements for Cat-M1 Ues is added to make the specification structure consistent","","46","5.4.3.1","BL/CE UE [LTE_MTCe2_L1-Core]",571500,"withdrawn","2017-05-04T21:49:35.010",null,"","","Rel-13","36.133","13.7.0","LTE_MTCe2_L1-Core","4966","","D","","","","","",""]
["R4-1705150","CR to cleanup Random access  Requirements for Cat-M1","Qualcomm Incorporated","Achaleshwar Sahai","63246","CR","Approval","New (independent) section for Random access requirements for Cat-M1 Ues is added to make the specification structure consistent","","46","5.4.3.1","BL/CE UE [LTE_MTCe2_L1-Core]",571600,"withdrawn","2017-05-04T21:49:35.930",null,"","","Rel-14","36.133","14.3.0","LTE_MTCe2_L1-Core","4967","","A","","","","","",""]
["R4-1705151","RSTD requirements in FeMTC","Qualcomm Incorporated","Achaleshwar Sahai","63246","discussion","Discussion","In this paper we provide input on NPRS, measurement period and desired RSTD accuracy for FeMTC Ues","","211","7.18.3.1.2","OTDOA [LTE_feMTC-Core]",50000,"noted","2017-05-04T21:49:36.727","2017-05-09T07:37:51.460","","","","","","","","","","","","","","",""]
["R4-1705152","Enhanced RLM event: mechanism to trigger & reporting contents","Qualcomm Incorporated","Achaleshwar Sahai","63246","discussion","Discussion","In this paper, we provide input on the mechanism to trigger enhanced RLM event and associated reporting content. We propose to trigger enhanced RLM event based on MPDCCH transmission parameters modified relative to RLM. We propose to not report anything b","","217","7.18.3.2.5","RLM and timing [LTE_feMTC-Core]",50270,"noted","2017-05-04T21:49:36.740","2017-05-06T09:57:52.927","","","","","","","","","","","","","","",""]
["R4-1705153","RLM test case for non-BL/CE UEs","Qualcomm Incorporated","Achaleshwar Sahai","63246","discussion","Discussion","In this paper we propose modifications to the Cat-M1 RLM test case so that they are applicable to non-BL/CE Ues","","51","5.4.5.2","Test cases for Non-BL/CE UE [LTE_MTCe2_L1-Perf]",51530,"noted","2017-05-04T21:49:36.740","2017-05-06T09:57:52.943","","","","","","","","","","","","","","",""]
["R4-1705154","On RRM requirements for sTTI and reduced processing time","Qualcomm Incorporated","Achaleshwar Sahai","63246","discussion","Discussion","In this paper, we provide our views on TA adjustment delay, Scell activation/ deactivation delay, CGI requirements and MRTD","","385","9.13.4.3","Maximum reception/transmission timing difference [LTE_sTTIandPT-core]",51540,"noted","2017-05-04T21:49:36.740","2017-05-06T09:57:52.943","","","","","","","","","","","","","","",""]
["R4-1705155","Configuration values for SS burst set periodicity","Nokia, Alcatel-Lucent Shanghai Bell","Lars Dalsgaard","69933","discussion","Discussion","In this paper we have looked at the SS burst periodicity values. We look at the synchronization as well as measurement aspects","","411","10.1.2","Topics related to incoming LS from other WG [NR_newRAT]",47010,"noted","2017-05-04T22:08:16.320","2017-05-05T19:22:04.947","","","Rel-14","","","NR_newRAT-Core","","","","","","","","",""]
["R4-1705156","NR measurements for enabling NSA operation","Nokia, Alcatel-Lucent Shanghai Bell","Lars Dalsgaard","69933","discussion","Discussion","In this paper, we have looked at the work ahead and based on incoming LSs from RAN1","","452","10.6.4","Expected Measurement requirements for NSA [NR_newRAT]",51780,"noted","2017-05-04T22:24:25.387","2017-05-05T19:22:04.963","","","Rel-14","","","NR_newRAT-Core","","","","","","","","",""]
["R4-1705157","UE NR RRM measurement capabilities","Nokia, Alcatel-Lucent Shanghai Bell","Lars Dalsgaard","69933","discussion","Discussion","In this paper, welook at the agreements related to beam management which can be used as input to the discussion on UE measurement capability and related requirements","","450","10.6.2","UE measurement capability [NR_newRAT]",49880,"noted","2017-05-04T22:34:41.937","2017-05-05T19:22:04.963","","","Rel-14","","","NR_newRAT-Core","","","","","","","","",""]
["R4-1705158","WF on NR cell detection","Nokia, Alcatel-Lucent Shanghai Bell","Lars Dalsgaard","69933","discussion","Approval","WF on NR cell detection","","453","10.6.5","System level and link level Simulation plan [NR_newRAT]",50710,"noted","2017-05-04T22:40:00.703","2017-05-05T19:22:42.997","","","Rel-15","","","NR_newRAT-Core","","","","","","","","",""]
["R4-1705159","WF on NR LL Measurement performance","Nokia, Alcatel-Lucent Shanghai Bell","Lars Dalsgaard","69933","discussion","Approval","WF on NR LL Measurement performance","","453","10.6.5","System level and link level Simulation plan [NR_newRAT]",56130,"noted","2017-05-04T22:43:57.473","2017-05-05T19:22:42.997","","","Rel-15","","","NR_newRAT-Core","","","","","","","","",""]
["R4-1705160","TP on Maximum output power for Band 71","Samsung, T-Mobile, Nokia, Intel, Skyworks","Haijie Qiu","46265","pCR","","","","336","9.8.2","UE RF (36.101) [LTE600_US-core]",51620,"approved","2017-05-05T00:47:54.537","2017-05-05T17:57:52.737","","","Rel-15","36.755","0.0.1","LTE600_US-Core","","","","","","","","",""]
["R4-1705161","TP on Spurious emission on Band 71 UE co-existence","SAMSUNG Electronics Co., Ltd.","Haijie Qiu","46265","pCR","Approval","","","336","9.8.2","UE RF (36.101) [LTE600_US-core]",52380,"approved","2017-05-05T00:50:47.087","2017-05-05T17:57:52.737","","","Rel-15","36.755","0.0.1","LTE600_US-Core","","","","","","","","",""]
["R4-1705162","Consideration on Transmission BW configuration and CHBW in NR UE specification","SAMSUNG Electronics Co., Ltd.","Haijie Qiu","46265","pCR","","","","336","9.8.2","UE RF (36.101) [LTE600_US-core]",55060,"revised","2017-05-05T00:52:22.820","2017-05-05T17:57:52.737","","R4-1705863","Rel-15","36.755","0.0.1","LTE600_US-Core","","","","","","","","",""]
["R4-1705163","TP on section 6 in TR36.755","SAMSUNG Electronics Co., Ltd.","Haijie Qiu","46265","pCR","","","","335","9.8.1","General [LTE600_US]",51630,"revised","2017-05-05T00:55:53.307","2017-05-05T17:57:52.737","","R4-1705886","Rel-15","36.755","0.0.1","LTE600_US-Core","","","","","","","","",""]
["R4-1705164","Further discussion on the framework of LTE BHH OTA","Guangdong OPPO Mobile Telecom.","Zhi Zhang","65210","discussion","Decision","","","139","7.10.1","General [LTE_UTRA_TRP_TRS-Core]",52270,"noted","2017-05-05T01:07:13.750","2017-05-06T06:17:52.190","","","Rel-14","","","","","","","","","","","",""]
["R4-1705165","Further consideration for NR band and band combination in Rel15 WI","NTT DOCOMO, INC.","Yousuke Sano","59654","other","Approval","This contribution provides the handling scheme of NR band and band combination in Rel.15 WI.","","412","10.2","NR bands and NR-LTE band combinations [NR_newRAT]",47830,"revised","2017-05-05T01:25:34.873","2017-05-06T13:47:52.233","","R4-1706048","Rel-15","","","NR_newRAT","","","","","","","","",""]
["R4-1705166","Consideration on NR band definition for 3.3-4.2GHz","China Telecommunications","Bin Han","70669","discussion","","In this paper, we provide our consideration on NR band definition for 3.3-4.2GHz.","","415","10.2.1.2","Band definition for NR bands [NR_newRAT]",52250,"noted","2017-05-05T01:33:56.013","2017-05-05T01:55:25.827","","","","","","NR_newRAT","","","","","","","","",""]
["R4-1705167","Consideration on power class 2 UE for 3.5GHz","China Telecommunications","Bin Han","70669","discussion","","In this contribution, we provide the initial link budget results and discuss the introduction of power class 2 for 3.5GHz.","","427","10.4.3.1","UE power class and MPR/A-MPR [NR_newRAT]",567500,"noted","2017-05-05T01:45:50.650","2017-05-05T01:55:25.827","","","","","","NR_newRAT","","","","","","","","",""]
["R4-1705168","CR for E-UTRAN TDD intra-frequency MBB handover test cases","ZTE","Qian Yang","45032","CR","Agreement","","","240","7.20.2","RRM performance (36.133) [LTE_eMob-Perf]",49860,"agreed","2017-05-05T02:13:13.860","2017-05-06T07:52:37.500","","","Rel-14","36.133","14.3.0","LTE_eMob","4968","","B","RP-171259","","","","",""]
["R4-1705169","CR for E-UTRAN FDD intra-frequency MBB handover test cases","ZTE","Qian Yang","45032","CR","Agreement","","","240","7.20.2","RRM performance (36.133) [LTE_eMob-Perf]",49870,"agreed","2017-05-05T02:13:14.670","2017-05-06T07:52:37.500","","","Rel-14","36.133","14.3.0","LTE_eMob","4969","","B","RP-171259","","","","",""]
["R4-1705170","CR for correction of handover test cases","ZTE","Qian Yang","45032","CR","Agreement","","","240","7.20.2","RRM performance (36.133) [LTE_eMob-Perf]",51700,"agreed","2017-05-05T02:13:15.467","2017-05-06T07:52:37.440","","","Rel-14","36.133","14.3.0","LTE_eMob","4970","","F","RP-171259","","","","",""]
["R4-1705171","CR for correction of handover requirements for mobility enhancement","ZTE","Qian Yang","45032","CR","Agreement","","","239","7.20.1","RRM core maintenance (36.133) [LTE_eMob-Core]",51710,"agreed","2017-05-05T02:13:16.230","2017-05-06T07:52:37.440","","","Rel-14","36.133","14.3.0","LTE_eMob-Core","4971","","F","RP-171286","","","","",""]
["R4-1705172","LS to RAN5 on handover tests","ZTE","Qian Yang","45032","LS out","Approval","","","240","7.20.2","RRM performance (36.133) [LTE_eMob-Perf]",51720,"revised","2017-05-05T02:13:17.027","2017-05-06T07:52:37.440","","R4-1706005","Rel-14","","","LTE_eMob","","","","","","RAN5","","",""]
["R4-1705173","Alignment and impairment results for PDSCH demodulation for eCRS-IM","ZTE","Qian Yang","45032","discussion","Discussion","","","277","7.27.2.1","PDSCH [LTE_eCRSIM_eSUMIMO]",46380,"noted","2017-05-05T02:13:17.153","2017-05-06T07:52:37.440","","","Rel-14","","","LTE_eCRSIM_eSUMIMO","","","","","","","","",""]
["R4-1705174","Alignment and impairment results for control channel demodulation for eCRS-IM","ZTE","Qian Yang","45032","discussion","Discussion","","","278","7.27.2.2","Control channel [LTE_eCRSIM_eSUMIMO]",51290,"noted","2017-05-05T02:13:17.167","2017-05-06T07:52:37.440","","","Rel-14","","","LTE_eCRSIM_eSUMIMO","","","","","","","","",""]
["R4-1705175","Simulation results without TO&FO for BS IC receiver","ZTE","Qian Yang","45032","discussion","Discussion","","","300","8.1.3","Link level evaluation [FS_LTE _IC_BS]",55170,"noted","2017-05-05T02:13:17.167","2017-05-06T07:52:37.453","","","Rel-14","","","FS_LTE_IC_BS","","","","","","","","",""]
["R4-1705176","Simulation results with TO&FO for BS IC receiver","ZTE","Qian Yang","45032","discussion","Discussion","","","300","8.1.3","Link level evaluation [FS_LTE _IC_BS]",55180,"noted","2017-05-05T02:13:17.183","2017-05-06T07:52:37.500","","","Rel-14","","","FS_LTE_IC_BS","","","","","","","","",""]
["R4-1705177","Discussion on test cases and test metric for BS IC receiver","ZTE","Qian Yang","45032","discussion","Discussion","","","298","8.1.1","General [FS_LTE _IC_BS]",55220,"noted","2017-05-05T02:13:17.197","2017-05-06T07:52:37.500","","","Rel-14","","","FS_LTE_IC_BS","","","","","","","","",""]
["R4-1705178","Discussion on cell identification in NR","ZTE","Qian Yang","45032","discussion","Discussion","","","452","10.6.4","Expected Measurement requirements for NSA [NR_newRAT]",49890,"noted","2017-05-05T02:13:17.213","2017-05-06T07:52:37.500","","","Rel-15","","","NR_newRAT","","","","","","","","",""]
["R4-1705179","TP for 36.789: On the need for inclusion of future Wi-Fi system","Huawei, Ericsson, Qualcomm, Nokia","Xiang (Steven) Chen","41576","pCR","Approval","","","82","6.1.1","General [FS_LTE_LAA_multinode_test]",622400,"noted","2017-05-05T02:20:01.590","2017-05-06T19:17:51.940","","","Rel-13","36.789","0.0.3","FS_LTE_LAA_multinode_test","","","","","","","","",""]
["R4-1705180","TP for 36.789: Updates on section 5 and 6.1","Huawei, Ericsson, Qualcomm, Nokia","Xiang (Steven) Chen","41576","pCR","Approval","","","82","6.1.1","General [FS_LTE_LAA_multinode_test]",622500,"noted","2017-05-05T02:20:01.933","2017-05-06T19:17:51.953","","","Rel-13","36.789","0.0.3","FS_LTE_LAA_multinode_test","","","","","","","","",""]
["R4-1705181","Some corrections on V2X in TS 36.101","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","Agreement","","","177","7.16.2","UE RF Maintenance (36.101) [LTE_V2X-Core]",51810,"agreed","2017-05-05T02:20:01.980","2017-05-05T11:12:35.590","","","Rel-14","36.101","14.3.0","LTE_V2X-Core","4442","","F","RP-171282","","","","",""]
["R4-1705182","RAN4 work plan for V2X phase 2","Huawei, HiSilicon","Xiang (Steven) Chen","41576","other","Approval","This contribution is for approval.","","399","9.16.1","General [LTE_eV2X]",51820,"noted","2017-05-05T02:20:02.807","2017-05-05T11:12:35.590","","","","","","LTE_eV2X-Core","","","","","","","","",""]
["R4-1705183","V2X scenarios for V2X phase 2","Huawei, HiSilicon","Xiang (Steven) Chen","41576","other","Approval","This contribution is for approval.","","399","9.16.1","General [LTE_eV2X]",52960,"noted","2017-05-05T02:20:02.837","2017-05-05T11:12:35.607","","","","","","LTE_eV2X-Core","","","","","","","","",""]
["R4-1705184","Draft CR on BS for TS 36.104","Huawei","Xiang (Steven) Chen","41576","draftCR","","","","378","9.13.3","BS RF (36.104) [LTE_sTTIandPT-core]",51840,"noted","2017-05-05T02:20:02.837","2017-05-05T11:12:35.607","","","Rel-14","36.104","14.3.0","LTE_sTTIandPT-Core","","","","","","","","",""]
["R4-1705185","WF on UE RF remaining issues","Huawei, HiSilicon","Xiang (Steven) Chen","41576","other","Approval","This contribution is for approval.","","371","9.13.2","UE RF (36.101) [LTE_sTTIandPT-core]",51850,"noted","2017-05-05T02:20:02.853","2017-05-05T11:12:35.607","","","","","","LTE_sTTIandPT-Core","","","","","","","","",""]
["R4-1705186","UE ON/OFF time mask for all use cases","Huawei, HiSilicon","Xiang (Steven) Chen","41576","other","Approval","This contribution is for approval.","","374","9.13.2.2.1","ON/OFF time mask [LTE_sTTIandPT-core]",609800,"noted","2017-05-05T02:20:02.870","2017-05-05T11:12:35.607","","","","","","LTE_sTTIandPT-Core","","","","","","","","",""]
["R4-1705187","Work plan on supporting 1024 QAM","Huawei, HiSilicon","Xiang (Steven) Chen","41576","other","Approval","This contribution is for approval.","","405","9.17.1","General [LTE_HCS]",51270,"approved","2017-05-05T02:20:02.900","2017-05-05T11:12:35.607","","","","","","LTE_1024QAM_DL-Core","","","","","","","","",""]
["R4-1705188","Initial consideration on 1024 QAM","Huawei, HiSilicon","Xiang (Steven) Chen","41576","other","Approval","This contribution is for approval.","","405","9.17.1","General [LTE_HCS]",51870,"noted","2017-05-05T02:20:02.917","2017-05-05T11:12:35.607","","","","","","LTE_1024QAM_DL-Core","","","","","","","","",""]
["R4-1705189","Reply LS on regarding 1024 QAM","Huawei, HiSilicon","Xiang (Steven) Chen","41576","LS out","Approval","","","405","9.17.1","General [LTE_HCS]",56610,"revised","2017-05-05T02:20:02.993","2017-05-05T11:12:35.623","","R4-1705880","","","","LTE_1024QAM_DL-Core","","","","","R1-1706842","RAN1","","",""]
["R4-1705190","TP for TR 36.714-00-02: finalize MSD for CA_3A-7A-8A 3DL/2UL CA","CHTTL","Bo-Han Hsieh","61837","pCR","Approval","","","125","7.7.2","UE RF (36.101) [LTE_CA_R14_xDL2UL-Core]",48600,"noted","2017-05-05T02:26:07.497","2017-05-06T08:32:28.873","","","Rel-14","36.714-00-02","0.8.0","LTE_CA_R14_xDL2UL-Core","","","","","","","","",""]
["R4-1705191","Measurement uncertainty of the RTS system for harmonization test campaign","CATR","Ruixin Wang","64036","discussion","Discussion","","","146","7.11.3","Harmonization [LTE_MIMO_OTA-Core]",51910,"noted","2017-05-05T02:37:13.573","2017-05-06T16:30:58.800","","","Rel-14","","","LTE_MIMO_OTA-Core","","","","","","","","",""]
["R4-1705192","Measurement uncertainty of the MPAC system for harmonization test campaign","CATR","Ruixin Wang","64036","discussion","Discussion","","","146","7.11.3","Harmonization [LTE_MIMO_OTA-Core]",51920,"noted","2017-05-05T02:40:16.103","2017-05-06T16:30:58.817","","","Rel-14","","","LTE_MIMO_OTA-Core","","","","","","","","",""]
["R4-1705193","Revision of WID_LTE Advanced inter-band CA Rel-14 for 2DL1UL","Qualcomm Incorporated","Ville Vintola","44963","other","Endorsement","","","94","7.2.1","Rapporteur Input (WID/CRs) [LTE_CA_R14_2DL1UL-Core]",51940,"endorsed","2017-05-05T02:41:13.963","2017-05-23T15:07:51.350","","","Rel-14","","","LTE_CA_R14_2DL1UL","","","","","","","","",""]
["R4-1705194","TR 36.714-02-01_Rel14_2DL 1UL CA","Qualcomm Incorporated","Ville Vintola","44963","draft TR","Approval","","","94","7.2.1","Rapporteur Input (WID/CRs) [LTE_CA_R14_2DL1UL-Core]",51930,"approved","2017-05-05T02:41:13.980","2017-05-06T06:37:52.720","","","Rel-14","36.714-02-01","0.7.0","LTE_CA_R14_2DL1UL","","","","","","","","",""]
["R4-1705195","Introduction of completed R14 2DL band combinations to TS 36.101","Qualcomm Incorporated","Ville Vintola","44963","CR","Agreement","","","94","7.2.1","Rapporteur Input (WID/CRs) [LTE_CA_R14_2DL1UL-Core]",51960,"agreed","2017-05-05T02:41:17.160","2017-05-23T15:07:51.367","","","Rel-14","36.101","14.3.0","LTE_CA_R14_2DL1UL-Core","4443","","B","RP-171273","","","","",""]
["R4-1705196","Introduction of completed R14 2DL band combinations to TS 36.104","Qualcomm Incorporated","Ville Vintola","44963","CR","Agreement","","","94","7.2.1","Rapporteur Input (WID/CRs) [LTE_CA_R14_2DL1UL-Core]",51970,"agreed","2017-05-05T02:41:17.893","2017-05-23T15:07:51.367","","","Rel-14","36.104","14.3.0","LTE_CA_R14_2DL1UL-Core","4673","","B","RP-171273","","","","",""]
["R4-1705197","Introduction of completed combination to 36.141","Qualcomm Incorporated","Ville Vintola","44963","CR","Agreement","","","94","7.2.1","Rapporteur Input (WID/CRs) [LTE_CA_R14_2DL1UL-Core]",51980,"revised","2017-05-05T02:41:18.660","2017-05-23T15:07:51.383","","R4-1706106","Rel-14","36.141","14.3.0","LTE_CA_R14_2DL1UL","1035","","B","","","","","",""]
["R4-1705198","New WID: LTE Advanced inter-band CA Rel-15 for 2DL1UL","Qualcomm Incorporated","Ville Vintola","44963","other","Endorsement","","","94","7.2.1","Rapporteur Input (WID/CRs) [LTE_CA_R14_2DL1UL-Core]",51950,"revised","2017-05-05T02:41:19.407",null,"","R4-1705900","Rel-15","","","","","","","","","","","",""]
["R4-1705199","LS Reply on LS on transient period for NR","Qualcomm Incorporated","Ville Vintola","44963","LS out","Approval","LS Reply on Transient period for NR","","428","10.4.3.2","ON/OFF time mask [NR_newRAT]",577600,"noted","2017-05-05T02:41:19.423","2017-05-06T06:37:52.750","","","Rel-15","","","NR_newRAT-Core","","","","","","RAN1","","R1-1703782",""]
["R4-1705200","3.5 GHz Band arrangement","Qualcomm Incorporated","Ville Vintola","44963","other","Approval","","","415","10.2.1.2","Band definition for NR bands [NR_newRAT]",47750,"revised","2017-05-05T02:41:19.440","2017-05-06T06:37:52.750","","R4-1706052","Rel-15","","","NR_newRAT-Core","","","","","","","","",""]
["R4-1705201","Output power Requirement for mmW","Qualcomm Incorporated","Ville Vintola","44963","other","Approval","","","427","10.4.3.1","UE power class and MPR/A-MPR [NR_newRAT]",46860,"noted","2017-05-05T02:41:19.453","2017-05-06T06:37:52.750","","","Rel-15","","","NR_newRAT-Core","","","","","","","","",""]
["R4-1705202","Reference sensitivity requirements for mmW UE","Qualcomm Incorporated","Ville Vintola","44963","other","Approval","","","432","10.4.4.1","REFSENS and MSD evaluation assumption [NR_newRAT]",567200,"noted","2017-05-05T02:41:19.453","2017-05-06T06:37:52.767","","","Rel-15","","","NR_newRAT-Core","","","","","","","","",""]
["R4-1705203","Initial MPR considerations","Qualcomm Incorporated","Ville Vintola","44963","other","Approval","","","427","10.4.3.1","UE power class and MPR/A-MPR [NR_newRAT]",52220,"noted","2017-05-05T02:41:19.470","2017-05-06T06:37:52.767","","","Rel-15","","","NR_newRAT-Core","","","","","","","","",""]
["R4-1705204","Definitions for mmW blockers","Qualcomm Incorporated","Ville Vintola","44963","other","Approval","","","433","10.4.4.2","Blocking Requirements [NR_newRAT]",567800,"approved","2017-05-05T02:41:19.470","2017-05-06T06:37:52.767","","","Rel-15","","","NR_newRAT-Core","","","","","","","","",""]
["R4-1705205","mmW reference architecture","Qualcomm Incorporated","Ville Vintola","44963","other","Approval","","","425","10.4.2","Reference architecture [NR_newRAT]",52050,"noted","2017-05-05T02:41:19.487","2017-05-06T06:37:52.783","","","Rel-15","","","NR_newRAT-Core","","","","","","","","",""]
["R4-1705206","Non-contiguous allocations for NR","Qualcomm Incorporated","Ville Vintola","44963","other","Approval","","","427","10.4.3.1","UE power class and MPR/A-MPR [NR_newRAT]",52260,"noted","2017-05-05T02:41:19.533","2017-05-06T06:37:52.783","","","Rel-15","","","NR_newRAT-Core","","","","","","","","",""]
["R4-1705207","Way Forward on Spectrum Utilization","Qualcomm Incorporated","Ville Vintola","44963","other","Approval","","","420","10.3.3","Spectrum utilization [NR_newRAT]",46530,"noted","2017-05-05T02:41:19.547","2017-05-06T19:17:51.970","","","Rel-15","","","NR_newRAT-Core","","","","","","","","",""]
["R4-1705208","Feasible Spectral Utilization for NR.","Qualcomm Incorporated","Ville Vintola","44963","discussion","","","","420","10.3.3","Spectrum utilization [NR_newRAT]",49490,"noted","2017-05-05T02:41:19.563","2017-05-06T06:37:52.797","","","Rel-15","","","NR_newRAT-Core","","","","","","","","",""]
["R4-1705209","New WID: Lower Complexity Higher Order MIMO for LTE","Qualcomm Incorporated","Ville Vintola","44963","WID new","Information","","","473","13","Revision of the Work Plan",52100,"noted","2017-05-05T02:41:19.563","2017-05-06T06:37:52.797","","","Rel-15","","","","","","","","","","","",""]
["R4-1705210","Motivation for the New WID: Low complexity higher order MIMO","Qualcomm Incorporated","Ville Vintola","44963","discussion","Information","","","473","13","Revision of the Work Plan",52420,"noted","2017-05-05T02:41:19.580","2017-05-06T06:37:52.813","","","Rel-15","","","","","","","","","","","",""]
["R4-1705211","Measurement uncertainty of the RC+CE system for harmonization test campaign","CATR","Ruixin Wang","64036","discussion","Discussion","","","146","7.11.3","Harmonization [LTE_MIMO_OTA-Core]",52110,"noted","2017-05-05T02:42:21.150","2017-05-06T16:30:58.817","","","Rel-14","","","LTE_MIMO_OTA-Core","","","","","","","","",""]
["R4-1705212","Revised WID: LTE Advanced inter-band CA Rel-14 for 3DL/1UL","Huawei, HiSilicon","Huiping Shan","56652","WID revised","Endorsement","R14 3DL CA WID revision","","100","7.3.1","Rapporteur Input (WID/CRs) [LTE_CA_R14_3DL1UL-Core]",52130,"endorsed","2017-05-05T03:05:55.437","2017-05-23T15:07:51.383","","","Rel-14","","","LTE_CA_R14_3DL1UL-Core","","","","","","","","",""]
["R4-1705213","TR 36.714-03-01: 3DL/1UL inter-band CA R14 v0.8.0","Huawei, HiSilicon","Huiping Shan","56652","draft TR","Approval","3DL/1UL TR v0.8.0","","100","7.3.1","Rapporteur Input (WID/CRs) [LTE_CA_R14_3DL1UL-Core]",52120,"approved","2017-05-05T03:05:55.450","2017-05-05T10:53:07.040","","","Rel-14","36.714-03-01","0.8.0","LTE_CA_R14_3DL1UL-Core","","","","","","","","",""]
["R4-1705214","Introduction of completed R14 3DL band combinations to TS 36.101","Huawei, HiSilicon","Huiping Shan","56652","CR","Agreement","Big CR for 3DL/1UL","","100","7.3.1","Rapporteur Input (WID/CRs) [LTE_CA_R14_3DL1UL-Core]",0,"agreed","2017-05-05T03:05:58.523","2017-05-23T15:07:51.383","","","Rel-14","36.101","14.3.0","LTE_CA_R14_3DL1UL-Core","4444","","B","RP-171274","","","","",""]
["R4-1705215","Introduction of completed R14 3DL band combinations to TS 36.104","Huawei, HiSilicon","Huiping Shan","56652","CR","Agreement","Big CR for 3DL/1UL","","100","7.3.1","Rapporteur Input (WID/CRs) [LTE_CA_R14_3DL1UL-Core]",0,"agreed","2017-05-05T03:05:59.413","2017-05-23T15:07:51.397","","","Rel-14","36.104","14.3.0","LTE_CA_R14_3DL1UL-Core","4674","","B","RP-171274","","","","",""]
["R4-1705216","Introduction of completed R14 3DL band combinations to TS 36.141","Huawei, HiSilicon","Huiping Shan","56652","CR","Agreement","Big CR for 3DL/1UL","","100","7.3.1","Rapporteur Input (WID/CRs) [LTE_CA_R14_3DL1UL-Core]",0,"agreed","2017-05-05T03:06:00.270","2017-05-23T15:07:51.397","","","Rel-14","36.141","14.3.0","LTE_CA_R14_3DL1UL-Core","1036","","B","RP-171274","","","","",""]
["R4-1705217","New work item proposal: Introduction new band support for 4Rx antenna ports R15 for LTE","Huawei, HiSilicon","Huiping Shan","56652","WID new","Endorsement","R15 4Rx bands basket WID to include the new requests.","","135","7.9.1","Rapporteur Input [LTE_4Rx_AP_DL_bands]",52170,"endorsed","2017-05-05T03:06:01.083","2017-05-23T15:07:51.397","","","Rel-15","","","","","","","","","","","",""]
["R4-1705218","4Rx REFSENS requirements spec improvement for 36.101","Huawei, HiSilicon","Huiping Shan","56652","CR","Agreement","The CR is to improve 4Rx REFSENS spec according to the approved R4-1704020.","","30","5.2.1","UE RF core(36.101) [LTE_4Rx_AP_DL-Core]",52180,"revised","2017-05-05T03:06:01.097","2017-05-05T11:01:46.320","","R4-1705866","Rel-13","36.101","13.7.0","LTE_4Rx_AP_DL-Core","4445","","F","","","","","",""]
["R4-1705219","4Rx REFSENS requirements spec improvement for 36.101","Huawei, HiSilicon","Huiping Shan","56652","CR","Agreement","The CR is to improve 4Rx REFSENS spec according to the approved R4-1704020.","","30","5.2.1","UE RF core(36.101) [LTE_4Rx_AP_DL-Core]",52190,"revised","2017-05-05T03:06:01.940","2017-05-05T11:02:37.097","","R4-1706077","Rel-14","36.101","14.3.0","LTE_4Rx_AP_DL-Core","4446","","F","","","","","",""]
["R4-1705220","On 3.3-4.2 GHz band definition","Huawei, HiSilicon","Huiping Shan","56652","discussion","Discussion","This contribution provides the views on how to define 3.3-4.2 GHz band.","","415","10.2.1.2","Band definition for NR bands [NR_newRAT]",51050,"noted","2017-05-05T03:06:02.767","2017-05-05T11:02:37.080","","","Rel-15","","","NR_newRAT","","","","","","","","",""]
["R4-1705221","Discussion of 38.101 specification structure","Huawei, HiSilicon","Huiping Shan","56652","discussion","Discussion","This contribution provides some idea on how to arrange the 38.101 spec structure, mainly focus on RF spec.","","424","10.4.1","UE RF General (ad-hoc MoM, Plan, Spec Structure) [NR_newRAT]",615700,"noted","2017-05-05T03:06:02.767","2017-05-05T11:02:37.097","","","Rel-15","","","NR_newRAT","","","","","","","","",""]
["R4-1705222","Further discussion on mmWave power class definition","Huawei, HiSilicon","Huiping Shan","56652","other","Approval","This contribution proposes how to define the mmWave power class.","","427","10.4.3.1","UE power class and MPR/A-MPR [NR_newRAT]",51670,"noted","2017-05-05T03:06:02.783","2017-05-05T11:02:37.097","","","Rel-15","","","NR_newRAT","","","","","","","","",""]
["R4-1705223","Further discussion on mmWave EIRP/EIS requirement following CDF approach","Huawei, HiSilicon","Huiping Shan","56652","other","Approval","This contribution makes two proposals to move on the CDF test  approach.","","430","10.4.3.4","Other Tx requirements [NR_newRAT]",54770,"noted","2017-05-05T03:06:02.800","2017-05-05T11:02:37.097","","","Rel-15","","","NR_newRAT","","","","","","","","",""]
["R4-1705224","TR 36.755 V0.1.0: US 600 MHz Band for LTE","Samsung","Yankun Li","66748","draft TR","Approval","","","334","9.8","US 600 MHz Band for LTE [LTE600_US]",0,"approved","2017-05-05T03:15:29.117","2017-05-05T11:32:56.380","","","Rel-15","36.755","0.1.0","LTE600_US-Core","","","","","","","","",""]
["R4-1705225","3.5GHz band definition","Sumitomo Elec. Industries, Ltd","Li Yue","58006","other","Approval","This contribution presents our views on the three options and proposes that Option 1 should be adopted following the discussion.","","415","10.2.1.2","Band definition for NR bands [NR_newRAT]",52000,"noted","2017-05-05T03:54:48.960","2017-05-05T04:11:47.433","","","Rel-15","","","NR_newRAT","","","","","","","","",""]
["R4-1705226","mmWave UE power class definition","Sumitomo Elec. Industries, Ltd","Li Yue","58006","other","Approval","This contribution discusses the power class definition using TRP and EIRP.","","427","10.4.3.1","UE power class and MPR/A-MPR [NR_newRAT]",52010,"noted","2017-05-05T04:01:51.493","2017-05-05T04:11:47.433","","","Rel-15","","","NR_newRAT","","","","","","","","",""]
["R4-1705227","Further Consideration on E-UTRA TRP/TRS Requirements","Beijing Xiaomi Mobile Software","Jay Zhou","65347","other","","","","139","7.10.1","General [LTE_UTRA_TRP_TRS-Core]",578000,"noted","2017-05-05T05:55:31.473","2017-05-05T06:15:54.007","","","Rel-14","","","","","","","","","","","",""]
["R4-1705228","Discussion on measurement capability for NR","CMCC","jingjing chen","59689","discussion","Discussion","","","450","10.6.2","UE measurement capability [NR_newRAT]",51560,"noted","2017-05-05T06:04:53.580","2017-05-05T10:23:05.377","","","","","","","","","","","","","","",""]
["R4-1705229","Simulation results on PUSCH transmission in UpPTS","CMCC","jingjing chen","59689","discussion","Discussion","","","150","7.12.3","Demodulation (36.104/36.141) [LTE_UL_CAP_enh-Core/Perf]",572200,"noted","2017-05-05T06:04:53.610","2017-05-05T10:23:05.393","","","","","","","","","","","","","","",""]
["R4-1705230","Simulation results for MUST case3","CMCC","jingjing chen","59689","discussion","Discussion","","","256","7.24.1.2","Case 3 [LTE_MUST-Perf]",55330,"noted","2017-05-05T06:04:53.610","2017-05-05T10:23:05.393","","","","","","","","","","","","","","",""]
["R4-1705231","Considerations on OTA sensitivity","CMCC","jingjing chen","59689","discussion","Approval","","","363","9.12.2.6","Other Receiver requirements [AASenh_BS_LTE_UTRA-Core]",48760,"noted","2017-05-05T06:04:53.627","2017-05-06T04:47:53.080","","","","","","","","","","","","","","",""]
["R4-1705232","Considerations on OTA blocking","CMCC","jingjing chen","59689","discussion","Approval","","","363","9.12.2.6","Other Receiver requirements [AASenh_BS_LTE_UTRA-Core]",56420,"noted","2017-05-05T06:04:53.643","2017-05-06T04:47:53.097","","","","","","","","","","","","","","",""]
["R4-1705233","Discussion for OTA EIS Reference and minimum EIS","CMCC","jingjing chen","59689","discussion","Approval","","","363","9.12.2.6","Other Receiver requirements [AASenh_BS_LTE_UTRA-Core]",48770,"noted","2017-05-05T06:04:53.643","2017-05-06T04:47:53.110","","","","","","","","","","","","","","",""]
["R4-1705234","Further discussion of flexible grid setting for ACLR","CMCC","jingjing chen","59689","discussion","Discussion","","","367","9.12.3.2","Measurement Grid [AASenh_BS_LTE_UTRA-Perf]",52340,"noted","2017-05-05T06:04:53.657","2017-05-06T04:47:53.110","","","","","","","","","","","","","","",""]
["R4-1705235","Discussion on NR band definition for 3.3-4.2 GHz","CMCC","jingjing chen","59689","discussion","Approval","","","415","10.2.1.2","Band definition for NR bands [NR_newRAT]",46850,"noted","2017-05-05T06:04:53.657","2017-05-06T04:47:53.110","","","","","","","","","","","","","","",""]
["R4-1705236","Proposal on BS specific requirements for NR","CMCC","jingjing chen","59689","discussion","Approval","","","436","10.5.1","BS RF General (ad-hoc MoM, Plan, Spec structure) [NR_newRAT]",53050,"noted","2017-05-05T06:04:53.673","2017-05-06T04:47:53.110","","","","","","","","","","","","","","",""]
["R4-1705237","4Rx UE for 5G NR in 3.5GHz","CMCC","jingjing chen","59689","discussion","Approval","","","431","10.4.4","Receiver characteristics [NR_newRAT]",52370,"approved","2017-05-05T06:04:53.673","2017-05-06T04:47:53.110","","","","","","","","","","","","","","",""]
["R4-1705238","B71 REFSENS","Dish Network","Antti Immonen","70951","discussion","","This contribution includes our proposal for B71 REFSENS","","336","9.8.2","UE RF (36.101) [LTE600_US-core]",55070,"noted","2017-05-05T06:43:40.990","2017-05-05T12:21:40.400","","","","","","","","","","","","","","",""]
["R4-1705239","Discussion on spectrum utilization","SAMSUNG Electronics Co., Ltd.","Haijie Qiu","46265","discussion","Discussion","","","420","10.3.3","Spectrum utilization [NR_newRAT]",582900,"withdrawn","2017-05-05T06:50:52.227",null,"","","Rel-15","","","","","","","","","","","",""]
["R4-1705240","Discussion on spectrum utilization","SAMSUNG Electronics Co., Ltd.","Haijie Qiu","46265","discussion","Discussion","","","420","10.3.3","Spectrum utilization [NR_newRAT]",53420,"revised","2017-05-05T06:52:06.763","2017-05-05T17:57:52.863","","R4-1706059","Rel-15","","","","","","","","","","","",""]
["R4-1705241","TP for TR 36.714-02-01:  MSD for CA_66A-70A","Dish Network","Antti Immonen","70951","pCR","","This contribution provides a TP to capture MSD for CA_66A-70A","","95","7.2.2","UE RF (36.101) [LTE_CA_R14_2DL1UL-Core]",568000,"noted","2017-05-05T06:54:22.823","2017-05-05T07:17:24.800","","","Rel-14","36.714-02-01","0.7.0","LTE_CA_R14_2DL1UL-Core","","","","","","","","",""]
["R4-1705242","High power UE for LTE Band 40","Reliance Jio","Satish Nanjunda Swamy","61788","WID new","Discussion","In 3GPP, the study of high power UE (HPUE) operation, i.e. power class 2, for TDD Band 41 has been completed. The work item has also been completed, motivated by significant benefits in cell coverage and cell edge user throughput. TDD Band 40 has seen com","","473","13","Revision of the Work Plan",53820,"revised","2017-05-05T07:01:41.223","2017-05-05T11:02:15.490","","R4-1706066","Rel-15","","","","","","","","","","","",""]
["R4-1705243","Discussion on NR-SS periodicity","CMCC","jingjing chen","59689","discussion","Discussion","","","411","10.1.2","Topics related to incoming LS from other WG [NR_newRAT]",47000,"noted","2017-05-05T07:05:58.743","2017-05-05T10:33:07.243","","","","","","","","","","","","","","",""]
["R4-1705244","Considerations on 3.5GHz NR RF issues","CMCC","jingjing chen","59689","other","Approval","","","415","10.2.1.2","Band definition for NR bands [NR_newRAT]",45230,"noted","2017-05-05T07:05:58.757","2017-05-06T04:47:53.127","","","","","","","","","","","","","","",""]
["R4-1705245","MPR measurement for power class 2 contiguous 2CC UL CA","MediaTek Inc.","Huanren Fu","69911","discussion","Decision","","","332","9.7.1","UE RF (36.101) [LTE_CA_C_B41_PC2-core]",568100,"noted","2017-05-05T07:12:49.297","2017-05-05T07:27:53.437","","","","","","","","","","","","","","",""]
["R4-1705246","NR band considerations on 3.3-4.2GHz frequency range","ZTE Corporation","Zhifeng Ma","61569","discussion","","Three options for NR bands on frequency range 3.3-4.2GHz are suggested to be selected. In this proposal, we provide our views on NR band definition for frequency range 3.3-4.2GHz.","","415","10.2.1.2","Band definition for NR bands [NR_newRAT]",52200,"noted","2017-05-05T07:17:18.733","2017-05-06T07:57:51.877","","","","","","","","","","","","","","",""]
["R4-1705247","Discussion on UE maximum output power and UL bandwidth","CMCC","jingjing chen","59689","discussion","Discussion","","","427","10.4.3.1","UE power class and MPR/A-MPR [NR_newRAT]",55090,"noted","2017-05-05T07:24:16.027","2017-05-06T04:47:53.143","","","","","","","","","","","","","","",""]
["R4-1705248","NR band considerations on 24.25-29.5GHz frequency range","ZTE Corporation","Zhifeng Ma","61569","discussion","","Two options for NR bands on frequency range 24.25 - 29.5GHz are suggested to be selected in RAN4#83. In this proposal, we provide our views on NR band definition for frequency range 24.25 - 29.5GHz.","","415","10.2.1.2","Band definition for NR bands [NR_newRAT]",604900,"noted","2017-05-05T07:26:21.977","2017-05-06T07:57:51.893","","","","","","","","","","","","","","",""]
["R4-1705249","1024 QAM TX EVM range","Ericsson","Patrizia Testa","66129","discussion","Approval","This paper presents  a proposal about TX EVM range for 1024 QAM.","","405","9.17.1","General [LTE_HCS]",51890,"noted","2017-05-05T07:30:20.807","2017-05-05T09:01:13.563","","","Rel-15","","","","","","","","","","","",""]
["R4-1705250","TP for TR 36.714-02-01: Uplink configuration of REFSENS requirements for CA 3+32 and 7+32","TELECOM ITALIA S.p.A.","Paolo Goria","23040","pCR","Approval","This document contains two TPs that complete requirements for CA 3+32 and 7+32, introducing missing uplink configuration of REFSENS requirements.","","95","7.2.2","UE RF (36.101) [LTE_CA_R14_2DL1UL-Core]",569200,"approved","2017-05-05T07:37:02.923","2017-05-05T15:36:19.430","","","Rel-14","36.714-02-01","0.7.0","LTE_CA_R14_2DL1UL-Core","","","","","","","","",""]
["R4-1705251","TR 36.751 V0.1.0: FDD operating band in the L-band for LTE","NTT DOCOMO, INC.","Kei Ando","57164","draft TR","Approval","","","314","9.4","FDD operating band in the L-band for LTE [LTE_FDD_L_Band]",52510,"revised","2017-05-05T07:59:14.590","2017-05-06T13:47:52.297","","R4-1705923","Rel-15","36.751","0.1.0","LTE_FDD_L_Band-Core","","","","","","","","",""]
["R4-1705252","TP for TR 36.751: Updates on the FDD operation in L-band","NTT DOCOMO, INC.","Kei Ando","57164","pCR","Approval","","","316","9.4.2","UE RF (36.101) [LTE_FDD_L_Band-core]",52520,"revised","2017-05-05T07:59:18.380","2017-05-06T13:47:52.310","","R4-1705924","Rel-15","36.751","0.1.0","LTE_FDD_L_Band-Core","","","","","","","","",""]
["R4-1705253","Requirements associated with the FDD L-band (Band 74) for TS 36.101","NTT DOCOMO, INC.","Kei Ando","57164","discussion","Discussion","","","316","9.4.2","UE RF (36.101) [LTE_FDD_L_Band-core]",52530,"noted","2017-05-05T07:59:18.427","2017-05-06T13:47:52.327","","","Rel-15","","","LTE_FDD_L_Band-Core","","","","","","","","",""]
["R4-1705254","[Draft] Introduction of FDD L-band into TS 36.101","NTT DOCOMO, INC.","Kei Ando","57164","draftCR","Endorsement","","","316","9.4.2","UE RF (36.101) [LTE_FDD_L_Band-core]",52540,"revised","2017-05-05T07:59:18.443","2017-05-06T13:47:52.327","","R4-1705925","Rel-15","36.101","14.3.0","LTE_FDD_L_Band-Core","","","","","","","","",""]
["R4-1705255","[Draft] Introduction of FDD L-band into TS 25.101","NTT DOCOMO, INC.","Kei Ando","57164","draftCR","Endorsement","","","319","9.4.5","Other specifications [LTE_FDD_L_Band]",52550,"endorsed","2017-05-05T07:59:18.460","2017-05-06T13:47:52.343","","","Rel-15","25.101","14.0.0","LTE_FDD_L_Band-Core","","","","","","","","",""]
["R4-1705256","[Draft] Introduction of FDD L-band into TS 25.466","NTT DOCOMO, INC.","Kei Ando","57164","draftCR","Endorsement","","","319","9.4.5","Other specifications [LTE_FDD_L_Band]",52560,"noted","2017-05-05T07:59:18.460","2017-05-06T13:47:52.343","","","Rel-15","25.466","14.1.0","LTE_FDD_L_Band-Core","","","","","","","","",""]
["R4-1705257","[Draft] Introduction of FDD L-band into TS 25.461","NTT DOCOMO, INC.","Kei Ando","57164","draftCR","Endorsement","","","319","9.4.5","Other specifications [LTE_FDD_L_Band]",52570,"endorsed","2017-05-05T07:59:18.473","2017-05-06T13:47:52.357","","","Rel-15","25.461","14.1.0","LTE_FDD_L_Band-Core","","","","","","","","",""]
["R4-1705258","[Draft] Introduction of FDD L-band into TS 36.124","NTT DOCOMO, INC.","Kei Ando","57164","draftCR","Endorsement","","","319","9.4.5","Other specifications [LTE_FDD_L_Band]",52580,"endorsed","2017-05-05T07:59:18.473","2017-05-06T13:47:52.373","","","Rel-15","36.124","14.1.0","LTE_FDD_L_Band-Core","","","","","","","","",""]
["R4-1705259","A single band of 3.3-4.2 GHz","NTT DOCOMO, INC.","Kei Ando","57164","other","Approval","","","415","10.2.1.2","Band definition for NR bands [NR_newRAT]",47700,"noted","2017-05-05T07:59:18.490","2017-05-06T13:47:52.373","","","Rel-15","","","NR_newRAT","","","","","","","","",""]
["R4-1705260","On altimeter protection for 3.3-4.2 GHz and 4.4-4.99 GHz bands","NTT DOCOMO, INC.","Kei Ando","57164","other","Approval","","","415","10.2.1.2","Band definition for NR bands [NR_newRAT]",52440,"noted","2017-05-05T07:59:18.507","2017-05-06T13:47:52.373","","","Rel-15","","","NR_newRAT","","","","","","","","",""]
["R4-1705261","General spurious emission for NR UE","NTT DOCOMO, INC.","Kei Ando","57164","other","Approval","","","429","10.4.3.3","Spurious emission [NR_newRAT]",46650,"noted","2017-05-05T07:59:18.507","2017-05-06T13:47:52.390","","","Rel-15","","","NR_newRAT","","","","","","","","",""]
["R4-1705262","Forward compatibility for adding new NR channel bandwidth","NTT DOCOMO, INC.","Kei Ando","57164","other","Approval","","","418","10.3.1","Channel bandwidth and subcarrier spacing [NR_newRAT]",49560,"noted","2017-05-05T07:59:18.520","2017-05-06T13:47:52.390","","","Rel-15","","","NR_newRAT","","","","","","","","",""]
["R4-1705263","Further discussion on the channel raster for NR","ZTE Corporation","Wubin Zhou","43891","discussion","","In this paper, we provide some further considerations and discussions on channel raster for NR.","","419","10.3.2","Channel Raster [NR_newRAT]",569700,"withdrawn","2017-05-05T08:06:44.890",null,"","","","","","","","","","","","","","",""]
["R4-1705264","Further discussion on the channel raster for NR","ZTE Corporation","Wubin Zhou","43891","discussion","","In this paper, we provide some further considerations and discussions on channel raster for NR.","","419","10.3.2","Channel Raster [NR_newRAT]",582500,"withdrawn","2017-05-05T08:07:04.283",null,"","","","","","","","","","","","","","",""]
["R4-1705265","Further discussion on the channel raster for NR","ZTE Corporation","Wubin Zhou","43891","discussion","","In this paper, we provide some further considerations and discussions on channel raster for NR.","","419","10.3.2","Channel Raster [NR_newRAT]",605600,"withdrawn","2017-05-05T08:07:23.967",null,"","","","","","","","","","","","","","",""]
["R4-1705266","Further discussion on the channel raster for NR","ZTE Corporation","Wubin Zhou","43891","discussion","Discussion","In this paper, we provide some further considerations and discussions on channel raster for NR.","","419","10.3.2","Channel Raster [NR_newRAT]",51590,"noted","2017-05-05T08:09:18.470","2017-05-06T09:27:52.507","","","","","","","","","","","","","","",""]
["R4-1705267","Consideration on transmitter intermodulation for below 6GHz NR","ZTE Corporation","Wubin Zhou","43891","other","Approval","In this paper, we provide some preliminary discussion on the conduct transmitter intermodulation requirement for NR BS, i.e. Range 1-C-N and Range 1-C-A.","","442","10.5.3.4","Other Tx requirements [NR_newRAT]",53740,"noted","2017-05-05T08:12:40.127","2017-05-06T09:27:52.523","","","","","","","","","","","","","","",""]
["R4-1705268","The boundary between out-of-band and spurious domain below 6 GHz NR BS","ZTE Corporation","Wubin Zhou","43891","other","Approval","Based on the above, this contribution give some considerations on the boundary between out-of-band and spurious domain below 6 GHz NR BS.","","440","10.5.3.2","Unwanted emission requirements [NR_newRAT]",52890,"noted","2017-05-05T08:14:24.367","2017-05-06T09:27:52.537","","","","","","","","","","","","","","",""]
["R4-1705269","TP for TR 36.714-00-00: operating bands, channel bandwidths REFSENS requirements and other receiver RF requirements for CA_1C_BCS1","China Unicom","Rongyi Hu","70322","pCR","","","","89","7.1.2","UE RF (36.101) [LTE_CA_R14_intra-Core]",53810,"approved","2017-05-05T08:14:54.457","2017-05-06T06:17:52.330","","","Rel-14","36.714-00-00","0.6.0","LTE_CA_R14_intra-Core","","","","","","","","",""]
["R4-1705270","TP to TR 36.790 on BS specific aspects","Ericsson, AT&T","Patrizia Testa","66129","other","Approval","This document is a text proposal to TR 36.790 on BS specific aspects.","","353","9.11.3","BS RF (Downlink only in 3.5GHz) (36.104/36.141) [LTE_ 3550_CBRS_US_LAA]",52700,"revised","2017-05-05T08:24:52.423","2017-05-05T09:14:45.607","","R4-1705889","Rel-15","","","LTE_3550_CBRS_US_LAA","","","","","","","","",""]
["R4-1705271","CR to 36.104: Introduction of Band 49 (3.5 GHz LAA in US)","Ericsson, AT&T","Patrizia Testa","66129","CR","Approval","This CR introduces B49 in the specification","","353","9.11.3","BS RF (Downlink only in 3.5GHz) (36.104/36.141) [LTE_ 3550_CBRS_US_LAA]",52710,"revised","2017-05-05T08:24:52.440","2017-05-05T09:32:55.177","","R4-1705890","Rel-15","36.104","14.3.0","LTE_3550_CBRS_US_LAA","4675","","B","","","","","",""]
["R4-1705272","CR to 36.113: Introduction of Band 49 (3.5 GHz LAA in US)","Ericsson, AT&T","Patrizia Testa","66129","CR","Approval","This CR introduces B49 in the specification","","354","9.11.4","Other specifications [LTE_ 3550_CBRS_US_LAA]",52730,"endorsed","2017-05-05T08:24:53.237","2017-05-05T09:32:55.177","","","Rel-15","36.113","14.2.0","LTE_3550_CBRS_US_LAA","0065","","B","","","","","",""]
["R4-1705273","CR to 36.124: Introduction of Band 49 (3.5 GHz LAA in US)","Ericsson, AT&T","Patrizia Testa","66129","CR","Approval","This CR introduces B49 in the specification","","354","9.11.4","Other specifications [LTE_ 3550_CBRS_US_LAA]",52740,"revised","2017-05-05T08:24:54.030","2017-05-05T09:32:55.177","","R4-1705892","Rel-15","36.124","14.1.0","LTE_3550_CBRS_US_LAA","0037","","B","","","","","",""]
["R4-1705274","CR to 37.104: Introduction of Band 49 (3.5 GHz LAA in US)","Ericsson, AT&T","Patrizia Testa","66129","CR","Approval","This CR introduces B49 in the specification","","354","9.11.4","Other specifications [LTE_ 3550_CBRS_US_LAA]",52750,"revised","2017-05-05T08:24:54.873","2017-05-06T11:57:51.873","","R4-1705893","Rel-15","37.104","14.3.0","LTE_3550_CBRS_US_LAA","0781","","B","","","","","",""]
["R4-1705275","CR to 37.113: Introduction of Band 49 (3.5 GHz LAA in US)","Ericsson, AT&T","Patrizia Testa","66129","CR","Approval","This CR introduces B49 in the specification","","354","9.11.4","Other specifications [LTE_ 3550_CBRS_US_LAA]",52760,"endorsed","2017-05-05T08:24:55.607","2017-05-06T11:57:51.873","","","Rel-15","37.113","14.1.0","LTE_3550_CBRS_US_LAA","0069","","B","","","","","",""]
["R4-1705276","CR to 25.104: Introduction of Band 49 (3.5 GHz LAA in US)","Ericsson, AT&T","Patrizia Testa","66129","CR","Approval","This CR introduces B49 in the specification","","354","9.11.4","Other specifications [LTE_ 3550_CBRS_US_LAA]",52770,"revised","2017-05-05T08:24:56.497","2017-05-06T11:57:51.873","","R4-1705894","Rel-15","25.104","14.1.0","LTE_3550_CBRS_US_LAA","0950","","B","","","","","",""]
["R4-1705277","CR to 25.461: Introduction of Band 49 (3.5 GHz LAA in US)","Ericsson, AT&T","Patrizia Testa","66129","draftCR","Endorsement","This CR introduces B49 in the specification","","354","9.11.4","Other specifications [LTE_ 3550_CBRS_US_LAA]",52780,"revised","2017-05-05T08:24:57.277","2017-05-06T11:57:51.890","","R4-1705895","Rel-15","25.461","14.1.0","LTE_3550_CBRS_US_LAA","","","B","","","","","",""]
["R4-1705278","CR to 37.141: Introduction of Band 49 (3.5 GHz LAA in US)","Ericsson, AT&T","Patrizia Testa","66129","CR","Approval","This CR introduces B49 in the specification","","354","9.11.4","Other specifications [LTE_ 3550_CBRS_US_LAA]",52800,"revised","2017-05-05T08:24:57.307","2017-05-06T11:57:51.890","","R4-1705896","Rel-15","37.141","14.3.0","LTE_3550_CBRS_US_LAA","0779","","B","","","","","",""]
["R4-1705279","CR to 36.141: Introduction of Band 49 (3.5 GHz LAA in US)","Ericsson, AT&T","Patrizia Testa","66129","CR","Approval","This CR introduces B49 in the specification","","353","9.11.3","BS RF (Downlink only in 3.5GHz) (36.104/36.141) [LTE_ 3550_CBRS_US_LAA]",52790,"revised","2017-05-05T08:24:58.087","2017-05-06T11:57:51.890","","R4-1705891","Rel-15","36.141","14.3.0","LTE_3550_CBRS_US_LAA","1037","","B","","","","","",""]
["R4-1705280","CR to 25.141: Introduction of Band 49 (3.5 GHz LAA in US)","Ericsson, AT&T","Patrizia Testa","66129","CR","Approval","This CR introduces B49 in the specification","","354","9.11.4","Other specifications [LTE_ 3550_CBRS_US_LAA]",53350,"revised","2017-05-05T08:24:58.850","2017-05-06T11:57:51.890","","R4-1705897","Rel-15","25.141","14.1.0","LTE_3550_CBRS_US_LAA","0980","","B","","","","","",""]
["R4-1705281","On spectrum utilization","Huawei, HiSilicon","Xiang (Steven) Chen","41576","other","Approval","This contribution is for approval.","","420","10.3.3","Spectrum utilization [NR_newRAT]",45750,"noted","2017-05-05T08:28:16.873","2017-05-06T19:17:52","","","","","","NR_newRAT","","","","","","","","",""]
["R4-1705282","EVM requirement for single numerology","Huawei, HiSilicon","Xiang (Steven) Chen","41576","other","Approval","This contribution provides the proposed EVM requirement for single numerology.","","421","10.3.4","In-band requirements [NR_newRAT]",52830,"noted","2017-05-05T08:28:16.873","2017-05-05T12:52:53.747","","","","","","NR_newRAT","","","","","","","","",""]
["R4-1705283","BS in-band requirements","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","Discussion","","","421","10.3.4","In-band requirements [NR_newRAT]",52840,"noted","2017-05-05T08:28:16.890","2017-05-05T12:52:53.747","","","","","","NR_newRAT","","","","","","","","",""]
["R4-1705284","UE in-band requirements","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","Discussion","","","421","10.3.4","In-band requirements [NR_newRAT]",53430,"noted","2017-05-05T08:28:16.890","2017-05-05T12:52:53.747","","","","","","NR_newRAT","","","","","","","","",""]
["R4-1705285","BS spectrum emission mask for below 6GHz","Huawei, HiSilicon","Xiang (Steven) Chen","41576","other","Approval","This contribution is for approval.","","440","10.5.3.2","Unwanted emission requirements [NR_newRAT]",56640,"noted","2017-05-05T08:28:16.907","2017-05-05T16:40:01.220","","","","","","NR_newRAT","","","","","","","","",""]
["R4-1705286","BS ACLR for below 6GHz","Huawei, HiSilicon","Xiang (Steven) Chen","41576","other","Approval","This contribution is for approval.","","440","10.5.3.2","Unwanted emission requirements [NR_newRAT]",56660,"noted","2017-05-05T08:28:16.907","2017-05-05T16:40:01.220","","","","","","NR_newRAT","","","","","","","","",""]
["R4-1705287","On channel bandwidth set","Huawei, HiSilicon","Xiang (Steven) Chen","41576","other","Approval","This contribution is for approval.","","418","10.3.1","Channel bandwidth and subcarrier spacing [NR_newRAT]",52990,"noted","2017-05-05T08:28:16.920","2017-05-05T16:40:01.220","","","","","","NR_newRAT","","","","","","","","",""]
["R4-1705288","BS ACLR for mmWave bands","Huawei, HiSilicon","Xiang (Steven) Chen","41576","other","Approval","This contribution is for approval.","","440","10.5.3.2","Unwanted emission requirements [NR_newRAT]",52680,"noted","2017-05-05T08:28:16.937","2017-05-05T16:40:01.220","","","","","","NR_newRAT","","","","","","","","",""]
["R4-1705289","BS ACS for mmWave bands","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","Discussion","","","440","10.5.3.2","Unwanted emission requirements [NR_newRAT]",52850,"withdrawn","2017-05-05T08:28:16.953",null,"","","","","","NR_newRAT","","","","","","","","",""]
["R4-1705290","BS receiver dynamic range for mmWave bands","Huawei, HiSilicon","Xiang (Steven) Chen","41576","other","Approval","This contribution is for approval.","","444","10.5.4.1","Dynamic Range [NR_newRAT]",52900,"noted","2017-05-05T08:28:16.967","2017-05-05T11:41:46.390","","","","","","NR_newRAT","","","","","","","","",""]
["R4-1705291","BS in-band blocking requirement for mmWave bands","Huawei, HiSilicon","Xiang (Steven) Chen","41576","other","Approval","This contribution is for approval.","","445","10.5.4.2","Blocking Requirements [NR_newRAT]",53260,"noted","2017-05-05T08:28:17","2017-05-05T11:41:46.390","","","","","","NR_newRAT","","","","","","","","",""]
["R4-1705292","On synchronization signal raster and subcarrier spacing","Huawei, HiSilicon","Xiang (Steven) Chen","41576","other","Approval","This contribution is for approval.","","419","10.3.2","Channel Raster [NR_newRAT]",45680,"noted","2017-05-05T08:28:17.013","2017-05-05T11:12:35.623","","","","","","NR_newRAT","","","","","","","","",""]
["R4-1705293","Some discussions on SCS grid","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","Discussion","","","411","10.1.2","Topics related to incoming LS from other WG [NR_newRAT]",577400,"noted","2017-05-05T08:28:17.030","2017-05-05T11:12:35.623","","","","","","NR_newRAT","","","","","","","","",""]
["R4-1705294","On NR band numbering","Huawei, HiSilicon","Xiang (Steven) Chen","41576","other","Approval","This contribution is for approval.","","413","10.2.1","NR frequency range and bands [NR_newRAT]",46130,"noted","2017-05-05T08:28:17.047","2017-05-05T11:12:35.623","","","","","","NR_newRAT","","","","","","","","",""]
["R4-1705295","TS skeleton for 38.141 v0.0.1","Huawei, HiSilicon","Xiang (Steven) Chen","41576","draft TS","Approval","","","436","10.5.1","BS RF General (ad-hoc MoM, Plan, Spec structure) [NR_newRAT]",52950,"noted","2017-05-05T08:28:17.060","2017-05-06T19:17:52.017","","","Rel-15","38.141","0.0.1","NR_newRAT","","","","","","","","",""]
["R4-1705296","TR skeleton for LTE V2X phase 2","Huawei, HiSilicon","Xiang (Steven) Chen","41576","other","Approval","This Tdoc is actually a draft TR 36.7XX for WI LTE_eV2X-Core, TR number pending","","399","9.16.1","General [LTE_eV2X]",51830,"revised","2017-05-05T08:28:18.480","2017-05-05T11:12:35.623","","R4-1705877","","","","LTE_eV2X-Core","","","","","","","","",""]
["R4-1705297","TP for TR 36.714-03-01: Uplink configuration of REFSENS requirements for CA 3+20+32 and CA 3+7+32","TELECOM ITALIA S.p.A.","Paolo Goria","23040","pCR","Approval","This document contains two TPs that complete requirements for CA 3+20+32 and 3+7+32, introducing missing uplink configuration of REFSENS requirements.","","101","7.3.2","UE RF (36.101) [LTE_CA_R14_3DL1UL-Core]",53110,"approved","2017-05-05T08:32:49.713","2017-05-05T15:36:19.430","","","Rel-14","36.714-03-01","0.8.0","LTE_CA_R14_3DL1UL-Core","","","","","","","","",""]
["R4-1705298","TS 38.104 v0.0.1 NR Base Station (BS) radio transmission and reception (Skeleton)","Ericsson","Johan Skold","10425","draft TS","Approval","Proposed skeleton for the NR BS RF specification.","","436","10.5.1","BS RF General (ad-hoc MoM, Plan, Spec structure) [NR_newRAT]",48580,"withdrawn","2017-05-05T08:46:21.667",null,"R4-1704619","","Rel-15","38.104","0.0.1","NR_newRAT","","","","","","","","",""]
["R4-1705299","channel bandwidth for NR","ZTE Corporation","Shengxiang Guo","72253","other","","For approval.in this contribution, we would like to share our view on how to define channel bandwidth for NR.","","418","10.3.1","Channel bandwidth and subcarrier spacing [NR_newRAT]",55890,"noted","2017-05-05T09:01:41.610","2017-05-06T07:57:51.957","","","","","","","","","","","","","","",""]
["R4-1705300","Practical Simulation Results for new PRACH","Ericsson","Magnus Larsson","43293","discussion","Discussion","Results with implementation margin and updated ideal results for cases not reported in previous meeting.","","266","7.25.5","BS demodulation (36.104/36.141) [LTE_high_speed-Perf]",55370,"noted","2017-05-05T09:02:12.530","2017-05-05T13:31:51.167","","","Rel-14","","","LTE_high_speed-Perf","","","","","","","","",""]
["R4-1705301","Practical results for BS performance requirements for 256QAM","Ericsson","Magnus Larsson","43293","discussion","Discussion","Results with implementation margin","","150","7.12.3","Demodulation (36.104/36.141) [LTE_UL_CAP_enh-Core/Perf]",53020,"noted","2017-05-05T09:02:12.577","2017-05-05T13:37:52.737","","","Rel-14","","","LTE_UL_CAP_enh-Perf","","","","","","","","",""]
["R4-1705302","FRC for 256 QAM","Ericsson","Magnus Larsson","43293","discussion","Discussion","New FRC for 256QAM, explanation of design.","","150","7.12.3","Demodulation (36.104/36.141) [LTE_UL_CAP_enh-Core/Perf]",572300,"noted","2017-05-05T09:02:12.607","2017-05-05T17:57:52.957","","","Rel-14","","","LTE_UL_CAP_enh-Perf","","","","","","","","",""]
["R4-1705303","Introduction of BS performance requirements for 256QAM in 36.104","Ericsson","Magnus Larsson","43293","CR","Approval","CR for 36.104","","150","7.12.3","Demodulation (36.104/36.141) [LTE_UL_CAP_enh-Core/Perf]",595900,"revised","2017-05-05T09:02:12.623","2017-05-05T17:57:52.957","","R4-1706186","Rel-14","36.104","14.3.0","LTE_UL_CAP_enh-Perf","4676","","B","","","","","",""]
["R4-1705304","Introduction of BS performance requirements for 256QAM in 36.141","Ericsson","Magnus Larsson","43293","CR","Approval","CR for 36.141","","150","7.12.3","Demodulation (36.104/36.141) [LTE_UL_CAP_enh-Core/Perf]",600600,"revised","2017-05-05T09:02:13.480","2017-05-05T17:57:52.957","","R4-1706187","Rel-14","36.141","14.3.0","LTE_UL_CAP_enh-Perf","1038","","B","","","","","",""]
["R4-1705305","TDD switching considering multiple steps and levels","Ericsson","Magnus Larsson","43293","discussion","Discussion","Introduction of two times and two power levels in TDD ON OFF requirement.","","442","10.5.3.4","Other Tx requirements [NR_newRAT]",54680,"noted","2017-05-05T09:02:14.230","2017-05-05T17:57:52.957","","","Rel-15","","","NR_newRAT","","","","","","","","",""]
["R4-1705306","Consideration of requirements for NR UE timing advance","Ericsson","Magnus Larsson","43293","discussion","Discussion","Consideration of requirements for NR UE timing advance","","451","10.6.3","UE transmit timing [NR_newRAT]",53220,"noted","2017-05-05T09:02:14.247","2017-05-05T17:57:52.970","","","Rel-15","","","NR_newRAT","","","","","","","","",""]
["R4-1705307","Finalization of CA 4DL_3A_7A_20A_32A_1UL and next steps","TELECOM ITALIA S.p.A.","Paolo Goria","23040","other","Discussion","This document address finalization of CA 3+7+20+32 with 1UL and discusses next evolutionary steps towards 2UL.","","125","7.7.2","UE RF (36.101) [LTE_CA_R14_xDL2UL-Core]",55120,"noted","2017-05-05T09:06:17.070","2017-05-05T15:36:19.430","","","","","","","","","","","","","","",""]
["R4-1705308","NR UE Tx spurious emissions","ZTE Corporation","Shengxiang Guo","72253","other","","The spurious limits -30 dBm/MHz and out of band boundary for less than 20 MHz for NR Range1 have been agreed, the remained open issues are out of band boundary for more than 20 MHz channel bandwidth NR Range1 and spurious emission limits and out of band b","","429","10.4.3.3","Spurious emission [NR_newRAT]",53080,"approved","2017-05-05T09:12:33.430","2017-05-06T07:57:51.973","","","","","","","","","","","","","","",""]
["R4-1705309","Framework parameters for multi-band support","TELECOM ITALIA S.p.A.","Paolo Goria","23040","other","Approval","This contribution present same analysis submitted in RAN4#82bis, and exploits it in order to define parameters for framework applicability in case of multi-band support on the basis of approved way-forward   at last meeting.","","140","7.10.2","Hand phantom for smartphones [LTE_UTRA_TRP_TRS-Core]",609600,"noted","2017-05-05T09:16:12.417","2017-05-05T15:36:19.430","","","","","","","","","","","","","","",""]
["R4-1705310","LAA CA_2A-49A reference sensitivity","MediaTek Inc.","James Wang","56966","other","Approval","In this contribution, CA_2A-49A REFSENS exception due to B2 UL harmonic interference is defined.","","352","9.11.2","UE RF (Downlink only in 3.5GHz) (36.101) [LTE_ 3550_CBRS_US_LAA]",50980,"noted","2017-05-05T09:28:55.747","2017-05-06T16:57:51.867","","","Rel-15","36.101","","","","","","","","","","",""]
["R4-1705311","TP for TR36.714-03-01: delta Tib and delta Rib for CA_39A-40C_BCS0","ZTE Corporation","Wubin Zhou","43891","pCR","","This contribution provides a text proposal on delta Tib/Rib for CA_3DL_39A-40C_1UL_BCS0 for TR36.714-03-01","","101","7.3.2","UE RF (36.101) [LTE_CA_R14_3DL1UL-Core]",53120,"approved","2017-05-05T09:30:46.960","2017-05-06T09:27:52.583","","","Rel-14","36.714-03-01","0.8.0","LTE_CA_R14_3DL1UL-Core","","","","","","","","",""]
["R4-1705312","TP for TR36.714-03-01: delta Tib and delta Rib for CA_39C-40A_BCS0","ZTE Corporation","Wubin Zhou","43891","pCR","","This contribution provides a text proposal on delta Tib/Rib for CA_3DL_39C-40A_1UL_BCS0 for TR36.714-03-01","","101","7.3.2","UE RF (36.101) [LTE_CA_R14_3DL1UL-Core]",53250,"approved","2017-05-05T09:32:54.927","2017-05-06T09:27:52.583","","","Rel-14","36.714-03-01","0.8.0","LTE_CA_R14_3DL1UL-Core","","","","","","","","",""]
["R4-1705313","Measurement results of PAD devices for lab alignment","CATR","Ruixin Wang","64036","other","Discussion","","","145","7.11.2","Performance requirements [LTE_MIMO_OTA-Core]",582800,"noted","2017-05-05T09:43:04.047","2017-06-06T13:47:53.747","","","Rel-14","","","LTE_MIMO_OTA-Core","","","","","","","","",""]
["R4-1705314","TP to TR 37.843: BS classification for eAAS BS","NEC","Tetsu Ikeda","58067","pCR","Approval","We provide a text proposal on BS classification for eAAS BS based on the agreement in RAN4#82bis..","","356","9.12.1","General [AASenh_BS_LTE_UTRA]",53140,"revised","2017-05-05T09:43:07.370","2017-05-05T13:13:06.587","","R4-1706125","Rel-15","37.843","0.2.0","AASenh_BS_LTE_UTRA","","","","","","","","",""]
["R4-1705315","Operating band unwanted emission for eAAS","NEC","Tetsu Ikeda","58067","pCR","Approval","We provide a text proposal to correct the text approved in RAN4#82bis.","","362","9.12.2.5","Other Transmitter Requirements [AASenh_BS_LTE_UTRA-Core]",580200,"approved","2017-05-05T09:43:08.230","2017-05-05T13:13:06.587","","","Rel-15","37.843","0.2.0","AASenh_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-1705316","OTA output power requirements for eAAS","NEC","Tetsu Ikeda","58067","other","Approval","Proposal 1: Maximum output power condition for conformance testing shall be demonstrated by maximum TRP power.\nProposal 2: Maximum TRP output power shall be declared per system.\nProposal 3: Maximum EIRP output power shall be declared per beam.\nProposal 4:","","358","9.12.2.1","TRP accuracy [AASenh_BS_LTE_UTRA-Core]",53160,"noted","2017-05-05T09:43:08.493","2017-05-05T13:13:06.587","","","Rel-15","","","AASenh_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-1705317","TP to TR 37.843: OTA sensitivity requirements for eAAS","NEC","Tetsu Ikeda","58067","pCR","Approval","We further discuss the agreements in the WF approved in RAN4#82bis and make a text proposal based on it","","363","9.12.2.6","Other Receiver requirements [AASenh_BS_LTE_UTRA-Core]",49441,"revised","2017-05-05T09:43:08.587","2017-05-05T13:13:06.603","","R4-1706141","Rel-15","37.843","0.2.0","AASenh_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-1705318","TP to TS 38.104 BS classification for NR BS","NEC","Tetsu Ikeda","58067","pCR","Approval","We provide a text proposal on BS classification for NR BS based on the agreement in RAN4#82.","","437","10.5.2","BS class [NR_newRAT]",53180,"revised","2017-05-05T09:43:09.383","2017-05-05T13:13:06.603","","R4-1706161","Rel-15","38.104","0.0.1","NR_newRAT","","","","","","","","",""]
["R4-1705319","TX and RX loss factor for eAAS","NEC","Tetsu Ikeda","58067","other","Approval","Proposal 1: The transmitter loss factor for transmitter in-band region shall be 0 dB\nProposal 2: The alignment between receiver loss factor and transmitter loss factor for OTA in-band region is not needed","","359","9.12.2.2","Tx and Rx loss values [AASenh_BS_LTE_UTRA-Core]",53190,"noted","2017-05-05T09:43:09.540","2017-05-05T13:13:06.603","","","Rel-15","","","AASenh_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-1705320","Handover Requirement Enhancement in FeMTC","Ericsson","Muhammad Kazmi","31117","discussion","Discussion","This paper analyzes enhancement of handover requirements in FeMTC","","214","7.18.3.2.2","Idle mode and handover [LTE_feMTC-Core]",53200,"noted","2017-05-05T09:43:09.663","2017-05-05T12:02:38.723","","","Rel-14","","","LTE_feMTC-Core","","","","","","","","",""]
["R4-1705321","Enhanced Handover Requirement for FeMTC","Ericsson","Muhammad Kazmi","31117","CR","Approval","This paper specfies enhanced handover requirements for FeMTC for the cases: when the UE does not require SFN of target cell and when the UE needs to acquire SFN of the target cell","","214","7.18.3.2.2","Idle mode and handover [LTE_feMTC-Core]",53210,"revised","2017-05-05T09:43:11.240","2017-05-05T12:02:38.723","","R4-1705982","Rel-14","36.133","14.3.0","LTE_feMTC-Core","4972","","B","","","","","",""]
["R4-1705322","Analysis of UE Initial Transmit Timing Requirement","Ericsson","Muhammad Kazmi","31117","other","Discussion","This paper analyzes UE initial transmit timing accuracy for NR","","451","10.6.3","UE transmit timing [NR_newRAT]",53060,"noted","2017-05-05T09:43:12.380","2017-05-05T12:02:38.723","","","Rel-15","","","NR_newRAT","","","","","","","","",""]
["R4-1705323","Signal Quality Measurement for Mobility in NR","Ericsson","Muhammad Kazmi","31117","other","Discussion","This paper analyzes the need for signal quality measurement in NR","","454","10.6.6","Measurement definition and reference point [NR_newRAT]",578500,"noted","2017-05-05T09:43:12.397","2017-05-05T12:02:38.723","","","Rel-15","","","NR_newRAT","","","","","","","","",""]
["R4-1705324","TP for TR36.714-04-01: delta Tib and delta Rib for CA_39A-40D_BCS0","ZTE Corporation","Wubin Zhou","43891","pCR","","This contribution provides a text proposal on delta Tib/Rib for CA_3DL_39A-40D_1UL_BCS0 for TR36.714-04-01","","107","7.4.2","UE RF (36.101) [LTE_CA_R14_4DL1UL-Core]",53300,"withdrawn","2017-05-05T10:01:54.060",null,"","","Rel-14","36.714-04-01","0.7.0","LTE_CA_R14_4DL1UL-Core","","","","","","","","",""]
["R4-1705325","TP for TR36.714-03-01: delta Tib/Rib values for CA_39A-42C_BCS0","ZTE Corporation","Shengxiang Guo","72253","pCR","","This contribution provide a text proposal on delta Tib/Rib values for CA_3DL_39A-42C_1UL_BCS0 for TR36.714-03-01","","101","7.3.2","UE RF (36.101) [LTE_CA_R14_3DL1UL-Core]",54640,"approved","2017-05-05T10:02:00.080","2017-05-06T07:57:51.973","","","Rel-14","36.714-03-01","0.8.0","LTE_CA_R14_3DL1UL-Core","","","","","","","","",""]
["R4-1705326","Discussion on blocking requirement of mmWave NR BS in dense urban scenario","ZTE Corporation","Fei Xue","59676","discussion","","","","445","10.5.4.2","Blocking Requirements [NR_newRAT]",53270,"noted","2017-05-05T10:02:14.713","2017-05-06T09:27:52.600","","","Rel-14","","","","","","","","","","","",""]
["R4-1705327","Discussion on blocking requirement of mmWave NR BS in dense urban scenario","ZTE Corporation","Fei Xue","59676","discussion","","","","445","10.5.4.2","Blocking Requirements [NR_newRAT]",53360,"withdrawn","2017-05-05T10:03:05.553",null,"","","Rel-14","","","","","","","","","","","",""]
["R4-1705328","TP for TR36.714-04-01: delta Tib and delta Rib for CA_39A-40D_BCS0","ZTE Corporation","Wubin Zhou","43891","pCR","","This contribution provides a text proposal on delta Tib/Rib for CA_3DL_39A-40D_1UL_BCS0 for TR36.714-04-01","","107","7.4.2","UE RF (36.101) [LTE_CA_R14_4DL1UL-Core]",53750,"withdrawn","2017-05-05T10:03:06.303",null,"","","Rel-14","36.714-04-01","0.7.0","LTE_CA_R14_4DL1UL-Core","","","","","","","","",""]
["R4-1705329","TP for TR36.714-04-01: delta Tib/Rib values for CA_39A-42D_BCS0","ZTE Corporation","Shengxiang Guo","72253","pCR","","This contribution provide a text proposal on delta Tib/Rib values for CA_4DL_39A-42D_1UL_BCS0 for TR36.714-04-01.","","107","7.4.2","UE RF (36.101) [LTE_CA_R14_4DL1UL-Core]",576900,"approved","2017-05-05T10:21:51.227","2017-05-06T07:57:51.987","","","Rel-14","36.714-04-01","0.7.0","LTE_CA_R14_4DL1UL-Core","","","","","","","","",""]
["R4-1705330","TP for TR36.714-04-01: delta Tib/Rib values for CA_39A-42D_BCS0","ZTE Corporation","Shengxiang Guo","72253","pCR","","This contribution provide a text proposal on delta Tib/Rib values for CA_4DL_39A-42D_1UL_BCS0 for TR36.714-04-01.","","107","7.4.2","UE RF (36.101) [LTE_CA_R14_4DL1UL-Core]",577100,"withdrawn","2017-05-05T10:22:47.327",null,"","","Rel-14","36.714-04-01","0.7.0","LTE_CA_R14_4DL1UL-Core","","","","","","","","",""]
["R4-1705331","CR for PHR maping for NB-IoT R13","Huawei, HiSilicon","Qiming Li","61879","CR","Agreement","","","195","7.17.3.2.3","PHR [NB_IOTenh-Core]",53310,"revised","2017-05-05T10:23:05.517","2017-05-06T13:47:52.437","R4-1703621","R4-1706040","Rel-13","36.133","13.7.0","NB_IOTenh-Core","4765","2","F","","","","","",""]
["R4-1705332","TS 38.104 v0.0.2 NR Base Station (BS) radio transmission and reception (Skeleton)","Ericsson","Johan Skold","10425","draft TS","Approval","Proposed skeleton for the NR BS RF specification.","","436","10.5.1","BS RF General (ad-hoc MoM, Plan, Spec structure) [NR_newRAT]",0,"revised","2017-05-05T10:41:24.260","2017-05-05T19:35:25.630","R4-1704619","R4-1706228","Rel-15","38.104","0.0.2","NR_newRAT","","","","","","","","",""]
["R4-1705333","Discussion on blocking requirement of mmWave NR BS in hotspot scenario","ZTE Corporation","Fei Xue","59676","discussion","","","","445","10.5.4.2","Blocking Requirements [NR_newRAT]",53330,"noted","2017-05-05T10:43:07.477","2017-05-06T09:27:52.647","","","","","","","","","","","","","","",""]
["R4-1705334","Discussion on blocking requirement of mmWave NR BS in Urban Macro scenario","ZTE Corporation","Fei Xue","59676","other","Approval","","","445","10.5.4.2","Blocking Requirements [NR_newRAT]",53340,"noted","2017-05-05T10:52:40.817","2017-05-06T09:27:52.663","","","","","","","","","","","","","","",""]
["R4-1705335","CR to 36.133: Introduction of Band 49 (3.5 GHz LAA in US)","Ericsson, AT&T","Patrizia Testa","66129","CR","Approval","This CR introduces B49 in the specification","","354","9.11.4","Other specifications [LTE_ 3550_CBRS_US_LAA]",52720,"endorsed","2017-05-05T10:52:55.247","2017-05-06T11:57:51.920","","","Rel-15","36.133","14.3.0","LTE_3550_CBRS_US_LAA","4973","","B","","","","","",""]
["R4-1705336","Discussion on blocking requirement of mmWave NR BS in Urban Macro scenario","ZTE Corporation","Fei Xue","59676","other","Approval","","","445","10.5.4.2","Blocking Requirements [NR_newRAT]",54310,"withdrawn","2017-05-05T10:53:09.177",null,"","","","","","","","","","","","","","",""]
["R4-1705337","Discussion on DL RS power accuracy of NR BS","ZTE Corporation","Fei Xue","59676","other","Approval","","","442","10.5.3.4","Other Tx requirements [NR_newRAT]",49540,"noted","2017-05-05T11:02:54.973","2017-05-06T09:27:52.663","","","","","","","","","","","","","","",""]
["R4-1705338","TR 36.714-02-02: 2DL/2UL inter-band CA R14 v0.8.0","Huawei Technologies France","Ye Liu","57639","draft TR","","","","118","7.6.1","Rapporteur Input (WID/CRs) [LTE_CA_R14_2DL2UL-Core]",53380,"approved","2017-05-05T11:11:50.837","2017-05-05T11:32:19.690","","","Rel-14","36.714-02-02","0.8.0","LTE_CA_R14_2DL2UL-Core","","","","","","","","",""]
["R4-1705339","Discussion on dynamic range requirement of mmWave NR BS in dense urban scenario","ZTE Corporation","Fei Xue","59676","discussion","","","","444","10.5.4.1","Dynamic Range [NR_newRAT]",53440,"noted","2017-05-05T11:12:46.650","2017-05-06T09:27:52.677","","","","","","","","","","","","","","",""]
["R4-1705340","NR UE Tx requirements","Nokia, Alcatel-Lucent Shanghai Bell","Tuomo Säynäjäkangas","69937","discussion","Approval","Discuss NR UE Tx requirements needed for eMBB services following the agreements made in the NR study. It also give some examples using LTE requirements as starting point.","","426","10.4.3","Transmitter characteristics [NR_newRAT]",49350,"noted","2017-05-05T11:16:43.340","2017-05-05T15:52:41.943","","","Rel-15","","","","","","","","","","","",""]
["R4-1705341","Definition of NR Channel Bandwidths and Spectrum Utilization requirements","Nokia, Alcatel-Lucent Shanghai Bell","Tuomo Säynäjäkangas","69937","discussion","Approval","Discuss how NR channel bandwidths and spectrum utilization requirements should be defined for NR for frequencies below 6 GHz and above 24 GHz.","","418","10.3.1","Channel bandwidth and subcarrier spacing [NR_newRAT]",52620,"noted","2017-05-05T11:16:43.357","2017-05-05T15:52:41.960","","","Rel-15","","","","","","","","","","","",""]
["R4-1705342","Spectrum Utilization simulation results","Nokia, Alcatel-Lucent Shanghai Bell","Tuomo Säynäjäkangas","69937","discussion","Discussion","Presents DL spectrum utilization simulation results for RAN4 requirement discussion and further analyses. Some UL results are also presented for the comparison purposes.","","420","10.3.3","Spectrum utilization [NR_newRAT]",52390,"noted","2017-05-05T11:16:43.370","2017-05-05T15:52:41.960","","","Rel-15","","","","","","","","","","","",""]
["R4-1705343","NR in-band mixed numerology requirements","Nokia, Alcatel-Lucent Shanghai Bell","Tuomo Säynäjäkangas","69937","discussion","Approval","Discuss what in-band mixed numerology requirements need to be defined for NR eMBB services","","421","10.3.4","In-band requirements [NR_newRAT]",49480,"noted","2017-05-05T11:16:43.370","2017-05-05T15:52:41.960","","","Rel-15","","","","","","","","","","","",""]
["R4-1705344","Discussion on dynamic range requirement of mmWave NR BS in hotspot scenario","ZTE Corporation","Fei Xue","59676","discussion","","","","444","10.5.4.1","Dynamic Range [NR_newRAT]",53450,"noted","2017-05-05T11:22:47.420","2017-05-06T09:27:52.677","","","","","","","","","","","","","","",""]
["R4-1705345","Discussion on dynamic range requirement of mmWave NR BS in hotspot scenario","ZTE Corporation","Fei Xue","59676","discussion","","","","444","10.5.4.1","Dynamic Range [NR_newRAT]",53490,"withdrawn","2017-05-05T11:23:10.993",null,"","","","","","","","","","","","","","",""]
["R4-1705346","Study about TDD L-Band UE emission level to protect MSS above 1518MHz","ETISALAT, Huawei , Hisilicon","Abdulhadi AbouAlmal","59505","discussion","Approval","Study about TDD L-Band UE emission level to protect MSS above 1518MHz","","326","9.6","TDD operating band in the L-band for LTE [LTE_TDD_L_Band]",53730,"withdrawn","2017-05-05T11:31:18.103",null,"","","","","","","","","","","","","","",""]
["R4-1705347","CR for PHR maping for NB-IoT R14","Huawei, HiSilicon","Qiming Li","61879","CR","Approval","","","195","7.17.3.2.3","PHR [NB_IOTenh-Core]",53470,"withdrawn","2017-05-05T11:32:15.057",null,"R4-1703622","","Rel-14","36.133","14.3.0","NB_IOTenh-Core","4766","1","A","","","","","",""]
["R4-1705348","Discussion on receiver dynamic range of mmWave NR BS in Urban Macro scenario","ZTE Corporation","Fei Xue","59676","other","Approval","","","444","10.5.4.1","Dynamic Range [NR_newRAT]",53710,"withdrawn","2017-05-05T11:32:41.747",null,"","","","","","","","","","","","","","",""]
["R4-1705349","Discussion on receiver dynamic range of mmWave NR BS in Urban Macro scenario","ZTE Corporation","Fei Xue","59676","other","Approval","","","444","10.5.4.1","Dynamic Range [NR_newRAT]",53720,"withdrawn","2017-05-05T11:33:01.370",null,"","","","","","","","","","","","","","",""]
["R4-1705350","Provisional measurement uncertainty values for UE RF baseline test method","Keysight Technologies UK Ltd","Moray Rumney","6630","other","Discussion","","","461","10.7.2.2","Measurement uncertainty and test tolerance [FS_NR_test_methods]",53500,"noted","2017-05-05T11:33:06.410","2017-05-06T19:31:50.580","","","","","","","","","","","","","","",""]
["R4-1705351","Discussion of UE capability siganling structure","Ericsson","Maomao Chen","46060","discussion","Discussion","discussion","","293","7.29.4","Demodulation [WI code or TEI14]",53520,"noted","2017-05-05T11:33:10.043","2017-05-06T12:16:26.250","","","Rel-14","","","TEI14","","","","","","","","",""]
["R4-1705352","Draft LS to RAN2 for UE capability related to baseband and RF feature","Ericsson","Maomao Chen","46060","LS out","Approval","LS out","","293","7.29.4","Demodulation [WI code or TEI14]",620100,"noted","2017-05-05T11:33:11.400","2017-05-06T12:16:26.250","","","Rel-14","","","TEI14","","","","","","RAN2","RAN1","",""]
["R4-1705353","CR for adding TDD 4 DL CA bandwidth combination for CQI CA tests in Rel-13","Ericsson","Maomao Chen","46060","CR","Agreement","CR","","70","5.6.3","Demodulation and CSI [WI code or TEI13]",53530,"agreed","2017-05-05T11:33:11.417","2017-05-06T12:16:26.250","","","Rel-13","36.101","13.7.0","TEI13","4447","","F","RP-171311","","","","",""]
["R4-1705354","CR for adding TDD 4 DL CA bandwidth combination for CQI CA tests in Rel-14","Ericsson","Maomao Chen","46060","CR","Agreement","CR","","70","5.6.3","Demodulation and CSI [WI code or TEI13]",53540,"agreed","2017-05-05T11:33:12.353","2017-05-23T15:07:51.460","","","Rel-14","36.101","14.3.0","TEI13","4448","","A","RP-171311","","","","",""]
["R4-1705355","CR for adding applicability rule for MU TM9 4Rx tests in Rel-13","Ericsson","Maomao Chen","46060","CR","Approval","CR","","32","5.2.3","UE demodulation and CSI (36.101) [LTE_4Rx_AP_DL-Perf]",53550,"revised","2017-05-05T11:33:13.337","2017-05-06T12:16:26.250","","R4-1706181","Rel-13","36.101","13.7.0","LTE_4Rx_AP_DL-Perf","4449","","F","","","","","",""]
["R4-1705356","CR for adding applicability rule for MU TM9 4Rx tests in Rel-14","Ericsson","Maomao Chen","46060","CR","Agreement","CR","","32","5.2.3","UE demodulation and CSI (36.101) [LTE_4Rx_AP_DL-Perf]",53560,"agreed","2017-05-05T11:33:14.193","2017-05-23T15:07:51.490","","","Rel-14","36.101","14.3.0","LTE_4Rx_AP_DL-Perf","4450","","A","RP-171304","","","","",""]
["R4-1705357","CR for updating applicability rule for SDR CA tests for 4Rx CA in Rel-14","Ericsson","Maomao Chen","46060","CR","Approval","CR","","244","7.21.2","UE demodulation (36.101) [LTE_4Rx_AP_DL_CA-Perf]",55570,"revised","2017-05-05T11:33:14.957","2017-05-06T12:16:26.267","","R4-1706180","Rel-14","36.101","14.3.0","LTE_4Rx_AP_DL_CA-Perf","4451","","F","","","","","",""]
["R4-1705358","Smmary of alignment and impairment results for IRC TM9 tests for 4Rx CA","Ericsson","Maomao Chen","46060","discussion","Discussion","discussion","","244","7.21.2","UE demodulation (36.101) [LTE_4Rx_AP_DL_CA-Perf]",46310,"revised","2017-05-05T11:33:15.753","2017-05-06T12:16:26.267","","R4-1706176","Rel-14","","","LTE_4Rx_AP_DL_CA-Perf","","","","","","","","",""]
["R4-1705359","CR for further updating IRC tests for 4Rx CA in Rel-14","Ericsson, Qualcomm","Maomao Chen","46060","CR","Approval","CR","","244","7.21.2","UE demodulation (36.101) [LTE_4Rx_AP_DL_CA-Perf]",53570,"revised","2017-05-05T11:33:15.770","2017-05-06T12:16:26.267","","R4-1706177","Rel-14","36.101","14.3.0","LTE_4Rx_AP_DL_CA-Perf","4452","","B","","","","","",""]
["R4-1705360","UE receiver design for 256QAM and higher layer with CA","Ericsson","Maomao Chen","46060","other","Approval","other","","244","7.21.2","UE demodulation (36.101) [LTE_4Rx_AP_DL_CA-Perf]",53580,"noted","2017-05-05T11:33:16.580","2017-05-06T12:16:26.283","","","Rel-14","","","LTE_4Rx_AP_DL_CA-Perf","","","","","","","","",""]
["R4-1705361","CR for introducing applicability rule for 256QAM or high layer 4Rx CA tests","Ericsson","Maomao Chen","46060","CR","Approval","CR","","244","7.21.2","UE demodulation (36.101) [LTE_4Rx_AP_DL_CA-Perf]",53640,"revised","2017-05-05T11:33:16.597","2017-05-06T12:16:26.283","","R4-1706198","Rel-14","36.101","14.3.0","LTE_4Rx_AP_DL_CA-Perf","4453","","B","","","","","",""]
["R4-1705362","CR for introducing 256QAM tests for 4Rx CA in Rel-14","Ericsson","Maomao Chen","46060","CR","Approval","CR","","244","7.21.2","UE demodulation (36.101) [LTE_4Rx_AP_DL_CA-Perf]",53650,"revised","2017-05-05T11:33:17.343","2017-05-06T12:16:26.283","","R4-1706199","Rel-14","36.101","14.3.0","LTE_4Rx_AP_DL_CA-Perf","4454","","B","","","","","",""]
["R4-1705363","CR for introducing 3 and 4 layers tests for 4Rx CA in Rel-14","Ericsson","Maomao Chen","46060","CR","Approval","CR","","244","7.21.2","UE demodulation (36.101) [LTE_4Rx_AP_DL_CA-Perf]",53660,"revised","2017-05-05T11:33:18.157","2017-05-06T12:16:26.283","","R4-1706200","Rel-14","36.101","14.3.0","LTE_4Rx_AP_DL_CA-Perf","4455","","B","","","","","",""]
["R4-1705364","Summary of alignment and impairment results for 256QAM tests for 4Rx CA","Ericsson","Maomao Chen","46060","discussion","Discussion","discussion","","244","7.21.2","UE demodulation (36.101) [LTE_4Rx_AP_DL_CA-Perf]",53610,"revised","2017-05-05T11:33:18.903","2017-05-06T12:16:26.297","","R4-1706178","Rel-14","","","LTE_4Rx_AP_DL_CA-Perf","","","","","","","","",""]
["R4-1705365","Summary of alignment and impairment results for 3 and 4 layers tests for 4Rx CA","Ericsson","Maomao Chen","46060","discussion","Discussion","discussion","","244","7.21.2","UE demodulation (36.101) [LTE_4Rx_AP_DL_CA-Perf]",53620,"revised","2017-05-05T11:33:18.920","2017-05-06T12:16:26.297","","R4-1706179","Rel-14","","","LTE_4Rx_AP_DL_CA-Perf","","","","","","","","",""]
["R4-1705366","Simulation results for remaining issues for 4Rx CA performance","Ericsson","Maomao Chen","46060","discussion","Discussion","discussion","","244","7.21.2","UE demodulation (36.101) [LTE_4Rx_AP_DL_CA-Perf]",53630,"noted","2017-05-05T11:33:18.937","2017-05-06T12:16:26.313","","","Rel-14","","","LTE_4Rx_AP_DL_CA-Perf","","","","","","","","",""]
["R4-1705367","Discussion on eCRS-IM UE capability and network assistant info","Ericsson","Maomao Chen","46060","discussion","Discussion","discussion","","275","7.27.1.1","Capability and signaling [LTE_eCRSIM_eSUMIMO]",51280,"noted","2017-05-05T11:33:18.937","2017-05-06T12:16:26.313","","","Rel-14","","","LTE_eCRSIM_eSUMIMO","","","","","","","","",""]
["R4-1705368","WF for test proposal for performance part of FeMBMS","Ericsson, Qualcomm","Maomao Chen","46060","other","Approval","other","","157","7.13.5","Demodulation (36.101) [MBMS_LTE_enh2-Perf]",55270,"revised","2017-05-05T11:33:18.950","2017-05-06T12:16:26.313","","R4-1706035","Rel-14","","","MBMS_LTE_enh2-Perf","","","","","","","","",""]
["R4-1705369","CR for introduction of PMCH and PDSCH demodulation tests for FeMBMS","Ericsson","Maomao Chen","46060","CR","Approval","CR","","157","7.13.5","Demodulation (36.101) [MBMS_LTE_enh2-Perf]",574700,"revised","2017-05-05T11:33:18.950","2017-05-06T12:16:26.313","","R4-1706013","Rel-14","36.101","14.3.0","MBMS_LTE_enh2-Perf","4456","","B","","","","","",""]
["R4-1705370","Test method and test scope for NR UE performance","Ericsson","Maomao Chen","46060","discussion","Discussion","discussion","","466","10.7.5","UE Demodulation [FS_NR_test_methods]",583000,"noted","2017-05-05T11:33:19.700","2017-05-06T12:16:26.330","","","Rel-15","","","FS_NR_test_methods","","","","","","","","",""]
["R4-1705371","Discussion on receiver dynamic range of mmWave NR BS in Urban Macro scenario","ZTE Corporation","Fei Xue","59676","other","Approval","","","444","10.5.4.1","Dynamic Range [NR_newRAT]",54300,"withdrawn","2017-05-05T11:33:19.980",null,"","","","","","","","","","","","","","",""]
["R4-1705372","Discussion on receiver dynamic range of mmWave NR BS in Urban Macro scenario","ZTE Corporation","Fei Xue","59676","other","","","","444","10.5.4.1","Dynamic Range [NR_newRAT]",53480,"noted","2017-05-05T11:42:46.870","2017-05-06T09:27:52.787","","","","","","","","","","","","","","",""]
["R4-1705373","Study about TDD L-Band UE emission level to protect MSS above 1518MHz","ETISALAT, Huawei , Hisilicon","Abdulhadi AbouAlmal","59505","discussion","Approval","Study about TDD L-Band UE emission level to protect MSS above 1518MHz","","327","9.6.1","Band Arrangement [LTE_TDD_L_Band-core]",610400,"noted","2017-05-05T11:43:01.097","2017-05-06T16:57:51.927","","","","","","","","","","","","","","",""]
["R4-1705374","Discussion on frequency error requirement of NR BS","ZTE Corporation","Fei Xue","59676","other","","","","442","10.5.3.4","Other Tx requirements [NR_newRAT]",56320,"noted","2017-05-05T12:01:26.417","2017-05-06T09:27:52.803","","","","","","","","","","","","","","",""]
["R4-1705375","TP for TR36.714-04-01: delta Tib/Rib values for CA_39C-42C_BCS0","ZTE Corporation","Shengxiang Guo","72253","pCR","","This contribution provides a text proposal on delta Tib/Rib values for CA_4DL_39C-42C_1UL_BCS0 for TR36.714-04-01","","107","7.4.2","UE RF (36.101) [LTE_CA_R14_4DL1UL-Core]",578200,"approved","2017-05-05T12:01:55.057","2017-05-06T07:57:52.067","","","Rel-14","36.714-04-01","0.7.0","LTE_CA_R14_4DL1UL-Core","","","","","","","","",""]
["R4-1705376","Correction CR on 2UL CA for CA_2A-66A","Huawei, Hisilicon","Ye Liu","57639","CR","Agreement","","","119","7.6.2","UE RF (36.101) [LTE_CA_R14_2DL2UL-Core]",53760,"agreed","2017-05-05T12:03:29.047","2017-05-05T12:42:02.893","","","Rel-14","36.101","14.3.0","LTE_CA_R14_2DL2UL-Core","4457","","F","RP-171277","","","","",""]
["R4-1705377","Introduction of completed R14 2DL2UL band combinations to TS 36.101","Huawei, Hisilicon","Ye Liu","57639","CR","Agreement","Big CR for 2DL/2UL","","118","7.6.1","Rapporteur Input (WID/CRs) [LTE_CA_R14_2DL2UL-Core]",53800,"agreed","2017-05-05T12:03:31.417","2017-05-23T15:07:51.490","","","Rel-14","36.101","14.3.0","LTE_CA_R14_2DL2UL-Core","4458","","B","RP-171277","","","","",""]
["R4-1705378","Revised 2DL/2UL CA WID","Huawei, Hisilicon","Ye Liu","57639","WID revised","Endorsement","Rel-14 2UL CA WID revision","","118","7.6.1","Rapporteur Input (WID/CRs) [LTE_CA_R14_2DL2UL-Core]",53780,"endorsed","2017-05-05T12:03:32.277","2017-05-23T15:07:51.507","","","Rel-14","","","LTE_CA_R14_2DL2UL-Core","","","","","","","","",""]
["R4-1705379","TP for TR 36.714-02-02: update the scope","Huawei, Hisilicon","Ye Liu","57639","pCR","Approval","Band combinations with Band 46 under LAA WI are captured in the scope.","","118","7.6.1","Rapporteur Input (WID/CRs) [LTE_CA_R14_2DL2UL-Core]",53770,"approved","2017-05-05T12:03:32.307","2017-05-05T12:42:02.893","","","Rel-14","36.714-02-02","0.8.0","LTE_CA_R14_2DL2UL-Core","","","","","","","","",""]
["R4-1705380","Draft 2DL/2UL CA WID for Rel-15","Huawei, Hisilicon","Ye Liu","57639","WID new","Endorsement","2UL CA WID for Rel-15","","118","7.6.1","Rapporteur Input (WID/CRs) [LTE_CA_R14_2DL2UL-Core]",53790,"endorsed","2017-05-05T12:03:32.353","2017-05-23T15:07:51.507","","","","","","","","","","","","","","",""]
["R4-1705381","TP for TR 36.714-00-00: MSD for CA_1A-1A_BCS0","Huawei, Hisilicon","Ye Liu","57639","pCR","Approval","","","89","7.1.2","UE RF (36.101) [LTE_CA_R14_intra-Core]",568900,"approved","2017-05-05T12:03:32.353","2017-05-05T12:42:02.910","","R4-1705873","Rel-14","36.714-00-02","0.7.0","LTE_CA_R14_xDL2UL-Core","","","","","","","","",""]
["R4-1705382","New work item proposal on high power UE for LTE Band 42","Huawei, Hisilicon","Ye Liu","57639","WID new","Information","","","473","13","Revision of the Work Plan",53830,"noted","2017-05-05T12:03:32.400","2017-05-05T12:42:02.893","","","","","","","","","","","","","","",""]
["R4-1705383","Motivation for Band 42 HPUE","Huawei, Hisilicon","Ye Liu","57639","discussion","Discussion","","","473","13","Revision of the Work Plan",53840,"noted","2017-05-05T12:03:32.417","2017-05-05T12:42:02.910","","","","","","","","","","","","","","",""]
["R4-1705384","New WID on TDD 3300-3400 MHz band for LTE","Huawei, Hisilicon","Ye Liu","57639","WID new","Information","","","473","13","Revision of the Work Plan",53850,"noted","2017-05-05T12:03:32.417","2017-05-05T12:42:02.910","","","","","","","","","","","","","","",""]
["R4-1705385","Motivation for TDD 3300-3400 MHz band for LTE","Huawei, Hisilicon","Ye Liu","57639","discussion","Discussion","","","473","13","Revision of the Work Plan",55300,"noted","2017-05-05T12:03:32.430","2017-05-05T12:42:02.877","","","","","","","","","","","","","","",""]
["R4-1705386","Framework on Uncertainty Budget for ACLR","Ericsson","Esther Sienkiewicz","59234","discussion","Approval","In previous work, in Release 13, the uncertainty budget was a requirement to determine the overall test tolerance.  Transmit power and receiver sensitivity are requirements of absolute measurement.","","366","9.12.3.1","RF conformance requirements [AASenh_BS_LTE_UTRA-Perf]",53860,"noted","2017-05-05T12:05:17.807","2017-05-05T18:13:27.070","","","Rel-15","","","AASenh_BS_LTE_UTRA-Perf","","","","","","","","",""]
["R4-1705387","TP for TR 37.843: Section 5.6.6 Spurious Emissions","Ericsson","Esther Sienkiewicz","59234","pCR","Approval","In this contribution a proposed test method is described to capture spurious emissions testing.   In addition to keeping different sparse grids to estimate TRP in the goal of reducing test time but not compromising TRP accuracy","","366","9.12.3.1","RF conformance requirements [AASenh_BS_LTE_UTRA-Perf]",53870,"noted","2017-05-05T12:05:17.820","2017-05-05T18:13:27.070","","","Rel-15","37.843","0.2.0","AASenh_BS_LTE_UTRA-Perf","","","","","","","","",""]
["R4-1705388","TP for TR 37.843: Section 10 Conformance Testing Aspects","Ericsson","Esther Sienkiewicz","59234","pCR","Approval","This contribution presents proposed changes to Section 10 of TR 37.843.  As the discussion progresses, it is time to start draft text for conformance testing aspects for each OTA requirement for eAAS.","","366","9.12.3.1","RF conformance requirements [AASenh_BS_LTE_UTRA-Perf]",53880,"noted","2017-05-05T12:05:17.853","2017-05-05T18:13:27.070","","","Rel-15","37.843","0.2.0","AASenh_BS_LTE_UTRA-Perf","","","","","","","","",""]
["R4-1705389","TP for TR 37.843: Section 4.4","Ericsson","Esther Sienkiewicz","59234","pCR","Approval","In the last RAN4 meeting in Spokane, discussion on unwanted emissions scaling lead to an agreed WF [1].","","362","9.12.2.5","Other Transmitter Requirements [AASenh_BS_LTE_UTRA-Core]",56520,"revised","2017-05-05T12:05:17.900","2017-05-05T18:14:07.837","","R4-1706138","Rel-15","37.843","0.2.0","AASenh_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-1705390","TRP Measurements for mmWave","Ericsson","Esther Sienkiewicz","59234","discussion","Discussion","Total radiated power is estimated in practice by measuring discrete points over a sphere of the device under test.  One difference between sub 6 GHz and millimeter wave could be the method in which the density of the TRP sampling grid is determined.","","447","10.5.5","Testability [NR_newRAT]",53900,"noted","2017-05-05T12:05:17.930","2017-05-05T18:14:07.853","","","Rel-15","","","NR_newRAT","","","","","","","","",""]
["R4-1705391","Receiver link simulation results","Ericsson","Esther Sienkiewicz","59234","discussion","Discussion","Link level simulation results have been presented specifically forfor DL transmit considering the 15 kHz and 60khz subcarrier spacing [1] in previous meetings. The results suggested that, in 20MHz spectrum, 107-109 PRB utilization optimizes efficiency for","","420","10.3.3","Spectrum utilization [NR_newRAT]",52080,"noted","2017-05-05T12:05:17.947","2017-05-05T18:14:07.867","","","Rel-15","","","NR_newRAT","","","","","","","","",""]
["R4-1705392","Draft TS 37.105 Specification text for Section 6.6 Unwanted Emissions","Ericsson","Esther Sienkiewicz","59234","discussion","Discussion","In this contribution a text proposal is presented for unwanted emissions section of TS 37.105 and we would like to encourage feedback from other companies on the proposed text.","","356","9.12.1","General [AASenh_BS_LTE_UTRA]",56541,"revised","2017-05-05T12:05:17.947","2017-05-05T18:14:07.867","","R4-1706130","Rel-15","","","AASenh_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-1705393","Dual probe CATR test method for off-axis measurements of beamlocked UEs","Keysight Technologies UK Ltd","Moray Rumney","6630","other","Discussion","","","459","10.7.2","UE RF [FS_NR_test_methods]",581800,"withdrawn","2017-05-05T12:11:14.303",null,"","","","","","","","","","","","","","",""]
["R4-1705394","Simplification of baseline method for off-axis measurements of beamlocked UEs","Keysight Technologies UK Ltd","Moray Rumney","6630","other","Discussion","","","459","10.7.2","UE RF [FS_NR_test_methods]",581900,"noted","2017-05-05T12:12:09.620","2017-05-05T21:18:50.977","","","","","","","","","","","","","","",""]
["R4-1705395","Discussion on E-UTRA REFSENS requirement with in-band NB-IoT operation","ZTE Corporation","Fei Xue","59676","other","Approval","","","59","5.5.2","BS RF core(36.104) [NB_IOT-Core]",55690,"noted","2017-05-05T12:13:17.917","2017-05-06T09:27:52.817","","","","","","","","","","","","","","",""]
["R4-1705396","A-MPR Simulation results for Band 68 ? LTE 10MHz and 15MHz","Airbus DS SLC","Eric Georgeaux","38175","discussion","Discussion","Simulations results for LTE signal with 10 and 15MHz bandwidth confined in the lower part of the Band 68 are presented.","","312","9.3.1","A-MPR requirements [LTE700_Europe_PPDR-core]",53960,"noted","2017-05-05T12:22:25.250","2017-05-05T12:32:10.850","","","","","","LTE700_Europe_PPDR-Core","","","","","","","","",""]
["R4-1705397","Discussion on ICS requirement of mmWave NR BS in Urban Macro scenario","ZTE Corporation","Fei Xue","59676","other","Approval","","","446","10.5.4.3","Other Rx requirements [NR_newRAT]",55000,"noted","2017-05-05T12:22:54.810","2017-05-06T09:27:52.817","","","","","","","","","","","","","","",""]
["R4-1705398","Channel Raster For Multiple Standalone NB-IoT Carriers (TS 36.101)","Nokia, Alcatel-Lucent Shanghai Bell","Man Hung Ng","68815","CR","Agreement","Allow a deviation from the 100 kHz channel raster positions for standalone NB-IoT carrier.","","58","5.5.1","UE RF core(36.101) [NB_IOT-Core]",46710,"not pursued","2017-05-05T12:23:10.147","2017-05-05T15:54:51.327","","","Rel-13","36.101","13.7.0","NB_IOT-Core","4459","","F","","","","","",""]
["R4-1705399","Channel Raster For Multiple Standalone NB-IoT Carriers (TS 36.101)","Nokia, Alcatel-Lucent Shanghai Bell","Man Hung Ng","68815","CR","Agreement","Allow a deviation from the 100 kHz channel raster positions for standalone NB-IoT carrier.","","58","5.5.1","UE RF core(36.101) [NB_IOT-Core]",46720,"agreed","2017-05-05T12:23:11.033","2017-05-23T15:07:51.507","","","Rel-14","36.101","14.3.0","NB_IOT-Core","4460","","F","RP-171299","","","","",""]
["R4-1705400","Channel Raster For Multiple Standalone NB-IoT Carriers (TS 36.104)","Nokia, Alcatel-Lucent Shanghai Bell","Man Hung Ng","68815","CR","Agreement","Allow a deviation from the 100 kHz channel raster positions for standalone NB-IoT carrier.","","59","5.5.2","BS RF core(36.104) [NB_IOT-Core]",48230,"not pursued","2017-05-05T12:23:11.970","2017-05-05T15:54:51.327","","","Rel-13","36.104","13.7.0","NB_IOT-Core","4677","","F","","","","","",""]
["R4-1705401","Channel Raster For Multiple Standalone NB-IoT Carriers (TS 36.104)","Nokia, Alcatel-Lucent Shanghai Bell","Man Hung Ng","68815","CR","Agreement","Allow a deviation from the 100 kHz channel raster positions for standalone NB-IoT carrier.","","59","5.5.2","BS RF core(36.104) [NB_IOT-Core]",48240,"agreed","2017-05-05T12:23:12.780","2017-05-23T15:07:51.523","","","Rel-14","36.104","14.3.0","NB_IOT-Core","4678","","F","RP-171299","","","","",""]
["R4-1705402","Channel Raster For Multiple Standalone NB-IoT Carriers (TS 36.141)","Nokia, Alcatel-Lucent Shanghai Bell","Man Hung Ng","68815","CR","Agreement","Allow a deviation from the 100 kHz channel raster positions for standalone NB-IoT carrier.","","61","5.5.4","BS RF Conformance testing (36.141) [NB_IOT-Perf]",48270,"not pursued","2017-05-05T12:23:13.657","2017-05-05T15:54:51.327","","","Rel-13","36.141","13.7.0","NB_IOT-Perf","1039","","F","","","","","",""]
["R4-1705403","Channel Raster For Multiple Standalone NB-IoT Carriers (TS 36.141)","Nokia, Alcatel-Lucent Shanghai Bell","Man Hung Ng","68815","CR","Agreement","Allow a deviation from the 100 kHz channel raster positions for standalone NB-IoT carrier.","","61","5.5.4","BS RF Conformance testing (36.141) [NB_IOT-Perf]",48320,"agreed","2017-05-05T12:23:14.590","2017-05-23T15:07:51.523","","","Rel-14","36.141","14.3.0","NB_IOT-Perf","1040","","F","RP-171303","","","","",""]
["R4-1705404","Narrowband blocking requirement for NB-IoT guard band operation (TS 36.104)","Nokia, Alcatel-Lucent Shanghai Bell","Man Hung Ng","68815","CR","Agreement","Clarify that the NB-IoT PRB should be placed adjacent to the LTE PRB edge as close as possible (i.e., away from edge of channel bandwidth) to meet the current requirements.","","59","5.5.2","BS RF core(36.104) [NB_IOT-Core]",54040,"agreed","2017-05-05T12:23:15.527","2017-05-05T15:54:51.310","","","Rel-13","36.104","13.7.0","NB_IOT-Core","4679","","F","RP-171299","","","","",""]
["R4-1705405","Narrowband blocking requirement for NB-IoT guard band operation (TS 36.104)","Nokia, Alcatel-Lucent Shanghai Bell","Man Hung Ng","68815","CR","Agreement","Clarify that the NB-IoT PRB should be placed adjacent to the LTE PRB edge as close as possible (i.e., away from edge of channel bandwidth) to meet the current requirements.","","59","5.5.2","BS RF core(36.104) [NB_IOT-Core]",54050,"agreed","2017-05-05T12:23:16.260","2017-05-23T15:07:51.537","","","Rel-14","36.104","14.3.0","NB_IOT-Core","4680","","A","RP-171299","","","","",""]
["R4-1705406","Narrowband blocking requirement for NB-IoT guard band operation (TS 37.104)","Nokia, Alcatel-Lucent Shanghai Bell","Man Hung Ng","68815","CR","Agreement","Clarify that the NB-IoT PRB should be placed adjacent to the LTE PRB edge as close as possible (i.e., away from edge of channel bandwidth) to meet the current requirements.","","59","5.5.2","BS RF core(36.104) [NB_IOT-Core]",54060,"agreed","2017-05-05T12:23:17.027","2017-05-05T15:54:51.373","","","Rel-13","37.104","13.5.0","NB_IOT-Core","0782","","F","RP-171299","","","","",""]
["R4-1705407","Narrowband blocking requirement for NB-IoT guard band operation (TS 37.104)","Nokia, Alcatel-Lucent Shanghai Bell","Man Hung Ng","68815","CR","Agreement","Clarify that the NB-IoT PRB should be placed adjacent to the LTE PRB edge as close as possible (i.e., away from edge of channel bandwidth) to meet the current requirements.","","59","5.5.2","BS RF core(36.104) [NB_IOT-Core]",54070,"agreed","2017-05-05T12:23:17.820","2017-05-23T15:07:51.537","","","Rel-14","37.104","14.3.0","NB_IOT-Core","0783","","A","RP-171299","","","","",""]
["R4-1705408","Narrowband blocking requirement for NB-IoT guard band operation (TS 36.141)","Nokia, Alcatel-Lucent Shanghai Bell","Man Hung Ng","68815","CR","Agreement","Clarify that the NB-IoT PRB should be placed adjacent to the LTE PRB edge as close as possible (i.e., away from edge of channel bandwidth) to meet the current requirements.","","61","5.5.4","BS RF Conformance testing (36.141) [NB_IOT-Perf]",54030,"agreed","2017-05-05T12:23:18.587","2017-05-05T15:54:51.373","","","Rel-13","36.141","13.7.0","NB_IOT-Perf","1041","","F","RP-171300","","","","",""]
["R4-1705409","Narrowband blocking requirement for NB-IoT guard band operation (TS 36.141)","Nokia, Alcatel-Lucent Shanghai Bell","Man Hung Ng","68815","CR","Agreement","Clarify that the NB-IoT PRB should be placed adjacent to the LTE PRB edge as close as possible (i.e., away from edge of channel bandwidth) to meet the current requirements.","","61","5.5.4","BS RF Conformance testing (36.141) [NB_IOT-Perf]",54080,"agreed","2017-05-05T12:23:19.410","2017-05-23T15:07:51.537","","","Rel-14","36.141","14.3.0","NB_IOT-Perf","1042","","A","RP-171300","","","","",""]
["R4-1705410","Narrowband blocking requirement for NB-IoT guard band operation (TS 37.141)","Nokia, Alcatel-Lucent Shanghai Bell","Man Hung Ng","68815","CR","Agreement","Clarify that the NB-IoT PRB should be placed adjacent to the LTE PRB edge as close as possible (i.e., away from edge of channel bandwidth) to meet the current requirements.","","61","5.5.4","BS RF Conformance testing (36.141) [NB_IOT-Perf]",54090,"agreed","2017-05-05T12:23:20.160","2017-05-05T15:54:51.373","","","Rel-13","37.141","13.6.0","NB_IOT-Perf","0780","","F","RP-171300","","","","",""]
["R4-1705411","Narrowband blocking requirement for NB-IoT guard band operation (TS 37.141)","Nokia, Alcatel-Lucent Shanghai Bell","Man Hung Ng","68815","CR","Agreement","Clarify that the NB-IoT PRB should be placed adjacent to the LTE PRB edge as close as possible (i.e., away from edge of channel bandwidth) to meet the current requirements.","","61","5.5.4","BS RF Conformance testing (36.141) [NB_IOT-Perf]",54100,"agreed","2017-05-05T12:23:20.987","2017-05-23T15:07:51.537","","","Rel-14","37.141","14.3.0","NB_IOT-Perf","0781","","A","RP-171300","","","","",""]
["R4-1705412","Intermodulation performance requirement for NB-IoT operation (TS 36.104)","Nokia, Alcatel-Lucent Shanghai Bell","Man Hung Ng","68815","CR","Agreement","To shift the CW interfering signal frequency away from the wanted signal by 100 kHz and the E-UTRA interfering signal frequency away from the wanted signal by 200 kHz, if a BS RF receiver fails the test of the corresponding requirement. If the BS RF recei","","59","5.5.2","BS RF core(36.104) [NB_IOT-Core]",54150,"revised","2017-05-05T12:23:21.877","2017-05-05T15:54:51.373","","R4-1705871","Rel-13","36.104","13.7.0","NB_IOT-Core","4681","","F","","","","","",""]
["R4-1705413","Intermodulation performance requirement for NB-IoT operation (TS 36.104)","Nokia, Alcatel-Lucent Shanghai Bell","Man Hung Ng","68815","CR","Agreement","To shift the CW interfering signal frequency away from the wanted signal by 100 kHz and the E-UTRA interfering signal frequency away from the wanted signal by 200 kHz, if a BS RF receiver fails the test of the corresponding requirement. If the BS RF recei","","59","5.5.2","BS RF core(36.104) [NB_IOT-Core]",55560,"agreed","2017-05-05T12:23:22.797","2017-05-23T15:07:51.553","","","Rel-14","36.104","14.3.0","NB_IOT-Core","4682","","A","RP-171300","","","","",""]
["R4-1705414","Intermodulation performance requirement for NB-IoT operation (TS 37.104)","Nokia, Alcatel-Lucent Shanghai Bell","Man Hung Ng","68815","CR","Agreement","To shift the CW interfering signal frequency away from the wanted signal by 100 kHz and the E-UTRA interfering signal frequency away from the wanted signal by 200 kHz, if a BS RF receiver fails the test of the corresponding requirement. If the BS RF recei","","59","5.5.2","BS RF core(36.104) [NB_IOT-Core]",55650,"revised","2017-05-05T12:23:23.670","2017-05-05T15:54:51.357","","R4-1706108","Rel-13","37.104","13.5.0","NB_IOT-Core","0784","","F","","","","","",""]
["R4-1705415","Intermodulation performance requirement for NB-IoT operation (TS 37.104)","Nokia, Alcatel-Lucent Shanghai Bell","Man Hung Ng","68815","CR","Agreement","To shift the CW interfering signal frequency away from the wanted signal by 100 kHz and the E-UTRA interfering signal frequency away from the wanted signal by 200 kHz, if a BS RF receiver fails the test of the corresponding requirement. If the BS RF recei","","59","5.5.2","BS RF core(36.104) [NB_IOT-Core]",55680,"agreed","2017-05-05T12:23:24.653","2017-05-23T15:07:51.553","","","Rel-14","37.104","14.3.0","NB_IOT-Core","0785","","A","RP-171300","","","","",""]
["R4-1705416","Intermodulation performance requirement for NB-IoT operation (TS 36.141)","Nokia, Alcatel-Lucent Shanghai Bell","Man Hung Ng","68815","CR","Agreement","To shift the CW interfering signal frequency away from the wanted signal by 100 kHz and the E-UTRA interfering signal frequency away from the wanted signal by 200 kHz, if a BS RF receiver fails the test of the corresponding requirement. If the BS RF recei","","61","5.5.4","BS RF Conformance testing (36.141) [NB_IOT-Perf]",54170,"revised","2017-05-05T12:23:25.637","2017-05-05T15:54:51.357","","R4-1706109","Rel-13","36.141","13.7.0","NB_IOT-Perf","1043","","F","","","","","",""]
["R4-1705417","Intermodulation performance requirement for NB-IoT operation (TS 36.141)","Nokia, Alcatel-Lucent Shanghai Bell","Man Hung Ng","68815","CR","Agreement","To shift the CW interfering signal frequency away from the wanted signal by 100 kHz and the E-UTRA interfering signal frequency away from the wanted signal by 200 kHz, if a BS RF receiver fails the test of the corresponding requirement. If the BS RF recei","","61","5.5.4","BS RF Conformance testing (36.141) [NB_IOT-Perf]",54180,"agreed","2017-05-05T12:23:26.477","2017-05-23T15:07:51.553","","","Rel-14","36.141","14.3.0","NB_IOT-Perf","1044","","A","RP-171303","","","","",""]
["R4-1705418","Intermodulation performance requirement for NB-IoT operation (TS 37.141)","Nokia, Alcatel-Lucent Shanghai Bell","Man Hung Ng","68815","CR","Agreement","To shift the CW interfering signal frequency away from the wanted signal by 100 kHz and the E-UTRA interfering signal frequency away from the wanted signal by 200 kHz, if a BS RF receiver fails the test of the corresponding requirement. If the BS RF recei","","61","5.5.4","BS RF Conformance testing (36.141) [NB_IOT-Perf]",54190,"revised","2017-05-05T12:23:27.320","2017-05-05T15:54:51.357","","R4-1706110","Rel-13","37.141","13.6.0","NB_IOT-Perf","0782","","F","","","","","",""]
["R4-1705419","Intermodulation performance requirement for NB-IoT operation (TS 37.141)","Nokia, Alcatel-Lucent Shanghai Bell","Man Hung Ng","68815","CR","Agreement","To shift the CW interfering signal frequency away from the wanted signal by 100 kHz and the E-UTRA interfering signal frequency away from the wanted signal by 200 kHz, if a BS RF receiver fails the test of the corresponding requirement. If the BS RF recei","","61","5.5.4","BS RF Conformance testing (36.141) [NB_IOT-Perf]",54200,"agreed","2017-05-05T12:23:28.147","2017-05-23T15:07:51.570","","","Rel-14","37.141","14.3.0","NB_IOT-Perf","0783","","A","RP-171303","","","","",""]
["R4-1705420","Clarification on small BW support for in-band and guard band operation (TS 36.141)","Nokia, Alcatel-Lucent Shanghai Bell","Man Hung Ng","68815","CR","Agreement","To clarify that NB-IoT in-band operation is not applicable in 1.4 MHz E-UTRA channel bandwidth and guard band operation is not applicable in 1.4 MHz and 3 MHz in the clauses that do not clearly state this.","","61","5.5.4","BS RF Conformance testing (36.141) [NB_IOT-Perf]",48350,"revised","2017-05-05T12:23:29.053","2017-05-05T15:54:51.357","","R4-1705940","Rel-13","36.141","13.7.0","NB_IOT-Perf","1045","","F","","","","","",""]
["R4-1705421","Clarification on small BW support for in-band and guard band operation (TS 36.141)","Nokia, Alcatel-Lucent Shanghai Bell","Man Hung Ng","68815","CR","Agreement","To clarify that NB-IoT in-band operation is not applicable in 1.4 MHz E-UTRA channel bandwidth and guard band operation is not applicable in 1.4 MHz and 3 MHz in the clauses that do not clearly state this.","","61","5.5.4","BS RF Conformance testing (36.141) [NB_IOT-Perf]",48360,"agreed","2017-05-05T12:23:29.847","2017-05-23T15:07:51.570","","","Rel-14","36.141","14.3.0","NB_IOT-Perf","1046","","A","RP-171303","","","","",""]
["R4-1705422","Testing for software upgraded BS supporting NB-IoT operation (TS 36.141)","Nokia, Alcatel-Lucent Shanghai Bell","Man Hung Ng","68815","CR","Agreement","State that for a BS is previously conformance tested against the requirements without NB-IoT and later updated to support NB-IoT in-band or standalone by software upgrade, only test configurations where NB-IoT carriers are present are required to be used","","61","5.5.4","BS RF Conformance testing (36.141) [NB_IOT-Perf]",54250,"noted","2017-05-05T12:23:30.660","2017-05-05T16:40:04.560","","","Rel-13","36.141","13.7.0","NB_IOT-Perf","1047","","F","","","","","",""]
["R4-1705423","Testing for software upgraded BS supporting NB-IoT operation (TS 36.141)","Nokia, Alcatel-Lucent Shanghai Bell","Man Hung Ng","68815","CR","Agreement","State that for a BS is previously conformance tested against the requirements without NB-IoT and later updated to support NB-IoT in-band or standalone by software upgrade, only test configurations where NB-IoT carriers are present are required to be used","","61","5.5.4","BS RF Conformance testing (36.141) [NB_IOT-Perf]",55660,"withdrawn","2017-05-05T12:23:31.470",null,"","","Rel-14","36.141","14.3.0","NB_IOT-Perf","1048","","A","","","","","",""]
["R4-1705424","Testing for software upgraded BS supporting NB-IoT operation (TS 37.141)","Nokia, Alcatel-Lucent Shanghai Bell","Man Hung Ng","68815","CR","Agreement","State that for a BS is previously conformance tested against the requirements without NB-IoT and later updated to support NB-IoT in-band or standalone by software upgrade, only test configurations where NB-IoT carriers are present are required to be used","","61","5.5.4","BS RF Conformance testing (36.141) [NB_IOT-Perf]",55670,"revised","2017-05-05T12:23:32.327","2017-05-05T16:40:04.547","","R4-1706080","Rel-13","37.141","13.6.0","NB_IOT-Perf","0784","","F","","","","","",""]
["R4-1705425","Testing for software upgraded BS supporting NB-IoT operation (TS 37.141)","Nokia, Alcatel-Lucent Shanghai Bell","Man Hung Ng","68815","CR","Agreement","State that for a BS is previously conformance tested against the requirements without NB-IoT and later updated to support NB-IoT in-band or standalone by software upgrade, only test configurations where NB-IoT carriers are present are required to be used","","61","5.5.4","BS RF Conformance testing (36.141) [NB_IOT-Perf]",573800,"revised","2017-05-05T12:23:33.123",null,"","R4-1706081","Rel-14","37.141","14.3.0","NB_IOT-Perf","0785","","A","","","","","",""]
["R4-1705426","Reference sensitivity for microcell NB-IoT BS","Nokia, Alcatel-Lucent Shanghai Bell","Man Hung Ng","68815","other","Approval","This contribution provides the simulation results for NB-IoT standalone operation in microcell deployment using the agreed assumptions, and proposes a way forward to specify the reference sensitivity requirement for microcell NB-IoT BS in the RAN4 specifi","","392","9.14.2.1","eNB power classes [NB_IOTenh2-core]",54280,"approved","2017-05-05T12:23:33.950","2017-05-05T15:54:51.357","","","","","","NB_IOTenh2-Core","","","","","","","","",""]
["R4-1705427","Receiver dynamic range for microcell NB-IoT BS","Nokia, Alcatel-Lucent Shanghai Bell","Man Hung Ng","68815","other","Approval","This contribution provides the simulation results for NB-IoT standalone operation in microcell deployment using the agreed assumptions, and proposes a way forward to specify the receiver dynamic range requirement for microcell NB-IoT BS in the RAN4 specif","","392","9.14.2.1","eNB power classes [NB_IOTenh2-core]",54370,"approved","2017-05-05T12:23:33.967","2017-05-05T15:54:51.343","","","","","","NB_IOTenh2-Core","","","","","","","","",""]
["R4-1705428","ACS/in-band blocking for microcell NB-IoT BS","Nokia, Alcatel-Lucent Shanghai Bell","Man Hung Ng","68815","other","Approval","This contribution provides the simulation results for NB-IoT standalone operation in microcell deployment using the agreed assumptions, and proposes a way forward to specify the ACS/in-band blocking requirement for microcell NB-IoT BS in the RAN4 specific","","392","9.14.2.1","eNB power classes [NB_IOTenh2-core]",55720,"noted","2017-05-05T12:23:33.983","2017-05-05T15:54:51.343","","","","","","NB_IOTenh2-Core","","","","","","","","",""]
["R4-1705429","Proposal on below 6GHz NR BS ACLR and ACS","Nokia, Alcatel-Lucent Shanghai Bell","Man Hung Ng","68815","other","Approval","This contribution provides a proposal to specify the below 6GHz NR BS ACLR and ACS conducted requirements in the RAN4 specifications.","","422","10.3.5","ACLR and ACS [NR_newRAT]",567100,"noted","2017-05-05T12:23:33.997","2017-05-05T15:54:51.343","","","","","","NR_newRAT","","","","","","","","",""]
["R4-1705430","Proposal on mmWave NR BS Receiver Dynamic Range","Nokia, Alcatel-Lucent Shanghai Bell","Man Hung Ng","68815","other","Approval","This contribution provides a proposal to specify the mmWave NR BS receiver dynamic range requirement in the RAN4 specifications per the agreed way forward.","","444","10.5.4.1","Dynamic Range [NR_newRAT]",53390,"noted","2017-05-05T12:23:34.027","2017-05-05T15:54:51.343","","","","","","NR_newRAT","","","","","","","","",""]
["R4-1705431","Proposal on mmWave NR BS Receiver In-band Blocking","Nokia, Alcatel-Lucent Shanghai Bell","Man Hung Ng","68815","other","Approval","This contribution provides a proposal to specify the mmWave NR BS receiver in-band blocking requirement in the RAN4 specifications per the agreed way forward.","","445","10.5.4.2","Blocking Requirements [NR_newRAT]",52910,"noted","2017-05-05T12:23:34.043","2017-05-05T15:54:51.327","","","","","","NR_newRAT","","","","","","","","",""]
["R4-1705432","Test cases for cell reselection on idle mode under high speed scenario","Huawei, HiSilicon","Qiming Li","61879","CR","Agreement","","","261","7.25.3","RRM performance (36.133) [LTE_high_speed-Perf]",54350,"withdrawn","2017-05-05T12:31:55.453",null,"R4-1704248","","Rel-14","36.133","14.3.0","LTE_high_speed-Perf","4813","2","B","","","","","",""]
["R4-1705433","TP for TR36.714-05-01: delta Tib/Rib values for CA_39A-42E_BCS0","ZTE Corporation","Shengxiang Guo","72253","pCR","","This contribution provide a text proposal on delta Tib/Rib values for CA_5DL_39A-42E_1UL_BCS0 for TR36.714-05-01","","113","7.5.2","UE RF (36.101) [LTE_CA_R14_5DL1UL-Core]",577000,"approved","2017-05-05T12:31:58.683","2017-05-06T07:57:52.113","","","Rel-14","36.714-05-01","0.7.0","LTE_CA_R14_5DL1UL-Core","","","","","","","","",""]
["R4-1705434","Test cases for cell reselection on idle mode under high speed scenario","Huawei, HiSilicon","Qiming Li","61879","CR","Agreement","","","261","7.25.3","RRM performance (36.133) [LTE_high_speed-Perf]",54690,"withdrawn","2017-05-05T12:32:20.257",null,"R4-1704248","","Rel-14","36.133","14.3.0","LTE_high_speed-Perf","4813","3","B","","","","","",""]
["R4-1705435","Test cases for cell reselection on idle mode under high speed scenario","Huawei, HiSilicon","Qiming Li","61879","CR","Agreement","","","261","7.25.3","RRM performance (36.133) [LTE_high_speed-Perf]",54320,"revised","2017-05-05T12:32:57.617","2017-05-06T13:47:52.530","R4-1704248","R4-1706038","Rel-14","36.133","14.3.0","LTE_high_speed-Perf","4813","4","B","","","","","",""]
["R4-1705436","New work item proposal: LTE Advanced inter-band CA Rel-15 for 3DL/1UL","HuaWei Technologies Co., Ltd","Xiang (Steven) Chen","41576","WID new","Endorsement","3DL CA WID for Rel-15","","100","7.3.1","Rapporteur Input (WID/CRs) [LTE_CA_R14_3DL1UL-Core]",52140,"endorsed","2017-05-05T12:33:59.080","2017-05-23T15:07:51.587","","","","","","","","","","","","","","",""]
["R4-1705437","Simnulation assumption for  NB-IoT small cells","HuaWei Technologies Co., Ltd","Xiang (Steven) Chen","41576","other","","This contribution is for approval.","","392","9.14.2.1","eNB power classes [NB_IOTenh2-core]",54270,"noted","2017-05-05T12:41:48.837","2017-05-05T12:52:29.477","","","","","","","","","","","","","","",""]
["R4-1705438","Proposed changes related to Band 31 in the scope of LTE450_Europe_PPDR Work item","Airbus DS SLC","Eric Georgeaux","38175","discussion","Approval","It is proposed that the following changes are included in the future CR on TS36.101 linked with the work item LTE450_Europe_PPDR:\n- Proposal 1: Include the DTT protection requirement (-42dBm/8MHz over 470-694MHz) \n- Proposal 2: Include Band 31 in the list","","308","9.2.2","UE RF (36.101) [LTE450_Europe_PPDR-core]",54380,"approved","2017-05-05T12:41:57.090","2017-05-05T12:52:20.677","","","Rel-15","","","LTE450_Europe_PPDR-Core","","","","","","","","",""]
["R4-1705439","MPR and A-MPR for CA_41C UL in Power class 2","Nokia","Petri Vasenkari","69954","discussion","Discussion","","","332","9.7.1","UE RF (36.101) [LTE_CA_C_B41_PC2-core]",568200,"noted","2017-05-05T12:43:17.773","2017-05-06T09:07:53.820","","","","","","LTE_CA_C_B41_PC2-Core","","","","","","","","",""]
["R4-1705440","A-MPR for CA_41C UL in Power class 3","Nokia","Petri Vasenkari","69954","discussion","Discussion","","","13","4.2.1","UE RF (core / EMC) [WI code or TEI12]",54400,"noted","2017-05-05T12:43:17.787","2017-05-06T09:07:53.820","","","","","","TEI12","","","","","","","","",""]
["R4-1705441","Band 28 PC1 duplex-filter data","Nokia","Petri Vasenkari","69954","other","Approval","","","304","9.1.2","UE RF (36.101) [LTE_HPUE_B3_B20_B28]",48180,"approved","2017-05-05T12:43:17.803","2017-05-06T09:07:53.837","","","","","","LTE_HPUE_B3_B20_B28","","","","","","","","",""]
["R4-1705442","new draft CR Band 68 modification to enable operation in Europe REL-14","Nokia, Airbus DS SLC","Petri Vasenkari","69954","draftCR","Agreement","","","311","9.3","E-UTRA 700MHz in Europe for Broadband-PPDR [LTE700_Europe_PPDR]",54420,"endorsed","2017-05-05T12:43:17.837","2017-05-06T09:07:53.853","","","Rel-14","36.101","14.3.0","LTE700_Europe_PPDR","","","","","","","","",""]
["R4-1705443","Open issues for Band 68 introduction to Europe","Nokia","Petri Vasenkari","69954","discussion","Discussion","","","311","9.3","E-UTRA 700MHz in Europe for Broadband-PPDR [LTE700_Europe_PPDR]",54430,"noted","2017-05-05T12:43:17.850","2017-05-06T09:07:53.883","","","","","","LTE700_Europe_PPDR","","","","","","","","",""]
["R4-1705444","5DL UE CR","Nokia, Alcatel-Lucent Shanghai Bell","Petri Vasenkari","69954","CR","Agreement","","","112","7.5.1","Rapporteur Input (WID/CRs) [LTE_CA_R14_5DL1UL-Core]",0,"agreed","2017-05-05T12:43:17.867","2017-05-23T15:07:51.587","","","Rel-14","36.101","14.3.0","LTE_CA_R14_5DL1UL-Core","4461","","B","RP-171276","","","","",""]
["R4-1705445","CA bandwidth class Class B 256-QAM non-contigous resource allocation MPR","Nokia, Alcatel-Lucent Shanghai Bell","Petri Vasenkari","69954","other","Approval","","","148","7.12.1","UE RF Maintenance (36.101) [LTE_UL_CAP_enh-Core]",54450,"approved","2017-05-05T12:43:18.707","2017-05-06T09:07:53.917","","","","","","LTE_UL_CAP_enh-Core","","","","","","","","",""]
["R4-1705446","CA bandwidth class Class B 256-QAM non-contigous resource allocation MPR","Nokia, Alcatel-Lucent Shanghai Bell","Petri Vasenkari","69954","CR","Agreement","","","148","7.12.1","UE RF Maintenance (36.101) [LTE_UL_CAP_enh-Core]",54460,"agreed","2017-05-05T12:43:18.723","2017-05-06T09:07:53.930","","","Rel-14","36.101","14.3.0","LTE_UL_CAP_enh-Core","4462","","B","RP-171287","","","","",""]
["R4-1705447","Corrections to CA configurations and bandwidth combination sets","Nokia, Alcatel-Lucent Shanghai Bell","Petri Vasenkari","69954","CR","Agreement","","","291","7.29.2","RF [WI code or TEI14]",54480,"agreed","2017-05-05T12:43:19.550","2017-05-06T09:07:53.947","","","Rel-14","36.101","14.3.0","TEI14","4463","","F","RP-171280","","","","",""]
["R4-1705448","DRAFT LS on extension of NS and CA_NS signalling space","Nokia, Alcatel-Lucent Shanghai Bell","Petri Vasenkari","69954","LS out","Approval","","","291","7.29.2","RF [WI code or TEI14]",569000,"revised","2017-05-05T12:43:20.440","2017-05-06T09:07:53.977","","R4-1705865","","","","TEI14","","","","","","RAN2","","",""]
["R4-1705449","Necessary A-MPR to meet band 71 spectrum emission mask","Nokia","Petri Vasenkari","69954","other","Approval","","","336","9.8.2","UE RF (36.101) [LTE600_US-core]",54490,"approved","2017-05-05T12:43:20.457","2017-05-06T09:07:54.010","","","","","","LTE600_US-Core","","","","","","","","",""]
["R4-1705450","TP to TR 36.748: Expected specification changes to TS 36.101 due to introduction of Band 72","Nokia","Petri Vasenkari","69954","other","Approval","","","308","9.2.2","UE RF (36.101) [LTE450_Europe_PPDR-core]",54510,"revised","2017-05-05T12:43:20.470","2017-05-06T09:07:54.040","","R4-1705882","","","","LTE450_Europe_PPDR-Core","","","","","","","","",""]
["R4-1705451","TP to TR 36.748: Band 72 receiver requirements","Nokia","Petri Vasenkari","69954","other","Approval","","","308","9.2.2","UE RF (36.101) [LTE450_Europe_PPDR-core]",54520,"revised","2017-05-05T12:43:20.487","2017-05-06T09:07:54.070","","R4-1705883","","","","LTE450_Europe_PPDR-Core","","","","","","","","",""]
["R4-1705452","TP to TR 36.748: Band 72 transmitter requirements","Nokia","Petri Vasenkari","69954","other","Approval","","","308","9.2.2","UE RF (36.101) [LTE450_Europe_PPDR-core]",54530,"approved","2017-05-05T12:43:20.487","2017-05-06T09:07:54.087","","","","","","LTE450_Europe_PPDR-Core","","","","","","","","",""]
["R4-1705453","B31 emissons to DTT Approval","Nokia","Petri Vasenkari","69954","other","Approval","","","308","9.2.2","UE RF (36.101) [LTE450_Europe_PPDR-core]",54500,"approved","2017-05-05T12:43:20.517","2017-05-06T09:07:54.117","","","","","","LTE450_Europe_PPDR-Core","","","","","","","","",""]
["R4-1705454","TP to TR 36.748: Expected specification changes to TS 36.101 due to introduction of Band 73","Nokia, Alcatel-Lucent Shanghai Bell","Petri Vasenkari","69954","discussion","Discussion","","","347","9.10.3","UE RF (36.101) [LTE450_Reg3-core]",54540,"noted","2017-05-05T12:43:20.517","2017-05-06T09:07:54.133","","","","","","LTE450_Reg3-Core","","","","","","","","",""]
["R4-1705455","NB1/NB2 OOB note 3 correction","Nokia, Alcatel-Lucent Shanghai Bell","Petri Vasenkari","69954","CR","Agreement","","","131","7.8.2","UE RF (36.101) [NB_IOT_R14_bands]",54550,"agreed","2017-05-05T12:43:20.533","2017-05-06T09:07:54.150","","","Rel-14","36.101","14.3.0","NB_IOT-Core","4464","","F","RP-171300","","","","",""]
["R4-1705456","Intra-frequency RSRP absolute accuracy for non-BL UE","Ericsson","Joakim Axmon","62375","discussion","Discussion","In this contribution we are providing simulation results that show that there is a possibility to tightening the RSRP measurement absolute accuracy requirements for non-BL UEs by some 1.5 dB compared to cat M1 UEs.","","224","7.18.6","RRM performance for non-BL/CE UE (36.133) [LTE_feMTC-Perf]",618500,"noted","2017-05-05T12:43:25.103","2017-05-06T08:09:32.643","","","Rel-14","","","LTE_feMTC-Perf","","","","","","","","",""]
["R4-1705457","CR on 36.133: Intra and inter-frequency RSRP and RSRQ measurement accuracies for UE cat M1","Ericsson","Joakim Axmon","62375","CR","Agreement","In this CR (endorsed at RAN4#82bis) measurement accuracy subsections for intra- and inter frequency RSRP and RSRQ for Rel.14 cat M1 are introduced.","","208","7.18.3","RRM core for BL/CE UE (36.133) [LTE_feMTC-Core]",622000,"agreed","2017-05-05T12:43:25.150","2017-05-06T08:09:32.643","","","Rel-14","36.133","14.3.0","LTE_feMTC-Core","4974","","F","RP-171266","","","","",""]
["R4-1705458","Correction of applicability rule for NRSRP and NRSRQ in NB-IoT","Ericsson","Joakim Axmon","62375","CR","Approval","Current wording for applicability of NRSRQ and NRSRP measurements for UE category NB1 state that measurment accuracy as specified in Section 9 is to be met while in idle mode. Measurement accuracy is however not observable in idle mode, hence it is errone","","188","7.17.3","RRM core (36.133) [NB_IOTenh-Core]",621900,"noted","2017-05-05T12:43:26.027","2017-05-06T08:09:32.643","","","Rel-14","36.133","14.3.0","NB_IOTenh-Core","4975","","F","","","","","",""]
["R4-1705459","Improvement of NPRACH repetition level selection","Ericsson","Joakim Axmon","62375","discussion","Discussion","Selection of NPRACH repetition level under coverage enhancement mode of operation has been identified as one of the improvement areas for NB-IoT. In this contribution we are arguing for NPRACH repetition level selection being based on 2 Tx ports when the","","194","7.17.3.2.2","Random access [NB_IOTenh-Core]",54590,"noted","2017-05-05T12:43:26.930","2017-05-06T08:09:32.613","","","Rel-14","","","NB_IOTenh-Core","","","","","","","","",""]
["R4-1705460","CR on 36.133: NPRACH repetition level selection in NB-IoT","Ericsson","Joakim Axmon","62375","CR","Approval","NPRACH repetition level selection has been identified as one area of improvement for NB-IoT. Compared to legacy there is a loss of radio propagation diversity as the UE cat NB1 device only has a single Rx branch, and only is mandated to conduct RSRP measu","","194","7.17.3.2.2","Random access [NB_IOTenh-Core]",54600,"noted","2017-05-05T12:43:26.947","2017-05-06T08:09:32.630","","","Rel-14","36.133","14.3.0","NB_IOTenh-Core","4976","","B","","","","","",""]
["R4-1705461","Improved CE level selection for RACH in feMTC","Ericsson","Joakim Axmon","62375","discussion","Discussion","Selection of PRACH repetition level under CE has been identified as one area where improvements under the feMTC WI are desirable. In this contribution we are investigating the diversity gains that come from carrying out RSRP measurements over 2 TX ports,","","215","7.18.3.2.3","Random access [LTE_feMTC-Core]",50220,"noted","2017-05-05T12:43:27.820","2017-05-06T08:09:32.630","","","Rel-14","","","LTE_feMTC-Core","","","","","","","","",""]
["R4-1705462","CR on 36.133: PRACH repetition level selection","Ericsson","Joakim Axmon","62375","CR","Approval","PRACH repetition level selection has been identified as one area of improvement in the feMTC WI. Compared to legacy there is a loss of radio propagation diversity as the f/eMTC device only has a single Rx branch, and currently only is mandated to conduct","","215","7.18.3.2.3","Random access [LTE_feMTC-Core]",54620,"noted","2017-05-05T12:43:27.850","2017-05-06T08:09:32.630","","","Rel-14","36.133","14.3.0","LTE_feMTC-Core","4977","","B","","","","","",""]
["R4-1705463","MIMO OTA Harmonization - Results of First Set of Bands","CTTC","David Sanchez-hernandez","44508","other","Approval","RAN4 is currently analyzing the MIMO OTA harmonization across test methodologies, and has a test plan in force to conclude on the first set of bands [1]. This contribution analyses the harmonization results using the data made available by the single test","","146","7.11.3","Harmonization [LTE_MIMO_OTA-Core]",54630,"revised","2017-05-05T12:51:59.727","2017-05-05T13:27:56.613","","R4-1705920","Rel-13","","","LTE_MIMO_OTA","","","","","","","","",""]
["R4-1705464","TP for TR36.714-03-01: delta Tib/Rib values for CA_39C-42A_BCS0","ZTE Corporation","Shengxiang Guo","72253","pCR","","This contribution provide a text proposal on delta Tib/Rib values for CA_3DL_39C-42A_1UL_BCS0 for TR36.714-03-01","","101","7.3.2","UE RF (36.101) [LTE_CA_R14_3DL1UL-Core]",54650,"approved","2017-05-05T12:52:34.107","2017-05-06T07:57:52.160","","","Rel-14","36.714-03-01","0.8.0","LTE_CA_R14_3DL1UL-Core","","","","","","","","",""]
["R4-1705465","TP for TR36.714-03-01: delta Tib/Rib values for CA_39C-42A_BCS0","ZTE Corporation","Shengxiang Guo","72253","pCR","","This contribution provide a text proposal on delta Tib/Rib values for CA_3DL_39C-42A_1UL_BCS0 for TR36.714-03-01","","101","7.3.2","UE RF (36.101) [LTE_CA_R14_3DL1UL-Core]",578100,"withdrawn","2017-05-05T12:53:33.887",null,"","","Rel-14","36.714-03-01","0.8.0","LTE_CA_R14_3DL1UL-Core","","","","","","","","",""]
["R4-1705466","Simplified sectorized MPAC for RRM/Demodulation baseline","Keysight Technologies UK Ltd","Moray Rumney","6630","other","Approval","","","465","10.7.4.1","Baseline measurement setup [FS_NR_test_methods]",583400,"withdrawn","2017-05-05T13:21:58.253","2017-05-06T19:31:50.580","","","","","","","","","","","","","","",""]
["R4-1705467","Simplified sectorized MPAC for RRM/Demodulation baseline","Keysight Technologies UK Ltd","Moray Rumney","6630","other","Approval","","","465","10.7.4.1","Baseline measurement setup [FS_NR_test_methods]",583800,"withdrawn","2017-05-05T13:22:29.417",null,"","","","","","","","","","","","","","",""]
["R4-1705468","Discussion on output power dynamic requirement of NR BS","ZTE Corporation","Fei Xue","59676","other","Approval","","","442","10.5.3.4","Other Tx requirements [NR_newRAT]",581200,"noted","2017-05-05T13:25:35.913","2017-05-06T09:27:52.880","","","","","","","","","","","","","","",""]
["R4-1705469","Test cases for measurement reporting on connected mode under high speed scenario","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","Agreement","","","261","7.25.3","RRM performance (36.133) [LTE_high_speed-Perf]",54340,"revised","2017-05-05T14:01:27.757","2017-05-06T11:56:27.273","R4-1704249","R4-1706039","Rel-14","36.133","14.3.0","LTE_high_speed-Perf","4814","2","B","","","","","",""]
["R4-1705470","Applicability of requirements for UE Cat.NB2","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","Agreement","","","197","7.17.3.2.5","Others [NB_IOTenh-Core]",49850,"revised","2017-05-05T14:01:30.723","2017-05-06T11:56:27.287","R4-1703616","R4-1706264","Rel-14","36.133","14.3.0","NB_IOTenh-Core","4761","2","B","","","","","",""]
["R4-1705471","Link-budget coverage analysis of TRP/TRS requirements on network","TELECOM ITALIA S.p.A.","Paolo Goria","23040","other","Discussion","This contribution starts from way-forward approved at RAN4#82bis meeting, focusing on impacts on coverage of network pointed in the way-forward and exploiting a link-budget coverage analysis of the TRP/TRS values on network for such purpose.","","140","7.10.2","Hand phantom for smartphones [LTE_UTRA_TRP_TRS-Core]",610300,"noted","2017-05-05T14:44:26.243","2017-05-05T15:36:19.430","","","","","","","","","","","","","","",""]
["R4-1705472","Evaluation criteria for multi-node outage tests for Rel-13 LAA","Ericsson","Rahman Imadur","57720","discussion","Approval","In this contribution, we provide discussions related to different traffic test cases and our proposals related to this for multi-node tests.","","84","6.1.3","Outage Test [FS_LTE_LAA_multinode_test]",0,"withdrawn","2017-05-05T14:45:31.777",null,"","","Rel-13","","","FS_LTE_LAA_multinode_test","","","","","","","","",""]
["R4-1705473","Removing notes in two tables in UE spec wrt applicability of UL and DL requirements for band 46","Ericsson","Rahman Imadur","57720","CR","Approval","Removing notes in two tables in 36.101with respect to applicability of UL and DL requirements for band 46","","161","7.14.2","UE RF Maintenance(36.101) [LTE_eLAA-Core]",54730,"revised","2017-05-05T14:45:31.827","2017-05-05T14:54:54.050","","R4-1705862","Rel-14","36.101","14.3.0","LTE_eLAA-Core","4465","","F","","","","","",""]
["R4-1705474","Corrections to Tables in Rel-14 MBS performance requirements","NextNav, AT&T","Bill Shvodian","61097","CR","Agreement","Correction to the precision of the code phase accuracy to 1 ns and correction of typographical errors.","","252","7.23.2.2","RAT-independent enhancement [UTRA_LTE_iPos_enh2-Perf]",582100,"withdrawn","2017-05-05T14:50:51.677",null,"","","Rel-14","37.171","14.1.0","UTRA_LTE_iPos_enh2-Perf","0015","","F","","","","","",""]
["R4-1705475","Way forward on multi-node tests","Qualcomm, Ericsson, Huawei, HiSilicon, Nokia, Alcatel-Lucent, Shanghai Bell, Skyworks, AT&T, T-Mobile USA, Verizon, Deutsche Telekom, Vodafone","Marco Papaleo","49190","other","Discussion","In this contribution we propose a Way Forward to finalize the multi-node tests study item.","","82","6.1.1","General [FS_LTE_LAA_multinode_test]",51790,"noted","2017-05-05T14:50:55.250","2017-05-06T19:17:52.127","","","","","","FS_LTE_LAA_multinode_test","","","","","","","","",""]
["R4-1705476","TP for TR 36.789: update on section 6.2","Qualcomm Incorporated, Huawei, Ericsson, Nokia","Marco Papaleo","49190","pCR","Approval","In this TP for TR 36.789 we provide the text procedure for the outage tests described in section 6.2.","","84","6.1.3","Outage Test [FS_LTE_LAA_multinode_test]",54760,"noted","2017-05-05T14:50:57.277","2017-05-06T19:17:52.127","","","Rel-13","36.789","0.0.3","FS_LTE_LAA_multinode_test","","","","","","","","",""]
["R4-1705477","UE minimum output power requirement for mmW","Qualcomm Incorporated","Marco Papaleo","49190","other","Approval","In this contribution we discuss the UE minimum output power requirement for NR operating in mmW bands. We provide proposals based on system level and minimum coupling loss analysis.","","430","10.4.3.4","Other Tx requirements [NR_newRAT]",574100,"noted","2017-05-05T14:50:57.403","2017-05-06T19:17:52.127","","","","","","NR_newRAT","","","","","","","","",""]
["R4-1705478","UE ACLR, ACS and IBB requirements for mmW","Qualcomm Incorporated","Marco Papaleo","49190","other","Approval","In this contribution we propose UE ACLR, ACS and IBB requirements for mmW.","","422","10.3.5","ACLR and ACS [NR_newRAT]",574300,"noted","2017-05-05T14:50:57.447","2017-05-06T19:17:52.127","","","","","","NR_newRAT","","","","","","","","",""]
["R4-1705479","LAA REFSENS exclusion range in case of two contiguous UL licensed carriers","Qualcomm Incorporated","Marco Papaleo","49190","other","Approval","In this contribution we discuss the extension of B46 REFSENS exclusion region in case of 2 UL intra-band contiguous CA in licensed carriers.","","34","5.3.1","UE RF core (36.101) [LTE_LAA-Core]",577300,"approved","2017-05-05T14:50:57.480","2017-05-06T19:17:52.143","","","","","","LTE_LAA-Core","","","","","","","","",""]
["R4-1705480","Discussion on receiver spurious emission requirement of NR BS","ZTE Corporation","Fei Xue","59676","other","Approval","","","446","10.5.4.3","Other Rx requirements [NR_newRAT]",55010,"noted","2017-05-05T14:51:06.310","2017-05-06T09:27:52.913","","","","","","","","","","","","","","",""]
["R4-1705481","Discussion on TAE requirement of NR BS","ZTE Corporation","Fei Xue","59676","other","Approval","","","441","10.5.3.3","TAE requirements [NR_newRAT]",54810,"noted","2017-05-05T14:52:29.550","2017-05-06T09:27:52.913","","","","","","","","","","","","","","",""]
["R4-1705482","LTE450_Europe_PPDR: Performance Part","Airbus DS SLC","Eric Georgeaux","38175","discussion","Discussion","The main required changes required by the Performance Part of the work item LTE450_Europe_PPDR are presented in this contribution","","310","9.2.4","Other specifications [LTE450_Europe_PPDR]",54820,"noted","2017-05-05T14:54:26.987","2017-05-05T15:17:02.410","","","Rel-15","","","LTE450_Europe_PPDR-Perf","","","","","","","","",""]
["R4-1705483","TP for TR36.714-05-01: delta Tib/Rib values for CA_39C-42D_BCS0","ZTE Corporation","Shengxiang Guo","72253","pCR","","This contribution provide a text proposal on delta Tib/Rib values for CA_5DL_39C-42D_1UL_BCS0 for TR36.714-05-01","","113","7.5.2","UE RF (36.101) [LTE_CA_R14_5DL1UL-Core]",577200,"approved","2017-05-05T14:54:31.617","2017-05-06T07:57:52.207","","","Rel-14","36.714-05-01","0.7.0","LTE_CA_R14_5DL1UL-Core","","","","","","","","",""]
["R4-1705484","Discussion on CRS muting","Ericsson","Chunhui Zhang","71195","discussion","Approval","In this paper, we dicuss the CRS muting on the different RAN4 aspect, namely RRM and RF and UE implementation.","","395","9.15.1","General [LTE_eMTC4]",573300,"noted","2017-05-05T14:55:18.347","2017-05-05T15:36:37.827","","","Rel-15","","","LTE_eMTC4","","","","","","","","",""]
["R4-1705485","efeMTC Work Plan","Ericsson","Chunhui Zhang","71195","Work Plan","Approval","We propose to adopt the above workplan for RF work for latency WI.","","394","9.15","Even further enhanced MTC for LTE [LTE_eMTC4]",54840,"approved","2017-05-05T14:55:18.370","2017-05-05T15:36:37.840","","","Rel-15","","","","","","","","","","","",""]
["R4-1705486","System simulation assumption for low power class BL UE","Ericsson","Chunhui Zhang","71195","discussion","Approval","In this contribution, the system level simulation assumption is discussed for the new low output power BL UE","","397","9.15.2.1","Lower power class [LTE_eMTC4-core]",54860,"approved","2017-05-05T14:55:18.410","2017-05-05T15:36:37.827","","","Rel-15","","","LTE_eMTC4","","","","","","","","",""]
["R4-1705487","Refsens for feMTC in R14","Ericsson","Chunhui Zhang","71195","discussion","Approval","This paper investigates the R13 eMTC REFSENS open issues and propose no tightening for R13 CAT-M1 REFSENS, the REFSENS for both R13 CAT M1 and R14 CAT M2 UE are proposed based on previous agreement.","","207","7.18.2.2","REFSENS [LTE_feMTC-Core]",54870,"noted","2017-05-05T14:55:18.427","2017-05-05T15:36:37.827","","","Rel-14","","","LTE_feMTC-Core","","","","","","","","",""]
["R4-1705488","CR for CAT-M2 REFSENS, MPR and adding note for protection band 5","Ericsson","Chunhui Zhang","71195","draftCR","Endorsement","Adding MPR, REFSENS for CAT-M2","","207","7.18.2.2","REFSENS [LTE_feMTC-Core]",54880,"noted","2017-05-05T14:55:18.437","2017-05-05T15:36:37.827","","","Rel-14","36.101","14.3.0","LTE_feMTC-Core","","","","","","","","",""]
["R4-1705489","CR for removing bracket  in A-MPR table for NS_7","Ericsson","Chunhui Zhang","71195","draftCR","Endorsement","Removing bracket in A-MPR table for NS_7","","206","7.18.2.1","MPR/A-MPR [LTE_feMTC-Core]",54890,"endorsed","2017-05-05T14:55:18.667","2017-05-05T15:36:37.827","","","Rel-14","36.101","14.3.0","LTE_feMTC-Core","","","","","","","","",""]
["R4-1705490","Discussion on OTA testability of Transmission ON/OFF power of NR BS","ZTE Corporation","Fei Xue","59676","other","Approval","","","442","10.5.3.4","Other Tx requirements [NR_newRAT]",54900,"noted","2017-05-05T14:55:25.377","2017-05-06T09:27:52.913","","","","","","","","","","","","","","",""]
["R4-1705491","TP for TR 37.843 on testing EMC immunity for OTA AAS BS - general section","Ericsson","Bjoern Flach","60350","pCR","Approval","This contribution is adding background information for the general section of the EMC radiated immunity section.","","364","9.12.2.7","EMC requirements [AASenh_BS_LTE_UTRA-Core]",54940,"revised","2017-05-05T15:01:15.387","2017-05-06T13:27:52.223","","R4-1706148","Rel-15","37.843","0.2.0","AASenh_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-1705492","TP for TR 37.843 on testing EMC immunity for OTA AAS BS - measurement setup","Ericsson","Bjoern Flach","60350","pCR","Approval","This contribution is adding measurement setup description and requirements for the EMC radiated immunity section.","","364","9.12.2.7","EMC requirements [AASenh_BS_LTE_UTRA-Core]",578300,"revised","2017-05-05T15:01:20.287","2017-05-06T13:27:52.240","","R4-1706149","Rel-15","37.843","0.2.0","AASenh_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-1705493","TP for TR 37.843 EMC immunity for OTA AAS BS ? frequency boundaries and limits","Ericsson","Bjoern Flach","60350","pCR","Approval","This contribution proposes frequency boundaries and limits for radiated immunity testing which aims to provide a radiated immunity test method which does not risk to result in an inoperable receiver","","364","9.12.2.7","EMC requirements [AASenh_BS_LTE_UTRA-Core]",614700,"noted","2017-05-05T15:01:20.393","2017-05-06T13:27:52.240","","","Rel-15","37.843","0.2.0","AASenh_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-1705494","How to combine OTA RF and EMC requirements","Ericsson","Bjoern Flach","60350","discussion","Approval","This contribution is discussing the strategy on how to introduce the OTA AAS BS RF and EMC requirements which will be utilizing the same test methods and limits","","364","9.12.2.7","EMC requirements [AASenh_BS_LTE_UTRA-Core]",54910,"noted","2017-05-05T15:01:20.487","2017-05-06T13:27:52.240","","","Rel-15","","","AASenh_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-1705495","General OOB blocking challenges","Ericsson","Bjoern Flach","60350","discussion","Approval","This contribution discusses the challenges performing OOB blocking testing OTA using traditional test equipment and ordinary anechoic shielded chambers","","363","9.12.2.6","Other Receiver requirements [AASenh_BS_LTE_UTRA-Core]",56490,"noted","2017-05-05T15:01:20.503","2017-05-06T13:27:52.240","","","Rel-15","","","AASenh_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-1705496","Simulation results for eLAA PUSCH","Nokia, Alcatel-Lucent Shanghai Bell","Riikka Nurminen","70015","discussion","Discussion","Simulation results for eLAA PUSCH demodulation performance.","","166","7.14.7","BS demodulation (36.104/36.141) [LTE_eLAA-Perf]",55160,"noted","2017-05-05T15:01:22.470","2017-05-05T18:15:05.967","","","","","","LTE_eLAA-Perf","","","","","","","","",""]
["R4-1705497","Support of FS3-only sTAGs in eLAA","Nokia, Alcatel-Lucent Shanghai Bell","Riikka Nurminen","70015","discussion","Discussion","Further discussion on the support of FS3-only sTAGs in eLAA.","","164","7.14.5","RRM core Maintenance (36.133) [LTE_eLAA-Core]",51410,"noted","2017-05-05T15:01:22.533","2017-05-05T18:15:05.967","","","","","","LTE_eLAA-Core","","","","","","","","",""]
["R4-1705498","Addition of FS3-only sTAG support","Nokia, Alcatel-Lucent Shanghai Bell","Riikka Nurminen","70015","CR","Approval","Addition of the definition of reliability of an FS3 cell as timing reference and the support of FS3-only sTAGs for eLAA.","","164","7.14.5","RRM core Maintenance (36.133) [LTE_eLAA-Core]",55940,"revised","2017-05-05T15:01:22.547","2017-05-05T18:15:05.980","","R4-1705971","Rel-14","36.133","14.3.0","LTE_eLAA-Core","4978","","B","","","","","",""]
["R4-1705499","Further discussion on shortened TTI RRM impacts","Nokia, Alcatel-Lucent Shanghai Bell","Riikka Nurminen","70015","discussion","Discussion","Discussion on possible RRM impacts of short TTI based on the WF agreed in the Spokane meeting.","","383","9.13.4.1","TA adjustment delay [LTE_sTTIandPT-core]",54990,"noted","2017-05-05T15:01:23.500","2017-05-05T18:15:05.980","","","","","","LTE_sTTIandPT","","","","","","","","",""]
["R4-1705500","Discussion on ACS and Narrowband Blocking requirement of mmWave NR BS","ZTE Corporation","Fei Xue","59676","other","Approval","","","446","10.5.4.3","Other Rx requirements [NR_newRAT]",56330,"withdrawn","2017-05-05T15:01:49.817",null,"","","","","","","","","","","","","","",""]
["R4-1705501","Discussion on ACS and Narrowband Blocking requirement of mmWave NR BS","ZTE Corporation","Fei Xue","59676","other","Approval","","","446","10.5.4.3","Other Rx requirements [NR_newRAT]",576700,"withdrawn","2017-05-05T15:01:52.093",null,"","","","","","","","","","","","","","",""]
["R4-1705502","Discussion on ACS and Narrowband Blocking requirement of mmWave NR BS","ZTE Corporation","Fei Xue","59676","other","Approval","","","446","10.5.4.3","Other Rx requirements [NR_newRAT]",55020,"noted","2017-05-05T15:01:55.370","2017-05-06T09:27:52.943","","","","","","","","","","","","","","",""]
["R4-1705503","Text Proposal for Section 7.2 of TR36.748","Airbus DS SLC","Eric Georgeaux","38175","other","Approval","","","306","9.2","450MHz E-UTRA FDD Band for LTE PPDR and PMR/PAMR in Europe [LTE450_Europe_PPDR]",55030,"revised","2017-05-05T15:19:25.817","2017-05-05T15:36:45.340","","R4-1705884","Rel-15","36.748","","LTE450_Europe_PPDR","","","","","","","","",""]
["R4-1705504","Text Proposal for Section 6 of TR36.748","Airbus DS SLC","Eric Georgeaux","38175","other","Approval","","","306","9.2","450MHz E-UTRA FDD Band for LTE PPDR and PMR/PAMR in Europe [LTE450_Europe_PPDR]",55040,"approved","2017-05-05T15:35:31.443","2017-05-05T15:36:45.340","","","Rel-15","36.748","","LTE450_Europe_PPDR","","","","","","","","",""]
["R4-1705505","TR36.748 v0.3.0","Airbus DS SLC","Eric Georgeaux","38175","draft TR","Approval","Update of the TR with the Text Proposals agreed at RAN4 meeting #83","","306","9.2","450MHz E-UTRA FDD Band for LTE PPDR and PMR/PAMR in Europe [LTE450_Europe_PPDR]",55050,"approved","2017-05-05T15:54:11.930","2017-05-23T15:07:51.600","","","Rel-15","36.748","0.3.0","LTE450_Europe_PPDR","","","","","","","","",""]
["R4-1705506","Band 71 UE PA Emissions REFSENS Impact for 20MHz Channel Bandwidth","Skyworks Solutions Inc.","Dominique Brunel","65099","discussion","Discussion","In this contribution measured PA noise contribution in 20MHz receive channels including transceiver impairment is presented. Based on this value and agreed system assumptions a proposal for the 20MHz REFSENS specification is made.","","336","9.8.2","UE RF (36.101) [LTE600_US-core]",568300,"noted","2017-05-05T16:13:36.847","2017-05-06T05:37:52.860","","","","","","","","","","","","","","",""]
["R4-1705507","Band 71 UE Split Duplexer Support","Skyworks Solutions Inc.","Dominique Brunel","65099","discussion","Approval","This contribution discusses the dual duplexer approach and its ability to enable all allocated 20MHz channels. A proposal is made to capture this possibility with the supported channel bandwidth table in 36.101 specification.","","336","9.8.2","UE RF (36.101) [LTE600_US-core]",51600,"approved","2017-05-05T16:15:52.603","2017-05-06T05:37:52.893","","","","","","","","","","","","","","",""]
["R4-1705508","CR on idle mode requirements for eMTC in R13","Nokia, Alcatel-Lucent Shanghai Bell, Qualcomm, Intel, Huawei, HiSilicon","Li Zhang","46368","CR","Agreement","CR on idle mode requirements for eMTC","","46","5.4.3.1","BL/CE UE [LTE_MTCe2_L1-Core]",571400,"revised","2017-05-05T16:36:20.113","2017-05-06T12:17:52.747","R4-1704251","R4-1705996","Rel-13","36.133","13.7.0","LTE_MTCe2_L1-Core","4831","1","F","","","","","",""]
["R4-1705509","Power Class Definition for sub-6GHz NR","Skyworks Solutions Inc.","Dominique Brunel","65099","discussion","Approval","In this contribution we come back to the different types of waveforms and related PA back-off in order to propose sub-6GHz power class including power boost options that enables the HPUE concept within the 23dBm power class definition.","","427","10.4.3.1","UE power class and MPR/A-MPR [NR_newRAT]",52030,"noted","2017-05-05T16:37:44.357","2017-05-06T05:37:52.907","","","","","","","","","","","","","","",""]
["R4-1705510","CR on idle mode requirements for feMTC","Nokia, Alcatel-Lucent Shanghai Bell","Li Zhang","46368","CR","Approval","CR on idle mode requirements for feMTC","","214","7.18.3.2.2","Idle mode and handover [LTE_feMTC-Core]",55100,"revised","2017-05-05T16:39:26.157","2017-05-06T12:17:52.763","R4-1704168","R4-1705983","Rel-14","36.133","14.3.0","LTE_feMTC-Core","4821","2","F","","","","","",""]
["R4-1705511","Wideband UL Signal ACLR Specification for Reduced MPR","Skyworks Solutions Inc.","Dominique Brunel","65099","discussion","Approval","In this contribution two different approaches to the ACLR specification for wide bandwidths signals are discussed and propose to adopt a new approach resulting in lower MPR versus bandwidth without impacting the system behaviour. Although this proposal is","","427","10.4.3.1","UE power class and MPR/A-MPR [NR_newRAT]",52470,"noted","2017-05-05T16:40:30.233","2017-05-06T05:37:52.907","","","","","","","","","","","","","","",""]
["R4-1705512","MSD for xDL/2UL CA","Qualcomm Incorporated","Prashanth Akula","67450","other","Approval","","","125","7.7.2","UE RF (36.101) [LTE_CA_R14_xDL2UL-Core]",51900,"noted","2017-05-05T16:50:24.357","2017-05-05T19:26:05.247","","","","","","","","","","","","","","",""]
["R4-1705513","Further discussion on eLAA performance requirements","Huawei","Xiang (Steven) Chen","41576","discussion","Discussion","In this contribution, we discuss the left issues for eLAA demodulation test: the number of contiguous interlace resource allocation and joint channel estimation, the UL burst transmission model","","166","7.14.7","BS demodulation (36.104/36.141) [LTE_eLAA-Perf]",55140,"noted","2017-05-05T17:02:43.377","2017-05-05T19:32:55.220","","","","","","LTE_eLAA-Perf","","","","","","","","",""]
["R4-1705514","Simulation assumptions for different number of interlace allocation for eLAA","Huawei","Xiang (Steven) Chen","41576","discussion","Discussion","This contribution provides the simulation assumptions for different number of interlaces allocation.","","166","7.14.7","BS demodulation (36.104/36.141) [LTE_eLAA-Perf]",56250,"noted","2017-05-05T17:02:43.393","2017-05-05T19:32:55.237","","","","","","LTE_eLAA-Perf","","","","","","","","",""]
["R4-1705515","Simulation results for eLAA with different number of interlace allocation","Huawei","Xiang (Steven) Chen","41576","discussion","Discussion","This contribution provides our simulation results for 1, 2, 5 and 7 contiguous interlaces allocation with joint channel estimation","","166","7.14.7","BS demodulation (36.104/36.141) [LTE_eLAA-Perf]",55150,"noted","2017-05-05T17:02:43.410","2017-05-05T19:32:55.237","","","","","","LTE_eLAA-Perf","","","","","","","","",""]
["R4-1705516","CR for PUSCH conformance test in TS 36.141","Huawei","Xiang (Steven) Chen","41576","CR","Agreement","This contribution provides the CR for eLAA PUSCH conformance test in TS 36.141","","166","7.14.7","BS demodulation (36.104/36.141) [LTE_eLAA-Perf]",56270,"noted","2017-05-05T17:02:43.423","2017-05-05T19:32:55.237","","","Rel-14","36.141","14.3.0","LTE_eLAA-Perf","1049","","B","","","","","",""]
["R4-1705517","Updated simulation results for BS IC with 2Rx without TO/FO","Huawei","Xiang (Steven) Chen","41576","discussion","Discussion","As per the agreed WF R4-1610661, provide our updated simulation results for 2Rx without TO/FO","","300","8.1.3","Link level evaluation [FS_LTE _IC_BS]",55190,"revised","2017-05-05T17:02:44.330","2017-05-05T19:32:55.237","","R4-1705988","","","","FS_LTE_IC_BS","","","","","","","","",""]
["R4-1705518","Updated simulation results for BS IC with 4Rx without TO/FO","Huawei","Xiang (Steven) Chen","41576","discussion","Discussion","As per the agreed WF R4-1610661, provide our updated simulation results for 4Rx  without TO/FO","","300","8.1.3","Link level evaluation [FS_LTE _IC_BS]",55200,"revised","2017-05-05T17:02:44.347","2017-05-05T19:32:55.253","","R4-1705989","","","","FS_LTE_IC_BS","","","","","","","","",""]
["R4-1705519","Simulation results for BS IC with 2Rx with TO/FO","Huawei","Xiang (Steven) Chen","41576","discussion","Discussion","As per the agreed simulation cases in WF R4-1702307, provide our simulation results for 2Rx 2UEs with TO/FO","","300","8.1.3","Link level evaluation [FS_LTE _IC_BS]",55230,"revised","2017-05-05T17:02:44.360","2017-05-05T19:32:55.253","","R4-1705990","","","","FS_LTE_IC_BS","","","","","","","","",""]
["R4-1705520","Simulation results for BS IC with 4Rx with TO/FO","Huawei","Xiang (Steven) Chen","41576","discussion","Discussion","As per the agreed simulation cases in WF R4-1702307, provide our simulation results for 4Rx 4UEs with TO/FO","","300","8.1.3","Link level evaluation [FS_LTE _IC_BS]",55240,"revised","2017-05-05T17:02:44.377","2017-05-05T19:32:55.253","","R4-1705991","","","","FS_LTE_IC_BS","","","","","","","","",""]
["R4-1705521","Discussion on MCS 21 with 64QAM selection in BS IC","Huawei","Xiang (Steven) Chen","41576","discussion","Discussion","As per the agreed WF R4-1610661, provide our view about MCS 21 with 64QAM selection in BS IC performance requirements definition","","298","8.1.1","General [FS_LTE _IC_BS]",573200,"noted","2017-05-05T17:02:44.393","2017-05-05T19:32:55.253","","","","","","FS_LTE_IC_BS","","","","","","","","",""]
["R4-1705522","Discussion on test metric and test case down selection for BS IC","Huawei","Xiang (Steven) Chen","41576","discussion","Discussion","As per the simulation results and observations, we provide our views about the test cases slection for the following WI.","","298","8.1.1","General [FS_LTE _IC_BS]",573100,"noted","2017-05-05T17:02:44.407","2017-05-05T19:32:55.267","","","","","","FS_LTE_IC_BS","","","","","","","","",""]
["R4-1705523","TP on simulation results updates for 2Rx and 4Rx without TO FO","Huawei","Xiang (Steven) Chen","41576","pCR","Approval","This TP captures our updated simulation results for both 2Rx and 4Rx without modelling of Timing Offset and Frequency Offset","","300","8.1.3","Link level evaluation [FS_LTE _IC_BS]",45570,"revised","2017-05-05T17:02:44.407","2017-05-05T19:32:55.267","","R4-1705992","Rel-15","36.766","1.0.0","FS_LTE_IC_BS","","","","","","","","",""]
["R4-1705524","TP on simulation results addition for 2Rx and 4Rx with TO FO","Huawei","Xiang (Steven) Chen","41576","pCR","Approval","This TP captures our simulation results for both 2Rx and 4Rx with modelling of Timing Offset and Frequency Offset","","300","8.1.3","Link level evaluation [FS_LTE _IC_BS]",45580,"revised","2017-05-05T17:02:44.500","2017-05-05T19:32:55.267","","R4-1705993","Rel-15","36.766","1.0.0","FS_LTE_IC_BS","","","","","","","","",""]
["R4-1705525","Discussion and simulation results for NB-IoT enhancements UE demodulation","Huawei, Hisilicon","Xiang (Steven) Chen","41576","discussion","Discussion","This contribution provides the initial ideal simulation results and corresponding observations as per the agreed simulation assumption R4-1704147 for NB-IoT UE demodulation performance","","202","7.17.6","UE demodulation(36.101) [NB_IOTenh-Perf]",46270,"noted","2017-05-05T17:02:44.547","2017-05-05T19:32:55.267","","","","","","NB_IOTenh-Perf","","","","","","","","",""]
["R4-1705526","Summary of NB-IoT enh UE simulation results","Huawei, Hisilicon","Xiang (Steven) Chen","41576","discussion","Discussion","This is the summary of simulation results for NB-IoT enhancements from companies","","202","7.17.6","UE demodulation(36.101) [NB_IOTenh-Perf]",55260,"noted","2017-05-05T17:02:44.580","2017-05-23T15:07:51.617","","","","","","NB_IOTenh-Perf","","","","","","","","",""]
["R4-1705527","Discussion on FeMBMS UE demodulation performance requirements","Huawei, Hisilicon","Xiang (Steven) Chen","41576","discussion","Discussion","As per the discussion during RAN4#82bis, we provide our views about the FeMBMS demodulation performance requirements","","157","7.13.5","Demodulation (36.101) [MBMS_LTE_enh2-Perf]",53690,"noted","2017-05-05T17:02:44.593","2017-05-05T19:32:55.283","","","","","","MBMS_LTE_enh2-Perf","","","","","","","","",""]
["R4-1705528","Correction on TDD-FDD CSI test cases (R13)","Huawei, Hisilicon","Xiang (Steven) Chen","41576","CR","Agreement","Square bracket removal and some corrections","","70","5.6.3","Demodulation and CSI [WI code or TEI13]",55280,"agreed","2017-05-05T17:02:44.610","2017-05-05T19:32:55.283","","","Rel-13","36.101","13.7.0","TEI13","4466","","F","RP-171311","","","","",""]
["R4-1705529","Correction on TDD-FDD CSI test cases (R14)","Huawei, Hisilicon","Xiang (Steven) Chen","41576","CR","Agreement","Mirror CR","","70","5.6.3","Demodulation and CSI [WI code or TEI13]",55290,"agreed","2017-05-05T17:02:45.607","2017-06-02T13:07:51.437","","","Rel-14","36.101","14.3.0","TEI13","4467","","A","RP-171311","","","","",""]
["R4-1705530","Motivation for new WI on LTE DL 8Rx antenna ports","Huawei, HiSilicon","Xiang (Steven) Chen","41576","other","Information","This paper provides the motivation for new WI on LTE DL 8Rx antenna ports.","","473","13","Revision of the Work Plan",55310,"noted","2017-05-05T17:02:46.483","2017-05-05T19:33:46.117","","","","","","","","","","","","","","",""]
["R4-1705531","New WI proposal: LTE DL 8Rx antenna ports","Huawei, HiSilicon","Xiang (Steven) Chen","41576","other","Information","This paper gives the description of new WI on LTE DL 8Rx antenna ports.","","473","13","Revision of the Work Plan",55750,"noted","2017-05-05T17:02:46.530","2017-05-05T19:33:46.117","","","","","","","","","","","","","","",""]
["R4-1705532","Simulation results for MUST case1 and case 2","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","Discussion","This paper provides the simulation reuslts for MUST case1 and case2.","","255","7.24.1.1","Case1 and Case 2 [LTE_MUST-Perf]",55320,"noted","2017-05-05T17:02:46.560","2017-05-05T19:33:46.130","","","","","","LTE_MUST-Perf","","","","","","","","",""]
["R4-1705533","Discussion on test cases for MUST Case3","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","Discussion","This paper provides the view on MUST case 3 and  the initial simulation results","","256","7.24.1.2","Case 3 [LTE_MUST-Perf]",47340,"noted","2017-05-05T17:02:46.577","2017-05-05T19:33:46.130","","","","","","LTE_MUST-Perf","","","","","","","","",""]
["R4-1705534","Discussion on MUST UE capability","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","Discussion","This paper provide the view on MUST UE capability.","","257","7.24.2","UE capbility [LTE_MUST]",47350,"noted","2017-05-05T17:02:46.607","2017-05-05T19:33:46.130","","","","","","LTE_MUST-Perf","","","","","","","","",""]
["R4-1705535","Clean up the requirements for UE enhancement in SFN scenario.","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","Agreement","This CR clean up the requirements for UE enhancement in SFN scenario.","","263","7.25.4.1","Enhancement for bi-directional RRH arrangement [LTE_high_speed-Perf]",55350,"revised","2017-05-05T17:02:46.623","2017-05-05T19:33:46.147","","R4-1706029","Rel-14","36.101","14.3.0","LTE_high_speed-Perf","4468","","F","","","","","",""]
["R4-1705536","PRACH simulation results","Huawei","Xiang (Steven) Chen","41576","discussion","Discussion","This paper provides impairment simualtion results for PRACH restricted set type B.","","266","7.25.5","BS demodulation (36.104/36.141) [LTE_high_speed-Perf]",55380,"noted","2017-05-05T17:02:49.413","2017-05-05T19:33:46.147","","","","","","LTE_high_speed-Perf","","","","","","","","",""]
["R4-1705537","Summary of the simulation results for PRACH","Huawei","Xiang (Steven) Chen","41576","other","Information","This summary is used for collecting the ideal and impairment simulation resutls for PRACH enhancement.","","266","7.25.5","BS demodulation (36.104/36.141) [LTE_high_speed-Perf]",53000,"noted","2017-05-05T17:02:49.430","2017-05-23T15:07:51.633","","","","","","LTE_high_speed-Perf","","","","","","","","",""]
["R4-1705538","CR for new PRACH performance requirements","Huawei","Xiang (Steven) Chen","41576","CR","Agreement","This CR introduces the specific requirements for PRACH restricted set type B.","","266","7.25.5","BS demodulation (36.104/36.141) [LTE_high_speed-Perf]",55390,"revised","2017-05-05T17:02:49.447","2017-05-05T19:33:46.147","R4-1704194","R4-1705967","Rel-14","36.104","14.3.0","LTE_high_speed-Perf","0976","2","B","","","","","",""]
["R4-1705539","CR for new PRACH conformance test","Huawei","Xiang (Steven) Chen","41576","CR","Agreement","This CR introduces the specific requirements for PRACH restricted set type B.","","266","7.25.5","BS demodulation (36.104/36.141) [LTE_high_speed-Perf]",573000,"revised","2017-05-05T17:02:50.413","2017-05-05T19:33:46.147","R4-1704195","R4-1705968","Rel-14","36.141","14.3.0","LTE_high_speed-Perf","1011","2","B","","","","","",""]
["R4-1705540","Simualtion results for FeMTC UE demodulation","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","Discussion","This paper provides the simualtion results for FeMTC UE demodulation","","227","7.18.8.1","BL/CE UE [LTE_feMTC-Perf]",621200,"noted","2017-05-05T17:02:51.473","2017-05-05T19:33:46.163","","","","","","LTE_feMTC-Perf","","","","","","","","",""]
["R4-1705541","Discussion on demodulation requirements for R14 Non-BL UE coverage enhancement.","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","Discussion","This paper provides the view on requirments applicability for Non-BL UE .","","228","7.18.8.2","Non-BL/CE UE [LTE_feMTC-Perf]",619600,"noted","2017-05-05T17:02:51.490","2017-05-05T19:33:46.163","","","","","","LTE_feMTC-Perf","","","","","","","","",""]
["R4-1705542","Discussion on demodulation requirements for R13 Non-BL UE coverage enhancement","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","Discussion","This paper provides the view on requirments applicability for Non-BL UE .","","54","5.4.6.2","Non-BL/CE UE [LTE_MTCe2_L1-Perf]",48120,"noted","2017-05-05T17:02:51.503","2017-05-05T19:33:46.163","","","","","","LTE_MTCe2_L1-Perf","","","","","","","","",""]
["R4-1705543","Discussion and simulation results for V2V PSSCH with small RBs","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","Discussion","In this contribution, we discuss V2V PSSCH tests and present simulation results.","","172","7.15.4.1","Single-link PSSCH and PSCCH [LTE_SL_V2V-Perf]",55450,"noted","2017-05-05T17:02:51.520","2017-05-05T19:35:29.517","","","","","","LTE_SL_V2V-Perf","","","","","","","","",""]
["R4-1705544","Discussion on resource pool configuration for V2V with small RBs","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","Discussion","In this contribution, we discuss V2V resource pool configuration.","","174","7.15.4.3","Others [LTE_SL_V2V-Perf]",55440,"noted","2017-05-05T17:02:51.537","2017-05-05T19:35:29.517","","","","","","LTE_SL_V2V-Perf","","","","","","","","",""]
["R4-1705545","Remaining issues for V2V demodulation requirements","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","Discussion","In this contribution, we discuss remaining issues for V2V demodulation requirements.","","172","7.15.4.1","Single-link PSSCH and PSCCH [LTE_SL_V2V-Perf]",49100,"noted","2017-05-05T17:02:51.550","2017-05-05T19:35:29.517","","","","","","LTE_SL_V2V-Perf","","","","","","","","",""]
["R4-1705546","CR for V2V FRCs","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","Agreement","This CR gives V2V FRC configurations.","","171","7.15.4","UE demodulation (36.101) [LTE_SL_V2V-Perf]",601900,"revised","2017-05-05T17:02:51.567","2017-05-05T19:35:29.530","","R4-1706206","Rel-14","36.101","14.3.0","LTE_SL_V2V-Perf","4469","","B","","","","","",""]
["R4-1705547","CR for V2V resource pool configuration","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","Agreement","This CR gives V2V resource pool configuration.","","174","7.15.4.3","Others [LTE_SL_V2V-Perf]",55470,"revised","2017-05-05T17:02:52.690","2017-05-05T19:35:29.530","","R4-1705970","Rel-14","36.101","14.3.0","LTE_SL_V2V-Perf","4470","","B","","","","","",""]
["R4-1705548","Discussion on PSSCH and PSCCH decoding capability tests for V2X","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","Discussion","In this contribution, we disucss PSSCH and PSCCH decoding capability tests for V2X.","","181","7.16.5.1","PSSCH/PSCCH maximum processing capability test [LTE_V2X-Perf]",55480,"noted","2017-05-05T17:02:53.610","2017-05-05T19:35:29.547","","","","","","LTE_V2X-Perf","","","","","","","","",""]
["R4-1705549","Discussion on PSBCH requirements for V2X","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","Discussion","In this contribution, we discuss new requirements for V2X.","","182","7.16.5.2","PSBCH, eNB sync and WAN SDR [LTE_V2X-Perf]",56300,"noted","2017-05-05T17:02:53.627","2017-05-05T19:35:29.563","","","","","","LTE_V2X-Perf","","","","","","","","",""]
["R4-1705550","Discussion on other requirements for V2X","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","Discussion","In this contribution, we discuss other requirements for V2X.","","182","7.16.5.2","PSBCH, eNB sync and WAN SDR [LTE_V2X-Perf]",49390,"noted","2017-05-05T17:02:53.640","2017-05-05T19:35:29.563","","","","","","LTE_V2X-Perf","","","","","","","","",""]
["R4-1705551","Summary of simulation results for V2X demodulation requirements","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","Discussion","In this contribution, we provide summary of V2X demodulation results.","","183","7.16.5.3","Others [LTE_V2X-Perf]",55500,"noted","2017-05-05T17:02:53.657","2017-05-23T15:07:51.647","","","","","","LTE_V2X-Perf","","","","","","","","",""]
["R4-1705552","Further discussion on enhanced SU-MIMO scenarios","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","Discussion","In this contribution, we further discuss  enhanced SU-MIMO further study cases.","","279","7.27.3","SU-MIMO IM [LTE_eCRSIM_eSUMIMO]",49400,"noted","2017-05-05T17:02:53.673","2017-05-05T19:35:29.563","","","","","","LTE_eCRSIM_eSUMIMO","","","","","","","","",""]
["R4-1705553","Draft CR for enhanced SU-MIMO performance requirements","Huawei, HiSilicon","Xiang (Steven) Chen","41576","draftCR","Endorsement","In this draft CR, we give the technical test structrue for enhanced SU-MIMO test cases.","","279","7.27.3","SU-MIMO IM [LTE_eCRSIM_eSUMIMO]",55540,"endorsed","2017-05-05T17:02:53.687","2017-05-05T19:35:29.563","","R4-1706163","Rel-14","36.101","14.3.0","LTE_eCRSIM_eSUMIMO","","","B","","","","","",""]
["R4-1705554","Draft CR for enhanced SU-MIMO FRCs","Huawei, HiSilicon","Xiang (Steven) Chen","41576","draftCR","Endorsement","In this draft CR, we give the technical test structrue for enhanced SU-MIMO FRCs.","","279","7.27.3","SU-MIMO IM [LTE_eCRSIM_eSUMIMO]",56310,"endorsed","2017-05-05T17:02:53.703","2017-05-05T19:35:29.577","","R4-1706164","Rel-14","36.101","14.3.0","LTE_eCRSIM_eSUMIMO","","","B","","","","","",""]
["R4-1705555","TR 36.747 v0.3.0 for enhanced SU-MIMO and CRS-IM receiver","Huawei, HiSilicon","Xiang (Steven) Chen","41576","other","Approval","We provide the draft TR by capturing the agreements reached in previous meeting.","","274","7.27.1","General [LTE_eCRSIM_eSUMIMO]",55550,"approved","2017-05-05T17:02:53.720","2017-05-05T19:35:29.577","","","","","","LTE_eCRSIM_eSUMIMO","","","","","","","","",""]
["R4-1705556","Note on BS in-channel selectivity for NB-IoT","Huawei, Nokia, Alcatel-Lucent Shanghai Bell","Liehai Liu","47239","CR","Agreement","","","59","5.5.2","BS RF core(36.104) [NB_IOT-Core]",54120,"agreed","2017-05-05T17:05:24.513","2017-05-05T17:33:46.030","","","Rel-13","36.104","13.7.0","NB_IOT-Core","4683","","F","RP-171299","","","","",""]
["R4-1705557","Discussion on remaining issues for 4Rx CA tests","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","Discussion","In this contribution, we discuss remaining issues for 4Rx CA tests, including 256QAM and 3/4-layer tests.","","244","7.21.2","UE demodulation (36.101) [LTE_4Rx_AP_DL_CA-Perf]",53600,"noted","2017-05-05T17:02:54.110","2017-05-05T19:35:29.577","","","","","","LTE_4Rx_AP_DL_CA","","","","","","","","",""]
["R4-1705558","Discussion on BS requirements for eFD-MIMO","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","Discussion","In this contribution, we will discusion performance for eFD-MIMO.","","288","7.28.3","Others [LTE_eFDMIMO-Perf]",55580,"noted","2017-05-05T17:02:54.140","2017-05-05T19:35:29.577","","","","","","LTE_eFDMIMO-Perf","","","","","","","","",""]
["R4-1705559","Discussion on Semi-open loop performance requirements for eFD-MIMO","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","Discussion","In this contribution, we will discusion performance for eFD-MIMO.","","283","7.28.2.1","Semi-open-loop transmission [LTE_eFDMIMO-Perf]",55590,"noted","2017-05-05T17:02:54.157","2017-05-05T19:35:29.577","","","","","","LTE_eFDMIMO-Perf","","","","","","","","",""]
["R4-1705560","Discussion on Class A PMI performance requirements for eFD-MIMO","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","Discussion","In this contribution, we will discusion performance for eFD-MIMO.","","284","7.28.2.2","Class A PMI [LTE_eFDMIMO-Perf]",575200,"noted","2017-05-05T17:02:54.157","2017-05-05T19:35:29.593","","","","","","LTE_eFDMIMO-Perf","","","","","","","","",""]
["R4-1705561","Discussion on advanced CSI requirements for eFD-MIMO","Huawei, HiSilicon","Xiang (Steven) Chen","41576","discussion","Discussion","In this contribution, we will discusion performance for eFD-MIMO.","","285","7.28.2.3","Advanced CSI [LTE_eFDMIMO-Perf]",55610,"noted","2017-05-05T17:02:54.173","2017-05-05T19:35:29.593","","","","","","LTE_eFDMIMO-Perf","","","","","","","","",""]
["R4-1705562","Corrections for inCoverage configuration in ProSe direct communication (Rel-12)","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","Agreement","In this CR, we provide corrections for inCoverage configuration.","","16","4.2.4","UE demodulation performance [WI code or TEI12]",55620,"revised","2017-05-05T17:02:54.173","2017-05-05T19:35:29.593","","R4-1706020","Rel-12","36.101","12.15.0","TEI12","4471","","F","","","","","",""]
["R4-1705563","Corrections for inCoverage configuration in ProSe direct communication (Rel-13)","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","Agreement","In this CR, we provide corrections for inCoverage configuration.","","16","4.2.4","UE demodulation performance [WI code or TEI12]",55630,"agreed","2017-05-05T17:02:55.077","2017-05-23T15:07:51.647","","","Rel-13","36.101","13.7.0","TEI12","4472","","A","RP-171297","","","","",""]
["R4-1705564","Corrections for inCoverage configuration in ProSe direct communication (Rel-14)","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","Agreement","In this CR, we provide corrections for inCoverage configuration.","","16","4.2.4","UE demodulation performance [WI code or TEI12]",55640,"agreed","2017-05-05T17:02:55.950","2017-05-23T15:07:51.647","","","Rel-14","36.101","14.3.0","TEI12","4473","","A","RP-171297","","","","",""]
["R4-1705565","Note on BS in-channel selectivity for NB-IoT","Huawei, Nokia, Alcatel-Lucent Shanghai Bell","Liehai Liu","47239","CR","Agreement","","","59","5.5.2","BS RF core(36.104) [NB_IOT-Core]",54130,"agreed","2017-05-05T17:05:26.290","2017-05-23T15:07:51.663","","","Rel-14","36.104","14.3.0","NB_IOT-Core","4684","","A","RP-171299","","","","",""]
["R4-1705566","Note on BS in-channel selectivity for NB-IoT","Huawei, Nokia, Alcatel-Lucent Shanghai Bell","Liehai Liu","47239","CR","Agreement","","","61","5.5.4","BS RF Conformance testing (36.141) [NB_IOT-Perf]",54110,"agreed","2017-05-05T17:05:27.757","2017-05-05T17:33:46.013","","","Rel-13","36.141","13.7.0","NB_IOT-Perf","1050","","F","RP-171300","","","","",""]
["R4-1705567","Note on BS in-channel selectivity for NB-IoT","Huawei, Nokia, Alcatel-Lucent Shanghai Bell","Liehai Liu","47239","CR","Agreement","","","61","5.5.4","BS RF Conformance testing (36.141) [NB_IOT-Perf]",54160,"agreed","2017-05-05T17:05:29.363","2017-05-23T15:07:51.663","","","Rel-14","36.141","14.3.0","NB_IOT-Perf","1051","","A","RP-171300","","","","",""]
["R4-1705568","Clarification on 1.4 MHz for in-band operation","Huawei, HiSilicon, Nokia, Ericsson","Liehai Liu","47239","CR","","","","59","5.5.2","BS RF core(36.104) [NB_IOT-Core]",48310,"revised","2017-05-05T17:05:30.207","2017-05-05T17:33:46.013","","R4-1705869","Rel-13","36.104","13.7.0","NB_IOT-Core","4685","","F","","","","","",""]
["R4-1705569","Clarification on 1.4 MHz for in-band operation","Huawei, HiSilicon, Nokia, Ericsson","Liehai Liu","47239","CR","Agreement","","","59","5.5.2","BS RF core(36.104) [NB_IOT-Core]",53950,"agreed","2017-05-05T17:05:31.237","2017-05-23T15:07:51.663","","","Rel-14","36.104","14.3.0","NB_IOT-Core","4686","","A","RP-171300","","","","",""]
["R4-1705570","Transient time for sTTI ON/OFF mask","Qualcomm Incorporated","Prashanth Akula","67450","other","Approval","","","369","9.13","Shortened TTI and processing time for LTE [LTE_sTTIandPT]",55700,"noted","2017-05-05T17:05:34.370","2017-05-05T19:21:43.797","","","","","","","","","","","","","","",""]
["R4-1705571","PCmax computation and evaluation for CA with sTTI","Qualcomm Incorporated","Prashanth Akula","67450","other","Discussion","","","371","9.13.2","UE RF (36.101) [LTE_sTTIandPT-core]",55710,"noted","2017-05-05T17:12:26.540","2017-05-05T19:21:43.797","","","","","","","","","","","","","","",""]
["R4-1705572","Consideration on NB-IoT new BS classes","Huawei","Liehai Liu","47239","other","Approval","This contribution is for approval.","","392","9.14.2.1","eNB power classes [NB_IOTenh2-core]",48450,"noted","2017-05-05T17:15:53.817","2017-05-05T18:24:32.147","","","","","","","","","","","","","","",""]
["R4-1705573","UE maximum output power and reference sensitivity for Band 73","Huawei, Hisilicon, China Unicom","Liehai Liu","47239","other","Approval","This contribution is for approval.","","347","9.10.3","UE RF (36.101) [LTE450_Reg3-core]",55730,"approved","2017-05-05T17:15:53.830","2017-05-05T18:24:32.147","","","","","","","","","","","","","","",""]
["R4-1705574","450MHz ? Frequency regulation background","Huawei, Hisilicon, China Unicom","Liehai Liu","47239","discussion","Discussion","","","345","9.10.1","General [LTE450_Reg3]",55740,"noted","2017-05-05T17:15:53.830","2017-05-05T18:24:32.147","","","","","","","","","","","","","","",""]
["R4-1705575","New WID on addition of band 28 and 40 to LTE MTC Cat.0","Huawei, Hisilicon","Liehai Liu","47239","WID new","Information","","","473","13","Revision of the Work Plan",56070,"noted","2017-05-05T17:15:53.847","2017-05-05T18:24:32.130","","","","","","","","","","","","","","",""]
["R4-1705576","CR for absolute power tolerance","Neul, Huawei, HiSilicon","Liehai Liu","47239","CR","","","","58","5.5.1","UE RF core(36.101) [NB_IOT-Core]",55760,"revised","2017-05-05T17:15:53.847","2017-05-05T18:24:32.130","","R4-1705867","Rel-13","36.101","13.7.0","NB_IOT-Core","4474","","F","","","","","",""]
["R4-1705577","CR for NB-IoT Absolute power tolerance","Neul, Huawei, HiSilicon","Liehai Liu","47239","CR","Agreement","","","58","5.5.1","UE RF core(36.101) [NB_IOT-Core]",55770,"agreed","2017-05-05T17:15:54.627","2017-05-23T15:07:51.663","","","Rel-14","36.101","14.3.0","NB_IOT-Core","4475","","A","RP-171299","","","","",""]
["R4-1705578","LS to RAN5 on NB-IoT absolute power tolerance","Neul, Huawei, HiSilicon","Liehai Liu","47239","LS out","","","","58","5.5.1","UE RF core(36.101) [NB_IOT-Core]",55780,"withdrawn","2017-05-05T17:15:55.377",null,"","","","","","","","","","","","RAN5","","",""]
["R4-1705579","NB-IoT additional spectrum emission mask","Neul, Huawei, HiSilicon","Liehai Liu","47239","discussion","Discussion","","","58","5.5.1","UE RF core(36.101) [NB_IOT-Core]",55790,"noted","2017-05-05T17:15:55.377","2017-05-05T18:24:32.130","","","","","","","","","","","","","","",""]
["R4-1705580","Discussion on NB-IoT demod requirements","Neul, Huawei, HiSilicon","Liehai Liu","47239","discussion","Discussion","","","64","5.5.6.1","UE Demodulation (36.101) [NB_IOT-Perf]",46240,"noted","2017-05-05T17:15:55.390","2017-05-05T18:24:32.117","","","","","","","","","","","","","","",""]
["R4-1705581","TR 36.753 V0.2.0","Huawei, Hisilicon","Liehai Liu","47239","draft TR","","","","326","9.6","TDD operating band in the L-band for LTE [LTE_TDD_L_Band]",53460,"approved","2017-05-05T17:15:55.390","2017-05-05T18:19:31.487","","","Rel-14","36.753","0.2.0","LTE_TDD_L_Band","","","","","","","","",""]
["R4-1705582","PCmax Teval window for sTTI","Qualcomm Incorporated","Prashanth Akula","67450","other","Discussion","","","371","9.13.2","UE RF (36.101) [LTE_sTTIandPT-core]",55840,"withdrawn","2017-05-05T17:22:50.493",null,"","","","","","","","","","","","","","",""]
["R4-1705583","Update of LAA REFSENS exclusion region","QUALCOMM UK Ltd","Marco Papaleo","49190","CR","Agreement","The values in Table 7.3.1A-0eA are modified based on what agreed in R4-1611019","","34","5.3.1","UE RF core (36.101) [LTE_LAA-Core]",54790,"revised","2017-05-05T17:23:19.023","2017-05-06T19:17:52.173","","R4-1705911","Rel-13","36.101","13.7.0","LTE_LAA-Core","4476","","F","","","","","",""]
["R4-1705584","PCmax Teval window for sTTI","Qualcomm Incorporated","Prashanth Akula","67450","other","Discussion","","","371","9.13.2","UE RF (36.101) [LTE_sTTIandPT-core]",55850,"withdrawn","2017-05-05T17:23:42.567",null,"","","","","","","","","","","","","","",""]
["R4-1705585","PCmax Teval window for sTTI","Qualcomm Incorporated","Prashanth Akula","67450","other","Discussion","","","371","9.13.2","UE RF (36.101) [LTE_sTTIandPT-core]",55860,"withdrawn","2017-05-05T17:24:05.263",null,"","","","","","","","","","","","","","",""]
["R4-1705586","PCmax Teval window for sTTI","Qualcomm Incorporated","Prashanth Akula","67450","other","Discussion","","","371","9.13.2","UE RF (36.101) [LTE_sTTIandPT-core]",55870,"withdrawn","2017-05-05T17:24:13.420",null,"","","","","","","","","","","","","","",""]
["R4-1705587","PCmax Teval window for sTTI","Qualcomm Incorporated","Prashanth Akula","67450","other","Discussion","","","371","9.13.2","UE RF (36.101) [LTE_sTTIandPT-core]",55880,"withdrawn","2017-05-05T17:24:15.840",null,"","","","","","","","","","","","","","",""]
["R4-1705588","PCmax Teval window for sTTI","Qualcomm Incorporated","Prashanth Akula","67450","other","Discussion","","","371","9.13.2","UE RF (36.101) [LTE_sTTIandPT-core]",609200,"noted","2017-05-05T17:24:25.073","2017-05-05T19:21:43.797","","","","","","","","","","","","","","",""]
["R4-1705589","NR UE sub-channel-bandwidth operation","MediaTek Inc.","James Wang","56966","other","Approval","In this contribution, we bring up the potential concerns in NR UE sub-channel-bandwidth operation under MU-OFDMA and propose to apply UE bandwidth adaptation to mitigate the power consumption and UL coverage issues.","","418","10.3.1","Channel bandwidth and subcarrier spacing [NR_newRAT]",46880,"noted","2017-05-05T17:26:01.137","2017-05-06T16:57:52.053","","","Rel-15","38.101","","NR_newRAT","","","","","","","","",""]
["R4-1705590","On RSTD requirements in shared cells","Ericsson","Iana Siomina","42857","discussion","Discussion","On RSTD requirements in shared cells","","249","7.23.1","RRM core maintenance (36.133) [UTRA_LTE_iPos_enh2-Core]",55900,"noted","2017-05-05T17:32:08.217","2017-05-05T20:24:42.133","","","Rel-14","","","UTRA_LTE_iPos_enh2-Core","","","","","","","","",""]
["R4-1705591","Impact on requiremets for RSTD in shared cell","Ericsson","Iana Siomina","42857","CR","Approval","Impact on requiremets for RSTD in shared cell","","249","7.23.1","RRM core maintenance (36.133) [UTRA_LTE_iPos_enh2-Core]",55910,"noted","2017-05-05T17:32:08.217","2017-05-05T20:24:42.133","","","Rel-14","36.133","14.3.0","UTRA_LTE_iPos_enh2-Core","4979","","F","","","","","",""]
["R4-1705592","On RSTD requirements with new PRS configurations","Ericsson","Iana Siomina","42857","discussion","Discussion","On RSTD requirements with new PRS configurations","","249","7.23.1","RRM core maintenance (36.133) [UTRA_LTE_iPos_enh2-Core]",55920,"noted","2017-05-05T17:32:10.497","2017-05-05T20:24:42.133","","","Rel-14","","","UTRA_LTE_iPos_enh2-Core","","","","","","","","",""]
["R4-1705593","Clarification on requirements for new PRS configurations","Ericsson","Iana Siomina","42857","CR","Approval","Clarification on requirements for new PRS configurations","","249","7.23.1","RRM core maintenance (36.133) [UTRA_LTE_iPos_enh2-Core]",55930,"noted","2017-05-05T17:32:10.510","2017-05-05T20:24:42.147","","R4-1706215","Rel-14","36.133","14.3.0","UTRA_LTE_iPos_enh2-Core","4980","","F","","","","","",""]
["R4-1705594","On timing reference for FS3 SCell","Ericsson","Iana Siomina","42857","discussion","Discussion","On timing reference for FS3 SCell","","164","7.14.5","RRM core Maintenance (36.133) [LTE_eLAA-Core]",54970,"noted","2017-05-05T17:32:11.477","2017-05-05T20:24:42.147","","","Rel-14","","","LTE_eLAA-Core","","","","","","","","",""]
["R4-1705595","LS response on timing reference for FS3 SCell","Ericsson","Iana Siomina","42857","LS out","Approval","LS response on timing reference for FS3 SCell","","164","7.14.5","RRM core Maintenance (36.133) [LTE_eLAA-Core]",55960,"revised","2017-05-05T17:32:11.493","2017-05-05T20:24:42.147","","R4-1706216","Rel-14","","","LTE_eLAA-Core","","","","","R2-165965","RAN WG2","RAN WG1","R2-165965",""]
["R4-1705596","Clarification on timing reference for FS3 Scell","Ericsson","Iana Siomina","42857","CR","Approval","Clarification on timing reference for FS3 Scell","","164","7.14.5","RRM core Maintenance (36.133) [LTE_eLAA-Core]",55950,"noted","2017-05-05T17:32:11.993","2017-05-05T20:24:42.147","","","Rel-14","36.133","14.3.0","LTE_eLAA-Core","4981","","F","","","","","",""]
["R4-1705597","Requirements applicability for LAA and eLAA","Ericsson","Iana Siomina","42857","CR","Approval","Requirements applicability for LAA and eLAA","","164","7.14.5","RRM core Maintenance (36.133) [LTE_eLAA-Core]",55970,"revised","2017-05-05T17:32:12.943","2017-05-05T20:24:42.147","","R4-1706214","Rel-14","36.133","14.3.0","LTE_eLAA-Core","4982","","F","","","","","",""]
["R4-1705598","Corrections in LAA requirements","Ericsson, Verizon Wireless, Rohde & Schwarz, Anritsu, Nokia","Iana Siomina","42857","CR","Agreement","Corrections in LAA requirements","","36","5.3.3","RRM Core (36.133) [LTE_LAA-Core]",55980,"agreed","2017-05-05T17:32:13.973","2017-05-05T20:24:42.163","","","Rel-13","36.133","13.7.0","LTE_LAA-Core","4983","","F","RP-171307","","","","",""]
["R4-1705599","Corrections in LAA requirements","Ericsson, Verizon Wireless, Rohde & Schwarz, Anritsu, Nokia","Iana Siomina","42857","CR","Agreement","Corrections in LAA requirements","","36","5.3.3","RRM Core (36.133) [LTE_LAA-Core]",55990,"agreed","2017-05-05T17:32:14.863","2017-05-23T15:07:51.693","","","Rel-14","36.133","14.3.0","LTE_LAA-Core","4984","","A","RP-171307","","","","",""]
["R4-1705600","On RRM requirements impact with eMBMS enhancements","Ericsson","Iana Siomina","42857","discussion","Discussion","On RRM requirements impact with eMBMS enhancements","","155","7.13.3","RRM core (36.133) [MBMS_LTE_enh2-Core]",601200,"withdrawn","2017-05-05T17:32:15.673",null,"","","Rel-14","","","MBMS_LTE_enh2-Core","","","","","","","","",""]
["R4-1705601","RRM requirements with eMBMS enhancements","Ericsson","Iana Siomina","42857","CR","Approval","RRM requirements with eMBMS enhancements","","155","7.13.3","RRM core (36.133) [MBMS_LTE_enh2-Core]",574400,"revised","2017-05-05T17:32:15.690","2017-05-06T18:55:27.090","","R4-1706217","Rel-14","36.133","14.3.0","MBMS_LTE_enh2-Core","4985","","B","","","","","",""]
["R4-1705602","RRM requirements under configurable MPDCCH monitoring","Ericsson","Iana Siomina","42857","CR","Approval","RRM requirements under configurable MPDCCH monitoring","","213","7.18.3.2.1","UE MPDCCH monitoring configuration [LTE_feMTC-Core]",56020,"revised","2017-05-05T17:32:16.563","2017-05-05T20:24:42.163","","R4-1705979","Rel-14","36.133","14.3.0","LTE_feMTC-Core","4986","","F","","","","","",""]
["R4-1705603","On RSTD requirements for FeMTC","Ericsson","Iana Siomina","42857","discussion","Discussion","On RSTD requirements for FeMTC","","211","7.18.3.1.2","OTDOA [LTE_feMTC-Core]",50010,"noted","2017-05-05T17:32:17.467","2017-05-05T20:24:42.163","","","Rel-14","","","LTE_feMTC-Core","","","","","","","","",""]
["R4-1705604","On E-CID requirements for FeMTC","Ericsson","Iana Siomina","42857","discussion","Discussion","On E-CID requirements for FeMTC","","210","7.18.3.1.1","E-CID [LTE_feMTC-Core]",50050,"noted","2017-05-05T17:32:17.483","2017-05-05T20:24:42.163","","","Rel-14","","","LTE_feMTC-Core","","","","","","","","",""]
["R4-1705605","LS on measurement gaps for intra-frequency RSTD for FeMTC UE","Ericsson","Iana Siomina","42857","LS out","Approval","LS on measurement gaps for intra-frequency RSTD for FeMTC UE","","211","7.18.3.1.2","OTDOA [LTE_feMTC-Core]",51510,"noted","2017-05-05T17:32:17.500","2017-05-05T20:24:42.163","","R4-1705977","Rel-14","","","LTE_feMTC-Core","","","","","","RAN WG2","","",""]
["R4-1705606","On RSTD requirements with NB-IoT","Ericsson","Iana Siomina","42857","discussion","Discussion","On RSTD requirements with NB-IoT","","191","7.17.3.1.2","UTODA/OTDOA [NB_IOTenh-Core]",49950,"noted","2017-05-05T17:32:17.517","2017-05-05T20:24:42.133","","","Rel-14","","","NB_IOTenh-Core","","","","","","","","",""]
["R4-1705607","Motivation for new Work Item on network based CRS mitigation for LTE","Ericsson","Iana Siomina","42857","other","Information","Motivation for new Work Item on network based CRS mitigation for LTE","","473","13","Revision of the Work Plan",56080,"noted","2017-05-05T17:32:17.530","2017-05-05T20:24:42.180","","","Rel-15","","","","","","","","","","","",""]
["R4-1705608","New Work Item on UE requirements for network-based CRS mitigation for LTE","Ericsson","Iana Siomina","42857","other","Information","New Work Item on UE requirements for network-based CRS mitigation for LTE","","473","13","Revision of the Work Plan",577800,"noted","2017-05-05T17:32:17.547","2017-05-05T20:24:42.117","","","Rel-15","","","","","","","","","","","",""]
["R4-1705609","On measurement capacity in NR","Ericsson","Iana Siomina","42857","discussion","Discussion","On measurement capacity in NR","","450","10.6.2","UE measurement capability [NR_newRAT]",47140,"noted","2017-05-05T17:32:17.547","2017-05-05T20:24:42.117","","","Rel-15","","","NR_newRAT","","","","","","","","",""]
["R4-1705610","Further considerations on RLM for NR","Ericsson","Iana Siomina","42857","discussion","Discussion","Further considerations on RLM for NR","","452","10.6.4","Expected Measurement requirements for NSA [NR_newRAT]",56090,"noted","2017-05-05T17:32:17.560","2017-05-05T20:24:42.117","","","Rel-15","","","NR_newRAT","","","","","","","","",""]
["R4-1705611","Further discussion on cell identification in NR","Ericsson","Iana Siomina","42857","discussion","Discussion","Further discussion on cell identification in NR","","452","10.6.4","Expected Measurement requirements for NSA [NR_newRAT]",48010,"noted","2017-05-05T17:32:17.577","2017-05-05T20:24:42.117","","","Rel-15","","","NR_newRAT","","","","","","","","",""]
["R4-1705612","On SS block numerology","Ericsson","Iana Siomina","42857","discussion","Discussion","On SS block numerology","","419","10.3.2","Channel Raster [NR_newRAT]",52630,"noted","2017-05-05T17:32:17.577","2017-05-05T20:24:42.117","","","Rel-15","","","NR_newRAT","","","","","","","","",""]
["R4-1705613","Draft link level simulations plan for NR","Ericsson","Iana Siomina","42857","discussion","Discussion","Draft link level simulations plan for NR","","453","10.6.5","System level and link level Simulation plan [NR_newRAT]",47950,"noted","2017-05-05T17:32:17.593","2017-05-05T20:24:42.133","","","Rel-15","","","NR_newRAT","","","","","","","","",""]
["R4-1705614","LS on SS block numerology","Ericsson","Iana Siomina","42857","LS out","Approval","LS on SS block numerology","","419","10.3.2","Channel Raster [NR_newRAT]",52640,"noted","2017-05-05T17:32:17.607","2017-05-05T20:24:42.133","","","Rel-15","","","NR_newRAT","","","","","R1-1706717","RAN WG1","RAN WG2","R1-1706717",""]
["R4-1705615","[Draft] Introduction of TDD L band into TS 36.101","Huawei, Hisilicon, Etisalat","Liehai Liu","47239","draftCR","","","","328","9.6.2","UE RF (36.101) [LTE_TDD_L_Band-core]",576600,"revised","2017-05-05T17:50:30.427","2017-05-06T12:42:53.233","","R4-1705929","Rel-15","36.101","14.3.0","LTE_TDD_L_Band-Core","","","","","","","","",""]
["R4-1705616","[Draft] Introduction of TDD L band into TS 36.104","Huawei, Hisilicon, Etisalat","Liehai Liu","47239","draftCR","","","","329","9.6.3","BS RF (36.104, 36.141) [LTE_TDD_L_Band-core/Perf]",56160,"revised","2017-05-05T17:50:30.443","2017-05-05T20:42:14.200","","R4-1705827","Rel-15","36.104","14.3.0","LTE_TDD_L_Band-Core","","","","","","","","",""]
["R4-1705617","[Draft] Introduction of TDD L band into TS 36.141","Huawei, Hisilicon, Etisalat","Liehai Liu","47239","draftCR","","","","329","9.6.3","BS RF (36.104, 36.141) [LTE_TDD_L_Band-core/Perf]",582700,"postponed","2017-05-05T17:50:30.457","2017-05-05T20:37:49.267","","","Rel-15","36.141","14.3.0","LTE_TDD_L_Band-Perf","","","","","","","","",""]
["R4-1705618","[Draft] Introduction of TDD L band into TS 25.123","Huawei, Hisilicon, Etisalat","Liehai Liu","47239","draftCR","","","","330","9.6.4","Other specifications [LTE_TDD_L_Band]",56180,"noted","2017-05-05T17:50:30.473","2017-05-05T20:33:36.657","","R4-1706016","Rel-15","25.123","14.2.0","LTE_TDD_L_Band-Core","","","","","","","","",""]
["R4-1705619","A-MPR implementation to comply to ¡°TDD L-Band UE emission level to protect MSS above 1518MHz¡±","Huawei, Hisilicon, Etisalat","Liehai Liu","47239","other","Approval","This contribution is for approval.","","328","9.6.2","UE RF (36.101) [LTE_TDD_L_Band-core]",56190,"noted","2017-05-05T17:50:30.490","2017-05-06T12:34:41.143","","","","","","","","","","","","","","",""]
["R4-1705620","TDD L-Band - Channel numbering for E-UTRA, MSR","Huawei, Hisilicon","Liehai Liu","47239","other","Approval","This contribution is for approval.","","327","9.6.1","Band Arrangement [LTE_TDD_L_Band-core]",56200,"revised","2017-05-05T17:50:30.507","2017-05-05T20:25:34.927","","R4-1706116","","","","","","","","","","","","",""]
["R4-1705621","Study about TDD L-Band - UE reference sensitivity power level","Huawei, Hisilicon","Liehai Liu","47239","other","Approval","This contribution is for approval.","","328","9.6.2","UE RF (36.101) [LTE_TDD_L_Band-core]",576500,"noted","2017-05-05T17:50:30.507","2017-05-05T20:21:51.540","","","","","","","","","","","","","","",""]
["R4-1705622","Study TDD L-Band Tx BTS in the band 1427-1432MHz to protect EESS & propose a preferred TDD band plan","Huawei, Hisilicon","Liehai Liu","47239","other","Discussion","","","327","9.6.1","Band Arrangement [LTE_TDD_L_Band-core]",56220,"noted","2017-05-05T17:50:30.520","2017-05-05T20:16:38.680","","","","","","","","","","","","","","",""]
["R4-1705623","Study SDL L-Band in the band 1427-1432MHz to protect EESS","Huawei, Hisilicon","Liehai Liu","47239","other","Discussion","","","321","9.5.1","Co-exitence requirements with EESS and MSS [LTE_SDL_1500ext]",56230,"noted","2017-05-05T17:50:30.520","2017-05-05T19:04:45.590","","","","","","","","","","","","","","",""]
["R4-1705624","Further discussion on PUSCH setup in eLAA","Ericsson","Shaohua Li","46382","discussion","Discussion","Provide further discussion on the PUSCH setup in eLAA","","166","7.14.7","BS demodulation (36.104/36.141) [LTE_eLAA-Perf]",54960,"noted","2017-05-05T18:03:54.047","2017-05-06T10:33:51.040","","","","","","LTE_eLAA-Perf","","","","","","","","",""]
["R4-1705625","link level simulation results for eLAA PUSCH with impairment results","Ericsson","Shaohua Li","46382","discussion","Discussion","Provide link level simulation results and its corresponding impairment results","","166","7.14.7","BS demodulation (36.104/36.141) [LTE_eLAA-Perf]",55130,"noted","2017-05-05T18:03:54.060","2017-05-06T10:33:51.040","","","","","","LTE_eLAA-Perf","","","","","","","","",""]
["R4-1705626","Summary of link level simulation results for eLAA PUSCH","Ericsson","Shaohua Li","46382","discussion","Discussion","Collect companies simulation results for eLAA PUSCH","","166","7.14.7","BS demodulation (36.104/36.141) [LTE_eLAA-Perf]",56240,"noted","2017-05-05T18:03:54.060","2017-05-23T15:07:51.693","","","","","","LTE_eLAA-Perf","","","","","","","","",""]
["R4-1705627","Introduce test case for eLAA PUSCH","Ericsson","Shaohua Li","46382","CR","Approval","Introduce test case for eLAA PUSCH","","166","7.14.7","BS demodulation (36.104/36.141) [LTE_eLAA-Perf]",56260,"revised","2017-05-05T18:03:54.077","2017-05-06T10:33:51.027","","R4-1706205","Rel-14","36.104","14.3.0","LTE_eLAA-Perf","4687","","B","","","","","",""]
["R4-1705628","Introduce conformance test for eLAA PUSCH","Ericsson","Shaohua Li","46382","CR","Approval","Introduce conformance test for eLAA PUSCH","","166","7.14.7","BS demodulation (36.104/36.141) [LTE_eLAA-Perf]",56280,"noted","2017-05-05T18:03:54.873","2017-05-06T10:33:51.040","","","Rel-14","36.141","14.3.0","LTE_eLAA-Perf","1052","","B","","","","","",""]
["R4-1705629","Introduce LBT model for multile LAA Scell(s) in LAA demodualtion","Ericsson","Shaohua Li","46382","CR","Approval","Introduce LBT model for multile LAA Scell(s) in LAA demodualtion","","294","7.29.4.1","Demodulation with multiple LAA SCC-s [WI code or TEI14]",56290,"revised","2017-05-05T18:03:55.620","2017-05-06T10:33:51.040","","R4-1705975","Rel-14","36.101","14.3.0","LTE_LAA-Perf","4477","","B","","","","","",""]
["R4-1705630","Further discussion V2X demodulation","Ericsson","Shaohua Li","46382","discussion","Discussion","Disucssion on the V2X demodulation","","182","7.16.5.2","PSBCH, eNB sync and WAN SDR [LTE_V2X-Perf]",49130,"noted","2017-05-05T18:03:56.400","2017-05-06T10:33:51.027","","","","","","LTE_V2X-Perf","","","","","","","","",""]
["R4-1705631","TP for enhanced SU-MIMO IM receiver","Huawei, HiSilicon","Xiang (Steven) Chen","41576","other","Approval","In this draft TP, we will capture more simulation results to TR 36.747 for enhanced SU-MIMO.","","279","7.27.3","SU-MIMO IM [LTE_eCRSIM_eSUMIMO]",616800,"revised","2017-05-05T18:33:57.227","2017-05-05T19:35:29.593","","R4-1706165","Rel-14","36.747","","LTE_eCRSIM_eSUMIMO","","","","","","","","",""]
["R4-1705632","NR Range 2 - Output power accuracy","Huawei","Richard Kybett","47339","discussion","Discussion","Discuss output power accuracy and how it should be based on network performance not just capability","","442","10.5.3.4","Other Tx requirements [NR_newRAT]",52670,"noted","2017-05-05T18:43:29.957","2017-05-05T19:23:57.807","","","","","","NR_newRAT","","","","","","","","",""]
["R4-1705633","NR Range 2 - OTA minimum EIS","Huawei","Richard Kybett","47339","discussion","Approval","discuss min EIS and min antenna gain requirements","","446","10.5.4.3","Other Rx requirements [NR_newRAT]",53970,"noted","2017-05-05T18:43:29.973","2017-05-05T19:23:57.823","","","","","","NR_newRAT","","","","","","","","",""]
["R4-1705634","NR BS Specification structure","Huawei","Richard Kybett","47339","discussion","Discussion","Our view on the TS structure","","436","10.5.1","BS RF General (ad-hoc MoM, Plan, Spec structure) [NR_newRAT]",46180,"noted","2017-05-05T18:43:29.973","2017-05-05T19:23:57.807","","","","","","NR_newRAT","","","","","","","","",""]
["R4-1705635","NR Range 2 - beam specific requirements","Huawei","Richard Kybett","47339","discussion","Approval","Further discussion on beam specific requirements","","436","10.5.1","BS RF General (ad-hoc MoM, Plan, Spec structure) [NR_newRAT]",53370,"noted","2017-05-05T18:43:29.990","2017-05-05T19:23:57.807","","","","","","NR_newRAT","","","","","","","","",""]
["R4-1705636","Ad-hoc agenda and minutes","Huawei","Richard Kybett","47339","report","Approval","Ad-hoc agenda and minutes (submit during meeting)","","356","9.12.1","General [AASenh_BS_LTE_UTRA]",48510,"approved","2017-05-05T18:44:59.180","2017-05-23T15:07:51.727","","","","","","AASenh_BS_LTE_UTRA","","","","","","","","",""]
["R4-1705637","TR 37.843 v0.3.0 - updated TR","Huawei","Richard Kybett","47339","draft TR","Approval","Updated TR with TP's from last meeting","","356","9.12.1","General [AASenh_BS_LTE_UTRA]",48520,"approved","2017-05-05T18:44:59.197","2017-05-05T19:14:25.097","","","Rel-15","37.843","0.3.0","AASenh_BS_LTE_UTRA","","","","","","","","",""]
["R4-1705638","Generating REL15  TS text","Huawei","Richard Kybett","47339","discussion","Discussion","Discuss allocation of authors etc","","356","9.12.1","General [AASenh_BS_LTE_UTRA]",53920,"noted","2017-05-05T18:45:02.287","2017-05-05T19:15:00.773","","","","","","AASenh_BS_LTE_UTRA","","","","","","","","",""]
["R4-1705639","TP to TR37.843 - Capturing TRP accuracy requirement","Huawei","Richard Kybett","47339","pCR","Approval","Capturing agreements on TRP accuracy","","358","9.12.2.1","TRP accuracy [AASenh_BS_LTE_UTRA-Core]",581300,"noted","2017-05-05T18:45:02.333","2017-05-05T19:15:16.247","","","Rel-15","37.843","0.2.0","AASenh_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-1705640","TRP accuracy value","Huawei","Richard Kybett","47339","discussion","Discussion","Proposal for TRP accuracy value","","358","9.12.2.1","TRP accuracy [AASenh_BS_LTE_UTRA-Core]",56390,"noted","2017-05-05T18:45:02.397","2017-05-05T19:15:16.247","","","","","","AASenh_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-1705641","TP to TR37.843 - Capturing emissions scaling agreements","Huawei","Richard Kybett","47339","pCR","Approval","Capturing agreements on emissions scaling","","362","9.12.2.5","Other Transmitter Requirements [AASenh_BS_LTE_UTRA-Core]",56550,"noted","2017-05-05T18:45:02.427","2017-05-05T19:15:16.233","","","Rel-15","37.843","0.2.0","AASenh_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-1705642","TP to TR37.843 - Capturing OTA REFSENS requirements","Huawei","Richard Kybett","47339","pCR","Approval","Capturing agreements on OTA REFSENS","","363","9.12.2.6","Other Receiver requirements [AASenh_BS_LTE_UTRA-Core]",49451,"noted","2017-05-05T18:45:02.473","2017-05-05T19:15:16.233","","R4-1706142","Rel-15","37.843","0.2.0","AASenh_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-1705643","TP to TR37.843 - Capturing Blocking requirements","Huawei","Richard Kybett","47339","pCR","Approval","Capturing agreement on in band blocking","","363","9.12.2.6","Other Receiver requirements [AASenh_BS_LTE_UTRA-Core]",56450,"noted","2017-05-05T18:45:02.503","2017-05-05T19:17:53.500","","","Rel-15","37.843","0.2.0","AASenh_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-1705644","On receiver OTA REFSENS redirection range","Huawei","Richard Kybett","47339","discussion","Approval","Discuss how redirection capability is handled for the OTA REFSENS requirement","","363","9.12.2.6","Other Receiver requirements [AASenh_BS_LTE_UTRA-Core]",53170,"noted","2017-05-05T18:45:02.567","2017-05-05T19:17:53.517","","","","","","AASenh_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-1705645","TP to TR37.843 - Clarifying Declarations for OTA sensitivity and OTA REFSENS","Huawei","Richard Kybett","47339","pCR","Approval","TP on the direction capability for OTA REFSENS requirement","","363","9.12.2.6","Other Receiver requirements [AASenh_BS_LTE_UTRA-Core]",53171,"revised","2017-05-05T18:45:02.583","2017-05-05T19:17:53.517","","R4-1706144","Rel-15","37.843","0.2.0","AASenh_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-1705646","Antenna loss factors","Huawei","Richard Kybett","47339","discussion","Discussion","Discuss Tx and Rx in-band and out of band loss factors","","359","9.12.2.2","Tx and Rx loss values [AASenh_BS_LTE_UTRA-Core]",56460,"noted","2017-05-05T18:45:02.660","2017-05-05T19:17:53.517","","","","","","AASenh_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-1705647","Co-location requirements","Huawei","Richard Kybett","47339","discussion","Discussion","Discussing how to specify and test  all the co-location requirements","","360","9.12.2.3","Co-location requirements [AASenh_BS_LTE_UTRA-Core]",56470,"noted","2017-05-05T18:45:02.690","2017-05-05T19:17:53.533","","","","","","AASenh_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-1705648","Unwanted emission co-existence requirements","Huawei","Richard Kybett","47339","discussion","Discussion","discussing the co-existence (same geographical area) emissions requirements and how they can be specified OTA","","362","9.12.2.5","Other Transmitter Requirements [AASenh_BS_LTE_UTRA-Core]",56500,"noted","2017-05-05T18:45:02.737","2017-05-05T19:15:50.007","","","","","","AASenh_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-1705649","Receiver out of band blocking","Huawei","Richard Kybett","47339","discussion","Discussion","Discussing receiver out of band blocking","","363","9.12.2.6","Other Receiver requirements [AASenh_BS_LTE_UTRA-Core]",580300,"noted","2017-05-05T18:45:02.770","2017-05-05T19:15:50.023","","","","","","AASenh_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-1705650","OTA TX off power","Huawei","Richard Kybett","47339","discussion","Discussion","Discussing the TX off power requirement and how it applies to OAT requirements","","362","9.12.2.5","Other Transmitter Requirements [AASenh_BS_LTE_UTRA-Core]",56410,"noted","2017-05-05T18:45:02.817","2017-05-05T19:15:50.023","","","","","","AASenh_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-1705651","Tx control signal power accuracy","Huawei","Richard Kybett","47339","discussion","Approval","Discussion and proposals on how to specify control channel power accuracy OTA.","","362","9.12.2.5","Other Transmitter Requirements [AASenh_BS_LTE_UTRA-Core]",49220,"noted","2017-05-05T18:45:02.863","2017-05-05T19:15:49.990","","","","","","AASenh_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-1705652","TP for TR 37.843 - TX Power requirements for control channels","Huawei","Richard Kybett","47339","pCR","Approval","TP to capture how OTA control channel accuracy requirements are specified.","","362","9.12.2.5","Other Transmitter Requirements [AASenh_BS_LTE_UTRA-Core]",49430,"revised","2017-05-05T18:45:02.893","2017-05-05T19:15:50.007","","R4-1706135","Rel-15","37.843","0.2.0","AASenh_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-1705653","Draft CR to TS 37.105 - TX output power","Huawei","Richard Kybett","47339","discussion","Discussion","Example text to show how OTA output power requirements will be captured in TS 37.105","","356","9.12.1","General [AASenh_BS_LTE_UTRA]",56361,"revised","2017-05-05T18:45:02.987","2017-05-05T19:15:50.007","","R4-1706127","","","","AASenh_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-1705654","Draft CR to TS 37.105 - Rx sensitivity output power","Huawei","Richard Kybett","47339","discussion","Discussion","Example text to show how OTA Rx sensitivity requirements will be captured in TS 37.105","","356","9.12.1","General [AASenh_BS_LTE_UTRA]",56371,"revised","2017-05-05T18:45:03.037","2017-05-05T19:15:50.007","","R4-1706128","","","","AASenh_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-1705655","TP to TR 37.843 ? Clarify example in sub-clause 5.1","Huawei","Richard Kybett","47339","pCR","Approval","Clarify the examples in section 5.1 to try to make clearer.","","362","9.12.2.5","Other Transmitter Requirements [AASenh_BS_LTE_UTRA-Core]",580500,"revised","2017-05-05T18:45:03.067","2017-05-05T19:15:50.007","","R4-1706140","Rel-15","37.843","0.2.0","AASenh_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-1705656","NR BS Work plan and status","Ericsson","Johan Skold","10425","discussion","Discussion","The document presents the status of work on NR BS RF in relation to the worl plan.","","436","10.5.1","BS RF General (ad-hoc MoM, Plan, Spec structure) [NR_newRAT]",622700,"withdrawn","2017-05-05T19:30:16.273",null,"","","Rel-15","","","NR_newRAT","","","","","","","","",""]
["R4-1705657","UE sub-6 GHz ACS considerations and proposals","Intel Corporation","Yang Tang","56725","other","Discussion","","","422","10.3.5","ACLR and ACS [NR_newRAT]",54290,"noted","2017-05-05T20:06:50.650","2017-05-06T17:38:10.957","","","","","","","","","","","","","","",""]
["R4-1705658","Draft LS on Rel-14 RAN4 UE feature list","Intel Corporation","Yang Tang","56725","LS out","Approval","The LS provides a list of Rel-14 UE features introduced as a part of RAN4-led WI","","289","7.29","TEI14",56580,"revised","2017-05-05T20:28:17.030","2017-05-06T17:38:10.957","","R4-1706270","Rel-14","","","","","","","","","RAN2","RAN, RAN1","",""]
["R4-1705659","Discussion on FeD2D co-existence","Intel Corporation","Yang Tang","56725","discussion","Discussion","","","471","11.1.1","Co-existence study [FS_feD2D_IoT_relay_wearable]",56590,"noted","2017-05-05T20:28:17.063","2017-05-06T17:38:10.957","","","Rel-15","","","FS_feD2D_IoT_relay_wearable","","","","","","","","",""]
["R4-1705660","Discussion on the GNSS side conditions for V2V performance requirements","Intel Corporation","Yang Tang","56725","discussion","Discussion","","","170","7.15.3","RRM performance (36.133) [LTE_SL_V2V-Perf]",45360,"noted","2017-05-05T20:28:17.063","2017-05-06T17:38:10.973","","","Rel-14","","","LTE_SL_V2V-Perf","","","","","","","","",""]
["R4-1705661","On EVM for 1024QAM","Intel Corporation","Yang Tang","56725","discussion","Discussion","","","405","9.17.1","General [LTE_HCS]",52490,"noted","2017-05-05T20:28:17.077","2017-05-06T17:38:10.973","","","Rel-15","","","","","","","","","","","",""]
["R4-1705662","Correction of references in the NB-IOT accurcy requirements","Ericsson","Santhan Thangarasa","59137","CR","Approval","In this contribution, we correct the incorrect references used in the measurement accuracy requirements.","","62","5.5.5","RRM Performance (36.133) [NB_IOT-Perf]",56630,"noted","2017-05-05T20:33:30.290","2017-05-05T21:32:47.653","","","Rel-13","36.133","13.7.0","NB_IOT-Perf","4987","","B","","","","","",""]
["R4-1705663","Correction of references in the NB-IOT accurcy requirements","Ericsson","Santhan Thangarasa","59137","CR","Approval","In this contribution, we correct the incorrect references used in the measurement accuracy requirements.","","62","5.5.5","RRM Performance (36.133) [NB_IOT-Perf]",573900,"withdrawn","2017-05-05T20:33:31.087",null,"","","Rel-14","36.133","14.3.0","NB_IOT-Perf","4988","","A","","","","","",""]
["R4-1705664","NR BS Tx mask for above 6 GHz","Nokia, Alcatel-Lucent Shanghai Bell","Bartlomiej Golebiowski","68311","other","Approval","In this contribution, we discuss and propose NR BS spectrum mask for BS above 6 GHz.","","440","10.5.3.2","Unwanted emission requirements [NR_newRAT]",45420,"noted","2017-05-06T09:23:54.997","2017-05-06T17:46:53.707","","","","","","","","","","","","","","",""]
["R4-1705665","Frequency limit for BS spurious emission above 6 GHz","Nokia, Alcatel-Lucent Shanghai Bell","Bartlomiej Golebiowski","68311","other","Approval","In this contribution we discuss and proposed uppare range of fundametal frequency range and upper limit for BS spurious emission.","","440","10.5.3.2","Unwanted emission requirements [NR_newRAT]",622200,"withdrawn","2017-05-06T09:23:56.310","2017-05-06T18:57:52.473","","","","","","","","","","","","","","",""]
["R4-1705666","Boundary between spurious and OOB domain for NR BS above 6 GHz","Nokia, Alcatel-Lucent Shanghai Bell","Bartlomiej Golebiowski","68311","other","Approval","In this contribution we discuss and propose boundary between spurius and OOB domain for NR BS above 6 GHz","","440","10.5.3.2","Unwanted emission requirements [NR_newRAT]",622300,"withdrawn","2017-05-06T09:23:56.343","2017-05-06T18:57:52.490","","","","","","","","","","","","","","",""]
["R4-1705667","RTS applicability for > 2 Rx","Keysight Technologies","Kyoungseok Oh","66120","CR","Agreement","","","144","7.11.1","General [LTE_MIMO_OTA-Core]",45760,"revised","2017-05-08T10:23:41.047","2017-05-08T10:27:53.133","","R4-1705919","Rel-14","37.977","14.3.0","LTE_MIMO_OTA-Core","0058","","F","","","","","",""]
["R4-1705668","ULA (uniform linear antenna array) minimum FF distance calculation based on main beam width","Rohde & Schwarz","Kyoungseok Oh","66120","discussion","Discussion","","","459","10.7.2","UE RF [FS_NR_test_methods]",46120,"noted","2017-05-08T10:23:42.907","2017-05-08T10:27:53.147","","","","","","","","","","","","","","",""]
["R4-1705669","CR on Theoretical V/H Limits","ROHDE & SCHWARZ, Spirent Communications, Keysight Technologies","Kyoungseok Oh","66120","CR","Agreement","","","144","7.11.1","General [LTE_MIMO_OTA-Core]",45770,"agreed","2017-05-08T10:23:43.157","2017-05-23T15:07:51.727","","","Rel-14","37.977","14.3.0","LTE_MIMO_OTA","0059","","F","RP-171258","","","","",""]
["R4-1705670","Justification for two sub-band approach for 3.3-4.2GHz NR frequency range","Skyworks Solutions Inc","Kyoungseok Oh","66120","discussion","Discussion","","","415","10.2.1.2","Band definition for NR bands [NR_newRAT]",51660,"noted","2017-05-08T10:23:45.153","2017-05-08T10:27:53.163","","","","","","","","","","","","","","",""]
["R4-1705671","Sub6 ACS","Qualcomm Incorporated","Kyoungseok Oh","66120","other","","","","422","10.3.5","ACLR and ACS [NR_newRAT]",50960,"noted","2017-05-08T10:23:45.450","2017-05-08T10:27:53.163","","","","","","","","","","","","","","",""]
["R4-1705672","Sub6 Reference Sensitivity","Qualcomm Incorporated","Kyoungseok Oh","66120","other","","","","432","10.4.4.1","REFSENS and MSD evaluation assumption [NR_newRAT]",52020,"noted","2017-05-08T10:23:45.717","2017-05-08T10:27:53.180","","","","","","","","","","","","","","",""]
["R4-1705673","On Off Mask Transients","Qualcomm Incorporated","Kyoungseok Oh","66120","other","","","","428","10.4.3.2","ON/OFF time mask [NR_newRAT]",46870,"noted","2017-05-08T10:23:45.980","2017-05-08T10:27:53.180","","","","","","","","","","","","","","",""]
["R4-1705674","Sub6 SEM","Qualcomm Incorporated","Kyoungseok Oh","66120","other","","","","429","10.4.3.3","Spurious emission [NR_newRAT]",567400,"noted","2017-05-08T10:23:46.263","2017-05-08T10:27:53.180","","","","","","","","","","","","","","",""]
["R4-1705675","mmW SEM","Qualcomm Incorporated","Kyoungseok Oh","66120","other","","","","429","10.4.3.3","Spurious emission [NR_newRAT]",567700,"revised","2017-05-08T10:23:46.620","2017-05-08T10:27:53.193","","R4-1706073","","","","","","","","","","","","",""]
["R4-1705676","NR channel bandwidth definition","MediaTek Inc.","Kyoungseok Oh","66120","other","","","","418","10.3.1","Channel bandwidth and subcarrier spacing [NR_newRAT]",45660,"noted","2017-05-08T10:23:46.933","2017-05-08T10:27:53.193","","","Rel-15","","","NR_newRAT","","","","","","","","",""]
["R4-1705677","mmW UE power class","MediaTek Inc.","Kyoungseok Oh","66120","other","","","","427","10.4.3.1","UE power class and MPR/A-MPR [NR_newRAT]",51060,"noted","2017-05-08T10:23:47.230","2017-05-08T10:27:53.193","","","Rel-15","","","NR_newRAT","","","","","","","","",""]
["R4-1705678","mmWave phase noise impact on ACS & blocking requirements for UE receiver","MediaTek Inc.","Kyoungseok Oh","66120","other","","","","433","10.4.4.2","Blocking Requirements [NR_newRAT]",52040,"noted","2017-05-08T10:23:47.510","2017-05-08T10:27:53.210","","","Rel-15","","","NR_newRAT","","","","","","","","",""]
["R4-1705679","CA_1A-41A with uplink in Band 41","Qualcomm Incorporated","Kyoungseok Oh","66120","other","","","","95","7.2.2","UE RF (36.101) [LTE_CA_R14_2DL1UL-Core]",45260,"noted","2017-05-08T10:23:47.837","2017-05-08T10:27:53.227","","","","","","","","","","","","","","",""]
["R4-1705680","Filter considerations for CA_66-70","Qualcomm Incorporated","Kyoungseok Oh","66120","other","","","","95","7.2.2","UE RF (36.101) [LTE_CA_R14_2DL1UL-Core]",567900,"noted","2017-05-08T10:23:48.103","2017-05-08T10:27:53.227","","","","","","","","","","","","","","",""]
["R4-1705681","MPR for Power Class 2 with UL CA in Band 41","Qualcomm Incorporated","Kyoungseok Oh","66120","other","","","","332","9.7.1","UE RF (36.101) [LTE_CA_C_B41_PC2-core]",52450,"noted","2017-05-08T10:23:48.383","2017-05-08T10:27:53.227","","","","","","","","","","","","","","",""]
["R4-1705682","CA_NS_04 A-MPR for Power Class 2 with UL CA in Band 41","Qualcomm Incorporated","Kyoungseok Oh","66120","other","","","","332","9.7.1","UE RF (36.101) [LTE_CA_C_B41_PC2-core]",54390,"noted","2017-05-08T10:23:48.743","2017-05-08T10:27:53.240","","","","","","","","","","","","","","",""]
["R4-1705683","TP for TR 36.755: Frequency ranges","Qualcomm Incorporated, Skyworks Solutions, Inc., T-Mobile USA","Kyoungseok Oh","66120","pCR","","","","336","9.8.2","UE RF (36.101) [LTE600_US-core]",51610,"approved","2017-05-08T10:23:49.007","2017-05-08T10:27:53.240","","","Rel-15","36.755","0.0.1","LTE600_US-Core","","","","","","","","",""]
["R4-1705684","TP for TR 36.755: Rx blocking","Qualcomm Incorporated,  T-Mobile USA, Skyworks Solutions, Inc., Intel, Samsung, Nokia, Ericsson","Kyoungseok Oh","66120","pCR","","","","336","9.8.2","UE RF (36.101) [LTE600_US-core]",568400,"approved","2017-05-08T10:23:49.367","2017-05-08T10:27:53.257","","","Rel-15","36.755","0.0.1","LTE600_US-Core","","","","","","","","",""]
["R4-1705685","Update to CA_NS_04 SEM and additional spurious emissions","Qualcomm Incorporated","Kyoungseok Oh","66120","CR","","","","13","4.2.1","UE RF (core / EMC) [WI code or TEI12]",568500,"postponed","2017-05-08T10:23:49.710","2017-05-08T10:27:53.257","","","Rel-11","36.101","11.20.0","LTE_CA_B41-Core","4478","","F","","","","","",""]
["R4-1705686","Update to CA_NS_04 SEM and additional spurious emissions","Qualcomm Incorporated","Kyoungseok Oh","66120","CR","","","","13","4.2.1","UE RF (core / EMC) [WI code or TEI12]",568600,"withdrawn","2017-05-08T10:23:54.347",null,"","","Rel-12","36.101","12.15.0","LTE_CA_B41-Core","4479","","A","","","","","",""]
["R4-1705687","Update to CA_NS_04 SEM and additional spurious emissions","Qualcomm Incorporated","Kyoungseok Oh","66120","CR","","","","13","4.2.1","UE RF (core / EMC) [WI code or TEI12]",568700,"withdrawn","2017-05-08T10:23:59.087",null,"","","Rel-13","36.101","13.7.0","LTE_CA_B41-Core","4480","","A","","","","","",""]
["R4-1705688","Update to CA_NS_04 SEM and additional spurious emissions","Qualcomm Incorporated","Kyoungseok Oh","66120","CR","","","","13","4.2.1","UE RF (core / EMC) [WI code or TEI12]",568800,"withdrawn","2017-05-08T10:24:04.070",null,"","","Rel-14","36.101","14.3.0","LTE_CA_B41-Core","4481","","A","","","","","",""]
["R4-1705689","Missing entries in list of intra-band CA bands","Qualcomm Incorporated","Kyoungseok Oh","66120","CR","Agreement","","","89","7.1.2","UE RF (36.101) [LTE_CA_R14_intra-Core]",52690,"agreed","2017-05-08T10:24:09.643","2017-05-08T10:27:53.273","","","Rel-14","36.101","14.3.0","LTE_CA-Core","4482","","F","RP-171395","","","","",""]
["R4-1705690","Correction to NS_27 A-MPR table","Qualcomm Incorporated","Kyoungseok Oh","66120","CR","Agreement","","","291","7.29.2","RF [WI code or TEI14]",48610,"agreed","2017-05-08T10:24:14.793","2017-05-08T10:27:53.273","","","Rel-14","36.101","14.3.0","LTE_TDD_3550_CBRS_US-Core","4483","","F","RP-171289","","","","",""]
["R4-1705691","Introduction of Band 71 to 36.101","Qualcomm Incorporated","Kyoungseok Oh","66120","draftCR","","","","336","9.8.2","UE RF (36.101) [LTE600_US-core]",569100,"revised","2017-05-08T10:24:19.710","2017-05-08T10:27:53.273","","R4-1705887","Rel-14","36.101","14.3.0","LTE600_US-Core","","","B","","","","","",""]
["R4-1705692","TP for TR 36.714-02-01: CA between Band 5 and Band 48","Qualcomm Incorporated, Nokia","Kyoungseok Oh","66120","pCR","","","","95","7.2.2","UE RF (36.101) [LTE_CA_R14_2DL1UL-Core]",52410,"approved","2017-05-08T10:24:20.117","2017-05-08T10:27:53.287","","","Rel-14","36.714-02-01","0.7.0","LTE_CA_R14_2DL1UL-Core","","","","","","","","",""]
["R4-1705693","TP for TR 36.714-02-01: CA between Band 13 and Band 48","Qualcomm Incorporated, Nokia","Kyoungseok Oh","66120","pCR","","","","95","7.2.2","UE RF (36.101) [LTE_CA_R14_2DL1UL-Core]",52500,"approved","2017-05-08T10:24:20.477","2017-05-08T10:27:53.287","","","Rel-14","36.714-02-01","0.7.0","LTE_CA_R14_2DL1UL-Core","","","","","","","","",""]
["R4-1705694","A-MPR simulation for L-band FDD own band protection","Nokia, Alcatel-Lucent Shanghai Bell","Kyoungseok Oh","66120","discussion","","","","314","9.4","FDD operating band in the L-band for LTE [LTE_FDD_L_Band]",569400,"noted","2017-05-08T10:24:20.837","2017-05-08T10:27:53.287","","","","","","LTE_FDD_L_Band","","","","","","","","",""]
["R4-1705695","L-band TDD UE coexistence with MSS","Nokia, Alcatel-Lucent Shanghai Bell","Kyoungseok Oh","66120","other","","","","327","9.6.1","Band Arrangement [LTE_TDD_L_Band-core]",569500,"noted","2017-05-08T10:24:21.117","2017-05-08T10:27:53.303","","","","","","LTE_FDD_L_Band","","","","","","","","",""]
["R4-1705696","Channel raster and numbering scheme in NR","Nokia, Alcatel-Lucent Shanghai Bell","Kyoungseok Oh","66120","other","","","","419","10.3.2","Channel Raster [NR_newRAT]",45240,"noted","2017-05-08T10:24:21.383","2017-05-08T10:27:53.303","","","","","","NR_newRAT","","","","","","","","",""]
["R4-1705697","Sync signal raster and subcarrier spacing","Nokia, Alcatel-Lucent Shanghai Bell","Kyoungseok Oh","66120","other","","","","419","10.3.2","Channel Raster [NR_newRAT]",45670,"noted","2017-05-08T10:24:21.647","2017-05-08T10:27:53.303","","","","","","NR_newRAT","","","","","","","","",""]
["R4-1705698","Wide band operation and channel bandwidth in the NR","Nokia, Alcatel-Lucent Shanghai Bell","Kyoungseok Oh","66120","discussion","","","","418","10.3.1","Channel bandwidth and subcarrier spacing [NR_newRAT]",47710,"noted","2017-05-08T10:24:21.927","2017-05-08T10:27:53.320","","","","","","NR_newRAT","","","","","","","","",""]
["R4-1705699","UE capability for wideband operation","Nokia, Alcatel-Lucent Shanghai Bell","Kyoungseok Oh","66120","discussion","","","","418","10.3.1","Channel bandwidth and subcarrier spacing [NR_newRAT]",48620,"noted","2017-05-08T10:24:22.193","2017-05-08T10:27:53.320","","","","","","NR_newRAT","","","","","","","","",""]
["R4-1705700","Way-forward on 3.3-4.2 GHz band plan","Nokia, Alcatel-Lucent Shanghai Bell","Kyoungseok Oh","66120","other","","","","415","10.2.1.2","Band definition for NR bands [NR_newRAT]",47740,"noted","2017-05-08T10:24:22.457","2017-05-08T10:27:53.320","","","","","","NR_newRAT","","","","","","","","",""]
["R4-1705701","Handling of coexistence requirement with Altimeter for the bands 3.3-4.2 and 4.4-4.99GHz","Nokia, Alcatel-Lucent Shanghai Bell","Kyoungseok Oh","66120","other","","","","415","10.2.1.2","Band definition for NR bands [NR_newRAT]",52480,"noted","2017-05-08T10:24:22.723","2017-05-08T10:27:53.337","","","","","","NR_newRAT","","","","","","","","",""]
["R4-1705702","Conducted UE ACLR for frequency range 1","Nokia, Alcatel-Lucent Shanghai Bell, Qualcomm Incorporated","Kyoungseok Oh","66120","other","","","","422","10.3.5","ACLR and ACS [NR_newRAT]",54780,"noted","2017-05-08T10:24:23.003","2017-05-08T10:27:53.337","","","","","","NR_newRAT","","","","","","","","",""]
["R4-1705703","Conducted UE ACS for frequency range 1","Nokia, Alcatel-Lucent Shanghai Bell","Kyoungseok Oh","66120","other","","","","422","10.3.5","ACLR and ACS [NR_newRAT]",56570,"withdrawn","2017-05-08T10:24:23.270",null,"","","","","","NR_newRAT","","","","","","","","",""]
["R4-1705704","Cleanup of TS 36.307","ETSI MCC","Kyoungseok Oh","66120","CR","Agreement","related to RP-162523 (RAN #74), R4-1703922 (RAN4 #82bis) and corresponding email discussions","","18","4.2.6","Other specifications [WI code or TEI12]",570400,"revised","2017-05-08T10:24:23.580","2017-05-08T10:27:53.350","","R4-1706064","Rel-8","36.307","8.16.0","TEI8","0743","","F","","","","","",""]
["R4-1705705","Cleanup of TS 36.307","ETSI MCC","Kyoungseok Oh","66120","CR","Agreement","related to RP-162523 (RAN #74), R4-1703922 (RAN4 #82bis) and corresponding email discussions","","18","4.2.6","Other specifications [WI code or TEI12]",570500,"revised","2017-05-08T10:24:29.247","2017-05-08T10:27:53.350","","R4-1706065","Rel-9","36.307","9.18.0","TEI8","0744","","A","","","","","",""]
["R4-1705706","Cleanup of TS 36.307","ETSI MCC","Kyoungseok Oh","66120","CR","Agreement","related to RP-162523 (RAN #74), R4-1703922 (RAN4 #82bis) and corresponding email discussions","","18","4.2.6","Other specifications [WI code or TEI12]",570600,"revised","2017-05-08T10:24:33.257","2017-05-08T10:27:53.350","","R4-1706046","Rel-10","36.307","10.21.0","TEI10, LTE_4Rx_AP_DL","0745","","F","","","","","",""]
["R4-1705707","Cleanup of TS 36.307","ETSI MCC","Kyoungseok Oh","66120","CR","Agreement","related to RP-162523 (RAN #74), R4-1703922 (RAN4 #82bis) and corresponding email discussions","","18","4.2.6","Other specifications [WI code or TEI12]",570700,"revised","2017-05-08T10:24:37.097","2017-05-08T10:27:53.367","","R4-1706045","Rel-11","36.307","11.18.0","TEI10, LTE_4Rx_AP_DL","0746","","A","","","","","",""]
["R4-1705708","Cleanup of TS 36.307","ETSI MCC","Kyoungseok Oh","66120","CR","Agreement","related to RP-162523 (RAN #74), R4-1703922 (RAN4 #82bis) and corresponding email discussions","","18","4.2.6","Other specifications [WI code or TEI12]",570800,"revised","2017-05-08T10:24:41.340","2017-05-08T10:27:53.367","","R4-1706044","Rel-12","36.307","12.14.0","LC_MTC_LTE_cat0_B25_B26-Core, TEI12","0747","","F","","","","","",""]
["R4-1705709","Cleanup of TS 36.307","ETSI MCC","Kyoungseok Oh","66120","CR","Agreement","related to RP-162523 (RAN #74), R4-1703922 (RAN4 #82bis) and corresponding email discussions","","18","4.2.6","Other specifications [WI code or TEI12]",570900,"revised","2017-05-08T10:24:45.150","2017-05-08T10:27:53.367","","R4-1706043","Rel-13","36.307","13.6.0","LC_MTC_LTE_cat0_B25_B26-Core, LTE_MTCe2_L1_cat1_B25_B40-Core, NB_IOT_R14_bands-Core, LTE_4Rx_AP_DL_CA-Core, LTE_4Rx_AP_DL_CA-Perf, TEI13, LTE_high_speed-Perf","0748","","F","","","","","",""]
["R4-1705710","Cleanup of TS 36.307","ETSI MCC","Kyoungseok Oh","66120","CR","Agreement","related to RP-162523 (RAN #74), R4-1703922 (RAN4 #82bis) and corresponding email discussions","","18","4.2.6","Other specifications [WI code or TEI12]",571000,"revised","2017-05-08T10:24:49.177","2017-05-08T10:27:53.383","","R4-1706042","Rel-14","36.307","14.2.0","LC_MTC_LTE_cat0_B25_B26-Core, LTE_MTCe2_L1_cat1_B25_B40-Core, NB_IOT_R14_bands-Core, LTE_4Rx_AP_DL_CA-Core, LTE_4Rx_AP_DL_CA-Perf, LTE_high_speed-Perf","0749","","F","","","","","",""]
["R4-1705711","MPAC SCME UMi V/H clarification","Spirent, R&S","Kyoungseok Oh","66120","other","","","","144","7.11.1","General [LTE_MIMO_OTA-Core]",45790,"noted","2017-05-08T10:24:53.287","2017-05-10T07:07:51.767","","","","","","","","","","","","","","",""]
["R4-1705712","TS 38.101 User Equipment radio transmission and reception (Skeleton)","Qualcomm Incorporated","Kyoungseok Oh","66120","draft TS","Approval","","","424","10.4.1","UE RF General (ad-hoc MoM, Plan, Spec Structure) [NR_newRAT]",571200,"noted","2017-05-08T10:24:53.583","2017-05-08T10:27:53.383","","","Rel-15","38.101","0.0.1","NR_newRAT-Core","","","","","","","","",""]
["R4-1705713","Gapless measurement in eMTC","Nokia, Alcatel-Lucent Shanghai Bell","Kyoungseok Oh","66120","discussion","","","","46","5.4.3.1","BL/CE UE [LTE_MTCe2_L1-Core]",50110,"noted","2017-05-08T10:24:54.143","2017-05-08T10:27:53.397","","","Rel-13","","","","","","","","","","","",""]
["R4-1705714","Introducing gapless measurement requirement for eMTC R13","Nokia, Alcatel-Lucent Shanghai Bell","Kyoungseok Oh","66120","CR","Agreement","","","46","5.4.3.1","BL/CE UE [LTE_MTCe2_L1-Core]",50120,"revised","2017-05-08T10:24:54.457","2017-05-08T10:27:53.397","","R4-1705994","Rel-13","36.133","13.7.0","LTE_MTCe2_L1-Core","4989","","F","","","","","",""]
["R4-1705715","Introducing gapless measurement requirement for eMTC R14","Nokia, Alcatel-Lucent Shanghai Bell","Kyoungseok Oh","66120","CR","Agreement","","","46","5.4.3.1","BL/CE UE [LTE_MTCe2_L1-Core]",50130,"revised","2017-05-08T10:24:59.233","2017-05-23T15:07:51.740","","R4-1706273","Rel-14","36.133","14.3.0","LTE_MTCe2_L1-Core","4990","","A","","","","","",""]
["R4-1705716","[draft] LS on gapless measurement for eMTC","Nokia, Alcatel-Lucent Shanghai Bell","Kyoungseok Oh","66120","LS out","","","","46","5.4.3.1","BL/CE UE [LTE_MTCe2_L1-Core]",51470,"noted","2017-05-08T10:25:04.647","2017-05-08T10:27:53.413","","","Rel-13","","","","","","","","","RAN2","RAN1","",""]
["R4-1705717","eMTC BS PRACH performance test","Nokia, Alcatel-Lucent Shanghai Bell","Kyoungseok Oh","66120","discussion","","","","55","5.4.7","BS performance (36.104/36.141) [LTE_MTCe2_L1-Perf]",48170,"noted","2017-05-08T10:25:04.943","2017-05-08T10:27:53.413","","","Rel-13","","","","","","","","","","","",""]
["R4-1705718","CR on eMTC BS PRACH requirements R13","Nokia, Alcatel-Lucent Shanghai Bell","Kyoungseok Oh","66120","CR","Agreement","","","55","5.4.7","BS performance (36.104/36.141) [LTE_MTCe2_L1-Perf]",48171,"noted","2017-05-08T10:25:05.240","2017-05-08T10:27:53.413","","R4-1705999","Rel-13","36.104","13.7.0","LTE_MTCe2_L1-Perf","4688","","F","","","","","",""]
["R4-1705719","CR on eMTC BS PRACH requirements R14","Nokia, Alcatel-Lucent Shanghai Bell","Kyoungseok Oh","66120","CR","Agreement","","","55","5.4.7","BS performance (36.104/36.141) [LTE_MTCe2_L1-Perf]",571800,"withdrawn","2017-05-08T10:25:10.090",null,"","","Rel-14","36.104","14.3.0","LTE_MTCe2_L1-Perf","4689","","A","","","","","",""]
["R4-1705720","CR on eMTC BS PRACH conformance tests R13","Nokia, Alcatel-Lucent Shanghai Bell","Kyoungseok Oh","66120","CR","Agreement","","","55","5.4.7","BS performance (36.104/36.141) [LTE_MTCe2_L1-Perf]",571801,"noted","2017-05-08T10:25:14.443","2017-05-08T10:27:53.427","","R4-1706000","Rel-13","36.141","13.7.0","LTE_MTCe2_L1-Perf","1053","","F","","","","","",""]
["R4-1705721","CR on eMTC BS PRACH conformance tests R14","Nokia, Alcatel-Lucent Shanghai Bell","Kyoungseok Oh","66120","CR","Agreement","","","55","5.4.7","BS performance (36.104/36.141) [LTE_MTCe2_L1-Perf]",572000,"withdrawn","2017-05-08T10:25:18.470",null,"","","Rel-14","36.141","14.3.0","LTE_MTCe2_L1-Perf","1054","","A","","","","","",""]
["R4-1705722","Simulation results for UL 256QAM","Nokia, Alcatel-Lucent Shanghai Bell","Kyoungseok Oh","66120","discussion","","","","150","7.12.3","Demodulation (36.104/36.141) [LTE_UL_CAP_enh-Core/Perf]",53010,"noted","2017-05-08T10:25:22.527","2017-05-08T10:27:53.443","","","Rel-14","","","","","","","","","","","",""]
["R4-1705723","Simulation results for PUSCH in UpPTS","Nokia, Alcatel-Lucent Shanghai Bell","Kyoungseok Oh","66120","discussion","","","","150","7.12.3","Demodulation (36.104/36.141) [LTE_UL_CAP_enh-Core/Perf]",53030,"noted","2017-05-08T10:25:22.807","2017-05-08T10:27:53.443","","","Rel-14","","","","","","","","","","","",""]
["R4-1705724","Further discussion on RRM requirements for feMBMS","Nokia, Alcatel-Lucent Shanghai Bell","Kyoungseok Oh","66120","discussion","","","","155","7.13.3","RRM core (36.133) [MBMS_LTE_enh2-Core]",50360,"noted","2017-05-08T10:25:23.073","2017-05-08T10:27:53.460","","","Rel-14","","","","","","","","","","","",""]
["R4-1705725","CR on measurement performance scaling with MPDCCH monitoring CEModeA","Nokia, Alcatel-Lucent Shanghai Bell","Kyoungseok Oh","66120","CR","Agreement","","","213","7.18.3.2.1","UE MPDCCH monitoring configuration [LTE_feMTC-Core]",572500,"revised","2017-05-08T10:25:23.337","2017-05-08T10:27:53.460","","R4-1705980","Rel-14","36.133","14.3.0","LTE_feMTC-Core","4991","","B","","","","","",""]
["R4-1705726","CR on measurement performance scaling with MPDCCH monitoring CEModeB","Nokia, Alcatel-Lucent Shanghai Bell","Kyoungseok Oh","66120","CR","Agreement","","","213","7.18.3.2.1","UE MPDCCH monitoring configuration [LTE_feMTC-Core]",572600,"revised","2017-05-08T10:25:27.940","2017-05-08T10:27:53.460","","R4-1705981","Rel-14","36.133","14.3.0","LTE_feMTC-Core","4992","","B","","","","","",""]
["R4-1705727","RLM enhancement for feMTC","Nokia, Alcatel-Lucent Shanghai Bell","Kyoungseok Oh","66120","discussion","","","","217","7.18.3.2.5","RLM and timing [LTE_feMTC-Core]",50210,"noted","2017-05-08T10:25:32.780","2017-05-08T10:27:53.477","","","Rel-14","","","","","","","","","","","",""]
["R4-1705728","SI acquisition time for non-BL/CE UE","Nokia, Alcatel-Lucent Shanghai Bell","Kyoungseok Oh","66120","discussion","","","","219","7.18.4","RRM core for non-BL/CE UE (36.133) [LTE_feMTC-Core]",47080,"noted","2017-05-08T10:25:33.077","2017-05-08T10:27:53.477","","","Rel-14","","","","","","","","","","","",""]
["R4-1705729","RLM for non-BL/CE UE","Nokia, Alcatel-Lucent Shanghai Bell","Kyoungseok Oh","66120","discussion","","","","219","7.18.4","RRM core for non-BL/CE UE (36.133) [LTE_feMTC-Core]",572800,"noted","2017-05-08T10:25:33.367","2017-05-08T10:27:53.490","","","Rel-14","","","","","","","","","","","",""]
["R4-1705730","Simulation results for HST PRACH performance","Nokia, Alcatel-Lucent Shanghai Bell","Kyoungseok Oh","66120","discussion","","","","266","7.25.5","BS demodulation (36.104/36.141) [LTE_high_speed-Perf]",55360,"noted","2017-05-08T10:25:33.667","2017-05-08T10:27:53.490","","","Rel-14","","","","","","","","","","","",""]
["R4-1705731","TP on updated simulation results for BS IC with TO/FO","Nokia, Alcatel-Lucent Shanghai Bell, China Telecom","Kyoungseok Oh","66120","other","","","","298","8.1.1","General [FS_LTE _IC_BS]",45620,"approved","2017-05-08T10:25:33.967","2017-05-23T15:07:51.757","","","Rel-14","","","","","","","","","","","",""]
["R4-1705732","Discussion on test case for BS IC","Nokia, Alcatel-Lucent Shanghai Bell","Kyoungseok Oh","66120","discussion","","","","298","8.1.1","General [FS_LTE _IC_BS]",55210,"noted","2017-05-08T10:25:34.240","2017-05-08T10:27:53.490","","","Rel-14","","","","","","","","","","","",""]
["R4-1705733","Initial discussion on minimum amount of CRS for efeMTC","Nokia, Alcatel-Lucent Shanghai Bell","Kyoungseok Oh","66120","discussion","","","","395","9.15.1","General [LTE_eMTC4]",54850,"noted","2017-05-08T10:25:34.540","2017-05-08T10:27:53.507","","","Rel-15","","","","","","","","","","","",""]
["R4-1705734","Channel model Validation results","ETS-Lindgren, MVG Industries","Kyoungseok Oh","66120","discussion","Discussion","","","145","7.11.2","Performance requirements [LTE_MIMO_OTA-Core]",45280,"noted","2017-05-08T10:25:34.823","2017-05-08T10:27:53.507","","","","","","","","","","","","","","",""]
["R4-1705735","Channel model validation results","ETS-Lindgren, MVG Industries","Kyoungseok Oh","66120","CR","Agreement","","","145","7.11.2","Performance requirements [LTE_MIMO_OTA-Core]",45290,"revised","2017-05-08T10:25:35.120","2017-05-08T10:27:53.507","","R4-1705921","Rel-14","37.977","14.3.0","LTE_MIMO_OTA-Core","0060","","B","","","","","",""]
["R4-1705736","On Qin and Qout convergence in NB-IoT RLM","Intel Corporation","Kyoungseok Oh","66120","discussion","Discussion","","","60","5.5.3","RRM core (36.133) [NB_IOT-Core]",46740,"noted","2017-05-08T10:25:37.147","2017-05-08T10:27:53.523","","","Rel-13","","","NB_IOT-Core","","","","","","","","",""]
["R4-1705737","Rel-13 CR on corrections for RLM for NB-IoT","Intel Corporation","Kyoungseok Oh","66120","CR","Agreement","","","60","5.5.3","RRM core (36.133) [NB_IOT-Core]",46750,"noted","2017-05-08T10:25:37.427","2017-05-08T10:27:53.523","","","Rel-13","36.133","13.7.0","NB_IOT-Core","4993","","F","","","","","",""]
["R4-1705738","Rel-14 CR on corrections for RLM for NB-IoT","Intel Corporation","Kyoungseok Oh","66120","CR","Agreement","","","60","5.5.3","RRM core (36.133) [NB_IOT-Core]",49790,"withdrawn","2017-05-08T10:25:42.030",null,"","","Rel-14","36.133","14.3.0","NB_IOT-Core","","","A","","","","","",""]
["R4-1705739","Rel-13 CR on corrections for RLM test cases for NB-IoT","Intel Corporation","Kyoungseok Oh","66120","CR","Agreement","","","62","5.5.5","RRM Performance (36.133) [NB_IOT-Perf]",49730,"noted","2017-05-08T10:25:47.150","2017-05-08T10:27:53.537","","","Rel-13","36.133","13.7.0","NB_IOT-Perf","4995","","F","","","","","",""]
["R4-1705740","Rel-14 CR on corrections for RLM test cases for NB-IoT","Intel Corporation","Kyoungseok Oh","66120","CR","Agreement","","","62","5.5.5","RRM Performance (36.133) [NB_IOT-Perf]",49740,"withdrawn","2017-05-08T10:25:51.850",null,"","","Rel-14","36.133","14.3.0","NB_IOT-Perf","","","A","","","","","",""]
["R4-1705741","On defining the unwanted emissions requirements for mmWave","Intel Corporation","Kyoungseok Oh","66120","discussion","Discussion","","","429","10.4.3.3","Spurious emission [NR_newRAT]",52230,"noted","2017-05-08T10:25:56.280","2017-05-08T10:27:53.537","","","Rel-15","","","NR_newRAT","","","","","","","","",""]
["R4-1705742","Discussion on channel bandwidth and subcarrier spacing","NTT DOCOMO, INC.","Kyoungseok Oh","66120","other","","","","418","10.3.1","Channel bandwidth and subcarrier spacing [NR_newRAT]",577900,"noted","2017-05-08T10:25:56.560","2017-05-23T15:07:51.757","","","","","","","","","","","","","","",""]
["R4-1705743","Discussion on co-existence study for NR uplink","NTT DOCOMO, INC.","Kyoungseok Oh","66120","other","","","","422","10.3.5","ACLR and ACS [NR_newRAT]",49290,"noted","2017-05-08T10:25:56.827","2017-05-08T10:27:53.553","","","","","","","","","","","","","","",""]
["R4-1705744","Discussion on MBSFN measurement requirement for FeMBMS","Qualcomm Incorporated","Kyoungseok Oh","66120","discussion","Discussion","","","155","7.13.3","RRM core (36.133) [MBMS_LTE_enh2-Core]",56000,"noted","2017-05-08T10:25:57.107","2017-05-08T10:27:53.553","","","","","","MBMS_LTE_enh2-Core","","","","","","","","",""]
["R4-1705745","Discussion on RRM Requirement for FeMBMS","Qualcomm Incorporated","Kyoungseok Oh","66120","discussion","Discussion","","","155","7.13.3","RRM core (36.133) [MBMS_LTE_enh2-Core]",56010,"noted","2017-05-08T10:25:57.390","2017-05-08T10:27:53.570","","","","","","MBMS_LTE_enh2-Core","","","","","","","","",""]
["R4-1705746","Test Configuration for Burst Gap","Qualcomm Incorporated","Kyoungseok Oh","66120","discussion","Discussion","","","272","7.26.3","RRM performance (36.133) [LTE_meas_gap_enh-Perf]",47150,"noted","2017-05-08T10:25:57.670","2017-05-08T10:27:53.570","","","","","","LTE_meas_gap_enh-Perf","","","","","","","","",""]
["R4-1705747","Discussion on Demodulation Test for FeMBMS","Qualcomm Incorporated","Kyoungseok Oh","66120","discussion","Discussion","","","157","7.13.5","Demodulation (36.101) [MBMS_LTE_enh2-Perf]",53680,"noted","2017-05-08T10:25:57.950","2017-05-08T10:27:53.570","","","","","","MBMS_LTE_enh2-Perf","","","","","","","","",""]
["R4-1705748","Test Configuration for NCSG","Qualcomm Incorporated","Kyoungseok Oh","66120","discussion","Discussion","","","272","7.26.3","RRM performance (36.133) [LTE_meas_gap_enh-Perf]",47170,"noted","2017-05-08T10:25:58.233","2017-05-08T10:27:53.583","","","","","","LTE_meas_gap_enh-Perf","","","","","","","","",""]
["R4-1705749","LS response on NCSG non-CA","Qualcomm Incorporated","Kyoungseok Oh","66120","LS out","","","","270","7.26.2.1","Gap pattern, signaling and capability (RAN2 related) [LTE_meas_gap_enh-Core]",51130,"revised","2017-05-08T10:25:58.497","2017-05-08T10:27:53.583","","R4-1705951","Rel-14","","","LTE_meas_gap_enh-Core","","","","","","RAN2","","",""]
["R4-1705750","LS on system information and measurement signalling on FeMBMS carrier","Qualcomm Incorporated","Kyoungseok Oh","66120","LS out","","","","155","7.13.3","RRM core (36.133) [MBMS_LTE_enh2-Core]",572400,"revised","2017-05-08T10:25:58.777","2017-05-08T10:27:53.600","","R4-1706262","Rel-14","","","MBMS_LTE_enh2-Core","","","","","","RAN2","","",""]
["R4-1705751","Discussion on test configuration for Class B eFD-MIMO enhancement","Qualcomm Incorporated","Kyoungseok Oh","66120","discussion","Discussion","","","287","7.28.2.5","CRI-RS Enhancement [LTE_eFDMIMO-Perf]",47770,"noted","2017-05-08T10:25:59.077","2017-05-08T10:27:53.600","","","","","","LTE_eFDMIMO-Perf","","","","","","","","",""]
["R4-1705752","MIMO beam steering matrix for class A eFD-MIMO","Qualcomm Incorporated","Kyoungseok Oh","66120","discussion","Discussion","","","284","7.28.2.2","Class A PMI [LTE_eFDMIMO-Perf]",47790,"noted","2017-05-08T10:25:59.340","2017-05-08T10:27:53.600","","","","","","LTE_eFDMIMO-Perf","","","","","","","","",""]
["R4-1705753","Introduction of test case for Burst gap","Qualcomm Incorporated","Kyoungseok Oh","66120","CR","Agreement","","","272","7.26.3","RRM performance (36.133) [LTE_meas_gap_enh-Perf]",47160,"revised","2017-05-08T10:25:59.620","2017-05-08T10:27:53.617","","R4-1706171","Rel-14","36.133","14.3.0","LTE_meas_gap_enh-Perf","4997","","B","","","","","",""]
["R4-1705754","Introduction of test case for NCSG","Qualcomm Incorporated","Kyoungseok Oh","66120","CR","Agreement","","","272","7.26.3","RRM performance (36.133) [LTE_meas_gap_enh-Perf]",47180,"revised","2017-05-08T10:26:04.147","2017-05-08T10:27:53.617","","R4-1706170","Rel-14","36.133","14.3.0","LTE_meas_gap_enh-Perf","4998","","B","","","","","",""]
["R4-1705755","[DRAFT] Introduction of TDD L band into TS 36.113","Etisalat, Huawei, Hisilicon","Kyoungseok Oh","66120","draftCR","Endorsement","","","330","9.6.4","Other specifications [LTE_TDD_L_Band]",575700,"postponed","2017-05-08T10:26:08.950","2017-05-08T10:27:53.647","","","Rel-15","36.113","14.2.0","LTE_TDD_L_Band-Core","","","","","","","","",""]
["R4-1705756","[DRAFT] Introduction of TDD L band into TS 36.124","Etisalat, Huawei, Hisilicon","Kyoungseok Oh","66120","draftCR","Endorsement","","","330","9.6.4","Other specifications [LTE_TDD_L_Band]",575800,"postponed","2017-05-08T10:26:09.263","2017-05-08T10:27:53.663","","","Rel-15","36.124","14.1.0","LTE_TDD_L_Band-Core","","","","","","","","",""]
["R4-1705757","[DRAFT] Introduction of TDD L band into TS 36.133","Etisalat, Huawei, Hisilicon","Kyoungseok Oh","66120","draftCR","Endorsement","","","330","9.6.4","Other specifications [LTE_TDD_L_Band]",575500,"noted","2017-05-08T10:26:09.560","2017-05-08T10:27:53.663","","R4-1706017","Rel-15","36.133","14.3.0","LTE_TDD_L_Band-Core","","","","","","","","",""]
["R4-1705758","[DRAFT] Introduction of TDD L band into TS 37.104","Etisalat, Huawei, Hisilicon","Kyoungseok Oh","66120","draftCR","Endorsement","","","330","9.6.4","Other specifications [LTE_TDD_L_Band]",575900,"postponed","2017-05-08T10:26:09.857","2017-05-08T10:27:53.663","","","Rel-15","37.104","14.3.0","LTE_TDD_L_Band-Core","","","","","","","","",""]
["R4-1705759","[DRAFT] Introduction of TDD L band into TS 37.141","Etisalat, Huawei, Hisilicon","Kyoungseok Oh","66120","draftCR","Endorsement","","","330","9.6.4","Other specifications [LTE_TDD_L_Band]",576000,"postponed","2017-05-08T10:26:10.137","2017-05-08T10:27:53.677","","","Rel-15","37.141","14.3.0","LTE_TDD_L_Band-Perf","","","","","","","","",""]
["R4-1705760","[DRAFT] Introduction of TDD L band into TS 37.113","Etisalat, Huawei, Hisilicon","Kyoungseok Oh","66120","draftCR","Endorsement","","","330","9.6.4","Other specifications [LTE_TDD_L_Band]",576100,"postponed","2017-05-08T10:26:10.420","2017-05-08T10:27:53.677","","","Rel-15","37.113","14.1.0","LTE_TDD_L_Band-Core","","","","","","","","",""]
["R4-1705761","[DRAFT] Introduction of TDD L band into TS 25.101","Etisalat, Huawei, Hisilicon","Kyoungseok Oh","66120","draftCR","Endorsement","","","330","9.6.4","Other specifications [LTE_TDD_L_Band]",576200,"postponed","2017-05-08T10:26:10.717","2017-05-08T10:27:53.693","","","Rel-15","25.101","14.0.0","LTE_TDD_L_Band-Core","","","","","","","","",""]
["R4-1705762","[DRAFT] Introduction of TDD L band into TS 25.104","Etisalat, Huawei, Hisilicon","Kyoungseok Oh","66120","draftCR","Endorsement","","","330","9.6.4","Other specifications [LTE_TDD_L_Band]",576300,"postponed","2017-05-08T10:26:11.027","2017-05-08T10:27:53.693","","","Rel-15","25.104","14.1.0","LTE_TDD_L_Band-Core","","","","","","","","",""]
["R4-1705763","[DRAFT] Introduction of TDD L band into TS 25.133","Etisalat, Huawei, Hisilicon","Kyoungseok Oh","66120","draftCR","Endorsement","","","330","9.6.4","Other specifications [LTE_TDD_L_Band]",575600,"noted","2017-05-08T10:26:11.323","2017-05-08T10:27:53.693","","R4-1706018","Rel-15","25.133","14.1.0","LTE_TDD_L_Band-Core","","","","","","","","",""]
["R4-1705764","[DRAFT] Introduction of TDD L band into TS 25.141","Etisalat, Huawei, Hisilicon","Kyoungseok Oh","66120","draftCR","Endorsement","","","330","9.6.4","Other specifications [LTE_TDD_L_Band]",576400,"postponed","2017-05-08T10:26:11.603","2017-05-08T10:27:53.710","","","Rel-15","36.141","14.3.0","LTE_TDD_L_Band-Perf","","","","","","","","",""]
["R4-1705765","TP for TR: A-MPR summary for EESS protection for TDD operation in L-band","Etisalat, Huawei, Hisilicon","Kyoungseok Oh","66120","other","Approval","Add text in the TR","","328","9.6.2","UE RF (36.101) [LTE_TDD_L_Band-core]",56150,"revised","2017-05-08T10:26:11.870","2017-05-08T10:27:53.710","","R4-1706117","","36.753","","LTE_TDD_L_Band-Perf","","","","","","","","",""]
["R4-1705766","TP for TR: A-MPR summary for MSS protection for TDD operation in L-band","Etisalat, Huawei, Hisilicon","Kyoungseok Oh","66120","other","Approval","Add text in the TR","","328","9.6.2","UE RF (36.101) [LTE_TDD_L_Band-core]",56210,"noted","2017-05-08T10:26:12.167","2017-05-08T10:27:53.727","","","","36.753","","LTE_TDD_L_Band-Perf","","","","","","","","",""]
["R4-1705767","REFSENS for flexible channel bandwidth","ZTE Corporation","Kyoungseok Oh","66120","discussion","Discussion","","","446","10.5.4.3","Other Rx requirements [NR_newRAT]",54800,"noted","2017-05-08T10:26:12.430","2017-05-08T10:27:53.727","","","","","","","","","","","","","","",""]
["R4-1705768","CR to TR38.803: Occupied bandwidth","ZTE","Kyoungseok Oh","66120","CR","Agreement","","","410","10.1.1","TR maintenance [NR_newRAT]",576800,"agreed","2017-05-08T10:26:12.727","2017-05-08T10:27:53.727","","","Rel-14","38.803","14.0.0","NR_newRAT","0011","","B","RP-171253","","","","",""]
["R4-1705769","TP for TR36.714-04-01: delta Tib and delta Rib for CA_39A-40D_BCS0","ZTE","Kyoungseok Oh","66120","pCR","Approval","","","107","7.4.2","UE RF (36.101) [LTE_CA_R14_4DL1UL-Core]",45100,"approved","2017-05-08T10:26:14.587","2017-05-08T10:27:53.740","","","Rel-14","36.714-04-01","0.7.0","LTE_CA_R14_4DL1UL-Core","","","","","","","","",""]
["R4-1705770","TP for TR36.714-05-01: delta Tib and delta Rib for CA_39A-40E_BCS0","ZTE","Kyoungseok Oh","66120","pCR","Approval","","","113","7.5.2","UE RF (36.101) [LTE_CA_R14_5DL1UL-Core]",47250,"approved","2017-05-08T10:26:14.913","2017-05-08T10:27:53.740","","","Rel-14","36.714-05-01","0.7.0","LTE_CA_R14_5DL1UL-Core","","","","","","","","",""]
["R4-1705771","TP for TR36.714-04-01: delta Tib and delta Rib for CA_39C-40C_BCS0","ZTE","Kyoungseok Oh","66120","pCR","Approval","","","107","7.4.2","UE RF (36.101) [LTE_CA_R14_4DL1UL-Core]",47240,"approved","2017-05-08T10:26:15.240","2017-05-08T10:27:53.757","","","Rel-14","36.714-04-01","0.7.0","LTE_CA_R14_4DL1UL-Core","","","","","","","","",""]
["R4-1705772","TP for TR36.714-05-01: delta Tib and delta Rib for CA_39C-40D_BCS0","ZTE","Kyoungseok Oh","66120","pCR","Approval","","","113","7.5.2","UE RF (36.101) [LTE_CA_R14_5DL1UL-Core]",48950,"approved","2017-05-08T10:26:15.570","2017-05-08T10:27:53.757","","","Rel-14","36.714-05-01","0.7.0","LTE_CA_R14_5DL1UL-Core","","","","","","","","",""]
["R4-1705773","Update of LAA REFSENS exclusion region","Qualcomm Incorporated","Kyoungseok Oh","66120","CR","Agreement","","","34","5.3.1","UE RF core (36.101) [LTE_LAA-Core]",55830,"revised","2017-05-08T10:26:15.897","2017-05-08T10:27:53.773","","R4-1705910","Rel-14","36.101","14.3.0","LTE_LAA-Core","4484","","F","","","","","",""]
["R4-1705774","Reply LS on configuration values for SS burst set periodicity","Nokia, Alcatel-Lucent Shanghai Bell","Kyoungseok Oh","66120","LS out","Approval","","","411","10.1.2","Topics related to incoming LS from other WG [NR_newRAT]",49150,"noted","2017-05-08T10:26:21.717","2017-05-08T10:27:53.773","","","Rel-15","","","NR_newRAT","","","","","","RAN1","","",""]
["R4-1705775","On transmit timing requirements for FeMTC (Cat-M2)","Qualcomm Incorporated","Kyoungseok Oh","66120","discussion","Discussion","","","217","7.18.3.2.5","RLM and timing [LTE_feMTC-Core]",51520,"noted","2017-05-08T10:26:21.983","2017-05-08T10:27:53.773","","","","","","","","","","","","","","",""]
["R4-1705776","Usecases for ON/OFF time mask for NR","Ericsson","Kyoungseok Oh","66120","discussion","","","","428","10.4.3.2","ON/OFF time mask [NR_newRAT]",49180,"withdrawn","2017-05-08T10:26:22.263",null,"","","Rel-15","","","NR_newRAT","","","","","","","","",""]
["R4-1705777","Impact of UL processing time on UE RF for sTTi operation","Ericsson","Kyoungseok Oh","66120","discussion","","","","377","9.13.2.3","Other UE requirements [LTE_sTTIandPT-core]",577700,"withdrawn","2017-05-08T10:26:22.543",null,"","","Rel-15","","","NR_newRAT","","","","","","","","",""]
["R4-1705778","New work item proposal: High Power UE for LTE Band 38","Vodafone","Kyoungseok Oh","66120","discussion","","","","473","13","Revision of the Work Plan",45350,"noted","2017-05-08T10:26:22.827","2017-05-08T10:27:53.803","","","","","","","","","","","","","","",""]
["R4-1705779","NR channel bandwidths","Vodafone","Kyoungseok Oh","66120","discussion","","","","420","10.3.3","Spectrum utilization [NR_newRAT]",53910,"noted","2017-05-08T10:26:23.120","2017-05-08T10:27:53.803","","","","","","","","","","","","","","",""]
["R4-1705780","LTE TRP and TRS BHH measurement further analysis","Vodafone","Kyoungseok Oh","66120","discussion","","","","139","7.10.1","General [LTE_UTRA_TRP_TRS-Core]",610200,"noted","2017-05-08T10:26:23.417","2017-05-08T10:27:53.817","","","","","","","","","","","","","","",""]
["R4-1705781","CA_3DL_3A-8A-20A_1UL_BCS0 delta TIB/RIB text proposal","Vodafone","Kyoungseok Oh","66120","discussion","","","","101","7.3.2","UE RF (36.101) [LTE_CA_R14_3DL1UL-Core]",45990,"revised","2017-05-08T10:26:23.697","2017-05-08T10:27:53.833","","R4-1705904","","","","","","","","","","","","",""]
["R4-1705782","CA_4DL_1A-3A-8A-20A_1UL_BCS0 delta TIB/RIB text proposal","Vodafone","Kyoungseok Oh","66120","discussion","","","","107","7.4.2","UE RF (36.101) [LTE_CA_R14_4DL1UL-Core]",48920,"approved","2017-05-08T10:26:23.980","2017-05-08T10:27:53.833","","","","","","","","","","","","","","",""]
["R4-1705783","Refinement of the emission limits and frequency ranges for EMC RE and RF RSE requirements","Huawei","Kyoungseok Oh","66120","discussion","","","","364","9.12.2.7","EMC requirements [AASenh_BS_LTE_UTRA-Core]",54920,"noted","2017-05-08T10:26:24.260","2017-05-08T10:27:53.850","","","","","","AASenh_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-1705784","Alignment of the frequency ranges for the NR RRM requirements and NR testability","Huawei, HiSilicon","Kyoungseok Oh","66120","discussion","","","","449","10.6.1","RRM General (ad-hoc MoM, Plan, Spec structure) [NR_newRAT]",47960,"noted","2017-05-08T10:26:24.557","2017-05-08T10:27:53.850","","","","","","NR_newRAT","","","","","","","","",""]
["R4-1705785","On the relations among the conducted and OTA requirements for NR RRM","Huawei, HiSilicon","Kyoungseok Oh","66120","discussion","","","","454","10.6.6","Measurement definition and reference point [NR_newRAT]",48030,"noted","2017-05-08T10:26:24.840","2017-05-08T10:27:53.867","","","","","","NR_newRAT","","","","","","","","",""]
["R4-1705786","CR to TS 37.105: Correction of the spurious emissions requirement","Huawei","Kyoungseok Oh","66120","CR","","","","24","5.1.2","BS RF (37.105) [AAS_BS_LTE_UTRA-Core]",578600,"revised","2017-05-08T10:26:25.120","2017-05-08T10:27:53.867","","R4-1706154","Rel-13","37.105","13.4.0","AAS_BS_LTE_UTRA-Core","0059","","F","","","","","",""]
["R4-1705787","CR to TS 37.105: Correction of the spurious emissions requirement","Huawei","Kyoungseok Oh","66120","CR","","","","24","5.1.2","BS RF (37.105) [AAS_BS_LTE_UTRA-Core]",578700,"revised","2017-05-08T10:26:27.213","2017-05-08T10:27:53.880","","R4-1706155","Rel-14","37.105","14.0.0","AAS_BS_LTE_UTRA-Core","0060","","A","","","","","",""]
["R4-1705788","On updating the non-AAS BS references to Rel-14 versions","Huawei","Kyoungseok Oh","66120","discussion","","","","22","5.1","Base Station (BS) RF requirements for Active Antenna System (AAS) [AAS_BS_LTE_UTRA-Core]",578800,"noted","2017-05-08T10:26:29.600","2017-05-08T10:27:53.880","","","","","","AAS_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-1705789","Clarification on the need for Cat. A CR's for Rel-14 versions of the AAS specifications","Huawei","Kyoungseok Oh","66120","discussion","","","","22","5.1","Base Station (BS) RF requirements for Active Antenna System (AAS) [AAS_BS_LTE_UTRA-Core]",578900,"noted","2017-05-08T10:26:29.880","2017-05-08T10:27:53.880","","","","","","AAS_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-1705790","CR to TS 37.105: BS demodulation requirements update","Huawei, Ericsson, Nokia","Kyoungseok Oh","66120","CR","Agreement","","","24","5.1.2","BS RF (37.105) [AAS_BS_LTE_UTRA-Core]",579000,"agreed","2017-05-08T10:26:30.193","2017-05-08T10:27:53.897","","","Rel-14","37.105","14.0.0","AAS_BS_LTE_UTRA-Core","0061","","A","RP-171305","","","","",""]
["R4-1705791","CR to TS 37.105: Addition of 1.4 and 3 MHz channel bandwidths for Band 65","Huawei, Ericsson, Nokia","Kyoungseok Oh","66120","CR","Agreement","","","24","5.1.2","BS RF (37.105) [AAS_BS_LTE_UTRA-Core]",579100,"agreed","2017-05-08T10:26:32.613","2017-05-08T10:27:53.897","","","Rel-14","37.105","14.0.0","AAS_BS_LTE_UTRA-Core","0062","","A","RP-171305","","","","",""]
["R4-1705792","CR to TS 37.114: Isolation of Band 46 and NB-IoT from the AAS BS specification","Huawei, Ericsson, Nokia","Kyoungseok Oh","66120","CR","Agreement","","","28","5.1.4","Other specifications [AAS_BS_LTE_UTRA-Core/Perf]",579200,"agreed","2017-05-08T10:26:34.267","2017-05-08T10:27:53.913","","","Rel-14","37.114","14.0.0","AAS_BS_LTE_UTRA-Core, AAS_BS_LTE_UTRA-Perf","0009","","A","RP-171306","","","","",""]
["R4-1705793","CR to TS 37.145-1: Isolation of Band 46 from the AAS BS specification","Huawei, Ericsson, Nokia","Kyoungseok Oh","66120","CR","Agreement","","","26","5.1.3.1","Maintenance for TS37.145-1 [AAS_BS_LTE_UTRA-Perf]",579300,"agreed","2017-05-08T10:26:36.173","2017-05-08T10:27:53.913","","","Rel-14","37.145-1","14.0.0","AAS_BS_LTE_UTRA-Perf","0058","","A","RP-171306","","","","",""]
["R4-1705794","CR to TS 37.145-1: Isolation of the NB-IoT from the AAS BS specification","Huawei, Ericsson, Nokia","Kyoungseok Oh","66120","CR","Agreement","","","26","5.1.3.1","Maintenance for TS37.145-1 [AAS_BS_LTE_UTRA-Perf]",579400,"agreed","2017-05-08T10:26:38.013","2017-05-08T10:27:53.927","","","Rel-14","37.145-1","14.0.0","AAS_BS_LTE_UTRA-Perf","0059","","A","RP-171306","","","","",""]
["R4-1705795","CR to TS 37.145-1: BS demodulation requirements update","Huawei, Ericsson, Nokia","Kyoungseok Oh","66120","CR","Agreement","","","26","5.1.3.1","Maintenance for TS37.145-1 [AAS_BS_LTE_UTRA-Perf]",579500,"agreed","2017-05-08T10:26:39.857","2017-05-08T10:27:53.927","","","Rel-14","37.145-1","14.0.0","AAS_BS_LTE_UTRA-Perf","0060","","A","RP-171306","","","","",""]
["R4-1705796","CR to TS 37.145-1: Correction of the 256QAM test requirement for EVM","Huawei","Kyoungseok Oh","66120","CR","Agreement","","","26","5.1.3.1","Maintenance for TS37.145-1 [AAS_BS_LTE_UTRA-Perf]",579600,"agreed","2017-05-08T10:26:41.667","2017-05-08T10:27:53.943","","","Rel-14","37.145-1","14.0.0","AAS_BS_LTE_UTRA-Perf","0061","","A","RP-171306","","","","",""]
["R4-1705797","CR to TS 37.145-1: Update of Rel-13 references to the UTRA, EUTRA and MSR specifications","Huawei, Ericsson, Nokia","Kyoungseok Oh","66120","CR","Agreement","","","26","5.1.3.1","Maintenance for TS37.145-1 [AAS_BS_LTE_UTRA-Perf]",579700,"agreed","2017-05-08T10:26:43.510","2017-05-08T10:27:53.960","","","Rel-14","37.145-1","14.0.0","AAS_BS_LTE_UTRA-Perf","0062","","A","RP-171306","","","","",""]
["R4-1705798","CR to TS 37.145-1: Introduction of Rel-13 bands: 45, 65, 66 and 68","Huawei, Ericsson, Nokia","Kyoungseok Oh","66120","CR","Agreement","","","26","5.1.3.1","Maintenance for TS37.145-1 [AAS_BS_LTE_UTRA-Perf]",579800,"agreed","2017-05-08T10:26:45.163","2017-05-08T10:27:53.960","","","Rel-14","37.145-1","14.0.0","AAS_BS_LTE_UTRA-Perf","0063","","A","RP-171306","","","","",""]
["R4-1705799","CR to TS 37.145-2: Isolation of Band 46 from the AAS BS specification","Huawei, Ericsson, Nokia","Kyoungseok Oh","66120","CR","Agreement","","","27","5.1.3.2","Maintenance for TS37.145-2 [AAS_BS_LTE_UTRA-Perf]",579900,"agreed","2017-05-08T10:26:46.917","2017-05-08T10:27:53.973","","","Rel-14","37.145-2","14.0.0","AAS_BS_LTE_UTRA-Perf","0011","","A","RP-171306","","","","",""]
["R4-1705800","CR to TS 37.145-1: Correction of the test setup for the Tx spurious emissions requirement","Huawei","Kyoungseok Oh","66120","CR","Agreement","","","26","5.1.3.1","Maintenance for TS37.145-1 [AAS_BS_LTE_UTRA-Perf]",580000,"agreed","2017-05-08T10:26:49.333","2017-05-08T10:27:53.973","","","Rel-14","37.145-1","14.0.0","AAS_BS_LTE_UTRA-Perf","0064","","A","RP-171306","","","","",""]
["R4-1705801","CR to TS 37.145-1: MB-MSR update","Huawei, Ericsson, Nokia","Kyoungseok Oh","66120","CR","Agreement","","","26","5.1.3.1","Maintenance for TS37.145-1 [AAS_BS_LTE_UTRA-Perf]",580100,"agreed","2017-05-08T10:26:51.113","2017-05-08T10:27:53.973","","","Rel-14","37.145-1","14.0.0","AAS_BS_LTE_UTRA-Perf","0065","","A","RP-171306","","","","",""]
["R4-1705802","TP to TR 37.843: Total power dynamic range requirement","Huawei","Kyoungseok Oh","66120","pCR","","","","362","9.12.2.5","Other Transmitter Requirements [AASenh_BS_LTE_UTRA-Core]",580600,"approved","2017-05-08T10:26:52.860","2017-05-08T10:27:53.990","","","Rel-15","37.843","0.3.0","AASenh_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-1705803","TP to TR 37.843: Rx spurious requirement OTA","Huawei","Kyoungseok Oh","66120","pCR","","","","363","9.12.2.6","Other Receiver requirements [AASenh_BS_LTE_UTRA-Core]",631100,"approved","2017-05-08T10:26:53.187","2017-05-08T10:27:54.007","","","Rel-15","37.843","0.3.0","AASenh_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-1705804","TP to TR 37.843: Further details on the frequency error requirement OTA","Huawei","Kyoungseok Oh","66120","pCR","","","","362","9.12.2.5","Other Transmitter Requirements [AASenh_BS_LTE_UTRA-Core]",613600,"approved","2017-05-08T10:26:53.517","2017-05-08T10:27:54.007","","","Rel-15","37.843","0.3.0","AASenh_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-1705805","TP to TR 37.843: Consideration of missing aspects for core and conformance Tx spurious requirement OTA","Huawei","Kyoungseok Oh","66120","pCR","","","","362","9.12.2.5","Other Transmitter Requirements [AASenh_BS_LTE_UTRA-Core]",580400,"revised","2017-05-08T10:26:53.907","2017-05-08T10:27:54.007","","R4-1706139","Rel-15","37.843","0.3.0","AASenh_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-1705806","TP to TR 37.843: Alignment of the requirements structure in the eAAS TR","Huawei","Kyoungseok Oh","66120","pCR","","","","356","9.12.1","General [AASenh_BS_LTE_UTRA]",48590,"approved","2017-05-08T10:26:54.233","2017-05-08T10:27:54.007","","","Rel-15","37.843","0.3.0","AASenh_BS_LTE_UTRA","","","","","","","","",""]
["R4-1705807","TP to TR 37.843: UTRA demodulation requirements analysis","Huawei","Kyoungseok Oh","66120","pCR","","","","368","9.12.4","Demodulation requirements [AASenh_BS_LTE_UTRA-Perf]",580700,"approved","2017-05-08T10:26:54.560","2017-05-08T10:27:54.020","","","Rel-15","37.843","0.3.0","AASenh_BS_LTE_UTRA-Perf","","","","","","","","",""]
["R4-1705808","Consideration of the AWGN test conditions OTA","Huawei","Kyoungseok Oh","66120","discussion","","","","368","9.12.4","Demodulation requirements [AASenh_BS_LTE_UTRA-Perf]",580800,"noted","2017-05-08T10:26:54.873","2017-05-08T10:27:54.020","","","","","","AASenh_BS_LTE_UTRA-Perf","","","","","","","","",""]
["R4-1705809","TP to TR 37.843: Additional considerations for the OTA test setups","Huawei","Kyoungseok Oh","66120","pCR","","","","368","9.12.4","Demodulation requirements [AASenh_BS_LTE_UTRA-Perf]",580900,"revised","2017-05-08T10:26:55.153","2017-05-08T10:27:54.020","","R4-1706151","Rel-15","37.843","0.3.0","AASenh_BS_LTE_UTRA-Perf","","","","","","","","",""]
["R4-1705810","TP to TR 37.843: Further details on the definition of core and conformance requirements for BS demodulation requirements","Huawei","Kyoungseok Oh","66120","pCR","","","","368","9.12.4","Demodulation requirements [AASenh_BS_LTE_UTRA-Perf]",581000,"revised","2017-05-08T10:26:55.483","2017-05-08T10:27:54.020","","R4-1706152","Rel-15","37.843","0.3.0","AASenh_BS_LTE_UTRA-Perf","","","","","","","","",""]
["R4-1705811","TP to TR 37.843: Placeholder for the BS performance requirements doable OTA","Huawei","Kyoungseok Oh","66120","pCR","","","","368","9.12.4","Demodulation requirements [AASenh_BS_LTE_UTRA-Perf]",581100,"revised","2017-05-08T10:26:55.797","2017-05-08T10:27:54.037","","R4-1706153","Rel-15","37.843","0.3.0","AASenh_BS_LTE_UTRA-Perf","","","","","","","","",""]
["R4-1705812","On mathematical modelling of the output power accuracy window for NR BS operating above 6 GHz","Nokia, Alcatel-Lucent Shanghai Bell","Kyoungseok Oh","66120","other","","","","442","10.5.3.4","Other Tx requirements [NR_newRAT]",45390,"noted","2017-05-08T10:26:56.123","2017-05-08T10:27:54.037","","","","","","","","","","","","","","",""]
["R4-1705813","TP to TR 37.843 ? TRP accuracy","Nokia, Alcatel-Lucent Shanghai Bell","Kyoungseok Oh","66120","pCR","","","","358","9.12.2.1","TRP accuracy [AASenh_BS_LTE_UTRA-Core]",581400,"revised","2017-05-08T10:26:56.403","2017-05-08T10:27:54.053","","R4-1706131","Rel-15","37.843","0.3.0","AASenh_BS_LTE_UTRA","","","","","","","","",""]
["R4-1705814","eAAS BS output power accuracy window requirements","Nokia, Alcatel-Lucent Shanghai Bell","Kyoungseok Oh","66120","other","","","","358","9.12.2.1","TRP accuracy [AASenh_BS_LTE_UTRA-Core]",56400,"noted","2017-05-08T10:26:56.730","2017-05-08T10:27:54.053","","","","","","","","","","","","","","",""]
["R4-1705815","eAAS co-location requirements","Nokia, Alcatel-Lucent Shanghai Bell","Kyoungseok Oh","66120","other","","","","360","9.12.2.3","Co-location requirements [AASenh_BS_LTE_UTRA-Core]",581500,"noted","2017-05-08T10:26:56.997","2017-05-08T10:27:54.053","","","","","","","","","","","","","","",""]
["R4-1705816","TRP uncertainty contributors","Nokia, Alcatel-Lucent Shanghai Bell","Kyoungseok Oh","66120","discussion","","","","367","9.12.3.2","Measurement Grid [AASenh_BS_LTE_UTRA-Perf]",581600,"noted","2017-05-08T10:26:57.277","2017-05-08T10:27:54.053","","","","","","","","","","","","","","",""]
["R4-1705817","Proposed NR frequency range and band combination","NTT DOCOMO, INC.","Kyoungseok Oh","66120","other","","","","412","10.2","NR bands and NR-LTE band combinations [NR_newRAT]",581700,"revised","2017-05-08T10:26:57.557","2017-05-23T15:07:51.773","","R4-1706325","","","","","","","","","","","","",""]
["R4-1705818","Radiation Patterns and Current Distributions for 5G antenna types at mmWave ? Preliminary results","MVG Industries, Sony Mobile","Kyoungseok Oh","66120","discussion","","","","459","10.7.2","UE RF [FS_NR_test_methods]",53930,"noted","2017-05-08T10:26:57.837","2017-05-08T10:27:54.067","","","Rel-15","","","FS_NR_test_methods","","","","","","","","",""]
["R4-1705819","On TRP measurements sampling grid at >6 GHz","MVG Industries, Sony Mobile","Kyoungseok Oh","66120","discussion","","","","459","10.7.2","UE RF [FS_NR_test_methods]",53940,"noted","2017-05-08T10:26:58.137","2017-05-08T10:27:54.067","","","Rel-15","","","FS_NR_test_methods","","","","","","","","",""]
["R4-1705820","Measurement Noise Floor for EIRP/TRP measurements","MVG Industries","Kyoungseok Oh","66120","discussion","","","","360","9.12.2.3","Co-location requirements [AASenh_BS_LTE_UTRA-Core]",48500,"noted","2017-05-08T10:26:58.400","2017-05-08T10:27:54.083","","","Rel-15","","","AASenh_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-1705821","CR on test case for Bluetooth identification","Huawei, HiSilicon","Kyoungseok Oh","66120","CR","Agreement","","","252","7.23.2.2","RAT-independent enhancement [UTRA_LTE_iPos_enh2-Perf]",45190,"revised","2017-05-08T10:26:58.697","2017-05-08T10:27:54.083","","R4-1706026","Rel-14","37.171","14.1.0","UTRA_LTE_iPos_enh2-Perf","0016","","B","","","","","",""]
["R4-1705822","Unresolved issues in multi-node tests","Broadcom Limited","Kyoungseok Oh","66120","discussion","","","","82","6.1.1","General [FS_LTE_LAA_multinode_test]",51800,"noted","2017-05-08T10:27:00.663","2017-05-08T10:27:54.083","","","","","","","","","","","","","","",""]
["R4-1705823","Wi-Fi LTE Coexistence Testing at Test laboratories","Wi-Fi Alliance","Kyoungseok Oh","66120","discussion","","","","82","6.1.1","General [FS_LTE_LAA_multinode_test]",54750,"noted","2017-05-08T10:27:00.957","2017-05-08T10:27:54.083","","","","","","","","","","","","","","",""]
["R4-1705824","Considerations for Orthogonal Test Design for the LBT Algorithm","Wi-Fi Alliance","Kyoungseok Oh","66120","discussion","","","","82","6.1.1","General [FS_LTE_LAA_multinode_test]",582200,"noted","2017-05-08T10:27:01.270","2017-05-08T10:27:54.100","","","","","","","","","","","","","","",""]
["R4-1705825","Synchronization Block Design Implications on RAN4","Qualcomm Incorporated","Kyoungseok Oh","66120","other","Approval","In this paper we show that initial system acquisition will be impacted due to the RAN1 agreements on synchronization burst design. We propose to send an LS to RAN1 to ask them to reconsider the PBCH design.","","419","10.3.2","Channel Raster [NR_newRAT]",52920,"noted","2017-05-08T10:27:01.550","2017-05-08T10:27:54.100","R4-1704568","","Rel-15","","","","","","","","","","","",""]
["R4-1705826","Handling of  More Than 2CC LTE-NR band combinations","Vodafone","Kyoungseok Oh","66120","discussion","","","","416","10.2.2","NR-LTE band combinations proposals [NR_newRAT]",45110,"noted","2017-05-08T10:27:01.863","2017-05-08T10:27:54.117","","","","","","","","","","","","","","",""]
["R4-1705827","[Draft] Introduction of TDD L band into TS 36.104","Huawei, Hisilicon, Etisalat","Kyoungseok Oh","66120","draftCR","","","","329","9.6.3","BS RF (36.104, 36.141) [LTE_TDD_L_Band-core/Perf]",56170,"revised","2017-05-08T10:27:02.143","2017-05-08T10:27:54.117","R4-1705616","R4-1706120","Rel-15","36.104","14.3.0","LTE_TDD_L_Band-Core","","","","","","","","",""]
["R4-1705828","CTIA & CCSA Combined comparison test plan and proposa","Huawei, CATR","Kyoungseok Oh","66120","other","","","","145","7.11.2","Performance requirements [LTE_MIMO_OTA-Core]",45300,"noted","2017-05-08T10:27:02.463","2017-05-23T15:07:51.787","","","","","","","","","","","","","","",""]
["R4-1705829","Baseline for spectrum utilization","Ericsson","Kyoungseok Oh","66120","discussion","","","","420","10.3.3","Spectrum utilization [NR_newRAT]",49500,"noted","2017-05-08T10:27:02.760","2017-05-08T10:27:54.130","","","Rel-15","","","NR_newRAT","","","","","","","","",""]
["R4-1705830","Proposal to base NR demod requirements on variable MCS/rank rather than FRC","Keysight Technologies","Kyoungseok Oh","66120","other","Discussion","","","466","10.7.5","UE Demodulation [FS_NR_test_methods]",53700,"noted","2017-05-08T10:27:03.150","2017-05-08T10:27:54.130","","","","","","","","","","","","","","",""]
["R4-1705831","Metrics for Simplified sectorized MPAC RRM/Demodulation Measurement Setup","Keysight Technologies","Kyoungseok Oh","66120","other","Discussion","","","465","10.7.4.1","Baseline measurement setup [FS_NR_test_methods]",45910,"noted","2017-05-08T10:27:03.460","2017-05-08T10:27:54.130","","","","","","","","","","","","","","",""]
["R4-1705832","Frequency limit for BS spurious emission above 6 GHz","Nokia, Alcatel-Lucent Shanghai Bell","Kyoungseok Oh","66120","other","Approval","In this contribution we discuss and proposed uppare range of fundametal frequency range and upper limit for BS spurious emission.","","440","10.5.3.2","Unwanted emission requirements [NR_newRAT]",45440,"noted","2017-05-08T10:27:03.757","2017-05-08T10:27:54.130","","","","","","","","","","","","","","",""]
["R4-1705833","Boundary between spurious and OOB domain for NR BS above 6 GHz","Nokia, Alcatel-Lucent Shanghai Bell","Kyoungseok Oh","66120","other","Approval","In this contribution we discuss and propose boundary between spurius and OOB domain for NR BS above 6 GHz","","440","10.5.3.2","Unwanted emission requirements [NR_newRAT]",45430,"noted","2017-05-08T10:27:04.070","2017-05-08T10:27:54.147","","","","","","","","","","","","","","",""]
["R4-1705834","Baseline RRM and demod measurement system considerations and channel models","Keysight Technologies","Kyoungseok Oh","66120","other","Discussion","","","465","10.7.4.1","Baseline measurement setup [FS_NR_test_methods]",46690,"noted","2017-05-08T10:27:04.413","2017-05-08T10:27:54.147","","","","","","","","","","","","","","",""]
["R4-1705835","Further study on the feasibility of 3.3 GHz ? 4.2 GHz NR spectrum","Intel Corporation, Qorvo Incorporation","Kyoungseok Oh","66120","other","","","","415","10.2.1.2","Band definition for NR bands [NR_newRAT]",52590,"withdrawn","2017-05-08T10:27:04.693","2017-05-08T10:27:54.147","","","","","","","","","","","","","","",""]
["R4-1705836","Consideration of the manufacturer's declarations for Hybrid AAS BS and OTA AAS BS","Huawei","Kyoungseok Oh","66120","discussion","","","","366","9.12.3.1","RF conformance requirements [AASenh_BS_LTE_UTRA-Perf]",583600,"noted","2017-05-08T10:27:05.053","2017-05-08T10:27:54.147","","","","","","AASenh_BS_LTE_UTRA-Perf","","","","","","","","",""]
["R4-1705837","Spatial separation for the OTA demodulation requirements","Huawei","Kyoungseok Oh","66120","discussion","","","","368","9.12.4","Demodulation requirements [AASenh_BS_LTE_UTRA-Perf]",583700,"noted","2017-05-08T10:27:05.430","2017-05-08T10:27:54.147","","","","","","AASenh_BS_LTE_UTRA-Perf","","","","","","","","",""]
["R4-1705838","Simplified sectorized MPAC for RRM/Demodulation baseline","Keysight Technologies UK Ltd","Kyoungseok Oh","66120","other","Approval","","","465","10.7.4.1","Baseline measurement setup [FS_NR_test_methods]",54660,"noted","2017-05-08T10:27:05.803","2017-05-08T10:27:54.163","","","","","","","","","","","","","","",""]
["R4-1705839","NR subcarrier spacing considerations for above 6GHz bands","AT&T","Kyoungseok Oh","66120","discussion","Decision","","","418","10.3.1","Channel bandwidth and subcarrier spacing [NR_newRAT]",569800,"noted","2017-05-09T12:14:23.727","2017-05-11T09:44:11.150","R4-1704862","","","","","","","","","","","","","",""]
["R4-1705840","NR channel raster for sub 6GHz and above 6GHz bands","AT&T","Kyoungseok Oh","66120","discussion","Decision","","","419","10.3.2","Channel Raster [NR_newRAT]",51580,"noted","2017-05-09T12:14:24.010","2017-05-11T09:44:11.167","R4-1704863","","","","","","","","","","","","","",""]
["R4-1705841","Open issues related to the definition of LAA/802.11 coexistence tests in 3GPP RAN4","IEEE 802.11 WG","Kyoungseok Oh","66120","LS in","Discussion","","","3","3","Letters / reports from other groups / meetings",584100,"noted","2017-05-10T15:18:49.717","2017-05-11T09:41:23.527","","","","","","","","","","","","RAN4","","11-17-0738-03-0000-proposed-ls-to-3gpp-ran4-on-sir-for-below-ed-tests",""]
["R4-1705842","Basket WI for LTE Advanced Intra-band CA Rel-15","Ericsson","Kyoungseok Oh","66120","WID new","Endorsement","","","88","7.1.1","Rapporteur Input (WID/CRs) [LTE_CA_R14_intra-Core]",48842,"withdrawn","2017-05-24T17:13:19.420","2017-05-24T17:17:51.067","","","","","","","","","","","","","","",""]
["R4-1705843","New WID: LTE Advanced inter-band CA Rel-15 for 2DL1UL","Qualcomm Incorporated","Kyoungseok Oh","66120","other","Endorsement","","","94","7.2.1","Rapporteur Input (WID/CRs) [LTE_CA_R14_2DL1UL-Core]",51951,"withdrawn","2017-05-24T17:13:19.750",null,"","","Rel-15","","","","","","","","","","","",""]
["R4-1705844","TP to 36.714-03-01: Introduction of CA_2A-48A-66A","Nokia, Verizon","Kyoungseok Oh","66120","other","Approval","","","101","7.3.2","UE RF (36.101) [LTE_CA_R14_3DL1UL-Core]",46001,"withdrawn","2017-05-24T17:13:20.013","2017-05-24T17:17:51.097","","","","","","","","","","","","","","",""]
["R4-1705845","TP to 36.714-03-01: Introduction of CA_2A-48C","Nokia, Verizon","Kyoungseok Oh","66120","other","Approval","","","101","7.3.2","UE RF (36.101) [LTE_CA_R14_3DL1UL-Core]",46011,"withdrawn","2017-05-24T17:13:20.297","2017-05-24T17:17:51.097","","","","","","","","","","","","","","",""]
["R4-1705846","CA_3DL_2A-48A-48A _1UL_BCS0","Ericsson, Verizon","Kyoungseok Oh","66120","pCR","Approval","","","101","7.3.2","UE RF (36.101) [LTE_CA_R14_3DL1UL-Core]",52971,"withdrawn","2017-05-24T17:13:20.577","2017-05-24T17:17:51.097","","","Rel-14","36.714-03-01","0.6.0","LTE_CA_R14_3DL1UL-Core","","","","","","","","",""]
["R4-1705847","CA_3DL_3A-8A-20A_1UL_BCS0 delta TIB/RIB text proposal","Vodafone","Kyoungseok Oh","66120","discussion","","","","101","7.3.2","UE RF (36.101) [LTE_CA_R14_3DL1UL-Core]",45991,"withdrawn","2017-05-24T17:13:20.873","2017-05-24T17:17:51.097","","","","","","","","","","","","","","",""]
["R4-1705848","CA_4DL_3A-7A-20A-28A_1UL_BCS0","Ericsson","Kyoungseok Oh","66120","pCR","Approval","","","107","7.4.2","UE RF (36.101) [LTE_CA_R14_4DL1UL-Core]",48961,"withdrawn","2017-05-24T17:13:21.153","2017-05-24T17:17:51.113","","","Rel-14","36.714-04-01","0.7.0","LTE_CA_R14_4DL1UL-Core","","","","","","","","",""]
["R4-1705849","CA_4DL_1A-7A-20A-28A_1UL_BCS0","Ericsson","Kyoungseok Oh","66120","pCR","Approval","","","107","7.4.2","UE RF (36.101) [LTE_CA_R14_4DL1UL-Core]",48971,"withdrawn","2017-05-24T17:13:21.497","2017-05-24T17:17:51.113","","","Rel-14","36.714-04-01","0.7.0","LTE_CA_R14_4DL1UL-Core","","","","","","","","",""]
["R4-1705850","CA_4DL_1A-3A-20A-28A_1UL_BCS0","Ericsson","Kyoungseok Oh","66120","pCR","Approval","","","107","7.4.2","UE RF (36.101) [LTE_CA_R14_4DL1UL-Core]",48981,"withdrawn","2017-05-24T17:13:21.807","2017-05-24T17:17:51.113","","","Rel-14","36.714-04-01","0.7.0","LTE_CA_R14_4DL1UL-Core","","","","","","","","",""]
["R4-1705851","CA_4DL_2A-48A-48A-66A_1UL_BCS0","Ericsson, Verizon","Kyoungseok Oh","66120","pCR","Approval","","","107","7.4.2","UE RF (36.101) [LTE_CA_R14_4DL1UL-Core]",53241,"withdrawn","2017-05-24T17:13:22.120","2017-05-24T17:17:51.113","","","Rel-14","36.714-04-01","0.7.0","LTE_CA_R14_4DL1UL-Core","","","","","","","","",""]
["R4-1705852","Correction on Duplex mode for Prose operating band","CATT","Kyoungseok Oh","66120","other","Approval","","","13","4.2.1","UE RF (core / EMC) [WI code or TEI12]",49311,"withdrawn","2017-05-24T17:13:22.433","2017-05-24T17:17:51.127","","","Rel-12","36.101","","TEI","","","","","","","","",""]
["R4-1705853","Update of LAA REFSENS exclusion region","Qualcomm Incorporated","Kyoungseok Oh","66120","other","Agreement","","","34","5.3.1","UE RF core (36.101) [LTE_LAA-Core]",55831,"withdrawn","2017-05-24T17:13:22.697","2017-05-24T17:17:51.127","","","Rel-14","36.101","","LTE_LAA-Core","","","","","","","","",""]
["R4-1705854","Update of LAA REFSENS exclusion region","QUALCOMM UK Ltd","Kyoungseok Oh","66120","other","Agreement","","","34","5.3.1","UE RF core (36.101) [LTE_LAA-Core]",54791,"withdrawn","2017-05-24T17:13:22.963",null,"","","Rel-13","36.101","","LTE_LAA-Core","","","","","","","","",""]
["R4-1705855","CR NB-IoT FRC clarification","Ericsson","Kyoungseok Oh","66120","other","Approval","","","62","5.5.5","RRM Performance (36.133) [NB_IOT-Perf]",48261,"withdrawn","2017-05-24T17:13:23.273","2017-05-24T17:17:51.127","","","Rel-13","36.104","","NB_IOT-Core","","","","","","","","",""]
["R4-1705856","CR NB-IoT Missing note Output power","Ericsson","Kyoungseok Oh","66120","other","Approval","","","59","5.5.2","BS RF core(36.104) [NB_IOT-Core]",48291,"withdrawn","2017-05-24T17:13:23.540","2017-05-24T17:17:51.143","","","Rel-13","37.104","","NB_IOT-Core","","","","","","","","",""]
["R4-1705857","CR NB-IoT Remove 1.4 MHz inband support","Ericsson","Kyoungseok Oh","66120","other","Approval","","","59","5.5.2","BS RF core(36.104) [NB_IOT-Core]",54001,"withdrawn","2017-05-24T17:13:23.820","2017-05-24T17:17:51.143","","","Rel-13","37.104","","NB_IOT-Core","","","","","","","","",""]
["R4-1705858","CR NB-IoT FRC clarification - test","Ericsson","Kyoungseok Oh","66120","other","Approval","","","61","5.5.4","BS RF Conformance testing (36.141) [NB_IOT-Perf]",48330,"withdrawn","2017-05-24T17:13:24.087","2017-05-24T17:17:51.143","","","Rel-13","36.141","","NB_IOT-Perf","","","","","","","","",""]
["R4-1705859","CR NB-IoT Remove 1.4 MHz inband support - Test","Ericsson","Kyoungseok Oh","66120","other","Approval","","","61","5.5.4","BS RF Conformance testing (36.141) [NB_IOT-Perf]",48370,"withdrawn","2017-05-24T17:13:24.337","2017-05-24T17:17:51.160","","","Rel-13","37.141","","NB_IOT-Perf","","","","","","","","",""]
["R4-1705860","NB-IoT Cell-ID value in Test Model N-TM and some editorials","Ericsson","Kyoungseok Oh","66120","other","Approval","","","61","5.5.4","BS RF Conformance testing (36.141) [NB_IOT-Perf]",54210,"withdrawn","2017-05-24T17:13:24.600","2017-05-24T17:17:51.160","","","Rel-13","36.141","","NB_IOT-Perf","","","","","","","","",""]
["R4-1705861","Add NB-IoT support to Band 21","Ericsson","Kyoungseok Oh","66120","CR","Agreement","","","132","7.8.3","BS RF (36.104) [NB_IOT_R14_bands]",48471,"agreed","2017-05-24T17:13:24.867","2017-05-24T17:17:51.177","R4-1704847","","Rel-14","37.141","14.3.0","NB_IOT_R14_bands","0778","1","B","RP-171279","","","","",""]
["R4-1705862","Removing notes in two tables in UE spec wrt applicability of UL and DL requirements for band 46","Ericsson","Kyoungseok Oh","66120","CR","Agreement","","","161","7.14.2","UE RF Maintenance(36.101) [LTE_eLAA-Core]",54731,"agreed","2017-05-24T17:13:26.083","2017-05-24T17:17:51.177","R4-1705473","","Rel-14","36.101","14.3.0","LTE_eLAA-Core","4465","1","F","RP-171285","","","","",""]
["R4-1705863","TP on REFSENS for Band 71","SAMSUNG Electronics Co., Ltd.","Kyoungseok Oh","66120","pCR","","","","336","9.8.2","UE RF (36.101) [LTE600_US-core]",55061,"approved","2017-05-24T17:13:27.283","2017-05-24T17:17:51.177","R4-1705162","","Rel-15","36.755","0.0.1","LTE600_US-Core","","","","","","","","",""]
["R4-1705864","Correction on the additional SE for Band 41 UE in rel-14","LG Electronics Inc.","Kyoungseok Oh","66120","CR","Agreement","","","291","7.29.2","RF [WI code or TEI14]",54471,"agreed","2017-05-24T17:13:27.690","2017-05-24T17:17:51.177","R4-1704861","","Rel-14","36.101","14.3.0","LTE_B41_UE_PC2-Core","4419","1","F","RP-171290","","","","",""]
["R4-1705865","DRAFT LS on extension of NS and CA_NS signalling space","Nokia, Alcatel-Lucent Shanghai Bell","Kyoungseok Oh","66120","LS out","Approval","","","291","7.29.2","RF [WI code or TEI14]",569001,"revised","2017-05-24T17:13:28.967","2017-05-24T17:17:51.190","R4-1705448","R4-1706076","","","","TEI14","","","","","","RAN2","","",""]
["R4-1705866","4Rx REFSENS requirements spec improvement for 36.101","Huawei, HiSilicon","Kyoungseok Oh","66120","CR","Agreement","","","30","5.2.1","UE RF core(36.101) [LTE_4Rx_AP_DL-Core]",52181,"agreed","2017-05-24T17:13:29.280","2017-05-24T17:17:51.190","R4-1705218","","Rel-13","36.101","13.7.0","LTE_4Rx_AP_DL-Core","4445","1","F","RP-171304","","","","",""]
["R4-1705867","CR for NB-IoT Absolute power tolerance","Neul, Huawei, HiSilicon","Kyoungseok Oh","66120","CR","Agreement","","","58","5.5.1","UE RF core(36.101) [NB_IOT-Core]",55761,"agreed","2017-05-24T17:13:30.467","2017-05-24T17:17:51.190","R4-1705576","","Rel-13","36.101","13.7.0","NB_IOT-Core","4474","1","F","RP-171299","","","","",""]
["R4-1705868","WF on NB-IoT additional spectrum emission mask","Neul, Huawei, HiSilicon","Kyoungseok Oh","66120","other","Discussion","","","58","5.5.1","UE RF core(36.101) [NB_IOT-Core]",586800,"approved","2017-05-24T17:13:31.747","2017-05-24T17:17:51.207","","","","","","","","","","","","","","",""]
["R4-1705869","Clarification on 1.4 MHz for in-band operation","Huawei, HiSilicon, Nokia, Ericsson","Kyoungseok Oh","66120","CR","Agreement","","","59","5.5.2","BS RF core(36.104) [NB_IOT-Core]",48311,"agreed","2017-05-24T17:13:32.043","2017-05-24T17:17:51.207","R4-1705568","","Rel-13","36.104","13.7.0","NB_IOT-Core","4685","1","F","RP-171300","","","","",""]
["R4-1705870","CR NB-IoT Remove 1.4 MHz inband support","Ericsson","Kyoungseok Oh","66120","CR","Approval","","","59","5.5.2","BS RF core(36.104) [NB_IOT-Core]",54001,"revised","2017-05-24T17:13:33.167","2017-05-24T17:17:51.207","R4-1704830","R4-1706078","Rel-13","37.104","13.5.0","NB_IOT-Core","0779","1","F","","","","","",""]
["R4-1705871","Intermodulation performance requirement for NB-IoT operation (TS 36.104)","Nokia, Alcatel-Lucent Shanghai Bell","Kyoungseok Oh","66120","CR","Agreement","","","59","5.5.2","BS RF core(36.104) [NB_IOT-Core]",54151,"agreed","2017-05-24T17:13:34.383","2017-05-24T17:17:51.207","R4-1705412","","Rel-13","36.104","13.7.0","NB_IOT-Core","4681","1","F","RP-171300","","","","",""]
["R4-1705872","CR for CAT-M2 REFSENS, MPR and adding note for protection band 5","Ericsson, KDDI, Sony","Kyoungseok Oh","66120","CR","Agreement","","","207","7.18.2.2","REFSENS [LTE_feMTC-Core]",587500,"revised","2017-05-24T17:13:35.613","2017-05-24T17:17:51.223","","R4-1706082","Rel-14","36.101","14.3.0","LTE_feMTC-Core","4485","","B","","","","","",""]
["R4-1705873","TP for TR 36.714-00-00: MSD for CA_1A-1A_BCS0","Huawei, Hisilicon","Kyoungseok Oh","66120","pCR","Approval","","","89","7.1.2","UE RF (36.101) [LTE_CA_R14_intra-Core]",568901,"withdrawn","2017-05-24T17:13:41.870",null,"R4-1705381","","Rel-14","36.714-00-02","0.7.0","LTE_CA_R14_xDL2UL-Core","","","","","","","","",""]
["R4-1705874","TP on summay of MSD levels for xDL/2UL CA with self desense issues","LG Electronics Inc.","Kyoungseok Oh","66120","pCR","Approval","","","125","7.7.2","UE RF (36.101) [LTE_CA_R14_xDL2UL-Core]",53071,"approved","2017-05-24T17:13:42.213","2017-05-24T17:17:51.223","R4-1704849","","Rel-14","36.714-00-02","0.8.0","LTE_CA_R14_xDL2UL-Core","","","","","","","","",""]
["R4-1705875","WAY FORWARD ON REL-14 CAT M2 REFSENS","Ericsson","Kyoungseok Oh","66120","other","Discussion","","","207","7.18.2.2","REFSENS [LTE_feMTC-Core]",587200,"approved","2017-05-24T17:13:42.573","2017-05-24T17:17:51.223","","","","","","","","","","","","","","",""]
["R4-1705876","CR on introduction of V2X_20-47 band combination","LG Electronics Inc.","Kyoungseok Oh","66120","CR","Agreement","","","341","9.9.2","UE RF (36.101) [LTE_V2X_CA_bands-core]",0,"endorsed","2017-05-24T17:13:42.837","2017-05-24T17:17:51.237","R4-1704901","","Rel-15","36.101","14.3.0","LTE_V2X_CA_bands-Core","4427","1","B","","","","","",""]
["R4-1705877","TR skeleton for LTE V2X phase 2","Huawei, HiSilicon","Kyoungseok Oh","66120","other","Approval","","","399","9.16.1","General [LTE_eV2X]",51831,"approved","2017-05-24T17:13:44.320","2017-05-24T17:17:51.237","R4-1705296","","","","","LTE_eV2X-Core","","","","","","","","",""]
["R4-1705878","WF on V2X scenarios for V2X phase 2","Huawei, HiSilicon","Kyoungseok Oh","66120","other","Discussion","","","399","9.16.1","General [LTE_eV2X]",587800,"revised","2017-05-24T17:13:44.617","2017-05-24T17:17:51.253","","R4-1706123","","","","","","","","","","","","",""]
["R4-1705879","CR on applicability of V2X contiguous intraband multi-carrier operation requirements.","Qualcomm Inc.","Kyoungseok Oh","66120","CR","Agreement","","","177","7.16.2","UE RF Maintenance (36.101) [LTE_V2X-Core]",45211,"agreed","2017-05-24T17:13:44.913","2017-05-24T17:17:51.253","R4-1704521","","Rel-14","36.101","14.3.0","LTE_V2X-Core","4380","1","F","RP-171282","","","","",""]
["R4-1705880","Reply LS on regarding 1024 QAM","Huawei, HiSilicon","Kyoungseok Oh","66120","LS out","Approval","","","405","9.17.1","General [LTE_HCS]",56611,"revised","2017-05-24T17:13:46.190","2017-05-24T17:17:51.253","R4-1705189","R4-1706112","","","","LTE_1024QAM_DL-Core","","","","","R1-1706842","RAN1","","",""]
["R4-1705881","Introduction of power class 1 HPUE in Band 3, 20 and 28","Huawei, Nokia, Motorola solutions, NTT DOCOMO","Kyoungseok Oh","66120","CR","Agreement","","","304","9.1.2","UE RF (36.101) [LTE_HPUE_B3_B20_B28]",54411,"endorsed","2017-05-24T17:13:46.520","2017-05-24T17:17:51.253","R4-1704818","","Rel-15","36.101","14.3.0","LTE_HPUE_B3_B20_B28","4416","1","B","","","","","",""]
["R4-1705882","TP to TR 36.748: Expected specification changes to TS 36.101 due to introduction of Band 72","Nokia","Kyoungseok Oh","66120","other","Approval","","","308","9.2.2","UE RF (36.101) [LTE450_Europe_PPDR-core]",54511,"approved","2017-05-24T17:13:47.783","2017-05-24T17:17:51.270","R4-1705450","","","","","LTE450_Europe_PPDR-Core","","","","","","","","",""]
["R4-1705883","TP to TR 36.748: Band 72 receiver requirements","Nokia","Kyoungseok Oh","66120","other","Approval","","","308","9.2.2","UE RF (36.101) [LTE450_Europe_PPDR-core]",54521,"approved","2017-05-24T17:13:48.080","2017-05-24T17:17:51.270","R4-1705451","","","","","LTE450_Europe_PPDR-Core","","","","","","","","",""]
["R4-1705884","Text Proposal for Section 7.2 of TR36.748","Airbus DS SLC","Kyoungseok Oh","66120","other","Approval","","","306","9.2","450MHz E-UTRA FDD Band for LTE PPDR and PMR/PAMR in Europe [LTE450_Europe_PPDR]",55031,"approved","2017-05-24T17:13:48.360","2017-05-24T17:17:51.270","R4-1705503","","Rel-15","36.748","","LTE450_Europe_PPDR","","","","","","","","",""]
["R4-1705885","TP to TR 36.755 Update of section on Coexistence with WMTS services","Ericsson, Qorvo","Kyoungseok Oh","66120","other","Approval","","","335","9.8.1","General [LTE600_US]",49661,"approved","2017-05-24T17:13:48.640","2017-05-24T17:17:51.270","R4-1704966","","Rel-15","36.755","","LTE600_US","","","","","","","","",""]
["R4-1705886","TP on section 6 in TR36.755","SAMSUNG Electronics Co., Ltd.","Kyoungseok Oh","66120","pCR","","","","335","9.8.1","General [LTE600_US]",51631,"approved","2017-05-24T17:13:48.920","2017-05-24T17:17:51.283","R4-1705163","","Rel-15","36.755","0.0.1","LTE600_US-Core","","","","","","","","",""]
["R4-1705887","Introduction of Band 71 to 36.101","Qualcomm Incorporated","Kyoungseok Oh","66120","draftCR","","","","336","9.8.2","UE RF (36.101) [LTE600_US-core]",569101,"endorsed","2017-05-24T17:13:49.233","2017-05-24T17:17:51.283","R4-1705691","","Rel-14","36.101","14.3.0","LTE600_US-Core","","","B","","","","","",""]
["R4-1705888","Draft CR 25.123: Introduction of Band 71 (600MHz FDD band for US)","Ericsson, Nokia","Kyoungseok Oh","66120","draftCR","Endorsement","","","338","9.8.4","Other specifications [LTE600_US]",49631,"endorsed","2017-05-24T17:13:49.513","2017-05-24T17:17:51.283","R4-1704963","","Rel-15","25.123","14.2.0","LTE600_US","","","B","","","","","",""]
["R4-1705889","TP to TR 36.790 on BS specific aspects","Ericsson, AT&T","Kyoungseok Oh","66120","other","Approval","","","353","9.11.3","BS RF (Downlink only in 3.5GHz) (36.104/36.141) [LTE_ 3550_CBRS_US_LAA]",52701,"approved","2017-05-24T17:13:49.797","2017-05-24T17:17:51.300","R4-1705270","","Rel-15","","","LTE_3550_CBRS_US_LAA","","","","","","","","",""]
["R4-1705890","CR to 36.104: Introduction of Band 49 (3.5 GHz LAA in US)","Ericsson, AT&T","Kyoungseok Oh","66120","CR","Approval","","","353","9.11.3","BS RF (Downlink only in 3.5GHz) (36.104/36.141) [LTE_ 3550_CBRS_US_LAA]",52711,"endorsed","2017-05-24T17:13:50.107","2017-05-24T17:17:51.300","R4-1705271","","Rel-15","36.104","14.3.0","LTE_3550_CBRS_US_LAA","4675","1","B","","","","","",""]
["R4-1705891","CR to 36.141: Introduction of Band 49 (3.5 GHz LAA in US)","Ericsson, AT&T","Kyoungseok Oh","66120","CR","Approval","","","353","9.11.3","BS RF (Downlink only in 3.5GHz) (36.104/36.141) [LTE_ 3550_CBRS_US_LAA]",52791,"endorsed","2017-05-24T17:13:51.293","2017-05-24T17:17:51.300","R4-1705279","","Rel-15","36.141","14.3.0","LTE_3550_CBRS_US_LAA","1037","1","B","","","","","",""]
["R4-1705892","CR to 36.124: Introduction of Band 49 (3.5 GHz LAA in US)","Ericsson, AT&T","Kyoungseok Oh","66120","CR","Approval","","","354","9.11.4","Other specifications [LTE_ 3550_CBRS_US_LAA]",52741,"endorsed","2017-05-24T17:13:52.447","2017-05-24T17:17:51.300","R4-1705273","","Rel-15","36.124","14.1.0","LTE_3550_CBRS_US_LAA","0037","1","B","","","","","",""]
["R4-1705893","CR to 37.104: Introduction of Band 49 (3.5 GHz LAA in US)","Ericsson, AT&T","Kyoungseok Oh","66120","CR","Approval","","","354","9.11.4","Other specifications [LTE_ 3550_CBRS_US_LAA]",52751,"noted","2017-05-24T17:13:53.647","2017-05-24T17:17:51.317","R4-1705274","","Rel-15","37.104","14.3.0","LTE_3550_CBRS_US_LAA","0781","1","B","","","","","",""]
["R4-1705894","CR to 25.104: Introduction of Band 49 (3.5 GHz LAA in US)","Ericsson, AT&T","Kyoungseok Oh","66120","CR","Approval","","","354","9.11.4","Other specifications [LTE_ 3550_CBRS_US_LAA]",52771,"endorsed","2017-05-24T17:13:54.910","2017-05-24T17:17:51.317","R4-1705276","","Rel-15","25.104","14.1.0","LTE_3550_CBRS_US_LAA","0950","1","B","","","","","",""]
["R4-1705895","CR to 25.461: Introduction of Band 49 (3.5 GHz LAA in US)","Ericsson, AT&T","Kyoungseok Oh","66120","draftCR","Endorsement","","","354","9.11.4","Other specifications [LTE_ 3550_CBRS_US_LAA]",52781,"endorsed","2017-05-24T17:13:56.143","2017-05-24T17:17:51.317","R4-1705277","","Rel-15","25.461","14.1.0","LTE_3550_CBRS_US_LAA","","","B","","","","","",""]
["R4-1705896","CR to 37.141: Introduction of Band 49 (3.5 GHz LAA in US)","Ericsson, AT&T","Kyoungseok Oh","66120","CR","Approval","","","354","9.11.4","Other specifications [LTE_ 3550_CBRS_US_LAA]",52801,"noted","2017-05-24T17:13:56.440","2017-05-24T17:17:51.330","R4-1705278","","Rel-15","37.141","14.3.0","LTE_3550_CBRS_US_LAA","0779","1","B","","","","","",""]
["R4-1705897","CR to 25.141: Introduction of Band 49 (3.5 GHz LAA in US)","Ericsson, AT&T","Kyoungseok Oh","66120","CR","Approval","","","354","9.11.4","Other specifications [LTE_ 3550_CBRS_US_LAA]",53351,"endorsed","2017-05-24T17:13:57.703","2017-05-24T17:17:51.330","R4-1705280","","Rel-15","25.141","14.1.0","LTE_3550_CBRS_US_LAA","0980","1","B","","","","","",""]
["R4-1705898","On the 450 MHz band for LTE in Region 3 ? UE RF","Intel Corporation","Kyoungseok Oh","66120","other","Approval","","","347","9.10.3","UE RF (36.101) [LTE450_Reg3-core]",46821,"approved","2017-05-24T17:13:59.013","2017-05-24T17:17:51.330","R4-1704682","","","","","NR_newRAT","","","","","","","","",""]
["R4-1705899","Basket WI for LTE Advanced Intra-band CA Rel-15","Ericsson","Kyoungseok Oh","66120","WID new","Endorsement","","","88","7.1.1","Rapporteur Input (WID/CRs) [LTE_CA_R14_intra-Core]",48841,"endorsed","2017-05-24T17:13:59.297","2017-06-07T07:58:10.697","R4-1704882","","","","","","","","","","","","","",""]
["R4-1705900","New WID: LTE Advanced inter-band CA Rel-15 for 2DL1UL","Qualcomm Incorporated","Kyoungseok Oh","66120","other","Endorsement","","","94","7.2.1","Rapporteur Input (WID/CRs) [LTE_CA_R14_2DL1UL-Core]",51951,"endorsed","2017-05-24T17:13:59.590","2017-05-24T17:17:51.330","R4-1705198","","Rel-15","","","","","","","","","","","",""]
["R4-1705901","TP to 36.714-03-01: Introduction of CA_2A-48A-66A","Nokia, Verizon","Kyoungseok Oh","66120","other","Approval","","","101","7.3.2","UE RF (36.101) [LTE_CA_R14_3DL1UL-Core]",46001,"approved","2017-05-24T17:13:59.920","2017-06-06T13:47:53.980","R4-1704598","","","","","","","","","","","","","",""]
["R4-1705902","TP to 36.714-03-01: Introduction of CA_2A-48C","Nokia, Verizon","Kyoungseok Oh","66120","other","Approval","","","101","7.3.2","UE RF (36.101) [LTE_CA_R14_3DL1UL-Core]",46011,"approved","2017-05-24T17:14:00.217","2017-06-06T13:47:53.997","R4-1704599","","","","","","","","","","","","","",""]
["R4-1705903","CA_3DL_2A-48A-48A _1UL_BCS0","Ericsson, Verizon","Kyoungseok Oh","66120","pCR","Approval","","","101","7.3.2","UE RF (36.101) [LTE_CA_R14_3DL1UL-Core]",52971,"approved","2017-05-24T17:14:00.497","2017-06-07T07:58:10.963","R4-1704899","","Rel-14","36.714-03-01","0.6.0","LTE_CA_R14_3DL1UL-Core","","","","","","","","",""]
["R4-1705904","CA_3DL_3A-8A-20A_1UL_BCS0 delta TIB/RIB text proposal","Vodafone","Kyoungseok Oh","66120","discussion","","","","101","7.3.2","UE RF (36.101) [LTE_CA_R14_3DL1UL-Core]",45991,"approved","2017-05-24T17:14:00.840","2017-06-06T13:47:54.010","R4-1705781","","","","","","","","","","","","","",""]
["R4-1705905","CA_4DL_3A-7A-20A-28A_1UL_BCS0","Ericsson","Kyoungseok Oh","66120","pCR","Approval","","","107","7.4.2","UE RF (36.101) [LTE_CA_R14_4DL1UL-Core]",48961,"approved","2017-05-24T17:14:01.150","2017-06-07T07:58:10.963","R4-1704892","","Rel-14","36.714-04-01","0.7.0","LTE_CA_R14_4DL1UL-Core","","","","","","","","",""]
["R4-1705906","CA_4DL_1A-7A-20A-28A_1UL_BCS0","Ericsson","Kyoungseok Oh","66120","pCR","Approval","","","107","7.4.2","UE RF (36.101) [LTE_CA_R14_4DL1UL-Core]",48971,"approved","2017-05-24T17:14:01.463","2017-06-07T07:58:10.977","R4-1704893","","Rel-14","36.714-04-01","0.7.0","LTE_CA_R14_4DL1UL-Core","","","","","","","","",""]
["R4-1705907","CA_4DL_1A-3A-20A-28A_1UL_BCS0","Ericsson","Kyoungseok Oh","66120","pCR","Approval","","","107","7.4.2","UE RF (36.101) [LTE_CA_R14_4DL1UL-Core]",48981,"approved","2017-05-24T17:14:01.807","2017-06-07T07:58:10.993","R4-1704894","","Rel-14","36.714-04-01","0.7.0","LTE_CA_R14_4DL1UL-Core","","","","","","","","",""]
["R4-1705908","CA_4DL_2A-48A-48A-66A_1UL_BCS0","Ericsson, Verizon","Kyoungseok Oh","66120","pCR","Approval","","","107","7.4.2","UE RF (36.101) [LTE_CA_R14_4DL1UL-Core]",53241,"approved","2017-05-24T17:14:02.133","2017-06-07T07:58:10.993","R4-1704896","","Rel-14","36.714-04-01","0.7.0","LTE_CA_R14_4DL1UL-Core","","","","","","","","",""]
["R4-1705909","Correction on Duplex mode for Prose operating band","CATT","Kyoungseok Oh","66120","CR","Approval","","","13","4.2.1","UE RF (core / EMC) [WI code or TEI12]",49311,"postponed","2017-05-24T17:14:02.477",null,"R4-1704931","","Rel-12","36.101","12.15.0","LTE_D2D_Prox-Core","4429","1","F","","","","","",""]
["R4-1705910","Update of LAA REFSENS exclusion region","Qualcomm Incorporated","Kyoungseok Oh","66120","CR","Agreement","","","34","5.3.1","UE RF core (36.101) [LTE_LAA-Core]",55831,"agreed","2017-05-24T17:14:04.007","2017-05-24T17:17:51.363","R4-1705773","","Rel-14","36.101","14.3.0","LTE_LAA-Core","4484","1","F","RP-171307","","","","",""]
["R4-1705911","Update of LAA REFSENS exclusion region","QUALCOMM UK Ltd","Kyoungseok Oh","66120","CR","Agreement","","","34","5.3.1","UE RF core (36.101) [LTE_LAA-Core]",54791,"revised","2017-05-24T17:14:05.193","2017-05-24T17:17:51.363","R4-1705583","R4-1706111","Rel-13","36.101","13.7.0","LTE_LAA-Core","4476","1","F","","","","","",""]
["R4-1705912","CR NB-IoT FRC clarification","Ericsson","Kyoungseok Oh","66120","CR","Approval","","","59","5.5.2","BS RF core(36.104) [NB_IOT-Core]",48251,"postponed","2017-05-24T17:14:06.987","2017-06-07T13:57:52.717","R4-1704824","","Rel-13","36.104","13.7.0","NB_IOT-Core","4669","1","F","","","","","",""]
["R4-1705913","Missing clarification note related to BS output power when considering NB-IoT","Ericsson","Kyoungseok Oh","66120","CR","Agreement","","","59","5.5.2","BS RF core(36.104) [NB_IOT-Core]",48291,"agreed","2017-05-24T17:14:09.140","2017-05-24T18:07:51.247","R4-1704828","","Rel-13","37.104","13.5.0","NB_IOT-Core","0777","1","F","RP-171300","","","","",""]
["R4-1705914","Void","Void","Kyoungseok Oh","66120","other","Discussion","","","86","7","Rel-14 Work Items",591400,"reserved","2017-05-24T17:14:11.120",null,"","","","","","","","","","","","","","",""]
["R4-1705915","CR NB-IoT FRC clarification - test","Ericsson","Kyoungseok Oh","66120","CR","Approval","","","61","5.5.4","BS RF Conformance testing (36.141) [NB_IOT-Perf]",48322,"noted","2017-05-24T17:14:11.387","2017-06-07T13:57:52.780","R4-1704826","","Rel-13","36.141","13.7.0","NB_IOT-Perf","1027","1","F","","","","","",""]
["R4-1705916","CR NB-IoT Remove 1.4 MHz inband support - Test","Ericsson","Kyoungseok Oh","66120","CR","Approval","","","61","5.5.4","BS RF Conformance testing (36.141) [NB_IOT-Perf]",48362,"revised","2017-05-24T17:14:12.557",null,"R4-1704832","R4-1705941","Rel-13","37.141","13.6.0","NB_IOT-Perf","0776","1","F","","","","","",""]
["R4-1705917","NB-IoT Cell-ID value in Test Model N-TM and some editorials","Ericsson","Kyoungseok Oh","66120","CR","Agreement","","","61","5.5.4","BS RF Conformance testing (36.141) [NB_IOT-Perf]",54202,"agreed","2017-05-24T17:14:13.677","2017-05-24T18:07:51.277","R4-1704834","","Rel-13","36.141","13.7.0","NB_IOT-Perf","1029","1","F","RP-171302","","","","",""]
["R4-1705918","CR on Channel model validation procedures for RTS","ROHDE & SCHWARZ, Keysight Technologies, Spirent Communications","Kyoungseok Oh","66120","CR","Agreement","","","144","7.11.1","General [LTE_MIMO_OTA-Core]",46631,"agreed","2017-05-24T17:14:14.910","2017-05-24T17:17:51.393","R4-1704620","","Rel-14","37.977","14.3.0","LTE_MIMO_OTA","0056","1","F","RP-171258","","","","",""]
["R4-1705919","RTS applicability for > 2 Rx","Keysight Technologies","Kyoungseok Oh","66120","CR","Agreement","","","144","7.11.1","General [LTE_MIMO_OTA-Core]",45761,"revised","2017-05-24T17:14:16.550","2017-05-24T17:17:51.393","R4-1705667","R4-1705937","Rel-14","37.977","14.3.0","LTE_MIMO_OTA-Core","0058","1","F","","","","","",""]
["R4-1705920","MIMO OTA Harmonization - Results of First Set of Bands","CTTC","Kyoungseok Oh","66120","other","Approval","","","146","7.11.3","Harmonization [LTE_MIMO_OTA-Core]",54631,"noted","2017-05-24T17:14:17.750","2017-05-24T17:17:51.393","R4-1705463","","Rel-13","","","LTE_MIMO_OTA","","","","","","","","",""]
["R4-1705921","Channel model validation results","ETS-Lindgren, MVG Industries","Kyoungseok Oh","66120","CR","Agreement","","","145","7.11.2","Performance requirements [LTE_MIMO_OTA-Core]",45291,"revised","2017-05-24T17:14:18.047","2017-05-24T17:17:51.410","R4-1705735","R4-1706097","Rel-14","37.977","14.3.0","LTE_MIMO_OTA-Core","0060","1","B","","","","","",""]
["R4-1705922","LS on MIMO OTA progress","Intel Corporation","Kyoungseok Oh","66120","LS out","Approval","","","144","7.11.1","General [LTE_MIMO_OTA-Core]",566901,"approved","2017-05-24T17:14:19.200","2017-05-24T17:17:51.410","R4-1704663","","Rel-14","","","LTE_MIMO_OTA-Core","","","","","","GCF CAG, GCF PAG, CTIA MOSG","RAN, RAN5","",""]
["R4-1705923","TR 36.751 V0.1.0: FDD operating band in the L-band for LTE","NTT DOCOMO, INC.","Kyoungseok Oh","66120","draft TR","Approval","","","314","9.4","FDD operating band in the L-band for LTE [LTE_FDD_L_Band]",52511,"approved","2017-05-24T17:14:19.483","2017-05-24T17:17:51.410","R4-1705251","","Rel-15","36.751","0.1.0","LTE_FDD_L_Band-Core","","","","","","","","",""]
["R4-1705924","TP for TR 36.751: Updates on the FDD operation in L-band","NTT DOCOMO, INC.","Kyoungseok Oh","66120","pCR","Approval","","","316","9.4.2","UE RF (36.101) [LTE_FDD_L_Band-core]",52521,"approved","2017-05-24T17:14:21.867","2017-05-24T17:17:51.410","R4-1705252","","Rel-15","36.751","0.1.0","LTE_FDD_L_Band-Core","","","","","","","","",""]
["R4-1705925","[Draft] Introduction of FDD L-band into TS 36.101","NTT DOCOMO, INC.","Kyoungseok Oh","66120","draftCR","Endorsement","","","316","9.4.2","UE RF (36.101) [LTE_FDD_L_Band-core]",52541,"endorsed","2017-05-24T17:14:22.227","2017-05-24T17:17:51.427","R4-1705254","","Rel-15","36.101","14.3.0","LTE_FDD_L_Band-Core","","","","","","","","",""]
["R4-1705926","Introduction of the FDD L-band (Band 74) into TS 36.104","NTT DOCOMO, INC.","Kyoungseok Oh","66120","draftCR","Endorsement","","","317","9.4.3","BS RF (36.104, 36.141) [LTE_FDD_L_Band-core/Perf]",45481,"endorsed","2017-05-24T17:14:22.557","2017-05-24T17:17:51.427","R4-1704548","","Rel-15","36.104","14.3.0","LTE_FDD_L_Band-Core","","","","","","","","",""]
["R4-1705927","Introduction of the FDD L-band (Band 74) into TS 36.141","NTT DOCOMO, INC.","Kyoungseok Oh","66120","draftCR","Endorsement","","","317","9.4.3","BS RF (36.104, 36.141) [LTE_FDD_L_Band-core/Perf]",49711,"endorsed","2017-05-24T17:14:22.850","2017-05-24T17:17:51.427","R4-1704549","","Rel-15","36.141","14.3.0","LTE_FDD_L_Band-Perf","","","","","","","","",""]
["R4-1705928","Introduction of the FDD L-band (Band 74) into TS 25.104","NTT DOCOMO, INC.","Kyoungseok Oh","66120","draftCR","Endorsement","","","319","9.4.5","Other specifications [LTE_FDD_L_Band]",45530,"endorsed","2017-05-24T17:14:23.193","2017-05-24T17:17:51.440","R4-1704551","","Rel-15","25.104","14.1.0","LTE_FDD_L_Band","","","","","","","","",""]
["R4-1705929","[Draft] Introduction of TDD L band into TS 36.101","Huawei, Hisilicon, Etisalat","Kyoungseok Oh","66120","draftCR","","","","328","9.6.2","UE RF (36.101) [LTE_TDD_L_Band-core]",576601,"revised","2017-05-24T17:14:23.523",null,"R4-1705615","R4-1706119","Rel-15","36.101","14.3.0","LTE_TDD_L_Band-Core","","","","","","","","",""]
["R4-1705930","Introduction of the FDD L-band (Band 74) into TS 25.141","NTT DOCOMO, INC.","Kyoungseok Oh","66120","draftCR","Endorsement","","","319","9.4.5","Other specifications [LTE_FDD_L_Band]",45540,"endorsed","2017-05-24T17:14:23.803","2017-05-24T17:17:51.440","R4-1704552","","Rel-15","25.141","14.1.0","LTE_FDD_L_Band","","","","","","","","",""]
["R4-1705931","Introduction of the FDD L-band (Band 74) into TS 37.104","NTT DOCOMO, INC.","Kyoungseok Oh","66120","draftCR","Endorsement","","","319","9.4.5","Other specifications [LTE_FDD_L_Band]",45550,"endorsed","2017-05-24T17:14:24.083","2017-05-24T17:17:51.457","R4-1704553","","Rel-15","37.104","14.3.0","LTE_FDD_L_Band","","","","","","","","",""]
["R4-1705932","Introduction of the FDD L-band (Band 74) into TS 37.141","NTT DOCOMO, INC.","Kyoungseok Oh","66120","draftCR","Endorsement","","","319","9.4.5","Other specifications [LTE_FDD_L_Band]",45730,"endorsed","2017-05-24T17:14:24.363","2017-05-24T17:17:51.457","R4-1704555","","Rel-15","37.141","14.3.0","LTE_FDD_L_Band","","","","","","","","",""]
["R4-1705933","Draft CR sTTI 2OS introduction","Ericsson","Kyoungseok Oh","66120","draftCR","Endorsement","","","378","9.13.3","BS RF (36.104) [LTE_sTTIandPT-core]",48381,"revised","2017-05-24T17:14:24.693","2017-05-24T17:17:51.457","R4-1704838","R4-1706121","Rel-14","36.104","14.3.0","LTE_sTTIandPT-Core","","","B","","","","","",""]
["R4-1705934","CR on 25.466: Introduction of new bands of49, 50, 71, 72, 72, 73, 74 and 75","Ericsson","Kyoungseok Oh","66120","other","Discussion","","","301","9","Rel-15 Work Items for LTE",593400,"endorsed","2017-05-24T17:14:25.003","2017-05-24T17:17:51.470","","","Rel-14","25.466","","LTE600_US-Core","","","","","","","","",""]
["R4-1705935","Proposals on concluding the MIMO OTA WI","CATR","Kyoungseok Oh","66120","other","Approval","","","146","7.11.3","Harmonization [LTE_MIMO_OTA-Core]",593500,"approved","2017-05-24T17:14:25.287","2017-05-24T17:17:51.487","","","","","","","","","","","","","","",""]
["R4-1705936","Alignment results from three labs","Intel","Kyoungseok Oh","66120","other","Discussion","","","146","7.11.3","Harmonization [LTE_MIMO_OTA-Core]",593900,"noted","2017-05-24T17:14:25.550","2017-05-24T17:17:51.487","","","","","","","","","","","","","","",""]
["R4-1705937","RTS applicability for > 2 Rx","Keysight Technologies","Kyoungseok Oh","66120","CR","Agreement","","","144","7.11.1","General [LTE_MIMO_OTA-Core]",45762,"revised","2017-05-24T17:14:25.830","2017-05-24T17:17:51.487","R4-1705919","","Rel-14","37.977","14.3.0","LTE_MIMO_OTA","0058","2","F","","","","","",""]
["R4-1705938","CR to 37.977 Definition of RTS 2nd stage isolation","ROHDE & SCHWARZ, Keysight Technologies","Kyoungseok Oh","66120","CR","Agreement","","","144","7.11.1","General [LTE_MIMO_OTA-Core]",46571,"agreed","2017-05-24T17:14:26.970","2017-05-24T17:17:51.487","","","Rel-14","37.977","14.3.0","LTE_MIMO_OTA","0053","2","F","RP-171258","","","","",""]
["R4-1705939","Work plan for performance lab alignment","MVG Industries, ETS-Lindgren","Kyoungseok Oh","66120","other","Discussion","","","146","7.11.3","Harmonization [LTE_MIMO_OTA-Core]",593600,"approved","2017-05-24T17:14:28.107","2017-05-24T17:17:51.503","","","","","","","","","","","","","","",""]
["R4-1705940","Clarification on small BW support for in-band and guard band operation (36.141)","Nokia, Alcatel-Lucent Shanghai Bell","Kyoungseok Oh","66120","CR","Agreement","","","61","5.5.4","BS RF Conformance testing (36.141) [NB_IOT-Perf]",48351,"agreed","2017-05-24T17:14:28.390","2017-05-24T17:17:51.503","R4-1705420","","Rel-13","36.141","13.7.0","NB_IOT-Perf","1045","1","F","RP-171303","","","","",""]
["R4-1705941","Remove NB-IoT inband support for 1.4 MHz - Tests","Ericsson, Huawei, Nokia, Alcatel-Lucent Shanghai Bell","Kyoungseok Oh","66120","CR","Agreement","","","61","5.5.4","BS RF Conformance testing (36.141) [NB_IOT-Perf]",48363,"agreed","2017-05-24T17:14:29.607","2017-05-24T17:17:51.503","R4-1705916","","Rel-13","37.141","13.6.0","NB_IOT-Perf","0776","2","F","RP-171302","","","","",""]
["R4-1705942","Maintenance CR for LLA demodulation tests","Qualcomm Incorporated","Kyoungseok Oh","66120","CR","Approval","","","39","5.3.6","UE Demodulation (36.101) [LTE_LAA-Perf]",51421,"revised","2017-05-24T17:14:30.887","2017-05-24T17:17:51.517","R4-1705142","R4-1706021","Rel-13","36.101","13.7.0","LTE_LAA-Perf","4439","1","D","","","","","",""]
["R4-1705943","Maintenance CR for LAA demodulation tests","Qualcomm Incorporated","Kyoungseok Oh","66120","CR","Agreement","","","39","5.3.6","UE Demodulation (36.101) [LTE_LAA-Perf]",51431,"agreed","2017-05-24T17:14:31.993","2017-05-24T17:17:51.517","R4-1705143","","Rel-14","36.101","14.3.0","LTE_LAA-Perf","4440","1","A","RP-171307","","","","",""]
["R4-1705944","Correction on reliability of GNSS singal for V2V","CATT","Kyoungseok Oh","66120","CR","Agreement","","","169","7.15.2","RRM core maintenance (36.133) [LTE_SL_V2V-Core]",0,"agreed","2017-05-24T17:14:33.177","2017-05-24T17:17:51.517","R4-1704903","","Rel-14","36.133","14.3.0","LTE_SL_V2V-Core","4868","1","B","RP-171281","","","","",""]
["R4-1705945","CR on reliability of GNSS singal for V2X","CATT","Kyoungseok Oh","66120","CR","Agreement","","","178","7.16.3","RRM core Maintenance (36.133) [LTE_V2X-Core]",0,"agreed","2017-05-24T17:14:34.317","2017-05-24T17:17:51.517","R4-1704904","","Rel-14","36.133","14.3.0","LTE_V2X-Core","4869","1","B","RP-171282","","","","",""]
["R4-1705946","CR on Modification of Selection/Reselection of V2X Synchronization Reference","Huawei, HiSilicon","Kyoungseok Oh","66120","CR","Agreement","","","178","7.16.3","RRM core Maintenance (36.133) [LTE_V2X-Core]",50840,"agreed","2017-05-24T17:14:35.627","2017-05-24T17:17:51.533","R4-1705037","","Rel-14","36.133","14.3.0","LTE_V2X-Core","4917","1","F","RP-171282","","","","",""]
["R4-1705947","Clarification on V2X requirements for V2X UEs in RRC_CONNECTED state","Ericsson","Kyoungseok Oh","66120","CR","Approval","","","178","7.16.3","RRM core Maintenance (36.133) [LTE_V2X-Core]",622100,"endorsed","2017-05-24T17:14:36.843","2017-05-24T17:17:51.533","R4-1705084","","Rel-14","36.133","14.3.0","LTE_V2X-Core","4945","1","F","","","","","",""]
["R4-1705948","CR on reference configurations for V2X RRM","CATT","Kyoungseok Oh","66120","CR","Agreement","","","179","7.16.4","RRM performance (36.133) [LTE_V2X-Perf]",50501,"agreed","2017-05-24T17:14:38.047","2017-05-24T17:17:51.533","R4-1704902","","Rel-14","36.133","14.3.0","LTE_V2X-Perf","4867","1","B","RP-171265","","","","",""]
["R4-1705949","CR for V2V Performance Requirements","LG Electronics Inc.","Kyoungseok Oh","66120","CR","Agreement","","","171","7.15.4","UE demodulation (36.101) [LTE_SL_V2V-Perf]",49360,"agreed","2017-05-24T17:14:39.247","2017-05-24T17:17:51.550","R4-1704936","","Rel-14","36.101","14.3.0","LTE_SL_V2V-Perf","4432","1","B","RP-171256","","","","",""]
["R4-1705950","CR on performance requirements for MUST Case 3","MediaTek inc.","Kyoungseok Oh","66120","CR","Agreement","","","254","7.24.1","Demodulation performance (36.101) [LTE_MUST-Perf]",47291,"agreed","2017-05-24T17:14:40.433","2017-05-24T17:17:51.550","R4-1704729","","Rel-14","36.101","14.3.0","LTE_MUST-Perf","4399","1","B","RP-171263","","","","",""]
["R4-1705951","LS response on NCSG non-CA","Qualcomm Incorporated","Kyoungseok Oh","66120","LS out","Approval","","","270","7.26.2.1","Gap pattern, signaling and capability (RAN2 related) [LTE_meas_gap_enh-Core]",51131,"approved","2017-05-24T17:14:41.603","2017-05-24T17:17:51.567","R4-1705749","","Rel-14","","","LTE_meas_gap_enh-Core","","","","","R2-1703948","RAN2","","",""]
["R4-1705952","Introduction of interruption control for Network Controlled Short Gap pattern for inter-frequency measurements","Nokia, Alcatel-Lucent Shanghai Bell","Kyoungseok Oh","66120","CR","Approval","","","271","7.26.2.2","RRM core requirement [LTE_meas_gap_enh-Core]",574901,"withdrawn","2017-05-24T17:14:41.900",null,"R4-1705115","","Rel-14","36.133","14.3.0","LTE_meas_gap_enh-Core","4951","1","B","","","","","",""]
["R4-1705953","E-UTRAN FDD-FDD Inter-frequency event triggered reporting with MGL=3ms under fading propagation conditions in synchronous cells","Intel Corporation","Kyoungseok Oh","66120","CR","Agreement","","","272","7.26.3","RRM performance (36.133) [LTE_meas_gap_enh-Perf]",47841,"agreed","2017-05-24T17:14:43.240","2017-05-24T17:17:51.567","R4-1704715","","Rel-14","36.133","14.3.0","LTE_meas_gap_enh-Core","4853","1","B","RP-171264","","","","",""]
["R4-1705954","E-UTRAN TDD-TDD Inter-frequency event triggered reporting with MGL=3ms under fading propagation conditions in synchronous cells","Intel Corporation","Kyoungseok Oh","66120","CR","Agreement","","","272","7.26.3","RRM performance (36.133) [LTE_meas_gap_enh-Perf]",574601,"agreed","2017-05-24T17:14:44.457","2017-05-24T17:17:51.567","R4-1704716","","Rel-14","36.133","14.3.0","LTE_meas_gap_enh-Core","4854","1","B","RP-171264","","","","",""]
["R4-1705955","CR on performance requirements for MUST Case 1 and Case 2","MediaTek inc.","Kyoungseok Oh","66120","CR","Agreement","","","254","7.24.1","Demodulation performance (36.101) [LTE_MUST-Perf]",47281,"agreed","2017-05-24T17:14:45.643","2017-05-24T17:17:51.580","R4-1704728","","Rel-14","36.101","14.3.0","LTE_MUST-Perf","4398","1","B","RP-171263","","","","",""]
["R4-1705956","CR on applicability rule for MUST Case 3","MediaTek inc.","Kyoungseok Oh","66120","CR","Agreement","","","254","7.24.1","Demodulation performance (36.101) [LTE_MUST-Perf]",47311,"agreed","2017-05-24T17:14:46.830","2017-05-24T17:17:51.580","R4-1704731","","Rel-14","36.101","14.3.0","LTE_MUST-Perf","4401","1","B","RP-171263","","","","",""]
["R4-1705957","CR on intra frequency RSTD measurement requirement for eNB-IOT","Huawei, HiSilicon","Kyoungseok Oh","66120","CR","Agreement","","","191","7.17.3.1.2","UTODA/OTDOA [NB_IOTenh-Core]",49961,"agreed","2017-05-24T17:14:48.170","2017-05-24T17:17:51.580","R4-1704995","","Rel-14","36.133","14.3.0","NB_IOTenh-Core","4889","1","B","RP-171267","","","","",""]
["R4-1705958","CR on inter frequency RSTD measurement requirement for eNB-IOT","Huawei, HiSilicon","Kyoungseok Oh","66120","CR","Agreement","","","191","7.17.3.1.2","UTODA/OTDOA [NB_IOTenh-Core]",56061,"agreed","2017-05-24T17:14:50.010","2017-05-24T17:17:51.580","R4-1704996","","Rel-14","36.133","14.3.0","NB_IOTenh-Core","4890","1","B","RP-171267","","","","",""]
["R4-1705959","Summary of simulation results for UL 256QAM","Ericsson","Kyoungseok Oh","66120","other","Discussion","","","150","7.12.3","Demodulation (36.104/36.141) [LTE_UL_CAP_enh-Core/Perf]",52290,"noted","2017-05-24T17:14:51.367","2017-05-24T17:17:51.597","","","","","","","","","","","","","","",""]
["R4-1705960","Correction on PHR reporting requirements for NB1","Ericsson","Kyoungseok Oh","66120","CR","Approval","","","62","5.5.5","RRM Performance (36.133) [NB_IOT-Perf]",48260,"withdrawn","2017-05-24T17:14:51.650",null,"R4-1705082","","Rel-13","36.133","13.7.0","NB_IOT-Perf","4943","1","F","","","","","",""]
["R4-1705961","Correction to inter-frequency RRC re-establishment test case in NB-IOT","Qualcomm Incorporated","Kyoungseok Oh","66120","CR","Agreement","","","62","5.5.5","RRM Performance (36.133) [NB_IOT-Perf]",49811,"agreed","2017-05-24T17:14:52.867","2017-05-24T17:17:51.597","R4-1705145","","Rel-13","36.133","13.7.0","NB_IOT-Perf","4962","1","F","RP-171302","","","","",""]
["R4-1705962","Correction on timing advance test for NB-IoT R13","Huawei, HiSilicon","Kyoungseok Oh","66120","CR","Agreement","","","62","5.5.5","RRM Performance (36.133) [NB_IOT-Perf]",50821,"agreed","2017-05-24T17:14:54.083","2017-05-24T17:17:51.597","R4-1704977","","Rel-13","36.133","13.7.0","NB_IOT-Perf","4878","1","F","RP-171303","","","","",""]
["R4-1705963","Inter-frequency cell reselection under enhanced coverage for NB-IOT","Ericsson","Kyoungseok Oh","66120","CR","Approval","","","62","5.5.5","RRM Performance (36.133) [NB_IOT-Perf]",51161,"revised","2017-05-24T17:14:55.567","2017-05-24T17:17:51.597","R4-1705072","","Rel-13","36.133","13.7.0","NB_IOT-Perf","4936","1","B","","","","","",""]
["R4-1705964","Contention Based Random Access Test for UE category NB1 UEs in Normal Coverage","Nokia, Alcatel-Lucent Shanghai Bell","Kyoungseok Oh","66120","CR","Agreement","","","62","5.5.5","RRM Performance (36.133) [NB_IOT-Perf]",51181,"agreed","2017-05-24T17:14:56.767","2017-05-24T17:17:51.613","R4-1705116","","Rel-13","36.133","13.7.0","NB_IOT-Perf","4952","1","F","RP-171303","","","","",""]
["R4-1705965","Contention Based Random Access Test for UE category NB1 UEs in Enhanced Coverage","Nokia, Alcatel-Lucent Shanghai Bell","Kyoungseok Oh","66120","CR","Agreement","","","62","5.5.5","RRM Performance (36.133) [NB_IOT-Perf]",51221,"agreed","2017-05-24T17:14:57.950","2017-05-24T17:17:51.613","R4-1705118","","Rel-13","36.133","13.7.0","NB_IOT-Perf","4954","1","F","RP-171303","","","","",""]
["R4-1705966","Wrong tolerance for NPUSCH format 1","Ericsson","Kyoungseok Oh","66120","CR","Agreement","","","65","5.5.6.2","BS Demodulation (36.104) [NB_IOT-Perf]",54231,"agreed","2017-05-24T17:14:59.183","2017-05-24T17:17:51.613","R4-1704836","","Rel-13","36.141","13.7.0","NB_IOT-Perf","1031","1","F","RP-171302","","","","",""]
["R4-1705967","CR for new PRACH performance requirements","Huawei","Kyoungseok Oh","66120","CR","Agreement","","","266","7.25.5","BS demodulation (36.104/36.141) [LTE_high_speed-Perf]",55391,"agreed","2017-05-24T17:15:00.480","2017-05-24T17:17:51.627","R4-1705538","","Rel-14","36.104","14.3.0","LTE_high_speed-Perf","0976","3","B","RP-171257","","","","",""]
["R4-1705968","CR for new PRACH conformance test","Huawei","Kyoungseok Oh","66120","CR","Agreement","","","266","7.25.5","BS demodulation (36.104/36.141) [LTE_high_speed-Perf]",573001,"agreed","2017-05-24T17:15:01.837","2017-05-24T17:17:51.627","R4-1705539","","Rel-14","36.141","14.3.0","LTE_high_speed-Perf","1011","3","B","RP-171257","","","","",""]
["R4-1705969","Void","Void","Kyoungseok Oh","66120","other","Discussion","","","86","7","Rel-14 Work Items",596900,"reserved","2017-05-24T17:15:03.147",null,"","","","","","","","","","","","","","",""]
["R4-1705970","CR for V2V resource pool configuration","Huawei, HiSilicon","Kyoungseok Oh","66120","CR","Agreement","","","174","7.15.4.3","Others [LTE_SL_V2V-Perf]",55471,"agreed","2017-05-24T17:15:03.427","2017-05-24T17:17:51.627","R4-1705547","","Rel-14","36.101","14.3.0","LTE_SL_V2V-Perf","4470","1","B","RP-171256","","","","",""]
["R4-1705971","Addition of FS3-only sTAG support","Nokia, Alcatel-Lucent Shanghai Bell","Kyoungseok Oh","66120","CR","Approval","","","164","7.14.5","RRM core Maintenance (36.133) [LTE_eLAA-Core]",55941,"noted","2017-05-24T17:15:04.677","2017-05-24T17:17:51.643","R4-1705498","","Rel-14","36.133","14.3.0","LTE_eLAA-Core","4978","1","B","","","","","",""]
["R4-1705972","Introduction of event triggered reporting LAA test cases for multiple Scells","Ericsson","Kyoungseok Oh","66120","CR","Agreement","","","165","7.14.6","RRM performance (36.133) [LTE_eLAA-Perf]",47871,"noted","2017-05-24T17:15:05.987","2017-05-24T17:17:51.643","R4-1704787","","Rel-14","36.133","14.3.0","LTE_eLAA-Perf","4865","1","B","","","","","",""]
["R4-1705973","Corrections on the LAA test cases R13","Huawei, HiSilicon","Kyoungseok Oh","66120","CR","Agreement","","","38","5.3.5","RRM Performance (36.133) [LTE_LAA-Perf]",50611,"agreed","2017-05-24T17:15:07.203","2017-05-24T17:17:51.660","R4-1705061","","Rel-13","36.133","13.7.0","LTE_LAA-Perf","4927","1","F","RP-171307","","","","",""]
["R4-1705974","LAA RRM: Correction to test case A.9.11.x and A.9.12.x (Rel-13)","Rohde & Schwarz","Kyoungseok Oh","66120","CR","","","","38","5.3.5","RRM Performance (36.133) [LTE_LAA-Perf]",45141,"withdrawn","2017-05-24T17:15:08.437",null,"R4-1704514","","Rel-13","36.133","13.7.0","LTE_LAA-Perf","4833","1","F","","","","","",""]
["R4-1705975","Introduce LBT model for multile LAA Scell(s) in LAA demodualtion","Ericsson, Huawei","Kyoungseok Oh","66120","CR","Agreement","","","294","7.29.4.1","Demodulation with multiple LAA SCC-s [WI code or TEI14]",56291,"agreed","2017-05-24T17:15:09.667","2017-05-24T17:17:51.660","R4-1705629","","Rel-14","36.101","14.3.0","LTE_LAA-Perf","4477","1","B","RP-171307","","","","",""]
["R4-1705976","CR on UE Rx-Tx measurement requirement for FeMTC","Huawei, HiSilicon","Kyoungseok Oh","66120","CR","Agreement","","","210","7.18.3.1.1","E-CID [LTE_feMTC-Core]",56040,"agreed","2017-05-24T17:15:10.917","2017-05-24T17:17:51.660","R4-1704299","","Rel-14","36.133","14.3.0","LTE_feMTC-Core","4797","3","B","RP-171266","","","","",""]
["R4-1705977","LS on measurement gaps for intra-frequency RSTD for FeMTC UE","Ericsson","Kyoungseok Oh","66120","LS out","Approval","","","211","7.18.3.1.2","OTDOA [LTE_feMTC-Core]",51511,"withdrawn","2017-05-24T17:15:12.100",null,"R4-1705605","","Rel-14","","","LTE_feMTC-Core","","","","","","RAN WG2","","",""]
["R4-1705978","CR on intra frequency RSTD measurement requirement for FeMTC","Huawei, HiSilicon","Kyoungseok Oh","66120","CR","Agreement","","","211","7.18.3.1.2","OTDOA [LTE_feMTC-Core]",56031,"agreed","2017-05-24T17:15:12.397","2017-05-24T17:17:51.673","R4-1705000","","Rel-14","36.133","14.3.0","LTE_feMTC-Core","4893","1","B","RP-171266","","","","",""]
["R4-1705979","Measurement requirements under discontonuous MPDCCH monitoring","Ericsson","Kyoungseok Oh","66120","CR","Agreement","","","213","7.18.3.2.1","UE MPDCCH monitoring configuration [LTE_feMTC-Core]",56021,"agreed","2017-05-24T17:15:13.630","2017-05-24T17:17:51.690","R4-1705602","","Rel-14","36.133","14.3.0","LTE_feMTC-Core","4986","1","F","RP-171266","","","","",""]
["R4-1705980","CR on measurement performance scaling with MPDCCH monitoring CEModeA","Nokia, Alcatel-Lucent Shanghai Bell","Kyoungseok Oh","66120","CR","Agreement","","","213","7.18.3.2.1","UE MPDCCH monitoring configuration [LTE_feMTC-Core]",572501,"noted","2017-05-24T17:15:15.003","2017-05-24T17:17:51.690","R4-1705725","","Rel-14","36.133","14.3.0","LTE_feMTC-Core","4991","1","B","","","","","",""]
["R4-1705981","CR on measurement performance scaling with MPDCCH monitoring CEModeB","Nokia, Alcatel-Lucent Shanghai Bell","Kyoungseok Oh","66120","CR","Agreement","","","213","7.18.3.2.1","UE MPDCCH monitoring configuration [LTE_feMTC-Core]",572601,"noted","2017-05-24T17:15:16.203","2017-05-24T17:17:51.707","R4-1705726","","Rel-14","36.133","14.3.0","LTE_feMTC-Core","4992","1","B","","","","","",""]
["R4-1705982","Enhanced Handover Requirement for FeMTC","Ericsson","Kyoungseok Oh","66120","CR","Agreement","","","214","7.18.3.2.2","Idle mode and handover [LTE_feMTC-Core]",53211,"agreed","2017-05-24T17:15:17.407","2017-05-24T17:17:51.707","R4-1705321","","Rel-14","36.133","14.3.0","LTE_feMTC-Core","4972","1","B","RP-171266","","","","",""]
["R4-1705983","Refinement of idle mode requirements for feMTC in R14","Nokia, Alcatel-Lucent Shanghai Bell","Kyoungseok Oh","66120","CR","Agreement","","","214","7.18.3.2.2","Idle mode and handover [LTE_feMTC-Core]",55101,"agreed","2017-05-24T17:15:18.683","2017-05-24T17:17:51.707","R4-1705510","","Rel-14","36.133","14.3.0","LTE_feMTC-Core","4821","3","F","RP-171266","","","","",""]
["R4-1705984","LS on RLM enhancement for FeMTC UE","Intel Corporation","Kyoungseok Oh","66120","LS out","Approval","","","217","7.18.3.2.5","RLM and timing [LTE_feMTC-Core]",50281,"approved","2017-05-24T17:15:19.887","2017-05-24T17:17:51.720","R4-1704710","","Rel-14","","","LTE_feMTC-Core","","","","","","RAN2","","",""]
["R4-1705985","CR on UE timer accuracy for FeMTC in R14","Huawei, HiSilicon","Kyoungseok Oh","66120","CR","Agreement","","","217","7.18.3.2.5","RLM and timing [LTE_feMTC-Core]",598601,"agreed","2017-05-24T17:15:20.243","2017-05-24T17:17:51.720","R4-1705028","","Rel-14","36.133","14.3.0","LTE_feMTC-Core","4909","1","A","RP-171266","","","","",""]
["R4-1705986","CR on UE timer accuracy for FeMTC in R13","Huawei, HiSilicon","Kyoungseok Oh","66120","CR","Agreement","","","217","7.18.3.2.5","RLM and timing [LTE_feMTC-Core]",577500,"agreed","2017-05-24T17:15:21.727","2017-05-24T17:17:51.720","","","Rel-13","36.133","13.7.0","LTE_feMTC-Core","4999","","F","RP-171266","","","","",""]
["R4-1705987","Correction to minimum requirement for Cat M1 Single-Layer Spatial Multiplexing","ANRITSU LTD","Kyoungseok Oh","66120","CR","","","","53","5.4.6.1","BL/CE UE [LTE_MTCe2_L1-Perf]",45870,"revised","2017-05-24T17:15:28.137","2017-05-24T17:17:51.720","R4-1704585","R4-1706202","Rel-13","36.101","13.7.0","LTE_MTCe2_L1-Perf","4384","1","F","","","","","",""]
["R4-1705988","Updated simulation results for BS IC with 2Rx without TO/FO","Huawei","Kyoungseok Oh","66120","discussion","Discussion","","","300","8.1.3","Link level evaluation [FS_LTE _IC_BS]",55191,"noted","2017-05-24T17:15:29.370","2017-05-24T17:17:51.737","R4-1705517","","","","","FS_LTE_IC_BS","","","","","","","","",""]
["R4-1705989","Updated simulation results for BS IC with 4Rx without TO/FO","Huawei","Kyoungseok Oh","66120","discussion","Discussion","","","300","8.1.3","Link level evaluation [FS_LTE _IC_BS]",55201,"noted","2017-05-24T17:15:29.667","2017-05-24T17:17:51.737","R4-1705518","","","","","FS_LTE_IC_BS","","","","","","","","",""]
["R4-1705990","Simulation results for BS IC with 2Rx with TO/FO","Huawei","Kyoungseok Oh","66120","discussion","Discussion","","","300","8.1.3","Link level evaluation [FS_LTE _IC_BS]",55231,"noted","2017-05-24T17:15:29.977","2017-05-24T17:17:51.753","R4-1705519","","","","","FS_LTE_IC_BS","","","","","","","","",""]
["R4-1705991","Simulation results for BS IC with 4Rx with TO/FO","Huawei","Kyoungseok Oh","66120","discussion","Discussion","","","300","8.1.3","Link level evaluation [FS_LTE _IC_BS]",55241,"noted","2017-05-24T17:15:30.290","2017-05-24T17:17:51.753","R4-1705520","","","","","FS_LTE_IC_BS","","","","","","","","",""]
["R4-1705992","TP on simulation results updates for 2Rx and 4Rx without TO FO","Huawei, China Telecom","Kyoungseok Oh","66120","pCR","Approval","","","300","8.1.3","Link level evaluation [FS_LTE _IC_BS]",45571,"approved","2017-05-24T17:15:30.587","2017-05-24T17:17:51.753","R4-1705523","","Rel-15","36.766","1.0.0","FS_LTE_IC_BS","","","","","","","","",""]
["R4-1705993","TP on simulation results addition for 2Rx and 4Rx with TO FO","Huawei, China Telecom","Kyoungseok Oh","66120","pCR","Approval","","","300","8.1.3","Link level evaluation [FS_LTE _IC_BS]",45581,"approved","2017-05-24T17:15:30.947","2017-05-24T17:17:51.767","R4-1705524","","Rel-15","36.766","1.0.0","FS_LTE_IC_BS","","","","","","","","",""]
["R4-1705994","Introducing gapless measurement requirement for eMTC R13","Nokia, Alcatel-Lucent Shanghai Bell","Kyoungseok Oh","66120","CR","Agreement","","","46","5.4.3.1","BL/CE UE [LTE_MTCe2_L1-Core]",50121,"agreed","2017-05-24T17:15:31.290","2017-05-24T17:17:51.767","R4-1705714","","Rel-13","36.133","13.7.0","LTE_MTCe2_L1-Core","4989","1","F","RP-171308","","","","",""]
["R4-1705995","CR on RSRP range for eMTC R13","Huawei, HiSilicon","Kyoungseok Oh","66120","CR","","","","46","5.4.3.1","BL/CE UE [LTE_MTCe2_L1-Core]",51491,"withdrawn","2017-05-24T17:15:32.537",null,"R4-1705012","","Rel-13","36.133","13.7.0","LTE_MTCe2_L1-Core","4900","1","F","","","","","",""]
["R4-1705996","CR on idle mode requirements for eMTC in R13","Nokia, Alcatel-Lucent Shanghai Bell, Qualcomm, Intel, Huawei, HiSilicon","Kyoungseok Oh","66120","CR","Agreement","","","46","5.4.3.1","BL/CE UE [LTE_MTCe2_L1-Core]",571401,"agreed","2017-05-24T17:15:33.787","2017-05-24T17:17:51.767","R4-1705508","","Rel-13","36.133","13.7.0","LTE_MTCe2_L1-Core","4831","2","F","RP-171308","","","","",""]
["R4-1705997","Correction on transmit timing requirement R13","Huawei, HiSilicon","Kyoungseok Oh","66120","CR","Agreement","","","50","5.4.5.1","Test cases for BL/CE UE [LTE_MTCe2_L1-Perf]",49921,"agreed","2017-05-24T17:15:35.003","2017-05-24T17:17:51.783","R4-1704992","","Rel-13","36.133","13.7.0","LTE_MTCe2_L1-Perf","4887","1","F","RP-171310","","","","",""]
["R4-1705998","Correction to Test Parameters for Cat M1 PUCCH 1-0 static test","ANRITSU LTD","Kyoungseok Oh","66120","CR","","","","53","5.4.6.1","BL/CE UE [LTE_MTCe2_L1-Perf]",47680,"withdrawn","2017-05-24T17:15:36.173",null,"R4-1704748","","Rel-13","36.101","13.7.0","LTE_MTCe2_L1-Perf","4408","1","F","","","","","",""]
["R4-1705999","CR on eMTC BS PRACH requirements R13","Nokia, Alcatel-Lucent Shanghai Bell","Kyoungseok Oh","66120","CR","Agreement","","","55","5.4.7","BS performance (36.104/36.141) [LTE_MTCe2_L1-Perf]",571700,"withdrawn","2017-05-24T17:15:37.343",null,"R4-1705718","","Rel-13","36.104","13.7.0","LTE_MTCe2_L1-Perf","","","F","","","","","",""]
["R4-1706000","CR on eMTC BS PRACH conformance tests R13","Nokia, Alcatel-Lucent Shanghai Bell","Kyoungseok Oh","66120","CR","Agreement","","","55","5.4.7","BS performance (36.104/36.141) [LTE_MTCe2_L1-Perf]",571900,"withdrawn","2017-05-24T17:15:42.803",null,"R4-1705720","","Rel-13","36.141","13.7.0","LTE_MTCe2_L1-Perf","","","F","","","","","",""]
["R4-1706001","E-UTRAN FDD - FDD Intra frequency RACH-less handover","Intel Corporation, ZTE","Kyoungseok Oh","66120","CR","Agreement","","","240","7.20.2","RRM performance (36.133) [LTE_eMob-Perf]",46891,"agreed","2017-05-24T17:15:47.873","2017-05-24T17:17:51.800","R4-1704689","","Rel-14","36.133","14.3.0","LTE_eMob","4844","1","B","RP-171259","","","","",""]
["R4-1706002","E-UTRAN FDD - FDD Inter frequency RACH-less handover","Intel Corporation, ZTE","Kyoungseok Oh","66120","CR","Agreement","","","240","7.20.2","RRM performance (36.133) [LTE_eMob-Perf]",46901,"agreed","2017-05-24T17:15:49.167","2017-05-24T17:17:51.800","R4-1704690","","Rel-14","36.133","14.3.0","LTE_eMob","4845","1","B","RP-171259","","","","",""]
["R4-1706003","E-UTRAN TDD - TDD Intra frequency RACH-less handover","Intel Corporation, ZTE","Kyoungseok Oh","66120","CR","Agreement","","","240","7.20.2","RRM performance (36.133) [LTE_eMob-Perf]",46911,"agreed","2017-05-24T17:15:50.430","2017-05-24T17:17:51.800","R4-1704691","","Rel-14","36.133","14.3.0","LTE_eMob","4846","1","B","RP-171259","","","","",""]
["R4-1706004","E-UTRAN TDD - TDD Inter frequency RACH-less handover","Intel Corporation, ZTE","Kyoungseok Oh","66120","CR","Agreement","","","240","7.20.2","RRM performance (36.133) [LTE_eMob-Perf]",46921,"agreed","2017-05-24T17:15:51.570","2017-05-24T17:17:51.800","R4-1704692","","Rel-14","36.133","14.3.0","LTE_eMob","4847","1","B","RP-171259","","","","",""]
["R4-1706005","LS to RAN5 on handover tests","ZTE","Kyoungseok Oh","66120","LS out","Approval","","","240","7.20.2","RRM performance (36.133) [LTE_eMob-Perf]",51721,"approved","2017-05-24T17:15:52.740","2017-05-24T17:17:51.817","R4-1705172","","Rel-14","","","LTE_eMob","","","","","","RAN5","","",""]
["R4-1706006","Summary of simulation results for PUSCH transmission in UpPTS","CMCC","Kyoungseok Oh","66120","other","Discussion","","","150","7.12.3","Demodulation (36.104/36.141) [LTE_UL_CAP_enh-Core/Perf]",49830,"noted","2017-05-24T17:15:53.050","2017-05-24T17:17:51.817","","","","","","","","","","","","","","",""]
["R4-1706007","TP on TR conclusions","China Telecom, ZTE, Nokia, Alcatel-Lucent Shanghai Bell, Huawei","Kyoungseok Oh","66120","pCR","Approval","","","298","8.1.1","General [FS_LTE _IC_BS]",45611,"approved","2017-05-24T17:15:53.333","2017-05-24T17:17:51.817","R4-1704562","","Rel-15","36.766","1.0.0","FS_LTE_IC_BS","","","","","","","","",""]
["R4-1706008","WF on BS IC receiver","China Telecom","Kyoungseok Oh","66120","other","Discussion","","","298","8.1.1","General [FS_LTE _IC_BS]",45560,"approved","2017-05-24T17:15:53.677","2017-05-24T17:17:51.817","","","","","","","","","","","","","","",""]
["R4-1706009","CR on BS synchronization requirements for eMBMS enhancements","Huawei, HiSilicon","Kyoungseok Oh","66120","CR","Agreement","","","155","7.13.3","RRM core (36.133) [MBMS_LTE_enh2-Core]",575001,"noted","2017-05-24T17:15:53.987","2017-05-24T17:17:51.830","R4-1705036","","Rel-14","36.133","14.3.0","MBMS_LTE_enh2-Core","4916","1","F","","","","","",""]
["R4-1706010","Simulation results for PUSCH in UpPTS","Huawei, HiSilicon","Kyoungseok Oh","66120","discussion","Discussion","","","150","7.12.3","Demodulation (36.104/36.141) [LTE_UL_CAP_enh-Core/Perf]",53041,"noted","2017-05-24T17:15:55.127","2017-05-24T17:17:51.830","R4-1704983","","","","","LTE_UL_CAP_enh-Perf","","","","","","","","",""]
["R4-1706011","Corrections of Table 8.7.5.1-2 and Table 8.7.5.2-27","Korea Testing Laboratory","Kyoungseok Oh","66120","CR","Agreement","","","98","7.2.5","Other Specifications [LTE_CA_R14_2DL1UL-Core]",569301,"agreed","2017-05-24T17:15:55.423","2017-05-24T17:17:51.830","R4-1704526","","Rel-13","36.101","13.7.0","LTE_CA_TDD_FDD-Perf","4381","1","F","RP-171296","","","","",""]
["R4-1706012","Way forward on FeMBMS RRM requirement","Ericsson","Kyoungseok Oh","66120","other","Discussion","","","155","7.13.3","RRM core (36.133) [MBMS_LTE_enh2-Core]",50350,"noted","2017-05-24T17:15:56.560","2017-05-24T17:17:51.830","","","","","","","","","","","","","","",""]
["R4-1706013","CR for introduction of PMCH and PDSCH demodulation tests for FeMBMS","Ericsson","Kyoungseok Oh","66120","CR","Approval","","","157","7.13.5","Demodulation (36.101) [MBMS_LTE_enh2-Perf]",574701,"noted","2017-05-24T17:15:57.047","2017-05-24T17:17:51.847","R4-1705369","","Rel-14","36.101","14.3.0","MBMS_LTE_enh2-Perf","4456","1","B","","","","","",""]
["R4-1706014","[draft] Introduction of the FDD L-band (Band 74) into 36.133","DOCOMO Communications Lab.","Kyoungseok Oh","66120","draftCR","Endorsement","","","318","9.4.4","RRM core (36.133) [LTE_FDD_L_Band-core]",45711,"endorsed","2017-05-24T17:15:58.230","2017-05-24T17:17:51.847","R4-1704571","","Rel-15","36.133","14.3.0","LTE_FDD_L_Band-Core","","","B","","","","","",""]
["R4-1706015","[draft] Introduction of the FDD L-band (Band 74) into 25.133","DOCOMO Communications Lab.","Kyoungseok Oh","66120","draftCR","Endorsement","","","319","9.4.5","Other specifications [LTE_FDD_L_Band]",45501,"endorsed","2017-05-24T17:15:58.557","2017-05-24T17:17:51.847","R4-1704573","","Rel-15","25.133","14.1.0","LTE_FDD_L_Band","","","B","","","","","",""]
["R4-1706016","[Draft] Introduction of TDD L band into TS 25.123","Huawei, Hisilicon, Etisalat","Kyoungseok Oh","66120","draftCR","","","","330","9.6.4","Other specifications [LTE_TDD_L_Band]",56181,"withdrawn","2017-05-24T17:15:58.870",null,"R4-1705618","","Rel-15","25.123","14.2.0","LTE_TDD_L_Band-Core","","","","","","","","",""]
["R4-1706017","[DRAFT] Introduction of TDD L band into TS 36.133","Etisalat, Huawei, Hisilicon","Kyoungseok Oh","66120","draftCR","Endorsement","","","330","9.6.4","Other specifications [LTE_TDD_L_Band]",575501,"withdrawn","2017-05-24T17:15:59.213",null,"R4-1705757","","Rel-15","36.133","14.3.0","LTE_TDD_L_Band-Core","","","","","","","","",""]
["R4-1706018","[DRAFT] Introduction of TDD L band into TS 25.133","Etisalat, Huawei, Hisilicon","Kyoungseok Oh","66120","draftCR","Endorsement","","","330","9.6.4","Other specifications [LTE_TDD_L_Band]",575601,"withdrawn","2017-05-24T17:15:59.527",null,"R4-1705763","","Rel-15","25.133","14.1.0","LTE_TDD_L_Band-Core","","","","","","","","",""]
["R4-1706019","Summary of simulation results for V2V demodulation requirements","Huawei, HiSilicon","Kyoungseok Oh","66120","other","Discussion","","","171","7.15.4","UE demodulation (36.101) [LTE_SL_V2V-Perf]",46440,"noted","2017-05-24T17:15:59.853","2017-05-24T17:17:51.860","","","","","","","","","","","","","","",""]
["R4-1706020","Corrections for inCoverage configuration in ProSe direct communication (Rel-12)","Huawei, HiSilicon","Kyoungseok Oh","66120","CR","Agreement","","","16","4.2.4","UE demodulation performance [WI code or TEI12]",55621,"revised","2017-05-24T17:16:00.150","2017-05-24T17:17:51.860","R4-1705562","R4-1706188","Rel-12","36.101","12.15.0","TEI12","4471","1","F","","","","","",""]
["R4-1706021","Maintenance CR for LAA demodulation tests","Qualcomm Incorporated","Kyoungseok Oh","66120","CR","Agreement","","","39","5.3.6","UE Demodulation (36.101) [LTE_LAA-Perf]",51422,"agreed","2017-05-24T17:16:01.943","2017-05-24T17:17:51.877","R4-1705942","","Rel-13","36.101","13.7.0","LTE_LAA-Perf","4439","2","D","RP-171307","","","","",""]
["R4-1706022","CR for correction for RRM core requirement for Cat.1bis UE","Qualcomm Incorporated","Kyoungseok Oh","66120","CR","Agreement","","","232","7.19.3","RRM core (36.133) [LTE_UE_cat_1RX-Core]",51241,"agreed","2017-05-24T17:16:03.097","2017-05-24T17:17:51.877","R4-1705124","","Rel-14","36.133","14.3.0","LTE_UE_cat_1RX-Core","4706","3","F","RP-171269","","","","",""]
["R4-1706023","CR for RRM tests for Cat.1 UE with single receiver chain","Qualcomm Incorporated","Kyoungseok Oh","66120","CR","Agreement","","","235","7.19.4","RRM performance (36.133) [LTE_UE_cat_1RX-Perf]",51251,"agreed","2017-05-24T17:16:04.360","2017-05-24T17:17:51.877","R4-1705125","","Rel-14","36.133","14.3.0","LTE_UE_cat_1RX-Perf","4708","3","B","RP-171269","","","","",""]
["R4-1706024","CR for RSTD measurement requirement for Cat.1bis UE","Qualcomm Incorporated","Kyoungseok Oh","66120","CR","Agreement","","","233","7.19.3.1","E-CID and OTDOA [LTE_UE_cat_1RX-Core]",51401,"agreed","2017-05-24T17:16:05.547","2017-05-24T17:17:51.877","R4-1705140","","Rel-14","36.133","14.3.0","LTE_UE_cat_1RX-Core","4960","1","B","RP-171269","","","","",""]
["R4-1706025","Ad hoc minutes on measurement gap","Intel","Kyoungseok Oh","66120","other","Discussion","","","270","7.26.2.1","Gap pattern, signaling and capability (RAN2 related) [LTE_meas_gap_enh-Core]",602500,"approved","2017-05-24T17:16:06.747","2017-05-24T17:17:51.893","","","","","","","","","","","","","","",""]
["R4-1706026","CR on test case for Bluetooth identification","Huawei, HiSilicon","Kyoungseok Oh","66120","CR","Agreement","","","252","7.23.2.2","RAT-independent enhancement [UTRA_LTE_iPos_enh2-Perf]",45191,"revised","2017-05-24T17:16:07.060","2017-05-24T17:17:51.893","R4-1705821","R4-1706272","Rel-14","37.171","14.1.0","UTRA_LTE_iPos_enh2-Perf","0016","1","B","","","","","",""]
["R4-1706027","InDoPos: New WLAN delay test case in nominal conditions with LTE FDD and TDD (Rel-14)","Rohde & Schwarz","Kyoungseok Oh","66120","CR","","","","252","7.23.2.2","RAT-independent enhancement [UTRA_LTE_iPos_enh2-Perf]",50061,"revised","2017-05-24T17:16:08.153","2017-05-24T17:17:51.893","R4-1704519","R4-1706269","Rel-14","37.171","14.1.0","UTRA_LTE_iPos_enh2-Perf","0013","1","F","","","","","",""]
["R4-1706028","InDoPos: New WLAN delay test case in dynamic range conditions with LTE FDD and TDD (Rel-14)","Rohde & Schwarz","Kyoungseok Oh","66120","CR","Agreement","","","252","7.23.2.2","RAT-independent enhancement [UTRA_LTE_iPos_enh2-Perf]",50071,"agreed","2017-05-24T17:16:09.383","2017-05-24T17:17:51.907","R4-1704520","","Rel-14","37.171","14.1.0","UTRA_LTE_iPos_enh2-Perf","0014","1","F","RP-171270","","","","",""]
["R4-1706029","Clean up the requirements for UE enhancement in SFN scenario","Huawei, HiSilicon, NTT DOCOMO","Kyoungseok Oh","66120","CR","Agreement","","","263","7.25.4.1","Enhancement for bi-directional RRH arrangement [LTE_high_speed-Perf]",55351,"agreed","2017-05-24T17:16:10.647","2017-05-24T17:17:51.907","R4-1705535","","Rel-14","36.101","14.3.0","LTE_high_speed-Perf","4468","1","F","RP-171257","","","","",""]
["R4-1706030","TR 36.747 text proposal on Enhanced CRS-IM","Intel Corporation","Kyoungseok Oh","66120","other","Approval","","","274","7.27.1","General [LTE_eCRSIM_eSUMIMO]",46361,"approved","2017-05-24T17:16:11.990","2017-05-24T17:17:51.907","R4-1704636","","Rel-14","36.747","","LTE_eCRSIM_eSUMIMO","","","","","","","","",""]
["R4-1706031","WF on CRS-IM capability and assistance signalling","Qualcomm Incorporated","Kyoungseok Oh","66120","other","Approval","","","275","7.27.1.1","Capability and signaling [LTE_eCRSIM_eSUMIMO]",53671,"noted","2017-05-24T17:16:12.300","2017-05-24T17:17:51.907","R4-1705128","","","","","LTE_eCRSIM_eSUMIMO","","","","","","","","",""]
["R4-1706032","Draft CR on Enhanced CRS-IM PDSCH performance requirements","Intel Corporation, Qualcomm","Kyoungseok Oh","66120","draftCR","Endorsement","","","277","7.27.2.1","PDSCH [LTE_eCRSIM_eSUMIMO]",49231,"endorsed","2017-05-24T17:16:12.597","2017-05-24T17:17:51.923","R4-1704637","","Rel-14","36.101","14.3.0","LTE_eCRSIM_eSUMIMO","","","","","","","","",""]
["R4-1706033","Draft CR on Enhanced CRS-IM PDCCH/PCFICH performance requirements","Intel Corporation, Qualcomm","Kyoungseok Oh","66120","draftCR","Endorsement","","","278","7.27.2.2","Control channel [LTE_eCRSIM_eSUMIMO]",51741,"endorsed","2017-05-24T17:16:12.927","2017-05-24T17:17:51.923","R4-1704639","","Rel-14","36.101","14.3.0","LTE_eCRSIM_eSUMIMO","","","","","","","","",""]
["R4-1706034","Tes case design for advacned CSI","Samsung","Kyoungseok Oh","66120","discussion","Approval","","","285","7.28.2.3","Advanced CSI [LTE_eFDMIMO-Perf]",47801,"noted","2017-05-24T17:16:13.223","2017-05-24T17:17:51.923","R4-1704780","","Rel-14","","","LTE_eFDMIMO-Perf","","","","","","","","",""]
["R4-1706035","WF for test proposal for performance part of FeMBMS","Ericsson, Qualcomm","Kyoungseok Oh","66120","other","Approval","","","157","7.13.5","Demodulation (36.101) [MBMS_LTE_enh2-Perf]",55271,"approved","2017-05-24T17:16:13.533","2017-05-24T17:17:51.923","R4-1705368","","Rel-14","","","MBMS_LTE_enh2-Perf","","","","","","","","",""]
["R4-1706036","[draft] Introduction of the FDD L-band (Band 74) into 25.123","DOCOMO Communications Lab.","Kyoungseok Oh","66120","draftCR","Endorsement","","","319","9.4.5","Other specifications [LTE_FDD_L_Band]",45511,"endorsed","2017-05-24T17:16:13.830","2017-05-24T17:17:51.940","R4-1704572","","Rel-15","25.123","14.2.0","LTE_FDD_L_Band","","","B","","","","","",""]
["R4-1706037","Clarification of PRB allocation for PUSCH test for eMTC (Rel-13)","Ericsson","Kyoungseok Oh","66120","CR","Agreement","","","55","5.4.7","BS performance (36.104/36.141) [LTE_MTCe2_L1-Perf]",572100,"agreed","2017-05-24T17:16:14.143","2017-05-24T17:17:51.940","R4-1704816","","Rel-13","36.141","13.7.0","LTE_MTCe2_L1-Perf","1025","1","F","RP-171310","","","","",""]
["R4-1706038","Test case for cell reselection on idle mode under high speed scenario","Huawei, HiSilicon","Kyoungseok Oh","66120","CR","Agreement","","","261","7.25.3","RRM performance (36.133) [LTE_high_speed-Perf]",54321,"agreed","2017-05-24T17:16:15.327","2017-05-24T17:17:51.940","R4-1705435","","Rel-14","36.133","14.3.0","LTE_high_speed-Perf","4813","5","B","RP-171257","","","","",""]
["R4-1706039","Test case for measurement reporting on connected mode under high speed scenario","Huawei, HiSilicon","Kyoungseok Oh","66120","CR","Agreement","","","261","7.25.3","RRM performance (36.133) [LTE_high_speed-Perf]",54341,"agreed","2017-05-24T17:16:16.513","2017-05-24T17:17:51.957","R4-1705469","","Rel-14","36.133","14.3.0","LTE_high_speed-Perf","4814","3","B","RP-171257","","","","",""]
["R4-1706040","CR for PHR requirement for NB-IoT R13","Huawei, HiSilicon","Kyoungseok Oh","66120","CR","Agreement","","","195","7.17.3.2.3","PHR [NB_IOTenh-Core]",53311,"agreed","2017-05-24T17:16:17.717","2017-05-24T17:17:51.957","R4-1705331","","Rel-13","36.133","13.7.0","NB_IOTenh-Core","4765","3","F","RP-171267","","","","",""]
["R4-1706041","4DL FDD RSRQ for E-UTRAN in Carrier Aggregation in R13","Huawei, HiSilicon","Kyoungseok Oh","66120","CR","Agreement","","Post-meeting note: It was noted before RAN#76 that there is a cover sheet error. So it was revised to R4-1706299","292","7.29.3","RRM [WI code or TEI14]",50291,"revised","2017-05-24T17:16:18.963","2017-05-24T17:17:51.957","R4-1705029","","Rel-13","36.133","13.7.0","TEI14","4910","1","F","","","","","",""]
["R4-1706042","Cleanup of TS 36.307","ETSI MCC, Nokia,. Ericsson, Fujitsu","Kyoungseok Oh","66120","CR","Agreement","","","18","4.2.6","Other specifications [WI code or TEI12]",571001,"agreed","2017-05-24T17:16:20.180","2017-05-24T17:17:51.957","R4-1705710","","Rel-14","36.307","14.2.0","LC_MTC_LTE_cat0_B25_B26-Core, LTE_MTCe2_L1_cat1_B25_B40-Core, NB_IOT_R14_bands-Core, LTE_4Rx_AP_DL_CA-Core, LTE_4Rx_AP_DL_CA-Perf, LTE_high_speed-Perf","0749","1","F","RP-171291","","","","",""]
["R4-1706043","Cleanup of TS 36.307","ETSI MCC, Nokia, Ericsson, Fujitsu","Kyoungseok Oh","66120","CR","Agreement","","","18","4.2.6","Other specifications [WI code or TEI12]",570901,"agreed","2017-05-24T17:16:21.443","2017-05-24T17:17:51.970","R4-1705709","","Rel-13","36.307","13.6.0","LC_MTC_LTE_cat0_B25_B26-Core, LTE_MTCe2_L1_cat1_B25_B40-Core, NB_IOT_R14_bands-Core, LTE_4Rx_AP_DL_CA-Core, LTE_4Rx_AP_DL_CA-Perf, TEI13, LTE_high_speed-Perf","0748","1","F","RP-171291","","","","",""]
["R4-1706044","Cleanup of TS 36.307","ETSI MCC, Nokia, Ericsson, Fujitsu","Kyoungseok Oh","66120","CR","Agreement","","","18","4.2.6","Other specifications [WI code or TEI12]",570801,"agreed","2017-05-24T17:16:22.707","2017-05-24T17:17:51.970","R4-1705708","","Rel-12","36.307","12.14.0","LC_MTC_LTE_cat0_B25_B26-Core, TEI12","0747","1","F","RP-171291","","","","",""]
["R4-1706045","Cleanup of TS 36.307","ETSI MCC, Nokia, Ericsson, Fujitsu","Kyoungseok Oh","66120","CR","Agreement","","","18","4.2.6","Other specifications [WI code or TEI12]",570701,"agreed","2017-05-24T17:16:24.063","2017-05-24T17:17:51.970","R4-1705707","","Rel-11","36.307","11.18.0","TEI11, LTE_4Rx_AP_DL","0746","1","F","RP-171295","","","","",""]
["R4-1706046","Cleanup of TS 36.307","ETSI MCC, Nokia, Ericsson, Fujitsu","Kyoungseok Oh","66120","CR","Agreement","","","18","4.2.6","Other specifications [WI code or TEI12]",570601,"agreed","2017-05-24T17:16:25.343","2017-05-24T17:17:51.987","R4-1705706","","Rel-10","36.307","10.21.0","TEI10, LTE_4Rx_AP_DL","0745","1","F","RP-171294","","","","",""]
["R4-1706047","Draft LS on Rel-14 RAN4 UE feature list","Intel Corporation","Kyoungseok Oh","66120","LS out","Approval","","","289","7.29","TEI14",56581,"withdrawn","2017-05-24T17:16:26.747",null,"","","Rel-14","","","","","","","","","RAN2","RAN, RAN1","",""]
["R4-1706048","Further consideration for NR band and band combination in Rel15 WI","NTT DOCOMO, INC.","Kyoungseok Oh","66120","other","Approval","","","412","10.2","NR bands and NR-LTE band combinations [NR_newRAT]",47831,"approved","2017-05-24T17:16:27.060","2017-05-24T17:17:51.987","R4-1705165","","Rel-15","","","NR_newRAT","","","","","","","","",""]
["R4-1706049","Further study on the feasibility of 3.3 GHz ? 4.2 GHz NR spectrum","Intel Corporation","Kyoungseok Oh","66120","other","Discussion","","","415","10.2.1.2","Band definition for NR bands [NR_newRAT]",52350,"noted","2017-05-24T17:16:27.357","2017-05-24T17:17:51.987","","","","","","","","","","","","","","",""]
["R4-1706050","WF on NR band numbering","Ericsson","Kyoungseok Oh","66120","other","Discussion","","","413","10.2.1","NR frequency range and bands [NR_newRAT]",605000,"approved","2017-05-24T17:16:27.653","2017-05-24T17:17:51.987","","","","","","","","","","","","","","",""]
["R4-1706051","NR band numbering","Ericsson","Kyoungseok Oh","66120","other","Approval","","","413","10.2.1","NR frequency range and bands [NR_newRAT]",52941,"noted","2017-05-24T17:16:27.947","2017-05-24T17:17:52.003","R4-1704613","","Rel-15","","","NR_newRAT","","","","","","","","",""]
["R4-1706052","3.5 GHz Band arrangement","Qualcomm Incorporated","Kyoungseok Oh","66120","other","Approval","","","415","10.2.1.2","Band definition for NR bands [NR_newRAT]",47751,"noted","2017-05-24T17:16:28.247","2017-05-24T17:17:52.003","R4-1705200","","Rel-15","","","NR_newRAT-Core","","","","","","","","",""]
["R4-1706053","WF on NR band definition for 3.3-4.2GHz","NTT DoCoMo","Kyoungseok Oh","66120","other","Discussion","","","415","10.2.1.2","Band definition for NR bands [NR_newRAT]",567000,"noted","2017-05-24T17:16:28.540","2017-05-24T17:17:52.003","","","","","","","","","","","","","","",""]
["R4-1706054","WF on Maximum Channel Bandwidth","Qualcomm Incorporated","Kyoungseok Oh","66120","other","Approval","","","418","10.3.1","Channel bandwidth and subcarrier spacing [NR_newRAT]",52401,"revised","2017-05-24T17:16:28.853","2017-05-24T17:17:52.017","R4-1704566","R4-1706321","Rel-15","","","","","","","","","","","",""]
["R4-1706055","WF on supporting channel bandwidth and SCS","Ericsson","Kyoungseok Oh","66120","other","Discussion","","","418","10.3.1","Channel bandwidth and subcarrier spacing [NR_newRAT]",605500,"revised","2017-05-24T17:16:29.307","2017-05-24T17:17:52.017","","R4-1706315","","","","","","","","","","","","",""]
["R4-1706056","WF on Channel Raster and Sychronization Raster/SCS","Huawei","Kyoungseok Oh","66120","other","Discussion","","","419","10.3.2","Channel Raster [NR_newRAT]",52650,"revised","2017-05-24T17:16:29.603","2017-05-24T17:17:52.017","","R4-1706323","","","","","","","","","","","","",""]
["R4-1706057","NR Sync channel raster and channel arrangement","Ericsson","Kyoungseok Oh","66120","other","Approval","","","419","10.3.2","Channel Raster [NR_newRAT]",486302,"noted","2017-05-24T17:16:29.897","2017-06-12T07:47:51.333","R4-1704614","","Rel-15","","","NR_newRAT","","","","","","","","",""]
["R4-1706058","Correction on PHR reporting requirements for NB1","Ericsson","Kyoungseok Oh","66120","other","Approval","","","62","5.5.5","RRM Performance (36.133) [NB_IOT-Perf]",48261,"withdrawn","2017-05-24T17:16:30.210",null,"R4-1705082","","","36.133","","NB_IOT-Perf","","","","","","","","",""]
["R4-1706059","Discussion on spectrum utilization","SAMSUNG Electronics Co., Ltd.","Kyoungseok Oh","66120","discussion","Discussion","","","420","10.3.3","Spectrum utilization [NR_newRAT]",53421,"noted","2017-05-24T17:16:30.553","2017-06-07T07:58:11.087","R4-1705240","","Rel-15","","","","","","","","","","","",""]
["R4-1706060","WF on spectrum utiliztion","Huawei, Qualcomm Incorporated","Kyoungseok Oh","66120","other","Discussion","","","420","10.3.3","Spectrum utilization [NR_newRAT]",606000,"approved","2017-05-24T17:16:30.867","2017-05-24T17:17:52.033","","","","","","","","","","","","","","",""]
["R4-1706061","WF on the mixed numerology and associated in-band requirements","Huawei","Kyoungseok Oh","66120","other","Discussion","","","421","10.3.4","In-band requirements [NR_newRAT]",606100,"revised","2017-05-24T17:16:31.163","2017-05-24T17:17:52.050","","R4-1706320","","","","","","","","","","","","",""]
["R4-1706062","WF on sub 6GHz ACLR and ACS","Nokia, Alcatel-Lucent Shanghai Bell","Kyoungseok Oh","66120","other","Discussion","","","422","10.3.5","ACLR and ACS [NR_newRAT]",606200,"revised","2017-05-24T17:16:31.457","2017-05-24T17:17:52.050","","R4-1706316","","","","","","","","","","","","",""]
["R4-1706063","WF on ACLR and ACS for mmWave","Qualcomm Incorporated","Kyoungseok Oh","66120","other","Discussion","","","422","10.3.5","ACLR and ACS [NR_newRAT]",606300,"approved","2017-05-24T17:16:31.770","2017-05-24T17:17:52.063","","","","","","","","","","","","","","",""]
["R4-1706064","Cleanup of TS 36.307","ETSI MCC, Fujitsu, Ericsson, Nokia","Kyoungseok Oh","66120","CR","Agreement","","","18","4.2.6","Other specifications [WI code or TEI12]",570401,"agreed","2017-05-24T17:16:32.067","2017-05-24T17:17:52.063","R4-1705704","","Rel-8","36.307","8.16.0","TEI8","0743","1","F","RP-171292","","","","",""]
["R4-1706065","Cleanup of TS 36.307","ETSI MCC, Fujitsu, Ericsson, Nokia","Kyoungseok Oh","66120","CR","Agreement","","","18","4.2.6","Other specifications [WI code or TEI12]",570501,"agreed","2017-05-24T17:16:33.330","2017-05-24T17:17:52.063","R4-1705705","","Rel-9","36.307","9.18.0","TEI9","0744","1","F","RP-171293","","","","",""]
["R4-1706066","High power UE for LTE Band 40","Reliance Jio, Samsung, PT Smartfren Telecom","Kyoungseok Oh","66120","WID new","Discussion","","","473","13","Revision of the Work Plan",53821,"noted","2017-05-24T17:16:34.487","2017-05-24T17:17:52.063","R4-1705242","","Rel-15","","","","","","","","","","","",""]
["R4-1706067","WF on UE reference architecture","Sony","Kyoungseok Oh","66120","other","Discussion","","","425","10.4.2","Reference architecture [NR_newRAT]",606700,"approved","2017-05-24T17:16:34.827","2017-05-24T17:17:52.080","","","","","","","","","","","","","","",""]
["R4-1706068","WF on High power UE","CMCC, Skyworks, Qorvo, Broadcom, MediaTek, Vodafone, CATT, Huawei, HiSilicon, ZTE","Kyoungseok Oh","66120","other","Discussion","","","427","10.4.3.1","UE power class and MPR/A-MPR [NR_newRAT]",606800,"approved","2017-05-24T17:16:35.123","2017-05-24T17:17:52.080","","","","","","","","","","","","","","",""]
["R4-1706069","Reply LS on supporting Rel-14 feature of performance enhancement for high speed scenarios from Rel-13 UEs","RAN2, Huawei","Kyoungseok Oh","66120","LS in","Discussion","","","3","3","Letters / reports from other groups / meetings",606900,"noted","2017-05-24T17:16:35.437","2017-05-24T17:17:52.080","","","Rel-14","","","LTE_high_speed","","","","","","RAN4","","R2-1705861","R4-1702308"]
["R4-1706070","Standardisation of a new E-UTRA band","ATU","Kyoungseok Oh","66120","LS in","Discussion","","","3","3","Letters / reports from other groups / meetings",607000,"noted","2017-05-24T17:16:35.763","2017-05-24T17:17:52.097","","","","","","","","","","","","RAN, RAN4","","Standardisation of a new E-UTRA band",""]
["R4-1706071","WF on On Off Mask Transient Time","Qualcomm, Intel, CATT, Ericsson, Huawei","Kyoungseok Oh","66120","other","Approval","","","428","10.4.3.2","ON/OFF time mask [NR_newRAT]",577601,"revised","2017-05-24T17:16:36.093","2017-05-24T17:17:52.097","","R4-1706317","","","","","","","","","","","","",""]
["R4-1706072","WF on General spurious emission for NR UE","NTT DOCOMO, INC.","Kyoungseok Oh","66120","other","Discussion","","","429","10.4.3.3","Spurious emission [NR_newRAT]",52610,"approved","2017-05-24T17:16:36.387","2017-05-24T17:17:52.097","","","","","","","","","","","","","","",""]
["R4-1706073","mmW SEM","Qualcomm Incorporated","Kyoungseok Oh","66120","other","","","","429","10.4.3.3","Spurious emission [NR_newRAT]",567701,"approved","2017-05-24T17:16:36.683","2017-05-24T17:17:52.110","R4-1705675","","","","","","","","","","","","","",""]
["R4-1706074","LS on RAN4 agreements for FeD2D","Intel Corporation","Kyoungseok Oh","66120","LS out","Approval","","","471","11.1.1","Co-existence study [FS_feD2D_IoT_relay_wearable]",607400,"approved","2017-05-24T17:16:37.013","2017-05-24T17:17:52.110","","","Rel-14","","","FS_feD2D_IoT_relay_wearable","","","","","","RAN1, RAN2","","",""]
["R4-1706075","Way forward on testing for BS supporting E-UTRA and NB-IoT operation","Nokia, Alcatel-Lucent Shanghai Bell","Kyoungseok Oh","66120","other","Discussion","","","59","5.5.2","BS RF core(36.104) [NB_IOT-Core]",607500,"revised","2017-05-24T17:16:37.307","2017-05-24T17:17:52.110","","R4-1706079","","","","","","","","","","","","",""]
["R4-1706076","DRAFT LS on extension of NS and CA_NS signalling space","Nokia, Alcatel-Lucent Shanghai Bell","Kyoungseok Oh","66120","LS out","Approval","","","291","7.29.2","RF [WI code or TEI14]",569002,"approved","2017-05-24T17:16:37.607","2017-05-24T17:17:52.110","R4-1705865","","Rel-14","","","TEI14","","","","","","RAN2","","",""]
["R4-1706077","4Rx REFSENS requirements spec improvement for 36.101","Huawei, HiSilicon","Kyoungseok Oh","66120","CR","Agreement","","","30","5.2.1","UE RF core(36.101) [LTE_4Rx_AP_DL-Core]",0,"agreed","2017-05-24T17:16:37.917","2017-05-24T17:17:52.127","R4-1705219","","Rel-14","36.101","14.3.0","LTE_4Rx_AP_DL-Core, LTE_4Rx_AP_DL_bands-Core","4446","1","F","RP-171304","","","","",""]
["R4-1706078","Remove NB-IoT inband support for 1.4 MHz","Ericsson, Huawei, Nokia, Alcatel-Lucent Shanghai Bell","Kyoungseok Oh","66120","CR","Agreement","","","59","5.5.2","BS RF core(36.104) [NB_IOT-Core]",54002,"agreed","2017-05-24T17:16:39.133","2017-05-24T17:17:52.127","R4-1705870","","Rel-13","37.104","13.5.0","NB_IOT-Core","0779","2","F","RP-171299","","","","",""]
["R4-1706079","Way forward on testing for BS supporting E-UTRA and NB-IoT operation","Nokia, Alcatel-Lucent Shanghai Bell","Kyoungseok Oh","66120","other","Discussion","","","59","5.5.2","BS RF core(36.104) [NB_IOT-Core]",607501,"approved","2017-05-24T17:16:40.337","2017-05-24T17:17:52.127","R4-1706075","","","","","","","","","","","","","",""]
["R4-1706080","Testing for BS supporting NB-IoT operation (TS 37.141)","Nokia, Alcatel-Lucent Shanghai Bell","Kyoungseok Oh","66120","CR","Agreement","","","61","5.5.4","BS RF Conformance testing (36.141) [NB_IOT-Perf]",55671,"agreed","2017-05-24T17:16:40.663","2017-05-24T17:17:52.143","R4-1705424","","Rel-13","37.141","13.6.0","NB_IOT-Perf","0784","1","F","RP-171302","","","","",""]
["R4-1706081","Testing for BS supporting NB-IoT operation (TS 37.141)","Nokia, Alcatel-Lucent Shanghai Bell","Kyoungseok Oh","66120","CR","Agreement","","","61","5.5.4","BS RF Conformance testing (36.141) [NB_IOT-Perf]",573801,"agreed","2017-05-24T17:16:41.897","2017-05-24T17:17:52.143","R4-1705425","","Rel-14","37.141","14.3.0","NB_IOT-Perf","0785","1","A","RP-171302","","","","",""]
["R4-1706082","CR for CAT-M2 REFSENS, MPR and adding note for protection band 5","Ericsson, KDDI","Kyoungseok Oh","66120","CR","Agreement","","","207","7.18.2.2","REFSENS [LTE_feMTC-Core]",587501,"revised","2017-05-24T17:16:43.097","2017-05-24T17:17:52.143","R4-1705872","R4-1706105","Rel-14","36.101","14.3.0","LTE_feMTC-Core","4485","1","B","","","","","",""]
["R4-1706083","Introduction of 5DL CA combinations to 36.104","Nokia","Kyoungseok Oh","66120","CR","Agreement","","","112","7.5.1","Rapporteur Input (WID/CRs) [LTE_CA_R14_5DL1UL-Core]",0,"agreed","2017-05-24T17:16:44.327","2017-05-24T17:17:52.157","R4-1704594","","Rel-14","36.104","14.3.0","LTE_CA_R14_5DL1UL-Core","4668","1","B","RP-171276","","","","",""]
["R4-1706084","Introduction of 5DL CA combinations to 36.141","Nokia","Kyoungseok Oh","66120","CR","Agreement","","","112","7.5.1","Rapporteur Input (WID/CRs) [LTE_CA_R14_5DL1UL-Core]",0,"agreed","2017-05-24T17:16:45.547","2017-05-24T17:17:52.157","R4-1704595","","Rel-14","36.141","14.3.0","LTE_CA_R14_5DL1UL-Perf","1024","1","B","RP-171276","","","","",""]
["R4-1706085","Introduction of Rel-14 4DL/1UL combinations in 36.101","Ericsson","Kyoungseok Oh","66120","CR","Agreement","","","106","7.4.1","Rapporteur Input (WID/CRs) [LTE_CA_R14_4DL1UL-Core]",0,"revised","2017-05-24T17:16:46.747","2017-05-24T17:17:52.157","R4-1704889","","Rel-14","36.101","14.3.0","LTE_CA_R14_4DL1UL","4426","1","B","","","","","",""]
["R4-1706086","Introduction of Rel-14 4DL/1UL combinations in 36.104","Ericsson","Kyoungseok Oh","66120","CR","Agreement","","","106","7.4.1","Rapporteur Input (WID/CRs) [LTE_CA_R14_4DL1UL-Core]",0,"revised","2017-05-24T17:16:47.900","2017-05-24T17:17:52.173","R4-1704890","","Rel-14","36.104","14.3.0","LTE_CA_R14_4DL1UL","4672","1","B","","","","","",""]
["R4-1706087","Introduction of Rel-14 4DL/1UL combinations in 36.141","Ericsson","Kyoungseok Oh","66120","CR","Approval","","","106","7.4.1","Rapporteur Input (WID/CRs) [LTE_CA_R14_4DL1UL-Core]",48911,"revised","2017-05-24T17:16:49.227","2017-05-24T17:17:52.173","R4-1704891","R4-1706107","Rel-14","36.141","14.3.0","LTE_CA_R14_4DL1UL","1034","1","B","","","","","",""]
["R4-1706088","Correction to A-MPR tables and in-band emissions for eLAA","Ericsson","Kyoungseok Oh","66120","CR","Agreement","","","161","7.14.2","UE RF Maintenance(36.101) [LTE_eLAA-Core]",51021,"agreed","2017-05-24T17:16:50.490","2017-05-24T17:17:52.173","R4-1705102","","Rel-14","36.101","14.3.0","LTE_eLAA-Core","4435","1","F","RP-171285","","","","",""]
["R4-1706089","CR on V2X Pumax for non-concurrent operaion","LG Electronics Inc.","Kyoungseok Oh","66120","CR","Agreement","","","177","7.16.2","UE RF Maintenance (36.101) [LTE_V2X-Core]",48651,"agreed","2017-05-24T17:16:51.753","2017-05-24T17:17:52.173","R4-1704865","","Rel-14","36.101","14.3.0","LTE_V2X-Core","4420","1","F","RP-171282","","","","",""]
["R4-1706090","Introduction of Band 49 LAA operation in UE spec","Ericsson","Kyoungseok Oh","66120","CR","Approval","","","352","9.11.2","UE RF (Downlink only in 3.5GHz) (36.101) [LTE_ 3550_CBRS_US_LAA]",53101,"revised","2017-05-24T17:16:52.940","2017-05-24T17:17:52.190","R4-1705098","R4-1706114","Rel-15","36.101","14.3.0","LTE_3550_CBRS_US_LAA","4434","1","B","","","","","",""]
["R4-1706091","WF on LTE extended 1.5GHz SDL band plan","Nokia","Kyoungseok Oh","66120","other","Approval","","","320","9.5","LTE Extended 1.5 GHz SDL band (1427 ? 1518 MHz) and LTE Carrier Aggregation (2DL/1UL) with Band 20 [LTE_SDL_1500ext]",49700,"approved","2017-05-24T17:16:54.140","2017-05-24T17:17:52.190","","","","","","","","","","","","","","",""]
["R4-1706092","WF on PCmax computation and evaluation for single CC and CA with sTTI","Qualcomm Incorporated","Kyoungseok Oh","66120","other","Approval","","","371","9.13.2","UE RF (36.101) [LTE_sTTIandPT-core]",55820,"withdrawn","2017-05-24T17:16:54.453",null,"","","","","","","","","","","","","","",""]
["R4-1706093","TRP/TRS joint band passing rate worksheet","Intel Corporation","Kyoungseok Oh","66120","discussion","Discussion","","","140","7.10.2","Hand phantom for smartphones [LTE_UTRA_TRP_TRS-Core]",54710,"noted","2017-05-24T17:16:54.750","2017-05-24T17:17:52.190","R4-1704655","","Rel-14","","","LTE_UTRA_TRP_TRS-Core","","","","","","","","",""]
["R4-1706094","Additional TRP/TRS LTE BHH data","Sony","Kyoungseok Oh","66120","other","Discussion","","","140","7.10.2","Hand phantom for smartphones [LTE_UTRA_TRP_TRS-Core]",46550,"noted","2017-05-24T17:16:55.077","2017-05-24T17:17:52.207","","","","","","","","","","","","","","",""]
["R4-1706095","Updated information on TRP/TRS LTE BHH data","Telecom Italia","Kyoungseok Oh","66120","other","Discussion","","","140","7.10.2","Hand phantom for smartphones [LTE_UTRA_TRP_TRS-Core]",46551,"noted","2017-05-24T17:16:55.390","2017-05-24T17:17:52.207","","","","","","","","","","","","","","",""]
["R4-1706096","WF on LTE BHH TRP/TRS","Telecom Italia","Kyoungseok Oh","66120","other","Discussion","","","140","7.10.2","Hand phantom for smartphones [LTE_UTRA_TRP_TRS-Core]",609400,"approved","2017-05-24T17:16:55.700","2017-05-24T17:17:52.207","","","","","","","","","","","","","","",""]
["R4-1706097","CR on Channel Model Validation","ETS-Lindgren Europe, MVG Industries","Kyoungseok Oh","66120","CR","Agreement","","","145","7.11.2","Performance requirements [LTE_MIMO_OTA-Core]",45292,"revised","2017-05-24T17:16:56.030","2017-05-24T17:17:52.220","R4-1705921","","Rel-14","37.977","14.3.0","LTE_MIMO_OTA","0060","2","B","","","","","",""]
["R4-1706098","WF on transient time for sTTI","Ericsson","Kyoungseok Oh","66120","other","Discussion","","","374","9.13.2.2.1","ON/OFF time mask [LTE_sTTIandPT-core]",48390,"approved","2017-05-24T17:16:57.323","2017-05-24T17:17:52.220","","","","","","","","","","","","","","",""]
["R4-1706099","Introduction of additional band combinations for Intra-band CA","Ericsson","Kyoungseok Oh","66120","CR","Agreement","","","88","7.1.1","Rapporteur Input (WID/CRs) [LTE_CA_R14_intra-Core]",48861,"agreed","2017-05-24T17:16:57.650","2017-05-24T17:17:52.220","R4-1704886","","Rel-14","36.101","14.3.0","LTE_CA_R14_intra-Core","4425","1","B","RP-171272","","","","",""]
["R4-1706100","Introduction of additional band combinations for Intra-band CA","Ericsson","Kyoungseok Oh","66120","CR","Agreement","","","88","7.1.1","Rapporteur Input (WID/CRs) [LTE_CA_R14_intra-Core]",48871,"agreed","2017-05-24T17:16:59.087","2017-05-24T17:17:52.237","R4-1704887","","Rel-14","36.104","14.3.0","LTE_CA_R14_intra-Core","4671","1","B","RP-171272","","","","",""]
["R4-1706101","Introduction of additional band combinations for Intra-band CA","Ericsson","Kyoungseok Oh","66120","CR","Agreement","","","88","7.1.1","Rapporteur Input (WID/CRs) [LTE_CA_R14_intra-Core]",48881,"agreed","2017-05-24T17:17:00.413","2017-05-24T17:17:52.237","R4-1704888","","Rel-14","36.141","14.3.0","LTE_CA_R14_intra-Core","1033","1","B","RP-171272","","","","",""]
["R4-1706102","LTE OTA TRP-TRS AH meeting minutes","Telecom Italia","Kyoungseok Oh","66120","report","Approval","","","139","7.10.1","General [LTE_UTRA_TRP_TRS-Core]",47550,"noted","2017-05-24T17:17:01.723","2017-05-24T17:17:52.237","","","","","","","","","","","","","","",""]
["R4-1706103","Updated information on TRP/TRS LTE BHH data","Vodafone","Kyoungseok Oh","66120","other","Discussion","","","140","7.10.2","Hand phantom for smartphones [LTE_UTRA_TRP_TRS-Core]",46560,"noted","2017-05-24T17:17:02.067","2017-05-24T17:17:52.250","","","","","","","","","","","","","","",""]
["R4-1706104","Band plan + EESS/MSS protection levels for TDD L-band","Huawei, Nokia, Etisalat","Kyoungseok Oh","66120","other","Discussion","","","327","9.6.1","Band Arrangement [LTE_TDD_L_Band-core]",55810,"approved","2017-05-24T17:17:02.377","2017-05-24T17:17:52.250","","","","","","","","","","","","","","",""]
["R4-1706105","CR for CAT-M2 REFSENS, MPR and adding note for protection band 5","Ericsson, KDDI, Sony , Nokia","Kyoungseok Oh","66120","CR","Agreement","","","207","7.18.2.2","REFSENS [LTE_feMTC-Core]",587502,"agreed","2017-05-24T17:17:02.707","2017-05-24T17:17:52.250","R4-1706082","","Rel-14","36.101","14.3.0","LTE_feMTC-Core","4485","2","B","RP-171266","","","","",""]
["R4-1706106","Introduction of completed R14 2DL band combinations to TS 36.141","Qualcomm Incorporated","Kyoungseok Oh","66120","CR","Agreement","","","94","7.2.1","Rapporteur Input (WID/CRs) [LTE_CA_R14_2DL1UL-Core]",51981,"agreed","2017-05-24T17:17:04.030","2017-05-24T17:17:52.250","R4-1705197","","Rel-14","36.141","14.3.0","LTE_CA_R14_2DL1UL-Perf","1035","1","B","RP-171273","","","","",""]
["R4-1706107","Introduction of Rel-14 4DL/1UL combinations in 36.141","Ericsson","Kyoungseok Oh","66120","CR","Agreement","","","106","7.4.1","Rapporteur Input (WID/CRs) [LTE_CA_R14_4DL1UL-Core]",0,"revised","2017-05-24T17:17:05.390","2017-05-24T17:17:52.267","R4-1706087","","Rel-14","36.141","14.3.0","LTE_CA_R14_4DL1UL","1034","2","B","","","","","",""]
["R4-1706108","Intermodulation performance requirement for NB-IoT operation (TS 37.104)","Nokia, Alcatel-Lucent Shanghai Bell","Kyoungseok Oh","66120","CR","Agreement","","","59","5.5.2","BS RF core(36.104) [NB_IOT-Core]",55651,"agreed","2017-05-24T17:17:06.887","2017-05-24T17:17:52.267","R4-1705414","","Rel-13","37.104","13.5.0","NB_IOT-Core","0784","1","F","RP-171300","","","","",""]
["R4-1706109","Intermodulation performance requirement for NB-IoT operation (TS 36.141)","Nokia, Alcatel-Lucent Shanghai Bell","Kyoungseok Oh","66120","CR","Agreement","","","61","5.5.4","BS RF Conformance testing (36.141) [NB_IOT-Perf]",54171,"agreed","2017-05-24T17:17:08.243","2017-05-24T17:17:52.267","R4-1705416","","Rel-13","36.141","13.7.0","NB_IOT-Perf","1043","1","F","RP-171303","","","","",""]
["R4-1706110","Intermodulation performance requirement for NB-IoT operation (TS 37.141)","Nokia, Alcatel-Lucent Shanghai Bell","Kyoungseok Oh","66120","CR","Agreement","","","61","5.5.4","BS RF Conformance testing (36.141) [NB_IOT-Perf]",54191,"agreed","2017-05-24T17:17:09.523","2017-05-24T17:17:52.283","R4-1705418","","Rel-13","37.141","13.6.0","NB_IOT-Perf","0782","1","F","RP-171303","","","","",""]
["R4-1706111","Update of LAA REFSENS exclusion region","QUALCOMM UK Ltd","Kyoungseok Oh","66120","CR","Agreement","","","34","5.3.1","UE RF core (36.101) [LTE_LAA-Core]",54792,"agreed","2017-05-24T17:17:10.787","2017-05-24T17:17:52.283","R4-1705911","","Rel-13","36.101","13.7.0","LTE_LAA-Core","4476","2","F","RP-171307","","","","",""]
["R4-1706112","Reply LS regarding 1024QAM","Huawei, HiSilicon","Kyoungseok Oh","66120","LS out","Approval","","","405","9.17.1","General [LTE_HCS]",56612,"approved","2017-05-24T17:17:12.067","2017-05-24T17:17:52.297","R4-1705880","","Rel-15","","","LTE_1024QAM_DL-Core","","","","","R1-1706842","RAN1","","",""]
["R4-1706113","Reference sensitivity for the extended L-band","ORANGE","Kyoungseok Oh","66120","other","Approval","","","322","9.5.2","UE RF (36.101) [LTE_SDL_1500ext-core]",50881,"noted","2017-05-24T17:17:12.423","2017-05-24T17:17:52.313","R4-1705088","","Rel-14","","","LTE_SDL_1500ext-Core","","","","","","","","",""]
["R4-1706114","Introduction of Band 49 LAA operation in UE spec","Ericsson","Kyoungseok Oh","66120","CR","Approval","","","352","9.11.2","UE RF (Downlink only in 3.5GHz) (36.101) [LTE_ 3550_CBRS_US_LAA]",53102,"revised","2017-05-24T17:17:12.783","2017-05-24T17:17:52.313","R4-1706090","R4-1706118","Rel-15","36.101","14.3.0","LTE_3550_CBRS_US_LAA","4434","2","B","","","","","",""]
["R4-1706115","WF on LTE band numbers in Rel-15","Nokia","Kyoungseok Oh","66120","other","Discussion","","","301","9","Rel-15 Work Items for LTE",611500,"approved","2017-05-24T17:17:14.017","2017-05-24T17:17:52.313","","","","","","","","","","","","","","",""]
["R4-1706116","TDD L-Band - Channel numbering for E-UTRA, MSR","Huawei, Hisilicon","Kyoungseok Oh","66120","other","Approval","","","327","9.6.1","Band Arrangement [LTE_TDD_L_Band-core]",56201,"approved","2017-05-24T17:17:14.373","2017-05-24T17:17:52.313","R4-1705620","","","","","","","","","","","","","",""]
["R4-1706117","TP for TR: A-MPR summary for EESS protection for TDD operation in L-band","Etisalat, Huawei, Hisilicon","Kyoungseok Oh","66120","other","Approval","","","328","9.6.2","UE RF (36.101) [LTE_TDD_L_Band-core]",56151,"noted","2017-05-24T17:17:14.703","2017-05-24T17:17:52.330","R4-1705765","","","36.753","","LTE_TDD_L_Band-Perf","","","","","","","","",""]
["R4-1706118","Introduction of Band 49 LAA operation in UE spec","Ericsson","Kyoungseok Oh","66120","CR","Approval","","","352","9.11.2","UE RF (Downlink only in 3.5GHz) (36.101) [LTE_ 3550_CBRS_US_LAA]",53103,"endorsed","2017-05-24T17:17:15.030","2017-05-24T17:17:52.330","R4-1706114","","Rel-15","36.101","14.3.0","LTE_3550_CBRS_US_LAA","4434","3","B","","","","","",""]
["R4-1706119","[Draft] Introduction of TDD L band into TS 36.101","Huawei, Hisilicon, Etisalat","Kyoungseok Oh","66120","draftCR","","","","328","9.6.2","UE RF (36.101) [LTE_TDD_L_Band-core]",576602,"withdrawn","2017-05-24T17:17:16.120",null,"R4-1705929","","Rel-15","36.101","14.3.0","LTE_TDD_L_Band-Core","","","","","","","","",""]
["R4-1706120","[Draft] Introduction of TDD L band into TS 36.104","Huawei, Hisilicon, Etisalat","Kyoungseok Oh","66120","draftCR","","","","329","9.6.3","BS RF (36.104, 36.141) [LTE_TDD_L_Band-core/Perf]",56171,"revised","2017-05-24T17:17:16.433","2017-05-24T17:17:52.330","R4-1705827","R4-1706231","Rel-15","36.104","14.3.0","LTE_TDD_L_Band-Core","","","","","","","","",""]
["R4-1706121","Draft CR sTTI 2OS introduction","Ericsson","Kyoungseok Oh","66120","draftCR","Endorsement","","","378","9.13.3","BS RF (36.104) [LTE_sTTIandPT-core]",48382,"endorsed","2017-05-24T17:17:16.777","2017-05-24T17:17:52.347","R4-1705933","","Rel-14","36.104","14.3.0","LTE_sTTIandPT-Core","","","B","","","","","",""]
["R4-1706122","sTTI ON/OFF Mask: List of use cases","Ericsson","Kyoungseok Oh","66120","discussion","Approval","","","374","9.13.2.2.1","ON/OFF time mask [LTE_sTTIandPT-core]",51861,"approved","2017-05-24T17:17:17.103","2017-05-24T17:17:52.347","R4-1704843","","Rel-15","","","LTE_sTTIandPT-Core","","","","","","","","",""]
["R4-1706123","WF on V2X scenarios for V2X phase 2","Huawei, HiSilicon","Kyoungseok Oh","66120","other","Discussion","","","399","9.16.1","General [LTE_eV2X]",587801,"approved","2017-05-24T17:17:17.417","2017-05-24T17:17:52.347","R4-1705878","","","","","","","","","","","","","",""]
["R4-1706124","TP for TR 37.843: Improvements of definitions of spatial angles in sub-clause 4.6","Ericsson","Kyoungseok Oh","66120","pCR","Approval","","","356","9.12.1","General [AASenh_BS_LTE_UTRA]",48751,"approved","2017-05-24T17:17:17.727","2017-05-24T17:17:52.360","R4-1704875","","Rel-15","37.843","0.2.0","AASenh_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-1706125","TP to TR 37.843: BS classification for eAAS BS","NEC","Kyoungseok Oh","66120","pCR","Approval","","","356","9.12.1","General [AASenh_BS_LTE_UTRA]",53141,"approved","2017-05-24T17:17:18.117","2017-05-24T17:17:52.360","R4-1705314","","Rel-15","37.843","0.2.0","AASenh_BS_LTE_UTRA","","","","","","","","",""]
["R4-1706126","WF on specification drafting","Huawei","Kyoungseok Oh","66120","other","Discussion","","","356","9.12.1","General [AASenh_BS_LTE_UTRA]",56360,"approved","2017-05-24T17:17:18.507","2017-05-24T17:17:52.360","","","","","","","","","","","","","","",""]
["R4-1706127","Draft CR to TS 37.105 - TX output power","Huawei","Kyoungseok Oh","66120","discussion","Discussion","","","356","9.12.1","General [AASenh_BS_LTE_UTRA]",56370,"noted","2017-05-24T17:17:18.807","2017-05-24T17:17:52.377","R4-1705653","","","","","AASenh_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-1706128","Draft CR to TS 37.105 - Rx sensitivity output power","Huawei","Kyoungseok Oh","66120","discussion","Discussion","","","356","9.12.1","General [AASenh_BS_LTE_UTRA]",56380,"noted","2017-05-24T17:17:19.117","2017-05-24T17:17:52.377","R4-1705654","","","","","AASenh_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-1706129","Draft TS 37.105 specification text for Transmit signal quality (sub-clause 9.6) and bandwidth (sub-clause 9.7)","Ericsson","Kyoungseok Oh","66120","discussion","Discussion","","","356","9.12.1","General [AASenh_BS_LTE_UTRA]",56540,"noted","2017-05-24T17:17:19.443","2017-05-24T17:17:52.377","R4-1704852","","Rel-15","","","AASenh_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-1706130","Draft TS 37.105 Specification text for Section 6.6 Unwanted Emissions","Ericsson","Kyoungseok Oh","66120","discussion","Discussion","","","356","9.12.1","General [AASenh_BS_LTE_UTRA]",612600,"noted","2017-05-24T17:17:19.757","2017-05-24T17:17:52.393","R4-1705392","","Rel-15","","","AASenh_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-1706131","TP to TR 37.843 ? TRP accuracy","Nokia, Alcatel-Lucent Shanghai Bell","Kyoungseok Oh","66120","pCR","","","","358","9.12.2.1","TRP accuracy [AASenh_BS_LTE_UTRA-Core]",581401,"approved","2017-05-24T17:17:20.053","2017-05-24T17:17:52.393","R4-1705813","","Rel-15","37.843","0.3.0","AASenh_BS_LTE_UTRA","","","","","","","","",""]
["R4-1706132","WF on TX and Rx loss factors","Ericsson","Kyoungseok Oh","66120","other","Discussion","","","359","9.12.2.2","Tx and Rx loss values [AASenh_BS_LTE_UTRA-Core]",613200,"revised","2017-05-24T17:17:20.427","2017-05-24T17:17:52.393","","R4-1706319","","","","","","","","","","","","",""]
["R4-1706133","WF on co-location","Huawei","Kyoungseok Oh","66120","other","Discussion","","","360","9.12.2.3","Co-location requirements [AASenh_BS_LTE_UTRA-Core]",582000,"approved","2017-05-24T17:17:20.723","2017-05-24T17:17:52.407","","","","","","","","","","","","","","",""]
["R4-1706134","WF on Tx IMD","Huawei","Kyoungseok Oh","66120","other","Discussion","","","361","9.12.2.4","TX IMD [AASenh_BS_LTE_UTRA-Core]",613400,"approved","2017-05-24T17:17:21.020","2017-05-24T17:17:52.407","","","","","","","","","","","","","","",""]
["R4-1706135","TP for TR 37.843 - TX Power requirements for control channels","Huawei","Kyoungseok Oh","66120","pCR","Approval","","","362","9.12.2.5","Other Transmitter Requirements [AASenh_BS_LTE_UTRA-Core]",49431,"approved","2017-05-24T17:17:21.333","2017-05-24T17:17:52.407","R4-1705652","","Rel-15","37.843","0.2.0","AASenh_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-1706136","WF on Tx OFF power","Huawei","Kyoungseok Oh","66120","other","Discussion","","","362","9.12.2.5","Other Transmitter Requirements [AASenh_BS_LTE_UTRA-Core]",56480,"approved","2017-05-24T17:17:21.707","2017-05-24T17:17:52.423","","","","","","","","","","","","","","",""]
["R4-1706137","Discussion scaling factor for OTA AAS BS","CATT","Kyoungseok Oh","66120","discussion","Discussion","","","362","9.12.2.5","Other Transmitter Requirements [AASenh_BS_LTE_UTRA-Core]",56511,"noted","2017-05-24T17:17:22.033","2017-05-24T17:17:52.423","R4-1704922","","Rel-14","","","AASenh_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-1706138","TP for TR 37.843: Section 4.4","Ericsson","Kyoungseok Oh","66120","pCR","Approval","","","362","9.12.2.5","Other Transmitter Requirements [AASenh_BS_LTE_UTRA-Core]",56521,"approved","2017-05-24T17:17:22.347","2017-05-24T17:17:52.423","R4-1705389","","Rel-15","37.843","0.2.0","AASenh_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-1706139","TP to TR 37.843: Consideration of missing aspects for core and conformance Tx spurious requirement OTA","Huawei","Kyoungseok Oh","66120","pCR","","","","362","9.12.2.5","Other Transmitter Requirements [AASenh_BS_LTE_UTRA-Core]",580401,"approved","2017-05-24T17:17:22.737","2017-05-24T17:17:52.423","R4-1705805","","Rel-15","37.843","0.3.0","AASenh_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-1706140","TP to TR 37.843 ? Clarify example in sub-clause 5.1","Huawei","Kyoungseok Oh","66120","pCR","Approval","","","362","9.12.2.5","Other Transmitter Requirements [AASenh_BS_LTE_UTRA-Core]",580501,"approved","2017-05-24T17:17:23.127","2017-05-24T17:17:52.440","R4-1705655","","Rel-15","37.843","0.2.0","AASenh_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-1706141","TP to TR 37.843: OTA sensitivity requirements for eAAS","NEC","Kyoungseok Oh","66120","pCR","Approval","","","363","9.12.2.6","Other Receiver requirements [AASenh_BS_LTE_UTRA-Core]",49450,"approved","2017-05-24T17:17:23.500","2017-05-24T17:17:52.440","R4-1705317","","Rel-15","37.843","0.2.0","AASenh_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-1706142","TP to TR37.843 - Capturing OTA REFSENS requirements","Huawei","Kyoungseok Oh","66120","pCR","Approval","","","363","9.12.2.6","Other Receiver requirements [AASenh_BS_LTE_UTRA-Core]",52310,"withdrawn","2017-05-24T17:17:23.890",null,"R4-1705642","","Rel-15","37.843","0.2.0","AASenh_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-1706143","LS to add support for PUSCH repetition factor for reference channel for eMTC CEModeB","RAN5, Ericsson","Kyoungseok Oh","66120","LS in","Discussion","","","3","3","Letters / reports from other groups / meetings",614300,"noted","2017-05-24T17:17:24.267","2017-05-24T17:17:52.440","","","Rel-13","","","LTE_MTCe2_L1-UEConTest","","","","","","RAN4","","R5-173297",""]
["R4-1706144","TP to TR37.843 - Clarifying Declarations for OTA sensitivity and OTA REFSENS","Huawei","Kyoungseok Oh","66120","pCR","Approval","","","363","9.12.2.6","Other Receiver requirements [AASenh_BS_LTE_UTRA-Core]",54950,"approved","2017-05-24T17:17:24.577","2017-05-24T17:17:52.453","R4-1705645","","Rel-15","37.843","0.2.0","AASenh_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-1706145","WF on OTA blocking","CMCC","Kyoungseok Oh","66120","other","Discussion","","","363","9.12.2.6","Other Receiver requirements [AASenh_BS_LTE_UTRA-Core]",56430,"noted","2017-05-24T17:17:24.937","2017-05-24T17:17:52.470","","","","","","","","","","","","","","",""]
["R4-1706146","TP to 37.843: In band blocking requirement","Ericsson","Kyoungseok Oh","66120","pCR","Approval","","","363","9.12.2.6","Other Receiver requirements [AASenh_BS_LTE_UTRA-Core]",56440,"withdrawn","2017-05-24T17:17:25.233",null,"R4-1704945","","Rel-15","37.843","0.2.0","AASenh_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-1706147","WF on alignment of EMC emission and RF RSE requirements","Huawei","Kyoungseok Oh","66120","other","Discussion","","","364","9.12.2.7","EMC requirements [AASenh_BS_LTE_UTRA-Core]",54930,"approved","2017-05-24T17:17:25.607","2017-05-24T17:17:52.470","","","","","","","","","","","","","","",""]
["R4-1706148","TP for TR 37.843 on testing EMC immunity for OTA AAS BS - general section","Ericsson","Kyoungseok Oh","66120","pCR","Approval","","","364","9.12.2.7","EMC requirements [AASenh_BS_LTE_UTRA-Core]",54941,"revised","2017-05-24T17:17:25.917",null,"R4-1705491","R4-1706229","Rel-15","37.843","0.2.0","AASenh_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-1706149","TP for TR 37.843 on testing EMC immunity for OTA AAS BS - measurement setup","Ericsson","Kyoungseok Oh","66120","pCR","Approval","","","364","9.12.2.7","EMC requirements [AASenh_BS_LTE_UTRA-Core]",578301,"revised","2017-05-24T17:17:26.307",null,"R4-1705492","R4-1706230","Rel-15","37.843","0.2.0","AASenh_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-1706150","TP for TR: Consideration of the manufacturer's declarations for Hybrid AAS BS and OTA AAS BS","Huawei","Kyoungseok Oh","66120","other","Discussion","","","366","9.12.3.1","RF conformance requirements [AASenh_BS_LTE_UTRA-Perf]",615000,"approved","2017-05-24T17:17:26.697","2017-05-24T17:17:52.487","","","","","","","","","","","","","","",""]
["R4-1706151","TP to TR 37.843: Additional considerations for the OTA test setups","Huawei","Kyoungseok Oh","66120","pCR","","","","368","9.12.4","Demodulation requirements [AASenh_BS_LTE_UTRA-Perf]",580901,"approved","2017-05-24T17:17:27.043","2017-05-24T17:17:52.487","R4-1705809","","Rel-15","37.843","0.3.0","AASenh_BS_LTE_UTRA-Perf","","","","","","","","",""]
["R4-1706152","TP to TR 37.843: Further details on the definition of core and conformance requirements for BS demodulation requirements","Huawei","Kyoungseok Oh","66120","pCR","","","","368","9.12.4","Demodulation requirements [AASenh_BS_LTE_UTRA-Perf]",581001,"approved","2017-05-24T17:17:27.417","2017-05-24T17:17:52.500","R4-1705810","","Rel-15","37.843","0.3.0","AASenh_BS_LTE_UTRA-Perf","","","","","","","","",""]
["R4-1706153","TP to TR 37.843: Placeholder for the BS performance requirements doable OTA","Huawei","Kyoungseok Oh","66120","pCR","","","","368","9.12.4","Demodulation requirements [AASenh_BS_LTE_UTRA-Perf]",581101,"approved","2017-05-24T17:17:27.777","2017-05-24T17:17:52.500","R4-1705811","","Rel-15","37.843","0.3.0","AASenh_BS_LTE_UTRA-Perf","","","","","","","","",""]
["R4-1706154","CR to TS 37.105: Correction of the spurious emissions requirement","Huawei","Kyoungseok Oh","66120","CR","Agreement","","","24","5.1.2","BS RF (37.105) [AAS_BS_LTE_UTRA-Core]",578601,"agreed","2017-05-24T17:17:28.167","2017-05-24T17:17:52.500","R4-1705786","","Rel-13","37.105","13.4.0","AAS_BS_LTE_UTRA-Core","0059","1","F","RP-171305","","","","",""]
["R4-1706155","CR to TS 37.105: Correction of the spurious emissions requirement","Huawei","Kyoungseok Oh","66120","CR","Agreement","","","24","5.1.2","BS RF (37.105) [AAS_BS_LTE_UTRA-Core]",578701,"agreed","2017-05-24T17:17:29.337","2017-05-24T17:17:52.500","R4-1705787","","Rel-14","37.105","14.0.0","AAS_BS_LTE_UTRA-Core","0060","1","A","RP-171305","","","","",""]
["R4-1706156","UE RF evening adhoc minutes","Qualcomm Inc","Kyoungseok Oh","66120","report","Approval","","","424","10.4.1","UE RF General (ad-hoc MoM, Plan, Spec Structure) [NR_newRAT]",49170,"approved","2017-05-24T17:17:30.660","2017-05-24T17:17:52.517","","","","","","","","","","","","","","",""]
["R4-1706157","WF on the 38.101 specification structure","Qualcomm Incorporated","Kyoungseok Oh","66120","other","Discussion","","","424","10.4.1","UE RF General (ad-hoc MoM, Plan, Spec Structure) [NR_newRAT]",52210,"approved","2017-05-24T17:17:31.050","2017-05-24T17:17:52.517","","","","","","","","","","","","","","",""]
["R4-1706158","WF on new BS requirements","NTT DoCoMo, CMCC","Kyoungseok Oh","66120","other","Discussion","","","436","10.5.1","BS RF General (ad-hoc MoM, Plan, Spec structure) [NR_newRAT]",56560,"approved","2017-05-24T17:17:31.427","2017-05-24T17:17:52.517","","","","","","","","","","","","","","",""]
["R4-1706159","WF on the exclusion of the Tx requirements in Range 2","Ericsson","Kyoungseok Oh","66120","other","Discussion","","","436","10.5.1","BS RF General (ad-hoc MoM, Plan, Spec structure) [NR_newRAT]",615900,"approved","2017-05-24T17:17:31.783","2017-05-24T17:17:52.533","","","","","","","","","","","","","","",""]
["R4-1706160","WF on the exclusion of the Rx requirements in Range 2","Ericsson","Kyoungseok Oh","66120","other","Discussion","","","436","10.5.1","BS RF General (ad-hoc MoM, Plan, Spec structure) [NR_newRAT]",616000,"approved","2017-05-24T17:17:32.157","2017-05-24T17:17:52.533","","","","","","","","","","","","","","",""]
["R4-1706161","TP to TS 38.104 BS classification for NR BS","NEC","Kyoungseok Oh","66120","pCR","Approval","","","437","10.5.2","BS class [NR_newRAT]",53181,"noted","2017-05-24T17:17:32.533","2017-05-24T17:17:52.533","R4-1705318","","Rel-15","38.104","0.0.1","NR_newRAT","","","","","","","","",""]
["R4-1706162","Draft CR for test applicability rule for enhanced SU-MIMO","LG Electronics Inc.","Kyoungseok Oh","66120","draftCR","Endorsement","","","279","7.27.3","SU-MIMO IM [LTE_eCRSIM_eSUMIMO]",55531,"withdrawn","2017-05-24T17:17:33.017",null,"R4-1704955","","Rel-14","36.101","14.3.0","LTE_eCRSIM_eSUMIMO-Perf","","","","","","","","",""]
["R4-1706163","Draft CR for enhanced SU-MIMO performance requirements","Huawei, HiSilicon","Kyoungseok Oh","66120","draftCR","Endorsement","","","279","7.27.3","SU-MIMO IM [LTE_eCRSIM_eSUMIMO]",55541,"withdrawn","2017-05-24T17:17:33.423",null,"R4-1705553","","Rel-14","36.101","14.3.0","LTE_eCRSIM_eSUMIMO","","","B","","","","","",""]
["R4-1706164","Draft CR for enhanced SU-MIMO FRCs","Huawei, HiSilicon","Kyoungseok Oh","66120","draftCR","Endorsement","","","279","7.27.3","SU-MIMO IM [LTE_eCRSIM_eSUMIMO]",56311,"withdrawn","2017-05-24T17:17:33.827",null,"R4-1705554","","Rel-14","36.101","14.3.0","LTE_eCRSIM_eSUMIMO","","","B","","","","","",""]
["R4-1706165","TP for enhanced SU-MIMO IM receiver","Huawei, HiSilicon, Intel Corporation","Kyoungseok Oh","66120","other","Approval","","","279","7.27.3","SU-MIMO IM [LTE_eCRSIM_eSUMIMO]",616801,"approved","2017-05-24T17:17:34.187","2017-05-24T17:17:52.547","R4-1705631","","Rel-14","36.747","","LTE_eCRSIM_eSUMIMO","","","","","","","","",""]
["R4-1706166","Way forward on CRS-IM performance requirements","Intel Corporation, Qualcomm, LGE, CATT","Kyoungseok Oh","66120","other","Discussion","","","276","7.27.2","CRS-IM [LTE_eCRSIM_eSUMIMO]",46320,"approved","2017-05-24T17:17:34.513","2017-05-24T17:17:52.563","","","","","","","","","","","","","","",""]
["R4-1706167","LS on CRS-IM capability and assistance signalling","Qualcomm","Kyoungseok Oh","66120","other","Approval","","","275","7.27.1.1","Capability and signaling [LTE_eCRSIM_eSUMIMO]",616700,"withdrawn","2017-05-24T17:17:34.843",null,"","","","","","","","","","","","","","",""]
["R4-1706168","Way forward on enhanced SU-MIMO receiver performance requirements","Huawei","Kyoungseok Oh","66120","other","Discussion","","","279","7.27.3","SU-MIMO IM [LTE_eCRSIM_eSUMIMO]",46400,"approved","2017-05-24T17:17:35.170","2017-05-24T17:17:52.563","","","","","","","","","","","","","","",""]
["R4-1706169","TX timing requirements for sTTI and reduced processing time","Ericsson","Kyoungseok Oh","66120","CR","Endorsement","","","388","9.13.4.6","Others: PHR, measurement, timing [LTE_sTTIandPT-core]",47921,"endorsed","2017-05-24T17:17:35.467","2017-05-24T17:17:52.580","R4-1704792","","Rel-15","36.133","14.3.0","LTE_sTTIandPT-Core","4866","1","B","","","","","",""]
["R4-1706170","Introduction of test cases for NCSG","Qualcomm Incorporated","Kyoungseok Oh","66120","CR","Agreement","","","272","7.26.3","RRM performance (36.133) [LTE_meas_gap_enh-Perf]",47181,"agreed","2017-05-24T17:17:36.793","2017-05-24T17:17:52.580","R4-1705754","","Rel-14","36.133","14.3.0","LTE_meas_gap_enh-Perf","4998","1","B","RP-171264","","","","",""]
["R4-1706171","Introduction of test cases for burst gap","Qualcomm Incorporated","Kyoungseok Oh","66120","CR","Agreement","","","272","7.26.3","RRM performance (36.133) [LTE_meas_gap_enh-Perf]",47161,"agreed","2017-05-24T17:17:38.413","2017-05-24T17:17:52.597","R4-1705753","","Rel-14","36.133","14.3.0","LTE_meas_gap_enh-Perf","4997","1","B","RP-171264","","","","",""]
["R4-1706172","4DL TDD RSRQ for E-UTRAN in Carrier Aggregation in R13","Huawei, HiSilicon","Kyoungseok Oh","66120","CR","","","Post-meeting note: It was noted before RAN#76 that there is a cover sheet error. So it was revised to R4-1706300","292","7.29.3","RRM [WI code or TEI14]",50311,"revised","2017-05-24T17:17:40.257","2017-05-24T17:17:52.597","R4-1705031","","Rel-13","36.133","13.7.0","TEI14","4912","1","F","","","","","",""]
["R4-1706173","Correction on the test cases of RLM for Cat-M1 UE in R13","Huawei, HiSilicon","Kyoungseok Oh","66120","CR","","","Post-meeting note: It was noted before RAN#76 that there is a cover sheet error. So it was revised to R4-1706301","292","7.29.3","RRM [WI code or TEI14]",50331,"revised","2017-05-24T17:17:41.830","2017-05-24T17:17:52.597","R4-1705033","","Rel-13","36.133","13.7.0","TEI14","4914","1","F","","","","","",""]
["R4-1706174","List of RRM test cases for V2X requirements","Huawei, HiSilicon","Kyoungseok Oh","66120","other","Approval","","","179","7.16.4","RRM performance (36.133) [LTE_V2X-Perf]",49021,"approved","2017-05-24T17:17:43.203","2017-05-24T17:17:52.610","R4-1705038","","","","","","","","","","","","","",""]
["R4-1706175","LS on RSRP range","Huawei","Kyoungseok Oh","66120","LS out","Approval","","","49","5.4.5","RRM performance (36.133) [LTE_MTCe2_L1-Perf]",45160,"approved","2017-05-24T17:17:43.577","2017-05-24T17:17:52.627","","","Rel-13","","","LTE_MTCe2_L1-Core","","","","","","RAN2","","",""]
["R4-1706176","Smmary of alignment and impairment results for IRC TM9 tests for 4Rx CA","Ericsson","Kyoungseok Oh","66120","discussion","Discussion","","","244","7.21.2","UE demodulation (36.101) [LTE_4Rx_AP_DL_CA-Perf]",46311,"noted","2017-05-24T17:17:43.937","2017-05-24T17:17:52.627","R4-1705358","","Rel-14","","","LTE_4Rx_AP_DL_CA-Perf","","","","","","","","",""]
["R4-1706177","CR for further updating IRC tests for 4Rx CA in Rel-14","Ericsson, Qualcomm","Kyoungseok Oh","66120","CR","Agreement","","","244","7.21.2","UE demodulation (36.101) [LTE_4Rx_AP_DL_CA-Perf]",53571,"agreed","2017-05-24T17:17:44.263","2017-05-24T17:17:52.627","R4-1705359","","Rel-14","36.101","14.3.0","LTE_4Rx_AP_DL_CA-Perf","4452","1","B","RP-171268","","","","",""]
["R4-1706178","Summary of alignment and impairment results for 256QAM tests for 4Rx CA","Ericsson","Kyoungseok Oh","66120","discussion","Discussion","","","244","7.21.2","UE demodulation (36.101) [LTE_4Rx_AP_DL_CA-Perf]",53611,"noted","2017-05-24T17:17:45.560","2017-05-24T17:17:52.640","R4-1705364","","Rel-14","","","LTE_4Rx_AP_DL_CA-Perf","","","","","","","","",""]
["R4-1706179","Summary of alignment and impairment results for 3 and 4 layers tests for 4Rx CA","Ericsson","Kyoungseok Oh","66120","discussion","Discussion","","","244","7.21.2","UE demodulation (36.101) [LTE_4Rx_AP_DL_CA-Perf]",53621,"noted","2017-05-24T17:17:45.980","2017-05-24T17:17:52.640","R4-1705365","","Rel-14","","","LTE_4Rx_AP_DL_CA-Perf","","","","","","","","",""]
["R4-1706180","CR for updating applicability rule for SDR CA tests for 4Rx CA in Rel-14","Ericsson","Kyoungseok Oh","66120","CR","Agreement","","","244","7.21.2","UE demodulation (36.101) [LTE_4Rx_AP_DL_CA-Perf]",55571,"agreed","2017-05-24T17:17:46.480","2017-05-24T17:17:52.640","R4-1705357","","Rel-14","36.101","14.3.0","LTE_4Rx_AP_DL_CA-Perf","4451","1","F","RP-171268","","","","",""]
["R4-1706181","CR for adding applicability rule for MU TM9 4Rx tests in Rel-13","Ericsson","Kyoungseok Oh","66120","CR","Agreement","","","32","5.2.3","UE demodulation and CSI (36.101) [LTE_4Rx_AP_DL-Perf]",53551,"agreed","2017-05-24T17:17:47.713","2017-05-24T17:17:52.657","R4-1705355","","Rel-13","36.101","13.7.0","LTE_4Rx_AP_DL-Perf","4449","1","F","RP-171304","","","","",""]
["R4-1706182","Timing requirements for Cat-M2","Ericsson, Qualcomm Incorporated","Kyoungseok Oh","66120","CR","Discussion","","","217","7.18.3.2.5","RLM and timing [LTE_feMTC-Core]",618200,"revised","2017-05-24T17:17:49.007","2017-05-24T17:27:51.437","R4-1704169","","Rel-14","36.133","14.3.0","LTE_feMTC-Core","4701","2","B","","","","","",""]
["R4-1706183","Way forward on SI acquisition time requirements fro non-BL/CE UE","Ericsson","Kyoungseok Oh","66120","other","Discussion","","","219","7.18.4","RRM core for non-BL/CE UE (36.133) [LTE_feMTC-Core]",47040,"approved","2017-05-24T17:17:50.503","2017-05-24T17:27:51.467","","","","","","","","","","","","","","",""]
["R4-1706184","Way forward on non-BL/CE UE RLM evaluation period","Ericsson","Kyoungseok Oh","66120","other","Discussion","","","219","7.18.4","RRM core for non-BL/CE UE (36.133) [LTE_feMTC-Core]",47050,"approved","2017-05-24T17:17:50.847","2017-05-24T17:27:51.467","","","","","","","","","","","","","","",""]
["R4-1706185","Way forward on RSRP and RSRQ requirements for Rel-14 non-BL/CE UE","Ericsson, Intel","Kyoungseok Oh","66120","other","Discussion","","","224","7.18.6","RRM performance for non-BL/CE UE (36.133) [LTE_feMTC-Perf]",54560,"approved","2017-05-24T17:17:51.190","2017-05-24T17:27:51.467","","","","","","","","","","","","","","",""]
["R4-1706186","Introduction of BS performance requirements for 256QAM in 36.104","Ericsson","Kyoungseok Oh","66120","CR","Agreement","","","150","7.12.3","Demodulation (36.104/36.141) [LTE_UL_CAP_enh-Core/Perf]",595901,"agreed","2017-05-24T17:17:51.517","2017-05-24T17:27:51.483","R4-1705303","","Rel-14","36.104","14.3.0","LTE_UL_CAP_enh-Perf","4676","1","B","RP-171260","","","","",""]
["R4-1706187","Introduction of BS performance requirements for 256QAM in 36.141","Ericsson","Kyoungseok Oh","66120","CR","Agreement","","","150","7.12.3","Demodulation (36.104/36.141) [LTE_UL_CAP_enh-Core/Perf]",600601,"agreed","2017-05-24T17:17:52.673","2017-05-24T17:27:51.483","R4-1705304","","Rel-14","36.141","14.3.0","LTE_UL_CAP_enh-Perf","1038","1","B","RP-171260","","","","",""]
["R4-1706188","Corrections for inCoverage configuration in ProSe direct communication (Rel-12)","Huawei, HiSilicon","Kyoungseok Oh","66120","CR","Agreement","","","16","4.2.4","UE demodulation performance [WI code or TEI12]",55622,"agreed","2017-05-24T17:17:53.907","2017-05-24T17:27:51.497","R4-1706020","","Rel-12","36.101","12.15.0","TEI12","4471","2","F","RP-171297","","","","",""]
["R4-1706189","Introduction of enhanced RLM requirements for feMTC","Ericsson","Kyoungseok Oh","66120","CR","Agreement","","","217","7.18.3.2.5","RLM and timing [LTE_feMTC-Core]",50811,"agreed","2017-05-24T17:17:55.123","2017-05-24T17:27:51.497","R4-1705079","","Rel-14","36.133","14.3.0","LTE_feMTC-Core","4942","1","B","RP-171266","","","","",""]
["R4-1706190","PHR reporting for NB-IOT low-power class UEs","Ericsson, Intel Corporation","Kyoungseok Oh","66120","CR","Agreement","","","195","7.17.3.2.3","PHR [NB_IOTenh-Core]",50871,"agreed","2017-05-24T17:17:56.260","2017-05-24T17:27:51.513","R4-1705087","","Rel-14","36.133","14.3.0","NB_IOTenh-Core","4695","3","F","RP-171267","","","","",""]
["R4-1706191","CONNECTED mode requirements for feMTC UEs in CEModeA","Ericsson","Kyoungseok Oh","66120","CR","Approval","","","216","7.18.3.2.4","Gap sharing and measurement [LTE_feMTC-Core]",50751,"revised","2017-05-24T17:17:57.523","2017-05-24T17:27:51.513","R4-1705075","R4-1706281","Rel-14","36.133","14.3.0","LTE_feMTC-Core","4938","1","B","","","","","",""]
["R4-1706192","CONNECTED mode requirements for feMTC UEs in CEModeB","Ericsson","Kyoungseok Oh","66120","CR","Approval","","","216","7.18.3.2.4","Gap sharing and measurement [LTE_feMTC-Core]",50761,"revised","2017-05-24T17:17:58.727","2017-05-24T17:27:51.513","R4-1705076","R4-1706282","Rel-14","36.133","14.3.0","LTE_feMTC-Core","4939","1","B","","","","","",""]
["R4-1706193","CR for correction of 4RX demodulation requirements (Rel-13)","Samsung","Kyoungseok Oh","66120","CR","Agreement","","","32","5.2.3","UE demodulation and CSI (36.101) [LTE_4Rx_AP_DL-Perf]",47561,"agreed","2017-05-24T17:17:59.910","2017-05-24T17:27:51.530","R4-1704756","","Rel-13","36.101","13.7.0","LTE_4Rx_AP_DL-Perf","4413","1","F","RP-171304","","","","",""]
["R4-1706194","Way forward on eFD-MIMO performance requirements","Samsung","Kyoungseok Oh","66120","other","Discussion","","","282","7.28.2","UE Demodualtion/CSI (36.101) [LTE_eFDMIMO-Perf]",619400,"approved","2017-05-24T17:18:01.127","2017-05-24T17:27:51.530","","","","","","","","","","","","","","",""]
["R4-1706195","Simulation assumptions for V2X demodulation test cases","Huawei, HiSilicon","Kyoungseok Oh","66120","other","Discussion","","","180","7.16.5","UE demodulation (36.101) [LTE_V2X-Perf]",619500,"agreed","2017-05-24T17:18:01.440","2017-05-24T17:27:51.530","","","","","","","","","","","","","","",""]
["R4-1706196","Way forward on non-BL/CE UE performance requirements","Huawei, HiSilicon, Ericsson, Intel Corporation, Qualcomm","Kyoungseok Oh","66120","other","Discussion","","","228","7.18.8.2","Non-BL/CE UE [LTE_feMTC-Perf]",46220,"approved","2017-05-24T17:18:01.753","2017-05-24T17:27:51.547","","","","","","","","","","","","","","",""]
["R4-1706197","Timing advance requirements for Cat M1 UEs","Ericsson","Kyoungseok Oh","66120","CR","Agreement","","","45","5.4.3","RRM Core (36.133) [LTE_MTCe2_L1-Core]",50771,"agreed","2017-05-24T17:18:02.080","2017-05-24T17:27:51.560","R4-1705077","","Rel-13","36.133","13.7.0","LTE_MTCe2_L1-Core","4940","1","F","RP-171308","","","","",""]
["R4-1706198","CR for introducing applicability rule for 256QAM and higher layer tests for 4Rx CA","Ericsson","Kyoungseok Oh","66120","CR","Agreement","","","244","7.21.2","UE demodulation (36.101) [LTE_4Rx_AP_DL_CA-Perf]",53641,"agreed","2017-05-24T17:18:03.313","2017-05-24T17:27:51.560","R4-1705361","","Rel-14","36.101","14.3.0","LTE_4Rx_AP_DL_CA-Perf","4453","1","B","RP-171268","","","","",""]
["R4-1706199","CR for introducing 256QAM tests for 4Rx CA in Rel-14","Ericsson","Kyoungseok Oh","66120","CR","Agreement","","","244","7.21.2","UE demodulation (36.101) [LTE_4Rx_AP_DL_CA-Perf]",53651,"agreed","2017-05-24T17:18:04.607","2017-05-24T17:27:51.560","R4-1705362","","Rel-14","36.101","14.3.0","LTE_4Rx_AP_DL_CA-Perf","4454","1","B","RP-171268","","","","",""]
["R4-1706200","CR for introducing high layers tests for 4Rx CA in Rel-14","Ericsson, Qualcomm","Kyoungseok Oh","66120","CR","Agreement","","","244","7.21.2","UE demodulation (36.101) [LTE_4Rx_AP_DL_CA-Perf]",53661,"agreed","2017-05-24T17:18:05.900","2017-05-24T17:27:51.577","R4-1705363","","Rel-14","36.101","14.3.0","LTE_4Rx_AP_DL_CA-Perf","4455","1","B","RP-171268","","","","",""]
["R4-1706201","Summary of discussion on UE capabilities related to MIMO layer","Ericsson","Kyoungseok Oh","66120","other","Discussion","","","293","7.29.4","Demodulation [WI code or TEI14]",53510,"noted","2017-05-24T17:18:07.167","2017-05-24T17:27:51.577","","","","","","","","","","","","","","",""]
["R4-1706202","Correction to minimum requirement for CatM1 Single-Layer Spatial Multiplexing","Anritsu, Rohde & Schwarz","Kyoungseok Oh","66120","CR","Agreement","","","53","5.4.6.1","BL/CE UE [LTE_MTCe2_L1-Perf]",45871,"agreed","2017-05-24T17:18:07.557","2017-05-24T17:27:51.593","R4-1705987","","Rel-13","36.101","13.7.0","LTE_MTCe2_L1-Perf","4384","2","F","RP-171310","","","","",""]
["R4-1706203","Correction on UE transmit timing test for NB-IoT R13","Huawei, HiSilicon","Kyoungseok Oh","66120","CR","Agreement","","","62","5.5.5","RRM Performance (36.133) [NB_IOT-Perf]",50721,"revised","2017-05-24T17:18:09.020","2017-05-24T17:27:51.593","R4-1704975","R4-1706274","Rel-13","36.133","13.7.0","NB_IOT-Perf","4876","1","F","","","","","",""]
["R4-1706204","Way forward on eMTC subband CQI test","Ericsson, Anritsu, Qualcomm","Kyoungseok Oh","66120","other","Discussion","","","53","5.4.6.1","BL/CE UE [LTE_MTCe2_L1-Perf]",45830,"noted","2017-05-24T17:18:10.410","2017-05-24T17:27:51.593","","","","","","","","","","","","","","",""]
["R4-1706205","Introduce test case for eLAA PUSCH","Ericsson","Kyoungseok Oh","66120","CR","Approval","","","166","7.14.7","BS demodulation (36.104/36.141) [LTE_eLAA-Perf]",56261,"noted","2017-05-24T17:18:10.723","2017-05-24T17:27:51.607","R4-1705627","","Rel-14","36.104","14.3.0","LTE_eLAA-Perf","4687","1","B","","","","","",""]
["R4-1706206","CR for V2V FRCs","Huawei, HiSilicon","Kyoungseok Oh","66120","CR","Agreement","","","171","7.15.4","UE demodulation (36.101) [LTE_SL_V2V-Perf]",601901,"agreed","2017-05-24T17:18:11.907","2017-05-24T17:27:51.607","R4-1705546","","Rel-14","36.101","14.3.0","LTE_SL_V2V-Perf","4469","1","B","RP-171256","","","","",""]
["R4-1706207","Correction to RSTD test cases for carrier aggregation (R12)","Qualcomm Incorporated","Kyoungseok Oh","66120","CR","Agreement","","","15","4.2.3","RRM (Radio Resource Management) [WI code or TEI12]",51341,"agreed","2017-05-24T17:18:13.123","2017-05-24T17:27:51.623","R4-1705134","","Rel-12","36.133","12.15.0","TEI12","4957","1","F","RP-171297","","","","",""]
["R4-1706208","Correction to RSTD test cases for carrier aggregation (R13)","Qualcomm Incorporated","Kyoungseok Oh","66120","CR","Agreement","","","15","4.2.3","RRM (Radio Resource Management) [WI code or TEI12]",51351,"agreed","2017-05-24T17:18:14.387","2017-05-24T17:27:51.623","R4-1705135","","Rel-13","36.133","13.7.0","TEI12","4958","1","A","RP-171297","","","","",""]
["R4-1706209","Correction to RSTD test cases for carrier aggregation (R14)","Qualcomm Incorporated","Kyoungseok Oh","66120","CR","Agreement","","","15","4.2.3","RRM (Radio Resource Management) [WI code or TEI12]",51361,"agreed","2017-05-24T17:18:15.683","2017-05-24T17:27:51.637","R4-1705136","","Rel-14","36.133","14.3.0","TEI12","4959","1","A","RP-171297","","","","",""]
["R4-1706210","Correction of test points for Single-antenna port performance TDD FDD CA","Rohde & Schwarz","Kyoungseok Oh","66120","CR","Agreement","","","70","5.6.3","Demodulation and CSI [WI code or TEI13]",48731,"agreed","2017-05-24T17:18:16.883","2017-05-24T17:27:51.637","R4-1704873","","Rel-13","36.101","13.7.0","TEI13","4423","1","F","RP-171311","","","","",""]
["R4-1706211","Introduction of additional gap patterns and measurement capabilities for measurement gap enhancement","Ericsson, Nokia, Huawei","Kyoungseok Oh","66120","CR","Agreement","","","270","7.26.2.1","Gap pattern, signaling and capability (RAN2 related) [LTE_meas_gap_enh-Core]",51151,"agreed","2017-05-24T17:18:18.117","2017-05-24T17:27:51.637","R4-1704769","","Rel-14","36.133","14.3.0","LTE_meas_gap_enh-Core","4864","1","B","RP-171264","","","","",""]
["R4-1706212","Way forward on FeMTC UE demodulation requirements","Ericsson","Kyoungseok Oh","66120","other","Discussion","","","227","7.18.8.1","BL/CE UE [LTE_feMTC-Perf]",46230,"approved","2017-05-24T17:18:19.410","2017-05-24T17:27:51.653","","","","","","","","","","","","","","",""]
["R4-1706213","Way forward on demodulation performance for V2X UE","CATT","Kyoungseok Oh","66120","other","Discussion","","","180","7.16.5","UE demodulation (36.101) [LTE_V2X-Perf]",621300,"approved","2017-05-24T17:18:19.770","2017-05-24T17:27:51.653","","","","","","","","","","","","","","",""]
["R4-1706214","Requirements applicability for eLAA","Ericsson","Kyoungseok Oh","66120","CR","Agreement","","","164","7.14.5","RRM core Maintenance (36.133) [LTE_eLAA-Core]",55971,"agreed","2017-05-24T17:18:20.083","2017-05-24T17:27:51.653","R4-1705597","","Rel-14","36.133","14.3.0","LTE_eLAA-Core","4982","1","F","RP-171285","","","","",""]
["R4-1706215","Clarification on requirements for new PRS configurations","Ericsson","Kyoungseok Oh","66120","CR","Approval","","","249","7.23.1","RRM core maintenance (36.133) [UTRA_LTE_iPos_enh2-Core]",55931,"withdrawn","2017-05-24T17:18:21.313",null,"R4-1705593","","Rel-14","36.133","14.3.0","UTRA_LTE_iPos_enh2-Core","4980","1","F","","","","","",""]
["R4-1706216","LS response on timing reference for FS3 SCell","Ericsson","Kyoungseok Oh","66120","LS out","Approval","","","164","7.14.5","RRM core Maintenance (36.133) [LTE_eLAA-Core]",55961,"noted","2017-05-24T17:18:22.563","2017-05-24T17:27:51.670","R4-1705595","","Rel-14","","","LTE_eLAA-Core","","","","","R2-165965","RAN WG2","RAN WG1","R2-165965",""]
["R4-1706217","RRM requirements with eMBMS enhancements","Ericsson","Kyoungseok Oh","66120","CR","Approval","","","155","7.13.3","RRM core (36.133) [MBMS_LTE_enh2-Core]",574401,"revised","2017-05-24T17:18:22.953","2017-05-24T17:27:51.670","R4-1705601","R4-1706279","Rel-14","36.133","14.3.0","MBMS_LTE_enh2-Core","4985","1","B","","","","","",""]
["R4-1706218","Way forward on FeMTC positioning","Ericsson","Kyoungseok Oh","66120","other","Discussion","","","209","7.18.3.1","Positioning [LTE_feMTC-Core]",621800,"approved","2017-05-24T17:18:24.200","2017-05-24T17:27:51.670","","","","","","","","","","","","","","",""]
["R4-1706219","Ad hoc minutes for eNB-IOT and NB-IOT RRM","Huawei","Kyoungseok Oh","66120","other","Discussion","","","188","7.17.3","RRM core (36.133) [NB_IOTenh-Core]",54580,"approved","2017-05-24T17:18:24.527","2017-05-24T17:27:51.670","","","","","","","","","","","","","","",""]
["R4-1706220","Ad hoc minutes for FeMTC/eMTC RRM and demodulation performance","Ericsson","Kyoungseok Oh","66120","report","Approval","","","208","7.18.3","RRM core for BL/CE UE (36.133) [LTE_feMTC-Core]",54570,"approved","2017-05-24T17:18:24.840","2017-05-24T17:27:51.687","","","","","","","","","","","","","","",""]
["R4-1706221","Ad hoc minutes for V2V/V2X RRM and demodulation performance","Huawei","Kyoungseok Oh","66120","report","Approval","","","178","7.16.3","RRM core Maintenance (36.133) [LTE_V2X-Core]",49040,"approved","2017-05-24T17:18:25.183","2017-05-24T17:27:51.687","","","","","","","","","","","","","","",""]
["R4-1706222","WF on NR BS mmWave unwanted emission","Nokia","Kyoungseok Oh","66120","other","Discussion","","","440","10.5.3.2","Unwanted emission requirements [NR_newRAT]",46170,"approved","2017-05-24T17:18:25.510","2017-05-24T17:27:51.687","","","","","","","","","","","","","","",""]
["R4-1706223","WF on BS spectrum emission mask for below 6GHz","ZTE,Huawei,Nokia,Ericsson","Kyoungseok Oh","66120","other","Discussion","","","440","10.5.3.2","Unwanted emission requirements [NR_newRAT]",56650,"approved","2017-05-24T17:18:25.837","2017-05-24T17:27:51.700","","","","","","","","","","","","","","",""]
["R4-1706224","WF on Muti-node test","Qualcomm, Ericsson, Huawei, HiSilicon, Nokia, Alcatel-Lucent, Shanghai Bell, Verizon, AT&T, US Cellular, Vodafone, Orange, Skyworks, Samsung, T-Mobile USA, MediaTek, Broadcom, Blackberry, CableLabs, Brocade, Blackberry","Kyoungseok Oh","66120","other","Discussion","","","82","6.1.1","General [FS_LTE_LAA_multinode_test]",50890,"approved","2017-05-24T17:18:26.150","2017-05-24T17:27:51.700","","","","","","","","","","","","","","",""]
["R4-1706225","TP for TR 36.789","Qualcomm, Ericsson, Huawei, HiSilicon, Nokia, Alcatel-Lucent, Shanghai Bell, Verizon, AT&T, US Cellular, Vodafone, Orange, Skyworks, Samsung, T-Mobile USA, MediaTek, Broadcom, Blackberry, CableLabs, Brocade, Blackberry","Kyoungseok Oh","66120","other","Discussion","","","82","6.1.1","General [FS_LTE_LAA_multinode_test]",50900,"approved","2017-05-24T17:18:26.477","2017-05-24T17:27:51.700","","","","","","","","","","","","","","",""]
["R4-1706226","Reply LS on the feasibility of DC-related mobility enhancements in NR","Huawei, HiSilicon","Kyoungseok Oh","66120","LS out","Approval","","","411","10.1.2","Topics related to incoming LS from other WG [NR_newRAT]",52431,"noted","2017-05-24T17:18:26.820","2017-05-24T17:27:51.717","R4-1704991","","","","","NR_newRAT","","","","","R2-1703971","RAN2","RAN1","",""]
["R4-1706227","NR BS RF Ad hoc meeting minutes","Ericsson","Kyoungseok Oh","66120","report","Approval","","","436","10.5.1","BS RF General (ad-hoc MoM, Plan, Spec structure) [NR_newRAT]",45400,"approved","2017-05-24T17:18:27.197","2017-05-24T17:27:51.717","","","","","","","","","","","","","","",""]
["R4-1706228","TS 38.104 v0.0.2 NR Base Station (BS) radio transmission and reception (Skeleton)","Ericsson","Kyoungseok Oh","66120","draft TS","Approval","","","436","10.5.1","BS RF General (ad-hoc MoM, Plan, Spec structure) [NR_newRAT]",0,"approved","2017-05-24T17:18:27.523","2017-05-24T17:27:51.717","R4-1705332","","Rel-15","38.104","0.0.3","NR_newRAT","","","","","","","","",""]
["R4-1706229","TP for TR 37.843 on testing EMC immunity for OTA AAS BS - general section","Ericsson","Kyoungseok Oh","66120","pCR","Approval","","","364","9.12.2.7","EMC requirements [AASenh_BS_LTE_UTRA-Core]",54942,"approved","2017-05-24T17:18:29.193","2017-05-24T17:27:51.733","R4-1706148","","Rel-15","37.843","0.2.0","AASenh_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-1706230","TP for TR 37.843 on testing EMC immunity for OTA AAS BS - measurement setup","Ericsson","Kyoungseok Oh","66120","pCR","Approval","","","364","9.12.2.7","EMC requirements [AASenh_BS_LTE_UTRA-Core]",578302,"approved","2017-05-24T17:18:29.613","2017-05-24T17:27:51.733","R4-1706149","","Rel-15","37.843","0.2.0","AASenh_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-1706231","[Draft] Introduction of TDD L band into TS 36.104","Huawei, Hisilicon, Etisalat","Kyoungseok Oh","66120","draftCR","","","","329","9.6.3","BS RF (36.104, 36.141) [LTE_TDD_L_Band-core/Perf]",56172,"endorsed","2017-05-24T17:18:30.020","2017-05-24T17:27:51.747","R4-1706120","","Rel-15","36.104","14.3.0","LTE_TDD_L_Band-Core","","","","","","","","",""]
["R4-1706232","Void","Void","Kyoungseok Oh","66120","other","Discussion","","","86","7","Rel-14 Work Items",623200,"reserved","2017-05-24T17:18:30.363",null,"","","","","","","","","","","","","","",""]
["R4-1706233","Void","Void","Kyoungseok Oh","66120","other","Discussion","","","86","7","Rel-14 Work Items",623300,"reserved","2017-05-24T17:18:30.690",null,"","","","","","","","","","","","","","",""]
["R4-1706234","Void","Void","Kyoungseok Oh","66120","other","Discussion","","","86","7","Rel-14 Work Items",623400,"reserved","2017-05-24T17:18:31.033",null,"","","","","","","","","","","","","","",""]
["R4-1706235","Void","Void","Kyoungseok Oh","66120","other","Discussion","","","86","7","Rel-14 Work Items",623500,"reserved","2017-05-24T17:18:31.360",null,"","","","","","","","","","","","","","",""]
["R4-1706236","Void","Void","Kyoungseok Oh","66120","other","Discussion","","","86","7","Rel-14 Work Items",623600,"reserved","2017-05-24T17:18:31.703",null,"","","","","","","","","","","","","","",""]
["R4-1706237","Void","Void","Kyoungseok Oh","66120","other","Discussion","","","86","7","Rel-14 Work Items",623700,"reserved","2017-05-24T17:18:32.033",null,"","","","","","","","","","","","","","",""]
["R4-1706238","Void","Void","Kyoungseok Oh","66120","other","Discussion","","","86","7","Rel-14 Work Items",623800,"reserved","2017-05-24T17:18:32.343",null,"","","","","","","","","","","","","","",""]
["R4-1706239","Void","Void","Kyoungseok Oh","66120","other","Discussion","","","86","7","Rel-14 Work Items",623900,"reserved","2017-05-24T17:18:32.687",null,"","","","","","","","","","","","","","",""]
["R4-1706240","Void","Void","Kyoungseok Oh","66120","other","Discussion","","","86","7","Rel-14 Work Items",624000,"reserved","2017-05-24T17:18:33.013",null,"","","","","","","","","","","","","","",""]
["R4-1706241","Void","Void","Kyoungseok Oh","66120","other","Discussion","","","86","7","Rel-14 Work Items",624100,"reserved","2017-05-24T17:18:33.327",null,"","","","","","","","","","","","","","",""]
["R4-1706242","Void","Void","Kyoungseok Oh","66120","other","Discussion","","","86","7","Rel-14 Work Items",624200,"reserved","2017-05-24T17:18:33.653",null,"","","","","","","","","","","","","","",""]
["R4-1706243","Void","Void","Kyoungseok Oh","66120","other","Discussion","","","86","7","Rel-14 Work Items",624300,"reserved","2017-05-24T17:18:33.983",null,"","","","","","","","","","","","","","",""]
["R4-1706244","Void","Void","Kyoungseok Oh","66120","other","Discussion","","","86","7","Rel-14 Work Items",624400,"reserved","2017-05-24T17:18:34.310",null,"","","","","","","","","","","","","","",""]
["R4-1706245","Void","Void","Kyoungseok Oh","66120","other","Discussion","","","86","7","Rel-14 Work Items",624500,"reserved","2017-05-24T17:18:34.653",null,"","","","","","","","","","","","","","",""]
["R4-1706246","Void","Void","Kyoungseok Oh","66120","other","Discussion","","","86","7","Rel-14 Work Items",624600,"reserved","2017-05-24T17:18:34.963",null,"","","","","","","","","","","","","","",""]
["R4-1706247","Void","Void","Kyoungseok Oh","66120","other","Discussion","","","86","7","Rel-14 Work Items",624700,"reserved","2017-05-24T17:18:35.293",null,"","","","","","","","","","","","","","",""]
["R4-1706248","Void","Void","Kyoungseok Oh","66120","other","Discussion","","","86","7","Rel-14 Work Items",624800,"reserved","2017-05-24T17:18:35.620",null,"","","","","","","","","","","","","","",""]
["R4-1706249","Void","Void","Kyoungseok Oh","66120","other","Discussion","","","86","7","Rel-14 Work Items",624900,"reserved","2017-05-24T17:18:35.963",null,"","","","","","","","","","","","","","",""]
["R4-1706250","Void","Void","Kyoungseok Oh","66120","other","Discussion","","","86","7","Rel-14 Work Items",625000,"reserved","2017-05-24T17:18:36.307",null,"","","","","","","","","","","","","","",""]
["R4-1706251","Void","Void","Kyoungseok Oh","66120","other","Discussion","","","86","7","Rel-14 Work Items",625100,"reserved","2017-05-24T17:18:36.650",null,"","","","","","","","","","","","","","",""]
["R4-1706252","Void","Void","Kyoungseok Oh","66120","other","Discussion","","","86","7","Rel-14 Work Items",625200,"reserved","2017-05-24T17:18:36.977",null,"","","","","","","","","","","","","","",""]
["R4-1706253","Void","Void","Kyoungseok Oh","66120","other","Discussion","","","86","7","Rel-14 Work Items",625300,"reserved","2017-05-24T17:18:37.303",null,"","","","","","","","","","","","","","",""]
["R4-1706254","Void","Void","Kyoungseok Oh","66120","other","Discussion","","","86","7","Rel-14 Work Items",625400,"reserved","2017-05-24T17:18:37.617",null,"","","","","","","","","","","","","","",""]
["R4-1706255","Void","Void","Kyoungseok Oh","66120","other","Discussion","","","86","7","Rel-14 Work Items",625500,"reserved","2017-05-24T17:18:37.943",null,"","","","","","","","","","","","","","",""]
["R4-1706256","Void","Void","Kyoungseok Oh","66120","other","Discussion","","","86","7","Rel-14 Work Items",625600,"reserved","2017-05-24T17:18:38.273",null,"","","","","","","","","","","","","","",""]
["R4-1706257","Void","Void","Kyoungseok Oh","66120","other","Discussion","","","86","7","Rel-14 Work Items",625700,"reserved","2017-05-24T17:18:38.617",null,"","","","","","","","","","","","","","",""]
["R4-1706258","Void","Void","Kyoungseok Oh","66120","other","Discussion","","","86","7","Rel-14 Work Items",625800,"reserved","2017-05-24T17:18:38.943",null,"","","","","","","","","","","","","","",""]
["R4-1706259","Void","Void","Kyoungseok Oh","66120","other","Discussion","","","86","7","Rel-14 Work Items",625900,"reserved","2017-05-24T17:18:39.287",null,"","","","","","","","","","","","","","",""]
["R4-1706260","Void","Void","Kyoungseok Oh","66120","other","Discussion","","","86","7","Rel-14 Work Items",626000,"reserved","2017-05-24T17:18:39.597",null,"","","","","","","","","","","","","","",""]
["R4-1706261","Way forward on NB-IOT RLM test cases","Intel","Kyoungseok Oh","66120","other","Discussion","","","60","5.5.3","RRM core (36.133) [NB_IOT-Core]",46730,"approved","2017-05-24T17:18:39.927","2017-05-24T17:27:51.873","","","","","","","","","","","","","","",""]
["R4-1706262","LS on system information and measurement signalling on FeMBMS carrier","Qualcomm Incorporated","Kyoungseok Oh","66120","LS out","","","","155","7.13.3","RRM core (36.133) [MBMS_LTE_enh2-Core]",572401,"noted","2017-05-24T17:18:40.267","2017-05-24T17:27:51.873","R4-1705750","","Rel-14","","","MBMS_LTE_enh2-Core","","","","","","RAN2","","",""]
["R4-1706263","Way forward on eMTC BS PRACH performance test","Nokia, Alcatel-Lucent Shanghai Bell, Huawei","Kyoungseok Oh","66120","other","Discussion","","","55","5.4.7","BS performance (36.104/36.141) [LTE_MTCe2_L1-Perf]",48160,"approved","2017-05-24T17:18:40.627","2017-05-24T17:27:51.887","","","","","","","","","","","","","","",""]
["R4-1706264","Applicability of requirements for UE Cat.NB2","Huawei, HiSilicon","Kyoungseok Oh","66120","CR","Agreement","","","197","7.17.3.2.5","Others [NB_IOTenh-Core]",49851,"agreed","2017-05-24T17:18:40.957","2017-05-24T17:27:51.887","R4-1705470","","Rel-14","36.133","14.3.0","NB_IOTenh-Core","4761","3","B","RP-171267","","","","",""]
["R4-1706265","CR on intra frequency RSTD accuracy requirement for eNB-IOT","Huawei, HiSilicon","Kyoungseok Oh","66120","CR","Agreement","","","199","7.17.4.1","Positioning [NB_IOTenh-Perf]",49971,"agreed","2017-05-24T17:18:42.313","2017-05-24T17:27:51.887","R4-1704997","","Rel-14","36.133","14.3.0","NB_IOTenh-Perf","4891","1","B","RP-171267","","","","",""]
["R4-1706266","CR on intra frequency RSTD accuracy requirement for FeMTC","Huawei, HiSilicon","Kyoungseok Oh","66120","CR","","","","221","7.18.5.1","Positioning [LTE_feMTC-Perf]",50021,"withdrawn","2017-05-24T17:18:43.637",null,"R4-1705002","","Rel-14","36.133","14.3.0","LTE_feMTC-Perf","4895","1","B","","","","","",""]
["R4-1706267","CR on applicability rule for FeMTC in R14","Huawei, HiSilicon","Kyoungseok Oh","66120","CR","Agreement","","","223","7.18.5.3","Applicability of requirements and test cases [LTE_feMTC-Perf]",50231,"agreed","2017-05-24T17:18:45.073","2017-05-24T17:27:51.903","R4-1705024","","Rel-14","36.133","14.3.0","LTE_feMTC-Perf","4906","1","B","RP-171266","","","","",""]
["R4-1706268","Simulation assumption for eFD-MIMO performance","Samsung","Kyoungseok Oh","66120","other","Discussion","","","281","7.28.1","General [LTE_eFDMIMO-Perf]",46470,"noted","2017-05-24T17:18:46.367","2017-05-24T17:27:51.920","","","","","","","","","","","","","","",""]
["R4-1706269","InDoPos: New WLAN delay test case in nominal conditions with LTE FDD and TDD (Rel-14)","Rohde & Schwarz","Kyoungseok Oh","66120","CR","Agreement","","","252","7.23.2.2","RAT-independent enhancement [UTRA_LTE_iPos_enh2-Perf]",50062,"agreed","2017-05-24T17:18:46.790","2017-05-24T17:27:51.920","R4-1706027","","Rel-14","37.171","14.1.0","UTRA_LTE_iPos_enh2-Perf","0013","2","F","RP-171270","","","","",""]
["R4-1706270","Draft LS on Rel-14 RAN4 UE feature list","Intel Corporation","Kyoungseok Oh","66120","LS out","Approval","","","289","7.29","TEI14",56581,"noted","2017-05-24T17:18:48.053","2017-05-24T17:27:51.937","R4-1705658","","Rel-14","","","","","","","","","RAN2","RAN, RAN1","",""]
["R4-1706271","LS on Maximum Transmission Timing Difference and Maximum Receive Timing Difference in CA for sTTI","Intel Corporation","Kyoungseok Oh","66120","LS out","Approval","","","385","9.13.4.3","Maximum reception/transmission timing difference [LTE_sTTIandPT-core]",46941,"approved","2017-05-24T17:18:48.457","2017-05-24T17:27:51.937","R4-1704694","","Rel-15","","","LTE_sTTIandPT-Core","","","","","","RAN1","","",""]
["R4-1706272","CR on test case for Bluetooth identification","Huawei, HiSilicon","Kyoungseok Oh","66120","CR","Agreement","","","252","7.23.2.2","RAT-independent enhancement [UTRA_LTE_iPos_enh2-Perf]",45192,"revised","2017-05-24T17:18:48.863","2017-05-24T17:27:51.950","R4-1706026","R4-1706275","Rel-14","37.171","14.1.0","UTRA_LTE_iPos_enh2-Perf","0016","2","B","","","","","",""]
["R4-1706273","Introducing gapless measurement requirement for eMTC R14","Nokia, Alcatel-Lucent Shanghai Bell","Kyoungseok Oh","66120","CR","Agreement","","","46","5.4.3.1","BL/CE UE [LTE_MTCe2_L1-Core]",50131,"agreed","2017-05-24T17:18:50.253","2017-05-24T17:27:51.950","R4-1705715","","Rel-14","36.133","14.3.0","LTE_feMTC-Core","4990","1","F","RP-171266","","","","",""]
["R4-1706274","Correction on UE transmit timing test for NB-IoT R13","Huawei, HiSilicon","Kyoungseok Oh","66120","CR","Agreement","","","62","5.5.5","RRM Performance (36.133) [NB_IOT-Perf]",50722,"agreed","2017-05-24T17:18:51.563","2017-05-24T17:27:51.967","R4-1706203","","Rel-13","36.133","13.7.0","NB_IOT-Perf","4876","2","F","RP-171302","","","","",""]
["R4-1706275","CR on test case for Bluetooth identification","Huawei, HiSilicon","Kyoungseok Oh","66120","CR","Agreement","","","252","7.23.2.2","RAT-independent enhancement [UTRA_LTE_iPos_enh2-Perf]",45193,"revised","2017-05-24T17:18:52.937","2017-05-24T17:27:51.967","R4-1706272","","Rel-14","37.171","14.1.0","UTRA_LTE_iPos_enh2-Perf","0016","3","B","","","","","",""]
["R4-1706276","CR on inter frequency RSTD accuracy requirement for eNB-IOT","Huawei, HiSilicon","Kyoungseok Oh","66120","CR","Agreement","","","199","7.17.4.1","Positioning [NB_IOTenh-Perf]",49981,"agreed","2017-05-24T17:18:54.323","2017-05-24T17:27:51.967","R4-1704998","","Rel-14","36.133","14.3.0","NB_IOTenh-Perf","4892","1","B","RP-171267","","","","",""]
["R4-1706277","CR on inter frequency RSTD measurement requirement for FeMTC","Huawei, HiSilicon","Kyoungseok Oh","66120","CR","Agreement","","","211","7.18.3.1.2","OTDOA [LTE_feMTC-Core]",56051,"agreed","2017-05-24T17:18:55.540","2017-05-24T17:27:51.983","R4-1705001","","Rel-14","36.133","14.3.0","LTE_feMTC-Core","4894","1","B","RP-171266","","","","",""]
["R4-1706278","CR on inter frequency RSTD accuracy requirement for FeMTC","Huawei, HiSilicon","Kyoungseok Oh","66120","CR","","","","221","7.18.5.1","Positioning [LTE_feMTC-Perf]",50031,"withdrawn","2017-05-24T17:18:56.867",null,"R4-1705003","","Rel-14","36.133","14.3.0","LTE_feMTC-Perf","4896","1","B","","","","","",""]
["R4-1706279","RRM requirements with eMBMS enhancements","Ericsson","Kyoungseok Oh","66120","CR","Approval","","","155","7.13.3","RRM core (36.133) [MBMS_LTE_enh2-Core]",574402,"revised","2017-05-24T17:18:58.317","2017-05-24T17:27:51.983","R4-1706217","R4-1706280","Rel-14","36.133","14.3.0","MBMS_LTE_enh2-Core","4985","2","B","","","","","",""]
["R4-1706280","RRM requirements with eMBMS enhancements","Ericsson","Kyoungseok Oh","66120","CR","Approval","","","155","7.13.3","RRM core (36.133) [MBMS_LTE_enh2-Core]",574403,"revised","2017-05-24T17:18:59.660","2017-05-24T17:27:51.997","R4-1706279","","Rel-14","36.133","14.3.0","MBMS_LTE_enh2-Core","4985","3","B","","","","","",""]
["R4-1706281","CONNECTED mode requirements for feMTC UEs in CEModeA","Ericsson","Kyoungseok Oh","66120","CR","Approval","","","216","7.18.3.2.4","Gap sharing and measurement [LTE_feMTC-Core]",50752,"revised","2017-05-24T17:19:00.877","2017-05-24T17:27:51.997","R4-1706191","","Rel-14","36.133","14.3.0","LTE_feMTC-Core","4938","2","B","","","","","",""]
["R4-1706282","CONNECTED mode requirements for feMTC UEs in CEModeB","Ericsson","Kyoungseok Oh","66120","CR","Approval","","","216","7.18.3.2.4","Gap sharing and measurement [LTE_feMTC-Core]",50762,"revised","2017-05-24T17:19:02.187","2017-05-24T17:27:51.997","R4-1706192","","Rel-14","36.133","14.3.0","LTE_feMTC-Core","4939","2","B","","","","","",""]
["R4-1706283","Correction to RRM 4DL FDD CA test cases","ANRITSU LTD","Ian Rose","9381","CR","Agreement","For A.8.16.55:\n- Correct Test Purpose and Environment.\n- Correct Cell 2 OCNG Pattern\n- Correct RSRP and SCH_RP for Cell 4\n- Correct Cell 5 OCNG Pattern","","74","5.7.1.2","RRM [WI code]",0,"agreed","2017-05-24T17:19:03.683","2017-06-02T13:07:51.797","","","Rel-14","36.133","14.3.0","LTE_CA_B1_B40-Perf","4839","1","A","RP-171298","","","","",""]
["R4-1706284","Timing advance requirements for Cat M1 UEs","Ericsson","Santhan Thangarasa","59137","CR","Agreement","This CR contians timing advance requirements for Cat-M1 UEs.","","45","5.4.3","RRM Core (36.133) [LTE_MTCe2_L1-Core]",50780,"agreed","2017-05-24T17:19:04.073","2017-06-02T13:07:51.813","","","Rel-14","36.133","14.3.0","LTE_MTCe2_L1-Core","4941","1","A","RP-171308","","","","",""]
["R4-1706285","RTS applicability for > 2 Rx","Keysight Technologies","Kyoungseok Oh","66120","CR","Agreement","","","144","7.11.1","General [LTE_MIMO_OTA-Core]",45762,"agreed","2017-05-24T17:19:04.450","2017-06-02T13:07:51.813","","","Rel-14","37.977","14.3.0","LTE_MIMO_OTA","0058","3","F","RP-171258","","","","",""]
["R4-1706286","Inter-frequency cell reselection under enhanced coverage for NB-IOT","Ericsson","Kyoungseok Oh","66120","CR","Agreement","","","62","5.5.5","RRM Performance (36.133) [NB_IOT-Perf]",51161,"agreed","2017-05-24T17:19:04.840","2017-06-02T13:07:51.813","","","Rel-13","36.133","13.7.0","NB_IOT-Perf","4936","2","B","RP-171303","","","","",""]
["R4-1706287","Introduction of Rel-14 4DL/1UL combinations in 36.101","Ericsson","Kyoungseok Oh","66120","CR","Agreement","","","106","7.4.1","Rapporteur Input (WID/CRs) [LTE_CA_R14_4DL1UL-Core]",0,"agreed","2017-05-24T17:19:05.230","2017-06-02T13:07:51.827","","","Rel-14","36.101","14.3.0","LTE_CA_R14_4DL1UL","4426","2","B","RP-171275","","","","",""]
["R4-1706288","Introduction of Rel-14 4DL/1UL combinations in 36.104","Ericsson","Kyoungseok Oh","66120","CR","Agreement","","","106","7.4.1","Rapporteur Input (WID/CRs) [LTE_CA_R14_4DL1UL-Core]",0,"agreed","2017-05-24T17:19:05.680","2017-06-02T13:07:51.827","","","Rel-14","36.104","14.3.0","LTE_CA_R14_4DL1UL","4672","2","B","RP-171275","","","","",""]
["R4-1706289","CR on Channel Model Validation","ETS-Lindgren Europe, MVG Industries","Kyoungseok Oh","66120","CR","Agreement","","","145","7.11.2","Performance requirements [LTE_MIMO_OTA-Core]",45292,"agreed","2017-05-24T17:19:06.197","2017-06-02T13:07:51.827","","","Rel-14","37.977","14.3.0","LTE_MIMO_OTA","0060","3","B","RP-171258","","","","",""]
["R4-1706290","Introduction of Rel-14 4DL/1UL combinations in 36.141","Ericsson","Kyoungseok Oh","66120","CR","Agreement","","","106","7.4.1","Rapporteur Input (WID/CRs) [LTE_CA_R14_4DL1UL-Core]",0,"agreed","2017-05-24T17:19:06.570","2017-06-02T13:07:51.843","","","Rel-14","36.141","14.3.0","LTE_CA_R14_4DL1UL","1034","3","B","RP-171275","","","","",""]
["R4-1706291","Timing requirements for Cat-M2","Ericsson, Qualcomm Incorporated","Kyoungseok Oh","66120","CR","Agreement","","","217","7.18.3.2.5","RLM and timing [LTE_feMTC-Core]",618200,"agreed","2017-05-24T17:19:06.930","2017-06-02T13:07:51.843","","","Rel-14","36.133","14.3.0","LTE_feMTC-Core","4701","3","B","RP-171266","","","","",""]
["R4-1706292","CR on test case for Bluetooth identification","Huawei, HiSilicon","Kyoungseok Oh","66120","CR","Agreement","","","252","7.23.2.2","RAT-independent enhancement [UTRA_LTE_iPos_enh2-Perf]",45193,"agreed","2017-05-24T17:19:07.257","2017-06-02T13:07:51.843","","","Rel-14","37.171","14.1.0","UTRA_LTE_iPos_enh2-Perf","0016","4","B","RP-171270","","","","",""]
["R4-1706293","RRM requirements with eMBMS enhancements","Ericsson","Kyoungseok Oh","66120","CR","Agreement","","","155","7.13.3","RRM core (36.133) [MBMS_LTE_enh2-Core]",0,"agreed","2017-05-24T17:19:07.583","2017-06-02T13:07:51.860","","","Rel-14","36.133","14.3.0","MBMS_LTE_enh2-Core","4985","4","B","RP-171261","","","","",""]
["R4-1706294","CONNECTED mode requirements for feMTC UEs in CEModeA","Ericsson","Kyoungseok Oh","66120","CR","Agreement","","","216","7.18.3.2.4","Gap sharing and measurement [LTE_feMTC-Core]",0,"agreed","2017-05-24T17:19:07.927","2017-06-02T13:07:51.860","","","Rel-14","36.133","14.3.0","LTE_feMTC-Core","4938","3","B","RP-171266","","","","",""]
["R4-1706295","CONNECTED mode requirements for feMTC UEs in CEModeB","Ericsson","Kyoungseok Oh","66120","CR","Agreement","","","216","7.18.3.2.4","Gap sharing and measurement [LTE_feMTC-Core]",0,"agreed","2017-05-24T17:19:08.257","2017-06-02T13:07:51.860","","","Rel-14","36.133","14.3.0","LTE_feMTC-Core","4939","3","B","RP-171266","","","","",""]
["R4-1706296","4DL FDD RSRQ for E-UTRAN in Carrier Aggregation in R14","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","Agreement","","","292","7.29.3","RRM [WI code or TEI14]",50300,"agreed","2017-05-24T17:19:08.647","2017-06-02T13:07:51.877","","","Rel-14","36.133","14.3.0","TEI13","4911","1","A","RP-171311","","","","",""]
["R4-1706297","4DL TDD RSRQ for E-UTRAN in Carrier Aggregation in R14","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","Agreement","","","292","7.29.3","RRM [WI code or TEI14]",50320,"agreed","2017-05-24T17:19:09.020","2017-06-02T13:07:51.877","","","Rel-14","36.133","14.3.0","TEI13","4913","1","A","RP-171311","","","","",""]
["R4-1706298","Correction on the test cases of RLM for Cat-M1 UE in R14","Huawei, HiSilicon","Xiang (Steven) Chen","41576","CR","Agreement","","","292","7.29.3","RRM [WI code or TEI14]",50340,"agreed","2017-05-24T17:19:09.377","2017-06-02T13:07:51.890","","","Rel-14","36.133","14.3.0","TEI13","4915","1","A","RP-171311","","","","",""]
["R4-1706299","4DL FDD RSRQ for E-UTRAN in Carrier Aggregation in R13","Huawei, HiSilicon","Kyoungseok Oh","66120","CR","Agreement","","","292","7.29.3","RRM [WI code or TEI14]",50291,"agreed","2017-05-24T17:19:09.707","2017-06-02T13:07:51.890","","","Rel-13","36.133","13.7.0","TEI13","4910","2","F","RP-171311","","","","",""]
["R4-1706300","4DL TDD RSRQ for E-UTRAN in Carrier Aggregation in R13","Huawei, HiSilicon","Kyoungseok Oh","66120","CR","Agreement","","","292","7.29.3","RRM [WI code or TEI14]",50311,"agreed","2017-05-24T17:19:10.050","2017-06-02T13:07:51.890","","","Rel-13","36.133","13.7.0","TEI13","4912","2","F","RP-171311","","","","",""]
["R4-1706301","Correction on the test cases of RLM for Cat-M1 UE in R13","Huawei, HiSilicon","Kyoungseok Oh","66120","CR","Agreement","","","292","7.29.3","RRM [WI code or TEI14]",50331,"agreed","2017-05-24T17:19:10.377","2017-06-02T13:07:51.907","","","Rel-13","36.133","13.7.0","TEI13","4914","2","F","RP-171311","","","","",""]
["R4-1706302","Void","Void","Kyoungseok Oh","66120","other","Discussion","","","86","7","Rel-14 Work Items",630200,"reserved","2017-05-24T17:19:10.720",null,"","","","","","","","","","","","","","",""]
["R4-1706303","Void","Void","Kyoungseok Oh","66120","other","Discussion","","","86","7","Rel-14 Work Items",630300,"reserved","2017-05-24T17:19:11.047",null,"","","","","","","","","","","","","","",""]
["R4-1706304","Void","Void","Kyoungseok Oh","66120","other","Discussion","","","86","7","Rel-14 Work Items",630400,"reserved","2017-05-24T17:19:11.390",null,"","","","","","","","","","","","","","",""]
["R4-1706305","Void","Void","Kyoungseok Oh","66120","other","Discussion","","","86","7","Rel-14 Work Items",630500,"reserved","2017-05-24T17:19:11.733",null,"","","","","","","","","","","","","","",""]
["R4-1706306","Void","Void","Kyoungseok Oh","66120","other","Discussion","","","86","7","Rel-14 Work Items",630600,"reserved","2017-05-24T17:19:12.077",null,"","","","","","","","","","","","","","",""]
["R4-1706307","Void","Void","Kyoungseok Oh","66120","other","Discussion","","","86","7","Rel-14 Work Items",630700,"reserved","2017-05-24T17:19:12.437",null,"","","","","","","","","","","","","","",""]
["R4-1706308","Void","Void","Kyoungseok Oh","66120","other","Discussion","","","86","7","Rel-14 Work Items",630800,"reserved","2017-05-24T17:19:12.780",null,"","","","","","","","","","","","","","",""]
["R4-1706309","Void","Void","Kyoungseok Oh","66120","other","Discussion","","","86","7","Rel-14 Work Items",630900,"reserved","2017-05-24T17:19:13.107",null,"","","","","","","","","","","","","","",""]
["R4-1706310","Void","Void","Kyoungseok Oh","66120","other","Discussion","","","86","7","Rel-14 Work Items",631000,"reserved","2017-05-24T17:19:13.450",null,"","","","","","","","","","","","","","",""]
["R4-1706311","WF on OTA REFSENS RoAoA defination","Ericsson","Kyoungseok Oh","66120","other","Discussion","","","363","9.12.2.6","Other Receiver requirements [AASenh_BS_LTE_UTRA-Core]",49440,"approved","2017-05-24T17:19:13.777","2017-05-24T17:27:52.107","","","","","","","","","","","","","","",""]
["R4-1706312","Draft CR on TS 37.105 General Sections","Huawei","Kyoungseok Oh","66120","other","Discussion","","","356","9.12.1","General [AASenh_BS_LTE_UTRA]",631200,"noted","2017-05-24T17:19:14.107","2017-05-24T17:27:52.107","","","","","","","","","","","","","","",""]
["R4-1706313","WF on NR BS blocking for mmWave operation","Ericsson, ZTE","Kyoungseok Oh","66120","other","Discussion","","","445","10.5.4.2","Blocking Requirements [NR_newRAT]",631300,"approved","2017-05-24T17:19:14.433","2017-05-24T17:27:52.107","","","","","","","","","","","","","","",""]
["R4-1706314","NR RRM ad hoc minutes","Huawei","Kyoungseok Oh","66120","report","Approval","","","449","10.6.1","RRM General (ad-hoc MoM, Plan, Spec structure) [NR_newRAT]",631400,"approved","2017-05-24T17:19:14.760","2017-05-24T17:27:52.123","","","","","","","","","","","","","","",""]
["R4-1706315","WF on supporting channel bandwidth and SCS","Ericsson","Kyoungseok Oh","66120","other","Discussion","","","418","10.3.1","Channel bandwidth and subcarrier spacing [NR_newRAT]",605501,"approved","2017-05-24T17:19:15.103","2017-05-24T17:27:52.123","R4-1706055","","","","","","","","","","","","","",""]
["R4-1706316","WF on sub 6GHz ACLR and ACS","Nokia, Alcatel-Lucent Shanghai Bell","Kyoungseok Oh","66120","other","Discussion","","","422","10.3.5","ACLR and ACS [NR_newRAT]",606201,"approved","2017-05-24T17:19:15.447","2017-05-24T17:27:52.123","R4-1706062","","","","","","","","","","","","","",""]
["R4-1706317","WF on On Off Mask Transient Time","Qualcomm, Intel, CATT, Ericsson, Huawei","Kyoungseok Oh","66120","other","Approval","","","428","10.4.3.2","ON/OFF time mask [NR_newRAT]",577602,"approved","2017-05-24T17:19:15.820","2017-05-24T17:27:52.137","R4-1706071","","","","","","","","","","","","","",""]
["R4-1706318","WF on RRM testability","Intel","Kyoungseok Oh","66120","other","Discussion","","","464","10.7.4","RRM requirements [FS_NR_test_methods]",631800,"approved","2017-05-24T17:19:16.150","2017-05-24T17:27:52.137","","","","","","","","","","","","","","",""]
["R4-1706319","WF on TX and Rx loss factors","Ericsson","Kyoungseok Oh","66120","other","Discussion","","","359","9.12.2.2","Tx and Rx loss values [AASenh_BS_LTE_UTRA-Core]",613201,"approved","2017-05-24T17:19:16.477","2017-05-24T17:27:52.137","R4-1706132","","","","","","","","","","","","","",""]
["R4-1706320","WF on mixed numerology and associated in-band requirements","Huawei","Kyoungseok Oh","66120","other","Discussion","","","421","10.3.4","In-band requirements [NR_newRAT]",606101,"approved","2017-05-24T17:19:16.803","2017-05-24T17:27:52.137","R4-1706061","","","","","","","","","","","","","",""]
["R4-1706321","WF on Maximum Channel Bandwidth","Qualcomm Incorporated","Kyoungseok Oh","66120","other","Approval","","","418","10.3.1","Channel bandwidth and subcarrier spacing [NR_newRAT]",52402,"approved","2017-05-24T17:19:17.147","2017-05-24T17:27:52.153","R4-1706054","","Rel-15","","","","","","","","","","","",""]
["R4-1706322","WF on mmWave UE output power","Qualcomm","Kyoungseok Oh","66120","other","Discussion","","","427","10.4.3.1","UE power class and MPR/A-MPR [NR_newRAT]",632200,"approved","2017-05-24T17:19:17.490","2017-05-24T17:27:52.153","","","","","","","","","","","","","","",""]
["R4-1706323","WF on Channel Raster and Sychronization Raster/SCS","Huawei","Kyoungseok Oh","66120","other","Discussion","","","419","10.3.2","Channel Raster [NR_newRAT]",52651,"approved","2017-05-24T17:19:17.833","2017-05-24T17:27:52.153","R4-1706056","","","","","","","","","","","","","",""]
["R4-1706324","Draft of TS38.133 v0.0.1","Intel Corporation","Kyoungseok Oh","66120","draft TS","Approval","","","449","10.6.1","RRM General (ad-hoc MoM, Plan, Spec structure) [NR_newRAT]",47601,"approved","2017-05-24T17:19:18.160","2017-05-24T17:27:52.170","R4-1704696","","Rel-15","38.133","0.0.1","NR_newRAT-Perf","","","","","","","","",""]
["R4-1706325","Proposed NR frequency range and band combination","NTT DOCOMO, INC.","Kyoungseok Oh","66120","other","","","","412","10.2","NR bands and NR-LTE band combinations [NR_newRAT]",581701,"approved","2017-05-24T17:19:19.830","2017-05-30T15:07:19.833","R4-1705817","","","","","","","","","","","","","",""]

{"sheet":"CR_Packs_List","index":1,"n_rows":1,"n_cols":11,"rows_kept":1,"cut":false,"hidden":false,"merged":[]}
["CR Pack TDoc","WG Tdoc","WG TDoc decision","CR Individual TSG decision","Spec","CR","CR revision","CR category","Release","Version","CR title"]

{"sheet":"Parameters","index":2,"n_rows":25,"n_cols":4,"rows_kept":25,"cut":false,"hidden":true,"merged":[]}
["Types of Tdocs","Possible statuses of Tdocs","Categories"]
[]
["agenda","reserved","A","Decision"]
["Work Plan","available","B","Agreement"]
["LS in","revised","C","Approval"]
["LS out","agreed","D","Information"]
["pCR","conditionally agreed","E","Discussion"]
["draftCR","approved","F","Action"]
["CR","conditionally approved",null,"Endorsement"]
["CR pack","partially approved",null,"Presentation"]
["ToR","treated"]
["WID new","endorsed"]
["WID revised","replied to"]
["SID new","merged"]
["SID revised","not pursued"]
["WI status report","postponed"]
["WI exception request","noted"]
["TS or TR cover","not concluded"]
["draft TS","withdrawn"]
["draft TR","reissued"]
["report","not treated"]
["discussion"]
["response"]
["other"]
["WI summary"]