{"text_format":"1","workbook":"xlsx","n_sheets":13,"sheets":["Cover","Parameters","PUSCH fading","PUSCH 350kmph","PUSCH 500kmph","PUSCH UL TA scenario X","PUSCH UL TA","PRACH format0 Type A fading","PRACH format0 Type B fading","PRACH 1.25kHz SCS Type A","PRACH 1.25kHz SCS Type B","PRACH 15kHz SCS","PRACH 30kHz SCS"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Cover","index":0,"n_rows":8,"n_cols":10,"rows_kept":8,"cut":false,"hidden":false,"merged":[]}
[]
[null,"3GPP TSG-RAN WG4 Meeting #97-e",null,null,null,null,null,null,null,"R4-2017557"]
[null,"Electronic Meeting, 2 - 13 Nov., 2020"]
[]
[null,"Source: CATT"]
[null,"Title: Summary of ideal and impairment results for NR HST demodulation requirements"]
[null,"Agenda: 7.15.3.2"]
[null,"Document for: Information"]

{"sheet":"Parameters","index":1,"n_rows":12,"n_cols":5,"rows_kept":12,"cut":false,"hidden":false,"merged":[[1,2,1,4],[7,2,7,4],[6,2,6,4]]}
[]
[null,null,"Parameters for deriving performance requirements"]
[null,null,"Ideal Span Threshold",2,"dB"]
[null,null,"Impairment Span Threshold",4,"dB"]
[]
[]
[null,"Notes","1. Call function DerivingPerfReq()"]
[null,null,"2. If the ruls does not apply, or fails, -100dB or less will be returned"]
[null,null,null,-100,"Not enough input"]
[null,null,null,-101,"Input should be pairs"]
[null,null,null,-102,"Too large span for impairment"]
[null,null,null,-103,"After removal iteration, not enough input"]

{"sheet":"PUSCH fading","index":2,"n_rows":6,"n_cols":33,"rows_kept":6,"cut":false,"hidden":false,"merged":[[4,1,5,1],[2,0,5,0],[2,1,3,1],[0,23,0,24],[0,25,0,26],[0,6,1,6],[0,7,1,7],[0,8,1,8],[0,9,1,9],[0,10,1,10],[0,11,1,11],[0,0,1,0],[0,1,1,1],[0,2,1,2],[0,3,1,3],[0,4,1,4],[0,5,1,5],[0,27,0,28],[0,29,0,30],[0,31,0,32],[0,12,1,12],[0,13,0,14],[0,15,0,16],[0,17,0,18],[0,19,0,20],[0,21,0,22]]}
["Channel model","Propagation condition","Carrier frequency (GHz)","SCS","CBW","Frequency Offset(Hz)","Tx/Rx","PUSCH mapping type","DMRS","l0","MCS","38.104 req","38.141 req","Samsung",null,"ZTE",null,"CMCC",null,"CATT",null,"Nokia",null,"Huawei",null,"Ericsson",null,"Intel",null,"SPAN",null,"AVERAGE"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment"]
["Multi-path fading","TDLC300-600",2.1,"15KHz","5MHz",0,"1T2R","Type A","1+1+1","2 or 3",2,{"$f":"DerivingPerfReq(N3:AC3)","v":-2},{"$f":"IF(L3>-100,L3+0.6,L3)","v":-1.4},-3.37,-1.37,null,null,null,null,-4.51,-2.0099999999999998,-4.6100000000000003,-2.11,-4.3899999999999997,-2.39,-4.0999999999999996,-2,-9.8000000000000007,-7.3,{"$f":"MAX(N3,P3,R3,T3,V3,X3,Z3,AB3)-MIN(N3,P3,R3,T3,V3,X3,Z3,AB3)","v":6.4300000000000006},{"$f":"MAX(O3,Q3,S3,U3,W3,Y3,AA3,AC3)-MIN(O3,Q3,S3,U3,W3,Y3,AA3,AC3)","v":5.93},{"$f":"AVERAGE(N3,P3,R3,T3,V3,X3,Z3,AB3)","v":-5.13},-2.8633333333333333]
[null,null,3.6,"30KHz","10MHz",0,"1T2R","Type A","1+1+1","2 or 3",2,-100,{"$f":"IF(L4>-100,L4+0.6,L4)","v":-100},null,null,null,null,null,null,-4.9400000000000004,-2.4400000000000004,null,null,null,null,null,null,null,null,0,0,-4.9400000000000004,-2.4400000000000004]
[null,"TDLC300-1200",2.1,"15KHz","5MHz",0,"1T2R","Type A","1+1+1","2 or 3",2,{"$f":"DerivingPerfReq(N5:AC5)","v":-100},-100,null,null,null,null,null,null,-1.46,1.04,null,null,null,null,null,null,null,null,{"$f":"MAX(N5,P5,R5,T5,V5,X5,Z5,AB5)-MIN(N5,P5,R5,T5,V5,X5,Z5,AB5)","v":0},{"$f":"MAX(O5,Q5,S5,U5,W5,Y5,AA5,AC5)-MIN(O5,Q5,S5,U5,W5,Y5,AA5,AC5)","v":0},{"$f":"AVERAGE(N5,P5,R5,T5,V5,X5,Z5,AB5)","v":-1.46},{"$f":"AVERAGE(O5,Q5,S5,U5,W5,Y5,AA5,AC5)","v":1.04}]
[null,null,3.6,"30KHz","10MHz",0,"1T2R","Type A","1+1+1","2 or 3",2,-1.8,-1.2000000000000002,-3.4,-1.4,null,null,null,null,-4.62,-2.12,-4.63,-2.13,-3.98,-1.98,-3.9,-1.6,-9.8000000000000007,-7.3,6.4,5.9,-5.0549999999999997,-2.7550000000000003]

{"sheet":"PUSCH 350kmph","index":3,"n_rows":30,"n_cols":33,"rows_kept":30,"cut":false,"hidden":false,"merged":[[2,4,4,4],[5,4,7,4],[2,5,4,5],[5,5,7,5],[8,5,11,5],[8,4,11,4],[5,3,7,3],[8,3,11,3],[12,3,15,3],[12,5,15,5],[12,4,15,4],[0,23,0,24],[0,25,0,26],[0,29,0,30],[0,31,0,32],[0,17,0,18],[0,19,0,20],[0,21,0,22],[0,27,0,28],[10,6,11,6],[12,6,13,6],[14,6,15,6],[3,6,4,6],[8,6,9,6],[6,6,7,6],[0,2,1,2],[0,4,1,4],[0,12,1,12],[0,13,0,14],[0,15,0,16],[0,8,1,8],[0,7,1,7],[2,0,15,0],[2,1,7,1],[8,1,15,1],[0,11,1,11],[0,1,1,1],[0,3,1,3],[0,5,1,5],[0,6,1,6],[0,9,1,9],[0,10,1,10],[0,0,1,0],[2,2,4,2],[5,2,7,2],[8,2,11,2],[12,2,15,2],[2,3,4,3],[16,0,29,0],[16,1,21,1],[16,2,18,2],[16,3,18,3],[16,4,18,4],[22,1,29,1],[22,2,25,2],[22,3,25,3],[22,4,25,4],[16,5,18,5],[17,6,18,6],[19,2,21,2],[19,3,21,3],[19,4,21,4],[19,5,21,5],[20,6,21,6],[22,5,25,5],[22,6,23,6],[24,6,25,6],[26,2,29,2],[26,3,29,3],[26,4,29,4],[26,5,29,5],[26,6,27,6],[28,6,29,6]]}
["Channel model","Propagation condition","Carrier frequency (GHz)","SCS","CBW","Maximum Doppler shift","Tx/Rx","PUSCH mapping type","DMRS","l0","MCS","38.104 req","38.141 req","Samsung",null,"ZTE",null,"CMCC",null,"CATT",null,"Nokia",null,"Huawei",null,"Ericsson",null,"Intel",null,"SPAN",null,"AVERAGE"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment"]
["AWGN","Tunnel",2.1,"15KHz","10MHz","1340Hz","1T1R","Type A","1+1+1","2 or 3",2,{"$f":"DerivingPerfReq(N3:AC3)","v":-0.8},{"$f":"IF(L3>-100,L3+0.3,L3)","v":-0.5},-2.83,-0.83,null,null,null,null,-3.47,-0.9700000000000002,-3.19,-0.69,-3.51,{"$f":"X3+2","v":-1.5099999999999998},-3,-0.9,-2.4,0.1,{"$f":"MAX(N3,P3,R3,T3,V3,X3,Z3,AB3)-MIN(N3,P3,R3,T3,V3,X3,Z3,AB3)","v":1.1099999999999999},{"$f":"MAX(O3,Q3,S3,U3,W3,Y3,AA3,AC3)-MIN(O3,Q3,S3,U3,W3,Y3,AA3,AC3)","v":1.6099999999999999},{"$f":"AVERAGE(N3,P3,R3,T3,V3,X3,Z3,AB3)","v":-3.0666666666666664},{"$f":"AVERAGE(O3,Q3,S3,U3,W3,Y3,AA3,AC3)","v":-0.80000000000000016}]
[null,null,null,"15KHz","10MHz","1340Hz","1T2R","Type A","1+1+1","2 or 3",2,{"$f":"DerivingPerfReq(N4:AC4)","v":-3.6},{"$f":"IF(L4>-100,L4+0.3,L4)","v":-3.3000000000000003},-5.84,-3.84,-5.62,{"$f":"P4+2.5","v":-3.12},null,null,-6.2,-3.7,-5.93,-3.4299999999999997,-6.6,{"$f":"X4+2","v":-4.5999999999999996},-6,-3.6,-5.2,-2.7,{"$f":"MAX(N4,P4,R4,T4,V4,X4,Z4,AB4)-MIN(N4,P4,R4,T4,V4,X4,Z4,AB4)","v":1.3999999999999995},{"$f":"MAX(O4,Q4,S4,U4,W4,Y4,AA4,AC4)-MIN(O4,Q4,S4,U4,W4,Y4,AA4,AC4)","v":1.8999999999999995},{"$f":"AVERAGE(N4,P4,R4,T4,V4,X4,Z4,AB4)","v":-5.9128571428571428},{"$f":"AVERAGE(O4,Q4,S4,U4,W4,Y4,AA4,AC4)","v":-3.57}]
[null,null,null,"15KHz","10MHz","1340Hz",null,"Type A","1+1+1","2 or 3",16,8.6999999999999993,9,7.32,9.32,6.13,{"$f":"P5+2.5","v":8.629999999999999},null,null,5.68,8.18,5.75,8.25,5.41,7.41,6.6,9.1,7.3,9.8000000000000007,1.9100000000000001,2.3900000000000006,6.3128571428571423,8.67]
[null,null,3.6,"30KHz","40MHz","2334Hz","1T1R","Type A","1+1+1","2 or 3",2,-0.8,-0.5,-2.82,-0.82,null,null,null,null,-3.37,-0.87000000000000011,-3.2,-0.70000000000000018,-3.51,-1.5099999999999998,-3,-1,-2.2999999999999998,0.2,1.21,1.7099999999999997,-3.0333333333333332,-0.78333333333333333]
[null,null,null,"30KHz","40MHz","2334Hz","1T2R","Type A","1+1+1","2 or 3",2,-3.6,-3.3000000000000003,-5.83,-3.83,-5.63,null,null,null,-6.11,-3.6100000000000003,-5.97,-3.4699999999999998,-6.59,-4.59,-6.9,-3.6,-5.0999999999999996,-2.6,1.8000000000000007,1.9899999999999998,-6.0185714285714287,-3.6166666666666671]
[null,null,null,"30KHz","40MHz","2334Hz",null,"Type A","1+1+1","2 or 3",16,8.6999999999999993,9,7.31,9.31,7.34,null,null,null,5.79,8.2899999999999991,5.74,8.24,5.41,7.41,6.5,9,7.2,9.6999999999999993,1.9299999999999997,2.2899999999999991,6.4700000000000006,8.6583333333333332]
[null,"Open space",2.1,"15KHz","10MHz","1340Hz","1T2R","Type A","1+1+1","2 or 3",2,-3.7,-3.4000000000000004,-5.89,-3.89,-5.66,{"$f":"P9+2.5","v":-3.16},null,null,-6.21,-3.71,-6,-3.5,-6.6,-4.5999999999999996,-6.1,-4,-5.5,-3,1.0999999999999996,1.5999999999999996,-5.9942857142857147,-3.6942857142857144]
[null,null,2.1,"15KHz","10MHz","1340Hz",null,"Type A","1+1+1","2 or 3",16,8.4,{"$f":"IF(L10>-100,L10+0.3,L10)","v":8.7000000000000011},6.87,8.8699999999999992,6.54,{"$f":"P10+2.5","v":9.0399999999999991},null,null,5.67,8.17,5.73,8.23,5.4,7.4,6.3,8.5,6.4,8.9,1.4699999999999998,1.6399999999999988,6.13,8.444285714285714]
[null,null,2.1,"15KHz","10MHz","1340Hz","1T8R","Type A","1+1+1","2 or 3",2,-9.1999999999999993,-8.8999999999999986,-11.29,-9.2899999999999991,-10.99,{"$f":"P11+2.5","v":-8.49},null,null,-11.2,-8.6999999999999993,-11.27,-8.77,-12.57,-10.57,-12,-9.9,-11.3,-8.8000000000000007,1.58,2.08,-11.517142857142856,-9.2171428571428571]
[null,null,2.1,"15KHz","10MHz","1340Hz",null,"Type A","1+1+1","2 or 3",16,2.6,2.9,1.07,3.07,0.2,2.7,null,null,-0.24,2.2599999999999998,-0.25,2.25,0.4,2.4,0.3,2.6,0.4,2.9,1.32,0.81999999999999984,0.26857142857142863,2.597142857142857]
[null,null,3.6,"30KHz","40MHz","2334Hz","1T2R","Type A","1+1+1","2 or 3",2,-3.7,-3.4000000000000004,-5.87,-3.87,-5.91,-3.41,null,null,-6.12,-3.62,-6.01,-3.51,-6.67,-4.67,-6,-3.6,-5.4,-2.9,1.2699999999999996,1.77,-5.9971428571428573,-3.6542857142857139]
[null,null,3.6,"30KHz","40MHz","2334Hz",null,"Type A","1+1+1","2 or 3",16,8.5,8.8000000000000007,6.9,8.9,6.65,9.15,null,null,5.76,8.26,5.72,8.2199999999999989,5.4,7.4,6.2,8.5,6.4,8.9,1.5,1.75,6.1471428571428577,8.475714285714286]
[null,null,3.6,"30KHz","40MHz","2334Hz","1T8R","Type A","1+1+1","2 or 3",2,-9.1,-8.7999999999999989,-11.29,-9.2899999999999991,-10.97,-8.4700000000000006,null,null,-11.05,-8.5500000000000007,-11.27,-8.77,-12.6,-10.6,-12,-9.5,-11.2,-8.6999999999999993,1.629999999999999,2.129999999999999,-11.482857142857144,-9.1257142857142846]
[null,null,3.6,"30KHz","40MHz","2334Hz",null,"Type A","1+1+1","2 or 3",16,2.7,3,1.1000000000000001,3.1,0.96,3.46,null,null,-0.11,2.39,-0.26,2.2400000000000002,0.4,2.4,0.3,2.4,0.4,2.9,1.36,1.2199999999999998,0.39857142857142852,2.6985714285714288]
["AWGN","Tunnel",2.1,"15KHz","5MHz","1340Hz","1T1R","Type A","1+1+1","2 or 3",2,{"$f":"DerivingPerfReq(N17:AC17)","v":-0.7},{"$f":"IF(L17>-100,L17+0.3,L17)","v":-0.39999999999999997},-2.81,-0.81,-2.92,{"$f":"P17+2.5","v":-0.41999999999999993},null,null,-3.45,-0.95000000000000018,-3.08,-0.57999999999999996,-3.51,-1.5099999999999998,-3,-0.9,-2.4,0.1,{"$f":"MAX(N17,P17,R17,T17,V17,X17,Z17,AB17)-MIN(N17,P17,R17,T17,V17,X17,Z17,AB17)","v":1.1099999999999999},{"$f":"MAX(O17,Q17,S17,U17,W17,Y17,AA17,AC17)-MIN(O17,Q17,S17,U17,W17,Y17,AA17,AC17)","v":1.6099999999999999},{"$f":"AVERAGE(N17,P17,R17,T17,V17,X17,Z17,AB17)","v":-3.024285714285714},{"$f":"AVERAGE(O17,Q17,S17,U17,W17,Y17,AA17,AC17)","v":-0.72428571428571431}]
[null,null,null,"15KHz",null,"1340Hz","1T2R","Type A","1+1+1","2 or 3",2,{"$f":"DerivingPerfReq(N18:AC18)","v":-3.6},{"$f":"IF(L18>-100,L18+0.3,L18)","v":-3.3000000000000003},-5.8,-3.8,-5.68,{"$f":"P18+2.5","v":-3.1799999999999997},null,null,-6.19,-3.6900000000000004,-5.86,-3.36,-6.51,-4.51,-6,-3.6,-5.3,-2.8,{"$f":"MAX(N18,P18,R18,T18,V18,X18,Z18,AB18)-MIN(N18,P18,R18,T18,V18,X18,Z18,AB18)","v":1.21},{"$f":"MAX(O18,Q18,S18,U18,W18,Y18,AA18,AC18)-MIN(O18,Q18,S18,U18,W18,Y18,AA18,AC18)","v":1.71},{"$f":"AVERAGE(N18,P18,R18,T18,V18,X18,Z18,AB18)","v":-5.9057142857142848},{"$f":"AVERAGE(O18,Q18,S18,U18,W18,Y18,AA18,AC18)","v":-3.5628571428571432}]
[null,null,null,"15KHz",null,"1340Hz",null,"Type A","1+1+1","2 or 3",16,8.5,8.8000000000000007,7.53,9.5299999999999994,6.65,{"$f":"P19+2.5","v":9.15},null,null,5.79,8.2899999999999991,5.84,8.34,5.49,7.49,6.7,9.1999999999999993,null,null,2.04,2.0399999999999991,6.333333333333333,8.6666666666666661]
[null,null,3.6,"30KHz","10MHz","2334Hz","1T1R","Type A","1+1+1","2 or 3",2,-0.8,-0.5,-2.88,-0.88,null,null,null,null,-3.47,-0.9700000000000002,-3.15,-0.65,-3.51,-1.5099999999999998,-3,-1,-2.5,0,1.0099999999999998,1.5099999999999998,-3.0849999999999995,-0.83499999999999996]
[null,null,null,"30KHz",null,"2334Hz","1T2R","Type A","1+1+1","2 or 3",2,-3.7,-3.4000000000000004,-5.87,-3.87,null,null,null,null,-6.23,-3.7300000000000004,-5.93,-3.43,-6.51,-4.51,-6,-3.6,-5.4,-2.9,1.1099999999999994,1.6099999999999999,-5.9899999999999993,-3.6733333333333333]
[null,null,null,"30KHz",null,"2334Hz",null,"Type A","1+1+1","2 or 3",16,8.4,8.7000000000000011,7,9,null,null,null,null,5.56,8.0599999999999987,5.72,8.2200000000000006,5.5,7.5,6.5,9,null,null,1.5,1.5,6.0559999999999992,8.3559999999999999]
[null,"Open space",2.1,"15KHz","5MHz","1340Hz","1T2R","Type A","1+1+1","2 or 3",2,-3.7,-3.4000000000000004,-5.87,-3.87,-5.74,{"$f":"P23+2.5","v":-3.24},null,null,-6.2,-3.7,-5.89,-3.39,-6.51,-4.51,-6.1,-4,-5.4,-2.9,1.1099999999999994,1.6099999999999999,-5.9585714285714291,-3.6585714285714284]
[null,null,2.1,"15KHz",null,"1340Hz",null,"Type A","1+1+1","2 or 3",16,8.5,8.8000000000000007,6.96,8.9600000000000009,6.56,{"$f":"P24+2.5","v":9.0599999999999987},null,null,5.77,8.27,5.76,8.26,5.49,7.49,6.3,8.5,6.7,9.1999999999999993,1.4699999999999998,1.7099999999999991,6.22,8.5342857142857138]
[null,null,2.1,"15KHz",null,"1340Hz","1T8R","Type A","1+1+1","2 or 3",2,-9.1,-8.7999999999999989,-11.18,-9.18,-10.96,{"$f":"P25+2.5","v":-8.4600000000000009},null,null,-11.27,-8.77,-11.22,-8.7200000000000006,-12.44,-10.44,-11.9,-9.8000000000000007,-10.7,-8.1999999999999993,1.7400000000000002,2.2400000000000002,-11.381428571428572,-9.0814285714285727]
[null,null,2.1,"15KHz",null,"1340Hz",null,"Type A","1+1+1","2 or 3",16,2.8,3.0999999999999996,1.1399999999999999,3.14,0.7,3.2,null,null,-0.13,2.37,-0.18,2.3199999999999998,0.49,2.4900000000000002,0.3,2.6,1.3,3.8,1.48,1.48,0.51714285714285713,2.8457142857142861]
[null,null,3.6,"30KHz","10MHz","2334Hz","1T2R","Type A","1+1+1","2 or 3",2,-3.7,-3.4000000000000004,-5.92,-3.92,null,null,null,null,-6.23,-3.7300000000000004,-5.95,-3.45,-6.54,-4.54,-6,-3.6,-5.4,-2.9,1.1399999999999997,1.6400000000000001,-6.0066666666666668,-3.69]
[null,null,3.6,"30KHz",null,"2334Hz",null,"Type A","1+1+1","2 or 3",16,8.3000000000000007,8.6000000000000014,6.62,8.6199999999999992,null,null,null,null,5.55,8.0500000000000007,5.65,8.15,5.49,7.49,6.2,8.5,6.3,8.8000000000000007,1.1299999999999999,1.3100000000000005,5.9683333333333337,8.2683333333333326]
[null,null,3.6,"30KHz",null,"2334Hz","1T8R","Type A","1+1+1","2 or 3",2,-9.1999999999999993,-8.8999999999999986,-11.18,-9.18,null,null,null,null,-11.29,-8.7899999999999991,-11.25,-8.75,-12.48,-10.48,-12,-9.5,-10.8,-8.3000000000000007,1.6799999999999997,2.1799999999999997,-11.5,-9.1666666666666661]
[null,null,3.6,"30KHz",null,"2334Hz",null,"Type A","1+1+1","2 or 3",16,2.5,2.8,0.87,2.87,null,null,null,null,-0.34,2.16,-0.27,2.23,0.49,2.4900000000000002,0.3,2.4,0.4,2.9,1.21,0.73999999999999977,0.2416666666666667,2.5083333333333333]

{"sheet":"PUSCH 500kmph","index":4,"n_rows":30,"n_cols":33,"rows_kept":30,"cut":false,"hidden":false,"merged":[[0,27,0,28],[10,6,11,6],[12,6,13,6],[14,6,15,6],[3,6,4,6],[6,6,7,6],[8,6,9,6],[0,10,1,10],[0,15,0,16],[0,6,1,6],[0,9,1,9],[8,5,11,5],[8,4,11,4],[8,3,11,3],[8,2,11,2],[12,2,15,2],[12,3,15,3],[12,4,15,4],[12,5,15,5],[2,2,4,2],[2,3,4,3],[2,4,4,4],[2,5,4,5],[5,2,7,2],[5,3,7,3],[5,4,7,4],[5,5,7,5],[0,0,1,0],[0,1,1,1],[0,2,1,2],[0,3,1,3],[0,4,1,4],[0,5,1,5],[0,7,1,7],[0,8,1,8],[0,31,0,32],[2,0,15,0],[2,1,7,1],[8,1,15,1],[0,17,0,18],[0,19,0,20],[0,21,0,22],[0,23,0,24],[0,25,0,26],[0,29,0,30],[0,11,1,11],[0,12,1,12],[0,13,0,14],[16,0,29,0],[16,1,21,1],[16,2,18,2],[16,3,18,3],[16,4,18,4],[22,1,29,1],[22,2,25,2],[22,3,25,3],[22,4,25,4],[16,5,18,5],[17,6,18,6],[19,2,21,2],[19,3,21,3],[19,4,21,4],[19,5,21,5],[20,6,21,6],[22,5,25,5],[22,6,23,6],[24,6,25,6],[26,2,29,2],[26,3,29,3],[26,4,29,4],[26,5,29,5],[26,6,27,6],[28,6,29,6]]}
["Channel model","Propagation condition","Carrier frequency (GHz)","SCS","CBW","Maximum Doppler shift","Tx/Rx","PUSCH mapping type","DMRS","l0","MCS","38.104 req","38.141 req","Samsung",null,"ZTE",null,"CMCC",null,"CATT",null,"Nokia",null,"Huawei",null,"Ericsson",null,"Intel",null,"SPAN",null,"AVERAGE"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment"]
["AWGN","Tunnel",1.8,"15KHz","10MHz","1740Hz","1T1R","Type A","1+1+1","2 or 3",2,{"$f":"DerivingPerfReq(N3:AC3)","v":-0.7},{"$f":"IF(L3>-100,L3+0.3,L3)","v":-0.39999999999999997},-2.69,-0.69,null,null,null,null,-3.46,-0.96,-3.05,-0.54999999999999982,-3.51,{"$f":"X3+2","v":-1.5099999999999998},-3,-0.8,-2.4,0.1,{"$f":"MAX(N3,P3,R3,T3,V3,X3,Z3,AB3)-MIN(N3,P3,R3,T3,V3,X3,Z3,AB3)","v":1.1099999999999999},{"$f":"MAX(O3,Q3,S3,U3,W3,Y3,AA3,AC3)-MIN(O3,Q3,S3,U3,W3,Y3,AA3,AC3)","v":1.6099999999999999},{"$f":"AVERAGE(N3,P3,R3,T3,V3,X3,Z3,AB3)","v":-3.0183333333333331},{"$f":"AVERAGE(O3,Q3,S3,U3,W3,Y3,AA3,AC3)","v":-0.73499999999999999}]
[null,null,null,"15KHz","10MHz","1740Hz","1T2R","Type A","1+1+1","2 or 3",2,{"$f":"DerivingPerfReq(N4:AC4)","v":-3.6},-3.3000000000000003,-5.69,-3.69,-5.59,{"$f":"P4+2.5","v":-3.09},null,null,-6.2,-3.7,-5.8,-3.3,-6.6,{"$f":"X4+2","v":-4.5999999999999996},-6,-3.9,-5.2,-2.7,{"$f":"MAX(N4,P4,R4,T4,V4,X4,Z4,AB4)-MIN(N4,P4,R4,T4,V4,X4,Z4,AB4)","v":1.3999999999999995},{"$f":"MAX(O4,Q4,S4,U4,W4,Y4,AA4,AC4)-MIN(O4,Q4,S4,U4,W4,Y4,AA4,AC4)","v":1.8999999999999995},{"$f":"AVERAGE(N4,P4,R4,T4,V4,X4,Z4,AB4)","v":-5.8685714285714292},{"$f":"AVERAGE(O4,Q4,S4,U4,W4,Y4,AA4,AC4)","v":-3.5685714285714285}]
[null,null,null,"15KHz","10MHz","1740Hz","1T2R","Type A","1+1+1","2 or 3",16,9.1999999999999993,9.5,7.62,9.6199999999999992,6.49,{"$f":"P5+2.5","v":8.99},null,null,5.7,8.1999999999999993,6.46,8.9600000000000009,5.41,7.41,7.5,10,8.6,11.1,3.1899999999999995,3.6899999999999995,6.8257142857142856,9.1828571428571415]
[null,null,3.6,"30KHz","40MHz","3334Hz","1T1R","Type A","1+1+1","2 or 3",2,-0.7,-0.39999999999999997,-2.67,-0.67,null,null,null,null,-3.37,-0.87000000000000011,-3.17,-0.66999999999999993,-3.5,-1.5,-3,-0.8,-2.2999999999999998,0.2,1.2000000000000002,1.7,-3.0016666666666669,-0.71833333333333327]
[null,null,3.6,null,"40MHz","3334Hz","1T2R","Type A","1+1+1","2 or 3",2,-3.6,-3.3000000000000003,-5.67,-3.67,null,null,null,null,-6.11,-3.6100000000000003,-5.91,-3.41,-6.59,-4.59,-6,-3.5,-5.0999999999999996,-2.6,1.4900000000000002,1.9899999999999998,-5.8966666666666674,-3.5633333333333339]
[null,null,3.6,null,"40MHz","3334Hz","1T2R","Type A","1+1+1","2 or 3",16,8,8.3000000000000007,7.48,9.48,null,null,null,null,5.83,8.33,5.81,8.3099999999999987,5.41,7.41,7.5,9.8000000000000007,8.3000000000000007,10.8,2.8900000000000006,3.3900000000000006,6.7216666666666667,9.0216666666666665]
[null,"Open space",1.8,"15KHz","10MHz","1740Hz","1T2R","Type A","1+1+1","2 or 3",2,-3.9,-3.6,-5.85,-3.85,-5.64,{"$f":"P9+2.5","v":-3.1399999999999997},-7.16,-5.16,-6.21,-3.71,-5.97,-3.4699999999999998,-6.6,-4.5999999999999996,-6.1,-4.0999999999999996,-5.5,-3,1.6600000000000001,2.16,-6.1287500000000001,-3.8787500000000001]
[null,null,1.8,"15KHz","10MHz","1740Hz","1T2R","Type A","1+1+1","2 or 3",16,8.5,8.8000000000000007,7.22,9.2200000000000006,6.66,{"$f":"P10+2.5","v":9.16},6.25,8.25,5.68,8.18,5.75,8.25,5.4,7.4,6.5,8.6,6.8,9.3000000000000007,1.8199999999999994,1.9000000000000004,6.2824999999999998,8.5449999999999999]
[null,null,1.8,"15KHz","10MHz","1740Hz","1T8R","Type A","1+1+1","2 or 3",2,-9.4,{"$f":"IF(L11>-100,L11+0.3,L11)","v":-9.1},-11.26,-9.26,-10.97,-8.4700000000000006,-12.96,-10.96,-11.2,-8.6999999999999993,-11.26,-8.76,-12.57,-10.57,-12,-10,-11.3,-8.8000000000000007,1.9900000000000002,2.4900000000000002,-11.69,-9.44]
[null,null,1.8,"15KHz","10MHz","1740Hz","1T8R","Type A","1+1+1","2 or 3",16,{"$f":"DerivingPerfReq(N12:AC12)","v":2.7},{"$f":"IF(L12>-100,L12+0.3,L12)","v":3},1.36,3.36,0.44,2.94,0.2,2.2000000000000002,-0.22,2.2799999999999998,-0.22,2.2799999999999998,0.4,2.4,0.5,2.5,0.8,3.3,1.58,1.1599999999999997,0.40749999999999997,2.6575000000000002]
[null,null,3.6,"30KHz","40MHz","3334Hz","1T2R","Type A","1+1+1","2 or 3",2,-3.9,-3.6,-5.81,-3.81,-5.95,-3.45,-7.14,-5.14,-6.12,-3.62,-5.98,-3.4800000000000004,-6.67,-4.67,-6,-3.8,-5.4,-2.9,1.7399999999999993,2.2399999999999998,-6.13375,-3.8587500000000001]
[null,null,3.6,"30KHz","40MHz","3334Hz","1T2R","Type A","1+1+1","2 or 3",16,8.6999999999999993,9,7.3,9.3000000000000007,7.22,9.7199999999999989,6.06,8.0599999999999987,5.79,8.2899999999999991,5.74,8.24,5.4,7.4,6.5,8.9,6.8,9.3000000000000007,1.8999999999999995,2.3199999999999985,6.3512499999999994,8.6512499999999992]
[null,null,3.6,"30KHz","40MHz","3334Hz","1T8R","Type A","1+1+1","2 or 3",2,-9.1999999999999993,-8.8999999999999986,-11.25,-9.25,-10.95,-8.4499999999999993,-13.12,-11.12,-11.04,-8.5399999999999991,-11.26,-8.76,-12.6,-10.6,-12,-9.9,-11.2,-8.6999999999999993,2.17,2.67,-11.6775,-9.4150000000000009]
[null,null,3.6,"30KHz","40MHz","3334Hz","1T8R","Type A","1+1+1","2 or 3",16,2.8,3.0999999999999996,1.43,3.43,1.43,3.9299999999999997,0.1,2.1,-0.1,2.4,-0.23,2.27,0.4,2.4,0.5,2.8,0.8,3.3,1.66,{"$f":"MAX(O16,Q16,S16,U16,W16,Y16,AA16,AC16)-MIN(O16,Q16,S16,U16,W16,Y16,AA16,AC16)","v":1.8299999999999996},{"$f":"AVERAGE(N16,P16,R16,T16,V16,X16,Z16,AB16)","v":0.54125000000000001},2.8287499999999999]
["AWGN","Tunnel",1.8,"15KHz","5MHz","1740Hz","1T1R","Type A","1+1+1","2 or 3",2,{"$f":"DerivingPerfReq(N17:AC17)","v":-0.6},{"$f":"IF(L17>-100,L17+0.3,L17)","v":-0.3},-2.68,-0.68,-2.91,-0.41000000000000014,null,null,-3.45,-0.95000000000000018,-2.76,-0.26,-3.51,-1.5099999999999998,-3,-0.8,-2.2999999999999998,0.2,{"$f":"MAX(N17,P17,R17,T17,V17,X17,Z17,AB17)-MIN(N17,P17,R17,T17,V17,X17,Z17,AB17)","v":1.21},{"$f":"MAX(O17,Q17,S17,U17,W17,Y17,AA17,AC17)-MIN(O17,Q17,S17,U17,W17,Y17,AA17,AC17)","v":1.7099999999999997},{"$f":"AVERAGE(N17,P17,R17,T17,V17,X17,Z17,AB17)","v":-2.9442857142857144},{"$f":"AVERAGE(O17,Q17,S17,U17,W17,Y17,AA17,AC17)","v":-0.63}]
[null,null,null,"15KHz",null,"1740Hz","1T2R","Type A","1+1+1","2 or 3",2,{"$f":"DerivingPerfReq(N18:AC18)","v":-3.5},-3.2,-5.68,-3.68,-5.65,{"$f":"P18+2.5","v":-3.1500000000000004},null,null,-6.2,-3.7,-5.57,-3.07,-6.51,-4.51,-6,-3.9,-5.2,-2.7,{"$f":"MAX(N18,P18,R18,T18,V18,X18,Z18,AB18)-MIN(N18,P18,R18,T18,V18,X18,Z18,AB18)","v":1.3099999999999996},{"$f":"MAX(O18,Q18,S18,U18,W18,Y18,AA18,AC18)-MIN(O18,Q18,S18,U18,W18,Y18,AA18,AC18)","v":1.8099999999999996},{"$f":"AVERAGE(N18,P18,R18,T18,V18,X18,Z18,AB18)","v":-5.83},{"$f":"AVERAGE(O18,Q18,S18,U18,W18,Y18,AA18,AC18)","v":-3.53}]
[null,null,null,"15KHz",null,"1740Hz","1T2R","Type A","1+1+1","2 or 3",16,8.8000000000000007,9.1000000000000014,8.5299999999999994,10.53,6.99,{"$f":"P19+2.5","v":9.49},null,null,5.82,8.32,9.52,12.02,5.5,7.5,7.1,9.6999999999999993,null,null,4.0199999999999996,4.5199999999999996,7.2433333333333332,9.5933333333333337]
[null,null,3.6,"30KHz","10MHz","3334Hz","1T1R","Type A","1+1+1","2 or 3",2,-0.7,-0.39999999999999997,-2.77,-0.77,null,null,null,null,-3.47,-0.9700000000000002,-3.11,-0.61,-3.51,-1.5099999999999998,-3,-0.8,-2.2999999999999998,0.2,1.21,1.7099999999999997,-3.0266666666666668,-0.74333333333333329]
[null,null,3.6,null,null,"3334Hz","1T2R","Type A","1+1+1","2 or 3",2,-3.6,-3.3000000000000003,-5.76,-3.76,null,null,null,null,-6.22,-3.7199999999999998,-5.88,-3.38,-6.52,-4.5199999999999996,-6,-3.5,-5.3,-2.8,1.2199999999999998,1.7199999999999998,-5.9466666666666663,-3.6133333333333333]
[null,null,3.6,null,null,"3334Hz","1T2R","Type A","1+1+1","2 or 3",16,8.4,8.7000000000000011,8.01,10.01,null,null,null,null,5.6,8.1,5.76,8.26,5.5,7.5,7.1,9.6999999999999993,null,null,2.5099999999999998,2.5099999999999998,6.3940000000000001,8.7139999999999986]
[null,"Open space",1.8,"15KHz","5MHz","1740Hz","1T2R","Type A","1+1+1","2 or 3",2,-3.6,-3.3000000000000003,-5.83,-3.83,-5.7,{"$f":"P23+2.5","v":-3.2},null,null,-6.2,-3.7,-5.87,-3.37,-6.51,-4.51,-6.1,-4.0999999999999996,-5.3,-2.8,1.21,1.71,-5.93,-3.6442857142857146]
[null,null,1.8,"15KHz",null,"1740Hz","1T2R","Type A","1+1+1","2 or 3",16,8.6999999999999993,9,7.33,9.33,6.64,{"$f":"P24+2.5","v":9.14},null,null,5.78,8.2800000000000011,5.82,8.32,5.49,7.49,6.5,8.6,7.1,9.6,1.8399999999999999,2.1099999999999994,6.3800000000000008,8.6800000000000015]
[null,null,1.8,"15KHz",null,"1740Hz","1T8R","Type A","1+1+1","2 or 3",2,-9.1,-8.7999999999999989,-11.11,-9.11,-10.95,{"$f":"P25+2.5","v":-8.4499999999999993},null,null,-11.26,-8.76,-11.21,-8.7100000000000009,-12.44,-10.44,-12,-10,-10.6,-8.1,1.8399999999999999,2.34,-11.367142857142856,-9.081428571428571]
[null,null,1.8,"15KHz",null,"1740Hz","1T8R","Type A","1+1+1","2 or 3",16,3,3.3,1.44,3.44,0.95,3.45,null,null,-0.12,2.38,-0.05,2.4500000000000002,0.49,2.4900000000000002,0.5,2.5,1.8,4.3,1.92,1.92,0.71571428571428564,3.0014285714285718]
[null,null,3.6,"30KHz","10MHz","3334Hz","1T2R","Type A","1+1+1","2 or 3",2,-3.7,-3.4000000000000004,-5.87,-3.87,null,null,null,null,-6.22,-3.7199999999999998,-5.93,-3.43,-6.54,-4.54,-6,-3.8,-5.4,-2.9,1.1399999999999997,1.6400000000000001,-5.9933333333333332,-3.7099999999999995]
[null,null,3.6,"30KHz",null,"3334Hz","1T2R","Type A","1+1+1","2 or 3",16,8.5,8.8000000000000007,7.01,9.01,null,null,null,null,5.57,8.07,5.7,8.1999999999999993,5.49,7.49,6.5,8.9,6.7,9.1999999999999993,1.5199999999999996,1.7099999999999991,6.161666666666668,8.4783333333333317]
[null,null,3.6,"30KHz",null,"3334Hz","1T8R","Type A","1+1+1","2 or 3",2,-9.1999999999999993,-8.8999999999999986,-11.14,-9.14,null,null,null,null,-11.27,-8.77,-11.24,-8.74,-12.42,-10.42,-12,-9.9,-10.8,-8.3000000000000007,1.6199999999999992,2.1199999999999992,-11.478333333333333,-9.211666666666666]
[null,null,3.6,"30KHz",null,"3334Hz","1T8R","Type A","1+1+1","2 or 3",16,2.7,3,1.18,3.18,null,null,null,null,-0.33,2.17,-0.25,2.25,0.49,2.4900000000000002,0.5,2.8,1.1000000000000001,3.6,1.51,{"$f":"MAX(O30,Q30,S30,U30,W30,Y30,AA30,AC30)-MIN(O30,Q30,S30,U30,W30,Y30,AA30,AC30)","v":1.4300000000000002},{"$f":"AVERAGE(N30,P30,R30,T30,V30,X30,Z30,AB30)","v":0.44833333333333331},2.7483333333333335]

{"sheet":"PUSCH UL TA scenario X","index":5,"n_rows":10,"n_cols":35,"rows_kept":10,"cut":false,"hidden":false,"merged":[[0,11,1,11],[0,0,1,0],[0,1,1,1],[0,2,1,2],[0,3,1,3],[0,4,1,4],[0,5,1,5],[0,6,1,6],[0,7,1,7],[0,8,1,8],[0,9,1,9],[0,10,1,10],[0,13,1,13],[0,14,1,14],[0,15,0,16],[0,17,0,18],[0,19,0,20],[6,0,9,0],[6,1,9,1],[6,2,7,2],[8,2,9,2],[0,33,0,34],[2,0,5,0],[2,1,5,1],[2,2,3,2],[4,2,5,2],[0,21,0,22],[0,23,0,24],[0,25,0,26],[0,27,0,28],[0,29,0,30],[0,31,0,32],[0,12,1,12]]}
["Scenario","PUSCH transmission","SRS transmission","CBW","SCS","Waveform","Tx/Rx","DMRS","l0","MCS","A","Δω","PUSCH mapping type","38.104 req","38.141 req","Samsung",null,"ZTE",null,"CMCC",null,"CATT",null,"Nokia",null,"Huawei",null,"Ericsson",null,"Intel",null,"SPAN",null,"AVERAGE"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment"]
["Scenario X","FDD or  TDD","Enabled or Disabled","10MHz","15KHz","CP-OFDM","1T2R","1+1+1",2,16,"10us","0.04s-1","Type A",{"$f":"DerivingPerfReq(P3:AE3)","v":11.1},{"$f":"IF(N3>-100,N3+0.6,N3)","v":11.7},9.3800000000000008,11.38,null,null,null,null,8.07,10.57,7.71,10.210000000000001,null,null,9.3000000000000007,11.8,8.9,11.4,{"$f":"MAX(P3,R3,T3,V3,X3,Z3,AB3,AD3)-MIN(P3,R3,T3,V3,X3,Z3,AB3,AD3)","v":1.6700000000000008},{"$f":"MAX(Q3,S3,U3,W3,Y3,AA3,AC3,AE3)-MIN(Q3,S3,U3,W3,Y3,AA3,AC3,AE3)","v":1.5899999999999999},{"$f":"AVERAGE(Q4,R3,T3,V3,X3,Z3,AB3,AD3)","v":9.1179999999999986},{"$f":"AVERAGE(Q3,S3,U3,W3,Y3,AA3,AC3,AE3)","v":11.072000000000001}]
[null,null,null,"10MHz","15KHz","CP-OFDM","1T2R","1+1+1",0,16,"10us","0.04s-1","Type B",11.6,{"$f":"IF(N4>-100,N4+0.6,N4)","v":12.2},9.61,11.61,null,null,null,null,8.06,10.56,7.72,10.220000000000001,null,null,9.4,11.9,9.9,12.4,{"$f":"MAX(P4,R4,T4,V4,X4,Z4,AB4,AD4)-MIN(P4,R4,T4,V4,X4,Z4,AB4,AD4)","v":2.1800000000000006},2.1799999999999997,{"$f":"AVERAGE(Q5,R4,T4,V4,X4,Z4,AB4,AD4)","v":9.1999999999999993},11.337999999999999]
[null,null,"Enabled or Disabled","40MHz","30KHz","CP-OFDM","1T2R","1+1+1",2,16,"5us","0.08s-1","Type A",12.1,12.7,8.92,10.92,null,null,null,null,10.7,13.2,7.68,10.18,null,null,9.9,12.2,9.6,12.1,3.0199999999999996,3.0199999999999996,9.6180000000000003,11.72]
[null,null,null,"40MHz","30KHz","CP-OFDM","1T2R","1+1+1",0,16,"5us","0.08s-1","Type B",12.6,13.2,8.2100000000000009,10.210000000000001,null,null,null,null,10.52,13.02,7.68,10.18,null,null,9.8000000000000007,12.3,10,12.5,2.84,2.84,9.7039999999999988,11.641999999999999]
["Scenario X","FDD or  TDD","Enabled or Disabled","5MHz","15KHz","CP-OFDM","1T2R","1+1+1",2,16,"10us","0.04s-1","Type A",{"$f":"DerivingPerfReq(P7:AE7)","v":10.6},11.2,8.52,10.52,null,null,null,null,8.61,11.11,7.31,9.81,8.26,10.76,8.3000000000000007,10.5,8.3000000000000007,10.8,{"$f":"MAX(P7,R7,T7,V7,X7,Z7,AB7,AD7)-MIN(P7,R7,T7,V7,X7,Z7,AB7,AD7)","v":1.2999999999999998},1.2999999999999989,8.5683333333333334,10.583333333333334]
[null,null,null,"5MHz","15KHz","CP-OFDM","1T2R","1+1+1",0,16,"10us","0.04s-1","Type B",10.6,11.2,8.6300000000000008,10.63,null,null,null,null,8.6300000000000008,11.13,7.32,9.82,8.18,10.68,8.4,10.8,8.3000000000000007,10.8,{"$f":"MAX(P8,R8,T8,V8,X8,Z8,AB8,AD8)-MIN(P8,R8,T8,V8,X8,Z8,AB8,AD8)","v":1.3100000000000005},1.3100000000000005,8.5,10.643333333333333]
[null,null,"Enabled or Disabled","10MHz","30KHz","CP-OFDM","1T2R","1+1+1",2,16,"5us","0.08s-1","Type A",10.8,11.4,8.17,10.17,null,null,null,null,10.42,12.92,7.42,9.92,9.09,11.59,8.8000000000000007,11.3,8.6999999999999993,11.2,3,3,9.0966666666666658,11.183333333333332]
[null,null,null,"10MHz","30KHz","CP-OFDM","1T2R","1+1+1",0,16,"5us","0.08s-1","Type B",10.7,11.299999999999999,8.15,10.15,null,null,null,null,10.29,12.79,7.42,9.92,8.9600000000000009,11.46,8.6999999999999993,10.8,8.8000000000000007,11.3,2.8699999999999992,2.8699999999999992,8.8339999999999996,11.07]

{"sheet":"PUSCH UL TA","index":6,"n_rows":18,"n_cols":35,"rows_kept":18,"cut":false,"hidden":false,"merged":[[10,0,13,0],[10,1,13,1],[10,2,11,2],[12,2,13,2],[14,0,17,0],[14,1,17,1],[14,2,15,2],[16,2,17,2],[0,13,1,13],[0,14,1,14],[0,15,0,16],[0,7,1,7],[0,31,0,32],[0,12,1,12],[0,9,1,9],[0,33,0,34],[2,0,5,0],[0,10,1,10],[0,11,1,11],[0,3,1,3],[0,17,0,18],[0,19,0,20],[0,21,0,22],[0,23,0,24],[0,25,0,26],[0,27,0,28],[0,6,1,6],[0,8,1,8],[0,29,0,30],[2,2,3,2],[4,2,5,2],[0,0,1,0],[0,1,1,1],[0,2,1,2],[0,4,1,4],[0,5,1,5],[6,0,9,0],[6,1,9,1],[6,2,7,2],[8,2,9,2],[2,1,5,1]]}
["Scenario","PUSCH transmission","SRS transmission","CBW","SCS","Waveform","Tx/Rx","DMRS","l0","MCS","A","Δω","PUSCH mapping type","38.104 req","38.141 req","Samsung",null,"ZTE",null,"CMCC",null,"CATT",null,"Nokia",null,"Huawei",null,"Ericsson",null,"Intel",null,"SPAN",null,"AVERAGE"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment"]
["Scenario Y","FDD or  TDD","Enabled or Disabled","10MHz","15KHz","CP-OFDM","1T2R","1+1+1",2,16,"10us","0.13s-1","Type A",{"$f":"DerivingPerfReq(P3:AE3)","v":8.5},{"$f":"IF(N3>-100,N3+0.3,N3)","v":8.8000000000000007},6.79,8.7899999999999991,6.75,{"$f":"R3+2.5","v":9.25},null,null,5.8,8.3000000000000007,5.74,8.24,5.9,{"$f":"Z3+2","v":7.9},6,8.3000000000000007,null,null,{"$f":"MAX(P3,R3,T3,V3,X3,Z3,AB3,AD3)-MIN(P3,R3,T3,V3,X3,Z3,AB3,AD3)","v":1.0499999999999998},{"$f":"MAX(Q3,S3,U3,W3,Y3,AA3,AC3,AE3)-MIN(Q3,S3,U3,W3,Y3,AA3,AC3,AE3)","v":1.3499999999999996},{"$f":"AVERAGE(Q4,R3,T3,V3,X3,Z3,AB3,AD3)","v":6.4966666666666661},{"$f":"AVERAGE(Q3,S3,U3,W3,Y3,AA3,AC3,AE3)","v":8.4633333333333329}]
[null,null,null,"10MHz","15KHz","CP-OFDM","1T2R","1+1+1",0,16,"10us","0.13s-1","Type B",8.5,8.8000000000000007,6.79,8.7899999999999991,6.83,{"$f":"R4+2.5","v":9.33},null,null,5.78,8.2800000000000011,5.74,8.24,6.1,{"$f":"Z4+2","v":8.1},6,8.1999999999999993,null,null,{"$f":"MAX(P4,R4,T4,V4,X4,Z4,AB4,AD4)-MIN(P4,R4,T4,V4,X4,Z4,AB4,AD4)","v":1.0899999999999999},1.2300000000000004,{"$f":"AVERAGE(Q5,R4,T4,V4,X4,Z4,AB4,AD4)","v":6.4816666666666665},8.49]
[null,null,"Enabled or Disabled","40MHz","30KHz","CP-OFDM","1T2R","1+1+1",2,16,"5us","0.26s-1","Type A",8.4,8.7000000000000011,6.44,8.44,6.74,9.24,null,null,5.86,8.36,5.7,8.1999999999999993,6.03,8.0300000000000011,6,8.3000000000000007,null,null,1.04,1.2099999999999991,6.458333333333333,8.4283333333333328]
[null,null,null,"40MHz","30KHz","CP-OFDM","1T2R","1+1+1",0,16,"5us","0.26s-1","Type B",8.4,8.7000000000000011,6.42,8.42,6.76,9.26,null,null,5.84,8.34,5.69,8.1900000000000013,6.25,8.25,6,8.1,null,null,1.0699999999999994,1.1600000000000001,6.5133333333333328,8.4266666666666676]
["Scenario Z","FDD or  TDD","Enabled or Disabled","10MHz","15KHz","CP-OFDM","1T2R","1+1+1",2,16,"10us","0.18s-1","Type A",{"$f":"DerivingPerfReq(P7:AE7)","v":8.4},{"$f":"IF(N7>-100,N7+0.3,N7)","v":8.7000000000000011},6.54,8.5399999999999991,6.71,9.2100000000000009,null,null,5.81,8.3099999999999987,5.7,8.1999999999999993,6.01,8.01,6,8.1999999999999993,null,null,1.0099999999999998,{"$f":"MAX(Q7,S7,U7,W7,Y7,AA7,AC7,AE7)-MIN(Q7,S7,U7,W7,Y7,AA7,AC7,AE7)","v":1.2000000000000011},6.46,{"$f":"AVERAGE(Q7,S7,U7,W7,Y7,AA7,AC7,AE7)","v":8.4116666666666671}]
[null,null,null,"10MHz","15KHz","CP-OFDM","1T2R","1+1+1",0,16,"10us","0.18s-1","Type B",{"$f":"DerivingPerfReq(P8:AE8)","v":8.5},{"$f":"IF(N8>-100,N8+0.3,N8)","v":8.8000000000000007},6.53,8.5299999999999994,6.82,9.32,null,null,5.78,8.2800000000000011,5.69,8.19,6.22,8.2199999999999989,6,8.4,null,null,1.1299999999999999,1.1300000000000008,6.5066666666666668,8.49]
[null,null,"Enabled or Disabled","40MHz","30KHz","CP-OFDM","1T2R","1+1+1",2,16,"5us","0.36s-1","Type A",8.5,8.8000000000000007,6.53,8.5299999999999994,6.72,{"$f":"R9+2.5","v":9.2199999999999989},null,null,5.86,8.36,5.67,8.17,6.04,8.0399999999999991,6,8.5,null,null,1.0499999999999998,1.1799999999999997,6.47,8.4700000000000006]
[null,null,null,"40MHz","30KHz","CP-OFDM","1T2R","1+1+1",0,16,"5us","0.36s-1","Type B",8.5,8.8000000000000007,6.53,8.5299999999999994,6.73,{"$f":"R10+2.5","v":9.23},null,null,5.84,8.34,5.67,8.17,6.26,8.26,6,8.5,null,null,1.0600000000000005,1.0600000000000005,6.4733333333333327,8.504999999999999]
["Scenario Y","FDD or  TDD","Enabled or Disabled","5MHz","15KHz","CP-OFDM","1T2R","1+1+1",2,16,"10us","0.13s-1","Type A",8.1999999999999993,8.5,6.34,8.34,null,null,null,null,6.2,8.6999999999999993,5.56,8.06,5.57,{"$f":"Z11+2","v":7.57},6,8.1,6.1,8.6,{"$f":"MAX(P11,R11,T11,V11,X11,Z11,AB11,AD11)-MIN(P11,R11,T11,V11,X11,Z11,AB11,AD11)","v":0.78000000000000025},1.129999999999999,6.291666666666667,8.2283333333333335]
[null,null,null,"5MHz","15KHz","CP-OFDM","1T2R","1+1+1",0,16,"10us","0.13s-1","Type B",8.3000000000000007,8.6000000000000014,6.32,8.32,null,null,null,null,6.17,8.67,5.56,8.06,5.87,{"$f":"Z12+2","v":7.87},6,8.4,6.1,8.6,{"$f":"MAX(P12,R12,T12,V12,X12,Z12,AB12,AD12)-MIN(P12,R12,T12,V12,X12,Z12,AB12,AD12)","v":0.76000000000000068},0.79999999999999982,6.3366666666666669,8.32]
[null,null,"Enabled or Disabled","10MHz","30KHz","CP-OFDM","1T2R","1+1+1",2,16,"5us","0.26s-1","Type A",8.3000000000000007,8.6000000000000014,6.34,8.32,null,null,null,null,6.2,8.6999999999999993,5.56,8.06,5.67,7.67,6,8.1999999999999993,6.1,8.6,0.78000000000000025,1.0299999999999994,6.3083333333333336,8.2583333333333346]
[null,null,null,"10MHz","30KHz","CP-OFDM","1T2R","1+1+1",0,16,"5us","0.26s-1","Type B",8.3000000000000007,8.6000000000000014,6.32,8.32,null,null,null,null,6.18,8.68,5.56,8.06,5.97,7.97,6,8.1,6.1,8.6,0.76000000000000068,0.71,6.3583333333333334,8.288333333333334]
["Scenario Z","FDD or  TDD","Enabled or Disabled","5MHz","15KHz","CP-OFDM","1T2R","1+1+1",2,16,"10us","0.18s-1","Type A",{"$f":"DerivingPerfReq(P15:AE15)","v":8.3000000000000007},{"$f":"IF(N15>-100,N15+0.3,N15)","v":8.6000000000000014},6.34,8.34,null,null,null,null,6.28,8.7800000000000011,5.57,8.07,5.57,7.57,6,8.3000000000000007,6.1,8.6,0.76999999999999957,{"$f":"MAX(Q15,S15,U15,W15,Y15,AA15,AC15,AE15)-MIN(Q15,S15,U15,W15,Y15,AA15,AC15,AE15)","v":1.2100000000000009},6.3083333333333336,{"$f":"AVERAGE(Q15,S15,U15,W15,Y15,AA15,AC15,AE15)","v":8.2766666666666673}]
[null,null,null,"5MHz","15KHz","CP-OFDM","1T2R","1+1+1",0,16,"10us","0.18s-1","Type B",{"$f":"DerivingPerfReq(P16:AE16)","v":8.3000000000000007},8.6000000000000014,6.33,8.33,null,null,null,null,6.25,8.75,5.57,8.07,5.87,7.87,6,8.1999999999999993,6.1,8.6,0.75999999999999979,0.87999999999999989,6.3550000000000004,8.3033333333333328]
[null,null,"Enabled or Disabled","10MHz","30KHz","CP-OFDM","1T2R","1+1+1",2,16,"5us","0.36s-1","Type A",8.3000000000000007,8.6000000000000014,6.34,8.34,null,null,null,null,6.27,8.77,5.57,8.07,5.67,7.67,6,8.1999999999999993,6.1,8.6,0.76999999999999957,1.0999999999999996,6.3233333333333341,8.2750000000000004]
[null,null,null,"10MHz","30KHz","CP-OFDM","1T2R","1+1+1",0,16,"5us","0.36s-1","Type B",8.4,8.7000000000000011,6.33,8.33,null,null,null,null,6.25,8.75,5.57,8.07,5.97,7.97,6,8.5,6.1,8.6,0.75999999999999979,0.78000000000000025,5.9779999999999998,8.3699999999999992]

{"sheet":"PRACH format0 Type A fading","index":7,"n_rows":5,"n_cols":33,"rows_kept":5,"cut":false,"hidden":false,"merged":[[0,5,1,5],[0,0,1,0],[0,1,1,1],[0,2,1,2],[0,3,1,3],[0,4,1,4],[0,21,0,22],[0,6,1,6],[0,7,1,7],[0,8,1,8],[0,9,1,9],[0,10,1,10],[0,11,1,11],[0,12,1,12],[0,13,0,14],[0,15,0,16],[0,17,0,18],[0,19,0,20],[0,23,0,24],[0,25,0,26],[0,27,0,28],[0,29,0,30],[0,31,0,32]]}
["Format","SCS","Restricted set type","Ncs","Logical sequence index","v","Tx/Rx","Carrier frequency(GHz)","Propagation condition","Frequency offset (Hz)","Timing error tolerance","38.104 req","38.141 req","Samsung",null,"ZTE",null,"CMCC",null,"CATT",null,"Nokia",null,"Huawei",null,"Ericsson",null,"Intel",null,"SPAN",null,"AVERAGE"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment"]
["Format 0","1.25kHz","Type A",15,384,0,"1T2R",2.1,"TDLC300-100",0,"2.55us",{"$f":"DerivingPerfReq(N3:AC3)","v":-6.4},{"$f":"IF(L3>-100,L3+0.6,L3)","v":-5.8000000000000007},-8.3800000000000008,-6.38,null,null,null,null,-8.8000000000000007,-6.8000000000000007,-7.87,-5.37,-9.3000000000000007,-7.3,-8.9,-6.4,-8.8000000000000007,-6.3,{"$f":"MAX(N3,P3,R3,T3,V3,X3,Z3,AB3)-MIN(N3,P3,R3,T3,V3,X3,Z3,AB3)","v":1.4300000000000006},1.9299999999999997,{"$f":"AVERAGE(N3,P3,R3,T3,V3,X3,Z3,AB3)","v":-8.6749999999999989},-6.4249999999999998]
["Format 0","1.25kHz","Type A",15,384,0,"1T4R",2.1,"TDLC300-100",0,"2.55us",-11.9,{"$f":"IF(L4>-100,L4+0.6,L4)","v":-11.3},-13.84,-11.84,null,null,null,null,-14.14,-12.14,-13.14,-10.64,-14.9,-12.9,-14.3,-11.8,-14.5,-12,1.7599999999999998,2.2599999999999998,-14.136666666666668,-11.886666666666668]
["Format 0","1.25kHz","Type A",15,384,0,"1T8R",2.1,"TDLC300-100",0,"2.55us",{"$f":"DerivingPerfReq(N5:AC5)","v":-16.399999999999999},{"$f":"IF(L5>-100,L5+0.6,L5)","v":-15.799999999999999},-18.18,-16.18,null,null,null,null,-16.04,-14.04,-17.05,-14.55,-19.2,-17.2,-18.399999999999999,-15.9,-18.899999999999999,-16.399999999999999,{"$f":"MAX(N5,P5,R5,T5,V5,X5,Z5,AB5)-MIN(N5,P5,R5,T5,V5,X5,Z5,AB5)","v":3.16},{"$f":"MAX(O5,Q5,S5,U5,W5,Y5,AA5,AC5)-MIN(O5,Q5,S5,U5,W5,Y5,AA5,AC5)","v":3.16},{"$f":"AVERAGE(N5,P5,R5,T5,V5,X5,Z5,AB5)","v":-17.96166666666667},{"$f":"AVERAGE(O5,Q5,S5,U5,W5,Y5,AA5,AC5)","v":-15.711666666666668}]

{"sheet":"PRACH format0 Type B fading","index":8,"n_rows":5,"n_cols":33,"rows_kept":5,"cut":false,"hidden":false,"merged":[[0,5,1,5],[0,0,1,0],[0,1,1,1],[0,2,1,2],[0,3,1,3],[0,4,1,4],[0,21,0,22],[0,6,1,6],[0,7,1,7],[0,8,1,8],[0,9,1,9],[0,10,1,10],[0,11,1,11],[0,12,1,12],[0,13,0,14],[0,15,0,16],[0,17,0,18],[0,19,0,20],[0,23,0,24],[0,25,0,26],[0,27,0,28],[0,29,0,30],[0,31,0,32]]}
["Format","SCS","Restricted set type","Ncs","Logical sequence index","v","Tx/Rx","Carrier frequency(GHz)","Propagation condition","Frequency offset (Hz)","Timing error tolerance","38.104 req","38.141 req","Samsung",null,"ZTE",null,"CMCC",null,"CATT",null,"Nokia",null,"Huawei",null,"Ericsson",null,"Intel",null,"SPAN",null,"AVERAGE"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment"]
["Format 0","1.25kHz","Type B",15,30,30,"1T2R",3.6,"TDLC300-100",0,"2.55us",{"$f":"DerivingPerfReq(N3:AC3)","v":-6.1},{"$f":"IF(L3>-100,L3+0.6,L3)","v":-5.5},-8.25,-6.25,null,null,null,null,-8.16,-6.16,-7.36,-4.8600000000000003,-9,-7,-8.8000000000000007,-6.3,-8.6999999999999993,-6.2,{"$f":"MAX(N3,P3,R3,T3,V3,X3,Z3,AB3)-MIN(N3,P3,R3,T3,V3,X3,Z3,AB3)","v":1.6399999999999997},2.1399999999999997,{"$f":"AVERAGE(N3,P3,R3,T3,V3,X3,Z3,AB3)","v":-8.3783333333333321},-6.1283333333333339]
["Format 0","1.25kHz","Type B",15,30,30,"1T4R",3.6,"TDLC300-100",0,"2.55us",{"$f":"DerivingPerfReq(N4:AC4)","v":-11.8},{"$f":"IF(L4>-100,L4+0.6,L4)","v":-11.200000000000001},-13.74,-11.74,null,null,null,null,-13.46,-11.46,-12.35,-9.85,-14.5,-12.5,-14.1,-11.6,-14.4,-11.9,2.1500000000000004,2.6500000000000004,-13.758333333333335,-11.508333333333335]
["Format 0","1.25kHz","Type B",15,30,30,"1T8R",3.6,"TDLC300-100",0,"2.55us",-16.2,{"$f":"IF(L5>-100,L5+0.6,L5)","v":-15.6},-18.079999999999998,-16.079999999999998,null,null,null,null,-15.86,-13.86,-16.329999999999998,-13.83,-18.8,-16.8,-18.2,-15.7,-18.8,-16.3,2.9400000000000013,2.9700000000000006,-17.678333333333331,-15.428333333333333]

{"sheet":"PRACH 1.25kHz SCS Type A","index":9,"n_rows":8,"n_cols":33,"rows_kept":8,"cut":false,"hidden":false,"merged":[[0,0,1,0],[0,1,1,1],[0,6,1,6],[0,7,1,7],[0,11,1,11],[0,3,1,3],[0,4,1,4],[0,5,1,5],[0,2,1,2],[0,10,1,10],[0,29,0,30],[0,31,0,32],[0,8,1,8],[0,9,1,9],[0,15,0,16],[0,17,0,18],[0,19,0,20],[0,21,0,22],[0,23,0,24],[0,25,0,26],[0,13,0,14],[0,12,1,12],[0,27,0,28]]}
["Format","SCS","Restricted set type","Ncs","Logical sequence index","v","Tx/Rx","Carrier frequency(GHz)","Propagation condition","Frequency offset (Hz)","Timing error tolerance","38.104 req","38.141 req","Samsung",null,"ZTE",null,"CMCC",null,"CATT",null,"Nokia",null,"Huawei",null,"Ericsson",null,"Intel",null,"SPAN",null,"AVERAGE"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment"]
["Format 0","1.25kHz","Type A",15,384,0,"1T2R",2.1,"AWGN",625,"1.04us",{"$f":"DerivingPerfReq(N3:AC3)","v":-12},{"$f":"IF(L3>-100,L3+0.3,L3)","v":-11.7},-14.36,-12.36,-16.5,-13.5,null,null,-13.75,-11.75,-14.56,-12.06,-14.11,-12.11,-14.3,-12,-14.3,-11.8,{"$f":"MAX(N3,P3,R3,T3,V3,X3,Z3,AB3)-MIN(N3,P3,R3,T3,V3,X3,Z3,AB3)","v":2.75},{"$f":"MAX(O3,Q3,S3,U3,W3,Y3,AA3,AC3)-MIN(O3,Q3,S3,U3,W3,Y3,AA3,AC3)","v":1.75},{"$f":"AVERAGE(N3,P3,R3,T3,V3,X3,Z3,AB3)","v":-14.554285714285713},{"$f":"AVERAGE(O3,Q3,S3,U3,W3,Y3,AA3,AC3)","v":-12.225714285714286}]
["Format 0","1.25kHz","Type A",15,384,0,"1T2R",2.1,"AWGN",1340,"1.04us",{"$f":"DerivingPerfReq(N4:AC4)","v":-13.8},-13.5,-16.09,-14.09,-16.5,-13.5,null,null,-16.350000000000001,-14.350000000000001,-15.2,-12.7,-16.55,-14.55,-15.5,-13.4,-16.5,-14,{"$f":"MAX(N4,P4,R4,T4,V4,X4,Z4,AB4)-MIN(N4,P4,R4,T4,V4,X4,Z4,AB4)","v":1.3500000000000014},{"$f":"MAX(O4,Q4,S4,U4,W4,Y4,AA4,AC4)-MIN(O4,Q4,S4,U4,W4,Y4,AA4,AC4)","v":1.8500000000000014},{"$f":"AVERAGE(N4,P4,R4,T4,V4,X4,Z4,AB4)","v":-16.098571428571429},{"$f":"AVERAGE(O4,Q4,S4,U4,W4,Y4,AA4,AC4)","v":-13.79857142857143}]
["Format 0","1.25kHz","Type A",15,384,0,"1T4R",2.1,"AWGN",625,"1.04us",-14.5,-14.2,-16.77,-14.77,-18.899999999999999,-15.899999999999999,null,null,-16.079999999999998,-14.079999999999998,-16.87,-14.370000000000001,-17.02,-15.02,-16.7,-14.5,-16.5,-14,2.8200000000000003,1.8999999999999986,-16.977142857142859,-14.662857142857144]
["Format 0","1.25kHz","Type A",15,384,0,"1T4R",2.1,"AWGN",1340,"1.04us",-16.2,-15.899999999999999,-18.54,-16.54,-18.899999999999999,-15.899999999999999,null,null,-18.760000000000002,-16.760000000000002,-17.510000000000002,-15.010000000000002,-19.41,-17.41,-17.899999999999999,-15.4,-18.8,-16.3,1.8999999999999986,2.3999999999999986,-18.54571428571429,-16.188571428571429]
["Format 0","1.25kHz","Type A",15,384,0,"1T8R",2.1,"AWGN",625,"1.04us",-16.5,-16.2,-19.09,-17.09,-21.4,-18.399999999999999,null,null,-18.12,-16.12,-18.96,-16.46,-18.82,-16.82,-18.899999999999999,-16.399999999999999,-18.7,-16.2,3.2799999999999976,2.2799999999999976,-19.14142857142857,-16.784285714285712]
["Format 0","1.25kHz","Type A",15,384,0,"1T8R",2.1,"AWGN",1340,"1.04us",-18.399999999999999,-18.099999999999998,-20.99,-18.989999999999998,-21.4,-18.399999999999999,null,null,-20.53,-18.53,-19.62,-17.12,-21.41,-19.41,-20.100000000000001,-17.7,-21.1,-18.600000000000001,1.7899999999999991,2.2899999999999991,-20.735714285714288,-18.392857142857142]

{"sheet":"PRACH 1.25kHz SCS Type B","index":10,"n_rows":8,"n_cols":33,"rows_kept":8,"cut":false,"hidden":false,"merged":[[0,5,1,5],[0,0,1,0],[0,1,1,1],[0,2,1,2],[0,3,1,3],[0,4,1,4],[0,6,1,6],[0,7,1,7],[0,8,1,8],[0,9,1,9],[0,11,1,11],[0,25,0,26],[0,29,0,30],[0,31,0,32],[0,10,1,10],[0,13,0,14],[0,15,0,16],[0,17,0,18],[0,19,0,20],[0,21,0,22],[0,23,0,24],[0,12,1,12],[0,27,0,28]]}
["Format","SCS","Restricted set type","Ncs","Logical sequence index","v","Tx/Rx","Carrier frequency(GHz)","Propagation condition","Frequency offset (Hz)","Timing error tolerance","38.104 req","38.141 req","Samsung",null,"ZTE",null,"CMCC",null,"CATT",null,"Nokia",null,"Huawei",null,"Ericsson",null,"Intel",null,"SPAN",null,"AVERAGE"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment"]
["Format 0","1.25kHz","Type B",15,30,30,"1T2R",3.6,"AWGN",625,"1.04us",{"$f":"DerivingPerfReq(N3:AC3)","v":-11.6},{"$f":"IF(L3>-100,L3+0.3,L3)","v":-11.299999999999999},-13.92,-11.92,-16.399999999999999,-13.399999999999999,null,null,-12.86,-10.86,-14.16,-11.66,-14.27,-12.27,-15.7,-13.6,-14,-11.5,{"$f":"MAX(N3,P3,R3,T3,V3,X3,Z3,AB3)-MIN(N3,P3,R3,T3,V3,X3,Z3,AB3)","v":3.5399999999999991},{"$f":"MAX(O3,Q3,S3,U3,W3,Y3,AA3,AC3)-MIN(O3,Q3,S3,U3,W3,Y3,AA3,AC3)","v":2.74},{"$f":"AVERAGE(N3,P3,R3,T3,V3,X3,Z3,AB3)","v":-14.472857142857142},{"$f":"AVERAGE(O3,Q3,S3,U3,W3,Y3,AA3,AC3)","v":-12.172857142857142}]
["Format 0","1.25kHz","Type B",15,30,30,"1T2R",3.6,"AWGN",2334,"1.04us",{"$f":"DerivingPerfReq(N4:AC4)","v":-13.1},{"$f":"IF(L4>-100,L4+0.3,L4)","v":-12.799999999999999},-15.8,-13.8,-16.399999999999999,-13.399999999999999,null,null,-15.51,-13.51,-14.61,-12.11,-14.87,-12.87,-14.4,-11.9,-16.3,-13.8,{"$f":"MAX(N4,P4,R4,T4,V4,X4,Z4,AB4)-MIN(N4,P4,R4,T4,V4,X4,Z4,AB4)","v":1.9999999999999982},{"$f":"MAX(O4,Q4,S4,U4,W4,Y4,AA4,AC4)-MIN(O4,Q4,S4,U4,W4,Y4,AA4,AC4)","v":1.9000000000000004},{"$f":"AVERAGE(N4,P4,R4,T4,V4,X4,Z4,AB4)","v":-15.412857142857144},{"$f":"AVERAGE(O4,Q4,S4,U4,W4,Y4,AA4,AC4)","v":-13.055714285714286}]
["Format 0","1.25kHz","Type B",15,30,30,"1T4R",3.6,"AWGN",625,"1.04us",-14,-13.7,-16.309999999999999,-14.31,-18.100000000000001,-15.100000000000001,null,null,-15.33,-13.33,-16.34,-13.84,-16.649999999999999,-14.65,-17.899999999999999,-15.7,-16.3,-13.8,2.7700000000000014,2.3699999999999992,-16.704285714285714,-14.39]
["Format 0","1.25kHz","Type B",15,30,30,"1T4R",3.6,"AWGN",2334,"1.04us",-15.4,-15.1,-18.28,-16.28,-18.100000000000001,-15.100000000000001,null,null,-18.010000000000002,-16.010000000000002,-16.72,-14.219999999999999,-17.63,-15.63,-16.7,-14.6,-18.5,-16,1.8000000000000007,2.0600000000000023,-17.705714285714286,-15.405714285714284]
["Format 0","1.25kHz","Type B",15,30,30,"1T8R",3.6,"AWGN",625,"1.04us",-16.3,-16,-18.55,-16.55,-19.5,-16.5,null,null,-17.34,-15.34,-18.32,-15.82,-18.63,-16.63,-20.100000000000001,-17.7,-18.399999999999999,-15.9,2.7600000000000016,2.3599999999999994,-18.69142857142857,-16.348571428571429]
["Format 0","1.25kHz","Type B",15,30,30,"1T8R",3.6,"AWGN",2334,"1.04us",-17.399999999999999,-17.099999999999998,-20.63,-18.63,-19.5,-16.5,null,null,-19.78,-17.78,-18.73,-16.23,-19.89,-17.89,-18.899999999999999,-16.899999999999999,-20.7,-18.2,1.9699999999999989,2.3999999999999986,-19.732857142857142,-17.447142857142858]

{"sheet":"PRACH 15kHz SCS","index":11,"n_rows":11,"n_cols":32,"rows_kept":11,"cut":false,"hidden":false,"merged":[[0,10,1,10],[0,0,1,0],[0,1,1,1],[0,2,1,2],[0,3,1,3],[0,4,1,4],[0,5,1,5],[0,6,1,6],[0,7,1,7],[0,8,1,8],[0,9,1,9],[0,22,0,23],[0,24,0,25],[0,28,0,29],[0,30,0,31],[0,11,1,11],[0,12,0,13],[0,14,0,15],[0,16,0,17],[0,18,0,19],[0,20,0,21],[0,26,0,27]]}
["Format","SCS","Ncs","Logical sequence index","v","Tx/Rx","Carrier frequency(GHz)","Propagation condition","Frequency offset (Hz)","Timing error tolerance","38.104 req","38.141 req","Samsung",null,"ZTE",null,"CMCC",null,"CATT",null,"Nokia",null,"Huawei",null,"Ericsson",null,"Intel",null,"SPAN",null,"AVERAGE"]
[null,null,null,null,null,null,null,null,null,null,null,null,"Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment"]
["Format A2","15kHz",23,0,0,"1T2R",1.8,"AWGN",1740,"0.52us ",{"$f":"DerivingPerfReq(M3:AB3)","v":-11.3},{"$f":"IF(K3>-100,K3+0.3,K3)","v":-11},-13.23,-11.23,-13.7,-10.7,null,null,-13.29,-11.29,-11.48,-8.98,-13.66,-11.66,-13.8,-11.4,-13.9,-11.4,{"$f":"MAX(M3,O3,Q3,S3,U3,W3,Y3,AA3)-MIN(M3,O3,Q3,S3,U3,W3,Y3,AA3)","v":2.42},{"$f":"MAX(N3,P3,R3,T3,V3,X3,Z3,AB3)-MIN(N3,P3,R3,T3,V3,X3,Z3,AB3)","v":2.6799999999999997},{"$f":"AVERAGE(M3,O3,Q3,S3,U3,W3,Y3,AA3)","v":-13.294285714285715},{"$f":"AVERAGE(N3,P3,R3,T3,V3,X3,Z3,AB3)","v":-10.951428571428574}]
["Format B4","15kHz",23,0,0,"1T2R",1.8,"AWGN",1740,"0.52us ",{"$f":"DerivingPerfReq(M4:AB4)","v":-14.3},-14,-16.73,-14.73,-17.100000000000001,-14.100000000000001,null,null,-16.510000000000002,-14.510000000000002,-15.58,-13.08,-17.149999999999999,-15.15,-16.399999999999999,-14.1,-16.899999999999999,-14.4,{"$f":"MAX(M4,O4,Q4,S4,U4,W4,Y4,AA4)-MIN(M4,O4,Q4,S4,U4,W4,Y4,AA4)","v":1.5699999999999985},{"$f":"MAX(N4,P4,R4,T4,V4,X4,Z4,AB4)-MIN(N4,P4,R4,T4,V4,X4,Z4,AB4)","v":2.0700000000000003},{"$f":"AVERAGE(M4,O4,Q4,S4,U4,W4,Y4,AA4)","v":-16.624285714285715},{"$f":"AVERAGE(N4,P4,R4,T4,V4,X4,Z4,AB4)","v":-14.295714285714286}]
["Format C2","15kHz",23,0,0,"1T2R",1.8,"AWGN",1740,"0.52us ",-11.1,-10.799999999999999,-13.25,-11.25,-13.7,-10.7,null,null,-13.31,-11.31,-11.51,-9.01,-13.63,-11.63,-13.1,-10.6,-13.9,-11.4,2.3900000000000006,2.620000000000001,-13.2,-10.842857142857143]
["Format A2","15kHz",23,0,0,"1T4R",1.8,"AWGN",1740,"0.52us ",-13.5,{"$f":"IF(K6>-100,K6+0.3,K6)","v":-13.2},-15.47,-13.47,-15.9,-12.9,null,null,-15.32,-13.32,-13.89,-11.39,-15.89,-13.89,-16.100000000000001,-13.6,-16.100000000000001,-13.6,2.2100000000000009,2.5,-15.524285714285712,-13.167142857142855]
["Format B4","15kHz",23,0,0,"1T4R",1.8,"AWGN",1740,"0.52us ",-16.7,-16.399999999999999,-18.84,-16.84,-19.8,-16.8,null,null,-18.489999999999998,-16.489999999999998,-17.600000000000001,-15.100000000000001,-19.309999999999999,-17.309999999999999,-18.7,-16.5,-18.899999999999999,-16.399999999999999,2.1999999999999993,2.2099999999999973,-18.805714285714284,-16.491428571428571]
["Format C2","15kHz",23,0,0,"1T4R",1.8,"AWGN",1740,"0.52us ",-13.4,-13.1,-15.48,-13.48,-16,-13,null,null,-15.34,-13.34,-13.89,-11.39,-15.82,-13.82,-15.5,-13.2,-16.100000000000001,-13.6,2.2100000000000009,2.4299999999999997,-15.447142857142856,-13.118571428571428]
["Format A2","15kHz",23,0,0,"1T8R",1.8,"AWGN",1740,"0.52us ",-15.6,{"$f":"IF(K9>-100,K9+0.3,K9)","v":-15.299999999999999},-17.59,-15.59,-18.100000000000001,-15.100000000000001,null,null,-17.350000000000001,-15.350000000000001,-15.51,-13.01,-17.96,-15.96,-18.3,-16,-18.2,-15.7,2.7900000000000009,2.99,-17.572857142857142,-15.244285714285715]
["Format B4","15kHz",23,0,0,"1T8R",1.8,"AWGN",1740,"0.52us ",-18.2,-17.899999999999999,-20.8,-18.8,-20.399999999999999,-17.399999999999999,null,null,-20.260000000000002,-18.260000000000002,-19.22,-16.72,-21.12,-19.12,-20.9,-18.600000000000001,-20.8,-18.3,1.9000000000000021,2.4000000000000021,-20.500000000000004,-18.171428571428571]
["Format C2","15kHz",23,0,0,"1T8R",1.8,"AWGN",1740,"0.52us ",-15.5,-15.2,-17.53,-15.53,-18,-15,null,null,-17.329999999999998,-15.329999999999998,-15.5,-13,-17.89,-15.89,-17.600000000000001,-15.5,-18.2,-15.7,{"$f":"MAX(M11,O11,Q11,S11,U11,W11,Y11,AA11)-MIN(M11,O11,Q11,S11,U11,W11,Y11,AA11)","v":2.6999999999999993},{"$f":"MAX(N11,P11,R11,T11,V11,X11,Z11,AB11)-MIN(N11,P11,R11,T11,V11,X11,Z11,AB11)","v":2.8900000000000006},{"$f":"AVERAGE(M11,O11,Q11,S11,U11,W11,Y11,AA11)","v":-17.435714285714287},{"$f":"AVERAGE(N11,P11,R11,T11,V11,X11,Z11,AB11)","v":-15.135714285714286}]

{"sheet":"PRACH 30kHz SCS","index":12,"n_rows":11,"n_cols":32,"rows_kept":11,"cut":false,"hidden":false,"merged":[[0,10,1,10],[0,0,1,0],[0,1,1,1],[0,2,1,2],[0,3,1,3],[0,4,1,4],[0,5,1,5],[0,6,1,6],[0,7,1,7],[0,8,1,8],[0,9,1,9],[0,22,0,23],[0,24,0,25],[0,28,0,29],[0,30,0,31],[0,11,1,11],[0,12,0,13],[0,14,0,15],[0,16,0,17],[0,18,0,19],[0,20,0,21],[0,26,0,27]]}
["Format","SCS","Ncs","Logical sequence index","v","Tx/Rx","Carrier frequency(GHz)","Propagation condition","Frequency offset (Hz)","Timing error tolerance","38.104 req","38.141 req","Samsung",null,"ZTE",null,"CMCC",null,"CATT",null,"Nokia",null,"Huawei",null,"Ericsson",null,"Intel",null,"SPAN",null,"AVERAGE"]
[null,null,null,null,null,null,null,null,null,null,null,null,"Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment"]
["Format A2","30kHz",46,0,0,"1T2R",3.6,"AWGN",3334,"0.26us",{"$f":"DerivingPerfReq(M3:AB3)","v":-11.2},{"$f":"IF(K3>-100,K3+0.3,K3)","v":-10.899999999999999},-13.1,-11.1,-14.8,-11.8,null,null,-13.19,-11.19,-13.54,-11.04,-13.42,-11.42,-13.7,-11.2,-13.4,-10.9,{"$f":"MAX(M3,O3,Q3,S3,U3,W3,Y3,AA3)-MIN(M3,O3,Q3,S3,U3,W3,Y3,AA3)","v":1.7000000000000011},{"$f":"MAX(N3,P3,R3,T3,V3,X3,Z3,AB3)-MIN(N3,P3,R3,T3,V3,X3,Z3,AB3)","v":0.90000000000000036},{"$f":"AVERAGE(M3,O3,Q3,S3,U3,W3,Y3,AA3)","v":-13.592857142857143},{"$f":"AVERAGE(N3,P3,R3,T3,V3,X3,Z3,AB3)","v":-11.235714285714286}]
["Format B4","30kHz",46,0,0,"1T2R",3.6,"AWGN",3334,"0.26us",{"$f":"DerivingPerfReq(M4:AB4)","v":-14.6},-14.299999999999999,-16.7,-14.7,-17.3,-14.3,null,null,-16.41,-14.41,-17.309999999999999,-14.809999999999999,-17.43,-15.43,-16.399999999999999,-14.4,-16.7,-14.2,{"$f":"MAX(M4,O4,Q4,S4,U4,W4,Y4,AA4)-MIN(M4,O4,Q4,S4,U4,W4,Y4,AA4)","v":1.0300000000000011},{"$f":"MAX(N4,P4,R4,T4,V4,X4,Z4,AB4)-MIN(N4,P4,R4,T4,V4,X4,Z4,AB4)","v":1.2300000000000004},{"$f":"AVERAGE(M4,O4,Q4,S4,U4,W4,Y4,AA4)","v":-16.892857142857146},{"$f":"AVERAGE(N4,P4,R4,T4,V4,X4,Z4,AB4)","v":-14.607142857142859}]
["Format C2","30kHz",46,0,0,"1T2R",3.6,"AWGN",3334,"0.26us",-11,-10.7,-13.13,-11.13,-13.8,-10.8,null,null,-13.19,-11.19,-13.55,-11.05,-13.66,-11.66,-13,-10.5,-13.4,-10.9,0.80000000000000071,1.1600000000000001,-13.39,-11.032857142857143]
["Format A2","30kHz",46,0,0,"1T4R",3.6,"AWGN",3334,"0.26us",-13.4,{"$f":"IF(K6>-100,K6+0.3,K6)","v":-13.1},-15.39,-13.39,-16,-13,null,null,-15.25,-13.25,-15.68,-13.18,-15.76,-13.76,-16.100000000000001,-13.9,-15.9,-13.4,0.85000000000000142,0.90000000000000036,-15.725714285714288,-13.411428571428573]
["Format B4","30kHz",46,0,0,"1T4R",3.6,"AWGN",3334,"0.26us",-16.7,-16.399999999999999,-18.739999999999998,-16.739999999999998,-20,-17,null,null,-18.329999999999998,-16.329999999999998,-19.260000000000002,-16.760000000000002,-19.510000000000002,-17.510000000000002,-18.600000000000001,-16.100000000000001,-18.8,-16.3,1.6700000000000017,1.4100000000000001,-19.034285714285716,-16.677142857142858]
["Format C2","30kHz",46,0,0,"1T4R",3.6,"AWGN",3334,"0.26us",-13.4,-13.1,-15.38,-13.38,-16,-13,null,null,-15.25,-13.25,-15.7,-13.2,-15.87,-13.87,-15.5,-13.5,-16,-13.5,0.75,0.86999999999999922,-15.671428571428573,-13.385714285714286]
["Format A2","30kHz",46,0,0,"1T8R",3.6,"AWGN",3334,"0.26us",-15.4,{"$f":"IF(K9>-100,K9+0.3,K9)","v":-15.1},-17.45,-15.45,-18.2,-15.2,null,null,-17.27,-15.27,-17.43,-14.93,-17.86,-15.86,-18.2,-15.8,-18.100000000000001,-15.6,0.92999999999999972,0.92999999999999972,-17.787142857142857,-15.444285714285714]
["Format B4","30kHz",46,0,0,"1T8R",3.6,"AWGN",3334,"0.26us",-18.399999999999999,-18.099999999999998,-20.65,-18.649999999999999,-20.100000000000001,-17.100000000000001,null,null,-20.2,-18.2,-20.8,-18.3,-21.49,-19.489999999999998,-20.8,-18.7,-20.6,-18.100000000000001,1.389999999999997,2.389999999999997,-20.662857142857142,-18.362857142857141]
["Format C2","30kHz",46,0,0,"1T8R",3.6,"AWGN",3334,"0.26us",-15.4,-15.1,-17.45,-15.45,-18.100000000000001,-15.100000000000001,null,null,-17.239999999999998,-15.239999999999998,-17.39,-14.89,-17.89,-15.89,-17.600000000000001,-15.6,-18.100000000000001,-15.6,0.86000000000000298,1,-17.681428571428569,-15.395714285714282]