**3GPP TSG-RAN WG4 Meeting #98-e R4-2103144**

**Electronic Meeting, 25 Jan – 5 Feb, 2021**

**Title:** LS to RAN2 on single-uplink operation in more than one band pair of a band combination

**Response to:**

**Release:** Rel-15

**Work Item:** NR\_newRAT-Core, LTE\_NR\_DC\_CA\_enh-Core

**Source:** RAN WG4

**To:** RAN WG2

**Cc:** -

**Contact Person:**

#### Name: Tsang-wei Yu

E-mail Address: ato.yu@mediatek.com

**Attachments:** -

**1. Overall Description:**

RAN4 would like to inform RAN2 that the UE capability *singleUL-Transmission* is reported per band combination and may not be sufficient for UE to indicate dual UL in one UL CC pair and single UL in another CC pair in one band combination. RAN4 agreed that it is left to RAN2 on whether and how to resolve this issue.

**2. To RAN WG1 and WG2 group.**

**ACTION:** RAN4 kindly ask RAN2 check above information and decide if any action is needed.

**3. Date of Next TSG-RAN WG4 Meetings:**

TSG RAN WG4 Meeting #98-e-bis 12 – 20 Apr 2021 E-meeting

TSG RAN WG4 Meeting #99-e 19 – 27 May 2021 E-meeting