{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["TDoc_List","CR_Packs_List","Parameters"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":6,"comments":1,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"TDoc_List","index":0,"n_rows":158,"n_cols":31,"rows_kept":158,"cut":false,"hidden":false,"merged":[]}
["TDoc","Title","Source","Contact","Contact ID","Type","For","Abstract","Secretary Remarks","Agenda item sort order","Agenda item","Agenda item description","TDoc sort order within agenda item","TDoc Status","Reservation date","Uploaded","Is revision of","Revised to","Release","Spec","Version","Related WIs","CR","CR revision","CR category","TSG CR Pack","Reply to","To","Cc","Original LS","Reply in"]
["R6-170001","Draft Agenda for TSG RAN WG6#3","ETSI","Paolino Usai","3209","agenda","Approval","","","2","2","Approval of the agenda",0,"approved","2017-01-20T17:22:41.327","2017-01-20T17:23:25.333","","","","","","","","","","","","","","",""]
["R6-170002","Provisioning of a Multilateration timer to the SGSN","Ericsson LM","Nicklas Johansson","47575","discussion","Discussion","","","15","6.1.1","Core aspects (WI code: ePOS_GERAN-Core)",0,"noted","2017-02-01T19:57:10.667","2017-02-03T13:59:12.700","","","","","","ePOS_GERAN-Core","","","","","","","","",""]
["R6-170003","PS domain transport","Ericsson LM","Nicklas Johansson","47575","discussion","Discussion","","","15","6.1.1","Core aspects (WI code: ePOS_GERAN-Core)",0,"revised","2017-02-01T19:59:30.847","2017-02-03T13:59:12.700","","R6-170089","","","","ePOS_GERAN-Core","","","","","","","","",""]
["R6-170004","Analysis of MS Transmission Accuracy","Ericsson LM","Nicklas Johansson","47575","discussion","Discussion","","","16","6.1.2","Performance aspects (WI code: ePOS_GERAN-Perf)",0,"noted","2017-02-01T20:01:16.597","2017-02-03T13:59:12.653","","","","","","ePOS_GERAN-Perf","","","","","","","","",""]
["R6-170005","Compact burst mapping","Ericsson LM","Nicklas Johansson","47575","discussion","Discussion","","","19","6.3.1","Core aspects (WI code: CIoT_EC_GSM_radio_enh-Core)",0,"noted","2017-02-01T20:06:33.803","2017-02-03T13:59:12.653","","","","","","CIoT_EC_GSM_radio_enh-Core","","","","","","","","",""]
["R6-170006","DECOR - work item summary","Ericsson LM","Nicklas Johansson","47575","other","Agreement","","","17","6.2","Dedicated core networks for GERAN (WI code: DECOR_GERAN)",0,"agreed","2017-02-01T20:09:10.113","2017-02-03T13:59:12.670","","","","","","DECOR_GERAN-Core","","","","","","","","",""]
["R6-170007","Minutes of Meeting: Telco#1 on Positioning enhancements for GERAN","Ericsson LM","Nicklas Johansson","47575","other","","","","15","6.1.1","Core aspects (WI code: ePOS_GERAN-Core)",0,"noted","2017-02-01T20:11:13.883","2017-02-03T13:59:12.670","","","","","","ePOS_GERAN-Core","","","","","","","","",""]
["R6-170008","CR 43.059-0081 rev 4 Introduction of Multilateration (Rel-14)","Ericsson LM","Nicklas Johansson","47575","CR","Approval","","Merge with R6-170048 and revised into R6-170091.","15","6.1.1","Core aspects (WI code: ePOS_GERAN-Core)",0,"revised","2017-02-01T20:46:24.910","2017-02-03T13:59:12.670","R6-160263","R6-170091","Rel-14","43.059","13.2.0","ePOS_GERAN-Core","0081","4","B","","","","","",""]
["R6-170009","Introduction of Timing Advance Multilateration","Ericsson LM","Nicklas Johansson","47575","draftCR","Endorsement","","","15","6.1.1","Core aspects (WI code: ePOS_GERAN-Core)",0,"revised","2017-02-01T20:49:38.377","2017-02-03T13:59:12.670","","R6-170104","Rel-14","24.008","14.2.0","ePOS_GERAN-Core","","","B","","","","","",""]
["R6-170010","Positioning enhancements for GERAN - Workplan Agreements","Ericsson LM","Nicklas Johansson","47575","other","","","","15","6.1.1","Core aspects (WI code: ePOS_GERAN-Core)",0,"revised","2017-02-01T20:51:48.497","2017-02-03T13:59:12.687","","R6-170145","Rel-14","","","ePOS_GERAN-Core","","","","","","","","",""]
["R6-170011","8PSK performance for EC-GSM-IoT BTS – removal of brackets","Ericsson LM, Nokia","Nicklas Johansson","47575","CR","Agreement","","","10","5.2","Extended Coverage GSM for support of Cellular Internet of Things (WI codes: CIoT_EC_GSM-Core, CIoT_EC_GSM-Perf)",0,"agreed","2017-02-01T20:54:58.627","2017-02-03T13:59:12.687","","","Rel-13","45.005","13.3.0","CIoT_EC_GSM-Perf","0596","","F","RP-170064","","","","",""]
["R6-170012","BTS sensitivity performance requirements for Overlaid CDMA – removal of brackets","Ericsson LM, Nokia","Nicklas Johansson","47575","CR","Agreement","","","10","5.2","Extended Coverage GSM for support of Cellular Internet of Things (WI codes: CIoT_EC_GSM-Core, CIoT_EC_GSM-Perf)",0,"agreed","2017-02-01T21:01:15.003","2017-02-03T13:59:12.687","","","Rel-13","45.005","13.3.0","CIoT_EC_GSM-Perf","0597","","F","RP-170064","","","","",""]
["R6-170013","BSIC Confirmation Clarification","Ericsson Inc.","John Diachina","25840","CR","Approval","For PEO and EC operation there is an unecessary requirement for BSIC to be confirmed by the MS using the strongest cell.","","9","5.1","Extended DRX for GSM (WI code: eDRX_GSM)",0,"agreed","2017-02-02T13:01:51.103","2017-02-03T15:17:41.157","","","Rel-13","45.008","13.4.0","eDRX_GSM-Core","0646","","F","RP-170063","","","","",""]
["R6-170014","Miscellaneous PEO Corrections","Ericsson Inc.","John Diachina","25840","CR","Approval","The sub-clause describing the initiation of the packet downlink assignment procedure needs to be modified to indicate how a MS identifies the CCCH block corresponding to its paging group when it is using eDRX.","","9","5.1","Extended DRX for GSM (WI code: eDRX_GSM)",0,"revised","2017-02-02T13:07:30.617","2017-02-03T15:17:41.157","","R6-170080","Rel-13","44.018","13.4.0","eDRX_GSM-Core","1051","","F","","","","","",""]
["R6-170015","Miscellaneous PEO Corrections","Ericsson Inc.","John Diachina","25840","CR","Approval","The sub-clause describing the initiation of the packet downlink assignment procedure needs to be modified to indicate how a MS identifies the CCCH block corresponding to its paging group when it is using eDRX.","","9","5.1","Extended DRX for GSM (WI code: eDRX_GSM)",0,"revised","2017-02-02T13:11:09.107","2017-02-03T15:17:41.157","","R6-170081","Rel-14","44.018","14.0.0","eDRX_GSM-Core","1052","","A","","","","","",""]
["R6-170016","Clarifying BSS Operation for EC-GSM","Ericsson Inc.","John Diachina","25840","CR","Approval","When the SGSN has downlink data available for a MS for which it has coverage class information and for which the Ready timer is running it sends a DL-UNITDATA PDU to the BSS managing the corresponding serving cell and includes the applicable coverage class information. It is not clear how the BSS, upon receiving the DL-UNITDATA PDU, determines how to reach the MS based on whether it is in idle mode or in packet transfer mode","","10","5.2","Extended Coverage GSM for support of Cellular Internet of Things (WI codes: CIoT_EC_GSM-Core, CIoT_EC_GSM-Perf)",0,"revised","2017-02-02T13:16:56.843","2017-02-03T15:17:41.173","","R6-170078","Rel-13","48.018","13.4.0","CIoT_EC_GSM-Core","0433","","F","","","","","",""]
["R6-170017","Clarifying BSS Operation for EC-GSM","Ericsson Inc.","John Diachina","25840","CR","Approval","When the SGSN has downlink data available for a MS for which it has coverage class information and for which the Ready timer is running it sends a DL-UNITDATA PDU to the BSS managing the corresponding serving cell and includes the applicable coverage class information. It is not clear how the BSS, upon receiving the DL-UNITDATA PDU, determines how to reach the MS based on whether it is in idle mode or in packet transfer mode.","","10","5.2","Extended Coverage GSM for support of Cellular Internet of Things (WI codes: CIoT_EC_GSM-Core, CIoT_EC_GSM-Perf)",0,"revised","2017-02-02T13:20:53.293","2017-02-03T15:17:41.173","","R6-170079","Rel-14","48.018","14.1.0","CIoT_EC_GSM-Core","0434","","A","","","","","",""]
["R6-170018","Clarifyifying EC_Access_Control_Class Operation for  EC-GSM","Ericsson Inc.","John Diachina","25840","CR","Approval","The EC-BCCH CHANGE MARK field is currently incremented every time one or more EC SI messages have changed. However, an exception condition needs to be supported to allow for the case where PLMN specific barring is enabled in a cell (i.e. EC SI 2 and EC SI 4 are transmitted and provide PLMN specific barring information) and changes are made to the EC_Access_Control_Class field or Exception_Report_Status field included in the EC SI 2 and EC SI 4 messages. In this case the network is expected to make frequent changes to these fields for as long as PLMN specific barring remains enabled. As such changes to these fields alone should not cause the value of EC-BCCH CHANGE MARK field to be incremented while PLMN specific barring remains enabled.","","10","5.2","Extended Coverage GSM for support of Cellular Internet of Things (WI codes: CIoT_EC_GSM-Core, CIoT_EC_GSM-Perf)",0,"revised","2017-02-02T13:24:08.487","2017-02-03T15:17:41.173","","R6-170082","Rel-13","44.018","13.4.0","CIoT_EC_GSM-Core","1053","","F","","","","","",""]
["R6-170019","Clarifyifying EC_Access_Control_Class Operation for  EC-GSM","Ericsson Inc.","John Diachina","25840","CR","Approval","The EC-BCCH CHANGE MARK field is currently incremented every time one or more EC SI messages have changed. However, an exception condition needs to be supported to allow for the case where PLMN specific barring is enabled in a cell (i.e. EC SI 2 and EC SI 4 are transmitted and provide PLMN specific barring information) and changes are made to the EC_Access_Control_Class field or Exception_Report_Status field included in the EC SI 2 and EC SI 4 messages. In this case the network is expected to make frequent changes to these fields for as long as PLMN specific barring remains enabled. As such changes to these fields alone should not cause the value of EC-BCCH CHANGE MARK field to be incremented while PLMN specific barring remains enabled.","","10","5.2","Extended Coverage GSM for support of Cellular Internet of Things (WI codes: CIoT_EC_GSM-Core, CIoT_EC_GSM-Perf)",0,"revised","2017-02-02T13:26:40.677","2017-02-03T15:17:41.173","","R6-170083","Rel-14","44.018","14.0.0","CIoT_EC_GSM-Core","1054","","A","","","","","",""]
["R6-170020","Multilateration Timing Advance Procedure","Ericsson Inc.","John Diachina","25840","discussion","Agreement","This contribution documents a proposed set of stage 3 pseudo CRs Applicable to ePOS_GERAN (blue shaded text in sections 2 through 11 below indicates proposed stage 3 modifications).","","15","6.1.1","Core aspects (WI code: ePOS_GERAN-Core)",0,"revised","2017-02-02T13:31:32.507","2017-02-03T15:17:41.187","","R6-170086","Rel-14","","","","","","","","","","","",""]
["R6-170021","Multilateration Timing Advance RRLP Message Content","Ericsson Inc.","John Diachina","25840","discussion","Agreement","This contribution documents a proposed content for the Multilateration Timing Advance RRLP Message using CSN.1 coding with the further objective of translating the CSN.1 coding format into ASN.1 format.","","15","6.1.1","Core aspects (WI code: ePOS_GERAN-Core)",0,"noted","2017-02-02T13:35:38.493","2017-02-03T15:17:41.187","","","Rel-14","","","","","","","","","","","",""]
["R6-170022","Rules for Multilateration Timing Advance Method Utilization","Ericsson Inc.","John Diachina","25840","discussion","Agreement","This contribution summarizes three types of Multilateration Timing Advance (MTA) methods and the rules that determine when they can be used.","","15","6.1.1","Core aspects (WI code: ePOS_GERAN-Core)",0,"noted","2017-02-02T13:48:40.600","2017-02-03T15:17:41.187","","","Rel-14","","","","","","","","","","","",""]
["R6-170023","Introduction of compact burst mapping","Ericsson Inc.","John Diachina","25840","CR","Approval","A description of the impacts of compact burst mapping to the triggering of cell re-selection is provided.","","19","6.3.1","Core aspects (WI code: CIoT_EC_GSM_radio_enh-Core)",0,"revised","2017-02-02T15:13:43.093","2017-02-03T15:17:41.187","","R6-170110","Rel-14","45.008","13.4.0","CIoT_EC_GSM_radio_enh-Core","0647","","B","","","","","",""]
["R6-170024","Introduction of Multilateration","Ericsson Inc.","John Diachina","25840","CR","Approval","A description of the Multilateration feature is provided.","Document not made available","15","6.1.1","Core aspects (WI code: ePOS_GERAN-Core)",0,"withdrawn","2017-02-02T17:40:17.697",null,"","","Rel-14","44.018","14.0.0","ePOS_GERAN-Core","1055","","B","","","","","",""]
["R6-170025","Introduction of Multilateration","Ericsson Inc.","John Diachina","25840","CR","Approval","A description of the Multilateration feature is provided.","Revised and merged with R6-170051 and R6-170056 into R6-170093.","15","6.1.1","Core aspects (WI code: ePOS_GERAN-Core)",0,"revised","2017-02-02T17:51:14.433","2017-02-03T15:17:41.187","R6-160238","R6-170093","Rel-14","44.018","14.0.0","ePOS_GERAN-Core","1047","2","B","","","","","",""]
["R6-170026","Introduction of Multilateration","Ericsson Inc.","John Diachina","25840","CR","Approval","A description of the Multilateration feature is provided.","Revised and merged with R6-170053 into R6-170095.","15","6.1.1","Core aspects (WI code: ePOS_GERAN-Core)",0,"revised","2017-02-02T17:56:49.907","2017-02-03T15:17:41.187","R6-160237","R6-170095","Rel-14","44.031","13.0.0","ePOS_GERAN-Core","0227","2","B","","","","","",""]
["R6-170027","Introduction of Multilateration","Ericsson Inc.","John Diachina","25840","CR","Approval","A description of the Multilateration feature is provided.","Revised and merged with R6-170052 into R6-170094.","15","6.1.1","Core aspects (WI code: ePOS_GERAN-Core)",0,"revised","2017-02-02T18:00:27.853","2017-02-03T15:17:41.203","R6-160239","R6-170094","Rel-14","44.060","13.4.0","ePOS_GERAN-Core","1631","2","B","","","","","",""]
["R6-170028","Reply LS on Flexible eNB-ID and Cell-ID in E-UTRAN","TSG SA WG5","Paolino Usai","3209","LS in","Information","","","7","4","Liaisons / reports from other groups / meetings",0,"noted","2017-02-02T18:48:34.143","2017-02-02T18:48:56.920","","","","","","","","","","","","","","",""]
["R6-170029","Introduction of Multilateration","Ericsson Inc.","John Diachina","25840","CR","Approval","A description of the Multilateration feature is provided.","","15","6.1.1","Core aspects (WI code: ePOS_GERAN-Core)",0,"revised","2017-02-02T20:50:47.487","2017-02-03T15:17:41.203","","R6-170099","Rel-14","45.008","13.4.0","ePOS_GERAN-Core","0648","","B","","","","","",""]
["R6-170030","Introduction of Multilateration","Ericsson Inc.","John Diachina","25840","CR","Approval","A description of the Multilateration feature is provided.","Revised and merged with R6-170054 into R6-170098.","15","6.1.1","Core aspects (WI code: ePOS_GERAN-Core)",0,"revised","2017-02-02T20:55:39.047","2017-02-03T15:17:41.203","R6-160240","R6-170098","Rel-14","48.008","13.3.0","ePOS_GERAN-Core","0410","2","B","","","","","",""]
["R6-170031","Introduction of Multilateration","Ericsson Inc.","John Diachina","25840","CR","Approval","A description of the Multilateration feature is provided.","","15","6.1.1","Core aspects (WI code: ePOS_GERAN-Core)",0,"revised","2017-02-02T21:01:02.490","2017-02-03T15:17:41.203","R6-160241","R6-170097","Rel-14","48.018","14.1.0","ePOS_GERAN-Core","0430","2","B","","","","","",""]
["R6-170032","Introduction of Multilateration","Ericsson Inc.","John Diachina","25840","CR","Approval","A description of the Multilateration feature is provided.","Revised and merged with  R6-170050 and R6-170055 into R6-170096.","15","6.1.1","Core aspects (WI code: ePOS_GERAN-Core)",0,"revised","2017-02-02T21:05:50.887","2017-02-03T15:17:41.157","R6-160242","R6-170096","Rel-14","49.031","13.0.0","ePOS_GERAN-Core","0066","2","B","","","","","",""]
["R6-170033","Introduction of compact burst mapping","Ericsson LM","Stefan Eriksson Löwenmark","22717","CR","Agreement","Compact burst mapping is introduced.","","19","6.3.1","Core aspects (WI code: CIoT_EC_GSM_radio_enh-Core)",0,"revised","2017-02-03T01:30:53.373","2017-02-03T17:44:43.617","","R6-170109","Rel-14","43.064","14.0.0","CIoT_EC_GSM_radio_enh-Core","0112","","B","","","","","",""]
["R6-170034","Introduction of compact burst mapping","Ericsson LM","Stefan Eriksson Löwenmark","22717","CR","Agreement","Compact burst mapping is introduced.","","19","6.3.1","Core aspects (WI code: CIoT_EC_GSM_radio_enh-Core)",0,"agreed","2017-02-03T01:30:53.483","2017-02-03T17:44:43.633","","","Rel-14","45.001","14.0.0","CIoT_EC_GSM_radio_enh-Core","0095","","B","RP-170061","","","","",""]
["R6-170035","Introduction of compact burst mapping","Ericsson LM","Stefan Eriksson Löwenmark","22717","CR","Agreement","Compact burst mapping is introduced.","","19","6.3.1","Core aspects (WI code: CIoT_EC_GSM_radio_enh-Core)",0,"revised","2017-02-03T01:30:53.543","2017-02-03T17:44:43.633","","R6-170111","Rel-14","45.002","14.0.0","CIoT_EC_GSM_radio_enh-Core","0204","","B","","","","","",""]
["R6-170036","Introduction of compact burst mapping","Ericsson LM","Stefan Eriksson Löwenmark","22717","CR","Agreement","Compact burst mapping is introduced.","","19","6.3.1","Core aspects (WI code: CIoT_EC_GSM_radio_enh-Core)",0,"revised","2017-02-03T01:30:53.653","2017-02-03T17:44:43.600","","R6-170112","Rel-14","45.003","14.0.0","CIoT_EC_GSM_radio_enh-Core","0143","","B","","","","","",""]
["R6-170037","Introduction of Timing Advance Multilateration","Ericsson LM","Nicklas Johansson","47575","CR","Agreement","","","16","6.1.2","Performance aspects (WI code: ePOS_GERAN-Perf)",0,"revised","2017-02-03T09:12:35.683","2017-02-03T13:59:12.700","R6-160160","R6-170107","Rel-14","45.010","13.4.0","ePOS_GERAN-Perf","0071","1","B","","","","","",""]
["R6-170038","Multilateration OTD – Design Aspects (update of R6-160233)","Nokia Germany","Juergen Hofmann","68332","discussion","Agreement","","","15","6.1.1","Core aspects (WI code: ePOS_GERAN-Core)",0,"revised","2017-02-03T14:50:50.820","2017-02-03T22:24:11.700","","R6-170090","Rel-14","","","ePOS_GERAN-Core","","","","","","","","",""]
["R6-170039","Introduction of Multilateration OTD","Nokia Germany","Juergen Hofmann","68332","CR","Agreement","","","15","6.1.1","Core aspects (WI code: ePOS_GERAN-Core)",0,"revised","2017-02-03T15:09:44.520","2017-02-03T22:24:11.687","","R6-170092","Rel-14","43.059","13.2.0","ePOS_GERAN-Core","0082","","B","","","","","",""]
["R6-170040","Introduction of Alternative Mappings for Higher Coverage Classes with 2 PDCHs","Nokia Germany","Juergen Hofmann","68332","CR","Agreement","","","19","6.3.1","Core aspects (WI code: CIoT_EC_GSM_radio_enh-Core)",0,"revised","2017-02-03T15:55:46.090","2017-02-03T19:30:59.317","","R6-170113","Rel-14","44.018","14.0.0","CIoT_EC_GSM_radio_enh-Core","1056","","B","","","","","",""]
["R6-170041","Introduction of Alternative Mappings for Higher Coverage Classes with 2 PDCHs","Nokia Germany","Juergen Hofmann","68332","CR","Agreement","","","19","6.3.1","Core aspects (WI code: CIoT_EC_GSM_radio_enh-Core)",0,"revised","2017-02-03T16:01:45.637","2017-02-03T19:30:59.270","","R6-170114","Rel-14","44.060","13.4.0","CIoT_EC_GSM_radio_enh-Core","1635","","B","","","","","",""]
["R6-170042","Handling of unknown message types on EC-CCCH","Nokia Germany","Juergen Hofmann","68332","CR","Agreement","","","10","5.2","Extended Coverage GSM for support of Cellular Internet of Things (WI codes: CIoT_EC_GSM-Core, CIoT_EC_GSM-Perf)",0,"revised","2017-02-03T16:06:28.037","2017-02-03T19:30:59.287","","R6-170084","Rel-13","44.018","13.4.0","CIoT_EC_GSM-Core","1057","","F","","","","","",""]
["R6-170043","Handling of unknown message types on EC-CCCH","Nokia Germany","Juergen Hofmann","68332","CR","Agreement","","","10","5.2","Extended Coverage GSM for support of Cellular Internet of Things (WI codes: CIoT_EC_GSM-Core, CIoT_EC_GSM-Perf)",0,"revised","2017-02-03T16:09:28.417","2017-02-03T19:30:59.303","","R6-170085","Rel-14","44.018","14.0.0","CIoT_EC_GSM-Core","1058","","A","","","","","",""]
["R6-170044","Clarification on spare bits setting in RLC/MAC header for MCS-1 in EC operation","Nokia Germany","Juergen Hofmann","68332","CR","Agreement","","","10","5.2","Extended Coverage GSM for support of Cellular Internet of Things (WI codes: CIoT_EC_GSM-Core, CIoT_EC_GSM-Perf)",0,"withdrawn","2017-02-03T16:16:24.183",null,"","","Rel-13","44.060","13.4.0","CIoT_EC_GSM-Core","1636","","F","","","","","",""]
["R6-170045","Serving Cell TA Estimation for Multilateration Positioning","Nokia Germany","Juergen Hofmann","68332","discussion","Agreement","","","15","6.1.1","Core aspects (WI code: ePOS_GERAN-Core)",0,"revised","2017-02-03T16:36:51.587","2017-02-03T22:25:15.910","","R6-170087","Rel-14","","","ePOS_GERAN-Core","","","","","","","","",""]
["R6-170046","Clarification on spare bits setting in RLC/MAC header for MCS-1 in EC operation","Nokia Germany","Juergen Hofmann","68332","CR","Agreement","","","10","5.2","Extended Coverage GSM for support of Cellular Internet of Things (WI codes: CIoT_EC_GSM-Core, CIoT_EC_GSM-Perf)",0,"withdrawn","2017-02-03T16:40:35.857",null,"","","Rel-14","44.060","13.4.0","CIoT_EC_GSM-Core","1637","","A","","","","","",""]
["R6-170047","Connectionless MTA Design Aspects","Nokia Germany","Juergen Hofmann","68332","discussion","Agreement","","","15","6.1.1","Core aspects (WI code: ePOS_GERAN-Core)",0,"revised","2017-02-03T16:46:04.770","2017-02-03T22:24:48.017","","R6-170088","Rel-14","","","ePOS_GERAN-Core","","","","","","","","",""]
["R6-170048","Introduction of Multilateration Timing Advance","Nokia Germany","Juergen Hofmann","68332","CR","Agreement","","Merged with TD R6-170008 into R6-170091","15","6.1.1","Core aspects (WI code: ePOS_GERAN-Core)",0,"merged","2017-02-03T16:53:34.250","2017-02-03T22:24:48.017","","","Rel-14","43.059","13.2.0","ePOS_GERAN-Core","0083","","B","","","","","",""]
["R6-170049","Introduction of Multilateration OTD","Nokia Germany","Juergen Hofmann","68332","CR","Agreement","","","15","6.1.1","Core aspects (WI code: ePOS_GERAN-Core)",0,"revised","2017-02-03T17:12:55.107","2017-02-03T22:52:13.750","","R6-170103","Rel-14","44.031","13.0.0","ePOS_GERAN-Core","0228","","B","","","","","",""]
["R6-170050","Introduction of Multilateration OTD","Nokia Germany","Juergen Hofmann","68332","CR","Agreement","","Merged with R6-170032 and R6-170055 into R6-170096.","15","6.1.1","Core aspects (WI code: ePOS_GERAN-Core)",0,"merged","2017-02-03T17:15:42.757","2017-02-09T10:42:14.340","","","Rel-14","49.031","13.0.0","ePOS_GERAN-Core","0067","","B","","","","","",""]
["R6-170051","Channel Request for Multilateration Positioning","Nokia Germany","Juergen Hofmann","68332","CR","Agreement","","Merged with TD R6-170025 and R6-170056 into R6-170093.","15","6.1.1","Core aspects (WI code: ePOS_GERAN-Core)",0,"merged","2017-02-03T17:24:23.277","2017-02-09T10:42:14.357","","","Rel-14","44.018","14.0.0","ePOS_GERAN-Core","1059","","B","","","","","",""]
["R6-170052","Channel request for Multilateration Positioning","Nokia Germany","Juergen Hofmann","68332","CR","Agreement","","Merged with TD R6-170027 into R6-170094","15","6.1.1","Core aspects (WI code: ePOS_GERAN-Core)",0,"merged","2017-02-03T17:27:19.367","2017-02-09T10:42:14.357","","","Rel-14","44.060","13.4.0","ePOS_GERAN-Core","1638","","B","","","","","",""]
["R6-170053","Introduction of MTA for connectionless packet access","Nokia Germany","Juergen Hofmann","68332","CR","Agreement","","Merged with TD R6-170026 into R6-170095","15","6.1.1","Core aspects (WI code: ePOS_GERAN-Core)",0,"merged","2017-02-03T17:32:51.797","2017-02-09T20:48:19.727","","","Rel-14","44.031","13.0.0","ePOS_GERAN-Core","0229","","B","","","","","",""]
["R6-170054","Introduction of MTA for connectionless packet access","Nokia Germany","Juergen Hofmann","68332","CR","Agreement","","Merged with TD R6-170030 into R6-170098","15","6.1.1","Core aspects (WI code: ePOS_GERAN-Core)",0,"merged","2017-02-03T17:35:17.627","2017-02-09T20:48:19.697","","","Rel-14","48.008","13.3.0","ePOS_GERAN-Core","0411","","B","","","","","",""]
["R6-170055","Introduction of MTA for connectionless packet access","Nokia Germany","Juergen Hofmann","68332","CR","Agreement","","Merged with TD R6-170032 and R6-170050 into R6-170096.","15","6.1.1","Core aspects (WI code: ePOS_GERAN-Core)",0,"merged","2017-02-03T17:37:31.267","2017-02-09T20:48:19.697","","","Rel-14","49.031","13.0.0","ePOS_GERAN-Core","0068","","B","","","","","",""]
["R6-170056","Introduction of MTA for connectionless packet access","Nokia Germany","Juergen Hofmann","68332","CR","Agreement","","Merged with TD R6-170025 and R6-170051 into R6-170093.","15","6.1.1","Core aspects (WI code: ePOS_GERAN-Core)",0,"merged","2017-02-03T17:39:54.770","2017-02-09T20:48:19.727","","","Rel-14","44.018","14.0.0","ePOS_GERAN-Core","1060","","B","","","","","",""]
["R6-170057","Introduction of Extended Access Burst for MTA with connectionless packet access","Nokia Germany","Juergen Hofmann","68332","CR","Agreement","","","15","6.1.1","Core aspects (WI code: ePOS_GERAN-Core)",0,"revised","2017-02-03T17:42:30.957","2017-02-03T23:06:37.620","","R6-170100","Rel-14","45.001","14.0.0","ePOS_GERAN-Core","0096","","B","","","","","",""]
["R6-170058","Introduction of Extended Access Burst for MTA with connectionless packet access","Nokia Germany","Juergen Hofmann","68332","CR","Agreement","","","15","6.1.1","Core aspects (WI code: ePOS_GERAN-Core)",0,"revised","2017-02-03T17:44:41.933","2017-02-03T23:12:48.647","","R6-170101","Rel-14","45.002","14.0.0","ePOS_GERAN-Core","0205","","B","","","","","",""]
["R6-170059","Introduction of Extended Access Burst for MTA with connectionless packet access","Nokia Germany","Juergen Hofmann","68332","CR","Agreement","","","15","6.1.1","Core aspects (WI code: ePOS_GERAN-Core)",0,"revised","2017-02-03T17:47:26.527","2017-02-03T23:21:02.817","","R6-170102","Rel-14","45.003","14.0.0","ePOS_GERAN-Core","0144","","B","","","","","",""]
["R6-170060","Introduction of Extended Access Burst for MTA with connectionless packet access","Nokia Germany","Juergen Hofmann","68332","CR","Agreement","","","16","6.1.2","Performance aspects (WI code: ePOS_GERAN-Perf)",0,"revised","2017-02-03T17:52:16.293","2017-02-03T23:30:25.017","","R6-170108","Rel-14","45.005","13.3.0","ePOS_GERAN-Perf","0598","","B","","","","","",""]
["R6-170061","MoM Radio Interface Enhancements for EC-GSM-IoT telco#1","Nokia Germany","Juergen Hofmann","68332","other","","","","18","6.3","Radio Interface Enhancements for EC-GSM-IoT",0,"noted","2017-02-03T18:15:00.213","2017-02-09T10:42:14.247","","","Rel-14","","","CIoT_EC_GSM_radio_enh-Core","","","","","","","","",""]
["R6-170062","Performance requirements for Alternative Mappings for Higher Coverage Classes with 2 PDCHs","Nokia Germany","Juergen Hofmann","68332","CR","Agreement","Template for Performance requirements","","20","6.3.2","Performance aspects (WI code: CIoT_EC_GSM_radio_enh-Perf)",0,"postponed","2017-02-03T18:21:20.223","2017-02-14T13:12:29.610","","","Rel-14","45.005","13.3.0","CIoT_EC_GSM_radio_enh-Perf","0599","","B","","","","","",""]
["R6-170063","New Uplink Coverage Class CC5 - Link Layer Aspects","Nokia Germany","Juergen Hofmann","68332","discussion","Agreement","","","19","6.3.1","Core aspects (WI code: CIoT_EC_GSM_radio_enh-Core)",0,"revised","2017-02-03T18:26:31.037","2017-02-09T10:42:14.247","","R6-170141","Rel-14","","","CIoT_EC_GSM_radio_enh-Core","","","","","","","","",""]
["R6-170064","New Uplink Coverage Class CC5 - EC-PACCH Message Changes","Nokia Germany","Juergen Hofmann","68332","discussion","Agreement","","All Was agreed.","19","6.3.1","Core aspects (WI code: CIoT_EC_GSM_radio_enh-Core)",0,"noted","2017-02-03T18:28:59.483","2017-02-09T10:42:14.263","","","Rel-14","","","CIoT_EC_GSM_radio_enh-Core","","","","","","","","",""]
["R6-170065","New Uplink Coverage Class CC5 - EC-PDTCH Message Changes","Nokia Germany","Juergen Hofmann","68332","discussion","Agreement","","","19","6.3.1","Core aspects (WI code: CIoT_EC_GSM_radio_enh-Core)",0,"noted","2017-02-03T18:31:56.447","2017-02-09T10:42:14.263","","","Rel-14","","","CIoT_EC_GSM_radio_enh-Core","","","","","","","","",""]
["R6-170066","New Uplink Coverage Class CC5 - EC-RACH Training Sequence Design","Nokia Germany","Juergen Hofmann","68332","discussion","Agreement","","","19","6.3.1","Core aspects (WI code: CIoT_EC_GSM_radio_enh-Core)",0,"revised","2017-02-03T18:33:59.093","2017-02-09T10:42:14.263","","R6-170115","Rel-14","","","CIoT_EC_GSM_radio_enh-Core","","","","","","","","",""]
["R6-170067","Introduction of new uplink coverage class CC5 for EC PDTCH and EC PACCH","Nokia Germany","Juergen Hofmann","68332","CR","Agreement","","","19","6.3.1","Core aspects (WI code: CIoT_EC_GSM_radio_enh-Core)",0,"revised","2017-02-03T18:36:27.010","2017-02-09T10:42:14.263","","R6-170117","Rel-14","45.001","14.0.0","CIoT_EC_GSM_radio_enh-Core","0097","","B","","","","","",""]
["R6-170068","Introduction of new uplink coverage class CC5 for EC PDTCH and EC PACCH","Nokia Germany","Juergen Hofmann","68332","CR","Agreement","","","19","6.3.1","Core aspects (WI code: CIoT_EC_GSM_radio_enh-Core)",0,"revised","2017-02-03T18:39:10.217","2017-02-09T10:42:14.310","","R6-170118","Rel-14","45.002","14.0.0","CIoT_EC_GSM_radio_enh-Core","0206","","B","","","","","",""]
["R6-170069","Introduction of new uplink coverage class CC5 for EC PDTCH and EC PACCH","Nokia Germany","Juergen Hofmann","68332","CR","Agreement","","","19","6.3.1","Core aspects (WI code: CIoT_EC_GSM_radio_enh-Core)",0,"revised","2017-02-03T18:41:12.580","2017-02-09T10:42:14.310","","R6-170119","Rel-14","45.003","14.0.0","CIoT_EC_GSM_radio_enh-Core","0145","","B","","","","","",""]
["R6-170070","Performance requirements for new uplink coverage class CC5 for UL MCL improvement","Nokia Germany","Juergen Hofmann","68332","CR","Agreement","Template for Performance requirements","","20","6.3.2","Performance aspects (WI code: CIoT_EC_GSM_radio_enh-Perf)",0,"revised","2017-02-03T18:49:32.740","2017-02-14T13:12:29.627","","R6-170123","Rel-14","45.005","13.3.0","CIoT_EC_GSM_radio_enh-Perf","0600","","B","","","","","",""]
["R6-170071","Introduction of new UL coverage class CC5 for UL MCL improvement","Nokia Germany","Juergen Hofmann","68332","CR","Agreement","","","19","6.3.1","Core aspects (WI code: CIoT_EC_GSM_radio_enh-Core)",0,"revised","2017-02-03T18:52:19.207","2017-02-09T10:42:14.323","","R6-170120","Rel-14","44.018","14.0.0","CIoT_EC_GSM_radio_enh-Core","1061","","B","","","","","",""]
["R6-170072","Introduction of new UL coverage class CC5 for UL MCL improvement","Nokia Germany","Juergen Hofmann","68332","CR","Agreement","","","19","6.3.1","Core aspects (WI code: CIoT_EC_GSM_radio_enh-Core)",0,"revised","2017-02-03T18:54:27.577","2017-02-09T10:42:14.323","","R6-170121","Rel-14","44.060","13.4.0","CIoT_EC_GSM_radio_enh-Core","1639","","B","","","","","",""]
["R6-170073","Introduction of new UL coverage class CC5 for UL MCL improvement","Nokia Germany","Juergen Hofmann","68332","CR","Agreement","","","19","6.3.1","Core aspects (WI code: CIoT_EC_GSM_radio_enh-Core)",0,"postponed","2017-02-03T18:57:12.980","2017-02-09T10:42:14.323","","","Rel-14","45.008","13.4.0","CIoT_EC_GSM_radio_enh-Core","0649","","B","","","","","",""]
["R6-170074","Introduction of PS domain transport for Multilateration Timing Advance information transfer","Ericsson LM","Paolino Usai","3209","CR","Agreement","","","15","6.1.1","Core aspects (WI code: ePOS_GERAN-Core)",0,"postponed","2017-02-08T10:30:57.920","2017-02-08T13:27:25.973","","","Rel-14","48.018","14.1.0","ePOS_GERAN-Core","0435","","B","","","","","",""]
["R6-170075","Throughput and Latency Performance Analysis for UL MCL Improvement","Nokia Germany","Paolino Usai","3209","discussion","Agreement","","","19","6.3.1","Core aspects (WI code: CIoT_EC_GSM_radio_enh-Core)",0,"noted","2017-02-08T16:50:06.043","2017-02-09T08:57:29.380","","","","","","","","","","","","","","",""]
["R6-170076","Draft CR 24.008 Introduction of capability support for EC-GSM-IoT radio interface enhancements (Rel-14)","Nokia Germany","Paolino Usai","3209","draftCR","Endorsement","","","19","6.3.1","Core aspects (WI code: CIoT_EC_GSM_radio_enh-Core)",0,"revised","2017-02-08T16:50:06.057","2017-02-09T08:57:29.877","","R6-170122","Rel-14","24.008","14.2.0","CIoT_EC_GSM_radio_enh-Core","","","","","","","","",""]
["R6-170077","LS on removal of exceptions from security profiles in 43.318","TSG SA WG3","Paolino Usai","3209","LS in","Action","","","7","4","Liaisons / reports from other groups / meetings",0,"noted","2017-02-13T07:04:21.117","2017-02-13T07:04:40.367","","","","","","","","","","","","","","S3-170484",""]
["R6-170078","Clarifying BSS Operation for EC-GSM","Ericsson Inc.","John Diachina","25840","CR","Approval","When the SGSN has downlink data available for a MS for which it has coverage class information and for which the Ready timer is running it sends a DL-UNITDATA PDU to the BSS managing the corresponding serving cell and includes the applicable coverage class information. It is not clear how the BSS, upon receiving the DL-UNITDATA PDU, determines how to reach the MS based on whether it is in idle mode or in packet transfer mode","","10","5.2","Extended Coverage GSM for support of Cellular Internet of Things (WI codes: CIoT_EC_GSM-Core, CIoT_EC_GSM-Perf)",0,"agreed","2017-02-03T15:17:41.173","2017-02-03T15:17:41.173","R6-170016","","Rel-13","48.018","13.4.0","CIoT_EC_GSM-Core","0433","1","F","RP-170064","","","","",""]
["R6-170079","Clarifying BSS Operation for EC-GSM","Ericsson Inc.","John Diachina","25840","CR","Approval","When the SGSN has downlink data available for a MS for which it has coverage class information and for which the Ready timer is running it sends a DL-UNITDATA PDU to the BSS managing the corresponding serving cell and includes the applicable coverage class information. It is not clear how the BSS, upon receiving the DL-UNITDATA PDU, determines how to reach the MS based on whether it is in idle mode or in packet transfer mode.","","10","5.2","Extended Coverage GSM for support of Cellular Internet of Things (WI codes: CIoT_EC_GSM-Core, CIoT_EC_GSM-Perf)",0,"agreed","2017-02-03T15:17:41.173","2017-02-03T15:17:41.173","R6-170017","","Rel-14","48.018","14.1.0","CIoT_EC_GSM-Core","0434","1","A","RP-170064","","","","",""]
["R6-170080","Miscellaneous PEO Corrections","Ericsson Inc.","John Diachina","25840","CR","Approval","The sub-clause describing the initiation of the packet downlink assignment procedure needs to be modified to indicate how a MS identifies the CCCH block corresponding to its paging group when it is using eDRX.","","9","5.1","Extended DRX for GSM (WI code: eDRX_GSM)",0,"agreed","2017-02-20T14:51:46.237","2017-02-20T14:57:25.437","R6-170014","","Rel-13","44.018","13.4.0","eDRX_GSM-Core","1051","1","F","RP-170063","","","","",""]
["R6-170081","Miscellaneous PEO Corrections","Ericsson Inc.","John Diachina","25840","CR","Approval","The sub-clause describing the initiation of the packet downlink assignment procedure needs to be modified to indicate how a MS identifies the CCCH block corresponding to its paging group when it is using eDRX.","","9","5.1","Extended DRX for GSM (WI code: eDRX_GSM)",0,"agreed","2017-02-20T14:51:47.563","2017-02-20T14:57:25.487","R6-170015","","Rel-14","44.018","14.0.0","eDRX_GSM-Core","1052","1","A","RP-170063","","","","",""]
["R6-170082","Clarifyifying EC_Access_Control_Class Operation for  EC-GSM","Ericsson Inc.","John Diachina","25840","CR","Approval","The EC-BCCH CHANGE MARK field is currently incremented every time one or more EC SI messages have changed. However, an exception condition needs to be supported to allow for the case where PLMN specific barring is enabled in a cell (i.e. EC SI 2 and EC SI 4 are transmitted and provide PLMN specific barring information) and changes are made to the EC_Access_Control_Class field or Exception_Report_Status field included in the EC SI 2 and EC SI 4 messages. In this case the network is expected to make frequent changes to these fields for as long as PLMN specific barring remains enabled. As such changes to these fields alone should not cause the value of EC-BCCH CHANGE MARK field to be incremented while PLMN specific barring remains enabled.","","10","5.2","Extended Coverage GSM for support of Cellular Internet of Things (WI codes: CIoT_EC_GSM-Core, CIoT_EC_GSM-Perf)",0,"revised","2017-02-20T14:51:48.343","2017-02-20T14:57:25.500","R6-170018","R6-170124","Rel-13","44.018","13.4.0","CIoT_EC_GSM-Core","1053","1","F","","","","","",""]
["R6-170083","Clarifyifying EC_Access_Control_Class Operation for  EC-GSM","Ericsson Inc.","John Diachina","25840","CR","Approval","The EC-BCCH CHANGE MARK field is currently incremented every time one or more EC SI messages have changed. However, an exception condition needs to be supported to allow for the case where PLMN specific barring is enabled in a cell (i.e. EC SI 2 and EC SI 4 are transmitted and provide PLMN specific barring information) and changes are made to the EC_Access_Control_Class field or Exception_Report_Status field included in the EC SI 2 and EC SI 4 messages. In this case the network is expected to make frequent changes to these fields for as long as PLMN specific barring remains enabled. As such changes to these fields alone should not cause the value of EC-BCCH CHANGE MARK field to be incremented while PLMN specific barring remains enabled.","","10","5.2","Extended Coverage GSM for support of Cellular Internet of Things (WI codes: CIoT_EC_GSM-Core, CIoT_EC_GSM-Perf)",0,"revised","2017-02-20T14:51:49.230","2017-02-20T14:57:25.500","R6-170019","R6-170125","Rel-14","44.018","14.0.0","CIoT_EC_GSM-Core","1054","1","A","","","","","",""]
["R6-170084","Handling of unknown message types on EC-CCCH/D","Nokia","Juergen Hofmann","68332","CR","Agreement","","","10","5.2","Extended Coverage GSM for support of Cellular Internet of Things (WI codes: CIoT_EC_GSM-Core, CIoT_EC_GSM-Perf)",0,"agreed","2017-02-20T14:51:50.043","2017-02-20T14:57:25.517","R6-170042","","Rel-13","44.018","13.4.0","CIoT_EC_GSM-Core","1057","1","F","RP-170064","","","","",""]
["R6-170085","Handling of unknown message types on EC-CCCH/D","Nokia","Juergen Hofmann","68332","CR","Agreement","","","10","5.2","Extended Coverage GSM for support of Cellular Internet of Things (WI codes: CIoT_EC_GSM-Core, CIoT_EC_GSM-Perf)",0,"agreed","2017-02-20T14:51:50.837","2017-02-20T14:57:25.517","R6-170043","","Rel-14","44.018","14.0.0","CIoT_EC_GSM-Core","1058","1","A","RP-170064","","","","",""]
["R6-170086","Multilateration Timing Advance Procedure","Ericsson Inc.","John Diachina","25840","discussion","Agreement","This contribution documents a proposed set of stage 3 changes Applicable to ePOS_GERAN (blue shaded text in sections 2 through 11 below indicates proposed stage 3 modifications).","","15","6.1.1","Core aspects (WI code: ePOS_GERAN-Core)",0,"revised","2017-02-20T14:51:51.617","2017-02-20T14:57:25.530","R6-170020","R6-170126","","","","","","","","","","","","",""]
["R6-170087","Serving Cell TA Estimation for Multilateration Positioning","Nokia Germany","Juergen Hofmann","68332","discussion","Agreement","","","15","6.1.1","Core aspects (WI code: ePOS_GERAN-Core)",0,"revised","2017-02-13T16:09:28","2017-02-13T16:09:28","R6-170045","R6-170127","","","","","","","","","","","","",""]
["R6-170088","Connectionless MTA Design Aspects","Nokia Germany","Juergen Hofmann","68332","discussion","Agreement","","","15","6.1.1","Core aspects (WI code: ePOS_GERAN-Core)",0,"revised","2017-02-13T16:09:28","2017-02-13T16:09:28","R6-170047","R6-170128","","","","","","","","","","","","",""]
["R6-170089","PS domain transport","Ericsson LM","Nicklas Johansson","47575","discussion","Discussion","","","15","6.1.1","Core aspects (WI code: ePOS_GERAN-Core)",0,"noted","2017-02-20T14:51:51.667","2017-02-20T14:57:25.530","R6-170003","","","","","","","","","","","","","",""]
["R6-170090","Multilateration OTD – Design Aspects (update of R6-170038)","Nokia Germany","Juergen Hofmann","68332","discussion","Agreement","","Six agreed WAs.","15","6.1.1","Core aspects (WI code: ePOS_GERAN-Core)",0,"revised","2017-02-20T14:51:51.697","2017-02-20T14:57:25.547","R6-170038","R6-170129","","","","","","","","","","","","",""]
["R6-170091","CR 43.059-0081 rev 5 Introduction of Multilateration (Rel-14)","Ericsson LM","Nicklas Johansson","47575","CR","Approval","","Merge of TD R6-170008 and R6-170048.","15","6.1.1","Core aspects (WI code: ePOS_GERAN-Core)",0,"revised","2017-02-20T14:51:51.710","2017-02-20T14:57:25.547","R6-170008","R6-170130","Rel-14","43.059","13.2.0","ePOS_GERAN-Core","0081","5","B","","","","","",""]
["R6-170092","Introduction of Multilateration OTD","Nokia Germany","Juergen Hofmann","68332","CR","Agreement","","","15","6.1.1","Core aspects (WI code: ePOS_GERAN-Core)",0,"revised","2017-02-20T14:51:52.490","2017-02-20T14:57:25.563","R6-170039","R6-170133","Rel-14","43.059","13.2.0","ePOS_GERAN-Core","0082","1","B","","","","","",""]
["R6-170093","Introduction of Multilateration","Ericsson Inc.","John Diachina","25840","CR","Approval","A description of the Multilateration feature is provided.","Merge of R6-170025 (revised) and R6-170051 and R6-170056","15","6.1.1","Core aspects (WI code: ePOS_GERAN-Core)",0,"postponed","2017-02-20T14:51:53.227","2017-02-20T14:57:25.593","R6-170025","","Rel-14","44.018","14.0.0","ePOS_GERAN-Core","1047","3","B","","","","","",""]
["R6-170094","Introduction of Multilateration","Ericsson Inc.","John Diachina","25840","CR","Approval","A description of the Multilateration feature is provided.","Merge of R6-170027 (revised) and R6-170052","15","6.1.1","Core aspects (WI code: ePOS_GERAN-Core)",0,"postponed","2017-02-20T14:51:53.990","2017-02-20T14:57:25.627","R6-170027","","Rel-14","44.060","13.4.0","ePOS_GERAN-Core","1631","3","B","","","","","",""]
["R6-170095","Introduction of Multilateration","Ericsson Inc.","John Diachina","25840","CR","Approval","A description of the Multilateration feature is provided.","Merge of R6-170026 (revised) and R6-170053","15","6.1.1","Core aspects (WI code: ePOS_GERAN-Core)",0,"postponed","2017-02-20T14:51:54.770","2017-02-20T14:57:25.687","R6-170026","","Rel-14","44.031","13.0.0","ePOS_GERAN-Core","0227","3","B","","","","","",""]
["R6-170096","Introduction of Multilateration","Ericsson Inc.","John Diachina","25840","CR","Approval","A description of the Multilateration feature is provided.","Merge of R6-170032 (revised) R6-170050 and R6-170055","15","6.1.1","Core aspects (WI code: ePOS_GERAN-Core)",0,"postponed","2017-02-20T14:51:55.517","2017-02-20T14:57:25.720","R6-170032","","Rel-14","49.031","13.0.0","ePOS_GERAN-Core","0066","3","B","","","","","",""]
["R6-170097","Introduction of Multilateration","Ericsson Inc.","John Diachina","25840","CR","Approval","A description of the Multilateration feature is provided.","","15","6.1.1","Core aspects (WI code: ePOS_GERAN-Core)",0,"postponed","2017-02-20T14:51:56.313","2017-02-20T14:57:25.720","R6-170031","","Rel-14","48.018","14.1.0","ePOS_GERAN-Core","0430","3","B","","","","","",""]
["R6-170098","Introduction of Multilateration","Ericsson Inc.","John Diachina","25840","CR","Approval","A description of the Multilateration feature is provided.","Merge of R6-170030 (revised) and R6-170054","15","6.1.1","Core aspects (WI code: ePOS_GERAN-Core)",0,"postponed","2017-02-20T14:51:57.170","2017-02-20T14:57:25.720","R6-170030","","Rel-14","48.008","13.3.0","ePOS_GERAN-Core","0410","3","B","","","","","",""]
["R6-170099","Introduction of Multilateration","Ericsson LM","Nicklas Johansson","47575","CR","Approval","A description of the Multilateration feature is provided.","","15","6.1.1","Core aspects (WI code: ePOS_GERAN-Core)",0,"agreed","2017-02-20T14:51:58.030","2017-02-20T14:57:25.720","R6-170029","","Rel-14","45.008","13.4.0","ePOS_GERAN-Core","0648","1","B","RP-170060","","","","",""]
["R6-170100","Introduction of Extended Access Burst for MTA with connectionless packet access","Nokia Germany","Juergen Hofmann","68332","CR","Agreement","","","15","6.1.1","Core aspects (WI code: ePOS_GERAN-Core)",0,"revised","2017-02-20T14:51:58.827","2017-02-20T14:57:25.733","R6-170057","R6-170134","Rel-14","45.001","14.0.0","ePOS_GERAN-Core","0096","1","B","","","","","",""]
["R6-170101","Introduction of Extended Access Burst for MTA with connectionless packet access","Nokia Germany","Juergen Hofmann","68332","CR","Agreement","","","15","6.1.1","Core aspects (WI code: ePOS_GERAN-Core)",0,"revised","2017-02-20T14:51:59.590","2017-02-20T14:57:25.733","R6-170058","R6-170135","Rel-14","45.002","14.0.0","ePOS_GERAN-Core","0205","1","B","","","","","",""]
["R6-170102","Introduction of Extended Access Burst for MTA with connectionless packet access","Nokia Germany","Juergen Hofmann","68332","CR","Agreement","","","15","6.1.1","Core aspects (WI code: ePOS_GERAN-Core)",0,"revised","2017-02-20T14:52:00.387","2017-02-20T14:57:25.733","R6-170059","R6-170136","Rel-14","45.003","14.0.0","ePOS_GERAN-Core","0144","1","B","","","","","",""]
["R6-170103","Introduction of Multilateration OTD","Nokia Germany","Juergen Hofmann","68332","CR","Agreement","","","15","6.1.1","Core aspects (WI code: ePOS_GERAN-Core)",0,"postponed","2017-02-20T14:52:01.197","2017-02-20T14:57:25.733","R6-170049","","Rel-14","44.031","13.0.0","ePOS_GERAN-Core","0228","1","B","","","","","",""]
["R6-170104","Introduction of Timing Advance Multilateration","Ericsson LM","Nicklas Johansson","47575","draftCR","Endorsement","","","15","6.1.1","Core aspects (WI code: ePOS_GERAN-Core)",0,"postponed","2017-02-20T14:39:52.093","2017-02-20T14:47:25.423","R6-170009","","Rel-14","24.008","14.2.0","ePOS_GERAN-Core","","","B","","","","","",""]
["R6-170105","3GPP security profile update","Ericsson LM","Nicklas Johansson","47575","CR","Approval","","","21","6.4","Small technical enhancements and improvements (WI code: TEI14)",0,"agreed","2017-02-20T14:52:01.993","2017-02-20T14:57:25.733","","","Rel-14","43.318","14.0.0","TEI14","0045","","C","RP-170062","","","","",""]
["R6-170106","Clarifying Order of B11 to B1 in in 11 Bit Access","Ericsson Inc.","John Diachina","25840","CR","Approval","","","9","5.1","Extended DRX for GSM (WI code: eDRX_GSM)",0,"agreed","2017-02-20T14:52:03.507","2017-02-20T14:57:25.750","","","Rel-13","44.060","13.4.0","eDRX_GSM-Core","1640","","F","RP-170063","","","","",""]
["R6-170107","Introduction of Timing Advance Multilateration","Ericsson LM","Nicklas Johansson","47575","CR","Agreement","","","16","6.1.2","Performance aspects (WI code: ePOS_GERAN-Perf)",0,"revised","2017-02-20T14:52:05.627","2017-02-20T14:57:25.767","R6-170037","R6-170137","Rel-14","45.010","13.4.0","ePOS_GERAN-Perf","0071","2","B","","","","","",""]
["R6-170108","Introduction of Extended Access Burst for MTA with connectionless packet access","Nokia Germany","Juergen Hofmann","68332","CR","Agreement","","","16","6.1.2","Performance aspects (WI code: ePOS_GERAN-Perf)",0,"revised","2017-02-20T14:52:06.470","2017-02-20T14:57:25.767","R6-170060","R6-170138","Rel-14","45.005","13.3.0","ePOS_GERAN-Perf","0598","1","B","","","","","",""]
["R6-170109","Introduction of compact burst mapping","Ericsson LM","Nicklas Johansson","47575","CR","Agreement","Compact burst mapping is introduced.","","19","6.3.1","Core aspects (WI code: CIoT_EC_GSM_radio_enh-Core)",0,"agreed","2017-02-20T14:52:07.263","2017-02-20T14:57:25.780","R6-170033","","Rel-14","43.064","14.0.0","CIoT_EC_GSM_radio_enh-Core","0112","1","B","RP-170061","","","","",""]
["R6-170110","Introduction of compact burst mapping","Ericsson LM","Nicklas Johansson","47575","CR","Approval","A description of the impacts of compact burst mapping to the triggering of cell re-selection is provided.","","19","6.3.1","Core aspects (WI code: CIoT_EC_GSM_radio_enh-Core)",0,"agreed","2017-02-20T14:52:08.030","2017-02-20T14:57:25.780","R6-170023","","Rel-14","45.008","13.4.0","CIoT_EC_GSM_radio_enh-Core","0647","1","B","RP-170061","","","","",""]
["R6-170111","Introduction of compact burst mapping","Ericsson LM","Nicklas Johansson","47575","CR","Agreement","Compact burst mapping is introduced.","","19","6.3.1","Core aspects (WI code: CIoT_EC_GSM_radio_enh-Core)",0,"agreed","2017-02-20T14:52:08.857","2017-02-20T14:57:25.780","R6-170035","","Rel-14","45.002","14.0.0","CIoT_EC_GSM_radio_enh-Core","0204","1","B","RP-170061","","","","",""]
["R6-170112","Introduction of compact burst mapping","Ericsson LM","Nicklas Johansson","47575","CR","Agreement","Compact burst mapping is introduced.","","19","6.3.1","Core aspects (WI code: CIoT_EC_GSM_radio_enh-Core)",0,"agreed","2017-02-20T14:52:09.667","2017-02-20T14:57:25.797","R6-170036","","Rel-14","45.003","14.0.0","CIoT_EC_GSM_radio_enh-Core","0143","1","B","RP-170061","","","","",""]
["R6-170113","Introduction of Alternative Mappings for Higher Coverage Classes with 2 PDCHs","Nokia Germany","Juergen Hofmann","68332","CR","Agreement","","","19","6.3.1","Core aspects (WI code: CIoT_EC_GSM_radio_enh-Core)",0,"revised","2017-02-20T14:52:10.493","2017-02-20T14:57:25.797","R6-170040","R6-170139","Rel-14","44.018","14.0.0","CIoT_EC_GSM_radio_enh-Core","1056","1","B","","","","","",""]
["R6-170114","Introduction of Alternative Mappings for Higher Coverage Classes with 2 PDCHs","Nokia Germany","Juergen Hofmann","68332","CR","Agreement","","","19","6.3.1","Core aspects (WI code: CIoT_EC_GSM_radio_enh-Core)",0,"revised","2017-02-20T14:52:11.307","2017-02-20T14:57:25.797","R6-170041","R6-170140","Rel-14","44.060","13.4.0","CIoT_EC_GSM_radio_enh-Core","1635","1","B","","","","","",""]
["R6-170115","New Uplink Coverage Class CC5 - EC-RACH Training Sequence Design","Nokia Germany","Juergen Hofmann","68332","discussion","Agreement","","The WA1 is applicable for the 2TS EC-RACH with TS7 for CC5. Tdoc 115 is one option for EC-RACH CC5 design.","19","6.3.1","Core aspects (WI code: CIoT_EC_GSM_radio_enh-Core)",0,"noted","2017-02-20T14:52:12.130","2017-02-20T14:57:25.813","R6-170066","","","","","","","","","","","","","",""]
["R6-170116","CR 48.018-0436 Introduction of new UL coverage class CC5 for UL MCL improvement (Rel-14)","Nokia","Juergen Hofmann","68332","CR","Agreement","","","19","6.3.1","Core aspects (WI code: CIoT_EC_GSM_radio_enh-Core)",0,"postponed","2017-02-20T14:52:12.177","2017-02-20T14:57:25.813","","","Rel-14","48.018","14.1.0","CIoT_EC_GSM_radio_enh-Core","0436","","B","","","","","",""]
["R6-170117","Introduction of new uplink coverage class CC5 for EC PDTCH and EC PACCH","Nokia Germany","Juergen Hofmann","68332","CR","Agreement","","","19","6.3.1","Core aspects (WI code: CIoT_EC_GSM_radio_enh-Core)",0,"revised","2017-02-20T14:52:14.970","2017-02-20T14:57:25.813","R6-170067","R6-170142","Rel-14","45.001","14.0.0","CIoT_EC_GSM_radio_enh-Core","0097","1","B","","","","","",""]
["R6-170118","Introduction of new uplink coverage class CC5 for EC PDTCH and EC PACCH","Nokia Germany","Juergen Hofmann","68332","CR","Agreement","","","19","6.3.1","Core aspects (WI code: CIoT_EC_GSM_radio_enh-Core)",0,"postponed","2017-02-20T14:52:16.220","2017-02-20T14:57:25.827","R6-170068","","Rel-14","45.002","14.0.0","CIoT_EC_GSM_radio_enh-Core","0206","1","B","","","","","",""]
["R6-170119","Introduction of new uplink coverage class CC5 for EC PDTCH and EC PACCH","Nokia Germany","Juergen Hofmann","68332","CR","Agreement","","","19","6.3.1","Core aspects (WI code: CIoT_EC_GSM_radio_enh-Core)",0,"postponed","2017-02-20T14:52:17.233","2017-02-20T14:57:25.827","R6-170069","","Rel-14","45.003","14.0.0","CIoT_EC_GSM_radio_enh-Core","0145","1","B","","","","","",""]
["R6-170120","Introduction of new UL coverage class CC5 for UL MCL improvement","Nokia Germany","Juergen Hofmann","68332","CR","Agreement","","","19","6.3.1","Core aspects (WI code: CIoT_EC_GSM_radio_enh-Core)",0,"postponed","2017-02-20T14:52:17.967","2017-02-20T14:57:25.827","R6-170071","","Rel-14","44.018","14.0.0","CIoT_EC_GSM_radio_enh-Core","1061","1","B","","","","","",""]
["R6-170121","Introduction of new UL coverage class CC5 for UL MCL improvement","Nokia Germany","Juergen Hofmann","68332","CR","Agreement","","","19","6.3.1","Core aspects (WI code: CIoT_EC_GSM_radio_enh-Core)",0,"postponed","2017-02-20T14:52:18.730","2017-02-20T14:57:25.843","R6-170072","","Rel-14","44.060","13.4.0","CIoT_EC_GSM_radio_enh-Core","1639","1","B","","","","","",""]
["R6-170122","Draft CR 24.008 Introduction of capability support for EC-GSM-IoT radio interface enhancements (Rel-14)","Nokia Germany","Paolino Usai","3209","draftCR","Endorsement","","","19","6.3.1","Core aspects (WI code: CIoT_EC_GSM_radio_enh-Core)",0,"postponed","2017-02-20T14:39:52.107","2017-02-20T14:47:25.487","R6-170076","","Rel-14","24.008","14.2.0","CIoT_EC_GSM_radio_enh-Core","","","","","","","","",""]
["R6-170123","Performance requirements for new uplink coverage class CC5 for UL MCL improvement","Nokia Germany","Juergen Hofmann","68332","CR","Agreement","Template for Performance requirements","","20","6.3.2","Performance aspects (WI code: CIoT_EC_GSM_radio_enh-Perf)",0,"postponed","2017-02-20T14:52:19.540","2017-02-20T14:57:25.843","R6-170070","","Rel-14","45.005","13.3.0","CIoT_EC_GSM_radio_enh-Perf","0600","1","B","","","","","",""]
["R6-170124","Clarifyifying EC_Access_Control_Class Operation for  EC-GSM","Ericsson Inc.","John Diachina","25840","CR","Approval","The EC-BCCH CHANGE MARK field is currently incremented every time one or more EC SI messages have changed. However, an exception condition needs to be supported to allow for the case where PLMN specific barring is enabled in a cell (i.e. EC SI 2 and EC SI 4 are transmitted and provide PLMN specific barring information) and changes are made to the EC_Access_Control_Class field or Exception_Report_Status field included in the EC SI 2 and EC SI 4 messages. In this case the network is expected to make frequent changes to these fields for as long as PLMN specific barring remains enabled. As such changes to these fields alone should not cause the value of EC-BCCH CHANGE MARK field to be incremented while PLMN specific barring remains enabled.","","10","5.2","Extended Coverage GSM for support of Cellular Internet of Things (WI codes: CIoT_EC_GSM-Core, CIoT_EC_GSM-Perf)",0,"revised","2017-02-20T14:52:20.337","2017-02-20T14:57:25.843","R6-170082","R6-170153","Rel-13","44.018","13.4.0","CIoT_EC_GSM-Core","1053","2","F","","","","","",""]
["R6-170125","Clarifyifying EC_Access_Control_Class Operation for  EC-GSM","Ericsson Inc.","John Diachina","25840","CR","Approval","The EC-BCCH CHANGE MARK field is currently incremented every time one or more EC SI messages have changed. However, an exception condition needs to be supported to allow for the case where PLMN specific barring is enabled in a cell (i.e. EC SI 2 and EC SI 4 are transmitted and provide PLMN specific barring information) and changes are made to the EC_Access_Control_Class field or Exception_Report_Status field included in the EC SI 2 and EC SI 4 messages. In this case the network is expected to make frequent changes to these fields for as long as PLMN specific barring remains enabled. As such changes to these fields alone should not cause the value of EC-BCCH CHANGE MARK field to be incremented while PLMN specific barring remains enabled.","","10","5.2","Extended Coverage GSM for support of Cellular Internet of Things (WI codes: CIoT_EC_GSM-Core, CIoT_EC_GSM-Perf)",0,"revised","2017-02-20T14:52:21.117","2017-02-20T14:57:25.860","R6-170083","R6-170154","Rel-14","44.018","14.0.0","CIoT_EC_GSM-Core","1054","2","A","","","","","",""]
["R6-170126","Multilateration Timing Advance Procedure","Ericsson Inc.","John Diachina","25840","discussion","Agreement","This contribution documents a proposed set of stage 3 changes Applicable to ePOS_GERAN (blue shaded text in sections 2 through 11 below indicates proposed stage 3 modifications).","","15","6.1.1","Core aspects (WI code: ePOS_GERAN-Core)",0,"noted","2017-02-20T14:52:21.880","2017-02-20T14:57:25.860","R6-170086","","","","","","","","","","","","","",""]
["R6-170127","Serving Cell TA Estimation for Multilateration Positioning","Nokia Germany","Juergen Hofmann","68332","discussion","Agreement","","","15","6.1.1","Core aspects (WI code: ePOS_GERAN-Core)",0,"noted","2017-02-20T14:52:21.897","2017-02-20T14:57:26.203","R6-170087","","","","","","","","","","","","","",""]
["R6-170128","Connectionless MTA Design Aspects","Nokia Germany","Juergen Hofmann","68332","discussion","Agreement","","","15","6.1.1","Core aspects (WI code: ePOS_GERAN-Core)",0,"noted","2017-02-20T14:52:21.913","2017-02-20T14:57:26.203","R6-170088","","","","","","","","","","","","","",""]
["R6-170129","Multilateration OTD – Design Aspects (update of R6-170090)","Nokia Germany","Juergen Hofmann","68332","discussion","Agreement","","Six agreed WAs.","15","6.1.1","Core aspects (WI code: ePOS_GERAN-Core)",0,"noted","2017-02-20T14:52:21.943","2017-02-20T14:57:25.860","R6-170090","","","","","","","","","","","","","",""]
["R6-170130","CR 43.059-0081 rev 6 Introduction of Multilateration (Rel-14)","Ericsson LM","Nicklas Johansson","47575","CR","Approval","","","15","6.1.1","Core aspects (WI code: ePOS_GERAN-Core)",0,"revised","2017-02-20T14:52:21.960","2017-02-20T14:57:25.860","R6-170091","R6-170148","Rel-14","43.059","13.2.0","ePOS_GERAN-Core","0081","6","B","","","","","",""]
["R6-170131","Synchronization sequence bits correction","Ericsson LM","Nicklas Johansson","47575","CR","Approval","","","9","5.1","Extended DRX for GSM (WI code: eDRX_GSM)",0,"agreed","2017-02-20T14:52:22.757","2017-02-20T14:57:25.877","","","Rel-13","45.002","13.4.0","eDRX_GSM","0207","","F","RP-170063","","","","",""]
["R6-170132","Synchronization sequence bits correction","Ericsson LM","Nicklas Johansson","47575","CR","Approval","","","9","5.1","Extended DRX for GSM (WI code: eDRX_GSM)",0,"agreed","2017-02-20T14:52:24.690","2017-02-20T14:57:25.877","","","Rel-14","45.002","14.0.0","eDRX_GSM","0208","","A","RP-170063","","","","",""]
["R6-170133","Introduction of Multilateration OTD","Nokia Germany","Juergen Hofmann","68332","CR","Agreement","","","15","6.1.1","Core aspects (WI code: ePOS_GERAN-Core)",0,"revised","2017-02-20T14:52:26.717","2017-02-20T14:57:25.877","R6-170092","R6-170150","Rel-14","43.059","13.2.0","ePOS_GERAN-Core","0082","2","B","","","","","",""]
["R6-170134","Introduction of Extended Access Burst for MTA with connectionless packet access","Nokia Germany","Juergen Hofmann","68332","CR","Agreement","","","15","6.1.1","Core aspects (WI code: ePOS_GERAN-Core)",0,"revised","2017-02-20T14:52:28.200","2017-02-20T14:57:25.890","R6-170100","R6-170149","Rel-14","45.001","14.0.0","ePOS_GERAN-Core","0096","2","B","","","","","",""]
["R6-170135","Introduction of Extended Access Burst for connectionless Multilateration Positioning","Nokia","Juergen Hofmann","68332","CR","Agreement","","","15","6.1.1","Core aspects (WI code: ePOS_GERAN-Core)",0,"agreed","2017-02-20T14:52:29.290","2017-02-20T14:57:25.890","R6-170101","","Rel-14","45.002","14.0.0","ePOS_GERAN-Core","0205","2","B","RP-170060","","","","",""]
["R6-170136","Introduction of Extended Access Burst for connectionless Multilateration Positioning","Nokia Germany","Juergen Hofmann","68332","CR","Agreement","","","15","6.1.1","Core aspects (WI code: ePOS_GERAN-Core)",0,"agreed","2017-02-20T14:52:30.103","2017-02-20T14:57:25.907","R6-170102","","Rel-14","45.003","14.0.0","ePOS_GERAN-Core","0144","2","B","RP-170060","","","","",""]
["R6-170137","Introduction of Timing Advance Multilateration","Ericsson LM","Nicklas Johansson","47575","CR","Agreement","","","16","6.1.2","Performance aspects (WI code: ePOS_GERAN-Perf)",0,"postponed","2017-02-20T14:52:30.883","2017-02-20T14:57:25.907","R6-170107","","Rel-14","45.010","13.4.0","ePOS_GERAN-Perf","0071","3","B","","","","","",""]
["R6-170138","Introduction of Extended Access Burst for connectionless Multilateration Positioning","Nokia","Juergen Hofmann","68332","CR","Agreement","","","16","6.1.2","Performance aspects (WI code: ePOS_GERAN-Perf)",0,"agreed","2017-02-20T14:52:31.727","2017-02-20T14:57:26.093","R6-170108","","Rel-14","45.005","13.3.0","ePOS_GERAN-Perf","0598","2","B","RP-170551","","","","",""]
["R6-170139","Introduction of Alternative Mappings for Higher Coverage Classes with 2 PDCHs","Nokia","Juergen Hofmann","68332","CR","Agreement","","","19","6.3.1","Core aspects (WI code: CIoT_EC_GSM_radio_enh-Core)",0,"agreed","2017-02-20T14:52:32.583","2017-02-20T14:57:26.093","R6-170113","","Rel-14","44.018","14.0.0","CIoT_EC_GSM_radio_enh-Core","1056","2","B","RP-170061","","","","",""]
["R6-170140","Introduction of Alternative Mappings for Higher Coverage Classes with 2 PDCHs","Nokia","Juergen Hofmann","68332","CR","Agreement","","","19","6.3.1","Core aspects (WI code: CIoT_EC_GSM_radio_enh-Core)",0,"agreed","2017-02-20T14:52:33.377","2017-02-20T14:57:26.110","R6-170114","","Rel-14","44.060","13.4.0","CIoT_EC_GSM_radio_enh-Core","1635","2","B","RP-170061","","","","",""]
["R6-170141","New Uplink Coverage Class CC5 - Link Layer Aspects","Nokia Germany","Juergen Hofmann","68332","discussion","Agreement","","All WAs agreed.","19","6.3.1","Core aspects (WI code: CIoT_EC_GSM_radio_enh-Core)",0,"noted","2017-02-20T14:52:34.157","2017-02-20T14:57:26.110","R6-170063","","","","","","","","","","","","","",""]
["R6-170142","Introduction of new uplink coverage class CC5 for EC PDTCH and EC PACCH","Nokia Germany","Juergen Hofmann","68332","CR","Agreement","","","19","6.3.1","Core aspects (WI code: CIoT_EC_GSM_radio_enh-Core)",0,"postponed","2017-02-20T14:52:34.190","2017-02-20T14:57:26.110","R6-170117","","Rel-14","45.001","14.0.0","CIoT_EC_GSM_radio_enh-Core","0097","2","B","","","","","",""]
["R6-170143","Exception request WI ePOS_GERAN","Rapporteur (Ericsson LM)","Paolino Usai","3209","WI exception request","Agreement","","","14","6.1","Positioning enhancements for GERAN",0,"revised","2017-02-20T14:52:34.953","2017-02-20T14:57:26.123","","R6-170152","","","","ePOS_GERAN","","","","","","","","",""]
["R6-170144","Exception request WI CIoT_EC_GSM_radio_enh","Rapporteur (Nokia)","Paolino Usai","3209","WI exception request","Agreement","","","18","6.3","Radio Interface Enhancements for EC-GSM-IoT",0,"revised","2017-02-20T14:52:34.970","2017-02-20T14:57:26.123","","R6-170156","","","","CIoT_EC_GSM_radio_enh","","","","","","","","",""]
["R6-170145","WI status report Positioning enhancements for GERAN (WI code: ePOS_GERAN)","Rapporteur (Ericsson LM)","Paolino Usai","3209","WI status report","Agreement","","","14","6.1","Positioning enhancements for GERAN",0,"agreed","2017-02-20T14:52:34.987","2017-02-20T14:57:26.123","R6-170010","","","","","ePOS_GERAN","","","","","","","","",""]
["R6-170146","WI status report Radio Interface Enhancements for EC-GSM-IoT (WI code: CIoT_EC_GSM_radio_enh)","Rapporteur (Nokia)","Paolino Usai","3209","WI status report","Agreement","","","18","6.3","Radio Interface Enhancements for EC-GSM-IoT",0,"revised","2017-02-20T14:52:35.017","2017-02-20T14:57:26.140","","R6-170155","","","","CIoT_EC_GSM_radio_enh","","","","","","","","",""]
["R6-170147","3GPP RAN WG6 Work Plan","Editor (Ericsson LM)","Paolino Usai","3209","Work Plan","Agreement","","","25","9","Revision of the work plan",0,"revised","2017-02-20T14:52:35.033","2017-02-20T14:57:26.140","","R6-170157","","","","","","","","","","","","",""]
["R6-170148","CR 43.059-0081 rev 6 Introduction of Multilateration (Rel-14)","Ericsson LM","Nicklas Johansson","47575","CR","Approval","","","15","6.1.1","Core aspects (WI code: ePOS_GERAN-Core)",0,"revised","2017-02-20T14:52:35.047","2017-02-20T14:57:26.140","R6-170130","R6-170151","Rel-14","43.059","13.2.0","ePOS_GERAN-Core","0081","7","B","","","","","",""]
["R6-170149","Introduction of Extended Access Burst for connectionless Multilateration Positioning","Nokia","Juergen Hofmann","68332","CR","Agreement","","","15","6.1.1","Core aspects (WI code: ePOS_GERAN-Core)",0,"agreed","2017-02-20T14:52:35.797","2017-02-20T14:57:26.157","R6-170134","","Rel-14","45.001","14.0.0","ePOS_GERAN-Core","0096","3","B","RP-170060","","","","",""]
["R6-170150","Introduction of Multilateration OTD","Nokia","Juergen Hofmann","68332","CR","Agreement","","","15","6.1.1","Core aspects (WI code: ePOS_GERAN-Core)",0,"agreed","2017-02-20T14:52:36.733","2017-02-20T14:57:26.157","R6-170133","","Rel-14","43.059","13.2.0","ePOS_GERAN-Core","0082","3","B","RP-170060","","","","",""]
["R6-170151","Introduction of Multilateration","Ericsson LM","Nicklas Johansson","47575","CR","Approval","","","15","6.1.1","Core aspects (WI code: ePOS_GERAN-Core)",0,"agreed","2017-02-20T14:52:37.607","2017-02-20T14:57:26.157","R6-170148","","Rel-14","43.059","13.2.0","ePOS_GERAN-Core","0081","8","B","RP-170060","","","","",""]
["R6-170152","Exception request WI ePOS_GERAN","Rapporteur (Ericsson LM)","Paolino Usai","3209","WI exception request","Agreement","","","14","6.1","Positioning enhancements for GERAN",0,"agreed","2017-02-20T14:52:38.417","2017-02-20T14:57:26.170","R6-170143","","","","","","","","","","","","","",""]
["R6-170153","Clarifyifying EC_Access_Control_Class Operation for  EC-GSM","Ericsson Inc.","John Diachina","25840","CR","Approval","The EC-BCCH CHANGE MARK field is currently incremented every time one or more EC SI messages have changed. However, an exception condition needs to be supported to allow for the case where PLMN specific barring is enabled in a cell (i.e. EC SI 2 and EC SI 4 are transmitted and provide PLMN specific barring information) and changes are made to the EC_Access_Control_Class field or Exception_Report_Status field included in the EC SI 2 and EC SI 4 messages. In this case the network is expected to make frequent changes to these fields for as long as PLMN specific barring remains enabled. As such changes to these fields alone should not cause the value of EC-BCCH CHANGE MARK field to be incremented while PLMN specific barring remains enabled.","","10","5.2","Extended Coverage GSM for support of Cellular Internet of Things (WI codes: CIoT_EC_GSM-Core, CIoT_EC_GSM-Perf)",0,"agreed","2017-02-20T14:52:38.433","2017-02-20T14:57:26.170","R6-170124","","Rel-13","44.018","13.4.0","CIoT_EC_GSM-Core","1053","3","F","RP-170064","","","","",""]
["R6-170154","Clarifyifying EC_Access_Control_Class Operation for  EC-GSM","Ericsson Inc.","John Diachina","25840","CR","Approval","The EC-BCCH CHANGE MARK field is currently incremented every time one or more EC SI messages have changed. However, an exception condition needs to be supported to allow for the case where PLMN specific barring is enabled in a cell (i.e. EC SI 2 and EC SI 4 are transmitted and provide PLMN specific barring information) and changes are made to the EC_Access_Control_Class field or Exception_Report_Status field included in the EC SI 2 and EC SI 4 messages. In this case the network is expected to make frequent changes to these fields for as long as PLMN specific barring remains enabled. As such changes to these fields alone should not cause the value of EC-BCCH CHANGE MARK field to be incremented while PLMN specific barring remains enabled.","","10","5.2","Extended Coverage GSM for support of Cellular Internet of Things (WI codes: CIoT_EC_GSM-Core, CIoT_EC_GSM-Perf)",0,"agreed","2017-02-20T14:52:39.290","2017-02-20T14:57:26.170","R6-170125","","Rel-14","44.018","14.0.0","CIoT_EC_GSM-Core","1054","3","A","RP-170064","","","","",""]
["R6-170155","WI status report Radio Interface Enhancements for EC-GSM-IoT (WI code: CIoT_EC_GSM_radio_enh)","Rapporteur (Nokia)","Paolino Usai","3209","WI status report","Agreement","","","18","6.3","Radio Interface Enhancements for EC-GSM-IoT",0,"agreed","2017-02-20T14:52:40.163","2017-02-20T14:57:26.187","R6-170146","","","","","CIoT_EC_GSM_radio_enh","","","","","","","","",""]
["R6-170156","Exception request WI CIoT_EC_GSM_radio_enh","Rapporteur (Nokia)","Paolino Usai","3209","WI exception request","Agreement","","","18","6.3","Radio Interface Enhancements for EC-GSM-IoT",0,"agreed","2017-02-20T14:52:40.197","2017-02-20T14:57:26.187","R6-170144","","","","","CIoT_EC_GSM_radio_enh","","","","","","","","",""]
["R6-170157","3GPP RAN WG6 Work Plan","Editor (Ericsson LM)","Paolino Usai","3209","Work Plan","Agreement","","","25","9","Revision of the work plan",0,"agreed","2017-02-20T14:52:40.227","2017-02-20T14:57:26.187","R6-170147","","","","","","","","","","","","","",""]

{"sheet":"CR_Packs_List","index":1,"n_rows":1,"n_cols":11,"rows_kept":1,"cut":false,"hidden":false,"merged":[]}
["CR Pack TDoc","WG Tdoc","WG TDoc decision","CR Individual TSG decision","Spec","CR","CR revision","CR category","Release","Version","CR title"]

{"sheet":"Parameters","index":2,"n_rows":25,"n_cols":4,"rows_kept":25,"cut":false,"hidden":true,"merged":[]}
["Types of Tdocs","Possible statuses of Tdocs","Categories"]
[]
["agenda","reserved","A","Decision"]
["Work Plan","available","B","Agreement"]
["LS in","revised","C","Approval"]
["LS out","agreed","D","Information"]
["pCR","conditionally agreed","E","Discussion"]
["draftCR","approved","F","Action"]
["CR","conditionally approved",null,"Endorsement"]
["CR pack","partially approved",null,"Presentation"]
["ToR","treated"]
["WID new","endorsed"]
["WID revised","replied to"]
["SID new","merged"]
["SID revised","not pursued"]
["WI status report","postponed"]
["WI exception request","noted"]
["TS or TR cover","not concluded"]
["draft TS","withdrawn"]
["draft TR","reissued"]
["report","not treated"]
["discussion"]
["response"]
["other"]
["WI summary"]