Association (gtpInclusions:GroupTerminationPoint) (theSNCCreateData:SNCCreateData)

Documentation
Specifies a list of GTPs that must be used by the bundled SNC. The list must be empty if no GTP constraint is required. If the EMS cannot fully satisfy the constraints, then the request will be rejected.

Derived | No | Link Class | --Not Defined--
Element 1 | GroupTerminationPoint | Element 2 | SNCCreateData
Role 1 | gtpInclusions | Role 2 | --Not Named--