tmf854.v1 > TandemSwitching_T LOCATION: file:/xsd/networkResources/PGPParameters.xsd
SECTIONS: Basic | XML | Reference Overview | TOC | No TOC | Help
tmf854.v1
The TandemSwitching_T Simple Type
This attribute specifies whether the switching capability of the protection group is independent of the switching of any other group (empty string) or if its operation is associated with, related to or synchronised to the operation of another identified group (PGPName). Value is Empty string or "PGPName".
<ApplicableTo>1+1 trail protection</ApplicableTo>
Simple Type TandemSwitching_T
TandemSwitching_T is derived from string type. There are several restrictions on the value. The schema processor preserves value's whitespace.

XML
-<xsd:simpleType name="TandemSwitching_T"> -<xsd:annotation> -<xsd:documentation> This attribute specifies whether the switching capability of the protection group is independent of the switching of any other group (empty string) or if its operation is associated with, related to or synchronised to the operation of another identified group (PGPName). Value is Empty string or "PGPName". <ApplicableTo>1+1 trail protection</ApplicableTo> </xsd:documentation> </xsd:annotation> <xsd:restriction base="xsd:string"> </xsd:restriction> </xsd:simpleType>

﻿

Uses
Type (1) string

Used-By
Element (1) PGPParameters_T/TandemSwitching

Generated by WSDLdoc ©