This operation deletes a Termination Point Pool.
This operation is idempotent; i.e. if the operation is called with the name of a non-existent Termination Point Pool, it will succeed.

Operation Exceptions:
1. NOT_IMPLEMENTED - Raised when the EMS does not support deletion of TPPools via this interface.
2. INTERNAL_ERROR - Raised in case of non-specific EMS internal failure.
3. INVALID_INPUT - Raised when the input parameter is syntactically incorrect.
4. OBJECT_IN_USE - Raised when the TPPool is used, i.e. not all of its members are idle.
