The name of the object to which this selection applies. This may be: 
- ManagedElement: The selection applies to all termination points contained within the managed element.
- TerminationPoint: The selection applies only to the named termination point which will be a PTP or a CTP.
Unlike the case for managed element, the operation will not apply to any "contained" TPs when a PTP or CTP is specified.
Note: as noted in the requirements, the possible scopes do not include "SNC".

Readable by NMS? Yes
Writeable by NMS? No
Invariant? Yes
