tmf854.v1 > SNCType_T LOCATION: file:/xsd/networkResources/SubnetworkConnection.xsd
SECTIONS: Basic | XML | Reference Overview | TOC | No TOC | Help
tmf854.v1
The SNCType_T Simple Type
The SNC Type describes the connection based on the signal flows. For a detailed description of the use of this attribute see SNC Types. In case of an ATM SNC (VP or VC), ST_SIMPLE is used to specify a 'plain' (hard or regular) PVC.
Simple Type SNCType_T
SNCType_T is derived from string type. There are several restrictions on the value. The schema processor preserves value's whitespace. Enumeration values are (ST_SIMPLE | ST_ADD_DROP_A | ST_ADD_DROP_Z | ST_INTERCONNECT | ST_DOUBLE_INTERCONNECT | ST_DOUBLE_ADD_DROP | ST_OPEN_ADD_DROP | ST_EXPLICIT).

Enumeration | Description
ST_SIMPLE |
ST_ADD_DROP_A |
ST_ADD_DROP_Z |
ST_INTERCONNECT |
ST_DOUBLE_INTERCONNECT |
ST_DOUBLE_ADD_DROP |
ST_OPEN_ADD_DROP |
ST_EXPLICIT |

XML
-<xsd:simpleType name="SNCType_T"> -<xsd:annotation> <xsd:documentation> The SNC Type describes the connection based on the signal flows. For a detailed description of the use of this attribute see SNC Types. In case of an ATM SNC (VP or VC), ST_SIMPLE is used to specify a 'plain' (hard or regular) PVC. </xsd:documentation> </xsd:annotation> -<xsd:restriction base="xsd:string"> <xsd:enumeration value="ST_SIMPLE" /> <xsd:enumeration value="ST_ADD_DROP_A" /> <xsd:enumeration value="ST_ADD_DROP_Z" /> <xsd:enumeration value="ST_INTERCONNECT" /> <xsd:enumeration value="ST_DOUBLE_INTERCONNECT" /> <xsd:enumeration value="ST_DOUBLE_ADD_DROP" /> <xsd:enumeration value="ST_OPEN_ADD_DROP" /> <xsd:enumeration value="ST_EXPLICIT" /> </xsd:restriction> </xsd:simpleType>

﻿

Uses
Type (1) string

Used-By
Element (2) CrossConnect_T/ccType SubnetworkConnection_T/sncType

Generated by WSDLdoc ©