tmf854.v1 > retrieveSwitchDataResponse_T > switchDataList
LOCATION: file:/xsd/interfaces/ProtectionMgr.xsd
SECTIONS: Basic | XML Instance | Attributes | XML | Reference Overview | TOC | No TOC | Help
tmf854.v1
The switchDataList Element
The current protection switch status of the CTP, FTP or PG provided.
Element retrieveSwitchDataResponse_T/switchDataList : SwitchDataList_T [1 .. 1]
The switchDataList element cannot have "xsi:nil" as an attribute. The switchDataList element in XML instance can be substituted with other elements.

XML Instance
The current protection switch status of the CTP, FTP or PG provided. <switchDataList extVersion="xsd:string" extAuthor="xsd:string" tmf854Version="TMF854_Version_T"> <switchData extVersion="xsd:string" extAuthor="xsd:string" tmf854Version="TMF854_Version_T">SwitchData_T</switchData> [0..*] </switchDataList>

﻿

Attributes |
﻿
Name | Type | Summary
--- | --- | ---
extAuthor | string | This attribute is optional. Its form is unqualified. Show details.
Base type of extAuthor is string. There are several restrictions on the value. The schema processor preserves value's whitespace.
extVersion | string | This attribute is optional. Its form is unqualified. Show details.
Base type of extVersion is string. There are several restrictions on the value. The schema processor preserves value's whitespace.
tmf854Version | TMF854_Version_T | This attribute is optional. Its form is unqualified. Show details.
Base type of tmf854Version is string. There are several restrictions on the value. The schema processor preserves value's whitespace. The value must match "`1\.([0-9]|[A-Z]|[a-z])*`".
﻿
Name | Type | Summary
--- | --- | ---
extAuthor | string | This attribute is optional. Its form is unqualified. Show details.
Base type of extAuthor is string. There are several restrictions on the value. The schema processor preserves value's whitespace.
extVersion | string | This attribute is optional. Its form is unqualified. Show details.
Base type of extVersion is string. There are several restrictions on the value. The schema processor preserves value's whitespace.
tmf854Version | TMF854_Version_T | This attribute is optional. Its form is unqualified. Show details.
Base type of tmf854Version is string. There are several restrictions on the value. The schema processor preserves value's whitespace. The value must match "`1\.([0-9]|[A-Z]|[a-z])*`".

﻿

XML
-<xsd:element name="switchDataList" type="SwitchDataList_T"> -<xsd:annotation> <xsd:documentation> The current protection switch status of the CTP, FTP or PG provided. </xsd:documentation> </xsd:annotation> </xsd:element>

﻿

Uses
Type (1) SwitchDataList_T

Used-By

Generated by WSDLdoc ©