tmf854.v1 > NonPreEmptibleTraffic_T LOCATION: file:/xsd/networkResources/PGPParameters.xsd
SECTIONS: Basic | XML | Reference Overview | TOC | No TOC | Help
tmf854.v1
The NonPreEmptibleTraffic_T Simple Type
This indicates whether the non-pre-emptible traffic is allowed within this group.
<ApplicableTo> 1:N trail protection,2-F MSSPRING</ApplicableTo>
Simple Type NonPreEmptibleTraffic_T
NonPreEmptibleTraffic_T is derived from string type. There are several restrictions on the value. The schema processor preserves value's whitespace. Enumeration values are (ALLOWED | NOT_ALLOWED).

Enumeration | Description
ALLOWED |
NOT_ALLOWED |

XML
-<xsd:simpleType name="NonPreEmptibleTraffic_T"> -<xsd:annotation> -<xsd:documentation> This indicates whether the non-pre-emptible traffic is allowed within this group. <ApplicableTo> 1:N trail protection,2-F MSSPRING</ApplicableTo> </xsd:documentation> </xsd:annotation> -<xsd:restriction base="xsd:string"> <xsd:enumeration value="ALLOWED" /> <xsd:enumeration value="NOT_ALLOWED" /> </xsd:restriction> </xsd:simpleType>

﻿

Uses
Type (1) string

Used-By
Element (1) PGPParameters_T/NonPreEmptibleTraffic

Generated by WSDLdoc ©