Class OperationsSystem {Analysis} derived from: CommonResourceInfo

Documentation
The Operations System (OS) object is used to represent an operations system. This is no restriction as to the TMN layer, e.g., an OS instance can be used to represent an EMS. In the context of the MTOSI, there are top-level OSs which are attached to the CCV and subordinate OS which are known to a given top-level OS but not attached to the CCV.
Object Lifecycle: NA
Object Creation Notification Issued? Yes
Object Deletion Notification Issued? Yes
Object Discovery Notification Issued? Yes

Parent Package | MTOSI | Abstract | No
Export Control | PublicAccess | Link Class for | None
Class Kind | NormalClass | Cardinality | n
Space |  | Concurrency | Sequential
Persistence | No |  |

Operations

Name | Signature | Class
getAllCapabilities | void getAllCapabilities (CIS SequenceOf Structs::AVP capabilities = NA) | OperationsSystem
getOS | void getOS (OperationsSystem os = NA) | OperationsSystem
getSubordinateOS | void getSubordinateOS (Name subordinateOSName = NA, OperationsSystem subordinateOS = NA) | OperationsSystem
getAllOSs | void getAllOSs (CIS SequenceOf Logical View::MTOSI::OperationsSystem osList = empty list) | OperationsSystem
getAllOSNames | void getAllOSNames (CIS SequenceOf Name nameList = empty list) | OperationsSystem
getMD | void getMD (Name mdName = NA, ManagementDomain md = NA) | OperationsSystem
getAllMDs | void getAllMDs (CIS SequenceOf Logical View::MTOSI::ManagementDomain mdList = empty list) | OperationsSystem
getAllMDNames | void getAllMDNames (CIS SequenceOf Name nameList = empty list) | OperationsSystem
getAllTLsBetweenMDs | void getAllTLsBetweenMDs (CIS SequenceOf Logical View::TopologicalLink tlList = empty list) | OperationsSystem
getAllTLNamesBetweenMDs | void getAllTLNamesBetweenMDs (CIS SequenceOf Name nameList = empty list) | OperationsSystem
getAllTLsWrtOS | void getAllTLsWrtOS (Name osName = NA, Name mdName = NA, CIS SequenceOf Logical View::TopologicalLink tlList = empty list) | OperationsSystem
getAllTLNamesWrtOS | void getAllTLNamesWrtOS (Name osName = NA, Name mdName = NA, CIS SequenceOf Name nameList = empty list) | OperationsSystem
getAllTMDsWrtOS | void getAllTMDsWrtOS (Name osName = NA, CIS SequenceOf Logical View::TransmissionDescriptor tmdList = empty list) | OperationsSystem
getAllTMDNamesWrtOS | void getAllTMDNamesWrtOS (Name osName = NA, CIS SequenceOf Name nameList = empty list) | OperationsSystem
getAllMEsWrtOS | void getAllMEsWrtOS (Name osName = NA, Name mdName = NA, CIS SequenceOf Logical View::ManagedElement meList = empty list) | OperationsSystem
getAllMENamesWrtOS | void getAllMENamesWrtOS (Name osName = NA, Name mdName = NA, CIS SequenceOf Name nameList = empty list) | OperationsSystem
getAllSNsWrtOS | void getAllSNsWrtOS (Name osName = NA, Name mdName = NA, CIS SequenceOf Logical View::MultiLayerSubnetwork snList = empty list) | OperationsSystem
getAllSNNamesWrtOS | void getAllSNNamesWrtOS (Name osName = NA, Name mdName = NA, CIS SequenceOf Name nameList = empty list) | OperationsSystem
getAllMEsPassingFilter | void getAllMEsPassingFilter (Name mdName = NA, MEFilter filter = NA, CIS SequenceOf Logical View::ManagedElement meList = empty list) | OperationsSystem
getAllMENamesPassingFilter | void getAllMENamesPassingFilter (Name mdName = NA, MEFilter filter = NA, CIS SequenceOf Name nameList = empty list) | OperationsSystem
getInventory | void getInventory (InventoryFilter filter = NA, CIS GeneralizedTime diffDateAndTime = NA, whereAndHowToReply, InventoryData inventoryData = NA) | OperationsSystem
getActiveAlarmsCount | void getActiveAlarmsCount (ActiveAlarmFilter filter = CIS Null, CIS Integer activeAlarmCount = NA) | OperationsSystem
getActiveAlarms | void getActiveAlarms (ActiveAlarmFilter filter = CIS Null, whereAndHowToReply, alarmReply = NA) | OperationsSystem
getAllTransmissionDescriptors | void getAllTransmissionDescriptors (CIS SequenceOf TransmissionDescriptor transmissionDescriptors = empty list) | OperationsSystem
getAllTransmissionDescriptorNames | void getAllTransmissionDescriptorNames (CIS SequenceOf Name transmissionDescriptorNames = empty list) | OperationsSystem
getTransmissionDescriptor | void getTransmissionDescriptor (Name transmissionDescriptorName = NA, TransmissionDescriptor transmissionDescriptor = NA) | OperationsSystem
setNativeEMSName | void setNativeEMSName (Name objectName, CIS CharcaterString nativeEMSName) | CommonResourceInfo
setOwner | void setOwner (Name objectName, CIS CharcaterString owner) | CommonResourceInfo
setUserLabel | void setUserLabel (Name objectName, CIS CharcaterString userLabel, Boolean enforceUniqueness) | CommonResourceInfo
setNetworkAccessDomain | void setNetworkAccessDomain (CIS CharcaterString networkAccessDomain = NA) | CommonResourceInfo
setAdditionalInfo | void setAdditionalInfo (CIS SequenceOf Structs::AVP additionalInfo = empty list) | CommonResourceInfo

Attributes

Name | Class | Type | Initial Value
softwareVersion | OperationsSystem | CIS CharacterString | NA
productName | OperationsSystem | CIS CharacterString | NA
manufacturer | OperationsSystem | CIS CharacterString | empty string
serviceState | OperationsSystem | ServiceState | SERV_NA
subordinateOS | OperationsSystem | CIS Boolean | NA
name | CommonResourceInfo | Name | NA
userLabel | CommonResourceInfo | CIS CharacterString | Value of the nativeEMSName attribute.
owner | CommonResourceInfo | CIS CharacterString | empty string
nativeEMSName | CommonResourceInfo | CIS CharacterString | empty string
discoveredName | CommonResourceInfo | CIS CharacterString | empty string
namingOS | CommonResourceInfo | Name | CIS Null
source | CommonResourceInfo | ObjectSource | UNKNOWN
aliasNameList | CommonResourceInfo | AVP | empty list
resourceState | CommonResourceInfo | ResourceState | UNKNOWN
additionalInfo | CommonResourceInfo | CIS SequenceOf Structs::AVP | empty list

Associations

Name | My Role | My Class | Other Role | Other Element
has subordinate | --Not Named-- | OperationsSystem | --Not Named-- | OperationsSystem
manages | --Not Named-- | OperationsSystem | --Not Named-- | ManagementDomain
manages | --Not Named-- | OperationsSystem | --Not Named-- | ManagedElement
manages | --Not Named-- | OperationsSystem | --Not Named-- | TopologicalLink
manages | --Not Named-- | OperationsSystem | --Not Named-- | MultiLayerSubnetwork
offers | --Not Named-- | OperationsSystem | --Not Named-- | TransmissionDescriptor
retrieve active | --Not Named-- | OperationsSystem | --Not Named-- | AlarmInformation

Generalization Relationships

Name | Class | Supplier
--Not Named-- | OperationsSystem | CommonResourceInfo