Operation void deleteGroupTerminationPoint (Name gtpName = NA), in Class ManagedElement

Documentation
The delete GTP operation is used to delete a GTP. An attempt to delete a GTP that is involved in a cross connection or SNC should be rejected by the EMS.
This operation is idempotent. If the operation is called with the name of a non-existent GTP, it will succeed.
Operation Exceptions:
1. NOT_IMPLEMENTED - Raised when the EMS does not support deletion of GTPs via this interface.
2. INTERNAL_ERROR - Raised in case of non-specific EMS internal failure.
3. INVALID_INPUT - Raised when input parameter is syntactically incorrect.
4. ENTITY_NOT_FOUND - Raised when the GTP to be deleted does not exist.
5. OBJECT_IN_USE - Raised when the GTP is used in a cross connection or SNC.

Protocol |  | Qualification |
Exceptions |  | Size |
Time |  | Concurrency | Sequential
Export Control | PublicAccess |  |

Preconditions
The GTP to be deleted has to exist and must not be involved in a cross connection or SNC.
Postconditions
Identified GTP no longer exists.
Semantics

Arguments

gtpName
/* in */ The name of the Group Termination Point to be deleted.