Operation void getContainingSubnetworkNames (CIS SequenceOf Name subnetworkNameList), in Class ManagedElement

Documentation
Get the name(s) of the containing subnetwork(s) of the Managed Element.
Operation Exceptions:
1. INTERNAL_ERROR - Raised in case of non-specific EMS internal failure.
2. COMM_LOSS - Raised when communication to managed element is lost.

Protocol |  | Qualification |
Exceptions |  | Size |
Time |  | Concurrency | Sequential
Export Control | PublicAccess |  |

Preconditions
None
Postconditions
No change in the system.
Semantics

Arguments

subnetworkNameList
/* out */ The containing subnetwork name(s) of the Managed Element.